{"text_format":"1","workbook":"xlsx","n_sheets":41,"sheets":["AER only","Contents","Instructions","Business & other details","CPI series","2.1 Expenditure summary","2.2 Repex","2.3 Augex (a)","2.3 Augex (b)","2.4 Augex model","2.5 Connections","2.6 Non-network","2.10 Overheads","2.11 Labour","2.14 Forecast price changes","2.16 Opex Summary","2.17 Step Changes","3.1 Revenue","3.2 Operating expenditure","3.3 Assets (RAB)","3.4 Operational data","3.5 Physical assets","3.6 Quality of service","3.7 Operating Environment","4.1 Public lighting","4.2 Metering","4.3 Fee-based services","4.4 Quoted services","5.4 MD & utilisation-Spatial","5.4.1 Non-COIN&COIN Max Demand","5.4.2 Expected Unserved Energy","6.1 Telephone answering","6.2 Reliability & Cust serv","7.1  Policies and Procedure ","7.1  Policies and Procedures","7.2 Contingent projects","7.3 Obligations","7.4 Shared Assets","7.6 Indicative bill impact","7.7 TSS-LRMC","Amendments"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":7,"defined_names":1744,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AER only","index":0,"n_rows":147,"n_cols":40,"rows_kept":147,"cut":false,"hidden":true,"merged":[[55,34,59,34],[63,34,64,34],[69,14,69,15],[69,22,69,25],[107,1,107,8],[52,34,54,34],[0,1,0,11],[4,28,4,38],[5,28,5,31],[5,34,5,38],[50,22,50,26],[50,28,50,31],[51,1,51,5],[51,14,51,21],[51,22,51,26],[51,28,51,31],[52,2,52,3]]}
[null,"Data in these columns used for data validation and database purposes."]
[null,"Date last modified:","2017-01-16","added (Albury and Victora) for AGN"]
[null,null,"2016-10-17","updated TransGrid's correct legal name, corrected TasNetworks (T) to June financial year"]
[null,null,"2017-02-01","inserted Power and Water, added NRs (dms_FeederCat_1 and dms_FeederCat_2)"]
[null,null,"2017-03-03","inserted AEMO as a business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOR ELECTRICITY BUSINESSES ONLY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feeder Types",null,null,null,"TasNetworks (D)","MAIFI flag","Feeder Names"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","long rural","EXTRA"]
[null,"dms_TradingName_List","dms_TradingNameFull_List","dms_ABN_List","dms_JurisdictionList","dms_Sector_List","dms_Segment_List","dms_FormControl_List","dms_RPT_List","dms_RPTMonth_List","dms_CRCPlength_List","dms_FRCPlength_List","dms_663_List","dms_DeterminationRef_List","dms_Addr1_List","dms_Addr2_List","dms_Suburb_List","dms_State_List","dms_PostCode_List","dms_PAddr1_List","dms_PAddr2_List","dms_PSuburb_List","dms_PState_List","dms_PPostCode_List","dms_ContactName1_List","dms_ContactPh1_List","dms_ContactEmail_List","Column1","dms_CBD_flag","dms_Urban_flag","dms_ShortRural_flag","dms_LongRural_flag","dms_FeederType_5_flag","dms_MAIFI_flag_List","dms_FeederName_1","dms_FeederName_2","dms_FeederName_3","dms_FeederName_4","dms_FeederName_5"]
[null,"ActewAGL Distribution","ActewAGL Distribution",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","40 Bunda Street",null,"CANBERRA","ACT","2600","GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au",null,"NO","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"ActewAGL Distribution"]
[null,"ActewAGL Distribution (Tx Assets)","ActewAGL Distribution (Tx Assets)",76670568688,"ACT","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","40 Bunda Street",null,"CANBERRA","ACT","2600","GPO BOX 366",null,"CANBERRA","ACT",2601,"Robert Walker","02 6248 3847","robert.walker@actewagle.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"ActewAGL Distribution (Tx Assets)"]
[null,"ActewAGL Gas","ActewAGL Gas",76670568688,"ACT","Gas","Distribution","Weighted average price cap","Financial","June",5,5,"x",null,"40 Bunda Street",null,"CANBERRA","ACT","2600","GPO BOX 366",null,"CANBERRA","ACT",2601,"Philip Deamer","02 6248 3438","GasAAReview@actewagl.com.au",null,null,null,null,null,null,null,null,null,null,null,null,"ActewAGL Gas"]
[null,"AEMO","Australian Energy Market Operator Ltd",94072010327,"Vic","Electricity","Transmission","-","Financial","March",5,5,"x","-","Level 22","530 Collins Street","MELBOURNE","VIC","3000","GPO Box 2008",null,"MELBOURNE","VIC","3001",null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"AEMO"]
[null,"AGN (Albury and Victoria)","Australian Gas Networks Limited (reporting data for Albury and Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA","5000","PO Box 6468","Halifax Street","ADELAIDE","SA","5000","Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"AGN (Albury)"]
[null,"AGN (Albury)","Australian Gas Networks Limited (reporting data for Albury)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 6","400 King William Street","ADELAIDE","SA","5000","PO Box 6468","Halifax Street","ADELAIDE","SA","5000","Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural"]
[null,"AGN (SA)","Australian Gas Networks Limited (reporting data for SA)",19078551685,"SA","Gas","Distribution","Weighted average price cap","Financial","June",5,5,5,"distribution determination","Level 6","400 King William Street","ADELAIDE","SA","5000","PO Box 6468","Halifax Street","ADELAIDE","SA","5000","Craig de Laine","08 8418 1129 ","craig.delaine@agn.com.au",null,null,null,null,null,null,null,null,null,null,null,null,"AGN (SA)"]
[null,"AGN (Victoria)","Australian Gas Networks Limited (reporting data for Victoria)",19078551685,"Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AGN (Victoria)"]
[null,"Amadeus","APT Pipelines (NT) Pty Ltd",39009737393,"NT","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","Level 19, HSBC Building","580 George Street","SYDNEY","NSW","2000","Level 19, HSBC Building","580 George Street","SYDNEY","NSW","2000","Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au",null,null,null,null,null,null,null,null,null,null,null,null,"Amadeus"]
[null,"APA GasNet","APA GasNet Australia (Operations) Pty Ltd","065083009","Vic","Gas","Transmission","Weighted average price cap","Calendar","December",5,5,"x",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW","2000","PO Box R41",null,"ROYAL EXCHANGE","NSW","1225",null,"02 9693 0000",null,null,null,null,null,null,null,null,null,null,null,null,null,"APA GasNet"]
[null,"Ausgrid","Ausgrid",78508211731,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","570 George St",null,"SYDNEY","NSW",2000,"GPO Box 4009",null,"SYDNEY","NSW","2001","John Thomson","(02) 9269 2312","john.thomson@ausgrid.com.au",null,"YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Ausgrid"]
[null,"Ausgrid (Tx Assets)","Ausgrid (Tx Assets)",67505337385,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination",null,null,null,"NSW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Ausgrid (Tx Assets)"]
[null,"AusNet (D)","AusNet Electricity Services Pty Ltd",91064651118,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic","3006","Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","VIC",8001,null,null,null,null,null,"YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"AusNet (D)"]
[null,"AusNet (Gas)","AusNet Gas Services","086015036","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"X",null,"Level 19, HSBC Building","580 George Street","SYDNEY","NSW","2000","PO Box R41",null,"ROYAL EXCHANGE","NSW","1225","Alexandra Curran","02 9275 0020","alexandra.curran@apa.com.au",null,null,null,null,null,null,null,null,null,null,null,null,"AusNet (Gas)"]
[null,"AusNet (T)","Ausnet Services (Transmission) Ltd",48116124362,"Vic","Electricity","Transmission","Revenue cap","Financial","March",5,5,2,"transmission determination","Level 32","2 Southbank Boulevard","SOUTHBANK","Vic","3006","Locked Bag 14051",null,"MELBOURNE CITY MAIL CENTRE","Vic","8001","Clare Thompson","03 9695 6670","clare.e.thompson@ausnetservices.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"AusNet (T)"]
[null,"Australian Distribution Co.","Australian Distribution Co.",11222333444,"-","Electricity","Distribution","Revenue cap","Financial","June",5,5,2,"distribution determination","123 Straight Street",null,"SYDNEY","NSW","2000","PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Australian Distribution Co."]
[null,"Australian Distribution Co. (Vic)","Australian Distribution Co. (Victoria)",11222333444,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"distribution determination","123 Straight Street",null,"MELBOURNE","Vic","3000","PO Box 123",null,"MELBOURNE","VIC","3000","Bob Smith","02 1234 5678","bob@auselec.net.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Australian Distribution Co. (Vic)"]
[null,"Australian Transmission Co.","Australian Transmission Co.",11222333444,"-","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","123 Straight Street",null,"SYDNEY","NSW","2000","PO Box 123",null,"SYDNEY","NSW",2000,"Bob Smith","02 1234 5678","bob@auselec.net.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Australian Transmission Co."]
[null,"CitiPower","CitiPower",76064651056,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic","3000","Locked Bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au",null,"YES","YES","NO","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"CitiPower"]
[null,"Directlink","Directlink",16779340889,"Qld","Electricity","Transmission","Revenue cap","Financial","June",9,5,5,"transmission determination","Level 19, HSBC Building","580 George Street","SYDNEY","NSW","2000","PO Box R41",null,"ROYAL EXCHANGE","NSW","1225","Scott Young","02 9275 0031","scott.young@apa.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Directlink"]
[null,"ElectraNet","ElectraNet",41094482416,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","52-55 East Terrace","Rymill Park","ADELAIDE","SA","5000","PO Box 7096","Hutt Street Post Office","ADELAIDE","SA",5000,"Bill Jackson","08 8404 7969","jackson.bill@electranet.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"ElectraNet"]
[null,"Endeavour Energy","Endeavour Energy",11247365823,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","51 Huntingwood Drive",null,"HUNTINGWOOD","NSW","2148","PO Box 811",null,"SEVEN HILLS","NSW","1730","Jon Hocking","02 9853 4386 / 0407 348 156","Jon.Hocking@Endeavourenergy.com.au",null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Endeavour Energy"]
[null,"Energex","Energex",40078849055,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","26 Reddacliff Street",null,"NEWSTEAD","Qld","4006","26 Reddacliff Street",null,"NEWSTEAD","QLD","4006","Nicola Roscoe","07 3664 5891","nicolaroscoe@energex.com.au",null,"YES","YES","YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"Energex"]
[null,"Ergon Energy","Ergon Energy",50087646062,"Qld","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","22 Walker Street",null,"TOWNSVILLE","Qld","4810","Po Box 264",null,"FORTITUDE VALLEY","QLD",4006,"Jenny Doyle, Group Manager Regulatory Affairs","(07) 3851 6416","jenny.doyle@ergon.com.au",null,"NO","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Ergon Energy"]
[null,"Essential Energy","Essential Energy",37428185226,"NSW","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2014-19 Distribution Determination","8 Buller Street",null,"PORT MACQUARIE","NSW","2444","PO Box 5730",null,"PORT MACQUARIE","NSW","2444","Catherine Waddell","02 6338 3553","catherine.waddell@essentialenergy.com.au",null,null,null,"YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Essential Energy"]
[null,"Jemena Electricity","Jemena Electricity",82064651083,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 16","567 Collins Street","MELBOURNE","VIC","3000","PO Box 16182",null,"MELBOURNE","VIC",8001,"Matthew Serpell","03 9173 8231","matthew.serpell@jemena.com.au",null,null,null,"YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"Jemena Electricity"]
[null,"JGN","Jemena Gas Networks (NSW) Ltd","003 004 322","NSW","Gas","Distribution","Weighted average price cap","Financial","June",5,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JGN"]
[null,"Multinet Gas","Multinet Gas (DB No.1) Pty Ltd (ACN 086 026 986), Multinet Gas (DB No.2) Pty Ltd (ACN 086 230 122)","086026986","Vic","Gas","Distribution","Weighted average price cap","Calendar","December",5,5,"x",null,"6 Nexus Court",null,"MULGRAVE","Vic","3149",null,null,null,null,null,"Stephanie McDougall","03 8846 9538","Stephanie.McDougall@ue.com.au",null,null,null,null,null,null,null,null,null,null,null,null,"Multinet Gas"]
[null,"Murraylink","Murraylink",79181207909,"SA","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","Level 19","580 George Street","SYDNEY","NSW","2000",null,null,null,null,null,"Scott Young","02 9275 0031","scott.young@apa.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Murraylink"]
[null,"Power and Water","Power and Water Corporation",15947352360,"NT","Electricity","Distribution","Revenue cap","Financial","June",5,5,"x","distribution determination","GPO Box 1921",null,"DARWIN","NT","0801","GPO Box 1921",null,"DARWIN","NT","0801","Lucy Moon","08 8924 5822","Lucy.Moon@powerwater.com.au",null,"YES","YES","YES","YES","NO",null,"CBD","Urban","Short rural","Long rural"]
[null,"Powercor Australia","Powercor Australia",89064651109,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","40 Market Street",null,"MELBOURNE","Vic","3000","Locked bag 14090",null,"MELBOURNE","VIC",8001,"Hannah Williams","03 9683 4088","hwilliams@powercor.com.au",null,null,null,"YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Powercor Australia"]
[null,"Powerlink","Queensland Electricity Transmission Corporation Limited trading as Powerlink Queensland",82078849233,"Qld","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","33 Harold St",null,"VIRGINIA","Qld","4014","PO Box 1193",null,"VIRGINIA","QLD",4014,"Jennifer Harris","07 3860 2667","jharris@powerlink.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Powerlink"]
[null,"Roma to Brisbane Pipeline","APT Petroleum Pipelines Limited t/a Roma to Brisbane Pipeline","009 737 393","Qld","Gas","Transmission","Weighted average price cap","Financial","June",5,5,"x","n/a","580 George Street",null,"SYDNEY","NSW","2000","PO Box R41",null,"ROYAL EXCHANGE","NSW","1225","Mark Allen","02 9275 0010","mark.allen@apa.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"Roma to Brisbane Pipeline"]
[null,"SA Power Networks","SA Power Networks",13332330749,"SA","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"2015-20 Distribution Determination","1 Anzac Highway",null,"KESWICK","SA","5035","GPO Box 77",null,"ADELAIDE","SA","5000","Richard Sibly","08 8404 5613","richard.sibly@sapowernetworks.com.au",null,null,null,"YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"SA Power Networks"]
[null,"TasNetworks (D)","TasNetworks (D)",24167357299,"Tas","Electricity","Distribution","Revenue cap","Financial","June",5,5,5,"distribution determination","1-7 Maria Street",null,"LENAH VALLEY","Tas","7008","PO Box 606",null,"MOONAH","Tas","7009","John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au",null,"YES","YES","YES","YES","YES",null,"Critical Infrastructure","High density commercial","Urban","High density rural","Low density rural","TasNetworks (D)"]
[null,"TasNetworks (T)","TasNetworks (T)",24167357299,"Tas","Electricity","Transmission","Revenue cap","Financial","June",5,5,5,"transmission determination","1-7 Maria Street",null,"LENAH VALLEY","Tas","7008","PO Box 606",null,"MOONAH","Tas","7009","John Sayers","03 6271 6469","john.sayers@tasnetworks.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"TasNetworks (T)"]
[null,"TransGrid","NSW Electricity Networks Operations Pty Ltd trading as TransGrid",609169959,"NSW","Electricity","Transmission","Revenue cap","Financial","June",5,4,5,"transmission determination","180 Thomas Street",null,"SYDNEY","NSW","2000","PO Box A1000",null,"SYDNEY SOUTH","NSW","1235","Garrie Chubb","0408 210 221","garrie.chubb@transgrid.com.au",null,null,null,null,null,null,null,"CBD","Urban","Short rural","Long rural",null,"TransGrid"]
[null,"United Energy","United Energy",70064651029,"Vic","Electricity","Distribution","Revenue cap","Calendar","December",5,5,2,"2016-20 Distribution Determination","Level 3","6 Nexus Court","MULGRAVE","Vic","3149","PO Box 449",null,"MOUNT WAVERLEY","VIC",3170,"Mathew Abraham","03 8846 9758","mathew.abraham@ue.com.au",null,null,null,"YES","NO","NO",null,"CBD","Urban","Short rural","Long rural",null,"United Energy"]
[null,"Western Power (D)","Western Power (D)",18540492861,"WA","Electricity","Distribution","Revenue cap","Financial","June",12,4,"x","distribution determination","363 Wellington Street",null,"PERTH","WA","6000","GPO Box L921",null,"PERTH","WA",6842,"Judy Hunter","08 9326 6239","judy.hunter@westernpower.com.au",null,null,null,"YES","YES","NO","NO","CBD","Urban","Short rural","Long rural",null,"Western Power (D)"]
[null,"Western Power (T)","Western Power (T)",18540492861,"WA","Electricity","Transmission","Revenue cap","Financial","June",12,4,"x","transmission determination","363 Wellington Street",null,"PERTH","WA","6000","GPO Box L921",null,"PERTH","WA",6842,"Judy Hunter","08 9326 6239","judy.hunter@westernpower.com.au",null,null,null,"YES","YES","NO",null,"CBD","Urban","Short rural","Long rural",null,"Western Power (T)"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For EB & Reset RINs only",null,null,null,null,null,"For AARs only"]
[null,"The Reg Year Ending (dms_RYE) must be set to the last year of the regulatory period. For forecast data is is usually (FRCP_y5) for actual it is a single year (CRY). For historical actual data the RYE will need to be set manually in the business details sheet by setting the dms_Multiyear_flag to 1 and putting the correct value in 'dms_Specified_FinalYear. See cells C67:C68",null,null,null,null,{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2013-14"},null,null,null,null,null,null,"Drop down selector box for CA & Reset RINs.","For CA & Reset RINs only",null,null,null,null,null,null,null,"for DNSP only",null,null,null,null,null,"For DNSPs only",null,null,null,null,null,"Reason for interruption","dms_Reason_Interruption_Detailed","dms_Reason_Interruption"]
[null,"dms_Model_List ","DELETE NR 'CRY' IF NOT AN ANNUAL RIN (EB, CA , ARR)",null,"dms_RYE_Formula_Result",null,null,null,null,null,null,null,null,"dms_0203_ProjectType","dms_020303_01_UOM","dms_020501_01_UOM","dms_020501_02_UOM","dms_020501_03_UOM","dms_020501_04_UOM","dms_020603_01_UOM","dms_040102_01_UOM","dms_040102_04_UOM","dms_030601_01_UOM","dms_030601_02_UOM","dms_030701_01_UOM","dms_030702_01_UOM","dms_030703_01_UOM",null,"dms_030605_UOM","dms_03060703_UOM",null,null,null,null,"Animal","Animal impact","Animal"]
[null,"ARR","ANNUAL REPORTING STATEMENT",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":{"$error":"#REF!"}},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","0's","days","minutes/customer","minutes/customer","Customer / km","%","km",null,"number","number",null,null,null,null,null,"Animal nesting/burrowing, etc and other","Asset failure"]
[null,"CA","CATEGORY ANALYSIS",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":{"$error":"#REF!"}},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"New line on new route - dual circuit","Circuit line length in km","0's","0's","0's","0's","0's","0's","0's","minutes/customer","minutes/customer","MWh/customer","Number of spans",null,null,"number","number",null,null,null,null,null,"Other","Other"]
[null,"CPI","CPI",null,null,null,null,null,null,null,null,null,null,"New line on new route - other","Circuit line length in km","MVA added","MVA added","MVA added","MVA added","0's","0's","$0s","interruptions/customer","interruptions/customer","kVA / customer","Number of spans",null,null,"number","number",null,null,null,null,"Asset failure","LV","Overloads"]
[null,"EB","ECONOMIC BENCHMARKING",null,{"$f":"LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)","v":{"$error":"#REF!"}},"=LEFT(dms_SingleYear_FinalYear_Result,2)&RIGHT(dms_SingleYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Line rebuild over existing route - single circuit","Circuit line length in km","0's","0's","0's","0's","0's","$0s","0's","interruptions/customer","interruptions/customer",null,"Number of spans",null,null,"number","number",null,null,null,null,null,"Distribution substation","Planned"]
[null,"PTRM","POST TAX REVENUE MODEL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2024"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Line rebuild over existing route - dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s","(per cent)",null,null,null,null,null,"Number of spans",null,null,"number","(per cent)",null,null,null,null,null,"HV","Network business"]
[null,"Reset","REGULATORY REPORTING STATEMENT",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2024"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,"Formula errors are OK",null,null,null,null,null,"Reconductor - Single circuit","Number","net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,null,null,null,null,null,"Years",null,null,"number",null,null,null,null,null,null,"Zone substation","Third party"]
[null,"RFM","ROLL FORWARD MODEL",null,{"$f":"LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)","v":"2019"},"=LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)",null,null,null,null,null,null,null,"Reconductor - Dual circuit","Number","total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,"Years",null,null,"number",null,null,null,null,null,null,"Subtransmission","Unknown"]
[null,"WACC","WEIGHTED AVERAGE COST OF CAPITAL",null,{"$f":"LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)","v":"2024"},"=LEFT(dms_MultiYear_FinalYear_Result,2)&RIGHT(dms_MultiYear_FinalYear_Result,2)",null,null,null,null,null,null,null,"Other",null,"net circuit km added","net circuit km added","net circuit km added","net circuit km added",null,null,null,null,null,null,"Trees",null,null,"number",null,null,null,null,null,"Other","insert description of 'other'","Vegetation"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total spend $0s","total spend $0s","total spend $0s","total spend $0s",null,null,null,null,null,null,"Trees",null,null,"number",null,null,null,null,null,"Overloads","-","Weather"]
[null,"dms_DataQuality_List",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,"$0s",null,null,null,null,null,null,null,"Defects",null,null,"number",null,null,null,null,null,"Planned","-","2 - STPIS Exclusion (3.3)(a)"]
[null,"Actual",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,"Defects",null,null,"number",null,null,null,null,null,"Network business","Network error","3 - STPIS Exclusion (3.3)(a)"]
[null,"Estimate",null,null,null,null,null,null,null,null,null,null,null,null,null,"0's",null,null,null,null,null,null,null,null,null,"Spans",null,null,"number",null,null,null,null,null,null,"Switching and protection error","4 - STPIS Exclusion (3.3)(a)"]
[null,"Consolidated",null,null,null,null,null,null,null,null,null,null,null,null,null,"$0s",null,null,null,null,null,null,null,null,null,"km",null,null,"(per cent)",null,null,null,null,null,"Third party","Fire","5 - STPIS Exclusion (3.3)(a)"]
[null,"Recast",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spans",null,null,"(per cent)","",null,null,null,null,null,"Other","6 - STPIS Exclusion (3.3)(a)"]
[null,"Public",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dig-in","7 - STPIS Exclusion (3.3)(a)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unauthorised access"]
[null,"For all files either AER or business needs to be able to specify the type of submission","For PTRM & RFM templates we must provide a choice in case they change their form of control - otherwise it is drawn from the business specific lookup table above.",null,null,null,null,null,null,null,null,null,null,null,"For PTRM files - this field set the text for the named range \"DMS_Xfactor\" which in all cases is simply the text \"x factors\" - this saves putting in each old gas PTRM file ",null,null,null,null,null,null,null,"for TNSP only",null,null,null,null,null,null,null,null,null,null,null,null,"Vehicle impact"]
[null,"dms_SourceList","dms_FormControl_Choices",null,null,null,null,null,null,null,null,null,null,null,"DMS_Xfactor",null,null,null,null,null,null,null,"dms_030601_01_UOM",null,"dms_030701_01_UOM","dms_030702_01_UOM",null,null,null,null,null,null,null,null,"Unknown","Unknown"]
[null,"After appeal","Revenue cap",null,null,null,null,null,null,null,null,null,null,null,"x factors",null,null,null,null,null,null,null,"%",null,"Number of spans","km",null,null,null,null,null,null,null,null,"Vegetation","Blow-in/Fall-in - NSP responsibility"]
[null,"Draft decision","Revenue yield",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Years","%",null,null,null,null,null,null,null,null,null,"Grow-in - NSP responsibility"]
[null,"Final decision","Weighted average price cap",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Trees","km",null,null,null,null,null,null,null,null,null,"Blow-in/Fall-in - Other responsible party"]
[null,"PTRM update 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"Defects","number",null,null,null,null,null,null,null,null,null,"Grow-in - Other responsible party"]
[null,"PTRM update 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans",null,null,null,null,null,null,null,null,null,"Weather"]
[null,"PTRM update 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"km",null,null,null,null,null,null,null,null,null,"2 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,"km",null,null,null,null,null,null,null,null,null,"3 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,"Number of spans",null,null,null,null,null,null,null,null,null,"4 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,null,null,null,null,null,null,null,null,null,null,"5 - STPIS Exclusion (3.3)(a)"]
[null,"PTRM update 7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%",null,null,null,null,null,null,null,null,null,null,null,"6 - STPIS Exclusion (3.3)(a)"]
[null,"Regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number",null,null,null,null,null,null,null,null,null,null,null,"7 - STPIS Exclusion (3.3)(a)"]
[null,"Reporting",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,"Revised regulatory proposal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"%"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"number"]
[]
[]
[]
[null,"These are indeces and lookup values for various dates. All step from the value placed in FRCP_y1 on the business and other details worksheet",null,null,null,null,null,null,null,null,null,"These date tables are currently used in the Recast templates to provide column headings and conditional formatting"]
[null,"dms_FRCPlength_Num_List","dms_FinalYear_List","dms_CRCPlength_Num_List","dms_CFinalYear_List","dms_FRCP_years",null,"dms_CRCP_years",null,"dms_CRCP_index",null,"CRY from input cell on business sheet","CRY - financial","dms_FinYears","CRY calendar","dms_CalYears"]
[null,1,"dms_FRCP_y1",1,"CRCP_y1",{"$f":"FRCP_y1","v":"2019-20"},"dms_FRCP_y1",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)-1)&\"-\"&TEXT(VALUE(MID(dms_FRCP_y1,3,2)),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)-1))","v":"2018-19"},"dms_CRCP_yZ",1,null,{"$f":"CRY","v":{"$error":"#REF!"}},{"$f":"VALUE(LEFT(CRY,4))&\"-\"&TEXT(MID(CRY,3,2)+1,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y1",{"$f":"VALUE(LEFT(CRY,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y1"]
[null,2,"dms_FRCP_y2",2,"CRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y1,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y1,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y1,4)+1))","v":"2020-21"},"dms_FRCP_y2",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yZ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yZ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yZ,4)-1))","v":"2017-18"},"dms_CRCP_yY",2,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y1,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y1,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y2",{"$f":"VALUE(LEFT(dms_CRYc_y1,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y2"]
[null,3,"dms_FRCP_y3",3,"CRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y2,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y2,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y2,4)+1))","v":"2021-22"},"dms_FRCP_y3",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yY,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yY,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yY,4)-1))","v":"2016-17"},"dms_CRCP_yX",3,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y2,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y2,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y3",{"$f":"VALUE(LEFT(dms_CRYc_y2,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y3"]
[null,4,"dms_FRCP_y4",4,"CRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y3,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y3,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y3,4)+1))","v":"2022-23"},"dms_FRCP_y4",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yX,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yX,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yX,4)-1))","v":"2015-16"},"dms_CRCP_yW",4,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y3,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y3,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y4",{"$f":"VALUE(LEFT(dms_CRYc_y3,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y4"]
[null,5,"dms_FRCP_y5",5,"CRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y4,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y4,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y4,4)+1))","v":"2023-24"},"dms_FRCP_y5",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yW,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yW,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yW,4)-1))","v":"2014-15"},"dms_CRCP_yV",5,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y4,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y4,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y5",{"$f":"VALUE(LEFT(dms_CRYc_y4,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y5"]
[null,6,"dms_FRCP_y6",6,"CRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y5,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y5,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y5,4)+1))","v":"2024-25"},"dms_FRCP_y6",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yV,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yV,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yV,4)-1))","v":"2013-14"},"dms_CRCP_yU",6,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y5,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y5,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y6",{"$f":"VALUE(LEFT(dms_CRYc_y5,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y6"]
[null,7,"dms_FRCP_y7",7,"CRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y6,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y6,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y6,4)+1))","v":"2025-26"},"dms_FRCP_y7",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yU,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yU,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yU,4)-1))","v":"2012-13"},"dms_CRCP_yT",7,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y6,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y6,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y7",{"$f":"VALUE(LEFT(dms_CRYc_y6,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y7"]
[null,8,"dms_FRCP_y8",8,"CRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y7,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y7,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y7,4)+1))","v":"2026-27"},"dms_FRCP_y8",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yT,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yT,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yT,4)-1))","v":"2011-12"},"dms_CRCP_yS",8,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y7,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y7,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y8",{"$f":"VALUE(LEFT(dms_CRYc_y7,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y8"]
[null,9,"dms_FRCP_y9",9,"CRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y8,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y8,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y8,4)+1))","v":"2027-28"},"dms_FRCP_y9",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yS,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yS,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yS,4)-1))","v":"2010-11"},"dms_CRCP_yR",9,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y8,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y8,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y9",{"$f":"VALUE(LEFT(dms_CRYc_y8,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y9"]
[null,10,"dms_FRCP_y10",10,"CRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y9,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y9,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y9,4)+1))","v":"2028-29"},"dms_FRCP_y10",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yR,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yR,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yR,4)-1))","v":"2009-10"},"dms_CRCP_yQ",10,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y9,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y9,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y10",{"$f":"VALUE(LEFT(dms_CRYc_y9,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y10"]
[null,11,"dms_FRCP_y11",11,"CRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y10,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y10,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y10,4)+1))","v":"2029-30"},"dms_FRCP_y11",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yQ,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yQ,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yQ,4)-1))","v":"2008-09"},"dms_CRCP_yP",11,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y10,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y10,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y11",{"$f":"VALUE(LEFT(dms_CRYc_y10,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y11"]
[null,12,"dms_FRCP_y12",12,"CRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y11,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y11,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y11,4)+1))","v":"2030-31"},"dms_FRCP_y12",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yP,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yP,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yP,4)-1))","v":"2007-08"},"dms_CRCP_yO",12,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y11,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y11,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y12",{"$f":"VALUE(LEFT(dms_CRYc_y11,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y12"]
[null,13,"dms_FRCP_y13",13,"CRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y12,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y12,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y12,4)+1))","v":"2031-32"},"dms_FRCP_y13",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yO,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yO,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yO,4)-1))","v":"2006-07"},"dms_CRCP_yN",13,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y12,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y12,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y13",{"$f":"VALUE(LEFT(dms_CRYc_y12,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y13"]
[null,14,"dms_FRCP_y14",14,"CRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y13,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y13,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y13,4)+1))","v":"2032-33"},"dms_FRCP_y14",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yN,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yN,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yN,4)-1))","v":"2005-06"},"dms_CRCP_yM",14,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y13,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y13,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y14",{"$f":"VALUE(LEFT(dms_CRYc_y13,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y14"]
[null,15,"dms_FRCP_y15",15,"CRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_FRCP_y14,4)+1)&\"-\"&TEXT(VALUE(RIGHT(dms_FRCP_y14,2)+1),\"00\"),VALUE(LEFT(dms_FRCP_y14,4)+1))","v":"2033-34"},"dms_FRCP_y15",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(dms_CRCP_yM,4)-1)&\"-\"&TEXT(VALUE(MID(dms_CRCP_yM,3,2)),\"00\"),VALUE(LEFT(dms_CRCP_yM,4)-1))","v":"2004-05"},"dms_CRCP_yL",15,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y14,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y14,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y15",{"$f":"VALUE(LEFT(dms_CRYc_y14,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y15"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y15,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y15,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y16",{"$f":"VALUE(LEFT(dms_CRYc_y15,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y16"]
[null,"These are drop down lists for businesses to select the correct FRCP_y1 on the business and other details worksheet.\nThis also populates the column headings in the worksheets",null,null,null,null,null,null,null,null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y16,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y16,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y17",{"$f":"VALUE(LEFT(dms_CRYc_y16,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y17"]
[null,"dms_RCP_fyear_list","dms_CRY_ListF","dms_CRY_ListC","dms_RCP_cyear_list","dms_FRCP_fyear_list","dms_FRCP_ListF","dms_FRCP_ListC","dms_FRCP_cyear_list",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y17,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y17,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y18",{"$f":"VALUE(LEFT(dms_CRYc_y17,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y18"]
[null,"dms_fy1","2006-07",2007,"dms_cy1","dms_frcp_fy1","2015-16",2016,"dms_crcp_cy1",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y18,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y18,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y19",{"$f":"VALUE(LEFT(dms_CRYc_y18,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y19"]
[null,"dms_fy2","2007-08","2008","dms_cy2","dms_frcp_fy2","2016-17",2017,"dms_crcp_cy2",null,null,null,{"$f":"VALUE(LEFT(dms_CRYf_y19,4)+1)&\"-\"&TEXT(MID(dms_CRYf_y19,3,2)+2,\"00\")","v":{"$error":"#REF!"}},"dms_CRYf_y20",{"$f":"VALUE(LEFT(dms_CRYc_y19,4)+1)","v":{"$error":"#REF!"}},"dms_CRYc_y20"]
[null,"dms_fy3","2008-09","2009","dms_cy3","dms_frcp_fy3","2017-18",2018,"dms_crcp_cy3"]
[null,"dms_fy4","2009-10","2010","dms_cy4","dms_frcp_fy4","2018-19",2019,"dms_crcp_cy4"]
[null,"dms_fy5","2010-11","2011","dms_cy5","dms_frcp_fy5","2019-20",2020,"dms_crcp_cy5"]
[null,"dms_fy6","2011-12","2012","dms_cy6","dms_frcp_fy6","2020-21",2021,"dms_crcp_cy6"]
[null,"dms_fy7","2012-13","2013","dms_cy7","dms_frcp_fy7","2021-22",2022,"dms_crcp_cy7"]
[null,"dms_fy8","2013-14","2014","dms_cy8","dms_frcp_fy8","2022-23",2023,"dms_crcp_cy8",null,null,"2005-06","2006"]
[null,"dms_fy9","2014-15","2015","dms_cy9","dms_frcp_fy9","2023-24",2024,"dms_crcp_cy9",null,null,"2006-07","2007"]
[null,"dms_fy10","2015-16","2016","dms_cy10","dms_frcp_fy10","2024-25",2025,"dms_crcp_cy10",null,null,"2007-08","2008"]
[null,"dms_fy11","2016-17","2017","dms_cy11","dms_frcp_fy11","2025-26",2026,"dms_crcp_cy11",null,null,"2008-09","2009"]
[null,"dms_fy12","2017-18","2018","dms_cy12","dms_frcp_fy12","2026-27",2027,"dms_crcp_cy12",null,null,"2009-10",2010]
[null,"dms_fy13","2018-19",2019,"dms_cy13","dms_frcp_fy13","2027-28",2028,"dms_crcp_cy13",null,null,"2010-11",2011]
[null,"dms_fy14","2019-20","2020","dms_cy14","dms_frcp_fy14","2028-29",2029,"dms_crcp_cy14",null,null,"2011-12",2012]
[null,"dms_fy15","2019-20","2020","dms_cy15","dms_frcp_fy15","2029-30",2030,"dms_crcp_cy15",null,null,"2012-13",2013]
[null,"dms_fy16","2020-21","2021","dms_cy16",null,null,null,null,null,null,"2013-14",2014]
[null,"dms_fy17","2021-22","2022","dms_cy17",null,null,null,null,null,null,"2014-15",2015]
[null,"dms_fy18","2022-23","2023","dms_cy18",null,null,null,null,null,null,"2015-16",2016]
[null,"dms_fy19","2023-24","2024","dms_cy19",null,null,null,null,null,null,"2016-17",2017]
[null,"dms_fy20","2024-25","2025","dms_cy20",null,null,null,null,null,null,"2017-18",2018]
[null,null,null,null,null,null,null,null,null,null,null,"2018-19",2019]
[null,null,null,null,null,null,null,null,null,null,null,"2019-20",2020]
[null,null,null,null,null,null,null,null,null,null,null,"2020-21",2021]
[null,null,null,null,null,null,null,null,null,null,null,"2021-22",2022]
[null,null,null,null,null,null,null,null,null,null,null,"2022-23",2023]
[null,null,null,null,null,null,null,null,null,null,null,"2023-24",2024]
[null,null,null,null,null,null,null,null,null,null,null,"2024-25",2025]
[null,null,null,null,null,null,null,null,null,null,null,"2025-26",2026]
[null,null,null,null,null,null,null,null,null,null,null,"2026-27",2027]
[null,null,null,null,null,null,null,null,null,null,null,"2027-28",2028]
[null,null,null,null,null,null,null,null,null,null,null,"2028-29",2029]
[null,null,null,null,null,null,null,null,null,null,null,"2029-30",2030]
[null,null,null,null,null,null,null,null,null,null,null,"2030-31",2031]
[null,null,null,null,null,null,null,null,null,null,null,"2031-32",2032]
[null,null,null,null,null,null,null,null,null,null,null,"2032-33",2033]
[null,null,null,null,null,null,null,null,null,null,null,"2033-34",2034]
[null,null,null,null,null,null,null,null,null,null,null,"2034-35",2035]
[null,null,null,null,null,null,null,null,null,null,null,"2035-36",2036]

{"sheet":"Contents","index":1,"n_rows":34,"n_cols":19,"rows_kept":34,"cut":false,"hidden":false,"merged":[[29,18,29,23]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"CONCATENATE(FRCP_y1,\" to \",FRCP_y5)","v":"2019-20 to 2023-24"}]
[null,"CONTENTS"]
[]
[]
[null,null,null,null,"1. Business and other details",null,null,null,null,null,null,"2. Expenditure",null,null,null,null,null,null,"3. Economic benchmarking"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"4. Alternative control services",null,null,null,null,null,null,"5. Network information",null,null,null,null,null,null,"6. Service & quality"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"7. Other templates"]

{"sheet":"Instructions","index":2,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[24,2,24,4],[25,2,25,3],[26,2,26,4],[8,2,8,4],[10,2,10,4],[12,2,12,4],[20,2,20,4],[22,2,22,4],[7,2,7,3],[1,1,1,5],[2,1,2,5],[3,2,3,4],[4,2,4,4],[5,2,5,4]]}
[]
[null,{"$f":"CONCATENATE(dms_Segment,\" Network Service Provider\")","v":"Distribution Network Service Provider"}]
[null,{"$f":"IF(dms_Model=\"Reset\",\"Regulatory Proposal RIN Template\",\"Annual Reporting RIN\")","v":"Regulatory Proposal RIN Template"}]
[null,null,{"$f":"CONCATENATE(\"This template is to be used by \",dms_TradingName,\" to fulfil its reporting obligations to the AER.\")","v":"This template is to be used by Essential Energy to fulfil its reporting obligations to the AER."}]
[null,null,"INSTRUCTIONS"]
[null,null,"Complete the Business & other details worksheet before entering data or values in any other worksheets. The Business & other details worksheet is linked to other worksheets within the workbook and automatically generates certain column headings and conditional formatting."]
[]
[null,null,"Identifying CONFIDENTIAL INFORMATION:\n\nPlease use the macro at the top of each \nworksheet to identify confidential information. \n\nSee Returning completed responses below, for how to deal with confidential and public information."]
[null,null,"-Do this by selecting the cell or cells that contain confidential information and then run the Mark selected cells as CONFIDENTIAL macro. This will format the cells a specific colour that is identified by the AER's database which in turn marks that information as confidential.\n\n-To reverse this, select the cell or cells and run the Return cells to NON-CONFIDENTIAL macro."]
[]
[null,null,"UNITS OF MEASURE\n\nAll amounts are to be unrounded and reported on a one for one basis: that is 1000 is to be entered as '1000'. Applicable units of measure may be identified in the table column headings or row descriptors.\n\n"]
[]
[null,null,"COLOUR CODING OF INPUT / NON-INPUT CELLS:"]
[null,null,null,"Yellow = Input cell (mandatory)"]
[null,null,null,"Darker yellow = input cell (mandatory)"]
[null,null,null,"Orange = input cell (if data available)"]
[null,null,null,"Grey = Not applicable/No inputs required"]
[null,null,null," \nPLEASE DO NOT ENTER TEXT into cells that are to contain numeric data."]
[]
[]
[null,null,"WORKSHEET NAVIGATION\n\nMany tables in the worksheets have been \"grouped\" to allow for easy navigation. To ungroup or group data use the outline symbols in the left margin (for Row groupings) or above the columns (for column groupings). \n\n\n\n"]
[]
[null,null,"RETURNING COMPLETED RESPONSES\n\nPlease return two (2) files to the AER: \n1. A confidential version which must contain a complete set of all responses with confidential information marked using the Mark selection CONFIDENTIAL macro and which has been completed using the locked template file provided by the AER. \n\n2. A public version with confidential information either removed completely or aggregated in some form together with writtten consent to disclose the public version of the response.\n\nUse the drop down box on the Business and other details worksheet to identify the file as either confidential ('consolidated') or public. "]
[]
[null,null,"SUBMITTING AMENDED DATA TO THE AER\n\nIf an NSP wishes to correct data previously submitted to the AER it should resubmit that data using the original completed submission as the starting point. Please make any necessary changes to the data. Data that is not being amended should be left unchanged. \n\nNSPs must identify the reason for the amendments in the Amendment Reason box on the  Business and other details worksheet. NSPs may provide further details regarding any amendments in the Amendments worksheet. \n\n."]
[null,null,"NSP may use Amended Data macro \nto highlight cells that contain amended data.\nNB: if data is also CONFIDENTIAL, re-apply \nthe Confidentiality macro after applying the \nAmended macro"]
[null,null,"Please resubmit two (2) files - a confidential version and a public version of the amended submission to the AER"]

{"sheet":"Business & other details","index":3,"n_rows":95,"n_cols":12,"rows_kept":95,"cut":false,"hidden":false,"merged":[[84,4,84,8],[18,4,18,7],[19,2,19,3],[19,4,19,7],[22,2,22,3],[22,4,22,7],[23,4,23,7],[24,2,24,3],[24,4,24,7],[32,1,32,8],[51,2,51,3],[53,2,53,8],[7,1,7,8],[11,1,11,8],[13,2,13,4],[14,2,14,4],[17,2,17,3],[17,4,17,7]]}
[null,{"$f":"IF(dms_DataQuality=\"backcast\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List))&\" BACKCAST\",INDEX(dms_Worksheet_List,MATCH(dms_Model,dms_Model_List)))","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Essential Energy"}]
[null,{"$f":"IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(CRY,\" to \",FRY),CONCATENATE(FRCP_y1,\" to \",dms_MultiYear_FinalYear_Result))","v":"2019-20 to 2023-24"}]
[null,"BUSINESS & OTHER DETAILS"]
[]
[]
[null,"Instructions"]
[null,"Complete the following business details regulatory template before entering data or values in any other regulatory template. This regulatory template is linked to other cells within the spreadsheet and automatically generates column headings and conditional formatting to distinguish business specific input and non-input cells. "]
[]
[null,"SUBMISSION PARTICULARS INPUT SHEETS"]
[]
[null,"ENTITY DETAILS"]
[]
[null,"Short name","Essential Energy",null,null,"Select business name from drop down list first"]
[null,"ACN / ABN",{"$f":"INDEX(dms_ABN_List,MATCH(dms_TradingName,dms_TradingName_List))","v":37428185226}]
[]
[]
[null,"Business address","Address 1",null,{"$f":"INDEX(dms_Addr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"8 Buller Street"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_Addr2_List,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_Suburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"PORT MACQUARIE"}]
[null,null,null,"State",{"$f":"INDEX(dms_State_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},"p/code",{"$f":"INDEX(dms_PostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2444"}]
[]
[null,"Postal address","Address 1",null,{"$f":"INDEX(dms_PAddr1_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"PO Box 5730"}]
[null,null,null,"Address 2",{"$f":"IF(ISBLANK(INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_PAddr2_List,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,null,"Suburb",null,{"$f":"INDEX(dms_PSuburb_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"PORT MACQUARIE"}]
[null,null,null,"State",{"$f":"INDEX(dms_PState_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},"p/code",{"$f":"INDEX(dms_PPostCode_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2444"}]
[]
[]
[null,"Contact name/s","Natalie Lindsay"]
[null,"Contact phone/s","02 6589 8419"]
[null,"Contact email address/s","natalie.lindsay@essentialenergy.com.au"]
[]
[null,"REGULATORY CONTROL PERIODS"]
[]
[null,"Forthcoming regulatory control period","2019-20",{"$f":"dms_FRCP_y2","v":"2020-21"},{"$f":"dms_FRCP_y3","v":"2021-22"},{"$f":"dms_FRCP_y4","v":"2022-23"},{"$f":"dms_FRCP_y5","v":"2023-24"},{"$f":"dms_FRCP_y6","v":"2024-25"},{"$f":"dms_FRCP_y7","v":"2025-26"},{"$f":"dms_FRCP_y8","v":"2026-27"},{"$f":"dms_FRCP_y9","v":"2027-28"},{"$f":"dms_FRCP_y10","v":"2028-29"}]
[]
[]
[null,"Current regulatory control period",{"$f":"dms_CRCP_FirstYear_Result","v":"2014-15"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)+1)&\"-\"&TEXT(MID(CRCP_y1,3,2)+2,\"00\"),VALUE(LEFT(CRCP_y1,4)+1))","v":"2015-16"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y2,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y2,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y2,4)+1))","v":"2016-17"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y3,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y3,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y3,4)+1))","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y4,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y4,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y4,4)+1))","v":"2018-19"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y5,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y5,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y5,4)+1))","v":"2019-20"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y6,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y6,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y6,4)+1))","v":"2020-21"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y7,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y7,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y7,4)+1))","v":"2021-22"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y8,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y8,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y8,4)+1))","v":"2022-23"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y9,4)+1)&\"-\"&TEXT(VALUE(MID(CRCP_y9,3,2)+2),\"00\"),VALUE(LEFT(CRCP_y9,4)+1))","v":"2023-24"}]
[]
[]
[null,"Previous regulatory control period",{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y2,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y2,3,2)),\"00\"),VALUE(LEFT(PRCP_y2,4)-1))","v":"2009-10"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y3,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y3,3,2)),\"00\"),VALUE(LEFT(PRCP_y3,4)-1))","v":"2010-11"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y4,4)-1)&\"-\"&TEXT(VALUE(MID(PRCP_y4,3,2)),\"00\"),VALUE(LEFT(PRCP_y4,4)-1))","v":"2011-12"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(PRCP_y5,4)-1)&\"-\"&TEXT(VALUE(RIGHT(PRCP_y5,2)-1),\"00\"),VALUE(LEFT(PRCP_y5,4)-1))","v":"2012-13"},{"$f":"IF(dms_RPT=\"financial\",VALUE(LEFT(CRCP_y1,4)-1)&\"-\"&TEXT(VALUE(RIGHT(CRCP_y1,2)-1),\"00\"),VALUE(LEFT(CRCP_y1,4)-1))","v":"2013-14"}]
[]
[]
[null,"Commencing regulatory year","2019-20","CRY"]
[]
[null,"Last completed regulatory year","2023-24","dms_FinalYear"]
[]
[]
[]
[]
[]
[null,"Source","Reporting",null,"Please select the correct submission type from the dropdown list."]
[null,"Data quality (actual, estimate, public, consolidated)","Consolidated"]
[null,"Amended RIN submission - amendment reason"]
[null,"Submission Date","dd/mm/yyyy","dms_SubmissionDate","Please enter date this file submitted to AER (dd/mm/yyyy)"]
[null,"EBSS - First application of scheme in forthcoming period?","No"]
[null,"Sector",{"$f":"INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Electricity"},"dms_Sector","=INDEX(dms_Sector_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Segment",{"$f":"INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Distribution"},"dms_Segment","=INDEX(dms_Segment_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Regulatory Year Ending",{"$f":"IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))","v":"2024"},"dms_RYE","=IF(dms_MultiYear_Flag=1,LEFT(dms_Specified_FinalYear,2)&RIGHT(dms_Specified_FinalYear,2),INDEX(dms_RYE_Formula_Result,MATCH(dms_Model,dms_Model_List)))"]
[null,"Reporting Period Type",{"$f":"INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Financial"},"dms_RPT","=INDEX(dms_RPT_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Model or RIN Type","Reset","dms_Model","Drop down selection"]
[null,"Security Classification","Public","dms_Classification","Always Public"]
[null,"Template - version no.",5,"dms_TemplateNumber"]
[null,"Dollar $ real month",{"$f":"INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"June"},"dms_RPTMonth","=INDEX(dms_RPTMonth_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Dollar $ real  (the last month before the FRCP_y1)",{"$f":"CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2)))","v":"June 2019"},"dms_DollarReal","=IF(SUM(dms_SingleYear_Model)>0,CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(CRY,2))&RIGHT(CRY,2)),CONCATENATE(dms_RPTMonth)&\" \"&VALUE((LEFT(dms_CRCP_FinalYear_Result,2)&RIGHT(dms_CRCP_FinalYear_Result,2))))"]
[null,"Form of control",{"$f":"INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Revenue cap"},"dms_FormControl","=INDEX(dms_FormControl_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"RIN response - version no.",1,"dms_RINversion"]
[null,"Jurisdiction",{"$f":"INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))","v":"NSW"},"dms_Jurisdiction","=INDEX(dms_JurisdictionList,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Backcast Multiyear EB, CA or ARR?",0,"dms_MultiYear_Flag","1=y, 0-n"]
[null,null,2013,"dms_Specified_FinalYear","The result here is returned to dms_CRCP_FinalYear_Result if dms_MultiYear_Flag is set to 1"]
[null,"Single Year Model T/F",{"$f":"IF(dms_Model=\"EB\",1,0)","v":0},"dms_EB"]
[null,null,{"$f":"IF(dms_Model=\"CA\",1,0)","v":0},"dms_CA","=dms_SingleYear_Model"]
[null,null,{"$f":"IF(dms_Model=\"ARR\",1,0)","v":0},"dms_ARR"]
[null,"Single Year Final Year Reference","CRY","dms_SingleYear_FinalYear_Ref","This is the reference for EB, CA & ARR RINs"]
[null,"Single Year Final Year Result",{"$f":"INDIRECT(dms_SingleYear_FinalYear_Ref)","v":{"$error":"#REF!"}},"dms_SingleYear_FinalYear_Result","=INDIRECT(dms_SingleYear_FinalYear_Ref)",null,null,null,"Formula errors OK"]
[null,"FRCP length in years",{"$f":"INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_FRCPlength_Num","=INDEX(dms_FRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"Multi Year Final Year Reference",{"$f":"INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))","v":"dms_FRCP_y5"},"dms_MultiYear_FinalYear_Ref","=INDEX(dms_FinalYear_List,MATCH(dms_FRCPlength_Num,dms_FRCPlength_Num_List))"]
[null,"Multi Year Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)","v":"2023-24"},"dms_MultiYear_FinalYear_Result","=IF(dms_MultiYear_Flag=0,INDIRECT(dms_MultiYear_FinalYear_Ref),dms_Specified_FinalYear)",null,null,null,"Formula errors OK"]
[null,"CRCP length in years",{"$f":"INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_CRCPlength_Num","=INDEX(dms_CRCPlength_List,MATCH(dms_TradingName,dms_TradingName_List))"]
[null,"CRCP Final Year Reference",{"$f":"INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))","v":"CRCP_y5"},"dms_CRCP_FinalYear_Ref","=INDEX(dms_CFinalYear_List,MATCH(dms_CRCPlength_Num,dms_CRCPlength_Num_List))"]
[null,"CRCP First Year Result",{"$f":"INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))","v":"2014-15"},"dms_CRCP_FirstYear_Result","=INDEX(dms_CRCP_years,MATCH(dms_CRCPlength_Num,dms_CRCP_index))"]
[null,"CRCP Final Year Result",{"$f":"IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)","v":"2018-19"},"dms_CRCP_FinalYear_Result","=IF(dms_MultiYear_Flag=0,(IF(SUM(dms_SingleYear_Model)>0,CRY,dms_CRCP_yZ)),dms_Specified_FinalYear)"]
[null,"Table 6.6.3 - Public lighting repair - no. business days",{"$f":"INDEX(dms_663_List,MATCH(dms_TradingName,dms_TradingName_List))","v":5},"dms_663"]
[null,"Distribution Determination Reference",{"$f":"INDEX(dms_DeterminationRef_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"2014-19 Distribution Determination"},"dms_DeterminationRef"]
[null,"Backcast templates only - unit of measure ","$0s","dms_Backcast_UOM","If the cover sheet is for Backcast data ensure to apply dms_Backcast_UOM named range to this field. Otherwise, do not apply this named range."]
[null,"EB/CA Unit of Measure for Monetary Values","$0s","dms_dollar_nom_UOM","If the cover sheet is attached to an EB files make sure this field is set"]
[]
[null,"discard this record?","NO","dms_DISCARD","If record is to be discarded from DB set this flag to YES"]
[null,"CBD Feeder for this business",{"$f":"INDEX(dms_CBD_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":0},"dms_CBD_flag_NSP"]
[null,"Urban Feeder for this business",{"$f":"INDEX(dms_Urban_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":0},"dms_Urban_flag_NSP"]
[null,"Short rural Feeder for this business",{"$f":"INDEX(dms_ShortRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_ShortRural_flag_NSP"]
[null,"Long rural Feeder for this business",{"$f":"INDEX(dms_LongRural_flag,MATCH(dms_TradingName,dms_TradingName_List))","v":"YES"},"dms_LongRural_flag_NSP"]
[]
[]
[null,"USES NAMED RANGES FLAG","yes","dms_Defined_Names_Used"]

{"sheet":"CPI series","index":4,"n_rows":13,"n_cols":12,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,2,9,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"CPI SERIES"]
[]
[]
[]
[null,"NOMINATED CPI SERIES"]
[]
[null,"Name of CPI series","ABS CPI index - December (rebased index in Dec 2012)"]
[]
[null,null,{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Series data",103.5,106.07500000000002,107.67500000000001,109.05000000000001,111.64539000000002,114.43652475000002,117.29743786875001,120.22987381546875,123.23562066085546,126.31651117737684]

{"sheet":"2.1 Expenditure summary","index":5,"n_rows":112,"n_cols":9,"rows_kept":112,"cut":false,"hidden":false,"merged":[[92,1,93,1],[92,2,92,8],[104,1,105,1],[104,2,104,8],[8,1,9,1],[20,1,21,1],[33,1,34,1],[8,2,8,8],[33,2,33,8],[20,2,20,3],[65,1,66,1],[43,1,44,1],[53,1,54,1],[43,2,43,8],[53,2,53,8],[65,2,65,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.1 EXPENDITURE SUMMARY & RECONCILIATION"]
[]
[]
[]
[null,"2.1.1 - STANDARD CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Replacement expenditure",172519859.76500002,178797800,170518829.19825009,166849456.22287801,165252967.66593897,160709962.00361678,156366185.15002066]
[null,"Connections",92749591.464999989,91926353.881406516,93438184.952150837,93376046.860848397,93350654.374988645,93348433.622383356,93365891.138585851]
[null,"Augmentation Expenditure",38070347.349999994,37615490,40626175.616801105,34686461.193383887,29650633.178281404,31165475.330118332,29999688.339262106]
[null,"Non-network",84672789.62279658,121110811.87172729,146093656.95122135,83472408.444659889,94783023.046602145,88505700.225471169,82361853.788045436]
[null,"Capitalised network overheads",105207128.97698709,97991647.53931208,102024708.2513717,90946543.459809482,88302711.406922802,86873461.349524021,87872330.617175281]
[null,"Capitalised corporate overheads",41952490.119718522,39014739.232196122,35520603.545180276,31548030.984081417,27270832.622878075,24649218.992442064,23800233.646575555]
[null,"capcons (included in the above)",90025077.941295296,87725558.929037482,89704585.249134511,89490377.460426524,89371265.388607219,89308328.182299614,89293564.878038704]
[]
[]
[null,"2.1.2 - STANDARD CONTROL SERVICES OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"}]
[null,"Vegetation management",104771317.51824997,118430560.80684499]
[null,"Maintenance",66076025.679707691,73747714.928074837]
[null,"Emergency response",36016740.744792268,38375200.713585615,null," "]
[null,"Non-network",0,0]
[null,"Metering",0,0]
[null,"Network overheads",93195586.512963861,89740884.225624487]
[null,"Corporate overheads",50030698.290311106,48830409.326415375]
[null,"Total Opex",{"$f":"SUM(C23:C29)","v":350090368.74602485},{"$f":"SUM(D23:D29)","v":369124770.00054532}]
[]
[]
[null,"2.1.3 - ALTERNATIVE CONTROL SERVICES CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Connections"]
[null,"Metering",0,0,0,0,0,0,0]
[null,"Public lighting",2925276,2714907,3097936,2543511,1491741,2412271,2228603]
[null,"Fee and quoted",0,0,0,0,0,0,0]
[null,"Total Capex",{"$f":"SUM(C36:C39)","v":2925276},2714907,3097936,2543511,1491741,2412271,2228603]
[]
[]
[null,"2.1.4 - ALTERNATIVE CONTROL SERVICES OPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Connections"]
[null,"Metering",18835554.171873815,18137529.922432382,19156594.380598921,17916526.525816083,17142540.918116547,17042678.087290764,16947598.116979472]
[null,"Public lighting",13665650.260431457,15089049.950680476,10518810.949806917,11196243.844404235,12325876.196083881,10514784.749833614,13099192.283939559]
[null,"Fee and quoted",26122770.324671473,24933215.219813682,19416582.393791981,19022936.033615522,18805677.497690018,18904453.080686875,19863086.648742501]
[null,"Total Opex",{"$f":"SUM(C46:C49)","v":58623974.756976746},58159795.092926539,49091987.72419782,48135706.403835841,48274094.61189045,46461915.917811252,49909877.049661532]
[]
[]
[null,"2.1.5 - DUAL FUNCTION ASSETS CAPEX"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Replacement expenditure"]
[null,"Connections"]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads"]
[null,"Capitalised corporate overheads"]
[null,"capcons (included in the above)"]
[]
[]
[null,"2.1.6 -  DUAL FUNCTION ASSETS OPEX BY CATEGORY"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's,  real \", dms_DollarReal, \")\")","v":"Forecast \n($0's,  real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total Opex",{"$f":"SUM(C68:C88)","v":0},{"$f":"SUM(D68:D88)","v":0}]
[]
[]
[null,"2.1.7 - STANDARD CONTROL SERVICES CAPCONS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Replacement expenditure"]
[null,"Connections",88030483.974999994,87241353.881406516,88481070.247566909,88389743.068503663,88332971.987676442,88298991.380449295,88282764.328954756]
[null,"Augmentation Expenditure"]
[null,"Non-network"]
[null,"Capitalised network overheads",1425972.0564433567,346319.98903336428,907546.46193065983,817170.01763391471,793296.79908805259,786248.87220541097,795373.51562328648]
[null,"Capitalised corporate overheads",568621.90985194803,137885.05859760326,315968.53963693255,283464.37428894354,244996.60184272841,223087.92964490259,215427.03346066037]
[null,"Total Capcons",{"$f":"SUM(C95:C100)","v":90025077.941295311},{"$f":"SUM(D95:D100)","v":87725558.929037496},89704585.249134511,89490377.460426524,89371265.388607219,89308328.182299599,89293564.878038704]
[]
[]
[null,"2.1.8 - STANDARD CONTROL SERVICES CAPITALISED OVERHEADS"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal, \")\")","v":"Forecast \n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Replacement expenditure",112527427.92851993,105397435.11676818,101222356.08848533,93227773.878688097,89690694.24183473,86325780.248685002,84847035.306478322]
[null,"Connections",5072668.7380419374,3245911.1957047135,4166127.4518060982,3886750.7687254101,3761629.7691636235,3721658.0289925188,3768994.3329272419]
[null,"Augmentation Expenditure",24831681.833478712,22173517.608496532,24116264.661987126,19381193.286414064,16092817.64818906,16740617.327960435,16278357.198921435]
[null,"Non-network",4727840.5966650397,6189522.8505387902,8040563.5942734778,5998856.5100633204,6028402.3706134707,4734624.736328125,6778177.4254238307]
[null,"capcons (included in the above)",1994593.9662953019,484205.04763096571,1223515.0015676022,1100634.3919228613,1038293.4009307772,1009336.8018503189,1010800.5490839481]
[null,"Total Capitalised Overheads",{"$f":"SUM(C107:C110)","v":147159619.09670562},{"$f":"SUM(D107:D110)","v":137006386.77150822},137545311.79655203,122494574.4438909,115573544.02980088,111522680.34196608,111672564.26375082]

{"sheet":"2.2 Repex","index":6,"n_rows":527,"n_cols":11,"rows_kept":527,"cut":false,"hidden":false,"merged":[[9,4,9,10],[183,4,183,10],[357,4,357,10],[11,1,35,1],[36,1,42,1],[43,1,48,1],[185,1,209,1],[210,1,216,1],[217,1,222,1],[111,1,124,1],[82,1,110,1],[66,1,81,1],[49,1,57,1],[58,1,65,1],[359,1,383,1],[384,1,390,1],[391,1,396,1],[130,1,137,1],[125,1,129,1],[304,1,311,1],[299,1,303,1],[285,1,298,1],[256,1,284,1],[240,1,255,1],[232,1,239,1],[223,1,231,1],[406,1,413,1],[397,1,405,1],[478,1,485,1],[473,1,477,1],[459,1,472,1],[430,1,458,1],[414,1,429,1]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.2 REPEX"]
[]
[null,"There is ONE table on this worksheet. The table has been sub-grouped for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.2.1 - REPLACEMENT EXPENDITURE, VOLUMES AND ASSET FAILURES BY ASSET CATEGORY"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($0's, real June 2019)"}]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - replacement of staked pole",null,392814.27869893587,410071.37659498217,433025.12877596216,411779.2019217147,400988.2050843754,395113.53836404142,395549.98689812253]
[null,null,"˂ = 1 kV; Wood - replacement of unstaked pole",null,6651909.8827285301,6944141.2660227828,7332839.6898277523,6973061.5491817687,6790327.0041327979,6690845.5042643165,6698236.3158375937]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of staked pole",null,606681.3603991369,780202.5678997949,755491.55778067023,718235.16826038656,714882.3681371545,687132.29735547758,685183.81559084624]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of unstaked pole",null,12210429.853214817,15702820.868554361,15205472.383242166,14455628.131356495,14388147.68216379,13829633.254625604,13790416.951867189]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of staked pole",null,562474.43873677321,711763.31883630611,703084.39421549556,668412.41702825378,650320.79832238238,639467.09934293129,637653.78044212179]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of unstaked pole",null,8867689.5587225147,11221303.078058882,11084475.510545334,10537854.528489552,10252631.152546022,10081517.184541091,10052929.309295675]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of staked pole",null,77172.458523381123,114348.63547172677,187649.60674547244,179198.13475863918,219214.66638998169,171051.12040599683,171020.72045702505]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of unstaked pole",null,1279898.7657530175,1896462.5490253544,3112153.0227626949,2971986.0671969759,3635656.895166704,2836868.5160130924,2836364.3354036831]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of staked pole",null,36910.525658966973,37140.323027759143,97857.220868390694,93449.870513533038,90800.310038450058,89201.291490365387,89185.438248930383]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of unstaked pole",null,168694.77282653796,169745.03191205472,447243.7427836819,427100.51930999913,414991.04662017548,407682.93962633662,407610.48444140778]
[null,null,"> 132 kV; Wood - replacement of staked pole",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood - replacement of unstaked pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,95016.63074870249,99190.89677592997,104743.10888619538,99603.997361252099,96993.796516975461,95572.791556599579,95678.362742405137]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,132619.08183267707,167818.11105628585,165771.81181984086,157596.92339251557,153331.31824425678,150772.25512242722,150344.71447145063]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,196165.72521083482,248230.95593742281,245204.13831684797,233112.11585142926,226802.57490296313,223017.2940352569,222384.89015568738]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,842164.42474017444,39359.801966687824,103705.09786658356,99034.367430680955,96226.47113101538,94531.896386831446,94515.095767112944]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,12110.981395121926,12186.381883421764,32108.645438039141,30662.517614159238,29793.151029801622,29268.485408259497,29263.283685752329]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,125939.20288585415,131471.9578568539,138831.10290241276,132019.49946106784,128559.82496924554,126676.36277324439,126816.2914455547]
[null,null,"> 1 kV & < = 11 kV; Steel",null,9148.065304660191,11576.094616493918,11434.940879119284,10871.037011304568,10576.795534731842,10400.27134052289,10370.779583066256]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,48789.68162485434,61739.171287967562,60986.351355302846,57978.864060291024,56409.576185236481,55468.113816122073,55310.824443020036]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,2264.5524262114677,2278.6510655492921,6003.7835545154248,5733.3816634268824,5570.8245473976904,5472.7207878880336,5471.7481521502868]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,9923534.8624833897,9898207.2816682048,9062485.8553510066,8595029.507876955,8314006.3876963342,8098239.9055778477,7959747.4912376432]
[null,null,"> 1 kV & < = 11 kV",null,31312443.061951719,31232525.125131574,28595513.219611689,27120514.595929105,26233782.139028601,25552958.644211754,25115963.57152506]
[null,null,"˃ 11 kV & < = 22 kV",null,8037243.1117634075,8016729.8644916043,7339864.5770611474,6961263.5683631552,6733658.0660681063,6558905.0474928031,6446737.6375313159]
[null,null,"> 22 kV & < = 66 kV",null,5273415.6335345618,5259956.4314980628,4815849.9214799162,4567441.3004668448,4418104.2208997877,4303444.8423855836,4229849.2866659546]
[null,null,"> 66 kV & < = 132 kV",null,128486.53954179594,128158.6066772467,117337.97112988906,111285.50602485312,107646.91466163297,104853.24395651757,103060.09148434413]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",860499.5103441797,1123581.9327848963,849527.23583560227,807274.64192899654,784250.03754433244,768451.52277176373,761113.75374625891]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",786742.40945753572,1027274.9099747625,776710.61562112218,738079.67262079683,717028.6057548183,702584.24939132691,695875.43199657963]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",688399.6082753439,898865.54622791731,679621.78866848187,645819.71354319726,627400.03003546607,614761.21821741108,608891.00299700722]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",122928.50147773996,160511.70468355666,121361.03369080034,115324.94884699951,112035.71964919037,109778.78896739484,108730.53624946557]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",1174083.5531756843,1137945.7539277282,882975.71708478767,1117640.5048438036,1016287.656146817,1291377.8916831459,1250177.3005055278]
[null,null,"> 1 kV & < = 11 kV","per km",10793529.387092879,8701185.0332322475,10389132.92366096,11729027.498388978,11112757.648047417,12677853.928557016,12415908.18983156]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",337388.65787240845,269746.29362924647,325110.69187737431,367040.47133379721,345096.40396296425,396732.42151386762,388535.26387067203]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",1731351.1410471527,1384236.0801733087,1668345.2576564923,1883513.0465309683,1770904.3823236639,2035880.9184931046,1993816.2020074157]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",2762566.8873131122,2208705.483624788,2662033.8625358986,3005358.4456712948,2825678.5646879901,3248478.6468792236,3181359.6262874249]
[null,null,"> 22 kV & < = 66 kV","per km",825201.30801465851,493435.23836472165,790218.71154546866,787294.77217798028,968456.76860740327,778659.77836264542,775173.00968121039]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",3137835.4697255688,2399309.83508828,2030632.5727729523,1951231.9865793721,1879005.2818100164,1814621.3981426512,1770565.4500117188]
[null,null,"> 1 kV & < = 11 kV","per km",803661.55277768127,698475.22407169943,489210.27892184863,470081.46978171135,452680.95781337831,437169.90076184471,426556.15263119782]
[null,null,"> 11 kV & < = 22 kV","per km",152468.68856836579,132512.9975965984,92811.768092646947,89182.697579828586,85881.515345764681,82938.795840541992,80925.181710711462]
[null,null,"> 22 kV & < = 33 kV","per km",943960.82029164396,400066.93765539047,249673.15290145332,239910.58188640076,231030.06389154645,223113.84731607797,217697.01926880004]
[null,null,"> 33 kV & < = 66 kV","per km",1763745.2843661858,1674007.3611757709,274640.46819159866,263901.64007504086,254133.07028070113,245425.2320476858,239466.72119568003]
[null,null,"> 66 kV & < = 132 kV","per km",835928.62496890663,484080.99456302245,302104.51501075854,290291.80408254493,279546.37730877131,269967.75525245437,263413.39331524802]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",5711335.2600399572,7134816.3018548107,5550348.6091674119,5550965.6652134694,5162427.3283173516,4977633.2449154845,4847111.1184770558]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",397201.24536235887,496198.83819266496,386021.91798460518,386057.89330537716,359041.48453072913,346189.49780180497,337112.11962860782]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,977483.6835443906,1297035.5135644337,1484814.0446960444,1685883.90390511,1640479.2562220825,1588380.3712794299,1523255.9144073331]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,23212.013593402415,30800.315625540647,35259.436417584169,40034.182414633222,38955.971783637848,37718.795096345304,36172.304036058034]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,3992.2163090285476,5297.3225208889125,6064.2432655409093,6885.4481456856456,6700.007531138911,6487.2264672176379,6221.2466629321334]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,594449.8354598966,788783.03607919568,902979.2306686861,1025258.4530587402,997645.93553167442,965962.36464125779,926357.38368479058]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,1228302.385984211,1629850.0351848591,1865811.8437638292,2118475.4861076749,2061420.173550836,1995952.9071816055,1914117.7552414048]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,4790.6595708342575,6356.7870250666956,7277.091918649091,8262.5377748227747,8040.0090373666917,7784.6717606611646,7465.4959955185595]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,11994.281527273797,13693.031892955905,12117.465538466762,11643.655613502877,11212.654644772954,10828.454419664486,10565.557802916115]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,543065.45197003509,619979.82429201785,548642.85821665963,527190.15173621697,507675.70767797087,490280.26232169184,478377.08415539621]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,259726.95529001683,296512.08987879119,262394.4104514459,252134.42039558207,242801.4254112035,234481.86458863522,228789.04024823295]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,330561.57946002134,377379.02348209784,333956.52239274932,320898.35323074082,309019.99597789533,298431.46402189939,291186.05122502381]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,291704.41791401454,335538.15476979897,292154.82658046263,274869.23534939939,270263.11905596819,250090.84506643444,247756.493370221]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,889143.06479709223,1065866.720071414,924485.89110139769,854636.45977442106,855014.67022429116,762985.1362384737,765947.97083174367]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,412799.11785017292,518887.73144167196,441613.75831003959,392748.81083319226,408226.0453206618,335421.25855674862,347423.47585707018]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,2470096.4691982167,3104906.7159333071,2642516.7544735512,2350119.9711211068,2442732.2384620639,2007084.8764646894,2078903.4276536352]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,946936.80167786498,1190297.817011321,1013035.8854662837,900942.58129726304,936446.44332271977,769436.56141187344,796968.93920037069]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,745121.5332272338,936616.39598016359,797133.29427620035,708929.80010538187,736866.92543520511,605450.91218805825,627115.47049311758]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,3329366.3135654787,2712327.2208966715,2786226.2485874048,2672930.471185986,2577291.3565253327,2494312.9276256664,2439205.4337949688]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,2060200.6787707475,1709734.0214097369,1917234.6036653977,2014761.1293460082,1957330.9656078494,1901780.9373250296,1846063.242692864]
[null,null,"˂ = 11 kV  ; Switch",null,835620.30855826405,862616.6969711961,1370630.5587048205,1375225.1712524132,1376600.1096698248,1175904.1000976763,1216416.4104674049]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,3615959.4285447798,4140472.2955148923,3893471.9149397723,3749064.1116357138,3617798.2786690006,3497195.5907755657,3415942.1091342503]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,6544187.3730271049,5875389.0130440602,7561812.0661825826,7732193.7194620557,7513734.0404742993,7274386.2636230318,7103345.724833101]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,2786930.4333020407,2872678.714078852,2759699.9933094047,2843175.9929728303,3052352.8696989799,2998747.2174331909,2570156.2659371765]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,110303.62892189992,87555.755671586754,190730.02049668552,179108.72557428712,190605.93270018787,124661.11953511136,150569.93802505417]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,2146733.5099468078,2012309.6450698595,758018.76991460915,1018348.3482351962,1457035.5815029412,1484355.3549059967,909260.01375769626]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,364114.7951876538,352962.13148469903,1317915.9176073682,1225030.2893559863,1382640.9966698748,646384.04978201189,954397.28922629356]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,5281803.7687624767,4899813.5583630539,1334424.2467293891,2034624.640236449,3195372.565372346,3286309.6367700719,1807839.4394487729]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,268834.75425547932,260191.73533980834,984094.52927992528,914576.28400744288,1033138.0473715519,480328.9144291422,711762.710069992]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,1767844.8583539519,1639990.9169807404,446638.14611880615,680998.55019131419,1069506.4049193782,1099943.4755002689,605092.46418062598]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires",null,589512,535032.96,476285.04,404730.48,343949.76,343949.76,343949.76]
[null,null,"Brackets",null,0,0,0,0,0,0,0]
[null,null,"Lamps",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns",null,2335764,2179874.04,2621650.96,2138780.52,1147791.24,2068321.24,1884653.24]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,901888.39439386385,1203837.7851266749,1652836.272207621,1588208.0520879731,1529419.0229620377,1477013.6692324362,1441154.2675594562]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,3001392.4405806102,3471065.6137819123,2448646.3291964754,1911731.9145503384,1793763.051622143,1276431.5660033398,1645762.5894969101]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,722743.32013515558,825632.08096604445,479526.57280097652,460776.4101736712,443720.33382231963,428516.3114439784,418112.65787218791]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"OTHER BY: \nenter DNSP defined asset group here","OTHER - Zone Sustation Property",null,1708609.7013205898,1474701.2867801767,1628451.8358460392,1252037.3477293523,1153767.2765196953,1114233.5834376297,1193934.0385750285]
[null,null,"OTHER - Zone Sustation Batteries",null,290331.99851547863,170543.68622627892,632566.96837575617,656851.47833268018,821354.66047961288,902619.46453093307,880705.3857307788]
[null,null,"OTHER - Zone Sustation Current transformers",null,962627.5955611181,1040335.2777414022,921292.97866713558,885269.12898451788,852500.05157067301,823289.24270382547,803301.16794044012]
[null,null,"OTHER - Zone Sustation Voltage transformers",null,344463.49589384178,719126.74715045106,449599.2785816954,431294.02371884522,418018.8625392018,402107.2067470508,392503.00848912442]
[null,null,"OTHER - Zone Sustation Surge Diverters",null,79938.815233675166,90287.833884500593,496193.69214837387,476791.821740899,125432.1856850366,121134.2673505498,118193.33156926968]
[null,null,"OTHER - Zone Sustation Protection Relays",null,2795934.5703575057,2437771.5148815168,2259896.5079875807,2171531.3798610251,2091150.0838647613,2019497.0847838551,1970467.1003976515]
[null,null,"OTHER - Frequency Injection Relays",null,1507514.0890001711,1855916.5854036238,2693510.9621161232,2588190.8996989192,2492386.5559381354,2406985.2387491544,2348547.6952820765]
[null,null,"OTHER - Zone Substation Earthing System Refurbishment ",null,166190.86372312639,80255.852341778329,316283.48418787809,303916.35564646398,292666.60315940226,282638.41818645381,275776.43391569844]
[null,null,"OTHER - Generation",null,370098.80083657254,259828.32195650734,918242.37344867829,98037.534079504519,141612.87249648495,319107.89150083496,44480.069986402967]
[null,null,"OTHER - Zone Substation Capacitor Bank Refurbishment",null,0,1402270.3800417217,51013.465191593241,49018.76703975226,47204.290832161656,45586.841642976418,44480.069986402967]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"ASSET REPLACEMENTS"]
[null,null,null,null,"ASSET REPLACEMENTS (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - replacement of staked pole",null,85.427202315158681,89.18018603617034,97.28517401334517,95.674780970603422,94.890995897565489,94.633516878112559,95.052099312836447]
[null,null,"˂ = 1 kV; Wood - replacement of unstaked pole",null,1446.6226971590811,1510.1756555347372,1647.4253751817312,1620.1550085556205,1606.8824063209345,1602.5222612677378,1609.6105286380043]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of staked pole",null,119.9435461351827,154.24944428177326,154.30162190285449,151.70749957083044,153.79255322909219,149.61348746057664,149.68378263716062]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of unstaked pole",null,2414.0551400259687,3104.5160478654443,3105.5662056973924,3053.3553569167429,3095.3203868257619,3011.2100238753351,3012.6248264038536]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of staked pole",null,111.20364526792068,140.71870679199245,143.59798100289586,141.18380852201486,139.90343089954672,139.23505446797537,139.30047338779758]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of unstaked pole",null,1753.1808312016587,2218.5004704191633,2263.8936618219041,2225.8330307472847,2205.647240083656,2195.1099528838099,2196.1413147240978]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of staked pole",null,10.783734154200211,15.978566828333619,27.088137057650815,26.752506175871783,33.331966172982241,26.323698719558863,26.406265728698386]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of unstaked pole",null,178.84732841558829,265.00319354074014,449.25448599168021,443.68807590760315,552.80786929959004,436.57634013318403,437.94570706941528]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of staked pole",null,3.5234964541394125,3.5454330210035874,9.6503069869518168,9.5307365256618581,9.4318183637832114,9.3779713656618728,9.4073863447538262]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of unstaked pole",null,16.103683794103834,16.203942029327504,44.105477118142751,43.558995824691607,43.106903188549936,42.860802463802777,42.995239812689711]
[null,null,"> 132 kV; Wood - replacement of staked pole",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood - replacement of unstaked pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,15.895170545223561,16.593476408955944,18.101546001225852,17.801905238500325,17.656068817909418,17.608160507498848,17.686044823113274]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,20.60093344165281,26.068720190178507,26.602117600274024,26.154882201870713,25.917686972190076,25.793867484550113,25.80598660897121]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,30.472214049111447,38.559981947972375,39.348965617071997,38.687429923600426,38.33657864636448,38.1534289875637,38.171355192436579]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,73.259812177090296,3.4239058486668297,9.3195224217496975,9.2040504894601405,9.1085229555907237,9.0565216765625784,9.0849283953906337]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0.98553690499963409,0.99167265580711317,2.6992318011399168,2.665787435895659,2.6381196064044143,2.6230583726093064,2.6312858670405435]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,19.563286824890533,20.422740195638085,22.278825847662585,21.910037216615788,21.730546237426971,21.671582163075502,21.767439782293255]
[null,null,"> 1 kV & < = 11 kV; Steel",null,1.2880674726751751,1.6299392756324327,1.6632897961755493,1.6353265307757647,1.6204959668651213,1.6127541888061778,1.6135119335951864]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,6.8696931876009319,8.693009470039641,8.8708789129362629,8.7217414974707435,8.6426451566139786,8.6013556736329484,8.6053969791743281]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0.17077301728054012,0.17183621509013924,0.46772064717396,0.46192543531043639,0.45713117676988463,0.45452137867291831,0.45594703208229692]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,7684.9083823443307,7665.2943898700387,7250.1047107710556,7111.2151402132749,7005.951669404013,6906.8032449141201,6811.1901705480768]
[null,null,"> 1 kV & < = 11 kV",null,17320.531407196369,17276.324663827512,16340.554773154596,16027.520310114691,15790.273597275396,15566.809202527811,15351.312910951925]
[null,null,"˃ 11 kV & < = 22 kV",null,3890.0879208147949,3880.1593502441306,3669.9910209481577,3599.6853499013482,3546.4011549669067,3496.2123863718166,3447.8132061658657]
[null,null,"> 22 kV & < = 66 kV",null,1361.2661404538305,1357.7918161670621,1284.2471980787298,1259.6449959110569,1240.999152459168,1223.4364976528318,1206.5000770419874]
[null,null,"> 66 kV & < = 132 kV",null,22.308433408715874,22.2514961723531,21.046246760473935,20.643065800884123,20.337497664988874,20.049680827719417,19.772126718239353]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",922.2931514942976,1204.2678807983884,940.6332055968951,924.40826156891717,914.65516894654877,907.08708440368537,901.40372202336539]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",843.23945279478642,1101.0449195870981,860.00750226001855,845.17326772015281,836.2561544654161,829.3367628833696,824.14054584993414]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",737.83452119543824,963.41430463871097,752.50656447751612,739.52660925513374,731.72413515723906,725.66966752294843,721.1229776186924]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",131.75616449918539,172.0382686854841,134.3761722281279,132.0583230812739,130.66502413522127,129.58386920052652,128.7719602890522]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",23.709953677728915,22.980171249667006,18.420656491220676,24.113374169275804,22.332268482170743,28.720976366159043,27.896821979286781]
[null,null,"> 1 kV & < = 11 kV","per km",206.55136767587715,166.51102753879294,205.38491484050371,239.80086892089548,231.40403552499944,267.19264046672697,262.53941306790972]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",8.8776449811831117,7.0977840361665123,8.8373730850757948,10.318234649438743,9.8808024700612158,11.496857260547559,11.296636584141117]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",36.445376355942727,29.138517144984622,36.280048229698721,42.359425942893232,40.563636581930346,47.198022748074344,46.3760572469374]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",48.460605674564292,38.744837630806359,48.240772545264768,56.324385764910261,53.936564625507742,62.758160230676019,61.665211000582602]
[null,null,"> 22 kV & < = 66 kV","per km",11.385858201353289,6.8082583013451572,11.263615452344457,11.605594227786591,14.540207040814821,11.832261422976146,11.818324946191872]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",5.6416076317807287,4.3137904479817868,3.771626697130726,3.7480533862363119,3.6760820792125002,3.5931296620969566,3.5175162816764787]
[null,null,"> 1 kV & < = 11 kV","per km",0.96328465769129934,0.8372062403635816,0.60576149955505132,0.60197538674390239,0.59041606489986942,0.57709306540422578,0.56494878963462758]
[null,null,"> 11 kV & < = 22 kV","per km",0.18275199052212057,0.15883270400120622,0.11492357834357543,0.11420528635474932,0.1120122803110884,0.1094846736912658,0.10718069163090282]
[null,null,"> 22 kV & < = 33 kV","per km",1.0285910355103929,0.43593468799827112,0.28105107728379758,0.27929446005891123,0.27393135946681041,0.26774997725012528,0.26211547953050429]
[null,null,"> 33 kV & < = 66 kV","per km",1.74715705589087,1.6582631282512741,0.28105107728379758,0.27929446005891123,0.27393135946681041,0.26774997725012534,0.26211547953050429]
[null,null,"> 66 kV & < = 132 kV","per km",0.7527878359355864,0.43593468799827106,0.28105107728379752,0.27929446005891118,0.27393135946681041,0.26774997725012528,0.26211547953050424]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",6561.5730760404813,8196.9655811131124,6587.4179614371396,6813.3862210627167,6453.6997314711753,6298.068232333555,6153.2521520012442]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",380.27666016714295,475.05600541252693,381.79099114605765,394.88047206860824,374.04012120306078,365.02037735507412,356.6275225365888]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,481.2851149248018,638.62333122930227,755.24806787002888,886.83888825921565,878.91756755029087,861.31413882712548,828.73791275474184]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,5.7144670637509449,7.582598919609131,8.9673253441032443,10.529749332893063,10.435696712338546,10.226685025651888,9.8398960617317606]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0.32049301833448174,0.42526625623250341,0.50292794303594945,0.59055570858242934,0.58528081454462932,0.57355849895752731,0.55186563396726906]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,111.99928045477039,148.61326760642868,175.75286985452507,206.37521145830519,204.53185043977533,200.43537770585453,192.85460330228929]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,120.95621951606168,160.49834379839328,189.8083864501854,222.87969421290322,220.88891374449929,216.46483304296495,208.27779997332237]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.32049301833448179,0.42526625623250347,0.50292794303594945,0.59055570858242934,0.58528081454462921,0.5735584989575272,0.55186563396726895]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0.97346680117325191,1.1113389263782638,1.0159757516474341,1.0096257297131339,0.99023857700096574,0.96789340577973859,0.94752517552361604]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,13.369497765699441,15.263020038527914,13.953311530793275,13.86610095107916,13.599839693318529,13.292953298881336,13.013218018158579]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,4.2627384180490981,4.8664701572117997,4.4488819373543782,4.4210756655614727,4.3361807717827201,4.2383329358752091,4.1491419768041844]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,8.137955161730094,9.2905339364952528,8.4933200622219935,8.4402353615264456,8.2781632915851908,8.0913628775799431,7.9210892284443526]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,3.5906736005748177,4.1302356780645146,3.7151010438308245,3.6147911272133828,3.6199635304481563,3.3903525997591388,3.3698408331301102]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,4.5857534551712398,5.4972053293076621,4.9256549651359407,4.7091727709001887,4.7984073266038534,4.3338041943075813,4.3650552723864759]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0.33278365939013033,0.4183084474140682,0.36778200022880675,0.33826904907365996,0.35810338887125936,0.2978022455354507,0.30948087371634281]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,6.9050298176448832,8.679609773088945,7.6312210840731751,7.018847844033524,7.4303966200963751,6.1791897743789184,6.4215131984497829]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,1.2669931113009125,1.5926080091909793,1.4002408099133632,1.2878774027789552,1.3633918434122902,1.1338098580766713,1.1782734037980931]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0.33278365939013027,0.41830844741406814,0.36778200022880675,0.33826904907365996,0.35810338887125936,0.2978022455354507,0.30948087371634292]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,65.571404447012696,53.418905714701495,56.688364402565028,56.242513069136756,55.233289695166398,54.102582229538775,53.082663283661709]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,819.63924000616589,680.2080536916967,787.9762314067541,856.36898623583727,847.34831755861148,833.27405050739242,811.5423942232328]
[null,null,"˂ = 11 kV  ; Switch",null,77.448665313819646,79.950799631836006,131.23509941466037,136.17673448952596,138.83444867048348,120.03033209112949,124.57722220472277]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,73.490384968472057,84.150530159886273,81.746404962450754,81.405545687728662,80.008441314440958,78.278239018123699,76.712987493846057]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,469.74786964689537,421.74089996258289,560.73751929403193,592.97443650244816,586.88012315176979,575.06853155469969,563.40859375236812]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,42.933433769258521,44.254409739655131,43.919360860891523,46.794777954079017,51.166855035615768,50.877235556547738,43.750240656345298]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,6.4606268562582354,5.1282543651610482,11.540604445818591,11.20793884739088,12.148027334159258,8.0413697524494285,9.7448363489680947]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,22.775089057679349,21.348961650684238,8.307809905106291,11.542568561083863,16.820410655161599,17.343389727660188,10.659122706399256]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,8.9011615107949673,8.6285231500153152,33.282864835060401,31.99479511531684,36.77919960710161,17.402559925664644,25.7803597366632]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,42.731967529421844,39.641509424203427,11.152935609776138,17.586486319844813,28.130446032923192,29.281495880655701,16.161508874190787]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,3.7291535593681702,3.609261528137599,14.102181986246457,13.554045567934171,15.594365137680482,7.3380004975094675,10.909667300825902]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,10.923400126359782,10.133398813319159,2.850979847001665,4.4955624090126376,7.1908722091727117,7.4851104289202759,4.1313011846915293]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires",null,2900,2632,2343,1991,1692,1692,1692]
[null,null,"Brackets",null,0,0,0,0,0,0,0]
[null,null,"Lamps",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns",null,612,925,823,1130,916,452,890]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,8.8671118582795074,11.835792949875776,16.787416536085015,16.682492316140287,16.362149820268591,15.992930676748077,15.656377402855496]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,164.5072503051513,190.25018255912028,138.64779395773647,111.9472425257958,106.98227317588123,77.050231182517976,99.673765557221557]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,1.7866017555128593,2.0409399632857568,1.2245625994276084,1.2169088740767036,1.1935414048411273,1.1666086154404443,1.1420586466565112]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"OTHER - Zone Sustation Property"},null,11.471353972623161,9.9009273162052196,11.294613497552483,8.9807632614077235,8.4289702100938531,8.2387667713088337,8.8573451377708103]
[null,{"$f":"IF(ISBLANK(B140),\"\",B140)","v":""},{"$f":"IF(ISBLANK(C140),\"\",C140)","v":"OTHER - Zone Sustation Batteries"},null,13.857485998929334,8.1400147285538065,31.190382274791155,33.495069080482068,42.65841934988709,47.44695991685294,46.448491905015487]
[null,"","OTHER - Zone Sustation Current transformers",null,11.764651788477389,12.714348043141499,11.631699505061796,11.558999396943509,11.337039833202912,11.08121451787131,10.848022797099471]
[null,"","OTHER - Zone Sustation Voltage transformers",null,24.907066667313082,51.997782194732977,33.583783903341008,33.317850101914388,32.889687430174419,32.021036573585313,31.359836450914006]
[null,"","OTHER - Zone Sustation Surge Diverters",null,87.874695663063378,99.251107256033151,563.48454421733481,559.96266959619641,150.03742611383029,146.65176527009757,143.56564348783189]
[null,"","OTHER - Zone Sustation Protection Relays",null,119.50537336497597,104.19657103319405,99.786921120754485,99.163235824284016,97.259071994282962,95.06437804172873,93.063854916406783]
[null,"","OTHER - Frequency Injection Relays",null,7380.7299339053661,9086.4949101768598,13623.268772652029,13538.121016533907,13278.157733250768,12978.53023444079,12705.411634166647]
[null,"","OTHER - Zone Substation Earthing System Refurbishment ",null,1.6619086372312639,0.80255852341778333,3.2673913655772528,3.2469696116075211,3.184620273769339,3.1127579095424429,3.0472534134331317]
[null,"","OTHER - Generation",null,1.0093603659179252E-2,7.0862269624502004E-3,2.5870840724511977E-2,2.8565715058130685E-3,4.2025780738891572E-3,9.5847384311424193E-3,1.3404340528298234E-3]
[null,"","OTHER - Zone Substation Capacitor Bank Refurbishment",null,0,30.156352258961757,1.1333303383896125,1.1262468302488802,1.1046202822647726,1.0796940373022694,1.0569730882529071]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"",""]
[null,"",""]
[]
[]
[]
[null,"ASSET FAILURES"]
[null,null,null,null,"ASSET FAILURES (0's)"]
[null,"ASSET GROUP","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"POLES BY: \nHIGHEST OPERATING VOLTAGE ; MATERIAL TYPE","˂ = 1 kV; Wood - replacement of staked pole",null,0.9479211087420043,0.9479211087420043,0.9479211087420043,1.0036811739621223,1.0036811739621223,1.1152013044023581,1.2824815000627117]
[null,null,"˂ = 1 kV; Wood - replacement of unstaked pole",null,16.052078891257995,16.052078891257995,16.052078891257995,16.996318826037879,16.996318826037879,18.884798695597642,21.717518499937288]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of staked pole",null,1.9406819026384243,1.9406819026384243,1.9406819026384243,1.9880156075808249,2.0353493125232256,2.2246841322928277,2.6033537718320328]
[null,null,"> 1 kV & < = 11 kV; Wood - replacement of unstaked pole",null,39.059318097361576,39.059318097361576,39.059318097361576,40.011984392419173,40.96465068747677,44.775315867707171,52.396646228167967]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of staked pole",null,3.2209004742620739,3.2209004742620739,3.2209004742620739,3.2805467793410013,3.3998393894988554,3.6384246098145647,4.2348876606038379]
[null,null,"˃ 11 kV & < = 22 kV; Wood - replacement of unstaked pole",null,50.779099525737927,50.779099525737927,50.779099525737927,51.719453220658998,53.600160610501142,57.361575390185436,66.765112339396154]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of staked pole",null,1.0236045305297383,1.0236045305297383,1.0236045305297383,1.0236045305297383,1.0804714488925016,1.2510722039807913,1.5354067957946074]
[null,null,"> 22 kV & < = 66 kV; Wood - replacement of unstaked pole",null,16.976395469470262,16.976395469470262,16.976395469470262,16.976395469470262,17.919528551107497,20.74892779601921,25.464593204205393]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of staked pole",null,0.17952127659574468,0.17952127659574468,0.17952127659574468,0.17952127659574468,0.17952127659574468,0.17952127659574468,0.17952127659574468]
[null,null,"> 66 kV & < = 132 kV; Wood - replacement of unstaked pole",null,0.82047872340425532,0.82047872340425532,0.82047872340425532,0.82047872340425532,0.82047872340425532,0.82047872340425532,0.82047872340425532]
[null,null,"> 132 kV; Wood - replacement of staked pole",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Wood - replacement of unstaked pole",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Concrete",null,2.3333333333333335,2.3333333333333335,2.3333333333333335,2.3333333333333335,2.5,2.8571428571428572,3.4693877551020407]
[null,null,"> 66 kV & < = 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Concrete",null,0,0,0,0,0,0,0]
[null,null,"˂ = 1 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV; Steel",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6833333333333333,1.7464583333333334,1.8905411458333334,2.19775408203125]
[null,"POLE TOP STRUCTURES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 kV",null,157,157,157,156.60749999999999,156.02022187499998,155.43514604296874,154.65797031275389]
[null,null,"> 1 kV & < = 11 kV",null,209.33333333333334,209.33333333333334,209.33333333333334,208.81,208.0269625,207.24686139062499,206.21062708367185]
[null,null,"˃ 11 kV & < = 22 kV",null,92.666666666666671,92.666666666666671,92.666666666666671,92.435000000000002,92.088368750000001,91.743037367187497,91.284322180351566]
[null,null,"> 22 kV & < = 66 kV",null,10,10,10,9.9749999999999996,9.9375937499999996,9.9003277734374997,9.8508261345703119]
[null,null,"> 66 kV & < = 132 kV",null,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66499999999999992,0.66250624999999996,0.66002185156249993,0.65672174230468738]
[null,null,"> 132 kV",null,0,0,0,0,0,0,0]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"STAKING WOODEN POLES BY: \nHIGHEST OPERATING VOLTAGE","˂ = 1 Kv","for year wooden pole staked",1.4,1.4,1.4,0,0,0,0]
[null,null,"> 1 kV & < = 11 kV","for year wooden pole staked",1.28,1.28,1.28,0,0,0,0]
[null,null,"˃ 11 kV & < = 22 kV","for year wooden pole staked",1.1200000000000001,1.1200000000000001,1.1200000000000001,0,0,0,0]
[null,null,"> 22 kV & < = 66 kV","for year wooden pole staked",0.2,0.2,0.2,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,null,"> 132 kV","for year wooden pole staked",0,0,0,0,0,0,0]
[null,"OVERHEAD CONDUCTORS BY: \nHighest operating voltage; Number of phases (at HV)","˂ = 1 kV","per km",348,348,348,360.66964195279189,374.02041350843905,388.06749729056895,402.84014784807221]
[null,null,"> 1 kV & < = 11 kV","per km",316.33333333333331,316.33333333333331,316.33333333333331,327.85008641111062,339.98598890757535,352.75484188577582,366.18323784273997]
[null,null,"˃ 11 kV & < = 22 kV  ; SWER","per km",19.333333333333332,19.333333333333332,19.333333333333332,20.037202330710659,20.778911861579946,21.559305405031608,22.380008213781789]
[null,null,"˃ 11 kV & < = 22 kV ; Single-Phase","per km",38.333333333333336,38.333333333333336,38.333333333333336,39.728935655719411,41.199566622098168,42.746898647907493,44.374154216981125]
[null,null,"˃ 11 kV & < = 22 kV ; Multiple-Phase","per km",85.333333333333329,85.333333333333329,85.333333333333329,88.440065459688427,91.71381787180114,95.158313511863639,98.780725909105826]
[null,null,"> 22 kV & < = 66 kV","per km",22.666666666666668,22.666666666666668,22.666666666666668,23.491892387729742,24.361482872197179,25.276427026588781,26.238630319606234]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"UNDERGROUND CABLES BY: \nHighest operating voltage","˂ = 1 kV","per km",54.666666666666664,54.666666666666664,54.666666666666664,54.666666666666664,54.666666666666664,54.666666666666664,54.666666666666664]
[null,null,"> 1 kV & < = 11 kV","per km",9.3333333333333339,9.3333333333333339,9.3333333333333339,9.3333333333333339,9.3333333333333339,9.3333333333333339,9.3333333333333339]
[null,null,"> 11 kV & < = 22 kV","per km",2.3333333333333335,2.3333333333333335,2.3333333333333335,2.3333333333333335,2.3333333333333335,2.3333333333333335,2.3333333333333335]
[null,null,"> 22 kV & < = 33 kV","per km",0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"> 33 kV & < = 66 kV","per km",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV","per km",0,0,0,0,0,0,0]
[null,null,">  132 kV","per km",0,0,0,0,0,0,0]
[null,null,"Other","per km",0,0,0,0,0,0,0]
[null,"SERVICE LINES BY: \nConnection voltage; Customer type; Connection complexity","˂ = 11 kV ; Residential ; Simple Type","per number of spans",1323.6666666666667,1323.6666666666667,1323.6666666666667,1323.6666666666667,1323.6666666666667,1323.6666666666667,1323.6666666666667]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Simple Type","per number\n of spans",194.33333333333334,194.33333333333334,194.33333333333334,194.33333333333334,194.33333333333334,194.33333333333334,194.33333333333334]
[null,null,"˂ = 11 kV ; Residential ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Commercial & Industrial ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"˂ = 11 kV ; Subdivision ; Complex Type","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 11 kV  & < = 22 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 22 kV & < = 33 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 33 kV & < = 66 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 66 kV & < = 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Commercial & Industrial  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Subdivision  ","per number\n of spans",0,0,0,0,0,0,0]
[null,null,"Other","per number\n of spans",0,0,0,0,0,0,0]
[null,"TRANSFORMERS BY: \nMounting type; Highest operating voltage; Ampere rating; Number of phases (at LV)","Pole Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,125,125,125,143.85964912280701,147.22478711398378,143.43654697771754,138.23592363700499]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,2,2,2,2.3017543859649123,2.3555965938237406,2.2949847516434807,2.2117747781920798]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Pole Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,44,44,44,50.638596491228071,51.823125064122294,50.489664536156575,48.659045120225748]
[null,null,"Pole Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,45.333333333333336,45.333333333333336,45.333333333333336,52.173099415204682,53.393522793338121,52.019654370585563,50.133561639020471]
[null,null,"Pole Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.76725146198830407,0.78519886460791355,0.76499491721449353,0.73725825939735989]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA ; Single Phase",null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  < = 60 kVA  ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 60 kVA and < = 600 kVA  ; Multiple Phase",null,4.333333333333333,4.333333333333333,4.333333333333333,4.333333333333333,4.333333333333333,4.333333333333333,4.333333333333333]
[null,null,"Kiosk Mounted ; < = 22kV ;  > 600 kVA  ; Multiple Phase",null,1,1,1,1,1,1,1]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂ 22 kV ;  < = 60 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Single Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  < = 60 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  > 60 kVA  and < = 600 kVA ; Multiple Phase",null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; ˂  22 kV ;  >  600 kVA ; Multiple Phase",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  < = 15 MVA",null,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.66666666666666663]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 15 MVA and < = 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > = 22 kV & < = 33 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  < = 15 MVA",null,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 15 MVA and < = 40 MVA",null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 33 kV & < = 66 kV ;  > 40 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  < = 100 MVA",null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 66 kV & < = 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  < = 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Ground Outdoor / Indoor Chamber Mounted; > 132 kV ;  > 100 MVA",null,0,0,0,0,0,0,0]
[null,null,"Other",null,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.6666666666666667]
[null,"SWITCHGEAR BY: \nHighest operating voltage; Switch function","˂ = 11 kV ;  Fuse",null,340.66666666666669,340.66666666666669,340.66666666666669,346,348.1,350.2,352.3]
[null,null,"˂ = 11 kV  ; Switch",null,69.666666666666671,69.666666666666671,69.666666666666671,69.666666666666671,67.086419753086432,64.601737540009154,64.601737540009154]
[null,null,"˂ = 11 kV ;  Circuit Breaker",null,38,38,38,38,36.479999999999997,36.479999999999997,35.020799999999994]
[null,null,"> 11 kV & < = 22 kV  ; Switch",null,40,40,40,40,38.518518518518519,37.091906721536354,37.091906721536354]
[null,null,"> 11 kV & < = 22 kV  ; Circuit Breaker",null,8,8,8,8,7.68,7.68,7.3727999999999998]
[null,null,"> 22 kV & < = 33 kV ; Switch",null,2.6666666666666665,2.6666666666666665,2.6666666666666665,2.7682539682539682,2.8275736961451248,2.9218261526832956,3.1861818522117842]
[null,null,"> 22 kV & < = 33 kV ; Circuit Breaker",null,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.4322916666666667,1.2457953559027779,1.2036199922914859,1.2036199922914859]
[null,null,"> 33 kV & < = 66 kV ; Switch",null,1,1,1,1.0380952380952382,1.0603401360544218,1.0956848072562357,1.194818194579419]
[null,null,"> 33 kV & < = 66 kV ; Circuit Breaker",null,1.6666666666666667,1.6666666666666667,1.6666666666666667,1.4322916666666667,1.2457953559027779,1.2036199922914859,1.2036199922914859]
[null,null,"> 66 kV & < = 132 kV ; Switch",null,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.69206349206349205,0.70689342403628119,0.7304565381708239,0.79654546305294605]
[null,null,"> 66 kV & < = 132 kV  ; Circuit Breaker",null,0.66666666666666663,0.66666666666666663,0.66666666666666663,0.57291666666666663,0.49831814236111105,0.48144799691659429,0.48144799691659429]
[null,null,"> 132 kV ; Switch",null,0,0,0,0,0,0,0]
[null,null,"> 132 kV ; Circuit Breaker",null,0,0,0,0,0,0,0]
[null,null,"Other",null,38.333333333333336,38.333333333333336,38.333333333333336,7,0,0,0]
[null,"PUBLIC LIGHTING BY: \nAsset type ; Lighting obligation","Luminaires",null,1668.0991037494805,1316,1171.5,995.5,846,846,846]
[null,null,"Brackets",null,0,0,0,0,0,0,0]
[null,null,"Lamps",null,0,0,0,0,0,0,0]
[null,null,"Poles / Columns",null,8,8,8,8,9,9,9]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,"SCADA, NETWORK CONTROL AND PROTECTION SYSTEMS BY: \nFunction","Field Devices",null,15.333333333333334,15.333333333333334,15.333333333333334,15.333333333333334,15.333333333333334,15.333333333333334,15.333333333333334]
[null,null,"Local Network Wiring Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Network Assets",null,11.333333333333334,11.333333333333334,11.333333333333334,11.333333333333334,11.333333333333334,11.333333333333334,11.333333333333334]
[null,null,"Master Station Assets",null,0,0,0,0,0,0,0]
[null,null,"Communications Site Infrastructure",null,0,0,0,0,0,0,0]
[null,null,"Communications Linear Assets",null,0,0,0,0,0,0,0]
[null,null,"AFLC",null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,null,"Other",null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B139),\"\",B139)","v":"OTHER BY: \nenter DNSP defined asset group here"},{"$f":"IF(ISBLANK(C139),\"\",C139)","v":"OTHER - Zone Sustation Property"},null,0,0,0,0,0,0,0]
[null,{"$f":"IF(ISBLANK(B140),\"\",B140)","v":""},{"$f":"IF(ISBLANK(C140),\"\",C140)","v":"OTHER - Zone Sustation Batteries"},null,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331,0.33333333333333331]
[null,"","OTHER - Zone Sustation Current transformers",null,3.3333333333333335,3.3333333333333335,3.3333333333333335,3.3055555555555558,3.4708333333333337,3.8468402777777779,3.7987547743055559]
[null,"","OTHER - Zone Sustation Voltage transformers",null,1,1,1,1.0063291139240507,1.0827591732094215,1.1649940471240612,1.1797408072142392]
[null,"","OTHER - Zone Sustation Surge Diverters",null,0,0,0,0,0,0,0]
[null,"","OTHER - Zone Sustation Protection Relays",null,43,43,43,43,43,43,43]
[null,"","OTHER - Frequency Injection Relays",null,7305,7305,7305,7305,7305,7305,7305]
[null,"","OTHER - Zone Substation Earthing System Refurbishment ",null,0,0,0,0,0,0,0]
[null,"","OTHER - Generation",null,0,0,0,0,0,0,0]
[null,"","OTHER - Zone Substation Capacitor Bank Refurbishment",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"","",null,0,0,0,0,0,0,0]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]
[null,"",""]

{"sheet":"2.3 Augex (a)","index":7,"n_rows":126,"n_cols":32,"rows_kept":126,"cut":false,"hidden":false,"merged":[[68,1,68,10],[69,7,69,10],[70,7,70,10],[68,11,68,22],[69,21,69,22],[69,17,69,19],[69,11,69,13],[69,3,70,3],[69,4,70,4],[69,5,70,5],[69,6,70,6],[69,1,70,1],[10,6,11,6],[10,7,10,8],[10,9,10,10],[10,11,10,13],[5,1,5,3],[9,11,9,22],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[10,21,10,22],[9,30,9,31],[9,23,9,24],[9,26,11,26],[11,27,11,29],[11,30,11,31],[9,27,9,28],[9,29,10,29],[9,25,11,25],[11,23,11,24],[68,30,68,31],[68,29,69,29],[69,14,69,16],[11,14,11,15],[10,14,10,16],[10,17,10,19],[11,17,11,18],[68,25,70,25],[68,26,70,26],[70,27,70,29],[70,30,70,31],[68,23,68,24],[68,27,68,28],[70,23,70,24]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are TWO tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation.  Both ROWS and COLUMNS have been grouped. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.1 - AUGEX ASSET DATA - SUBTRANSMISSION SUBSTATIONS, SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON-RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"SUBSTATION ID","SUBSTATION TYPE","PROJECT ID","PROJECT TYPE","PROJECT TRIGGER","VOLTAGE (KV)","SUBSTATION RATING\nNORMAL CYCLIC\n(MVA)",null,"SUBSTATION RATING\nN-1 EMERGENCY\n(MVA)",null,"TRANSFORMERS",null,null,"SWITCHGEAR",null,null,"CAPACITORS",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"PRE","POST","PRE","POST","UNITS ADDED ","MVA ADDED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"UNITS ADDED ",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"MVAR ADDED",null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2019)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"}]
[null,"COB (Cobaki 66/11kV)","Zone substation","ESS_1005",null,"Demand growth","66/11",0,16,null,null,1,16,545438.26560299995,11,null,547807.08932999999,null,null,null,1641252.7548884996,null,1186182.0721634778,1678887.2140499998,null,{"$f":"SUM(N13,Q13,T13,U13,W13,X13,Y13)","v":5599567.3960349765},"2018,2022,2023,2024",null,null,1678887.2140499998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N45,Q45,T45,U45,W45,X45,Y45)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Non material projects - [forecast]"]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.2 - AUGEX ASSET DATA - SUBTRANSMISSION LINES"]
[null,"PROJECT DESCRIPTION AND CHANGES",null,null,null,null,null,null,null,null,null,"PLANT AND EQUIPMENT EXPENDITURE AND VOLUME",null,null,null,null,null,null,null,null,null,null,null,"OTHER EXPENDITURE",null,"TOTAL DIRECT EXPENDITURE ($0's)","YEARS INCURRED","ALL RELATED PARTY CONTRACTS",null,"ALL NON RELATED PARTY CONTRACTS","LAND AND EASEMENTS"]
[null,"LINE ID",null,"PROJECT ID","PROJECT TYPE","PROJECT TRIGGER","VOLTAGE (KV)","ROUTE LINE LENGTH ADDED",null,null,null,"POLES/TOWERS (INCLUDING STRUCTURES, AND CIVIL WORKS)",null,null,"OVERHEAD LINES",null,null,"UNDERGROUND CABLES",null,null,"OTHER PLANT ITEM","INSTALLATION (LABOUR)",null,"CIVIL WORKS","OTHER DIRECT",null,null,"RELATED PARTY MARGINS","TOTAL",null,"LAND PURCHASE","EASEMENTS"]
[null,null,null,null,null,null,null,"KM ADDED",null,null,null,"POLES/TOWERS ADDED","POLES/TOWERS UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"CIRCUIT KM ADDED","CIRCUIT KM UPGRADED",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},"VOLUME",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"}]
[null,"Tharbogang to Tabbita Lane",null,"ESS_5025",null,"Demand growth","Other",30,null,null,null,200,null,1597000,30,null,400000,null,null,null,500000,10000,700000,null,800000,{"$f":"SUM(N72,Q72,T72,U72,W72,X72,Y72)","v":3997000},"2018,2019,2020,2021",null,null,1962437,null,1500000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(N104,Q104,T104,U104,W104,X104,Y104)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,"Non material projects - [forecast]"]

{"sheet":"2.3 Augex (b)","index":8,"n_rows":79,"n_cols":10,"rows_kept":79,"cut":false,"hidden":false,"merged":[[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[51,1,51,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[45,1,46,2],[5,1,5,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[9,1,10,1],[9,2,10,2],[34,1,34,2],[29,1,30,1],[29,2,30,2],[45,3,45,9],[47,1,47,2],[9,3,9,9],[29,3,29,9],[31,1,31,2],[32,1,32,2],[33,1,33,2],[68,1,69,2],[68,3,68,9],[70,1,70,2],[71,1,71,2],[60,1,61,2],[60,3,60,9],[62,1,62,2],[63,1,63,2],[77,1,77,2],[78,1,78,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.3 AUGEX PROJECT DATA"]
[]
[null,"There are FOUR tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"NOTE: DNSP must provide expenditure information on an 'as incurred' basis. "]
[null,"2.3.3 - AUGEX DATA - HV/LV FEEDERS AND DISTRIBUTION SUBSTATIONS"]
[null,"PROJECT TYPE","Units","VOLUMES (0's)"]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"DESCRIPTOR METRICS - UNITS ADDED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",0.11374125414624633,9.6002172368422872E-2,0.12425605663799631,0.11625814928139931,0.11277431662702017,0.11070765022362188,0.10986805703435466]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",109.97450086184732,73.511162064939441,80.017231657577497,74.866815468263397,72.623330103410396,71.292457960562416,70.75178473672554]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[null,"DESCRIPTOR METRICS - UNITS UPGRADED"]
[null,"HV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",16,16,16,16,16,16,16]
[null,"HV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines","Circuit Line Length in KM",16.019648417572846,15.178429167002859,17.39588929399638,16.276179601580019,15.788441870203654,15.499107885737388,15.381564559740513]
[null,"LV Feeder Augmentations - Underground Cables","Circuit Line Length in KM",0.15158650012555749,0.17620540048325029,0.16324266285522956,0.15273533042020773,0.14815840970639726,0.14544330562171631,0.14434028149847059]
[null,"Distribution Substation Augmentations - Pole Mounted","Number",173.50064065764917,107.38132167471292,115.72187188364603,108.27327874863443,105.02872353738491,103.10400041940406,102.32207237411106]
[null,"Distribution Substation Augmentations - Ground Mounted","Number",0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Indoor","Number",0,0,0,0,0,0,0]
[]
[null,"COST METRICS"]
[null,"PROJECT TYPE",null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"HV Feeder Augmentations - Overhead Lines",null,17533135.253748231,19079807.806804094,19523810.560680337,16132236.601615159,15201761.43888719,14945722.618634701,14845872.570994727]
[null,"HV Feeder Augmentations - Underground Cables",null,2635031.5484177186,2192563.969832649,2610854.4151900294,2269199.877978283,2164857.5934203351,2115545.5055997102,2099515.8059908319]
[null,"HV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"LV Feeder Augmentations - Overhead Lines",null,4600876.4223707933,4576401.0246851929,5201851.425189442,4461371.6175121684,4234150.8841322865,4095157.910783371,3896447.405102795]
[null,"LV Feeder Augmentations - Underground Cables",null,505168.11802497762,746989.2881011928,472118.18296316196,479532.15837593132,423051.03201154125,420187.543065965,528990.54519100219]
[null,"LV Feeder Non-Material Projects",null,0,0,0,0,0,0,0]
[null,"Distribution Substation Augmentations - Pole Mounted",null,3523944.2134962501,2332179.3181478474,2649223.365576366,2486374.0626329505,2414366.3100757459,2370511.5593612455,2352940.7519742819]
[null,"Distribution Substation Augmentations - Ground Mounted",null,65770.143148331466,136442.23297095747,306633.290882601,296951.27083191258,291329.15878257604,286501.72748929274,284862.19511022413]
[null,"Distribution Substation Augmentations - Indoor",null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"2.3.4 - AUGEX  - TOTAL EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,4859330.4517429993,5459767.5901455386,4955575.5423743473,3690043.8217823524,4323289.5530244531,6344159.7800850142,2555217.5713045676]
[null,"Subtransmission Lines",null,3319672.6397244162,2374066.0020453832,3783812.5997297675,4177716.0848323624,111859.57517790573,109725.20514836356,2960562.7079522782]
[null,"HV Feeders",null,20168166.802165948,21272371.776636742,22134664.975870367,18401436.479593441,17366619.032307524,17061268.124234412,16945388.376985557]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,3589714.3566445815,2468621.5511188051,2955856.6564589669,2783325.3334648632,2705695.4688583221,2657013.2868505381,2637802.947084506]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,5106044.5403957712,5323390.3127863854,5673969.6081526037,4940903.7758880993,4657201.9161438281,4515345.4538493361,4425437.9502937971]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,1027418.2093262812,717272.76726714894,1122296.2342150514,693035.697822758,485967.63276936382,477963.47995066515,475278.78564139834]
[]
[]
[]
[null,"2.3.5 - AUGEX - BY DRIVER"]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"\"Greenfield\" driven augex (network expansion capex)",null,4830863.6307551414,4531353.7589070303,7418009.1342105018,7583433.5757431937,4761375.8787648082,6858221.1884124652,6100733.7468661638]
[null,"Reinforcement driven augex (augmentation of the existing network)",null,33239483.369244859,33084136.241092969,33208166.482590605,27103027.617640678,24889257.299516592,24307254.141705863,23898954.592395943]
[]
[]
[]
[null,"2.3.6 - AUGEX - GREENFIELDS DRIVEN "]
[null,null,null,{"$f":"CONCATENATE(\"TOTAL DIRECT EXPENDITURE\n($0's, real \", dms_DollarReal,\")\")","v":"TOTAL DIRECT EXPENDITURE\n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Subtransmission Substations, Switching Stations, Zone Substations",null,529300.91759138787,256168.84545255319,0,0,1457902.8983080916,3764949.3514012382,0]
[null,"Subtransmission Lines",null,200471.91833214849,717272.76726714894,3060807.9114955948,3960203.9875586173,0,0,2851672.7138483897]
[null,"HV Feeders",null,1880091.3178799278,1710352.1976035833,1997453.0727570755,1788440.655498059,1793213.5897906646,1643304.9547708894,1725853.8026436088]
[null,"HV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Distribution Substations",null,1478411.7318150573,988226.93955838587,1075689.4834970441,1006451.2904764854,976291.61657425342,958400.40566524421,951132.01498436439]
[null,"Distribution Substations - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"LV Feeders",null,742587.74513662024,859333.00902535929,671897.08416166808,630327.44283210172,533967.77409179858,491566.47657509363,572075.21538980154]
[null,"LV Feeders - Land Purchases and Easements",null,0,0,0,0,0,0,0]
[null,"Other Assets",null,0,0,612161.58229911898,198010.19937793087,0,0,0]

{"sheet":"2.4 Augex model","index":9,"n_rows":7860,"n_cols":50,"rows_kept":7860,"cut":false,"hidden":false,"merged":[[1278,4,1278,5],[5,1,5,4],[1276,14,1276,15],[8,11,8,15],[8,16,10,16],[8,1,11,1],[8,2,10,2],[8,3,10,3],[8,4,10,4],[8,5,10,5],[1276,11,1277,11],[1276,12,1277,13],[1275,4,1277,5],[1275,3,1277,3],[1275,11,1275,15],[1275,16,1277,16],[8,17,11,17],[9,6,10,6],[6717,1,6720,1],[6717,2,6719,2],[6717,3,6719,3],[6717,4,6718,5],[6717,6,6717,13],[6717,14,6717,21],[9,7,10,8],[9,9,9,10],[9,11,10,11],[9,12,10,13],[9,14,9,15],[8,6,8,10],[1275,1,1278,1],[1275,2,1277,2],[1275,17,1278,17],[6717,22,6719,22],[6717,23,6720,23],[6718,6,6720,6],[6718,7,6719,8],[6718,9,6718,13],[6718,14,6720,14],[6718,15,6719,16],[6718,17,6718,21],[1275,6,1275,10],[7664,1,7667,1],[7664,2,7667,2],[7664,3,7664,14],[7664,15,7664,26],[7664,27,7666,27],[7664,28,7666,28],[7665,3,7665,13],[7665,14,7666,14],[7665,15,7665,25],[7665,26,7666,26],[7727,4,7727,7],[7727,8,7727,11],[7728,1,7733,1],[7728,2,7733,2],[7728,3,7732,3],[7728,4,7732,4],[7728,5,7733,5],[7728,6,7732,6],[7728,7,7732,7],[7728,8,7732,8],[7728,9,7733,9],[7728,10,7732,10],[7728,11,7732,11],[7839,1,7843,1],[7839,2,7839,9],[7839,10,7839,17],[7839,18,7839,25],[7839,26,7839,31],[7842,3,7842,9],[7842,11,7842,17],[7842,19,7842,25],[7840,2,7841,9],[7840,10,7841,17],[7840,18,7841,25],[7840,26,7840,31],[7842,26,7842,28],[7842,29,7842,31],[7842,38,7842,40],[7842,41,7842,43],[7842,44,7842,46],[7842,47,7842,49],[7842,32,7842,34],[7842,35,7842,37],[7839,38,7839,43],[7839,44,7839,49],[7840,38,7840,43],[7840,44,7840,49],[7841,26,7841,28],[7841,29,7841,31],[7841,32,7841,34],[7841,35,7841,37],[7841,38,7841,40],[7841,41,7841,43],[7841,44,7841,46],[7841,47,7841,49],[7839,32,7839,37],[7840,32,7840,37]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.4 AUGEX MODEL"]
[]
[null,"There are SIX tables on this worksheet. These tables have been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.4.1 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION LINES"]
[null,"Line ID","Primary type of area supplied by line","Line voltage","Originating substation","Terminating substation",{"$f":"CRCP_y4","v":"2017-18"},null,null,null,null,{"$f":"PRCP_y5","v":"2013-14"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual line maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual line maximum demand (50% PoE) from 2017-18 to 2018-19"},"Network Segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Line rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","N-1 emergency",null,null,null,"Thermal","N-1 emergency"]
[null,null," CBD, urban, long rural, or short rural "," kV "," name "," name "," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[null,"997/1","Short Rural",132,"Union Rd ZS","Corowa ZS",59.394999999999996,31.052770943407886,30.431715524539726,128,0,59.394999999999996,17.931277687860174,17.57265213410297,128,0,2.0843314840955866E-3,9]
[null,"997/2","Urban",132,"Corowa ZS","Mulwala ZS",40.515000000000001,15.9,15.582000000000001,128,0,40.515000000000001,14.942731406550143,14.643876778419139,128,0,3.077454988543853E-3,9]
[null,"99E","Urban",132,"Union Rd ZS","Jelbart ZS",2.734,20.892290365881657,20.474444558564024,148,0,2.734,26.896916531790254,26.358978201154446,148,0,7.0868170952076972E-3,9]
[null,"99G","Urban",132,"Union Rd ZS","Jelbart ZS",2.7490000000000001,20.892290365881657,20.474444558564024,148,0,2.7490000000000001,26.896916531790254,26.358978201154446,148,0,7.0868170952076972E-3,9]
[null,"661/1","Short Rural",66,"TransGrid Armidale 330/132/66kV STS","Hillgrove Tee",19.600000000000001,0.8,0.78400000000000003,20,0,19.600000000000001,1.9528834750221327,1.9138258055216899,12,0,1.2957813083787727E-2,9]
[null,"661/2","Short Rural",66,"Hillgrove Tee","Hillgrove ZS",4.8,0.4,0.39200000000000002,16,0,4.8,0.97644173751106644,0.95691290276084506,9,0,1.2957813083787727E-2,9]
[null,"661/3","Short Rural",66,"Hillgrove Tee","Oaky ZS",19.3,0.5,0.49,20,0,19.3,1.220552171888833,1.1961411284510564,12,0,1.2957813083787725E-2,9]
[null,"662/1","Short Rural",66,"TransGrid Armidale 330/132/66kV STS","Uralla Tee",23.8,6.6,6.468,9,0,23.8,6.3338707802679393,6.2071933646625803,15,0,1.2957813083787744E-2,9]
[null,"662/2","Short Rural",66,"Uralla Tee","Uralla ZS",13.8,3.9,3.8220000000000001,9,0,13.8,3.8501241304434508,3.7731216478345817,9,0,2.083376929627294E-3,9]
[null,"662/3","Short Rural",66,"Uralla Tee","Walcha ZS",0,0,0,0,0,30.2,3.1590762095946263,3.0958946854027336,16,0,0,9]
[null,"662/4","Long Rural",66,"Uralla Tee","Walcha South ZS",38.799999999999997,1.4,1.3719999999999999,9,0,38.799999999999997,1.3820958416976488,1.3544539248636958,9,0,1.2957813083787705E-2,9]
[null,664,"Short Rural",66,"TransGrid Armidale 330/132/66kV STS","Galloway St ZS",4.5999999999999996,19.3,18.914000000000001,28,0,4.5999999999999996,18.494955263444901,18.125056158176001,15,0,1.2957813083787725E-2,9]
[null,665,"Short Rural",66,"TransGrid Armidale 330/132/66kV STS","Madgwick Dr ZS",13.1,12.4,12.151999999999999,21,0,13.1,12.406553841317075,12.158422764490734,21,0,1.2957813083787711E-2,9]
[null,"66C","Short Rural",66,"Miller St ZS","Madgwick Dr ZS",3.6,3,2.94,21,0,3.6,3.1016384603292688,3.0396056911226834,21,0,1.2957813083787744E-2,9]
[null,"66F","Urban",66,"Galloway St ZS","Miller St ZS",12.14,7.6,7.4479999999999995,15,0,12.14,8.0412848971499571,7.8804591992069577,15,0,1.2957813083787699E-2,9]
[null,"89A","Short Rural",66,"Bega 132/66","Pambula ZS",24.1,14.6,14.308,38,0,24.1,23.411784355746999,22.943548668632058,38,0,0,9]
[null,"84G","Short Rural",66,"Bega 132/66kV STS","Eden South ZS",44,9.3000000000000007,9.1140000000000008,61,0,44,7.8031202900856833,7.6470578842839698,61,0,0,9]
[null,"84M","Short Rural",66,"Bega 132/66kV STS","Maher St ZS",4.3499999999999996,10.7,10.485999999999999,61,0,0,0,0,0,0,0,9]
[null,"89C","Short Rural",66,"Bega 132/66kV STS","Boundary St 66/33kV STS",3.4,10.8,10.584,38,0,3.4,22.943548668632058,22.484677695259418,38,0,0,9]
[null,"89B","Short Rural",66,"Boundary St 66/33kV STS","Maher St ZS",1.1000000000000001,4.2603880225799236,4.1751802621283254,39,0,1.1000000000000001,16.271190127244168,15.945766324699285,39,0,9.8625051674165634E-4,9]
[null,"84H","Short Rural",66,"Eden South ZS","Edrom ZS",17.399999999999999,2.5,2.4500000000000002,38,0,17.399999999999999,2.5752962791321696,2.5237903535495261,38,0,0,9]
[null,"89F","Short Rural",66,"Pambula ZS","Eden South ZS",26.3,1.8,1.764,16,0,26.3,7.8031202900856833,7.6470578842839698,16,0,0,9]
[null,"S839/1","Short Rural",66,"Brown Mountain Hydro","Quira ZS",20.399999999999999,1.1888256346938399,1.165049121999963,21,0,20.399999999999999,0,0,11,0,1.689639840843167E-3,9]
[null,"S839/2","Short Rural",66,"Boundary St 66/33kV STS","Quira ZS",19,1.4,1.3719999999999999,21,0,19,0,0,11,0,0,9]
[null,7803,"Short Rural",33,"Boundary St 66/33kV STS","Quira ZS",15,0,0,6,0,15,0.87794191334051241,0.84282423680689189,6,0,0,9]
[null,"7802/2","Short Rural",33,"Brogo ZS","Cobargo ZS",20.400000000000002,4.4000000000000004,4.2240000000000002,10,0,20.400000000000002,4.4660523417756508,4.2874102481046243,4,0,0,9]
[null,"7802/1","Short Rural",33,"Boundary St 66/33kV STS","Brogo ZS",16.8,5.4,5.1840000000000002,12,0,16.8,5.4738306512541364,5.2548774252039712,12,0,0,9]
[null,7814,"Short Rural",33,"Cobargo ZS","Bermagui ZS",16,2.9,2.7839999999999998,5,0,16,1.4558060242697171,1.3975737832989283,5,0,-6.9452278617925418E-3,10]
[null,7817,"Short Rural",33,"Narooma Tee","Cobargo ZS",26.990000000000002,0,0,10,0,26.990000000000002,0,0,10,0,0,9]
[null,974,"Short Rural",132,"TransGrid Cooma 132/66/11kV STS","Bega 132/66kV STS",92.5,22.3,21.853999999999999,128,0,92.5,44.955290029448854,44.056184228859877,128,0,0,9]
[null,"97R/1","Long Rural",132,"TransGrid Cooma 132/66/11kV STS","Steeple Flat 132/66kV STS",44.448,78.638782654574484,77.066007001482987,140,0,0,0,0,0,0,-2.9182793580734609E-4,10]
[null,"97R/2","Short Rural",132,"Steeple Flat 132/66kV STS","Bega 132/66kV STS",46.8,23.2,22.736000000000001,140,0,0,0,0,0,0,0,9]
[null,"97C","Urban",132,"Steeple Flat 132/66kV STS","Boco Rock Wind Farm",25,113.89999999999999,111.62199999999999,140,0,0,0,0,0,0,0,9]
[null,851,"Short Rural",66,"TransGrid Beryl 132/66kV STS","Gulgong ZS",6.76,4.2,4.1159999999999997,28,0,6.76,4.6091950450376897,4.5170111441369363,11,0,1.8823690385402565E-2,9]
[null,852,"Long Rural",66,"TransGrid Beryl 132/66kV STS","Dunedoo ZS",40.1,13.8,13.524000000000001,15,0,40.1,15.440803400876264,15.131987332858738,15,0,0,9]
[null,"86J","Long Rural",66,"TransGrid Beryl 132/66kV STS","Dunedoo ZS",38.870000000000005,12.602700931802994,12.350646913166933,61,0,0,0,0,0,0,-1.3686459788432262E-2,10]
[null,"80L","Short Rural",66,"Ulan Sw Stn","Ulan Town ZS",0.6,1.7,1.6659999999999999,15,0,0.6,2.0780473553498049,2.0364864082428089,15,0,0,9]
[null,"80T","Urban",66,"Ulan Sw Stn","Moolarben Mine ZS",4.95,28.6,28.028000000000002,43,0,4.95,7.2731657437243182,7.1277024288498314,43,0,2.2019845264441739E-2,9]
[null,"80T/2","Urban",66,"Moolarben Mine ZS","Wilpinjong Mine ZS",13.25,11.9,11.662000000000001,43,0,13.25,3.1170710330247076,3.0547296123642131,43,0,2.2617867195627327E-2,9]
[null,"80U","Short Rural",66,"TransGrid Beryl 132/66kV STS","Ulan Sw Stn",28.9,34,33.32,61,0,28.9,0,0,15,0,6.0551574015795015E-2,9]
[null,"80R","Short Rural",66,"TransGrid Beryl 132/66kV STS","Ulan Sw Stn",31.8,36.5,35.769999999999996,64,0,31.8,36.712169944513221,35.977926545622957,64,0,5.4228233724056253E-2,9]
[null,"85A","Long Rural",66,"Dunedoo ZS","Coonabarabran ZS",93,9.3000000000000007,9.1140000000000008,11,0,93,10.140229099082919,9.9374245171012614,11,0,-1.2814950007868321E-2,10]
[null,"94M/4","Short Rural",132,"TransGrid 94M Mudgee Tee","Mudgee ZS",1.5,22.435216952573157,21.986512613521693,128,0,1.5,23.967814234195988,23.488457949512068,128,0,6.759661654045238E-4,9]
[null,"5B1:MTG","Short Rural",66,"Mt Gipps ZS","Sunset Strip ZS",84.669000000000011,6.1714303285444734,6.0480017219735842,19,0,84.669000000000011,4.7380170166709483,4.6432566763375291,19,0,1.0219050572141461E-2,9]
[null,"5B1:PPL","Long Rural",66,"Pinnacles Place ZS","Mt Gipps ZS",22.318000000000001,8.0537165787505387,7.8926422471755275,19,0,22.318000000000001,6.3558764857781016,6.2287589560625394,19,0,1.0219050572141427E-2,9]
[null,"5B1:SUN","Short Rural",66,"Sunset Strip ZS","Menindee ZS",15.065,1.8514290985633424,1.8144005165920756,6,0,15.065,1.7334208597576641,1.6987524425625109,19,0,1.0219050572141444E-2,9]
[null,"X4","Urban",220,"TransGrid Broken Hill 220/22kV STS","Perilya Mine",2.972,22.745572401437489,22.131441946598677,213,0,2.972,30.431166204634547,29.609524717109412,213,0,1.0582712111421817E-2,9]
[null,"83H/1","Short Rural",66,"Ellerslie ZS","Ginkgo Snapper Tee",80.5,11.1,10.878,45,0,100,13.189648306024957,12.925855339904457,20,0,0,9]
[null,"83H/2","Short Rural",66,"Ginkgo Snapper Tee","Ginkgo ZS",10,6.7,6.5659999999999998,20,0,3.6629999999999998,7.8414100659273203,7.6845818646087736,20,0,0,9]
[null,"83H/3","Short Rural",66,"Ginkgo Snapper Tee","Snapper ZS",10,5.0999999999999996,4.9979999999999993,12,0,9.1790000000000003,5.9528501204183426,5.833793118009976,20,0,0,9]
[null,"83U","Short Rural",66,"Powercor Mildura ZS (NSW Border)","Buronga ZS",4.8869999999999996,7.1208771186471473,6.9784595762742043,22,0,4.8869999999999996,13.529679324414454,13.259085737926165,22,0,-9.6569239925490286E-3,10]
[null,"83W","Short Rural",66,"Buronga ZS","Dareton ZS",14.542999999999999,0,0,22,0,14.542999999999999,5.3889400698938932,5.2811612684960156,22,0,0,9]
[null,"Merbein - Dareton Line","Short Rural",66,"Powercor Mildura ZS (NSW Border)","Dareton ZS",9.2609999999999992,24.93345300599163,24.434783945871796,49,0,8.9049999999999994,27.403333546907245,26.8552668759691,22,0,-3.6141036155919876E-2,10]
[null,893,"Short Rural",66,"Lismore 132/66kV STS","Casino ZS",21.698999999999998,9.2477643361040982E-9,9.062809049382016E-9,34,0,21.698999999999998,0,0,38,0,-1.0873469372749472E-2,10]
[null,8401,"Short Rural",33,"Casino ZS","Mallanganee ZS",36.438000000000002,3.2868232395424717,3.1553503099607725,4,0,36.438000000000002,3.4668417195153283,3.3281680507347149,4,0,1.1678321276460373E-3,9]
[null,8402,"Short Rural",33,"Mallanganee ZS","Bonalbo ZS",22.4,1.9720939437254832,1.8932101859764638,4,0,22.4,2.0223243363839414,1.9414313629285838,4,0,1.1678321276460543E-3,9]
[null,8403,"Short Rural",33,"Bonalbo ZS","Urbenville ZS",31.5,1.1000000000000001,1.056,4,0,31.5,1.2145949130400102,1.1660111165184097,4,0,-1.585376714364379E-3,10]
[null,"96L","Short Rural",132,"Transgrid Casino 132kV 96L Tee","Casino ZS",0.95,25.82503973926228,25.308538944477036,140,0,0.95,27.762169440914516,27.206926052096225,140,0,1.1678321276460681E-3,9]
[null,702,"Short Rural",66,"Boambee South 132/66kV STS","Sawtell ZS",3.5790000000000002,7.8,7.6440000000000001,61,0,3.5790000000000002,7.8892683403322197,7.7314829735255755,61,0,3.0991042422010458E-2,9]
[null,705,"Short Rural",66,"TransGrid Coffs Harbour 132/66 kV STS","South Coffs ZS",11.071999999999999,13.566017404699648,13.294697056605655,52,0,11.071999999999999,11.949921162562042,11.710922739310801,52,0,-1.8707203470403114E-2,10]
[null,706,"Short Rural",66,"TransGrid Coffs Harbour 132/66 kV STS","South Coffs ZS",10.004000000000001,15.404443655432869,15.096354782324212,52,0,10.004000000000001,13.574182291453969,13.30269864562489,52,0,-1.8707203470403076E-2,10]
[null,7501,"Short Rural",66,"Nana Glen ZS","Woolgoolga ZS",20.6,5.0709198006006391,4.9695014045886259,29,0,20.6,0,0,29,0,-1.8707203470403076E-2,10]
[null,7502,"Short Rural",66,"Nana Glen ZS","Ulong ZS",14.77,0.7,0.68599999999999994,9,0,14.77,0.69611191238225489,0.68218967413460974,9,0,-1.8707203470403118E-2,10]
[null,7503,"Short Rural",66,"Ulong ZS","Dorrigo ZS",20.86,0,0,9,0,20.86,0,0,9,0,0,9]
[null,7509,"Short Rural",66,"Moonee ZS","Woolgoolga ZS",9.4,10.4,10.192,30,0,9.4,11.078529518965592,10.85695892858628,30,0,3.1362576415898328E-3,9]
[null,7510,"Short Rural",66,"North Coffs ZS","Moonee ZS",11,15.3,14.994,61,0,11,16.040787532668929,15.71997178201555,61,0,-1.8707203470403076E-2,10]
[null,"703:NGN","Short Rural",66,"TransGrid Coffs Harbour 132/66 kV STS","Nana Glen ZS",12.629999999999999,8.2947004298484686,8.1288064212514985,62,0,12.629999999999999,3.5965782139749831,3.5246466496954834,62,0,-1.8707203470403073E-2,10]
[null,"711:CHN","Urban",66,"TransGrid Coffs Harbour 132/66 kV STS","North Coffs ZS",11.29,37.9,37.141999999999996,62,0,11.29,38.774853316379563,37.999356250051974,62,0,-1.8707203470403097E-2,10]
[null,"87C","Short Rural",66,"North Coffs ZS","South Coffs ZS",6.09,10.40322721978894,10.195162675393162,68,0,0,0,0,0,0,-1.8707203470403107E-2,10]
[null,"96C/2(D)","Short Rural",132,"TransGrid 96C Armidale Coffs Harbour Dorrigo Tee","Dorrigo ZS",2.1469999999999998,3.2,3.1360000000000001,122,0,2.1469999999999998,3.4805595619112739,3.4109483706730486,122,0,-1.1134236990467323E-2,10]
[null,"82D","Short Rural",66,"TransGrid Cooma 132/66/11kV STS","Jindabyne East ZS",51.1,15.5,15.19,20,0,51.1,10.248874410858807,10.043896922641631,20,0,-1.6756570047690399E-2,10]
[null,"82R","Urban",66,"Jindabyne East ZS","Jindabyne ZS",16.600000000000001,11.4,11.172000000000001,20,0,16.600000000000001,6.2890820248451771,6.1633003843482737,20,0,-1.6756570047690367E-2,10]
[null,"82J/1","Urban",66,"Snowy Adit 132/66/11kV ZS","Snowy Lookout Sw Stn",9.1999999999999993,0,0,12,0,9.1999999999999993,6.2890820248451771,6.1633003843482737,12,0,0,9]
[null,"82J/2","Urban",66,"Jindabyne ZS","Snowy Lookout Sw Stn",9.2000000000000011,0,0,12,0,9.2000000000000011,7.4537268442609506,7.304652307375731,12,0,0,9]
[null,"810/3","Urban",66,"Steeple Flat 132/66kV STS","Brown Mountain Hydro",9.1999999999999993,5.25,5.1449999999999996,70,0,9.1999999999999993,0,0,11,0,0,9]
[null,"810/4","Short Rural",66,"Steeple Flat 132/66kV STS","Bombala ZS",41.4,8.6999999999999993,8.5259999999999998,21,0,41.4,4.3504994005208184,4.2634894125104017,11,0,-1.5366795021426273E-2,10]
[null,"849/1","Short Rural",33,"Adaminaby ZS","Providence Portal ZS",9.859,2,1.92,7,0,9.859,0.58232240970788673,0.55902951331957129,7,0,-1.6756570047690371E-2,10]
[null,"849/2","Short Rural",33,"Providence Portal ZS","Cabramurra ZS",26.173000000000002,1.8,1.728,7,0,26.173000000000002,0.52409016873709813,0.50312656198761418,7,0,-1.6756570047690381E-2,10]
[null,"888/1","Short Rural",66,"TransGrid Cooma 132/66/11kV STS","Rhine Falls Sw Stn",24,3.5,3.4299999999999997,16,0,24,3.261005494364166,3.1957853844768827,16,0,-1.6756570047690402E-2,10]
[null,"888/3","Short Rural",66,"Rhine Falls Sw Stn","Adaminaby ZS",28.5,3.3,3.234,16,0,28.5,3.261005494364166,3.1957853844768827,16,0,-1.6756570047690406E-2,10]
[null,"888/4","Short Rural",66,"Rhine Falls Sw Stn","Eucumbene Tee",24.5,0.3,0.29399999999999998,15,0,24.5,1.4883287422834377,1.4585621674377689,15,0,-2.5852490928496199E-3,10]
[null,"888/6","Short Rural",66,"Eucumbene Tee","Eucumbene ZS",8,0.2,0.19600000000000001,15,0,8,0.2329289638831547,0.22827038460549159,15,0,-2.5852490928496038E-3,10]
[null,"888/7","Short Rural",66,"Eucumbene Tee","Snowy Adit 132/66/11kV ZS",19.3,0,0,20,0,19.3,0,0,20,0,0,9]
[null,865,"Short Rural",66,"TransGrid Cowra 132/66kV STS","Cowra Town ZS",3.9380000000000002,9.8173529020798398,9.6210058440382422,15,0,3.45,20.825570960374719,20.409059541167224,15,0,-1.3570332483347205E-3,10]
[null,"866:COW","Short Rural",66,"TransGrid Cowra 132/66kV STS","Cowra Town ZS",3.5539999999999998,8.7146792065563812,8.5403856224252532,15,0,3.93,0,0,15,0,-1.3570332483347392E-3,10]
[null,"863:CWD","Short Rural",66,"TransGrid Cowra 132/66kV STS","Canowindra ZS",36,5.5845087160381706,5.4728185417174071,9,0,36,6.5583289764715973,6.4271623969421654,9,0,-1.357033248334745E-3,10]
[null,"891/1","Urban",66,"TransGrid Cowra 132/66kV STS","Wyangala Dam Tee",16.968,2.0097117353895326,1.969517500681742,20,0,16.100000000000001,21.139195132152025,20.716411229508985,20,0,-1.357033248334724E-3,10]
[null,"891/2","Urban",66,"Wyangala Dam Tee","Wyangala Dam",28.695,0,0,19,0,29,22.896622216102596,22.438689771780545,19,0,0,9]
[null,"891:BMU/1","Long Rural",66,"Wyangala Dam Tee","Bendick Murrell Tee",30.2,2.3031652188756149,2.2571019144981026,19,0,30.2,2.4162264650158516,2.3679019357155346,19,0,-1.3570332483346919E-3,10]
[null,"891/7","Long Rural",66,"Bendick Murrell Tee","Bendick Murrell ZS",0.1,1.6717956028904075,1.6383596908325992,19,0,0.1,1.7,1.6659999999999999,19,0,-1.3570332483347162E-3,10]
[null,"891:BMU/2","Urban",66,"Bendick Murrell Tee","Monteagle Tee",12.75,0.72029491401129275,0.70588901573106688,19,0,12.75,0.8054088216719506,0.78930064523851162,19,0,-1.3570332483347285E-3,10]
[null,"891/5","Urban",66,"Monteagle Tee","Monteagle ZS",3.2480000000000002,0.80922021203737815,0.79303580779663052,13,0,3,0.8,0.78400000000000003,13,0,-1.3570332483347056E-3,10]
[null,"891/6","Short Rural",66,"Monteagle Tee","Young ZS",9.8460000000000001,0,0,19,0,10,0,0,19,0,0,9]
[null,"893/1","Short Rural",66,"TransGrid Cowra 132/66kV STS","Grenfell Tee",8.9359999999999999,4.1972740668312358,4.1133285854946111,12,0,8.5299999999999994,4.7173945269357107,4.623046636396996,12,0,-1.3570332483347546E-3,10]
[null,"893/4","Short Rural",66,"Grenfell Tee","Payten'sBridge ZS",35.5,0,0,12,0,35.5,0,0,12,0,0,9]
[null,"893/6","Short Rural",66,"Grenfell Tee","Grenfell ZS",47.1,4.286199364857322,4.2004753775601751,12,0,47.1,4.8222255164231704,4.7257810060947065,12,0,-1.3570332483347175E-3,10]
[null,"CLY1526","Short Rural",33,"Coleambally 132/33kV STS","Coleambally Tee",10,3.8630578644607194,3.7085355498822903,8,0,10,5.1699118529719623,4.9631153788530833,8,0,1.4847666646090971E-2,9]
[null,"CLY1530","Short Rural",33,"Coleambally 132/33kV STS","Ringwood Rd ZS",7.83,5.7685554094642546,5.5378131930856842,8,0,11,4.3082598774766359,4.1359294823775699,8,0,1.4847666646090944E-2,9]
[null,"99N","Long Rural",132,"TransGrid Darlington Point 330/132kV STS","Hillston ZS",163.03700000000001,11.023452268006414,10.802983222646287,128,0,163.03700000000001,13.676711731828329,13.403177497191761,128,0,3.8260619188908245E-3,9]
[null,"99R","Long Rural",132,"TransGrid Darlington Point 330/132kV STS","Hay 132 ZS",116.41500000000001,8.3646867280955846,8.197392993533672,128,0,116.41500000000001,17.38565050656144,17.03793749643021,128,0,3.8260619188908111E-3,9]
[null,"HAT 22","Short Rural",33,"Hay 132 ZS","Hay ZS",2.6,5.7474355703138302,5.517538147501277,8,0,2.6,3.4771301013122877,3.3380448972597963,8,0,3.8260619188908193E-3,9]
[null,"HAT 32","Short Rural",33,"Hay 132 ZS","Hay ZS",2.4499999999999997,1.0147960075995528,0.97420416729557069,8,0,2.4499999999999997,3.3032735962466733,3.171142652396806,8,0,3.8260619188908362E-3,9]
[null,"HAT 42","Short Rural",33,"Hay 132 ZS","Carrathool ZS",54.79,1.8543090684319095,1.7801367056946331,7,0,54.79,1.4488042088801196,1.3908520405249147,7,0,3.8260619188908171E-3,9]
[null,"HIL1117","Long Rural",33,"Hillston ZS","Ivanhoe ZS",160,3.053613441049563,2.9314689034075805,8,0,160,1.5647085455905294,1.5021202037669081,8,0,1.4373665554521534E-2,9]
[null,844,"Short Rural",66,"TransGrid Deniliquin 132/66kV STS","Barham ZS",174.56200000000001,5.6431156508256937,5.5302533378091798,11,0,86.9,6.4349484156553993,6.3062494473422914,11,0,-7.1896890590118605E-4,10]
[null,845,"Long Rural",66,"TransGrid Deniliquin 132/66kV STS","Deniliquin ZS",5.2679999999999998,21.463057514053759,21.033796363772684,38,0,5.6,24.01614676557104,23.53582383025962,38,0,-7.1896890590113997E-4,10]
[null,"822/1","Short Rural",66,"TransGrid Deniliquin 132/66kV STS","Murgha ZS",74.23099999999998,7.3552683869895255,7.208163019249735,11,0,95.699999999999989,8.2735051058426539,8.1080350037258011,11,0,-7.1896890590114366E-4,10]
[null,"822/2","Long Rural",66,"Murgha ZS","Moulamein ZS",35.317,6.1759795125909678,6.052459922339148,11,0,15,6.8766795684925954,6.7391459771227433,11,0,-7.1896890590114593E-4,10]
[null,"84Y","Short Rural",66,"TransGrid Deniliquin 132/66kV STS","Moama ZS",70.02300000000001,8.3074349596520651,8.1412862604590241,66,0,0,9.3076932440729845,9.1215393791915247,20,0,-7.189689059011726E-4,10]
[null,"MM61","Short Rural",66,"Moulamein ZS","Koraleigh ZS",56.75,4.0969369043920283,4.0149981663041876,15,0,56,4.7113015186048441,4.6170754882327474,34,0,-7.1896890590111959E-4,10]
[null,"No.6 Moama","Short Rural",66,"TransGrid Deniliquin 132/66kV STS","Moama ZS",69,5.7916186942684744,5.6757863203831045,34,0,69,6.5498582087921013,6.4188610446162588,34,0,-7.1896890590116968E-4,10]
[null,"81X","Urban",66,"Dubbo 132/66kV STS","Yarrandale ZS",4.33,10.983483322070887,10.76381365562947,28,0,4.33,14.425739473395494,14.137224683927583,15,0,-2.1768204034273604E-3,10]
[null,"81P","Urban",66,"Dubbo 132/66kV STS","Yarrandale ZS",5.57,10.034415456257383,9.8337271471322349,61,0,5.57,13.137727020413754,12.874972480005479,61,0,3.8720804815331228E-4,9]
[null,"81T","Short Rural",66,"Yarrandale ZS","Gilgandra ZS",59.17,5.8822435433232938,5.7645986724568274,43,0,59.17,0,0,43,0,-2.1768204034273253E-3,10]
[null,812,"Short Rural",66,"Yarrandale ZS","Gilgandra ZS",59.2,5.8822435433232938,5.7645986724568274,15,0,59.2,16.329616704315562,16.003024370229252,15,0,-2.1768204034273253E-3,10]
[null,815,"Urban",66,"Dubbo 132/66kV STS","Phillip St ZS",1.4,12.19599555871112,11.952075647536898,24,0,1.4,15.518926513321174,15.20854798305475,27,0,1.3644799465601033E-2,9]
[null,816,"Urban",66,"Dubbo 132/66kV STS","Phillip St ZS",1.38,12.19599555871112,11.952075647536898,24,0,1.38,15.634739397748943,15.322044609793963,27,0,1.3644799465601033E-2,9]
[null,"813:EUL","Short Rural",66,"Eulomogo ZS","Geurie ZS",29.96,1.1985809089157571,1.1746092907374419,12,0,29.96,1.3897546131332392,1.3619595208705744,12,0,-6.6954922016748018E-3,10]
[null,"814/1","Long Rural",66,"Gilgandra ZS","Gulargambone ZS",48,6.891797607507943,6.7539616553577844,11,0,48,7.8752761410883565,7.7177706182665888,11,0,1.5994124217035135E-2,9]
[null,"814/2","Short Rural",66,"Gulargambone ZS","Coonamble ZS",44.5,5.4922300904508425,5.3823854886418259,11,0,44.5,6.4855215279551173,6.3558110973960149,11,0,3.6268365886519042E-4,9]
[null,"81M","Short Rural",66,"Dubbo 132/66kV STS","Eulomogo ZS",2.14,9.3918174221128208,9.2039810736705636,20,0,2.14,12.623604402626924,12.371132314574385,20,0,-2.1768204034273283E-3,10]
[null,"81R","Short Rural",66,"Dubbo 132/66kV STS","Eulomogo ZS",2.0499999999999998,9.8070346134062287,9.6108939211381035,20,0,2.0499999999999998,12.044539980488075,11.803649180878313,20,0,-2.176820403427317E-3,10]
[null,"943/1","Urban",132,"94F Tee","Dubbo South ZS",3.3679999999999999,39.514836038089413,38.724539317327626,106,0,3.3679999999999999,80.837393330583438,79.220645463971763,106,0,-2.1768204034273131E-3,10]
[null,"943/2","Short Rural",132,"Dubbo South ZS","Narromine South Sw Stn",31.6,25.209615185671257,24.705422881957833,106,0,31.6,64.855215279551174,63.558110973960147,106,0,-2.1768204034273253E-3,10]
[null,"94W/1","Short Rural",132,"Dubbo 132/66kV STS","Nevertire Tee",113.4,37.438750081622366,36.689975079989921,128,0,113.4,42.850767238274877,41.993751893509376,128,0,-2.176820403427327E-3,10]
[null,"94W/2","Short Rural",132,"Nevertire Tee","Nevertire ZS",0.46,8,7.84,124,0,0.46,8,7.84,124,0,8.5943289413758905E-3,9]
[null,"94W/3","Short Rural",132,"Nevertire Tee","Nyngan 132/66kV STS",60,30.291082717214405,29.685261062870115,128,0,60,35.670368403753145,34.956961035678084,128,0,-2.1768204034273235E-3,10]
[null,"9GW","Short Rural",132,"Dubbo 132/66kV STS","Dubbo West ZS",5.5,34.34439339412625,33.657505526243725,140,0,0,0,0,0,0,-2.1768204034273097E-3,10]
[null,"808D","Short Rural",66,"Dubbo 132/66kV STS","West Dubbo ZS",0,0,0,0,0,5.5,14.129171900187934,13.846588462184176,12,0,0,9]
[null,"9GP","Short Rural",132,"Narromine South Sw Stn","Narromine ZS",3.75,12,11.76,124,0,3.75,9.7282822919326737,9.5337166460940193,124,0,8.5982840078568309E-3,9]
[null,"9GR","Short Rural",132,"Narromine South Sw Stn","Narromine ZS",3.75,0,0,124,0,3.75,0,0,124,0,0,9]
[null,"9GT","Short Rural",132,"Dubbo West ZS","Narromine South Sw Stn",32.128,24.240775072653303,23.755959571200236,140,0,31,14.824049206754555,14.527568222619465,24,0,-2.1768204034273231E-3,10]
[null,"9GU","Short Rural",132,"Narromine South Sw Stn","Nyngan 132/66kV STS",133.80000000000001,37.339888845600136,36.593091068688132,106,0,133.80000000000001,32.427607639775587,31.779055486980074,106,0,-2.1768204034273179E-3,10]
[null,811,"Short Rural",66,"Nyngan 132/66kV STS","Cobar Town ZS",132,7.4,7.2519999999999998,10,0,132,9.7282822919326737,9.5337166460940193,10,0,-4.2924568468409264E-3,10]
[null,854,"Long Rural",66,"Nyngan 132/66kV STS","Nyngan Town ZS",3.54,5.9400593999712434,5.8212582119718181,15,0,3.54,5.9064571058162683,5.7883279636999427,15,0,7.0226221760005154E-3,9]
[null,"820/1:NYN","Short Rural",66,"Nyngan Town ZS","Nevertire Tee",4.8,0,0,15,0,4.8,0.11581288442776996,0.11349662673921457,15,0,0,9]
[null,"820:NVE","Short Rural",66,"Nyngan 132/66kV STS","Nevertire ZS",58.01,0,0,11,0,58.01,0.11581288442776996,0.11349662673921457,11,0,0,9]
[null,"855/1","Short Rural",66,"Nyngan 132/66kV STS","Girilambone Tee",47.3,15.8,15.484,28,0,47.3,12.971043055910235,12.71162219479203,28,0,2.0727527241097287E-2,9]
[null,"855/1a","Short Rural",66,"Girilambone Tee","Girilambone ZS",1.67,11.4,11.172000000000001,24,0,1.67,9.750045786992926,9.5550448712530667,24,0,4.5770594034448074E-2,9]
[null,"855/4","Urban",66,"Girilambone ZS","Tritton Mine ZS",23.8,10.6,10.388,24,0,23.8,6.948773065666197,6.8097976043528732,24,0,4.5958439094111611E-2,9]
[null,"855/2","Short Rural",66,"Girilambone Tee","Byrock ZS",82.7,8.4,8.2319999999999993,28,0,82.7,6.4855215279551173,6.3558110973960149,38,0,-1.0013864511084034E-2,10]
[null,"855/3","Short Rural",66,"Byrock ZS","Bourke ZS",78.400000000000006,8,7.84,28,0,78.400000000000006,6.7171472968106576,6.5828043508744445,38,0,-1.0766620513890313E-2,10]
[null,"946/1","Urban",132,"Nyngan 132/66kV STS","Scrubby Valley Sw Stn",118,39.9,39.101999999999997,106,0,118,37.986626092308541,37.226893570462366,106,0,1.5977740457964653E-2,9]
[null,"9UT","Urban",132,"Nyngan 132/66kV STS","Nyngan Solar Farm",3.4,57.897991184281707,56.74003136059607,106,0,0,0,0,106,0,-1.4062180583901802E-2,10]
[null,"9UW","Urban",132,"Nyngan Solar Farm","Scrubby Valley Sw Stn",118,35.36451624193451,34.657225917095822,106,0,118,0,0,106,0,1.5977740457964653E-2,9]
[null,"946/2","Long Rural",132,"Scrubby Valley Sw Stn","Cobar CSA ZS",20.3,27.5,26.95,106,0,20.3,26.636963418387086,26.104224150019345,106,0,1.6316193927924209E-2,9]
[null,"946/3","Urban",132,"Scrubby Valley Sw Stn","Cobar Peak ZS",9.5,17.847401413772044,17.490453385496604,102,0,9.5,12.739417287054694,12.4846289413136,102,0,3.6270776588858168E-2,9]
[null,"94R","Urban",132,"Cobar CSA ZS","Cobar Elura ZS",32.6,11.8,11.564,128,0,32.6,12.971043055910235,12.71162219479203,128,0,-1.7226265897921738E-2,10]
[null,"84A","Long Rural",66,"TransGrid Finley 132/66kV STS","Jerilderie ZS",43.018999999999998,5.4,5.2919999999999998,15,0,43.018999999999998,6.8863568827646446,6.7486297451093513,15,0,1.3141778756849037E-4,9]
[null,"84B","Long Rural",66,"TransGrid Finley 132/66kV STS","Finley ZS",5.7880000000000003,9.4703555099828183,9.2809483997831617,61,0,5.7880000000000003,8.6208065807020038,8.4483904490879631,61,0,3.0898434456477996E-3,9]
[null,"84C","Long Rural",66,"TransGrid Finley 132/66kV STS","Finley ZS",10.903,6.9126682554619112,6.7744148903526726,61,0,10.903,8.6208065807020038,8.4483904490879631,61,0,3.0898434456477718E-3,9]
[null,"9R4","Urban",132,"TransGrid Finley 132/66kV STS","Mulwala ZS",62.945999999999998,15.948513189387121,15.629542925599379,140,0,62.945999999999998,28.506133760187964,27.936011084984205,22,0,3.0898434456477844E-3,9]
[null,858,"Short Rural",66,"TransGrid Forbes 132/66kV STS","Forbes Town ZS",0.85,16.336340852130327,16.009614035087719,28,0,0.85,13.710434761051696,13.436226065830661,15,0,-4.5607094284584853E-3,10]
[null,859,"Short Rural",66,"TransGrid Forbes 132/66kV STS","Forbes Town ZS",0.85,0,0,28,0,0.85,0,0,15,0,0,9]
[null,"893/5","Short Rural",66,"TransGrid Forbes 132/66kV STS","Payten's Bridge ZS",49.6,2.6883890053001358,2.6346212251941332,12,0,49.6,3.8342741280907293,3.7575886455289145,12,0,-4.560709428458461E-3,10]
[null,"896:WJL","Short Rural",66,"TransGrid Forbes 132/66kV STS","West Jemalong ZS",36.6,5.4076790336496989,5.2995254529767051,11,0,36.6,10.340921133335602,10.134102710668889,16,0,-4.5607094284584463E-3,10]
[null,"89H","Short Rural",66,"TransGrid Forbes 132/66kV STS","West Jemalong ZS",36.6,9.7750236246353595,9.5795231521426523,43,0,36.6,5.693316129589264,5.5794498069974789,20,0,-4.5607094284584836E-3,10]
[null,"894:CDN","Short Rural",66,"Condobolin ZS","Lake Cargelligo ZS",88.9,3.8626278811783563,3.7853753235547893,15,0,88.9,4.066654378278046,3.9853212907124851,15,0,-4.5607094284584844E-3,10]
[null,"897:CDN","Long Rural",66,"West Jemalong ZS","Condobolin ZS",63.6,12.28830683265541,12.042540696002302,20,0,63.6,13.361864385770721,13.094627098055307,16,0,-4.5607094284585148E-3,10]
[null,886,"Short Rural",66,"TransGrid Glen Innes 132/66kV STS","Glen Innes ZS",3.0139999999999998,5.6,5.4879999999999995,70,0,13.05,6.7951903885082574,6.6592865807380921,70,0,-1.6543376130408185E-3,10]
[null,887,"Short Rural",66,"TransGrid Glen Innes 132/66kV STS","Glen Innes ZS",9.3000000000000007,6.6,6.468,19,0,9.3000000000000007,8.1772630098997663,8.0137177497017706,19,0,-1.6543376130407886E-3,10]
[null,"6AE/E","Short Rural",66,"Emmaville ZS","Pindari ZS",36.700000000000003,0.3,0.29399999999999998,17,0,36.700000000000003,0.23089415059442284,0.22627626758253438,17,0,-1.6543376130408048E-3,10]
[null,"6AE/A","Short Rural",66,"Pindari ZS","Ashford ZS",20.6,0,0,17,0,20.6,0,0,17,0,0,9]
[null,"6NE","Short Rural",66,"Glen Innes ZS","Emmaville ZS",39,1,0.98,17,0,39,1.4972453398408025,1.4673004330439865,17,0,-1.6543376130408189E-3,10]
[null,"6NY","Long Rural",66,"Glen Innes ZS","Guyra ZS",53.2,5.4,5.2919999999999998,11,0,53.2,5.873808640913917,5.7563324680956383,11,0,3.0897456440010233E-2,9]
[null,972,"Short Rural",132,"TransGrid Marulan 330/132kV STS","Goulburn 132/66/33kV STS",35.177,49.9,48.902000000000001,180,0,35.177,77.408321403798269,75.860154975722295,180,0,-2.1280522614536002E-3,10]
[null,"9UR","Urban",132,"TransGrid Marulan 330/132kV STS","Taralga Wind Farm",37,102,99.96,140,0,0,0,0,0,0,0,9]
[null,"860/1","Short Rural",66,"Goulburn 132/66/33kV STS","Marulan North Tee",7.29,5.9,5.782,25,0,7.29,12.357352513256952,12.110205462991813,12,0,-2.1280522614536166E-3,10]
[null,"86L","Short Rural",66,"Marulan North Tee","Marulan North ZS",16.39,2.1,2.0579999999999998,12,0,16.39,8.626830999820891,8.4542943798244732,12,0,-2.128052261453601E-3,10]
[null,"840:GOU","Short Rural",66,"Goulburn 132/66/33kV STS","Goulburn North ZS",6.8,13.3,13.034000000000001,61,0,6.8,5.3626246755643381,5.2553721820530512,9,0,-2.1280522614535941E-3,10]
[null,"841:GBN","Long Rural",66,"Goulburn North ZS","Crookwell ZS",42,6.1,5.9779999999999998,9,0,42,5.9455186620387224,5.8266082887979476,9,0,-2.1280522614535915E-3,10]
[null,843,"Short Rural",66,"Clinton St ZS","Goulburn North ZS",10.6,0,0,46,0,5.3,9.6760401754747836,9.4825193719652869,46,0,0,9]
[null,"850/2","Urban",66,"Clinton St Tee","Clinton St ZS",1.9,0,0,17,0,1.9,0,0,17,0,0,9]
[null,"870:GOU","Urban",66,"Goulburn 132/66/33kV STS","Clinton St ZS",1.9,18.495695844540172,18.125781927649367,34,0,1.9,16.321031621282767,15.994610988857112,17,0,-2.1280522614535789E-3,10]
[null,"850:GOU","Short Rural",66,"Goulburn 132/66/33kV STS","Woodlawn ZS",37.6,4.9175978366243172,4.819245879891831,15,0,37.6,9.7926189727696595,9.5967665933142658,15,0,-2.1280522614535993E-3,10]
[null,"GOU12","Long Rural",33,"Goulburn 132/66/33kV STS","Brisbane Grove ZS",2.931,2.2999999999999998,2.2079999999999997,7,0,2.931,1.3406561688910845,1.2870299221354411,7,0,-2.1280522614535841E-3,10]
[null,825,"Short Rural",66,"TransGrid Koolkhan 132/66kV STS","Koolkhan ZS",0.52700000000000002,17.877452441137244,17.5199033923145,62,0,0.52700000000000002,19.735585498198883,19.340873788234905,62,0,-2.6008843727167623E-3,10]
[null,826,"Urban",66,"TransGrid Koolkhan 132/66kV STS","Grafton North ZS",7.0739999999999998,14.611379399006401,14.319151811026272,61,0,7.0739999999999998,15.696138174006128,15.382215410526005,61,0,-2.6008843727167805E-3,10]
[null,6501,"Long Rural",66,"Casino ZS","Rappville Tee",84.558999999999997,1.0330015895704914,1.0123415577790815,16,0,84.558999999999997,0.69247668414732921,0.6786271504643826,16,0,1.1678321276460465E-3,9]
[null,6503,"Short Rural",66,"Grafton North ZS","South Grafton ZS",8.8219999999999992,9.5403712546453541,9.3495638295524461,24,0,8.8219999999999992,10.156324700827495,9.9531982068109457,14,0,-2.6008843727167528E-3,10]
[null,6504,"Short Rural",66,"Five Mile Sw Stn","South Grafton ZS",4.8,4.1255659479547475,4.0430546289956526,61,0,4.8,5.3089879117961907,5.2028081535602668,61,0,-2.6008843727167567E-3,10]
[null,6505,"Urban",66,"Koolkhan SS","Grafton ZS",6.0554999999999994,15.90061875774226,15.582606382587414,52,0,6.0554999999999994,17.888981007139339,17.531201386996553,52,0,-2.6008843727167619E-3,10]
[null,6506,"Short Rural",66,"Shannon Creek ZS","Nymboida ZS",12.5,0.4,0.39200000000000002,14,0,12.5,0.5770639034561077,0.5655226253869855,14,0,-6.1033858656492383E-3,10]
[null,6508,"Short Rural",66,"Maclean ZS","Yamba ZS",18.283000000000001,10.7,10.485999999999999,28,0,18.283000000000001,11.036827278081917,10.816090732520278,28,0,5.9636603850761949E-3,9]
[null,6509,"Short Rural",66,"Shannon Creek ZS","Five Mile Sw Stn",16.3,1.1173407775710777,1.0949939620196563,14,0,16.3,0.5770639034561077,0.5655226253869855,14,0,-2.6008843727167623E-3,10]
[null,6510,"Short Rural",66,"Grafton North ZS","Five Mile Sw Stn",11.8,5.1569574349434353,5.0538182862445664,28,0,11.8,5.5398134731786337,5.4290172037150608,15,0,-2.6008843727167727E-3,10]
[null,"896:MLN","Short Rural",66,"TransGrid Koolkhan 132/66kV STS","Maclean ZS",36.202999999999996,8.4917899095401914,8.3219541113493882,21,0,36.143000000000001,7.2429179012412588,7.0980595432164337,21,0,-2.6008843727167892E-3,10]
[null,"8G1","Short Rural",66,"TransGrid Koolkhan 132/66kV STS","Maclean ZS",40.339999999999996,10.898370045847127,10.680402644930185,68,0,37,12.991265441908924,12.731440133070745,70,0,-2.6008843727167901E-3,10]
[null,6404,"Short Rural",33,"Yamba Tee","Yamba ZS",17.29,0,0,10,0,19.493000000000002,0,0,14,0,0,9]
[null,6402,"Short Rural",33,"Maclean ZS","Yamba Tee",15.546000000000001,0.4297464529119529,0.4125565947954748,8,0,15.247,0.40394473241927542,0.38778694312250439,3,0,-2.6008843727167727E-3,10]
[null,6403,"Short Rural",33,"Yamba Tee","Redcliff ZS",3.14,0.4297464529119529,0.4125565947954748,3,0,2.7229999999999999,0,0,3,0,-2.6008843727167727E-3,10]
[null,"79C/1","Short Rural",33,"TransGrid Griffith 132/33kV STS","Widgelli / Willbriggie Tee",11.6,5.8395453302487335,5.6059635170387843,10,0,11.6,0.51786569774993785,0.49715106983994034,10,0,5.7977379352004681E-3,9]
[null,"79C/2","Short Rural",33,"Widgelli / Willbriggie Tee","Widgelli ZS",13.1,1.1006472873767246,1.0566213958816555,10,0,13.1,0.51786569774993785,0.49715106983994034,10,0,5.7977379352004465E-3,9]
[null,"79G","Urban",33,"Beelbangera ZS","Griffith ZS",5.2190000000000003,0,0,10,0,5.2190000000000003,0,0,10,0,0,9]
[null,"79F","Short Rural",33,"TransGrid Griffith 132/33kV STS","Yenda ZS",5.0389999999999997,11.403928838653284,10.947771685107153,22,0,5.0389999999999997,7.250119768499129,6.9601149777591633,10,0,5.7977379352004907E-3,9]
[null,"79J","Urban",33,"TransGrid Griffith 132/33kV STS","Griffith ZS",5.7,0,0,51,0,5.7,13.234345609165079,12.704971784798476,51,0,0,9]
[null,"79L","Short Rural",33,"TransGrid Griffith 132/33kV STS","Beelbangera ZS",7.8,12.718590876353263,12.209847241299132,22,0,7.8,11.335504717415306,10.882084528718693,10,0,5.7977379352004369E-3,9]
[null,"79M","Urban",33,"TransGrid Griffith 132/33kV STS","Hanwood ZS",9.5,10.395002158557954,9.9792020722156352,22,0,9.5,12.141073580581876,11.655430637358601,10,0,5.797737935200456E-3,9]
[null,"79P/1","Short Rural",33,"TransGrid Griffith 132/33kV STS","Warrawidgee Tee",16.96,8.9988106921634046,8.6388582644768679,20,0,14.959999999999999,8.1999999999999993,7.871999999999999,10,0,5.7977379352004699E-3,9]
[null,"79P/2","Short Rural",33,"Warrawidgee Tee","Warrawidgee ZS",18.7,2.0891916102984123,2.0056239458864757,6,0,18.7,1.9,1.8239999999999998,6,0,5.7977379352004638E-3,9]
[null,"79P/3","Short Rural",33,"Warrawidgee Tee","Nericon Tee",13.1,6.2777660094820584,6.0266553691027758,21,0,13.1,5.7,5.4719999999999995,6,0,5.7977379352004725E-3,9]
[null,"79P/4","Short Rural",33,"Nericon Tee","Nericon ZS",1.5,2.7720005756154547,2.6611205525908366,6,0,1.5,2.5,2.4,6,0,5.7977379352004473E-3,9]
[null,"79R","Short Rural",33,"TransGrid Griffith 132/33kV STS","Tharbogang ZS",16.183,16.45875341771676,15.800403281008089,31,0,16.183,16.053836630248075,15.41168316503815,10,0,5.7977379352004569E-3,9]
[null,"79U","Urban",33,"TransGrid Griffith 132/33kV STS","Griffith ZS",5.8,27.720005756154542,26.61120552590836,51,0,5.8,13.234345609165079,12.704971784798476,51,0,5.7977379352004569E-3,9]
[null,877,"Urban",66,"TransGrid Gunnedah 132/66kV STS","Keepit Dam ZS",18.400000000000002,0.21301682467646504,0.20875648818293574,10,0,18.400000000000002,0.34596398522574573,0.33904470552123078,10,0,1.1815631557005622E-4,9]
[null,"88K","Short Rural",66,"TransGrid Gunnedah 132/66kV STS","Gunnedah ZS",12.94,12.816512284700648,12.560182039006635,61,0,12.94,14.761130036298482,14.465907435572513,61,0,1.1815631557006201E-4,9]
[null,"88L","Short Rural",66,"TransGrid Gunnedah 132/66kV STS","Gunnedah ZS",11.85,13.029529109377114,12.768938527189571,61,0,11.85,15.10709402152423,14.804952141093745,61,0,1.1815631557006965E-4,9]
[null,"878/1","Short Rural",66,"Gunnedah ZS","Boggabri ZS",21.3,4.5999999999999996,4.508,24,0,21.3,5.2800661274114056,5.1744648048631774,14,0,5.2176691715817331E-4,9]
[null,"878/2","Short Rural",66,"Narrabri Coal Tee","Boggabri ZS",20.9,0,0,24,0,20.9,0,0,14,0,0,9]
[null,"878/3","Urban",66,"TransGrid Narrabri 132/66kV STS","Narrabri Coal Tee",25,11.987324107653185,11.747577625500121,61,0,25,0,0,61,0,-3.1832087216709121E-3,10]
[null,879,"Short Rural",66,"TransGrid Narrabri 132/66kV STS","Wee Waa ZS",43.767999999999994,4.4000000000000004,4.3120000000000003,18,0,43.8,3.8157893354621923,3.7394735487529482,10,0,-3.1832087216709061E-3,10]
[null,882,"Short Rural",66,"TransGrid Narrabri 132/66kV STS","Wee Waa ZS",41,11,10.78,64,0,41,9.7129183084492166,9.518659942280232,64,0,-3.1832087216709282E-3,10]
[null,885,"Urban",66,"Burren Junction ZS","Merrywinebone ZS",58.6,3.1,3.0379999999999998,15,0,58.6,1.9762952593778789,1.9367693541903213,15,0,-3.1832087216709212E-3,10]
[null,"833:NBI","Short Rural",66,"TransGrid Narrabri 132/66kV STS","Narrabri ZS",0.2,11,10.78,38,0,0.2,10.406698187624158,10.198564223871674,38,0,-3.1832087216709217E-3,10]
[null,"834:NBI","Short Rural",66,"TransGrid Narrabri 132/66kV STS","Narrabri ZS",0.2,11,10.78,38,0,0.2,10.406698187624158,10.198564223871674,38,0,-3.1832087216709217E-3,10]
[null,"861/1","Urban",66,"TransGrid Narrabri 132/66kV STS","Wilga Park ZS",18,12.1,11.857999999999999,64,0,18,11.747977375190727,11.513017827686912,64,0,-1.262103075064888E-3,10]
[null,"861/2","Long Rural",66,"Wilga Park ZS","Walgett ZS",165.6,13.131568681565536,12.868937307934225,64,0,165.6,12.372407845286503,12.124959688380773,64,0,-1.2621030750649131E-3,10]
[null,"880/1","Long Rural",66,"Wee Waa ZS","Burren Junction ZS",56,5.3,5.194,10,0,56,4.1626792750496646,4.0794256895486711,10,0,-3.1832087216709212E-3,10]
[null,"880/2","Long Rural",66,"Burren Junction ZS","Walgett ZS",84,0,0,10,0,49.6,0,0,10,0,0,9]
[null,"890:BRE","Short Rural",66,"Walgett ZS","Brewarrina ZS",130,3.4,3.3319999999999999,15,0,130,3.2376394361497387,3.1728866474267439,15,0,-1.2621030750649073E-3,10]
[null,"895:LGR","Short Rural",66,"Walgett ZS","Lightning Ridge ZS",76.099999999999994,3.2,3.1360000000000001,15,0,76.099999999999994,3.9314193153246828,3.8527909290181892,15,0,-1.2621030750649101E-3,10]
[null,836,"Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Cootamundra ZS",34.002000000000002,10.150638143793882,9.9476253809180051,12,0,34.002000000000002,10.534891424814273,10.324193596317986,12,0,6.5867451729699072E-3,9]
[null,837,"Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Jugiong ZS",31.381,2.0585546398958816,2.017383547097964,12,0,31.381,2.2901937880031022,2.2443899122430402,12,0,-1.1453880560106504E-2,10]
[null,847,"Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Boorowa ZS",39.503,4.652248576850095,4.5592036053130931,10,0,39.503,4.8094069548065157,4.7132188157103849,10,0,-1.07404962653782E-3,10]
[null,"83A","Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Murrumburrah ZS",1.577,4.5662311735026329,4.4749065500325802,15,0,1.577,2.9772519244040332,2.9177068859159525,15,0,9.9852407670987763E-3,9]
[null,"83D","Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Murrumburrah ZS",1.54,2.0676660341555977E-2,2.0263127134724859E-2,15,0,1.54,2.9772519244040332,2.9177068859159525,15,0,6.0159689824425665E-3,9]
[null,"890:YOU","Short Rural",66,"TransGrid Murrumburrah 132/66kV STS","Young ZS",28.075000000000003,16.794970950468944,16.459071531459564,24,0,28.075000000000003,18.436059993424973,18.067338793556473,27,0,9.4695004657811294E-3,9]
[null,"838/3","Long Rural",66,"Jugiong ZS","Bogalara Sw Stn",18.707000000000001,0,0,12,0,18.707000000000001,0,0,12,0,0,9]
[null,"7Y1","Short Rural",33,"Hawks Nest 132/33kV STS","Tea Gardens ZS",10.65,4.1866851151583422,4.0192177105520086,7,0,10.65,3.591262550046554,3.4476120480446917,7,0,1.6170822680608911E-2,9]
[null,"7Y2","Short Rural",33,"Hawks Nest 132/33kV STS","Tea Gardens ZS",7.3113000000000001,3.8400169209095627,3.6864162440731802,7,0,7.3113000000000001,5.5027410041035907,5.2826313639394469,7,0,1.6170822680608977E-2,9]
[null,"866:KEW","Short Rural",66,"Herons Creek 132/66kV STS","Kew ZS",4.4000000000000004,10.4,10.192,16,0,20.7,12.919829777632037,12.661433182079396,16,0,0,9]
[null,871,"Short Rural",66,"Kew ZS","Laurieton ZS",7.9560000000000004,7.2,7.056,36,0,7.9560000000000004,8.081295270804798,7.9196693653887023,36,0,5.0667089657932662E-3,9]
[null,"862/1","Short Rural",66,"Kew ZS","Johns River ZS",12.420999999999999,1.1000000000000001,1.0780000000000001,16,0,12.420999999999999,11.892942806535984,11.655083950405265,16,0,5.5533172261760876E-2,9]
[null,"862/2","Short Rural",66,"TransGrid Taree 132/66/33kV STS","Johns River ZS",32.35,0,0,16,0,32.35,12.892942806535984,12.635083950405264,16,0,0,9]
[null,861,"Urban",66,"TransGrid Taree 132/66/33kV STS","Whitbread ZS",0.68899999999999995,9.8920483213373451,9.6942073549105974,62,0,0.68899999999999995,11.297054748333005,11.071113653366345,62,0,-1.9868344280596991E-3,10]
[null,867,"Short Rural",66,"TransGrid Taree 132/66/33kV STS","Failford Tee",30.298000000000002,14.2,13.915999999999999,34,0,30.298000000000002,15.655716265079411,15.342601939777822,34,0,-1.4692569264428005E-2,10]
[null,868,"Short Rural",66,"TransGrid Taree 132/66/33kV STS","Bohnock Tee",11.936,20.5,20.09,36,0,11.936,21.066147621393618,20.644824668965747,36,0,-1.4692569264428013E-2,10]
[null,872,"Urban",66,"Tuncurry ZS","Forster ZS",5.2849999999999993,8.1,7.9379999999999997,30,0,5.2849999999999993,8.9790137402661312,8.7994334654608082,30,0,-1.4692569264428012E-2,10]
[null,"1a","Urban",33,"TransGrid Taree 132/66/33kV STS","Bootawa ZS",10.343,5.4698176742641573,5.2510249672935911,17,0,10.343,7.6866558081441063,7.3791895758183417,17,0,-3.6311791687229904E-3,10]
[null,"3a","Short Rural",33,"TransGrid Taree 132/66/33kV STS","Wingham ZS",13.052,5.7478261964630972,5.5179131486045732,18,0,13.052,8.0360492539688373,7.7146072838100839,18,0,-3.6311791687229831E-3,10]
[null,"7G2/1","Short Rural",33,"TransGrid Taree 132/66/33kV STS","Kanangra Tee",3.1819999999999999,5.2,4.992,22,0,3.1819999999999999,5.9979208199912346,5.7580039871915849,31,0,-3.6311791687229878E-3,10]
[null,"7G2/2","Short Rural",33,"Kanangra Tee","Coopernook ZS",15.58,4.7,4.5119999999999996,7,0,15.58,5.0458698961831026,4.8440351003357787,7,0,-3.6311791687229813E-3,10]
[null,"7G2/3","Short Rural",33,"Coopernook ZS","Harrington ZS",13.5,2.7,2.5920000000000001,8,0,13.5,2.9513578638052107,2.8333035492530021,8,0,9.3212755839424261E-3,9]
[null,"7G4","Short Rural",33,"Bootawa ZS","Wingham ZS",7.9119999999999999,2.2000000000000002,2.1120000000000001,18,0,7.9119999999999999,2.8533798075686452,2.7392446152658994,18,0,-3.6311791687229653E-3,10]
[null,"7G5","Short Rural",33,"TransGrid Taree 132/66/33kV STS","Kanangra Dr ZS",2.3394999999999997,7.7,7.3919999999999995,17,0,2.4549999999999996,10.656500097654328,10.230240093748154,17,0,-3.6311791687229683E-3,10]
[null,"863:WTE","Urban",66,"TransGrid Taree 132/66/33kV STS","Whitbread ZS",0.61,10.164462732940439,9.9611734782816299,62,0,0.61,11.529983712216158,11.299384037971834,62,0,-1.9868344280597199E-3,10]
[null,"867/1","Short Rural",66,"Failford ZS","Tuncurry ZS",11.959000000000001,11.7,11.465999999999999,39,0,11.959000000000001,11.626671638036912,11.394138205276175,39,0,0.10632268082815187,9]
[null,"868/2","Short Rural",66,"Bohnock Tee","Bohnock ZS",3.68,6.1,5.9779999999999998,16,0,3.68,14.389445096580339,14.101656194648731,16,0,1.9148051510743849E-2,9]
[null,"86C","Urban",66,"Tuncurry ZS","Forster ZS",5.0419999999999998,7.1,6.9579999999999993,42,0,5.0419999999999998,7.9429736933123483,7.784114219446101,42,0,-1.4692569264427998E-2,10]
[null,"86C","Urban",66,"Tuncurry ZS","Forster ZS",5.0419999999999998,7.1,6.9579999999999993,42,0,5.0419999999999998,7.9429736933123483,7.784114219446101,42,0,-1.4692569264427998E-2,10]
[null,"86R","Short Rural",66,"Hallidays Point ZS","Tuncurry ZS",11.891,9.5,9.31,38,0,8.34,0,0,39,0,-1.4692569264428005E-2,10]
[null,734,"Short Rural",66,"TransGrid Inverell 132/66kV STS","Borthwick St ZS",6.1,17.914964521107816,17.55666523068566,64,0,6.1,16.977887641341958,16.63832988851512,45,0,4.9096138259111882E-2,9]
[null,735,"Short Rural",66,"TransGrid Inverell 132/66kV STS","Borthwick St ZS",6,18.209819215269068,17.845622830963688,64,0,6,17.207318555414144,16.86317218430586,64,0,4.9096138259111861E-2,9]
[null,"6AB","Short Rural",66,"Borthwick St ZS","Ashford ZS",72,6.5478076910291909,6.4168515372086068,17,0,72,6.5387810510573754,6.4080054300362281,17,0,4.130673950825333E-2,9]
[null,"6AF/A","Short Rural",66,"Ashford ZS","Wallangra ZS",23.21,0.89473148573069672,0.87683685601608274,11,0,23.21,1.0322333456889097,1.0115886787751314,11,0,4.9096138259111813E-2,9]
[null,"6AF/F","Short Rural",66,"Wallangra ZS","Coolatai Sw Stn",14.79,0.74222043702660068,0.72737602828606862,11,0,14.79,0.80300819925266009,0.78694803526760693,11,0,4.9096138259111848E-2,9]
[null,"6AX","Long Rural",66,"Ashford ZS","Texas ZS",51.5,5.4497281403596993,5.3407335775525056,9,0,51.5,5.2769110236603387,5.1713728031871318,9,0,4.1306739508253289E-2,9]
[null,"6BC","Short Rural",66,"Borthwick St ZS","Copeton ZS",30.5,0.843894469495998,0.82701658010607804,21,0,30.5,0.80300819925266009,0.78694803526760693,21,0,4.9096138259111827E-2,9]
[null,"6BD","Short Rural",66,"Borthwick St ZS","Bundarra ZS",44.1,0.93540109871845578,0.91669307674408662,14,0,44.1,1.1471545703609431,1.1242114789537243,14,0,4.909613825911182E-2,9]
[null,"6BR","Urban",66,"Borthwick St ZS","Wynne St ZS",0.97,0,0,34,0,0.97,5.9652037658769039,5.8458996905593654,17,0,0,9]
[null,"6BW","Short Rural",66,"Borthwick St ZS","Warialda ZS",62.13,7.1883540955863943,7.0445870136746667,15,0,62.1,6.9976428792017531,6.8576900216177181,15,0,4.1306739508253316E-2,9]
[null,"6FH","Short Rural",66,"Coolatai Sw Stn","Yallaroi ZS",31.1,2.2774983273145009,2.2319483607682109,20,0,31.1,2.1795936836857916,2.1360018100120759,20,0,4.1306739508253289E-2,9]
[null,"6FW","Short Rural",66,"Warialda ZS","Coolatai Sw Stn",37.1,1.7284585519797553,1.6938893809401601,11,0,37.1,1.7207318555414146,1.6863172184305864,11,0,4.1306739508253316E-2,9]
[null,"6HG","Long Rural",66,"Yallaroi ZS","Goondiwindi ZS",69.3,0,0,20,0,69.3,1.0324391133248487,1.0117903310583518,20,0,0,9]
[null,"6WK","Short Rural",66,"Warialda ZS","Bingara ZS",38.299999999999997,2.785868489661488,2.7301511198682582,11,0,38.299999999999997,2.6384555118301694,2.5856864015935659,11,0,4.130673950825331E-2,9]
[null,"7R1","Short Rural",33,"TransGrid Kempsey 132/33kV STS","Prince St ZS",2.4089999999999998,6.7,6.4319999999999995,30,0,2.4089999999999998,6.7668630439606297,6.4961885222022042,30,0,-1.6531199975205761E-3,10]
[null,"7R2/1","Short Rural",33,"TransGrid Kempsey 132/33kV STS","North St Tee",6.8570000000000002,7.4,7.1040000000000001,26,0,6.8570000000000002,7.7456768250526604,7.4358497520505535,26,0,-1.6531199975205681E-3,10]
[null,"7R2/2","Short Rural",33,"North St Tee","Smithtown ZS",16.75,4.3,4.1280000000000001,19,0,16.75,4.4652616650596828,4.286651198457295,19,0,-1.6531199975205876E-3,10]
[null,"7R2/3","Short Rural",33,"North St Tee","North St ZS",0.05,3.4263520730199772,3.2892979900991781,10,0,0.05,3.8728384125263302,3.7179248760252768,10,0,-1.084995452278875E-2,10]
[null,"7R3","Short Rural",33,"TransGrid Kempsey 132/33kV STS","Prince St ZS",2.395,6.7,6.4319999999999995,26,0,2.395,6.5948241530124783,6.3310311868919786,26,0,-1.6531199975205865E-3,10]
[null,"7R4","Short Rural",33,"TransGrid Kempsey 132/33kV STS","Munga ZS",34.954000000000008,1.2,1.1519999999999999,3,0,34.954000000000008,1.5028925182938,1.4427768175620479,3,0,2.2553297192554028E-2,9]
[null,"7R5","Short Rural",33,"TransGrid Kempsey 132/33kV STS","North St ZS",5.7610000000000001,5.6,5.3759999999999994,19,0,5.7610000000000001,6.1849807483629462,5.937581518428428,19,0,-1.6531199975205748E-3,10]
[null,"7R6/1","Short Rural",33,"Prince St ZS","Smithtown Tee",16.166919999999998,5.3,5.0880000000000001,15,0,16.166919999999998,5.046474134479114,4.8446151690999493,15,0,-1.6531199975205872E-3,10]
[null,"7R6/2","Short Rural",33,"Smithtown Tee","South West Rocks ZS",18.207999999999998,2.7,2.5920000000000001,19,0,18.207999999999998,2.570845313791247,2.4680115012395971,19,0,-1.6531199975206019E-3,10]
[null,"7R6/3","Short Rural",33,"Smithtown Tee","Smithtown ZS",1.325,2.4,2.3039999999999998,19,0,1.325,2.2851958344811081,2.1937880011018636,19,0,-1.6531199975205364E-3,10]
[null,"7R7","Short Rural",33,"Prince St ZS","Crescent Head ZS",19.302,1.6,1.536,5,0,19.302,1.8350815034469505,1.7616782433090725,5,0,0,9]
[null,"7R8","Short Rural",33,"Smithtown ZS","South West Rocks ZS",20.3,3.2,3.0720000000000001,30,0,0,0,0,0,0,-1.6531199975205768E-3,10]
[null,892,"Short Rural",66,"Lismore 132/66kV STS","Woodburn ZS",36.815000000000005,6.4,6.2720000000000002,11,0,36.815000000000005,6.4106341115853516,6.2824214293536444,11,0,9.6568522022065315E-3,9]
[null,8502,"Short Rural",66,"Lismore East ZS","Alstonville ZS",13.769000000000002,9.9,9.702,62,0,13.769000000000002,8.9506966841003024,8.7716827504182966,62,0,-6.2876678144627553E-4,10]
[null,8503,"Short Rural",66,"Ballina ZS","Alstonville ZS",18.5,7.9,7.742,62,0,18.5,7.8620984387367514,7.7048564699620163,62,0,-6.2876678144625038E-4,10]
[null,8507,"Short Rural",66,"Alstonville ZS","Ballina ZS",14.84,9.1999999999999993,9.016,61,0,14.84,9.1926074052921987,9.0087552571863547,61,0,-6.2876678144622208E-4,10]
[null,8510,"Short Rural",66,"Lismore Sw Stn","East Lismore ZS",8.5779999999999994,21.2,20.776,61,0,8.5779999999999994,20.320500580119607,19.914090568517214,61,0,-6.2876678144621807E-4,10]
[null,8511,"Short Rural",66,"Lismore 132/66kV STS","Lismore Sw Stn",5.9200000000000008,17.5,17.149999999999999,62,0,5.9200000000000008,17.659482647008701,17.306292994068528,62,0,-6.2876678144623401E-4,10]
[null,8512,"Short Rural",66,"Lismore Sw Stn","Lismore University ZS",1,7.9617863852311457,7.8025506575265222,54,0,1,7.2998126525784421,7.1538163995268729,62,0,5.8330285112720833E-3,9]
[null,8513,"Short Rural",66,"Lismore Sw Stn","Lismore University ZS",1,7.9617863852311457,7.8025506575265222,54,0,1,7.2998126525784421,7.1538163995268729,62,0,5.8330285112720833E-3,9]
[null,8514,"Urban",66,"Lismore 132/66kV STS","South Lismore ZS",2.2599999999999998,11.61649143552453,11.38416160681404,68,0,2.2599999999999998,10.891783957815454,10.673948278659145,68,0,-2.1178584891602052E-3,10]
[null,8515,"Urban",66,"Lismore 132/66kV STS","South Lismore ZS",2.2799999999999998,11.51649143552453,11.286161606814039,68,0,2.2799999999999998,10.775913915711033,10.560395637396812,68,0,-2.1344094927771323E-3,10]
[null,8516,"Short Rural",66,"Lismore 132/66kV STS","Lismore Sw Stn",6.2799999999999994,17.5,17.149999999999999,62,0,6.2799999999999994,17.538527286412751,17.187756740684495,62,0,-6.2876678144627629E-4,10]
[null,"0897:LME","Short Rural",66,"Lismore 132/66kV STS","Alstonville ZS",22.302,17.7,17.346,62,0,22.302,16.933750483433002,16.595075473764343,62,0,-6.2876678144625417E-4,10]
[null,"894:LME","Short Rural",66,"Lismore 132/66kV STS","Kyogle ZS",34.825000000000003,7.1027685902181812,6.9607132184138178,11,0,34.825000000000003,7.3782769963529509,7.2307114564258921,11,0,2.0762892437560514E-2,9]
[null,"9U6","Short Rural",132,"Lismore 132/66kV STS","Mullumbimby ZS",34.709999999999994,24.2,23.715999999999998,107,0,34.709999999999994,22.497697070846705,22.047743129429769,107,0,-6.2876678144623758E-4,10]
[null,"9U7","Short Rural",132,"Lismore 132/66kV STS","Dunoon ZS",17.149999999999999,27,26.46,107,0,17.149999999999999,25.884447167533303,25.366758224182636,107,0,-6.2876678144623292E-4,10]
[null,"9U7/1","Short Rural",132,"Dunoon ZS","Mullumbimby ZS",17.555,21.4,20.971999999999998,107,0,17.555,20.515821088341209,20.105504666574383,107,0,-6.2876678144627824E-4,10]
[null,"9U8","Short Rural",132,"TransGrid Lismore 330/132 STS","Lismore 132/66kV STS",9.86,47.4,46.451999999999998,183,0,9.86,49.591697844339507,48.599863887452713,183,0,-6.2876678144625406E-4,10]
[null,"9U9","Short Rural",132,"TransGrid Lismore 330/132 STS","Lismore 132/66kV STS",9.86,43.9,43.021999999999998,128,0,9.86,45.963037026461002,45.043776285931784,128,0,-6.2876678144622555E-4,10]
[null,"9W1","Short Rural",132,"TransGrid Lismore 330/132 STS","Lismore 132/66kV STS",10.199999999999999,40.700000000000003,39.886000000000003,128,0,10.199999999999999,42.334376208582505,41.487688684410855,128,0,-6.2876678144622826E-4,10]
[null,"9G2","Short Rural",132,"Ballina ZS","Lennox Head ZS",12.754599999999998,9.7101525529093031,9.5159495018511162,124,0,12.754599999999998,11.127893174827403,10.905335311330854,124,0,-1.0873469372749451E-2,10]
[null,"9G3","Short Rural",132,"Lennox Head ZS","Suffolk Park ZS",13.64,13.8,13.524000000000001,124,0,13.64,15.240375435089701,14.935567926387908,124,0,-6.2876678144624528E-4,10]
[null,"9G4","Short Rural",132,"Suffolk Park ZS","Ewingsdale ZS",7.0600000000000005,20,19.600000000000001,124,0,7.0600000000000005,15.240375435089701,14.935567926387908,124,0,-6.2876678144628431E-4,10]
[null,"9G5","Short Rural",132,"Ewingsdale ZS","Mullumbimby ZS",13.580000000000002,37.9,37.141999999999996,122,0,13.580000000000002,36.044697457593109,35.323803508441245,122,0,-6.2876678144623086E-4,10]
[null,721,"Short Rural",66,"TransGrid Moree 132/66kV STS","Moree ZS",0.39,10.402807260227675,10.194751115023122,64,0,0.39,12.737222432271343,12.482477983625916,64,0,9.8262382088558885E-4,9]
[null,722,"Short Rural",66,"TransGrid Moree 132/66kV STS","Moree ZS",0.36,10.96766557300022,10.748312261540216,64,0,0.36,13.310971190481764,13.044751766672128,64,0,9.8262382088556998E-4,9]
[null,881,"Short Rural",66,"TransGrid Moree 132/66kV STS","Ashley ZS",54.730000000000004,12.2,11.956,10,0,54.730000000000004,3.5572423009046097,3.4860974548865173,10,0,1.5503725839473084E-2,9]
[null,"6PU/1","Long Rural",66,"Ashley ZS","Mungindi ZS",64.8,5.8,5.6840000000000002,10,0,64.8,2.2949950328416837,2.2490951321848498,10,0,1.5503725839473081E-2,9]
[null,"723:WTR/1","Urban",66,"TransGrid Moree 132/66kV STS","Wathagar ZS",35.099999999999994,5.6,5.4879999999999995,12,0,35.099999999999994,5.3867909412518618,5.2790551224268247,12,0,1.5503725839473065E-2,9]
[null,"723:WTR/2","Short Rural",66,"Wathagar ZS","Wenna ZS",67.2,0.9,0.88200000000000001,15,0,67.2,0.87018561661913829,0.85278190428675549,15,0,1.5503725839473037E-2,9]
[null,"876/2","Short Rural",66,"TransGrid Moree 132/66kV STS","Bellata ZS",55,0.9,0.88200000000000001,25,0,50.1,1.1474975164208419,1.1245475660924249,25,0,9.8262382088557844E-4,9]
[null,876,"Urban",66,"TransGrid Moree 132/66kV STS","Moree Solar Farm",12.5,0.97281153866382486,0.95335530789054834,70,0,0,0,0,0,0,2.928845971173238E-5,9]
[null,"87J","Short Rural",66,"Moree Solar Farm","Bellata ZS",42.5,0.97281153866382486,0.95335530789054834,25,0,0,0,0,0,0,9.8262382088557844E-4,9]
[null,7703,"Short Rural",33,"Moruya North 132/33kV STS","Moruya Town ZS",13.120000000000001,8.1999999999999993,7.871999999999999,30,0,13.120000000000001,9.8168881222751541,9.4242125973841482,30,0,1.1887342390272483E-2,9]
[null,7704,"Short Rural",33,"Moruya North 132/33kV STS","Moruya Town ZS",9.83,10.4,9.984,26,0,9.83,10.163366526590748,9.7568318655271167,30,0,1.1887342390272462E-2,9]
[null,7706,"Short Rural",33,"Moruya North 132/33kV STS","Mossy Point ZS",11.1,7.1,6.8159999999999998,25,0,11.1,6.8718216855926073,6.5969488181689027,25,0,1.1887342390272473E-2,9]
[null,"7711/1","Short Rural",33,"Moruya Town ZS","Tuross Tee",10.9,4,3.84,14,0,10.9,4.6774584582605137,4.4903601199300933,7,0,1.188734239027248E-2,9]
[null,"7711/2","Short Rural",33,"Tuross Tee","Tuross ZS",0.48,2.6,2.496,7,0,0.48,3.040347997869334,2.9187340779545603,7,0,1.1887342390272471E-2,9]
[null,"7711/3","Short Rural",33,"Tuross Tee","Bodalla Tee",10.1,1.4,1.3439999999999999,21,0,10.1,1.8139619562661464,1.7414034780155005,21,0,1.1887342390272492E-2,9]
[null,7713,"Short Rural",33,"Bodalla Tee","Narooma ZS",15.5,0,0,21,0,15.5,5.8026473334849497E-2,5.5705414401455516E-2,21,0,0,9]
[null,"7715/1","Short Rural",33,"Moruya Town ZS","Narooma Tee",45.57,7.5,7.1999999999999993,30,0,45.57,7.0450608877504042,6.7632584522403878,30,0,1.188734239027248E-2,9]
[null,"7715/2","Short Rural",33,"Narooma Tee","Narooma ZS",3.2,7,6.72,10,0,3.2,6.5753901619003772,6.3123745554243618,10,0,1.188734239027245E-2,9]
[null,7712,"Short Rural",33,"Bodalla Tee","Bodalla ZS",0.36099999999999999,1.4,1.3439999999999999,10,0,0.36099999999999999,1.3,1.248,10,0,1.1887342390272483E-2,9]
[null,"98H","Short Rural",132,"Endeavour Energy Evans Lane Sw Stn","Moruya North 132/33kV STS",41.47,21.2,20.776,180,0,72,20.557718656058558,20.146564282937387,180,0,1.1887342390272488E-2,9]
[null,"98M","Short Rural",132,"Endeavour Energy Evans Lane Sw Stn","Batemans Bay ZS",22.77,26.5,25.97,70,0,54,27.718272345247492,27.163906898342542,70,0,1.1887342390272494E-2,9]
[null,"98T","Short Rural",132,"Batemans Bay ZS","Moruya North 132/33kV STS",21,5.3,5.194,70,0,21,4.8506976604183123,4.7536837072099463,70,0,1.1887342390272488E-2,9]
[null,56,"Urban",33,"Smiggin Sw Stn","Perisher ZS",1.1000000000000001,12.8,12.288,20,0,1.1000000000000001,11.937609399011681,11.460105023051213,20,0,-3.2211089051760807E-3,10]
[null,58,"Urban",33,"Bullocks Flat ZS","Thredbo ZS",13.077999999999999,5.9,5.6639999999999997,6,0,12.899999999999999,5.7067596151372904,5.4784892305317987,6,0,-3.221108905176082E-3,10]
[null,59,"Urban",33,"Bullocks Flat ZS","Thredbo ZS",13.065999999999999,10.8,10.368,6,0,12.899999999999999,10.423571133771173,10.006628288420325,6,0,-3.2211089051760755E-3,10]
[null,"57A","Urban",33,"Smiggin Sw Stn","Perisher ZS",1.1000000000000001,9.8000000000000007,9.4079999999999995,20,0,1.1000000000000001,9.142461832413824,8.77676335911727,20,0,-3.2211089051760924E-3,10]
[null,"57B","Urban",33,"Smiggin Sw Stn","Perisher ZS",1.1000000000000001,9.8000000000000007,9.4079999999999995,20,0,1.1000000000000001,9.142461832413824,8.77676335911727,20,0,-3.2211089051760924E-3,10]
[null,"60/2","Urban",33,"Bullocks Portal ZS","Bullocks Flat ZS",2.9000000000000004,17.399999999999999,16.703999999999997,19,0,2.9000000000000004,16.421491953762409,15.764632275611913,7,0,-3.2211089051760937E-3,10]
[null,"Bullocks Portal Line","Short Rural",33,"Perisher ZS","Bullocks Portal ZS",3.5,18.600000000000001,17.856000000000002,20,0,5,17.411440050265814,16.714982448255181,20,0,-3.2211089051760729E-3,10]
[null,"No.1 Perisher","Urban",33,"TransGrid Munyang 132/33kV STS","Smiggin Sw Stn",5.6000000000000005,16.8,16.128,38,0,5.6000000000000005,16.479724194733198,15.820535226943869,38,0,-3.2211089051761171E-3,10]
[null,"No.2 Perisher","Urban",33,"TransGrid Munyang 132/33kV STS","Blue Cow  Tee",2.5,17.600000000000001,16.896000000000001,38,0,2.5,15.023918170463478,14.422961443644938,38,0,-3.2211089051760837E-3,10]
[null,"976/2 (M)","Long Rural",132,"TransGrid 132kV Line 976/2(Y) / Murrumbateman Tee","Murrumbateman ZS",0.2,6,5.88,42,0,23.099999999999998,5.7386307356372042,5.62385812092446,42,0,2.7957675980528366E-3,9]
[null,751,"Short Rural",66,"TransGrid Nambucca 132/66 kV STS","Nambucca ZS",3.1,9,8.82,15,0,3.1,9.2385095922561007,9.0537394004109792,15,0,-1.0767592721132195E-2,10]
[null,856,"Long Rural",66,"TransGrid Wallerawang 330/132/66kV STS","Oberon Town ZS",43.5,6.4,6.2720000000000002,28,0,43.5,12.075130769031032,11.833628153650411,28,0,9.7942548713385248E-4,9]
[null,"81B","Long Rural",33,"Oberon Town ZS","Burraga ZS",41.1,0.6,0.57599999999999996,8,0,41.1,0.46091950450376906,0.44248272432361829,8,0,9.7942548713387547E-4,9]
[null,"94C","Urban",132,"TransGrid Wallerawang 330/132/66kV STS","Oberon 132 ZS",66.400000000000006,24.121779859484779,23.639344262295083,128,0,66.400000000000006,26.910291428126303,26.372085599563778,128,0,3.5415458348860545E-3,9]
[null,"8C1","Short Rural",66,"TransGrid Molong 132/66kV STS","Cumnock ZS",34.643000000000001,1.5,1.47,9,0,34.643000000000001,1.6031356516021718,1.5710729385701283,9,0,-1.9222674910851594E-3,10]
[null,807,"Short Rural",66,"TransGrid Orange 132/66kV STS","Orange West & South Tee",3.55,14.1,13.818,61,0,3.55,7.5749925710411086,7.4234927196202865,12,0,4.4406545043233258E-3,9]
[null,"807/2","Urban",66,"Orange West & South Tee","Orange South ZS",0.97,0,0,63,0,0.97,0,0,21,0,0,9]
[null,"807/3","Short Rural",66,"Orange West & South Tee","Orange West ZS",4.8899999999999997,14.1,13.818,62,0,4.8899999999999997,7.5749925710411086,7.4234927196202865,21,0,4.4406545043233258E-3,9]
[null,"8C2","Short Rural",66,"TransGrid Orange 132/66kV STS","Orange West ZS",4.34,0,0,9,0,4.34,6.8863568827646446,6.7486297451093513,9,0,0,9]
[null,"8F1","Urban",66,"TransGrid Orange 132/66kV STS","Orange South ZS",2.76,24.8,24.303999999999998,63,0,2.76,18.24884573932631,17.883868824539782,21,0,4.4406545043233266E-3,9]
[null,"8M1","Short Rural",66,"TransGrid Orange 132/66kV STS","Orange Industrial ZS",3.77,4,3.92,11,0,3.77,4.1318141296587862,4.0491778470656108,11,0,4.440654504323331E-3,9]
[null,"8M2","Short Rural",66,"TransGrid Orange 132/66kV STS","Orange Industrial ZS",3.74,6.4,6.2720000000000002,21,0,3.74,6.6568116533391564,6.5236754202723732,21,0,4.4406545043233266E-3,9]
[null,"94G","Urban",132,"TransGrid Orange 132/66kV STS","Line 9MC",24.8,0,0,156,0,24.8,0,0,156,0,0,9]
[null,"9MC","Urban",132,"TransGrid Orange  North 132kV Sw Stn","Cadia ZS",2.2000000000000002,150.3876657176379,147.37991240328515,162,0,2.2000000000000002,131.39841106592345,128.77044284460499,162,0,1.1559575147975062E-2,9]
[null,"818/1","Short Rural",66,"TransGrid Orange 132/66kV STS","Blayney ZS",25,0,0,11,0,25,0,0,11,0,0,9]
[null,"66:MAN","Short Rural",66,"Blayney ZS","Mandurama ZS",24.8,2.1,2.0579999999999998,9,0,24.8,2.1915396381055943,2.1477088453434825,9,0,2.3211843288609389E-2,9]
[null,"81C","Short Rural",66,"TransGrid Panorama 132/66kV STS","Blayney ZS",28.1,11.9,11.662000000000001,19,0,28.1,13.765854844331317,13.490537747444691,16,0,4.1501082224852946E-4,9]
[null,"81F","Urban",66,"TransGrid Panorama 132/66kV STS","Russell St ZS",9.61,29.1,28.518000000000001,64,0,9.61,32.005612513070311,31.365500262808904,64,0,4.150108222485473E-4,9]
[null,"81G","Short Rural",66,"TransGrid Panorama 132/66kV STS","Stewart ZS",3.39,11.8,11.564,64,0,3.39,13.192277559150845,12.928432007967828,45,0,4.1501082224855505E-4,9]
[null,"81H","Short Rural",66,"TransGrid Panorama 132/66kV STS","Stewart ZS",4.4400000000000004,7.1,6.9579999999999993,62,0,4.4400000000000004,7.9153665354905076,7.7570592047806972,21,0,4.1501082224855608E-4,9]
[null,"81J","Urban",66,"Raglan ZS","Russell St ZS",6.04,6.4,6.2720000000000002,64,0,6.04,7.2270737932739415,7.0825323174084627,64,0,4.1501082224857814E-4,9]
[null,"81L","Short Rural",66,"TransGrid Panorama 132/66kV STS","Raglan ZS",18.3,17.5,17.149999999999999,64,0,18.3,19.27219678206384,18.886752846422564,64,0,4.1501082224856101E-4,9]
[null,300,"Urban",132,"TransGrid Parkes 132/66kV STS","North Parkes Mine ZS",21.2,32.5,31.849999999999998,87,0,21.2,30.964325391400074,30.345038883572073,97,0,3.7654522858767106E-3,9]
[null,898,"Short Rural",66,"TransGrid Parkes 132/66kV STS","Trundle ZS",40.299999999999997,2.6,2.548,11,0,40.299999999999997,2.7729246619164245,2.7174661686780959,11,0,-2.0009796019759485E-4,10]
[null,899,"Short Rural",66,"Parkes Town ZS","Peak Hill ZS",46.5,6.2,6.0759999999999996,13,0,46.5,1.7330779136977659,1.6984163554238105,13,0,0,9]
[null,"89L","Short Rural",66,"TransGrid Parkes 132/66kV STS","Parkes Town ZS",11.5,11.429556513965649,11.200965383686336,38,0,11.5,10.398467482186593,10.19049813254286,38,0,-2.0009796019758699E-4,10]
[null,"89G","Short Rural",66,"TransGrid Parkes 132/66kV STS","Parkes Town ZS",8.8800000000000008,11.636114764218041,11.40339246893368,68,0,0,0,0,0,0,-2.0009796019758902E-4,10]
[null,"89M","Urban",66,"Peak Hill ZS","Tomingley Mine ZS",21,5.0999999999999996,4.9979999999999993,17,0,0,0,0,0,0,9.1661157115928427E-2,9]
[null,701,"Short Rural",33,"TransGrid Port Macquarie 132/33kV STS","Rocks Ferry ZS",10.121,9.1999999999999993,8.831999999999999,22,0,10.121,9.5533455067783795,9.1712116865072435,22,0,-2.2518595268730471E-3,10]
[null,707,"Urban",33,"TransGrid Port Macquarie 132/33kV STS","Boronia Street ZS",6.9459999999999997,8.8000000000000007,8.4480000000000004,26,0,6.9459999999999997,9.4947360251417035,9.1149465841360353,26,0,-2.2518595268730237E-3,10]
[null,708,"Urban",33,"TransGrid Port Macquarie 132/33kV STS","Owen Street ZS",10.15,11.5,11.04,26,0,10.15,12.031593766726902,11.550330016057824,26,0,-2.2518595268730649E-3,10]
[null,710,"Short Rural",33,"TransGrid Port Macquarie 132/33kV STS","Clearwater ZS",7.5660000000000007,13.2,12.671999999999999,31,0,7.5660000000000007,13.891550291051832,13.335888279409758,31,0,-2.2518595268730874E-3,10]
[null,712,"Short Rural",33,"TransGrid Port Macquarie 132/33kV STS","Rocks Ferry ZS",10.250999999999999,6.1,5.8559999999999999,12,0,10.250999999999999,7.0329606076036475,6.7516421832995013,12,0,-2.2518595268730475E-3,10]
[null,715,"Urban",33,"Clearwater ZS","Owen Street ZS",4.2,4.310270136908021,4.1378593314316996,31,0,4.2,5.040415420754238,4.8387988039240684,31,0,-6.9276785375062457E-3,10]
[null,"719/1","Short Rural",33,"Clearwater ZS","Lake Cathie ZS",16.225999999999999,5.0999999999999996,4.8959999999999999,20,0,16.225999999999999,5.5798695729747951,5.3566747900558029,20,0,4.7304049515012631E-2,9]
[null,"719/2","Short Rural",33,"Lake Cathie ZS","Laurieton ZS",13.600000000000001,0,0,12,0,13.600000000000001,0,0,12,0,0,9]
[null,765,"Short Rural",33,"Rocks Ferry ZS","Koree ZS",6.5039999999999996,4.5,4.32,9,0,6.5039999999999996,6.1611059868263354,5.9146617473532821,9,0,-2.251859526873064E-3,10]
[null,784,"Short Rural",33,"Koree ZS","Byabarra ZS",15.54,1.1000000000000001,1.056,9,0,15.54,3.0805529934131677,2.957330873676641,9,0,-2.2518595268730957E-3,10]
[null,"703:BPM","Urban",33,"TransGrid Port Macquarie 132/33kV STS","Boronia Street ZS",7.6920000000000002,7.8,7.4879999999999995,26,0,7.6920000000000002,10.549706694601893,10.127718426817816,26,0,-2.2518595268730514E-3,10]
[null,"70Y","Short Rural",33,"Rocks Ferry ZS","Telegraph Point ZS",14.2,1.7,1.6319999999999999,8,0,14.2,0,0,8,0,1.666947079957274E-2,9]
[null,"711:CPM","Short Rural",33,"TransGrid Port Macquarie 132/33kV STS","Clearwater ZS",7.7960000000000003,13.2,12.671999999999999,20,0,7.7960000000000003,13.833426649666679,13.280089583680011,20,0,-2.2518595268730692E-3,10]
[null,975,"Short Rural",132,"TransGrid Queanbeyan 132/66kV STS","Googong Town ZS",0,0,0,41.8,0,0,0,0,0,0,0.13437282018847785,9]
[null,"82A","Short Rural",66,"TransGrid Queanbeyan 132/66kV STS","Queanbeyan South ZS",5.2,5.7,5.5860000000000003,30,0,5.2,5.7906442213884972,5.6748313369607271,30,0,-9.6219162167964596E-4,10]
[null,"82B","Short Rural",66,"TransGrid Queanbeyan 132/66kV STS","Queanbeyan South ZS",7.1,26.1,25.577999999999999,30,0,7.1,26.752776302814858,26.217720776758561,30,0,-9.6219162167964346E-4,10]
[null,"82F","Urban",66,"TransGrid Queanbeyan 132/66kV STS","Oaks Estate ZS",0.1,15.5,15.19,49,0,0.1,0,0,49,0,0,9]
[null,"82G","Long Rural",66,"TransGrid Queanbeyan 132/66kV STS","Captains Flat ZS",41.5,3,2.94,12,0,41.5,3.7060123016886388,3.6318920556548662,12,0,-9.6219162167965225E-4,10]
[null,"82K/1","Short Rural",66,"TransGrid Queanbeyan 132/66kV STS","Sutton / Bungendore Tee",13,12.1,11.857999999999999,15,0,13,13.434294593621315,13.165608701748889,15,0,-9.6219162167965279E-4,10]
[null,"82K/2","Short Rural",66,"Woodlawn ZS","Bungendore ZS",29,0,0,15,0,29,0,0,15,0,0,9]
[null,"82K/3","Short Rural",66,"Sutton / Bungendore Tee","Sutton ZS",6.1,4,3.92,15,0,6.1,4.9799540303941079,4.8803549497862253,15,0,-9.6219162167965127E-4,10]
[null,"82M","Urban",66,"TransGrid Queanbeyan 132/66kV STS","Oaks Estate ZS",0.1,0,0,20,0,0.1,20.846319196998593,20.42939281305862,20,0,-9.6219162167964823E-4,10]
[null,"830:QSH","Urban",66,"Queanbeyan South ZS","Googong Dam ZS",7,5.7,5.5860000000000003,15,0,7,5.7906442213884972,5.6748313369607271,15,0,-9.6219162167966677E-4,10]
[null,3801,"Short Rural",33,"Bulahdelah ZS","Pacific Palms ZS",35.376999999999995,4.4000000000000004,4.2240000000000002,7,0,35.376999999999995,5.4104313563142075,5.1940141020616393,7,0,8.4816212521572005E-5,9]
[null,3803,"Short Rural",33,"Bulahdelah ZS","Bungwahl Sw Stn",28.657,0,0,7,0,28.657,0,0,7,0,0,9]
[null,"7J1","Short Rural",33,"Ausgrid Recloser 33175 (Patterson)","Martins Creek Tee",8.4640000000000004,3.6,3.456,8,0,8.4640000000000004,6.4415729903791075,6.1839100707639432,8,0,0,9]
[null,"7J1/2","Short Rural",33,"Martins Creek Tee","Martins Creek ZS",0.85299999999999998,2.7024612836248871,2.5943628322798915,4,0,0.85299999999999998,3.3658669679458408,3.2312322892280072,4,0,-2.508445408382003E-2,10]
[null,"7J1/3","Short Rural",33,"Martins Creek Tee","Gresford ZS",16.399999999999999,1.9581970461003164,1.8798691642563037,4,0,16.399999999999999,3.0757060224332666,2.952677781535936,4,0,-2.508445408382003E-2,10]
[null,"BLH4B4","Short Rural",33,"Bulahdelah ZS","Hawks Nest 132/33kV STS",22.1328,0.2188243336220741,0.21007136027719112,7,0,22.1328,0,0,7,0,1.3947372414024452E-3,9]
[null,"STR4B2","Short Rural",33,"Stroud 132/33kV STS","Dungog ZS",15.940000000000001,7.2447199447230606,6.9549311469341379,27,0,15.940000000000001,5.1379035540480897,4.9323874118861664,27,0,8.7586795825271937E-4,9]
[null,"STR4B2/2","Short Rural",33,"Dungog ZS","Martins Creek ZS",35.119999999999997,5.6746842556393551,5.4476968854137811,21,0,35.119999999999997,0,0,21,0,-2.5494928035980024E-3,10]
[null,"STR4B3/1","Short Rural",33,"Stroud 132/33kV STS","Booral ZS",15.363000000000001,4.9000000000000004,4.7039999999999997,7,0,15.363000000000001,6.0615716087084213,5.8191087443600846,7,0,-7.5238697082402311E-3,10]
[null,"STR4B3/2","Short Rural",33,"Booral ZS","Bulahdelah ZS",22.745999999999999,3.6,3.456,7,0,22.745999999999999,4.3699702295339788,4.1951714203526196,7,0,-7.5238697082402311E-3,10]
[null,"STR4B4","Short Rural",33,"Stroud 132/33kV STS","Dungog ZS",15.288,2.4789162220498184,2.3797595731678256,4,0,15.288,1.7318776024881204,1.6626024983885954,4,0,8.7586795825268869E-4,9]
[null,"STR4B5/1","Short Rural",33,"Stroud 132/33kV STS","Wards River Sw Stn",13.945,5.8931656744427539,5.6574390474650436,17,0,13.945,7.5625321975314588,7.2600309096302,19,0,1.3947372414024677E-3,9]
[null,"STR4B5/2","Urban",33,"Wards River Sw Stn","Stratford Coal",8.01,7.5003926765635045,7.2003769695009643,19,0,8.01,10.102619347847369,9.6985145739334744,19,0,1.3947372414024348E-3,9]
[null,"STR4B5/3","Short Rural",33,"Stratford Coal","Gloucester ZS",16.649999999999999,2.3165196697233359,2.2238588829344024,19,0,16.649999999999999,3.108498260876114,2.9841583304410695,19,0,1.3947372414024421E-3,9]
[null,"STR4B6/1","Short Rural",33,"Stroud 132/33kV STS","Wards River Sw Stn",13.974,6.7986456756375437,6.5266998486120418,17,0,13.974,8.7171172658568725,8.368432575222597,19,0,1.3947372414024285E-3,9]
[null,"STR4B6/2","Short Rural",33,"Wards River Sw Stn","Gloucester ZS",25.237000000000002,4.6405850061232963,4.4549616058783643,17,0,25.237000000000002,6.2347593689572331,5.9853689941989439,19,0,1.3947372414024784E-3,9]
[null,"STR4B7","Short Rural",33,"Stroud 132/33kV STS","Dungog ZS",15.572000000000001,3.7532886460613444,3.6031571002188905,7,0,15.572000000000001,3.1173796844786166,2.9926844970994719,7,0,8.7586795825271839E-4,9]
[null,"STR4B8","Short Rural",33,"Stroud 132/33kV STS","Bulahdelah ZS",37.959000000000003,4.2,4.032,7,0,37.959000000000003,5.0075268936099571,4.8072258178655582,7,0,-7.5238697082402042E-3,10]
[null,798,"Short Rural",33,"Quirindi ZS","Murrurundi ZS",31.4,2.6442822883333741,2.538510996800039,4,0,31.4,2.7288560932194499,2.6197018494906716,4,0,-5.7007268396107764E-3,10]
[null,"799/1","Short Rural",33,"Quirindi ZS","Caroona Tee",22.099999999999998,3.0220369009524277,2.9011554249143305,6,0,22.099999999999998,1.9740661099885382,1.8951034655889964,6,0,-5.7007268396107695E-3,10]
[null,"799/2","Short Rural",33,"Caroona Tee","Caroona ZS",5.8,1.1332638378571604,1.087933284342874,4,0,5.8,0.74878369689220414,0.71883234901651594,4,0,-5.7007268396107825E-3,10]
[null,"799/3","Long Rural",33,"Caroona Tee","Spring Ridge ZS",21.9,1.8887730630952675,1.8132221405714568,3,0,21.9,1.2252824130963338,1.1762711165724804,3,0,-5.7007268396107929E-3,10]
[null,"799/4","Short Rural",33,"Spring Ridge ZS","Colly Blue ZS",8.3000000000000007,0.94438653154763375,0.9066110702857284,3,0,8.3000000000000007,0.65988745538259774,0.63349195716729378,3,0,-5.7007268396107929E-3,10]
[null,801,"Short Rural",66,"Transgrid Tamworth 132/66kV STS","Oxley Vale ZS",12.561,12.938095482202581,12.679333572558528,63,0,12.561,13.237855090511374,12.973097988701147,63,0,-5.7007268396107435E-3,10]
[null,803,"Urban",66,"Transgrid Tamworth 132/66kV STS","South Tamworth ZS",5.7919999999999998,24.270733860774186,23.785319183558702,70,0,5.7919999999999998,24.966130214560923,24.466807610269704,70,0,-5.7007268396107973E-3,10]
[null,804,"Short Rural",66,"Transgrid Tamworth 132/66kV STS","Nundle ZS",39.200000000000003,1.7943344099405039,1.7584477217416938,8,0,39.200000000000003,1.8579445741068596,1.8207856826247224,8,0,-5.7007268396107973E-3,10]
[null,806,"Short Rural",66,"Transgrid Tamworth 132/66kV STS","Goddard Lane ZS",10,12.182586256964475,11.938934531825186,38,0,10,12.541125875221301,12.290303357716875,38,0,-5.7007268396107843E-3,10]
[null,873,"Urban",66,"Transgrid Tamworth 132/66kV STS","East Tamworth ZS",4.3,16.149009689464538,15.826029495675247,53,0,4.3,16.605379631080059,16.273272038458458,53,0,-5.7007268396107626E-3,10]
[null,874,"Urban",66,"Transgrid Tamworth 132/66kV STS","East Tamworth ZS",4.5,15.393500464226431,15.085630454941903,53,0,4.5,15.792528879908305,15.476678302310139,53,0,-5.7007268396107643E-3,10]
[null,"803/2","Short Rural",66,"South Tamworth ZS","Oxley Vale ZS",6.8440000000000003,1.5,1.47,63,0,6.8440000000000003,1.6130582242685723,1.5807970597832008,63,0,-1.9869015975723424E-3,10]
[null,"806/1","Short Rural",66,"Goddard Lane ZS","Attunga ZS",16,11.993708950654947,11.753834771641847,18,0,16,8.7091151911259033,8.5349328873033858,18,0,-5.7007268396107955E-3,10]
[null,"806/2","Short Rural",66,"Manilla ZS","Upper Manilla ZS",14.18,3.0220369009524277,2.9615961629333789,18,0,37.200000000000003,3.2514030046870044,3.1863749445932643,18,0,-5.7007268396107695E-3,10]
[null,"806/4","Short Rural",66,"Upper Manilla ZS","Barraba ZS",34.799999999999997,2.2665276757143209,2.2211971222000346,15,0,11.7,2.3224307176335741,2.2759821032809024,15,0,-5.7007268396107825E-3,10]
[null,"80C","Short Rural",66,"Transgrid Tamworth 132/66kV STS","Goddard Lane ZS",7.9210000000000012,11.049322419107314,10.828335970725167,61,0,14.211,11.263788980522836,11.03851320091238,61,0,-5.7007268396107678E-3,10]
[null,"813:CLA","Short Rural",66,"Transgrid Tamworth 132/66kV STS","Currububula ZS",26.6,16.810080261547881,16.473878656316923,28,0,26.6,17.18598731048845,16.842267564278682,28,0,-5.700726839610779E-3,10]
[null,"813:QDI/1","Short Rural",66,"Currububula ZS","Werris Creek ZS",14.9,14.826868545297847,14.53033117439189,28,0,14.9,15.328042736381592,15.02148188165396,28,0,-5.7007268396107582E-3,10]
[null,"813:QDI/2","Short Rural",66,"Werris Creek ZS","Quirindi ZS",15.3,12.088147603809711,11.846384651733516,28,0,15.3,12.481406228196439,12.231778103632511,28,0,-5.7007268396107695E-3,10]
[null,"870:KTL/1","Short Rural",66,"Transgrid Tamworth 132/66kV STS","Kootingal Tee",14,6.4218284145239091,6.2933918462334306,14,0,14,6.5028060093740088,6.3727498891865286,14,0,-5.7007268396108051E-3,10]
[null,"870:KTL/2","Short Rural",66,"Kootingal Tee","Kootingal ZS",2.6,5.7607578424405652,5.6455426855917539,12,0,2.6,5.7565823689540414,5.6414507215749605,12,0,-5.7007268396107617E-3,10]
[null,"870:KTL/3","Short Rural",66,"Kootingal Tee","Bendemeer ZS",25.5,0.7,0.68599999999999994,13,0,25.5,0.70777044534233269,0.69361503643548605,13,0,-1.9869015975723268E-3,10]
[null,"No 4 Temora","Short Rural",66,"Temora 132/66 STS","Temora Town ZS",0.17399999999999999,6.5192026673265815,6.3888186139800496,15,0,0.17399999999999999,4.0370467017734635,3.956305767737994,15,0,3.256564103961565E-3,9]
[null,901,"Urban",132,"Temora 132/66 STS","Lake Cowal",106.58,33.700000000000003,33.026000000000003,128,0,106.58,33.248757685596878,32.583782531884943,128,0,-3.40475718740171E-3,10]
[null,"20-60","Short Rural",66,"Ariah Park Tee","West Wyalong ZS",59.939,11.890828751560095,11.653012176528893,21,0,59.939,8.7508143609431368,8.5757980737242736,11,0,-5.5011330664735694E-2,10]
[null,"80-140","Short Rural",66,"Ariah Park Tee","Ariah Park ZS",29.486000000000001,2.2676058624891642,2.2222537452393807,11,0,29.486000000000001,1.7301628721886271,1.6955596147448546,11,0,-4.9139829497323387E-2,10]
[null,"60-70","Long Rural",66,"West Wyalong ZS","Anona ZS",62.825000000000003,1.3676328084885174,1.3402801523187471,7,0,62.825000000000003,1.731706129458171,1.6970720068690075,7,0,-5.0936674191438755E-3,10]
[null,"835/T","Short Rural",66,"Temora 132/66 STS","Junee Reefs ZS",26.96,0.17911150058926423,0.17552927057747894,12,0,26.96,14.64871231786371,14.355738071506435,12,0,4.4947783068561654E-2,9]
[null,"835/J","Short Rural",66,"Junee Reefs ZS","Junee ZS",22.29,0,0,12,0,22.29,0,0,12,0,0,9]
[null,757,"Short Rural",110,"Powerlink Mudgeeraba 275/110kV STS","Terranora 110/66kV STS",10.4,42.3,42.3,106,0,10.4,44.230439237247097,44.230439237247097,106,0,3.0800663141012253E-3,9]
[null,758,"Short Rural",110,"Powerlink Mudgeeraba 275/110kV STS","Terranora 110/66kV STS",10.4,42.3,42.3,106,0,10.4,44.230439237247097,44.230439237247097,106,0,3.0800663141012253E-3,9]
[null,9406,"Short Rural",33,"Cudgen ZS","Casuarina Sw Stn",5.67,10.5,10.08,17,0,5.67,10.475630345663786,10.056605131837234,19,0,1.3832979105863695E-2,9]
[null,9407,"Short Rural",33,"Casuarina Sw Stn","Hastings Pt ZS",7.5,0,0,20,0,7.5,10.708422131122983,10.280085245878064,20,0,0,9]
[null,9409,"Short Rural",33,"Casuarina Sw Stn","Hastings Pt ZS",7.5,10.5,10.08,20,0,7.5,0,0,20,0,1.3832979105863695E-2,9]
[null,9501,"Short Rural",66,"Terranora 110/66kV STS","Cudgen ZS",6.8210000000000006,22.1,21.658000000000001,59,0,6.8210000000000006,22.580803189541943,22.129187125751102,59,0,3.0800663141012079E-3,9]
[null,9502,"Short Rural",66,"Terranora 110/66kV STS","Murwillumbah ZS",14.67,9.8000000000000007,9.604000000000001,61,0,14.67,10.475630345663786,10.266117738750511,61,0,3.0800663141012184E-3,9]
[null,9503,"Urban",66,"Terranora 110/66kV STS","Banora Pt ZS",6.1280000000000001,27.6,27.048000000000002,59,0,6.1280000000000001,28.167806040562628,27.604449919751374,59,0,3.0800663141012318E-3,9]
[null,9504,"Urban",66,"Terranora 110/66kV STS","Condong Sw Stn",12.879999999999999,8.4,8.2319999999999993,61,0,12.879999999999999,9.0788796329086168,8.8973020402504446,61,0,3.0800663141012231E-3,9]
[null,9505,"Urban",66,"Cudgen ZS","Banora Point ZS",5.504999999999999,2.1496094289971444,2.1066172404172012,53,0,5.504999999999999,2.2158659452877378,2.1715486263819832,53,0,3.2727635025253739E-3,9]
[null,9508,"Urban",66,"Terranora 110/66kV STS","Tweed Heads ZS",14.27,13.118375399281678,12.856007891296045,41,0,14.27,13.295195671726427,13.029291758291897,41,0,3.2727635025253522E-3,9]
[null,9510,"Short Rural",66,"Banora Point ZS","Tweed Heads South ZS",5.319,16.112474246813413,15.790224761877145,43,0,5.319,16.444057804503736,16.115176648413662,49,0,3.2727635025253743E-3,9]
[null,9514,"Short Rural",66,"Condong Sw Stn","Murwillumbah ZS",3.9800000000000004,8.5,8.33,61,0,3.9800000000000004,9.0788796329086168,8.8973020402504446,61,0,3.0800663141012006E-3,9]
[null,9516,"Urban",66,"Tweed Head South ZS","Tweed Heads ZS",3.7379999999999995,3.9345529727179867,3.8558619132636269,43,0,3.7379999999999995,4.4317318905754757,4.3430972527639664,49,0,3.2727635025253509E-3,9]
[null,827,"Short Rural",66,"TransGrid Tumut 132/66kV STS","Tumut ZS",7.0000000000000007E-2,17.955932694547993,17.596814040657033,28,0,7.0000000000000007E-2,19.855662345304726,19.458549098398631,28,0,2.2662251088307805E-3,9]
[null,828,"Short Rural",66,"TransGrid Tumut 132/66kV STS","Gundagai South ZS",29.408000000000001,7.7289023182665417,7.5743242719012107,11,0,29.408000000000001,7.3454473416156203,7.1985383947833075,11,0,2.2662251088308295E-3,9]
[null,829,"Short Rural",66,"TransGrid Tumut 132/66kV STS","Tumut ZS",7.0000000000000007E-2,0,0,28,0,7.0000000000000007E-2,0,0,28,0,0,9]
[null,831,"Short Rural",66,"Gundagai South ZS","Nangus ZS",19.295000000000002,1.3561266600652375,1.3290041268639328,11,0,19.295000000000002,1.0329535324146966,1.0122944617664027,11,0,2.266225108830787E-3,9]
[null,"848/3","Short Rural",66,"TransGrid Tumut 132/66kV STS","Adelong Tee",2.8079999999999998,12.2,11.956,21,0,0,13.313623306678313,13.047350840544746,11,0,5.8736864341074127E-3,9]
[null,848,"Short Rural",66,"Adelong Tee","Adelong ZS",11.31,1.7333949790307546,1.6987270794501395,12,0,11.31,1.8363618354039051,1.7996345986958269,12,0,2.2662251088307822E-3,9]
[null,"848/1","Short Rural",66,"Adelong Tee","Batlow ZS",24.715,10.8,10.584,21,0,0,11.477261471274408,11.24771624184892,11,0,5.8736864341073954E-3,9]
[null,"848/2","Short Rural",66,"Batlow ZS","Tumbarumba ZS",32.944000000000003,8.4,8.2319999999999993,22,0,32.944000000000003,9.4113544064450139,9.2231273183161129,22,0,5.8736864341074127E-3,9]
[null,"830/1:PCR","Short Rural",66,"Bogalara Sw Stn","Parsons Creek ZS",29.579000000000001,0,0,11,0,0,0,0,0,0,0,9]
[null,"830/2:GUN","Short Rural",66,"Gundagai South ZS","Parsons Creek ZS",32.158000000000001,0.34667899580615097,0.33974541589002794,12,0,32.158000000000001,0.45909045885097627,0.44990864967395672,12,0,2.2662251088307736E-3,9]
[null,"850:TAL","Short Rural",66,"TransGrid Tumut 132/66kV STS","Talbingo ZS",42.497,1.5,1.47,18,0,46,14.231804224380264,13.947168139892659,18,0,5.8736864341073988E-3,9]
[null,"30-90","Short Rural",66,"Junee ZS","Coolamon ZS",40.122999999999998,5.3336574517326492,5.2269843026979963,6,0,40.122999999999998,5.7672095739620906,5.6518653824828489,6,0,0,9]
[null,"834:JUN","Short Rural",66,"Junee ZS","Bethungra ZS",25.347000000000001,1.6,1.5680000000000001,11,0,25.347000000000001,13.956647168988258,13.677514225608492,11,0,-7.7341947465516198E-4,10]
[null,"850:BET","Short Rural",66,"Bethungra ZS","Cootamundra ZS",24.565999999999999,0,0,12,0,24.565999999999999,0,0,12,0,0,9]
[null,"83F","Short Rural",66,"TransGrid Wagga North 132/66kV STS","Junee ZS",49.834999999999994,0,0,16,0,0,13.27641365917931,13.010885385995724,12,0,0,9]
[null,"9J5/2","Short Rural",132,"Temora 132/66 STS","Junee 132/66/11kV ZS",46.5,11.61821249266425,11.385848242810965,140,0,0,0,0,0,0,-6.5146579804560263E-3,10]
[null,"99U","Short Rural",132,"TransGrid Wagga North 132/66kV STS","Temora 132/66 STS",70.622,60.367955075519994,59.160595974009595,128,0,70.622,65.515500760209349,64.205190745005154,128,0,-0.12840452665131816,10]
[null,"83G","Urban",66,"TransGrid Wagga North 132/66kV STS","Bomen ZS",2.5140000000000002,23.086686621815161,22.624952889378857,34,0,1.806,20.761954466263528,20.346715376938256,34,0,1.2912615062834931E-3,9]
[null,"83J","Short Rural",66,"Bomen ZS","Cartwrights Hill ZS",5.1240000000000006,7.6213336698684921,7.4689069964711221,34,0,5.1240000000000006,9.6889120842563123,9.4951338425711853,34,0,2.7636897578333479E-2,9]
[null,"CHI2527","Short Rural",33,"Cartwrights Hill ZS","Euberta ZS",18.568999999999999,2.155763070461334,2.0695325476428805,4,0,18.568999999999999,2.1934944306470161,2.1057546534211355,4,0,-2.0650625099449166E-2,10]
[null,"Mates Gully/1","Short Rural",33,"Oura ZS","Mates Gully ZS",21.498000000000001,1.5,1.44,3,0,21.498000000000001,2.1338675423659734,2.0485128406713344,3,0,1.1475927445212515E-2,9]
[null,"Mates Gully/2","Short Rural",33,"Mates Gully ZS","Tarcutta ZS",13.092000000000001,0.9,0.86399999999999999,3,0,13.092000000000001,1.280320525419584,1.2291077044028005,3,0,-4.8550275690171837E-3,10]
[null,805,"Short Rural",66,"Wellington 132kV ZS","Mumbil ZS",20.8,1.2790646626674897,1.2534833694141398,11,0,20.8,1.6178594691071533,1.5855022797250102,11,0,9.0218852183221471E-3,9]
[null,"813:GUE","Short Rural",66,"Wellington 132kV ZS","Geurie Tee",15,0,0,12,0,15,1.3867366878061314,1.3590019540500087,12,0,0,9]
[null,"945/3","Short Rural",132,"TransGrid Line 945 Wellington 132kV Tee","Wellington 132kV ZS",0.1,10.432243224322432,10.223598359835984,124,0,0.1,12.249507408954161,12.004517260775078,124,0,-1.7774965871808163E-3,10]
[null,"947/1","Urban",132,"TransGrid Line 947 Burrendong Tee","Burrendong Hydro",8.7560000000000002,0,0,36,0,8.7560000000000002,21.263295879694013,20.838029962100133,36,0,0,9]
[null,"94F","Short Rural",132,"TransGrid Wellington 330/132kV STS","Dubbo 132/66kV STS",47.6,89.973610903840822,88.174138685764007,173,0,47.6,97.071568146429186,95.130136783500603,180,0,-2.1768204034273301E-3,10]
[null,"94J","Short Rural",132,"TransGrid Wellington 330/132kV STS","Dubbo 132/66kV STS",46.9,83.379566461157395,81.711975131934253,173,0,46.9,96.147077021225101,94.224135480800598,180,0,-2.1768204034273084E-3,10]
[null,"840/4","Short Rural",66,"Narrandra ZS","Kywong ZS",33.890999999999998,0.4,0.39200000000000002,16,0,33.890999999999998,0.34668417195153284,0.33975048851250217,16,0,2.1550446656868464E-3,9]
[null,"841:YNC","Short Rural",66,"TransGrid Yanco 132/66kV STS","Narrandra ZS",22.029,10.348139524551383,10.141176734060355,15,0,22.029,10.727009807569488,10.512469611418098,15,0,1.7175065110139863E-4,9]
[null,"YNC102","Short Rural",33,"TransGrid Yanco 132/66kV STS","Cudgel ZS",0,0.9,0.86399999999999999,8,0,0,0.98227182052934314,0.94298094770816943,8,0,1.7175065110141164E-4,9]
[null,"YNC52","Short Rural",33,"TransGrid Yanco 132/66kV STS","Whitton / Murrami Tee",22.338999999999999,4.3347821537782085,4.1613908676270803,8,0,22.338999999999999,5.5365211910036072,5.3150603433634629,8,0,1.7175065110137515E-4,9]
[null,"YNC72","Short Rural",33,"TransGrid Yanco 132/66kV STS","Yanco ZS",0,8.9001378263744062,8.5441323133194302,6,0,0,10.842353999048729,10.408659839086779,6,0,1.7175065110138868E-4,9]
[null,"YNC92","Short Rural",33,"TransGrid Yanco 132/66kV STS","Leeton ZS",6.16,14.452348159511601,13.874254233131136,22,0,0,20.242905604606936,19.433189380422657,10,0,1.7175065110138361E-4,9]
[null,824,"Short Rural",66,"TransGrid Yass 330/132/66kV STS","Yass ZS",3.7,12.512499999999999,12.26225,20,0,3.7,9.6505021255476642,9.4574920830367102,12,0,-1.8616041189553118E-4,10]
[null,"823/5","Long Rural",66,"Yass ZS","Marilba ZS",18.7,1.4,1.3719999999999999,12,0,18.7,1.0339823705943927,1.0133027231825049,12,0,-1.8616041189552463E-4,10]
[null,"823/3","Long Rural",66,"Bogalara Sw Stn","Marilba ZS",39.512,0,0,12,0,19.3,0,0,12,0,0,9]
[null,"971(2)","Urban",132,"TransGrid Yass 330/132/66kV STS","Cullerin Range Wind Farm",47.043999999999997,76.5,74.97,106,0,47.043999999999997,0,0,106,0,3.7012473859303655E-4,9]
[null,"971(1)","Short Rural",132,"Cullerin Range Wind Farm","Goulburn 132/66/33kV STS",31.809000000000001,0,0,106,0,31.809000000000001,0,0,106,0,0,9]
[null,"971(3)","Urban",132,"Cullerin Range Wind Farm","Gunning Wind Farm",13.821,46.5,45.57,140,0,13.821,0,0,140,0,1.1840512936520903E-5,9]
[null,"83M","Short Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Uranquinty ZS",18.974,7.3107676362764265,7.1645522835508979,28,0,0,16.756401644324086,16.421273611437606,15,0,-2.3902927611062056E-2,10]
[null,"83M/1","Short Rural",66,"Uranquinty","Henty",40.473999999999997,2.6075393154486592,2.5553885291396861,15,0,40.473999999999997,11.902823237002627,11.664766772262574,15,0,-2.3902927611062035E-2,10]
[null,"83M/2","Short Rural",66,"Henty","Culcairn",19.376999999999999,0,0,15,0,19.376999999999999,9.2449112520408736,9.0600130270000552,15,0,0,9]
[null,"83M/3","Short Rural",66,"Culcairn","Holbrook",20.09,3.4,3.3319999999999999,15,0,0,4.5068942353699271,4.4167563506625287,15,0,1.7247875385011868E-3,9]
[null,"8WO","Short Rural",66,"Ashmont ZS","Bourkelands ZS",4.2379999999999995,0.8,0.78400000000000003,34,0,4.2379999999999995,10.053840986594452,9.8527641668625616,34,0,-1.5694710022045411E-2,10]
[null,"845/6","Short Rural",66,"Bourkelands T","Bourkelands ZS",4.0380000000000003,9,8.82,34,0,4.0380000000000003,18.374261113431242,18.006775891162615,34,0,-2.3902927611062014E-2,10]
[null,"845/4","Short Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Bourkelands T",4.0380000000000003,9,8.82,34,0,4.0380000000000003,18.374261113431242,18.006775891162615,34,0,-2.3902927611062014E-2,10]
[null,"843/3","Short Rural",66,"Ashmont T","Ashmont ZS",3.46,20.078052728954674,19.67649167437558,34,0,3.46,6.4714378764286131,6.3420091189000409,34,0,-2.3902927611062059E-2,10]
[null,"843/2","Short Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Ashmont T",3.46,20.078052728954674,19.67649167437558,34,0,3.46,16.525278863023061,16.194773285762601,34,0,-2.3902927611062059E-2,10]
[null,"843/6","Short Rural",66,"Morrow St T","Cartwrights Hill ZS",7.6219999999999999,0,0,34,0,7.6219999999999999,0.11556139065051094,0.11325016283750071,34,0,0,9]
[null,"8WM","Urban",66,"Hammond Ave ZS","Morrow St ZS",2.3409999999999997,13.018381471202934,12.758013841778876,34,0,2.3409999999999997,6.5869992670791238,6.4552592817375416,34,0,-2.3902927611062053E-2,10]
[null,"83L","Urban",66,"Hammond Ave ZS","Bomen ZS",5.7059999999999995,0,0,54,0,5.7059999999999995,0,0,54,0,0,9]
[null,"No2 Forest","Urban",66,"TransGrid Wagga 132/66kV STS (Copland St)","Hammond Ave T",0.19800000000000001,34.88041428458348,34.182805998891808,52,0,0.19800000000000001,38.481943086620142,37.712304224887738,52,0,-1.9122342088849612E-2,10]
[null,"No2 Forest/1","Urban",66,"Hammond Ave T","Hammond Ave ZS",0.55300000000000005,11.3,11.074,52,0,0.55300000000000005,12.508927983895154,12.25874942421725,52,0,-1.9122342088849612E-2,10]
[null,"No2 Forest/2","Urban",66,"Hammond Ave T","Forest Hill T",0.76600000000000001,23.580414284583483,23.108805998891814,34,0,0.76600000000000001,26.335407978273565,25.808699818708092,34,0,-1.912234208884963E-2,10]
[null,"No2 Forest/3","Urban",66,"Forest Hill T","Kooringal ZS",4.5250000000000004,16.820127170457329,16.483724627048183,34,0,4.5250000000000004,18.811005698766834,18.434785584791499,34,0,-0.136929081502491,10]
[null,"No2 Forest/4","Urban",66,"Forest Hill T","Forest Hill ZS",6.9829999999999997,6.7602871141261529,6.6250813718436294,34,0,6.9829999999999997,7.5244022795067327,7.3739142339165982,34,0,-2.3902927611062039E-2,10]
[null,"83C","Short Rural",66,"TransGrid Wagga North 132/66kV STS","Oura ZS",8.1470000000000002,4.3360464284398814,4.2493254998710839,24,0,1.179,4.7333300871856672,4.6386634854419535,24,0,-2.9585878748494398E-3,10]
[null,"No 4 Hammond","Urban",66,"TransGrid Wagga 132/66kV STS (Copland St)","Hammond Ave ZS",0.76200000000000001,11.5,11.27,52,0,0.76200000000000001,39.059750039872696,38.278555039075243,52,0,-2.3902927611062018E-2,10]
[null,"840/1","Long Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Lockhart Tee",23.815000000000001,4.0851449275362324,4.0034420289855079,15,0,23.815000000000001,7.8581745642347451,7.7010110729500498,15,0,-1.912234208884963E-2,10]
[null,"840/2","Long Rural",66,"Lockhart Tee","Lockhart ZS",25.4,4.0561722684756916,3.9750488231061776,15,0,25.4,4.715051062193071,4.6207500409492095,15,0,-1.912234208884963E-2,10]
[null,"840/3","Short Rural",66,"Lockhart Tee","Kywong ZS",3.48,0,0,16,0,0,0,0,0,0,0,9]
[null,"845/1","Short Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Macleay St 4 Way",1.9370000000000001,0,0,54,0,1.9370000000000001,33.397241897997667,32.729297060037716,54,0,-1.9122342088849612E-2,10]
[null,"843/1","Short Rural",66,"TransGrid Wagga 132/66kV STS (Copland St)","Macleay St T",0.46500000000000002,0,0,54,0,0.46500000000000002,4.5068942353699271,4.4167563506625287,54,0,-1.9122342088849612E-2,10]
[null,"843/4","Short Rural",66,"Macleay St T","Macleay St ZS",1.5669999999999999,0,0,34,0,1.5669999999999999,4.7380170166709483,4.6432566763375291,34,0,0,9]
[null,"996/1","Short Rural",132,"TransGrid 132kV Line 996 Tee","Morven 132/66kV STS",0.04,8.2901554404145088,8.1243523316062181,45,0,0,0,0,0,0,-5.788589605629604E-3,10]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.2 - AUGEX MODEL INPUTS - ASSET STATUS - HIGH VOLTAGE FEEDERS"]
[null,"High voltage feeder ID","High voltage feeder type","Voltage level","Originating substation",null,{"$f":"CRCP_y4","v":"2017-18"},null,null,null,null,{"$f":"PRCP_y5","v":"2013-14"},null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from \", CRCP_y4, \" to \",dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual high voltage feeder maximum demand (50% PoE) from 2017-18 to 2018-19"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Route line length as at 30 June \",\"Route line length as at 31 December \"))","v":"Route line length as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,"Rating"]
[null,null,null,null,null,null,null,null,null,"Thermal","Operational",null,null,null,"Thermal","Operational"]
[null,null," CBD, urban, short rural, or long rural "," kV "," name ",null," km "," MVA "," MW "," MVA "," MVA "," km "," MVA "," MW "," MVA "," MVA "," % "]
[null,"ADA12","Short Rural",11,"ADA_11",0,132.012,0.75,0.74378435075202765,2.3941445492701559,2.2120020863462133,132.316,0.81799999999999995,0.80957459999999992,2.3941445492701559,2.2120020863462133,0,3]
[null,"ADE22","Short Rural",11,"ADE",0,156.423,0.63173528864153816,0.61591949266522472,2.0357659166760795,1.3889315425894828,156.53200000000001,0.49286282683004784,0.45979173114975158,2.0357659166760795,1.3889315425894828,-1.5659343892107227E-11,4]
[null,"ADE32","Short Rural",11,"ADE",0,37.494999999999997,1.2239871217429801,1.1933440170388729,2.0357659166760795,1.4889574767265854,37.649000000000001,1.045283508390872,0.97514498497784452,2.0357659166760795,1.4889574767265854,-1.5659343892107227E-11,4]
[null,"AFD2A04","Short Rural",22,"AFD",0,119.417,0.73920758372306583,0.70224720453691247,2.7835788528439425,1.9166874236557199,119.72199999999999,0.62603776817004297,0.61351701280664206,2.7835788528439425,1.9166874236557199,3.6805943253704038E-2,3]
[null,"AHY2T04","Long Rural",22,"AHY",0,398.238,1.22,1.2006434733635536,2.7835788528439425,2.7835788528439425,398.42899999999997,0.91400000000000003,0.87744,2.7835788528439425,2.7835788528439425,-2.0765092695678045E-3,6]
[null,"AHY2T05","Short Rural",22,"AHY",0,45.383000000000003,5.53,5.4422609899184033,5.5530588121142745,3.970553271270894,45.539000000000001,5.79,5.5583999999999998,5.5530588121142745,3.970553271270894,-2.0765092695678045E-3,4]
[null,"ALJ8B1","Urban",22,"ALJ",0,1.579,1.0714777237196065,1.070077507711672,16.042254579702941,16.042254579702941,1.8260000000000001,4.1979547115755684,3.9154323594865326,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B2","Urban",22,"ALJ",0,4.8710000000000004,6.4385192947835801,6.4301053841773426,16.042254579702941,16.042254579702941,4.6829999999999998,5.2018134469523352,4.8517314019724429,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B3","Short Rural",22,"ALJ",0,28.667999999999999,8.2436214059148085,8.2328485728447536,16.042254579702941,15.230615571276166,20.800999999999998,6.1144122972948498,5.7029123496869065,16.042254579702941,15.230615571276166,-8.8022447416971333E-3,4]
[null,"ALJ8B4","Urban",22,"ALJ",0,7.3490000000000002,4.0831988930936349,4.0778629347931279,16.042254579702941,16.042254579702941,7.3879999999999999,4.2892145966098196,4.0005504542579784,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B5","Urban",22,"ALJ",0,7.5369999999999999,7.6161794956285531,7.6062266088694512,16.042254579702941,16.042254579702941,7.7750000000000004,6.6619716075003588,6.2136209183155842,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B6","Urban",22,"ALJ",0,20.76,7.1721436821952027,7.1627710651330823,16.042254579702941,16.042254579702941,21.565000000000001,7.0270111476373645,6.5540932974013693,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B7","Urban",22,"ALJ",0,7.56,6.1778895782031356,6.1698162606799096,16.042254579702941,16.042254579702941,7.6929999999999996,5.2930733319865864,4.9368494967438892,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALJ8B8","Urban",22,"ALJ",0,20.085000000000001,6.6991490113640255,6.6903945076747773,16.042254579702941,16.042254579702941,21.303000000000001,8.2133896530826345,7.6606285294301726,16.042254579702941,16.042254579702941,-8.8022447416971333E-3,2]
[null,"ALU12","Short Rural",22,"ALU",0,13.625999999999999,3.8606299337827523,3.8596296526693079,16.042254579702941,16.042254579702941,13.587999999999999,4.6248200097312084,4.4587889713818578,16.042254579702941,16.042254579702941,3.3664286634431987E-3,3]
[null,"ALU22","Short Rural",22,"ALU",0,119.363,5.1069012473582527,5.1055780599630411,16.042254579702941,6.7674689153331187,116.965,3.3796761609574211,3.2583457867790493,16.042254579702941,6.7674689153331187,3.3664286634431987E-3,3]
[null,"ALU32","Long Rural",22,"ALU",0,663.50400000000002,7.8243349386131023,7.8223076698516314,16.042254579702941,10.743737954268987,515.38499999999999,7.8266184780066599,7.5456428746462203,16.042254579702941,10.739927442492339,3.3664286634431987E-3,5]
[null,"ALU42","Urban",22,"ALU",0,6.62,5.7534630566568197,5.7519723464537744,16.042254579702941,16.042254579702941,6.7889999999999997,5.9589027048459799,5.7449780977420088,16.042254579702941,16.042254579702941,3.3664286634431987E-3,1]
[null,"ALU52","Short Rural",22,"ALU",0,10.363,2.8205087623024476,2.8197779744016063,7.2399723756379064,7.2399723756379064,10.803000000000001,2.668165390229543,2.5723782527203025,7.2399723756379064,7.2399723756379064,3.3664286634431987E-3,3]
[null,"ALU62","Short Rural",22,"ALU",0,122.818,8.4990081309246523,8.4968060557550071,7.2399723756379064,7.2399723756379064,120.66200000000001,6.8482911682558276,6.6024375153154429,7.2399723756379064,7.2399723756379064,3.3664286634431987E-3,3]
[null,"ALU72","Urban",22,"ALU",0,19.635999999999999,6.4562476319813502,6.4545748317697891,18.862033294425075,15.971760111834888,19.881,6.2257192438689337,6.0022159230140391,18.671507705592497,15.971760111834888,3.3664286634431987E-3,1]
[null,"ALU82","Urban",22,"ALU",0,16.010999999999999,6.934141143202031,6.93234452178468,16.042254579702941,16.042254579702941,14.503,6.2257192438689337,6.0022159230140391,16.042254579702941,16.042254579702941,3.3664286634431987E-3,1]
[null,"ALU8B10","Long Rural",22,"ALU",0,210.50299999999999,4.6477486581462264,4.6465444362232446,18.862033294425075,14.960069235133908,208.34200000000001,4.0911869316852991,3.9443133208377965,18.862033294425075,14.960069235133908,3.3664286634431987E-3,5]
[null,"ALU92","Urban",22,"ALU",0,8.798,3.8887413167957336,3.887733752081949,7.2399723756379064,7.2399723756379064,9.016,3.2907373146164365,3.1725998450217063,7.2399723756379064,7.2399723756379064,3.3664286634431987E-3,1]
[null,"ANN8B1","Long Rural",22,"ANN",0,411.46199999999999,1.1175222264229063,1.1168762103450969,2.7835788528439425,1.4860995928940965,411.89600000000002,1.0008083145517588,1.0008083145517588,2.7835788528439425,1.377500007259528,-1.0324886230313706E-4,6]
[null,"ANN8B2","Long Rural",22,"ANN",0,359.23700000000002,0.67639503178228544,0.67600402205097976,6.3048727856476212,1.4060788455844144,359.90199999999999,0.71902733278475872,0.71902733278475872,6.3048727856476212,1.4060788455844144,-1.0324886230313706E-4,6]
[null,"APA3B1","Short Rural",11,"APA",0,188.33,0.41485559507670378,0.40491970213791878,3.5163402674940318,1.6575726228434156,188.47,0.33936680232709182,0.31418578559442162,3.5163402674940318,1.6575726228434156,4.6744261672422463E-4,3]
[null,"APA3B2","Short Rural",11,"APA",0,92.584999999999994,0.18767276920136602,0.1831779604909633,2.2863070659909179,1.2679477936807964,92.644999999999996,0.22326763310992884,0.20670117473317209,1.2679477936807964,1.2679477936807964,4.6744261672422463E-4,3]
[null,"APA3B3","Short Rural",11,"APA",0,195.03,0.37534553840273205,0.3663559209819266,3.583405274763098,1.6832935773358135,195.28700000000001,0.35722821297588614,0.33072187957307536,3.583405274763098,1.6832935773358135,4.6744261672422463E-4,3]
[null,"APA3B4","Short Rural",11,"APA",0,7.4930000000000003,0.43461062341368972,0.42420159271591495,2.2863070659909179,2.09863936099083,7.5620000000000003,0.35722821297588614,0.33072187957307536,2.09863936099083,2.09863936099083,4.6744261672422463E-4,3]
[null,"ARD No.1","Short Rural",11,"ARD",0,31.016999999999999,9.6925210259613176E-2,9.3909056031271101E-2,2.3394637052752065,1.50038901205654,31.027999999999999,0.10756699461821194,9.7036185845088996E-2,2.3394637052752065,1.50038901205654,7.7380018619637012E-12,3]
[null,"ARD No.2","Short Rural",11,"ARD",0,99.492000000000004,0.8141717661807506,0.78883607066267714,2.4440622535442911,1.0802800886807087,99.661000000000001,0.82142068617543662,0.74100360099886142,2.4440622535442911,1.4479944751275813,7.7380018619637012E-12,3]
[null,"ASM3B1","Urban",11,"ASM",0,4.1040000000000001,2.7643182554773995,2.6098759438944827,9.0880705873138989,9.0880705873138989,4.5739999999999998,3.3897444119118414,2.9887376479826706,9.0880705873138989,9.0880705873138989,1.4092152310280369E-3,1]
[null,"ASM3B10","Short Rural",11,"ASM",0,19.965,2.3171491259148786,2.1876901294409632,9.0880705873138989,9.0880705873138989,20.312999999999999,2.0798431789901564,1.833797730915621,9.0880705873138989,9.0880705873138989,1.4092152310280369E-3,3]
[null,"ASM3B2","Short Rural",11,"ASM",0,6.0389999999999997,2.3984526040171552,2.2644511866143304,9.0880705873138989,6.2606708490384646,6.8029999999999999,2.2698288539940648,2.0013081005665669,9.0880705873138989,6.7055480989625309,1.4092152310280369E-3,3]
[null,"ASM3B3","Short Rural",11,"ASM",0,12.699,3.9635445574859771,3.742101537201648,6.763658403556466,6.2273288709927632,13.826000000000001,3.939702944817892,3.4736360864459357,9.0880705873138989,8.6612932683289277,1.4092152310280369E-3,3]
[null,"ASM3B4","Short Rural",11,"ASM",0,10.115,3.3232796674305503,3.137608211961382,9.0880705873138989,9.0518707254357107,11.244999999999999,3.0897670303267222,2.7242475906390711,9.0880705873138989,9.048060213659058,1.4092152310280369E-3,3]
[null,"ASM3B7","Urban",11,"ASM",0,3.5979999999999999,3.9838704270115461,3.7612918014949899,9.0880705873138989,9.0880705873138989,3.899,2.9297790934813261,2.5831862267224852,9.0880705873138989,9.0880705873138989,1.4092152310280369E-3,1]
[null,"ASM3B8","Short Rural",11,"ASM",0,8.7919999999999998,2.3171491259148786,2.1876901294409632,6.763658403556466,6.763658403556466,9.2899999999999991,2.2498303618883901,1.9836754300769937,6.763658403556466,6.763658403556466,1.4092152310280369E-3,3]
[null,"ASM3B9","Short Rural",11,"ASM",0,12.526,3.3436055369561193,3.1567984762547239,9.0880705873138989,9.0880705873138989,13.266,3.2897519513834683,2.9005742955348039,9.0880705873138989,9.0880705873138989,1.4092152310280369E-3,3]
[null,"ATA3B1","Short Rural",11,"ATA",0,108.55800000000001,2.0180204941596611,1.917119469451678,2.7258495994276717,2.7258495994276717,115.581,1.8501817860346421,1.665163607431178,2.7258495994276717,2.7258495994276717,4.5163445077403279E-12,3]
[null,"ATA3B2","Short Rural",11,"ATA",0,166.77500000000001,1.8522893424653895,1.7596748753421199,2.7258495994276717,2.7258495994276717,166.88300000000001,1.4834790897034515,1.3351311807331063,2.7258495994276717,2.7258495994276717,4.5163445077403279E-12,3]
[null,"AVE3B1","Short Rural",11,"AVE",0,44.247999999999998,1.1998292931526036,1.1998029831261079,6.763658403556466,4.8355394445707915,44.643000000000001,0.87508030169223439,0.85757869565838973,6.763658403556466,4.8355394445707915,-4.5792596720635184E-9,4]
[null,"AVE3B2","Short Rural",11,"AVE",0,5.202,1.2216443712099236,1.2216175828193099,6.763658403556466,2.9588623945699131,5.3570000000000002,2.7893184616439974,2.7335320924111173,2.9588623945699131,2.9588623945699131,-4.5792596720635184E-9,4]
[null,"AVE3B3","Short Rural",11,"AVE",0,49.765000000000001,3.0977410841394488,3.097673156434678,6.763658403556466,5.7586359224646246,50.128,2.5523175466023504,2.5012711956703035,5.7586359224646246,5.7586359224646246,-4.5792596720635184E-9,4]
[null,"AVE3B4","Short Rural",11,"AVE",0,58.694000000000003,1.2216443712099236,1.2216175828193099,6.763658403556466,5.3518637903070747,58.524999999999999,0.91154198092941086,0.89331114131082268,5.3518637903070747,5.3518637903070747,-4.5792596720635184E-9,4]
[null,"AVE3B5","Short Rural",11,"AVE",0,9.5879999999999992,2.2796756569899466,2.2796256679396047,6.763658403556466,3.8219433119814847,9.3919999999999995,1.7501606033844688,1.7151573913167795,4.7374187663220146,4.7374187663220146,-4.5792596720635184E-9,4]
[null,"AVE3B6","Short Rural",11,"AVE",0,119.93,2.2251379618466465,2.2250891687065999,6.763658403556466,6.763658403556466,120.20399999999999,1.5678522071985868,1.5364951630546151,7.1809094430998091,7.1809094430998091,-4.5792596720635184E-9,4]
[null,"AVE3B7","Short Rural",11,"AVE",0,50.481999999999999,3.2613541695693495,3.261282654133693,6.1920816370587364,6.1920816370587364,50.484000000000002,2.7893184616439974,2.7335320924111173,6.1920816370587364,6.1920816370587364,-4.5792596720635184E-9,4]
[null,"BAL3B10","Urban",11,"BAL_11",0,3.5350000000000001,2.1043392487985155,2.0678742946145232,6.763658403556466,6.763658403556466,8.7059999999999995,3.6318414132492234,3.5592045849842386,6.763658403556466,6.763658403556466,1.0202722675691061E-2,1]
[null,"BAL3B11","Short Rural",11,"BAL_11",0,14.711,3.5072320813308591,3.446457157690872,8.9547026751310952,8.5841304048517344,14.518000000000001,3.2931204524280524,3.2272580433794915,6.763658403556466,6.763658403556466,1.0202722675691061E-2,3]
[null,"BAL3B12","Urban",11,"BAL_11",0,6.431,2.2446285320517498,2.2057325809221582,6.763658403556466,6.763658403556466,6.6349999999999998,2.352228894591466,2.3051843166996369,6.763658403556466,6.763658403556466,1.0202722675691061E-2,1]
[null,"BAL3B13","Short Rural",11,"BAL_11",0,14.845000000000001,2.1043392487985155,2.0678742946145232,6.1920816370587364,6.1920816370587364,8.8249999999999993,1.0537985447769769,1.0327225738814374,6.1920816370587364,6.1920816370587364,1.0202722675691061E-2,3]
[null,"BAL3B2","Short Rural",11,"BAL_11",0,13.403,2.684201619578551,2.6376885446860809,8.9547026751310952,8.9547026751310952,10.978,2.6721320242559052,2.618689383770787,8.9547026751310952,8.9547026751310952,1.0202722675691061E-2,3]
[null,"BAL3B3","Urban",11,"BAL_11",0,6.101,3.151832563755999,3.0972161657115307,8.9547026751310952,8.9547026751310952,6.125,3.5189344263088334,3.4485557377826566,6.763658403556466,6.763658403556466,1.0202722675691061E-2,1]
[null,"BAL3B4","Short Rural",11,"BAL_11",0,33.027999999999999,1.084903790491679,1.066104080779043,8.9547026751310952,7.4666978263486738,31.131,1.1855233628740989,1.1618128956166169,8.9547026751310952,7.4666978263486738,1.0202722675691061E-2,3]
[null,"BAL3B5","Short Rural",11,"BAL_11",0,21.706,3.0115432805027647,2.9593578794038957,6.763658403556466,6.763658403556466,22.393000000000001,3.2178491278011254,3.153492145245103,6.763658403556466,6.763658403556466,1.0202722675691061E-2,3]
[null,"BAL3B6","Short Rural",11,"BAL_11",0,42.408999999999999,0.67338855961552491,0.66171977427664741,6.763658403556466,6.763658403556466,41.290999999999997,0.60217059701541531,0.59012718507510697,6.763658403556466,6.763658403556466,1.0202722675691061E-2,3]
[null,"BAL3B7","Urban",11,"BAL_11",0,4.0309999999999997,2.8619013783659812,2.812309040675752,6.763658403556466,6.763658403556466,3.76,2.9355816604501497,2.8768700272411465,6.763658403556466,6.763658403556466,1.0202722675691061E-2,1]
[null,"BAL3B8","Urban",11,"BAL_11",0,4.1459999999999999,2.5813228118595122,2.5365924680604817,6.9732365512722998,6.9732365512722998,4.3819999999999997,2.5968606996289783,2.5449234856363985,6.9732365512722998,6.9732365512722998,1.0202722675691061E-2,1]
[null,"BAL3B9","Short Rural",11,"BAL_11",0,20.474,2.6000280496266099,2.5549735729014995,6.763658403556466,6.763658403556466,20.731000000000002,2.9732173227636132,2.913752976308341,6.763658403556466,6.763658403556466,1.0202722675691061E-2,3]
[null,"BAR12","Short Rural",22,"BAR",0,40.383000000000003,0.68623343515007273,0.66078185149262991,4.2597711151187454,3.0465041654328986,40.182000000000002,0.79190579544863937,0.73053309630136976,4.2597711151187454,3.0465041654328986,-3.8595147731386808E-3,4]
[null,"BAR22","Long Rural",22,"BAR",0,546.21,1.6523778767429382,1.5910931424098851,4.8881245070885821,2.9074204855851171,543.72799999999995,2.8217851890273637,2.603096836877743,4.8881245070885821,2.8921784384785116,-3.8595147731386808E-3,6]
[null,"BAR32","Short Rural",22,"BAR",0,133.85599999999999,0.96614444159286561,0.93031129091725528,4.2597711151187454,2.9112309973617689,133.57599999999999,1.0655060873767326,0.98292936560503574,2.8845574149252085,2.8845574149252085,-3.8595147731386808E-3,4]
[null,"BAR42","Short Rural",22,"BAR",0,20.643999999999998,2.96163903591084,2.851795359073455,4.7882890985403117,3.9210166181744244,21.465,2.997864584822671,2.7655300794989142,3.9591217359409399,3.9591217359409399,-3.8595147731386808E-3,4]
[null,"BAT12","Short Rural",11,"BAT",0,49.597000000000001,0.65039630982119678,0.63967838525039078,3.5163402674940318,0.16099412256352716,48.529000000000003,0.39950701960237622,0.37749418282228525,3.5163402674940318,0.16099412256352716,-2.1618055414211541E-2,4]
[null,"BAT22","Urban",11,"BAT",0,1.881,0.68291612531225654,0.67166230451291031,3.5163402674940318,0.18576244911176207,2.359,0.58389487480347291,0.55172226720180151,3.5163402674940318,0.18576244911176207,-2.1618055414211541E-2,2]
[null,"BAT32","Short Rural",11,"BAT",0,72.569000000000003,0.56096681722078212,0.55172260727846201,2.7765294060571373,0.1143153532995459,72.668999999999997,0.23048481900137086,0.21778510547439531,2.7765294060571373,0.1143153532995459,-2.1618055414211541E-2,4]
[null,"BAT42","Short Rural",11,"BAT",0,6.8220000000000001,0.89429492600414551,0.87955777971928728,2.0357659166760795,0.18195193733511056,6.7960000000000003,0.81437969380484376,0.76950737267619684,2.0357659166760795,0.18195193733511056,-2.1618055414211541E-2,4]
[null,"BBA3B1","Long Rural",11,"BBA",0,367.50099999999998,0.57929391985472323,0.55934348241177889,2.1298855575593727,2.0910183374375269,367.79300000000001,0.57331250178222004,0.53891375167528677,2.1298855575593727,2.0910183374375269,9.5640258909984255E-4,5]
[null,"BBA3B2","Short Rural",11,"BBA",0,140.61600000000001,0.19621245672498691,0.18945505049431219,1.7337828583764461,1.7337828583764461,140.66,0.20930456414271528,0.19674629029415236,1.7337828583764461,1.7337828583764461,9.5640258909984255E-4,3]
[null,"BBA3B3","Long Rural",11,"BBA",0,237.85900000000001,0.55126356889401085,0.53227847519830573,1.3504453736453019,1.224126908249304,237.947,0.50051091425431915,0.47048025939905996,1.3504453736453019,1.224126908249304,9.5640258909984255E-4,5]
[null,"BBA3B4","Short Rural",11,"BBA",0,72.921999999999997,1.4388913493165707,1.3893370369582894,1.7337828583764461,1.7337828583764461,73.498999999999995,1.4560317505580194,1.3686698455245381,1.7337828583764461,1.7337828583764461,9.5640258909984255E-4,3]
[null,"BBI0101","Long Rural",11,"BBI",0,263.90699999999998,1.52,1.4974651569732531,2.1298855575593727,2.0748236623867582,263.76100000000002,1.79,1.7183999999999999,2.1298855575593727,2.0748236623867582,3.2263901545654818E-2,5]
[null,"BBI0201","Short Rural",11,"BBI",0,140.94399999999999,0.253,0.24924913468041646,1.7337828583764461,1.7337828583764461,141.029,0.44,0.4224,1.7337828583764461,1.7337828583764461,3.2263901545654818E-2,3]
[null,"BBI0301","Short Rural",11,"BBI",0,96.677999999999997,1.22,1.2019128233601111,2.1298855575593727,2.1298855575593727,94.625,0.66,0.63360000000000005,2.1298855575593727,2.1298855575593727,3.2263901545654818E-2,3]
[null,"BBI0401","Short Rural",11,"BBI",0,184.87799999999999,0.38,0.37436628924331328,3.5163402674940318,3.0074464197222204,183.61600000000001,1.81,1.7376,3.5163402674940318,3.0074464197222204,3.2263901545654818E-2,3]
[null,"BBI1101","Short Rural",11,"BBI",0,99.977000000000004,1.62,1.5959826015109673,3.4774730473721855,1.4756206855083052,100.041,3.23,3.1008,3.4774730473721855,1.4756206855083052,3.2263901545654818E-2,3]
[null,"BBI2601","Short Rural",11,"BBI",0,4.7759999999999998,0.78,0.76843606739416936,2.1298855575593727,2.1298855575593727,5.0250000000000004,0.89500000000000002,0.85919999999999996,2.1298855575593727,2.1298855575593727,3.2263901545654818E-2,3]
[null,"BBI2801","Short Rural",11,"BBI",0,7.1840000000000002,0.91,0.89650874529319757,2.1298855575593727,2.1298855575593727,7.44,0.72399999999999998,0.69503999999999999,2.1298855575593727,2.1298855575593727,3.2263901545654818E-2,3]
[null,"BBN3B1","Short Rural",11,"BBN",0,4.5149999999999997,1.06,1.0487365920122975,9.0880705873138989,7.0561151824144712,4.5659999999999998,1,0.87385000000000024,9.0880705873138989,7.0561151824144712,2.0492676826217446E-2,3]
[null,"BBN3B2","Urban",11,"BBN",0,0.82699999999999996,0.87,0.86075550476481011,9.0880705873138989,9.0880705873138989,1.081,0.84,0.73403400000000019,9.0880705873138989,9.0880705873138989,2.0492676826217446E-2,1]
[null,"BBN3B3","Short Rural",11,"BBN",0,8.2070000000000007,1.86,1.8402359067385596,9.0880705873138989,9.0880705873138989,8.3070000000000004,1.81,1.5816685000000004,9.0880705873138989,9.0880705873138989,2.0492676826217446E-2,3]
[null,"BBN3B5","Urban",11,"BBN",0,6.0830000000000002,2.59,2.5624790314262738,9.0880705873138989,9.0880705873138989,6.1020000000000003,2.42,2.1147170000000006,9.0880705873138989,9.0880705873138989,2.0492676826217446E-2,1]
[null,"BBN3B6","Urban",11,"BBN",0,0.47399999999999998,6.22,6.1539071719966882,9.0880705873138989,9.0880705873138989,0.47499999999999998,6.08,5.3130080000000017,9.0880705873138989,9.0880705873138989,2.0492676826217446E-2,1]
[null,"BBN3B7","Short Rural",11,"BBN",0,6.3920000000000003,1.1299999999999999,1.1179927820508453,9.0880705873138989,8.3707417453592488,6.56,1.35,1.1796975000000003,9.0880705873138989,8.3707417453592488,2.0492676826217446E-2,3]
[null,"BBS3B10","Urban",11,"BBS_11",0,4.7750000000000004,1.6102860916084603,1.5847169551993443,5.0489281040632772,5.0489281040632772,5.056,2.7010063119055268,2.6199761225483611,5.0489281040632772,5.0489281040632772,3.2595032079466096E-2,1]
[null,"BBS3B3","Short Rural",11,"BBS_11",0,23.59,1.1132842114823922,1.095606783841522,5.0489281040632772,3.8800536165754207,23.696000000000002,0.69454448020427839,0.67370814579814997,5.0489281040632772,3.8800536165754207,3.2595032079466096E-2,3]
[null,"BBS3B4","Short Rural",11,"BBS_11",0,23.218,1.6301661668135028,1.6042813620536569,6.1920816370587364,3.9686480153825685,23.338000000000001,0.9260593069390376,0.89827752773086644,6.1920816370587364,3.9686480153825685,3.2595032079466096E-2,3]
[null,"BBS3B5","Short Rural",11,"BBS_11",0,9.1539999999999999,1.799146806056366,1.7705788203153165,7.2399723756379064,5.1832486441902441,10.993,3.7042372277561504,3.5931101109234658,7.2399723756379064,5.1832486441902441,3.2595032079466096E-2,3]
[null,"BBS3B6","Short Rural",11,"BBS_11",0,13.554,3.4790131608824755,3.4237711995047557,9.0880705873138989,5.8815249272616379,8.3699999999999992,3.2412075742866322,3.1439713470580331,9.0880705873138989,5.8815249272616379,3.2595032079466096E-2,3]
[null,"BBS3B7","Short Rural",11,"BBS_11",0,5.4589999999999996,1.5307657907882892,1.5064593277820926,6.1920816370587364,5.0251124054592049,5.7119999999999997,1.0804025247622109,1.0479904490193446,6.1920816370587364,5.0251124054592049,3.2595032079466096E-2,3]
[null,"BBS3B8","Urban",11,"BBS_11",0,2.3290000000000002,6.9580263217649513E-2,6.8475423990095124E-2,9.0880705873138989,5.6043101955102381,2.331,3.179470287157363,3.0840861785426421,9.0880705873138989,5.6043101955102381,3.2595032079466096E-2,1]
[null,"BBS3B9","Short Rural",11,"BBS_11",0,2.65,0.18886071444790581,0.18586186511597244,6.763658403556466,5.9948876526170203,2.4969999999999999,0.32412075742866325,0.31439713470580333,6.763658403556466,5.9948876526170203,3.2595032079466096E-2,3]
[null,"BBYF2","Short Rural",11,"BBY",0,69.45,3.7020789720163569,3.6952772326455472,9.0880705873138989,8.0135062662981689,65.41,2.7880232673414516,2.7874656626879832,6.4778700203076003,6.4778700203076003,4.2205517178034941E-3,3]
[null,"BBYG2","Urban",11,"BBY",0,10.756,3.9943483645439639,3.9870096457491426,6.4778700203076003,6.4778700203076003,11.138,2.9744119421969701,2.9738170598085309,6.4778700203076003,6.4778700203076003,4.2205517178034941E-3,1]
[null,"BBYH2","Short Rural",11,"BBY",0,116.22499999999999,3.5072327103312855,3.5007889572431496,6.4778700203076003,6.2873444314750238,115.218,2.41622177456683,2.4157385302119168,6.4778700203076003,6.2873444314750238,4.2205517178034941E-3,3]
[null,"BBYJ2","Urban",11,"BBY",0,8.8670000000000009,2.2407320093783212,2.2366151671275678,6.4778700203076003,6.4778700203076003,20.879000000000001,4.0898164205208341,4.0889984572367304,6.4778700203076003,6.4778700203076003,4.2205517178034941E-3,1]
[null,"BBYK2","Urban",11,"BBY",0,5.1289999999999996,4.0917714953865003,4.0842537834503423,6.4778700203076003,6.4778700203076003,5.306,4.2762050953763522,4.2753498543572768,6.4778700203076003,6.4778700203076003,4.2205517178034941E-3,1]
[null,"BBYL2","Short Rural",11,"BBY",0,28.431000000000001,5.2608490654969291,5.2511834358647258,6.4778700203076003,6.4778700203076003,29.643000000000001,3.9414861661855514,3.9406978689523142,6.4778700203076003,6.4778700203076003,4.2205517178034941E-3,3]
[null,"BBYM2","Short Rural",11,"BBY",0,14.791,3.2149633178036781,3.2090565441395538,8.9547026751310952,8.9547026751310952,0,"","","","",4.2205517178034941E-3,3]
[null,"BCW","Urban",11,"BCW",0,12.839,7.76,6.2080000925064089,8.8022822040650333,8.8022822040650333,10,5.48,4.6508760000000002,8.8022822040650333,8.8022822040650333,-4.0659757437604267E-5,2]
[null,"BDA2D06","Short Rural",22,"BDA",0,188.077,0.41730634847469206,0.28618917222445972,5.5530588121142745,1.8328561645693859,188.483,0.52109015980427731,0.49503565181406339,5.5530588121142745,1.8328561645693859,-1.4288845607839393E-2,4]
[null,"BDA2D08","Long Rural",22,"BDA",0,267.82600000000002,0.43545010275620033,0.29863217971247963,5.5530588121142745,1.8176141174627798,267.86599999999999,0.52109015980427731,0.49503565181406339,5.5530588121142745,1.8176141174627798,-1.4288845607839393E-2,6]
[null,"BEE1341","Short Rural",11,"BEE",0,15.484999999999999,3.2866507032184646,3.0548916253045397,9.011860351780868,4.0524792744689027,15.670999999999999,3.0051539167987666,2.7953941734062129,9.011860351780868,4.0524792744689027,9.888320294012631E-3,3]
[null,"BEE1342","Short Rural",11,"BEE",0,38.85,1.6384490152543085,1.5229133324960313,9.011860351780868,3.4656604608645667,38.783000000000001,1.3577502636139007,1.2629792952136505,9.011860351780868,3.4656604608645667,9.888320294012631E-3,3]
[null,"BEE1346","Short Rural",11,"BEE",0,32.533000000000001,1.0435359799536372,0.96995075343497261,9.011860351780868,3.4208869474889112,32.673999999999999,1.1224068845874913,1.0440628840432844,9.011860351780868,3.4208869474889112,9.888320294012631E-3,3]
[null,"BEE1347","Urban",11,"BEE",0,9.3940000000000001,4.1058752108456185,3.8163482915525551,6.9732365512722998,4.9279443551545921,10.818,5.0689343174918955,4.7151227021309614,6.9732365512722998,4.9279443551545921,9.888320294012631E-3,1]
[null,"BERA2","Short Rural",11,"BER",0,6.6909999999999998,1.2436810099317746,1.2338365424652087,2.1298855575593727,2.1298855575593727,6.74,1.1234579681787313,1.1168295661664769,2.1298855575593727,2.1298855575593727,1.2677560132266734E-8,3]
[null,"BERB2","Short Rural",11,"BER",0,33.412999999999997,1.2436810099317746,1.2338365424652087,2.1298855575593727,1.721398695102329,34.066000000000003,1.1234579681787313,1.1168295661664769,2.1298855575593727,1.721398695102329,1.2677560132266734E-8,3]
[null,"BERC2","Short Rural",11,"BER",0,36.189,0.23096933041590101,0.22914107217211022,2.1298855575593727,1.7614090687571697,36.161000000000001,0.16981464912805008,0.16881274269819457,2.1298855575593727,1.7614090687571697,1.2677560132266734E-8,3]
[null,"BERD2","Short Rural",11,"BER",0,42.774999999999999,0.52412271132839072,0.51997397146748081,2.4440622535442911,1.6861514611683019,42.442999999999998,0.51033770869535056,0.50732671621404801,2.4440622535442911,1.6861514611683019,1.2677560132266734E-8,3]
[null,"BET1","Short Rural",11,"BET",0,12.349,0.50896551191942152,0.47786463991316797,1.8397150857673588,1.2022164655335579,12.353,0.56051444082701773,0.52497782527858483,1.8397150857673588,1.2022164655335579,-2.1608159752800993E-2,4]
[null,"BET2","Short Rural",11,"BET",0,111.29,0.31935090943963701,0.29983663680826222,1.8397150857673588,0.80497061281763571,111.346,0.34200881135207861,0.32032545271235685,1.8397150857673588,0.80497061281763571,-2.1608159752800993E-2,4]
[null,"BFTCB4","Urban",11,"BFT",0,1.9179999999999999,0.9,0.8934539723809708,3.4751867403061953,3.4751867403061953,2.64,0.79900000000000004,0.75905,3.4751867403061953,3.4751867403061953,8.2778654621569071E-3,1]
[null,"BGA2K09","Long Rural",22,"BGA",0,210.227,0.42362723065778091,0.40244586912489183,4.0715318333521591,1.2974792599498461,211.08699999999999,0.37461731556729028,0.36712496925594446,4.0715318333521591,1.2974792599498461,2.4003459312308251E-9,5]
[null,"BGA2K13","Short Rural",22,"BGA",0,133.83099999999999,0.46397268119661722,0.44077404713678636,4.0715318333521591,1.3184370747214293,133.58000000000001,0.41029515514512749,0.40208925204222495,4.0715318333521591,1.3184370747214293,2.4003459312308251E-9,3]
[null,"BGA2K17","Short Rural",22,"BGA",0,149.56899999999999,2.2290861422707042,2.117631835157169,5.5530588121142745,1.2803319569549141,150.33000000000001,1.76605305910294,1.7307319979208811,5.5530588121142745,1.2803319569549141,2.4003459312308251E-9,3]
[null,"BHL32","Short Rural",22,"NBKG",0,40.518000000000001,9.1115787134781989,8.7145614051890057,7.166810549526196,7.166810549526196,40.765000000000001,5.490938319417606,5.1439110176304128,7.166810549526196,7.166810549526196,5.3076948014376714E-3,3]
[null,"BHL42","Urban",22,"NBKG",0,41.481000000000002,12.105880700971833,11.578393168733282,7.166810549526196,7.166810549526196,35.222999999999999,11.863368344041717,11.113603464698281,7.166810549526196,7.166810549526196,5.3076948014376714E-3,1]
[null,"BHL52","Urban",22,"NBKG",0,6.8559999999999999,8.18,8.1366530475637653,7.166810549526196,7.166810549526196,5.641,1.802,1.802,7.166810549526196,7.166810549526196,-2.6609529967382993E-5,2]
[null,"BHL72","Short Rural",22,"NBKG",0,98.71,9.9968085417679173,9.5612192609702706,7.166810549526196,7.166810549526196,93.787999999999997,11.711387015557838,10.971227356174582,7.166810549526196,7.166810549526196,5.3076948014376714E-3,3]
[null,"BHL82","Long Rural",22,"NBKG",0,229.95099999999999,6.3339887276642353,6.0579988872130404,7.166810549526196,7.166810549526196,228.88499999999999,9.5640379227855945,8.9595907260655441,7.166810549526196,7.166810549526196,5.3076948014376714E-3,5]
[null,"BJK12","Short Rural",11,"BJK",0,6.32,0.26,0.247,2.0576763593918264,2.0576763593918264,6.6230000000000002,0.248,0.23559999999999998,5.2394536928958528,5.2394536928958528,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"BJN8B1","Short Rural",22,"BJN",0,3.37,0.24991999919203178,0.24903717024264438,3.330387292793437,3.330387292793437,3.4660000000000002,0.32679551366210896,0.32352755852548787,3.330387292793437,3.330387292793437,-5.7100833642474537E-3,4]
[null,"BJN8B2","Long Rural",22,"BJN",0,272.15800000000002,0.70720396056197221,0.70470580062469634,3.330387292793437,2.2958333454325466,273.87900000000002,0.83461478124783517,0.82626863343535684,3.330387292793437,2.2958333454325466,-5.7100833642474537E-3,6]
[null,"BJN8B3","Long Rural",22,"BJN",0,327.76900000000001,0.58959454917748666,0.58751183815756958,2.7008907472906039,2.2577282276660311,356.61599999999999,0.79841003046311165,0.79042593015848051,2.7008907472906039,2.2577282276660311,-5.7100833642474537E-3,6]
[null,"BJN8B4","Short Rural",22,"BJN",0,92.885999999999996,0.18569907060708241,0.18504309863230539,7.2399723756379064,3.8829115004079089,93.5,0.36204750784723444,0.35842703276876209,7.2399723756379064,3.8829115004079089,-5.7100833642474537E-3,4]
[null,"BJN8B5","Long Rural",22,"BJN",0,241.81,0.44103529269182074,0.43947735925172532,7.2399723756379064,1.4594260104575363,242.51300000000001,0.50496099778693226,0.49991138780906291,7.2399723756379064,1.4594260104575363,-5.7100833642474537E-3,6]
[null,"BKE4B1","Long Rural",33,"BKE_33",0,555.80700000000002,0.74299999999999999,0.55226755066164457,4.3811359152050962,2.8407365294937157,556.23299999999995,0.46200000000000002,0.20535900000000001,4.3811359152050962,2.8435944133262043,0,5]
[null,"BKE4B2","Long Rural",33,"BKE_33",0,1828.2929999999999,1.82,1.3527953461698428,4.3811359152050962,1.2831898407874029,1828.6279999999999,0.99,0.44005500000000003,4.3811359152050962,1.2917634922848689,0,5]
[null,"BKE4B3","Long Rural",33,"BKE_33",0,611.26,0.81100000000000005,0.60281155260645203,7.3321867606328732,1.3031950276148232,607.87400000000002,0.42899999999999999,0.19069050000000001,7.3321867606328732,1.3060529114473121,0,5]
[null,"BKE8B1","Short Rural",22,"BKE_22",0,25.335000000000001,2.4380000000000002,2.3733447767012654,4.2597711151187454,1.8671507705592496,26.091000000000001,0.68200000000000005,0.6496050000000001,4.2597711151187454,0.91452282639636717,4.1355205294676698E-5,3]
[null,"BKE8B2","Short Rural",22,"BKE_22",0,92.253,0.26600000000000001,0.25894573855723402,4.2597711151187454,1.5394467577672182,92.287000000000006,0.154,0.14668500000000001,4.2597711151187454,0.76019709944198044,4.1355205294676698E-5,3]
[null,"BKE8B3","Short Rural",22,"BKE_22",0,52.5,6.4020000000000001,6.2322203693361358,3.4675657167528922,1.9090664001024165,52.966000000000001,2.3959999999999999,2.2821899999999999,3.4675657167528922,0.8821334762948293,4.1355205294676698E-5,3]
[null,"BLH3B1","Short Rural",11,"BLH",0,72.531000000000006,0.35137358267987512,0.31052486446641026,2.4440622535442911,2.1662759450263946,72.561999999999998,0.29728558433408575,0.24971989084063201,2.4440622535442911,2.1557970376406033,1.207014535833777E-10,3]
[null,"BLH3B2","Short Rural",11,"BLH",0,54.173000000000002,1.7568679133993754,1.5526243223320513,2.7258495994276717,1.7899879070820561,53.74,1.4467898437592175,1.2153034687577426,2.7258495994276717,1.7899879070820561,1.207014535833777E-10,3]
[null,"BLH3B3","Long Rural",11,"BLH",0,227.81800000000001,2.0906728169452569,1.847622943575141,1.6651936463967185,1.6651936463967185,228.03,1.8233515839157264,1.5316153304892102,1.6651936463967185,1.6651936463967185,1.207014535833777E-10,5]
[null,"BMR668","Short Rural",11,"BMR",0,100.53700000000001,0.17123219633776596,0.16501334635609186,1.3466348618686506,0.75448133177700294,100.627,0.24005652349386897,0.23525539302399159,1.3466348618686506,0.80306535692931003,8.8022419959372464E-3,3]
[null,"BMR669","Short Rural",11,"BMR",0,55.433,0.28839106751623744,0.27791721491552318,1.5693592752139327,0.81640214814759027,55.612000000000002,0.36931772845210609,0.36193137388306396,1.5693592752139327,0.81640214814759027,8.8022419959372464E-3,3]
[null,"BMR670","Short Rural",11,"BMR",0,148.94200000000001,0.18024441719764839,0.17369825932220198,2.1298855575593727,0.79544433337600684,149.00200000000001,0.38778361487471147,0.38002794257721723,2.1298855575593727,0.79544433337600684,8.8022419959372464E-3,3]
[null,"BMU1417","Long Rural",11,"BMU",0,360.53199999999998,1.7669904118516471,1.586843591869477,2.2965954477878769,1.5832676431987109,308.36399999999998,1.4918254843137915,1.2680516616667228,2.2965954477878769,1.5832676431987109,-2.0631382200464905E-11,6]
[null,"BNG8B1","Long Rural",22,"BNG",0,267.86099999999999,4.5932759321579848,4.3152811184531314,12.536583745183533,8.1792635285825082,271.37,5.1182290743691263,4.7456219977550544,12.536583745183533,11.677313339548613,-7.1706297624718847E-3,6]
[null,"BNG8B2","Short Rural",22,"BNG",0,19.12,3.9937111534028502,3.7520032733453115,12.536583745183533,11.271493835335226,16.757000000000001,1.2598717721524004,1.1681531071397058,12.536583745183533,12.536583745183533,-7.1706297624718847E-3,4]
[null,"BNG8B4","Short Rural",22,"BNG",0,39.756999999999998,7.6012619408278166,7.1412174261127044,12.536583745183533,12.536583745183533,15.627000000000001,1.3090855132521035,1.2137840878873505,12.536583745183533,12.536583745183533,-7.1706297624718847E-3,4]
[null,"BNK24787","Short Rural",11,"BNK",0,19.167999999999999,0.83683529061646778,0.82416002602659344,2.7765294060571373,2.7740525734023134,18.646999999999998,0.70494467868053301,0.63445021081247976,2.7765294060571373,2.7740525734023134,1.4037803698992235E-2,3]
[null,"BNK24792","Short Rural",11,"BNK",0,17.302,3.5224927349204811,3.4691387142049637,3.5163402674940318,3.1674879143415842,17.923999999999999,3.1436722157375123,2.8293049941637611,3.5163402674940318,3.1674879143415842,1.4037803698992235E-2,3]
[null,"BNK24796","Short Rural",11,"BNK",0,89.003,1.2065997213539768,1.1883237584569486,2.7765294060571373,2.3196490440366189,88.957999999999998,1.1812586507619742,1.0631327856857768,2.7765294060571373,2.3196490440366189,1.4037803698992235E-2,3]
[null,"BNK24798","Short Rural",11,"BNK",0,76.518000000000001,1.0411787918135122,1.0254084044749476,6.763658403556466,2.2510598320568915,77.010999999999996,0.83831259086333665,0.75448133177700305,6.763658403556466,2.1853285039096524,1.4037803698992235E-2,3]
[null,"BNY3B1","Short Rural",11,"BNY",0,116.402,1.1599999999999999,1.1511577169041836,7.2399723756379064,5.5509630306371163,90.58,0.42,0.41516999999999998,7.2399723756379064,5.5433420070838126,-6.1674117608842369E-3,4]
[null,"BNY3B2","Short Rural",11,"BNY",0,79.921000000000006,1.43,1.4190995992870539,6.763658403556466,5.2204011340125964,80.409000000000006,1.33,1.3147050000000002,6.763658403556466,5.2204011340125964,-6.1674117608842369E-3,4]
[null,"BNY3B3","Short Rural",11,"BNY",0,5.0190000000000001,0.95,0.94275847505083998,6.763658403556466,6.763658403556466,4.758,0.48,0.47448000000000001,6.763658403556466,6.763658403556466,-6.1674117608842369E-3,4]
[null,"BNY3B4","Long Rural",11,"BNY",0,203.58,3.14,3.1160648543785658,5.2394536928958528,5.2394536928958528,203.36500000000001,1.91,1.8880349999999999,5.2394536928958528,5.2394536928958528,-6.1674117608842369E-3,6]
[null,"BNY3B5","Short Rural",11,"BNY",0,3.1030000000000002,0.56999999999999995,0.56565508503050399,8.8022822040650333,8.1725951329733704,3.117,0.61,0.60298499999999999,8.8022822040650333,8.1725951329733704,-6.1674117608842369E-3,4]
[null,"BNY3B6","Short Rural",11,"BNY",0,69.14,2.67,2.6496475035639397,5.2394536928958528,4.6840716014488937,69.858000000000004,2.1,2.07585,5.2394536928958528,5.2394536928958528,-6.1674117608842369E-3,4]
[null,"BNY3B7","Urban",11,"BNY",0,3.3410000000000002,5.14,5.1008195386961237,8.8022822040650333,7.0180100646479557,3.3570000000000002,4.76,4.70526,8.8022822040650333,7.0180100646479557,-6.1674117608842369E-3,2]
[null,"BODA2","Short Rural",11,"BOD",0,42.637,0.67561318324502651,0.67106445117638602,3.5163402674940318,1.4375155677417897,43.46,0.77225556340272572,0.70321591603452205,3.5163402674940318,1.4365629397976269,5.4256278117838511E-8,3]
[null,"BODB2","Short Rural",11,"BOD",0,39.054000000000002,0.33780659162251325,0.33553222558819301,3.5163402674940318,1.4013157058635999,38.814999999999998,0.29442243354728914,0.26810106798816147,3.5163402674940318,1.4013157058635999,5.4256278117838511E-8,3]
[null,"BODC2","Short Rural",11,"BOD",0,31.428000000000001,0.93835164339587018,0.93203395996720284,3.5163402674940318,1.6375674360159951,31.488,0.84561984192598461,0.7700214280578016,3.5163402674940318,1.6375674360159951,5.4256278117838511E-8,3]
[null,"BOM8B1","Urban",22,"BOM",0,6.3890000000000002,3.7,3.6958341428507206,12.536583745183533,3.4980498109661049,6.4139999999999997,2.702,2.6330990000000001,12.536583745183533,2.6787897789860255,2.1459260890154163E-2,1]
[null,"BOM8B2","Short Rural",22,"BOM",0,145.39400000000001,0.38,0.37957215521169557,4.0715318333521591,3.4332711107630289,450.59399999999999,1.446,1.409127,4.0715318333521591,2.0900657094933641,2.1459260890154163E-2,3]
[null,"BOM8B3","Long Rural",22,"BOM",0,474.346,1.3,1.2985363204610638,4.0715318333521591,3.3246715251284598,471.46699999999998,1.256,1.2239720000000001,4.0715318333521591,2.0786341741634096,2.1459260890154163E-2,5]
[null,"BOM8B4","Short Rural",22,"BOM",0,22.393000000000001,1.3,1.2985363204610638,4.0715318333521591,4.0715318333521591,21.908000000000001,1.218,1.186941,4.0715318333521591,3.8200380560931584,2.1459260890154163E-2,3]
[null,"BOM8B5","Short Rural",22,"BOM",0,84.126999999999995,0.31,0.3096509687253306,4.0715318333521591,3.0579357007628527,83.95,0.28500000000000003,0.27773250000000005,4.0715318333521591,2.0367185446202432,2.1459260890154163E-2,3]
[null,"BON3B1","Short Rural",11,"BON",0,17.994,0.39111414073713707,0.35200272666342336,1.3350128009498634,0.92785961761464764,17.702999999999999,0.26213865813283099,0.24903172522618944,1.3350128009498634,0.92785961761464764,7.1546892405346021E-2,3]
[null,"BON3B2","Short Rural",11,"BON",0,109.718,0.52491634677878918,0.47242471210091025,1.3350128009498634,0.8821334762948293,109.67400000000001,0.45196320367729487,0.42936504349343008,1.3350128009498634,0.8821334762948293,7.1546892405346021E-2,3]
[null,"BON3B3","Short Rural",11,"BON",0,39.677999999999997,0.23672697991984612,0.21305428192786152,3.5163402674940318,0.63445021081247976,39.529000000000003,9.0392640735458982E-2,8.5873008698686026E-2,3.5163402674940318,0.85069675413745416,7.1546892405346021E-2,3]
[null,"BOO1012","Long Rural",11,"BOO",0,594.26900000000001,1.33,1.299034573438332,2.7258495994276717,2.7258495994276717,619.43899999999996,1.08,1.0514880000000002,2.7258495994276717,2.7258495994276717,3.0469379630147848E-2,5]
[null,"BOO1022","Short Rural",11,"BOO",0,122.809,0.4,0.39068708975588934,2.7258495994276717,2.7258495994276717,122.937,0.31,0.30181600000000003,2.7258495994276717,2.7258495994276717,3.0469379630147848E-2,3]
[null,"BOO1032","Short Rural",11,"BOO",0,19.263999999999999,1.83,1.7873934356331938,1.3917894264219712,1.3917894264219712,20.058,1.6500000000000001,1.6064400000000001,1.3917894264219712,1.3917894264219712,3.0469379630147848E-2,3]
[null,"BOO1042","Long Rural",11,"BOO",0,227.631,0.44,0.42975579873147823,1.3917894264219712,1.3917894264219712,227.41300000000001,0.47000000000000003,0.45759200000000005,1.3917894264219712,1.3917894264219712,3.0469379630147848E-2,5]
[null,"BOU3B1","Short Rural",11,"BOU",0,9.2650000000000006,1.8434627181461707,1.7843126327908843,7.2399723756379064,7.2399723756379064,9.2579999999999991,1.406409018235099,1.3145705093443469,7.2399723756379064,7.2399723756379064,-1.0463506034967681E-2,4]
[null,"BOU3B2","Short Rural",11,"BOU",0,11.603,2.3296506877671384,2.2549005799005677,5.715767664977295,5.715767664977295,11.311,1.1251272145880791,1.0516564074754775,5.715767664977295,5.715767664977295,-1.0463506034967681E-2,4]
[null,"BOU3B4","Short Rural",11,"BOU",0,10.182,3.0994483063336715,2.9999981628242338,9.0880705873138989,7.6315024606888517,11.106,0,0,9.0880705873138989,7.058973066246959,-1.0463506034967681E-2,4]
[null,"BOU3B6","Short Rural",11,"BOU",0,8.8460000000000001,3.1197061384012117,3.019605993953804,5.2394536928958528,5.2394536928958528,9.3889999999999993,1.8752120243134653,1.7527606791257959,5.2394536928958528,5.2394536928958528,-1.0463506034967681E-2,4]
[null,"BOU3B8","Short Rural",11,"BOU",0,20.056000000000001,2.5018422603412316,2.4215671445019145,9.0880705873138989,7.1475674650541077,20.959,1.8752120243134653,1.7527606791257959,9.0880705873138989,7.2294934682521159,-1.0463506034967681E-2,4]
[null,"BPM3B10","Urban",11,"BPM",0,8.7680000000000007,5.275469735340371,5.1707770497588195,8.9547026751310952,8.9547026751310952,9.7029999999999994,4.4594802515177356,4.3702906464873807,8.9547026751310952,8.8013295761208727,3.5402833183294444E-11,1]
[null,"BPM3B2","Urban",11,"BPM",0,3.387,1.7936597100157261,1.7580641969179986,8.9547026751310952,8.9547026751310952,3.71,1.3913578384735334,1.3635306817040627,8.9547026751310952,8.9547026751310952,3.5402833183294444E-11,1]
[null,"BPM3B3","Urban",11,"BPM",0,8.7629999999999999,4.6424133670995271,4.550283803787762,8.9547026751310952,6.3378337125156579,11.164,3.3892049911534787,3.3214208913304093,8.9547026751310952,7.1523306047749218,3.5402833183294444E-11,1]
[null,"BPM3B4","Short Rural",11,"BPM",0,10.497999999999999,3.69282881473826,3.619543934831174,9.0880705873138989,8.8975449984813224,0,"","","","",3.5402833183294444E-11,3]
[null,"BPM3B6","Short Rural",11,"BPM",0,7.359,2.7432442623769933,2.6888040658745864,8.9547026751310952,8.3678838615267619,14.814,3.4783945961838332,3.4088267042601563,8.9547026751310952,8.3678838615267619,3.5402833183294444E-11,3]
[null,"BPM3B7","Urban",11,"BPM",0,6.05,4.1781720303895744,4.0952554234089851,8.9547026751310952,8.9547026751310952,6.508,3.3892049911534787,3.3214208913304093,8.9547026751310952,8.9547026751310952,3.5402833183294444E-11,1]
[null,"BPM3B9","Short Rural",11,"BPM",0,28.960999999999999,4.220375788272297,4.1366216398070552,8.9547026751310952,8.9547026751310952,30.292999999999999,3.0324465710320596,2.9717976396114185,8.9547026751310952,7.7601072331508414,3.5402833183294444E-11,3]
[null,"BPO3","Short Rural",11,"BPO",0,2.7829999999999999,0.25,0.24844078918401472,3.1436722157375119,3.1436722157375119,2.1309999999999998,0.218,0.21627779999999999,3.1436722157375119,3.1436722157375119,7.6039160398502495E-3,3]
[null,"BPT3B1","Urban",11,"BPT",0,13.8,4.6587646536939609,4.5973685340199166,5.715767664977295,5.715767664977295,14.739000000000001,4.3405344674466182,4.2103184334232191,17.811284672013414,17.811284672013414,4.428728082394124E-2,1]
[null,"BPT3B2","Urban",11,"BPT",0,3.645,3.7307612317307774,3.6815949226155471,8.9547026751310952,8.5136359369836807,4.0110000000000001,3.9607377015450393,3.841915570498688,8.5136359369836807,8.5136359369836807,4.428728082394124E-2,1]
[null,"BPT3B3","Short Rural",11,"BPT",0,14.765000000000001,3.1402135995723883,3.0988298971764032,5.715767664977295,5.715767664977295,15.067,2.5319784393438605,2.4560190861635447,17.107292621277047,17.107292621277047,4.428728082394124E-2,3]
[null,"BPT3B4","Short Rural",11,"BPT",0,6.63,1.5841674576947271,1.5632903063367525,5.715767664977295,5.715767664977295,6.891,1.4468448224822064,1.4034394778077401,5.715767664977295,5.715767664977295,4.428728082394124E-2,3]
[null,"BPT3B5","Short Rural",11,"BPT",0,3.4039999999999999,0.49680991276816888,0.49026264044880402,5.715767664977295,5.715767664977295,3.5139999999999998,0.687251290679048,0.66663375195867658,18.675318217369149,18.675318217369149,4.428728082394124E-2,3]
[null,"BPT3B7","Urban",11,"BPT",0,5.6609999999999996,2.3528167566945353,2.3218098632575432,8.9547026751310952,8.9547026751310952,6.0190000000000001,2.0979249925991987,2.0349872428212228,8.9547026751310952,8.9547026751310952,4.428728082394124E-2,1]
[null,"BRD12","Short Rural",22,"NBAL",0,34.844999999999999,1.4499159956091607,1.4358716848359601,4.8881245070885821,1.5775518755337337,35.048999999999999,0.81524766495014056,0.79894271165113773,5.7172918696879558,1.9605083090872122,-1.9770074958852671E-3,4]
[null,"BRD22","Long Rural",22,"NBAL",0,1440.979,2.7234908566172074,2.6971103269216008,5.4516991988553434,1.3717842395945505,1439.5060000000001,1.3982732677629683,1.3703078024077089,5.4516991988553434,1.3679737278178992,-1.9770074958852671E-3,6]
[null,"BRE8B1","Short Rural",22,"BRE",0,160.74600000000001,0.74286612980586186,0.73789440931199157,3.4675657167528922,1.4746680575641422,160.84,0.1723794243741496,0.1706556301304081,3.4675657167528922,1.4746680575641422,-1.7055363524815418E-12,4]
[null,"BRE8B2","Long Rural",22,"BRE",0,698.649,0.46890859298519183,0.46577036609886763,4.0715318333521591,1.4575207545692102,698.92700000000002,0.32560557937339368,0.32234952357965974,4.0715318333521591,1.4575207545692102,-1.7055363524815418E-12,6]
[null,"BRE8B4","Long Rural",22,"BRE",0,415.77600000000001,1.2117747227910538,1.2036647754108594,3.330387292793437,1.4880048487824227,416.34500000000003,0.61290461999697632,0.60677557379700653,3.330387292793437,1.4880048487824227,-1.7055363524815418E-12,6]
[null,"BRE8B5","Short Rural",22,"BRE",0,6.6189999999999998,0.8988269747374793,0.89281146762058661,3.330387292793437,2.116739291929925,6.8840000000000003,0.42137192624792125,0.41715820698544204,3.330387292793437,2.116739291929925,-1.7055363524815418E-12,4]
[null,"BRE8B6","Short Rural",22,"BRE",0,78.936999999999998,0.19495105616452177,0.19364632288574365,4.8881245070885821,1.6404253198484839,78.989000000000004,9.5766346874527564E-2,9.4808683405782287E-2,4.8881245070885821,1.6404253198484839,-1.7055363524815418E-12,4]
[null,"BRE8B7","Long Rural",22,"BRE",0,300.92399999999998,0.30473928253085769,0.3026997784056098,4.0715318333521591,1.7394986260414236,301.05099999999999,0.15322615499924408,0.15169389344925163,4.0715318333521591,1.7394986260414236,-1.7055363524815418E-12,6]
[null,"BRI","Long Rural",22,"BRI",0,954.94500000000005,2.35,2.3445337059285665,4.0715318333521591,2.0957814771583414,947.846,1.8,1.7481599999999999,4.0715318333521591,2.0957814771583414,4.622854386858246E-2,5]
[null,"BRL20408","Short Rural",11,"BRL",0,125.117,1.3348065187818674,1.2680661928427739,2.7765294060571373,1.5089626635540059,123.23099999999999,0.92118308614618161,0.84748843925448714,2.7765294060571373,1.5089626635540059,6.9283989129884094E-2,3]
[null,"BRL20420","Short Rural",11,"BRL",0,34.043999999999997,1.1259592403330039,1.0696612783163537,2.7765294060571373,1.6223253889093889,34.000999999999998,0.86699584578464162,0.79763617812187038,2.7765294060571373,1.7433091378180749,6.9283989129884094E-2,3]
[null,"BRO3B1","Short Rural",11,"BRO",0,68.010000000000005,0.49397038003933696,0.47382062581701251,2.7258495994276717,1.6632883905083931,67.703999999999994,0.45605351609993994,0.42385613786328419,2.7258495994276717,1.6632883905083931,4.2897323643723353E-2,3]
[null,"BRO3B2","Short Rural",11,"BRO",0,31.370999999999999,0.25117137968101882,0.24092574194085384,2.7258495994276717,1.6118464815235973,31.376999999999999,0.22759894049265295,0.21153045529387166,2.7258495994276717,1.5746939917012448,4.2897323643723353E-2,3]
[null,"BTA3B1","Long Rural",11,"BTA",0,217.49,0.60931233083552827,0.54048391085345293,2.0357659166760795,1.460378638401699,217.642,0.60375696251123145,0.5433812662601083,2.0357659166760795,1.460378638401699,6.2571702866993706E-8,5]
[null,"BTA3B2","Short Rural",11,"BTA",0,159.971,0.7355068475773533,0.65242339161753737,2.0357659166760795,1.4813364531732822,160.053,0.72414628187254149,0.6517316536852874,2.0357659166760795,1.4813364531732822,6.2571702866993706E-8,3]
[null,"BTH102","Urban",11,"BTH",0,6.3869999999999996,2.2574408120721787,2.1979892515985497,9.827309871984296,9.827309871984296,6.907,3.62,3.470494,9.827309871984296,9.827309871984296,8.102371618059216E-6,1]
[null,"BTH112","Short Rural",11,"BTH",0,10.627000000000001,3.2110149482061168,3.1264502285669034,11.850691625386258,11.850691625386258,11.387,3.048,2.9221176,11.850691625386258,11.850691625386258,8.102371618059216E-6,3]
[null,"BTH22","Urban",11,"BTH",0,9.9109999999999996,4.0770159493889793,3.9696443811197959,13.203423306097552,13.203423306097552,10.561,4.5730000000000004,4.3841351,13.114828907290402,13.114828907290402,8.102371618059216E-6,1]
[null,"BTH32","Urban",11,"BTH",0,7.4459999999999997,4.2229711743074381,4.1117557551455635,6.763658403556466,6.763658403556466,7.6890000000000001,3.4289999999999998,3.2873823,6.763658403556466,6.763658403556466,8.102371618059216E-6,1]
[null,"BTH42","Urban",11,"BTH",0,10.220000000000001,3.522386094698831,3.4296211598218758,10.844716516350257,10.844716516350257,10.243,2.2400000000000002,2.1474880000000001,10.844716516350257,10.844716516350257,8.102371618059216E-6,1]
[null,"BTH52","Urban",11,"BTH",0,3.8170000000000002,1.984991058891054,1.9327146867504492,14.244645649067584,14.244645649067584,3.9550000000000001,2.19,2.0995529999999998,14.244645649067584,14.244645649067584,8.102371618059216E-6,1]
[null,"BTH62","Short Rural",11,"BTH",0,7.431,1.7222716540378262,1.6769142135040662,8.4088468631257633,8.4088468631257633,7.85,2.4769999999999999,2.3746999,8.4821992148263075,8.4821992148263075,8.102371618059216E-6,3]
[null,"BTH72","Urban",11,"BTH",0,3.367,2.6563850935159694,2.5864270072689837,16.168954096276607,16.168954096276607,3.2610000000000001,2.8580000000000001,2.7399646,16.168954096276607,16.168954096276607,8.102371618059216E-6,1]
[null,"BTH82","Long Rural",11,"BTH",0,301.40899999999999,2.559081610236996,2.4916860912518044,4.0886791363470918,4.0886791363470918,299.44,2.9529999999999998,2.8310410999999998,4.0886791363470918,4.0886791363470918,8.102371618059216E-6,5]
[null,"BTH92","Long Rural",11,"BTH",0,300.99400000000003,1.595777125775161,1.5537510226817337,6.3025864785816301,6.3025864785816301,294.67700000000002,1.3340000000000001,1.2789058,6.3025864785816301,6.3025864785816301,8.102371618059216E-6,5]
[null,"BTS8B10","Short Rural",22,"BTS",0,165.27500000000001,1.5482127588114738,1.5463946207018293,12.536583745183533,8.7279772244203304,164.76300000000001,1.87,1.8326,12.536583745183533,5.0946542453830963,-4.6488205352926354E-3,4]
[null,"BTS8B11","Short Rural",22,"BTS",0,34.957000000000001,4.7414015738601387,4.7358335258993529,12.536583745183533,12.536583745183533,27.187999999999999,4.96,4.8608000000000002,12.536583745183533,10.757074745487269,-4.6488205352926354E-3,4]
[null,"BTS8B12","Urban",11,"BTS",0,5.593,2.14814520285092,2.1456225362237884,6.2682918725917665,6.2682918725917665,0,"","","","",-4.6488205352926354E-3,2]
[null,"BTS8B2","Urban",11,"BTS",0,3.831,1.2579228665343225,1.2564456293202364,6.2682918725917665,6.2682918725917665,0,"","","","",-4.6488205352926354E-3,2]
[null,"BTS8B3","Short Rural",22,"BTS",0,14.896000000000001,3.8705318970286844,3.8659865517545731,12.536583745183533,12.536583745183533,14.898999999999999,4.05,3.9689999999999999,12.536583745183533,8.103053293049479,-4.6488205352926354E-3,4]
[null,"BTS8B4","Long Rural",22,"BTS",0,473.89800000000002,1.4514494613857567,1.449744956907965,12.536583745183533,4.608813993860025,473.90199999999999,1.18,1.1563999999999999,12.536583745183533,3.8371853590880907,-4.6488205352926354E-3,6]
[null,"BTS8B5","Long Rural",22,"BTS",0,276.572,0.65799042249487638,0.65721771379827743,12.536583745183533,9.459595485537422,277.38900000000001,0.76,0.74480000000000002,12.536583745183533,4.7364661383778524,-4.6488205352926354E-3,6]
[null,"BTS8B6","Short Rural",22,"BTS",0,41.597999999999999,4.5962566277215631,4.5908590302085557,12.536583745183533,12.536583745183533,38.567,4.7699999999999996,4.6745999999999999,12.536583745183533,8.318347208430291,-4.6488205352926354E-3,4]
[null,"BTS8B8","Long Rural",22,"BTS",0,300.17500000000001,1.2869518557620376,1.2854405284583956,12.536583745183533,10.774222048482201,299.98599999999999,1.1499999999999999,1.127,12.536583745183533,5.4814211907132258,-4.6488205352926354E-3,6]
[null,"BTS8B9","Short Rural",22,"BTS",0,135.46899999999999,0.35802420047515332,0.35760375603729805,12.536583745183533,12.536583745183533,134.95500000000001,0.38,0.37240000000000001,12.536583745183533,5.7672095739620897,-4.6488205352926354E-3,4]
[null,"BUL4806","Short Rural",22,"BUL",0,8.1839999999999993,0.27,0.26458215318430078,5.4516991988553434,5.4516991988553434,8.1859999999999999,0.1,9.8000000000000004E-2,5.4516991988553434,5.4516991988553434,-1.0782195568307161E-2,4]
[null,"BUN3B1","Long Rural",11,"BUN",0,260.06900000000002,2.2175620521807615,2.2128998767973522,6.763658403556466,3.1370038201283719,183.78399999999999,1.8460869341272736,1.8307644125740172,6.763658403556466,3.1370038201283719,8.2801307925803522E-3,5]
[null,"BUN3B2","Short Rural",11,"BUN",0,37.106999999999999,2.7539026415454111,2.748112870255317,5.2394536928958528,3.3246715251284598,36.656999999999996,2.5421524994539504,2.5210526337084826,5.2394536928958528,3.3246715251284598,8.2801307925803522E-3,3]
[null,"BUN3B3","Long Rural",11,"BUN",0,245.76499999999999,2.9086162730929059,2.9025012337528064,6.763658403556466,3.0922303067527168,245.26400000000001,2.8649655152576265,2.8411863014809882,6.763658403556466,3.0960408185293682,8.2801307925803522E-3,5]
[null,"BUN3B4","Short Rural",11,"BUN",0,27.414999999999999,1.9700202417047696,1.965878495201369,10.155013884776327,10.155013884776327,27.414999999999999,1.5737134520429217,1.5606516303909654,10.155013884776327,10.155013884776327,8.2801307925803522E-3,3]
[null,"BWA3B1","Short Rural",11,"BWA",0,35.393999999999998,1.68,1.6085682769777625,6.763658403556466,6.763658403556466,35.853000000000002,0,0,6.763658403556466,3.0617462125395045,-7.9436509180213898E-3,4]
[null,"BWA3B2","Urban",11,"BWA",0,8.1000000000000003E-2,1.28,1.2255758300782953,6.763658403556466,6.763658403556466,8.1000000000000003E-2,1.6194675050769001,1.538494129823055,6.763658403556466,6.763658403556466,-7.9436509180213898E-3,2]
[null,"BWA3B3","Urban",11,"BWA",0,8.2000000000000003E-2,0.61,0.58406348152168763,6.763658403556466,6.763658403556466,8.2000000000000003E-2,0.40010373654841069,0.38009854972099016,6.763658403556466,5.9443983715763862,-7.9436509180213898E-3,2]
[null,"BWA3B4","Long Rural",11,"BWA",0,267.5,1.81,1.7330408222200895,6.763658403556466,6.763658403556466,266.29599999999999,2.2672545071076602,2.1538917817522769,6.763658403556466,2.9864886049506367,-7.9436509180213898E-3,6]
[null,"BYA7881","Short Rural",11,"BYA",0,144.96700000000001,0.77948374317978975,0.71181225040146801,1.7337828583764461,1.3822631469803424,144.98500000000001,0.81017463154941538,0.70485192944799135,1.7337828583764461,1.3822631469803424,2.2648599179423967E-2,3]
[null,"BYA7882","Short Rural",11,"BYA",0,158.99799999999999,1.1384565196441667,1.0396205236126705,1.7337828583764461,1.2927161202290318,158.386,1.2538416916836188,1.0908422717647484,1.7337828583764461,1.2927161202290318,2.2648599179423967E-2,3]
[null,"BYR8A1","Short Rural",22,"BYR",0,127.783,0.104,9.8145484408588543E-2,2.7008907472906039,0.89165975573645817,127.81699999999999,4.3999999999999997E-2,3.8258E-2,2.7008907472906039,0.89165975573645817,4.0805081164307595E-2,3]
[null,"CAR2217","Short Rural",11,"CAR",0,43.65,0.53,0.47466142780071968,2.7258495994276717,2.7258495994276717,43.667999999999999,0.3619047619047619,0.32064761904761907,2.7258495994276717,2.7258495994276717,1.1996425695580836E-6,3]
[null,"CAR2218","Short Rural",11,"CAR",0,44.497999999999998,0.55000000000000004,0.4925731797931997,2.7258495994276717,0.41629841159917963,44.55,0.43809523809523809,0.38815238095238097,2.7258495994276717,0.41629841159917963,1.1996425695580836E-6,3]
[null,"CB 82578","Short Rural",11,"ABH",0,29.353999999999999,0.78,0.74099999999999999,2.3941445492701559,0.62397130342668805,37.325000000000003,0.3,0.28499999999999998,2.3941445492701559,0.45726141319818359,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"CBB42","Long Rural",22,"CBB",0,701.20399999999995,1.3356591368021928,1.3256042106376946,4.2597711151187454,1.9738451003054927,703.30200000000002,1.1891173358537648,1.1653349891366895,4.2597711151187454,1.9738451003054927,6.0816191290128437E-4,5]
[null,"CBB52","Long Rural",22,"CBB",0,497.40699999999998,2.9725947706274365,2.950216889840283,4.2597711151187454,1.8480982116759919,498.43799999999999,2.6414743872782105,2.5886448995326461,4.2597711151187454,1.8480982116759919,6.0816191290128437E-4,5]
[null,"CBB62","Short Rural",22,"CBB",0,14.667999999999999,3.5550626648720018,3.5282999290657435,3.4675657167528922,3.2960926868035729,15.334,3.4493479971330578,3.3803610371903967,3.4675657167528922,3.2960926868035729,6.0816191290128437E-4,3]
[null,"CBB72","Long Rural",22,"CBB",0,458.95400000000001,1.9281695809475263,1.9136541988153186,4.2597711151187454,1.9833713797471213,459.33699999999999,2.0060681772800151,1.9659468137344147,4.2597711151187454,1.9833713797471213,6.0816191290128437E-4,5]
[null,"CBC8B1","Long Rural",11,"CBC",0,1288.885,0,0,11.548708567086624,11.548708567086624,1288.9469999999999,0.76,0.72199999999999998,11.548708567086624,11.548708567086624,2.6706904662701588E-2,5]
[null,"CBL3B1","Long Rural",11,"CBL",0,218.928,0.50933684772242804,0.4640594876467945,1.3504453736453019,0.53632953256370286,219.03200000000001,0.5390188404420353,0.45816601437573001,1.3504453736453019,0.53632953256370286,7.9910171218784646E-5,5]
[null,"CBL3B2","Short Rural",11,"CBL",0,85.945999999999998,0.56490086747396551,0.51468415902644471,1.3504453736453019,0.38676694533013029,86.097999999999999,0.57379424950281166,0.48772511207738989,1.3504453736453019,0.38676694533013029,7.9910171218784646E-5,3]
[null,"CBP142A","Urban",22,"CBP",0,10.502000000000001,2.4,2.200241484470649,12.536583745183533,12.536583745183533,11.711,2.87,2.4882900000000001,12.536583745183533,0.37343015411184993,2.5953684815395117E-2,1]
[null,"CBP142B","Short Rural",33,"CBP",0,35.384,1.4999999999999999E-2,1.3751509277941555E-2,16.404253198484835,16.404253198484835,35.430999999999997,0.14000000000000001,0.12138000000000002,16.404253198484835,0.77448651860442352,2.5953684815395117E-2,3]
[null,"CBR22","Short Rural",22,"CBR",0,19.16,2.5646543729505193,2.4364216543029933,7.0326805349880637,2.6159163346712759,20.056999999999999,2.3602607201580144,2.2422476841501133,7.0326805349880637,2.6159163346712759,-8.7542260372801377E-3,4]
[null,"CBR32","Short Rural",22,"CBR",0,27.344999999999999,2.6996361820531782,2.5646543729505193,7.0326805349880637,2.0062344504070309,28.212,2.5781309404802921,2.4492243934562774,7.0326805349880637,2.0062344504070309,-8.7542260372801377E-3,4]
[null,"CBR42","Long Rural",22,"CBR",0,1120.664,0.84588600370999578,0.80359170352449594,7.0326805349880637,2.4311065135036762,1120.9380000000001,0.98041599145025216,0.93139519187773956,7.0326805349880637,2.4501590723869335,-8.7542260372801377E-3,6]
[null,"CBY1392","Urban",11,"CBY",0,2.0510000000000002,0.56999999999999995,0.51753684916525744,3.583405274763098,3.583405274763098,2.0870000000000002,3.43,2.9841000000000002,3.583405274763098,3.583405274763098,-6.634397531592744E-3,2]
[null,"CBY802","Short Rural",11,"CBY",0,40.633000000000003,0.23,0.2088306584351039,2.7765294060571373,2.4292012576153503,40.287999999999997,0.23,0.2001,2.7765294060571373,2.7765294060571373,-6.634397531592744E-3,4]
[null,"CBY804","Short Rural",11,"CBY",0,64.953000000000003,0.25,0.22698984612511292,2.0357659166760795,2.0357659166760795,64.971000000000004,0.25,0.2175,2.0357659166760795,2.0357659166760795,-6.634397531592744E-3,4]
[null,"CBY806","Short Rural",11,"CBY",0,4.4210000000000003,1.1599999999999999,1.0532328860205238,1.3917894264219712,1.3917894264219712,4.6989999999999998,1.1200000000000001,0.97440000000000004,1.3917894264219712,1.3917894264219712,-6.634397531592744E-3,4]
[null,"CBY808","Short Rural",11,"CBY",0,38.338999999999999,0.84,0.76268588298037931,1.5693592752139327,1.5693592752139327,38.436999999999998,0.72,0.62639999999999996,1.5693592752139327,1.5693592752139327,-6.634397531592744E-3,4]
[null,"CCN3B1","Long Rural",11,"CCN",0,412.68099999999998,1.5884158900229617,1.5280767153769945,2.4440622535442911,2.3415594867523652,415.30599999999998,1.6330076533135827,1.5441720369733238,2.581431203092579,2.3415594867523652,-1.6644868745720905E-2,6]
[null,"CCN3B2","Short Rural",11,"CCN",0,23.988,0.17245658234535011,0.16590547195521652,1.3504453736453019,1.3504453736453019,23.983000000000001,0.15513572706479037,0.14669634351246577,1.3504453736453019,1.3504453736453019,-1.6644868745720905E-2,4]
[null,"CCN3B3","Short Rural",11,"CCN",0,83.671000000000006,0.63536635600918456,0.61123068615079768,5.6205048705610059,2.3796646045188803,85.122,0.65320306132543315,0.61766881478932956,5.6205048705610059,2.3796646045188803,-1.6644868745720905E-2,4]
[null,"CCN3B4","Short Rural",11,"CCN",0,94.307000000000002,1.9151757302562564,1.8424239253974044,3.583405274763098,2.3815698604072062,94.028000000000006,1.959609183976299,1.8530064443679883,3.583405274763098,2.3815698604072062,-1.6644868745720905E-2,4]
[null,"CDN32","Short Rural",22,"CDN",0,21.145,1.4793419082648305,1.4523432472550868,3.8931998822048688,3.3608713870066493,21.507999999999999,2.1565736025919993,2.1134421305401592,3.8931998822048688,3.3608713870066493,-4.0258007484222223E-2,4]
[null,"CDN42","Long Rural",22,"CDN",0,412.98599999999999,0.45596154706792724,0.44764004196218432,4.2597711151187454,2.4311065135036762,412.10599999999999,0.77006048977277586,0.7546592799773203,4.2597711151187454,2.4311065135036762,-4.0258007484222223E-2,6]
[null,"CDN52","Long Rural",22,"CDN",0,564.36300000000006,0.36476923765434177,0.35811203356974741,3.8931998822048688,2.6063900552296468,564.90899999999999,0.73165852309119372,0.71702535262936984,3.8931998822048688,2.6063900552296468,-4.0258007484222223E-2,6]
[null,"CDN62","Long Rural",22,"CDN",0,923.86,0.97271796707824476,0.95496542285265984,4.2597711151187454,2.5282745638082904,922.43899999999996,2.2333775359551633,2.1887099852360601,4.2597711151187454,2.5282745638082904,-4.0258007484222223E-2,6]
[null,"CDN72","Long Rural",22,"CDN",0,375.762,0.5775512929527078,0.56701071981876672,4.2597711151187454,2.2786860424376152,377.065,1.1550907346591637,1.1319889199659803,4.2597711151187454,2.2786860424376152,-4.0258007484222223E-2,6]
[null,"CDN82","Short Rural",22,"CDN",0,8.6489999999999991,1.4489444717936355,1.4225005777909412,3.8931998822048688,3.8931998822048688,9.15,3.0034380257279394,2.9433692652133807,3.8931998822048688,3.8931998822048688,-4.0258007484222223E-2,4]
[null,"CFL","Long Rural",22,"CFL",0,696.97500000000002,3.1362412977026275,3.1318788047530179,10.821853445690346,3.5018603227427563,702.84799999999996,2.3710427346795622,2.3544454355368054,3.5018603227427563,3.5018603227427563,2.6504691260260515E-5,5]
[null,"CFN3B11","Urban",11,"CFN",0,4.165,1.686153843765329,1.671617993330422,9.0880705873138989,5.6652783839366627,4.4130000000000003,3.2979774577577614,3.232017908602606,9.0880705873138989,5.6652783839366627,4.3412710250305728E-2,1]
[null,"CFN3B12","Short Rural",11,"CFN",0,15.473000000000001,4.1620253105599891,4.1261456797396496,7.2399723756379064,3.9629322477175912,16.286000000000001,3.1697227788449593,3.1063283232680603,7.2399723756379064,3.9629322477175912,4.3412710250305728E-2,3]
[null,"CFN3B13","Short Rural",11,"CFN",0,135.60900000000001,5.9548977520319841,5.9035622802428831,9.0880705873138989,2.2910702057117325,136.017,3.7377077854587961,3.6629536297496199,9.0880705873138989,2.2910702057117325,4.3412710250305728E-2,3]
[null,"CFN3B15","Urban",11,"CFN",0,2.5019999999999998,4.0446348530826564,4.0097672118495566,5.6205048705610059,5.6205048705610059,2.7040000000000002,3.8476403673840549,3.7706875600363738,5.6205048705610059,5.6205048705610059,4.3412710250305728E-2,1]
[null,"CFN3B20","Urban",11,"CFN",0,9.2739999999999991,3.3509639679893248,3.3220762652262823,7.2399723756379064,7.2399723756379064,9.9550000000000001,4.2873706950850892,4.2016232811833873,7.2399723756379064,7.2399723756379064,4.3412710250305728E-2,1]
[null,"CFN3B21","Urban",11,"CFN",0,5.1219999999999999,1.590107105829329,1.5763992468748915,9.0880705873138989,9.0880705873138989,5.3170000000000002,3.1147564878823299,3.0524613581246833,9.0880705873138989,9.0880705873138989,4.3412710250305728E-2,1]
[null,"CFN3B22","Short Rural",11,"CFN",0,27.161999999999999,1.2592794529386633,1.2484235646391759,7.2399723756379064,4.542130037768624,27.1,0.9527490433522422,0.93369406248519737,7.2399723756379064,4.542130037768624,4.3412710250305728E-2,3]
[null,"CFN3B5","Short Rural",11,"CFN",0,9.7430000000000003,2.742667961061326,2.719024204341256,9.0880705873138989,8.7813243892934523,9.9619999999999997,2.015430668629743,1.975122055257148,9.0880705873138989,8.7813243892934523,4.3412710250305728E-2,3]
[null,"CFN3B6","Urban",11,"CFN",0,4.6779999999999999,3.0628237541813252,3.0364200258596905,9.0880705873138989,9.0880705873138989,4.6710000000000003,2.9681797119819855,2.9088161177423459,9.0880705873138989,9.0880705873138989,4.3412710250305728E-2,1]
[null,"CFN3B7","Urban",11,"CFN",0,7.0510000000000002,2.8173709794559927,2.7930832293622241,9.0880705873138989,8.5660304739126403,7.2850000000000001,2.5284493842809503,2.4778803965953311,9.0880705873138989,8.5660304739126403,4.3412710250305728E-2,1]
[null,"CFN3B8","Urban",11,"CFN",0,3.6349999999999998,1.1845764345439971,1.1743645396182081,9.0880705873138989,9.0880705873138989,3.7320000000000002,1.0260374313024145,1.0055166826763662,9.0880705873138989,9.0880705873138989,4.3412710250305728E-2,1]
[null,"CHD3B1","Short Rural",11,"CHD",0,10.49,1.1668776130553913,1.1433565516619477,2.7765294060571373,2.0881604536050387,10.941000000000001,1.2384163274117472,1.1393430212188076,2.7765294060571373,2.0881604536050387,1.8508220679817639E-2,3]
[null,"CHD3B2","Short Rural",11,"CHD",0,93.706999999999994,0.63900440714938089,0.62612382591011417,2.7765294060571373,1.6470937154576237,91.674999999999997,0.55252420761447185,0.50832227100531413,2.7765294060571373,1.6470937154576237,1.8508220679817639E-2,3]
[null,"CHI3B2","Short Rural",11,"CHI",0,107.378,2.1878529139276495,2.1053914316880626,9.0499654695473861,4.6307244365757718,130.56800000000001,2.9269793714318695,2.5994503797686432,9.0499654695473861,4.6307244365757718,1.3341632112329211E-2,3]
[null,"CHI3B3","Short Rural",11,"CHI",0,41.314,0.64825271523782202,0.62381968346312966,9.0499654695473861,9.0499654695473861,23.155999999999999,0.4878298952386449,0.43324172996144056,5.0489281040632772,5.0222545216267171,1.3341632112329211E-2,3]
[null,"CHI3B4","Short Rural",11,"CHI",0,12.167,3.0488135513528816,2.9339019487875313,5.0489281040632772,5.0222545216267171,0,"","","","",1.3341632112329211E-2,3]
[null,"CHI3B5","Short Rural",11,"CHI",0,31.117999999999999,2.1979818626032404,2.115138614242174,5.0489281040632772,5.0489281040632772,31.523,1.3659237066682057,1.2130768438920334,5.0489281040632772,5.0489281040632772,1.3341632112329211E-2,3]
[null,"CHS3B1","Short Rural",11,"CHS",0,6.8810000000000002,1.8831167455450346,1.8259763030432961,8.8213347629482932,8.8213347629482932,6.3630000000000004,0,0,8.8213347629482932,8.8213347629482932,5.3737333510736627E-3,3]
[null,"CHS3B11","Short Rural",11,"CHS",0,16.253,3.1959181338678588,3.0989426400220514,8.3173945804861269,8.3173945804861269,15.141999999999999,2.9538930291085461,2.9066307406428091,8.3173945804861269,8.3173945804861269,5.3737333510736627E-3,3]
[null,"CHS3B12","Short Rural",11,"CHS",0,6.5439999999999996,2.1090907550104387,2.0450934594084917,5.715767664977295,5.715767664977295,6.8049999999999997,2.3955352004355888,2.3572066372286193,5.715767664977295,5.715767664977295,5.3737333510736627E-3,3]
[null,"CHS3B2","Urban",11,"CHS",0,3.7730000000000001,3.9922075005554731,3.8710697624517878,5.6205048705610059,5.6205048705610059,3.871,2.845823771946038,2.8002905915949015,5.6205048705610059,5.6205048705610059,5.3737333510736627E-3,1]
[null,"CHS3B3","Short Rural",11,"CHS",0,8.48,2.1090907550104387,2.0450934594084917,8.6155671270091094,8.6155671270091094,9.6869999999999994,2.7017314290626944,2.6585037261976914,8.6155671270091094,8.6155671270091094,5.3737333510736627E-3,3]
[null,"CHS3B4","Urban",11,"CHS",0,4.5590000000000002,2.8730981203458525,2.7859181309289145,9.505321626857242,9.505321626857242,4.6020000000000003,3.0619622862710534,3.0129708896907164,9.505321626857242,9.505321626857242,5.3737333510736627E-3,1]
[null,"CHS3B5","Urban",11,"CHS",0,8.2799999999999994,4.6916508631864868,4.5492895321535842,6.3826072258913129,6.3826072258913129,6.0449999999999999,2.3415005718543354,2.3040365627046659,6.3826072258913129,6.3826072258913129,5.3737333510736627E-3,1]
[null,"CHS3B6","Urban",11,"CHS",0,4.8920000000000003,1.904638079779835,1.8468446036495052,9.6329737713750667,9.6329737713750667,5.165,2.845823771946038,2.8002905915949015,9.6329737713750667,9.6329737713750667,5.3737333510736627E-3,1]
[null,"CHS3B7","Short Rural",11,"CHS",0,10.397,1.7862707414884327,1.732068950315355,5.715767664977295,5.715767664977295,16.140999999999998,1.5129696002751092,1.4887620866707074,5.715767664977295,5.715767664977295,5.3737333510736627E-3,3]
[null,"CHS3B8","Short Rural",11,"CHS",0,4.2450000000000001,0.97922070768341807,0.94950767758251409,9.3624274352328101,9.3624274352328101,4.3810000000000002,2.4135467432960072,2.3749299954032712,9.3624274352328101,9.3624274352328101,5.3737333510736627E-3,3]
[null,"CHS3B9","Short Rural",11,"CHS",0,16.367000000000001,2.3565860987106433,2.2850789163798964,7.9611117293692093,7.9611117293692093,17.356999999999999,1.8011542860417964,1.7723358174651276,7.9611117293692093,7.9611117293692093,5.3737333510736627E-3,3]
[null,"CLA3B1","Short Rural",11,"CLA",0,14.045,0,0,1.7337828583764461,1.3374896336046871,14.053000000000001,0.99816122131454377,0.94825316024881656,1.7337828583764461,1.3232002144422439,1.6082087138755217E-9,3]
[null,"CLA3B2","Short Rural",11,"CLA",0,133.97499999999999,1.0752560078299218,1.0214932074384258,1.3917894264219712,1.1726849992645083,133.96,0.99816122131454377,0.94825316024881656,1.3917894264219712,1.2631846539599823,1.6082087138755217E-9,3]
[null,"CLA3B3","Short Rural",11,"CLA",0,137.18899999999999,0.43806726244922745,0.41616389932676606,2.7258495994276717,1.2479426068533761,137.23099999999999,0.39213476551642795,0.37252802724060652,2.7258495994276717,1.2479426068533761,1.6082087138755217E-9,3]
[null,"CLM2","Long Rural",11,"CLM",0,"","","","","",369.63499999999999,1.4635558703589917,1.3611069594338623,1.541733064833209,1.541733064833209,-2.4454083364751269E-2,6]
[null,"CLN3B1","Long Rural",11,"CLN",0,266.64699999999999,1.4472553418502738,1.4095765999029564,6.1920816370587364,6.1920816370587364,266.88900000000001,1.0976669027692436,1.0208302195753967,2.3941445492701559,2.0824446859400614,-2.4454083364751269E-2,6]
[null,"CLN3B2","Long Rural",11,"CLN",0,219.62799999999999,0.76006935219474814,0.74028123592025763,6.1920816370587364,6.1920816370587364,0,"","","","",-2.4454083364751269E-2,6]
[null,"CLN3B3","Short Rural",11,"CLN",0,148.20099999999999,1.2181933452984319,1.1864781452420567,6.1920816370587364,6.1920816370587364,0,"","","","",-2.4454083364751269E-2,4]
[null,"CLN3B4","Short Rural",11,"CLN",0,180.91800000000001,2.0511460600324023,1.9977452530998732,6.1920816370587364,6.1920816370587364,179.58500000000001,1.1891391446666808,1.1058994045400132,2.4440622535442911,2.0833973138842241,-2.4454083364751269E-2,4]
[null,"CLY1523","Short Rural",33,"CLY",0,106.54300000000001,2.3817862972224981,2.1814276221605544,10.549020802482097,9.5110373945222175,89.543999999999997,2.6223649052174101,2.2080312501930592,9.4573091784714318,9.4573091784714318,2.1610255017645253E-8,3]
[null,"CLY1526","Short Rural",33,"CLY",0,50.225000000000001,2.1191558690116525,1.9408899756105313,9.4573091784714318,9.4573091784714318,60.139000000000003,4.8950811564058316,4.12165833369371,10.750215824289295,10.411270801756142,2.1610255017645253E-8,3]
[null,"CLY1530","Short Rural",33,"CLY",0,26.66,5.8503191939381516,5.3581834369418937,9.4573091784714318,9.4573091784714318,26.344999999999999,5.8478737386348243,4.9239096879305215,9.4573091784714318,9.4573091784714318,2.1610255017645253E-8,3]
[null,"CLY4B4","Short Rural",33,"CLY",0,38.823,2.2278305289609679,2.0404227948726095,10.549020802482097,10.549020802482097,0,"","","","",2.1610255017645253E-8,3]
[null,"CMK4005","Short Rural",11,"CMK",0,198.233,0.46618647626193621,0.4661589393307411,2.7138464873312196,1.206979605254372,198.523,0.40551489423675846,0.3852391495249205,2.7138464873312196,1.206979605254372,-1.129368711092716E-2,4]
[null,"CMK4006","Short Rural",11,"CMK",0,99.552999999999997,0.56771153109231343,0.56767799722943579,2.7765294060571373,1.5727887358129191,99.564999999999998,0.48275582647233151,0.45861803514871491,2.7765294060571373,1.5727887358129191,-1.129368711092716E-2,4]
[null,"CMK4022","Short Rural",11,"CMK",0,179.339,0.70963941386539187,0.70959749653679483,2.1298855575593727,0.30388831418795953,179.654,0.81102978847351692,0.770478299049841,2.1298855575593727,0.30388831418795953,-1.129368711092716E-2,4]
[null,"CNA3B1","Short Rural",11,"CNA",0,83.698999999999998,0.34204161614367368,0.28742380688694757,2.1298855575593727,0.72971300522876814,83.094999999999999,0.3428766522512372,0.27430132180098976,2.1298855575593727,0.72971300522876814,1.7298696401315827E-2,3]
[null,"CNA3B2","Short Rural",11,"CNA",0,29.225000000000001,0.46175618179395944,0.38802213929737922,2.1298855575593727,1.053606506244148,29.242999999999999,0.52247870819236142,0.41798296655388917,2.1298855575593727,1.0231224120309359,1.7298696401315827E-2,3]
[null,"CNA3B3","Short Rural",11,"CNA",0,29.224,0.42755202017959204,0.35927975860868444,1.5061047797215172,1.1593482080462278,29.234000000000002,0.40818649077528241,0.32654919262022597,1.5061047797215172,1.134579881497993,1.7298696401315827E-2,3]
[null,"CNB22","Long Rural",22,"CNB",0,518.14,0.96274817009586688,0.95728461821001243,4.2597711151187454,2.0843499418283868,519.57399999999996,0.55411525490208013,0.54303294980403849,4.2597711151187454,2.0843499418283868,1.0071497962923391E-3,5]
[null,"CNB32","Short Rural",22,"CNB",0,6.718,1.6949221986141523,1.6853035925630051,2.4657821706712051,2.4657821706712051,7.4450000000000003,1.0016698838614526,0.9816364861842235,2.4657821706712051,2.4657821706712051,1.0071497962923391E-3,3]
[null,"CNB42","Long Rural",22,"CNB",0,1068.346,1.0598320191811645,1.0538175208866525,3.4675657167528922,2.3072648807625016,1076.0709999999999,0.5967395052791632,0.5848047151735799,3.4675657167528922,2.3072648807625016,1.0071497962923391E-3,5]
[null,"CNB52","Short Rural",22,"CNB",0,14.84,2.8508267767859756,2.8346484650567492,4.2597711151187454,3.1284301686309064,15.468999999999999,1.449224512820825,1.4202400225644085,4.2597711151187454,3.1284301686309064,1.0071497962923391E-3,3]
[null,"CNK3B1","Short Rural",11,"CNK",0,16.622,0.16984213782803573,0.16262611281350528,6.4778700203076003,2.559711285965665,16.658000000000001,0.19001476775316245,0.17671373401044108,6.4778700203076003,2.5549481462448509,1.2675980809492545E-8,3]
[null,"CNK3B2","Short Rural",11,"CNK",0,37.173999999999999,0.31970284767630253,0.30611974176659817,6.4778700203076003,2.0919709653816905,37.195999999999998,0.25465896709186725,0.23683283939543656,6.4778700203076003,2.0919709653816905,1.2675980809492545E-8,3]
[null,"CNK3B3","Short Rural",11,"CNK",0,63.895000000000003,1.1389413948468277,1.0905515800435059,6.4778700203076003,2.3634699294681116,63.762,0.80315520390511974,0.74693433963176137,6.4778700203076003,2.3472752544173421,1.2675980809492545E-8,3]
[null,"CNK3B4","Short Rural",11,"CNK",0,130.92699999999999,1.8083192321690862,1.7314897893673209,6.4778700203076003,2.5625691697981536,130.93600000000001,1.2928839867740951,1.2023821076999086,6.4778700203076003,2.5625691697981536,1.2675980809492545E-8,3]
[null,"COBD2","Long Rural",11,"COB",0,211.24100000000001,1.349812109954371,1.3257406011092483,3.583405274763098,1.4175103809143692,210.54400000000001,1.1230778191440511,1.1087024230590072,3.583405274763098,1.4175103809143692,2.9363166754222871E-2,5]
[null,"COBE2","Short Rural",11,"COB",0,7.7969999999999997,0.42422666312851665,0.41666133177719233,2.7258495994276717,2.2148599701787015,7.7050000000000001,0.3984501322788801,0.39334997058571042,2.7258495994276717,2.2148599701787015,2.9363166754222871E-2,3]
[null,"COO102","Long Rural",11,"COO_11",0,585.50199999999995,2.13,2.1087767432720548,4.3820885431492593,3.2417928939862892,585.90800000000002,2.1586189211788236,2.1342265273695031,2.3941445492701559,2.3941445492701559,-6.0731643571309453E-3,6]
[null,"COO12","Short Rural",11,"COO_11",0,115.67700000000001,1.44,1.4256518827754736,4.3820885431492593,2.5825743566255746,116.057,2.131846890461401,2.1077570205991871,2.0357659166760795,2.0357659166760795,-6.0731643571309453E-3,4]
[null,"COO22","Short Rural",11,"COO_11",0,105.38500000000001,1.68,1.6632605299047192,4.3820885431492593,2.9769623255090076,106.119,1.5299719776660194,1.5126832943183934,2.4440622535442911,2.4440622535442911,-6.0731643571309453E-3,4]
[null,"COO32","Short Rural",11,"COO_11",0,10.077,2.16,2.1384778241632105,4.3820885431492593,4.0172320405348758,10.654,2.1348215605411149,2.1106980769070005,4.3820885431492593,4.0172320405348758,-6.0731643571309453E-3,4]
[null,"COO52","Urban",11,"COO_11",0,5.226,2.41,2.3859868315895079,9.0880705873138989,4.4716355699005712,5.4180000000000001,3.5319249413132612,3.4920141894764214,9.0880705873138989,4.4716355699005712,-6.0731643571309453E-3,2]
[null,"COO62","Urban",11,"COO_11",0,7.4740000000000002,2.56,2.5344922360452866,4.3820885431492593,3.2246455909913569,7.9189999999999996,2.5185540008241669,2.4900943406148537,4.3820885431492593,3.2246455909913569,-6.0731643571309453E-3,2]
[null,"COO82","Short Rural",11,"COO_11",0,8.9809999999999999,2.14,2.1186771035691065,4.3820885431492593,4.3820885431492593,9.6470000000000002,1.8651181399804166,1.8440423049986381,4.3820885431492593,4.3820885431492593,-6.0731643571309453E-3,4]
[null,"COO92","Long Rural",11,"COO_11",0,291.93200000000002,2.06,2.0394742211926915,4.3820885431492593,3.0122095594430349,292.50299999999999,1.9335355518138289,1.9116866000783326,3.0122095594430349,3.0122095594430349,-6.0731643571309453E-3,6]
[null,"COW102","Long Rural",11,"COW",0,479.822,2.9611641980975283,2.9351153494837985,2.5999121852093392,2.5999121852093392,439.16300000000001,2.8230085941544805,2.6818581644467563,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,6]
[null,"COW32","Long Rural",11,"COW",0,388.32,2.1021233897757199,2.0836313743775774,2.5999121852093392,2.5999121852093392,347.15300000000002,1.953603773490963,1.8559235848164148,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,6]
[null,"COW42","Short Rural",11,"COW",0,117.11799999999999,2.2031870142841679,2.1838059596841912,2.5999121852093392,2.5999121852093392,116.57899999999999,1.953603773490963,1.8559235848164148,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,4]
[null,"COW52","Short Rural",11,"COW",0,17.295000000000002,4.3053104040598873,4.2674373340617677,2.5999121852093392,2.5999121852093392,18.699000000000002,3.7026417068258048,3.5175096214845145,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,4]
[null,"COW62","Urban",11,"COW",0,10.215,4.1132895174938362,4.077105621979201,2.5999121852093392,2.5999121852093392,10.775,4.1015450951302421,3.8964678403737296,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,2]
[null,"COW72","Short Rural",11,"COW",0,7.7,2.8702069360399247,2.8449582227078452,2.5999121852093392,2.5999121852093392,8.4960000000000004,2.5366164179359103,2.4097855970391149,2.5999121852093392,2.5999121852093392,-8.1133405290337399E-12,4]
[null,"COW82","Short Rural",11,"COW",0,23.73,3.5069077704431479,3.4760581101395158,2.7765294060571373,2.7765294060571373,24.925999999999998,3.1196290623808571,2.9636476092618143,2.7765294060571373,2.7765294060571373,-8.1133405290337399E-12,4]
[null,"COW92","Long Rural",11,"COW",0,252.13800000000001,1.9101025032096681,1.8932996622950096,2.7765294060571373,2.7765294060571373,251.286,1.8513208534129024,1.7587548107422573,2.7765294060571373,2.7765294060571373,-8.1133405290337399E-12,6]
[null,"CPD2C03","Short Rural",22,"CPD",0,31.861999999999998,0.44052852920203239,0.41850210274193073,4.2597711151187454,0.93738589705627651,31.9,1.0519397370990178,1.0309009423570374,4.2597711151187454,0.93738589705627651,3.603764799355582E-2,3]
[null,"CPM3B10","Short Rural",11,"CPM",0,11.068,3.9889371846267991,3.9846381598179934,9.0880705873138989,6.2273288709927632,11.779,3.1962225458320059,3.1642603203736859,9.0880705873138989,6.2273288709927632,1.6948523219440594E-2,3]
[null,"CPM3B3","Short Rural",11,"CPM",0,6.8230000000000004,1.9038109290264269,1.901759121731315,6.763658403556466,6.763658403556466,7.2359999999999998,1.6580404456503532,1.6414600411938498,6.763658403556466,6.763658403556466,1.6948523219440594E-2,3]
[null,"CPM3B4","Short Rural",11,"CPM",0,20.943999999999999,4.0795948479137714,4.0751981179956749,6.763658403556466,6.763658403556466,18.559999999999999,2.8965766821602559,2.8676109153386533,6.763658403556466,6.763658403556466,1.6948523219440594E-2,3]
[null,"CPM3B5","Short Rural",11,"CPM",0,16.625,4.3515678377746898,4.3468779925287198,8.9547026751310952,4.7974343268042769,18.023,4.0951601368472579,4.0542085354787849,8.9547026751310952,4.7974343268042769,1.6948523219440594E-2,3]
[null,"CPM3B6","Short Rural",11,"CPM",0,14.866,3.9889371846267991,3.9846381598179934,6.763658403556466,6.0691926322617249,14.564,3.1962225458320059,3.1642603203736859,6.763658403556466,6.0691926322617249,1.6948523219440594E-2,3]
[null,"CPM3B7","Short Rural",11,"CPM",0,30.315000000000001,1.813153265739454,1.8111991635536333,6.763658403556466,6.2158973356628087,28.462,1.8378279638534036,1.8194496842148695,6.763658403556466,6.2158973356628087,1.6948523219440594E-2,3]
[null,"CPM3B8","Urban",11,"CPM",0,3.58,2.0851262556003718,2.082879038086678,6.1920816370587364,6.1920816370587364,6.5570000000000004,1.598111272916003,1.5821301601868429,6.1920816370587364,6.1920816370587364,1.6948523219440594E-2,1]
[null,"CPM3B9","Short Rural",11,"CPM",0,3.6840000000000002,0.80685320325405707,0.80598362778136678,9.0880705873138989,9.0880705873138989,0,"","","","",1.6948523219440594E-2,3]
[null,"CRA12","Short Rural",22,"CRA",0,28.181999999999999,3.7528733566997006,3.5821323673921688,6.4252849577898106,6.4252849577898106,28.605,3.584208795843761,3.3537441702710069,6.4252849577898106,6.4252849577898106,7.1324351407621592E-3,3]
[null,"CRA22","Long Rural",22,"CRA",0,454.05900000000003,2.0291126285567938,1.9367959781700443,6.4252849577898106,6.4252849577898106,392.13400000000001,1.5091405456184257,1.4121028085351608,6.4252849577898106,6.4252849577898106,7.1324351407621592E-3,5]
[null,"CRA32","Urban",22,"CRA",0,18.55,6.5699908895503949,6.2710821234923273,6.3048727856476212,6.3048727856476212,19.004000000000001,6.9797750234852192,6.5309754894751197,6.3048727856476212,6.3048727856476212,7.1324351407621592E-3,1]
[null,"CRA42","Short Rural",22,"CRA",0,112.5,3.6445226823592893,3.4787112229267785,4.8881245070885821,4.8881245070885821,106.663,3.7728513640460641,3.5302570213379023,4.8881245070885821,4.8881245070885821,7.1324351407621592E-3,3]
[null,"CRA52","Short Rural",22,"CRA",0,132.19900000000001,4.6590789966376862,4.4471092120118003,9.5720055829486448,9.5720055829486448,134.60400000000001,6.1308834665748542,5.7366676596740911,9.5720055829486448,9.5720055829486448,7.1324351407621592E-3,3]
[null,"CRO5502","Long Rural",11,"CRO",0,232.054,1.137370810068385,1.1313897104498203,5.2394536928958528,3.0245937227171518,232.214,0.89797803796058151,0.89600248627706824,3.0245937227171518,3.0245937227171518,4.5800472531305541E-3,5]
[null,"CRO5512","Long Rural",11,"CRO",0,200.58,0.95107731531580486,0.94607587856579822,5.2394536928958528,2.4063381869554412,199.83699999999999,0.97373546523509624,0.97159324721157903,2.4063381869554412,2.4063381869554412,4.5800472531305541E-3,5]
[null,"CRO5522","Long Rural",11,"CRO",0,443.53899999999999,1.2648347801622559,1.2581833848967832,5.2394536928958528,2.6168689626154378,441.25599999999997,1.2151491334832167,1.2124758053895537,2.6168689626154378,2.6168689626154378,4.5800472531305541E-3,5]
[null,"CRO5532","Long Rural",11,"CRO",0,387.077,0.6667346127987086,0.66322845095334315,5.2394536928958528,2.0919709653816905,385.03199999999998,0.64242298328788505,0.64100965272465171,2.0919709653816905,2.0919709653816905,4.5800472531305541E-3,5]
[null,"CRO5542","Long Rural",11,"CRO",0,217.13200000000001,1.823715264419997,1.8141248805488501,5.2394536928958528,2.7988208999505488,217.45699999999999,1.8989861770145031,1.8948084074250713,2.7988208999505488,2.7988208999505488,4.5800472531305541E-3,5]
[null,"CSO3B1","Short Rural",11,"CSO_11",0,15.096,5.0787806846040704,4.9993289164895973,6.763658403556466,6.763658403556466,15.683999999999999,6.3095665910379912,6.1833752592172315,6.763658403556466,6.763658403556466,-8.7865259488469315E-9,4]
[null,"CSO3B2","Long Rural",11,"CSO_11",0,276.48399999999998,4.1726081973095681,4.1073324708088803,6.763658403556466,3.11985651713344,275.678,3.4902056573988887,3.420401544250911,6.763658403556466,3.11985651713344,-8.7865259488469315E-9,6]
[null,"CSO3B3","Short Rural",11,"CSO_11",0,192.90100000000001,1.9071769790733126,1.8773413566070891,6.763658403556466,6.763658403556466,193.00399999999999,1.2419692858796048,1.2171299001620126,6.763658403556466,6.763658403556466,-8.7865259488469315E-9,4]
[null,"CSO3B4","Urban",11,"CSO_11",0,9.2189999999999994,4.5203255470853652,4.4496101767096201,6.763658403556466,6.763658403556466,9.4879999999999995,3.3723545572789266,3.304907466133348,6.763658403556466,6.763658403556466,-8.7865259488469315E-9,2]
[null,"CSO3B6","Short Rural",11,"CSO_11",0,75.278000000000006,5.0577069058297797,4.9785848131016737,6.763658403556466,1.3022423996706605,75.721999999999994,3.5264675343588774,3.4559381836716998,6.763658403556466,1.3022423996706605,-8.7865259488469315E-9,4]
[null,"CSO3B7","Short Rural",11,"CSO_11",0,123.598,3.0873085904335946,3.0390111463308132,6.763658403556466,6.763658403556466,123.143,2.8828192183190824,2.8251628339527008,6.763658403556466,6.763658403556466,-8.7865259488469315E-9,4]
[null,"CSO3B8","Urban",11,"CSO_11",0,7.3869999999999996,4.1304606397609867,4.065844264033033,6.763658403556466,6.763658403556466,7.4850000000000003,4.1066575657186926,4.0245244144043184,6.763658403556466,6.763658403556466,-8.7865259488469315E-9,2]
[null,"CSO3B9","Urban",11,"CSO_11",0,9.8369999999999997,4.3306615381167486,4.2629132462183073,6.763658403556466,4.5125985714995753,10.592000000000001,4.0975920964786949,4.0156402545491208,6.763658403556466,5.7224360605864355,-8.7865259488469315E-9,2]
[null,"CST5342","Urban",11,"CST",0,7.3150000000000004,3.3088436717081731,3.195915483923919,6.763658403556466,6.763658403556466,7.5679999999999996,3.1388573972744163,3.0089087010272553,6.763658403556466,6.763658403556466,4.6296722437253791E-4,1]
[null,"CST5352","Urban",11,"CST",0,2.1970000000000001,3.9463273148813069,3.8116423202762335,10.036888019700131,10.036888019700131,2.198,3.8619031356220699,3.7020203458073162,10.036888019700131,10.036888019700131,4.6296722437253791E-4,1]
[null,"CST5362","Long Rural",11,"CST",0,301.43299999999999,4.2296533785138104,4.0852986919883731,2.7258495994276717,2.7258495994276717,292.84699999999998,3.3955186607486523,3.2549441881936581,2.7258495994276717,2.7258495994276717,4.6296722437253791E-4,5]
[null,"CST5372","Short Rural",11,"CST",0,144.10599999999999,1.0017600107006395,0.96757074283935163,2.7765294060571373,2.7765294060571373,143.542,0.79195479352167097,0.75916786506987377,2.7765294060571373,2.7765294060571373,4.6296722437253791E-4,3]
[null,"CST5382","Short Rural",11,"CST",0,57.316000000000003,1.9225697175062777,1.856953950903806,6.763658403556466,5.3423375108654456,56.008000000000003,1.7936327984425233,1.7193764005870029,6.763658403556466,5.3413848829212833,4.6296722437253791E-4,3]
[null,"CST5392","Urban",11,"CST",0,3.8290000000000002,4.3308412583825628,4.1830331104569947,2.7765294060571373,2.7765294060571373,3.94,0.8948190353031743,0.85777352724162292,2.7765294060571373,2.7765294060571373,4.6296722437253791E-4,1]
[null,"CST5402","Urban",11,"CST",0,1.5189999999999999,1.7707878977031506,1.7103523232008739,9.6101107007151594,9.6101107007151594,1.625,1.7706631133845179,1.6973576604903988,9.6101107007151594,9.6101107007151594,4.6296722437253791E-4,1]
[null,"CTM3B1","Short Rural",11,"CTM",0,21.513999999999999,4.736743742661079,4.7367059679781462,3.583405274763098,3.583405274763098,22.809000000000001,4.2029937814892619,3.8289273349367177,3.583405274763098,3.583405274763098,5.6643231600904259E-3,3]
[null,"CTM3B2","Long Rural",11,"CTM",0,449.76499999999999,1.8764402406687359,1.8764252763939122,3.2126424788949053,3.2126424788949053,449.55399999999997,1.7194065469728796,1.5663793642922934,3.2126424788949053,3.2126424788949053,5.6643231600904259E-3,5]
[null,"CTM3B3","Short Rural",11,"CTM",0,16.556000000000001,4.077453928372063,4.0774214114073111,3.583405274763098,3.583405274763098,17.422999999999998,4.0119486096033858,3.6548851833486848,3.583405274763098,3.583405274763098,5.6643231600904259E-3,3]
[null,"CTM3B4","Short Rural",11,"CTM",0,198.71600000000001,1.6228672351729607,1.6228542930974377,1.5693592752139327,1.5693592752139327,198.571,1.5283613750870042,1.3923372127042608,1.5693592752139327,1.5693592752139327,5.6643231600904259E-3,3]
[null,"CUD3B1","Short Rural",11,"CUD_11",0,16.338000000000001,2.4207828771363857,2.4090307331616629,6.9732365512722998,4.9860546597485262,17.085000000000001,2.8463013068363545,2.7893752806996273,6.9732365512722998,4.9860546597485262,-1.6855636882572502E-3,4]
[null,"CUD3B3","Short Rural",11,"CUD_11",0,41.543999999999997,1.2478262253280339,1.2417684191554965,6.9732365512722998,4.3611307283776757,44.085000000000001,1.1954465488712689,1.1715376178938435,6.9732365512722998,4.3611307283776757,-1.6855636882572502E-3,4]
[null,"CUD3B4","Short Rural",11,"CUD_11",0,9.41,3.3608119668835044,3.3444962755921366,6.9732365512722998,4.1058264393420227,9.9260000000000002,3.5863396466138062,3.51461285368153,6.9732365512722998,4.1058264393420227,-1.6855636882572502E-3,4]
[null,"CUD3B5","Urban",11,"CUD_11",0,9.6780000000000008,1.1396812857996044,1.1341484894953535,6.9732365512722998,4.7393240222103401,12.103999999999999,1.0246684704610876,1.0041751010518658,6.9732365512722998,4.7155083236062687,-1.6855636882572502E-3,2]
[null,"CUD3B6","Short Rural",11,"CUD_11",0,7.6529999999999996,0.68214500317932514,0.67883340247167134,6.9732365512722998,4.3058783076162293,7.5919999999999996,0.60721094545842225,0.59506672654925374,6.9732365512722998,4.3058783076162293,-1.6855636882572502E-3,4]
[null,"CUD3B7","Short Rural",11,"CUD_11",0,15.561999999999999,1.8717393379920508,1.8626526287332446,6.9732365512722998,3.7581172397225715,15.926,2.0683122829677512,2.0269460373083961,6.9732365512722998,3.7581172397225715,-1.6855636882572502E-3,4]
[null,"CUD3B8","Short Rural",11,"CUD_11",0,14.106999999999999,2.1712176320707788,2.1606770493305634,6.9732365512722998,3.6123651642656509,0,"","","","",-1.6855636882572502E-3,4]
[null,"CWD13","Long Rural",11,"CWD",0,408.23700000000002,1.8132232039543625,1.7257938549037506,2.7258495994276717,2.4501590723869335,427.87299999999999,1.8853559864858025,1.7345275075669384,2.7765294060571373,2.4501590723869335,3.3597856977992373E-3,5]
[null,"CWD23","Short Rural",11,"CWD",0,83.691999999999993,1.4314920031218652,1.3624688328187504,2.7765294060571373,2.6835529187068397,84.031999999999996,1.0855079922190984,0.9986673528415706,2.7765294060571373,2.6835529187068397,3.3597856977992373E-3,3]
[null,"CWD33","Short Rural",11,"CWD",0,97.147999999999996,0.89706832195636876,0.8538138018997502,2.7258495994276717,2.7258495994276717,97.108999999999995,1.0188539926968732,0.93734567328112339,2.7258495994276717,2.7258495994276717,3.3597856977992373E-3,3]
[null,"CWD53","Short Rural",11,"CWD",0,11.207000000000001,1.603271043496489,1.5259650927570005,2.7258495994276717,2.7258495994276717,11.438000000000001,2.8089899798652112,2.5842707814759942,2.0738710344425955,2.0738710344425955,3.3597856977992373E-3,3]
[null,"CWD63","Short Rural",11,"CWD",0,23.658000000000001,2.0231753644122361,1.9256226170505006,2.7258495994276717,2.7258495994276717,24.170999999999999,0,0,1.5693592752139327,1.5693592752139327,3.3597856977992373E-3,3]
[null,"DBS3B1","Long Rural",11,"DBS",0,458.75599999999997,4.5768737612601305,4.4070842680411761,9.011860351780868,6.9684734115514848,456.17899999999997,3.374308606013352,3.2055931757126843,9.011860351780868,6.9684734115514848,2.2312017250554865E-2,5]
[null,"DBS3B2","Urban",11,"DBS",0,11.513,5.8211775025010635,5.6052277451682091,9.011860351780868,9.011860351780868,12.506,4.7802705251855819,4.5412569989263023,9.011860351780868,9.011860351780868,2.2312017250554865E-2,1]
[null,"DBS3B8","Short Rural",11,"DBS",0,14.867000000000001,5.4100162662649289,5.2093194657697115,9.011860351780868,8.1516373182017858,15.632999999999999,4.3116165521281715,4.0960357245217631,9.011860351780868,8.1516373182017858,2.2312017250554865E-2,3]
[null,"DBS3B9","Urban",11,"DBS",0,12.994,5.2044356481468608,5.0113653260704618,9.011860351780868,9.011860351780868,9.1379999999999999,3.5617701952363161,3.3836816854745,9.011860351780868,9.011860351780868,2.2312017250554865E-2,1]
[null,"DBW3B2","Short Rural",11,"DBW",0,38.579000000000001,7.1973669090025849,6.8939670188369693,9.011860351780868,3.0665093522603191,37.692999999999998,5.626656951598898,5.2890575345029642,9.011860351780868,2.9293309283008635,8.8773968167260679E-3,3]
[null,"DBW3B3","Short Rural",11,"DBW",0,139.9,2.7470114468012605,2.6312131303085016,9.011860351780868,4.5916666908650932,143.39699999999999,2.3595658184124413,2.2179918693076948,9.011860351780868,4.3954253343675402,8.8773968167260679E-3,3]
[null,"DBW3B4","Urban",11,"DBW",0,10.475,3.9777513423215383,3.8100720596581885,9.011860351780868,6.4092808083278738,11.507,3.4485961961412603,3.2416804243727846,9.011860351780868,6.1053924941399149,8.8773968167260679E-3,1]
[null,"DBW3B5","Short Rural",11,"DBW",0,114.614,2.0873348628023916,1.9993447441770693,9.011860351780868,4.1477420688851909,109.53,1.9058031610254331,1.791454971363907,9.011860351780868,3.9257797578952389,8.8773968167260679E-3,3]
[null,"DEN12","Long Rural",22,"DEN",0,498.28800000000001,3.1526243130890372,3.0201105753188706,4.8881245070885821,4.8881245070885821,423.75,3.8917768004381617,3.6718914112134056,4.8881245070885821,4.8881245070885821,-2.023633564774942E-3,6]
[null,"DEN22","Urban",22,"DEN",0,12.994,4.6301228717606158,4.4355056807668189,4.0715318333521591,4.0715318333521591,13.547000000000001,5.3128790688559144,5.0127014014655549,8.2364212052322827,8.2364212052322827,-2.023633564774942E-3,2]
[null,"DEN32","Urban",22,"DEN",0,21.882999999999999,5.3829883793639679,5.1567261166638625,4.0715318333521591,4.0715318333521591,22.189,5.6658325734302588,5.3457130330314495,4.0715318333521591,4.0715318333521591,-2.023633564774942E-3,2]
[null,"DEN42","Short Rural",22,"DEN",0,29.731000000000002,5.8064752273908535,5.5624126118559492,11.241009741122012,7.8915698894453197,30.800999999999998,6.0187860780046032,5.6787246645973433,11.241009741122012,7.8915698894453197,-2.023633564774942E-3,4]
[null,"DEN52","Long Rural",22,"DEN",0,415.959,1.6845365732625004,1.6137307253196351,4.8881245070885821,4.8881245070885821,416.089,1.7647675228717199,1.6650581578294676,4.8881245070885821,4.8881245070885821,-2.023633564774942E-3,6]
[null,"DEN62","Long Rural",22,"DEN",0,901.26300000000003,3.1902675884692049,3.0561715971137229,4.8881245070885821,4.8881245070885821,869.33699999999999,2.8329162867151294,2.6728565165157248,4.8881245070885821,4.8881245070885821,-2.023633564774942E-3,6]
[null,"DNO112","Long Rural",22,"DNO",0,583.00900000000001,1.4505515242300075,1.4384393196893008,5.5530588121142745,3.5171023698493626,583.88599999999997,1.0887694887777628,1.0561064041144299,5.5530588121142745,3.5171023698493626,5.4155769600972665E-4,5]
[null,"DNO122","Long Rural",22,"DNO",0,486.04199999999997,2.4365669198326367,2.4162214192301685,5.5530588121142745,3.4370816225396803,484.59500000000003,1.9471390698268984,1.8887248977320914,5.5530588121142745,3.4370816225396803,5.4155769600972665E-4,5]
[null,"DNO132","Short Rural",22,"DNO",0,5.5,0.97802337618538393,0.96985681403293766,5.5530588121142745,5.5530588121142745,5.6239999999999997,0.72584632585184194,0.70407093607628668,5.5530588121142745,5.5530588121142745,5.4155769600972665E-4,3]
[null,"DNO142","Long Rural",22,"DNO",0,468.267,1.3966053931636024,1.3849436425107733,10.821853445690346,3.6561860496971432,468.67099999999999,1.0887694887777628,1.0561064041144299,10.821853445690346,3.6466597702555141,5.4155769600972665E-4,5]
[null,"DOR3B1","Long Rural",11,"DOR",0,216.696,0.47126801970856197,0.44770461872313383,1.7337828583764461,1.7337828583764461,216.68600000000001,0.50991491262072564,0.48441916698968934,1.7337828583764461,1.7337828583764461,-1.7895469471319776E-2,6]
[null,"DOR3B2","Short Rural",11,"DOR",0,30.992000000000001,0.73517811074535666,0.69841920520808876,2.7765294060571373,2.7765294060571373,31.14,0.64150585781317104,0.60943056492251246,2.7765294060571373,2.7765294060571373,-1.7895469471319776E-2,4]
[null,"DOR3B3","Short Rural",11,"DOR",0,4.1079999999999997,0.63149914640947302,0.59992418908899936,2.7765294060571373,2.7765294060571373,4.26,0.57571038521694839,0.5469248659561009,2.7765294060571373,2.7765294060571373,-1.7895469471319776E-2,4]
[null,"DOR3B4","Short Rural",11,"DOR",0,92.218000000000004,0.47126801970856197,0.44770461872313383,2.7765294060571373,2.7765294060571373,92.444000000000003,0.67440359411128237,0.64068341440571819,2.7765294060571373,2.7765294060571373,-1.7895469471319776E-2,4]
[null,"DOR3B5","Short Rural",11,"DOR",0,33.5,0.41471585734353456,0.39398006447635781,2.2965954477878769,2.2965954477878769,33.57,0.42767057187544738,0.40628704328167498,2.2965954477878769,2.2965954477878769,-1.7895469471319776E-2,4]
[null,"DOR3B6","Short Rural",11,"DOR",0,67.944000000000003,0.61264842562113053,0.58201600434007394,3.5163402674940318,3.5163402674940318,68.346000000000004,0.49346604447166992,0.46879274224808642,3.5163402674940318,3.5163402674940318,-1.7895469471319776E-2,4]
[null,"DPR1100","Short Rural",33,"DPR",0,71.917000000000002,2.86,2.3470515364797664,9.4573091784714318,9.4573091784714318,0,"","","","",{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"DPT930","Short Rural",11,"DPT",0,35.220999999999997,0.13,0.1066841607490803,3.0379305139354327,3.0379305139354327,35.222999999999999,2.1,1.73481,3.0379305139354327,3.0379305139354327,1.7376151177270989E-2,3]
[null,"DPT931","Short Rural",11,"DPT",0,53.124000000000002,2.84,2.3306385886722154,2.8321628779962498,2.8321628779962498,53.01,2.9,2.3956899999999997,2.8321628779962498,2.8321628779962498,1.7376151177270989E-2,3]
[null,"DPT933","Short Rural",11,"DPT",0,15.098000000000001,0.91,0.74678912524356211,2.1653233170822319,2.1653233170822319,15.119,0.4,0.33044000000000001,2.1653233170822319,2.1653233170822319,1.7376151177270989E-2,3]
[null,"DPT934","Short Rural",11,"DPT",0,14.544,1.43,1.1735257682398832,6.763658403556466,2.7083212452550751,14.444000000000001,1.5,1.23915,6.763658403556466,2.7083212452550751,1.7376151177270989E-2,3]
[null,"DTN23","Long Rural",22,"DTN",0,364.512,3.8102489359651943,3.5521030033948393,10.821853445690346,6.7731846829980942,364.88799999999998,3.0882442383229147,2.8624935845015096,6.4340491348761102,6.4340491348761102,-7.1706297624720434E-3,6]
[null,"DTN24","Short Rural",22,"DTN",0,50.77,2.8767379466537215,2.6818377675631035,10.821853445690346,7.0570678103586344,118.372,8.5668196064746205,7.9405850932413253,7.0913624163484981,7.0913624163484981,-7.1706297624720434E-3,4]
[null,"DTN25","Short Rural",22,"DTN",0,81.590999999999994,3.3911215530090231,3.161371673021407,10.821853445690346,7.3542877289374529,82.161000000000001,3.9249677542305257,3.6380526113962741,7.028488972033748,7.028488972033748,-7.1706297624720434E-3,4]
[null,"DUG3B1","Short Rural",11,"DUG",0,125.976,3.4285130581674874,3.4098577371653702,9.0880705873138989,2.5987690316763432,125.652,2.446600831766061,2.373202806813079,9.0880705873138989,2.5987690316763432,2.5500831223981241E-7,3]
[null,"DUG3B4","Short Rural",11,"DUG",0,4.3869999999999996,0.1719313333004345,0.17099581572805694,9.0880705873138989,5.227069529621736,4.3890000000000002,0.18349506238245458,0.17799021051098093,9.0880705873138989,5.4861843304340399,2.5500831223981241E-7,3]
[null,"DUG3B5","Short Rural",11,"DUG",0,68.247,3.4689674895322957,3.4500920467484426,9.0880705873138989,3.8200380560931584,68.48,2.9155326578545568,2.8280666781189199,9.0880705873138989,3.8200380560931584,2.5500831223981241E-7,3]
[null,"DUG3B6","Short Rural",11,"DUG",0,116.504,2.4474930975708906,2.4341757297758688,9.0880705873138989,5.4004478154593807,114.67400000000001,1.9572806654128496,1.898562245450464,9.0880705873138989,5.4052109551801948,2.5500831223981241E-7,3]
[null,"DUG3B7","Short Rural",11,"DUG",0,122.554,0.8293158429785662,0.82480334645298037,9.0880705873138989,3.8695747091896293,121.616,0.69320356900038405,0.67240746193037249,9.0880705873138989,3.8695747091896293,2.5500831223981241E-7,3]
[null,"DUN3B1","Short Rural",11,"DUN",0,53.444000000000003,1.2410402964753626,1.2394984987350757,2.7765294060571373,2.7765294060571373,53.619,1.1422476228519862,1.1194026703949465,2.7765294060571373,2.7765294060571373,-5.6163006635975392E-3,4]
[null,"DUN3B2","Short Rural",11,"DUN",0,56.581000000000003,1.809767430734939,1.8075190788135094,2.7765294060571373,2.7765294060571373,55.948999999999998,1.3785747172351559,1.3510032228904527,2.7765294060571373,2.7765294060571373,-5.6163006635975392E-3,4]
[null,"DUN3B3","Short Rural",11,"DUN",0,84.576999999999998,1.373510889919362,1.371804518262977,3.583405274763098,3.583405274763098,80.364999999999995,1.2210233209797097,1.1966028545601155,3.583405274763098,3.583405274763098,-5.6163006635975392E-3,4]
[null,"DUN3B4","Short Rural",11,"DUN",0,114.524,1.3057815639479939,1.304159335346456,3.5163402674940318,2.775005201346477,115.517,1.1816354719158479,1.1580027624775309,2.7765294060571373,2.7765294060571373,-5.6163006635975392E-3,4]
[null,"DUN3B5","Short Rural",11,"DUN",0,121.77800000000001,1.6514003303018869,1.6493487246410556,2.7765294060571373,2.7765294060571373,120.633,1.4573504153628791,1.4282034070556215,2.7765294060571373,2.7765294060571373,-5.6163006635975392E-3,4]
[null,"EGA1208","Short Rural",11,"EGA",0,56.828000000000003,0.55000000000000004,0.47531765576948398,1.2250795361934668,1.2250795361934668,56.238,0.7,0.61075000000000002,1.2250795361934668,1.2250795361934668,-5.4325763083287245E-7,4]
[null,"EGA1211","Short Rural",11,"EGA",0,26.423999999999999,0.99,0.85557178038507109,1.6575726228434156,1.6575726228434156,26.420999999999999,0.86,0.75035000000000007,1.6575726228434156,1.6575726228434156,-5.4325763083287245E-7,4]
[null,"ELI3B10","Short Rural",11,"ELI",0,50.625999999999998,1.0093790716864084,1.0061499625871757,5.0489281040632772,5.0489281040632772,50.484999999999999,0.92720564835443164,0.92349682576101388,8.9547026751310952,5.6262206382259841,-1.117809511447931E-2,4]
[null,"ELI3B3","Short Rural",11,"ELI",0,4.91,1.0956679386496602,1.0921627824504929,6.763658403556466,4.049621390636414,4.79,0.79994212799205866,0.79674235948009042,3.583405274763098,3.583405274763098,-1.117809511447931E-2,4]
[null,"ELI3B4","Short Rural",11,"ELI",0,65.570999999999998,1.7006933663105988,1.6952526705618916,5.0489281040632772,5.0489281040632772,65.572000000000003,1.5271622443484756,1.5210535953710818,2.0357659166760795,2.0357659166760795,-1.117809511447931E-2,4]
[null,"ELI3B5","Short Rural",11,"ELI",0,12.239000000000001,3.362255734812281,3.3514995274648367,5.0489281040632772,5.0489281040632772,12.148999999999999,2.5998119159741906,2.5894126683102936,7.2399723756379064,7.2399723756379064,-1.117809511447931E-2,4]
[null,"ELI3B6","Short Rural",11,"ELI",0,26.588999999999999,3.04519431666824,3.0354524219205548,5.0489281040632772,5.0489281040632772,26.077999999999999,2.7997974479722054,2.7885982581803166,2.0357659166760795,2.0357659166760795,-1.117809511447931E-2,4]
[null,"ELI3B7","Short Rural",11,"ELI",0,7.6040000000000001,2.2746146675080396,2.2673379375597684,6.763658403556466,6.763658403556466,7.6059999999999999,2.0907578345246987,2.0823948031865998,3.583405274763098,3.583405274763098,-1.117809511447931E-2,4]
[null,"ELI3B8","Short Rural",11,"ELI",0,58.1,2.0458488341636052,2.0393039500151602,5.0489281040632772,5.0489281040632772,57.295000000000002,1.3998987239861027,1.3942991290901583,2.0357659166760795,2.0357659166760795,-1.117809511447931E-2,4]
[null,"ELI3B9","Short Rural",11,"ELI",0,6.5389999999999997,1.6435019079744899,1.6382441736757392,6.763658403556466,6.763658403556466,6.8070000000000004,1.3089962094415504,1.3037602246037843,3.583405274763098,3.583405274763098,-1.117809511447931E-2,4]
[null,"ELL8B1","Short Rural",22,"ELL",0,29.350999999999999,0.50558204310823307,0.4997362668927755,7.2399723756379064,7.2399723756379064,29.375,0.45726141319818359,0.45172855009848556,7.2399723756379064,7.2399723756379064,-7.1706297624706599E-3,4]
[null,"ELL8B2","Long Rural",22,"ELL",0,654.03300000000002,3.0723831850423395,3.0368588526560973,7.2399723756379064,7.2399723756379064,654.09,2.9721991857881931,2.9362355756401559,7.2399723756379064,7.2399723756379064,-7.1706297624706599E-3,6]
[null,"EME1E08","Short Rural",11,"EME_11",0,78.811000000000007,7.1235731865974747E-2,6.7673945272676006E-2,1.7337828583764461,0.92881224555881048,78.843999999999994,0.12888863332432748,0.12502197432459766,1.7337828583764461,0.92881224555881048,-4.8708168329081325E-4,4]
[null,"EME1E09","Short Rural",11,"EME_11",0,19.919,0.24932506153091163,0.23685880845436605,1.7337828583764461,1.0678959254065914,20.081,0.30933271997838596,0.3000527383790344,1.7337828583764461,1.0678959254065914,-4.8708168329081325E-4,4]
[null,"EME1E10","Short Rural",11,"EME_11",0,151.20500000000001,0.46303225712883589,0.43988064427239409,2.0357659166760795,0.8840387321831551,151.50800000000001,0.45540650441262381,0.44174430928024511,2.0357659166760795,0.8840387321831551,-4.8708168329081325E-4,4]
[null,"EME2E04","Short Rural",22,"EME_22",0,77.248999999999995,0.148547458858339,0.14112008591542205,3.4675657167528922,1.8842980735541817,77.277000000000001,0.12971338428981158,0.12582198276111722,3.4675657167528922,1.8271403969044089,1.63370366122337E-2,3]
[null,"ESH3B1","Short Rural",11,"ESH",0,107.61499999999999,0.84,0.81133508201137805,7.2399723756379064,3.6104599083773246,109.295,0.70399999999999996,0.67450239999999995,7.2399723756379064,3.6104599083773246,0,3]
[null,"ESH3B2","Short Rural",11,"ESH",0,8.3610000000000007,2.2000000000000002,2.1249252147917046,7.2399723756379064,4.7936238150276251,8.8840000000000003,2.0190000000000001,1.9344039,7.2399723756379064,4.7936238150276251,0,3]
[null,"ESH3B5","Short Rural",11,"ESH",0,10.076000000000001,0.61,0.58918380955588168,7.2399723756379064,4.0096110169815731,10.279,0.45700000000000002,0.43785170000000001,7.2399723756379064,4.0096110169815731,0,3]
[null,"ESH3B6","Short Rural",11,"ESH",0,35.890999999999998,3,2.8976252928977786,7.2399723756379064,3.9114903387327957,36.234000000000002,2.476,2.3722555999999999,7.2399723756379064,3.9114903387327957,0,3]
[null,"ETH3B10","Urban",11,"ETH",0,4.532,3.1181312436411464,3.1025519687737786,5.1441908984795655,5.1441908984795655,4.9390000000000001,3.0217127531948624,3.0035824766756933,5.1441908984795655,5.1441908984795655,3.3904961459936166E-8,1]
[null,"ETH3B11","Urban",11,"ETH",0,1.9930000000000001,3.8263503273703656,3.8072325421230278,6.4778700203076003,6.4778700203076003,1.98,2.6544327500441054,2.6385061535438408,6.4778700203076003,6.4778700203076003,3.3904961459936166E-8,1]
[null,"ETH3B12","Urban",11,"ETH",0,6.5880000000000001,2.3902394075861153,2.3782969350537164,5.715767664977295,5.715767664977295,6.6109999999999998,3.4891600299321892,3.468225069752596,5.715767664977295,5.715767664977295,3.3904961459936166E-8,1]
[null,"ETH3B13","Short Rural",11,"ETH",0,54.231999999999999,1.9967843610698821,1.9868077276374667,5.715767664977295,5.715767664977295,55.293999999999997,1.9365672893403538,1.9249478856043116,5.715767664977295,5.715767664977295,3.3904961459936166E-8,3]
[null,"ETH3B14","Short Rural",11,"ETH",0,191.32499999999999,2.0951481226989404,2.0846800294915289,9.0499654695473861,3.8829115004079089,213.36099999999999,4.3405818554180344,4.314538364285526,9.0499654695473861,3.8829115004079089,3.3904961459936166E-8,3]
[null,"ETH3B2","Urban",11,"ETH",0,1.698,4.4263692733076212,4.4042535834328085,8.9547026751310952,8.9547026751310952,4.0830000000000002,4.6076945849822213,4.5800484174723275,8.9547026751310952,8.9547026751310952,3.3904961459936166E-8,1]
[null,"ETH3B3","Urban",11,"ETH",0,6.8179999999999996,2.3607302790973979,2.3489352444974978,5.715767664977295,5.715767664977295,7.335,2.0868181997202089,2.0742972905218875,5.715767664977295,5.715767664977295,3.3904961459936166E-8,1]
[null,"ETH3B4","Urban",11,"ETH",0,1.698,0.77707371686956017,0.77319118464709302,5.715767664977295,5.715767664977295,2.0369999999999999,2.5041818396642506,2.4891567486262649,5.715767664977295,5.715767664977295,3.3904961459936166E-8,1]
[null,"ETH3B5","Urban",11,"ETH",0,2.9620000000000002,3.4033861523654152,3.3863816441505592,8.9547026751310952,8.9547026751310952,0.65700000000000003,3.4056873019433809,3.3852531781317206,8.9547026751310952,8.9547026751310952,3.3904961459936166E-8,1]
[null,"ETH3B6","Urban",11,"ETH",0,10.279,4.7017878058689844,4.6782960286241835,5.715767664977295,5.715767664977295,11.054,4.023385489060562,3.9992451761261987,5.715767664977295,5.715767664977295,3.3904961459936166E-8,1]
[null,"ETH3B7","Short Rural",11,"ETH",0,28.542000000000002,5.3116431279691456,5.2851043001193707,5.715767664977295,3.7304910293418478,6.6749999999999998,1.2520909198321253,1.2445783743131325,5.715767664977295,3.7304910293418478,3.3904961459936166E-8,3]
[null,"ETH3B8","Urban",11,"ETH",0,9.3309999999999995,1.4262745436213444,1.4191483768839048,6.4778700203076003,6.4778700203076003,9.6739999999999995,1.5358981949940735,1.5266828058241091,6.4778700203076003,6.4778700203076003,3.3904961459936166E-8,1]
[null,"ETH3B9","Urban",11,"ETH",0,5.1550000000000002,2.6459851878216667,2.6327649198742789,5.1441908984795655,5.1441908984795655,5.4290000000000003,4.6243891305799822,4.5966427957965026,5.1441908984795655,5.1441908984795655,3.3904961459936166E-8,1]
[null,"EUB1180","Short Rural",11,"EUB",0,114.592,0.60259640780686263,0.54747269048340497,1.541733064833209,0.63635546670080545,112.991,0.60501276995843001,0.54451149296258705,1.541733064833209,0.63635546670080545,-3.0649963261818954E-2,4]
[null,"EUB1201","Short Rural",11,"EUB",0,41.71,0.22720848163209575,0.20642412919866091,1.3504453736453019,0.66683956091401775,41.78,0.24381111625190463,0.21943000462671416,1.3504453736453019,0.66683956091401775,-3.0649963261818954E-2,4]
[null,"EUB417","Short Rural",11,"EUB",0,80.045000000000002,0.64211092635157496,0.58337253903969388,1.5693592752139327,0.59062932538098711,80.384,0.72240330741305081,0.65016297667174572,1.5693592752139327,0.59062932538098711,-3.0649963261818954E-2,4]
[null,"EUC1412 No.2","Short Rural",11,"EUC",0,4.3289999999999997,0.13,0.12217314429846957,2.3941445492701559,0.78972856571102967,4.4349999999999996,0.112,0.1083712,2.4440622535442911,0.78972856571102967,2.8891371806835747E-2,3]
[null,"EUC1412 No.3","Short Rural",11,"EUC",0,69.488,0.13,0.12217314429846957,2.4440622535442911,0.45059301758904347,69.566999999999993,0.27600000000000002,0.26705760000000001,2.4440622535442911,0.45059301758904347,2.8891371806835747E-2,3]
[null,"EUC76","Short Rural",11,"EUC",0,5.0000000000000001E-3,0.1,9.3979341768053504E-2,2.4440622535442911,2.4440622535442911,5.0000000000000001E-3,9.8000000000000004E-2,9.4824800000000001E-2,2.4440622535442911,2.4440622535442911,2.8891371806835747E-2,3]
[null,"EUL32","Short Rural",11,"EUL",0,11.05,4.3307118894013499,4.1229431934450993,9.011860351780868,9.011860351780868,13.183,3.6902550267855077,3.4319371749105221,9.011860351780868,9.011860351780868,0,3]
[null,"EUL42","Long Rural",11,"EUL",0,341.45699999999999,6.1851999014469774,5.8884609470738178,9.011860351780868,7.6867548814502999,339.24900000000002,5.4382705657891695,5.0575916261839282,9.011860351780868,7.6867548814502999,0,5]
[null,"EUL52","Long Rural",11,"EUL",0,341.512,2.3047105352012136,2.1941405608680604,9.011860351780868,7.359050868658267,343.15699999999998,1.4566796158363846,1.3547120427278379,9.011860351780868,7.359050868658267,0,5]
[null,"EUL62","Urban",11,"EUL",0,8.5730000000000004,5.3597919423284033,5.102652467135024,9.011860351780868,8.7689402260193337,10.64,5.0498226682327996,4.6963350814565041,9.011860351780868,8.7689402260193337,0,1]
[null,"EUL72","Short Rural",11,"EUL",0,13.074,2.8835680649726809,2.7452270273186432,9.011860351780868,9.011860351780868,13.507999999999999,2.7191352828945847,2.5287958130919641,9.011860351780868,9.011860351780868,0,3]
[null,"EUL82","Short Rural",11,"EUL",0,6.8120000000000003,2.3690280385091542,2.2553723904736809,9.011860351780868,9.011860351780868,6.5620000000000003,1.3595676414472924,1.2643979065459821,9.011860351780868,9.011860351780868,0,3]
[null,"EWE3B1","Short Rural",11,"EWE",0,27.817,1.72826864425265,1.7168775147864677,9.0499654695473861,6.1539765192922209,28.154,3.2954723979723188,3.2295629500128724,9.0499654695473861,6.1539765192922209,1.064220297536742E-2,3]
[null,"EWE3B10","Short Rural",11,"EWE",0,11.204000000000001,0.20275777390673547,0.20142138441628948,8.9547026751310952,8.9547026751310952,11.234,0.18618488124137395,0.18246118361654645,8.9547026751310952,8.9547026751310952,1.064220297536742E-2,3]
[null,"EWE3B11","Short Rural",11,"EWE",0,9.5359999999999996,2.5779202682427798,2.5609290304356809,6.1920816370587364,5.9501141392413635,9.2360000000000007,1.936322764910289,1.8975963096120831,6.1920816370587364,5.9501141392413635,1.064220297536742E-2,3]
[null,"EWE3B2","Short Rural",11,"EWE",0,9.6080000000000005,0.83034135980853574,0.82486852665718557,8.9547026751310952,8.9547026751310952,9.6809999999999992,1.750137883668915,1.7151351259955367,8.9547026751310952,8.9547026751310952,1.064220297536742E-2,3]
[null,"EWE3B3","Short Rural",11,"EWE",0,39.643000000000001,0.42482581199506481,0.42202575782460661,9.0499654695473861,2.7254685482500074,39.646999999999998,0.42822522685516007,0.41966072231805684,9.0499654695473861,2.7254685482500074,1.064220297536742E-2,3]
[null,"EWE3B4","Short Rural",11,"EWE",0,10.789,2.9448152876930629,2.9254058212842047,9.0499654695473861,5.236595809063366,10.79,2.8672471711171585,2.8099022276948151,9.0499654695473861,5.236595809063366,1.064220297536742E-2,3]
[null,"EWE3B5","Short Rural",11,"EWE",0,18.654,0.58896305753861256,0.58508116425684098,8.9547026751310952,8.9547026751310952,18.035,0.65164708434480878,0.63861414265791261,8.9547026751310952,8.9547026751310952,1.064220297536742E-2,3]
[null,"EWE3B6","Short Rural",11,"EWE",0,8.0329999999999995,1.9503366823409793,1.9374818881947848,8.9547026751310952,8.9547026751310952,8.2680000000000007,2.2156000867723495,2.1712880850369025,8.9547026751310952,8.9547026751310952,1.064220297536742E-2,3]
[null,"EWE3B7","Short Rural",11,"EWE",0,39.829000000000001,3.5241232131408786,3.5008954910450321,9.0499654695473861,9.0499654695473861,40.6,3.314090886096456,3.2478090683745267,9.0499654695473861,9.0499654695473861,1.064220297536742E-2,3]
[null,"EWE3B8","Short Rural",11,"EWE",0,106.703,1.72826864425265,1.7168775147864677,9.0499654695473861,3.4170764357122598,106.316,1.4708605618068542,1.4414433505707172,9.0499654695473861,4.6793084617280796,1.064220297536742E-2,3]
[null,"EWE3B9","Short Rural",11,"EWE",0,66.760000000000005,0.9558580769888958,0.94955795510536478,9.0499654695473861,3.744780448504291,39.246000000000002,0.80059498933790796,0.78458308955114975,9.0499654695473861,3.9076798269561444,1.064220297536742E-2,3]
[null,"FBS102","Short Rural",11,"FBS",0,73.254000000000005,0.94013578826133182,0.93650260264271268,3.583405274763098,3.4361289945955176,72.8,0.736204743665409,0.72884269622875486,3.583405274763098,3.4361289945955176,5.2294710830278584E-10,3]
[null,"FBS32","Short Rural",11,"FBS",0,1.9490000000000001,3.0993487525098846E-2,3.0873712175034478E-2,1.6651936463967185,1.6651936463967185,1.9590000000000001,3.1014150112976487E-2,3.0704008611846721E-2,1.6651936463967185,1.6651936463967185,5.2294710830278584E-10,3]
[null,"FBS42","Long Rural",11,"FBS",0,289.74599999999998,1.281064151037419,1.2761134365680917,2.7765294060571373,2.7765294060571373,292.202,1.220228856903993,1.2080265683349529,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,5]
[null,"FBS52","Short Rural",11,"FBS",0,15.516999999999999,4.7420035913401239,4.7236779627802754,2.7765294060571373,2.7765294060571373,16.72,4.6500888021849667,4.6035879141631169,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,3]
[null,"FBS62","Short Rural",11,"FBS",0,133.774,1.425700426154547,1.420190760051586,2.7765294060571373,2.7765294060571373,133.87299999999999,1.2781897276069325,1.2654078303308631,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,3]
[null,"FBS72","Short Rural",11,"FBS",0,65.997,3.3266343276939434,3.3137784401203678,2.7765294060571373,2.7765294060571373,66.528999999999996,3.1776793148541485,3.1459025217056071,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,3]
[null,"FBS82","Short Rural",11,"FBS",0,19.734999999999999,2.9340501523760243,2.9227114192365975,2.7765294060571373,2.7765294060571373,20.225999999999999,2.8095769430214435,2.7814811735912288,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,3]
[null,"FBS92","Short Rural",11,"FBS",0,127.557,1.9215962265561286,1.9141701548521377,2.7765294060571373,2.7765294060571373,127.10599999999999,1.6666292470547037,1.6499629545841568,2.7765294060571373,2.7765294060571373,5.2294710830278584E-10,3]
[null,"FFD3381","Short Rural",11,"FFD",0,0,"","","","",245.00299999999999,2.247459059173309,2.0676623344394445,2.7765294060571373,2.7765294060571373,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"FFD3382","Short Rural",11,"FFD",0,0,"","","","",48.674999999999997,1.746227182667031,1.6065290080536687,2.7765294060571373,2.7765294060571373,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"FHL3B1","Short Rural",11,"FHL",0,1.2709999999999999,1.8121291531087547,1.7099250364958936,9.0880705873138989,5.7386307356372033,0.95899999999999996,1.5769417865043451,1.3597969025026968,9.0880705873138989,5.7386307356372033,-1.3036310997015349E-2,4]
[null,"FHL3B2","Short Rural",11,"FHL",0,65.510999999999996,1.6736092977085417,1.5792177034152033,9.0880705873138989,3.6076020245448368,66.400000000000006,1.409971479698003,1.2158184069435878,9.0880705873138989,3.6076020245448368,-1.3036310997015349E-2,4]
[null,"FHL3B5","Short Rural",11,"FHL",0,2.1469999999999998,3.5849765561786429,3.3827838143569644,9.0880705873138989,5.6300311500026359,2.5369999999999999,3.107502932229151,2.6795997784611969,9.0880705873138989,5.6300311500026359,-1.3036310997015349E-2,4]
[null,"FHL3B6","Short Rural",11,"FHL",0,19.462,1.0637084418419329,1.0037152667166425,9.0880705873138989,3.8876746401287239,22.207999999999998,1.3264863262948317,1.1438291591640333,9.0880705873138989,3.8876746401287239,-1.3036310997015349E-2,4]
[null,"FIN22","Long Rural",22,"FIN",0,336.09100000000001,2.6270307977892395,2.5491858195111221,4.7882890985403117,4.6735926940631014,336.59300000000002,4.9175971993146232,4.6904042087062878,4.7882890985403117,4.6735926940631014,-1.2520246584434272E-2,6]
[null,"FIN32","Urban",22,"FIN",0,7.274,2.7381744084649382,2.6570359887981314,4.7882890985403117,4.7882890985403117,7.4509999999999996,2.5498652144594338,2.4320614415514079,4.7882890985403117,4.7882890985403117,-1.2520246584434272E-2,2]
[null,"FIN42","Long Rural",22,"FIN",0,433.16,3.7384669045462258,3.6276875123812129,4.0715318333521591,4.0715318333521591,433.49599999999998,4.0069310512933969,3.8218108367236421,4.0715318333521591,4.0715318333521591,-1.2520246584434272E-2,6]
[null,"FIN52","Long Rural",22,"FIN",0,321.233,6.6686166405419147,6.4710101572205403,4.0715318333521591,4.0715318333521591,323.07400000000001,5.7256717346940684,5.4611457005512021,4.0715318333521591,4.0715318333521591,-1.2520246584434272E-2,6]
[null,"FOR17253","Urban",11,"FOR",0,3.7080000000000002,2.7289813931883318,2.7275975456226158,7.9258644954351825,7.9258644954351825,3.8679999999999999,2.3654201296429931,2.318111727050133,7.9258644954351825,7.9258644954351825,-1.6359218092576427E-2,2]
[null,"FOR17254","Urban",11,"FOR",0,2.6219999999999999,2.3663894598276443,2.3651894801203102,7.2399723756379064,7.0875519045718454,2.9390000000000001,2.2509643169183327,2.2059450305799659,7.2399723756379064,7.0875519045718454,-1.6359218092576427E-2,2]
[null,"FOR17255","Short Rural",11,"FOR",0,5.4409999999999998,1.5076190913418057,1.5068545881411655,7.9258644954351825,6.8998841995717584,5.64,1.5260775029954794,1.4955559529355698,7.9258644954351825,6.8998841995717584,-1.6359218092576427E-2,4]
[null,"FOR17256","Urban",11,"FOR",0,4.9459999999999997,2.6335624633565717,2.6322270020693774,7.2399723756379064,6.0625242366525853,4.9550000000000001,1.8122170348071318,1.7759726941109892,7.2399723756379064,6.7341269372874173,-1.6359218092576427E-2,2]
[null,"FOR17259","Short Rural",11,"FOR",0,4.173,1.2022785158801743,1.2016688487708029,7.9258644954351825,5.8691407639875184,4.2560000000000002,1.239937971183827,1.2151392117601505,7.9258644954351825,5.8691407639875184,-1.6359218092576427E-2,4]
[null,"FOR17260","Urban",11,"FOR",0,4.734,1.7270826299548534,1.7262068383136135,7.9258644954351825,6.5093067424649771,5.0910000000000002,1.7168371908699145,1.6825004470525162,7.9258644954351825,7.3942981025922947,-1.6359218092576427E-2,2]
[null,"FOR17261","Short Rural",11,"FOR",0,16.792000000000002,5.1812478898645598,5.1786205149408397,7.2399723756379064,5.9034353699773829,17.422999999999998,3.6244340696142636,3.5519453882219785,7.2399723756379064,5.9034353699773829,-1.6359218092576427E-2,4]
[null,"FOR17262","Short Rural",11,"FOR",0,30.218,3.0534057546163158,3.0518573937036266,9.0880705873138989,5.8758091595966597,30.725999999999999,3.1475348499281766,3.084584152929613,9.0880705873138989,5.8758091595966597,-1.6359218092576427E-2,4]
[null,"GAN4951","Short Rural",11,"GAN",0,97.433000000000007,0.29577629226366786,0.2851390273094449,6.6683956091401777,0.58015041799519551,97.494,0.28308319995648129,0.25477487996083314,6.6683956091401777,0.57443465033021823,-4.3783572313951039E-2,4]
[null,"GAN4952","Short Rural",11,"GAN",0,90.138999999999996,0.33521313123215696,0.32315756428403764,6.6683956091401777,0.46869294852813825,90.837999999999994,0.37744426660864178,0.33969983994777758,6.6683956091401777,0.46869294852813825,-4.3783572313951039E-2,4]
[null,"GBN5702","Short Rural",11,"GBN",0,66.558000000000007,0.62840178706746741,0.62058846813900725,6.763658403556466,3.3780186900015816,69.070999999999998,1.0639703033162116,1.0213050941532316,6.763658403556466,3.3780186900015816,4.5141952178377125E-2,3]
[null,"GBN5712","Short Rural",11,"GBN",0,6.3380000000000001,0.93454624743366943,0.92292643979647226,6.763658403556466,6.763658403556466,2.7629999999999999,0,0,6.763658403556466,5.7500622709671587,4.5141952178377125E-2,3]
[null,"GBN5722","Urban",11,"GBN",0,3.484,0.95065911376873269,0.93883896462054928,6.763658403556466,6.0472821895459781,3.7949999999999999,0.77735653327644905,0.74618453629206338,6.763658403556466,6.0472821895459781,4.5141952178377125E-2,1]
[null,"GBN5732","Short Rural",11,"GBN",0,3.964,0.88620764842847977,0.87518886532424101,6.763658403556466,5.7433938753580174,4.2839999999999998,0.71736760466347538,0.68860116371646996,6.763658403556466,5.7433938753580174,4.5141952178377125E-2,3]
[null,"GBN5742","Short Rural",11,"GBN",0,2.4369999999999998,0.36253949253892354,0.35803180854173494,6.763658403556466,6.763658403556466,2.262,0.18746540191554237,0.1799480392987291,6.763658403556466,6.763658403556466,4.5141952178377125E-2,3]
[null,"GBN5752","Short Rural",11,"GBN",0,6.83,1.9093746607049973,1.8856341916531374,6.763658403556466,6.763658403556466,7.8470000000000004,1.6188678929862168,1.5539512904774695,6.763658403556466,6.763658403556466,4.5141952178377125E-2,3]
[null,"GBN6212","Short Rural",22,"GBN",0,161.65899999999999,1.1923521087946818,1.177526836981706,12.536583745183533,1.0936168798989894,161.56,0.88816941529763627,0.85255382174420102,1.0936168798989894,1.0936168798989894,4.5141952178377125E-2,3]
[null,"GBN6222","Long Rural",22,"GBN",0,483.97300000000001,1.1923521087946818,1.177526836981706,12.536583745183533,0.9964488295943752,482.72,1.0981306654430436,1.0540956257587775,0.9964488295943752,0.9964488295943752,4.5141952178377125E-2,5]
[null,"GDG3B2","Short Rural",11,"GDG",0,145.27000000000001,0.63657423150237635,0.62151980696707854,6.1920816370587364,6.1920816370587364,0,"","","","",1.4641812133948176E-2,3]
[null,"GDG3B3","Short Rural",11,"GDG",0,26.611000000000001,0.44759125652510839,0.4370061142737271,6.1920816370587364,6.1920816370587364,0,"","","","",1.4641812133948176E-2,3]
[null,"GDG3B6","Short Rural",11,"GDG",0,9.9600000000000009,1.4322920208803467,1.3984195656759266,6.1920816370587364,6.1920816370587364,0,"","","","",1.4641812133948176E-2,3]
[null,"GDG3B7","Short Rural",11,"GDG",0,12.646000000000001,2.4866180918061573,2.4278117459651503,6.1920816370587364,6.1920816370587364,0,"","","","",1.4641812133948176E-2,3]
[null,"GDG8B1","Long Rural",22,"GDG",0,216.952,1.1935766840669555,1.165349638063272,12.536583745183533,12.536583745183533,0,"","","","",1.4641812133948176E-2,5]
[null,"GDG8B8","Short Rural",22,"GDG",0,167.76599999999999,0.56694892493180382,0.55354107808005415,12.536583745183533,12.536583745183533,0,"","","","",1.4641812133948176E-2,3]
[null,"GDH6101","Long Rural",11,"GDH",0,246.12899999999999,1.0541525964562202,1.0533777805869105,3.5163402674940318,1.1688744874878569,245.91800000000001,0.89554238301593814,0.88658695918577879,2.4440622535442911,1.2755688172340998,1.2295611912729525E-2,5]
[null,"GDH6201","Short Rural",11,"GDH",0,140.279,1.7569209940937003,1.7556296343115174,3.5163402674940318,1.5118205473864945,140.40799999999999,1.2714258596228378,1.2587116010266095,2.0357659166760795,1.5118205473864945,1.2295611912729525E-2,3]
[null,"GDH6301","Short Rural",11,"GDH",0,114.449,1.7167627999429871,1.7155009569558255,2.0357659166760795,1.2736635613457741,114.754,1.3785526504558041,1.364767123951246,2.0357659166760795,1.2736635613457741,1.2295611912729525E-2,3]
[null,"GDH6501","Short Rural",11,"GDH",0,146.197,1.3352599555112121,1.334278522076753,2.0357659166760795,2.0357659166760795,146.09899999999999,1.0205236389877324,1.0103184025978551,2.7950103881738979,2.7950103881738979,1.2295611912729525E-2,3]
[null,"GDH6601","Short Rural",11,"GDH",0,21.96,0.28110735905499207,0.28090074148984279,2.0357659166760795,1.3127213070564521,55.481999999999999,1.0205236389877324,1.0103184025978551,1.3127213070564521,1.3127213070564521,1.2295611912729525E-2,3]
[null,"GDH6801","Short Rural",11,"GDH",0,108.411,0.42166103858248805,0.42135111223476412,2.1298855575593727,2.1298855575593727,109.139,0.35802901146807181,0.35444872135339112,4.1810840469308914,4.1810840469308914,1.2295611912729525E-2,3]
[null,"GDH6901","Short Rural",11,"GDH",0,103.565,0.57225426664766232,0.5718336523186085,2.1298855575593727,2.1298855575593727,103.626,0.50086473257869368,0.49585608525290675,2.62067947439209,2.62067947439209,1.2295611912729525E-2,3]
[null,"GDH8B1","Short Rural",22,"GDH",0,19.561,5.1603279483666391,5.156535040206399,7.0326805349880637,7.0326805349880637,20.417999999999999,4.5115414279743122,4.4664260136945693,4.8881245070885821,4.8881245070885821,1.2295611912729525E-2,3]
[null,"GDH8B15","Short Rural",22,"GDH",0,2.5249999999999999,0.50197742688391433,0.5016084669461478,12.536583745183533,12.536583745183533,1.6970000000000001,0.32232008119041639,0.31909688037851219,12.536583745183533,12.536583745183533,1.2295611912729525E-2,3]
[null,"GDH8B2","Long Rural",22,"GDH",0,328.56099999999998,2.7709153963992068,2.7688787375427353,7.0326805349880637,6.8341528714245197,296.84199999999998,2.8999410220222299,2.8709416118020075,4.0715318333521591,4.0715318333521591,1.2295611912729525E-2,5]
[null,"GDH8B3","Short Rural",22,"GDH",0,10.98,2.7909944934745634,2.7889430762205816,4.2597711151187454,4.2597711151187454,11.000999999999999,2.6142695798009865,2.5881268840029765,4.2597711151187454,4.2597711151187454,1.2295611912729525E-2,3]
[null,"GDH8B6","Short Rural",22,"GDH",0,11.827999999999999,0.57225426664766232,0.5718336523186085,7.0326805349880637,7.0326805349880637,11.846,0.25090222063510548,0.24839319842875443,7.0326805349880637,7.0326805349880637,1.2295611912729525E-2,3]
[null,"GDH8B9","Urban",22,"GDH",0,11.007,5.5518703413360928,5.5477896444243946,4.8881245070885821,4.8881245070885821,11.81,6.3373954155923267,6.2740214614364032,4.8881245070885821,4.8881245070885821,1.2295611912729525E-2,1]
[null,"GDI4B1","Long Rural",33,"GDI_33",0,1042.4590000000001,5.1050267834492811,5.1012237035714403,8.3295882181714092,8.3295882181714092,1038.7,4.5388025543125643,4.4480265032263127,8.3295882181714092,8.3295882181714092,1.8271961429889242E-2,5]
[null,"GDI4B2","Long Rural",33,"GDI_33",0,679.375,1.9410748226042893,1.9396287846279241,4.0513361209359067,4.0513361209359067,679.92700000000002,1.6409516927130039,1.6081326588587437,4.0513361209359067,4.0513361209359067,1.8271961429889242E-2,5]
[null,"GDI4B3","Short Rural",19.100000000000001,"GDI_33",0,66.228999999999999,0.18440210814740748,0.18426473453965278,2.3448642396932065,2.3448642396932065,65.328000000000003,0.26185399351803257,0.25661691364767192,2.3448642396932065,2.3448642396932065,1.8271961429889242E-2,3]
[null,"GDI4B4","Short Rural",19.100000000000001,"GDI_33",0,42.764000000000003,0.16693243474396888,0.16680807547800147,2.3448642396932065,2.3448642396932065,42.774000000000001,0.26185399351803257,0.25661691364767192,2.3448642396932065,2.3448642396932065,1.8271961429889242E-2,3]
[null,"GDI8B1","Long Rural",22,"GDI_22",0,291.95,1.6565450985045713,1.6422025334256118,4.7882890985403117,4.7882890985403117,292.95299999999997,1.5982652394724437,1.574291260880357,4.7882890985403117,4.7882890985403117,1.0918583097448253E-2,5]
[null,"GDI8B2","Long Rural",22,"GDI_22",0,297.66199999999998,3.6339916035257356,3.6025280707085421,5.5530588121142745,5.5530588121142745,297.05200000000002,3.7768529766104773,3.72020018196132,5.5530588121142745,5.5530588121142745,1.0918583097448253E-2,5]
[null,"GDI8B3","Long Rural",22,"GDI_22",0,766.25300000000004,2.0468305929166433,2.0291088894682954,6.4252849577898106,4.8946023771088916,766.40599999999995,2.3973978592086658,2.3614368913205359,6.4252849577898106,4.8946023771088916,1.0918583097448253E-2,5]
[null,"GDI8B4","Short Rural",22,"GDI_22",0,26.44,5.7848983282855979,5.7348119884548865,4.0715318333521591,4.0715318333521591,28.149000000000001,6.1361969015459898,6.0441539480227995,4.0715318333521591,4.0715318333521591,1.0918583097448253E-2,3]
[null,"GDI8B5","Urban",22,"GDI_22",0,18.254999999999999,3.798778812277499,3.7658885321487858,5.5530588121142745,5.5530588121142745,17.814,5.232415962558596,5.1539297231202168,5.5530588121142745,5.5530588121142745,1.0918583097448253E-2,1]
[null,"GDI8B6","Urban",22,"GDI_22",0,7.05,3.6339916035257356,3.6025280707085421,5.5530588121142745,5.5530588121142745,7.7960000000000003,4.2810676057297599,4.2168515916438132,5.5530588121142745,5.5530588121142745,1.0918583097448253E-2,1]
[null,"GDL3B1","Short Rural",11,"GDL",0,17.611999999999998,2.9713521245472139,2.9536597417753194,8.9547026751310952,6.6131431883787313,18.555,2.6195645660751063,2.5671732747536042,8.9547026751310952,6.6131431883787313,3.6519432317881843E-2,3]
[null,"GDL3B2","Urban",11,"GDL",0,1.3129999999999999,0.62398394615491493,0.62026854577281709,8.9547026751310952,8.9547026751310952,0,"","","","",3.6519432317881843E-2,1]
[null,"GDL3B5","Short Rural",11,"GDL",0,24.559000000000001,3.1199197307745745,3.1013427288640854,8.9547026751310952,8.0487535002321948,25.045000000000002,2.5664652843303406,2.5151359786437339,8.0344640810697516,8.0344640810697516,3.6519432317881843E-2,3]
[null,"GDL3B6","Urban",11,"GDL",0,1.401,2.3770816996377713,2.3629277934202557,9.0880705873138989,8.3335892555368964,1.57,2.6726638478198721,2.6192105708634745,8.3335892555368964,8.3335892555368964,3.6519432317881843E-2,1]
[null,"GDL3B8","Short Rural",11,"GDL",0,85.406999999999996,2.3275591642286511,2.3137001310573337,9.0880705873138989,9.079496935816433,78.426000000000002,2.1416710303722151,2.0988376097647707,9.079496935816433,9.079496935816433,3.6519432317881843E-2,3]
[null,"GDL3B9","Short Rural",11,"GDL",0,15.359,2.1690870509194662,2.1561716114959832,9.0880705873138989,3.6971490512961473,15.587,3.3806542710834142,3.3130411856617457,3.6971490512961473,3.6971490512961473,3.6519432317881843E-2,3]
[null,"GDM5422","Urban",11,"GDM",0,5.3250000000000002,1.4156093379433412,0.99265451331056365,3.905774571067818,3.905774571067818,375.46699999999998,1.1324945635586108,1.1255863467209033,3.905774571067818,3.905774571067818,3.9737476301020473E-2,1]
[null,"GDM5482","Short Rural",11,"GDM",0,3.056,1.4629277559247342,1.02583516556607,3.791459217768272,3.791459217768272,2.746,2.9156364102457463E-2,2.8978510281432474E-2,3.791459217768272,3.791459217768272,3.9737476301020473E-2,3]
[null,"GFH3B1","Short Rural",11,"GFH",0,9.1669999999999998,2.8863519100879778,2.8705036725713273,8.0020747309682125,8.0020747309682125,8.4589999999999996,3.0478145731743318,2.9387028114546907,7.9449170543184398,7.9449170543184398,3.3210249699695125E-11,3]
[null,"GFH3B10","Short Rural",11,"GFH",0,9.7639999999999993,2.0546911902321199,2.0434093940338265,9.0880705873138989,8.5222095884811466,10.545999999999999,2.1906167244690513,2.1121926457330593,8.5222095884811466,8.5222095884811466,3.3210249699695125E-11,3]
[null,"GFH3B2","Urban",11,"GFH",0,7,2.6123930847236951,2.5980490867001507,8.0020747309682125,7.8648963070087579,11.263999999999999,3.1430587785860298,3.0305372743126497,7.9449170543184398,7.8648963070087579,3.3210249699695125E-11,1]
[null,"GFH3B3","Urban",11,"GFH",0,0.99099999999999999,2.8472149350359377,2.8315815888754452,9.0880705873138989,9.0880705873138989,0.99099999999999999,3.2383029839977278,3.1223717371706088,9.0880705873138989,9.0880705873138989,3.3210249699695125E-11,1]
[null,"GFH3B4","Urban",11,"GFH",0,6.2629999999999999,3.1113895166372103,3.0943056538226514,9.0880705873138989,9.0880705873138989,5.8289999999999997,3.7145240110562172,3.5815440514604044,9.0880705873138989,9.0880705873138989,3.3210249699695125E-11,1]
[null,"GFH3B5","Short Rural",11,"GFH",0,32.709000000000003,2.9841943477180788,2.9678088818110333,9.0880705873138989,7.7562967213741896,33.146000000000001,3.2383029839977278,3.1223717371706088,9.0880705873138989,7.7562967213741896,3.3210249699695125E-11,3]
[null,"GFH3B6","Urban",11,"GFH",0,10.8,4.0995981367012302,4.0770882671436821,8.0020747309682125,8.0020747309682125,7.6980000000000004,3.3335471894094257,3.2142062000285683,7.9449170543184398,7.9449170543184398,3.3210249699695125E-11,1]
[null,"GFH3B7","Urban",11,"GFH",0,3.911,3.0722525415851698,3.0553835701267689,9.0880705873138989,9.0880705873138989,4.0570000000000004,2.8573261623509363,2.7550338857387726,9.0880705873138989,9.0880705873138989,3.3210249699695125E-11,1]
[null,"GFH3B8","Urban",11,"GFH",0,2.9780000000000002,3.3755640982384825,3.3570297187698572,9.0880705873138989,9.0880705873138989,4.0439999999999996,4.7622102705848937,4.5917231428979539,9.0880705873138989,9.0880705873138989,3.3210249699695125E-11,1]
[null,"GFH3B9","Short Rural",11,"GFH",0,8.9160000000000004,2.5145506470935941,2.5007438774604442,9.0880705873138989,6.5235961616274203,4.5270000000000001,1.7143956974105616,1.6530203314432634,9.0880705873138989,8.6641511521614163,3.3210249699695125E-11,3]
[null,"GGB112","Long Rural",22,"GGB",0,342.834,1.1212811607247934,1.0652171026885537,2.7008907472906039,1.4117946132493921,343.553,0.72845232323301101,0.70434055133399831,2.7008907472906039,1.4117946132493921,1.6105720423742417E-3,5]
[null,"GGB122","Long Rural",22,"GGB",0,271.58100000000002,0.39070894860577532,0.37117350117548653,2.7008907472906039,1.4251314044676722,271.65499999999997,0.29995095662535748,0.29002257996105812,2.7008907472906039,1.4251314044676722,1.6105720423742417E-3,5]
[null,"GGG12","Short Rural",22,"GGG",0,7.7009999999999996,0.80260075130422159,0.79000486099676803,7.2399723756379064,5.0127282421850881,8.0860000000000003,0.97600048829371489,0.88816044434728059,7.2399723756379064,5.0127282421850881,2.702294703882108E-3,3]
[null,"GGG22","Short Rural",22,"GGG",0,78.25,1.4819644581904967,1.4587067404216321,7.2399723756379064,3.1932088688339828,78.022000000000006,1.9200009605777997,1.7472008741257978,7.2399723756379064,3.1932088688339828,2.702294703882108E-3,3]
[null,"GGG32","Short Rural",22,"GGG",0,53.563000000000002,1.9031543568341116,1.8732865508572538,10.7075380923908,3.2198824512705428,53.845999999999997,1.6760008385043712,1.5251607630389779,10.7075380923908,3.2198824512705428,2.702294703882108E-3,3]
[null,"GID12","Short Rural",11,"GID",0,9.7850000000000001,1.9130631713795772,1.8470508844833882,1.2328910853356025,1.2328910853356025,10.576000000000001,1.0340637226818552,0.992701173774581,1.2328910853356025,1.2328910853356025,-1.1184192852423298E-3,4]
[null,"GID22","Long Rural",11,"GID",0,728.46500000000003,2.1256257459773078,2.0522787605370976,1.2328910853356025,1.2328910853356025,728.02800000000002,1.1801814226260303,1.1329741657209891,1.2328910853356025,1.2328910853356025,-1.1184192852423298E-3,6]
[null,"GID32","Long Rural",11,"GID",0,528.18799999999999,1.6792443393220733,1.6213002208243072,1.2328910853356025,1.2328910853356025,528.26599999999996,0.91042566888293774,0.87400864212762019,1.2328910853356025,1.2328910853356025,-1.1184192852423298E-3,6]
[null,"GID42","Short Rural",11,"GID",0,10.151999999999999,2.6570321824716348,2.565348450671372,1.2328910853356025,1.2328910853356025,11.273,1.3487787687154633,1.2948276179668448,1.2328910853356025,1.2328910853356025,-1.1184192852423298E-3,4]
[null,"GLR3B1","Urban",11,"GLR",0,2.5529999999999999,1.4132343315657443,1.3475301971870326,9.0499654695473861,5.003201962743459,2.0859999999999999,0.8583789808382174,0.84121140122145299,9.0499654695473861,5.003201962743459,2.1718732775233603E-13,1]
[null,"GLR3B2","Short Rural",11,"GLR",0,88.605000000000004,0.97222503660905812,0.92702432005065361,9.0499654695473861,2.3510857661939939,88.834999999999994,0.77254108275439559,0.75709026109930766,9.0499654695473861,2.3510857661939939,2.1718732775233603E-13,3]
[null,"GLR3B3","Short Rural",11,"GLR",0,100.096,2.5358034460009455,2.417908793534179,9.0499654695473861,3.2046404041639369,100.515,2.0386500794907665,1.9978770779009511,9.0499654695473861,3.2046404041639369,2.1718732775233603E-13,3]
[null,"GLR3B5","Long Rural",11,"GLR",0,397.55900000000003,2.7663310320010313,2.6377186838554678,9.0499654695473861,2.1691338288588837,397.541,3.1116238055385383,3.0493913294277677,9.0499654695473861,2.1691338288588837,2.1718732775233603E-13,5]
[null,"GLR3B6","Short Rural",11,"GLR",0,3.3,1.43328020860923,1.3666441006932317,9.0499654695473861,4.6869294852813814,0,"","","","",2.1718732775233603E-13,3]
[null,"GLR3B7","Long Rural",11,"GLR",0,227.292,1.513463716783173,1.443099714718028,6.1920816370587364,3.5247233934026649,226.137,1.1158926750896827,1.0935748215878891,6.1920816370587364,3.5247233934026649,2.1718732775233603E-13,5]
[null,"GLS3B1","Short Rural",11,"GLS",0,82.49,0.46060960266612799,0.46040053259837077,3.9057745710678189,3.9057745710678189,0,"","","","",-1.8922271819264466E-2,4]
[null,"GLS3B2","Short Rural",11,"GLS",0,147.27600000000001,1.7322926361139159,1.7315063508590898,3.9057745710678189,3.9057745710678189,147.18600000000001,1.872170560205044,1.8347271490009431,4.7564713252052728,4.7564713252052728,-1.8922271819264466E-2,4]
[null,"GLS3B3","Short Rural",11,"GLS",0,7.7809999999999997,1.2316300245202987,1.2310709893391218,3.9057745710678189,3.9057745710678189,8.3810000000000002,3.7946682860069978,3.7187749202868576,5.5966891719569345,5.5966891719569345,-1.8922271819264466E-2,4]
[null,"GLS3B4","Short Rural",11,"GLS",0,12.368,1.8824914195920011,1.8816369593150803,7.2399723756379064,6.0091770717794635,13.12,3.9859115152752547,3.9061932849697496,7.2399723756379064,6.0091770717794635,-1.8922271819264466E-2,4]
[null,"GLS3B5","Urban",11,"GLS",0,4.6340000000000003,1.2716830334477882,1.2711058182607193,7.2399723756379064,6.1377818442414531,5.0739999999999998,2.5666854454423986,2.5153517365335505,7.2399723756379064,6.1377818442414531,-1.8922271819264466E-2,2]
[null,"GLS3B6","Urban",11,"GLS",0,6.423,1.9025179240557459,1.9016543737758791,7.2399723756379064,6.6245747237086858,7.0359999999999996,2.1439372544283568,2.1010585093397895,7.2399723756379064,6.6245747237086858,-1.8922271819264466E-2,2]
[null,"GLS3B7","Urban",11,"GLS",0,4.6900000000000004,2.283021508866895,2.281985248531055,7.2399723756379064,5.832940902109331,4.96,4.8918004960196315,4.793964486099239,7.2399723756379064,5.832940902109331,-1.8922271819264466E-2,2]
[null,"GLS3B8","Short Rural",11,"GLS",0,133.90199999999999,0.79104692631791551,0.79068787120154982,3.9057745710678189,3.9057745710678189,0,"","","","",-1.8922271819264466E-2,4]
[null,"GLS5/9","Short Rural",11,"GLS",0,0,"","","","",192.04599999999999,1.4796186685491477,1.4500262951781646,5.1775328765252659,5.1775328765252659,-1.8922271819264466E-2,4]
[null,"GNF12","Long Rural",11,"GNF",0,548.22400000000005,1.6845110558629028,1.6002855030697576,1.6907240753002839,1.6842462052799763,563.11500000000001,1.6358822498905627,1.5540881373960345,1.6907240753002839,1.6842462052799763,-1.0951140848920016E-2,6]
[null,"GNF22","Short Rural",11,"GNF",0,14.519,1.3553537231080828,1.2875860369526786,2.7765294060571373,2.6483056847728133,14.574999999999999,1.1030520313547794,1.0478994297870403,2.7765294060571373,2.6483056847728133,-1.0951140848920016E-2,4]
[null,"GNF32","Short Rural",11,"GNF",0,3.1629999999999998,0.9874719982644603,0.93809839835123721,2.7765294060571373,2.7765294060571373,3.3340000000000001,0.85065876994309264,0.80812583144593797,2.7765294060571373,2.7765294060571373,-1.0951140848920016E-2,4]
[null,"GNF42","Long Rural",11,"GNF",0,494.56900000000002,1.1907750567306727,1.1312363038941391,2.7765294060571373,2.335843719087388,492.404,1.2432705099168277,1.1811069844209863,2.7765294060571373,2.335843719087388,-1.0951140848920016E-2,6]
[null,"GNG5212","Long Rural",11,"GNG",0,305.83999999999997,0.51004728143071698,0.49842726953153954,2.2965954477878769,0.53728216050786581,305.67899999999997,0.88221126660447946,0.8654492525389943,2.2965954477878769,0.53728216050786581,3.3369909020345061E-12,5]
[null,"GNG5222","Short Rural",11,"GNG",0,89.914000000000001,0.3800352293013185,0.37137718121957841,2.0357659166760795,0.42296680720831992,88.498999999999995,0.34477221913278511,0.33822154696926221,2.0357659166760795,0.55538209144696049,3.3369909020345061E-12,3]
[null,"GNI3B1","Short Rural",11,"GNI",0,154.24600000000001,0.22682772663906564,0.22467311103486884,1.7337828583764461,1.7337828583764461,154.232,0.30856583283561345,0.29930885785054506,1.7337828583764461,1.7337828583764461,6.1802037013924824E-7,3]
[null,"GNI3B3","Long Rural",11,"GNI",0,363.52699999999999,0.64267855881068603,0.63657381459879514,2.7765294060571373,2.7765294060571373,363.63400000000001,0.77141458208903357,0.7482721446263626,2.7765294060571373,2.7765294060571373,6.1802037013924824E-7,5]
[null,"GNI3B4","Short Rural",11,"GNI",0,36.140999999999998,2.7030304091155322,2.6773545731655202,2.7765294060571373,2.7765294060571373,36.167999999999999,2.7385217664160688,2.6563661134235868,2.7765294060571373,2.7765294060571373,6.1802037013924824E-7,3]
[null,"GNI3B5","Long Rural",11,"GNI",0,232.809,0.75609242213021888,0.74891037011622952,2.0357659166760795,2.0357659166760795,231.81700000000001,0.64605971249956562,0.62667792112457865,2.0357659166760795,2.0357659166760795,6.1802037013924824E-7,5]
[null,"GNI3B6","Short Rural",11,"GNI",0,131.29,1.3704175151110216,1.3574000458356659,1.3504453736453019,0.6106345122084077,131.28800000000001,1.1956926022380019,1.1598218241708618,1.3504453736453019,0.6106345122084077,6.1802037013924824E-7,3]
[null,"GNI3B7","Short Rural",11,"GNI",0,37.356999999999999,0.94511552766277351,0.93613796264528681,3.204640404163936,2.2748755306609634,37.368000000000002,1.1185511440290985,1.0849946097082255,3.204640404163936,3.204640404163936,6.1802037013924824E-7,3]
[null,"GNI3B8","Short Rural",11,"GNI",0,14.519,2.5234584588596052,2.4994883602629159,3.204640404163936,3.204640404163936,14.522,2.6228095791027144,2.5441252917296331,3.204640404163936,3.204640404163936,6.1802037013924824E-7,3]
[null,"GRN3B1","Urban",11,"GRN",0,8.9149999999999991,5.2993848703390727,5.2245707035629652,5.6205048705610059,5.6205048705610059,9.3569999999999993,5.1309383591376623,4.9257008247721554,5.6205048705610059,5.6205048705610059,5.8866076435834525E-3,1]
[null,"GRN3B2","Long Rural",11,"GRN",0,294.209,1.3422456988663691,1.3232965196641655,5.6205048705610059,5.6205048705610059,294.35399999999998,0.86614005328562371,0.83149445115419873,5.6205048705610059,5.6205048705610059,5.8866076435834525E-3,5]
[null,"GRN3B3","Short Rural",11,"GRN",0,77.427000000000007,1.0837391198254389,1.0684394121732892,5.6205048705610059,4.7679028605352265,76.998000000000005,0.86614005328562371,0.83149445115419873,5.6205048705610059,4.7679028605352265,5.8866076435834525E-3,3]
[null,"GRN3B4","Short Rural",11,"GRN",0,8.0760000000000005,2.3066740899036859,2.274109574533973,9.0880705873138989,8.6193776387857621,8.4139999999999997,1.5816470538259213,1.5183811716728843,9.0880705873138989,8.6193776387857621,5.8866076435834525E-3,3]
[null,"GRN3B5","Short Rural",11,"GRN",0,14.858000000000001,1.8990290998776036,1.8722195204137451,5.6205048705610059,5.6205048705610059,14.994999999999999,2.2406666595867217,2.1510399932032529,5.6205048705610059,5.6205048705610059,5.8866076435834525E-3,3]
[null,"GRN3B6","Urban",11,"GRN",0,13.131,5.6076042530417194,5.5284387932636241,5.6205048705610059,5.6205048705610059,13.702,3.4833893447356603,3.3440537709462337,5.6205048705610059,5.6205048705610059,5.8866076435834525E-3,1]
[null,"GRN3B7","Urban",11,"GRN",0,8.8789999999999996,4.0167945358667643,3.9600873625505399,9.0880705873138989,8.1602109696992517,9.3209999999999997,3.568120436904906,3.4253956194287096,9.0880705873138989,8.1602109696992517,5.8866076435834525E-3,1]
[null,"GRS3B1","Short Rural",11,"GRS",0,66.173000000000002,0.66321611105531664,0.66314536981789374,6.763658403556466,1.6518568551784383,66.293000000000006,0.53349371757190811,0.53082624898404862,6.763658403556466,1.6518568551784383,-4.8536813517790368E-3,4]
[null,"GRS3B2","Short Rural",11,"GRS",0,122.572,1.7124833912323847,1.7123007310223224,6.763658403556466,1.2622320260158193,120.41,1.4978862070288186,1.4903967759936745,6.763658403556466,1.2622320260158193,-4.8536813517790368E-3,4]
[null,"GRS3B3","Short Rural",11,"GRS",0,67.572999999999993,0.79189983409590048,0.79181536694673871,6.763658403556466,1.5880307829195253,76.551000000000002,0.77972158722048102,0.7758229792843786,6.763658403556466,1.5880307829195253,-4.8536813517790368E-3,4]
[null,"GUE112","Short Rural",11,"GUE",0,130.93600000000001,0.83336434464536413,0.79188653192094827,2.7765294060571373,2.1376971067015083,130.81200000000001,0.40925020090268899,0.38060268683950077,2.7765294060571373,2.7016528496459351,-6.9351393890255908E-11,4]
[null,"GUE122","Short Rural",11,"GUE",0,25.960999999999999,0.43297113492293821,0.41142150208251027,2.7765294060571373,2.7765294060571373,26.202000000000002,0.19439384542877727,0.18078627624876287,2.7765294060571373,2.7765294060571373,-6.9351393890255908E-11,4]
[null,"GUE132","Short Rural",11,"GUE",0,54.793999999999997,0.5611810340991481,0.53325019930111772,2.7765294060571373,2.7730999454581511,54.847999999999999,0.2455501205416134,0.22836161210370048,2.7765294060571373,2.7730999454581511,-6.9351393890255908E-11,4]
[null,"GYA3B1","Long Rural",11,"GYA",0,219.37700000000001,0.5275982486403209,0.50072120792752861,2.7765294060571373,2.7765294060571373,218.767,0.30943337001326998,0.30015036891287189,1.5623098284271273,1.5623098284271273,-1.516902527184246E-3,6]
[null,"GYA3B2","Short Rural",11,"GYA",0,2.3029999999999999,3.3498301500972757E-2,3.1791822725557375E-2,2.7765294060571373,2.7765294060571373,2.3069999999999999,0.48993616918767746,0.4752380841120471,3.6085546524889986,3.6085546524889986,-1.516902527184246E-3,4]
[null,"GYA3B3","Short Rural",11,"GYA",0,191.886,2.7971081753312248,2.6546171975840402,3.583405274763098,3.583405274763098,192.18100000000001,2.8880447867905201,2.8014034431868042,1.6156569933002491,1.6156569933002491,-1.516902527184246E-3,4]
[null,"GYA3B4","Long Rural",11,"GYA",0,317.32600000000002,0.55272197476605045,0.52456507497169669,2.7765294060571373,2.7765294060571373,317.423,0.47274542640916256,0.45856306361688765,1.8090404659653139,1.8090404659653139,-1.516902527184246E-3,6]
[null,"GYA8K1","Long Rural",22,"GYA",0,220.47,0.28473556275826845,0.27023049316723768,4.7882890985403117,4.7882890985403117,218.45699999999999,0.32662411279178499,0.31682538940803145,0.71828146989881347,0.71828146989881347,-1.516902527184246E-3,6]
[null,"HAM3B1","Urban",11,"HAM",0,7.95,2.1284889164855745,1.996212231296165,9.0880705873138989,1.6766251817266733,8.516,2.1209365761788388,1.8551832231836303,9.0880705873138989,8.4288520499531838,-1.520889858288531E-2,2]
[null,"HAM3B2","Urban",11,"HAM",0,2.86,2.8821165711264003,2.7030050787407407,6.9732365512722998,6.9732365512722998,3.7330000000000001,4.2817029472154955,3.7452055679293941,6.9732365512722998,6.9732365512722998,-1.520889858288531E-2,2]
[null,"HAM3B4","Urban",11,"HAM",0,13.968999999999999,4.2264253604857114,3.9637706985067402,7.2399723756379064,7.2399723756379064,11.558999999999999,3.7340432679204909,3.2661676464500533,3.1436722157375119,3.1436722157375119,-1.520889858288531E-2,2]
[null,"HAM3B5","Urban",11,"HAM",0,5.2830000000000004,3.9107164781361754,3.6676818029556335,8.8022822040650333,8.8022822040650333,5.3769999999999998,3.5846815372036711,3.1355209405920514,8.8022822040650333,8.8022822040650333,-1.520889858288531E-2,2]
[null,"HAM3B6","Short Rural",11,"HAM",0,15.734999999999999,0.95731080454375128,0.89781794134851445,9.0880705873138989,9.0880705873138989,16.806999999999999,1.0455321150177375,0.91452694100601495,8.8022822040650333,8.0878112459428717,-1.520889858288531E-2,4]
[null,"HAM3B7","Urban",11,"HAM",0,4.4219999999999997,2.3932770113593786,2.2445448533712868,8.8022822040650333,5.348053278530422,4.3440000000000003,3.7937879602072186,3.3184263287932541,8.8022822040650333,8.8022822040650333,-1.520889858288531E-2,2]
[null,"HAM3B8","Urban",11,"HAM",0,8.6440000000000001,3.1367205085050576,2.9417864461206649,9.0880705873138989,9.0880705873138989,9.7010000000000005,3.0370218579086656,2.6564830191127098,9.0880705873138989,9.0880705873138989,-1.520889858288531E-2,2]
[null,"HAN3B2","Short Rural",11,"HAN",0,1.208,0.11,0.10104966710953867,5.0489281040632772,5.0489281040632772,1.212,0,0,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,3]
[null,"HAN3B3","Urban",11,"HAN",0,1.1539999999999999,3.14,2.8845086793086492,5.0489281040632772,5.0489281040632772,1.1579999999999999,3.4285714285714284,2.8847999999999998,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,1]
[null,"HAN3B4","Short Rural",11,"HAN",0,27.234000000000002,2.1,1.9291300084548291,5.0489281040632772,5.0489281040632772,27.477,2.1904761904761907,1.8430666666666669,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,3]
[null,"HAN3B5","Short Rural",11,"HAN",0,7.7110000000000003,0.36,0.33070800144939927,5.0489281040632772,2.6597372201027678,7.7309999999999999,0.38095238095238093,0.32053333333333334,5.0489281040632772,2.6597372201027678,8.7820631757730572E-3,3]
[null,"HAN3B6","Urban",11,"HAN",0,0.90100000000000002,4.29,3.9409370172720082,5.0489281040632772,5.0489281040632772,0.91100000000000003,3.6190476190476191,3.045066666666667,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,1]
[null,"HAN3B7","Urban",11,"HAN",0,1.526,1.49,1.3687636726655692,5.0489281040632772,5.0489281040632772,1.536,1.8095238095238095,1.5225333333333335,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,1]
[null,"HAN3B8","Short Rural",11,"HAN",0,22.6,2.06,1.8923846749604514,2.0357659166760795,2.0357659166760795,21.47,1.7142857142857142,1.4423999999999999,2.0357659166760795,2.0357659166760795,8.7820631757730572E-3,3]
[null,"HAN3B9","Urban",11,"HAN",0,2.492,1.73,1.5892356736318354,5.0489281040632772,5.0489281040632772,2.492,2.038095238095238,1.7148533333333333,5.0489281040632772,5.0489281040632772,8.7820631757730572E-3,1]
[null,"HAT12","Long Rural",33,"HAT",0,359.57100000000003,0.55000000000000004,0.53554308915917359,10.549020802482097,10.549020802482097,359.69900000000001,5.7142857142857141E-2,5.6708571428571421E-2,3.3105726315548494,3.3105726315548494,9.8126072731200501E-3,5]
[null,"HAT22","Long Rural",33,"HAT",0,482.90300000000002,2.79,2.7166640340983532,10.549020802482097,5.7357728518047155,510.49400000000003,2.2857142857142856,2.2683428571428568,8.3295882181714092,5.5785892410178404,9.8126072731200501E-3,5]
[null,"HAT32","Urban",33,"HAT",0,18.835999999999999,6.68,6.5044142465150534,10.549020802482097,8.7565560627452168,12.336,4.1142857142857139,4.083017142857142,8.3295882181714092,8.3295882181714092,9.8126072731200501E-3,1]
[null,"HAT42","Long Rural",33,"HAT",0,418.97699999999998,5.77,5.6183338626335111,10.549020802482097,10.549020802482097,454.53500000000003,2.8571428571428572,2.8354285714285714,7.182433647810468,7.182433647810468,9.8126072731200501E-3,5]
[null,"HAY1305","Short Rural",11,"HAY",0,18.478999999999999,0.76,0.7529443140384865,2.7765294060571373,2.3634699294681116,18.530999999999999,0.27619047619047621,0.26696571428571431,2.7765294060571373,2.3634699294681116,-8.5921920952062962E-3,4]
[null,"HAY1306","Short Rural",11,"HAY",0,11.734,2.33,2.3083687522495704,2.7765294060571373,2.7765294060571373,12.154999999999999,2.323809523809524,2.246194285714286,2.7765294060571373,2.7765294060571373,-8.5921920952062962E-3,4]
[null,"HAY2036","Short Rural",11,"HAY",0,24.498999999999999,0.35,0.34675067093877665,2.7765294060571373,1.9357399825389774,24.370999999999999,0.43809523809523809,0.42346285714285714,3.1524363928238106,1.9357399825389774,-8.5921920952062962E-3,4]
[null,"HAY355","Short Rural",11,"HAY",0,22.145,2.39,2.3678117244105037,2.7765294060571373,2.5187482843666618,22.645,2.2285714285714286,2.154137142857143,2.7765294060571373,2.5187482843666618,-8.5921920952062962E-3,4]
[null,"HEN3B1","Short Rural",11,"HEN",0,172.62299999999999,0.56492132062966427,0.54243479501968395,2.4440622535442911,2.4440622535442911,172.803,1.850471754619488,1.724639675305363,2.581431203092579,2.581431203092579,-1.1967425302522311E-2,4]
[null,"HEN3B3","Long Rural",11,"HEN",0,442.06099999999998,2.3829408433833108,2.288088589901212,3.5163402674940318,3.5163402674940318,442.51600000000002,0.462617938654872,0.43115991882634075,3.5163402674940318,2.1977126671837701,-1.1967425302522311E-2,6]
[null,"HGE3B1","Short Rural",11,"HGE",0,166.38200000000001,0.34,0.25482729065681775,1.7337828583764461,1.7337828583764461,166.566,0.4,0.36000000000000004,1.7337828583764461,1.7337828583764461,2.2088922878472323E-2,3]
[null,"HGE3B2","Short Rural",11,"HGE",0,1.9159999999999999,0,0,1.6651936463967185,1.6651936463967185,2.0150000000000001,0.19,0.17100000000000001,1.6651936463967185,1.6651936463967185,2.2088922878472323E-2,3]
[null,"HGE3B3","Short Rural",11,"HGE",0,17.782,0.68,0.5096545813136355,1.6651936463967185,1.3241528423864066,18.213999999999999,1.43,1.2869999999999999,1.6651936463967185,1.313673935000615,2.2088922878472323E-2,3]
[null,"HGN3B1","Short Rural",11,"HGN",0,15.468,1.6998062318868983,1.6886396094175866,6.763658403556466,2.8674101119302762,16.375,1.5144853643770979,1.3630368279393881,6.763658403556466,2.8674101119302762,1.7249808806619145E-2,3]
[null,"HGN3B2","Short Rural",11,"HGN",0,6.8730000000000002,0.14086791976963245,0.13994250906775579,6.763658403556466,2.5835269845697373,6.9020000000000001,9.7082395152378057E-2,8.7374155637140252E-2,6.763658403556466,2.5835269845697373,1.7249808806619145E-2,3]
[null,"HGN3B3","Short Rural",11,"HGN",0,7.9020000000000001,2.1505835751497222,2.1364556384344051,6.763658403556466,3.7724066588850147,8.5779999999999994,1.4562359272856711,1.3106123345571039,6.763658403556466,3.7724066588850147,1.7249808806619145E-2,3]
[null,"HIL1108","Short Rural",33,"HIL",0,12.278,1.71,1.7094728923350231,8.1775487982830146,8.1775487982830146,12.249000000000001,1.7142857142857142,1.6503428571428571,8.1775487982830146,8.1775487982830146,9.4957294124694957E-3,3]
[null,"HIL1111","Long Rural",33,"HIL",0,1170.6479999999999,2.86,2.8591184047240734,8.3507365585318283,8.3507365585318283,510.92099999999999,0.45714285714285713,0.44009142857142858,9.4573091784714318,8.1506846902576218,9.4957294124694957E-3,5]
[null,"HIL1114","Short Rural",33,"HIL",0,87.293999999999997,2.46,2.4592417047626647,8.1775487982830146,5.5471525188604653,87.515000000000001,2.2285714285714286,2.1454457142857142,8.1775487982830146,5.4871369583782021,9.4957294124694957E-3,3]
[null,"HIL1117","Long Rural",33,"HIL",0,418.90699999999998,4,3.9987669996140891,8.3295882181714092,6.5216909057390939,400.94299999999998,3.4285714285714284,3.3006857142857142,8.3295882181714092,6.2930601991400019,9.4957294124694957E-3,5]
[null,"HIL1401","Long Rural",33,"HIL",0,273.06900000000002,3.43,3.4289427021690817,8.1775487982830146,8.1621162255875781,271.334,3.6,3.4657200000000001,8.1775487982830146,8.1135322004352695,9.4957294124694957E-3,5]
[null,"HLP3B1","Short Rural",11,"HLP",0,32.261000000000003,2.1317576789644859,2.1301377359488582,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,3]
[null,"HLP3B2","Long Rural",11,"HLP",0,251.78700000000001,3.2414397584254511,3.2389765574016884,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,5]
[null,"HLP3B3","Short Rural",11,"HLP",0,20.417000000000002,0.4867026664302479,0.48633281642667991,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,3]
[null,"HLP3B5","Short Rural",11,"HLP",0,6.2069999999999999,5.8404319971629745E-2,5.8359937971201585E-2,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,3]
[null,"HLP3B7","Short Rural",11,"HLP",0,4.9619999999999997,0.77872426628839664,0.77813250628268782,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,3]
[null,"HOL1843","Long Rural",22,"HOL",0,217.988,1.0017415174231032,0.9872109845730862,4.8881245070885821,2.6521161965494651,218.316,1.0772499042235695,1.0287736585335088,4.8881245070885821,2.6521161965494651,-5.2805580401750502E-3,6]
[null,"HOL1845","Short Rural",22,"HOL",0,97.305999999999997,0.74896562050325477,0.73810167070884947,4.8881245070885821,2.2424861805594256,97.843000000000004,0.53862495211178474,0.51438682926675439,4.8881245070885821,2.2424861805594256,-5.2805580401750502E-3,4]
[null,"HOL1853","Short Rural",22,"HOL",0,7.718,1.4792071004939282,1.4577507996499779,4.8881245070885821,3.9305428976160535,8.5779999999999994,2.154499808447139,2.0575473170670175,4.8881245070885821,3.9305428976160535,-5.2805580401750502E-3,4]
[null,"HOL1890","Long Rural",22,"HOL",0,299.14499999999998,0.88939667434761494,0.87649573396675862,4.8881245070885821,2.1853285039096524,296.52499999999998,1.436333205631426,1.3716982113780118,4.8881245070885821,2.1853285039096524,-5.2805580401750502E-3,6]
[null,"HPT3B1","Short Rural",11,"HPT",0,14.295999999999999,1.9743945056374468,1.9663158945448349,6.763658403556466,2.6635477318794196,14.385,1.4789817501184477,1.4494021151160787,6.763658403556466,2.6635477318794196,1.7147745686360734E-4,3]
[null,"HPT3B2","Short Rural",11,"HPT",0,8.282,2.1002137633496369,2.0916203388050447,6.763658403556466,4.8298236769058143,8.4770000000000003,1.7444400129602204,1.709551212701016,6.763658403556466,4.8298236769058143,1.7147745686360734E-4,3]
[null,"HPT3B3","Short Rural",11,"HPT",0,85.430999999999997,1.4904742836674842,1.4843757243132576,6.763658403556466,4.3068309355603915,85.46,1.4410591411410516,1.4122379583182305,6.763658403556466,4.3068309355603915,1.7147745686360734E-4,3]
[null,"HPT3B4","Short Rural",11,"HPT",0,17.349,3.1358030383653568,3.1229723031006205,6.763658403556466,4.0639108097988572,18.163,3.1286152406351775,3.0660429358224737,6.763658403556466,4.0639108097988572,1.7147745686360734E-4,3]
[null,"HPT3B5","Short Rural",11,"HPT",0,13.911,2.429279514289211,2.419339654562517,6.763658403556466,5.0851279659414681,13.795999999999999,2.2184726251776716,2.1741031726741182,6.763658403556466,5.0851279659414681,1.7147745686360734E-4,3]
[null,"HPT3B6","Short Rural",11,"HPT",0,7.3620000000000001,0.85169959066713385,0.84821469960757578,6.763658403556466,4.6335823204082605,7.5990000000000002,0.79637478852531796,0.78044729275481162,6.1920816370587364,4.6335823204082605,1.7147745686360734E-4,3]
[null,"IVA10215","Short Rural",11,"IVA",0,5.383,0.48067689369212085,0.47073951027035155,1.3917894264219712,0.8211652878684047,5.54,0.43969412088711729,0.42522818430993109,0.8211652878684047,0.8211652878684047,9.9861826325724507E-3,3]
[null,"IVA1144","Long Rural",33,"IVA",0,241.68199999999999,0.29040895660565635,0.28440512078833741,8.3295882181714092,1.8176141174627798,241.75399999999999,0.2748088255544483,0.26576761519370695,8.3295882181714092,1.8176141174627798,9.9861826325724507E-3,5]
[null,"IVA1325","Long Rural",19.100000000000001,"IVA",0,268.63299999999998,0.11015512147111103,0.10787780443695556,2.4166525495145139,1.1065986007017179,268.654,0.1025952948736607,9.9219909672317266E-2,2.4166525495145139,1.1065986007017179,9.9861826325724507E-3,5]
[null,"IVA1326","Long Rural",19.100000000000001,"IVA",0,230.249,0.17023973318262617,0.16672024322074955,2.4166525495145139,2.3703375109201219,230.29300000000001,0.14656470696237245,0.1417427281033104,2.4166525495145139,2.3703375109201219,9.9861826325724507E-3,5]
[null,"IVA1365","Short Rural",19.100000000000001,"IVA",0,91.228999999999999,8.011281561535348E-2,7.8456585045058591E-2,2.4166525495145139,2.0064336362499011,91.242999999999995,4.9465588599800707E-2,4.7838170734867264E-2,2.4166525495145139,2.0064336362499011,9.9861826325724507E-3,3]
[null,"JER8B1","Long Rural",22,"JER",0,354.43299999999999,0.58623354103776282,0.58538811713008765,4.1934682102050092,4.1934682102050092,358.15,2.4282376118401996,2.4282376118401996,6.3048727856476212,4.1934682102050092,1.5131656307212006E-2,5]
[null,"JER8B2","Short Rural",22,"JER",0,127.423,1.4455986182408469,1.443513879741239,3.4770919961945208,3.4770919961945208,128.453,1.734455437028714,1.734455437028714,6.3048727856476212,3.4770919961945208,1.5131656307212006E-2,3]
[null,"JER8B3","Long Rural",22,"JER",0,458.83699999999999,1.3190254673349662,1.317123263542697,4.0886791363470918,4.0886791363470918,459.31900000000002,1.734455437028714,1.734455437028714,4.8881245070885821,4.0886791363470918,1.5131656307212006E-2,5]
[null,"JER8B4","Long Rural",22,"JER",0,282.00900000000001,0.5262778379770825,0.52551887787814688,4.0601002980222054,4.0601002980222054,293.14400000000001,0.58971484858976275,0.58971484858976275,4.8881245070885821,4.0601002980222054,1.5131656307212006E-2,5]
[null,"JGG3B1","Short Rural",11,"JGG",0,107.297,0.27,0.23806917061242372,9.0880705873138989,3.1970193806106342,107.383,0.27,0.23101200000000002,9.0880705873138989,3.1893983570573305,-9.1691456641609707E-14,4]
[null,"JGG3B4","Short Rural",11,"JGG",0,137.381,1.03,0.90818979900294972,9.0880705873138989,3.2055930321080996,137.88200000000001,0.88,0.75292800000000004,9.0880705873138989,3.1989246364989596,-9.1691456641609707E-14,4]
[null,"JIN22","Long Rural",11,"JIN_11",0,335.18200000000002,1.9035280951794822,1.9024931934370786,4.3820885431492593,1.9586030531988867,334.017,1.682362081682758,1.6355924158119772,4.3820885431492593,1.9586030531988867,5.0331228389908958E-4,5]
[null,"JIN2442","Short Rural",33,"JIN_33",0,45.564,5.4983594238770754,5.4983594238770754,13.146265629447779,12.949071645006063,43.795999999999999,3.1576993903842143,3.1576993903842143,12.949071645006063,12.949071645006063,8.2624050007568256E-3,3]
[null,"JIN32","Urban",11,"JIN_11",0,7.8070000000000004,3.6998151709122329,3.6978036717509415,4.3820885431492593,3.2132140556614028,8.0790000000000006,3.5830864514241818,3.4834766480745896,4.3820885431492593,3.2132140556614028,5.0331228389908958E-4,1]
[null,"JIN62","Urban",11,"JIN_11",0,5.4169999999999998,2.26099816000192,2.259768910514464,4.3820885431492593,3.7171542381235683,5.0129999999999999,2.6910720844152998,2.6162602804685542,4.3820885431492593,3.7171542381235683,5.0331228389908958E-4,1]
[null,"JIN72","Urban",11,"JIN_11",0,5.0389999999999997,2.5648477151009925,2.5634532700302421,4.3820885431492593,4.3658938680984898,5.4260000000000002,3.7377965745426698,3.6338858297703833,4.3820885431492593,4.3658938680984898,5.0331228389908958E-4,1]
[null,"JIN82","Short Rural",11,"JIN_11",0,160.06200000000001,1.7337298143888242,1.7327872278253205,4.3820885431492593,3.3494398516766952,160.23500000000001,2.6946083158008651,2.6196982046216011,4.3820885431492593,3.3494398516766952,5.0331228389908958E-4,3]
[null,"JNR4081","Short Rural",11,"JNR",0,71.882000000000005,1.3378741826817908,1.2798956859346931,1.8738191661683901,1.709967159772374,71.447000000000003,0.95262794416288255,0.85736514974659428,1.8738191661683901,1.709967159772374,1.3241566957842782E-2,3]
[null,"JRF 131/132","Short Rural",11,"JRF",0,108.375,0.18356503457769308,0.16549486279723738,0.44868776170071767,0.44868776170071767,108.375,0.16181768438951538,0.13900139089059371,4.3820885431492593,0.44868776170071767,1.0754924388912304E-9,3]
[null,"JUN3B1","Short Rural",11,"JUN_11",0,9.9619999999999997,2.4888944540197855,2.4077515069957687,9.0880705873138989,9.0880705873138989,10.574,1.6,1.50976,3.1524363928238106,3.1524363928238106,1.8720618955433881E-3,3]
[null,"JUN3B2","Long Rural",11,"JUN_11",0,209.59899999999999,0.80611966122098311,0.77983854477595738,9.0880705873138989,9.0880705873138989,209.15199999999999,0.8,0.75488,3.1524363928238106,3.1524363928238106,1.8720618955433881E-3,5]
[null,"JUN3B6","Long Rural",11,"JUN_11",0,275.61799999999999,0.89680812310834357,0.86757038106325246,9.0880705873138989,9.0880705873138989,276.81900000000002,0.9,0.84923999999999999,3.1524363928238106,3.1524363928238106,1.8720618955433881E-3,5]
[null,"JUN3B7","Short Rural",11,"JUN_11",0,20.045000000000002,3.2547081321797191,3.1485981245329278,9.0880705873138989,9.0880705873138989,19.835999999999999,1.7,1.60412,3.1524363928238106,3.1524363928238106,1.8720618955433881E-3,3]
[null,"JYE3B2","Short Rural",11,"JYE",0,132.56899999999999,2.383689676260826,2.3485199669456747,9.011860351780868,0.5782451621068696,131.75800000000001,2.2680492940284527,2.2254099673007177,9.011860351780868,0.5782451621068696,1.7788741830794898E-2,3]
[null,"JYE3B3","Short Rural",11,"JYE",0,27.373999999999999,2.2600909523065607,2.2267448575484914,9.011860351780868,0.65826590941655194,27.68,1.390235048660325,1.3640986297455109,9.011860351780868,0.65826590941655194,1.7788741830794898E-2,3]
[null,"KEW3B1","Short Rural",11,"KEW",0,43.591000000000001,1.8205860169276635,1.6985714320547796,4.5726141319818359,3.0131621873871972,43.58,2.5614093645613099,2.3821107090420184,4.5726141319818359,3.0131621873871972,1.5452558305398079E-9,3]
[null,"KEW3B2","Short Rural",11,"KEW",0,79.561000000000007,0.9582031668040335,0.89398496423935769,4.5726141319818359,2.5806691007372491,78.912000000000006,0.69523968466664121,0.64657290673997636,4.5726141319818359,2.5806691007372491,1.5452558305398079E-9,3]
[null,"KEW3B3","Short Rural",11,"KEW",0,54.106999999999999,1.0540234834844369,0.98338346066329341,8.9547026751310952,3.153198495179141,40.207000000000001,0.91478905877189653,0.85075382465786387,4.5726141319818359,3.1484353554583269,1.5452558305398079E-9,3]
[null,"KIN12I2","Short Rural",22,"KIN",0,20.204999999999998,0.90500000000000003,0.85975000000000001,0.84555256323897443,0.84555256323897443,20.204999999999998,0.1,9.5000000000000001E-2,0.84555256323897443,0.84555256323897443,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"KIS7681","Short Rural",11,"KIS",0,85.236000000000004,1.0314054416663134,0.99949301163408977,2.7765294060571373,2.7765294060571373,83.683000000000007,0.79112955040275024,0.75157307288261266,2.7765294060571373,2.7765294060571373,7.4545317727334672E-7,3]
[null,"KIS7682","Short Rural",11,"KIS",0,163.249,1.0314054416663134,0.99949301163408977,6.763658403556466,2.6159163346712759,163.16800000000001,0.86576441364829271,0.82247619296587804,6.763658403556466,2.6159163346712759,7.4545317727334672E-7,3]
[null,"KIS7683","Urban",11,"KIS",0,0.12,0,0,6.763658403556466,5.3423375108654456,0.13900000000000001,0,0,6.763658403556466,5.3423375108654456,7.4545317727334672E-7,1]
[null,"KKN3B1","Short Rural",11,"KKN",0,148.55799999999999,1.64,1.6236488785106973,9.0880705873138989,3.1017565861943459,148.17699999999999,1.96,1.8619999999999999,9.0880705873138989,3.0941355626410423,4.5438326394111952E-9,3]
[null,"KKN3B2","Short Rural",11,"KKN",0,5.867,1.1200000000000001,1.10883338044633,9.0880705873138989,4.7097925559412914,5.593,0.67,0.63649999999999995,9.0880705873138989,4.6993136485555,4.5438326394111952E-9,3]
[null,"KOO3B1","Short Rural",11,"KOO",0,74.570999999999998,4.4910663146355549,4.485393216601631,7.8096438862473114,7.8096438862473114,74.858999999999995,2.6378207861643377,2.4734845511862993,7.8096438862473114,7.8096438862473114,-9.9663576578988425E-4,4]
[null,"KOO3B2","Urban",11,"KOO",0,8.0060000000000002,3.1811719728668515,3.1771535284261554,8.9547026751310952,8.9547026751310952,8.9269999999999996,2.6378207861643377,2.4734845511862993,9.8825622927457442,9.8825622927457442,-9.9663576578988425E-4,2]
[null,"KOO3B3","Short Rural",11,"KOO",0,44.042000000000002,2.9212723018809976,2.9175821617246722,6.3683178067288688,6.3683178067288688,43.673999999999999,1.1304946226418591,1.0600648076512713,6.3683178067288688,6.3683178067288688,-9.9663576578988425E-4,4]
[null,"KOO3B4","Urban",11,"KOO",0,7.9969999999999999,2.5886007230191046,2.5853308123467733,7.9611117293692093,7.9611117293692093,8.6790000000000003,0.9420788522015493,0.88338733970939276,7.9611117293692093,7.9611117293692093,-9.9663576578988425E-4,2]
[null,"KOO3B6","Short Rural",11,"KOO",0,101.831,2.9108763150415631,2.9071993070566124,7.9706380088108384,7.9706380088108384,102.95699999999999,2.1667813600635633,2.0317908813316032,7.9706380088108384,7.9706380088108384,-9.9663576578988425E-4,4]
[null,"KOO3B7","Urban",11,"KOO",0,11.930999999999999,4.3143345383651743,4.3088846872446229,6.3978492729979193,6.3978492729979193,12.935,1.1304946226418591,1.0600648076512713,6.3978492729979193,6.3978492729979193,-9.9663576578988425E-4,2]
[null,"KOR22","Short Rural",22,"KOR",0,68.447000000000003,0.16191832256157285,0.15791944971602287,5.7172918696879558,1.7261618348231431,68.36,1.338941797532508,1.2655677870277267,1.7109197877165372,1.7109197877165372,2.2299277129837979E-3,3]
[null,"KOR23","Short Rural",22,"KOR",0,184.678,1.8287245842248225,1.7835608438515522,2.2070484210365664,1.6213727609652262,182.00899999999999,1.6298263625336282,1.5405118778667855,1.5127731753306575,1.5127731753306575,2.2299277129837979E-3,3]
[null,"KOR24","Long Rural",22,"KOR",0,231.16900000000001,2.6954638402897126,2.6288943688020279,5.4516991988553434,1.5908886667520137,206.376,2.5245527509917136,2.3862072602373678,1.4518049869042329,1.4518049869042329,2.2299277129837979E-3,5]
[null,"KPT28","Short Rural",11,"KPT",0,9.0619999999999994,0.25,0.23080355739471126,0.42277628161948722,0.42277628161948722,9.0969999999999995,0.38,0.35947999999999997,0.42277628161948722,0.42277628161948722,-1.4967939107362509E-11,4]
[null,"KTE3B3","Short Rural",11,"KTE",0,23.036000000000001,1.4994897117111041,1.4911101973518233,9.0880705873138989,9.0880705873138989,23.224,1.1980720966890237,1.1381684918545725,9.0880705873138989,9.0880705873138989,1.5356204462535857E-2,3]
[null,"KTE3B4","Short Rural",11,"KTE",0,33.435000000000002,2.0716634174956043,2.0600864568676505,9.0499654695473861,6.4397649025410857,32.826000000000001,1.4872619131312017,1.4128988174746415,9.0499654695473861,6.4397649025410857,1.5356204462535857E-2,3]
[null,"KTE3B5","Urban",11,"KTE",0,6.9240000000000004,2.6241069954944325,2.6094428453656908,9.0880705873138989,8.1716425050292063,7.2750000000000004,2.4787698552186694,2.3548313624577357,9.0880705873138989,8.1011480371611526,1.5356204462535857E-2,1]
[null,"KTE3B6","Short Rural",11,"KTE",0,36.872999999999998,4.3208979850622606,4.2967517528953856,9.0880705873138989,6.4483385540385525,36.969000000000001,3.3050264736248929,3.1397751499436479,9.0880705873138989,6.4483385540385525,1.5356204462535857E-2,3]
[null,"KTE3B7","Short Rural",11,"KTE",0,2.9580000000000002,1.0752919643191472,1.0692829704693996,9.0880705873138989,9.0880705873138989,3.0630000000000002,0.86756944932653457,0.82419097686020781,9.0880705873138989,9.0880705873138989,1.5356204462535857E-2,3]
[null,"KTE3B8","Urban",11,"KTE",0,7.9029999999999996,3.1962807012789325,3.1784191048815176,9.0499654695473861,5.6490837088858923,8.4359999999999999,2.375487777917892,2.2567133890219973,9.0499654695473861,5.6490837088858923,1.5356204462535857E-2,1]
[null,"KTL3B1","Short Rural",11,"KTL",0,136.04,1.658812111299911,1.5922591044809948,2.7765294060571373,2.7765294060571373,136.43100000000001,1.546287081735922,1.4535098568317666,2.7765294060571373,2.7765294060571373,4.9572618281095667E-12,3]
[null,"KTL3B2","Short Rural",11,"KTL",0,70.338999999999999,2.3466122550096302,2.2524640990218954,1.7337828583764461,1.7337828583764461,70.093000000000004,1.9043746164537143,1.7901121394664914,1.7337828583764461,1.7337828583764461,4.9572618281095667E-12,3]
[null,"KTL3B3","Short Rural",11,"KTL",0,39.514000000000003,0.98112667558592292,0.94176300691863712,1.7337828583764461,1.7337828583764461,40.023000000000003,0.79755860005326507,0.74970508405006908,1.7337828583764461,1.7337828583764461,4.9572618281095667E-12,3]
[null,"KTL3B4","Short Rural",11,"KTL",0,86.227000000000004,1.9217945191889212,1.8446904259231036,3.5163402674940318,1.9595556811430495,0,"","","","",4.9572618281095667E-12,3]
[null,"KYG3B1","Long Rural",11,"KYG",0,219.41200000000001,2.2614491401289629,2.1527257638544484,3.5163402674940318,3.5163402674940318,219.44300000000001,1.4572208348736242,1.3552153764324706,3.5163402674940318,3.5163402674940318,5.5053395170581105E-3,5]
[null,"KYG3B2","Urban",11,"KYG",0,4.569,2.2614491401289629,2.1527257638544484,2.7765294060571373,2.7765294060571373,4.8840000000000003,1.8682318395815694,1.7374556108108596,2.7765294060571373,2.7765294060571373,5.5053395170581105E-3,1]
[null,"KYG3B3","Short Rural",11,"KYG",0,9.6579999999999995,1.3076843018334381,1.2448149452453856,2.0357659166760795,2.0357659166760795,9.7919999999999998,0.86872780540542982,0.80791685902704979,2.0357659166760795,2.0357659166760795,5.5053395170581105E-3,3]
[null,"KYG3B4","Short Rural",11,"KYG",0,190.684,1.2830917107114681,1.2214046887117436,2.0357659166760795,1.9586030531988867,189.821,1.1769860589363887,1.0945970348108416,2.0357659166760795,1.9586030531988867,5.5053395170581105E-3,3]
[null,"KYG3B5","Long Rural",11,"KYG",0,206.874,2.0251464167396005,1.9277837336833687,1.8738191661683901,1.8738191661683901,206.93199999999999,1.4759031532694398,1.372589932540579,1.8738191661683901,1.8738191661683901,5.5053395170581105E-3,5]
[null,"KYG3B6","Short Rural",11,"KYG",0,82.307000000000002,0.70463119779904793,0.6707547415508659,2.7258495994276717,2.4977904695950777,82.385999999999996,0.49508143748911593,0.46042573686487781,2.7258495994276717,2.4977904695950777,5.5053395170581105E-3,3]
[null,"KYW2198","Short Rural",11,"KYW",0,39.173999999999999,0.27,0.25478653797708872,1.4136998691377176,1.4136998691377176,42.037999999999997,0.4,0.34740000000000004,2.0357659166760795,1.4136998691377176,1.9755274035350114E-6,3]
[null,"KYW2199","Short Rural",11,"KYW",0,105.45,0.19,0.17929423042832171,0.85736514974659417,0.85736514974659417,103.13500000000001,0.2,0.17370000000000002,2.0357659166760795,1.517536315051472,1.9755274035350114E-6,3]
[null,"LCO22","Long Rural",22,"LCO",0,776.41600000000005,3.9007946941416405,3.8797901563844253,3.8931998822048688,1.7394986260414236,794.73099999999999,2.2771871924004774,2.2771871924004774,3.8931998822048688,1.7394986260414236,6.7011420746839381E-3,5]
[null,"LCO32","Short Rural",22,"LCO",0,196.01400000000001,1.9011448888114559,1.890907828742914,3.8931998822048688,1.7814142555845902,196.11799999999999,0.5075425691536658,0.5075425691536658,3.8931998822048688,1.7814142555845902,6.7011420746839381E-3,3]
[null,"LEE3B1","Short Rural",11,"LEE",0,61.969000000000001,0.94167430852541889,0.86685597629862055,9.0499654695473861,9.0499654695473861,64.603999999999985,3.2121548533968496,2.829587210357285,6.763658403556466,5.5376262394188371,2.4493450431886951E-3,3]
[null,"LEE3B2","Short Rural",11,"LEE",0,8.3970000000000002,2.1906318124643955,2.0165807448631066,9.0499654695473861,9.0499654695473861,9.4719999999999995,2.6281266982337863,2.3151168084741425,7.0713572295210767,7.0713572295210767,2.4493450431886951E-3,3]
[null,"LEE3B3","Urban",11,"LEE",0,4.8899999999999997,3.1521308432745605,2.9016863206627512,9.0499654695473861,9.0499654695473861,5.367,3.4068309051178711,3.0010773443183325,7.5514817133791698,7.5514817133791698,2.4493450431886951E-3,1]
[null,"LEE3B4","Short Rural",11,"LEE",0,3.1619999999999999,0.94167430852541889,0.86685597629862055,9.0499654695473861,9.0499654695473861,3.3769999999999998,2.7254647240942966,2.400861875454666,6.8655895935818947,6.8655895935818947,2.4493450431886951E-3,3]
[null,"LEE3B6","Urban",11,"LEE",0,3.726,4.9660929323287881,4.5715246750064091,9.0499654695473861,9.0499654695473861,4.76,4.9642393188860403,4.3729984160067126,7.0704046015769144,7.0704046015769144,2.4493450431886951E-3,1]
[null,"LEE3B7","Short Rural",11,"LEE",0,57.966999999999999,3.4891511221152363,3.2119295121801517,9.0499654695473861,9.0499654695473861,58.436999999999998,3.2121548533968496,2.829587210357285,5.0698859188348617,5.0698859188348617,2.4493450431886951E-3,3]
[null,"LEE3B8","Urban",11,"LEE",0,10.002000000000001,3.7567848729593027,3.4582991054439702,9.0499654695473861,9.0499654695473861,10.01,3.7961830085599133,3.3440576122404275,1.6651936463967185,1.6651936463967185,2.4493450431886951E-3,1]
[null,"LGR8B1","Short Rural",22,"LGR",0,11.41,1.3491470525223797,1.2846511261964126,4.8881245070885821,2.0691078947217809,11.778,1.1227220940922182,1.0778132103285294,4.8881245070885821,2.0691078947217809,-2.7531462329814255E-3,4]
[null,"LGR8B2","Long Rural",22,"LGR",0,391.149,0.96655311225483909,0.92034707548399697,4.8881245070885821,1.5337309901022409,391.40499999999997,0.7484813960614789,0.71854214021901974,4.8881245070885821,1.5337309901022409,-2.7531462329814255E-3,6]
[null,"LGR8B3","Short Rural",22,"LGR",0,15.938000000000001,1.2585326982484886,1.1983685878697878,4.8881245070885821,1.7947510468028707,16.436,1.0104498846829966,0.97003188929567663,4.8881245070885821,1.8252351410160832,-2.7531462329814255E-3,4]
[null,"LHD3B3","Short Rural",11,"LHD",0,10.1,0.39047874502450469,0.39019504736123495,6.1920816370587364,5.3204270681496979,10.263999999999999,0.34038346755978199,0.33357579820858635,6.1920816370587364,5.3204270681496979,1.1046619425980153E-2,3]
[null,"LHD3B4","Short Rural",11,"LHD",0,67.784999999999997,1.3178657644577034,1.316908284844168,6.1920816370587364,5.09274898949477,67.409000000000006,1.128639918750856,1.1060671203758388,6.1920816370587364,5.09274898949477,1.1046619425980153E-2,3]
[null,"LHD3B5","Short Rural",11,"LHD",0,11.335000000000001,1.0933404860686131,1.0925461326114578,6.1920816370587364,6.1920816370587364,11.587,1.0748951607151009,1.0533972575007988,6.1920816370587364,6.1920816370587364,1.1046619425980153E-2,3]
[null,"LHD3B6","Short Rural",11,"LHD",0,12.768000000000001,2.3233485328958028,2.3216605317993477,6.1920816370587364,3.4999550668544308,13.374000000000001,2.3110245955374671,2.2648041036267177,6.1920816370587364,3.4999550668544308,1.1046619425980153E-2,3]
[null,"LHD3B7","Short Rural",11,"LHD",0,31.257000000000001,0.70286174104410837,0.70235108525022283,6.1920816370587364,5.2423115767283432,31.315999999999999,0.64493709642906061,0.6320383545004794,6.1920816370587364,5.2156379942917814,1.1046619425980153E-2,3]
[null,"LHD3B8","Short Rural",11,"LHD",0,8.27,0.16595346663541449,0.16583289512852484,6.1920816370587364,5.9120090214748489,7.7370000000000001,1.7914919345251683E-2,1.7556620958346651E-2,6.1920816370587364,6.1920816370587364,1.1046619425980153E-2,3]
[null,"LIU3B3","Short Rural",11,"LIU",0,6.9260000000000002,2.1916524373876958,2.1371168528012867,7.2399723756379064,7.2399723756379064,7.2169999999999996,1.6508837362397695,1.568339549427781,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,3]
[null,"LIU3B4","Urban",11,"LIU",0,5.65,6.3770350353115264,6.2183532445102214,7.2399723756379064,7.2399723756379064,5.2480000000000002,3.6856939227678573,3.5014092266294643,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,1]
[null,"LIU3B5","Short Rural",11,"LIU",0,14.676,3.5532748027434553,3.4648575358182563,7.2399723756379064,6.3749862023380102,14.994999999999999,2.9946263122488843,2.8448949966364401,7.2399723756379064,6.3749862023380102,3.018703319138021E-12,3]
[null,"LIU3B6","Short Rural",11,"LIU",0,9.17,2.2900954546698853,2.2331102811777037,7.2399723756379064,7.2399723756379064,9.298,1.8812396064127606,1.7871776260921224,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,3]
[null,"LIU3B7","Urban",11,"LIU",0,4.7149999999999999,2.7439695764551386,2.6756905088500269,7.2399723756379064,7.2399723756379064,4.8520000000000003,2.6682888295038132,2.5348743880286224,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,1]
[null,"LIU3B8","Urban",11,"LIU",0,7.0019999999999998,2.3097840581263234,2.2523089668529872,7.2399723756379064,7.2399723756379064,7.2220000000000004,4.2807799207147514,4.0667409246790136,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,1]
[null,"LIU3B9","Short Rural",11,"LIU",0,9.0399999999999991,1.0859819169656288,1.0589590835630016,7.2399723756379064,7.2399723756379064,9.1069999999999993,0.86383451314871662,0.82064278749128072,7.2399723756379064,7.2399723756379064,3.018703319138021E-12,3]
[null,"LKC7781","Short Rural",11,"LKC",0,9.48,2.1591060456876461,2.1359578686019574,6.1920816370587364,4.0477161347480877,10.117000000000001,1.9720625150356388,1.9129006395845696,6.1920816370587364,4.0477161347480877,1.3606130350422567E-2,3]
[null,"LKC7782","Short Rural",11,"LKC",0,4.8179999999999996,0.46937087949731443,0.46433866708738208,6.1920816370587364,3.4990024389102672,4.6289999999999996,0.41319405076937199,0.40079822924629083,6.1920816370587364,3.4990024389102672,1.3606130350422567E-2,3]
[null,"LKC7784","Short Rural",11,"LKC",0,22.425000000000001,3.1917219805817378,3.1575029361941978,6.1920816370587364,3.7123910984027533,22.902999999999999,2.5355089479029642,2.4594436794658754,6.1920816370587364,3.7123910984027533,1.3606130350422567E-2,3]
[null,"LOC3781","Short Rural",22,"LOC",0,127.837,0.18247389922322932,0.18239588792678058,5.4516991988553434,2.2386756687827738,128.01599999999999,0.18971696451318842,0.18774390808225128,5.4516991988553434,2.2386756687827738,-1.571544268419194E-7,4]
[null,"LOC3786","Long Rural",22,"LOC",0,630.66300000000001,1.6422650930090641,1.6415629913410255,4.8881245070885821,2.2805912983259411,704.35199999999998,0.66400937579615948,0.65710367828787941,4.8881245070885821,2.2805912983259411,-1.571544268419194E-7,6]
[null,"LOC3794","Long Rural",22,"LOC",0,306.95400000000001,2.1288621576043423,2.1279520258124403,4.8881245070885821,2.320601671980782,307.31900000000002,0.7588678580527537,0.7509756323290051,4.8881245070885821,2.320601671980782,-1.571544268419194E-7,6]
[null,"LRN3B1","Short Rural",11,"LRN",0,6.7119999999999997,0.65252797943638152,0.64380295434693613,3.2389350101538001,3.2389350101538001,6.7910000000000004,0.48150275026964856,0.46224264025886258,3.2389350101538001,3.2389350101538001,-1.1575441029890464E-2,4]
[null,"LRN3B3","Urban",11,"LRN",0,2.9489999999999998,1.305055958872763,1.2876059086938723,3.2389350101538001,3.2389350101538001,3.1509999999999998,0.83460476713405773,0.80122057644869538,3.2389350101538001,3.2389350101538001,-1.1575441029890464E-2,2]
[null,"LRN3B4","Short Rural",11,"LRN",0,4.8109999999999999,1.3982742416493892,1.3795777593148635,3.2389350101538001,3.2389350101538001,5.2480000000000002,1.2037568756741217,1.1556066006471568,3.2389350101538001,3.2389350101538001,-1.1575441029890464E-2,4]
[null,"LRN3B5","Short Rural",11,"LRN",0,23.081,4.1948227249481675,4.1387332779445902,9.0880705873138989,4.0343793435298068,23.128,2.4877642097265182,2.3882536413374575,3.2389350101538001,3.2389350101538001,-1.1575441029890464E-2,4]
[null,"LRN3B6","Short Rural",11,"LRN",0,23.648,2.0508022210857706,2.0233807136617994,7.2399723756379064,4.4459146154081726,24.09,1.5247587091872206,1.4637683608197316,7.2399723756379064,4.4459146154081726,-1.1575441029890464E-2,4]
[null,"MAH3B1","Short Rural",11,"MAH",0,112.944,3.5,3.4874919201354722,9.0499654695473861,5.0374965687333235,110.62,2.762,2.6073279999999999,9.0499654695473861,5.0374965687333235,3.0047419018678196E-3,3]
[null,"MAH3B2","Urban",11,"MAH",0,5.9660000000000002,3.6,3.5871345464250575,7.9258644954351825,7.6095920179731058,6.2539999999999996,4.1909999999999998,3.9563039999999998,7.9258644954351825,7.6095920179731058,3.0047419018678196E-3,1]
[null,"MAH3B3","Short Rural",11,"MAH",0,42.945999999999998,3.5,3.4874919201354722,7.9258644954351825,6.0549032130992808,42.302,3.2189999999999999,3.0387359999999997,7.9258644954351825,6.0549032130992808,3.0047419018678196E-3,3]
[null,"MAH3B4","Short Rural",11,"MAH",0,182.875,3.1,3.0889214149771327,7.9258644954351825,5.8138883432260728,182.65,3.048,2.8773119999999999,7.9258644954351825,5.9463036274647125,3.0047419018678196E-3,3]
[null,"MAH3B5","Urban",11,"MAH",0,3.4630000000000001,2.5,2.491065657239623,7.9258644954351825,7.9258644954351825,3.6589999999999998,2.4950000000000001,2.35528,7.9258644954351825,7.9258644954351825,3.0047419018678196E-3,1]
[null,"MAH3B6","Short Rural",11,"MAH",0,42.218000000000004,1.7,1.6939246469229436,7.9258644954351825,6.271149756424256,42.302999999999997,1.657,1.564208,7.9258644954351825,6.271149756424256,3.0047419018678196E-3,3]
[null,"MAH3B7","Short Rural",11,"MAH",0,165.489,2.2000000000000002,2.1921377783708684,6.9732365512722998,6.073955771982539,165.244,1.829,1.7265759999999999,6.9732365512722998,6.073955771982539,3.0047419018678196E-3,3]
[null,"MBL112","Short Rural",11,"MBL",0,37.616,0.53270378089069703,0.50606859184616215,1.2328910853356025,1.2328910853356025,37.752000000000002,0.32387056627115413,0.29834956564898718,1.2328910853356025,1.2328910853356025,-2.8663841837645986E-2,4]
[null,"MBL122","Long Rural",11,"MBL",0,231.90100000000001,0.74407722501165496,0.70687336376107224,2.7765294060571373,1.3994104499752744,232.14,0.32387056627115413,0.29834956564898718,2.7765294060571373,1.3994104499752744,-2.8663841837645986E-2,6]
[null,"MBL142","Short Rural",11,"MBL",0,32.942999999999998,0.20390064559142912,0.19370561331185765,2.2965954477878769,1.4041735896960887,46.594000000000001,0.31434496138082607,0.28957457842401696,2.2965954477878769,1.4527576148483956,-2.8663841837645986E-2,4]
[null,"MBM6212","Long Rural",22,"MBM",0,254.01,2.280340446511937,2.280339687335279,5.4516991988553434,3.2827558955852933,245.39400000000001,2.3561951282763323,2.3557238892506769,5.4516991988553434,3.2827558955852933,1.4228516945916717E-2,5]
[null,"MBM6222","Long Rural",22,"MBM",0,297.17200000000003,3.8675377617052673,3.8675364741149001,5.4516991988553434,2.8807469031485571,284.12299999999999,3.9034750299869176,3.9026943349809202,5.4516991988553434,3.1951141247223083,1.4228516945916717E-2,5]
[null,"MCR3B1","Short Rural",11,"MCR",0,78.606999999999999,2.86,2.8265669834455189,6.763658403556466,1.9519346575897463,78.212999999999994,2.324412183757433,2.2546798182447101,6.763658403556466,1.9519346575897463,1.0337352472287899E-2,3]
[null,"MCR3B3","Short Rural",11,"MCR",0,40.526000000000003,0.8,0.7906481072574878,6.763658403556466,2.2615387394426829,40.6,0.57157676649772937,0.55442946350279743,6.763658403556466,2.221528365787842,1.0337352472287899E-2,3]
[null,"MCR3B4","Short Rural",11,"MCR",0,38.094000000000001,1.22,1.2057383635676688,6.763658403556466,2.0100449621836818,27.809000000000001,0.80020747309682139,0.77620124890391673,6.763658403556466,2.0100449621836818,1.0337352472287899E-2,3]
[null,"MCV3B10","Short Rural",11,"MCV",0,105.523,1.271674465192359,1.262858391529581,9.0880705873138989,3.5247233934026649,104.84099999999999,0.82177897100685793,0.80534339158672075,9.0880705873138989,3.5247233934026649,-1.1313172947442639E-9,4]
[null,"MCV3B2","Short Rural",11,"MCV",0,169.172,0.72667112296706227,0.72163336658833188,9.0880705873138989,2.6759318951535374,168.745,0.46691986989026019,0.45758147249245495,9.0880705873138989,2.6759318951535374,-1.1313172947442639E-9,4]
[null,"MCV3B3","Short Rural",11,"MCV",0,5.4569999999999999,0.78403989583288292,0.77860442184530543,9.0880705873138989,6.3578388993430792,4.5609999999999999,0.63501102305075374,0.6223108025897387,9.0880705873138989,6.3578388993430792,-1.1313172947442639E-9,4]
[null,"MCV3B4","Short Rural",11,"MCV",0,51.246000000000002,1.6732558752531039,1.6616557783283958,7.2399723756379064,3.6523755379204919,49.643999999999998,1.6062043524224949,1.5740802653740451,7.2399723756379064,3.64856502614384,-1.1313172947442639E-9,4]
[null,"MCV3B5","Short Rural",11,"MCV",0,47.802,1.4915880945113384,1.4812474366813131,9.0880705873138989,4.0172320405348758,36.94,1.2886988408971178,1.2629248640791755,9.0880705873138989,4.0172320405348758,-1.1313172947442639E-9,4]
[null,"MCV3B6","Short Rural",11,"MCV",0,7.3680000000000003,0.84140866869870368,0.83557547710227908,9.0880705873138989,4.4802092213980371,7.6,1.0832540981454035,1.0615890161824955,9.0880705873138989,4.4802092213980371,-1.1313172947442639E-9,4]
[null,"MCV3B7","Urban",11,"MCV",0,6.2069999999999999,2.1322060581796696,2.1174242203841844,9.0880705873138989,5.3623426976928652,6.633,2.0731242223127548,2.0316617378664996,9.0880705873138989,5.3623426976928652,-1.1313172947442639E-9,2]
[null,"MCV3B8","Short Rural",11,"MCV",0,33.218000000000004,1.8931695045720833,1.8800448234801279,7.2399723756379064,4.0562897862455536,33.847999999999999,1.8303258899698196,1.7937193721704232,7.2399723756379064,4.0562897862455536,-1.1313172947442639E-9,4]
[null,"MCV3B9","Long Rural",11,"MCV",0,228.21899999999999,1.309920313769573,1.3008390950342301,7.2399723756379064,2.5016009813717295,227.01400000000001,0.97119332937174108,0.95176946278430619,7.2399723756379064,2.5016009813717295,-1.1313172947442639E-9,6]
[null,"MDA12","Urban",11,"MDA",0,2.258,7.18,6.8979138258200194,12.231742803051411,6.6369588869828027,2.2599999999999998,7.14,6.9393659999999997,12.231742803051411,6.6369588869828027,7.3743641965842493E-3,1]
[null,"MDA22","Short Rural",11,"MDA",0,93.100999999999999,0.93,0.89346237576777421,12.231742803051411,4.000084737539944,93.200999999999993,0.88,0.85527200000000003,12.231742803051411,4.5573720848752304,7.3743641965842493E-3,3]
[null,"MDA42","Short Rural",11,"MDA",0,137.87100000000001,2.42,2.3249236014602292,12.231742803051411,3.9457849447226598,138.12799999999999,2.29,2.225651,12.231742803051411,3.9457849447226598,7.3743641965842493E-3,3]
[null,"MDA52","Short Rural",11,"MDA",0,161.05500000000001,1.49,1.4314612256924553,12.231742803051411,4.878407702058122,161.26,1.3,1.2634700000000001,12.231742803051411,4.878407702058122,7.3743641965842493E-3,3]
[null,"MDI3B1","Long Rural",11,"MDI",0,229.54900000000001,0.81100396691300192,0.80669202458866285,6.1920816370587364,1.2612793980716566,231.42,0.81400767403095142,0.80586759729064195,6.1920816370587364,1.2612793980716566,2.6735018762460154E-3,5]
[null,"MDI3B3","Short Rural",11,"MDI",0,24.233000000000001,1.0656214914089444,1.0599557997502198,6.1920816370587364,1.4298945441884865,24.718,1.1547550724625124,1.1432075217378872,6.1920816370587364,1.4298945441884865,2.6735018762460154E-3,3]
[null,"MDI3B4","Short Rural",11,"MDI",0,187.411,0.80157368822796704,0.79731188476786452,6.1920816370587364,1.3717842395945505,187.346,0.73828602993504899,0.73090316963569846,6.1920816370587364,1.3717842395945505,2.6735018762460154E-3,3]
[null,"MEN8B1","Short Rural",22,"MEN",0,107.13500000000001,0.19,0.17680071185703566,10.821853445690346,1.6366148080718321,98.631,0.75,0.69000000000000006,10.821853445690346,1.6366148080718321,0,3]
[null,"MGA3B1","Short Rural",11,"MGA",0,134.47499999999999,0.84888326901809852,0.83239722861127974,1.1250536020563644,1.1250536020563644,134.51499999999999,0.7016149434530945,0.66653419628043975,1.1250536020563644,1.1250536020563644,7.1815727021506406E-4,3]
[null,"MGA3B2","Long Rural",11,"MGA",0,314.149,1.0455757337905849,1.0252697571919422,1.2328910853356025,1.2328910853356025,307.60899999999998,0.46158877858756225,0.43850933965818412,1.2328910853356025,1.2328910853356025,7.1815727021506406E-4,5]
[null,"MGE3B1","Short Rural",11,"MGE",0,106.648,0.37458824987240191,0.37038905774318681,6.763658403556466,1.2050743493660463,106.97499999999999,0.27158075971485934,0.26343333692341353,6.763658403556466,1.2050743493660463,1.7332757829226497E-2,3]
[null,"MGE3B2","Short Rural",11,"MGE",0,41.718000000000004,0.4370196248511356,0.43212056736705129,6.763658403556466,0.66207642119320331,41.738999999999997,0.37342354460793159,0.36222083826969365,6.763658403556466,0.66207642119320331,1.7332757829226497E-2,3]
[null,"MGE3B3","Short Rural",11,"MGE",0,0.97299999999999998,0.11445752079434504,0.1131744343104182,6.763658403556466,2.0614868711684777,0.98899999999999999,9.3355886151982898E-2,9.0555209567423411E-2,6.763658403556466,2.0405290563968945,1.7332757829226497E-2,3]
[null,"MGE3B4","Long Rural",11,"MGE",0,289.43099999999998,1.0301176871491053,1.0185699087937639,6.763658403556466,1.0564643900766366,289.41000000000003,0.61105670935843348,0.59272500807768047,6.763658403556466,1.320342330609755,1.7332757829226497E-2,5]
[null,"MGH21","Short Rural",22,"MGH",0,25.599,0.68,0.60210244947835856,6.2111341959419937,1.0002593413710266,25.617999999999999,0.66649999999999998,0.57812209999999997,6.0587137248759326,1.5184889429956347,6.898627202006527E-3,3]
[null,"MGI2U23","Long Rural",22,"MGI",0,356.27,3.24,3.0779999999999998,4.0715318333521591,2.0481500799501973,356.27300000000002,3.01,2.8594999999999997,4.0715318333521591,2.0481500799501973,-6.3469664617800863E-3,6]
[null,"MGI2U24","Short Rural",22,"MGI",0,6.306,1.07,1.0165,3.6794301715347175,3.4332711107630289,7.2930000000000001,1.105,1.04975,2.4657821706712051,2.4657821706712051,-6.3469664617800863E-3,4]
[null,"MGI2U30","Long Rural",22,"MGI",0,415.16500000000002,2.21,2.0994999999999999,5.8247483017895272,2.1929495274629556,414.32499999999999,2.21,2.0994999999999999,5.8247483017895272,2.1929495274629556,-6.3469664617800863E-3,6]
[null,"MGY2221","Short Rural",11,"MGY",0,31.3,0.30945083420959629,0.2902631801466814,0.75810131796482183,0.75810131796482183,31.279,0.18578042590512223,0.16785261480527794,0.75810131796482183,0.75810131796482183,2.0640523003965846E-2,3]
[null,"MGY2223","Short Rural",11,"MGY",0,108.221,0.58022031414299302,0.54424346277502755,1.3504453736453019,0.66017116530487752,108.277,0.16154819643923671,0.14595879548285037,1.3504453736453019,0.66017116530487752,2.0640523003965846E-2,3]
[null,"MLA3B1","Short Rural",11,"MLA",0,106.883,0.62551392639741565,0.56296253375767413,1.5693592752139327,1.5693592752139327,106.907,0.48,0.432,1.5693592752139327,1.5693592752139327,4.4895282505084226E-2,3]
[null,"MLA3B2","Short Rural",11,"MLA",0,101.07299999999999,1.0176271339898255,0.91586442059084294,2.7258495994276717,2.7258495994276717,100.505,0.69,0.621,2.7258495994276717,2.7258495994276717,4.4895282505084226E-2,3]
[null,"MLA3B3","Short Rural",11,"MLA",0,187.072,1.2230197665382305,1.1007177898844076,2.1298855575593727,2.1298855575593727,187.208,0.56999999999999995,0.51300000000000001,2.1298855575593727,2.1298855575593727,4.4895282505084226E-2,3]
[null,"MLA3B4","Short Rural",11,"MLA",0,14.945,2.5860799643594645,2.3274719679235183,2.1298855575593727,2.1298855575593727,15.875999999999999,2.46,2.214,2.1298855575593727,2.1298855575593727,4.4895282505084226E-2,3]
[null,"MLN3B1","Short Rural",11,"MLN_11",0,28.007999999999999,1.3722867599708575,1.3657530687681461,8.9547026751310952,3.9095850828444698,28.373999999999999,2.0832706203679812,2.0207725017569418,8.9547026751310952,3.9095850828444698,6.8784016167019292E-3,3]
[null,"MLN3B2","Urban",11,"MLN_11",0,5.76,2.0786108276029163,2.0687142071046916,8.9547026751310952,6.481680532084253,6.1189999999999998,2.3937187912463473,2.321907227508957,8.9547026751310952,6.481680532084253,6.8784016167019292E-3,1]
[null,"MLN3B3","Short Rural",11,"MLN_11",0,118.04,1.2175681546800254,1.2117711051325215,8.9547026751310952,3.8143222884281816,117.65,2.4917550557342523,2.4170024040622247,8.9547026751310952,3.8143222884281816,6.8784016167019292E-3,3]
[null,"MLN3B4","Short Rural",11,"MLN_11",0,79.459999999999994,1.5740936364371598,1.5665991082928732,8.9547026751310952,5.1975380633526864,79.841999999999999,1.5277317882698531,1.4818998346217576,8.9547026751310952,5.1975380633526864,6.8784016167019292E-3,3]
[null,"MLN3B5","Short Rural",11,"MLN_11",0,116.88,1.1166647164468742,1.1113480853701578,8.9547026751310952,4.1201158585044668,116.336,0.98036264487905012,0.95095176553267857,8.9547026751310952,4.1201158585044668,6.8784016167019292E-3,3]
[null,"MLN3B6","Short Rural",11,"MLN_11",0,50.188000000000002,0.49779029528354635,0.49542023082766079,8.9547026751310952,5.616694358784355,50.082999999999998,0.547369143390803,0.53094806908907888,8.9547026751310952,5.616694358784355,6.8784016167019292E-3,3]
[null,"MLS3B1","Short Rural",11,"MLS",0,83.397999999999996,1.007724723796243,0.98378018545941726,9.0880705873138989,4.3906621946467261,82.887,1.26,1.2222,9.0880705873138989,4.3906621946467261,1.564398406726988E-2,3]
[null,"MLS3B2","Urban",11,"MLS",0,4.0830000000000002,4.1091687766448741,4.0115308533296625,7.2399723756379064,6.0863399352566576,3.9969999999999999,3.7,3.589,2.7765294060571373,2.7765294060571373,1.564398406726988E-2,1]
[null,"MLS3B3","Short Rural",11,"MLS",0,36.015999999999998,1.9567470364975592,1.9102527872998392,7.2399723756379064,5.2947061136573019,7.7789999999999999,1.96,1.9012,9.0880705873138989,8.7841822731259391,1.564398406726988E-2,3]
[null,"MLS3B4","Urban",11,"MLS",0,7.1589999999999998,2.5144199418993636,2.4546748316802933,9.0880705873138989,8.7841822731259391,4.3170000000000002,2.95,2.8614999999999999,7.2399723756379064,6.0863399352566576,1.564398406726988E-2,1]
[null,"MLS3B5","Urban",11,"MLS",0,3.762,2.4263663252569736,2.3687134562518009,2.7765294060571373,2.7765294060571373,35.201000000000001,2.17,2.1048999999999998,7.2399723756379064,5.2947061136573019,1.564398406726988E-2,1]
[null,"MLS3B6","Short Rural",11,"MLS",0,22.919,0.73378013868658476,0.71634479523743977,9.0880705873138989,5.2737482988857174,0,"","","","",1.564398406726988E-2,3]
[null,"MNE3B3","Short Rural",11,"MNE",0,35.017000000000003,2.970935059178379,2.9637252268347645,7.2399723756379064,4.5345090142153204,34.93,2.3750962904262338,2.3275943646177093,7.2399723756379064,4.5345090142153204,1.8313935207909287E-2,3]
[null,"MNE3B6","Short Rural",11,"MNE",0,21.274999999999999,2.0720852801275953,2.0670567664866666,7.2399723756379064,6.4931120674142075,21.696000000000002,1.7857866845310033,1.7500709508403831,7.2399723756379064,6.4931120674142075,1.8313935207909287E-2,3]
[null,"MNE3B8","Urban",11,"MNE",0,0.627,0.22707783891809266,0.2265267689300457,6.763658403556466,6.763658403556466,0.627,0.19643653529841035,0.19250780459244213,6.763658403556466,6.763658403556466,1.8313935207909287E-2,1]
[null,"MOA22","Short Rural",22,"MOA",0,125.664,1.1651146166701556,1.1381887846347305,4.8881245070885821,3.4332711107630289,125.51300000000001,1.2810307115753041,1.2359384305278533,4.8881245070885821,3.4332711107630289,-4.3635035836797446E-3,4]
[null,"MOA23","Short Rural",22,"MOA",0,28.135000000000002,4.5785363451960022,4.4727262396192922,4.8881245070885821,3.7590698676667342,32.081000000000003,4.5222963375074494,4.3631115064271873,4.8881245070885821,3.7552593558900833,-4.3635035836797446E-3,4]
[null,"MOA24","Long Rural",22,"MOA",0,223.87299999999999,2.3484341492257821,2.2941617690293783,12.536583745183533,3.4904287874128017,215.89099999999999,1.702309267730941,1.6423879815068119,12.536583745183533,3.4904287874128017,-4.3635035836797446E-3,6]
[null,"MOA25","Short Rural",22,"MOA",0,35.578000000000003,5.6890362142097439,5.557562424974269,4.8881245070885821,4.5383195259919722,36.115000000000002,5.2444881480599701,5.0598821652482595,4.8881245070885821,4.5383195259919722,-4.3635035836797446E-3,4]
[null,"MON1012","Short Rural",11,"MON",0,166.56200000000001,0.68061713211797703,0.6353855889099016,2.0597721408689846,0.77829703038107501,166.715,0.7107473927195177,0.62545770559317559,2.0597721408689846,0.77829703038107501,-5.5443878542444766E-9,4]
[null,"MOU12","Long Rural",22,"MOU",0,280.42599999999999,1.32,1.3011300081408741,3.4675657167528922,2.0271922651786141,280.47899999999998,1.48745022101582,1.3421263344225745,1.9090664001024165,1.9090664001024165,1.4059381103902049E-8,5]
[null,"MOU22","Long Rural",22,"MOU",0,357.96899999999999,4.8600000000000003,4.7905241208823091,4.7882890985403117,1.9948029150770761,372.59199999999998,4.7860386960408103,4.318442715437623,4.7882890985403117,1.850003467564318,1.4059381103902049E-8,5]
[null,"MPTA2","Short Rural",11,"MPT",0,68.221000000000004,0.67819900512910569,0.67549906258790449,2.4440622535442911,2.4440622535442911,40.966000000000001,0.561731510468929,0.55566481015586455,1.3917894264219712,1.3917894264219712,9.2482727313590602E-3,3]
[null,"MPTB2","Short Rural",11,"MPT",0,19.244,1.4781260368198457,1.4722415466659455,3.583405274763098,2.7359474556357983,19.832000000000001,1.2295371156897905,1.2162581148403406,3.583405274763098,2.7359474556357983,9.2482727313590602E-3,3]
[null,"MPTC2","Short Rural",11,"MPT",0,12.26,2.5215091216338541,2.5114708737242597,3.583405274763098,3.583405274763098,12.722,2.0024944322299589,1.9808674923618752,3.583405274763098,3.583405274763098,9.2482727313590602E-3,3]
[null,"MPTD2","Short Rural",11,"MPT",0,48.533000000000001,3.5648922064478628,3.5507002007825741,3.583405274763098,3.2446507778187779,53.497,3.3390280261043075,3.3029665234223811,3.583405274763098,3.2446507778187779,9.2482727313590602E-3,3]
[null,"MRE8B1","Urban",22,"MRE",0,8.2159999999999993,4.9472267657542162,4.8039320790512603,12.536583745183533,12.536583745183533,9.0500000000000007,4.4359662932673354,4.2141679786039683,5.5530588121142745,5.5530588121142745,3.8747922506888635E-5,1]
[null,"MRE8B10","Long Rural",22,"MRE",0,348.76799999999997,2.0212405074093103,1.9626959856046007,12.536583745183533,12.536583745183533,349.22399999999999,1.9011284114002867,1.8060719908302723,5.5530588121142745,4.1477420688851909,3.8747922506888635E-5,5]
[null,"MRE8B2","Long Rural",22,"MRE",0,274.17700000000002,2.0501153718008718,1.9907344996846663,12.536583745183533,12.536583745183533,274.67599999999999,1.1002386800783426,1.0452267460744253,4.7882890985403117,4.7882890985403117,3.8747922506888635E-5,5]
[null,"MRE8B3","Short Rural",22,"MRE",0,198.149,2.5698629308489802,2.4954277531258495,12.536583745183533,12.536583745183533,197.36799999999999,2.4683158932545157,2.3449000985917898,5.5530588121142745,5.0717911747231854,3.8747922506888635E-5,3]
[null,"MRE8B4","Long Rural",22,"MRE",0,360.60599999999999,3.1184853542886501,3.0281595206470984,12.536583745183533,12.536583745183533,359.99200000000002,3.0346280857848957,2.8828966814956507,5.5530588121142745,4.8545920034540497,3.8747922506888635E-5,5]
[null,"MRE8B5","Short Rural",22,"MRE",0,11.592000000000001,2.7912368911842855,2.7103896944063535,12.536583745183533,12.536583745183533,11.587999999999999,3.0687643694150113,2.9153261509442605,6.0587137248759326,6.0587137248759326,3.8747922506888635E-5,3]
[null,"MRE8B6","Long Rural",22,"MRE",0,581.21400000000006,1.2801189880258965,1.2430407908829137,12.536583745183533,12.536583745183533,579.06700000000001,1.1676359580147249,1.1092541601139885,2.7008907472906039,2.7008907472906039,3.8747922506888635E-5,5]
[null,"MRE8B7","Short Rural",22,"MRE",0,31.25,4.2927298395454878,4.1683924265697714,12.536583745183533,12.536583745183533,30.26,3.6018155676391252,3.4217247892571687,5.5530588121142745,5.5530588121142745,3.8747922506888635E-5,3]
[null,"MRE8B8","Short Rural",22,"MRE",0,10.228,3.1569851734773988,3.0655442060871856,12.536583745183533,12.536583745183533,10.881,2.8018011256410302,2.6617110693589785,5.5530588121142745,5.5530588121142745,3.8747922506888635E-5,3]
[null,"MRE8B9","Short Rural",22,"MRE",0,13.247,3.0414857159111528,2.953390149766923,12.536583745183533,12.536583745183533,14.268000000000001,2.6346208647858482,2.5028898215465558,5.5530588121142745,5.5530588121142745,3.8747922506888635E-5,3]
[null,"MRH3B2","Short Rural",11,"MRH",0,173.68700000000001,0.63267242298336512,0.60286654330675649,6.763658403556466,4.2525311427431083,174.03899999999999,0.55785093264797692,0.51846665680302972,6.763658403556466,4.2515785147989442,-1.352720297997603E-12,4]
[null,"MRH3B3","Short Rural",11,"MRH",0,21.184999999999999,1.3334787992110928,1.2706571758927023,6.763658403556466,4.2868257487329711,20.994,1.2953487758097093,1.2038971522375439,6.763658403556466,4.2868257487329711,-1.352720297997603E-12,4]
[null,"MRH3B4","Short Rural",11,"MRH",0,8.7070000000000007,1.3724124867792997,1.3077566554808102,6.763658403556466,5.245169460560831,9.3640000000000008,1.3331691780231314,1.2390474340546984,6.763658403556466,5.2975639974897897,-1.352720297997603E-12,4]
[null,"MRH3B5","Short Rural",11,"MRH",0,139.63499999999999,1.1290769394780054,1.0758849080551345,6.763658403556466,3.1913036129456565,138.72900000000001,0.99278555810233193,0.92269489770030733,6.763658403556466,3.1913036129456565,-1.352720297997603E-12,4]
[null,"MRH3B6","Long Rural",11,"MRH",0,214.77500000000001,1.0609429862336432,1.0109608187759456,6.763658403556466,4.2477680030222933,223.53200000000001,1.3331691780231314,1.2390474340546984,6.763658403556466,4.2468153750781301,-1.352720297997603E-12,6]
[null,"MRN8B2","Short Rural",22,"MRN",0,162.47800000000001,1.0934739283659076,1.0908827542776498,10.7075380923908,4.8793603300022843,161.4,0.54350282735972077,0.5314914148750709,10.7075380923908,4.8907918653322389,5.6110267395684199E-2,3]
[null,"MRN8B3","Long Rural",22,"MRN",0,221.06,2.3269125195626517,2.3213985011028391,10.7075380923908,5.9253458126931289,181.01,0.74265495826087391,0.72624228368330856,10.7075380923908,5.9234405568048043,5.6110267395684199E-2,5]
[null,"MSS W390","Short Rural",11,"MSS",0,9.0069999999999997,0.51,0.48449999999999999,2.3941445492701559,0.66493430502569195,9.2129999999999992,0.495,0,2.0357659166760795,0.66493430502569195,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"MSS W590","Short Rural",11,"MSS",0,2.4470000000000001,0.03,2.8499999999999998E-2,2.3941445492701559,0.67065007269066923,0,"","","","",{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"MSW3B1","Urban",11,"MSW",0,4.6180000000000003,3.0784524012452374,2.8335870952375992,8.9547026751310952,8.9547026751310952,3.8809999999999998,2.21335727380951,1.9134473632083215,9.5424741166795943,9.5424741166795943,7.0052571221460233E-3,1]
[null,"MSW3B2","Urban",11,"MSW",0,0.69599999999999995,0.84049851744524562,0.77364384508131812,8.9547026751310952,8.9547026751310952,1.9419999999999999,2.1363709338509187,1.8468926723141192,5.6205048705610059,5.6205048705610059,7.0052571221460233E-3,1]
[null,"MSW3B3","Urban",11,"MSW",0,6.8940000000000001,2.5417485286597188,2.3395735556073594,8.9547026751310952,8.9547026751310952,7.327,1.9246584989647915,1.6638672723550623,6.4083281803837107,6.4083281803837107,7.0052571221460233E-3,1]
[null,"MSW3B4","Urban",11,"MSW",0,3.0249999999999999,2.8455431735194465,2.6192038610584389,8.9547026751310952,8.9547026751310952,4.1500000000000004,2.4346930011904608,2.1047920995291536,10.021645972593523,10.021645972593523,7.0052571221460233E-3,1]
[null,"MSW3B5","Urban",11,"MSW",0,1.7809999999999999,2.8759226380054188,2.647166891603546,7.9258644954351825,7.9258644954351825,1.84,2.5694190961179966,2.221262808594008,7.9258644954351825,7.9258644954351825,7.0052571221460233E-3,1]
[null,"MSW3B6","Urban",11,"MSW",0,3.91,3.6455357383167284,3.3555636654129462,5.6205048705610059,5.6205048705610059,2.2719999999999998,2.5694190961179966,2.221262808594008,5.6205048705610059,5.6205048705610059,7.0052571221460233E-3,1]
[null,"MTG11B1","Long Rural",19.100000000000001,"MTG_6_6",0,238.36699999999999,0.11016040699198874,0.10811611732886868,1.9161193109908372,0.2448080611417851,237.14400000000001,8.232307239143527E-2,6.9974611532719971E-2,1.9161193109908372,0.2448080611417851,1.1196435634343726E-2,5]
[null,"MTG4B1","Long Rural",33,"MTG_33",0,1905.768,1.084506537135085,1.0382906480283607,7.3321867606328732,1.5889834108636878,2001.4780000000001,0.89241026725733352,0.82994154854932023,7.3321867606328732,1.5889834108636878,8.3021844373043652E-3,5]
[null,"MUA5005","Long Rural",11,"MUA",0,259.755,1.2285913107795696,1.2156604488604719,2.7765294060571373,1.0193119002542841,260.19799999999998,1.1758273393562892,1.1700657853934433,2.7765294060571373,1.0193119002542841,-1.4381301232469373E-2,6]
[null,"MUA5006","Short Rural",11,"MUA",0,154.874,0.45947317313707486,0.45463724103724973,2.7138464873312196,1.167921859543694,155.03299999999999,1.0035078154851091,0.99859062718923208,2.7138464873312196,1.167921859543694,-1.4381301232469373E-2,4]
[null,"MUA5027","Short Rural",11,"MUA",0,69.881,0.45947317313707486,0.45463724103724973,2.7765294060571373,1.5489730372088473,69.492999999999995,0,0,2.7765294060571373,1.5489730372088473,-1.4381301232469373E-2,4]
[null,"MUD32","Short Rural",22,"MUD",0,29.53,5.8484406630627737,5.8465420930708278,4.7882890985403117,4.7882890985403117,44.008000000000003,7.0080284473524612,6.9470585998604948,4.7882890985403117,4.7882890985403117,1.472707800495951E-2,3]
[null,"MUD42","Long Rural",22,"MUD",0,592.65,2.2746610976707178,2.273922678055869,4.7882890985403117,4.7882890985403117,589.96799999999996,3.8080640015801754,3.7749338447664278,4.7882890985403117,4.7882890985403117,1.472707800495951E-2,5]
[null,"MUD52","Urban",22,"MUD",0,11.646000000000001,6.0622318415906724,6.0602638689084234,4.7882890985403117,4.7882890985403117,11.972,6.3605937804171377,6.305256614527508,4.7882890985403117,4.7882890985403117,1.472707800495951E-2,1]
[null,"MUD62","Long Rural",22,"MUD",0,379.86,2.9872983594303837,2.986328597514524,10.821853445690346,10.273139749852525,367.51499999999999,2.7141226677929056,2.690509800583107,10.821853445690346,10.273139749852525,1.472707800495951E-2,5]
[null,"MUD72","Short Rural",22,"MUD",0,123.485,2.4142994800425446,2.4135157298416869,10.821853445690346,8.6917773625421422,123.11,1.8232355563121165,1.8073734069722009,10.821853445690346,8.6917773625421422,1.472707800495951E-2,3]
[null,"MUD82","Short Rural",22,"MUD",0,130.749,1.5783952324649901,1.5778828405307239,4.7882890985403117,4.7882890985403117,130.46199999999999,2.0252266675070447,2.0076071954997334,4.7882890985403117,4.7882890985403117,1.472707800495951E-2,3]
[null,"MUD92","Short Rural",22,"MUD",0,32.960999999999999,6.5100376885072198,6.5079243453250113,10.821853445690346,10.821853445690346,15.522,5.7928924468482341,5.7424942825606546,10.821853445690346,10.821853445690346,1.472707800495951E-2,3]
[null,"MUL3B1","Short Rural",11,"MUL_11",0,57.558999999999997,0.90658945654973777,0.90473809830300511,6.763658403556466,3.7895539618799465,81.381,1.2686357401565249,1.2432630253533945,6.763658403556466,2.3310805793665734,-2.6343315471663638E-2,4]
[null,"MUL3B2","Short Rural",11,"MUL_11",0,87.289000000000001,1.1892893946136345,1.1868607311071679,3.5163402674940318,3.5163402674940318,89.164000000000001,1.1753537004391332,1.1518466264303506,3.5163402674940318,2.3548962779706457,-2.6343315471663638E-2,4]
[null,"MUL3B3","Short Rural",11,"MUL_11",0,25.015999999999998,3.1389441398818878,3.1325340607910497,3.5163402674940318,3.5163402674940318,25.135999999999999,2.8357740074087023,2.7790585272605282,3.5163402674940318,2.3587067897472971,-2.6343315471663638E-2,4]
[null,"MUL3B5","Short Rural",11,"MUL_11",0,51.311,2.7880062857336019,2.7823128614479509,3.5163402674940318,3.5163402674940318,51.103000000000002,2.5559278882565279,2.5048093304913972,3.5163402674940318,2.3415594867523652,-2.6343315471663638E-2,4]
[null,"MUL3B6","Short Rural",11,"MUL_11",0,19.300999999999998,0.98457564636046779,0.98256503149036023,3.6457071423113514,3.6457071423113514,19.201000000000001,0.89550758128695862,0.87759742966121945,2.5311324476407786,2.5311324476407786,-2.6343315471663638E-2,4]
[null,"MUN12662","Urban",33,"MUN",0,2.2869999999999999,3.42,3.0702134431201418,4.1753682792659141,4.1753682792659141,2.2669999999999999,1.33,1.2088370000000002,4.1753682792659141,4.1753682792659141,1.3812866552133769E-2,1]
[null,"MUN7292","Urban",33,"MUN",0,4.3330000000000002,4.5999999999999996,4.1295268533194882,10.549020802482097,10.549020802482097,4.0439999999999996,7.1450000000000005,6.4940905000000004,10.549020802482097,10.549020802482097,1.3812866552133769E-2,1]
[null,"MUR1483","Short Rural",11,"MUR",0,59.045999999999999,0.55000000000000004,0.49639818587503043,5.1822960162460801,1.7318776024881204,59.073,0.5,0.42485000000000001,5.1822960162460801,1.7318776024881204,1.6193892807575619E-6,3]
[null,"MUR823","Short Rural",11,"MUR",0,15.955,0.3,0.27076264684092566,5.1822960162460801,2.3758540927422289,15.98,0.28999999999999998,0.24641299999999999,5.1822960162460801,2.320601671980782,1.6193892807575619E-6,3]
[null,"MUR825","Urban",11,"MUR",0,1.2310000000000001,0.53,0.47834734275230201,5.1822960162460801,3.4342237387071912,1.2549999999999999,1.3,1.1046100000000001,5.1822960162460801,2.5778112169047604,1.6193892807575619E-6,1]
[null,"MWA8B1","Short Rural",22,"MWA",0,156.28299999999999,3.9646142282576551,3.8318974876563918,4.0715318333521591,4.0715318333521591,156.92699999999999,3.6563532012627822,3.5188743208953017,4.0715318333521591,4.0715318333521591,1.4584748047235196E-4,3]
[null,"MWA8B2","Urban",22,"MWA",0,9.7309999999999999,3.3699220940190067,3.257112864507933,4.8881245070885821,4.8881245070885821,9.8759999999999994,3.486290261669164,3.3552057478304036,7.166810549526196,6.544553976399003,1.4584748047235196E-4,1]
[null,"MWA8B3","Urban",22,"MWA",0,9.8109999999999999,4.8115999952036086,4.6505301327466206,6.4252849577898106,6.4252849577898106,9.7159999999999993,5.0168567180117245,4.8282229054144841,6.4252849577898106,6.4252849577898106,1.4584748047235196E-4,1]
[null,"MWA8B4","Long Rural",22,"MWA",0,309.34500000000003,1.6849610470095033,1.6285564322539665,4.8881245070885821,4.5802351555351386,309.67,1.4455349865457512,1.391182871051631,4.8881245070885821,4.5802351555351386,1.4584748047235196E-4,5]
[null,"MWB8B1","Long Rural",22,"MWB",0,611.745,1.28,1.28,4.0715318333521591,1.5985096903053171,546.66,1.1299999999999999,1.1073999999999999,4.0715318333521591,1.5985096903053171,1.6833504577804304E-2,5]
[null,"MWB8B2","Urban",22,"MWB",0,1.5589999999999999,2.11,2.11,4.0715318333521591,3.4218395754330744,1.5589999999999999,2.2999999999999998,2.254,4.0715318333521591,3.4218395754330744,1.6833504577804304E-2,1]
[null,"MWN3B10","Short Rural",11,"MWN",0,79.009,1.0657976676604757,1.0137036011152072,8.9547026751310952,8.9547026751310952,0,"","","","",-1.4241200508519343E-3,4]
[null,"MWN3B2","Short Rural",11,"MWN",0,71.77,2.305998590029029,2.1932859733219936,8.9547026751310952,8.9547026751310952,72.119,2.1146723321940994,1.9032050989746896,8.9547026751310952,8.9337448603595124,-1.4241200508519343E-3,4]
[null,"MWN3B3","Short Rural",11,"MWN",0,16.539000000000001,4.4085267162319663,4.1930467137038105,8.9547026751310952,8.9547026751310952,13.877000000000001,2.9143383401666583,2.6229045061499927,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,4]
[null,"MWN3B4","Short Rural",11,"MWN",0,104.80500000000001,1.5502511529606917,1.4744779652584832,8.9547026751310952,8.9547026751310952,222.89400000000001,2.4345387353831232,2.1910848618448111,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,4]
[null,"MWN3B5","Short Rural",11,"MWN",0,11.294,2.4319564962070848,2.3130873079992451,8.9547026751310952,6.8427265229219856,11.204000000000001,1.9369687748668645,1.743271897380178,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,4]
[null,"MWN3B6","Short Rural",11,"MWN",0,91.061999999999998,2.3253767294410372,2.2117169478877243,8.9547026751310952,8.9547026751310952,84.95,1.6881837946087348,1.5193654151478613,8.9547026751310952,6.8427265229219856,-1.4241200508519343E-3,4]
[null,"MWN3B7","Urban",11,"MWN",0,4.1120000000000001,3.9240732309317505,3.7322723495605352,8.9547026751310952,8.9337448603595124,4.3079999999999998,3.820626482535558,3.4385638342820024,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,2]
[null,"MWN3B8","Long Rural",11,"MWN",0,264.99599999999998,3.9143841612257466,3.7230568622776699,8.9547026751310952,8.9547026751310952,79.024000000000001,1.954739130599588,1.7592652175396293,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,6]
[null,"MWN3B9","Short Rural",11,"MWN",0,54.622999999999998,2.877653702683284,2.7369997230110594,8.9547026751310952,8.9547026751310952,54.58,2.8610272729684878,2.5749245456716392,8.9547026751310952,8.9547026751310952,-1.4241200508519343E-3,4]
[null,"MYT3B2","Short Rural",11,"MYT",0,87.561999999999998,2.2974988288302853,2.2523688950413536,6.763658403556466,3.381829201778233,88.12,2.2977357163056902,2.2441984741157674,6.763658403556466,3.381829201778233,-6.9553432592323267E-3,4]
[null,"MYT3B3","Urban",11,"MYT",0,10.006,3.396302616531726,3.3295888013654795,9.0880705873138989,5.3823478845202866,10.430999999999999,2.866936190930657,2.8001365776819727,9.0880705873138989,5.3632953256370284,-6.9553432592323267E-3,2]
[null,"MYT3B6","Short Rural",11,"MYT",0,56.963999999999999,2.097716321975478,2.0565107302551491,6.763658403556466,4.1677472557126114,56.939,2.184094991074085,2.1332055777820589,6.763658403556466,4.1677472557126114,-6.9553432592323267E-3,4]
[null,"MYT3B7","Short Rural",11,"MYT",0,73.97,0.99891253427403714,0.9792908239310234,6.763658403556466,3.2132140556614028,74.510999999999996,0.98687998227446116,0.96388567868746622,6.763658403556466,3.2132140556614028,-6.9553432592323267E-3,4]
[null,"NAN3B1","Short Rural",11,"NAN",0,110.88500000000001,0.69547099013188762,0.6219095925107444,1.2328910853356025,0.93738589705627651,112.402,0.67772102114728661,0.59043055362351604,1.2328910853356025,0.93738589705627651,-1.3257497085294091E-2,4]
[null,"NAN3B2","Short Rural",11,"NAN",0,48.246000000000002,0.42930308032832565,0.38389481019181748,2.0357659166760795,1.0174066443659586,48.277999999999999,0.37969754646328752,0.33079250247881609,2.0357659166760795,1.0174066443659586,-1.3257497085294091E-2,4]
[null,"NAN3B3","Short Rural",11,"NAN",0,68.326999999999998,0.18889335534446328,0.16891371648439968,0.42277628161948722,0.42277628161948722,68.695999999999998,0.28064601260329947,0.24449880617999448,0.42277628161948722,0.42277628161948722,-1.3257497085294091E-2,4]
[null,"NARC2","Short Rural",11,"NAR",0,16.518000000000001,1.9183237774261586,1.897409799595497,2.7130843849758892,2.7130843849758892,16.614000000000001,1.6235655919894032,1.5962896900439811,2.7130843849758892,2.7130843849758892,-3.674214335533341E-3,4]
[null,"NARD2","Short Rural",11,"NAR",0,14.255000000000001,2.206072344040082,2.1820212695348213,2.5035062372600549,2.5035062372600549,14.619,2.0650360212960028,2.0303434161382299,2.5035062372600549,2.5035062372600549,-3.674214335533341E-3,4]
[null,"NARE2","Short Rural",11,"NAR",0,12.826000000000001,1.9183237774261586,1.897409799595497,3.0312621183262927,3.0312621183262927,13.215,1.7145704611885708,1.6857656774406027,3.0312621183262927,3.0312621183262927,-3.674214335533341E-3,4]
[null,"NARF2","Short Rural",11,"NAR",0,138.12200000000001,1.7264913996835427,1.7076688196359473,2.1577022935289287,2.1577022935289287,138.577,1.5490190501985959,1.5229955301552593,6.763658403556466,2.1577022935289287,-3.674214335533341E-3,4]
[null,"NBI3B1","Short Rural",11,"NBI",0,110.896,0.42405231509394475,0.41405906676377996,1.3917894264219712,1.3917894264219712,110.876,0.41904584078511714,0.40647446556156364,1.3917894264219712,1.3917894264219712,1.5209428285254338E-10,3]
[null,"NBI3B2","Short Rural",11,"NBI",0,131.10599999999999,1.0964781290286285,1.0706384440606311,2.7258495994276717,1.2879529805082173,134.56200000000001,1.6680465506980391,1.6180051541770979,2.7258495994276717,1.2879529805082173,1.5209428285254338E-10,3]
[null,"NBI8B1","Short Rural",22,"NBI",0,60.087000000000003,4.0224391031768469,3.9276460047307125,11.029526337517852,11.029526337517852,60.332000000000001,5.0387211049744423,4.8875594718252087,11.029526337517852,11.029526337517852,1.5209428285254338E-10,3]
[null,"NBI8B2","Short Rural",22,"NBI",0,53.767000000000003,0.77454453471240936,0.7562915607215982,7.3923928467039675,7.3923928467039675,53.85,1.2784966550167287,1.2401417553662268,10.981894940309708,10.981894940309708,1.5209428285254338E-10,3]
[null,"NBI8B3","Short Rural",22,"NBI",0,17.77,2.8022069311718227,2.736169914655346,7.3923928467039675,7.3923928467039675,18.417999999999999,3.7592073484024104,3.6464311279503381,11.065726199396044,11.065726199396044,1.5209428285254338E-10,3]
[null,"NBI8B5","Long Rural",22,"NBI",0,355.80700000000002,2.1427623105563414,2.0922658149124884,7.3923928467039675,7.3923928467039675,410.00400000000002,1.3568134747751124,1.316109070531859,10.648475159852699,10.648475159852699,1.5209428285254338E-10,5]
[null,"NBI8B6","Short Rural",22,"NBI",0,30.096,5.2755569649238518,5.1512327979428632,7.3923928467039675,7.3923928467039675,30.51,6.8206830298664949,6.6160625389704997,8.0973375253844999,8.0973375253844999,1.5209428285254338E-10,3]
[null,"NBI8B7","Urban",22,"NBI",0,11.994,4.4516838955984728,4.3467751825160903,7.3923928467039675,7.3923928467039675,12.314,5.3092701186852223,5.1499920151246652,13.666400486960715,13.666400486960715,1.5209428285254338E-10,1]
[null,"NBI8B8","Short Rural",22,"NBI",0,113.172,0.72521600009944021,0.70812550601642377,7.3923928467039675,7.3923928467039675,113.232,0.81368124424294597,0.78927080691565754,8.5088727972628675,8.5088727972628675,1.5209428285254338E-10,3]
[null,"NDA3B2","Short Rural",11,"NDA",0,189.93600000000001,3.5371989431183284,3.430991555304912,7.9449170543184398,4.645013855738215,190.02500000000001,4.1815589022694839,3.9967339987891726,4.645013855738215,4.645013855738215,-1.0149906809839605E-3,4]
[null,"NDA3B3","Long Rural",11,"NDA",0,262.29500000000002,0.95736153731122842,0.92861594801699898,8.0020747309682125,3.9924637139866408,262.58800000000002,1.4586833380009829,1.3942095344613394,3.9924637139866408,3.9924637139866408,-1.0149906809839605E-3,6]
[null,"NDA3B4","Short Rural",11,"NDA",0,21.224,2.6906897943378736,2.6098995591635656,7.9449170543184398,2.2605861114985202,21.885999999999999,2.7228755642685014,2.6025244643278338,7.9449170543184398,4.6678769263981241,-1.0149906809839605E-3,4]
[null,"NDA3B5","Urban",11,"NDA",0,4.6769999999999996,2.9426270409987234,2.8542721770627759,7.9449170543184398,5.4938053539873435,5.2649999999999997,3.0146122318686981,2.8813663712201016,5.4938053539873435,5.4938053539873435,-1.0149906809839605E-3,2]
[null,"NDA3B6","Short Rural",11,"NDA",0,61.616999999999997,0.61472688185247304,0.59626918767407311,8.0020747309682125,4.308736191448717,61.755000000000003,0.68071889106712535,0.65063111608195845,4.308736191448717,4.308736191448717,-1.0149906809839605E-3,4]
[null,"NDA3B7","Short Rural",11,"NDA",0,116.24299999999999,0.59457190211960498,0.57671937824213615,7.9449170543184398,1.6042254579702941,116.1,0.97245555866732192,0.92947302297422629,7.9449170543184398,1.6042254579702941,-1.0149906809839605E-3,4]
[null,"NDL615","Short Rural",11,"NDL",0,122.209,0.75463513736183352,0.68681698055863682,2.1298855575593727,1.0088329928684927,126.04300000000001,0.70164029866764432,0.63147626880087993,2.1298855575593727,1.3041476555589862,1.3818430333111189E-2,3]
[null,"NDL616","Long Rural",11,"NDL",0,204.10300000000001,1.1738768803406299,1.0683819697578794,2.1298855575593727,1.5899360388078509,203.899,1.2812561975670027,1.1531305778103025,2.1298855575593727,1.5899360388078509,1.3818430333111189E-2,5]
[null,"NER3B1","Short Rural",11,"NER",0,12.705,0.6530652267174879,0.59456822175570079,1.3917894264219712,1.3917894264219712,12.750999999999999,0.56441234257487161,0.51536491000511531,1.3917894264219712,1.3917894264219712,-1.9159985861147668E-2,4]
[null,"NER3B2","Short Rural",11,"NER",0,24.948,1.1736244654053407,1.068499413010245,2.7258495994276717,1.9252610751531858,25.010999999999999,1.2699277707934609,1.1595710475115091,2.7258495994276717,1.9252610751531858,-1.9159985861147668E-2,4]
[null,"NER3B3","Short Rural",11,"NER",0,2.1560000000000001,1.8929426861376462E-2,1.7233861500165242E-2,2.7258495994276717,2.5368482153057563,2.1659999999999999,8.8189428527323671E-2,8.0525767188299249E-2,3.1524363928238106,2.5368482153057563,-1.9159985861147668E-2,4]
[null,"NGN3B1","Short Rural",11,"NGN",0,92.611999999999995,1.7162481580360833,1.630435750134279,2.7258495994276717,2.7258495994276717,92.632000000000005,1.3713573922950277,1.289075948757326,2.7258495994276717,2.7258495994276717,1.7846107055534452E-3,3]
[null,"NGN3B2","Short Rural",11,"NGN",0,47.558999999999997,0.89998379018965347,0.85498460068017079,2.7258495994276717,2.1643706891380692,47.667999999999999,0.88734890089678264,0.83410796684297561,2.7258495994276717,2.1643706891380692,1.7846107055534452E-3,3]
[null,"NGN3B3","Short Rural",11,"NGN",0,73.507999999999996,1.0150979959115858,0.96434309611600644,2.0357659166760795,2.0357659166760795,71.956999999999994,0.54854295691801103,0.51563037950293034,2.0357659166760795,2.0357659166760795,1.7846107055534452E-3,3]
[null,"NHD3B1","Short Rural",11,"NHD",0,13.577,3.3612232108613949,3.3456679543955712,3.5163402674940318,3.5163402674940318,14.425000000000001,2.8994867177563703,2.8704918505788064,3.5163402674940318,3.5163402674940318,-3.906734492208578E-2,4]
[null,"NHD3B2","Short Rural",11,"NHD",0,11.311,2.7003085345684239,2.6878118959470036,2.7765294060571373,2.7765294060571373,11.991,2.450533935652158,2.4260285962956365,2.7765294060571373,2.7765294060571373,-3.906734492208578E-2,4]
[null,"NHD3B3","Short Rural",11,"NHD",0,19.716000000000001,0.61370648512918724,0.61086633998795536,2.7765294060571373,2.7765294060571373,19.169,0.31800822065715023,0.31482813845057872,2.7765294060571373,2.7765294060571373,-3.906734492208578E-2,4]
[null,"NHD3B4","Short Rural",11,"NHD",0,78.956999999999994,1.9638607524133993,1.9547722879614573,2.7765294060571373,2.7765294060571373,79.391000000000005,1.8145174943378575,1.7963723193944789,2.7765294060571373,2.7765294060571373,-3.906734492208578E-2,4]
[null,"NME8B1","Long Rural",22,"NME",0,783.11900000000003,3.7116819395202723,3.7047760098091365,12.536583745183533,6.5959958853837994,783.41499999999996,3.1399960084641494,3.1365420128548389,12.536583745183533,6.5959958853837994,1.1648015341008439E-7,5]
[null,"NME8B2","Short Rural",22,"NME",0,11.779,2.6323985386668594,2.6275007161766921,12.536583745183533,9.9873513666036615,12.493,2.3952533654309858,2.3926185867290117,12.536583745183533,9.9873513666036615,1.1648015341008439E-7,3]
[null,"NME8B3","Long Rural",22,"NME",0,407.32799999999997,2.7464691420090896,2.7413590805443486,12.536583745183533,7.4381189880237875,405.887,2.8783296744254701,2.8751635117836019,12.536583745183533,7.4381189880237875,1.1648015341008439E-7,5]
[null,"NME8B4","Short Rural",22,"NME",0,7.077,1.8251296534756891,1.8217338298825065,12.536583745183533,12.536583745183533,7.8689999999999998,1.912177056436501,1.9100736616744209,12.536583745183533,10.576075436096321,1.1648015341008439E-7,3]
[null,"NME8B5","Short Rural",22,"NME",0,130.12100000000001,1.4039458872889918,1.401333715294236,12.536583745183533,8.7165456890903759,129.44399999999999,1.5096134656077642,1.5079528907955957,12.536583745183533,8.7165456890903759,1.1648015341008439E-7,3]
[null,"NME8B6","Long Rural",22,"NME",0,237.792,5.1770504593781572,5.167418075147495,12.536583745183533,8.8137137393949896,242.971,2.6669837892403834,2.6640501070722191,12.536583745183533,8.8137137393949896,1.1648015341008439E-7,5]
[null,"NSK3B1","Short Rural",11,"NSK",0,6.6379999999999999,1.96,1.9580000005117593,4.3820885431492593,4.3820885431492593,7.0190000000000001,1.9814661238587956,1.9418368013816196,4.3820885431492593,4.3820885431492593,-3.6198551845436208E-3,4]
[null,"NSK3B2","Short Rural",11,"NSK",0,123.113,2.5,2.4974489802445907,5.0489281040632772,5.0489281040632772,122.125,1.8480982116759919,1.8111362474424719,5.0489281040632772,5.0489281040632772,-3.6198551845436208E-3,4]
[null,"NSK3B3","Short Rural",11,"NSK",0,83.537000000000006,3.91,3.9060102051025405,5.0489281040632772,4.6030982261950486,83.084000000000003,3.0484094213212236,2.987441232894799,5.0489281040632772,4.5992877144183968,-3.6198551845436208E-3,4]
[null,"NSK3B4","Short Rural",11,"NSK",0,9.5519999999999996,3.27,3.2666632661599251,4.3820885431492593,4.3820885431492593,9.8160000000000007,2.7054633614225865,2.6513540941941347,4.3820885431492593,4.3820885431492593,-3.6198551845436208E-3,4]
[null,"NSK3B5","Urban",11,"NSK",0,2.3290000000000002,1.23,1.2287448982803388,4.3820885431492593,4.3820885431492593,2.27,0.70494467868053301,0.69084578510692229,4.3820885431492593,4.3820885431492593,-3.6198551845436208E-3,2]
[null,"NVE12","Long Rural",22,"NVE",0,563.55399999999997,0.92996513245242207,0.89979800332462134,7.166810549526196,7.166810549526196,563.04899999999998,0.74669248675141286,0.73407338372531394,7.166810549526196,7.166810549526196,3.0900112931556666E-2,5]
[null,"NVE22","Short Rural",22,"NVE",0,151.852,1.9613810066269262,1.8977557888301102,7.166810549526196,7.166810549526196,151.727,0.83629558516158231,0.82216218977235156,7.166810549526196,7.166810549526196,3.0900112931556666E-2,3]
[null,"NVE32","Short Rural",22,"NVE",0,71.822999999999993,3.5676844172265643,3.4519523400271832,7.166810549526196,5.3728216050786566,72.450999999999993,4.9281704125593251,4.8448843325870721,7.166810549526196,5.460463375941643,3.0900112931556666E-2,3]
[null,"NVE42","Long Rural",22,"NVE",0,797.35699999999997,2.2319163178858128,2.1595152079790911,7.166810549526196,7.166810549526196,797.06100000000004,2.2500333600775906,2.2120077962922791,7.166810549526196,7.166810549526196,3.0900112931556666E-2,5]
[null,"NYM70","Short Rural",11,"NYM",0,52.567,0.14272341712000455,0.1399518247964511,1.3504453736453019,0.19243084472090227,52.570999999999998,0.10389689897985362,9.8702054030860936E-2,1.3504453736453019,0.19243084472090227,0,3]
[null,"NYM71","Short Rural",11,"NYM",0,35.280999999999999,0.12593242687059222,0.1234869042321627,1.3504453736453019,0.37438278205601283,35.284999999999997,0.13586517558903935,0.12907191680958738,1.3504453736453019,0.37438278205601283,0,3]
[null,"NYM72","Short Rural",11,"NYM",0,34.676000000000002,0.35261079523765826,0.34576333185005559,0.72247303285313003,0.33818292017782331,34.555,0.23976207456889292,0.22777397084044826,0.72247303285313003,0.33818292017782331,0,3]
[null,"NYN42","Short Rural",22,"NYN",0,47.848999999999997,0.52913439960415953,0.52904010449756711,5.5530588121142745,4.0867738804587654,48.146000000000001,1.2223868663934019,1.1734913917376657,5.5530588121142745,3.4618499490879153,4.5332988413981548E-2,3]
[null,"NYN52","Long Rural",22,"NYN",0,571.17999999999995,0.88219955941008743,0.8820423458523361,5.5530588121142745,4.363035984266002,1808.384,2.2394873888123392,2.1499078932598454,5.5530588121142745,4.3420781694944184,4.5332988413981548E-2,5]
[null,"NYN62","Long Rural",22,"NYN",0,1363.77,2.1183909588355672,2.1180134481286141,5.5530588121142745,4.12106848644863,36.761000000000003,3.0419703698034271,2.92029155501129,5.5530588121142745,3.4694709726412185,4.5332988413981548E-2,5]
[null,"OBR3B7","Short Rural",11,"OBR",0,154.881,1.2337140969162053,1.2166735659258525,2.7765294060571373,2.7765294060571373,154.74,1.1737760951318106,1.1497136851816085,2.7765294060571373,2.7765294060571373,-4.3189016092631477E-3,4]
[null,"OBR3B8","Long Rural",11,"OBR",0,229.958,0.83854005024773315,0.82695781434022775,1.2328910853356025,1.2328910853356025,228.12899999999999,0.88487767584807764,0.86673768349319213,1.2328910853356025,1.2328910853356025,-4.3189016092631477E-3,6]
[null,"OES5512","Urban",11,"OES",0,6.3040000000000003,3.5276024340258738,3.4166047018609524,5.3985425595710561,5.3985425595710561,6.8579999999999997,3.460709204551681,3.3337011767446345,5.3985425595710561,5.3985425595710561,1.9866812569266214E-13,1]
[null,"OES5522","Short Rural",11,"OES",0,11.196999999999999,4.3092286293202369,4.1736366474627964,6.4597700893685062,6.4597700893685062,11.752000000000001,1.2208613027168429,1.1760556929071349,6.4597700893685062,6.4597700893685062,1.9866812569266214E-13,3]
[null,"OES5532","Urban",11,"OES",0,8.1950000000000003,3.6407325412395313,3.5261751150401666,8.9499395354102802,8.9499395354102802,8.593,3.0516191967296766,2.9396247722096978,8.8670609042681114,8.8670609042681114,1.9866812569266214E-13,1]
[null,"OES5542","Urban",11,"OES",0,4.8380000000000001,2.1906102578644635,2.1216816370156932,10.211218933481938,10.211218933481938,4.6890000000000001,1.4238041264405525,1.3715505150001843,3.583405274763098,3.583405274763098,1.9866812569266214E-13,1]
[null,"OES5552","Urban",11,"OES",0,4.4320000000000004,4.3503668501252033,4.2134804340734204,8.6889194787096518,8.6889194787096518,4.7919999999999998,4.2724804994465195,4.1156804651168324,8.6889194787096518,8.6889194787096518,1.9866812569266214E-13,1]
[null,"OES5562","Urban",11,"OES",0,9.4749999999999996,3.7435780932519478,3.6257845815667253,6.763658403556466,6.763658403556466,9.5489999999999995,5.0874561547159427,4.9007465138378681,6.763658403556466,6.763658403556466,1.9866812569266214E-13,1]
[null,"OES5572","Short Rural",11,"OES",0,17.649000000000001,3.445325992415941,3.3369171286397061,2.8169208308896434,2.8169208308896434,18.911999999999999,3.6636520282753908,3.5291959988376842,2.7765294060571373,2.7765294060571373,1.9866812569266214E-13,3]
[null,"OES5582","Short Rural",11,"OES",0,1.944,0,0,5.7500622709671587,5.7500622709671587,1.9490000000000001,0,0,2.0357659166760795,2.0357659166760795,1.9866812569266214E-13,3]
[null,"OKY3B1","Short Rural",11,"OKY",0,78.975999999999999,0.10912680415549897,0.10367046394772401,2.7258495994276717,1.6051780859144569,79.042000000000002,0.20122151990463918,0.1931726591084536,2.7258495994276717,1.6051780859144569,-1.9129839602184017E-2,4]
[null,"OKY3B2","Short Rural",11,"OKY",0,107.06399999999999,0.30919261177391377,0.29373298118521807,2.7258495994276717,1.346063285102153,107.291,0.35869923113435676,0.34435126188898246,2.7258495994276717,1.346063285102153,-1.9129839602184017E-2,4]
[null,"OKY3B3","Short Rural",11,"OKY",0,0.67700000000000005,0,0,1.2328910853356025,1.2328910853356025,0.67900000000000005,0,0,1.2328910853356025,1.2328910853356025,-1.9129839602184017E-2,4]
[null,"OPM3B1","Short Rural",11,"OPM",0,8.2309999999999999,2.3602927668634393,2.3284043401455521,9.0880705873138989,5.6195522426168436,8.8379999999999992,2.1228883021909035,2.0804305361470856,9.0880705873138989,5.6195522426168436,1.7543718262201797E-11,3]
[null,"OPM3B2","Urban",11,"OPM",0,4.4779999999999998,2.1714693455143639,2.142131992933908,8.9547026751310952,6.4588174614243439,4.9930000000000003,2.1228883021909035,2.0804305361470856,8.9547026751310952,6.4588174614243439,1.7543718262201797E-11,1]
[null,"OPM3B3","Urban",11,"OPM",0,2.6829999999999998,1.8882342134907515,1.8627234721164418,9.0880705873138989,6.5836117221096808,2.9209999999999998,1.7562075954488383,1.7210834435398614,9.0880705873138989,6.5836117221096808,1.7543718262201797E-11,1]
[null,"OPM3B4","Urban",11,"OPM",0,7.0620000000000003,5.570290929797717,5.4950342427435039,9.0880705873138989,6.1434976119064304,7.4359999999999999,4.9019420796044502,4.803903238012361,9.0880705873138989,6.1434976119064304,1.7543718262201797E-11,1]
[null,"OPM3B5","Urban",11,"OPM",0,2.657,1.1329405280944509,1.117634083269865,6.5721801867797272,6.5721801867797272,2.9079999999999999,0.94565024370322059,0.92673723882915615,6.5721801867797272,6.5721801867797272,1.7543718262201797E-11,1]
[null,"OPM3B6","Urban",11,"OPM",0,3.5659999999999998,2.8323513202361275,2.7940852081746628,9.0880705873138989,6.3035391065257933,3.8780000000000001,3.049239561328752,2.9882547701021767,9.0880705873138989,6.3035391065257933,1.7543718262201797E-11,1]
[null,"OPM3B7","Urban",11,"OPM",0,5.2850000000000001,3.9652918483305784,3.9117192914445282,9.0880705873138989,7.108509719343429,5.7149999999999999,3.9562918359012289,3.8771659991832044,9.0880705873138989,7.108509719343429,1.7543718262201797E-11,1]
[null,"OPM3B8","Short Rural",11,"OPM",0,3.9380000000000002,1.0385288174199134,1.0244979096640432,6.6683956091401777,5.8110304593935824,4.2649999999999997,0.8684543054417333,0.8510852193328986,6.6683956091401777,5.8110304593935824,1.7543718262201797E-11,3]
[null,"ORI825","Short Rural",11,"ORI",0,6.351,1.3826843594259937,1.3755794273897768,5.1822960162460801,3.8810062445195834,6.383,1.6287108316796617,1.6094920438658415,5.1822960162460801,3.8810062445195834,2.4966189146298051E-4,3]
[null,"ORI826","Short Rural",11,"ORI",0,12.787000000000001,1.6611416262548395,1.6526058398502179,7.2399723756379064,6.9760944351047893,12.962999999999999,1.743006328639638,1.7224388539616902,7.2399723756379064,6.9760944351047893,2.4966189146298051E-4,3]
[null,"ORI827","Short Rural",11,"ORI",0,127.824,1.1042270925971476,1.0985530149293354,5.2394536928958528,4.962238961144454,127.18300000000001,2.3049591886928544,2.2777606702662787,5.2394536928958528,4.962238961144454,2.4966189146298051E-4,3]
[null,"ORI828","Short Rural",11,"ORI",0,25.26,1.142634991470092,1.1367635545790515,5.2394536928958528,5.2394536928958528,143.06800000000001,1.6668093306663205,1.6471409805644579,5.2394536928958528,5.2394536928958528,2.4966189146298051E-4,3]
[null,"ORI829","Short Rural",11,"ORI",0,14.923,2.9535674233294142,2.938390499063162,5.2394536928958528,5.2394536928958528,15.272,2.5811733063461304,2.5507154613312459,5.2394536928958528,5.2394536928958528,2.4966189146298051E-4,3]
[null,"ORI830","Short Rural",11,"ORI",0,18.073,3.0438259856808334,3.0281852672399947,5.2394536928958528,5.2394536928958528,37.661999999999999,2.5049763083728127,2.4754175879340132,5.2394536928958528,5.2394536928958528,2.4966189146298051E-4,3]
[null,"ORI831","Short Rural",11,"ORI",0,139.70099999999999,0.66445665050193581,0.6610423359400871,5.2394536928958528,3.09318293469688,16.846,0.35241111562659344,0.3482526644621996,5.2394536928958528,4.7688554884793906,2.4966189146298051E-4,3]
[null,"ORI832","Short Rural",11,"ORI",0,6.0810000000000004,1.1042270925971476,1.0985530149293354,7.2399723756379064,7.2399723756379064,4.4320000000000004,0.78101922922650435,0.77180320232163158,7.2399723756379064,7.2399723756379064,2.4966189146298051E-4,3]
[null,"ORN3B1","Short Rural",11,"ORN",0,101.586,2.7539591331528528,2.7091530167379183,8.9547026751310952,6.9408472011707616,9.9410000000000007,2.3640584430679423,2.2962099657518924,8.9547026751310952,6.9408472011707616,1.2599892872026169E-11,3]
[null,"ORN3B3","Urban",11,"ORN",0,2.165,2.6660668203926559,2.6226906864164961,8.9547026751310952,8.2383264611206091,2.23,1.806594880073755,1.7547456070156384,8.9547026751310952,8.2383264611206091,1.2599892872026169E-11,1]
[null,"ORN3B4","Urban",11,"ORN",0,1.825,3.2324839470694835,3.1798923707101103,5.1822960162460801,5.1822960162460801,1.768,3.5409259649445599,3.4393013897506512,5.1822960162460801,5.1822960162460801,1.2599892872026169E-11,1]
[null,"ORN3B5","Urban",11,"ORN",0,4.2489999999999997,2.0898838811869171,2.0558820765316126,4.3820885431492593,4.3820885431492593,4.5759999999999996,1.5898034944649044,1.5441761341737616,5.1822960162460801,5.1822960162460801,1.2599892872026169E-11,1]
[null,"ORN3B6","Urban",11,"ORN",0,6.1269999999999998,1.9043334431376111,1.8733504902974969,7.2399723756379064,7.2399723756379064,78.524000000000001,3.1383133916709802,3.0482437973300232,7.2399723756379064,7.2399723756379064,1.2599892872026169E-11,1]
[null,"ORN3B7","Urban",11,"ORN",0,2.4060000000000001,1.9922257558978087,1.95981282061892,6.9732365512722998,6.9732365512722998,2.496,2.2092074533473349,2.1458031994362665,6.9732365512722998,6.9732365512722998,1.2599892872026169E-11,1]
[null,"ORN3B8","Urban",11,"ORN",0,4.0510000000000002,4.1016412621425475,4.0349087483330708,9.0499654695473861,9.0499654695473861,4.399,1.5381864978913684,1.4940405454018861,5.1822960162460801,5.1822960162460801,1.2599892872026169E-11,1]
[null,"ORN3B9","Urban",11,"ORN",0,2.9169999999999998,2.1875420064760256,2.1519513324443049,8.9547026751310952,8.9547026751310952,3.246,2.4156754396414781,2.3463455545237677,8.9547026751310952,8.9547026751310952,1.2599892872026169E-11,1]
[null,"ORS3B2","Short Rural",11,"ORS",0,150.1,2.60292666086765,2.537814278058685,5.2394536928958528,5.2394536928958528,150.309,3.1034463884806724,3.0249291948521115,5.2394536928958528,5.2394536928958528,-3.2497853095867148E-2,4]
[null,"ORS3B4","Urban",11,"ORS",0,6.68,3.2312193031460485,3.150390138279747,7.9449170543184398,7.9449170543184398,7.2329999999999997,3.6470436858260133,3.5547734805746152,7.9449170543184398,7.9449170543184398,-3.2497853095867148E-2,2]
[null,"ORS3B5","Urban",11,"ORS",0,8.61,2.6926827526217068,2.6253251152331223,8.4736255633288398,8.4736255633288398,9.2710000000000008,2.7278700739511641,2.6588549610801997,8.4736255633288398,8.4736255633288398,-3.2497853095867148E-2,2]
[null,"ORS3B6","Short Rural",11,"ORS",0,174.09100000000001,3.7697558536703899,3.6754551613263713,5.1822960162460801,5.1822960162460801,197.809,4.5464501232519403,4.4314249351336663,5.1822960162460801,5.1822960162460801,-3.2497853095867148E-2,4]
[null,"ORS3B7","Short Rural",11,"ORS",0,50.405000000000001,4.1287802206866173,4.0254985100241205,7.9449170543184398,7.9449170543184398,50.555999999999997,4.3290112043138045,4.2194872208446652,7.9449170543184398,6.9046473392925725,-3.2497853095867148E-2,4]
[null,"ORS3B8","Urban",11,"ORS",0,4.8,1.795121835081138,1.7502167434887483,5.2394536928958528,5.2394536928958528,5.0030000000000001,1.6900934153827865,1.6473340519736019,5.2394536928958528,5.2394536928958528,-3.2497853095867148E-2,2]
[null,"ORS3B9","Urban",11,"ORS",0,2.589,1.6156096515730243,1.5751950691398735,5.2394536928958528,5.2394536928958528,2.77,1.9767174448921481,1.9267064935363767,5.2394536928958528,5.2394536928958528,-3.2497853095867148E-2,2]
[null,"ORW3B1","Short Rural",11,"ORW",0,119.33799999999999,2.774389658494155,2.752830820998549,7.2399723756379064,6.1034872382515886,116.129,1.7690720577479135,1.7460741209971906,7.2399723756379064,6.1034872382515886,1.6250434370809636E-9,3]
[null,"ORW3B2","Short Rural",11,"ORW",0,9.2799999999999994,2.8725981419806734,2.8502761597949577,4.1534578365501673,4.1534578365501673,11.083,3.0882067135252593,3.0480600262494311,4.1534578365501673,4.1534578365501673,1.6250434370809636E-9,3]
[null,"ORW3B3","Short Rural",11,"ORW",0,2.8809999999999998,2.0132739114736342,1.9976294453263805,4.1534578365501673,4.1534578365501673,3.0870000000000002,0.77716460340370763,0.76706146355945948,4.1534578365501673,4.1534578365501673,1.6250434370809636E-9,3]
[null,"ORW3B4","Urban",11,"ORW",0,3.0579999999999998,0.86128840017676944,0.85459562124450528,7.2399723756379064,7.2399723756379064,3.1509999999999998,0.82829385362763586,0.81752603353047659,7.2399723756379064,7.2399723756379064,1.6250434370809636E-9,1]
[null,"ORW3B5","Short Rural",11,"ORW",0,2.1030000000000002,0.38203100076255797,0.37906236791803033,4.1534578365501673,4.1534578365501673,2.258,0.44993740197056759,0.44408821574495022,4.1534578365501673,4.1534578365501673,1.6250434370809636E-9,3]
[null,"ORW3B6","Short Rural",11,"ORW",0,13.784000000000001,3.8301308559742311,3.8003682130599437,4.1534578365501673,4.1534578365501673,14.957000000000001,4.0903400179142508,4.0371655976813656,4.1534578365501673,4.1534578365501673,1.6250434370809636E-9,3]
[null,"ORW3B7","Short Rural",11,"ORW",0,144.113,2.3962869970710576,2.3776662666323753,4.1534578365501673,4.1534578365501673,143.47399999999999,2.4337523106589791,2.4021135306204124,4.1534578365501673,4.1534578365501673,1.6250434370809636E-9,3]
[null,"ORW3B8","Short Rural",11,"ORW",0,110.239,1.335635375416655,1.3252566076311598,7.2399723756379064,5.7691148298504169,109.182,1.2373278554190608,1.2212425932986131,7.2399723756379064,5.7691148298504169,1.6250434370809636E-9,3]
[null,"OUR2557","Short Rural",11,"OUR_11",0,140.465,0.67861247251778167,0.63153861813749068,2.4440622535442911,2.4225328620062099,139.518,0.65912709766864075,0.60870387469698972,2.4440622535442911,2.4177697222853958,-1.2248298410292157E-2,4]
[null,"OUR2580","Short Rural",11,"OUR_11",0,5.2160000000000002,1.3285511785911501,1.2363925059311438,1.3504453736453019,1.3504453736453019,6.5220000000000002,0.84744912557396679,0.78261926746755828,1.3504453736453019,1.3504453736453019,-1.2248298410292157E-2,4]
[null,"OXY3B1","Short Rural",11,"OXY",0,14.141999999999999,0.92526261887448891,0.92519918280609847,7.2399723756379064,7.2399723756379064,14.518000000000001,1.8145017871412801,1.7963567692698672,7.2399723756379064,7.2399723756379064,1.9979836522744966E-2,3]
[null,"OXY3B2","Urban",11,"OXY",0,5.3849999999999998,3.3699038540060333,3.3696728131674747,7.2399723756379064,7.2399723756379064,4.1189999999999998,2.3847737773856825,2.3609260396118259,7.2399723756379064,7.2399723756379064,1.9979836522744966E-2,1]
[null,"OXY3B3","Short Rural",11,"OXY",0,16.596,4.226989227279244,4.2266994246089133,5.6205048705610059,5.6205048705610059,14.523999999999999,3.2142603086502675,3.1821177055637646,5.6205048705610059,5.6205048705610059,1.9979836522744966E-2,3]
[null,"OXY3B5","Urban",11,"OXY",0,7.0529999999999999,2.7855274631379348,2.7853364871846753,6.1920816370587364,6.1920816370587364,7.7869999999999999,2.8513599512220114,2.8228463517097913,6.1920816370587364,6.1920816370587364,1.9979836522744966E-2,1]
[null,"OXY3B6","Short Rural",11,"OXY",0,34.860999999999997,2.5615165133051638,2.5613408955579358,5.6205048705610059,5.6205048705610059,35.39,2.3502118385829913,2.3267097201971616,5.6205048705610059,5.6205048705610059,1.9979836522744966E-2,3]
[null,"OXY3B8","Urban",11,"OXY",0,8.0760000000000005,4.0906347360766881,4.0903542818795939,7.2399723756379064,7.2399723756379064,8.4489999999999998,3.6635655130852514,3.6269298579543987,7.2399723756379064,7.2399723756379064,1.9979836522744966E-2,1]
[null,"OXY3B9","Short Rural",11,"OXY",0,52.692999999999998,4.0906347360766881,4.0903542818795939,9.0499654695473861,7.9887379397499325,50.404000000000003,2.9032028594260484,2.8741708308317877,9.0499654695473861,7.9887379397499325,1.9979836522744966E-2,3]
[null,"PAM3B1","Long Rural",11,"PAM",0,353.55799999999999,2.9942615420627878,2.9913086205095158,2.7765294060571373,2.7765294060571373,352.53800000000001,2.8822649272111098,2.8808237947475046,2.7765294060571373,1.9595556811430495,-5.3212919205567694E-3,6]
[null,"PAM3B2","Short Rural",11,"PAM",0,17.085000000000001,2.801083378058737,2.7983209675734182,2.4440622535442911,2.4440622535442911,18.135999999999999,2.8635999532448482,2.8621681532682257,2.4440622535442911,2.3634699294681116,-5.3212919205567694E-3,4]
[null,"PAM3B3","Short Rural",11,"PAM",0,19.274999999999999,4.1533305260870925,4.1492345381261027,2.4440622535442911,2.4440622535442911,20.361999999999998,3.9864454923731025,3.984452269626916,2.4440622535442911,2.4440622535442911,-5.3212919205567694E-3,4]
[null,"PAM3B4","Short Rural",11,"PAM",0,21.972000000000001,3.477206952072915,3.4737777528497604,3.583405274763098,3.583405274763098,22.693999999999999,3.1818868777221487,3.1802959342832877,3.583405274763098,3.583405274763098,-5.3212919205567694E-3,4]
[null,"PAM3B5","Short Rural",11,"PAM",0,34.515000000000001,3.6703851160769658,3.6667654057858585,3.5163402674940318,3.5163402674940318,35.11,3.574833698064495,3.5730462812154631,3.5163402674940318,1.5232520827164493,-5.3212919205567694E-3,4]
[null,"PCR12","Short Rural",11,"PCR",0,17.786000000000001,1.6352606720356471E-2,1.632141265624067E-2,0.42277628161948722,0.42277628161948722,17.797999999999998,1.4357283607934479E-2,1.4357283607934479E-2,0.42277628161948722,0.42277628161948722,-2.5196439408119862E-2,4]
[null,"PCR22","Short Rural",11,"PCR",0,21.716999999999999,2.4528910080534705E-2,2.4482118984361007E-2,2.7258495994276717,0.22577282276660318,21.733000000000001,5.7429134431737916E-2,5.7429134431737916E-2,2.7258495994276717,0.22577282276660318,-2.5196439408119862E-2,4]
[null,"PCR32","Short Rural",11,"PCR",0,52.948999999999998,7.3586730241604115E-2,7.344635695308302E-2,0.29702939298998676,0.29702939298998676,53.46,0.10911535542030204,0.10911535542030204,0.29702939298998676,0.29702939298998676,-2.5196439408119862E-2,4]
[null,"PER3B1","Short Rural",11,"PER",0,16.786000000000001,3.047000928091371,2.8946508816868022,3.2389350101538001,3.2389350101538001,16.792999999999999,2.9150582912545162,2.8567571254294259,3.2389350101538001,3.2389350101538001,-2.0753612962449455E-2,4]
[null,"PER3B2","Urban",11,"PER",0,0.88800000000000001,1.3760649352670706,1.3072616885037169,2.4768326548234945,2.4768326548234945,0.88800000000000001,1.3043172299043375,1.2782308853062507,2.4768326548234945,2.4768326548234945,-2.0753612962449455E-2,2]
[null,"PER3B3","Urban",11,"PER",0,1.5049999999999999,4.0299044532821355,3.8284092306180284,6.763658403556466,5.8167462270585606,1.5049999999999999,3.9895576475744732,3.9097664946229838,6.763658403556466,5.8167462270585606,-2.0753612962449455E-2,2]
[null,"PER3B4","Urban",11,"PER",0,1.101,0.72734860864116602,0.69098117820910765,6.763658403556466,5.9986981643936712,1.101,0.59369617342631742,0.58182224995779108,6.763658403556466,5.9986981643936712,-2.0753612962449455E-2,2]
[null,"PER3B5","Short Rural",11,"PER",0,21.454000000000001,2.4277717072211895,2.3063831218601298,3.791459217768272,3.567591650889995,21.43,2.5310205288174585,2.4804001182411093,3.791459217768272,3.567591650889995,-2.0753612962449455E-2,4]
[null,"PER3B6","Short Rural",11,"PER",0,8.2949999999999999,0.72734860864116602,0.69098117820910765,2.934094068021678,2.934094068021678,8.2870000000000008,0.7096130833482639,0.6954208216812986,2.934094068021678,2.934094068021678,-2.0753612962449455E-2,4]
[null,"PHS3B1","Urban",11,"PHS",0,6.8380000000000001,3.6867902992869532,3.3976723407200669,9.011860351780868,9.011860351780868,7.3390000000000004,2.8078443280204572,2.5551383384986162,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PHS3B2","Urban",11,"PHS",0,8.6959999999999997,5.3433207351309546,4.9242977212079877,7.2399723756379064,7.2399723756379064,8.4830000000000005,4.7099324211956057,4.2860385032880011,7.2399723756379064,7.2399723756379064,-2.5296058438408268E-8,2]
[null,"PHS3B3","Urban",11,"PHS",0,9.1639999999999997,2.7171139465977818,2.5040379716539669,9.011860351780868,9.011860351780868,9.6329999999999991,3.4418736924121736,3.1321050600950779,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PHS3B4","Urban",11,"PHS",0,4.4630000000000001,3.5958831412223438,3.3138941186201203,9.011860351780868,9.011860351780868,4.3259999999999996,3.4418736924121736,3.1321050600950779,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PHS3B5","Urban",11,"PHS",0,3.1120000000000001,2.1413686121885869,1.9734425650209706,9.011860351780868,9.011860351780868,4.1920000000000002,2.1738149636287409,1.9781716169021544,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PHS3B6","Urban",11,"PHS",0,3.177,3.3433632577095387,3.0811768350091566,9.011860351780868,9.011860351780868,2.8029999999999999,3.4418736924121736,3.1321050600950779,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PHS3B7","Short Rural",11,"PHS",0,21.832999999999998,1.9393527053783426,1.7872687381321997,9.0880705873138989,9.0880705873138989,22.637,1.6303612227215558,1.4836287126766159,9.0880705873138989,9.0880705873138989,-2.5296058438408268E-8,4]
[null,"PHS3B8","Urban",11,"PHS",0,8.3940000000000001,3.8888062060971973,3.5838461676088378,9.011860351780868,9.011860351780868,9.2910000000000004,2.9889955749895187,2.7199859732404623,9.011860351780868,9.011860351780868,-2.5296058438408268E-8,2]
[null,"PIN2J01","Short Rural",22,"PIN",0,16.184999999999999,0.04,3.9199999999999999E-2,0.84555256323897443,0.33723029223366036,16.184999999999999,0.114,0.11172,0.84555256323897443,0.33723029223366036,0,3]
[null,"PKH22","Short Rural",11,"PKH",0,28.326000000000001,0.23210858352455002,0.22438711750084697,2.7765294060571373,2.4006224192904639,28.393000000000001,0.19054644022768771,0.17530272500947269,2.7765294060571373,2.4006224192904639,-4.3182282173932504E-3,4]
[null,"PKH32","Short Rural",11,"PKH",0,14.427,1.151258574281768,1.1129601028042009,2.7765294060571373,2.320601671980782,14.571,1.0630485612702578,0.97800467636863719,2.7765294060571373,2.2558229717777056,-4.3182282173932504E-3,4]
[null,"PKH42","Short Rural",11,"PKH",0,172.24100000000001,0.25067727020651404,0.24233808690091474,2.7765294060571373,2.3120280204833161,172.39699999999999,0.23066148027562197,0.21220856185357223,2.7765294060571373,2.3120280204833161,-4.3182282173932504E-3,4]
[null,"PKH52","Long Rural",11,"PKH",0,215.48500000000001,0.529207570435974,0.51160262790193101,2.0738710344425955,0.69160788746225277,215.31700000000001,0.51146676061116181,0.47054941976226888,2.0738710344425955,0.69160788746225277,-4.3182282173932504E-3,6]
[null,"PKT3B10","Long Rural",11,"PKT",0,285.53699999999998,4.3720643831307004,4.1854908659949741,8.9547026751310952,5.9424931156880625,285.16500000000002,3.4277160503908419,3.1534987663595748,8.9547026751310952,5.9424931156880625,9.1923232411651441E-4,5]
[null,"PKT3B2","Short Rural",11,"PKT",0,28.077999999999999,5.7282139834536485,5.4837681253545254,8.9547026751310952,4.5907140629209309,27.931000000000001,5.3725194832367107,4.9427179245777744,8.9547026751310952,4.5907140629209309,9.1923232411651441E-4,3]
[null,"PKT3B3","Short Rural",11,"PKT",0,148.91200000000001,0.89060570767477221,0.85259999122119834,8.9547026751310952,2.6406846612195101,156.45500000000001,0.75944574052631142,0.69869008128420651,8.9547026751310952,2.6406846612195101,9.1923232411651441E-4,3]
[null,"PKT3B4","Long Rural",11,"PKT",0,304.18200000000002,0.89060570767477221,0.85259999122119834,8.9547026751310952,6.4959699512466971,302.32299999999998,0.79639700575038286,0.73268524529035228,8.9547026751310952,6.4959699512466971,9.1923232411651441E-4,5]
[null,"PKT3B7","Short Rural",11,"PKT",0,4.726,0.13156675227013681,0.1259522714304043,8.9547026751310952,7.9487275660950925,5.218,0.40840872089763225,0.37573602322582167,8.9547026751310952,7.9487275660950925,9.1923232411651441E-4,3]
[null,"PKT3B8","Urban",11,"PKT",0,8.1229999999999993,6.1127937208586633,5.8519363033818603,8.9547026751310952,7.8277438171864056,8.3680000000000003,5.2986169527885671,4.8747275965654824,8.9547026751310952,7.8277438171864056,9.1923232411651441E-4,1]
[null,"PKT3B9","Short Rural",11,"PKT",0,41.893000000000001,6.1127937208586633,5.8519363033818603,8.9547026751310952,5.6243153823376577,43.040999999999997,4.6315493753224342,4.2610254252966397,8.9547026751310952,5.6243153823376577,9.1923232411651441E-4,3]
[null,"PPM3B1","Short Rural",11,"PPM",0,27.059000000000001,2.15,2.0938809295423728,6.763658403556466,1.5994623182494798,27.492000000000001,2.0005186827420531,1.960508309087212,6.763658403556466,1.5994623182494798,5.5042574708635732E-3,3]
[null,"PPM3B2","Short Rural",11,"PPM",0,98.001999999999995,1,0.97389810676389443,6.763658403556466,1.8042773262444993,67.673000000000002,0.80020747309682139,0.78420332363488499,6.763658403556466,1.8042773262444993,5.5042574708635732E-3,3]
[null,"PPM3B3","Short Rural",11,"PPM",0,10.866,1.52,1.4803251222811196,6.763658403556466,2.3872856280721839,11.259,1.2193637685284895,1.1949764931579197,6.763658403556466,2.3872856280721839,5.5042574708635732E-3,3]
[null,"PPM3B4","Short Rural",11,"PPM",0,36.905999999999999,0.61,0.59407784512597561,6.1920816370587364,1.6489989713459499,36.975999999999999,0.4953665309646989,0.48545920034540491,6.1920816370587364,1.6489989713459499,5.5042574708635732E-3,3]
[null,"PPTW150","Short Rural",11,"PPT",0,1.1180000000000001,0.12,0.1190995991843497,0.72247303285313003,0.72247303285313003,1.1200000000000001,0.124,0.11779999999999999,0.72247303285313003,0.72247303285313003,-3.0020555589904537E-9,4]
[null,"PPTW190","Short Rural",11,"PPT",0,17.510999999999999,0.13,0.12902456578304553,0.72247303285313003,0.45821404114234648,17.515000000000001,0.114,0.10829999999999999,0.72247303285313003,0.45821404114234648,-3.0020555589904537E-9,4]
[null,"PSK3B1","Short Rural",11,"PSK",0,12.067,1.3334312482378581,1.2068379411720316,6.9732365512722998,6.342596852236472,142.131,1.6684013285001376,1.6183492886451334,6.9732365512722998,6.3454547360689606,4.0255566019314931E-2,3]
[null,"PSK3B2","Short Rural",11,"PSK",0,111.065,2.2115445092725454,2.0015848780414185,6.9732365512722998,6.9284630378966447,111.36199999999999,1.2804010195466173,1.2419889889602187,6.9732365512722998,6.9284630378966447,4.0255566019314931E-2,3]
[null,"PSK3B3","Short Rural",11,"PSK",0,26.785,1.1057722546362727,1.0007924390207092,6.9732365512722998,4.2544363986314337,27.106000000000002,1.3580010813373213,1.3172610488972016,6.9732365512722998,4.255389026575596,4.0255566019314931E-2,3]
[null,"PSK3B4","Short Rural",11,"PSK",0,4.734,1.4960448150961334,1.3540132998515475,6.9732365512722998,6.9732365512722998,4.9870000000000001,1.2416009886512651,1.2043529589917272,6.9732365512722998,6.9732365512722998,4.0255566019314931E-2,3]
[null,"PSK3B5","Urban",11,"PSK",0,4.2869999999999999,2.6560215920184982,2.4038641917654289,6.9732365512722998,6.5969485133279617,4.4610000000000003,1.8818014984245737,1.8253474534718364,6.9732365512722998,6.5969485133279617,4.0255566019314931E-2,1]
[null,"PSK3B6","Urban",11,"PSK",0,4.6589999999999998,2.3091126493875103,2.0898900932491276,6.9732365512722998,6.9732365512722998,4.8639999999999999,2.134001699244362,2.069981648267031,6.9732365512722998,6.9732365512722998,4.0255566019314931E-2,1]
[null,"PSK3B8","Short Rural",11,"PSK",0,130.82300000000001,1.5285675284677884,1.3834483715874506,6.9732365512722998,6.9732365512722998,0,"","","","",4.0255566019314931E-2,3]
[null,"PYB3B1","Short Rural",11,"PYB",0,169.20099999999999,1.4450952771832561,1.3738765694216291,2.7730999454581511,2.7730999454581511,169.91300000000001,1.4328209967877632,1.2895388971089869,2.7765294060571373,2.2539177158893802,2.039004751061611E-2,3]
[null,"PYB3B2","Short Rural",11,"PYB",0,105.34699999999999,2.6620176158638924,2.5308252594608951,2.7765294060571373,2.7765294060571373,105.65900000000001,1.4328209967877632,1.2895388971089869,2.7765294060571373,2.3387016029198762,2.039004751061611E-2,3]
[null,"PYB3B3","Long Rural",11,"PYB",0,202.09700000000001,0.22817293850261935,0.21692787938236247,2.6816476628185142,2.6816476628185142,199.38900000000001,1.0691048976031772,0.96219440784285948,2.7765294060571373,2.3177437881482934,2.039004751061611E-2,5]
[null,"QDI3B1","Short Rural",11,"QDI_11",0,163.01300000000001,1.654102842176024,1.6468666790629725,2.0357659166760795,2.0357659166760795,163.512,1.6770713944060578,1.6603006804619973,2.0357659166760795,2.0357659166760795,5.6623387826411054E-11,3]
[null,"QDI3B2","Short Rural",11,"QDI_11",0,52.779000000000003,1.4734824168809408,1.4670364095101189,0.72247303285313003,0.72247303285313003,53.152999999999999,1.2886969662278129,1.2758099965655347,0.72247303285313003,0.72247303285313003,5.6623387826411054E-11,3]
[null,"QDI3B3","Short Rural",11,"QDI_11",0,8.984,2.2530021471018258,2.2431459938961176,3.583405274763098,3.583405274763098,9.9250000000000007,2.1959526907129416,2.1739931638058123,3.583405274763098,3.583405274763098,5.6623387826411054E-11,3]
[null,"QDI3B4","Long Rural",11,"QDI_11",0,213.11600000000001,2.2244831325815495,2.2147517408088251,2.7765294060571373,2.7765294060571373,213.785,2.5758432405831129,2.5500848081772816,2.7765294060571373,2.7765294060571373,5.6623387826411054E-11,5]
[null,"QSH5232","Short Rural",11,"QSH",0,16.928000000000001,1.5127371700614243,1.5036461806580723,5.0489281040632772,5.0489281040632772,2.464,4.5033596579116839,4.4781408438273784,5.6709941516016409,5.6709941516016409,2.0412761671834527E-3,3]
[null,"QSH5242","Short Rural",11,"QSH",0,10.086,2.5483022126538084,2.5329878613770211,6.736984821119905,6.736984821119905,10.547000000000001,2.5498474775390356,2.535568331664817,6.736984821119905,6.736984821119905,2.0412761671834527E-3,3]
[null,"QSH5252","Short Rural",11,"QSH",0,105.935,2.6498281972216895,2.6339037124278986,4.2029944896466374,4.2029944896466374,178.506,2.9405499136135651,2.9240828340973288,4.2249049323623842,4.2249049323623842,2.0412761671834527E-3,3]
[null,"QSH5262","Urban",11,"QSH",0,6.649,3.5229516645054648,3.5017800314654441,9.5481898843445716,9.5481898843445716,7.0709999999999997,3.8967427176907039,3.8749209584716358,8.8984976264254847,8.8984976264254847,2.0412761671834527E-3,1]
[null,"QSH5272","Short Rural",11,"QSH",0,15.333,5.1067570237644055,5.0760673078591303,7.2066303975922059,7.2066303975922059,18.138000000000002,5.9119447563909091,5.8788378657551199,7.3333299141658701,7.3333299141658701,2.0412761671834527E-3,3]
[null,"QSH5282","Urban",11,"QSH",0,8.5570000000000004,4.0204289888880806,3.9962677016147428,8.4945833781004243,8.4945833781004243,9.1470000000000002,4.153783794055526,4.1305226048088146,7.8563226555112928,7.8563226555112928,2.0412761671834527E-3,1]
[null,"QSH5292","Urban",11,"QSH",0,4.8929999999999998,1.6244157530860932,1.6146536168140375,9.6815577965273754,9.6815577965273754,5.1150000000000002,1.8198508206629409,1.8096596560672285,9.5300899534054775,9.5300899534054775,2.0412761671834527E-3,1]
[null,"QSH5312","Short Rural",11,"QSH",0,13.393000000000001,3.5432568614190409,3.5219632016756193,8.1964108315774418,8.1964108315774418,13.567,3.4649137093978029,3.445510192625175,7.4790819896227907,7.4790819896227907,2.0412761671834527E-3,3]
[null,"QUI3B1","Short Rural",11,"QUI",0,96.695999999999998,0.93,0.8590885502893183,3.5163402674940318,2.5940058919555291,90.39,0.97099999999999997,0.90050540000000001,3.5163402674940318,2.6768845230977001,3.3534320727600056E-2,3]
[null,"QUI3B2","Short Rural",11,"QUI",0,111.86799999999999,0.36,0.33255040656360702,1.3917894264219712,0.76972337888360909,111.262,0.47600000000000003,0.44144240000000001,2.1298855575593727,0.76972337888360909,3.3534320727600056E-2,3]
[null,"QUI3B3","Short Rural",11,"QUI",0,65.858999999999995,0.8,0.73900090347468239,2.0357659166760795,1.5794571314220593,65.516999999999996,0.68500000000000005,0.63526900000000008,2.0357659166760795,1.5794571314220593,3.3534320727600056E-2,3]
[null,"RAG3B10","Short Rural",11,"RAG",0,6.37,0.95,0.94995000983547007,5.2394536928958528,5.2394536928958528,6.6120000000000001,0.9526,0.94040671999999992,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,4]
[null,"RAG3B11","Short Rural",11,"RAG",0,22.792999999999999,5.05,5.0497342628096042,5.2394536928958528,5.2394536928958528,20.721,3.62,3.573664,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,4]
[null,"RAG3B12","Urban",11,"RAG",0,7.3999999999999996E-2,2.87,2.8698489770818938,8.9547026751310952,8.9547026751310952,7.0999999999999994E-2,1.905,1.8806160000000001,8.9547026751310952,8.9547026751310952,-2.3248865373625558E-2,2]
[null,"RAG3B2","Urban",11,"RAG",0,7.5839999999999996,3.81,3.8097995131296223,8.9547026751310952,2.4911220739859377,7.798,2.86,2.8233919999999997,8.9547026751310952,2.4911220739859377,-2.3248865373625558E-2,2]
[null,"RAG3B3","Short Rural",11,"RAG",0,148.10400000000001,1.1399999999999999,1.139940011802564,5.2394536928958528,4.1305947658902591,102.092,1.33368,1.316608896,5.2394536928958528,4.1305947658902591,-2.3248865373625558E-2,4]
[null,"RAG3B4","Urban",11,"RAG",0,0.224,0.99,0.98994790498643725,5.2394536928958528,5.2394536928958528,0.222,4.57,4.5115040000000004,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,2]
[null,"RAG3B5","Long Rural",11,"RAG",0,253.61699999999999,1.68,1.6799115963406208,5.2394536928958528,5.2394536928958528,250.31100000000001,2.6669999999999998,2.6328623999999996,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,6]
[null,"RAG3B6","Long Rural",11,"RAG",0,279.39,3.01,3.009841610110279,5.2394536928958528,5.2394536928958528,278.93200000000002,2.286,2.2567392000000002,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,6]
[null,"RAG3B7","Short Rural",11,"RAG",0,18.234999999999999,4.91,4.9097416297812195,5.2394536928958528,5.2394536928958528,19.135999999999999,4.9569999999999999,4.8935503999999996,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,4]
[null,"RAG3B8","Short Rural",11,"RAG",0,3.254,0.84,0.83995579817031041,5.2394536928958528,5.2394536928958528,3.4649999999999999,0.76200000000000001,0.75224639999999998,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,4]
[null,"RAG3B9","Urban",11,"RAG",0,3.6789999999999998,2.29,2.28987949739287,5.2394536928958528,5.2394536928958528,3.6920000000000002,1.524,1.5044928,5.2394536928958528,5.2394536928958528,-2.3248865373625558E-2,2]
[null,"RBV","Long Rural",22,"Robinvale",0,208.53100000000001,5.1070347700939802,4.7554397703513311,5.7172918696879558,4.7021715323879878,208.679,4.7487086513097445,4.4529743879235344,4.9441390302053598,4.9441390302053598,2.3480038149497586E-2,5]
[null,"RCF10","Short Rural",11,"RCF",0,15.791,0.48,0.45599999999999996,1.3504453736453019,0.52966113695456274,15.821,0.88,0.83599999999999997,1.3504453736453019,0.52966113695456274,3.1599756578547238E-2,3]
[null,"RGL3B11","Short Rural",11,"RGL",0,30.106000000000002,1.6873207357425863,1.6660073508494881,9.0880705873138989,4.4154305211949607,30.228000000000002,1.5895298094638801,1.5577392132746024,9.0880705873138989,4.4154305211949607,1.9347771717373695E-2,3]
[null,"RGL3B5","Short Rural",11,"RGL",0,15.462,2.2432587816230916,2.2149230676033653,5.715767664977295,4.2410996074131537,15.736000000000001,2.1924549096053516,2.1486058114132445,5.715767664977295,4.2410996074131537,1.9347771717373695E-2,3]
[null,"RGL3B6","Short Rural",11,"RGL",0,33.834000000000003,3.3258749762324968,3.2838642002293379,5.715767664977295,3.8600484297480002,33.286000000000001,2.3751594854057978,2.3276562956976816,5.715767664977295,3.8600484297480002,1.9347771717373695E-2,3]
[null,"RGL3B7","Short Rural",11,"RGL",0,163.29900000000001,2.7504303322509212,2.715688282887605,5.715767664977295,3.8724325930221171,171.43600000000001,3.1059777886075817,3.0438582328354298,5.715767664977295,3.8724325930221171,1.9347771717373695E-2,3]
[null,"RGL3B8","Short Rural",11,"RGL",0,120.664,1.4825014556813476,1.4637752446770069,5.715767664977295,2.3177437881482934,121.733,1.3337434033432556,1.3070685352763904,5.715767664977295,2.3177437881482934,1.9347771717373695E-2,3]
[null,"RKF3B1","Short Rural",11,"RKF",0,17.420000000000002,3.2003898980133778,3.0685605779607257,6.9732365512722998,5.0679806629465345,15.295,1.3463138996978596,1.2722666352144774,5.6205048705610059,4.645013855738215,1.5572092111692105E-6,3]
[null,"RKF3B2","Short Rural",11,"RKF",0,15.273,2.2402729286093646,2.1479924045725078,5.6205048705610059,4.645013855738215,18.57,1.9689840783081198,1.8606899540011732,6.9732365512722998,5.0679806629465345,1.5572092111692105E-6,3]
[null,"RKF3B3","Short Rural",11,"RKF",0,94.016999999999996,1.1734762959382388,1.1251388785855996,5.6205048705610059,3.6942911674636583,93.971999999999994,0.75730156858004627,0.7156499823081437,5.6205048705610059,3.6942911674636583,1.5572092111692105E-6,3]
[null,"RKF3B4","Short Rural",11,"RKF",0,12.433999999999999,3.8404678776160539,3.6822726935528713,6.9732365512722998,4.2010892337583119,12.946,2.4401939432023712,2.3059832763262404,6.9732365512722998,4.2010892337583119,1.5572092111692105E-6,3]
[null,"RKF3B5","Short Rural",11,"RKF",0,78.778999999999996,2.6669915816778151,2.5571338149672718,5.6205048705610059,4.3239782385553234,77.950999999999993,1.5482609846525388,1.4631066304966491,5.6205048705610059,4.3239782385553234,1.5572092111692105E-6,3]
[null,"RVL3K1","Long Rural",11,"RVL",0,228.55,0.98500917715586478,0.9487118184414538,2.7258495994276717,2.6654529877677451,228.25700000000001,0.93010908400249659,0.88360362980237173,2.7258495994276717,2.6654529877677451,5.3552375921995223E-2,5]
[null,"RWR2447","Short Rural",11,"RWR",0,24.667999999999999,1.8385912496038712,1.4825339414522802,6.763658403556466,2.0919709653816905,24.667999999999999,1.9006230714349974,1.5969035046196847,6.763658403556466,2.0919709653816905,-1.065265948046383E-5,4]
[null,"RWR2448","Short Rural",11,"RWR",0,11.09,0.65874659745165443,0.53117526244546942,6.763658403556466,2.4444433047219567,11.084,0.57018692143049921,0.47907105138590539,2.4444433047219567,2.4444433047219567,-1.065265948046383E-5,4]
[null,"SFP3B1","Short Rural",11,"SFP",0,17.774999999999999,3.9006215470498105,3.8903465959204082,7.2399723756379064,6.5464592322873285,0,"","","","",-1.43789441120124E-6,4]
[null,"SFP3B3","Short Rural",11,"SFP",0,45.715000000000003,2.1413205915505404,2.1356799611624924,9.0880705873138989,6.2482866857643478,46.072000000000003,1.8133671562154439,1.7770998130911349,9.0880705873138989,6.1206345412465195,-1.43789441120124E-6,4]
[null,"SFP3B4","Short Rural",11,"SFP",0,87.658000000000001,3.1566885715815478,3.1483732760799183,9.0880705873138989,5.1413330146470768,87.379000000000005,3.7932680308588367,3.7174026702416598,9.0880705873138989,4.7736186282002047,-1.43789441120124E-6,4]
[null,"SFP3B5","Short Rural",11,"SFP",0,10.076000000000001,2.241852074721927,2.2359466260058016,7.2399723756379064,7.2399723756379064,11.356,2.0724196071033649,2.0309712149612977,7.2399723756379064,7.2399723756379064,-1.43789441120124E-6,4]
[null,"SGN3B1","Long Rural",11,"SGN",0,248.446,3.1551846807885369,3.0103571419021886,5.6205048705610059,5.6205048705610059,245.99799999999999,2.9503258419205136,2.861816066662898,5.6205048705610059,5.6205048705610059,1.6300013487306384E-3,5]
[null,"SGN3B2","Short Rural",11,"SGN",0,64.304000000000002,1.923893098041791,1.8355836231110907,5.6205048705610059,5.6205048705610059,64.596000000000004,1.8451549239372593,1.7898002762191414,5.6205048705610059,5.6205048705610059,1.6300013487306384E-3,3]
[null,"SGN3B3","Short Rural",11,"SGN",0,123.93600000000001,1.904654167061373,1.8172277868799798,5.6205048705610059,3.3627766428949748,124.22499999999999,1.4126967386394642,1.3703158364802803,5.6205048705610059,3.3627766428949748,1.6300013487306384E-3,3]
[null,"SGN3B4","Long Rural",11,"SGN",0,204.453,2.1643797352970147,2.0650315759999769,5.6205048705610059,5.6205048705610059,206.46299999999999,1.4799680119080103,1.43556897155077,5.6205048705610059,5.6205048705610059,1.6300013487306384E-3,5]
[null,"SGN3B5","Urban",11,"SGN",0,4.8310000000000004,3.4052907835339701,3.2489830129066304,5.6205048705610059,5.6205048705610059,4.9279999999999999,3.2194109349946975,3.1228286069448568,5.6205048705610059,5.6205048705610059,1.6300013487306384E-3,1]
[null,"SGN3B6","Short Rural",11,"SGN",0,81.186000000000007,4.3095205396136125,4.111707315768844,5.6205048705610059,5.6205048705610059,81.7,2.9695462057115267,2.8804598195401807,5.6205048705610059,5.6205048705610059,1.6300013487306384E-3,3]
[null,"SGN3B7","Urban",11,"SGN",0,10.039,4.9828831239282385,4.7541615838577247,7.2399723756379064,7.2399723756379064,10.683,4.8147011296487863,4.670260095759323,7.2399723756379064,7.2399723756379064,1.6300013487306384E-3,1]
[null,"SLI3B1","Urban",11,"SLI",0,2.5859999999999999,2.0449356848704832,1.8780947315071717,6.9732365512722998,6.9732365512722998,2.6560000000000001,2.2821852090983725,2.236541504916405,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,1]
[null,"SLI3B10","Short Rural",11,"SLI",0,180.41800000000001,2.3628283372076377,2.1700513538872364,6.9732365512722998,6.9732365512722998,183.01499999999999,1.4834203859139421,1.4537519781956632,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,3]
[null,"SLI3B2","Short Rural",11,"SLI",0,141.369,2.1449937000323418,1.9699892749448316,6.9732365512722998,6.9732365512722998,140.71799999999999,1.3693111254590233,1.3419249029498428,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,3]
[null,"SLI3B3","Urban",11,"SLI",0,4.5250000000000004,2.1241482802069545,1.950844578395319,6.9732365512722998,6.9732365512722998,4.7190000000000003,2.1110213184159945,2.0688008920476744,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,1]
[null,"SLI3B4","Urban",11,"SLI",0,5.6139999999999999,3.4947346337261624,3.2096083765257633,6.9732365512722998,6.9732365512722998,5.78,3.6134599144057562,3.541190716117641,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,1]
[null,"SLI3B5","Urban",11,"SLI",0,4.3259999999999996,3.1174325348866545,2.8630893689795878,6.9732365512722998,5.997745536449508,4.2969999999999997,2.9668407718278842,2.9075039563913263,6.9732365512722998,5.997745536449508,2.0660614101397193E-2,1]
[null,"SLI3B6","Short Rural",11,"SLI",0,90.03,1.7478884523587159,1.6052828056766193,6.763658403556466,6.763658403556466,90.015000000000001,1.2171654448524654,1.1928221359554161,6.763658403556466,6.763658403556466,2.0660614101397193E-2,3]
[null,"SLI3B7","Urban",11,"SLI",0,4.4370000000000003,2.3034188907052844,2.115488968721126,6.9732365512722998,6.9732365512722998,4.516,2.2631669990225527,2.2179036590421015,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,1]
[null,"SLI3B8","Short Rural",11,"SLI",0,20.934000000000001,4.8215456056120578,4.4281683119022315,6.9732365512722998,6.9732365512722998,20.881,4.3361518972869071,4.2494288593411689,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,3]
[null,"SLI3B9","Urban",11,"SLI",0,3.4830000000000001,3.4155220383896912,3.1368585296376157,6.9732365512722998,6.9732365512722998,3.3079999999999998,3.7465873849364946,3.6716556372377647,6.9732365512722998,6.9732365512722998,2.0660614101397193E-2,1]
[null,"SMN3B1","Short Rural",11,"SMN",0,92.878,0.71,0.69251311384211156,2.7616684101281965,2.7616684101281965,92.632999999999996,0.59062932538098711,0.56109785911193777,2.7616684101281965,2.7616684101281965,2.2748641885862432E-2,3]
[null,"SMN3B2","Short Rural",11,"SMN",0,110.131,2.02,1.9702485774099512,4.5726141319818359,2.7959630161180598,110.1,2.0957814771583414,1.9909924033004243,4.5726141319818359,2.7959630161180598,2.2748641885862432E-2,3]
[null,"SMN3B3","Short Rural",11,"SMN",0,39.997,0.32,0.31211858652038832,2.5587586580215023,2.5587586580215023,40.045999999999999,0.26673582436560705,0.2533990331473267,2.5587586580215023,2.5587586580215023,2.2748641885862432E-2,3]
[null,"SMN3B4","Urban",11,"SMN",0,1.4630000000000001,2.06,2.0092634007249996,4.7936238150276251,4.7936238150276251,1.6759999999999999,1.5813623873103848,1.5022942679448654,4.7936238150276251,4.7936238150276251,2.2748641885862432E-2,1]
[null,"SRG3B1","Long Rural",11,"SRG",0,207.733,0.75453101058912375,0.72059713931449576,1.3504453736453019,0.65826590941655194,207.79300000000001,0.75523272445382228,0.67970945200844002,1.3504453736453019,0.65826590941655194,-8.6186952502145663E-9,6]
[null,"STF8B1","Long Rural",22,"STF_22",0,305.84199999999998,0.92558484454049772,0.88923486902212434,5.4516991988553434,5.4516991988553434,0,"","","","",1.9425961620774684E-2,5]
[null,"STH3B1","Urban",11,"STH",0,9.4969999999999999,4.3213819814363559,4.1233166394943819,9.0499654695473861,9.0499654695473861,20.704999999999998,4.0935907246350567,4.0526548173887065,9.0499654695473861,9.0499654695473861,2.7765045996324352E-3,1]
[null,"STH3B10","Urban",11,"STH",0,7.5339999999999998,3.208750298859639,3.0616810909349086,9.0880705873138989,9.0880705873138989,7.944,5.0111196801567068,4.9610084833551396,9.0880705873138989,9.0880705873138989,2.7765045996324352E-3,1]
[null,"STH3B11","Urban",11,"STH",0,6.444,3.0398687041828163,2.9005399808857031,9.0880705873138989,9.0880705873138989,6.7190000000000003,2.8055212293835083,2.7774660170896732,9.0880705873138989,9.0880705873138989,2.7765045996324352E-3,1]
[null,"STH3B12","Short Rural",11,"STH",0,3.7040000000000002,1.1722369512861839,1.1185088815180162,9.0499654695473861,9.0499654695473861,3.9489999999999998,1.0410424687649498,1.0306320440773002,9.0499654695473861,9.0499654695473861,2.7765045996324352E-3,3]
[null,"STH3B2","Short Rural",11,"STH",0,10.029,3.2186845103112174,3.0711599797613331,9.0499654695473861,6.871305361246872,8.9689999999999994,1.79976833583093,1.7817706524726207,9.0499654695473861,6.871305361246872,2.7765045996324352E-3,3]
[null,"STH3B3","Long Rural",11,"STH",0,221.35900000000001,3.4074345278911959,3.251258867463386,9.0880705873138989,9.0880705873138989,210.179,2.9290347426268077,2.8997443952005395,9.0880705873138989,9.0880705873138989,2.7765045996324352E-3,5]
[null,"STH3B4","Urban",11,"STH",0,9.0399999999999991,2.6027634003133917,2.4834688725230532,9.0499654695473861,9.0499654695473861,9.8529999999999998,2.2938223888041267,2.2708841649160854,9.0499654695473861,9.0499654695473861,2.7765045996324352E-3,1]
[null,"STH3B5","Urban",11,"STH",0,5.3220000000000001,1.9471054445092546,1.8578622099790776,9.0499654695473861,6.9008368275159215,5.7389999999999999,2.9466795302329931,2.9172127349306631,9.0499654695473861,6.9008368275159215,2.7765045996324352E-3,1]
[null,"STH3B6","Short Rural",11,"STH",0,21.657,1.3709211803177404,1.3080866580464934,9.0499654695473861,3.5933126053823932,20.564,1.9056370614680433,1.8865806908533629,9.0499654695473861,3.5933126053823932,2.7765045996324352E-3,3]
[null,"STH3B8","Short Rural",11,"STH",0,7.6040000000000001,2.6226318232165471,2.5024266501759005,9.0499654695473861,6.9513261085565539,8.9130000000000003,5.6639768215855737,5.6073370533697178,9.0499654695473861,6.9513261085565539,2.7765045996324352E-3,3]
[null,"STH3B9","Short Rural",11,"STH",0,159.631,1.1325001054798725,1.0805933262123206,9.0499654695473861,5.2480273443933196,165.72900000000001,1.0939768315835066,1.0830370632676716,9.0499654695473861,5.2480273443933196,2.7765045996324352E-3,3]
[null,"STL3B2","Short Rural",11,"STL",0,4.0410000000000004,0.94034047556028466,0.93929398248710727,5.6205048705610059,5.6205048705610059,4.2320000000000002,2.1474979865157384,2.0830730469202661,5.6205048705610059,5.6205048705610059,9.9511904170942224E-3,3]
[null,"STL3B4","Short Rural",11,"STL",0,42.121000000000002,1.0986156051100355,1.0973929696384026,5.6205048705610059,5.6205048705610059,42.356999999999999,2.7298703218420406,2.6479742121867793,5.6205048705610059,5.6205048705610059,9.9511904170942224E-3,3]
[null,"STL3B5","Short Rural",11,"STL",0,10.305999999999999,3.4168807379269746,3.4130781343838446,5.6205048705610059,5.6205048705610059,10.92,4.0402080763262198,3.919001834036433,5.6205048705610059,5.6205048705610059,9.9511904170942224E-3,3]
[null,"STL3B7","Short Rural",11,"STL",0,11.215999999999999,3.4261910396651958,3.4223780748045098,5.6205048705610059,5.6205048705610059,11.853999999999999,3.0938530314209789,3.0010374404783495,5.6205048705610059,5.6205048705610059,9.9511904170942224E-3,3]
[null,"STL3B8","Urban",11,"STL",0,0.35199999999999998,0.13965452607330958,0.1394991063099664,5.6205048705610059,5.6205048705610059,0.35199999999999998,0.90995677394734686,0.88265807072892644,5.6205048705610059,5.6205048705610059,9.9511904170942224E-3,1]
[null,"STR3B1","Short Rural",11,"STR_11",0,66.334999999999994,1.4491983185617026,1.3767384026336174,6.763658403556466,2.8502628089353443,63.143999999999998,1.2874182205616709,1.1844247629167373,6.763658403556466,2.8502628089353443,1.7484805400258818E-2,3]
[null,"STR3B2","Short Rural",11,"STR_11",0,131.35300000000001,1.5445403132039199,1.467313297543724,6.763658403556466,2.920757276803398,131.38399999999999,1.5605069340141466,1.4356663792930149,6.763658403556466,2.920757276803398,1.7484805400258818E-2,3]
[null,"SUN4B1","Long Rural",33,"SUN_33",0,776.68,1.8879999999999999,1.8314870644328889,9.4573091784714318,1.1574429521579022,707.27200000000005,1.609,1.609,9.4573091784714318,1.1574429521579022,2.0291436718229996E-2,5]
[null,"SUN4B2","Short Rural",33,"SUN_33",0,190.011,0.29099999999999998,0.28228958461333192,7.3321867606328732,1.6718620420058588,189.96199999999999,1.306,1.306,7.3321867606328732,1.6718620420058588,2.0291436718229996E-2,3]
[null,"SUN8B1","Short Rural",22,"SUN_22",0,73.524000000000001,0.624,0.58690563340761792,0.84555256323897443,0.84555256323897443,73.53,0.80020747309682116,0.80020747309682116,0.84555256323897443,0.84555256323897443,-6.0722387824375491E-9,4]
[null,"SUT5323","Long Rural",11,"SUT",0,271.48200000000003,1.6306984277511878,1.6001515142775384,5.1822960162460801,2.9407624636308189,271.173,1.5241988886923026,1.4836551982530874,5.2394536928958528,2.9379045797983299,-3.6956778568778672E-5,6]
[null,"SUT5333","Short Rural",11,"SUT",0,117.373,1.4616626151184429,1.4342821499926719,5.1822960162460801,3.2665612205345247,118.232,1.544386953443194,1.5033062604816052,3.2656085925903611,3.2656085925903611,-3.6956778568778672E-5,4]
[null,"SWR3B1","Short Rural",11,"SWR",0,5.585,0.92771788940070132,0.92264438659512393,9.0880705873138989,1.5918412946961769,5.968,0.77981428579347067,0.77513540007870985,9.0880705873138989,1.5918412946961769,7.8206407091932183E-3,3]
[null,"SWR3B3","Short Rural",11,"SWR",0,9.98,2.1997434490944463,2.1877134939884382,9.0880705873138989,1.517536315051472,10.239000000000001,1.9041976746119633,1.8927724885642916,9.0880705873138989,1.517536315051472,7.8206407091932183E-3,3]
[null,"SWR3B4","Short Rural",11,"SWR",0,11.057,0.48776919958181203,0.48510168779743629,9.0880705873138989,1.467047034010839,10.63,0.47151561466581948,0.46868652097782454,9.0880705873138989,1.467047034010839,7.8206407091932183E-3,3]
[null,"SWR3B5","Short Rural",11,"SWR",0,6.3339999999999996,1.8363075748962334,1.8262651775903482,9.0880705873138989,1.5051521517773543,6.6120000000000001,1.99487375435539,1.9829045118292576,9.0880705873138989,1.5051521517773543,7.8206407091932183E-3,3]
[null,"SWR3B6","Short Rural",11,"SWR",0,65.194999999999993,1.6450255358445425,1.6360292215913537,6.763658403556466,1.0802800886807087,65.33,1.3601411961514025,1.3519803489744942,6.763658403556466,1.0802800886807087,7.8206407091932183E-3,3]
[null,"SWT12","Long Rural",11,"SWT",0,510.75400000000002,4.1500000000000004,4.1370993186220195,5.8110304593935824,5.8110304593935824,506.03699999999998,3.4289999999999998,3.4289999999999998,5.8110304593935824,5.8110304593935824,-8.0206859371066683E-12,6]
[null,"SWT22","Short Rural",11,"SWT",0,80.206000000000003,1.94,1.9339693200305343,5.8110304593935824,5.8110304593935824,80.757000000000005,2,2,5.8110304593935824,5.8110304593935824,-8.0206859371066683E-12,4]
[null,"SWT32","Short Rural",11,"SWT",0,13.057,3.66,3.6486225316039982,5.2394536928958528,5.2394536928958528,12.041,3.048,3.048,5.2394536928958528,5.2394536928958528,-8.0206859371066683E-12,4]
[null,"SWT42","Urban",11,"SWT",0,9.9280000000000008,5.45,5.4330581413228938,5.8110304593935824,5.8110304593935824,10.523,5.7149999999999999,5.7149999999999999,5.8110304593935824,5.8110304593935824,-8.0206859371066683E-12,2]
[null,"SWT52","Urban",11,"SWT",0,11.379,4,3.9875656083103803,5.8110304593935824,5.147048782312055,11.79,4.1920000000000002,4.1920000000000002,5.8110304593935824,5.147048782312055,-8.0206859371066683E-12,2]
[null,"SWT72","Short Rural",11,"SWT",0,6.8280000000000003,0.5,0.49844570103879754,9.0880705873138989,2.1538917817522774,0,"","","","",-8.0206859371066683E-12,4]
[null,"SWT82","Short Rural",11,"SWT",0,21.884,4.0199999999999996,4.0075034363519322,5.8110304593935824,4.4944986405604794,21.744,4.9537000000000004,4.9537000000000004,5.8110304593935824,4.4944986405604794,-8.0206859371066683E-12,4]
[null,"TAL1414","Short Rural",11,"TAL",0,17.170999999999999,0.63,-0.52820349857205562,5.0489281040632772,1.0564643900766366,17.170999999999999,0.68400000000000005,0.6467904000000001,5.0489281040632772,1.0364592032492161,1.2887383370909914E-2,3]
[null,"TAR436","Short Rural",11,"TAR",0,35.963999999999999,0.35430477612970163,0.31887429851673149,1.3350128009498634,0.7373340287820711,36.323999999999998,0.36486713153155176,0.34819270362055987,1.3350128009498634,0.7373340287820711,0,3]
[null,"TAR437","Short Rural",11,"TAR",0,63.085000000000001,0.31381280171487858,0.28243152154339074,1.3350128009498634,0.7106604463455104,63.203000000000003,0.32646006505454633,0.31154084008155358,1.3350128009498634,0.7106604463455104,0,3]
[null,"TAR438","Short Rural",11,"TAR",0,135.88900000000001,0.3846737569408189,0.34620638124673703,1.6651936463967185,0.74304979644704827,136.04300000000001,0.36486713153155176,0.34819270362055987,1.6651936463967185,0.74304979644704827,0,3]
[null,"TAR439","Short Rural",11,"TAR",0,134.01400000000001,0.32393579531858435,0.2915422157867259,1.6651936463967185,0.70399205073637017,134.047,0.35526536491230037,0.33902973773580825,1.6651936463967185,0.70399205073637017,0,3]
[null,"TDL3B1","Short Rural",11,"TDL",0,56.168999999999997,0.10031959527512853,9.8651053055256566E-2,0.42277628161948722,0.42277628161948722,56.201000000000001,9.1402277511077074E-2,8.3176072535080137E-2,0.42277628161948722,0.42277628161948722,-1.8448718515977191E-2,4]
[null,"TDL3B2","Short Rural",11,"TDL",0,183.18700000000001,0.26083094771533416,0.25649273794366706,2.1298855575593727,0.88308610423899214,183.23699999999999,0.20311617224683795,0.18483571674462254,2.1298855575593727,0.88308610423899214,-1.8448718515977191E-2,4]
[null,"TDL3B3","Short Rural",11,"TDL",0,17.021000000000001,0.11035155480264137,0.10851615836078221,2.0738710344425955,0.58681881360433552,17.030999999999999,5.0779043061709488E-2,4.6208929186155635E-2,2.0738710344425955,0.58681881360433552,-1.8448718515977191E-2,4]
[null,"TDL8B1","Long Rural",22,"TDL",0,208.50399999999999,0.69220520739838676,0.6806922660812702,4.1477420688851909,3.0846092831994136,206.46299999999999,0.34529749281962452,0.31422071846585831,4.1477420688851909,3.0846092831994136,-1.8448718515977191E-2,6]
[null,"TDL8B2","Long Rural",22,"TDL",0,1037.4760000000001,2.4076702866030844,2.3676252733261571,4.2597711151187454,2.4539695841635853,1035.8679999999999,2.0108501052436956,1.8298735957717631,4.2597711151187454,2.4520643282752599,-1.8448718515977191E-2,6]
[null,"TDL8B4","Short Rural",22,"TDL",0,46.658000000000001,0.91290831700366959,0.89772458280283474,4.1477420688851909,2.9664834181232163,45.65,0.7109066028639327,0.64692500860617874,4.1477420688851909,2.9512413710166103,-1.8448718515977191E-2,4]
[null,"TEA3B1","Short Rural",11,"TEA",0,94.518000000000001,2.6993121338364223,2.6978494096990078,9.0880705873138989,1.5451625254321955,93.872,1.9772565497566057,1.9574839842590397,9.0880705873138989,1.5451625254321955,1.9516370037800428E-2,3]
[null,"TEA3B3","Short Rural",11,"TEA",0,22.023,2.2692522345472295,2.2680225545944199,9.0880705873138989,4.5573720848752304,22.282,2.3035998637941035,2.2805638651561626,9.0880705873138989,4.5573720848752304,1.9516370037800428E-2,3]
[null,"TEA3B4","Short Rural",11,"TEA",0,10.496,2.8640159250535597,2.8624639499518283,9.0880705873138989,3.2884716632502711,11.051,2.0156498808198409,1.9954933820116425,9.0880705873138989,3.2884716632502711,1.9516370037800428E-2,3]
[null,"TEA3B8","Short Rural",11,"TEA",0,15.314,2.790814240068165,2.7893019320616852,9.0880705873138989,3.3027610824127143,15.718999999999999,2.5339598501735141,2.508620251671779,9.0880705873138989,3.3027610824127143,1.9516370037800428E-2,3]
[null,"TEM3B1","Short Rural",11,"TEM",0,15.446999999999999,2.7352097028614062,2.5897985926324778,3.5163402674940318,3.5163402674940318,15.997999999999999,2.8773959747013298,2.5585805007044224,3.5163402674940318,3.5163402674940318,-1.998530174345817E-3,4]
[null,"TEM3B2","Long Rural",11,"TEM",0,573.23699999999997,1.3187618210224639,1.2486528928763734,3.2126424788949053,3.2126424788949053,575.428,1.3302060079766804,1.1828191822928642,3.2126424788949053,3.2126424788949053,-1.998530174345817E-3,6]
[null,"TEM3B3","Long Rural",11,"TEM",0,246.22,0.62519078922546434,0.59195396403028067,2.4511117003310967,2.4511117003310967,244.39,0.42453383233298314,0.37749548371048858,3.5163402674940318,2.4520643282752599,-1.998530174345817E-3,6]
[null,"TEM3B4","Short Rural",11,"TEM",0,20.649000000000001,3.2236400069437998,3.0522626270311339,2.7502368747982415,2.7502368747982415,21.268000000000001,3.1132481037752093,2.7683002138769162,1.3350128009498634,1.3350128009498634,-1.998530174345817E-3,4]
[null,"TFD102","Short Rural",11,"TFD",0,113.39,0.62612698106209608,0.62294243368303626,2.7765294060571373,2.7765294060571373,113.042,0.62233305849975851,0.59121640557477051,2.7765294060571373,2.7765294060571373,-1.0924470900616691E-2,4]
[null,"TFD112","Short Rural",11,"TFD",0,52.487000000000002,1.3270153926987707,1.3202660534774797,2.7765294060571373,2.7765294060571373,52.982999999999997,0.47590175061746237,0.45210666308658926,2.7765294060571373,2.7765294060571373,-1.0924470900616691E-2,4]
[null,"TFD32","Long Rural",22,"NTTF",0,244.53700000000001,0.83172091514218727,0.82749069548940624,5.5530588121142745,5.5530588121142745,243.66800000000001,1.9219109159551366,1.8258153701573798,5.5530588121142745,5.5530588121142745,-1.1078842375846986E-2,6]
[null,"TFD62","Long Rural",22,"NTTF",0,229.03399999999999,2.7101018583284753,2.6963179965385149,5.5530588121142745,5.5530588121142745,233.947,1.6473522136758314,1.5649846029920398,5.5530588121142745,5.5530588121142745,-1.1078842375846986E-2,6]
[null,"THA2222","Urban",11,"THA",0,3.851,1.39,1.3828236507509066,7.9258644954351825,6.3521231316781011,3.7,1.4285714285714286,1.2942857142857143,6.3521231316781011,6.3521231316781011,-4.1456142869727416E-2,2]
[null,"THA2223","Short Rural",11,"THA",0,10.97,3.47,3.4520849410831986,3.583405274763098,3.583405274763098,11.29,3.7523809523809524,3.3996571428571429,3.583405274763098,3.583405274763098,-4.1456142869727416E-2,4]
[null,"THA2224","Short Rural",11,"THA",0,76.844999999999999,1.71,1.7011715415712592,6.763658403556466,3.131288052463395,77.129000000000005,2.2857142857142856,2.0708571428571427,6.763658403556466,3.131288052463395,-4.1456142869727416E-2,4]
[null,"THA2225","Short Rural",11,"THA",0,24.382000000000001,2.59,2.5766282413272288,7.9258644954351825,3.8124170325398565,24.074999999999999,2.9523809523809526,2.6748571428571433,3.8124170325398565,3.8124170325398565,-4.1456142869727416E-2,4]
[null,"THA2229","Short Rural",11,"THA",0,24.37,2.8,2.785544044678085,7.9258644954351825,4.7317029986570383,24.596,3.0476190476190474,2.7611428571428571,4.7317029986570383,4.7317029986570383,-4.1456142869727416E-2,4]
[null,"THA2230","Short Rural",11,"THA",0,85.397999999999996,0.9,0.89535344293224173,6.763658403556466,4.3477939371593957,84.954999999999998,0.95238095238095233,0.86285714285714288,6.763658403556466,4.3477939371593957,-4.1456142869727416E-2,4]
[null,"THA2231","Short Rural",11,"THA",0,39.524999999999999,2.02,2.0095710608034758,7.9258644954351825,2.5654270536306427,39.600999999999999,2.0952380952380953,1.8982857142857144,2.5263693079199645,2.5263693079199645,-4.1456142869727416E-2,4]
[null,"THA2232","Short Rural",11,"THA",0,28.228000000000002,1.94,1.9299840880983876,7.9258644954351825,2.8188260867779693,33.466999999999999,2.1904761904761907,1.9845714285714289,2.8188260867779693,2.8188260867779693,-4.1456142869727416E-2,4]
[null,"THN3B1","Urban",11,"THN",0,3.141,1.000125656695301,0.9579989352189876,7.2399723756379064,7.2399723756379064,3.4390000000000001,0.92055744600025402,0.90214629708024896,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B2","Urban",11,"THN",0,3.0649999999999999,4.1292316717023807,3.955302534517998,7.2399723756379064,7.2399723756379064,2.6509999999999998,4.4337052501236718,4.3450311451211983,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B3","Short Rural",11,"THN",0,1.7,0.49511171123529746,0.47425689862326115,9.0499654695473861,9.0499654695473861,1.7130000000000001,0.52603282628585946,0.51551216976014225,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,4]
[null,"THN3B4","Urban",11,"THN",0,3.786,3.6341199604670833,3.4810456358947368,9.0499654695473861,9.0499654695473861,4.226,3.5319346907764846,3.4612959969609549,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B5","Urban",11,"THN",0,1.5129999999999999,1.6635753497505994,1.5935031793741574,7.2399723756379064,7.2399723756379064,1.746,1.7096066854290433,1.6754145517204624,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B6","Urban",11,"THN",0,3.6110000000000002,1.4556284310317744,1.3943152819523876,7.2399723756379064,7.2399723756379064,3.85,1.5780984788575783,1.5465365092804266,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B7","Urban",11,"THN",0,7.0419999999999998,3.4855864470964941,3.3387685663077584,7.2399723756379064,7.2399723756379064,7.4329999999999998,3.1561969577151565,3.0930730185608533,7.2399723756379064,7.2399723756379064,-2.5642492892111336E-2,2]
[null,"THN3B8","Urban",11,"THN",0,6.6280000000000001,2.0002513133906019,1.9159978704379752,7.2399723756379064,6.7407953328965569,6.9139999999999997,2.4610821515516994,2.4118605085206655,7.2399723756379064,6.7407953328965569,-2.5642492892111336E-2,2]
[null,"THR","Urban",11,"THR",0,0.17100000000000001,0.24,0.23328796640131849,1.9090664001024165,1.9090664001024165,0.17199999999999999,0.253,0.24576734388042723,1.9090664001024165,1.9090664001024165,-6.2476531217539108E-8,2]
[null,"THRR31","Urban",11,"THR",0,2.1669999999999998,2.62,2.5467269665477272,3.1436722157375119,3.1436722157375119,2.1739999999999999,2.3780000000000001,2.3100187499907352,3.1436722157375119,3.1436722157375119,-6.2476531217539108E-8,2]
[null,"THRR48","Urban",11,"THR",0,3.4630000000000001,1.1599999999999999,1.1275585042730394,3.1436722157375119,2.8693153678186016,3.4670000000000001,1.103,1.0714679063245502,3.1436722157375119,2.8693153678186016,-6.2476531217539108E-8,2]
[null,"THRR55","Urban",11,"THR",0,3.3079999999999998,2.4300000000000002,2.3620406598133501,3.791459217768272,3.1770141937832133,3.3679999999999999,2.4740000000000002,2.4032743429256009,3.791459217768272,3.1770141937832133,-6.2476531217539108E-8,2]
[null,"THRR84","Urban",11,"THR",0,5.5410000000000004,2.19,2.1287526934120313,5.2394536928958528,2.853120692767833,5.7130000000000001,2.1880000000000002,2.1254503889738134,5.2394536928958528,2.6130584508387869,-6.2476531217539108E-8,2]
[null,"TMT12","Short Rural",11,"TMT",0,11.699,3.81,3.563402345396816,3.5163402674940318,3.5163402674940318,12.606999999999999,4,3.5928,3.5163402674940318,3.5163402674940318,-6.8336024860463944E-3,4]
[null,"TMT22","Short Rural",11,"TMT",0,17.655000000000001,3.13,2.927414525221006,3.5163402674940318,3.5163402674940318,19.128,4.26,3.8263319999999998,3.5163402674940318,3.5163402674940318,-6.8336024860463944E-3,4]
[null,"TMT32","Urban",11,"TMT",0,0.93100000000000005,4.83,4.5173840756605301,3.5163402674940318,3.5163402674940318,1.022,4.76,4.2754319999999995,3.5163402674940318,3.5163402674940318,-6.8336024860463944E-3,2]
[null,"TMT42","Urban",11,"TMT",0,1.046,3.43,3.2079973870632754,3.5163402674940318,3.5163402674940318,1.0549999999999999,3.5,3.1436999999999999,3.5163402674940318,3.5163402674940318,-6.8336024860463944E-3,2]
[null,"TMT52","Short Rural",11,"TMT",0,77.774000000000001,0.36,0.33669943421072274,4.1292610867684303,2.2301020172853083,84.739000000000004,0.19,0.170658,4.1292610867684303,2.2301020172853083,-6.8336024860463944E-3,4]
[null,"TMT62","Long Rural",11,"TMT",0,366.66899999999998,2.4300000000000002,2.2727211809223786,4.1534578365501673,4.1534578365501673,365.99700000000001,3.12,2.802384,4.1534578365501673,4.1534578365501673,-6.8336024860463944E-3,6]
[null,"TMT72","Urban",11,"TMT",0,0.995,1.58,1.4777364057026166,3.583405274763098,3.583405274763098,1,2,1.7964,3.583405274763098,3.583405274763098,-6.8336024860463944E-3,2]
[null,"TMT82","Short Rural",11,"TMT",0,13.881,1.05,0.98204001644794148,1.3350128009498634,1.3350128009498634,13.965999999999999,3.74,3.3592680000000001,1.3350128009498634,1.3350128009498634,-6.8336024860463944E-3,4]
[null,"TNA3B1","Short Rural",11,"TNA_11",0,52.046999999999997,3.586912808072579,3.5811765125478612,7.9449170543184398,7.9449170543184398,52.930999999999997,3.2208683438355545,3.0598249266437767,7.9449170543184398,7.9449170543184398,-2.2385253952713111E-2,4]
[null,"TNA3B2","Short Rural",11,"TNA_11",0,17.260000000000002,2.4847347484491986,2.4807610882070086,7.9449170543184398,7.9449170543184398,17.742000000000001,2.1960465980696964,2.0862442681662117,7.9449170543184398,7.9449170543184398,-2.2385253952713111E-2,4]
[null,"TPT3B1","Short Rural",11,"TPT",0,69.376999999999995,0.88690795006075729,0.88381370298775463,6.763658403556466,3.2055930321080996,19.466999999999999,0.2170991096579056,0.20841514527158936,6.763658403556466,3.1932088688339828,-3.2219589982083251E-3,4]
[null,"TPT3B2","Short Rural",11,"TPT",0,33.170999999999999,0.68981729449170004,0.68741065787936462,6.763658403556466,2.1215024316507392,82.533000000000001,0.57376193266732201,0.55081145536062914,6.763658403556466,2.7626210380723593,-3.2219589982083251E-3,4]
[null,"TPT3B3","Short Rural",11,"TPT",0,117.658,0.78836262227622866,0.78561218043355963,6.763658403556466,2.7835788528439425,117.408,0.51173361562220609,0.49126427099731784,6.763658403556466,2.7835788528439425,-3.2219589982083251E-3,4]
[null,"TSH3B1","Short Rural",11,"TSH",0,42.348999999999997,2.5603637261145504,2.5548992307463188,7.2399723756379064,4.9260390992662648,42.261000000000003,2.4984141504557091,2.448445867446595,7.2399723756379064,4.9260390992662648,9.5330612456536491E-3,3]
[null,"TSH3B10","Urban",11,"TSH",0,6.4429999999999996,3.6393741535485398,3.6316067637036964,7.2399723756379064,7.2399723756379064,6.78,3.2933641074188893,3.2274968252705114,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,1]
[null,"TSH3B2","Urban",11,"TSH",0,2.7829999999999999,0.90527146030478745,0.90333937087101979,7.2399723756379064,7.2399723756379064,2.6070000000000002,0.83280471681856971,0.81614862248219833,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,1]
[null,"TSH3B4","Urban",11,"TSH",0,3.4260000000000002,1.6733805781391526,1.6698091400949155,7.2399723756379064,7.2399723756379064,3.51,1.8738106128417817,1.836334400584946,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,1]
[null,"TSH3B5","Short Rural",11,"TSH",0,11.121,3.2918962192901366,3.2848704395309816,7.2399723756379064,7.2399723756379064,11.536,3.066235548286552,3.0049108373208209,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,3]
[null,"TSH3B6","Short Rural",11,"TSH",0,3.1139999999999999,0.36576624658779294,0.3649856043923313,7.2399723756379064,6.7884267301047005,3.1150000000000002,0.79494995696318016,0.77905095782391653,7.2399723756379064,6.7884267301047005,9.5330612456536491E-3,3]
[null,"TSH3B7","Short Rural",11,"TSH",0,4.0860000000000003,0.88698314797539779,0.88509009065140332,7.2399723756379064,7.2399723756379064,4.2670000000000003,0.92744161645704348,0.90889278412790264,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,3]
[null,"TSH3B8","Short Rural",11,"TSH",0,10.548999999999999,2.8895533480435645,2.8833862746994172,7.2399723756379064,7.2399723756379064,11.012,2.8391069891542147,2.7823248493711303,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,3]
[null,"TSH3B9","Urban",11,"TSH",0,2.3359999999999999,1.4264883616923925,1.423443857130092,7.2399723756379064,7.2399723756379064,2.4790000000000001,1.4195534945771073,1.3911624246855652,7.2399723756379064,7.2399723756379064,9.5330612456536491E-3,1]
[null,"TUM12","Short Rural",22,"TUM",0,157.477,1.2340376929102488,1.2334680458781093,5.4516991988553434,3.4027870165498166,156.78800000000001,2.7311230388850714,2.6898830809979066,5.4516991988553434,3.381829201778233,-5.2112360120174827E-3,4]
[null,"TUM22","Long Rural",22,"TUM",0,296.05900000000003,1.0564110552943795,1.0559234029108056,3.330387292793437,3.1722510540623983,296.53300000000002,2.5360428218218516,2.4977485752123418,3.330387292793437,3.1493879834024896,-5.2112360120174827E-3,6]
[null,"TUM32","Short Rural",22,"TUM",0,43.12,1.8323589985637025,1.8315131590311318,4.0715318333521591,3.3246715251284598,43.606999999999999,1.0924492155540286,1.0759532323991627,4.0715318333521591,3.0655567243161559,-5.2112360120174827E-3,4]
[null,"TUM42","Long Rural",22,"TUM",0,211.10599999999999,0.7198553208643117,0.71952302676223034,3.330387292793437,3.1874931011690051,212.22499999999999,0.6779037542946873,0.66766740760483756,3.330387292793437,3.1608195187324442,-5.2112360120174827E-3,6]
[null,"TUM52","Urban",22,"TUM",0,3.661,5.4690306844886019,5.466506112414347,3.330387292793437,3.330387292793437,3.7109999999999999,5.7090225523551146,5.6228163118145522,3.330387292793437,3.330387292793437,-5.2112360120174827E-3,2]
[null,"TUN3B2","Short Rural",11,"TUN",0,9.1280000000000001,1.3391818474308728,1.3385200962874575,7.9258644954351825,5.4537949803325017,9.2539999999999996,2.0557215758591161,1.9940499285833426,7.9258644954351825,5.4537949803325017,-5.7283153223945888E-4,4]
[null,"TUN3B3","Short Rural",11,"TUN",0,3.3149999999999999,1.0207749746151409,1.0202705629044257,7.9258644954351825,6.9913364822113957,3.4079999999999999,0.76622349645657961,0.74323679156288225,7.9258644954351825,7.2199671888104877,-5.7283153223945888E-4,4]
[null,"TUN3B4","Short Rural",11,"TUN",0,4.5759999999999996,1.6013992721026522,1.600607947308778,8.9547026751310952,8.9547026751310952,4.6589999999999998,1.308186457364892,1.2689408636439452,8.9547026751310952,8.9547026751310952,-5.7283153223945888E-4,4]
[null,"TUN3B5","Short Rural",11,"TUN",0,30.170999999999999,2.5847146146218245,2.5834373886387296,7.9258644954351825,6.9046473392925725,48.426000000000002,4.1114431517182322,3.9880998571666852,7.9258644954351825,6.9046473392925725,-5.7283153223945888E-4,4]
[null,"TUN3B6","Urban",11,"TUN",0,3.5630000000000002,2.2288481097101238,2.2277467336812231,7.9258644954351825,7.9258644954351825,3.8519999999999999,1.6819540166120042,1.631495396113644,7.9258644954351825,7.9258644954351825,-5.7283153223945888E-4,2]
[null,"TURA2","Short Rural",11,"TUR",0,19.468,2.5805108834282318,2.5593125492656563,6.763658403556466,2.8864626708135339,20.108000000000001,2.2877066222828897,2.2607116841399515,2.8864626708135339,2.8864626708135339,7.0872610910209825E-3,3]
[null,"TXS2X04","Long Rural",22,"TXS_22",0,301.63900000000001,0.88,0.83599999999999997,4.8881245070885821,2.2005705510162583,301.61500000000001,0.84,0.80639999999999989,4.8881245070885821,2.2005705510162583,9.5318255784868008E-10,5]
[null,"TXS2X08","Long Rural",22,"TXS_22",0,283.47800000000001,1.5,1.4249999999999998,4.2597711151187454,2.324412183757433,284.13299999999998,1.87,1.7952000000000001,4.2597711151187454,2.324412183757433,9.5318255784868008E-10,5]
[null,"TXS2X18","Short Rural",22,"TXS_22",0,18.981999999999999,0.96,0.91199999999999992,4.2597711151187454,3.4008817606614903,19.413,1.22,1.1712,4.2597711151187454,3.4008817606614903,9.5318255784868008E-10,3]
[null,"TXS3X06","Long Rural",33,"TXS_33",0,571.39599999999996,1.83,1.7384999999999999,9.4561660249384349,4.6126245056366768,496.64800000000002,2.29,2.1755,9.4561660249384349,4.6126245056366768,-4.6029440914541017E-2,6]
[null,"UBV3B1","Short Rural",11,"UBV",0,58.656999999999996,0.65378248336849343,0.65231486482986156,6.763658403556466,0.55633471939112344,58.777999999999999,0.50849567202957335,0.48307088842809465,6.763658403556466,0.79163382159935547,-4.023560372607552E-10,4]
[null,"UBV3B2","Short Rural",11,"UBV",0,21.588000000000001,0.10422619300077433,0.10399222482794895,6.763658403556466,0.4696455764723011,21.597999999999999,9.8130743725005382E-2,9.3224206538755114E-2,6.763658403556466,0.79353907748768115,-4.023560372607552E-10,4]
[null,"UBV3B3","Short Rural",11,"UBV",0,7.8959999999999999,3.7900433818463392E-2,3.7815354482890529E-2,6.763658403556466,0.31817773335040272,7.8979999999999997,3.568390680909287E-2,3.3899711468638224E-2,6.763658403556466,0.31817773335040272,-4.023560372607552E-10,4]
[null,"UBV3B4","Short Rural",11,"UBV",0,70.539000000000001,0.37900433818463397,0.37815354482890534,6.763658403556466,0.66017116530487752,70.441999999999993,3.568390680909287E-2,3.3899711468638224E-2,6.763658403556466,0.79353907748768115,-4.023560372607552E-10,4]
[null,"ULG3B1","Short Rural",11,"ULG",0,68.509,0.53,0.45659470975849881,1.5478298836758515,0.90594917489890137,68.625,0.30484094213212237,0.28045366676155259,1.5478298836758515,0.90594917489890137,-1.2996554332746209E-2,4]
[null,"ULN27","Short Rural",22,"ULN",0,76.36,0.18058425589084437,0.17155504309630215,4.8881245070885821,1.7528354172597038,76.427999999999997,0.09,8.8253999999999999E-2,4.8881245070885821,1.7528354172597038,3.1349101583293848E-2,3]
[null,"ULN28","Short Rural",22,"ULN",0,113.863,0.6812951472245492,0.64723038986332171,4.8881245070885821,2.8026314117271998,112.652,0.65100000000000002,0.63837060000000001,4.8881245070885821,2.8026314117271998,3.1349101583293848E-2,3]
[null,"ULN29","Long Rural",22,"ULN",0,277.99799999999999,1.4665630478407967,1.3932348954487568,4.8881245070885821,1.8042773262444993,281.17899999999997,1.1559999999999999,1.1335735999999998,4.8881245070885821,1.8042773262444993,3.1349101583293848E-2,5]
[null,"UMA590","Short Rural",11,"UMA",0,52.993000000000002,0.45549028182573481,0.41771189688182014,1.3466348618686506,1.3222475864980812,53.015000000000001,0.58005102185680846,0.52204591967112768,1.3466348618686506,1.2908108643407057,-1.3278108859399031E-9,4]
[null,"UMA591","Short Rural",11,"UMA",0,63.164000000000001,0.10717418395899643,9.8285152207487098E-2,1.3466348618686506,0.87737033657401486,63.173999999999999,0.15744242021827659,0.14169817819644895,1.3466348618686506,0.87737033657401486,-1.3278108859399031E-9,4]
[null,"UNI3B1","Urban",11,"UNI",0,1.8220000000000001,1.5276328165618369,1.5201549113191037,4.5726141319818359,4.5726141319818359,2.056,1.1149397883346392,1.0814915946846,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,1]
[null,"UNI3B2","Short Rural",11,"UNI",0,164.47499999999999,0.60713611940278134,0.60416413142169501,4.5726141319818359,4.5726141319818359,165.10400000000001,0.84109492804192099,0.81586208020066331,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,3]
[null,"UNI3B3","Short Rural",11,"UNI",0,89.087000000000003,1.0771769860371927,1.0719041041352655,6.2435235460435337,6.2435235460435337,88.944000000000003,0.65527162998614774,0.63561348108656324,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,3]
[null,"UNI3B4","Short Rural",11,"UNI",0,4.3049999999999997,0.67568374578696633,0.67237621077575738,6.9732365512722998,6.9732365512722998,4.5430000000000001,0.92911649027886611,0.90124299557050014,6.9732365512722998,6.9732365512722998,8.6252327106734923E-3,3]
[null,"UNI3B5","Short Rural",11,"UNI",0,20.652999999999999,1.9976736831962483,1.987894884032674,4.5726141319818359,4.5726141319818359,20.745000000000001,1.8582329805577322,1.8024859911410003,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,3]
[null,"UNI3B6","Short Rural",11,"UNI",0,5.6070000000000002,3.2707010303311121,3.2546906434652603,6.5740854426680526,6.5740854426680526,5.9649999999999999,0.83816087596735611,0.81301604968833541,7.2399723756379064,6.5740854426680526,8.6252327106734923E-3,3]
[null,"UNI3B7","Urban",11,"UNI",0,4.9180000000000001,1.6941056234948575,1.6858128183218264,4.5726141319818359,4.5726141319818359,5.4470000000000001,1.5843881202650141,1.5368564766570636,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,1]
[null,"UNI3B8","Short Rural",11,"UNI",0,6.8540000000000001,2.9475479345199544,2.9331194122246806,4.5726141319818359,4.5726141319818359,6.9950000000000001,2.0489463654044471,1.9874779744423137,4.5726141319818359,4.5726141319818359,8.6252327106734923E-3,3]
[null,"UQT8B1","Long Rural",22,"UQT",0,449.13499999999999,2.3424464410693124,2.3032854331433468,18.862033294425075,18.862033294425075,448.17500000000001,0.71684822499829082,0.69484098449084331,3.0834661296664181,3.0834661296664181,7.5691823478888246E-6,5]
[null,"UQT8B2","Short Rural",22,"UQT",0,44.814999999999998,1.2804050461777174,1.2589992409978463,12.536583745183533,12.536583745183533,45.570999999999998,0.45274624736734154,0.43884693757316418,12.536583745183533,6.5940906294954731,7.5691823478888246E-6,3]
[null,"UQT8B4","Short Rural",22,"UQT",0,16.846,2.193562133374229,2.1568901725622016,12.536583745183533,12.536583745183533,16.98,0.84889921381376543,0.69484098449084331,11.241009741122012,6.687448168023435,7.5691823478888246E-6,3]
[null,"UQT8B5","Short Rural",22,"UQT",0,113.61199999999999,0.41687606154623352,0.4099067296272057,18.862033294425075,18.862033294425075,113.43899999999999,0.35842411249914541,0.34742049224542165,2.7008907472906039,2.7008907472906039,7.5691823478888246E-6,3]
[null,"URA3B1","Short Rural",11,"URA",0,160.72999999999999,0.68367208265713431,0.6494884785242776,3.9057745710678189,3.9057745710678189,160.66999999999999,0.91421025023808622,0.86849973772618183,2.3758540927422289,2.3758540927422289,-1.378792177464875E-9,4]
[null,"URA3B2","Long Rural",11,"URA",0,249.88800000000001,0.72062733036833082,0.68459596384991428,1.6651936463967185,1.6651936463967185,249.929,1.1251818464468755,1.0689227541245316,1.6651936463967185,1.6651936463967185,-1.378792177464875E-9,6]
[null,"URA3B3","Short Rural",11,"URA",0,5.7430000000000003,1.0532245597690988,1.0005633317806437,1.6651936463967185,1.6651936463967185,6.2119999999999997,1.3160609096833988,1.2502578641992288,1.6651936463967185,1.6651936463967185,-1.378792177464875E-9,4]
[null,"URA3B4","Short Rural",11,"URA",0,113.39,0.99779168820230413,0.94790210379218887,2.7258495994276717,2.7258495994276717,113.95399999999999,1.4567086404892582,1.3838732084647951,2.7258495994276717,2.5587586580215023,-1.378792177464875E-9,4]
[null,"WAR2123","Short Rural",11,"WAR",0,62.412999999999997,1.0490786631346709,0.88461166752513343,3.5163402674940318,0.80878112459428719,65.003,0.8335588648508041,0.65876157089159049,3.5163402674940318,0.80878112459428719,-7.2331329211782092E-2,4]
[null,"WAR2124","Short Rural",11,"WAR",0,60.399000000000001,0.50002814784923566,0.42163733685777388,3.5163402674940318,1.2717583054574482,60.274999999999999,0.41677943242540205,0.32938078544579524,3.5163402674940318,1.2717583054574482,-7.2331329211782092E-2,4]
[null,"WBG3B1","Short Rural",11,"WBG",0,6.4660000000000002,0.55000000000000004,0.52414446828221761,6.763658403556466,6.763658403556466,0,"","","","",-5.8934682800675464E-10,4]
[null,"WBG3B2","Short Rural",11,"WBG",0,42.75,0.17,0.16200829019632179,6.763658403556466,6.763658403556466,0,"","","","",-5.8934682800675464E-10,4]
[null,"WBG3B3","Short Rural",11,"WBG",0,16.649999999999999,0.13,0.12388869250306961,6.763658403556466,6.763658403556466,0,"","","","",-5.8934682800675464E-10,4]
[null,"WBN3B2","Short Rural",11,"WBN",0,21.88,1.88,1.848570169370785,8.9547026751310952,2.0405290563968945,22.047000000000001,1.81,1.7195,8.9547026751310952,2.0405290563968945,-1.6894593834091906E-9,4]
[null,"WBN3B3","Short Rural",11,"WBN",0,104.43899999999999,2.02,1.9862296500686096,8.9547026751310952,3.4608973211437517,104.33799999999999,2.06,1.9569999999999999,8.9547026751310952,3.4608973211437517,-1.6894593834091906E-9,4]
[null,"WBN3B4","Short Rural",11,"WBN",0,31.736000000000001,0.82,0.80629124408725728,8.9547026751310952,1.7347354863206093,31.718,0.63,0.59849999999999992,8.9547026751310952,1.7347354863206093,-1.6894593834091906E-9,4]
[null,"WBN3B5","Short Rural",11,"WBN",0,15.768000000000001,1.71,1.6814122285234268,8.9547026751310952,1.8985874927166249,16.190000000000001,2.5,2.375,8.9547026751310952,1.8985874927166249,-1.6894593834091906E-9,4]
[null,"WBN3B6","Short Rural",11,"WBN",0,148.80000000000001,0.99,0.97344918493461552,8.9547026751310952,2.8378786456612275,148.97800000000001,0.78,0.74099999999999999,8.9547026751310952,2.8378786456612275,-1.6894593834091906E-9,4]
[null,"WBN3B7","Short Rural",11,"WBN",0,12.949,0.04,3.9331280199378406E-2,8.9547026751310952,4.0782002289613004,12.885,0,0,8.9547026751310952,4.0782002289613004,-1.6894593834091906E-9,4]
[null,"WBN3B8","Short Rural",11,"WBN",0,37.93,0.99,0.97344918493461552,8.9547026751310952,2.1100708963207846,38.08,2,1.9,8.9547026751310952,2.1100708963207846,-1.6894593834091906E-9,4]
[null,"WCK516","Short Rural",11,"WCK",0,56.42,2.0146623761160409,1.9139292573102389,2.1298855575593727,2.1298855575593727,56.503,2.0197918186516493,1.8582084731595174,2.1298855575593727,2.1298855575593727,9.8510063086315481E-3,3]
[null,"WCK519","Short Rural",11,"WCK",0,59.944000000000003,0.77839228168119756,0.7394726675971377,2.1298855575593727,2.1298855575593727,59.12,0.62683194371947726,0.57668538822191906,2.1298855575593727,2.1298855575593727,9.8510063086315481E-3,3]
[null,"WGA3B1","Short Rural",11,"WGA",0,25.344999999999999,1.3476783082900237,1.3476662610343042,9.0880705873138989,8.7498876671360755,25.466999999999999,1.1260991583747051,1.103577175207211,9.0880705873138989,8.7498876671360755,8.5187717541299204E-10,3]
[null,"WGA3B2","Short Rural",11,"WGA",0,24.771000000000001,1.6079196367874076,1.6079052631650665,9.0880705873138989,7.8210754215772651,24.513000000000002,1.4530311720963935,1.4239705486544656,9.0880705873138989,7.8210754215772651,8.5187717541299204E-10,3]
[null,"WGA3B3","Short Rural",11,"WGA",0,162.85599999999999,1.9982816295334833,1.9982637663612097,9.0880705873138989,9.0880705873138989,159.672,2.5428045511686888,2.491948460145315,9.0880705873138989,9.0880705873138989,8.5187717541299204E-10,3]
[null,"WGA3B4","Short Rural",11,"WGA",0,4.1829999999999998,0.47401099119166351,0.47400675388103114,9.0880705873138989,9.0880705873138989,4.2770000000000001,0.36325779302409839,0.3559926371636164,9.0880705873138989,9.0880705873138989,8.5187717541299204E-10,3]
[null,"WGA3B5","Short Rural",11,"WGA",0,10.340999999999999,2.2864059575127298,2.2863855187202677,9.0880705873138989,9.0880705873138989,10.848000000000001,2.17954675814459,2.1359558229816979,9.0880705873138989,9.0880705873138989,8.5187717541299204E-10,3]
[null,"WGA3B6","Short Rural",11,"WGA",0,26.882999999999999,3.1321902751292279,3.1321622756452454,9.0880705873138989,5.6033575675660749,27.074000000000002,2.9060623441927871,2.8479410973089312,9.0880705873138989,5.6033575675660749,8.5187717541299204E-10,3]
[null,"WGM4981","Long Rural",11,"WGM",0,467.70299999999997,2.512783505794443,2.32164842434746,6.6683956091401777,4.9546179375911512,468.012,1.6842567436415012,1.5158310692773511,6.6683956091401777,5.1384751308145882,4.6541320293914126E-2,5]
[null,"WGM4982","Short Rural",11,"WGM",0,35.234999999999999,3.4753417035786045,3.2109895546418499,6.6683956091401777,3.0036359079455686,36.369,2.5263851154622516,2.2737466039160266,6.6683956091401777,2.8321628779962498,4.6541320293914126E-2,3]
[null,"WGM4983","Short Rural",11,"WGM",0,120.506,3.3740197880223772,3.1173746988213877,4.5726141319818359,4.5726141319818359,141.02199999999999,5.6843665097900677,5.1159298588110609,4.5726141319818359,4.5726141319818359,4.6541320293914126E-2,3]
[null,"WGM4984","Urban",11,"WGM",0,4.3410000000000002,3.667853343135437,3.3888577807007279,6.763658403556466,4.8974602609413784,4.6749999999999998,3.2632474408054093,2.9369226967248685,4.5726141319818359,4.5726141319818359,4.6541320293914126E-2,1]
[null,"WGN32","Long Rural",11,"WGN",0,395.28,2.015864672366483,1.9150714387481589,3.583405274763098,2.0757762903309209,395.23500000000001,1.1007980600512863,1.0237421958476964,3.583405274763098,2.0757762903309209,2.8337609034178837E-3,5]
[null,"WGN42","Short Rural",11,"WGN",0,13.167,2.8624220150925654,2.719300914337937,3.583405274763098,2.2491545761685656,13.502000000000001,1.4257955825426183,1.3259898917646351,3.583405274763098,2.2491545761685656,2.8337609034178837E-3,3]
[null,"WGN52","Short Rural",11,"WGN",0,25.425999999999998,4.2137391734190741,4.00305221474812,2.7765294060571373,2.3044069969300125,26.835999999999999,1.9080499707555625,1.7744864728026732,2.7765294060571373,2.1824706200771637,2.8337609034178837E-3,3]
[null,"WGN62","Short Rural",11,"WGN",0,4.2510000000000003,0.78624013205684873,0.74692812545400622,2.7765294060571373,2.7765294060571373,4.5069999999999997,0.30402994039511716,0.28274784456745899,2.7765294060571373,2.7765294060571373,2.8337609034178837E-3,3]
[null,"WGN72","Long Rural",11,"WGN",0,314.08,0.88676881650557104,0.84243037568029244,2.7765294060571373,2.0938762212700159,314.30599999999998,0.97499256747399632,0.90674308775081658,2.7765294060571373,2.0938762212700159,2.8337609034178837E-3,5]
[null,"WGN82","Short Rural",11,"WGN",0,155.13300000000001,0.9269802902850599,0.88063127577080691,2.7765294060571373,2.1091182683766219,154.94399999999999,0.85967086594481401,0.79949390532867703,2.7765294060571373,2.1091182683766219,2.8337609034178837E-3,3]
[null,"WGT8B10","Short Rural",22,"WGT",0,127.50700000000001,0.1766641149808362,0.17665325281424687,7.2399723756379064,1.257468886295005,127.54300000000001,0.13521197132608226,0.13385985161282143,7.2399723756379064,1.257468886295005,1.3100968388162794E-3,3]
[null,"WGT8B2","Long Rural",22,"WGT",0,283.08300000000003,0.57906571021496311,0.57903010644669806,7.2399723756379064,2.5797164727930859,283.24299999999999,0.43460990783383574,0.43026380875549736,7.2399723756379064,2.5797164727930859,1.3100968388162794E-3,5]
[null,"WGT8B3","Short Rural",22,"WGT",0,8.3710000000000004,1.5409036695550713,1.5408089273242644,7.2399723756379064,3.7304910293418478,8.9600000000000009,1.2555397337421923,1.2429843364047704,7.2399723756379064,3.7304910293418478,1.3100968388162794E-3,3]
[null,"WGT8B4","Short Rural",22,"WGT",0,11.465,1.96293461089818,1.9628139201582986,7.2399723756379064,3.6066493966006732,11.862,1.6998076395278909,1.6828095631326121,7.2399723756379064,3.4980498109661049,1.3100968388162794E-3,3]
[null,"WGT8B5","Long Rural",22,"WGT",0,352.25099999999998,0.5594363641059813,0.55940196724511504,7.2399723756379064,2.0233817534019622,352.37900000000002,0.43460990783383574,0.43026380875549736,7.2399723756379064,2.0195712416253109,1.3100968388162794E-3,5]
[null,"WGT8B6","Long Rural",22,"WGT",0,316.858,0.58888038326945402,0.58884417604748962,7.2399723756379064,2.2310546452294711,317.23,0.49255789554501384,0.48763231658956369,7.2399723756379064,2.2310546452294711,1.3100968388162794E-3,5]
[null,"WGT8B7","Long Rural",22,"WGT",0,323.08,0.5496216910514905,0.5495878976443237,7.2399723756379064,2.4939799578184267,346.43900000000002,0.39597791602638366,0.3920181368661198,7.2399723756379064,2.4939799578184267,1.3100968388162794E-3,5]
[null,"WGT8B8","Long Rural",22,"WGT",0,244.952,0.32388421079819973,0.32386429682611928,7.2399723756379064,0.50108229862967624,248.81200000000001,0.27042394265216452,0.26771970322564287,7.2399723756379064,0.50108229862967624,1.3100968388162794E-3,5]
[null,"WGT8B9","Long Rural",22,"WGT",0,307.07,0.39258692217963603,0.39256278403165973,7.2399723756379064,1.613751737411923,308.80399999999997,0.30905593445961654,0.30596537511502037,7.2399723756379064,1.613751737411923,1.3100968388162794E-3,5]
[null,"WHI716","Short Rural",11,"WHI",0,72.123999999999995,1.1784116217565734,1.0502837000970169,5.1822960162460801,1.8538139793409696,69.774000000000001,0.9956013563639764,0.86915998410575135,5.1822960162460801,1.8538139793409696,-5.8023466250069376E-3,4]
[null,"WHI717","Short Rural",11,"WHI",0,81.929000000000002,2.4803663974069812,2.2106777881074304,5.1822960162460801,1.831903536625223,81.863,2.0817119269428597,1.8173345122211164,5.1822960162460801,1.831903536625223,-5.8023466250069376E-3,4]
[null,"WHI718","Short Rural",11,"WHI",0,5.016,1.0643717873930341,0.94864334202311196,5.1822960162460801,3.0617462125395045,5.0380000000000003,1.1585179419508089,1.0113861633230561,3.0617462125395045,3.0617462125395045,-5.8023466250069376E-3,4]
[null,"WHI719","Short Rural",11,"WHI",0,43.78,1.3019547756504077,1.1603940880104138,5.1822960162460801,1.1260062300005269,43.906999999999996,1.2671289990086971,1.1062036161345925,5.1822960162460801,1.1260062300005269,-5.8023466250069376E-3,4]
[null,"WJL3B1","Short Rural",11,"WJL",0,145.477,0.99159585404632333,0.94964162470311275,2.7765294060571373,1.7442617657622381,145.322,1.1301956910524673,1.0510819926787947,2.7765294060571373,1.7442617657622381,-1.89719369799597E-12,4]
[null,"WJL3B2","Short Rural",11,"WJL",0,112.235,0.58934470570677711,0.56440964487071799,2.7765294060571373,1.104095787284781,112.04600000000001,0.55595512651083501,0.51703826765507654,2.7765294060571373,1.5346836180464041,-1.89719369799597E-12,4]
[null,"WJL3B3","Long Rural",11,"WJL",0,317.31799999999998,0.77643826307400787,0.74358730990904109,2.1298855575593727,1.7385459980972604,318.03699999999998,0.98216145337760885,0.91341015164117623,2.1298855575593727,1.7385459980972604,-1.89719369799597E-12,6]
[null,"WLC2B1","Short Rural",6.6,"WLC",0,29.576000000000001,1.3874146141396702,1.2199988783349685,2.1098041604964193,0.90251971429991473,29.664000000000001,1.2785850167144961,1.1986734531698402,2.1098041604964193,0.89051660220346252,1.6650223347498126E-2,3]
[null,"WLC4B1","Long Rural",33,"WLC",0,810.976,0.50522100795002001,0.44425729463178126,5.3848247171751096,0.53442427667537706,777.048,0.45832500599152298,0.42967969311705279,5.3848247171751096,0.5801504179951954,1.6650223347498126E-2,5]
[null,"WLS8B1","Short Rural",22,"WLS_22",0,115.19499999999999,0.28913830954201702,0.26022447858781533,3.330387292793437,3.330387292793437,115.779,0.28746289927801688,0.26446586733577554,3.330387292793437,3.330387292793437,2.9277069949928389E-2,3]
[null,"WLS8B4","Long Rural",22,"WLS_22",0,337.3,0.36624185875322157,0.32961767287789945,3.2637033367020356,3.2637033367020356,338.06700000000001,0.52856081480151484,0.48627594961739368,3.330387292793437,3.2637033367020356,2.9277069949928389E-2,5]
[null,"WLS8B5","Long Rural",22,"WLS_22",0,274.90300000000002,0.58791456273543463,0.5291231064618912,5.10608578071305,5.10608578071305,91.819000000000003,0.24109791552349805,0.22181008228161822,5.5530588121142745,5.10608578071305,2.9277069949928389E-2,5]
[null,"WLS8B8","Long Rural",22,"WLS_22",0,358.74299999999999,0.69393194290084081,0.62453874861075676,3.2446507778187779,3.2446507778187779,357.67500000000001,0.77893172707591662,0.71661718890984327,3.330387292793437,3.2446507778187779,2.9277069949928389E-2,5]
[null,"WNA2V04","Short Rural",22,"WNA",0,45.162999999999997,2.25,2.2050000000000001,5.5530588121142745,2.1091182683766219,45.070999999999998,2.5529999999999999,2.5019399999999998,5.5530588121142745,2.1091182683766219,-3.1765004668660585E-2,4]
[null,"WNA2V05","Short Rural",22,"WNA",0,118.854,0.3,0.29399999999999998,0.75028976882268616,0.75028976882268616,113.229,0.34300000000000003,0.33613999999999999,0.75028976882268616,0.75028976882268616,-3.1765004668660585E-2,4]
[null,"WOO8642","Short Rural",11,"WOO",0,0,"","","","",314.899,3.65,3.649635,6.763658403556466,2.8388312736053898,5.4310044284994762E-9,3]
[null,"WRA2W08","Long Rural",22,"WRA",0,245.702,0.64687820795110318,0.63627469775596468,4.7882890985403117,2.5778112169047604,245.245,0.5669815978182029,0.51028343803638265,4.7882890985403117,2.5778112169047604,4.5723976984611253E-2,5]
[null,"WRA2W09","Long Rural",22,"WRA",0,241.88900000000001,0.78750390533177772,0.77459528422465262,5.5530588121142745,2.6978423378692828,241.69399999999999,0.73271468025736985,0.65944321223163294,5.5530588121142745,2.6978423378692828,4.5723976984611253E-2,5]
[null,"WRA2W10","Short Rural",22,"WRA",0,141.11199999999999,0.28125139476134919,0.27664117293737595,2.7008907472906039,2.1929495274629556,140.49600000000001,0.33146616487833402,0.29831954839050062,2.7008907472906039,2.1929495274629556,4.5723976984611253E-2,3]
[null,"WRA2W11","Short Rural",22,"WRA",0,9.5389999999999997,1.8937593913930848,1.8627172311116649,2.4657821706712051,2.4657821706712051,9.5109999999999992,1.5613800924532049,1.4052420832078845,2.4657821706712051,2.4657821706712051,4.5723976984611253E-2,3]
[null,"WTE3681","Urban",11,"WTE",0,5.6820000000000004,4.1535476098498698,3.9183124510293594,9.0880705873138989,6.3225916654090515,5.9109999999999996,3.7508778414214055,3.3757900572792652,9.0880705873138989,6.1711238222871536,6.3965197954206753E-3,1]
[null,"WTE3682","Short Rural",11,"WTE",0,15.55,3.1126824570235296,2.9363964430148419,9.0880705873138989,8.129726875486039,15.742000000000001,2.737127073469674,2.4634143661227066,9.0880705873138989,8.129726875486039,6.3965197954206753E-3,3]
[null,"WTE3683","Urban",11,"WTE",0,3.1120000000000001,3.4992895137875983,3.3011081031345193,6.6683956091401777,6.6683956091401777,3.1949999999999998,3.0412523038551935,2.7371270734696744,6.6683956091401777,6.6683956091401777,6.3965197954206753E-3,1]
[null,"WTE3684","Short Rural",11,"WTE",0,43.54,2.458424360961259,2.3191920951200022,9.0880705873138989,2.2672545071076602,43.706000000000003,2.0275015359034625,1.8247513823131163,9.0880705873138989,2.2672545071076602,6.3965197954206753E-3,3]
[null,"WTE3685","Short Rural",11,"WTE",0,54.744,1.7546012576215437,1.6552298420816145,9.0880705873138989,2.0567237314476632,54.539000000000001,1.1759508908240082,1.0583558017416075,9.0880705873138989,2.0567237314476632,6.3965197954206753E-3,3]
[null,"WTE3686","Urban",11,"WTE",0,10.856,4.906935720467029,4.6290326092112952,9.0880705873138989,7.0389678794195394,10.747,3.3859275649587821,3.0473348084629039,9.0880705873138989,7.0389678794195394,6.3965197954206753E-3,1]
[null,"WTE3687","Short Rural",11,"WTE",0,12.452999999999999,3.5885065268869991,3.3852723323929066,9.0880705873138989,6.8417738949778224,12.273999999999999,5.8797544541200413,5.291779008708037,9.0880705873138989,6.7970003816021665,6.3965197954206753E-3,3]
[null,"WTE3688","Urban",11,"WTE",0,2.1920000000000002,2.8747704220917947,2.7119584983258092,9.0880705873138989,9.0880705873138989,2.38,2.8385021502648473,2.5546519352383625,9.0880705873138989,9.0880705873138989,6.3965197954206753E-3,1]
[null,"WTR2Z07","Short Rural",22,"WTR",0,72.046999999999997,0.27,0.25650000000000001,4.8881245070885821,2.2729702747726379,72.626000000000005,0.68600000000000005,0.67227999999999999,4.8881245070885821,2.2729702747726379,-9.3602852734484543E-3,4]
[null,"WTR2Z08","Long Rural",22,"WTR",0,211.56800000000001,3.51,3.3344999999999998,4.8881245070885821,1.9433610060922801,212.06700000000001,3.5819999999999999,3.5103599999999999,4.8881245070885821,1.9433610060922801,-9.3602852734484543E-3,6]
[null,"WTR2Z09","Urban",22,"WTR",0,0.39200000000000002,2.06,1.9569999999999999,10.745643210157313,4.9003181447738671,0.39400000000000002,2.0960000000000001,2.0540799999999999,10.745643210157313,4.9003181447738671,-9.3602852734484543E-3,2]
[null,"WWA8B1","Short Rural",22,"WWA",0,43.155000000000001,0.72399999999999998,0.70975992130853827,12.536583745183533,7.3790560554856874,43.283000000000001,0.95299999999999996,0.90534999999999988,12.536583745183533,7.3790560554856874,2.6960681870130004E-3,3]
[null,"WWA8B2","Short Rural",22,"WWA",0,171.01400000000001,0.503,0.49310668566048999,12.536583745183533,7.1351833017799899,169.44499999999999,0.83799999999999997,0.79609999999999992,12.536583745183533,7.1351833017799899,2.6960681870130004E-3,3]
[null,"WWA8B3","Short Rural",22,"WWA",0,143.93600000000001,3.4289999999999998,3.3615563123853285,7.7113326824097008,7.323803634724241,143.84100000000001,4.3819999999999997,4.1628999999999996,7.7113326824097008,7.323803634724241,2.6960681870130004E-3,3]
[null,"WWA8B4","Short Rural",22,"WWA",0,120.045,2.4,2.352795319254823,7.7113326824097008,7.2761722375160973,122.626,5.03,4.7785000000000002,7.7113326824097008,7.2761722375160973,2.6960681870130004E-3,3]
[null,"WWA8B5","Short Rural",22,"WWA",0,73.905000000000001,1.714,1.6802879905011527,7.7113326824097008,7.6248340650797131,77.325000000000003,1.677,1.5931500000000001,7.7113326824097008,7.6248340650797131,2.6960681870130004E-3,3]
[null,"WWA8B6","Short Rural",22,"WWA",0,8.5570000000000004,1.6,1.5685302128365488,7.7113326824097008,7.7113326824097008,9.0530000000000008,1.7529999999999999,1.6653499999999999,7.7113326824097008,7.7113326824097008,2.6960681870130004E-3,3]
[null,"WWA8B7","Long Rural",22,"WWA",0,224.398,2.3620000000000001,2.3155427266999551,12.536583745183533,1.9262137030973485,224.494,2.82,2.6789999999999998,12.536583745183533,7.2228250726429755,2.6960681870130004E-3,5]
[null,"WWA8B8","Short Rural",22,"WWA",0,38.726999999999997,0.438,0.42938514576400522,12.536583745183533,7.4190664291405293,39.514000000000003,0.53300000000000003,0.50634999999999997,12.536583745183533,7.4190664291405293,2.6960681870130004E-3,3]
[null,"WWL8B1","Short Rural",22,"WWL",0,17.010000000000002,3.2252789135499444,3.0637184730079783,5.4276929746624392,4.4144778932507975,17.827999999999999,3.0510184612323572,2.9148515073075574,5.4276929746624392,4.4144778932507975,-1.941621663373444E-2,4]
[null,"WWL8B2","Long Rural",22,"WWL",0,839.85500000000002,1.8935508460196449,1.7986992325401678,4.2597711151187454,2.947430859239959,838.15599999999995,1.4238086152417666,1.3602640367435266,4.2597711151187454,3.0407883977679218,-1.941621663373444E-2,6]
[null,"WWL8B3","Long Rural",22,"WWL",0,652.02,1.56061882913707,1.4824444224232154,2.4657821706712051,2.4657821706712051,691.97199999999998,1.4238086152417666,1.3602640367435266,2.4657821706712051,2.4657821706712051,-1.941621663373444E-2,6]
[null,"WWL8B4","Short Rural",22,"WWL",0,34.685000000000002,3.5374026793773581,3.3602073574926208,7.0326805349880637,4.1648893718801228,35.447000000000003,3.4578209227300047,3.3034983749485649,7.0326805349880637,4.1648893718801228,-1.941621663373444E-2,4]
[null,"YAM3B1","Short Rural",11,"YAM",0,8.1609999999999996,0.76377474134627354,0.76377419380950662,2.1232171619502322,2.1232171619502322,8.1560000000000006,0.79243949501978805,0.77659070511939232,2.1232171619502322,2.1232171619502322,-1.87473151549464E-9,4]
[null,"YAM3B2","Urban",11,"YAM",0,2.774,0.91475346928681611,0.91475281351603721,2.7258495994276717,2.7258495994276717,2.9460000000000002,1.1073833968866269,1.0852357289488943,2.7258495994276717,2.7258495994276717,-1.87473151549464E-9,2]
[null,"YAM3B3","Short Rural",11,"YAM",0,5.556,1.2877597383163915,1.2877588151439356,2.7765294060571373,2.7765294060571373,5.9930000000000003,1.4324867794588476,1.4038370438696706,2.7765294060571373,2.7765294060571373,-1.87473151549464E-9,4]
[null,"YAM3B4","Short Rural",11,"YAM",0,13.428000000000001,2.7442604078604482,2.7442584405481112,2.7765294060571373,2.7765294060571373,13.673999999999999,2.7125813483369665,2.6583297213702273,2.7765294060571373,2.7765294060571373,-1.87473151549464E-9,4]
[null,"YAM3B5","Short Rural",11,"YAM",0,38.122999999999998,2.841952525939623,2.8419504885935134,2.7765294060571373,2.7765294060571373,38.585000000000001,3.7488483802859203,3.6738714126802017,2.7765294060571373,2.7765294060571373,-1.87473151549464E-9,4]
[null,"YAM3B6","Short Rural",11,"YAM",0,61.475000000000001,2.4511840536229244,2.451182296411905,8.0020747309682125,3.5895020936057414,62.655999999999999,2.7329003097477305,2.6782423035527758,8.0020747309682125,3.5895020936057414,-1.87473151549464E-9,4]
[null,"YAN2313","Short Rural",11,"YAN",0,18.731000000000002,0.46835023870329684,0.43336448339087824,2.7258495994276717,2.7258495994276717,19.056000000000001,0.35605515500066293,0.32141098841909843,2.7258495994276717,2.7258495994276717,1.9736404398742163E-2,3]
[null,"YAN2314","Short Rural",11,"YAN",0,20.277999999999999,1.2489339698754582,1.1556386223756754,2.7765294060571373,2.7765294060571373,20.702000000000002,1.1571792537521544,1.0445857123620697,2.7765294060571373,2.7765294060571373,1.9736404398742163E-2,3]
[null,"YAN2318","Short Rural",11,"YAN",0,10.965,0.98548696060485386,0.91187110046830644,2.7765294060571373,2.7765294060571373,10.246,0.44506894375082862,0.40176373552387296,2.7765294060571373,2.7765294060571373,1.9736404398742163E-2,3]
[null,"YAN2319","Short Rural",11,"YAN",0,18.138000000000002,0.61470968829807715,0.56879088445052772,2.7765294060571373,2.7765294060571373,18.163,0.53408273250099436,0.48211648262864759,2.7765294060571373,2.7765294060571373,1.9736404398742163E-2,3]
[null,"YAR3B1","Short Rural",11,"YAR",0,11.55,3.46,3.4599327045363863,9.011860351780868,9.011860351780868,10.891,2.667358243656071,2.4006224192904639,9.011860351780868,6.0806241675916803,2.7011371949197367E-9,3]
[null,"YAR3B2","Long Rural",11,"YAR",0,363.75700000000001,3.17,3.1699383449076142,9.011860351780868,7.440024243912112,364.40300000000002,2.5720954492397827,2.3148859043158043,9.011860351780868,4.9012707727180302,2.7011371949197367E-9,5]
[null,"YAR3B3","Urban",11,"YAR",0,1.0189999999999999,3.85,3.8499251192095629,9.011860351780868,9.011860351780868,1.0189999999999999,4.0010373654841063,3.6009336289356959,9.011860351780868,9.011860351780868,2.7011371949197367E-9,1]
[null,"YAS6232","Long Rural",22,"YAS",0,325.899,0.87008065655828182,0.8502582833185085,10.821853445690346,4.4906881287838285,324.245,0.872070907218221,0.8555015599810748,4.0715318333521591,4.0715318333521591,3.3369909020345061E-12,5]
[null,"YAS6242","Short Rural",22,"YAS",0,17.771999999999998,4.0403745430982285,3.9483258213870975,10.821853445690346,6.8493949185311251,18.332000000000001,3.3970203943965589,3.3324770069030243,13.832157749245052,6.8836895245209888,3.3369909020345061E-12,3]
[null,"YAS6252","Short Rural",22,"YAS",0,46.363999999999997,2.2902123028947878,2.2380361710337753,10.821853445690346,3.892437779849538,45.988999999999997,3.5541959648835637,3.4866662415507759,4.0715318333521591,3.9153008505094467,3.3369909020345061E-12,3]
[null,"YAS6262","Long Rural",22,"YAS",0,251.67400000000001,1.5601446255527813,1.5246010597435327,10.821853445690346,5.0374965687333235,248.453,2.1244052914211315,2.0840415908841301,5.4516991988553434,5.0222545216267171,3.3369909020345061E-12,5]
[null,"YAS6272","Short Rural",22,"YAS",0,37.744999999999997,3.8103532201000618,3.7235448959120889,10.821853445690346,4.7802870238093442,37.023000000000003,3.4771292335480002,3.4110637781105879,4.0715318333521591,4.0715318333521591,3.3369909020345061E-12,3]
[null,"YAS6282","Long Rural",22,"YAS",0,228.995,1.3001205212939844,1.2705008831196105,10.821853445690346,5.1441908984795655,229.11,2.5888337513117654,2.539645910036842,13.832157749245052,5.0717911747231854,3.3369909020345061E-12,5]
[null,"YEN3B2","Short Rural",11,"YEN",0,25.277000000000001,1.91,1.9058233072431148,6.1920816370587364,3.6447545143671887,25.341000000000001,1.3333333333333333,1.1954666666666665,3.6447545143671887,3.6447545143671887,-1.2401643594302934E-7,4]
[null,"YEN3B3","Short Rural",11,"YEN",0,48.048999999999999,1.66,1.6563699947767385,6.1920816370587364,3.8800536165754207,11.64,1.4285714285714286,1.2808571428571429,3.8800536165754207,3.8800536165754207,-1.2401643594302934E-7,4]
[null,"YEN3B5","Urban",11,"YEN",0,5.01,1.62,1.6164574647821184,6.1920816370587364,4.9641442170327812,5.3319999999999999,2.5714285714285716,2.3055428571428571,4.9641442170327812,4.9641442170327812,-1.2401643594302934E-7,2]
[null,"YEN3B6","Short Rural",11,"YEN",0,46.210999999999999,1.43,1.4268729473076722,6.1920816370587364,2.4815957945443086,46.110999999999997,1.2380952380952381,1.1100761904761904,2.4815957945443086,2.4815957945443086,-1.2401643594302934E-7,4]
[null,"YEN3B7","Short Rural",11,"YEN",0,59.877000000000002,2.17,2.165254752208146,6.1920816370587364,3.7095332145702646,87.900999999999996,3.4285714285714284,3.0740571428571424,3.7095332145702646,3.7095332145702646,-1.2401643594302934E-7,4]
[null,"YLI2H03","Short Rural",22,"YLI",0,142.99100000000001,0.67108514821882359,0.63753089080788239,3.4675657167528922,2.1853285039096524,142.52099999999999,0.47906142229094345,0.46948019384512457,3.4675657167528922,2.1853285039096524,2.7431407765473137E-9,3]
[null,"YLI2H08","Long Rural",22,"YLI",0,260.94799999999998,0.88545957056650337,0.84118659203817814,5.5530588121142745,2.2005705510162583,259.98,1.1027451607451906,1.0806902575302868,5.5530588121142745,2.2005705510162583,2.7431407765473137E-9,5]
[null,"YLI2H13","Short Rural",22,"YLI",0,111.28,0.49399323410552298,0.46929357240024683,5.5530588121142745,2.320601671980782,111.596,0.45194473801032398,0.4429058432501175,5.5530588121142745,2.320601671980782,2.7431407765473137E-9,3]
[null,"YLI2H18","Long Rural",22,"YLI",0,203.97499999999999,0.74565016468758183,0.70836765645320265,5.5530588121142745,2.2558229717777056,205.79,0.75926715985734428,0.74408181666019735,5.5530588121142745,2.2558229717777056,2.7431407765473137E-9,5]
[null,"YOU3B1","Long Rural",11,"YOU",0,218.328,1.8299006811126521,1.8281532023117859,7.2399723756379064,3.1408143319050241,217.55600000000001,1.9172646047348176,1.8980919586874694,7.2399723756379064,3.1408143319050241,-9.0484314940439594E-3,6]
[null,"YOU3B10","Short Rural",11,"YOU",0,0.433,0,0,7.2399723756379064,7.2399723756379064,0.433,0,0,11.936428140360917,11.936428140360917,-9.0484314940439594E-3,4]
[null,"YOU3B2","Short Rural",11,"YOU",0,8.0619999999999994,1.4157652638082099,1.4144132670517502,7.2399723756379064,6.2006552885562032,7.9589999999999996,1.5338116837878542,1.5184735669499756,6.2006552885562032,6.2006552885562032,-9.0484314940439594E-3,4]
[null,"YOU3B3","Long Rural",11,"YOU",0,386.85700000000003,2.1862497611188001,2.1841619838146071,7.2399723756379064,6.0091770717794635,387.15699999999998,1.8693329896164472,1.8506396597202828,7.2399723756379064,6.0091770717794635,-9.0484314940439594E-3,6]
[null,"YOU3B4","Short Rural",11,"YOU",0,12.026999999999999,3.4960734065468038,3.4927348023114644,7.2399723756379064,7.0389678794195394,12.45,3.8345292094696353,3.7961839173749388,5.9062932538098716,5.9062932538098716,-9.0484314940439594E-3,4]
[null,"YOU3B6","Short Rural",11,"YOU",0,69.326999999999998,2.8218994714000374,2.8192046751439648,7.2399723756379064,6.0625242366525853,66.298000000000002,2.492443986155263,2.4675195462937105,7.2399723756379064,6.0625242366525853,-9.0484314940439594E-3,4]
[null,"YOU3B7","Short Rural",11,"YOU",0,37.759,3.2841901697863918,3.2810539052016789,7.2399723756379064,5.9091511376423602,38.287999999999997,3.0676233675757083,3.0369471338999512,7.2399723756379064,5.9091511376423602,-9.0484314940439594E-3,4]
[null,"YOU3B8","Short Rural",11,"YOU",0,22.532,4.921469726571396,4.9167699283227506,7.2399723756379064,6.3673651787847074,23.241,5.2724776630207488,5.2197528863905411,6.6683956091401777,6.3673651787847074,-9.0484314940439594E-3,4]
[null,"YOU3B9","Long Rural",11,"YOU",0,236.512,0.7319602724450609,0.73126128092471432,7.2399723756379064,6.1806501017287818,236.30199999999999,0.64228364258616399,0.63586080616030238,7.2399723756379064,7.2399723756379064,-9.0484314940439594E-3,6]
[null,"GOG3B1","Short Rural",11,"GOG",0,14.250999999999999,2.2666423854681716,2.2649284520176916,9.0499654695473861,9.0499654695473861,0,"","","","",0.1587539769274019,3]
[null,"GOG3B2","Short Rural",11,"GOG",0,66.804000000000002,2.8151905426819304,2.8130618216840739,9.0499654695473861,9.0499654695473861,0,"","","","",0.1587539769274019,3]
[null,"GOG3B5","Short Rural",11,"GOG",0,3.2850000000000001,0,0,9.0499654695473861,9.0499654695473861,0,"","","","",0.1587539769274019,3]
[null,"GOG3B6","Long Rural",11,"GOG",0,272.02699999999999,1.4800450279541029,1.4789258841942003,9.0499654695473861,9.0499654695473861,0,"","","","",0.1587539769274019,5]
[null,"WOO3B1","Short Rural",11,"WOO",0,156.72800000000001,0.69,-0.68945346150052922,6.763658403556466,6.763658403556466,0,"","","","",5.4310044284994762E-9,3]
[null,"WOO3B2","Short Rural",11,"WOO",0,139.97300000000001,0.44,-0.43965148269598969,6.763658403556466,6.763658403556466,0,"","","","",5.4310044284994762E-9,3]
[null,"WOO3B3","Short Rural",11,"WOO",0,20.789000000000001,1.6,-1.5987326643490534,6.763658403556466,6.763658403556466,0,"","","","",5.4310044284994762E-9,3]
[null,"HLP3B4","Short Rural",11,"HLP",0,48.962000000000003,1.6645231191914478,1.6632582321792453,9.0880705873138989,9.0880705873138989,0,"","","","",1.3336234435651852E-2,3]
[null,"WLS3B1","Short Rural",11,"WLS_11",0,14.654999999999999,0.27078086353427055,0.26625259921467914,6.1920816370587364,6.1920816370587364,0,"","","","",-3.1556259650528579E-2,4]
[null,"WLS3B2","Short Rural",11,"WLS_11",0,7.0970000000000004,1.2475261212828892,1.2266637606676289,6.1920816370587364,6.1920816370587364,0,"","","","",-3.1556259650528579E-2,4]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.3 - AUGEX MODEL INPUTS - ASSET STATUS - SUBTRANSMISSION SUBSTATIONS, SUBTRANSMISSION SWITCHING STATIONS AND ZONE SUBSTATIONS"]
[null,"Substation ID","Subtransmission substation, subtransmission switching station, or zone substation","Primary type of area supplied by substation","Substation voltage",null,{"$f":"CRCP_y4","v":"2017-18"},null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2013-14"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2017-18 to 2018-19"},"Network segment ID"]
[null,null,null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "},null,null,null,null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Number of transformers as at 30 June \",\"Number of transformers as at 31 December \"))","v":"Number of transformers as at 30 June "},"Maximum demand \n(weather corrected at 50% PoE)",null,{"$f":"CONCATENATE(IF(dms_RPT=\"Financial\",\"Substation rating as at 30 June \",\"Substation rating as at 31 December \"))","v":"Substation rating as at 30 June "}]
[null,null,null,null,"Primary","Secondary",null,null,null,"tx name plate total\n(ONAN)","tx name plate total\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency",null,null,null,"tx name plate\n(ONAN)","tx name plate\n(in service)","tx normal cyclic total","Substation normal cyclic","N-1 emergency"]
[null,null," STS, SSW or ZSS ","CBD, Urban, Short rural, Long rural"," kV "," kV ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA ",null," MVA "," MW "," MVA ","MVA "," MVA "," MVA "," MVA "," % "]
[null,"ADA_11","ZSS","Short Rural",66,11,2,1.501443259556178,1.4890000000000001,13,13,14.3,14.3,5.5,2,1.3761745983631404,1.3620000000000001,13,13,14.3,14.3,5.5,0,11]
[null,"ADA_66","STS","Short Rural",66,33,1,1.7401464220714113,1.7330000000000001,5,5,5.5,5.5,5.5,1,2.422159320663162,2.3959999999999999,5,5,5.5,5.5,5.5,2.2262841554093657E-3,11]
[null,"ADE","ZSS","Short Rural",66,11,2,1.5318169230065783,1.498,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.6882838460713903,1.575,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,-1.5659343892107227E-11,12]
[null,"AVE","ZSS","Short Rural",66,11,2,11.568253670303195,11.568,36,40,44,44,22,2,10.781632653061225,10.566000000000001,36,40,44,44,22,-4.5792596720635184E-9,12]
[null,"ANN","ZSS","Long Rural",66,22,2,1.4956387381189815,1.4930000000000001,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.494,1.494,5,5,5.5,5.5,2.75,-1.0324886230313706E-4,12]
[null,"ARD","ZSS","Short Rural",66,11,2,0.79239760742210641,0.76900000000000002,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,0.78372685954993893,0.70699999999999996,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,7.7380018619637012E-12,11]
[null,"APA","ZSS","Short Rural",66,11,2,0.99149766208369816,0.97399999999999998,6,6,6.6000000000000005,6.6000000000000005,3.3,2,1.0347807301793044,0.95799999999999996,6,6,6.6000000000000005,6.6000000000000005,3.3,4.6744261672422463E-4,11]
[null,"AFD","ZSS","Short Rural",66,22,1,0.72421740756039144,0.68799999999999994,3,3,3.3000000000000003,3.3000000000000003,0,1,0.59285714285714286,0.58099999999999996,3,3,3.3000000000000003,3.3000000000000003,0,3.6805943253704038E-2,11]
[null,"AHY","ZSS","Short Rural",66,22,1,5.6496371741372498,5.56,7.5,7.5,8.25,8.25,0,1,6.0635416666666666,5.8209999999999997,7.5,7.5,8.25,8.25,0,-2.0765092695678045E-3,12]
[null,"ASM","ZSS","Short Rural",66,11,2,21.269469028216655,20.260000000000002,40,60,66,66,33,2,21.974594533287966,19.375,40,60,66,66,33,1.4092152310280369E-3,11]
[null,"ATA","ZSS","Short Rural",66,11,2,3.6115773951829202,3.431,13,13,14.3,14.3,5.5,2,3.7722222222222221,3.395,13,13,14.3,14.3,5.5,4.5163445077403279E-12,11]
[null,"BAL_11","ZSS","Short Rural",66,11,2,24.206083362505847,24.097000000000001,60,60,66,66,33,2,23.857142857142858,23.38,60,60,66,66,33,1.0202722675691061E-2,11]
[null,"BAL_132","STS","Short Rural",132,66,1,16.561833742623751,16.518000000000001,75,112,123.20000000000002,123.20000000000002,0,1,16.823711340206184,16.318999999999999,75,112,123.20000000000002,123.20000000000002,0,9.6497111849540452E-3,11]
[null,"BPT","ZSS","Urban",66,11,2,12.846552380266887,12.815,48,60,66,66,33,2,13.148979591836735,12.885999999999999,48,60,66,66,33,4.428728082394124E-2,11]
[null,"BAR","ZSS","Short Rural",66,22,2,5.9835822422851388,5.7859999999999996,20,26,28.6,28.6,11,2,6.3728997289972895,5.8789999999999996,20,26,28.6,28.6,11,-3.8595147731386808E-3,12]
[null,"BBA","ZSS","Short Rural",66,11,2,2.6379963405320179,2.5710000000000002,10,10,11,11,5.5,2,2.4638297872340424,2.3159999999999998,10,10,11,11,5.5,9.5640258909984255E-4,11]
[null,"BBY","ZSS","Short Rural",132,11,2,20.439553092205728,20.402000000000001,60,90,99.000000000000014,99.000000000000014,49.5,2,19.824964992998602,19.821000000000002,60,90,99.000000000000014,99.000000000000014,49.5,4.2205517178034941E-3,11]
[null,"BAT","ZSS","Short Rural",66,11,2,1.84337713590911,1.8129999999999999,10,10,11,11,5.5,2,2.0827600804317918,1.968,10,10,11,11,5.5,-2.1618055414211541E-2,12]
[null,"BEE","ZSS","Short Rural",33,11,2,10.19135110301918,9.5350000000000001,20,25,27.500000000000004,27.500000000000004,13.75,2,10.132229628036981,9.4250000000000007,20,25,27.500000000000004,27.500000000000004,13.75,9.888320294012631E-3,11]
[null,"BEG","STS","Short Rural",132,66,2,42.231361924525643,41.628999999999998,70,120,132,132,66,2,40.154649528017671,39.985999999999997,70,120,132,132,66,0,11]
[null,"BTA","ZSS","Short Rural",66,11,2,1.3180115159277555,1.216,5.3,5.3,5.83,5.83,2.75,2,1.1755555555555557,1.0580000000000001,5.3,5.3,5.83,5.83,2.75,6.2571702866993706E-8,11]
[null,"BMR","ZSS","Short Rural",66,11,2,0.70666481397438619,0.68100000000000005,4,4,4.4000000000000004,4.4000000000000004,1.1000000000000001,2,0.67551020408163265,0.66200000000000003,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,8.8022419959372464E-3,11]
[null,"BMU","ZSS","Long Rural",66,11,1,1.7237407229595638,1.581,2.8,2.8,3.08,3.08,0,1,1.5623529411764707,1.3280000000000001,2.8,2.8,3.08,3.08,0,-2.0631382200464905E-11,12]
[null,"BER","ZSS","Short Rural",33,11,2,3.0864309179904796,3.0619999999999998,10,10,11,11,5.5,2,2.9916507393622376,2.9740000000000002,10,10,11,11,5.5,1.2677560132266734E-8,11]
[null,"BET","ZSS","Short Rural",66,11,2,0.74916565139585245,0.71699999999999997,6,6,6.6000000000000005,6.6000000000000005,3.3,2,0.82852872090540253,0.77600000000000002,6,6,6.6000000000000005,6.6000000000000005,3.3,-2.1608159752800993E-2,12]
[null,"BGA","ZSS","Short Rural",66,22,2,2.6336827543978241,2.5019999999999998,10.5,10.5,11.55,11.55,3.3,2,2.4153061224489796,2.367,10.5,10.5,11.55,11.55,3.3,2.4003459312308251E-9,11]
[null,"BNY","ZSS","Short Rural",66,11,2,11.49159650823162,11.404,28,40,44,44,22,2,11.112797167425391,10.984999999999999,28,40,44,44,22,-6.1674117608842369E-3,12]
[null,"BCW","ZSS","Urban",33,11,1,5.1049999239295731,4.0839999999999996,5,8,8.8000000000000007,8.8000000000000007,0,1,0,0,5,8,8.8000000000000007,8.8000000000000007,0,-4.0659757437604267E-5,12]
[null,"BBS_11","ZSS","Short Rural",132,11,1,9.9837362051044796,9.9730000000000008,30,30,33,33,33,1,8.5525773195876287,8.2959999999999994,30,30,33,33,33,3.2595032079466096E-2,11]
[null,"BBS_66","STS","Short Rural",132,66,1,8.7935800882794872,8.7889999999999997,30,30,33,33,33,1,8.3494736842105279,7.9320000000000004,30,30,33,33,33,1.1819880650352909E-4,11]
[null,"BOD","ZSS","Short Rural",33,11,2,1.4195575204520814,1.41,6,7,7.7000000000000011,7.7000000000000011,3.3,2,1.505328596802842,1.3560000000000001,6,7,7.7000000000000011,7.7000000000000011,3.3,5.4256278117838511E-8,11]
[null,"BBI","ZSS","Short Rural",66,11,2,4.5798995509599676,4.5119999999999996,15,16.5,18.150000000000002,18.150000000000002,7.15,2,5.8043956043956042,5.282,15,16.5,18.150000000000002,18.150000000000002,7.15,3.2263901545654818E-2,11]
[null,"BNK","ZSS","Short Rural",66,11,2,6.314645830900667,6.2190000000000003,10,14,15.400000000000002,15.400000000000002,7.7,2,2.8411111111111111,2.5569999999999999,10,14,15.400000000000002,15.400000000000002,7.7,1.4037803698992235E-2,11]
[null,"BOM","ZSS","Short Rural",66,22,2,4.7563552152372734,4.7510000000000003,20,29,31.900000000000002,31.900000000000002,14.3,2,4.290909090909091,4.2480000000000002,20,29,31.900000000000002,31.900000000000002,14.3,2.1459260890154163E-2,11]
[null,"BBN","ZSS","Urban",66,11,2,11.632467648939773,11.531000000000001,40,60,66,66,33,2,12.658923156148076,11.061999999999999,40,60,66,66,33,2.0492676826217446E-2,11]
[null,"BON","ZSS","Short Rural",33,11,2,0.96111058746023381,0.86499999999999999,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,0.72631578947368414,0.69,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,7.1546892405346021E-2,11]
[null,"BRL","ZSS","Short Rural",33,11,2,2.1020982004213864,1.9970000000000001,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.7,1.5640000000000001,5,5,5.5,5.5,2.75,6.9283989129884094E-2,11]
[null,"BOO","ZSS","Short Rural",66,11,2,3.2885978111533243,3.2,10,10,11,11,5.5,2,3.2715789473684214,3.1080000000000001,10,13,14.3,14.3,5.5,3.0469379630147848E-2,11]
[null,"BWA","ZSS","Urban",33,11,2,4.1457601654160783,3.99,10,10,11,11,5.5,2,3.958947368421053,3.7610000000000001,10,10,11,11,5.5,-7.9436509180213898E-3,12]
[null,"BPM","ZSS","Urban",33,11,2,20.016274222759353,19.946999999999999,40,60,66,66,33,2,18.733673469387757,18.359000000000002,40,60,66,66,33,3.5402833183294444E-11,11]
[null,"BTS","ZSS","Short Rural",66,22,2,20.073573328961679,20.05,45,60,66,66,33,0,0,0,0,0,0,0,0,-4.6488205352926354E-3,12]
[null,"BST","STS","Short Rural",66,33,2,5.0178947368421056,4.7670000000000003,22.5,22.5,24.750000000000004,24.750000000000004,8.25,2,4.5842105263157897,4.3550000000000004,22.5,22.5,24.750000000000004,24.750000000000004,8.25,1.6818620698069251E-2,11]
[null,"BKE_22","ZSS","Short Rural",66,22,2,8.2117744506925234,7.9939999999999998,20,20,22,22,11,2,7.7637795275590546,7.3949999999999996,20,20,22,22,11,4.1355205294676698E-5,11]
[null,"BKE_33","ZSS","Long Rural",66,33,1,3.0632064446896901,2.1469999999999998,5,8,8.8000000000000007,8.8000000000000007,0,1,4.2444444444444445,1.91,5,8,8.8000000000000007,8.8000000000000007,0,0,11]
[null,"BOU","ZSS","Short Rural",66,11,2,11.874431581255314,11.555999999999999,20,26,28.6,28.6,14.3,2,12.520594843265219,11.702999999999999,20,20,22,22,11,-1.0463506034967681E-2,12]
[null,"BRE","ZSS","Short Rural",66,22,1,2.9770784451152243,2.97,6.5,8,8.8000000000000007,8.8000000000000007,0,1,2.7262626262626259,2.6989999999999998,6.5,8,8.8000000000000007,8.8000000000000007,0,-1.7055363524815418E-12,12]
[null,"BRI","ZSS","Long Rural",33,22,2,2.1469940855494642,2.1419999999999999,5,5,5.5,5.5,2.75,2,2.0222405271828667,1.964,5,5,5.5,5.5,2.75,4.622854386858246E-2,11]
[null,"BRO","ZSS","Short Rural",33,11,1,0.72393040985391555,0.69,3,3,3.3000000000000003,3.3000000000000003,0,1,0.63589412524209166,0.59099999999999997,3,3,3.3000000000000003,3.3000000000000003,0,4.2897323643723353E-2,11]
[null,"BLH","ZSS","Short Rural",33,11,2,3.8590060667556672,3.7050000000000001,10,13,14.3,14.3,7.15,2,3.5214285714285718,2.9580000000000002,10,12.5,13.750000000000002,13.750000000000002,6.875,1.207014535833777E-10,11]
[null,"BUL","ZSS","Short Rural",66,22,1,0.35182843983025319,0.34799999999999998,2.5,2.5,2.75,2.75,0,1,0.26836734693877551,0.26300000000000001,2.5,2.5,2.75,2.75,0,-1.0782195568307161E-2,12]
[null,"BFT","ZSS","Urban",33,11,1,0.93882844100483087,0.93200000000000005,5,6.25,6.8750000000000009,6.8750000000000009,0,1,0.93157894736842106,0.88500000000000001,5,6.25,6.8750000000000009,6.8750000000000009,0,8.2778654621569071E-3,11]
[null,"BPO","ZSS","Short Rural",33,11,1,1.2548261540462808,1.2470000000000001,5,6.25,6.8750000000000009,6.8750000000000009,0,1,1.2367704868460843,1.2270000000000001,5,6.25,6.8750000000000009,6.8750000000000009,0,7.6039160398502495E-3,11]
[null,"BDA","ZSS","Short Rural",66,22,1,1.1738096445474679,0.80500000000000005,3,3,3.3000000000000003,3.3000000000000003,0,1,0.96736842105263166,0.91900000000000004,3,3,3.3000000000000003,3.3000000000000003,0,-1.4288845607839393E-2,12]
[null,"BUN","ZSS","Short Rural",66,11,2,8.0739746256746567,8.0570000000000004,15,20,22,22,11,2,8.3694665725521844,8.3000000000000007,15,20,22,22,11,8.2801307925803522E-3,11]
[null,"BNG","ZSS","Short Rural",66,22,2,10.35907273731968,9.9359999999999999,60,60,66,66,33,2,9.0012942191544436,8.3460000000000001,60,60,66,66,33,-7.1706297624718847E-3,12]
[null,"BRG","ZSS","Long Rural",33,11,1,0.5465609141518285,0.46899999999999997,2.5,2.5,2.75,2.75,0,2,0.68701298701298708,0.52900000000000003,0.5,0.5,0.55000000000000004,0.55000000000000004,0.27500000000000002,-1.3321445956121525E-2,12]
[null,"BJN","ZSS","Long Rural",66,22,2,2.3296730264793566,2.323,10,10,11,11,5.5,2,2.3464646464646464,2.323,10,10,11,11,5.5,-5.7100833642474537E-3,12]
[null,"BYA","ZSS","Short Rural",33,11,2,1.7092088566940085,1.5780000000000001,5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.5620689655172413,1.359,5,5.75,6.3250000000000002,6.3250000000000002,2.75,2.2648599179423967E-2,11]
[null,"BYR","ZSS","Short Rural",66,22,2,0.10702479144400467,0.10100000000000001,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,2,8.3333333333333343E-2,0.08,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,4.0805081164307595E-2,11]
[null,"CWD","ZSS","Short Rural",66,11,2,6.392781121349401,6.1189999999999998,13,13,14.3,14.3,5.5,2,6.5836956521739136,6.0570000000000004,13,13,14.3,14.3,5.5,3.3597856977992373E-3,11]
[null,"CFL","ZSS","Long Rural",66,22,2,3.291578566164056,3.2869999999999999,10,10,11,11,5.5,2,3.1430010070493455,3.121,10,10,11,11,5.5,2.6504691260260515E-5,11]
[null,"CAR","ZSS","Short Rural",33,11,2,0.89018674411054755,0.77800000000000002,3,3,3.3000000000000003,3.3000000000000003,1.65,2,0.8318284424379232,0.73699999999999999,3,3,3.3000000000000003,3.3000000000000003,1.65,1.1996425695580836E-6,11]
[null,"CNA","ZSS","Short Rural",33,11,2,1.1948795345951946,1.028,4.5,4.5,4.95,4.95,2.2000000000000002,2,1.1824999999999999,0.94599999999999995,5,5,5.5,5.5,2.2000000000000002,1.7298696401315827E-2,11]
[null,"CHI","ZSS","Short Rural",66,11,2,7.9115850368072884,7.6150000000000002,13.5,20,22,22,11,2,8.1049431370341178,7.1980000000000004,13.5,20,22,22,11,1.3341632112329211E-2,11]
[null,"CHI_33","STS","Short Rural",11,33,2,1.8266219914870112,1.784,9,9,9.9,9.9,4.4000000000000004,2,2.0544811811187356,1.976,9,9,9.9,9.9,4.4000000000000004,-2.4445342524331344E-2,12]
[null,"CSO_66","STS","Short Rural",132,66,1,29.13924516297995,28.539000000000001,35,60,66,66,0,1,26.41958762886598,25.626999999999999,35,60,66,66,0,2.9404526381544235E-3,11]
[null,"CSO_11","ZSS","Short Rural",66,11,2,22.920604115565251,22.690999999999999,40,60,66,66,33,2,23.038775510204083,22.577999999999999,40,60,66,66,33,-8.7865259488469315E-9,12]
[null,"CSO_33","STS","Short Rural",66,33,2,3.5335546788170902,3.45,11.5,11.5,12.65,12.65,3.85,2,3.0812500000000003,2.9580000000000002,11.5,11.5,12.65,12.65,3.85,7.8525720236942627E-10,11]
[null,"CPM","ZSS","Short Rural",33,11,2,18.86933617994184,18.849,40,60,66,66,33,2,16.702020202020201,16.535,40,60,66,66,33,1.6948523219440594E-2,11]
[null,"CST","ZSS","Urban",66,11,2,15.512067795726008,14.84,35,49,53.900000000000006,53.900000000000006,20.9,2,15.102232422282496,14.477,35,49,53.900000000000006,53.900000000000006,20.9,4.6296722437253791E-4,11]
[null,"CBC","ZSS","Long Rural",132,11,2,18.652063385862117,18.059000000000001,38,38,41.800000000000004,41.800000000000004,20.9,2,18.422105263157896,17.501000000000001,30,30,33,33,16.5,2.6706904662701588E-2,11]
[null,"CBE","ZSS","Urban",132,11,2,11.062669289452863,11.038,30,30,33,33,16.5,2,11.714548379682833,10.194000000000001,30,30,33,33,16.5,1.6305938051228508E-3,11]
[null,"CBP","ZSS","Urban",132,11,2,12.835804919939219,11.984999999999999,30,44,48.400000000000006,48.400000000000006,24.2,2,15.287058823529412,12.994,30,44,48.400000000000006,48.400000000000006,24.2,2.5953684815395117E-2,11]
[null,"CBR","ZSS","Short Rural",66,22,2,6.6431578947368424,6.3109999999999999,20,26,28.6,28.6,14.3,2,6.6294736842105264,6.298,20,26,28.6,28.6,14.3,-8.7542260372801377E-3,12]
[null,"COB","ZSS","Short Rural",33,11,2,1.4702187480290443,1.444,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.3371150729335495,1.32,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2.9363166754222871E-2,11]
[null,"CFN","ZSS","Urban",66,11,3,24.545829920046078,24.382999999999999,45,71,78.100000000000009,78.100000000000009,50.6,3,23.927551020408167,23.449000000000002,45,71,78.100000000000009,78.100000000000009,50.6,4.3412710250305728E-2,11]
[null,"CHS","ZSS","Short Rural",66,11,2,24.183820371698953,23.411000000000001,40,60,66,66,33,2,23.649390243902442,23.271000000000001,32,47,51.7,51.7,25.3,5.3737333510736627E-3,11]
[null,"CLY","STS","Short Rural",132,33,2,12.639550265806756,11.446999999999999,35,50,55.000000000000007,55.000000000000007,27.5,2,15.7541567695962,13.265000000000001,35,50,55.000000000000007,55.000000000000007,27.5,2.1610255017645253E-8,11]
[null,"CBY","ZSS","Short Rural",33,11,2,2.0698610017637891,1.8740000000000001,15,15,16.5,16.5,8.25,2,5.5860759493670891,4.4130000000000003,15,15,16.5,16.5,8.25,-6.634397531592744E-3,12]
[null,"CBL","ZSS","Short Rural",33,11,2,1.1958233710136037,1.095,4.5,4.5,4.95,4.95,1.65,2,1.168235294117647,0.99299999999999999,3,3,3.3000000000000003,3.3000000000000003,1.65,7.9910171218784646E-5,11]
[null,"CDN","ZSS","Long Rural",66,22,2,8.0837028269494446,7.7080000000000002,20,20,22,22,11,2,9.2122448979591844,9.0280000000000005,20,20,22,22,11,-4.0258007484222223E-2,12]
[null,"CLN","ZSS","Short Rural",66,11,2,4.5423177320359898,4.4790000000000001,16,16,17.600000000000001,17.600000000000001,8.8000000000000007,0,4.7624580136278478,4.4290859526738986,10,10,11,11,5.5,-2.4454083364751269E-2,12]
[null,"COO_11","ZSS","Short Rural",66,11,0,14.171201430091196,14.03,0,0,0,0,0,0,12.612521492869424,12.47,0,0,0,0,0,-6.0731643571309453E-3,12]
[null,"CBB","ZSS","Long Rural",66,22,2,9.0579934141005722,8.9450000000000003,20,20,22,22,11,2,8.887755102040817,8.7100000000000009,20,26,28.6,28.6,14.3,6.0816191290128437E-4,11]
[null,"CNB","ZSS","Short Rural",66,22,2,6.2072893409292522,6.1760000000000002,20,20,22,22,11,2,6.0061224489795917,5.8860000000000001,20,20,22,22,11,1.0071497962923391E-3,11]
[null,"CNK","ZSS","Short Rural",33,11,2,2.7595544536939651,2.665,10,14.5,15.950000000000001,15.950000000000001,7.15,2,2.510752688172043,2.335,10,14.5,15.950000000000001,15.950000000000001,7.15,1.2675980809492545E-8,11]
[null,"CTM","ZSS","Short Rural",66,11,2,10.820023745421739,10.775,30,38,41.800000000000004,41.800000000000004,20.9,2,10.962678375411635,9.9870000000000001,30,38,41.800000000000004,41.800000000000004,20.9,5.6643231600904259E-3,11]
[null,"CPD","ZSS","Short Rural",66,22,2,0.84736658102811702,0.80500000000000005,3,3,3.3000000000000003,3.3000000000000003,1.65,2,0.74183673469387756,0.72699999999999998,3,3,3.3000000000000003,3.3000000000000003,1.65,3.603764799355582E-2,11]
[null,"CRA","ZSS","Short Rural",132,22,2,17.703446441863054,16.917999999999999,57,60,66,66,33,2,17.811264294111361,16.666,47,60,66,66,33,7.1324351407621592E-3,11]
[null,"COW","ZSS","Short Rural",66,11,2,19.834458689008436,19.664999999999999,30,60,66,66,33,2,21.145263157894739,20.088000000000001,30,60,66,66,33,-8.1133405290337399E-12,12]
[null,"CHD","ZSS","Short Rural",33,11,2,1.8747906521958964,1.837,8,9,9.9,9.9,4.4000000000000004,2,0,0,7.5,8.25,9.0750000000000011,9.0750000000000011,3.5750000000000002,1.8508220679817639E-2,11]
[null,"CRO","ZSS","Long Rural",66,11,2,4.841459817688774,4.8159999999999998,15,20,22,22,11,2,4.3986770895971139,4.3890000000000002,15,20,22,22,11,4.5800472531305541E-3,11]
[null,"CUD_11","ZSS","Short Rural",66,11,2,12.838326058922462,12.776,60,60,66,66,33,2,11.618367346938776,11.385999999999999,60,60,66,66,33,-1.6855636882572502E-3,12]
[null,"CUD_33","ZSS","Short Rural",66,33,2,11.543444669811501,11.486000000000001,60,60,66,66,44,2,10.833673469387756,10.617000000000001,60,60,66,66,44,-1.0925338690146912E-2,12]
[null,"CCN","ZSS","Short Rural",66,11,2,3.8518144609251164,3.73,13,15,16.5,16.5,7.7,2,4.3464467005076148,4.1100000000000003,13,15,16.5,16.5,7.7,-1.6644868745720905E-2,12]
[null,"CMK","ZSS","Short Rural",66,11,2,1.5901375304301328,1.59,5,5,5.5,5.5,2.75,2,1.7378947368421054,1.651,5,5,5.5,5.5,2.75,-1.129368711092716E-2,12]
[null,"CLA","ZSS","Short Rural",66,11,1,1.3852581925951315,1.3160000000000001,3,3,3.3000000000000003,3.3000000000000003,0,2,1.4221052631578948,1.351,4,4,4.4000000000000004,4.4000000000000004,1.65,1.6082087138755217E-9,11]
[null,"DTN","ZSS","Short Rural",66,22,2,9.3194766187352034,8.8249999999999993,48,60,66,66,33,2,20.676448376308123,19.164999999999999,48,60,66,66,33,-7.1706297624720434E-3,12]
[null,"DPT","ZSS","Short Rural",33,11,2,4.4118856276085907,3.6120000000000001,20,26.5,29.150000000000002,29.150000000000002,13.75,2,4.1254085461808501,3.4079999999999999,20,22.5,24.750000000000004,24.750000000000004,11,1.7376151177270989E-2,11]
[null,"DEN","ZSS","Long Rural",66,22,2,21.843568971784091,20.8,36,60,66,66,33,2,21.947005829358773,20.707000000000001,36,60,66,66,33,-2.023633564774942E-3,12]
[null,"DOR","ZSS","Short Rural","132, 66",11,2,2.8884210526315792,2.7440000000000002,15,15,16.5,16.5,5.5,2,2.9063157894736844,2.7610000000000001,15,15,16.5,16.5,5.5,-1.7895469471319776E-2,12]
[null,"DUB","STS","Short Rural",132,66,3,63.822654408591937,61.427,90,135,148.5,148.5,99,3,64.892631578947373,61.648000000000003,90,135,148.5,148.5,99,-8.1238346510961474E-3,12]
[null,"PHS","ZSS","Urban",66,11,2,24.890104147163029,23.018000000000001,40,60,66,66,33,2,25.25714285714286,22.984000000000002,40,60,66,66,33,-2.5296058438408268E-8,12]
[null,"DBS","ZSS","Urban",132,11,2,17.499677006378437,17.026,60,60,66,66,33,2,16.84947368421053,16.007000000000001,60,60,66,66,33,2.2312017250554865E-2,11]
[null,"DBW","ZSS","Short Rural",132,11,2,15.472122462347295,14.846,30,46,50.6,50.6,25.3,2,14.276595744680852,13.42,25,33,36.300000000000004,36.300000000000004,16.5,8.8773968167260679E-3,11]
[null,"DNO","ZSS","Long Rural",66,22,2,5.3198388279591819,5.2789999999999999,15,15,16.5,16.5,8.25,2,4.855670103092784,4.71,15,20,22,22,11,5.4155769600972665E-4,11]
[null,"DUG","ZSS","Short Rural",33,11,2,8.4598678460546726,8.43,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,8.011340206185567,7.7709999999999999,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2.5500831223981241E-7,11]
[null,"DUN","ZSS","Short Rural",132,11,2,6.6963191252732956,6.6879999999999997,20,20,22,22,11,2,5.7795918367346939,5.6639999999999997,20,20,22,22,11,-5.6163006635975392E-3,12]
[null,"ESH","ZSS","Short Rural",66,11,2,4.9965052539699606,4.8259999999999996,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,4.9514664440037572,4.7439999999999998,20,32,35.200000000000003,35.200000000000003,17.600000000000001,0,11]
[null,"EDR","ZSS","Short Rural",66,11,2,2.6224290186035701,2.2589999999999999,10,10,11,11,5.5,2,2.920431043866333,2.6829999999999998,10,10,11,11,5.5,0.10184069306547298,11]
[null,"EGA","ZSS","Short Rural",33,11,2,1.3380066906118491,1.1830000000000001,7.5,7.5,8.25,8.25,2.75,2,1.4246418338108884,1.2430000000000001,7.5,7.5,8.25,8.25,2.75,-5.4325763083287245E-7,12]
[null,"ELL","ZSS","Short Rural",66,22,1,3.1871558363977259,3.1680000000000001,5,5,5.5,5.5,0,1,0,0,8,8,8.8000000000000007,8.8000000000000007,0,-7.1706297624706599E-3,12]
[null,"EME_11","ZSS","Short Rural",66,11,1,0.95578947368421063,0.90800000000000003,3,3,3.3000000000000003,3.3000000000000003,0,1,0.81030927835051547,0.78600000000000003,3,3,3.3000000000000003,3.3000000000000003,0,-4.8708168329081325E-4,12]
[null,"EME_22","ZSS","Short Rural",66,22,1,0.1810447439860432,0.17199999999999999,2.5,2.5,2.75,2.75,0,1,3.4020618556701035E-2,3.3000000000000002E-2,2.5,2.5,2.75,2.75,0,1.63370366122337E-2,11]
[null,"EUB","ZSS","Short Rural",33,11,2,1.5098259125404259,1.3819999999999999,5,5,5.5,5.5,1.1000000000000001,2,1.6877777777777776,1.5189999999999999,5,5,5.5,5.5,1.1000000000000001,-3.0649963261818954E-2,12]
[null,"EUC","ZSS","Short Rural",66,11,1,0.18940332699851672,0.17799999999999999,0.6,0.6,0.66,0.66,0,2,0.20979743695742042,0.20300000000000001,1.2,1.2,1.32,1.32,0.66,2.8891371806835747E-2,11]
[null,"EUL","ZSS","Short Rural",66,11,2,19.119904812446592,18.236999999999998,35,60,66,66,33,2,19.615053763440859,18.242000000000001,35,60,66,66,33,0,11]
[null,"EWE","ZSS","Short Rural",132,11,2,16.746376441049133,16.635999999999999,60,90,99.000000000000014,99.000000000000014,49.5,2,14.684693877551021,14.391,60,90,99.000000000000014,99.000000000000014,49.5,1.064220297536742E-2,11]
[null,"FFD","ZSS","Short Rural",66,11,0,0,0,0,0,0,0,0,2,4.5434782608695645,4.18,25,32,35.200000000000003,35.200000000000003,17.600000000000001,{"$error":"#N/A"},11]
[null,"FIN","ZSS","Long Rural",66,22,2,14.268226683238735,13.951000000000001,48,60,66,66,33,2,15.014678129586915,14.321,48,60,66,66,33,-1.2520246584434272E-2,12]
[null,"FBS","ZSS","Short Rural",66,11,2,14.422304180986561,14.359,33,60,66,66,33,2,14.871717171717172,14.723000000000001,33,60,66,66,33,5.2294710830278584E-10,11]
[null,"FHL","ZSS","Urban",66,11,2,6.8441884219352369,6.1139999999999999,15,20.9,22.990000000000002,22.990000000000002,7.59,2,7.3744636437434767,6.359,15,20.9,22.990000000000002,22.990000000000002,7.59,-1.3036310997015349E-2,12]
[null,"FOR","ZSS","Urban",66,11,2,16.84454175046967,16.835999999999999,30,50,55.000000000000007,55.000000000000007,27.5,2,16.177551020408163,15.853999999999999,30,50,55.000000000000007,55.000000000000007,27.5,-1.6359218092576427E-2,12]
[null,"GLS","ZSS","Short Rural",66,11,2,11.067023306720515,11.061999999999999,22.5,28.5,31.35,31.35,13.75,2,12.855102040816327,12.598000000000001,22.5,28.5,31.35,31.35,13.75,-1.8922271819264466E-2,12]
[null,"GAN","ZSS","Short Rural",33,11,1,0.50015507488031241,0.47499999999999998,2.5,2.5,2.75,2.75,0,1,0.56333333333333335,0.50700000000000001,2.5,2.5,2.75,2.75,0,-4.3783572313951039E-2,12]
[null,"GUE","ZSS","Short Rural",66,11,1,1.4029636383642816,1.3520000000000001,5,5,5.5,5.5,0,1,1.5290322580645159,1.4219999999999999,5,6.5,7.15,7.15,0,-6.9351393890255908E-11,12]
[null,"GID","ZSS","Short Rural",66,11,2,6.9355898079183556,6.73,16,24,26.400000000000002,26.400000000000002,13.2,2,7.291666666666667,7,16,24,26.400000000000002,26.400000000000002,13.2,-1.1184192852423298E-3,12]
[null,"GKO","ZSS","Short Rural",66,22,1,6.987424931939187,6.516,12.5,16,17.600000000000001,17.600000000000001,0,1,7.5550443641143605,6.8970000000000002,12.5,16,17.600000000000001,17.600000000000001,0,1.3260263890174854E-2,11]
[null,"GRB","ZSS","Short Rural",66,11,1,2.3184571611938432,1.901,10,12.5,13.750000000000002,13.750000000000002,0,1,1.5518457559369856,1.32,10,12.5,13.750000000000002,13.750000000000002,0,-2.8515120647688012E-13,12]
[null,"GNI","ZSS","Short Rural",66,11,2,8.3382038272541639,8.2590000000000003,30,40,44,44,22,2,8.0814432989690737,7.8390000000000004,30,40,44,44,22,6.1802037013924824E-7,11]
[null,"GLR","ZSS","Short Rural",33,11,2,9.1885336730647929,9.1560000000000006,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,8.7663265306122451,8.5909999999999993,20,26,28.6,28.6,11,2.1718732775233603E-13,11]
[null,"GDL","ZSS","Short Rural",66,11,2,12.891800943566764,12.778,40,60,66,66,33,2,11.033673469387756,10.813000000000001,40,60,66,66,33,3.6519432317881843E-2,11]
[null,"GDM","ZSS","Urban",66,11,2,1.9708489497650865,1.3819999999999999,17.5,22.5,24.750000000000004,24.750000000000004,11,2,3.5775510204081633,3.5059999999999998,17.5,22.5,24.750000000000004,24.750000000000004,11,3.9737476301020473E-2,11]
[null,"GOG","ZSS","Short Rural",132,11,1,5.4891506498660076,5.4850000000000003,30,30,33,33,0,0,0,0,0,0,0,0,0,0.1587539769274019,11]
[null,"GDI_22","ZSS","Long Rural",66,22,2,16.999180936450294,16.852,40,50,55.000000000000007,55.000000000000007,22,2,18.7248730964467,18.443999999999999,35,50,55.000000000000007,55.000000000000007,22,1.0918583097448253E-2,11]
[null,"GDI_33","ZSS","Short Rural",66,33,1,5.9213710856789001,5.9119999999999999,5,5,5.5,5.5,0,1,5.75204081632653,5.6369999999999996,5,5,5.5,5.5,0,1.8271961429889242E-2,11]
[null,"GOU_33","STS","Short Rural",132,33,2,8.8255776398678929,8.8030000000000008,30,60,66,66,33,2,8.9540764717782722,8.8520000000000003,30,60,66,66,33,5.7444375838291758E-3,11]
[null,"GOU_66","STS","Short Rural",132,66,2,39.949300390523,39.322000000000003,70,120,132,132,66,2,32.126139984617076,30.666,70,120,132,132,66,3.9276819747177699E-2,11]
[null,"GBN","ZSS","Short Rural",66,11,2,7.8917525440523173,7.883,27.5,35,38.5,38.5,17.600000000000001,2,6.8210976478973624,6.6989999999999998,27.5,35,38.5,38.5,17.600000000000001,4.5141952178377125E-2,11]
[null,"GRN","ZSS","Urban",66,11,2,17.663309608368358,17.413,39,55,60.500000000000007,60.500000000000007,27.5,2,16.463541666666668,15.805,39,55,60.500000000000007,60.500000000000007,27.5,5.8866076435834525E-3,11]
[null,"SGN","ZSS","Short Rural",66,11,2,18.808740710000198,17.934000000000001,30,49.5,54.45,54.45,26.95,2,17.273195876288661,16.754999999999999,30,49.5,54.45,54.45,26.95,1.6300013487306384E-3,11]
[null,"GNF","ZSS","Short Rural",66,11,2,4.8589449704302083,4.6159999999999997,13,13,14.3,14.3,5.5,2,5.1557894736842105,4.8979999999999997,13,13,14.3,14.3,5.5,-1.0951140848920016E-2,12]
[null,"GRS","ZSS","Short Rural",33,11,2,2.4325131868774403,2.3919999999999999,10,14.5,15.950000000000001,15.950000000000001,7.15,2,2.6984924623115578,2.6850000000000001,10,14.5,15.950000000000001,15.950000000000001,7.15,-4.8536813517790368E-3,12]
[null,"GFH","ZSS","Urban",33,11,2,28.50717798201109,27.661999999999999,100,100,110.00000000000001,110.00000000000001,55,2,28.977390582866629,27.94,80,100,110.00000000000001,110.00000000000001,55,3.3210249699695125E-11,11]
[null,"GGB","ZSS","Long Rural",66,22,1,1.6273669999302727,1.546,3,3,3.3000000000000003,3.3000000000000003,0,1,1.5885820663977661,1.536,3,3,3.3000000000000003,3.3000000000000003,0,1.6105720423742417E-3,11]
[null,"GGG","ZSS","Short Rural",66,22,1,3.2382602827375973,3.1789999999999998,5,5,5.5,5.5,0,1,4.5871274834437079,4.4329999999999998,5,5,5.5,5.5,0,2.702294703882108E-3,11]
[null,"GUN",{"$error":"#N/A"},"Short Rural",66,11,0,0,0,0,0,0,0,0,2,5.8689191768510467,5.5426072706181282,10,10,11,11,5.5,0,11]
[null,"GDG","ZSS","Short Rural",66,11,2,5.9129564708530795,5.78,16,16,17.600000000000001,17.600000000000001,8.8000000000000007,0,0,0,0,0,0,0,0,1.4641812133948176E-2,11]
[null,"GDH","ZSS","Short Rural",66,22,2,25.14537698238038,25.11,36,60,66,66,33,2,23.005050505050505,22.774999999999999,36,60,66,66,33,1.2295611912729525E-2,11]
[null,"GYA","ZSS","Long Rural",66,11,2,5.1630156210833862,4.9000000000000004,10,10,11,11,5.5,2,5.1979381443298971,5.0419999999999998,10,10,11,11,5.5,-1.516902527184246E-3,12]
[null,"HLP","ZSS","Short Rural",66,11,2,6.0150630292999487,6.0030000000000001,24,32,35.200000000000003,35.200000000000003,17.600000000000001,0,0,0,0,0,0,0,0,1.3336234435651852E-2,11]
[null,"HAM","ZSS","Urban",66,11,2,17.516153480972122,17.222000000000001,48,60,66,66,33,2,21.717160169200866,18.995999999999999,48,60,66,66,33,-1.520889858288531E-2,12]
[null,"HAN","ZSS","Urban",33,11,2,12.070351610708313,11.989000000000001,50,50,55.000000000000007,55.000000000000007,27.5,2,12.9783693843594,10.92,40,50,55.000000000000007,55.000000000000007,27.5,8.7820631757730572E-3,11]
[null,"HGN","ZSS","Short Rural",33,11,2,3.3042020194432178,3.2650000000000001,10,14.25,15.675000000000001,15.675000000000001,6.875,2,2.9333333333333336,2.64,10,14.25,15.675000000000001,15.675000000000001,6.875,1.7249808806619145E-2,11]
[null,"HPT","ZSS","Short Rural",33,11,2,11.134559169131728,11.089,30,33,36.300000000000004,36.300000000000004,16.5,2,10.333673469387756,10.127000000000001,30,30,33,33,16.5,1.7147745686360734E-4,11]
[null,"HKN","STS","Short Rural",132,33,1,10.409754611342423,10.307,50,50,55.000000000000007,55.000000000000007,0,1,8.085106382978724,7.98,50,50,55.000000000000007,55.000000000000007,0,2.3746730328295093E-2,11]
[null,"HAT","STS","Long Rural",132,33,2,13.458767643358984,13.105,48,60,66,66,33,2,9.0929203539823007,8.6310000000000002,48,60,66,66,33,9.8126072731200501E-3,11]
[null,"HAY","ZSS","Short Rural",33,11,2,6.1268807187834051,6.07,14.5,16.5,18.150000000000002,18.150000000000002,7.15,2,4.9843766835470316,4.7880000000000003,13,13,14.3,14.3,7.15,-8.5921920952062962E-3,12]
[null,"HEN","ZSS","Short Rural",66,11,2,2.3753493995398043,2.2999999999999998,10,10,11,11,5.5,2,2.6770386266094421,2.4950000000000001,10,10,11,11,5.5,-1.1967425302522311E-2,12]
[null,"HNC","STS","Short Rural",132,66,1,11.699678456260221,11.284000000000001,60,60,66,66,0,1,9.3096774193548377,8.6579999999999995,60,75,82.5,82.5,0,3.5750349213930499E-3,11]
[null,"HGE","ZSS","Short Rural",66,11,1,0.89607257887626246,0.73499999999999999,5,6.25,6.8750000000000009,6.8750000000000009,0,1,1.0044444444444445,0.90400000000000003,5,6.25,6.8750000000000009,6.8750000000000009,0,2.2088922878472323E-2,11]
[null,"HIL","STS","Long Rural",132,33,2,12.47385394583506,12.455,42,46,50.6,50.6,17.600000000000001,2,11.465669471278696,11.038,36.5,46,50.6,50.6,17.600000000000001,9.4957294124694957E-3,11]
[null,"HOL","ZSS","Short Rural",66,22,2,3.4290214957497653,3.3940000000000001,10,14,15.400000000000002,15.400000000000002,7.7,2,3.6356020942408378,3.472,10,14,15.400000000000002,15.400000000000002,7.7,-5.2805580401750502E-3,12]
[null,"IVA","ZSS","Long Rural",33,11,2,0.97535180574881641,0.95399999999999996,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,2,0.95750180953365738,0.92600000000000005,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,9.9861826325724507E-3,11]
[null,"ALJ","ZSS","Urban",132,22,2,43.289505602766546,43.109000000000002,60,88,96.800000000000011,96.800000000000011,48.4,2,48.572960223008472,45.304000000000002,60,88,96.800000000000011,96.800000000000011,48.4,-8.8022447416971333E-3,12]
[null,"JER","ZSS","Long Rural",66,22,2,5.1023582546067425,5.0949999999999998,17.600000000000001,20,22,22,11,2,5.46,5.46,17.600000000000001,20,22,22,11,1.5131656307212006E-2,11]
[null,"JIN_11","ZSS","Urban",66,11,2,15.845614873867083,15.837,30,60,66,66,33,2,14.690392923266819,14.282,30,60,66,66,33,5.0331228389908958E-4,11]
[null,"JIN_33","STS","Short Rural",66,33,1,0.79500000000000004,0.79500000000000004,15,15,16.5,16.5,0,1,0.79500000000000004,0.79500000000000004,10,10,11,11,0,8.2624050007568256E-3,11]
[null,"JYE","ZSS","Short Rural",66,11,2,4.6272722340131098,4.5590000000000002,16,20,22,22,11,2,3.9879739094985731,3.9129999999999998,16,20,22,22,11,1.7788741830794898E-2,11]
[null,"JNR","ZSS","Short Rural",66,11,1,1.2143569883820589,1.1200000000000001,3,3,3.3000000000000003,3.3000000000000003,0,1,0,0,3,3,3.3000000000000003,3.3000000000000003,0,1.3241566957842782E-2,11]
[null,"JGG","ZSS","Short Rural",66,11,2,2.1683755150139801,1.9590000000000001,11.8,12.75,14.025,14.025,6.875,2,1.9635343618513323,1.68,11.8,12.75,14.025,14.025,6.875,-9.1691456641609707E-14,12]
[null,"JUN","ZSS","Short Rural",66,11,2,6.1695826167203993,6.1680000000000001,25,33,36.300000000000004,36.300000000000004,16.5,2,6.3904196693514201,6.03,20,25,27.500000000000004,27.500000000000004,13.75,1.8720618955433881E-3,11]
[null,"JRF","ZSS","Short Rural",66,11,1,0.21220430920438577,0.19900000000000001,3,3,3.3000000000000003,3.3000000000000003,0,1,0.24330616996507567,0.20899999999999999,3,3,3.3000000000000003,3.3000000000000003,0,1.0754924388912304E-9,11]
[null,"KTE","ZSS","Short Rural",33,11,2,12.076404201744603,12.045,40,55,60.500000000000007,60.500000000000007,27.5,2,10.973684210526317,10.425000000000001,40,55,60.500000000000007,60.500000000000007,27.5,1.5356204462535857E-2,11]
[null,"KPT","ZSS","Urban",66,11,1,0.2115618072256783,0.19900000000000001,1,1,1.1000000000000001,1.1000000000000001,0,1,0.32663847780126853,0.309,1.5,1.5,1.6500000000000001,1.6500000000000001,0,-1.4967939107362509E-11,12]
[null,"KEW","ZSS","Short Rural",66,11,2,3.2466392938689856,3.1190000000000002,13,13,14.3,14.3,5.5,2,3.4935483870967743,3.2490000000000001,13,13,14.3,14.3,5.5,1.5452558305398079E-9,11]
[null,"KKN","ZSS","Short Rural",66,11,1,2.277300318708857,2.214,7.5,10,11,11,0,1,2.4947368421052634,2.37,5,6.9,7.5900000000000007,7.5900000000000007,0,4.5438326394111952E-9,11]
[null,"KOO","ZSS","Urban",66,11,2,18.39845184065247,17.655999999999999,36,50,55.000000000000007,55.000000000000007,27.5,2,18.6466887064093,17.484999999999999,36,50,55.000000000000007,55.000000000000007,27.5,-9.9663576578988425E-4,12]
[null,"KTL","ZSS","Short Rural",66,11,2,6.0239982999094455,5.7880000000000003,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,5.6010638297872344,5.2649999999999997,20,32,35.200000000000003,35.200000000000003,17.600000000000001,4.9572618281095667E-12,11]
[null,"KOR","ZSS","Short Rural",66,22,2,4.5319417826356707,4.4269999999999996,10,10,11,11,5.5,2,4.4889970376639869,4.2430000000000003,10,10,11,11,5.5,2.2299277129837979E-3,11]
[null,"KIS","ZSS","Short Rural",33,11,2,1.8402179405294403,1.7849999999999999,8.5,11.5,12.65,12.65,3.85,2,1.9063157894736842,1.8109999999999999,8.5,11.5,12.65,12.65,3.85,7.4545317727334672E-7,11]
[null,"KYG","ZSS","Short Rural",66,11,2,7.9941988110140993,7.6210000000000004,16,20,22,22,11,2,6.9817204301075266,6.4930000000000003,16,20,22,22,11,5.5053395170581105E-3,11]
[null,"KYW","ZSS","Short Rural",66,11,1,0.43102801274314101,0.40100000000000002,3,3,3.3000000000000003,3.3000000000000003,0,1,0.39723661485319511,0.34499999999999997,2.5,2.5,2.75,2.75,0,1.9755274035350114E-6,11]
[null,"LCO","ZSS","Short Rural",66,22,2,4.1245683922479106,4.08,13,13,14.3,14.3,5.5,2,3.988,3.988,13,15,16.5,16.5,7.7,6.7011420746839381E-3,11]
[null,"LKC","ZSS","Short Rural",33,11,2,5.6950577725421772,5.6340000000000003,15,21,23.1,23.1,5.5,2,5.1288659793814428,4.9749999999999996,15,21,23.1,23.1,5.5,1.3606130350422567E-2,11]
[null,"LRN","ZSS","Short Rural","66, 33",11,2,8.6835654306857215,8.5399999999999991,30,40,44,44,22,2,7.5708333333333337,7.2679999999999998,30,40,44,44,22,-1.1575441029890464E-2,12]
[null,"LEE","ZSS","Short Rural",33,11,2,20.253069983552322,18.863,30,50,55.000000000000007,55.000000000000007,27.5,2,20.942218185946192,18.448,30,50,55.000000000000007,55.000000000000007,27.5,2.4493450431886951E-3,11]
[null,"LHD","ZSS","Short Rural",132,11,2,6.037386390893686,6.0330000000000004,32,32,35.200000000000003,35.200000000000003,17.600000000000001,2,5.6061224489795913,5.4939999999999998,32,32,35.200000000000003,35.200000000000003,17.600000000000001,1.1046619425980153E-2,11]
[null,"LGR","ZSS","Short Rural",66,22,2,3.1635245092383326,3.141,13,13,14.3,14.3,5.5,2,3.1302083333333335,3.0049999999999999,13,13,14.3,14.3,5.5,-2.7531462329814255E-3,12]
[null,"LME","STS","Short Rural",132,66,3,87.042790604961183,83.391999999999996,240,360,396.00000000000006,396.00000000000006,264,3,86.131845841784994,84.926000000000002,240,360,396.00000000000006,396.00000000000006,264,-1.1644054296273534E-2,12]
[null,"ELI","ZSS","Short Rural",66,11,2,13.929954803500646,13.645,30,48,52.800000000000004,52.800000000000004,25.3,2,11.89558232931727,11.848000000000001,42,49.5,54.45,54.45,26.95,-1.117809511447931E-2,12]
[null,"SLI","ZSS","Urban",66,11,3,24.837519707239256,24.039000000000001,68,73,80.300000000000011,80.300000000000011,52.8,3,22.504081632653062,22.053999999999998,68,73,80.300000000000011,80.300000000000011,52.8,2.0660614101397193E-2,11]
[null,"LIU","ZSS","Short Rural",66,11,2,17.497088922549352,17.152000000000001,40,60,66,66,33,2,16.435789473684213,15.614000000000001,40,60,66,66,33,3.018703319138021E-12,11]
[null,"LOC","ZSS","Long Rural",66,22,2,2.975400812041967,2.9740000000000002,13,13,14.3,14.3,5.5,3,3.7782942603071947,3.7389999999999999,13,13,14.3,14.3,5.5,-1.571544268419194E-7,12]
[null,"MCV","ZSS","Short Rural",132,11,2,9.7858418138007597,9.718,48,60,66,66,33,2,8.8744897959183664,8.6969999999999992,48,60,66,66,33,-1.1313172947442639E-9,12]
[null,"MLN_11","ZSS","Short Rural",66,11,2,7.9400309621910461,7.9269999999999996,32,32,35.200000000000003,35.200000000000003,17.600000000000001,2,7.2663265306122451,7.1210000000000004,32,32,35.200000000000003,35.200000000000003,17.600000000000001,6.8784016167019292E-3,11]
[null,"MLN_33","STS","Short Rural",66,33,1,0.43052651049930535,0.40899999999999997,8,10,11,11,0,1,0.43368421052631578,0.41199999999999998,8,8,8.8000000000000007,8.8000000000000007,0,3.204834333500936E-2,11]
[null,"UNI","ZSS","Short Rural",66,11,2,10.158727921500574,10.109,20,28.5,31.35,31.35,13.75,2,12.465979381443299,12.092000000000001,20,28.5,31.35,31.35,13.75,8.6252327106734923E-3,11]
[null,"MAH","ZSS","Short Rural",66,11,2,15.872625453325584,15.744999999999999,48,60,66,66,33,2,14.378177966101696,13.695,48,60,66,66,33,3.0047419018678196E-3,11]
[null,"MGE","ZSS","Short Rural",33,11,2,1.4805952514698975,1.464,7.5,10.5,11.55,11.55,2.75,2,1.2785714285714285,1.2529999999999999,7.5,10.5,11.55,11.55,2.75,1.7332757829226497E-2,11]
[null,"MUA","ZSS","Short Rural",66,11,2,2.0199443464634927,1.9670000000000001,5.5,6.5,7.15,7.15,2.75,2,2.1455130137674603,2.1349999999999998,7.5,7.5,8.25,8.25,2.75,-1.4381301232469373E-2,12]
[null,"MDA","ZSS","Short Rural",132,11,2,11.230007685795886,10.768000000000001,36,48,52.800000000000004,52.800000000000004,26.4,2,11.111827956989247,10.334,36,48,52.800000000000004,52.800000000000004,26.4,7.3743641965842493E-3,11]
[null,"MLA","ZSS","Short Rural",66,11,2,5.2433319350114997,4.7190000000000003,10,12.5,13.750000000000002,13.750000000000002,6.875,2,0,0,10,12.5,13.750000000000002,13.750000000000002,6.875,4.4895282505084226E-2,11]
[null,"MAR","ZSS","Long Rural",66,11,2,1.5052274532105692,1.454,4,4,4.4000000000000004,4.4000000000000004,1.1000000000000001,2,1.3530927835051547,1.3,4,4,4.4000000000000004,4.4000000000000004,1.1000000000000001,9.7219884166048175E-3,11]
[null,"MCR","ZSS","Short Rural",33,11,2,3.6231969469400331,3.6019999999999999,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,2,3.3989690721649488,3.2970000000000002,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,1.0337352472287899E-2,11]
[null,"MRN","ZSS","Short Rural",66,22,2,5.4519192581061251,5.4390000000000001,25,30,33,33,16.5,2,1.6443399120564477,1.6080000000000001,25,30,33,33,16.5,5.6110267395684199E-2,11]
[null,"MUN_11","ZSS","Urban",33,11,0,0,0,0,0,0,0,0,2,1.2216720653318387,1.2216720653318387,3,3,3.3000000000000003,3.3000000000000003,1.65,{"$error":"#N/A"},11]
[null,"MUN","STS","Urban",66,33,1,8.4800134168658019,7.6360000000000001,15,15,16.5,16.5,0,1,7.8798547695015948,7.1619999999999999,15,15,16.5,16.5,0,1.3812866552133769E-2,11]
[null,"MGY","ZSS","Short Rural",33,11,1,0.65505827415228313,0.62,1,1,1.1000000000000001,1.1000000000000001,0,1,0.66187050359712229,0.59799999999999998,1,1,1.1000000000000001,1.1000000000000001,0,2.0640523003965846E-2,11]
[null,"MEN","ZSS","Short Rural",66,22,2,0.97739079108858684,0.92200000000000004,10,10,11,11,5.5,2,1.575,1.4490000000000001,9,10,11,11,5.5,0,11]
[null,"MWB","ZSS","Urban",66,22,1,2.806,2.806,5,5,5.5,5.5,0,1,3.0275510204081635,2.9670000000000001,5,5,5.5,5.5,0,1.6833504577804304E-2,11]
[null,"MLS","ZSS","Urban",66,11,2,14.737169761643491,14.387,22.5,32,35.200000000000003,35.200000000000003,17.600000000000001,2,8.6515463917525768,8.3919999999999995,22.5,32,35.200000000000003,35.200000000000003,17.600000000000001,1.564398406726988E-2,11]
[null,"MOA","ZSS","Short Rural",66,22,2,14.264029174328954,13.909000000000001,48,60,66,66,33,2,13.278399668325042,12.811,48,60,66,66,33,-4.3635035836797446E-3,12]
[null,"MLO","ZSS","Short Rural",66,11,2,3.4384045259891924,3.4049999999999998,11,11,12.100000000000001,12.100000000000001,3.3,1,0,0,5,5,5.5,5.5,0,1.0806146124880371E-2,11]
[null,"MON","ZSS","Urban",66,11,1,0.85794928247847779,0.82,1,1,1.1000000000000001,1.1000000000000001,0,1,0.91022727272727277,0.80100000000000005,1,1,1.1000000000000001,1.1000000000000001,0,-5.5443878542444766E-9,12]
[null,"MNE","ZSS","Short Rural",66,11,2,5.1895940494432251,5.1769999999999996,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,5.1642857142857146,5.0609999999999999,20,32,35.200000000000003,35.200000000000003,17.600000000000001,1.8313935207909287E-2,11]
[null,"MRE","ZSS","Short Rural",66,22,2,21.805671038324764,21.209,39,60,66,66,33,2,21.893684210526317,20.798999999999999,39,60,66,66,33,3.8747922506888635E-5,11]
[null,"MSW","ZSS","Urban",66,11,2,14.35883371081472,13.436999999999999,40,40,44,44,22,2,13.036437246963562,11.27,30,40,44,44,22,7.0052571221460233E-3,11]
[null,"MOR","STS","Short Rural",132,33,2,26.772487845584177,26.771999999999998,60,75,82.5,82.5,33,2,23.787971457696226,23.335999999999999,60,75,82.5,82.5,33,3.0718302369116298E-12,11]
[null,"MYT","ZSS","Short Rural",33,11,2,7.2198194293400562,7.0780000000000003,32,32,35.200000000000003,35.200000000000003,17.600000000000001,2,6.6417528411999589,6.4870000000000001,26,32,35.200000000000003,35.200000000000003,17.600000000000001,-6.9553432592323267E-3,12]
[null,"MVN","STS","Short Rural",132,66,1,7.4313105330671236,7.2869999999999999,30,30,33,33,0,0,0,0,0,0,0,0,0,-1.4340623478254014E-15,12]
[null,"MPT","ZSS","Short Rural",33,11,2,7.4707413772450115,7.4409999999999998,25,25,27.500000000000004,27.500000000000004,13.75,2,6.6043267286696326,6.5330000000000004,25,25,27.500000000000004,27.500000000000004,13.75,9.2482727313590602E-3,11]
[null,"MOU","ZSS","Long Rural",66,22,2,2.5859675658450452,2.5489999999999999,10,10,11,11,5.5,2,3.2827219328383022,2.9620000000000002,10,10,11,11,5.5,1.4059381103902049E-8,11]
[null,"MTG_33","ZSS","Long Rural",66,33,2,1.1539998074796169,1.105,3,3,3.3000000000000003,3.3000000000000003,1.65,2,0.96774193548387089,0.9,6.5,6.5,7.15,7.15,1.65,8.3021844373043652E-3,11]
[null,"MTG_6_6","ZSS","Short Rural",66,6.6,2,0.89668970100380718,0.88100000000000001,4,4,4.4000000000000004,4.4000000000000004,2.2000000000000002,2,1.4116177389131794,1.0129999999999999,3,3.5,3.8500000000000005,3.8500000000000005,1.65,1.1196435634343726E-2,11]
[null,"MUD","ZSS","Short Rural","132, 66",22,2,23.932245312180978,23.413,60,60,66,66,33,2,23.102105263157895,21.946999999999999,60,60,66,66,33,1.472707800495951E-2,11]
[null,"MUL_11","ZSS","Short Rural",132,11,2,8.0564521869164665,8.0399999999999991,26,26,28.6,28.6,11,2,7.8408163265306126,7.6840000000000002,26,26,28.6,28.6,11,-2.6343315471663638E-2,12]
[null,"MWA","ZSS","Urban",132,22,2,13.14646328972897,12.712,60,60,66,66,33,2,12.951995012468828,12.465,60,60,66,66,33,1.4584748047235196E-4,11]
[null,"MBL","ZSS","Short Rural",66,11,2,1.2736881181869262,1.21,5.3,5.3,5.83,5.83,2.75,2,1.474164133738602,1.3580000000000001,5.3,5.3,5.83,5.83,2.75,-2.8663841837645986E-2,12]
[null,"MGA","ZSS","Short Rural",33,11,2,1.4877342747432905,1.4550000000000001,5.5,6.25,6.8750000000000009,6.8750000000000009,3.3,2,1.1806122448979592,1.157,5.5,6.25,6.8750000000000009,6.8750000000000009,3.3,7.1815727021506406E-4,11]
[null,"MGI","ZSS","Long Rural",66,"22, 33",2,5.6863157894736842,5.4020000000000001,15.5,15.5,17.05,17.05,8.25,3,5.24,4.9779999999999998,25.5,25.5,28.05,28.05,17.05,-6.3469664617800863E-3,12]
[null,"MGH","ZSS","Short Rural",66,22,1,0.68007265641031822,0.59299999999999997,1,1,1.1000000000000001,1.1000000000000001,0,1,0.65828913995849669,0.57099999999999995,1,1,1.1000000000000001,1.1000000000000001,0,6.898627202006527E-3,11]
[null,"MUR","ZSS","Short Rural",33,11,2,0.74580793743206064,0.68700000000000006,10,10,11,11,5.5,2,0.74757281553398047,0.69299999999999995,10,10,11,11,5.5,1.6193892807575619E-6,11]
[null,"MBM","ZSS","Long Rural",132,22,1,6.2220020714445283,6.2220000000000004,10,12.5,13.750000000000002,13.750000000000002,0,1,5.6821364272854566,5.681,10,12.5,13.750000000000002,13.750000000000002,0,1.4228516945916717E-2,11]
[null,"MRH","ZSS","Short Rural",66,11,2,5.0252150377394766,4.7839999999999998,16,20,22,22,11,2,5.4615881213686244,5.0759999999999996,16,20,22,22,11,-1.352720297997603E-12,12]
[null,"MDI","ZSS","Short Rural",33,11,2,2.6296402989921273,2.5649999999999999,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,2,2.262626262626263,2.2400000000000002,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,2.6735018762460154E-3,11]
[null,"MWN","ZSS","Short Rural",66,11,2,17.935169005760223,17.318999999999999,30,50,55.000000000000007,55.000000000000007,27.5,2,16.853333333333332,15.228999999999999,30,50,55.000000000000007,55.000000000000007,27.5,-1.4241200508519343E-3,12]
[null,"NHD","ZSS","Short Rural",66,11,2,8.8660307120079089,8.8249999999999993,32,47,51.7,51.7,25.3,2,9.0868686868686872,8.9960000000000004,32,47.5,52.250000000000007,52.250000000000007,25.3,-3.906734492208578E-2,12]
[null,"NGN","ZSS","Short Rural",66,11,2,3.1631504112267592,3.0049999999999999,13,14.25,15.675000000000001,15.675000000000001,6.875,3,2.5760869565217392,2.37,13,14,15.400000000000002,15.400000000000002,6.6,1.7846107055534452E-3,11]
[null,"NAN","ZSS","Short Rural",66,11,2,1.2086890271148252,1.0900000000000001,3.8,3.8,4.18,4.18,1.1000000000000001,2,1.3613406795224976,1.1859999999999999,3.8,3.8,4.18,4.18,1.1000000000000001,-1.3257497085294091E-2,12]
[null,"NAR","ZSS","Short Rural",33,11,2,7.6918582911132809,7.6079999999999997,20,28.5,31.35,31.35,13.75,2,7.0463791700569569,6.9279999999999999,20,28.5,31.35,31.35,13.75,-3.674214335533341E-3,12]
[null,"NBI","ZSS","Short Rural",66,22,2,20.311666233977743,19.832999999999998,36,60,66,66,33,2,19.481521739130432,18.634,36,60,66,66,33,1.5209428285254338E-10,11]
[null,"NDA","ZSS","Short Rural",66,11,2,9.9290518164483874,9.6579999999999995,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,10.462439840970914,10,20,32,35.200000000000003,35.200000000000003,17.600000000000001,-1.0149906809839605E-3,12]
[null,"NME","ZSS","Short Rural",132,22,2,13.781097846675593,13.757999999999999,41,48,52.800000000000004,52.800000000000004,26.4,2,14.276842105263158,13.563000000000001,41,48,52.800000000000004,52.800000000000004,26.4,1.1648015341008439E-7,11]
[null,"NER","ZSS","Short Rural",33,11,1,1.8797731174183512,1.7290000000000001,8,8,8.8000000000000007,8.8000000000000007,0,1,2.2867155842733546,2.0880000000000001,8,8,8.8000000000000007,8.8000000000000007,0,-1.9159985861147668E-2,12]
[null,"NVE","ZSS","Short Rural","132, 66",22,2,9.216989836127329,8.9179999999999993,27,34,37.400000000000006,37.400000000000006,11,2,8.1283694435967853,7.9909999999999997,27,34,37.400000000000006,37.400000000000006,11,3.0900112931556666E-2,11]
[null,"NSK","ZSS","Short Rural",33,11,2,10.85340296226606,10.762,20,20,22,22,11,2,9.2377551020408166,9.0530000000000008,20,20,22,22,11,-3.6198551845436208E-3,12]
[null,"NDL","ZSS","Short Rural",66,11,2,1.6598128301062276,1.5389999999999999,5,5,5.5,5.5,2.75,2,1.9499999999999997,1.7549999999999999,5,5,5.5,5.5,2.75,1.3818430333111189E-2,11]
[null,"NYM","ZSS","Short Rural",66,11,2,0.50884398456170055,0.50700000000000001,1.2,1.2,1.32,1.32,0.66,2,0.62631578947368416,0.59499999999999997,1.2,1.2,1.32,1.32,0.66,0,11]
[null,"NYG","STS","Short Rural",132,66,2,32.164008425463621,32.033999999999999,48,75,82.5,82.5,33,2,29.169,29.169,48,75,82.5,82.5,33,1.2913398311444535E-2,11]
[null,"NYN","ZSS","Long Rural",66,22,2,7.5762926412428078,7.5650000000000004,20,20,22,22,11,2,6.5333333333333341,6.2720000000000002,20,20,22,22,11,4.5332988413981548E-2,11]
[null,"OES","ZSS","Urban",66,11,2,19.281708363730473,18.675000000000001,50,60,66,66,33,2,20.883421571680682,20.117000000000001,50,60,66,66,33,1.9866812569266214E-13,11]
[null,"OKY","ZSS","Short Rural",66,11,2,0.40526315789473688,0.38500000000000001,7,7,7.7000000000000011,7.7000000000000011,3.85,2,0.40104166666666669,0.38500000000000001,7,7,7.7000000000000011,7.7000000000000011,3.85,-1.9129839602184017E-2,12]
[null,"OBE","ZSS","Urban",132,11,2,29.421263762972625,24.954000000000001,50,90,99.000000000000014,99.000000000000014,49.5,2,27.755172413793101,24.146999999999998,50,90,99.000000000000014,99.000000000000014,49.5,-1.220165716882793E-2,12]
[null,"OBR","ZSS","Long Rural",66,11,2,5.8295195538122737,5.7489999999999997,20,30,33,33,16.5,2,5.4395099540581935,5.3280000000000003,20,30,33,33,16.5,-4.3189016092631477E-3,12]
[null,"ORI","ZSS","Short Rural",66,11,2,11.768472367224824,11.708,20,20,22,22,11,2,11.297308237198948,11.164,20,20,22,22,11,2.4966189146298051E-4,11]
[null,"ORN","ZSS","Urban",66,11,3,21.292421523121376,20.946000000000002,50,50,55.000000000000007,55.000000000000007,33,3,15.61618449500669,15.167999999999999,50,50,55.000000000000007,55.000000000000007,33,1.2599892872026169E-11,11]
[null,"ORS","ZSS","Urban",66,11,2,20.592113072283443,20.077000000000002,60,60,66,66,33,3,26.903662665435519,26.222999999999999,45,45,49.500000000000007,49.500000000000007,33,-3.2497853095867148E-2,12]
[null,"ORW","ZSS","Short Rural",66,11,2,14.174142435279846,14.064,60,60,66,66,33,2,13.780141843971633,13.601000000000001,60,60,66,66,33,1.6250434370809636E-9,11]
[null,"OUR_33","STS","Short Rural",11,33,2,1.6964555648857025,1.5569999999999999,6,6,6.6000000000000005,6.6000000000000005,2.2000000000000002,2,1.7522222222222221,1.577,6,6,6.6000000000000005,6.6000000000000005,2.2000000000000002,8.1069456969153179E-3,11]
[null,"OUR_11","ZSS","Short Rural",66,11,2,3.9738027918920391,3.7410000000000001,10,13.8,15.180000000000001,15.180000000000001,7.59,2,4.6247969680563079,4.2709999999999999,10,13.8,15.180000000000001,15.180000000000001,7.59,-1.2248298410292157E-2,12]
[null,"OPM","ZSS","Urban",33,11,2,16.873973613514554,16.646000000000001,30,40,44,44,22,2,16.417346938775509,16.088999999999999,30,40,44,44,22,1.7543718262201797E-11,11]
[null,"OXY","ZSS","Short Rural",66,11,2,18.812482909337721,18.385000000000002,40,60,66,66,33,2,14.327272727272726,14.183999999999999,40,60,66,66,33,1.9979836522744966E-2,11]
[null,"PPM","ZSS","Short Rural",33,11,2,4.7202063214550094,4.5970000000000004,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,2,4.2275510204081632,4.1429999999999998,10,16,17.600000000000001,17.600000000000001,8.8000000000000007,5.5042574708635732E-3,11]
[null,"PAM","ZSS","Short Rural",66,11,2,16.650420538081676,16.634,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,15.710855427713856,15.702999999999999,20,32,35.200000000000003,35.200000000000003,17.600000000000001,-5.3212919205567694E-3,12]
[null,"PKT","ZSS","Short Rural",66,11,2,19.593934941232796,18.731999999999999,60,60,66,66,33,2,19.586956521739129,18.02,60,60,66,66,33,9.1923232411651441E-4,11]
[null,"PCR","ZSS","Short Rural",66,11,1,0.11722361455950035,0.11700000000000001,3,3,3.3000000000000003,3.3000000000000003,0,1,0.129,0.129,3,3,3.3000000000000003,3.3000000000000003,0,-2.5196439408119862E-2,12]
[null,"PYB","ZSS","Short Rural",66,11,2,5.2304972229687445,4.9560000000000004,10,10,11,11,5.5,2,3.7222222222222223,3.35,10,10,11,11,5.5,2.039004751061611E-2,11]
[null,"PKH","ZSS","Short Rural",66,11,2,1.8242896628173171,1.77,10,10,11,11,5.5,2,1.8532608695652173,1.7050000000000001,10,10,11,11,5.5,-4.3182282173932504E-3,12]
[null,"PER","ZSS","Urban",33,11,2,11.457894736842105,10.885,16,20,22,22,11,2,11.656122448979593,11.423,16,20,22,22,11,-2.0753612962449455E-2,12]
[null,"PPL","STS","Short Rural",22,66,2,6.1393999544230855,5.9279999999999999,30,30,33,33,16.5,2,7.8780000000000001,7.8780000000000001,30,30,33,33,16.5,-2.6609529967382993E-5,12]
[null,"PSK","ZSS","Short Rural",33,11,2,8.7803244154962972,8.609,20,30,33,33,16.5,2,7.9371134020618559,7.6989999999999998,20,30,33,33,16.5,4.0255566019314931E-2,11]
[null,"PPT","ZSS","Short Rural",33,11,1,0.24282197587613907,0.24099999999999999,0.5,0.5,0.55000000000000004,0.55000000000000004,0,1,0.24210526315789477,0.23,0.5,0.5,0.55000000000000004,0.55000000000000004,0,-3.0020555589904537E-9,12]
[null,"QSH","ZSS","Short Rural",66,11,2,26.375507015981224,26.216999999999999,40,60,66,66,33,2,25.710981496379727,25.567,40,60,66,66,33,2.0412761671834527E-3,11]
[null,"QUI","ZSS","Short Rural",66,11,1,1.7486757470161491,1.657,5,5,5.5,5.5,0,1,1.4578391201207679,1.3520000000000001,5,5,5.5,5.5,0,3.3534320727600056E-2,11]
[null,"QDI_11","ZSS","Short Rural",66,11,2,7.1782992206212022,6.8879999999999999,20,26.6,29.260000000000005,29.260000000000005,14.63,2,6.3161616161616161,6.2530000000000001,20,26.6,29.260000000000005,29.260000000000005,14.63,5.6623387826411054E-11,11]
[null,"QDI_33","STS","Short Rural",66,33,2,5.4269371574928691,5.274,16,20,22,22,11,2,5.0447916666666668,4.843,16,20,22,22,11,2.877988946989125E-9,11]
[null,"RAG","ZSS","Short Rural",66,11,2,20.35207095092143,20.350999999999999,48,60,66,66,33,2,21.482982171799026,21.207999999999998,48,60,66,66,33,-2.3248865373625558E-2,12]
[null,"RGL","ZSS","Short Rural",132,33,2,10.852133302438508,10.670999999999999,60,60,66,66,33,2,9.9040816326530603,9.7059999999999995,100,120,132,132,66,1.9347771717373695E-2,11]
[null,"RVL","ZSS","Long Rural",66,11,2,1.204148474821862,1.17,10,11.25,12.375000000000002,12.375000000000002,5.5,1,1.1326315789473687,1.0760000000000001,5,6.25,6.8750000000000009,6.8750000000000009,0,5.3552375921995223E-2,11]
[null,"RCF","ZSS","Short Rural",33,11,2,0.4315791425543159,0.41,1,1,1.1000000000000001,1.1000000000000001,0.55000000000000004,2,0.43263157894736842,0.41099999999999998,1,1,1.1000000000000001,1.1000000000000001,0.55000000000000004,3.1599756578547238E-2,11]
[null,"RWR","ZSS","Short Rural",33,11,1,2.3461584357914527,1.8340000000000001,5,5,5.5,5.5,0,1,2.5124970245179723,2.1110000000000002,5,5,5.5,5.5,0,-1.065265948046383E-5,12]
[null,"RKF","ZSS","Short Rural",33,11,2,10.315563388283831,9.98,20,31,34.1,34.1,16.5,2,9.1908163265306122,9.0069999999999997,20,25,27.500000000000004,27.500000000000004,11,1.5572092111692105E-6,11]
[null,"BTH","ZSS","Urban",66,11,3,23.239532215148003,22.257999999999999,60,90,99.000000000000014,99.000000000000014,66,3,26.222222222222221,23.6,30,30,33,33,22,8.102371618059216E-6,11]
[null,"STL","ZSS","Short Rural",66,11,2,8.72370850533453,8.7140000000000004,30,50,55.000000000000007,55.000000000000007,27.5,2,8.1752577319587623,7.93,30,49.5,54.45,54.45,26.95,9.9511904170942224E-3,11]
[null,"SCK","ZSS","Short Rural",66,11,1,1.1295039413648458,1.117,8,8,8.8000000000000007,8.8000000000000007,0,1,0.64210832834975573,0.63500000000000001,8,8,8.8000000000000007,8.8000000000000007,0,6.1445934224637573E-2,11]
[null,"SMN","ZSS","Short Rural",33,11,1,4.0454553948907392,3.9430000000000001,5,5,5.5,5.5,0,2,3.5771739130434779,3.2909999999999999,10,11.5,12.65,12.65,5.5,2.2748641885862432E-2,11]
[null,"SPR","ZSS","Short Rural",66,22,1,6.0845964357785336,5.9139999999999997,10,16,17.600000000000001,17.600000000000001,0,1,5.4760435944889982,5.3259999999999996,10,16,17.600000000000001,17.600000000000001,0,1.9320053633729455E-2,11]
[null,"SNA_11","ZSS","Short Rural",132,11,1,2.9789419482432061E-2,1.4E-2,10,10,11,11,0,1.5,0.17293059718699563,0.15,1.5,3,3.3000000000000003,3.3000000000000003,0,-5.5177716395028388E-8,12]
[null,"SNA_66","STS","Short Rural",132,66,1,11.519232504179763,11.089,30,30,33,33,0,1,13.810667467227059,13.801,30,30,33,33,0,1.8383604876386052E-2,11]
[null,"SWR","ZSS","Short Rural",33,11,2,6.4472587632483345,6.4119999999999999,26,28.5,31.35,31.35,13.75,2,6.2283702213279675,6.1909999999999998,26,28.5,31.35,31.35,13.75,7.8206407091932183E-3,11]
[null,"SRG","ZSS","Long Rural",33,11,1,0.8337267295572659,0.79800000000000004,1.5,1.5,1.6500000000000001,1.6500000000000001,0,1,0.98777777777777775,0.88900000000000001,1,1,1.1000000000000001,1.1000000000000001,0,-8.6186952502145663E-9,12]
[null,"STF_66","STS","Short Rural",132,66,1,5.976963554881956,5.891,30,30,33,33,0,1,0,0,30,30,33,33,0,-3.9076857453213258E-2,12]
[null,"STF_22","ZSS","Long Rural",11,22,1,0.77857660313932964,0.748,5,5,5.5,5.5,0,1,0,0,5,5,5.5,5.5,0,1.9425961620774684E-2,11]
[null,"SWT","ZSS","Short Rural",66,11,2,17.728514043213625,17.675000000000001,30,50,55.000000000000007,55.000000000000007,27.5,2,19.849473684210526,19.716999999999999,30,50,55.000000000000007,55.000000000000007,27.5,-8.0206859371066683E-12,12]
[null,"STR_33","STS","Short Rural",132,33,2,41.874717389605728,41.837000000000003,100,120,132,132,66,2,30.686116700201207,30.501999999999999,100,120,132,132,66,7.2840528647201822E-2,11]
[null,"STR_11","ZSS","Short Rural",33,11,2,3.1221058055035775,2.9660000000000002,10,13,14.3,14.3,5.5,2,3.1119565217391303,2.863,10,13,14.3,14.3,5.5,1.7484805400258818E-2,11]
[null,"SFP","ZSS","Short Rural",132,11,1,11.794067733209658,11.763,30,30,33,33,0,1,10.993877551020407,10.773999999999999,30,30,33,33,0,-1.43789441120124E-6,12]
[null,"SUN_22","ZSS","Short Rural",66,22,1,0.56615303514444593,0.56000000000000005,5,5,5.5,5.5,0,1,0.60599999999999998,0.60599999999999998,5,5,5.5,5.5,0,-6.0722387824375491E-9,12]
[null,"SUN_33","ZSS","Short Rural",66,33,2,2.7108142097822001,2.6669999999999998,8,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,2,0,0,8,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,2.0291436718229996E-2,11]
[null,"SUT","ZSS","Short Rural",66,11,1,3.7940721190135189,3.7229999999999999,8,8,8.8000000000000007,8.8000000000000007,0,1,4.2469693856585167,4.1340000000000003,8,8,8.8000000000000007,8.8000000000000007,0,-3.6956778568778672E-5,12]
[null,"TAL","ZSS","Short Rural",66,11,1,1.3118348258421673,1.105,5,5,5.5,5.5,0,1,1.0423354735152488,1.0389999999999999,3.5,3.5,3.8500000000000005,3.8500000000000005,0,1.2887383370909914E-2,11]
[null,"ETH","ZSS","Urban",66,11,3,33.945460453179841,33.758000000000003,56,76,83.600000000000009,83.600000000000009,50.6,3,30.481891348088531,30.298999999999999,56,76,83.600000000000009,83.600000000000009,50.6,3.3904961459936166E-8,11]
[null,"STH","ZSS","Urban",66,11,2,24.759785409273945,23.806000000000001,40,60,66,66,33,2,24.014141414141417,23.774000000000001,40,60,66,66,33,2.7765045996324352E-3,11]
[null,"TAR","ZSS","Short Rural",33,11,2,1.0733395867145079,0.96599999999999997,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,2,1.0667504977470397,1.018,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,0,11]
[null,"TEA","ZSS","Short Rural",33,11,2,10.48941025468201,10.457000000000001,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,8.1686868686868692,8.0869999999999997,20,32,35.200000000000003,35.200000000000003,17.600000000000001,1.9516370037800428E-2,11]
[null,"TPT","ZSS","Short Rural",33,11,2,1.9518912807528601,1.911,7,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,2,1.9697916666666668,1.891,6,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,-3.2219589982083251E-3,12]
[null,"TRA","STS","Short Rural",132,66,2,19.819574382102374,19.754000000000001,70,120,132,132,66,2,20.968556104742877,19.939,70,120,132,132,66,-3.8403348195501551E-3,12]
[null,"TEM","ZSS","Short Rural",66,11,2,7.7627011247236011,7.415,16.75,22.5,24.750000000000004,24.750000000000004,11,2,8.3513270355375617,7.4260000000000002,16.75,22.5,24.750000000000004,24.750000000000004,11,-1.998530174345817E-3,12]
[null,"TNA_66","STS","Short Rural",110,66,3,82.409876320116666,82.066999999999993,210,300,330,330,220,3,95.375751503006015,95.185000000000002,210,300,330,330,220,1.6811395370088772E-2,11]
[null,"TNA_11","ZSS","Short Rural",66,11,2,5.9304842032172527,5.9210000000000003,48,60,66,66,33,2,6.2536842105263162,5.9409999999999998,48,60,66,66,33,-2.2385253952713111E-2,12]
[null,"TXS_22","ZSS","Long Rural",66,22,2,3.5094699277878849,3.3340000000000001,10,10,11,11,5.5,3,3.8583333333333338,3.7040000000000002,11,11,12.100000000000001,12.100000000000001,6.6,9.5318255784868008E-10,11]
[null,"TXS_33","ZSS","Long Rural",66,33,2,1.9463193017896461,1.849,12.5,12.5,13.750000000000002,13.750000000000002,5.5,2,2.8263157894736843,2.6850000000000001,12.5,12.5,13.750000000000002,13.750000000000002,5.5,-4.6029440914541017E-2,12]
[null,"THA","ZSS","Short Rural",33,11,2,14.38989847744126,14.369,50,50,55.000000000000007,55.000000000000007,27.5,2,17.923841059602648,16.239000000000001,50,50,55.000000000000007,55.000000000000007,27.5,-4.1456142869727416E-2,12]
[null,"THR","ZSS","Urban",33,11,2,16.091014285504887,15.641,32,32,35.200000000000003,35.200000000000003,17.600000000000001,2,15.652466024418642,15.205,20,32,35.200000000000003,35.200000000000003,17.600000000000001,-6.2476531217539108E-8,12]
[null,"TDL","ZSS","Short Rural",66,22,2,2.4952859500163398,2.4580000000000002,10,10,11,11,5.5,2,3.0021978021978022,2.7320000000000002,10,10,11,11,5.5,-1.8448718515977191E-2,12]
[null,"TUM","ZSS","Short Rural",66,22,2,8.1587661871846784,8.1549999999999994,20,25,27.500000000000004,27.500000000000004,13.75,2,8.5364057239057232,8.1809999999999992,20,25,27.500000000000004,27.500000000000004,13.75,-5.2112360120174827E-3,12]
[null,"TMT","ZSS","Short Rural",66,11,3,18.771860015378635,17.413,38,55,60.500000000000007,60.500000000000007,27.5,3,19.084836339345358,17.141999999999999,38,55,60.500000000000007,60.500000000000007,27.5,-6.8336024860463944E-3,12]
[null,"TUN","ZSS","Short Rural",66,11,2,8.6422705420655799,8.6379999999999999,22.5,32,35.200000000000003,35.200000000000003,17.600000000000001,2,9.0092783505154657,8.7390000000000008,22.5,32,35.200000000000003,35.200000000000003,17.600000000000001,-5.7283153223945888E-4,12]
[null,"TUR","ZSS","Short Rural",33,11,1,2.590278573607308,2.569,5,8,8.8000000000000007,8.8000000000000007,0,1,2.391216352964987,2.363,5,8,8.8000000000000007,8.8000000000000007,0,7.0872610910209825E-3,11]
[null,"THN","ZSS","Urban",66,33,2,16.445399418839411,15.887,50,50,55.000000000000007,55.000000000000007,27.5,2,16.585714285714289,16.254000000000001,50,50,55.000000000000007,55.000000000000007,27.5,-2.5642492892111336E-2,12]
[null,"TSH","ZSS","Short Rural",66,11,2,13.595015369089049,13.566000000000001,40,60,66,66,33,2,13.308163265306122,13.042,40,60,66,66,33,9.5330612456536491E-3,11]
[null,"ULN","ZSS","Short Rural",66,22,2,2.2252621421462151,2.1139999999999999,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,0,0,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,3.1349101583293848E-2,11]
[null,"ULG","ZSS","Short Rural",66,11,1,0.44341293421267358,0.38200000000000001,2.5,2.5,2.75,2.75,0,2,0.36304347826086958,0.33400000000000002,2,2,2.2000000000000002,2.2000000000000002,1.1000000000000001,-1.2996554332746209E-2,12]
[null,"ALU","ZSS","Urban",132,22,3,47.556535064890184,47.5,75,123,135.30000000000001,135.30000000000001,86.9,3,48.646405974483976,46.9,75,123,135.30000000000001,135.30000000000001,86.9,3.3664286634431987E-3,11]
[null,"UMA","ZSS","Short Rural",66,11,1,0.78776582303848397,0.72699999999999998,1.5,1.5,1.6500000000000001,1.6500000000000001,0,1,0.83666666666666667,0.753,1.5,1.5,1.6500000000000001,1.6500000000000001,0,-1.3278108859399031E-9,12]
[null,"URA","ZSS","Short Rural",66,11,2,3.46,3.2869999999999999,10,10,11,11,5.5,2,3.4389473684210525,3.2669999999999999,10,10,11,11,5.5,-1.378792177464875E-9,12]
[null,"UQT","ZSS","Short Rural",66,22,2,5.0947667400167944,5.0149999999999997,20,32,35.200000000000003,35.200000000000003,17.600000000000001,2,5.1067780872794799,4.95,15,21,23.1,23.1,5.5,7.5691823478888246E-6,11]
[null,"UBV","ZSS","Short Rural",33,11,2,0.91204737457654494,0.91,10.5,10.5,11.55,11.55,2.75,2,0.89263157894736844,0.84799999999999998,10.5,10.5,11.55,11.55,2.75,-4.023560372607552E-10,12]
[null,"WLA","ZSS","Short Rural",66,11,0,0,0,0,0,0,0,0,2,3.862841836800154,3.7083281633281477,6.25,6.25,6.8750000000000009,6.8750000000000009,3.4380000000000002,0,11]
[null,"WLS_22","ZSS","Long Rural",66,22,2,1.5377777777777777,1.3839999999999999,18,18,19.8,19.8,8.8000000000000007,2,1.3315217391304348,1.2250000000000001,20,20,22,22,11,2.9277069949928389E-2,11]
[null,"WLS_11","ZSS","Short Rural",22,11,2,1.5997526393947952,1.573,6,6,6.6000000000000005,6.6000000000000005,3.3,1,1.9760416666666667,1.897,3,3,3.3000000000000003,3.3000000000000003,0,-3.1556259650528579E-2,12]
[null,"WGT","ZSS","Long Rural",66,22,2,5.4560319223203519,5.4539999999999997,20,26,28.6,28.6,11,2,4.912121212121213,4.8630000000000004,20,26,28.6,28.6,11,1.3100968388162794E-3,11]
[null,"WLG","ZSS","Short Rural",66,22,1,0.18645068793274533,0.16300000000000001,1,1,1.1000000000000001,1.1000000000000001,0,1,0.15888888888888889,0.14299999999999999,1,1,1.1000000000000001,1.1000000000000001,0,2.2158369745695044E-6,11]
[null,"WRA","ZSS","Short Rural",66,22,2,3.1898744128531153,3.173,12,12,13.200000000000001,13.200000000000001,4.4000000000000004,2,3.028888888888889,2.726,12,12,13.200000000000001,13.200000000000001,4.4000000000000004,4.5723976984611253E-2,11]
[null,"WAR","ZSS","Short Rural",33,11,2,1.0180826176268765,0.85599999999999998,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,2,1.5715551056560799,1.242,5.5,5.5,6.0500000000000007,6.0500000000000007,2.75,-7.2331329211782092E-2,12]
[null,"WTR","ZSS","Urban",66,22,1,5.48,5.2060000000000004,5,5,5.5,5.5,0,1,5.0734693877551029,4.9720000000000004,5,5,5.5,5.5,0,-9.3602852734484543E-3,12]
[null,"WWA","ZSS","Short Rural",66,22,2,9.5702332522199658,9.3819999999999997,20,20,22,22,11,2,12.125263157894738,11.519,20,20,22,22,11,2.6960681870130004E-3,11]
[null,"WGN","ZSS","Short Rural","132, 66",11,2,10.206919282833208,9.8620000000000001,25,25,27.500000000000004,27.500000000000004,11,2,13.238709677419353,12.311999999999999,25,25,27.500000000000004,27.500000000000004,11,2.8337609034178837E-3,11]
[null,"WNA","ZSS","Short Rural",66,22,1,2.4836734693877554,2.4340000000000002,7.5,7.5,8.25,8.25,0,1,2.3928571428571432,2.3450000000000002,7.5,7.5,8.25,8.25,0,-3.1765004668660585E-2,12]
[null,"WCK","ZSS","Short Rural",66,11,2,2.6242092429546537,2.4929999999999999,13,14.25,15.675000000000001,15.675000000000001,6.875,2,2.5750000000000002,2.3690000000000002,10,14.25,15.675000000000001,15.675000000000001,6.875,9.8510063086315481E-3,11]
[null,"WJL","ZSS","Short Rural",66,11,2,2.0800821918959089,1.984,8,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,2,2.3752688172043008,2.2090000000000001,6,8,8.8000000000000007,8.8000000000000007,4.4000000000000004,-1.89719369799597E-12,12]
[null,"WWL","ZSS","Short Rural",66,22,2,8.4427629431353868,8.1259999999999994,20,25,27.500000000000004,27.500000000000004,13.75,2,9.2372588630582904,8.8249999999999993,20,25,27.500000000000004,27.500000000000004,13.75,-1.941621663373444E-2,12]
[null,"WTE","ZSS","Urban",66,11,3,22.077441129828358,20.78,55,59,64.900000000000006,64.900000000000006,42.9,3,20.904444444444444,18.814,55,59,64.900000000000006,64.900000000000006,42.9,6.3965197954206753E-3,11]
[null,"WHI","ZSS","Short Rural",33,11,2,5.2485960385709509,4.742,10,12.5,13.750000000000002,13.750000000000002,6.875,2,5.5269186712485681,4.8250000000000002,10,12.5,13.750000000000002,13.750000000000002,6.875,-5.8023466250069376E-3,12]
[null,"WID","ZSS","Short Rural",33,11,1,0.6850482714507371,0.57899999999999996,1,1,1.1000000000000001,1.1000000000000001,0,1,0,0,0.75,0.75,0.82500000000000007,0.82500000000000007,0,3.2454916790381386E-2,11]
[null,"WLC","ZSS","Short Rural",33,6.6,2,1.5258955678211716,1.389,7,7,7.7000000000000011,7.7000000000000011,3.85,2,1.3642666666666665,1.2789999999999999,7,7,7.7000000000000011,7.7000000000000011,3.85,1.6650223347498126E-2,11]
[null,"WBG","ZSS","Short Rural",33,11,1,1.2640898879032469,1.228,8,8,8.8000000000000007,8.8000000000000007,0,1,1.2224489795918367,1.198,8,8,8.8000000000000007,8.8000000000000007,0,-5.8934682800675464E-10,12]
[null,"WGM","ZSS","Short Rural",33,11,2,12.155285269049109,11.332000000000001,15,20,22,22,11,2,10.036666666666665,9.0329999999999995,15,20,22,22,11,4.6541320293914126E-2,11]
[null,"WBN","ZSS","Short Rural",66,11,2,6.7518778604159682,6.6390000000000002,16,20,22,22,11,2,6.2284210526315791,5.9169999999999998,16,20,22,22,11,-1.6894593834091906E-9,12]
[null,"WOO","ZSS","Short Rural",66,11,1,4.9994030817182988,4.9969999999999999,10,14,15.400000000000002,15.400000000000002,0,2,5.7765776577657766,5.7759999999999998,10,10,11,11,5.5,5.4310044284994762E-9,11]
[null,"WGA","ZSS","Short Rural",66,11,2,11.511102900817951,11.510999999999999,40,60,66,66,33,2,10.773469387755101,10.558,40,60,66,66,33,8.5187717541299204E-10,11]
[null,"IVL_11","ZSS","Urban",66,11,0,0,0,0,0,0,0,0,2,6.4515584455198693,6.1289805232438752,20,25,27.500000000000004,27.500000000000004,13.75,0,11]
[null,"IVL_22","ZSS","Short Rural",66,22,0,0,0,0,0,0,0,0,2,14.46970347921161,13.746218305251029,30,40,44,44,22,0,11]
[null,"YLI","ZSS","Short Rural",66,22,1,2.2863193595982945,2.1720000000000002,5,5,5.5,5.5,0,1,2.3510204081632651,2.3039999999999998,5,5,5.5,5.5,0,2.7431407765473137E-9,11]
[null,"YAM","ZSS","Short Rural",66,11,2,10.664007644840751,10.664,35,53,58.300000000000004,58.300000000000004,25.3,2,10.178571428571429,9.9749999999999996,35,53,58.300000000000004,58.300000000000004,25.3,-1.87473151549464E-9,12]
[null,"YAN","ZSS","Short Rural",33,11,1,2.7517412741724145,2.5609999999999999,5,5,5.5,5.5,0,1,2.5711753628004876,2.3210000000000002,5,5,5.5,5.5,0,1.9736404398742163E-2,11]
[null,"YNC","STS","Urban",33,66,1,11.436220328337315,11.420999999999999,15,15,16.5,16.5,0,1,10.403967351999174,10.07,15,15,16.5,16.5,0,9.5704796068099077E-3,11]
[null,"YAR","ZSS","Urban",66,11,2,7.6798488347445089,7.6740000000000004,48,55,60.500000000000007,60.500000000000007,27.5,2,8.1177777777777784,7.306,48,55,60.500000000000007,60.500000000000007,27.5,2.7011371949197367E-9,11]
[null,"YAS","ZSS","Short Rural",66,22,2,12.153898484663861,11.827999999999999,20,20,22,22,11,2,11.62902707909665,10.983000000000001,20,20,22,22,11,3.3369909020345061E-12,11]
[null,"YEN","ZSS","Short Rural",33,11,2,7.5335640658852041,7.4950000000000001,19,19,20.900000000000002,20.900000000000002,10.45,2,0,0,19,19,20.900000000000002,20.900000000000002,10.45,-1.2401643594302934E-7,12]
[null,"YOU","ZSS","Short Rural",66,11,2,16.274439957961633,16.228000000000002,54,60,66,66,33,2,16.661616161616163,16.495000000000001,54,60,66,66,33,-9.0484314940439594E-3,12]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.4.4 - AUGEX MODEL INPUTS - ASSET STATUS - DISTRIBUTION SUBSTATIONS"]
[null,"Distribution substation \ncategory ID","Description of distribution substation category",{"$f":"CRCP_y4","v":"2017-18"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"PRCP_y5","v":"2013-14"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Average per annum growth rate in annual substation maximum demand (50% PoE) from \", CRCP_y4, \" to \", dms_CRCP_FinalYear_Result)","v":"Average per annum growth rate in annual substation maximum demand (50% PoE) from 2017-18 to 2018-19"},"Network segment ID"]
[null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category","Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category that were within the following utilisation bands:",null,null,null,null,null,null,null,null,null,null,"Aggregate of the normal cyclic ratings of all individual distribution substations in the distribution substation category"]
[null,null,null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%",null,"0-20 %","20-40 %","40-60 %","60-80 %","80-100 %","100-120 %","120-140 %","140-160 %","160-180 %","180-200 %",">200%"]
[null,null,null," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," % "," MVA "," % "]
[null,7,"Distribution Substation Padmount",0.18118948824343015,0.33056708160442599,0.33886583679114801,0.11065006915629322,3.3195020746887967E-2,2.7662517289073307E-3,2.7662517289073403E-3,0,0,0,0,3758.1835000000001,0.16381418092909536,0.4352078239608802,0.31051344743276282,6.8459657701711488E-2,1.4669926650366748E-2,4.8899755501222494E-3,0,0,2.4449877750611247E-3,0,0,3427.7584999999999,1.0520373238202242E-2,7]
[null,8,"Distribution Substation - Poletop",0.17941176470588235,0.4,0.29705882352941176,0.11470588235294119,0,5.8823529411764705E-3,0,0,2.9411764705882353E-3,0,0,6295.9094999999998,0.19021739130434784,0.57608695652173914,0.15760869565217389,5.434782608695652E-2,1.6304347826086956E-2,5.434782608695652E-3,0,0,0,0,0,5966.7945,1.0520373238202242E-2,8]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"ED_AUG245_00001","ED_AUG245_00002","ED_AUG245_00003","ED_AUG245_00004","ED_AUG245_00005","ED_AUG245_00006","ED_AUG245_00007","ED_AUG245_00008"]
[null,"2.4.5 - AUGEX MODEL INPUTS - NETWORK SEGMENT DATA"]
[null,null,null,null,"Historical",null,null,null,"Forecast"]
[null,"Network segment ID","Network segment title","AER segment group","Average unit cost of augmentation for the network segment for the next regulatory control period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period","Average unit cost of augmentation for the network segment for the next regulatory control period","Capacity factor for the period","Mean value of the utilisation threshold for the period","Standard deviation of the utilisation threshold for the period"]
[]
[]
[]
[]
[null,null,null," ID ","$0's \nper MVA",null," % "," % ","$0's \nper MVA",null," % "," % "]
[null,1,"HV Feeder - Urban - Positive",5,1463460.6933886698,0.5945389718478814,0.44248265225750566,0.15258980299909375,1463460.6933886698,0.5945389718478814,0.44248265225750566,0.15258980299909375]
[null,2,"HV Feeder - Urban - Negative",5,1463460.6933886698,0.5945389718478814,0.61231520207459278,0.15258980299909375,1463460.6933886698,0.5945389718478814,0.61231520207459278,0.15258980299909375]
[null,3,"HV Feeder - Short Rural - Positive",6,311829.85742942011,0.86992503994635728,0.46356978552577255,0.32770537364744823,311829.85742942011,0.86992503994635728,0.46356978552577255,0.32770537364744823]
[null,4,"HV Feeder - Short Rural - Negative",6,311829.85742942011,0.86992503994635728,0.55745767964959758,0.15258980299909375,311829.85742942011,0.86992503994635728,0.55745767964959758,0.15258980299909375]
[null,5,"HV Feeder - Long Rural - Positive",7,369571.10559611482,1.124786714376786,0.51864342761785509,0.21752875236248459,369571.10559611482,1.124786714376786,0.51864342761785509,0.21752875236248459]
[null,6,"HV Feeder - Long Rural - Negative",7,369571.10559611482,1.124786714376786,0.47470879917489633,0.15258980299909375,369571.10559611482,1.124786714376786,0.47470879917489633,0.15258980299909375]
[null,7,"Distribution Substation Padmount",9,335739.75778546708,0.8112171855921857,0.91407371706254659,0.4012640150983865,335739.75778546708,0.8112171855921857,0.91407371706254659,0.4012640150983865]
[null,8,"Distribution Substation - Poletop",10,111684.67509025271,0.43200849002987174,0.91407371706254659,0.4012640150983865,111684.67509025271,0.43200849002987174,0.91407371706254659,0.4012640150983865]
[null,9,"Subtransmission Feeder - Positive",1,311046.41927835048,9.4292929292929291,0.63125889227883469,0.52307264655385777,311046.41927835048,9.4292929292929291,0.63125889227883469,0.52307264655385777]
[null,10,"Subtransmission Feeder - Negative",1,311046.41927835048,9.4292929292929291,0.78837535338409948,0.47184809193244548,311046.41927835048,9.4292929292929291,0.78837535338409948,0.47184809193244548]
[null,11,"Zone & Sub Substations - Positive",2,515059.68913027184,0.39801119864022022,0.26826813250334453,0.18362436485630373,515059.68913027184,0.39801119864022022,0.26826813250334453,0.18362436485630373]
[null,12,"Zone & Sub Substations - Negative",2,515059.68913027184,0.39801119864022022,0.51290889852695842,0.35378286377755325,515059.68913027184,0.39801119864022022,0.51290889852695842,0.35378286377755325]
[null,13]
[null,14]
[null,15]
[null,16]
[null,17]
[null,18]
[null,19]
[null,20]
[null,21]
[null,22]
[null,23]
[null,24]
[null,25]
[null,26]
[null,27]
[null,28]
[null,29]
[null,30]
[null,31]
[null,32]
[null,33]
[null,34]
[null,35]
[null,36]
[null,37]
[null,38]
[null,39]
[null,40]
[null,41]
[null,42]
[null,43]
[null,44]
[null,45]
[null,46]
[null,47]
[null,48]
[null,49]
[null,50]
[null,51]
[null,52]
[null,53]
[null,54]
[null,55]
[null,56]
[null,57]
[null,58]
[null,59]
[null,60]
[null,61]
[null,62]
[null,63]
[null,64]
[null,65]
[null,66]
[null,67]
[null,68]
[null,69]
[null,70]
[null,71]
[null,72]
[null,73]
[null,74]
[null,75]
[null,76]
[null,77]
[null,78]
[null,79]
[null,80]
[null,81]
[null,82]
[null,83]
[null,84]
[null,85]
[null,86]
[null,87]
[null,88]
[null,89]
[null,90]
[null,91]
[null,92]
[null,93]
[null,94]
[null,95]
[null,96]
[null,97]
[null,98]
[null,99]
[null,100]
[]
[]
[]
[]
[null,"2.4.6 - CAPEX AND NET CAPACITY ADDED BY SEGMENT GROUP"]
[null,"AER DNSP segment group",{"$f":"CONCATENATE(\"Capex ($0's, real \", dms_DollarReal, \")\")","v":"Capex ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Capex ($0's, real \", dms_DollarReal, \")\")","v":"Capex ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Capex ($0's, real \", dms_DollarReal, \")\")","v":"Capex ($0's, real June 2019)"},null,null,null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)",null,null,null,null,null,"Net capacity added (MVA)"]
[null,null,"In total for all purposes",null,null,null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,null,null,"In total for all purposes",null,null,null,null,null,"For customer-initiated & capacity-related augmentation",null,null,null,null,null,"For NSP-initiated & capacity-related augmentation",null,null,null,null,null,"Residual"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2017-18 to 2018-19"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2019-20 to 2023-24"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2017-18 to 2018-19"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2019-20 to 2023-24"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2017-18 to 2018-19"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2019-20 to 2023-24"},null,null,{"$f":"CONCATENATE(\"over period \", CRCP_y4, \" to \", CRCP_y5)","v":"over period 2017-18 to 2018-19"},null,null,{"$f":"CONCATENATE(\"over period \", FRCP_y1, \" to \", dms_MultiYear_FinalYear_Result)","v":"over period 2019-20 to 2023-24"}]
[null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Historical","Forecast",null,null,null,null,null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast",null,null,"Forecast"]
[null,null,{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2013-14 to 2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2013-14 to 2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CONCATENATE(PRCP_y5, \" to \", CRCP_y3)","v":"2013-14 to 2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},"type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3","type 1","type 2","type 3"]
[null,"Subtransmission lines",81617519.421000004,3319672.6397244162,2374066.0020453832,3783812.5997297675,4177716.0848323624,111859.57517790573,109725.20514836356,2960562.7079522782,0,0,0,0,0,0,0,0,81617519.421000004,3319672.6397244162,2374066.0020453832,3783812.5997297675,4177716.0848323624,111859.57517790573,109725.20514836356,2960562.7079522782,11.054521955279064,11.054521955279064,null,21.635698556914544,21.635698556914544,null,0,0,null,0,0,null,11.054521955279064,11.054521955279064,null,21.635698556914544,21.635698556914544,null,{"$f":"AA7845-AG7845-AM7845","v":0},{"$f":"AB7845-AH7845-AN7845","v":0},null,{"$f":"AD7845-AJ7845-AP7845","v":0},{"$f":"AE7845-AK7845-AQ7845","v":0}]
[null,"Subtransmission substations and subtransmission switching stations",0,"Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs",0,0,0,0,0,0,0,0,0,"Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs","Incl in Zone Subs",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"AA7846-AG7846-AM7846","v":0},{"$f":"AB7846-AH7846-AN7846","v":0},{"$f":"AC7846-AI7846-AO7846","v":0},{"$f":"AD7846-AJ7846-AP7846","v":0},{"$f":"AE7846-AK7846-AQ7846","v":0},{"$f":"AF7846-AL7846-AR7846","v":0}]
[null,"Zone substations",65765852.982000001,4859330.4517429993,5459767.5901455386,4955575.5423743473,3690043.8217823524,4323289.5530244531,6344159.7800850142,2555217.5713045676,0,0,0,0,0,0,0,0,65765852.982000001,4859330.4517429993,5459767.5901455386,4955575.5423743473,3690043.8217823524,4323289.5530244531,6344159.7800850142,2555217.5713045676,20.034761523102954,17.68946244863659,5.8621873787256202,42.45777087602692,37.487600873023624,12.423177998463176,0,0,0,0,0,0,20.034761523102954,17.68946244863659,5.8621873787256202,42.45777087602692,37.487600873023624,12.423177998463176,0,{"$f":"AB7847-AH7847-AN7847","v":0},{"$f":"AC7847-AI7847-AO7847","v":0},0,{"$f":"AE7847-AK7847-AQ7847","v":0},{"$f":"AF7847-AL7847-AR7847","v":0}]
[null,"High voltage feeders - CBD",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
[null,"High voltage feeders - urban",37952442.516830102,3555635.9871897842,3750306.6770434943,3902328.4627010194,3244162.4667544225,3061724.7572772019,3007891.5711420476,2987462.0396161466,1951500.1720107663,448027.0902540742,453318.92999445857,458610.76973483915,463902.60947521997,469194.4492156005,483814.71253237763,498434.97584915435,36000942.344819337,3107608.8969357098,3296987.7470490355,3443717.6929661804,2780259.8572792024,2592530.3080616016,2524076.8586096698,2489027.0637669922,4.9922370291450981,null,null,11.072090539016241,null,null,0.61590039576768529,null,null,1.6221532477993994,null,null,4.376336633377413,null,null,9.4499372912168411,null,null,0,null,null,0]
[null,"High voltage feeders - short rural",122978203.09504132,11521411.945245855,12152208.016483298,12644807.828028271,10512136.881122084,9920979.6274529807,9746542.672707675,9680344.3752986286,6323492.4705339596,1451752.8476042822,1468900.1219081907,1486047.3962120868,1503194.6705159836,1520341.9448198795,1567716.3321383316,1615090.7194567826,116654710.62450737,10069659.097641572,10683307.894575108,11158760.431816185,9008942.2106061,8400637.6826331019,8178826.3405693434,8065253.655841846,544.55583299734383,null,null,168.37647240528798,null,null,9.3661748544189241,null,null,24.668552032045771,null,null,535.18965814292494,null,null,143.70792037324222,null,null,0,null,null,0]
[null,"High voltage feeders - long rural",54342007.153128549,5091118.8697303077,5369857.0831099488,5587528.6851410745,4645137.1317169331,4383914.6475773398,4306833.8803846883,4277581.9620707808,2794245.3574552736,641505.25575753569,649082.34892875003,656659.44209995901,664236.53527116822,671813.62844237708,692747.57632698561,713681.52421159367,51547761.795673274,4449613.6139727719,4720774.7341811992,4930869.2430411158,3980900.5964457649,3712101.0191349629,3614086.3040577024,3563900.4378591869,28.305719236266587,null,null,62.778166246162087,null,null,3.4921225851912308,null,null,9.1975228985212585,null,null,24.813596651075358,null,null,53.58064334764083,null,null,0,null,null,0]
[null,"Distribution substations - CBD",68004693.306934327,7044146.1342705265,6312050.6098667569,6990736.2935257982,6257142.046496653,5964439.1899189046,5810090.1479798686,5721697.3989036279,6335914.479840409,1764181.6765899102,1712237.1943194228,1908353.1647071349,1907683.1426448538,1908786.7678177799,1867336.6639462125,1827445.7063583259,61668778.827093914,5279964.4576806165,4599813.4155473337,5082383.1288186628,4349458.9038517997,4055652.4221011247,3942753.4840336563,3894251.6925453022,119.58844607233804,null,null,275.27595036633676,null,null,11.641065859931794,null,null,29.102664649829489,null,null,107.94738021240624,null,null,246.17328571650728,null,null,0,null,null,0]
[null,"Distribution substations - urban ",15944788.375065664,1651612.7627698251,1479961.2540384335,1639089.9710857719,1467087.0628563096,1398458.1950832452,1362268.592720005,1341543.4984746752,1485556.5201595908,413640.61979419785,401461.40484917851,447443.93182991346,447286.83443751029,447545.59701656166,437826.95699014986,428473.88375523657,14459231.854906073,1237972.1429756272,1078499.8491892549,1191646.0392558584,1019800.2284187994,950912.59806668351,924441.63572985516,913069.6147194386,9.3273851076323506,null,null,21.470341694909131,null,null,2.7294341400682041,null,null,6.8235853501705117,null,null,6.597950967564147,null,null,14.64675634473862,null,null,0,null,null,0]
[null,"Distribution substations - short rural ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
[null,"Distribution substations - long rural ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0,null,null,0]
[]
[null,"Unmodelled augmentation",19238282.914000001,1027418.2093262812,717272.76726714894,1122296.2342150514,693035.697822758,485967.63276936382,477963.47995066515,475278.78564139834,0,0,0,0,0,0,0,0,19238282.914000001,1027418.2093262812,717272.76726714894,1122296.2342150514,693035.697822758,485967.63276936382,477963.47995066515,475278.78564139834,0]
[]
[]
[null,"Unmodelled augmentation - see comments in guidance paper - this should cover capex allocated to the augmentation category that is not considered to be primarily related to peak demand and capacity needs."]

{"sheet":"2.5 Connections","index":10,"n_rows":211,"n_cols":11,"rows_kept":211,"cut":false,"hidden":false,"merged":[[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,54,10],[138,1,139,1],[5,1,5,2],[9,4,9,10],[9,2,10,2],[9,1,10,1],[9,3,10,3],[195,4,195,10],[138,2,139,3],[138,4,138,10],[102,1,103,1],[102,2,103,3],[102,4,102,10],[120,4,120,10],[120,2,121,3],[120,1,121,1],[159,4,159,10],[177,4,177,10]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.5 CONNECTIONS"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.5.1 - DESCRIPTOR METRICS"]
[null,"VOLUMES AND EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Underground connections","0's",7119.2454421390075,5766.0397271045786,5586.5722142410877,5138.3512396962642,5111.1383154808809,5047.3429539023791,4376.8027225398528]
[null,null,"Overhead connections","0's",4373.5875726915556,3542.2686152724436,3432.0157955964032,3156.6588494113944,3139.9410514182914,3100.7494540976536,2688.8144468399555]
[null,null,"Distribution substations installed","MVA added",5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003]
[null,null,"Distribution substations installed","0's",69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791]
[null,null,"Distribution substations installed ","total spend $0's",867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578]
[null,null,"Augmentation HV ","net circuit KM added",32.090129500704045,33.241915591257353,34.393701681810633,35.545487772363934,36.697273862917214,37.849059953470523,39.000846044023795]
[null,null,"Augmentation HV","total spend $0's",2310489.324050691,2393417.9225705294,2476346.5210903655,2559275.1196102034,2642203.7181300395,2725132.3166498775,2808060.9151697131]
[null,null,"Augmentation LV","net circuit KM added",10.762083333333322,10.844166666666666,10.92625000000001,11.008333333333326,11.09041666666667,11.172499999999985,11.254583333333329]
[null,null,"Augmentation LV","total spend $0's",736943.75360987568,673679.88972770202,916638.22042948264,916670.93430813192,918893.15539344295,868584.24482879683,820200.04733933043]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",0,0,0,0,0,0,0]
[null,null,"Volume of GSL breaches for residential customers","0's",0,0,0,0,0,0,0]
[null,null,"Volume of customer complaints relating to connection services","0's",0,0,0,0,0,0,0]
[null,null,"GSL payments","$0's",0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",607.33539213699214,491.89482610201571,476.58464004554918,438.34737690416006,436.02587076507979,430.58355510737448,373.38046839432093]
[null,null,"Overhead connections","0's",993.89935287230037,804.98182005133322,779.92682702625314,717.35186172065437,713.55273609880931,704.64643147643687,611.03405254631537]
[null,null,"Distribution substations installed","MVA added",2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001]
[null,null,"Distribution substations installed","0's",14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762]
[null,null,"Distribution substations installed ","total spend $0's",364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549]
[null,null,"Augmentation HV ","net circuit KM added",2.6528260869563383,2.0446376811594291,1.4364492753622926,0.8282608695651561,0.22007246376801959,0.22007246376801959,0.22007246376801959]
[null,null,"Augmentation HV","total spend $0's",230795.86956520143,177883.47826087032,124971.08695651946,72058.695652168579,19146.304347817706,19146.304347817706,19146.304347817706]
[null,null,"Augmentation LV","net circuit KM added",3.1102777777777781,3.0974444444444451,3.0846111111111121,3.0717777777777755,3.0589444444444425,3.0461111111111094,3.0332777777777764]
[null,null,"Augmentation LV","total spend $0's",208388.61111111112,207528.77777777781,206668.9444444445,205809.11111111095,204949.27777777764,204089.44444444432,203229.61111111101]
[null,"SUBDIVISION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Cost per lot","$0's",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",3754.6645909205567,3723.3658787446802,3692.0671665687987,3660.7684543929222,3629.4697422170407,3598.1710300411642,3566.8723178652826]
[null,null,"Overhead connections","0's",9098.9174140364576,9332.686056216131,9566.4546983957953,9800.2233405754687,10033.991982755135,10267.760624934808,10501.529267114474]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[null,"VOLUMES AND EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,"CONNECTION SUBCATEGORY","DESCRIPTOR METRIC","Unit of Measure",{"$f":"CONCATENATE(\"VOLUMES and EXPENDITURE \n(0's, real \", dms_DollarReal, \")\")","v":"VOLUMES and EXPENDITURE \n(0's, real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Underground connections","0's",7119.2454421390075,5766.0397271045786,5586.5722142410877,5138.3512396962642,5111.1383154808809,5047.3429539023791,4376.8027225398528]
[null,null,"Overhead connections","0's",4373.5875726915556,3542.2686152724436,3432.0157955964032,3156.6588494113944,3139.9410514182914,3100.7494540976536,2688.8144468399555]
[null,null,"Distribution substations installed","MVA added",5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003,5.0772500000000003]
[null,null,"Distribution substations installed","0's",69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791,69.051825620221791]
[null,null,"Distribution substations installed ","total spend $0's",867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578,867674.50038177578]
[null,null,"Augmentation HV ","net circuit KM added",32.090129500704045,33.241915591257353,34.393701681810633,35.545487772363934,36.697273862917214,37.849059953470523,39.000846044023795]
[null,null,"Augmentation HV","total spend $0's",2310489.324050691,2393417.9225705294,2476346.5210903655,2559275.1196102034,2642203.7181300395,2725132.3166498775,2808060.9151697131]
[null,null,"Augmentation LV","net circuit KM added",10.762083333333322,10.844166666666666,10.92625000000001,11.008333333333326,11.09041666666667,11.172499999999985,11.254583333333329]
[null,null,"Augmentation LV","total spend $0's",736943.75360987568,673679.88972770202,916638.22042948264,916670.93430813192,918893.15539344295,868584.24482879683,820200.04733933043]
[null,null,"Mean days to connect residential customer with LV single phase connection","0's",0,0,0,0,0,0,0]
[null,null,"Volume of GSL breaches for residential customers","0's",0,0,0,0,0,0,0]
[null,null,"Volume of customer complaints relating to connection services","0's",0,0,0,0,0,0,0]
[null,null,"GSL payments","$0's",0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Underground connections","0's",607.33539213699214,491.89482610201571,476.58464004554918,438.34737690416006,436.02587076507979,430.58355510737448,373.38046839432093]
[null,null,"Overhead connections","0's",993.89935287230037,804.98182005133322,779.92682702625314,717.35186172065437,713.55273609880931,704.64643147643687,611.03405254631537]
[null,null,"Distribution substations installed","MVA added",2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001,2.1080000000000001]
[null,null,"Distribution substations installed","0's",14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762,14.418758544732762]
[null,null,"Distribution substations installed ","total spend $0's",364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549,364815.43128134549]
[null,null,"Augmentation HV ","net circuit KM added",2.6528260869563383,2.0446376811594291,1.4364492753622926,0.8282608695651561,0.22007246376801959,0.22007246376801959,0.22007246376801959]
[null,null,"Augmentation HV","total spend $0's",230795.86956520143,177883.47826087032,124971.08695651946,72058.695652168579,19146.304347817706,19146.304347817706,19146.304347817706]
[null,null,"Augmentation LV","net circuit KM added",3.1102777777777781,3.0974444444444451,3.0846111111111121,3.0717777777777755,3.0589444444444425,3.0461111111111094,3.0332777777777764]
[null,null,"Augmentation LV","total spend $0's",208388.61111111112,207528.77777777781,206668.9444444445,205809.11111111095,204949.27777777764,204089.44444444432,203229.61111111101]
[null,"SUBDIVISION","Underground connections","0's",0,0,0,0,0,0,0]
[null,null,"Overhead connections","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Cost per lot","$0's",0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Underground connections","0's",3754.6645909205567,3723.3658787446802,3692.0671665687987,3660.7684543929222,3629.4697422170407,3598.1710300411642,3566.8723178652826]
[null,null,"Overhead connections","0's",9098.9174140364576,9332.686056216131,9566.4546983957953,9800.2233405754687,10033.991982755135,10267.760624934808,10501.529267114474]
[null,null,"Distribution substations installed","MVA added",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed","0's",0,0,0,0,0,0,0]
[null,null,"Distribution substations installed ","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation HV ","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation HV","total spend $0's",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","net circuit KM added",0,0,0,0,0,0,0]
[null,null,"Augmentation LV","total spend $0's",0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.2 - COST METRICS BY CONNECTION CLASSIFICATION"]
[null,"EXPENDITURE - ALL"]
[null,"CONNECTION SUBCATEGORY","CONNECTION CLASSICIATION",null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,3915107.5780423423,3934772.312680007,4260659.241901624,4343620.5543001108,4428771.3739052583,4461391.0618604496,4495935.4628908187]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,803999.91195765801,750227.68731999351,696455.46268230944,642683.23804462503,588911.01340694085,588051.18007360748,587191.34674027422]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,3915107.5780423423,3934772.312680007,4260659.241901624,4343620.5543001108,4428771.3739052583,4461391.0618604496,4495935.4628908187]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,803999.91195765801,750227.68731999351,696455.46268230944,642683.23804462503,588911.01340694085,588051.18007360748,587191.34674027422]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[null,"EXPENDITURE - STANDARD CONTROL SERVICES - CAPITAL CONTRIBUTIONS"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($'0s,  real \", dms_DollarReal,\")\")","v":"EXPENDITURE \n($'0s,  real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,65433619.901351176,64847054.542097285,65768543.347380057,65700659.406122491,65658461.159939736,65633202.866030231,65621141.23349236]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,22596864.098648831,22394299.457902715,22712526.65261995,22689083.593877513,22674510.840060275,22665788.133969776,22661622.766507652]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,0,0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (small capacity)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0,0,0,0,0,0]
[]
[]
[]
[null,"2.5.3 - VOLUMES BY CONNECTION CLASSIFICATION"]
[null,"NEW CONNECTIONS - ALL"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,11492.833014830563,9308.3083423770222,9018.588009837491,8295.0100891076581,8251.0793668991719,8148.0924080000332,7065.6171693798078]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1601.2347450092925,1296.8766461533489,1256.5114670718024,1155.6992386248144,1149.578606863889,1135.2299865838113,984.41452094063629]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,"",0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,"",0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,12853.582004957014,13056.051934960811,13258.521864964594,13460.991794968391,13663.461724972176,13865.931654975971,14068.401584979758]
[null,null,"Complex connection HV (small capacity)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,"",0,0,0,0,0,0]
[]
[null,"NEW CONNECTIONS - STANDARD CONTROL SERVICES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,11492.833014830563,9308.3083423770222,9018.588009837491,8295.0100891076581,8251.0793668991719,8148.0924080000332,7065.6171693798078]
[null,null,"Complex connection LV",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV",null,0,0,0,0,0,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,1601.2347450092925,1296.8766461533489,1256.5114670718024,1155.6992386248144,1149.578606863889,1135.2299865838113,984.41452094063629]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection sub-transmission",null,"",0,0,0,0,0,0]
[null,"SUBDIVISION","Complex connection LV",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,"",0,0,0,0,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,12853.582004957014,13056.051934960811,13258.521864964594,13460.991794968391,13663.461724972176,13865.931654975971,14068.401584979758]
[null,null,"Complex connection HV (small capacity)",null,"",0,0,0,0,0,0]
[null,null,"Complex connection HV (large capacity)",null,"",0,0,0,0,0,0]
[]
[null,"EXISTING CONNECTIONS"]
[null,null,null,null,"VOLUMES\n(0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"RESIDENTIAL","Simple connection LV",null,785090.56991011242,792763.2838300775]
[null,null,"Complex connection LV",null,0,0]
[null,null,"Complex connection HV",null,0,0]
[null,"COMMERCIAL/INDUSTRIAL","Simple connection LV",null,111582.23874517753,112672.73534423744]
[null,null,"Complex connection HV (customer connected at LV, minor HV works)",null,0,0]
[null,null,"Complex connection HV (customer connected at LV, upstream asset works)",null,0,0]
[null,null,"Complex connection HV (customer connected at HV)",null,0,0]
[null,null,"Complex connection sub-transmission",null,0,0]
[null,"SUBDIVISION","Complex connection LV",null,0,0]
[null,null,"Complex connection HV (no upstream asset works)",null,0,0]
[null,null,"Complex connection HV (with upstream asset works)",null,0,0]
[null,"EMBEDDED GENERATION","Simple connection LV",null,141397.58200495702,154453.63393991784]
[null,null,"Complex connection HV (small capacity)",null,0,0]
[null,null,"Complex connection HV (large capacity)",null,0,0]

{"sheet":"2.6 Non-network","index":11,"n_rows":123,"n_cols":11,"rows_kept":123,"cut":false,"hidden":false,"merged":[[119,1,119,3],[120,1,120,3],[121,1,121,3],[122,1,122,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[117,1,117,3],[118,1,118,3],[107,1,107,3],[108,1,108,3],[110,1,110,3],[111,1,111,3],[112,1,112,3],[93,4,93,10],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[106,1,106,3],[100,1,100,3],[101,1,101,3],[103,1,103,3],[104,1,104,3],[105,1,105,3],[5,1,5,2],[19,1,29,1],[32,1,36,1],[39,1,49,1],[64,1,68,1],[69,1,73,1],[74,1,78,1],[79,1,83,1],[84,1,88,1],[55,4,55,10],[8,4,8,10],[62,4,62,10],[55,1,56,3],[12,1,16,1],[59,1,59,3],[58,1,58,3],[57,1,57,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.6 NON NETWORK EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet - each has been 'grouped' (and sub-grouped) for easy navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"2.6.1 - NON-NETWORK EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2019)"}]
[null,"SERVICE SUBCATEGORY","ASSET CATEGORY",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"OPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,null,null,null,null,"Not reported as Non System is included in overheads. As agreed with Kaye Johnston. See email from 15/3/18 10.55 am."]
[null,"MOTOR VEHICLES","Car"]
[null,null,"Light commercial vehicle"]
[null,null,"Elevated work platform (LCV)  "]
[null,null,"Elevated work platform (HCV)"]
[null,null,"Heavy commercial vehicle"]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure"]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"CAPEX"]
[null,"IT & COMMUNICATIONS","Total IT and communications",null,38342426.727203168,43331769.028011307,58846941.51592239,29356646.241275545,33674209.735372677,21306029.202946451,20860312.787244096]
[null,"MOTOR VEHICLES","Car",null,418975.30865361169,1364944.3124129893,186678.98140254238,215204.61926448203,316183.06748584216,639539.57710371853,966798.02735546383]
[null,null,"Light commercial vehicle",null,13229456.329704704,10129038.440015575,13922696.222507708,12644125.368372701,13552375.81853337,15699611.237412954,14558695.804794142]
[null,null,"Elevated work platform (LCV)  ",null,0,0,0,0,0,0,0]
[null,null,"Elevated work platform (HCV)",null,3136281.5704574757,12665341.428069348,8371041.1051021963,10550150.263465917,13205076.322183844,14024785.660820188,7645267.8020364558]
[null,null,"Heavy commercial vehicle",null,3041065.7411629129,7553178.1437314302,8206571.1279436946,6710470.1889523854,7111395.5402920088,9142673.664893223,10658134.893732535]
[null,"BUILDINGS AND PROPERTY","Total buildings and property expenditure",null,12526980.989843702,29707261.410150345,14466927.859163037,8865542.6818583105,12997018.710674476,12947101.655189555,12676251.761550667]
[null,"OTHER","Other expenditure"]
[null,"OTHER - DNSP nominated","Office furniture and equipment",null,74631.668820755032,66194.733415956958,9768.7816644515005,9599.4154689573497,9622.7155524409409,9718.6681005982045,9515.3561709121022]
[null,null,"Tools and equipment",null,6567376.7835818389,5705710.0776551766,2385074.1846198775,2343722.9747663136,2349411.7524998183,2372838.8239012789,2323199.67220602]
[null,null,"Other fleet assets",null,87171.50336841328,87374.298265148173,88020.489536508307,86494.434809276529,86704.377545731651,87568.947002925241,85737.028121504773]
[null,null,"Capitalised property leases",null,0,0,26064831.202994082,1954317.4650326706,373837.23799451842,3461532.3637694358,86310.953747445019]
[null,null,"LiDAR",null,7248423,10500000,13545105.480364876,10736134.791393343,11107187.768467415,8814300.424330838,12491629.701086177]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"2.6.2 - ANNUAL DESCRIPTOR METRICS"]
[null,"IT & COMMUNICATIONS"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Employee numbers",null,null,2602.8571032884979,2622.9124841717644,2547.2508968397597,2477.1388211603171,2410.3172842440149,2390.5801143868562,2321.7076556294237]
[null,"User numbers",null,null,2602.8571032884979,2622.9124841717644,2547.2508968397597,2477.1388211603171,2410.3172842440149,2390.5801143868562,2321.7076556294237]
[null,"Number of devices",null,null,4445.6032239689685,4398.3149384812332,4348.9864137129416,4263.2043468921793,4074.9968474629031,4115.6507463803018,4029.5516918235935]
[]
[null,"MOTOR VEHICLES "]
[null,null,null,null,"VOLUMES  (0's or %)"]
[null,"ASSET CATEGORY","DESCRIPTOR METRIC","Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"CAR","Average kilometres travelled ","0's",20130,20130,20130,20130,20130,20130,20130]
[null,null,"Number purchased","0's",12,15.726990244867341,4.4009172371108498,5.1895366365090441,7.8031854525885382,15.762066688264985,24.005839866183109]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",55.787962026277249,55.918187537306103,56.331740635018875,55.355057456096468,55.489318773962935,56.042903780497724,54.870491122704252]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.87168690666058202,0.87372168027040786,0.88018344742216992,0.86492277275150731,0.86702060584317087,0.87567037157027694,0.85735142379225393]
[null,"LIGHT COMMERCIAL VEHICLE","Average kilometres travelled ","0's",24090,24090,24090,24090,24090,24090,24090]
[null,null,"Number purchased","0's",322,230.66252359138767,192.76017498545522,190.28301000533162,197.68069813224295,252.19306701223977,234.91429011907758]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",1021.399132879537,1024.8755309571884,1032.4551838262053,1014.5544124375181,1017.0151706540395,1027.1613458519348,1005.6732201083139]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.87168690666058202,0.87372168027040786,0.88018344742216992,0.86492277275150731,0.86702060584317087,0.87567037157027694,0.85735142379225393]
[null,"ELEVATED WORK PLATFORM (LCV) ","Average kilometres travelled ","0's",0,0,0,0,0,0,0]
[null,null,"Number purchased","0's",0,0,0,0,0,0,0]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",0,0,0,0,0,0,0]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.87168690666058202,0.87372168027040786,0.88018344742216992,0.86492277275150731,0.86702060584317087,0.87567037157027694,0.85735142379225393]
[null,"ELEVATED WORK PLATFORM (HCV)","Average kilometres travelled ","0's",18180,18180,18180,18180,18180,18180,18180]
[null,null,"Number purchased","0's",3,8.7372168027040793,11.442384816488209,12.97384159127261,25.143597569451956,29.772792633389415,17.147028475845079]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",184.79762421204339,185.22899621732645,186.59889085350002,183.36362782331955,183.80836843875221,185.6421187728987,181.75850184395784]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.87168690666058202,0.87372168027040786,0.88018344742216992,0.86492277275150731,0.86702060584317087,0.87567037157027694,0.85735142379225393]
[null,"HEAVY COMMERCIAL VEHICLE ","Average kilometres travelled ","0's",13170,13170,13170,13170,13170,13170,13170]
[null,null,"Number purchased","0's",25,7.8634951224336707,24.645136527820757,27.677528728048234,27.744659386981468,37.653825977521912,31.722002680313395]
[null,null,"Number leased","0's",0,0,0,0,0,0,0]
[null,null,"Number in fleet","0's",265.8645065314775,266.48511248247439,268.45595146376183,263.80144568920974,264.44128478216709,267.07946332893448,261.49218425663747]
[null,null,"Proportion of total fleet expenditure allocated as regulatory expenditure","%",0.87168690666058202,0.87372168027040786,0.88018344742216992,0.86492277275150731,0.86702060584317087,0.87567037157027694,0.85735142379225393]
[]
[]
[]
[null,"2.6.4 - INFORMATION & COMMUNICATIONS TECHNOLOGY - CAPEX BY PURPOSE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE\n($'0s, real \", dms_DollarReal,\")\")","v":"EXPENDITURE\n($'0s, real June 2019)"}]
[null,null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"ICT CAPABILITY GROWTH"]
[null,null,null,null,0,1046239.896048563,2705202.6846125517,1726861.5436044438,833176.32334942708,651506.67810662708,635252.32356216596]
[null,"Asset Management and Planning",null,null,8821378.3586503882,0,0,0,0,0,0]
[null,"Customer and Market Interactions",null,null,628850.73447804747,1708858.4968793197,1914721.3806673256,1709592.9281683995,0,598681.81231419777,583745.37840847683]
[null,"Enterprise Services",null,null,6725209.243723562,0,0,0,2430097.6097691627,0,0]
[null,"Network Services and Works Management",null,null,7773293.8011869723,11334265.540526096,11945050.815172307,5871329.2482551085,10848650.043612331,6074859.5661293585,7468507.0472849216]
[null,"Technology and ICT",null,null,0,0,0,0,0,0,0]
[null,"ICT ASSET EXTENSIONS"]
[null,null,null,null,0,0,0,0,0,0,0]
[null,"Asset Management and Planning",null,null,0,0,0,0,0,0,0]
[null,"Customer and Market Interactions",null,null,0,0,0,0,0,0,0]
[null,"Enterprise Services",null,null,0,0,0,0,0,0,0]
[null,"Network Services and Works Management",null,null,579940.12179642147,1550178.7793119536,597252.54075861536,348826.03180809767,183993.10473966514,116214.70474334426,127050.46471243318]
[null,"Technology and ICT",null,null,0,0,0,0,0,0,0]
[null,"ICT ASSET REMEDITATION"]
[null,null,null,null,0,0,0,0,0,0,0]
[null,"Asset Management and Planning",null,null,0,0,0,0,0,0,0]
[null,"Customer and Market Interactions",null,null,0,0,0,0,0,0,0]
[null,"Enterprise Services",null,null,0,0,0,0,0,0,0]
[null,"Network Services and Works Management",null,null,149352.04943853625,629487.67078921851,250319.07958265502,65620.738656968882,32979.896132581496,33455.748335205171,48931.597896004649]
[null,"Technology and ICT",null,null,0,0,0,0,0,0,0]
[null,"ICT ASSET REPLACEMENT"]
[null,null,null,null,87340.379788617691,4184959.5841942518,10820810.738450207,6907446.1744177751,7498586.9101448441,2606026.7124265083,2541009.2942486638]
[null,"Asset Management and Planning",null,null,0,1830919.8180849848,12823363.375111446,0,0,0,2403657.440505492]
[null,"Customer and Market Interactions",null,null,3214125.9762211312,9799780.3596548717,10381654.458480638,6838371.712673598,0,2394727.2492567911,2334981.5136339073]
[null,"Enterprise Services",null,null,2008828.7351382072,2266853.1081052194,2810600.1918052486,0,3211200.4129092502,1320621.6448107304,1631053.2632001555]
[null,"Network Services and Works Management",null,null,8354107.3267812813,8980225.7744168304,4597966.2512813974,5888597.8636911539,8635525.4347154163,7509935.086823687,3086124.4637918728]
[null,"Technology and ICT",null,null,0,0,0,0,0,0,0]

{"sheet":"2.10 Overheads","index":12,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,3,8,9],[23,3,23,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.10 OVERHEADS"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and sub-grouped) for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"2.10.1 - NETWORK OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE ($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE ($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",93195586.512963861,89740884.225624487,93075701.398936525,87826453.781770319,84036148.579865128,76463958.127517581,69666629.571448609]
[null,"Alternative Control Services","Total  ",13612811.714626094,12291240.995765356,11480726.877674747,10767253.476374455,10795535.776265662,10323408.435664095,10883257.700915016]
[null,"CAPEX"]
[null,"Standard Control Services","Total  ",105207128.97698709,97991647.53931208,102024708.2513717,90946543.459809482,88302711.406922802,86873461.349524021,87872330.617175281]
[null,"Alternative Control Services","Total  ",1424490.0173289967,1205087.9634395619,1336426.8027512969,1041415.5514389003,733990.2329437033,983462.84571558097,939135.92939827079]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total  ",""]
[null,"Unregulated Distribution Services","Total  ",1798826.3173637898,1598266.2848012228,2760122.7354265661,2653815.1643955307,2640706.65355522,2600579.0567885661,2560734.2540900423]
[]
[]
[]
[null,"2.10.2 - CORPORATE OVERHEADS EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE  \n($0's, real \", dms_DollarReal,\")\")","v":"EXPENDITURE  \n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"OPEX"]
[null,"Standard Control Services","Total  ",50030698.290311106,48830409.326415375,46658484.344842277,43576976.643503681,39454488.457815677,36037232.266039602,33467706.156880751]
[null,"Alternative Control Services","Total  ",7992348.3115159264,7406289.1239022724,5786799.4580328744,5494447.1340987841,5065191.4457681878,4690382.2891255412,4978600.6065494819]
[null,"CAPEX"]
[null,"Standard Control Services","Total",41952490.119718522,39014739.232196122,35520603.545180276,31548030.984081417,27270832.622878075,24649218.992442064,23800233.646575555]
[null,"Alternative Control Services","Total",779392.1165657338,668480.15265219903,661416.21079767169,533053.25397769816,334826.51836827816,417876.79023311625,384665.45558658021]
[null,"OTHER DISTRIBUTION SERVICES"]
[null,"Negotiated Services","Total",""]
[null,"Unregulated Distribution Services","Total",751374.09797395195,662778.29488518741,964186.26866774925,913525.84981267492,827872.54843858082,782311.32014808792,766897.45076710999]

{"sheet":"2.11 Labour","index":13,"n_rows":25,"n_cols":14,"rows_kept":25,"cut":false,"hidden":false,"merged":[[5,1,5,2],[8,2,8,13],[9,7,9,13],[9,2,9,6]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.11 LABOUR"]
[]
[null,"Table numbering on this worksheet starts at 2.11.3."]
[]
[null,"2.11.3 - LABOUR / NON-LABOUR EXPENDITURE SPLIT - STANDARD CONTROL SERVICES"]
[null,null,"EXPENDITURE"]
[null,null,"($0's, nominal)",null,null,null,null,{"$f":"CONCATENATE(\"($0's, real \", dms_DollarReal,\")\")","v":"($0's, real June 2019)"}]
[null,null,{"$f":"PRCP_y4","v":"2012-13"},{"$f":"PRCP_y5","v":"2013-14"},{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"OPEX"]
[null,"In-house labour expenditure",302605483.52962822,301565424.8986094,263963951.67936847,232493650.22470075,226055318.81766963,231755639.40487126,224053580.17024937,232262950.40432307,232027889.66169226,230562698.90468612,230201624.05713743,229108039.58593833]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",74711791.598013192,72928277.73560746,59166439.434400931,41061978.545548268,59121071.439360164,70746840.310242072,84633695.422183871,82062845.5092296,75766407.9929474,69497282.624852285,55960596.022327453,43566950.448060587]
[null,"Controllable non-labour expenditure",80703628.833113551,77690089.365783155,64886984.577198565,37164880.610606968,32970449.026496232,43696712.01091896,56405501.898090713,53148974.317315057,46654962.178314187,42118561.716632009,32758912.61359328,22354301.631991632]
[null,"Uncontrollable non-labour expenditure",3021366.8391979393,3287437.31,3282491.3330000001,3216330.1729999995,3795853.2664730139,3891177.273967769,4031992.5094760652,3995530.7691322449,3926008.1670462014,3935581.7538296329,3974920.3069418361,3891339.3340095216]
[null,"Total",{"$f":"SUM(C13:C17)","v":461042270.79995292},{"$f":"SUM(D13:D17)","v":455471229.31},391299867.02396798,313936839.55385596,321942692.549999,350090369.00000006,{"$f":"SUM(I13:I17)","v":369124770},371470300.99999994,358375268.00000006,346114125.00000006,322896053,298920631.00000006]
[null,"CAPEX"]
[null,"In-house labour expenditure",218227211.35229269,218361425.82968518,193541676.41906625,155361098.88774917,150914804.55169541,160397812.89282224,157076783.19787955,155658506.49917749,140814190.40882042,132433809.94488238,127785090.93333513,125572308.59434757]
[null,"Labour expenditure outsourced to related parties",0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Labour expenditure outsourced to unrelated parties",23612642.462056633,20645726.229984585,14999454.183459831,20120613.269822188,16121699.091000214,22882652.358927682,24722825.602923933,28570871.537340105,16253734.899765588,17188255.944949333,12132759.179769121,11770892.509111814]
[null,"Controllable non-labour expenditure",398739788.5521667,325253500.36946428,415096460.9994669,345254240.66825771,309771991.6957044,261866663.74824998,296931674.1991964,314288194.96348232,254320644.69141388,259617491.11016816,256026072.8868956,247129416.89654052]
[null,"Uncontrollable non-labour expenditure",0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total",{"$f":"SUM(C20:C24)","v":640579642.36651599},{"$f":"SUM(D20:D24)","v":564260652.42913401},623637591.60199296,520735952.82582903,476808495.33840001,445147128.99999988,{"$f":"SUM(I20:I24)","v":478731282.99999988},{"$f":"SUM(J20:J24)","v":498517572.99999988},{"$f":"SUM(K20:K24)","v":411388569.99999988},{"$f":"SUM(L20:L24)","v":409239556.99999988},{"$f":"SUM(M20:M24)","v":395943922.99999988},{"$f":"SUM(N20:N24)","v":384472617.99999988}]

{"sheet":"2.14 Forecast price changes","index":14,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[[5,1,5,2],[7,1,7,2],[8,1,8,2],[11,4,11,8],[12,2,12,8],[11,1,13,1],[11,2,11,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.14 FORECAST PRICE CHANGES"]
[]
[null,"There is ONE table on this worksheet. It has been grouped for easy navigation.  See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName, \" must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. \"&\"If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year.\")","v":"Essential Energy must provide all forecast price changes used to forecast opex and capex, including forecast changes in CPI. Forecast price changes must be expressed in real terms, except for CPI. If the same escalators are not used for capex and opex, report capex and opex escalators separately. Add additional rows as required. If price changes for a given year were not used to forecast either opex or capex enter '0' for that year."}]
[]
[null,"2.14.2 - FORECAST CAPEX AND OPEX PRICE CHANGES"]
[null,null,"Price changes\n(% YoY real)\nCurrent regulatory period",null,"Price changes\n(%YoY real)\nForthcoming regulatory period "]
[null,null,"Forecast"]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"OPEX"]
[null,"CPI",1.2769909449732886E-2,1.95E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2,2.5000000000000001E-2]
[null,"Price growth",0,6.6878047675043018E-3,5.5625134352041972E-3,7.5613430923282543E-3,9.5757858904408355E-3,9.8649882803112376E-3,8.4998103107922773E-3]
[null,"Output growth",0,7.4668726106701232E-3,7.6144476198591934E-3,6.4438654867073073E-3,6.7541666148119633E-3,6.0695388708036464E-3,6.8085004407534358E-3]
[null,"CAPEX"]

{"sheet":"2.16 Opex Summary","index":15,"n_rows":67,"n_cols":12,"rows_kept":67,"cut":false,"hidden":false,"merged":[[29,2,29,11],[57,2,57,11],[43,2,43,11],[56,2,56,11],[5,1,5,6],[15,2,15,11],[14,2,14,11],[28,2,28,11],[42,2,42,11],[7,9,7,11],[9,1,9,7],[9,9,9,10],[8,11,9,11],[8,9,8,10],[8,1,8,7],[10,1,10,7],[10,9,10,10]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.16 OPEX SUMMARY"]
[]
[null,"There are FOUR tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions",null,null,null,null,null,null,null,"IMPORTANT!"]
[null,{"$f":"CONCATENATE(\"Complete the tables below in accordance with the regulatory information notice.\n\n\",dms_TradingName,\"'s total forecast opex must reconcile to Table 2.16.1 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.3). If \",dms_TradingName,\" did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if \",dms_TradingName,\" owns any dual function assets Table 2.16.4).\")","v":"Complete the tables below in accordance with the regulatory information notice.\n\nEssential Energy's total forecast opex must reconcile to Table 2.16.1 (and if Essential Energy owns any dual function assets Table 2.16.3). If Essential Energy did not forecast its total opex using a Base Year approach, total forecast opex must reconcile to Table 2.16.2 (and if Essential Energy owns any dual function assets Table 2.16.4)."},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Has \",dms_TradingName,\" used a base-step-trend model to derive its opex forecast? \")","v":"Has Essential Energy used a base-step-trend model to derive its opex forecast? "},null,"Yes"]
[null,{"$f":"CONCATENATE(\"If \",dms_TradingName,\" does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank.\")","v":"If Essential Energy does not own any dual function assets,Table 2.16.3 and 2.16.4 may be left blank."},null,null,null,null,null,null,null,"Yes /  No"]
[null,"The total step changes in Table 2.16.1 and Table 2.16.3 must \"&\"reconcile (in each year) to the total step changes for each year in Table 2.17.1 and Table 2.17.3 of worksheet '2.17 Step Changes', respectively.\")",null,null,null,null,null,null,null,"Please nominate the base year.",null,"2016-17"]
[]
[]
[null,"2.16.1 - STANDARD CONTROL SERVICES - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Base year total opex, excluding category specific",null,null,297958047.22348124,348844305.55572826,348844305.55572826,348844305.55572826,348844305.55572826,348844305.55572826,348844305.55572826,348844305.55572826]
[null,"Increment from base year to final year",null,null,null,null,0]
[null,"Price growth",null,null,null,null,null,4262492.6064419188,6893703.5177108897,10227503.357027799,13661294.321883732,16619963.125960073]
[null,"Output growth",null,null,null,null,null,5247455.1158415023,7489803.9912121398,9841260.031771455,11953936.412442219,14323883.166550376]
[null,"Productivity growth",null,null,null,null,null,-9509947.7222834211,-14383507.50892303,-20068763.388799254,-25615230.734325953,-30943846.29251045]
[null,"Step changes",null,null,null,null,null,22625995.231605142,9530962.1473151464,-2730180.5778496368,-25948252.670481697,-49923674.648737073]
[null,"Category specific",null,null,23984645.324081514,1246063.1902966332,20280464.444817066,0,0,0,0,0]
[null,"Total opex",{"$f":"SUM(C18:C24)","v":0},{"$f":"SUM(D18:D24)","v":0},{"$f":"SUM(E18:E24)","v":321942692.54756278},350090368.74602491,369124770.00054532,371470300.78733337,358375267.70304334,346114124.97787869,322896052.88524657,298920630.90699118]
[]
[]
[null,"2.16.2 - STANDARD CONTROL SERVICES - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C32:C38)","v":0},{"$f":"SUM(D32:D38)","v":0},0,0,0,{"$f":"SUM(H32:H38)","v":0},0,0,0,0]
[]
[]
[null,"2.16.3 - DUAL FUNCTION ASSETS - OPEX BY DRIVER"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Base year total opex, excluding category specific",null,null,0,0,0,0,0,0,0,0]
[null,"Increment from base year to final year",null,null,null,null,0]
[null,"Price growth",null,null,null,null,null,0,0,0,0,0]
[null,"Output growth",null,null,null,null,null,0,0,0,0,0]
[null,"Productivity growth",null,null,null,null,null,0,0,0,0,0]
[null,"Step changes",null,null,null,null,null,0,0,0,0,0]
[null,"Category specific",null,null,0,0,0,0,0,0,0,0]
[null,"Total opex",{"$f":"SUM(C46:C52)","v":0},{"$f":"SUM(D46:D52)","v":0},0,0,0,{"$f":"SUM(H46:H52)","v":0},0,0,0,0]
[]
[]
[null,"2.16.4 - DUAL FUNCTION ASSETS - OPEX BY CATEGORY"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Vegetation management"]
[null,"Maintenance"]
[null,"Emergency response"]
[null,"Non-network"]
[null,"Metering"]
[null,"Network overheads"]
[null,"Corporate overheads"]
[null,"Total opex",{"$f":"SUM(C60:C66)","v":0},{"$f":"SUM(D60:D66)","v":0},0,0,0,{"$f":"SUM(H60:H66)","v":0},0,0,0,0]

{"sheet":"2.17 Step Changes","index":16,"n_rows":93,"n_cols":11,"rows_kept":93,"cut":false,"hidden":false,"merged":[[32,2,32,3],[41,2,41,3],[47,2,47,3],[48,2,48,3],[70,2,70,3],[57,2,57,3],[42,1,42,3],[50,2,50,3],[51,2,51,3],[52,2,52,3],[53,2,53,3],[49,2,49,3],[54,2,54,3],[55,2,55,3],[56,2,56,3],[23,2,23,3],[24,2,24,3],[25,1,25,3],[26,1,26,3],[31,2,31,3],[92,1,92,2],[58,1,58,3],[59,1,59,3],[79,3,79,10],[80,3,80,10],[64,2,64,3],[65,2,65,3],[66,2,66,3],[67,2,67,3],[73,2,73,3],[74,2,74,3],[75,1,75,3],[68,2,68,3],[69,2,69,3],[71,2,71,3],[72,2,72,3],[46,4,46,10],[63,4,63,10],[45,4,45,10],[62,4,62,10],[33,2,33,3],[34,2,34,3],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,2,38,3],[39,2,39,3],[40,2,40,3],[8,1,8,2],[5,1,5,2],[13,4,13,10],[30,4,30,10],[9,1,9,2],[12,4,12,10],[29,4,29,10],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"2.17 STEP CHANGES"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Complete the Tables below in accordance with the regulatory information notice. If \",dms_TradingName,\" does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\"&\"\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively.\")","v":"Complete the Tables below in accordance with the regulatory information notice. If Essential Energy does not own any dual function assets,Table 2.17.3 and 2.17.4 may be left blank.\n\nThe total step changes in Table 2.17.1 and Table 2.17.3 must reconcile (in each year) to the total step changes for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary', respectively."}]
[null," The total category specific forecast in Table 2.17.5 must reconcile (in each year) to the total category specific forecasts for each year in Table 2.16.1 and Table 2.16.3 of worksheet '2.16 Opex Summary'."]
[]
[null,"2.17.1 - STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST OPEX "]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Strategic Initiatives","Spend and benefits related to opex",0,0,0,27287922.009623453,14232245.169170959,2100330.9394465275,-20929857.678220078,-44887427.845677659]
[null,"Property lease expenditure ","Reduction due to accounting standard change",0,0,0,-4661926.7780183107,-4701283.0218558125,-4830511.5172961643,-5018394.9922616165,-5036246.8030594159]
[null,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[]
[null,"Total",null,null,{"$f":"SUM(E16:E25)","v":0},0,22625995.231605142,9530962.1473151464,-2730180.5778496368,-25948252.670481697,-49923674.648737073]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$23=0,\"OK\",\"Error\")","v":"OK"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$23=0,\"OK\",\"Error\")","v":"OK"}]
[]
[null,"2.17.2 -   STEP CHANGES FOR STANDARD CONTROL SERVICES - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Strategic Initiatives","Spend and benefits related to capex",0,0,-4437573.5644727238,1481416.8361965604,-29993007.748022389,-42665270.624340266,-57561698.794757172,-59420984.915737003]
[null,"Capitalised property leases ","Accounting standard change",0,0,0,26064831.202994082,1954317.4650326706,373837.23799451842,3461532.3637694358,86310.953747445019]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[null,null,null,null,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E33:E42)","v":0},-4437573.5644727238,27546248.039190643,-28038690.282989718,-42291433.386345744,-54100166.430987738,-59334673.961989559]
[]
[null,"2.17.3 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST OPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E49:E58)","v":0},0,0,0,0,0,0]
[null,"Check",null,null,null,null,{"$f":"IF(G$26-'2.16 Opex Summary'!H$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(H$26-'2.16 Opex Summary'!I$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(I$26-'2.16 Opex Summary'!J$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(J$26-'2.16 Opex Summary'!K$51=0,\"OK\",\"Error\")","v":"Error"},{"$f":"IF(K$26-'2.16 Opex Summary'!L$51=0,\"OK\",\"Error\")","v":"Error"}]
[]
[null,"2.17.4 - STEP CHANGES FOR DUAL FUNCTION ASSETS - FORECAST CAPEX"]
[null,null,null,null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,"Step change","Description",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total",null,null,{"$f":"SUM(E66:E75)","v":0},0,0,0,0,0,0]
[]
[]
[null,"2.17.5 - FORECAST CATEGORY SPECIFIC OPEX"]
[null,null,null,"EXPENDITURE"]
[null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal, \")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,"Category","Description",{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,null,null,null,null,null,0,0,0,0,0]
[null,"Recognised underspend","Adjust base year",0,-12802066.521248043,0,0,0,0,0,0]
[null,"Strategic investment initiative & vegetation management","Transformation program",0,0,20280464.444817066,0,0,0,0,0]
[null,null,null,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[null,"Total",null,{"$f":"SUM(D90:D92)","v":0},0,0,0,0,0,0,0]

{"sheet":"3.1 Revenue","index":17,"n_rows":53,"n_cols":17,"rows_kept":53,"cut":false,"hidden":false,"merged":[[31,2,31,8],[31,10,31,16],[45,2,45,8],[45,10,45,16],[8,2,8,8],[8,10,8,16],[43,2,43,8],[43,10,43,16],[44,2,44,8],[44,10,44,16],[9,2,9,8],[9,10,9,16],[29,2,29,8],[29,10,29,16],[30,2,30,8],[30,10,30,16],[10,2,10,8],[10,10,10,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.1 REVENUE"]
[]
[null,"There are THREE tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"3.1.1 - REVENUE GROUPING BY CHARGEABLE QUANTITY"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DREV0101","Revenue from Fixed Customer Charges ",311988895.40163529,313056406.98988903,331089222.81586736,342652039.3554129,354378557.89369851,365300276.69142449,375730621.18435031]
["DREV0102","Revenue from Energy Delivery charges where time of use is not a determinant",361894993.07528573,362374552.53072459,348360758.92237544,335821241.62844533,323598740.94416958,311519567.48412454,299400906.03370607]
["DREV0103","Revenue from On–Peak Energy Delivery charges ",22543029.614179965,21722419.529575016,27676809.060244128,31902303.898858912,36245888.848388724,40862610.779438652,46020394.766035624]
["DREV0104","Revenue from Shoulder period Energy Delivery Charges",46601417.823074594,45018617.560396001,53196593.990303427,56504920.635124266,59592416.016111523,62744850.094120055,66685971.037261553]
["DREV0105","Revenue from Off–Peak Energy Delivery charges ",25084728.689793125,24232886.410779666,28718562.255600281,31219792.462565567,33678194.896020249,36256242.413260713,39297477.132576488]
["DREV0106","Revenue from controlled load customer charges",8662158.7714441586,8673637.2948358692,8225032.3086709138,8185355.0074625332,8146449.7526813094,8082291.8024795605,8022079.220293968]
["DREV0107","Revenue from unmetered supplies",9064411.7571500968,8994973.1524505373,6412501.6033671703,6617001.6826798553,6867389.421056401,7083354.6042926991,7333609.0612479169]
["DREV0108","Revenue from Contracted Maximum Demand charges",10271041.936942989,10457651.895167463,9010849.1059860382,9206338.9154652003,9383595.8518261574,9593343.3781393897,9806087.6916867513]
["DREV0109","Revenue from Measured Maximum Demand charges",186196405.27962026,190860674.81028745,186760202.55173054,191614496.48001704,196309043.21947101,201441266.51667464,205551515.86798453]
["DREV0110","Revenue from metering charges",0,0,0,0,0,0,0,null,33177588.500000004,33535433.000000004,29524239.510345839,28849431.624901384,28238859.585057694,28287155.906611435,28315594.858676374]
["DREV0111","Revenue from connection charges",0,0,0,0,0,0,0,null,33924882,33883082.5,28859028.018901456,28738083.129536938,28856318.20679076,29182399.063632395,30469327.842011824]
["DREV0112","Revenue from public lighting charges",0,0,0,0,0,0,0,null,14809257.000000002,15007040.000000002,13939349.69156668,12157858.223062828,11127322.611789746,11276019.763350189,10373825.568771262]
["DREV0113","Revenue from other Sources",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV01","Total revenue by chargeable quantity",{"$f":"SUM(C13:C25)","v":982307082.34912622},{"$f":"SUM(D13:D25)","v":985391820.17410576},999450532.61414528,1013723490.0660316,1028200276.8434234,1042883803.7639546,1057848661.9951434,null,{"$f":"SUM(K13:K25)","v":81911727.5},{"$f":"SUM(L13:L25)","v":82425555.5},72322617.220813975,69745372.977501154,68222500.403638199,68745574.733594015,69158748.269459456]
[]
[]
[null,"3.1.2 - REVENUE GROUPING BY CUSTOMER TYPE OR CLASS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DREV0201","Revenue from residential Customers ",509269709.29476327,509944560.03637052,523801699.47585589,532329223.41986674,541540696.67884612,549670550.82245779,557715706.7576499,null,81911727.5,82425555.5,72322617.220813975,69745372.977501154,68222500.403638199,68745574.733594015,69158748.269459456]
["DREV0202","Revenue from Non residential customers not on demand tariffs ",200477110.60742766,200708534.10684228,209549920.16244313,210153438.14360967,210507480.66570517,211626549.15173438,212874391.64969784,null,0,0,0,0,0,0,0]
["DREV0203","Revenue from Non-residential low voltage demand tariff customers ",200445153.56324318,202327885.03073728,195919190.52251491,199093838.01391307,202259739.85348666,205876226.07440194,209650451.24695757,null,0,0,0,0,0,0,0]
["DREV0204","Revenue from Non-residential high voltage demand tariff customers ",63050697.126542136,63415867.847704723,63767220.84996438,65529988.80596219,67024970.22432901,68627123.111067891,70274503.279589772,null,0,0,0,0,0,0,0]
["DREV0205","Revenue from unmetered supplies",9064411.7571500968,8994973.1524505373,6412501.6033671703,6617001.6826798553,6867389.421056401,7083354.6042926991,7333609.0612479169,null,0,0,0,0,0,0,0]
["DREV0206","Revenue from Other Customers",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV02","Total revenue by customer class",{"$f":"SUM(C34:C39)","v":982307082.34912622},{"$f":"SUM(D34:D39)","v":985391820.17410541},999450532.61414552,1013723490.0660316,1028200276.8434234,1042883803.7639548,1057848661.9951429,null,{"$f":"SUM(K34:K39)","v":81911727.5},{"$f":"SUM(L34:L39)","v":82425555.5},72322617.220813975,69745372.977501154,68222500.403638199,68745574.733594015,69158748.269459456]
[]
[]
[null,"3.1.3 - REVENUE (penalties) ALLOWED (deducted) THROUGH INCENTIVE SCHEMES"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"REVENUE",null,null,null,null,null,null,null,"REVENUE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \", dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DREV0301","EBSS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0302","STPIS",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0303","F-Factor",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0304","S-Factor True  up",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DREV0305","Other",649088.30760869547,658824.63222282589,956091.67946060922,966796.39754952374,977653.98763256753,988666.63282296609,999890.27649635728,null,0,0,0,0,0,0,0]
["DREV03","Total revenue of incentive schemes",{"$f":"SUM(C48:C52)","v":649088.30760869547},{"$f":"SUM(D48:D52)","v":658824.63222282589},956091.67946060922,966796.39754952374,977653.98763256753,988666.63282296609,999890.27649635728,null,{"$f":"SUM(K48:K52)","v":0},{"$f":"SUM(L48:L52)","v":0},0,0,0,0,0]

{"sheet":"3.2 Operating expenditure","index":18,"n_rows":88,"n_cols":17,"rows_kept":88,"cut":false,"hidden":false,"merged":[[85,2,85,8],[72,2,72,8],[72,10,72,16],[70,2,70,8],[70,10,70,16],[83,2,83,8],[71,2,71,8],[71,10,71,16],[84,2,84,8],[12,2,12,8],[12,10,12,16],[14,10,14,16],[14,2,14,8],[13,2,13,8],[13,10,13,16]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.2 OPERATING EXPENDITURE"]
[]
[null,"There are THREE tables on this worksheet. Both ROWS and COLUMNS have been grouped for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(\"Forecasts for opex in table 3.2.1 are to be for the opex categories that \",dms_TradingName,\" has reported in its response to its annual reporting RIN.\")","v":"Forecasts for opex in table 3.2.1 are to be for the opex categories that Essential Energy has reported in its response to its annual reporting RIN."}]
[]
[null,"3.2.1 - OPEX CATEGORIES"]
[null,"CURRENT OPEX CATEGORIES AND COST ALLOCATIONS"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOPEX0101","Inspections",50663947.37561819,52293090.945672326,52578723.2861121,51996654.891449794,51390790.589550056,50909042.319208041,50432882.194737725]
["DOPEX0102","Maintenance and repair",60611845.249431401,65779768.896766499,64134171.78964591,60340309.536388993,57411045.273034237,56562719.772482365,56687675.985606059]
["DOPEX0103","Vegetation management",177311732.82899171,189611773.33895558,193007360.72178128,184996928.08046824,177006644.45833957,155707936.87172428,132662034.73163702]
["DOPEX0104","Emergency response",60953616.539176047,61440136.819150873,61750044.989794232,61041375.194736175,60305644.65695481,59716353.921831913,59138037.995010391]
["DOPEX0105","Other network costs",549226.75280753686,0,0,0,0,0,0]
["DOPEX0106","Public Lighting",null,null,null,null,null,null,null,null,13665650.260431457,15089049.950680476,10518810.949806917,11196243.844404235,12325876.196083881,10514784.749833614,13099192.283939559]
["DOPEX0107","Metering",null,null,null,null,null,null,null,null,18835554.171873815,18137529.922432382,19156594.380598921,17916526.525816083,17142540.918116547,17042678.087290764,16947598.116979472]
["DOPEX0108","Ancillary Network Services",null,null,null,null,null,null,null,null,26122770.324671473,24933215.219813682,19416582.393791981,19022936.033615522,18805677.497690018,18904453.080686875,19863086.648742501]
["DOPEX0109"]
["DOPEX0110"]
["DOPEX0111"]
["DOPEX0112"]
["DOPEX0113"]
["DOPEX0114"]
["DOPEX0115"]
["DOPEX0116"]
["DOPEX0117"]
["DOPEX0118"]
["DOPEX0119"]
["DOPEX0120"]
["DOPEX0121"]
["DOPEX0122"]
["DOPEX0123"]
["DOPEX0124"]
["DOPEX0125"]
["DOPEX0126"]
["DOPEX0127"]
["DOPEX0128"]
["DOPEX0129"]
["DOPEX0130"]
["DOPEX0131"]
["DOPEX0132"]
["DOPEX0133"]
["DOPEX0134"]
["DOPEX0135"]
["DOPEX0136"]
["DOPEX0137"]
["DOPEX0138"]
["DOPEX0139"]
["DOPEX0140"]
["DOPEX0141"]
["DOPEX0142"]
["DOPEX0143"]
["DOPEX0144"]
["DOPEX0145"]
["DOPEX0146"]
["DOPEX0147"]
["DOPEX0148"]
["DOPEX0149"]
["DOPEX01","Total opex ",{"$f":"SUM(C17:C65)","v":350090368.74602491},{"$f":"SUM(D17:D65)","v":369124770.00054526},371470300.78733355,358375267.70304322,346114124.97787869,322896052.88524657,298920630.90699118,null,{"$f":"SUM(K17:K65)","v":58623974.756976746},{"$f":"SUM(L17:L65)","v":58159795.092926539},49091987.72419782,48135706.403835841,48274094.61189045,46461915.917811252,49909877.049661532]
[]
[]
[null,"3.2.2 - OPEX CONSISTENCY"]
[null,"OPEX CONSISTENCY - CURRENT COST ALLOCATION APPROACH"]
[null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"EXPENDITURE",null,null,null,null,null,null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOPEX0201","Opex for network services",350090368.74602491,369124770.00054526,371470300.78733355,358375267.70304322,346114124.97787869,322896052.88524657,298920630.90699118]
["DOPEX0202","Opex for metering",0,0,0,0,0,0,0,null,18835554.171873815,18137529.922432382,19156594.380598921,17916526.525816083,17142540.918116547,17042678.087290764,16947598.116979472]
["DOPEX0203","Opex for connection services",0,0,0,0,0,0,0,null,26122770.324671473,24933215.219813682,19416582.393791981,19022936.033615522,18805677.497690018,18904453.080686875,19863086.648742501]
["DOPEX0204","Opex for public lighting",0,0,0,0,0,0,0,null,13665650.260431457,15089049.950680476,10518810.949806917,11196243.844404235,12325876.196083881,10514784.749833614,13099192.283939559]
["DOPEX0205","Opex for amounts payable for easement levy or similar direct charges on DNSP",0,0,0,0,0,0,0]
["DOPEX0207","Opex for transmission connection point planning",0,0,0,0,0,0,0]
[]
[]
[null,"3.2.4 - OPEX FOR HIGH VOLTAGE CUSTOMERS"]
[null,null,"End user costs (not standard control services)"]
[null,null,"EXPENDITURE"]
[null,null,{"$f":"CONCATENATE(\"Forecast ($0's, real \",dms_DollarReal,\")\")","v":"Forecast ($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOPEX0401","Opex for high voltage customers",1602354.6221884042,1642413.4877431141,1663911.0464832073,1685408.6052233004,1706906.1639633935,1728403.7227034867,1749901.2814435798]

{"sheet":"3.3 Assets (RAB)","index":19,"n_rows":137,"n_cols":25,"rows_kept":137,"cut":false,"hidden":false,"merged":[[115,2,115,8],[114,2,114,8],[8,2,8,8],[8,10,8,16],[8,18,8,24],[9,2,9,8],[9,10,9,16],[9,18,9,24],[114,10,114,16],[114,18,114,24],[115,18,115,24],[115,10,115,16],[21,2,21,8],[21,10,21,16],[21,18,21,24],[22,2,22,8],[98,2,98,8],[98,10,98,16],[98,18,98,24],[22,10,22,16],[22,18,22,24],[97,2,97,8],[97,10,97,16],[97,18,97,24]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.3 ASSETS"]
[]
[null,"There are FOUR tables on this worksheet. Both ROWS and COLUMNS in each have been  grouped (and sub-grouped) for ease of navigation. see the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"3.3.1 - REGULATORY ASSET BASE VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"For total asset base:"]
["DRAB0101","Opening value",7664343275.9796543,7900804799.2281771,8215248070.0069714,8437199357.4104128,8537401094.2928419,8613296562.1534405,8652538557.4282074,null,7664343275.9796543,7900804799.2281771,8215248070.0069714,8437199357.4104128,8537401094.2928419,8613296562.1534405,8652538557.4282074,null,96751683.001841307,93310068.225909486,91043614.527021185,87512839.646701321,82121965.001334816,76872476.014239758,71464579.570543066]
["DRAB0102","Inflation addition",97872969.625929281,154065693.58494946,0,0,0,0,0,null,97872969.625929281,154065693.58494946,0,0,0,0,0,null,1235510.2310427739,1819546.3304052348,0,0,0,0,0]
["DRAB0103","Straight line depreciation",-322756211.89397907,-333797423.13233435,-285823287.50720972,-318636750.19861978,-340555042.19176167,-363484965.31194329,-359407743.09144664,null,-322756211.89397907,-333797423.13233435,-285823287.50720972,-318636750.19861978,-340555042.19176167,-363484965.31194329,-359407743.09144664,null,-6824286.8396256473,-6990542.7256310321,-7091623.8936608946,-7329013.8278836301,-7458223.1067181043,-7605472.0480263075,-7751977.0883149477]
["DRAB0105","Actual additions (recognised in RAB)",463678654.18121845,499554430.16092509,513015444.5013333,424240311.4329384,422840369.92464429,410886048.03521901,397820175.02210248,null,463678654.18121845,499554430.16092509,513015444.5013333,424240311.4329384,422840369.92464429,410886048.03521901,397820175.02210248,null,2147161.8326510452,2904542.6963375197,3560849.013341039,1938139.182517108,2208734.119623052,2197575.6043296023,2008982.4936639119]
["DRAB0106","Disposals ",-2333888.6646453966,-5379429.8347530132,-5240869.5906824386,-5401824.3518881965,-6389859.8722828375,-8159087.4485103814,-6938091.4277375136,null,-2333888.6646453966,-5379429.8347530132,-5240869.5906824386,-5401824.3518881965,-6389859.8722828375,-8159087.4485103814,-6938091.4277375136,null,0,0,0,0,0,0,0]
["DRAB0107","Closing value",{"$f":"SUM(C13+C14+C15+C16+C17)","v":7900804799.2281771},8215248070.0069637,8437199357.4104128,8537401094.2928429,8613296562.1534424,8652538557.4282055,8684012897.9311256,null,{"$f":"SUM(K13+K14+K15+K16+K17)","v":7900804799.2281771},8215248070.0069637,8437199357.4104128,8537401094.2928429,8613296562.1534424,8652538557.4282055,8684012897.9311256,null,{"$f":"SUM(S13+S14+S15+S16+S17)","v":93310068.225909486},91043614.527021214,87512839.646701336,82121965.001334801,76872476.014239758,71464579.570543051,65721584.97589203]
[]
[]
[null,"3.3.2 - ASSET VALUE ROLL FORWARD"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"For overhead network assets less than 33kV:"]
["DRAB0201","Opening value",3485919088.2890596,3657886688.7132869,3850927649.3242731,3976029845.0228848,4082130372.0752234,4174410737.5457377,4263264094.9509449,null,3485919088.2890596,3657886688.7132869,3850927649.3242731,3976029845.0228848,4082130372.0752234,4174410737.5457377,4263264094.9509449,null,0,0,0,0,0,0,0]
["DRAB0202","Inflation addition",44514871.106546707,71328790.429909095,0,0,0,0,0,null,44514871.106546707,71328790.429909095,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0203","Straight line depreciation",-93640674.235864922,-98802317.298099026,-96502353.100900576,-100113539.92858128,-103474751.80381157,-106665167.22845155,-109849022.36587982,null,-93640674.235864922,-98802317.298099026,-96502353.100900576,-100113539.92858128,-103474751.80381157,-106665167.22845155,-109849022.36587982,null,0,0,0,0,0,0,0]
["DRAB0205","Actual additions (recognised in RAB)",221093403.5535453,220514487.47917256,221604548.79951248,206214066.98091993,195755117.27432585,195518524.63365886,193689598.91909385,null,221093403.5535453,220514487.47917256,221604548.79951248,206214066.98091993,195755117.27432585,195518524.63365886,193689598.91909385,null,0,0,0,0,0,0,0]
["DRAB0206","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0207","Closing value",{"$f":"SUM(C26+C27+C28+C29+C30)","v":3657886688.7132869},3850927649.3242698,3976029845.0228848,4082130372.0752234,4174410737.5457377,4263264094.9509449,4347104671.504159,null,{"$f":"SUM(K26+K27+K28+K29+K30)","v":3657886688.7132869},3850927649.3242698,3976029845.0228848,4082130372.0752234,4174410737.5457377,4263264094.9509449,4347104671.504159,null,{"$f":"SUM(S26+S27+S28+S29+S30)","v":0},0,0,0,0,0,0]
[null,"For underground network assets less than 33kV:"]
["DRAB0301","Opening value",617211945.34416938,615736060.21401036,615711784.04849505,603129835.18526113,589647846.43937933,575352777.00354445,560346531.22317266,null,617211945.34416938,615736060.21401036,615711784.04849505,603129835.18526113,589647846.43937933,575352777.00354445,560346531.22317266,null,0,0,0,0,0,0,0]
["DRAB0302","Inflation addition",7881740.6533385264,12006853.174173202,0,0,0,0,0,null,7881740.6533385264,12006853.174173202,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0303","Straight line depreciation",-16534343.577988969,-17445746.454082683,-17039636.624525439,-17677271.970708285,-18270768.679665003,-18834107.476806097,-19396287.909341063,null,-16534343.577988969,-17445746.454082683,-17039636.624525439,-17677271.970708285,-18270768.679665003,-18834107.476806097,-19396287.909341063,null,0,0,0,0,0,0,0]
["DRAB0305","Actual additions (recognised in RAB)",7176717.7944914168,5414617.1143941442,4457687.7612914946,4195283.2248265045,3975699.2438300364,3827861.696434278,3741265.9734853101,null,7176717.7944914168,5414617.1143941442,4457687.7612914946,4195283.2248265045,3975699.2438300364,3827861.696434278,3741265.9734853101,null,0,0,0,0,0,0,0]
["DRAB0306","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0307","Closing value",{"$f":"SUM(C33+C34+C35+C36+C37)","v":615736060.21401036},615711784.04849505,603129835.18526113,589647846.43937933,575352777.00354445,560346531.22317266,544691509.28731692,null,{"$f":"SUM(K33+K34+K35+K36+K37)","v":615736060.21401036},615711784.04849505,603129835.18526113,589647846.43937933,575352777.00354445,560346531.22317266,544691509.28731692,null,{"$f":"SUM(S33+S34+S35+S36+S37)","v":0},0,0,0,0,0,0]
[null,"For distribution substations and transformers:"]
["DRAB0401","Opening value",602595267.86592138,599011004.45577657,596967332.2271744,585913394.36772656,575407389.70653796,563952233.9166615,551447829.20595264,null,602595267.86592138,599011004.45577657,596967332.2271744,585913394.36772656,575407389.70653796,563952233.9166615,551447829.20595264,null,0,0,0,0,0,0,0]
["DRAB0402","Inflation addition",7695087.0054853493,11680714.586887643,0,0,0,0,0,null,7695087.0054853493,11680714.586887643,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0403","Straight line depreciation",-26519159.023432758,-27245757.9453297,-24736378.471465617,-25249413.292157337,-25767404.524693754,-26298023.283630416,-26813409.497645367,null,-26519159.023432758,-27245757.9453297,-24736378.471465617,-25249413.292157337,-25767404.524693754,-26298023.283630416,-26813409.497645367,null,0,0,0,0,0,0,0]
["DRAB0405","Actual additions (recognised in RAB)",15239808.607802605,13521371.1298395,13682440.612017784,14743408.630968697,14312248.734817233,13793618.572921537,13347086.036563197,null,15239808.607802605,13521371.1298395,13682440.612017784,14743408.630968697,14312248.734817233,13793618.572921537,13347086.036563197,null,0,0,0,0,0,0,0]
["DRAB0406","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0407","Closing value",{"$f":"SUM(C40+C41+C42+C43+C44)","v":599011004.45577657},596967332.22717404,585913394.36772656,575407389.70653796,563952233.9166615,551447829.20595264,537981505.74487042,null,{"$f":"SUM(K40+K41+K42+K43+K44)","v":599011004.45577657},596967332.22717404,585913394.36772656,575407389.70653796,563952233.9166615,551447829.20595264,537981505.74487042,null,{"$f":"SUM(S40+S41+S42+S43+S44)","v":0},0,0,0,0,0,0]
[null,"For overhead network assets 33kV and above:"]
["DRAB0501","Opening value",974193838.39612103,982760254.06315994,999624891.38854432,1002959471.946038,1000424084.8509016,993103577.89278734,983206815.61221886,null,974193838.39612103,982760254.06315994,999624891.38854432,1002959471.946038,1000424084.8509016,993103577.89278734,983206815.61221886,null,0,0,0,0,0,0,0]
["DRAB0502","Inflation addition",12440367.102806177,19163824.95423162,0,0,0,0,0,null,12440367.102806177,19163824.95423162,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0503","Straight line depreciation",-28745709.265297592,-29710987.260212231,-28370781.373372395,-28969252.274304934,-29467201.146965764,-29890838.070868362,-30275715.269439798,null,-28745709.265297592,-29710987.260212231,-28370781.373372395,-28969252.274304934,-29467201.146965764,-29890838.070868362,-30275715.269439798,null,0,0,0,0,0,0,0]
["DRAB0505","Actual additions (recognised in RAB)",24871757.829530247,27411799.631364424,31705361.930866159,26433865.179168582,22146694.188851427,19994075.79029984,23471508.196554814,null,24871757.829530247,27411799.631364424,31705361.930866159,26433865.179168582,22146694.188851427,19994075.79029984,23471508.196554814,null,0,0,0,0,0,0,0]
["DRAB0506","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0507","Closing value",{"$f":"SUM(C47+C48+C49+C50+C51)","v":982760254.06315994},999624891.38854384,1002959471.946038,1000424084.8509016,993103577.89278734,983206815.61221886,976402608.53933382,null,{"$f":"SUM(K47+K48+K49+K50+K51)","v":982760254.06315994},999624891.38854384,1002959471.946038,1000424084.8509016,993103577.89278734,983206815.61221886,976402608.53933382,null,{"$f":"SUM(S47+S48+S49+S50+S51)","v":0},0,0,0,0,0,0]
[null,"For underground network assets 33kV and above:"]
["DRAB0601","Opening value",23407542.124281406,30296258.821932282,36723811.707227938,37956524.272548154,38797519.188040018,39737741.539199017,40642232.53420265,null,23407542.124281406,30296258.821932282,36723811.707227938,37956524.272548154,38797519.188040018,39737741.539199017,40642232.53420265,null,0,0,0,0,0,0,0]
["DRAB0602","Inflation addition",298912.1933678817,590777.04702767951,0,0,0,0,0,null,298912.1933678817,590777.04702767951,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0603","Straight line depreciation",-700872.3869708787,-724407.61047649628,-691730.96679820598,-706322.76987385924,-718463.66407654877,-728792.69855346309,-738176.70081842283,null,-700872.3869708787,-724407.61047649628,-691730.96679820598,-706322.76987385924,-718463.66407654877,-728792.69855346309,-738176.70081842283,null,0,0,0,0,0,0,0]
["DRAB0605","Actual additions (recognised in RAB)",7290676.8912538709,6561183.4487443976,1924443.5321184224,1547317.6853657234,1658686.0152355484,1633283.693557095,1431996.1704348437,null,7290676.8912538709,6561183.4487443976,1924443.5321184224,1547317.6853657234,1658686.0152355484,1633283.693557095,1431996.1704348437,null,0,0,0,0,0,0,0]
["DRAB0606","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0607","Closing value",{"$f":"SUM(C54+C55+C56+C57+C58)","v":30296258.821932282},36723811.707227863,37956524.272548154,38797519.188040018,39737741.539199017,40642232.53420265,41336052.003819078,null,{"$f":"SUM(K54+K55+K56+K57+K58)","v":30296258.821932282},36723811.707227863,37956524.272548154,38797519.188040018,39737741.539199017,40642232.53420265,41336052.003819078,null,{"$f":"SUM(S54+S55+S56+S57+S58)","v":0},0,0,0,0,0,0]
[null,"Zone substations and transformers"]
["DRAB0701","Opening value",1370991067.8699787,1400445016.9337816,1432356733.9729328,1433462915.8370333,1433119573.3397801,1434150815.4805942,1432374500.6691566,null,1370991067.8699787,1400445016.9337816,1432356733.9729328,1433462915.8370333,1433119573.3397801,1434150815.4805942,1432374500.6691566,null,0,0,0,0,0,0,0]
["DRAB0702","Inflation addition",17507431.793092221,27308677.830208741,0,0,0,0,0,null,17507431.793092221,27308677.830208741,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0703","Straight line depreciation",-60421533.284067333,-62077023.976844214,-56359627.159378789,-57528531.138080359,-58708727.858115822,-59917695.268278137,-61091956.686475366,null,-60421533.284067333,-62077023.976844214,-56359627.159378789,-57528531.138080359,-58708727.858115822,-59917695.268278137,-61091956.686475366,null,0,0,0,0,0,0,0]
["DRAB0705","Actual additions (recognised in RAB)",72368050.554778025,66680063.185784027,57465809.02347929,57185188.640827231,59739969.998929866,58141380.456840552,49241702.350335054,null,72368050.554778025,66680063.185784027,57465809.02347929,57185188.640827231,59739969.998929866,58141380.456840552,49241702.350335054,null,0,0,0,0,0,0,0]
["DRAB0706","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0707","Closing value",{"$f":"SUM(C61+C62+C63+C64+C65)","v":1400445016.9337816},1432356733.9729302,1433462915.8370333,1433119573.3397801,1434150815.4805942,1432374500.6691566,1420524246.3330164,null,{"$f":"SUM(K61+K62+K63+K64+K65)","v":1400445016.9337816},1432356733.9729302,1433462915.8370333,1433119573.3397801,1434150815.4805942,1432374500.6691566,1420524246.3330164,null,{"$f":"SUM(S61+S62+S63+S64+S65)","v":0},0,0,0,0,0,0]
[null,"For easements:"]
["DRAB0801","Opening value",106359415.49511483,107866312.20313682,110328012.83317594,110344573.9043301,110360285.83168721,110375544.55101632,110390490.33591647,null,106359415.49511483,107866312.20313682,110328012.83317594,110344573.9043301,110360285.83168721,110375544.55101632,110390490.33591647,null,0,0,0,0,0,0,0]
["DRAB0802","Inflation addition",1358200.1049991332,2103393.087961168,0,0,0,0,0,null,1358200.1049991332,2103393.087961168,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0803","Actual additions (recognised in RAB)",148696.60302283824,358307.54207805789,16561.071154165824,15711.927357100478,15258.71932910519,14945.784900162878,14907.919573342975,null,148696.60302283824,358307.54207805789,16561.071154165824,15711.927357100478,15258.71932910519,14945.784900162878,14907.919573342975,null,0,0,0,0,0,0,0]
["DRAB0804","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0805","Closing value",{"$f":"SUM(C68+C69+C70+C71)","v":107866312.20313682},{"$f":"SUM(D68+D69+D70+D71)","v":110328012.83317605},{"$f":"SUM(E68+E69+E70+E71)","v":110344573.9043301},110360285.83168721,110375544.55101632,110390490.33591647,110405398.25548981,null,{"$f":"SUM(K68+K69+K70+K71)","v":107866312.20313682},{"$f":"SUM(L68+L69+L70+L71)","v":110328012.83317605},{"$f":"SUM(M68+M69+M70+M71)","v":110344573.9043301},110360285.83168721,110375544.55101632,110390490.33591647,110405398.25548981,null,{"$f":"SUM(S68+S69+S70+S71)","v":0},{"$f":"SUM(T68+T69+T70+T71)","v":0},{"$f":"SUM(U68+U69+U70+U71)","v":0},0,0,0,0]
[null,"For meters:"]
["DRAB0901","Opening value",34537629.44879216,37277308.145104185,40385151.608536005,44866933.669337071,48088878.352317259,50546110.95437251,52630116.286371469,null,34537629.44879216,37277308.145104185,40385151.608536005,44866933.669337071,48088878.352317259,50546110.95437251,52630116.286371469,null,96561083.881480873,93130291.761263862,90873632.984157667,87356011.881787449,81978291.014370576,76741955.805225164,71347213.139478102]
["DRAB0902","Inflation addition",441042.40066950378,726907.50882953161,0,0,0,0,0,null,441042.40066950378,726907.50882953161,0,0,0,0,0,null,1233076.2975345724,1816040.6893446452,0,0,0,0,0]
["DRAB0903","Straight line depreciation",-1876103.7287679131,-2143674.8059328836,-2008356.8151439216,-2259190.7497223327,-2471028.2454711017,-2661497.9846619722,-2844904.424990207,null,-1876103.7287679131,-2143674.8059328836,-2008356.8151439216,-2259190.7497223327,-2471028.2454711017,-2661497.9846619722,-2844904.424990207,null,-6811030.250402634,-6977242.1627883343,-7078470.1157112559,-7315860.0499339914,-7445069.3287684657,-7592318.2700766688,-7738823.310365309]
["DRAB0905","Actual additions (recognised in RAB)",4174740.0244104401,4524610.760535432,6490138.8759449869,5481135.4327025162,4928260.8475263575,4745503.3166609323,4650493.1532653496,null,4174740.0244104401,4524610.760535432,6490138.8759449869,5481135.4327025162,4928260.8475263575,4745503.3166609323,4650493.1532653496,null,2147161.8326510452,2904542.6963375197,3560849.013341039,1938139.182517108,2208734.119623052,2197575.6043296023,2008982.4936639119]
["DRAB0906","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB0907","Closing value",{"$f":"SUM(C74+C75+C76+C77+C78)","v":37277308.145104185},40385151.608536266,44866933.669337071,48088878.352317259,50546110.95437251,52630116.286371469,54435705.014646612,null,{"$f":"SUM(K74+K75+K76+K77+K78)","v":37277308.145104185},40385151.608536266,44866933.669337071,48088878.352317259,50546110.95437251,52630116.286371469,54435705.014646612,null,{"$f":"SUM(S74+S75+S76+S77+S78)","v":93130291.761263862},90873632.984157696,87356011.881787449,81978291.014370576,76741955.805225164,71347213.139478102,65617372.322776705]
[null,"For “other” asset items with long lives:"]
["DRAB1001","Opening value",312597661.88327092,314416891.02281958,334742440.5922761,333064599.23976874,325151558.82901651,321078296.39247948,316521495.40499759,null,312597661.88327092,314416891.02281958,334742440.5922761,333064599.23976874,325151558.82901651,321078296.39247948,316521495.40499759,null,190599.12036043455,179776.4646456232,169981.54286351457,156827.76491387634,143673.98696423811,130520.20901459988,117366.43106496165]
["DRAB1002","Inflation addition",3991843.8364475868,6131129.3749449821,0,0,0,0,0,null,3991843.8364475868,6131129.3749449821,0,0,0,0,0,null,2433.9335082014886,3505.6410605896526,0,0,0,0,0]
["DRAB1003","Straight line depreciation",-22039109.068168566,-22778684.861079477,-18852719.38596265,-19335070.145056579,-19699894.969655514,-20149077.245907318,-20598868.665333834,null,-22039109.068168566,-22778684.861079477,-18852719.38596265,-19335070.145056579,-19699894.969655514,-20149077.245907318,-20598868.665333834,null,-13256.589223012848,-13300.562842697836,-13153.777949638225,-13153.777949638225,-13153.777949638225,-13153.777949638225,-13153.777949638225]
["DRAB1005","Actual additions (recognised in RAB)",19866494.371269632,36973105.055590831,17174878.033455312,11422029.734304355,15626632.533118475,15592276.258425413,15259178.248558218,null,19866494.371269632,36973105.055590831,17174878.033455312,11422029.734304355,15626632.533118475,15592276.258425413,15259178.248558218,null,0,0,0,0,0,0,0]
["DRAB1006","Disposals ",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1007","Closing value",{"$f":"SUM(C81+C82+C83+C84+C85)","v":314416891.02281958},334742440.59227592,333064599.23976874,325151558.82901651,321078296.39247948,316521495.40499759,311181804.988222,null,{"$f":"SUM(K81+K82+K83+K84+K85)","v":314416891.02281958},334742440.59227592,333064599.23976874,325151558.82901651,321078296.39247948,316521495.40499759,311181804.988222,null,{"$f":"SUM(S81+S82+S83+S84+S85)","v":179776.4646456232},169981.54286351503,156827.76491387634,143673.98696423811,130520.20901459988,117366.43106496165,104212.65311532342]
[null,"For “other” asset items with short lives:"]
["DRAB1101","Opening value",136529819.2629444,155109004.65516916,197480262.30433613,309471263.96548468,334273585.67995942,350588726.87705028,341714451.20527428,null,136529819.2629444,155109004.65516916,197480262.30433613,309471263.96548468,334273585.67995942,350588726.87705028,341714451.20527428,null,0,0,0,0,0,0,0]
["DRAB1102","Inflation addition",1743473.4291761967,3024625.5907757985,0,0,0,0,0,null,1743473.4291761967,3024625.5907757985,0,0,0,0,0,null,0,0,0,0,0,0,0]
["DRAB1103","Straight line depreciation",-72278707.323420152,-72868822.92027764,-41261703.609662138,-66798157.930134818,-81976801.299306631,-98339766.054785907,-87799401.571522757,null,-72278707.323420152,-72868822.92027764,-41261703.609662138,-66798157.930134818,-81976801.299306631,-98339766.054785907,-87799401.571522757,null,0,0,0,0,0,0,0]
["DRAB1105","Actual additions (recognised in RAB)",91448307.951114103,117594884.81342165,158493574.86149317,97002303.996497735,104681802.36868037,97624577.831520319,92972438.054238513,null,91448307.951114103,117594884.81342165,158493574.86149317,97002303.996497735,104681802.36868037,97624577.831520319,92972438.054238513,null,0,0,0,0,0,0,0]
["DRAB1106","Disposals ",-2333888.6646453966,-5379429.8347530132,-5240869.5906824386,-5401824.3518881965,-6389859.8722828375,-8159087.4485103814,-6938091.4277375136,null,-2333888.6646453966,-5379429.8347530132,-5240869.5906824386,-5401824.3518881965,-6389859.8722828375,-8159087.4485103814,-6938091.4277375136,null,0,0,0,0,0,0,0]
["DRAB1107","Closing value",{"$f":"SUM(C88+C89+C90+C91+C92)","v":155109004.65516916},197480262.30433595,309471263.96548468,334273585.67995942,350588726.87705028,341714451.20527428,339949396.26025248,null,{"$f":"SUM(K88+K89+K90+K91+K92)","v":155109004.65516916},197480262.30433595,309471263.96548468,334273585.67995942,350588726.87705028,341714451.20527428,339949396.26025248,null,{"$f":"SUM(S88+S89+S90+S91+S92)","v":0},0,0,0,0,0,0]
[]
[]
[]
[null,"3.3.3 - TOTAL DISAGGREGATED RAB ASSET VALUES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"},null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Forecast\n($0's, real \", dms_DollarReal,\")\")","v":"Forecast\n($0's, real June 2019)"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DRAB1201","Overhead network assets less than 33kV (wires and poles)",3571902888.501173,3754407169.0187783,3913478747.1735792,4029080108.5490541,4128270554.8104806,4218837416.2483416,4305184383.2275524,null,3571902888.501173,3754407169.0187783,3913478747.1735792,4029080108.5490541,4128270554.8104806,4218837416.2483416,4305184383.2275524,null,0,0,0,0,0,0,0]
["DRAB1202","Underground network assets less than 33kV (cables)",616474002.77908993,615723922.13125277,609420809.61687803,596388840.81232023,582500311.72146189,567849654.1133585,552519020.25524473,null,616474002.77908993,615723922.13125277,609420809.61687803,596388840.81232023,582500311.72146189,567849654.1133585,552519020.25524473,null,0,0,0,0,0,0,0]
["DRAB1203","Distribution substations including transformers",600803136.16084898,597989168.34147525,591440363.29745054,580660392.03713226,569679811.81159973,557700031.56130707,544714667.47541153,null,600803136.16084898,597989168.34147525,591440363.29745054,580660392.03713226,569679811.81159973,557700031.56130707,544714667.47541153,null,0,0,0,0,0,0,0]
["DRAB1204","Overhead network assets 33kV and above (wires and towers / poles etc) ",978477046.22964048,991192572.72585189,1001292181.6672912,1001691778.3984698,996763831.37184453,988155196.75250316,979804712.07577634,null,978477046.22964048,991192572.72585189,1001292181.6672912,1001691778.3984698,996763831.37184453,988155196.75250316,979804712.07577634,null,0,0,0,0,0,0,0]
["DRAB1205","Underground network assets 33kV and above(cables, ducts etc)",26851900.473106846,33510035.264580071,37340167.989888042,38377021.730294086,39267630.363619521,40189987.03670083,40989142.269010864,null,26851900.473106846,33510035.264580071,37340167.989888042,38377021.730294086,39267630.363619521,40189987.03670083,40989142.269010864,null,0,0,0,0,0,0,0]
["DRAB1206","Zone substations and transformers",1385718042.4018803,1416400875.4533558,1432909824.904983,1433291244.5884066,1433635194.4101872,1433262658.0748754,1426449373.5010865,null,1385718042.4018803,1416400875.4533558,1432909824.904983,1433291244.5884066,1433635194.4101872,1433262658.0748754,1426449373.5010865,null,0,0,0,0,0,0,0]
["DRAB1207","Easements ",107112863.84912583,109097162.51815644,110336293.36875302,110352429.86800866,110367915.19135177,110383017.4434664,110397944.29570314,null,107112863.84912583,109097162.51815644,110336293.36875302,110352429.86800866,110367915.19135177,110383017.4434664,110397944.29570314,null,0,0,0,0,0,0,0]
["DRAB1208","Meters",35907468.796948172,38831229.876820222,42626042.638936535,46477906.010827169,49317494.653344885,51588113.62037199,53532910.650509045,null,35907468.796948172,38831229.876820222,42626042.638936535,46477906.010827169,49317494.653344885,51588113.62037199,53532910.650509045,null,94845687.82137236,92001962.372710779,89114822.43297255,84667151.44807902,79360123.409797877,74044584.47235164,68482292.731127411]
["DRAB1209","“Other” assets with long lives",313507276.45304525,324579665.80754775,333903519.91602242,329108079.0343926,323114927.61074799,318799895.8987385,313851650.1966098,null,313507276.45304525,324579665.80754775,333903519.91602242,329108079.0343926,323114927.61074799,318799895.8987385,313851650.1966098,null,185187.79250302888,174879.0037545691,163404.65388869547,150250.87593905721,137097.09798941901,123943.32003978077,110789.54209014254]
["DRAB1210","“Other” assets with short lives",145819411.95905679,176294633.47975254,253475763.1349104,321872424.82272208,342431156.27850485,346151589.04116225,340831923.73276341,null,145819411.95905679,176294633.47975254,253475763.1349104,321872424.82272208,342431156.27850485,346151589.04116225,340831923.73276341,null,0,0,0,0,0,0,0]
["DRAB13","Value of Capital Contributions or Contributed Assets (included in the above)",0,0,0,0,0,0,0,null,0,0,0,0,0,0,0,null,0,0,0,0,0,0,0]
[]
[]
[null,"3.3.4 - ASSET LIVES"]
[null,null,"Network services",null,null,null,null,null,null,null,"Standard control services",null,null,null,null,null,null,null,"Alternative control services"]
[null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )",null,null,null,null,null,null,null,"Forecast\n( years )"]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Estimated service life of new assets"]
["DRAB1401","Overhead network assets less than 33kV (wires and poles)",53,53,53,53,53,53,53,null,53,53,53,53,53,53,53,null,0,0,0,0,0,0,0]
["DRAB1402","Underground network assets less than 33kV (cables)",54,54,54,54,54,54,54,null,54,54,54,54,54,54,54,null,0,0,0,0,0,0,0]
["DRAB1403","Distribution substations including transformers",45,45,45,45,45,45,45,null,45,45,45,45,45,45,45,null,0,0,0,0,0,0,0]
["DRAB1404","Overhead network assets 33kV and above (wires and towers / poles etc) ",55,55,55,55,55,55,55,null,55,55,55,55,55,55,55,null,0,0,0,0,0,0,0]
["DRAB1405","Underground network assets 33kV and above(cables, ducts etc)",54,54,54,54,54,54,54,null,54,54,54,54,54,54,54,null,0,0,0,0,0,0,0]
["DRAB1406","Zone substations and transformers",46,46,46,46,46,46,46,null,46,46,46,46,46,46,46,null,0,0,0,0,0,0,0]
["DRAB1407","Meters",26,26,26,26,26,26,26,null,26,26,26,26,26,26,26,null,15,15,15,15,15,15,15]
["DRAB1408","“Other” assets with long lives",30,34,34,38,40,43,45,null,30,34,34,38,40,43,45,null,15,15,15,15,15,15,15]
["DRAB1409","“Other” assets with short lives",6,6,6,6,6,6,7,null,6,6,6,6,6,6,7,null,0,0,0,0,0,0,0]
[null,"Estimated residual service life"]
["DRAB1501","Overhead network assets less than 33kV (wires and poles)",9.6017083741574822,8.7409797847366164,7.900154167763759,7.059772616258762,6.2224171857054387,5.3863884944894949,4.5538889316682543,null,9.6017083741574822,8.7409797847366164,7.900154167763759,7.059772616258762,6.2224171857054387,5.3863884944894949,4.5538889316682543,null,0,0,0,0,0,0,0]
["DRAB1502","Underground network assets less than 33kV (cables)",34.21573365268393,33.226989772334278,32.235721289624237,31.244775355964212,30.254030659857257,29.263483594363127,28.273164654319039,null,34.21573365268393,33.226989772334278,32.235721289624237,31.244775355964212,30.254030659857257,29.263483594363127,28.273164654319039,null,0,0,0,0,0,0,0]
["DRAB1503","Distribution substations including transformers",20.770877599199217,19.919258344283794,19.100192318325515,18.308984971625954,17.519429480334384,16.729517650013449,15.936688889835157,null,20.770877599199217,19.919258344283794,19.100192318325515,18.308984971625954,17.519429480334384,16.729517650013449,15.936688889835157,null,0,0,0,0,0,0,0]
["DRAB1504","Overhead network assets 33kV and above (wires and towers / poles etc) ",15.211397727683341,14.27609652159628,13.38807210220434,12.499280832275879,11.639281659415602,10.75065220908094,9.8637673741677219,null,15.211397727683341,14.27609652159628,13.38807210220434,12.499280832275879,11.639281659415602,10.75065220908094,9.8637673741677219,null,0,0,0,0,0,0,0]
["DRAB1505","Underground network assets 33kV and above (cables, ducts etc)",40.128859064442011,39.389102593245049,38.508999865351697,37.634305884645322,36.763144123645731,35.895298205854971,35.031046462482479,null,40.128859064442011,39.389102593245049,38.508999865351697,37.634305884645322,36.763144123645731,35.895298205854971,35.031046462482479,null,0,0,0,0,0,0,0]
["DRAB1506","Zone substations and transformers",20.459465872623738,19.692259002350411,18.904708782733977,18.136774690373588,17.36588164840644,16.57887166200284,15.795709487512919,null,20.459465872623738,19.692259002350411,18.904708782733977,18.136774690373588,17.36588164840644,16.57887166200284,15.795709487512919,null,0,0,0,0,0,0,0]
["DRAB1507","Meters",20.083954243014766,19.884712981450932,19.869863162181666,19.646084502121795,19.329675023436032,18.987994609435543,18.638472608487039,null,20.083954243014766,19.884712981450932,19.869863162181666,19.646084502121795,19.329675023436032,18.987994609435543,18.638472608487039,null,13.786727644408142,12.855593126739326,11.974159543109245,11.061540844561382,10.191106454198035,9.3528186219352882,8.534862836544308]
["DRAB1508","“Other” assets with long lives",23.825524494670727,27.048758509003797,28.775479344808133,29.865606007065253,31.446833876792894,33.143547087691829,34.954061643366835,null,23.825524494670727,27.048758509003797,28.775479344808133,29.865606007065253,31.446833876792894,33.143547087691829,34.954061643366835,null,13.922640439448021,12.922640439448021,11.922640439448021,10.922640439448021,9.9226404394480205,8.9226404394480205,7.9226404394480205]
["DRAB1509","“Other” assets with short lives",3.8481406280484407,4.2193093697025787,4.4511248126485068,4.2754273212034253,4.1762793906949707,4.0975749279481519,4.0896816271997354,null,3.8481406280484407,4.2193093697025787,4.4511248126485068,4.2754273212034253,4.1762793906949707,4.0975749279481519,4.0896816271997354,null,0,0,0,0,0,0,0]

{"sheet":"3.4 Operational data","index":20,"n_rows":88,"n_cols":10,"rows_kept":88,"cut":false,"hidden":false,"merged":[[44,3,44,9],[45,3,45,9],[9,3,9,9],[10,3,10,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.4 OPERATIONAL DATA"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[null,"3.4.1 - ENERGY DELIVERY"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOPED01","Total energy delivered","GWh",12306.4,12287.1,12288.6,12272.2,12248.6,12279.6,12307.1]
[null,"3.4.1.1 - Energy grouping - delivery by chargeable quantity"]
["DOPED0201","Energy Delivery where time of use is not a determinant","GWh",4368.2299999999977,4183.4378306290655,4007.9016488788789,3809.311332512274,3619.4845603521617,3444.6569356631089,3271.116836872362]
["DOPED0202","Energy Delivery at On-peak times","GWh",1085.0819999999999,1117.8364915815223,1152.2536295238865,1188.2206703349423,1221.3405072957344,1260.9625719947003,1299.6028842704914]
["DOPED0203","Energy Delivery at Shoulder times ","GWh",2252.9489999999996,2303.4806690748833,2358.3507179511657,2413.1648846806174,2462.8824827039489,2526.1986143128011,2588.040455849371]
["DOPED0204","Energy Delivery at Off-peak times","GWh",3417.1149999999998,3509.6400087145284,3607.7060036460689,3709.299112472168,3802.5974496481554,3915.0828780293891,4024.808823007776]
["DOPED0205","Controlled load energy deliveries","GWh",1023.77,1010.16,996.76,983.55,970.53,957.71,945.07]
["DOPED0206","Energy Delivery to unmetered supplies","GWh",159.25,162.54,165.63,168.65,171.76,174.99,178.46]
[null,"3.4.1.2 - Energy - received from TNSP and other DNSPs by time of receipt"]
["DOPED0301","Energy into DNSP network at On-peak times","GWh",1795.2956625549564,1635.5820457179821,1425.5829860879705,1340.435785316429,1246.1808368508,1153.2992132443533,1050.0711091951766]
["DOPED0302","Energy into DNSP network at Shoulder times ","GWh",3114.848989128343,2837.7448840325328,2473.3952271768221,2325.6643114384647,2162.1313975725175,2000.9812107629484,1821.8798169069546]
["DOPED0303","Energy into DNSP network at Off-peak times","GWh",5478.3395492690015,4990.9739069827647,4350.1623806834441,4090.3359424952969,3802.7172384213873,3519.2892312042536,3204.288968682677]
["DOPED0304","Energy received from TNSP and other DNSPs not included in the above categories","GWh",0,0,0,0,0,0,0]
[null,"3.4.1.3 - Energy - received into DNSP system from embedded generation by time of receipt"]
["DOPED0401","Energy into DNSP network at On-peak times from non-residential embedded generation","GWh",359.28635855336427,485.9597341158364,657.29426559026558,723.02369214929229,795.32606136422146,874.85866750064361,962.34453425070808]
["DOPED0402","Energy into DNSP network at Shoulder times from non-residential embedded generation","GWh",905.39355001044282,1224.607609943303,1656.3667791909409,1822.003457110035,2004.2038028210386,2204.6241831031425,2425.0866014134572]
["DOPED0403","Energy into DNSP network at Off-peak times from non-residential embedded generation","GWh",1255.6523199841513,1698.3569039980673,2297.1455772042914,2526.8601349247206,2779.5461484171929,3057.5007632589122,3363.2508395848035]
["DOPED0404","Energy received from embedded generation not included in above categories from non-residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0405","Energy into DNSP network at On-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0406","Energy into DNSP network at Shoulder times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0407","Energy into DNSP network at Off-peak times from residential embedded generation","GWh",0,0,0,0,0,0,0]
["DOPED0408","Energy received from embedded generation not included in above categories from residential embedded generation","GWh",182.74127000000001,197.80126000000001,212.67482999999999,226.85238999999999,239.96452999999997,252.49457000000001,265.38049000000001]
[null,"3.4.1.4 - Energy grouping  - customer type or class"]
["DOPED0501","Residential customers energy deliveries","GWh",4580.2700000000004,4554.46,4534.96,4518.55,4507.33,4502.8099999999995,4496.07]
["DOPED0502","Non residential customers not on demand tariffs energy deliveries","GWh",1897.4049999999997,1878.5169999999998,1865.0150000000001,1844.3530000000001,1820.9970000000001,1812.779,1804.9159999999999]
["DOPED0503","Non-residential low voltage demand tariff customers energy deliveries","GWh",2402.9499999999998,2411.34,2424.9300000000003,2428.85,2428.3599999999997,2445.79,2463.06]
["DOPED0504","Non-residential high voltage demand tariff customers energy deliveries","GWh",3425.799,3442.8630000000003,3463.674,3480.5119999999997,3491.9939999999997,3518.268,3543.04]
["DOPED0505","Other Customer Class Energy Deliveries","GWh",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.4.3 - SYSTEM DEMAND"]
[null,null,null,"Standard control services"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"3.4.3.1 - Annual system maximum demand characteristics at the zone substation level – MW measure"]
["DOPSD0102","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2709.9068600767578,2732.4529070081576,2752.4184319292344,2770.5103763417656,2787.3043499591436,2803.1310398768705,2818.4931153966845]
["DOPSD0103","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2445.4037490950768,2459.3184383474236,2471.1568228873903,2481.5215026031651,2490.7822817530268,2499.1815444609729,2506.8873007907564]
["DOPSD0105","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2132.8457043978983,2149.3311627741323,2164.0639548608915,2177.4801338749971,2189.982582360276,2201.8024653525067,2213.3782381020478]
["DOPSD0106","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",1923.3189538602355,1933.4847511345351,1942.2146442963212,1949.9105174610613,1956.8231601573368,1963.1196187627829,1968.9172691631588]
[null,"3.4.3.2 - Annual system maximum demand characteristics at the transmission connection point  – MW measure"]
["DOPSD0108","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2918.2097221674021,2923.6846015814458,2948.7959779029152,2975.7061229945202,3004.4713350097159,3035.1616753875751,3067.8603943159401]
["DOPSD0109","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2629.798291996533,2661.5223514855629,2684.0604343742511,2708.2753509567997,2734.1910455230222,2761.8472322505945,2791.3056208314406]
["DOPSD0111","Coincident Weather Adjusted System Annual Maximum Demand 10% POE","MW ",2466.007553771793,2474.540147192919,2478.7410848907361,2486.7310559897205,2488.7553873062011,2499.0131271985852,2502.9111036046497]
["DOPSD0112","Coincident Weather Adjusted System Annual Maximum Demand 50% POE","MW ",2300.7851553344949,2302.0015741467187,2309.5082114349207,2309.0724788118901,2314.3192343276364,2311.6168530204386,2331.8399050079088]
[null,"3.4.3.3 - Annual system maximum demand characteristics at the zone substation level – MVA measure"]
["DOPSD0202","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2786.4686534505281,2809.6293035842914,2830.1663655103225,2848.7891475128563,2866.0838890076816,2882.3909722592357,2898.2147510716568]
["DOPSD0203","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2514.5874571560412,2528.8969565675047,2541.0980652639005,2551.7976465609486,2561.3694489016134,2570.0591729226899,2578.0375253588991]
["DOPSD0205","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2191.5681747574008,2208.4981541589655,2223.6428647441167,2237.4407792409843,2250.3032586230579,2262.468951257189,2274.3784205118845]
["DOPSD0206","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",1976.3222498428131,1986.7714512648549,1995.7607278192856,2003.6959504721876,2010.8309921616374,2017.3353019713197,2023.328147972336]
[null,"3.4.3.4 - Annual system maximum demand characteristics at the transmission connection point – MVA measure"]
["DOPSD0208","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2965.2660231786317,2970.8291853407418,2996.3454840617269,3023.6895568035852,3052.9186095307614,3084.103833427097,3117.3298210945404]
["DOPSD0209","Non–coincident Summated Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2672.347967507535,2704.585316719681,2727.4880618398688,2752.0947715292309,2778.4297774919933,2806.5334364742666,2836.4684566199771]
["DOPSD0211","Coincident Weather Adjusted System Annual Maximum Demand 10% POE"," MVA",2517.2152638850057,2525.9250402874873,2530.2132122679022,2538.3690985617623,2540.4354659908531,2550.9062122748933,2554.8851318417055]
["DOPSD0212","Coincident Weather Adjusted System Annual Maximum Demand 50% POE"," MVA",2341.089969188678,2348.6890165153418,2349.9307619678143,2357.5936923848012,2357.1488875217842,2362.5048839404867,2359.7462372759182]
[null,"3.4.3.5 - Power factor conversion between MVA and MW"]
["DOPSD0301","Average overall network power factor conversion between MVA and MW","Factor",0.97093609743454978,0.97093609743454978,0.97093609743454978,0.97093609743454978,0.97093609743454978,0.97093609743454978,0.97093609743454978]
["DOPSD0302","Average power factor conversion for  low voltage distribution lines","Factor",0.85,0.85,0.85,0.85,0.85,0.85,0.85]
["DOPSD0303","Average power factor conversion for 3.3 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0304","Average power factor conversion for 6.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0305","Average power factor conversion for 7.6 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0306","Average power factor conversion for 11 kV lines","Factor",0.92,0.92,0.92,0.92,0.92,0.92,0.92]
["DOPSD0307","Average power factor conversion for  SWER lines","Factor",1,1,1,1,1,1,1]
["DOPSD0308","Average power factor conversion for 22 kV lines","Factor",0.94,0.94,0.94,0.94,0.94,0.94,0.94]
["DOPSD0309","Average power factor conversion for 33 kV lines","Factor",0.96,0.96,0.96,0.96,0.96,0.96,0.96]
["DOPSD0310","Average power factor conversion for 44 kV lines","Factor",0,0,0,0,0,0,0]
["DOPSD0311","Average power factor conversion for 66 kV lines","Factor",0.98,0.98,0.98,0.98,0.98,0.98,0.98]
["DOPSD0312","Average power factor conversion for 110 kV lines","Factor",1,1,1,1,1,1,1]
["DOPSD0313","Average power factor conversion for 132 kV lines","Factor",0.98,0.98,0.98,0.98,0.98,0.98,0.98]
["DOPSD0314","Average power factor conversion for 220 kV lines","Factor",0,0,0,0,0,0,0]
[null,"3.4.3.6 - Demand supplied (for customers charged on this basis) – MW measure"]
["DOPSD0401","Summated Chargeable Contracted Maximum Demand","MW ",0,0,0,0,0,0,0]
["DOPSD0402","Summated Chargeable Measured Maximum Demand ","MW ",469.84699999999998,469.84699999999998,469.84699999999998,469.84699999999998,469.84699999999998,469.84699999999998,469.84699999999998]
[null,"3.4.3.7 - Demand supplied (for customers charged on this basis) – MVA measure"]
["DOPSD0403","Summated Chargeable Contracted Maximum Demand"," MVA",915.2,902.9,892.7,880.7,867.7,860,852.6]
["DOPSD0404","Summated Chargeable Measured Maximum Demand "," MVA",31746.6,31818.5,31923,31978.9,32004.6,32136.2,32264.199999999997]

{"sheet":"3.5 Physical assets","index":21,"n_rows":97,"n_cols":10,"rows_kept":97,"cut":false,"hidden":false,"merged":[[10,3,10,9],[77,3,77,9],[93,3,93,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.5 PHYSICAL ASSETS DATA"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[]
[]
[null,"3.5.1 - NETWORK CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Circuit length"]
[null,"3.5.1.1 - Overhead network length of circuit at each voltage"]
["DPA0101","Overhead low voltage distribution","km",25576.223820377378,25496.468584452854,25416.71334852833,25336.958112603807,25257.202876679283,25177.447640754759,25097.692404830235]
["DPA0102","Overhead 2.2 kV","km",0,0,0,0,0,0,0]
["DPA0103","Overhead 7.6 kV","km",18.7393257384375,18.687190886125002,18.635056033812504,18.582921181500005,18.530786329187507,18.478651476875008,18.42651662456251]
["DPA0104","Overhead 11 kV","km",0,0,0,0,0,0,0]
["DPA0105","Overhead SWER","km",70499.700238764053,70533.443651685404,70567.187064606755,70600.930477528105,70634.673890449456,70668.417303370807,70702.160716292157]
["DPA0106","Overhead 22 kV","km",29614.668916669987,29592.202700003985,29569.736483337983,29547.270266671982,29524.80405000598,29502.337833339978,29479.871616673976]
["DPA0107","Overhead 33 kV","km",42483.964203967247,42526.957044760697,42569.949885554146,42612.942726347595,42655.935567141045,42698.928407934494,42741.921248727944]
["DPA0108","Overhead 44 kV","km",5417.4912122028136,5440.564015253517,5463.6368183042205,5486.7096213549239,5509.7824244056274,5532.8552274563308,5555.9280305070342]
["DPA0109","Overhead 66 kV","km",0,0,0,0,0,0,0]
["DPA0110","Overhead 132 kV","km",7618.02683692963,7618.02683692963,7618.02683692963,7619.02683692963,7620.02683692963,7621.02683692963,7621.02683692963]
["DPA0111","Overhead 6.6kv","km",21.017628800000001,21.017628800000001,21.017628800000001,21.017628800000001,21.017628800000001,21.017628800000001,21.017628800000001]
["DPA0112","Overhead 110kV","km",2187.1051617641701,2187.1051617641701,2187.1051617641701,2187.1051617641701,2187.1051617641701,2187.1051617641701,2187.1051617641701]
["DPA0113","Overhead 220kV","km",2.9724200500000002,2.9724200500000002,2.9724200500000002,2.9724200500000002,2.9724200500000002,2.9724200500000002,2.9724200500000002]
["DPA0114","Other ","km",0,0,0,0,0,0,0]
["DPA01","Total overhead circuit km",null,{"$f":"SUM(D15:D28)","v":183439.90976526373},{"$f":"SUM(E15:E28)","v":183437.44523458637},183434.98070390907,183433.51617323176,183432.0516425544,183430.58711187707,183428.12258119971]
[null,"3.5.1.2 - Underground network circuit length at each voltage"]
["DPA0201","Underground low voltage distribution","km",6276.1983928936997,6478.2380714724395,6680.2777500511793,6882.317428629919,7084.3571072086588,7286.3967857873986,7488.4364643661384]
["DPA0202","Underground 5 kV","km",0,0,0,0,0,0,0]
["DPA0203","Underground 6.6 Kv","km",1.4790265125E-2,1.7748318150000001E-2,2.0706371175000002E-2,2.3664424200000003E-2,2.6622477225000003E-2,2.9580530250000004E-2,3.2538583275000005E-2]
["DPA0204","Underground 7.6 kV","km",0,0,0,0,0,0,0]
["DPA0205","Underground 11 kV","km",2239.8019517408247,2300.5623420889897,2361.3227324371546,2422.0831227853196,2482.8435131334845,2543.6039034816495,2604.3642938298144]
["DPA0206","Underground SWER","km",40.199767596687508,40.439721116025012,40.679674635362517,40.919628154700021,41.159581674037526,41.39953519337503,41.639488712712534]
["DPA0207","Underground 22 kV","km",343.55045293584874,354.2605435230185,364.97063411018826,375.68072469735802,386.39081528452778,397.10090587169753,407.81099645886729]
["DPA0208","Underground 33 kV","km",48,48,48,48,48,48,48]
["DPA0209","Underground 66 kV","km",33.855774431939999,33.855774431939999,33.855774431939999,33.855774431939999,34.855774431939999,34.855774431939999,34.855774431939999]
["DPA0210","Underground 110 kV","km",0,0,0,0,0,0,0]
["DPA0211","Underground 132 kV","km",9.8715340699399992,9.8715340699399992,9.8715340699399992,9.8715340699399992,9.8715340699399992,9.8715340699399992,9.8715340699399992]
["DPA0212","Other ","km",0,0,0,0,0,0,0]
["DPA02","Total underground circuit km",null,{"$f":"SUM(D31:D42)","v":8991.4926639340665},{"$f":"SUM(E31:E42)","v":9265.2457350205023},9538.9988061069416,9812.7518771933774,10087.504948279813,10361.258019366252,10635.011090452686]
[]
[null,"Circuit Capacity MVA"]
[null,"3.5.1.3 - Estimated overhead network weighted average MVA capacity by voltage class"]
["DPA0301","Overhead low voltage distribution","MVA",8.8703662000000003E-2,8.8703662000000003E-2,8.8703662000000003E-2,8.8703662000000003E-2,8.8703662000000003E-2,8.8703662000000003E-2,8.8703662000000003E-2]
["DPA0302","Overhead 6.6 kV","MVA",0.72508863400000001,0.72508863400000001,0.72508863400000001,0.72508863400000001,0.72508863400000001,0.72508863400000001,0.72508863400000001]
["DPA0303","Overhead 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0304","Overhead 11 kV","MVA",2.0971776680000001,2.0971776680000001,2.0971776680000001,2.0971776680000001,2.0971776680000001,2.0971776680000001,2.0971776680000001]
["DPA0305","Overhead SWER","MVA",0.30277088699999999,0.30277088699999999,0.30277088699999999,0.30277088699999999,0.30277088699999999,0.30277088699999999,0.30277088699999999]
["DPA0306","Overhead 22 kV","MVA",2.5435528019999998,2.5435528019999998,2.5435528019999998,2.5435528019999998,2.5435528019999998,2.5435528019999998,2.5435528019999998]
["DPA0307","Overhead 33 kV","MVA",7.2916979810000004,7.2916979810000004,7.2916979810000004,7.2916979810000004,7.2916979810000004,7.2916979810000004,7.2916979810000004]
["DPA0308","Overhead 44 kV","MVA",0,0,0,0,0,0,0]
["DPA0309","Overhead 66 kV","MVA",24.894248730000001,24.894248730000001,24.894248730000001,24.894248730000001,24.894248730000001,24.894248730000001,24.894248730000001]
["DPA0310","Overhead 110 kV","MVA",106,106,106,106,106,106,106]
["DPA0311","Overhead 132 kV","MVA",126.99828479999999,126.99828479999999,126.99828479999999,126.99828479999999,126.99828479999999,126.99828479999999,126.99828479999999]
["DPA0312","Overhead 220 kV","MVA",213,213,213,213,213,213,213]
["DPA0313","Other ","MVA",0,0,0,0,0,0,0]
[null,"3.5.1.4 - Estimated underground network weighted average MVA capacity by voltage class"]
["DPA0401","Underground low voltage distribution","MVA",0.180956442,0.180956442,0.180956442,0.180956442,0.180956442,0.180956442,0.180956442]
["DPA0402","Underground 5 kV","MVA",0,0,0,0,0,0,0]
["DPA0403","Underground 6.6 kV","MVA",1.20912,1.20912,1.20912,1.20912,1.20912,1.20912,1.20912]
["DPA0404","Underground 7.6 kV","MVA",0,0,0,0,0,0,0]
["DPA0405","Underground 11 kV","MVA",5.4046325570000002,5.4046325570000002,5.4046325570000002,5.4046325570000002,5.4046325570000002,5.4046325570000002,5.4046325570000002]
["DPA0406","Underground SWER","MVA",0.91514572400000005,0.91514572400000005,0.91514572400000005,0.91514572400000005,0.91514572400000005,0.91514572400000005,0.91514572400000005]
["DPA0407","Underground 12.7 kV","MVA",0,0,0,0,0,0,0]
["DPA0408","Underground 22 kV","MVA",7.8635039869999996,7.8635039869999996,7.8635039869999996,7.8635039869999996,7.8635039869999996,7.8635039869999996,7.8635039869999996]
["DPA0409","Underground 33 kV","MVA",20.593610959999999,20.593610959999999,20.593610959999999,20.593610959999999,20.593610959999999,20.593610959999999,20.593610959999999]
["DPA0410","Underground 66 kV","MVA",77.339261980000003,77.339261980000003,77.339261980000003,77.339261980000003,77.339261980000003,77.339261980000003,77.339261980000003]
["DPA0411","Underground 110 kV","MVA",0,0,0,0,0,0,0]
["DPA0412","Underground 132 kV","MVA",185.14765689999999,185.14765689999999,185.14765689999999,185.14765689999999,185.14765689999999,185.14765689999999,185.14765689999999]
["DPA0413","Other","MVA",0,0,0,0,0,0,0]
[]
[]
[]
[null,"3.5.2 - TRANSFORMER CAPACITIES VARIABLES"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Distribution transformer total installed capacity"]
["DPA0501","Distribution transformer capacity owned by utility","MVA",10139.012999999999,10298.197,10457.381000000001,10616.565000000002,10775.749000000003,10934.933000000005,11094.117000000006]
["DPA0502","Distribution transformer capacity owned by High Voltage Customers","MVA",776.22602999999981,776.22602999999981,776.22602999999981,776.22602999999981,776.22602999999981,776.22602999999981,776.22602999999981]
["DPA0503","Cold spare capacity included in DPA0501","MVA",135.1825,135.464,135.74549999999999,136.02699999999999,136.30849999999998,136.58999999999997,136.87149999999997]
[null,"Zone substation transformer capacity"]
["DPA0601","Total installed capacity for first step transformation where there are two steps to reach distribution voltage","MVA",2152.5,2152.5,2152.5,2155.5,2171.5,2187.5,2187.5]
["DPA0602","Total installed capacity for second step transformation where there are two steps to reach distribution voltage","MVA",2178.6,2182.1,2188.1,2188.1,2188.1,2198.1,2198.1]
["DPA0603","Total zone substation transformer capacity where there is only a single step transformation to reach distribution voltage","MVA",6552.75,6559.95,6592.95,6604.45,6616.45,6618.45,6631.45]
["DPA0604","Total zone substation transformer  capacity ","MVA",11381.45,11392.150000000001,11431.150000000001,11445.650000000001,11474.650000000001,11502.650000000001,11515.650000000001]
["DPA0605","Cold spare capacity of zone substation transformers included in DPA0604","MVA",4413.8500000000004,4418.3500000000004,4425.6000000000004,4432.1000000000004,4438.1000000000004,4444.6000000000004,4444.6000000000004]
[]
[]
[]
[null,"3.5.3 - PUBLIC LIGHTING"]
[null,null,null,"VOLUMES"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DPA0701","Public lighting luminaires","0's",162016,164754,167538,170369,173248,176176,179153]
["DPA0702","Public lighting poles","0's",66514,67645,68795,69965,71154,72364,73594]

{"sheet":"3.6 Quality of service","index":22,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[[7,3,7,9],[14,3,14,9],[19,3,19,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.6 QUALITY OF SERVICE DATA"]
[]
[]
[null,"3.6.2 - ENERGY NOT SUPPLIED"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DQS0201","Energy Not Supplied (planned)","GWh",4.6882165144596648,4.7006750380517497,4.7131335616438355,4.7255920852359203,4.7380506088280061,4.750509132420091,4.7629676560121759]
["DQS0202","Energy Not Supplied (unplanned)","GWh",7.7355572488584476,7.7561138127853875,7.7766703767123282,7.7972269406392689,7.8177835045662096,7.8383400684931503,7.8588966324200911]
["DQS02","Total",null,{"$f":"SUM(D10:D11)","v":12.423773763318113},{"$f":"SUM(E10:E11)","v":12.456788850837137},12.489803938356165,12.52281902587519,12.555834113394216,12.588849200913241,12.621864288432267]
[]
[null,"3.6.3 - SYSTEM LOSSES"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DQS03","System losses","%",{"$f":"(SUM('3.4 Operational data'!D22:D34)-SUM('3.4 Operational data'!D15:D20))/SUM('3.4 Operational data'!D22:D34)","v":5.9974658289153458E-2},{"$f":"(SUM('3.4 Operational data'!E22:E34)-SUM('3.4 Operational data'!E15:E20))/SUM('3.4 Operational data'!E22:E34)","v":5.9974735274168196E-2},{"$f":"(SUM('3.4 Operational data'!F22:F34)-SUM('3.4 Operational data'!F15:F20))/SUM('3.4 Operational data'!F22:F34)","v":5.9974199757240491E-2},{"$f":"(SUM('3.4 Operational data'!G22:G34)-SUM('3.4 Operational data'!G15:G20))/SUM('3.4 Operational data'!G22:G34)","v":5.997465914062905E-2},{"$f":"(SUM('3.4 Operational data'!H22:H34)-SUM('3.4 Operational data'!H15:H20))/SUM('3.4 Operational data'!H22:H34)","v":5.9974736476528331E-2},{"$f":"(SUM('3.4 Operational data'!I22:I34)-SUM('3.4 Operational data'!I15:I20))/SUM('3.4 Operational data'!I22:I34)","v":5.9974276196922804E-2},{"$f":"(SUM('3.4 Operational data'!J22:J34)-SUM('3.4 Operational data'!J15:J20))/SUM('3.4 Operational data'!J22:J34)","v":5.9974429129495931E-2}]
[]
[null,"3.6.4 - CAPACITY UTILISATION"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DQS04","Overall utilisation","%",0.28799526501125727,0.28927962623955539,0.28938430657653708,0.29022270519484661,0.2909142941889834,0.29150395255771133,0.29197835963994762]

{"sheet":"3.7 Operating Environment","index":23,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[8,3,8,9],[15,3,15,9],[33,3,33,9]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"3.7 OPERATING ENVIRONMENT FACTORS"]
[]
[null,"There are THREE tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
["DOEF01","3.7.1 - DENSITY FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOEF0101","Customer density","Customer / km",4.9360853104616549]
["DOEF0102","Energy density","MWh/customer",13.724515655220431]
["DOEF0103","Demand density","kVA / customer",2.8043534195344715]
[]
["DOEF02","3.7.2 - TERRAIN FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOEF0201","Rural proportion","%",0.91]
["DOEF0202","Urban and CBD vegetation maintenance spans","0's",152685]
["DOEF0203","Rural vegetation maintenance spans","0's",271690]
["DOEF0204","Total vegetation maintenance spans","0's",424375]
["DOEF0205","Total number of spans","0's",1294305]
["DOEF0206","Average urban and CBD vegetation maintenance span cycle","Years",1.75]
["DOEF0207","Average rural vegetation maintenance span cycle","Years",2.82]
["DOEF0208","Average number of trees per urban and CBD vegetation maintenance span","Trees",2.7]
["DOEF0209","Average number of trees per rural vegetation maintenance span","Trees",3.2]
["DOEF0210","Average number of defects per urban and CBD vegetation maintenance span","Defects",1.18]
["DOEF0211","Average number of defects per rural vegetation maintenance span","Defects",1.32]
["DOEF0212","Tropical proportion","Spans",191380]
["DOEF0213","Standard vehicle access","km",111230,111230,111230,111230,111230,111230,{"$f":"I30","v":111230}]
["DOEF0214","Bushfire risk","Spans",980203]
[]
["DOEF03 ","3.7.3 - SERVICE AREA FACTORS"]
[null,null,null,"Forecast"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
["DOEF0301","Route Line length","km",181656.66763393665,181654.22706126791,181651.78648859923,181650.33619480641,181648.88590101353,181647.43560722069,{"$f":"I36","v":181647.43560722069}]

{"sheet":"4.1 Public lighting","index":24,"n_rows":180,"n_cols":10,"rows_kept":180,"cut":false,"hidden":false,"merged":[[182,1,182,2],[183,1,183,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[167,1,167,2],[168,1,168,2],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[156,1,156,2],[151,1,151,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[90,1,90,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[91,1,91,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[210,1,210,2],[191,1,191,2],[192,1,192,2],[193,1,193,2],[194,1,194,2],[195,1,195,2],[196,1,196,2],[197,1,197,2],[198,1,198,2],[199,1,199,2],[200,1,200,2],[201,1,201,2],[202,1,202,2],[203,1,203,2],[204,1,204,2],[205,1,205,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[189,1,189,2],[190,1,190,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[5,1,5,2],[8,3,8,9],[31,3,31,9],[184,1,184,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[57,1,57,2],[58,1,58,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"4.1 PUBLIC LIGHTING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been grouped (and sub-grouped) for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"4.1.2 - DESCRIPTOR METRICS ANNUALLY"]
[null,null,null,"VOLUMES & EXPENDITURE"]
[null,null,"Units",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"LIGHT INSTALLATION "]
[null,"Number of lights installed","0's",2688,2733,2779,2826,2874,2923,2972]
[null,"Number of poles installed ","0's",1112,1131,1150,1170,1189,1210,1230]
[null,"Total expenditure","$0's",0,0,0,0,0,0,0]
[null,"LIGHT REPLACEMENT"]
[null,"Number of lights replaced","0's",2900,2632,2343,1991,1692,1692,1692]
[null,"Number of poles replaced","0's",612,925,823,1130,916,452,890]
[null,"Total expenditure","$0's",2925276,2714907,3097936,2543511,1491741,2412271,2228603]
[null,"LIGHT MAINTENANCE"]
[null,"Number of lights maintained","0's",77080,96380,55660,59800,75000,67260,85840]
[null,"Number of poles maintained","0's",5300,11305,13170,18980,14900,5560,14640]
[null,"Total expenditure","$0's",8670000,10020000,6760000,7360000,8270000,7080000,8940000]
[null,"QUALITY OF SUPPLY"]
[null,"Mean days to rectify/replace public lighting assets ","days",7,7,7,7,7,7,7]
[null,"GSO breaches","0's",50,36,29,28,28,27,27]
[null,"GSL payments ","$0's",750,540,435,420,420,405,405]
[null,"Customer complaints ","0's",76,55,44,43,43,41,41]
[]
[]
[]
[null,"4.1.3 - COST METRICS"]
[null,null,null,{"$f":"CONCATENATE(\"AVERAGE UNIT COST \n($0's, real \",dms_DollarReal, \")\")","v":"AVERAGE UNIT COST \n($0's, real June 2019)"}]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"LIGHT INSTALLATION"]
[null,"Essential Energy does not install lights, these are installed by ASP only"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT REPLACEMENT"]
[]
[null,"High Pressure Sodium 400",null,509.75,511.7,0,0,0,0,0]
[null,"High Pressure Sodium 250",null,400.83,404.35,0,0,0,0,0]
[null,"High Pressure Sodium 150",null,490.37,492.13,0,0,0,0,0]
[null,"High Pressure Sodium 70",null,323.87,323.89,0,0,0,0,0]
[null,"Metal Halide 400",null,503.88,772.35,0,0,0,0,0]
[null,"Metal Halide 250",null,537.36,749.11,0,0,0,0,0]
[null,"Compact Flourescent 42",null,324.87,326.89999999999998,0,0,0,0,0]
[null,"LED 300W",null,0,0,1153,940.65,846.63,804.27,764.08500000000004]
[null,"LED 200W",null,0,0,1007.6,885.49,796.95,717.3,681.43499999999995]
[null,"LED 100W",null,0,0,1007.6,830.34,747.27,709.94,674.40499999999997]
[null,"LED 42W",null,410.83,405.5,390.23,390.2,390.2,390.2,390.2]
[null,"LED 35W",null,0,465,462.85,462.85,462.85,462.85,462.85]
[null,"LED 25W",null,392.83,355.56,355.6,355.6,355.6,355.6,355.6]
[null,"LED 17W",null,383.83,382.33,380.46,380.5,380.5,380.5,380.5]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LIGHT MAINTENANCE"]
[null,"High Pressure Sodium 1000",null,169.97,166.51,178.87,175.7,170.36,168.52,164.56]
[null,"High Pressure Sodium 400",null,136.32,130.33000000000001,158.12,153.22999999999999,135.30000000000001,135.26,121.96]
[null,"High Pressure Sodium 360",null,226.88,227.37,230.12,230.12,226.35,227.48,222.83]
[null,"High Pressure Sodium 250",null,113.29,106.8,138,132.13999999999999,112.22,112.18,98.7]
[null,"High Pressure Sodium 220",null,214.75,209.42,242.08,235.83,214.57,214.96,198.95]
[null,"High Pressure Sodium 150",null,245.72,111.14,140.21,134.38,115.83,115.79,104.3]
[null,"High Pressure Sodium 70",null,142.59,136.9,158.02000000000001,155.05000000000001,141.72,141.68,128.19999999999999]
[null,"Metal Halide 400",null,153.55000000000001,147.93,170.99,167.34,152.36000000000001,152.28,121.96]
[null,"Metal Halide 250",null,158.13,153.19,177.99,172.64,156.69999999999999,156.54,144.02000000000001]
[null,"Metal Halide 150",null,140.36000000000001,133.18,152.24,146.52000000000001,140.36000000000001,139.05000000000001,128.05000000000001]
[null,"Metal Halide 70",null,139.05000000000001,133.96,152.85,148.5,137.99,137.13,126.66]
[null,"Compact Flourescent 42",null,112.28,105.92,136.62,130.79,111.25,111.21,98.25]
[null,"Compact Flourescent 32",null,112.28,158.83000000000001,158.83000000000001,158.83000000000001,158.83000000000001,158.83000000000001,158.83000000000001]
[null,"Fluorescent 20, 26, 40, 80, 9",null,142.12,138.81,153.37,152.91,0,0,0]
[null,"Mercury Vapour 400",null,139.13,147.93,156.58000000000001,153.22999999999999,0,0,0]
[null,"Mercury Vapour 250",null,158.13,153.19,177.99,172.64,0,0,0]
[null,"Mercury Vapour 80",null,122.49,107.75,138.75,133.37,0,0,0]
[null,"Mercury Vapour 50",null,122.49,110.9,140.26,135.65,0,0,0]
[null,"Low Pressure Sodium 135",null,305.83,237.07,267.35000000000002,305.83,0,0,0]
[null,"Low Pressure Sodium 100",null,218.56,218.45,220.13,219.3,0,0,0]
[null,"Low Pressure Sodium 55",null,212.04,214.28,212.67,212.67,0,0,0]
[null,"Incandescent 60",null,160.72999999999999,160,160,160,0,0,0]
[null,"LED 300W",null,0,0,390,394.29,406.5,420,420]
[null,"LED 200W",null,0,0,390,394.29,406.5,420,420]
[null,"LED 100W",null,0,0,390,394.29,406.5,420,420]
[null,"LED 42W",null,158.16999999999999,0,160,161.80000000000001,166.8,172.37,172.4]
[null,"LED 35W",null,0,0,160,161.80000000000001,166.8,172.34,172.3]
[null,"LED25W",null,160.08000000000001,0,160,161.80000000000001,166.8,172.34,172.3]
[null,"LED17W",null,161.97999999999999,172.5,160,161.80000000000001,166.8,172.34,172.3]

{"sheet":"4.2 Metering","index":25,"n_rows":92,"n_cols":11,"rows_kept":92,"cut":false,"hidden":false,"merged":[[81,1,83,1],[84,1,86,1],[87,1,89,1],[18,1,21,1],[28,1,30,1],[31,1,33,1],[34,1,36,1],[37,1,39,1],[40,1,42,1],[43,1,45,1],[46,1,48,1],[49,1,51,1],[54,1,56,1],[66,1,68,1],[69,1,71,1],[72,1,74,1],[75,1,77,1],[78,1,80,1],[5,1,5,2],[8,4,8,10],[26,4,26,10],[64,4,64,10],[10,1,13,1],[14,1,17,1],[65,2,65,3],[27,2,27,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"4.2 METERING"]
[]
[null,"There are TWO tables on this worksheet. Each table has been 'grouped' (and 'sub-grouped') for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.2.1 - METERING DESCRIPTOR METRIC"]
[null,null,null,null,"VOLUMES (0's)"]
[null,"ASSET CATEGORY","ASSET SUBCATEGORY",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Meter Type 4","Single phase meter population ",null,0,0,0,0,0,0,0]
[null,null,"Multi phase meter population ",null,0,0,0,0,0,0,0]
[null,null,"Current transformer connected meter population ",null,0,0,0,0,0,0,0]
[null,null,"Direct connect meter population ",null,0,0,0,0,0,0,0]
[null,"Meter Type 5","Single phase meter population ",null,111,95,80,68,58,50,43]
[null,null,"Multi phase meter population ",null,337,287,244,207,176,150,127]
[null,null,"Current transformer connected meter population ",null,224,191,162,138,117,100,85]
[null,null,"Direct connect meter population ",null,224,191,162,138,117,100,85]
[null,"Meter Type 6","Single phase meter population ",null,1228966,1186163,1138324,1090486,1042647,994808,952005]
[null,null,"Multi phase meter population ",null,137728,132931,127570,122208,116847,111486,106689]
[null,null,"Current transformer connected meter population ",null,6502,6276,6023,5770,5517,5264,5037]
[null,null,"Direct connect meter population ",null,1360192,1312818,1259871,1206924,1153977,1101030,1053657]
[]
[]
[null,"4.2.2 - COST METRICS"]
[null,"EXPENDITURE"]
[null,null,null,null,{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \",dms_DollarReal,\")\")","v":"EXPENDITURE \n($0's, real June 2019)"}]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Meter purchase ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6"]
[null,"Meter testing ",null,"Meter Type 4"]
[null,null,null,"Meter Type 5"]
[null,null,null,"Meter Type 6",894353.48635472369,743127.11114252498,1286288.7692356161,773112.98703455564,443268.35222221952,546385.49571835669,610855.12888622226]
[null,"Meter investigation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",136116.27583004409,118326.66853958672,100360.83928488508,85492.566798235435,72482.828372417003,61951.135361040171,52658.465056884146]
[null,null,null,"Meter Type 6",9326806.0254352763,9565573.4344809949,9564714.3399621285,9543757.4546084944,9502611.9022800103,9439249.0812424887,9403433.8653738406]
[null,"Special meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Remote meter re-configuration ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Other metering ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",1215323.8913396795,1239022.7072208035,1239022.7072208035,1239022.7072208035,1239022.7072208035,1239022.7072208035,1239022.7072208035]
[null,null,null,"Meter Type 7",0,0,0,0,0,0,0]
[null,"IT infrastructure capex ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"IT infrastructure opex ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Communications infrastructure capex ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Communications infrastructure opex ",null,"Meter Type 4",0,0,0,0,0,0,0]
[]
[null,"VOLUMES"]
[null,null,null,null,"VOLUMES  (0's)"]
[null,"SERVICE SUBCATEGORY","METER TYPE",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Meter purchase ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter testing ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",3518,2857,2635,2957,1857,2125,2340]
[null,"Meter investigation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Scheduled meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",11648,9932,8424,7176,6084,5200,4420]
[null,null,null,"Meter Type 6",8746842,8442202,8101722,7761242,7420762,7080282,6775642]
[null,"Special meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"New meter installation ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter replacement ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Meter maintenance ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 5",0,0,0,0,0,0,0]
[null,null,null,"Meter Type 6",0,0,0,0,0,0,0]
[null,"Remote meter reading ",null,"Meter Type 4",0,0,0,0,0,0,0]
[null,"Remote meter re-configuration ",null,"Meter Type 4",0,0,0,0,0,0,0]

{"sheet":"4.3 Fee-based services","index":26,"n_rows":109,"n_cols":16,"rows_kept":109,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"4.3 ANCILLARY SERVICES - FEE BASED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.3.1 - COST METRICS FOR FEE-BASED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"COMMON FEE-BASED SERVICES"]
[null,"Energisation",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"De-energisation",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Re-energisation",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"MISCELLANEOUS FEE-BASED SERVICES"]
[null,"Design Information",845119.89999999991,866247.89749999996,593694.7408050712,593694.7408050712,600225.38295392692,614109.79651241715,634849.8643223258,2250,2250,2500,2500,2500,2500,2500]
[null,"Design Certification",572389.69999999995,586699.44249999989,617601.63436608727,617601.63436608727,624395.25234411401,638838.76332133811,781874.51548077201,2200,2200,2175,2175,2175,2175,2175]
[null,"Design Re- Checking",145385.5,149020.13749999998,144564.836668203,144564.836668203,146155.0498715532,149535.90848518198,154586.12084071187,1500,1500,1400,1400,1400,1400,1400]
[null,"Design Re - Certification (NEW)",0,0,51630.298810072498,51630.298810072498,52198.232096983294,53405.681601850702,55209.32887168281,0,0,500,500,500,500,500]
[null,"Administration",90848.16,93119.364000000001,291647.56533508265,291647.56533508265,294855.6885537685,301676.29034139431,311864.67481898289,1350,1350,1270,1270,1270,1270,1270]
[null,"Non - Standard Design Approval (NEW)",0,0,55335.902463824517,55335.902463824517,55857.774671257859,56967.296428464579,58624.662537886252,0,0,400,400,400,400,400]
[null,"Connections Customer Interface co-ordination",7729.96,7923.2089999999989,31515.594589676326,31515.594589676326,31808.00193036981,32429.671951967619,33358.301623578169,25,25,25,25,25,25,25]
[null,"Preliminary Enquiry Service",967.69999999999993,991.89249999999981,3843.2582397654392,3843.2582397654392,3879.0223764277043,3955.0584005525689,4068.6384440813954,30,30,30,30,30,30,30]
[null,"Connection / relocation process facilitation",43293.5,44375.837500000001,41304.239048058,41304.239048058,41758.585677586634,42724.545281480561,44167.463097346248,2,2,2,2,2,2,2]
[null,"Connection Offer Service",1087300.72,1114483.2379999999,759582.31787319004,759582.31787319004,767937.72336979501,785701.65878678509,812236.82525724242,32000,32000,32000,32000,32000,32000,32000]
[null,"Planning, Protection and Power Quality Studies",28535.739999999998,29249.133499999996,13066.63950340263,13066.63950340263,13188.666858022876,13448.102028160458,13835.637518821379,50,50,100,100,100,100,100]
[null,"Additional Services Requested by ASP / Connection Applicant (NEW)",0,0,6149.6516954245653,6149.6516954245653,6206.4450241156446,6327.1899746023864,6507.5547015855973,0,0,50,50,50,50,50]
[null,"Data Gatherine Fee - Failure to Provide Documentation (NEW)",0,0,12299.303390849131,12299.303390849131,12412.890048231289,12654.379949204773,13015.109403171195,0,0,100,100,100,100,100]
[null,"Pioneer Scheme Administration (NEW)",0,0,20647.615244961598,20647.615244961598,20874.739012656177,21357.613475496939,22078.915031432418,0,0,1100,1100,1100,1100,1100]
[null,"Substation Commissioning",720042.84000000008,738043.91099999985,993151.35416261852,993151.35416261852,1032850.0299647433,1115202.0023078364,1211181.345809245,800,800,785,785,815,875,935]
[null,"Testing & Commissioning of Streetlights / Mains / Cables / UG Pillars (NEW)",0,0,77801.653431647195,73939.029028203397,74659.72935846707,76191.967874839364,78480.773995216208,0,0,350,350,350,350,350]
[null,"Redundant Materical Coordination (NEW)",0,0,1843.537075443,1843.537075443,1863.8159832728729,1906.9297745979409,1971.3316992350371,0,0,50,50,50,50,50]
[null,"Access Permits",2049102.43,2100329.9907499994,2486531.4955158341,2486531.4955158341,2509913.3731096559,2559624.2056567273,2811132.1848328863,1400,1400,1230,1230,1230,1230,1330]
[null,"Access to Network Assets (Standby)",3819.1400000000003,3914.6184999999996,3689.7910172547395,3689.7910172547395,3723.867014469387,3796.3139847614316,3904.5328209513586,30,30,30,30,30,30,30]
[null,"Sale of Approved Materials /  Equipment to ASPs (NEW)",0,0,5515500,5515500,5515500,5515500,5515500,0,0,10000,10000,10000,10000,10000]
[null,"Services to supply and connect  temporary supply to one or more customers",4655.16,4771.5389999999998,5102.0937172624472,5102.0937172624472,5148.5577205891877,5247.3421009099766,5394.9028702418682,0,0,3,3,3,3,3]
[null,"Rectification of ASP Defects (NEW)",0,0,13123.877210771852,13123.877210771852,13205.28233854169,13378.352985191072,13636.88006898122,0,0,5,5,5,5,5]
[null,"Notice of Arrangement",148935.16,152658.53899999999,145282.30397679599,145282.30397679599,146880.40932054076,150278.04694894349,155353.32322976846,600,600,600,600,600,600,600]
[null,"Request for Early Notice of Arrangement (NEW)",0,0,61956.358572086996,61956.358572086996,62637.878516379948,64086.817922220842,66251.194646019372,0,0,600,600,600,600,600]
[null,"Completion Notice  - Other than Notice of Arrangement (NEW)",0,0,41304.239048058,41304.239048058,41758.585677586634,42724.545281480561,44167.463097346248,0,0,400,400,400,400,400]
[null,"Conveyancing Information",57810.22,59255.475499999993,92176.853772150003,92176.853772150003,93190.799163643649,95346.488729897043,98566.584961751854,2200,2200,2500,2500,2500,2500,2500]
[null,"Easement Processing - Conveyancing Review (NEW)",0,0,40300.428284466005,40300.428284466005,40743.732995595128,41686.217027249229,43094.067826558588,0,0,400,400,400,400,400]
[null,"Services Involved in Obtaining Deeds of Agreement (DOA)",100463.52,102975.10799999999,11101.538352958534,11101.538352958534,11206.197052641874,11428.705748689768,11761.081720126153,80,80,80,80,80,80,80]
[null,"Development Applications and Encroachment Processing (NEW)",0,0,20150.214142233002,20150.214142233002,20371.866497797564,20843.108513624615,21547.033913279294,0,0,400,400,400,400,400]
[null,"Crown Land Acquisition (NEW)",0,0,13833.975615956129,13833.975615956129,13964.443667814465,14241.824107116145,14656.165634471563,0,0,100,100,100,100,100]
[null,"Legal Review Services - customer funded works (NEW)",0,0,6916.9878079780647,6916.9878079780647,6982.2218339072324,7120.9120535580723,7328.0828172357815,0,0,50,50,50,50,50]
[null,"Site Establishment",70667.600000000006,72434.289999999994,553061.12263290002,553061.12263290002,559144.79498186184,572078.93237938231,591399.50977051118,10000,10000,10000,10000,10000,10000,10000]
[null,"Safe Approach Clearances - De energisation of Mains (NEW)",0,0,66402.632456446474,66402.632456446474,67024.533013881475,68346.719153447557,70321.75613116374,0,0,50,50,50,50,50]
[null,"Safe Approach Clearances - Disable Auto Reclose (NEW)",0,0,2212.696109849051,11063.480549245256,33503.442874059619,15945.484959940239,16409.366515781334,0,0,5,25,75,35,35]
[null,"Provision of Traffic Control by the DSNP (NEW)",0,0,15000,15000,15000,15000,15000,0,0,10,10,10,10,10]
[null,"Site Safety Supervision (NEW)",0,0,9957.0782758011337,9957.0782758011337,10044.900456917765,10231.614022664984,10510.520437999981,0,0,100,100,100,100,100]
[null,"Provision of construction work by DSNP (NEW)",0,0,29871.234827403401,29871.234827403401,30134.701370753293,30694.842067994952,31531.561313999944,0,0,300,300,300,300,300]
[null,"Vegetation Clearing of Private Trees Encroaching DNSP Assets (NEW)",0,0,8000,15000,15000,15000,15000,0,0,10,10,10,10,10]
[null,"Inspection of Private Trees Encroaching DSNP Assets (NEW)",0,0,13686.159608574017,16917.183708108354,8764.0831690834948,14331.948714672655,16552.860982307942,0,0,132.54,163.83000000000001,83.95,134.18,149.91]
[null,"Vegetation Clearing of Private Trees Encroaching Private Assets (NEW)",0,0,5000,5000,5000,5000,5000,0,0,5,5,5,5,5]
[null,"Rectification works by Essential Energy of Private Asset aerial mains defects (NEW)",0,0,0,43042.803773491149,43377.560587276996,44089.267328847498,45152.390810351368,0,0,5,5,5,5,5]
[null,"Rectification works by Essential Energy of DSNP's assets due to landowner encroachment issues (NEW)",0,0,46436.781026323879,46436.781026323879,46721.945824097915,47328.217901846299,48233.846645241567,0,0,3,3,3,3,3]
[null,"Retailer of Last Resort (ROLR)",0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Planned Interruption - Customer Requested (NEW)",0,0,26150.084485736188,26150.084485736188,26426.735415079282,27014.906658700893,27893.496987717066,0,0,5,5,5,5,5]
[null,"Attendance at customers' premises - Statutory Right",0,0,199.14156551602267,199.14156551602267,200.89800913835529,204.63228045329967,210.21040875999964,0,0,2,2,2,2,2]
[null,"Inspection of Construction Work (by Level 1 ASP's)",407642.38,417833.43949999992,859536.81746949151,859536.81746949151,867474.82102064358,884351.34275017562,908613.763698778,9200,9200,8880,8880,8880,8880,8880]
[null,"Inspection of service work (Level 2 ASP's)",1704498.86,1747111.3314999999,287487.63122792408,287487.63122792408,290213.71100509586,296009.46862845949,304666.97552365361,6609,6500,6500,6000,6000,6000,6000]
[null,"Re-inspection of work of a service provider (Level 1 & Level 2 ASP's work)",24672.240000000002,25289.046000000002,12299.303390849131,12299.303390849131,12412.890048231289,12654.379949204773,13015.109403171195,45,45,100,100,100,100,100]
[null,"Re-inspection Customer Installation",0,0,614.96516954245658,614.96516954245658,620.64450241156453,632.7189974602386,650.75547015855977,0,0,5,5,5,5,5]
[null,"Investigation, review & implementation of remedial actions associated with work performed by ASP's",20748.96,21267.683999999994,12907.574702518123,12907.574702518123,13049.558024245822,13351.420400462674,13802.332217920703,2,2,55,55,55,55,55]
[null,"Substation Inspection (NEW)",0,0,256132.99311443316,256132.99311443316,258498.4352544166,263527.4624421894,271039.65332104015,0,0,735,735,735,735,735]
[null,"Inspection Services of Privately Owned Electrical Infrastructure Assets (NEW)",0,0,38572.72028911885,38572.72028911885,38901.220900580738,39599.626698937493,40642.881680916529,0,0,3,3,3,3,3]
[null,"Inspection Customer Installation",0,0,46122.387715684243,46122.387715684243,46548.337680867335,47453.924809517899,48806.660261891979,0,0,1500,1500,1500,1500,1500]
[null,"Provision of Training to ASP's for Network  Access ",0,0,16233.993729373356,16233.993729373356,16386.520844495844,16710.799758724075,17195.19664319346,140,140,100,100,100,100,100]
[null,"Provision of Design Related Training for Design Complaince (Level 3 ASP's) (NEW)",0,0,4795.9132625205393,4795.9132625205393,4842.1566044331112,4940.4718495201969,5087.3318404923812,0,0,30,30,30,30,30]
[null,"Provision of Training - Entry into Electrical Stations",0,0,7230.468948652795,7230.468948652795,7300.8877215227585,7450.6009262156977,7674.2374524751422,0,0,35,35,35,35,35]
[null,"Night Watch Lighting (NEW)",0,0,2970.1166666666668,2970.1166666666668,3002.7879499999999,3072.2484408594,3176.0061749880097,0,0,200,200,200,200,200]
[null,"Provision of Luminaire Glare Shield (NEW)",0,0,11716.202620640906,11716.202620640906,11786.460365534213,11935.831218131987,12158.956350399985,0,0,40,40,40,40,40]
[null,"Off - Peak Conversion",2911610.0800000005,2564994.3820000002,74080.662371960439,74080.662371960439,74734.059399468169,76123.208328627472,78198.272058719856,1200,1200,1200,1200,1200,1200,1200]
[null,"Authorisation of ASPs",97755.92,100199.81799999998,176269.3130760382,176269.3130760382,178143.15848012303,182127.03080721863,188078.00467168237,1450,1450,1200,1200,1200,1200,1200]
[null,"ASP Authorisation Agreement (NEW)",0,0,2949.8000794296563,2949.8000794296563,2982.2478803033819,3051.2332382705599,3154.2812349398318,0,0,50,50,50,50,50]
[null,"Design and construction of asset relocations - customer funded (NEW)",0,0,0,48587.001716045874,0,0,50998.37921391362,0,0,0,2,0,0,2]
[null,"DSNP Provided cable jointing & termination services for contestable works (NEW)",0,0,10863.112221245767,10863.112221245767,10925.365990929989,11057.720063342638,11255.426104378654,0,0,4,4,4,4,4]
[null,"Design & Construction of Connections as POLR NEW)",0,0,32834.916991379388,32834.916991379388,33077.933866462619,33594.597728673893,34366.372747622292,0,0,1,1,1,1,1]
[null,"Part Design & Construction of Connections (NEW)",0,0,0,22239.957014001622,22404.318623685664,0,23275.739130654081,0,0,0,1,1,0,1]
[null,"Design & Construction of Extensions as POLR (NEW) ",0,0,32834.916991379388,32834.916991379388,33077.933866462619,33594.597728673893,34366.372747622292,0,0,1,1,1,1,1]
[null,"Design & Construction of Augmentations as POLR (NEW)",0,0,32834.916991379388,32834.916991379388,33077.933866462619,33594.597728673893,34366.372747622292,0,0,1,1,1,1,1]
[null,"Design & Construction of Shared Enhancement (NEW)",0,0,11651.102478392149,0,0,11820.088274833195,0,0,0,1,0,0,1,0]
[null,"Disconnect / Reconnect - Site Visit - ACS 30020",0,0,56072.27646915707,53829.385410390787,52244.648303908878,51315.044648135903,50926.162300080301,2400,2400,2500,2400,2304,2211.84,2123.3664000000003]
[null,"Disconnect / Reconnect - Vacant Premise (Site visit only) - ACS 30020",0,0,0,0,0,0,0,100,100,0,0,0,0,0]
[null,"Disconnect / Reconnect - Pole Top / Pillar ",1071730.28,1098523.537,26877.296834790963,26877.296834790963,27107.830060222121,27597.953170308567,28330.082510562941,150,150,150,150,150,150,150]
[null,"Disconnect / Reconnect -  Complete - 30030",719855.78,737852.17450000008,697756.8,669846.52799999993,650126.24621567992,638558.36788141541,633719.16177382984,24000,24000,24000,23040,22118.400000000001,21233.664000000001,20384.317439999999]
[null,"Disconnect / Reconnect - Technical Disconnection - 30030",0,0,116.2928,116.2928,117.57202079999999,120.29169678514558,124.35425687205739,2,2,4,4,4,4,4]
[null,"Disconnect / Reconnect - Vacant Premise - 30030",0,0,349512.79999999993,335532.28799999994,325654.21744127991,319859.76076716639,317435.75791052741,0,0,14000,13440,12902.4,12386.304,11890.851839999999]
[null,"Reconnect - Outside of Normal Business  Hours - ",589437.77999999991,604173.72449999989,183173.89622208968,175846.94037320607,170269.92735638539,166432.59010161873,164039.27417723479,2000,2000,2000,1920,1843.2,1769.472,1698.6931199999999]
[null,"Illegal Connections",16111.36,16514.144,5534.686525882109,5313.2990648468249,5147.8737608024803,5038.1034744328344,4974.4522798231983,50,50,45,43.2,41.472000000000001,39.813119999999998,38.220595199999998]
[null,"Move In / Move Out Read",2046327.82,2097486.0154999997,1425715.2,1368686.5919999999,1328392.4587315198,1304755.9997634212,1294868.1280816011,150000,150000,144000,138240,132710.39999999999,127401.984,122305.90463999999]
[null,"Special Meter Read (incl wasted visit)",824980.18,845604.68449999997,425734.40000000002,408705.02400000003,396672.74809343996,389614.63881824387,386662.0104688115,45000,45000,43000,41280,39628.800000000003,38043.648000000001,36521.90208]
[null,"Special Meter Test - 1st & additional",266993.56,273668.39899999998,39210.179210027025,37641.77204162594,36469.825665418452,35692.164169981945,35241.230817947449,102,102,98,94.08,90.316800000000001,86.704127999999997,83.235962879999988]
[null,"Special Meter Tests - CT Meter (NEW)",0,0,5042.7143902481439,4841.005814638218,4690.2849820644815,4590.27205448325,4532.2787438389141,0,0,10,9.6,9.2159999999999993,8.8473600000000001,8.4934656000000004]
[null,"Unplanned Outage - Meter Fault (Site attendance)  (NEW)",0,0,16401.583571304709,17057.646914156896,17905.394039222123,18987.414088928675,20720.727132597691,0,0,55,57.2,59.488,61.867519999999999,65.917030400000002]
[null,"Unplanned Outage - Meter HW Fault (Site attendance) (NEW)",0,0,4836.9082309286641,4643.4319016915179,4989.2253197717546,4882.4868398083672,5368.9046552754207,0,0,18,17.28,17.823999999999998,17.111039999999999,17.740198399999997]
[null,"Unplanned Outage - Retailer outage impacting non retailer customer (Site attendance) (NEW)",0,0,10321.106334342776,10733.950587716487,11264.130661807698,11937.621783584556,12761.44579130001,0,0,52,54.08,56.243200000000002,58.492927999999999,60.832645120000002]
[null,"Unplanned Outage - Remote De-Energisation - EE not notified (Site attendance) (NEW)",0,0,13012.360254324318,13532.854664497292,14205.742613674593,15064.892793019892,16442.211376027688,0,0,7,6.72,6.4512,6.1931519999999995,5.9454259199999999]
[null,"Redundant Meter Disposal (NEW)",0,0,553.06112263290004,645.23797640504995,745.52639330914917,858.11839856907341,985.66584961751857,0,0,30,35,40,45,50]
[null,"Retailer Requested Distributer Planned Interruption - Cancellation after notifcation (NEW)",0,0,13690.488112124327,14580.369839412406,15671.206396238356,11267.936776964261,9270.8053034990608,0,0,45,47.924999999999997,51.040124999999996,36,28.8]
[null,"Retailer Requested Distributer Planned Interruption - Initial Visit (NEW)",0,0,33019.995225270715,31699.195416259892,30711.910415867147,30056.307472073284,29675.564647698415,0,0,115,110.4,105.98399999999999,101.74463999999999,101.74463999999999]
[null,"Retailer Requested Distributer Planned Interruption -  Isolation Completed (NEW)",0,0,21653.545439214089,20787.403621645524,20135.574581437824,19696.852059480629,19434.83214481287,0,0,96,92.16,88.473600000000005,84.934656000000004,84.934656000000004]
[null,"Retailer Requested Distributer Planned Interruption - Early Cancellation (NEW)",0,0,1500.8567669355848,1598.4124567863978,1718.3265646803191,1236.0016743237561,1017.5041420874919,0,0,55,58.575000000000003,62.382375000000003,44,35.200000000000003]
[null,"Retailer Requested Distributer Planned Interruption - MC No Attendance (NEW)",0,0,13653.289126657932,14199.420691724252,14900.081967749042,15789.461539361255,16876.805017607025,0,0,65,67.600000000000009,70.304000000000002,73.116159999999994,76.040806399999994]
[null,"Provision of metering consumption data (NEW)",0,0,368.70741508859999,276.53056131645002,186.38159832728729,95.346488729897047,39.426633984700743,0,0,20,15,10,5,2]
[null,"Part C. Inspection, Maint & Testing (NEW).xlsx",0,0,11640.75086043219,11640.75086043219,11738.308155983903,11945.718975044811,12255.542248005548,0,0,1,1,1,1,1]
[null,"Commissioning - Other (NEW)",0,0,12795.187100007561,20670.652843675467,31312.663240445036,42619.581297431243,54897.759164637959,0,0,8,8,8,8,8]
[null,"Connections under Chapter 5 of the NER (NEW)",0,0,16575.099326021467,16575.099326021467,16699.463886702946,16963.868052964626,17358.826062129967,0,0,1,1,1,1,1]

{"sheet":"4.4 Quoted services","index":27,"n_rows":12,"n_cols":16,"rows_kept":12,"cut":false,"hidden":false,"merged":[[8,2,8,8],[8,9,8,15],[8,1,9,1],[5,1,5,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"4.4 ANCILLARY SERVICES - QUOTED SERVICES"]
[]
[null,"There are TWO tables on this worksheet. The COLUMNS representing each table have been 'grouped' for easy navigation. See the Instructions sheet on how to group or ungroup data."]
[]
[null,"4.4.1 - COST METRICS FOR QUOTED SERVICES"]
[null,"SERVICE SUBCATEGORY",{"$f":"CONCATENATE(\"EXPENDITURE \n($0's, real \", dms_DollarReal, \")\")","v":"EXPENDITURE \n($0's, real June 2019)"},null,null,null,null,null,null,"VOLUMES (0's)"]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"High Load Escorts",2144.62,2198.2354999999998,6149.6516954245653,6149.6516954245653,6206.4450241156446,6327.1899746023864,6507.5547015855973,1,1,5,5,5,5,5]
[null,"  Tiger Tails ",94638.599999999991,97004.564999999973,119088.22107468796,119088.22107468796,120037.88093928956,122056.89683381976,125072.83455315066,0,0,210,210,210,210,210]

{"sheet":"5.4 MD & utilisation-Spatial","index":28,"n_rows":11577,"n_cols":12,"rows_kept":11577,"cut":false,"hidden":true,"merged":[[11337,1,11337,2],[11338,1,11338,2],[11339,1,11339,2],[11340,1,11340,2],[11341,1,11341,2],[11342,1,11342,2],[11343,1,11343,2],[11344,1,11344,2],[11345,1,11345,2],[11346,1,11346,2],[11347,1,11347,2],[11348,1,11348,2],[11349,1,11349,2],[11350,1,11350,2],[11351,1,11351,2],[11352,1,11352,2],[11353,1,11353,2],[11354,1,11354,2],[11355,1,11355,2],[11125,1,11125,2],[11126,1,11126,2],[11127,1,11127,2],[11128,1,11128,2],[11129,1,11129,2],[11130,1,11130,2],[11131,1,11131,2],[11132,1,11132,2],[11133,1,11133,2],[11134,1,11134,2],[11271,1,11271,2],[11272,1,11272,2],[11273,1,11273,2],[11274,1,11274,2],[11275,1,11275,2],[11276,1,11276,2],[11277,1,11277,2],[11278,1,11278,2],[11279,1,11279,2],[11280,1,11280,2],[11281,1,11281,2],[11282,1,11282,2],[11283,1,11283,2],[11284,1,11284,2],[11285,1,11285,2],[11286,1,11286,2],[11287,1,11287,2],[11288,1,11288,2],[11289,1,11289,2],[11323,1,11323,2],[11324,1,11324,2],[11325,1,11325,2],[11326,1,11326,2],[11327,1,11327,2],[11328,1,11328,2],[11329,1,11329,2],[11330,1,11330,2],[11331,1,11331,2],[11332,1,11332,2],[11333,1,11333,2],[11334,1,11334,2],[11335,1,11335,2],[11336,1,11336,2],[11205,1,11205,2],[11206,1,11206,2],[11257,1,11257,2],[11258,1,11258,2],[11259,1,11259,2],[11260,1,11260,2],[11261,1,11261,2],[11262,1,11262,2],[11263,1,11263,2],[11264,1,11264,2],[11265,1,11265,2],[11266,1,11266,2],[11267,1,11267,2],[11268,1,11268,2],[11269,1,11269,2],[11270,1,11270,2],[11074,5,11074,6],[11074,7,11074,11],[11077,1,11077,2],[11078,1,11078,2],[11079,1,11079,2],[11080,1,11080,2],[11081,1,11081,2],[11082,1,11082,2],[11083,1,11083,2],[11084,1,11084,2],[11085,1,11085,2],[11086,1,11086,2],[11087,1,11087,2],[11088,1,11088,2],[11089,1,11089,2],[11090,1,11090,2],[11091,1,11091,2],[11092,1,11092,2],[11093,1,11093,2],[11094,1,11094,2],[11095,1,11095,2],[11096,1,11096,2],[11097,1,11097,2],[11098,1,11098,2],[11099,1,11099,2],[11100,1,11100,2],[11101,1,11101,2],[11102,1,11102,2],[11103,1,11103,2],[11104,1,11104,2],[11105,1,11105,2],[11106,1,11106,2],[11107,1,11107,2],[11108,1,11108,2],[11109,1,11109,2],[11110,1,11110,2],[11111,1,11111,2],[11112,1,11112,2],[11113,1,11113,2],[11114,1,11114,2],[11115,1,11115,2],[11116,1,11116,2],[11117,1,11117,2],[11118,1,11118,2],[11119,1,11119,2],[11120,1,11120,2],[11121,1,11121,2],[11122,1,11122,2],[11123,1,11123,2],[11124,1,11124,2],[11489,1,11489,2],[11490,1,11490,2],[11491,1,11491,2],[11492,1,11492,2],[11493,1,11493,2],[11494,1,11494,2],[11495,1,11495,2],[11496,1,11496,2],[11497,1,11497,2],[11455,1,11455,2],[11168,1,11168,2],[11169,1,11169,2],[11170,1,11170,2],[11171,1,11171,2],[11172,1,11172,2],[11173,1,11173,2],[11174,1,11174,2],[11175,1,11175,2],[11176,1,11176,2],[11177,1,11177,2],[11178,1,11178,2],[11179,1,11179,2],[11180,1,11180,2],[11181,1,11181,2],[11182,1,11182,2],[11183,1,11183,2],[11184,1,11184,2],[11185,1,11185,2],[11186,1,11186,2],[11187,1,11187,2],[11188,1,11188,2],[11189,1,11189,2],[11190,1,11190,2],[11191,1,11191,2],[11192,1,11192,2],[11193,1,11193,2],[11194,1,11194,2],[11195,1,11195,2],[11196,1,11196,2],[11197,1,11197,2],[11198,1,11198,2],[11199,1,11199,2],[11200,1,11200,2],[11201,1,11201,2],[11202,1,11202,2],[11203,1,11203,2],[11204,1,11204,2],[11240,1,11240,2],[11241,1,11241,2],[11242,1,11242,2],[11243,1,11243,2],[11244,1,11244,2],[11245,1,11245,2],[11246,1,11246,2],[11247,1,11247,2],[11248,1,11248,2],[11249,1,11249,2],[11250,1,11250,2],[11251,1,11251,2],[11252,1,11252,2],[11253,1,11253,2],[11254,1,11254,2],[11255,1,11255,2],[11256,1,11256,2],[11020,5,11020,6],[11020,7,11020,11],[201,2,202,2],[201,3,202,3],[203,2,204,2],[203,3,204,3],[247,2,248,2],[247,3,248,3],[249,2,250,2],[249,3,250,3],[261,2,262,2],[261,3,262,3],[719,3,720,3],[251,2,252,2],[251,3,252,3],[253,2,254,2],[253,3,254,3],[255,2,256,2],[255,3,256,3],[257,2,258,2],[257,3,258,3],[259,2,260,2],[259,3,260,3],[623,2,624,2],[1113,5,1113,6],[711,2,712,2],[711,3,712,3],[713,2,714,2],[713,3,714,3],[703,2,704,2],[315,2,316,2],[315,3,316,3],[317,2,318,2],[317,3,318,3],[319,2,320,2],[319,3,320,3],[321,2,322,2],[321,3,322,3],[323,2,324,2],[323,3,324,3],[325,2,326,2],[325,3,326,3],[327,2,328,2],[327,3,328,3],[329,2,330,2],[329,3,330,3],[1113,7,1113,11],[697,3,698,3],[699,2,700,2],[699,3,700,3],[701,2,702,2],[701,3,702,3],[691,2,692,2],[311,2,312,2],[311,3,312,3],[313,2,314,2],[331,3,332,3],[211,2,212,2],[211,3,212,3],[213,2,214,2],[205,2,206,2],[205,3,206,3],[207,2,208,2],[691,3,692,3],[9,7,9,11],[41,2,42,2],[41,3,42,3],[43,2,44,2],[43,3,44,3],[45,2,46,2],[45,3,46,3],[107,2,108,2],[107,3,108,3],[35,2,36,2],[35,3,36,3],[157,2,158,2],[157,3,158,3],[159,2,160,2],[159,3,160,3],[161,2,162,2],[161,3,162,3],[163,2,164,2],[163,3,164,3],[37,2,38,2],[37,3,38,3],[39,2,40,2],[39,3,40,3],[29,2,30,2],[29,3,30,3],[31,2,32,2],[537,2,538,2],[537,3,538,3],[495,2,496,2],[495,3,496,3],[497,2,498,2],[497,3,498,3],[499,2,500,2],[499,3,500,3],[137,2,138,2],[137,3,138,3],[139,2,140,2],[139,3,140,3],[141,2,142,2],[287,3,288,3],[289,2,290,2],[289,3,290,3],[291,2,292,2],[295,3,296,3],[297,2,298,2],[297,3,298,3],[11,2,12,2],[11,3,12,3],[13,2,14,2],[13,3,14,3],[15,2,16,2],[15,3,16,3],[71,2,72,2],[71,3,72,3],[73,2,74,2],[73,3,74,3],[169,2,170,2],[169,3,170,3],[109,2,110,2],[109,3,110,3],[111,2,112,2],[111,3,112,3],[101,2,102,2],[101,3,102,3],[95,3,96,3],[97,2,98,2],[97,3,98,3],[99,2,100,2],[99,3,100,3],[89,2,90,2],[89,3,90,3],[91,2,92,2],[91,3,92,3],[93,2,94,2],[93,3,94,3],[83,2,84,2],[83,3,84,3],[85,2,86,2],[85,3,86,3],[87,2,88,2],[87,3,88,3],[77,2,78,2],[77,3,78,3],[153,2,154,2],[131,2,132,2],[131,3,132,3],[133,2,134,2],[133,3,134,3],[79,2,80,2],[135,2,136,2],[135,3,136,3],[143,2,144,2],[143,3,144,3],[145,2,146,2],[145,3,146,3],[147,2,148,2],[147,3,148,3],[149,2,150,2],[149,3,150,3],[153,3,154,3],[167,2,168,2],[167,3,168,3],[23,2,24,2],[23,3,24,3],[25,2,26,2],[17,2,18,2],[17,3,18,3],[19,2,20,2],[19,3,20,3],[21,2,22,2],[21,3,22,3],[151,2,152,2],[151,3,152,3],[31,3,32,3],[33,2,34,2],[33,3,34,3],[797,2,798,2],[299,2,300,2],[299,3,300,3],[301,2,302,2],[301,3,302,3],[303,2,304,2],[303,3,304,3],[305,2,306,2],[305,3,306,3],[307,2,308,2],[307,3,308,3],[79,3,80,3],[81,2,82,2],[81,3,82,3],[539,2,540,2],[539,3,540,3],[507,2,508,2],[507,3,508,3],[509,2,510,2],[509,3,510,3],[511,2,512,2],[511,3,512,3],[501,2,502,2],[501,3,502,3],[503,2,504,2],[503,3,504,3],[505,2,506,2],[505,3,506,3],[533,2,534,2],[533,3,534,3],[535,2,536,2],[535,3,536,3],[199,2,200,2],[199,3,200,3],[281,2,282,2],[281,3,282,3],[283,2,284,2],[283,3,284,3],[285,2,286,2],[285,3,286,3],[287,2,288,2],[309,2,310,2],[309,3,310,3],[103,2,104,2],[103,3,104,3],[105,2,106,2],[105,3,106,3],[95,2,96,2],[649,3,650,3],[651,2,652,2],[651,3,652,3],[811,2,812,2],[811,3,812,3],[813,2,814,2],[703,3,704,3],[787,2,788,2],[787,3,788,3],[789,2,790,2],[789,3,790,3],[791,2,792,2],[667,2,668,2],[667,3,668,3],[669,2,670,2],[669,3,670,3],[629,2,630,2],[795,2,796,2],[795,3,796,3],[655,2,656,2],[655,3,656,3],[657,2,658,2],[657,3,658,3],[661,2,662,2],[661,3,662,3],[663,2,664,2],[769,3,770,3],[771,2,772,2],[771,3,772,3],[773,2,774,2],[773,3,774,3],[763,2,764,2],[663,3,664,3],[665,2,666,2],[665,3,666,3],[573,3,574,3],[575,2,576,2],[575,3,576,3],[341,3,342,3],[343,2,344,2],[343,3,344,3],[345,2,346,2],[345,3,346,3],[347,2,348,2],[347,3,348,3],[349,2,350,2],[349,3,350,3],[351,2,352,2],[541,2,542,2],[579,2,580,2],[579,3,580,3],[581,2,582,2],[275,2,276,2],[275,3,276,3],[277,2,278,2],[25,3,26,3],[27,2,28,2],[27,3,28,3],[207,3,208,3],[209,2,210,2],[209,3,210,3],[245,2,246,2],[245,3,246,3],[263,2,264,2],[263,3,264,3],[265,2,266,2],[265,3,266,3],[267,2,268,2],[267,3,268,3],[269,2,270,2],[269,3,270,3],[271,2,272,2],[271,3,272,3],[273,2,274,2],[273,3,274,3],[389,2,390,2],[389,3,390,3],[277,3,278,3],[279,2,280,2],[279,3,280,3],[313,3,314,3],[491,2,492,2],[491,3,492,3],[493,2,494,2],[291,3,292,3],[293,2,294,2],[293,3,294,3],[295,2,296,2],[331,2,332,2],[213,3,214,3],[215,2,216,2],[215,3,216,3],[217,2,218,2],[217,3,218,3],[155,2,156,2],[155,3,156,3],[141,3,142,3],[165,2,166,2],[165,3,166,3],[831,3,832,3],[833,2,834,2],[833,3,834,3],[815,2,816,2],[815,3,816,3],[805,2,806,2],[805,3,806,3],[807,2,808,2],[807,3,808,3],[809,2,810,2],[809,3,810,3],[877,2,878,2],[877,3,878,3],[783,3,784,3],[785,2,786,2],[785,3,786,3],[581,3,582,3],[583,2,584,2],[583,3,584,3],[585,2,586,2],[585,3,586,3],[587,2,588,2],[587,3,588,3],[589,2,590,2],[589,3,590,3],[591,2,592,2],[591,3,592,3],[593,2,594,2],[593,3,594,3],[595,2,596,2],[595,3,596,3],[597,2,598,2],[859,2,860,2],[859,3,860,3],[861,2,862,2],[861,3,862,3],[779,2,780,2],[779,3,780,3],[769,2,770,2],[853,2,854,2],[853,3,854,3],[855,2,856,2],[855,3,856,3],[857,2,858,2],[857,3,858,3],[847,2,848,2],[847,3,848,3],[849,2,850,2],[849,3,850,3],[851,2,852,2],[851,3,852,3],[841,2,842,2],[841,3,842,3],[843,2,844,2],[843,3,844,3],[845,2,846,2],[863,2,864,2],[863,3,864,3],[839,2,840,2],[839,3,840,3],[865,3,866,3],[659,2,660,2],[659,3,660,3],[649,2,650,2],[871,3,872,3],[873,2,874,2],[873,3,874,3],[875,2,876,2],[837,2,838,2],[837,3,838,3],[337,3,338,3],[339,2,340,2],[339,3,340,3],[405,2,406,2],[405,3,406,3],[407,2,408,2],[407,3,408,3],[341,2,342,2],[799,2,800,2],[799,3,800,3],[801,2,802,2],[801,3,802,3],[803,2,804,2],[803,3,804,3],[763,3,764,3],[765,2,766,2],[765,3,766,3],[767,2,768,2],[767,3,768,3],[673,2,674,2],[673,3,674,3],[675,2,676,2],[675,3,676,3],[677,2,678,2],[677,3,678,3],[747,3,748,3],[749,2,750,2],[749,3,750,3],[721,2,722,2],[721,3,722,3],[693,2,694,2],[693,3,694,3],[695,2,696,2],[469,2,470,2],[469,3,470,3],[471,2,472,2],[471,3,472,3],[473,2,474,2],[473,3,474,3],[475,2,476,2],[475,3,476,3],[477,2,478,2],[477,3,478,3],[479,2,480,2],[479,3,480,3],[481,2,482,2],[481,3,482,3],[483,2,484,2],[483,3,484,3],[485,2,486,2],[485,3,486,3],[487,2,488,2],[487,3,488,3],[489,2,490,2],[489,3,490,3],[829,2,830,2],[829,3,830,3],[831,2,832,2],[1069,2,1070,2],[1069,3,1070,3],[1071,2,1072,2],[1071,3,1072,3],[1073,2,1074,2],[1073,3,1074,3],[1063,2,1064,2],[1063,3,1064,3],[1065,2,1066,2],[1065,3,1066,3],[1067,2,1068,2],[1067,3,1068,3],[1057,2,1058,2],[1057,3,1058,3],[1059,2,1060,2],[1059,3,1060,3],[1061,2,1062,2],[1061,3,1062,3],[1051,2,1052,2],[1051,3,1052,3],[1053,2,1054,2],[1053,3,1054,3],[981,2,982,2],[981,3,982,3],[1055,2,1056,2],[1055,3,1056,3],[1021,2,1022,2],[879,2,880,2],[879,3,880,3],[881,2,882,2],[881,3,882,3],[883,2,884,2],[883,3,884,3],[885,2,886,2],[885,3,886,3],[887,2,888,2],[887,3,888,3],[889,2,890,2],[889,3,890,3],[891,2,892,2],[891,3,892,3],[893,2,894,2],[893,3,894,3],[1021,3,1022,3],[1023,2,1024,2],[1023,3,1024,3],[1025,2,1026,2],[1025,3,1026,3],[1027,2,1028,2],[1027,3,1028,3],[1029,2,1030,2],[1029,3,1030,3],[1031,2,1032,2],[1031,3,1032,3],[1033,2,1034,2],[1033,3,1034,3],[983,2,984,2],[983,3,984,3],[1039,3,1040,3],[1041,2,1042,2],[1041,3,1042,3],[1043,2,1044,2],[1043,3,1044,3],[1045,2,1046,2],[1105,2,1106,2],[1105,3,1106,3],[1107,2,1108,2],[1107,3,1108,3],[1109,2,1110,2],[1109,3,1110,3],[1099,2,1100,2],[1099,3,1100,3],[1101,2,1102,2],[1101,3,1102,3],[1103,2,1104,2],[1103,3,1104,3],[1093,2,1094,2],[1093,3,1094,3],[1095,2,1096,2],[1095,3,1096,3],[1097,2,1098,2],[1097,3,1098,3],[1087,2,1088,2],[1087,3,1088,3],[1089,2,1090,2],[1089,3,1090,3],[1091,2,1092,2],[1091,3,1092,3],[1081,2,1082,2],[1081,3,1082,3],[1083,2,1084,2],[1083,3,1084,3],[1085,2,1086,2],[1085,3,1086,3],[1075,2,1076,2],[1075,3,1076,3],[1077,2,1078,2],[1077,3,1078,3],[1079,2,1080,2],[1079,3,1080,3],[1045,3,1046,3],[1047,2,1048,2],[1047,3,1048,3],[1049,2,1050,2],[1049,3,1050,3],[1035,2,1036,2],[1035,3,1036,3],[1037,2,1038,2],[1037,3,1038,3],[1009,2,1010,2],[1009,3,1010,3],[1011,2,1012,2],[1011,3,1012,3],[1015,2,1016,2],[1015,3,1016,3],[1017,2,1018,2],[1017,3,1018,3],[1019,2,1020,2],[1019,3,1020,3],[1013,2,1014,2],[1013,3,1014,3],[1039,2,1040,2],[967,2,968,2],[967,3,968,3],[927,3,928,3],[929,2,930,2],[929,3,930,3],[919,2,920,2],[641,2,642,2],[641,3,642,3],[333,2,334,2],[333,3,334,3],[335,2,336,2],[335,3,336,3],[337,2,338,2],[351,3,352,3],[353,2,354,2],[353,3,354,3],[355,2,356,2],[355,3,356,3],[357,2,358,2],[357,3,358,3],[359,2,360,2],[359,3,360,3],[361,2,362,2],[361,3,362,3],[363,2,364,2],[363,3,364,3],[365,2,366,2],[365,3,366,3],[367,2,368,2],[367,3,368,3],[369,2,370,2],[369,3,370,3],[371,2,372,2],[371,3,372,3],[373,2,374,2],[373,3,374,3],[375,2,376,2],[375,3,376,3],[377,2,378,2],[597,3,598,3],[567,2,568,2],[567,3,568,3],[219,2,220,2],[219,3,220,3],[221,2,222,2],[221,3,222,3],[223,2,224,2],[223,3,224,3],[225,2,226,2],[225,3,226,3],[227,2,228,2],[227,3,228,3],[229,2,230,2],[229,3,230,3],[231,2,232,2],[231,3,232,3],[233,2,234,2],[233,3,234,3],[235,2,236,2],[235,3,236,3],[237,2,238,2],[237,3,238,3],[239,2,240,2],[239,3,240,3],[241,2,242,2],[241,3,242,3],[243,2,244,2],[243,3,244,3],[577,2,578,2],[577,3,578,3],[377,3,378,3],[379,2,380,2],[379,3,380,3],[381,2,382,2],[381,3,382,3],[383,2,384,2],[383,3,384,3],[385,2,386,2],[385,3,386,3],[387,2,388,2],[387,3,388,3],[527,2,528,2],[527,3,528,3],[447,2,448,2],[447,3,448,3],[449,2,450,2],[449,3,450,3],[451,2,452,2],[451,3,452,3],[453,2,454,2],[453,3,454,3],[455,2,456,2],[455,3,456,3],[457,2,458,2],[457,3,458,3],[459,2,460,2],[459,3,460,3],[461,2,462,2],[461,3,462,3],[529,2,530,2],[529,3,530,3],[569,2,570,2],[569,3,570,3],[571,2,572,2],[571,3,572,3],[573,2,574,2],[613,2,614,2],[613,3,614,3],[615,2,616,2],[615,3,616,3],[617,2,618,2],[995,3,996,3],[985,2,986,2],[985,3,986,3],[987,2,988,2],[987,3,988,3],[989,2,990,2],[989,3,990,3],[909,2,910,2],[971,2,972,2],[971,3,972,3],[949,2,950,2],[949,3,950,3],[951,2,952,2],[951,3,952,3],[953,2,954,2],[953,3,954,3],[955,2,956,2],[955,3,956,3],[957,2,958,2],[957,3,958,3],[959,2,960,2],[959,3,960,3],[961,2,962,2],[969,2,970,2],[969,3,970,3],[895,2,896,2],[895,3,896,3],[897,2,898,2],[897,3,898,3],[899,2,900,2],[899,3,900,3],[931,2,932,2],[931,3,932,3],[933,2,934,2],[933,3,934,3],[935,2,936,2],[935,3,936,3],[925,2,926,2],[925,3,926,3],[757,3,758,3],[759,2,760,2],[759,3,760,3],[919,3,920,3],[961,3,962,3],[963,2,964,2],[963,3,964,3],[965,2,966,2],[965,3,966,3],[937,2,938,2],[937,3,938,3],[939,2,940,2],[939,3,940,3],[943,2,944,2],[943,3,944,3],[945,2,946,2],[945,3,946,3],[947,2,948,2],[947,3,948,3],[941,2,942,2],[941,3,942,3],[909,3,910,3],[911,2,912,2],[679,3,680,3],[681,2,682,2],[681,3,682,3],[683,2,684,2],[683,3,684,3],[737,2,738,2],[737,3,738,3],[739,2,740,2],[739,3,740,3],[741,2,742,2],[741,3,742,3],[743,2,744,2],[743,3,744,3],[745,2,746,2],[745,3,746,3],[747,2,748,2],[715,2,716,2],[715,3,716,3],[717,2,718,2],[717,3,718,3],[775,2,776,2],[775,3,776,3],[845,3,846,3],[793,2,794,2],[793,3,794,3],[761,2,762,2],[761,3,762,3],[751,2,752,2],[751,3,752,3],[753,2,754,2],[753,3,754,3],[755,2,756,2],[755,3,756,3],[723,2,724,2],[723,3,724,3],[725,2,726,2],[725,3,726,3],[709,2,710,2],[709,3,710,3],[719,2,720,2],[777,2,778,2],[777,3,778,3],[757,2,758,2],[797,3,798,3],[927,2,928,2],[865,2,866,2],[813,3,814,3],[875,3,876,3],[869,2,870,2],[869,3,870,3],[823,2,824,2],[823,3,824,3],[825,2,826,2],[825,3,826,3],[827,2,828,2],[827,3,828,3],[835,2,836,2],[835,3,836,3]],"merged_total":11560,"flags":["merged_cut"]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Adaminaby 33kV","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3834378308186399,2.32067861739954,2.2632993313804901,2.2108387875863702,2.1628753351610497,2.11902346855469,2.0789307290285701]
[null,null,null,null,"Coincident",0.72225388812686064,0.70323594466652728,0.68584828223651217,0.66995114775344555,0.65541676823062112,0.64212832380445151,0.62997900879653645]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3928003812202845,2.3297946389044766,2.2721899572613338,2.2195233395016927,2.1713714784529281,2.1273473542336365,2.0870971235870437]
[null,null,null,null,"Coincident",0.72509102461220742,0.70599837542559896,0.68854241129131333,0.67258283015202813,0.65799135710694789,0.64465071340413227,0.63245367381425566]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1983853702753597,2.1425297568472801,2.0915544010126101,2.0450329013281099,2.0025761122099901,1.9638288887875599,1.92846711616811]
[null,null,null,null,"Coincident",0.66617738493192724,0.64925144146887281,0.63380436394321527,0.61970693979639691,0.6068412461242394,0.59509966326895758,0.58438397459639702]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2070210030429958,2.1509459792366914,2.0997703835081705,2.0530661394365817,2.010442572807897,1.9715431436817872,1.9360424639869522]
[null,null,null,null,"Coincident",0.66879424334636239,0.65180181188990649,0.63629405560853647,0.62214125437472179,0.60922502206299911,0.59743731626720831,0.58667953454150068]
[null,"Ballina 132kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Bega 132kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Boambee South 66kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Boundary Street","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Cartwrights Hill 33kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Casino 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Casino 66/33kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"Coleambally 132","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Dubbo 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Goulburn 132/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Goulburn 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Hawks Nest 132/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Hay 132","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Herons Creek","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Hillston","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Jindabyne 33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Junee 66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Lismore 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Maclean 66/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Marulan South 33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Moruya North","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Morven","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Nyngan 132","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Oura 11/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Pinnacles Place","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Quirindi 66/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Snowy Adit 66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Steeple Flat 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Stroud 132/33kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Temora 132/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Terranora 110/66kV","Substation Rating","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Date MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,0,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,0,null,null,"Coincident"]
[null,"Yanco 33/66kV","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[]
[]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Unit",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION",null,"Units","Max Demand",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]
[null,"<Enter substation name>",null,"MWh","Non-Coincident"]

{"sheet":"5.4.1 Non-COIN&COIN Max Demand","index":29,"n_rows":10642,"n_cols":12,"rows_kept":10642,"cut":false,"hidden":false,"merged":[[16,2,17,2],[16,3,17,3],[18,2,19,2],[18,3,19,3],[20,2,21,2],[20,3,21,3],[6,1,6,2],[10,5,10,6],[10,7,10,11],[12,2,13,2],[12,3,13,3],[14,2,15,2],[14,3,15,3],[52,2,53,2],[52,3,53,3],[54,2,55,2],[54,3,55,3],[56,2,57,2],[56,3,57,3],[46,2,47,2],[46,3,47,3],[48,2,49,2],[48,3,49,3],[50,2,51,2],[50,3,51,3],[40,2,41,2],[40,3,41,3],[42,2,43,2],[42,3,43,3],[44,2,45,2],[44,3,45,3],[34,2,35,2],[34,3,35,3],[36,2,37,2],[36,3,37,3],[38,2,39,2],[38,3,39,3],[28,2,29,2],[28,3,29,3],[30,2,31,2],[30,3,31,3],[32,2,33,2],[32,3,33,3],[22,2,23,2],[22,3,23,3],[24,2,25,2],[24,3,25,3],[26,2,27,2],[26,3,27,3],[88,2,89,2],[88,3,89,3],[90,2,91,2],[90,3,91,3],[92,2,93,2],[92,3,93,3],[82,2,83,2],[82,3,83,3],[84,2,85,2],[84,3,85,3],[86,2,87,2],[86,3,87,3],[76,2,77,2],[76,3,77,3],[78,2,79,2],[78,3,79,3],[80,2,81,2],[80,3,81,3],[70,2,71,2],[70,3,71,3],[72,2,73,2],[72,3,73,3],[74,2,75,2],[74,3,75,3],[64,2,65,2],[64,3,65,3],[66,2,67,2],[66,3,67,3],[68,2,69,2],[68,3,69,3],[58,2,59,2],[58,3,59,3],[60,2,61,2],[60,3,61,3],[62,2,63,2],[62,3,63,3],[124,2,125,2],[124,3,125,3],[126,2,127,2],[126,3,127,3],[128,2,129,2],[128,3,129,3],[118,2,119,2],[118,3,119,3],[120,2,121,2],[120,3,121,3],[122,2,123,2],[122,3,123,3],[112,2,113,2],[112,3,113,3],[114,2,115,2],[114,3,115,3],[116,2,117,2],[116,3,117,3],[106,2,107,2],[106,3,107,3],[108,2,109,2],[108,3,109,3],[110,2,111,2],[110,3,111,3],[100,2,101,2],[100,3,101,3],[102,2,103,2],[102,3,103,3],[104,2,105,2],[104,3,105,3],[94,2,95,2],[94,3,95,3],[96,2,97,2],[96,3,97,3],[98,2,99,2],[98,3,99,3],[160,2,161,2],[160,3,161,3],[162,2,163,2],[162,3,163,3],[164,2,165,2],[164,3,165,3],[154,2,155,2],[154,3,155,3],[156,2,157,2],[156,3,157,3],[158,2,159,2],[158,3,159,3],[148,2,149,2],[148,3,149,3],[150,2,151,2],[150,3,151,3],[152,2,153,2],[152,3,153,3],[142,2,143,2],[142,3,143,3],[144,2,145,2],[144,3,145,3],[146,2,147,2],[146,3,147,3],[136,2,137,2],[136,3,137,3],[138,2,139,2],[138,3,139,3],[140,2,141,2],[140,3,141,3],[130,2,131,2],[130,3,131,3],[132,2,133,2],[132,3,133,3],[134,2,135,2],[134,3,135,3],[196,2,197,2],[196,3,197,3],[198,2,199,2],[198,3,199,3],[200,2,201,2],[200,3,201,3],[190,2,191,2],[190,3,191,3],[192,2,193,2],[192,3,193,3],[194,2,195,2],[194,3,195,3],[184,2,185,2],[184,3,185,3],[186,2,187,2],[186,3,187,3],[188,2,189,2],[188,3,189,3],[178,2,179,2],[178,3,179,3],[180,2,181,2],[180,3,181,3],[182,2,183,2],[182,3,183,3],[172,2,173,2],[172,3,173,3],[174,2,175,2],[174,3,175,3],[176,2,177,2],[176,3,177,3],[166,2,167,2],[166,3,167,3],[168,2,169,2],[168,3,169,3],[170,2,171,2],[170,3,171,3],[232,2,233,2],[232,3,233,3],[234,2,235,2],[234,3,235,3],[236,2,237,2],[236,3,237,3],[226,2,227,2],[226,3,227,3],[228,2,229,2],[228,3,229,3],[230,2,231,2],[230,3,231,3],[220,2,221,2],[220,3,221,3],[222,2,223,2],[222,3,223,3],[224,2,225,2],[224,3,225,3],[214,2,215,2],[214,3,215,3],[216,2,217,2],[216,3,217,3],[218,2,219,2],[218,3,219,3],[208,2,209,2],[208,3,209,3],[210,2,211,2],[210,3,211,3],[212,2,213,2],[212,3,213,3],[202,2,203,2],[202,3,203,3],[204,2,205,2],[204,3,205,3],[206,2,207,2],[206,3,207,3],[268,2,269,2],[268,3,269,3],[270,2,271,2],[270,3,271,3],[272,2,273,2],[272,3,273,3],[262,2,263,2],[262,3,263,3],[264,2,265,2],[264,3,265,3],[266,2,267,2],[266,3,267,3],[256,2,257,2],[256,3,257,3],[258,2,259,2],[258,3,259,3],[260,2,261,2],[260,3,261,3],[250,2,251,2],[250,3,251,3],[252,2,253,2],[252,3,253,3],[254,2,255,2],[254,3,255,3],[244,2,245,2],[244,3,245,3],[246,2,247,2],[246,3,247,3],[248,2,249,2],[248,3,249,3],[238,2,239,2],[238,3,239,3],[240,2,241,2],[240,3,241,3],[242,2,243,2],[242,3,243,3],[304,2,305,2],[304,3,305,3],[306,2,307,2],[306,3,307,3],[308,2,309,2],[308,3,309,3],[298,2,299,2],[298,3,299,3],[300,2,301,2],[300,3,301,3],[302,2,303,2],[302,3,303,3],[292,2,293,2],[292,3,293,3],[294,2,295,2],[294,3,295,3],[296,2,297,2],[296,3,297,3],[286,2,287,2],[286,3,287,3],[288,2,289,2],[288,3,289,3],[290,2,291,2],[290,3,291,3],[280,2,281,2],[280,3,281,3],[282,2,283,2],[282,3,283,3],[284,2,285,2],[284,3,285,3],[274,2,275,2],[274,3,275,3],[276,2,277,2],[276,3,277,3],[278,2,279,2],[278,3,279,3],[340,2,341,2],[340,3,341,3],[342,2,343,2],[342,3,343,3],[344,2,345,2],[344,3,345,3],[334,2,335,2],[334,3,335,3],[336,2,337,2],[336,3,337,3],[338,2,339,2],[338,3,339,3],[328,2,329,2],[328,3,329,3],[330,2,331,2],[330,3,331,3],[332,2,333,2],[332,3,333,3],[322,2,323,2],[322,3,323,3],[324,2,325,2],[324,3,325,3],[326,2,327,2],[326,3,327,3],[316,2,317,2],[316,3,317,3],[318,2,319,2],[318,3,319,3],[320,2,321,2],[320,3,321,3],[310,2,311,2],[310,3,311,3],[312,2,313,2],[312,3,313,3],[314,2,315,2],[314,3,315,3],[376,2,377,2],[376,3,377,3],[378,2,379,2],[378,3,379,3],[380,2,381,2],[380,3,381,3],[370,2,371,2],[370,3,371,3],[372,2,373,2],[372,3,373,3],[374,2,375,2],[374,3,375,3],[364,2,365,2],[364,3,365,3],[366,2,367,2],[366,3,367,3],[368,2,369,2],[368,3,369,3],[358,2,359,2],[358,3,359,3],[360,2,361,2],[360,3,361,3],[362,2,363,2],[362,3,363,3],[352,2,353,2],[352,3,353,3],[354,2,355,2],[354,3,355,3],[356,2,357,2],[356,3,357,3],[346,2,347,2],[346,3,347,3],[348,2,349,2],[348,3,349,3],[350,2,351,2],[350,3,351,3],[412,2,413,2],[412,3,413,3],[414,2,415,2],[414,3,415,3],[416,2,417,2],[416,3,417,3],[406,2,407,2],[406,3,407,3],[408,2,409,2],[408,3,409,3],[410,2,411,2],[410,3,411,3],[400,2,401,2],[400,3,401,3],[402,2,403,2],[402,3,403,3],[404,2,405,2],[404,3,405,3],[394,2,395,2],[394,3,395,3],[396,2,397,2],[396,3,397,3],[398,2,399,2],[398,3,399,3],[388,2,389,2],[388,3,389,3],[390,2,391,2],[390,3,391,3],[392,2,393,2],[392,3,393,3],[382,2,383,2],[382,3,383,3],[384,2,385,2],[384,3,385,3],[386,2,387,2],[386,3,387,3],[448,2,449,2],[448,3,449,3],[450,2,451,2],[450,3,451,3],[452,2,453,2],[452,3,453,3],[442,2,443,2],[442,3,443,3],[444,2,445,2],[444,3,445,3],[446,2,447,2],[446,3,447,3],[436,2,437,2],[436,3,437,3],[438,2,439,2],[438,3,439,3],[440,2,441,2],[440,3,441,3],[430,2,431,2],[430,3,431,3],[432,2,433,2],[432,3,433,3],[434,2,435,2],[434,3,435,3],[424,2,425,2],[424,3,425,3],[426,2,427,2],[426,3,427,3],[428,2,429,2],[428,3,429,3],[418,2,419,2],[418,3,419,3],[420,2,421,2],[420,3,421,3],[422,2,423,2],[422,3,423,3],[484,2,485,2],[484,3,485,3],[486,2,487,2],[486,3,487,3],[488,2,489,2],[488,3,489,3],[478,2,479,2],[478,3,479,3],[480,2,481,2],[480,3,481,3],[482,2,483,2],[482,3,483,3],[472,2,473,2],[472,3,473,3],[474,2,475,2],[474,3,475,3],[476,2,477,2],[476,3,477,3],[466,2,467,2],[466,3,467,3],[468,2,469,2],[468,3,469,3],[470,2,471,2],[470,3,471,3],[460,2,461,2],[460,3,461,3],[462,2,463,2],[462,3,463,3],[464,2,465,2],[464,3,465,3],[454,2,455,2],[454,3,455,3],[456,2,457,2],[456,3,457,3],[458,2,459,2],[458,3,459,3],[520,2,521,2],[520,3,521,3],[522,2,523,2],[522,3,523,3],[524,2,525,2],[524,3,525,3],[514,2,515,2],[514,3,515,3],[516,2,517,2],[516,3,517,3],[518,2,519,2],[518,3,519,3],[508,2,509,2],[508,3,509,3],[510,2,511,2],[510,3,511,3],[512,2,513,2],[512,3,513,3],[502,2,503,2],[502,3,503,3],[504,2,505,2],[504,3,505,3],[506,2,507,2],[506,3,507,3],[496,2,497,2],[496,3,497,3],[498,2,499,2],[498,3,499,3],[500,2,501,2],[500,3,501,3],[490,2,491,2],[490,3,491,3],[492,2,493,2],[492,3,493,3],[494,2,495,2],[494,3,495,3],[556,2,557,2],[556,3,557,3],[558,2,559,2],[558,3,559,3],[560,2,561,2],[560,3,561,3],[550,2,551,2],[550,3,551,3],[552,2,553,2],[552,3,553,3],[554,2,555,2],[554,3,555,3],[544,2,545,2],[544,3,545,3],[546,2,547,2],[546,3,547,3],[548,2,549,2],[548,3,549,3],[538,2,539,2],[538,3,539,3],[540,2,541,2],[540,3,541,3],[542,2,543,2],[542,3,543,3],[532,2,533,2],[532,3,533,3],[534,2,535,2],[534,3,535,3],[536,2,537,2],[536,3,537,3],[526,2,527,2],[526,3,527,3],[528,2,529,2],[528,3,529,3],[530,2,531,2],[530,3,531,3],[592,2,593,2],[592,3,593,3],[594,2,595,2],[594,3,595,3],[596,2,597,2],[596,3,597,3],[586,2,587,2],[586,3,587,3],[588,2,589,2],[588,3,589,3],[590,2,591,2],[590,3,591,3],[580,2,581,2],[580,3,581,3],[582,2,583,2],[582,3,583,3],[584,2,585,2],[584,3,585,3],[574,2,575,2],[574,3,575,3],[576,2,577,2],[576,3,577,3],[578,2,579,2],[578,3,579,3],[568,2,569,2],[568,3,569,3],[570,2,571,2],[570,3,571,3],[572,2,573,2],[572,3,573,3],[562,2,563,2],[562,3,563,3],[564,2,565,2],[564,3,565,3],[566,2,567,2],[566,3,567,3],[628,2,629,2],[628,3,629,3],[630,2,631,2],[630,3,631,3],[632,2,633,2],[632,3,633,3],[622,2,623,2],[622,3,623,3],[624,2,625,2],[624,3,625,3],[626,2,627,2],[626,3,627,3],[616,2,617,2],[616,3,617,3],[618,2,619,2],[618,3,619,3],[620,2,621,2],[620,3,621,3],[610,2,611,2],[610,3,611,3],[612,2,613,2],[612,3,613,3],[614,2,615,2],[614,3,615,3],[604,2,605,2],[604,3,605,3],[606,2,607,2],[606,3,607,3],[608,2,609,2],[608,3,609,3],[598,2,599,2],[598,3,599,3],[600,2,601,2],[600,3,601,3],[602,2,603,2],[602,3,603,3],[664,2,665,2],[664,3,665,3],[666,2,667,2],[666,3,667,3],[668,2,669,2],[668,3,669,3],[658,2,659,2],[658,3,659,3],[660,2,661,2],[660,3,661,3],[662,2,663,2],[662,3,663,3],[652,2,653,2],[652,3,653,3],[654,2,655,2],[654,3,655,3],[656,2,657,2],[656,3,657,3],[646,2,647,2],[646,3,647,3],[648,2,649,2],[648,3,649,3],[650,2,651,2],[650,3,651,3],[640,2,641,2],[640,3,641,3],[642,2,643,2],[642,3,643,3],[644,2,645,2],[644,3,645,3],[634,2,635,2],[634,3,635,3],[636,2,637,2],[636,3,637,3],[638,2,639,2],[638,3,639,3],[700,2,701,2],[700,3,701,3],[702,2,703,2],[702,3,703,3],[704,2,705,2],[704,3,705,3],[694,2,695,2],[694,3,695,3],[696,2,697,2],[696,3,697,3],[698,2,699,2],[698,3,699,3],[688,2,689,2],[688,3,689,3],[690,2,691,2],[690,3,691,3],[692,2,693,2],[692,3,693,3],[682,2,683,2],[682,3,683,3],[684,2,685,2],[684,3,685,3],[686,2,687,2],[686,3,687,3],[676,2,677,2],[676,3,677,3],[678,2,679,2],[678,3,679,3],[680,2,681,2],[680,3,681,3],[670,2,671,2],[670,3,671,3],[672,2,673,2],[672,3,673,3],[674,2,675,2],[674,3,675,3],[736,2,737,2],[736,3,737,3],[740,5,740,6],[740,7,740,11],[742,2,743,2],[742,3,743,3],[730,2,731,2],[730,3,731,3],[732,2,733,2],[732,3,733,3],[734,2,735,2],[734,3,735,3],[724,2,725,2],[724,3,725,3],[726,2,727,2],[726,3,727,3],[728,2,729,2],[728,3,729,3],[718,2,719,2],[718,3,719,3],[720,2,721,2],[720,3,721,3],[722,2,723,2],[722,3,723,3],[712,2,713,2],[712,3,713,3],[714,2,715,2],[714,3,715,3],[716,2,717,2],[716,3,717,3],[706,2,707,2],[706,3,707,3],[708,2,709,2],[708,3,709,3],[710,2,711,2],[710,3,711,3],[774,2,775,2],[774,3,775,3],[776,2,777,2],[776,3,777,3],[778,2,779,2],[778,3,779,3],[768,2,769,2],[768,3,769,3],[770,2,771,2],[770,3,771,3],[772,2,773,2],[772,3,773,3],[762,2,763,2],[762,3,763,3],[764,2,765,2],[764,3,765,3],[766,2,767,2],[766,3,767,3],[756,2,757,2],[756,3,757,3],[758,2,759,2],[758,3,759,3],[760,2,761,2],[760,3,761,3],[750,2,751,2],[750,3,751,3],[752,2,753,2],[752,3,753,3],[754,2,755,2],[754,3,755,3],[744,2,745,2],[744,3,745,3],[746,2,747,2],[746,3,747,3],[748,2,749,2],[748,3,749,3],[810,2,811,2],[810,3,811,3],[812,2,813,2],[812,3,813,3],[814,2,815,2],[814,3,815,3],[804,2,805,2],[804,3,805,3],[806,2,807,2],[806,3,807,3],[808,2,809,2],[808,3,809,3],[798,2,799,2],[798,3,799,3],[800,2,801,2],[800,3,801,3],[802,2,803,2],[802,3,803,3],[792,2,793,2],[792,3,793,3],[794,2,795,2],[794,3,795,3],[796,2,797,2],[796,3,797,3],[786,2,787,2],[786,3,787,3],[788,2,789,2],[788,3,789,3],[790,2,791,2],[790,3,791,3],[780,2,781,2],[780,3,781,3],[782,2,783,2],[782,3,783,3],[784,2,785,2],[784,3,785,3],[846,2,847,2],[846,3,847,3],[848,2,849,2],[848,3,849,3],[850,2,851,2],[850,3,851,3],[840,2,841,2],[840,3,841,3],[842,2,843,2],[842,3,843,3],[844,2,845,2],[844,3,845,3],[834,2,835,2],[834,3,835,3],[836,2,837,2],[836,3,837,3],[838,2,839,2],[838,3,839,3],[828,2,829,2],[828,3,829,3],[830,2,831,2],[830,3,831,3],[832,2,833,2],[832,3,833,3],[822,2,823,2],[822,3,823,3],[824,2,825,2],[824,3,825,3],[826,2,827,2],[826,3,827,3],[816,2,817,2],[816,3,817,3],[818,2,819,2],[818,3,819,3],[820,2,821,2],[820,3,821,3],[882,2,883,2],[882,3,883,3],[884,2,885,2],[884,3,885,3],[886,2,887,2],[886,3,887,3],[876,2,877,2],[876,3,877,3],[878,2,879,2],[878,3,879,3],[880,2,881,2],[880,3,881,3],[870,2,871,2],[870,3,871,3],[872,2,873,2],[872,3,873,3],[874,2,875,2],[874,3,875,3],[864,2,865,2],[864,3,865,3],[866,2,867,2],[866,3,867,3],[868,2,869,2],[868,3,869,3],[858,2,859,2],[858,3,859,3],[860,2,861,2],[860,3,861,3],[862,2,863,2],[862,3,863,3],[852,2,853,2],[852,3,853,3],[854,2,855,2],[854,3,855,3],[856,2,857,2],[856,3,857,3],[918,2,919,2],[918,3,919,3],[920,2,921,2],[920,3,921,3],[922,2,923,2],[922,3,923,3],[912,2,913,2],[912,3,913,3],[914,2,915,2],[914,3,915,3],[916,2,917,2],[916,3,917,3],[906,2,907,2],[906,3,907,3],[908,2,909,2],[908,3,909,3],[910,2,911,2],[910,3,911,3],[900,2,901,2],[900,3,901,3],[902,2,903,2],[902,3,903,3],[904,2,905,2],[904,3,905,3],[894,2,895,2],[894,3,895,3],[896,2,897,2],[896,3,897,3],[898,2,899,2],[898,3,899,3],[888,2,889,2],[888,3,889,3],[890,2,891,2],[890,3,891,3],[892,2,893,2],[892,3,893,3],[954,2,955,2],[954,3,955,3],[956,2,957,2],[956,3,957,3],[958,2,959,2],[958,3,959,3],[948,2,949,2],[948,3,949,3],[950,2,951,2],[950,3,951,3],[952,2,953,2],[952,3,953,3],[942,2,943,2],[942,3,943,3],[944,2,945,2],[944,3,945,3],[946,2,947,2],[946,3,947,3],[936,2,937,2],[936,3,937,3],[938,2,939,2],[938,3,939,3],[940,2,941,2],[940,3,941,3],[930,2,931,2],[930,3,931,3],[932,2,933,2],[932,3,933,3],[934,2,935,2],[934,3,935,3],[924,2,925,2],[924,3,925,3],[926,2,927,2],[926,3,927,3],[928,2,929,2],[928,3,929,3],[990,2,991,2],[990,3,991,3],[992,2,993,2],[992,3,993,3],[994,2,995,2],[994,3,995,3],[984,2,985,2],[984,3,985,3],[986,2,987,2],[986,3,987,3],[988,2,989,2],[988,3,989,3],[978,2,979,2],[978,3,979,3],[980,2,981,2],[980,3,981,3],[982,2,983,2],[982,3,983,3],[972,2,973,2],[972,3,973,3],[974,2,975,2],[974,3,975,3],[976,2,977,2],[976,3,977,3],[966,2,967,2],[966,3,967,3],[968,2,969,2],[968,3,969,3],[970,2,971,2],[970,3,971,3],[960,2,961,2],[960,3,961,3],[962,2,963,2],[962,3,963,3],[964,2,965,2],[964,3,965,3],[1026,2,1027,2],[1026,3,1027,3],[1028,2,1029,2],[1028,3,1029,3],[1030,2,1031,2],[1030,3,1031,3],[1020,2,1021,2],[1020,3,1021,3],[1022,2,1023,2],[1022,3,1023,3],[1024,2,1025,2],[1024,3,1025,3],[1014,2,1015,2],[1014,3,1015,3],[1016,2,1017,2]],"merged_total":10631,"flags":["merged_cut"]}
[]
[null,"REGULATORY REPORTING STATEMENT"]
[null,"Australian Distribution Co."]
[null,"2019-20 to 2023-24"]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"There are two tables on this worksheet. The tables have been sub-grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"5.4.1 - NON-COINCIDENT & COINCIDENT MAXIMUM DEMAND"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","FORECASTING ELEMENTS","UNIT","MAX DEMAND","2017-18","2018-19","2019-20","2020-21","2021-22","2022-23","2023-24"]
[null,"Adaminaby 33kV","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.3834378308186399,2.32067861739954,2.2632993313804901,2.2108387875863702,2.1628753351610497,2.11902346855469,2.0789307290285701]
[null,null,null,null,"Coincident",0.72225388812686064,0.70323594466652728,0.68584828223651217,0.66995114775344555,0.65541676823062112,0.64212832380445151,0.62997900879653645]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3928003812202845,2.3297946389044766,2.2721899572613338,2.2195233395016927,2.1713714784529281,2.1273473542336365,2.0870971235870437]
[null,null,null,null,"Coincident",0.72509102461220742,0.70599837542559896,0.68854241129131333,0.67258283015202813,0.65799135710694789,0.64465071340413227,0.63245367381425566]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1983853702753597,2.1425297568472801,2.0915544010126101,2.0450329013281099,2.0025761122099901,1.9638288887875599,1.92846711616811]
[null,null,null,null,"Coincident",0.66617738493192724,0.64925144146887281,0.63380436394321527,0.61970693979639691,0.6068412461242394,0.59509966326895758,0.58438397459639702]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2070210030429958,2.1509459792366914,2.0997703835081705,2.0530661394365817,2.010442572807897,1.9715431436817872,1.9360424639869522]
[null,null,null,null,"Coincident",0.66879424334636239,0.65180181188990649,0.63629405560853647,0.62214125437472179,0.60922502206299911,0.59743731626720831,0.58667953454150068]
[null,"Ballina 132kV","Substation Rating","MVA","Non-Coincident",134.4,134.4,134.4,134.4,134.4,134.4,134.4]
[null,null,null,null,"Coincident",123.20000000000002,123.20000000000002,123.20000000000002,123.20000000000002,123.20000000000002,123.20000000000002,123.20000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.1906431204734,17.1906431204734,17.1906431204734,17.1906431204734,17.1906431204734,17.1906431204734,17.1906431204734]
[null,null,null,null,"Coincident",8.773231073166043,8.773231073166043,8.773231073166043,8.773231073166043,8.773231073166043,8.773231073166043,8.773231073166043]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.444955491715959,17.444955491715959,17.444955491715959,17.444955491715959,17.444955491715959,17.444955491715959,17.444955491715959]
[null,null,null,null,"Coincident",8.9030191899944686,8.9030191899944686,8.9030191899944686,8.9030191899944686,8.9030191899944686,8.9030191899944686,8.9030191899944686]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.570761494829799,15.5707614948297,15.5707614948297,15.5707614948297,15.5707614948297,15.5707614948297,15.5707614948297]
[null,null,null,null,"Coincident",7.9465257711391697,7.9465257711391191,7.9465257711391191,7.9465257711391191,7.9465257711391191,7.9465257711391191,7.9465257711391191]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.801109902975536,15.801109902975435,15.801109902975435,15.801109902975435,15.801109902975435,15.801109902975435,15.801109902975435]
[null,null,null,null,"Coincident",8.0640838984201491,8.0640838984200975,8.0640838984200975,8.0640838984200975,8.0640838984200975,8.0640838984200975,8.0640838984200975]
[null,"Bega 132kV","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",42.050039640523799,41.8638058582996,41.678346102254601,41.493657155375601,41.309735814020001,43.199675170589401,43.199675170589401]
[null,null,null,null,"Coincident",38.393154940571165,38.223116992516253,38.0537857573986,37.885158297972787,37.717231689201213,39.442812334674024,39.442812334674024]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",42.077946900811739,41.89158952120976,41.706006681483295,41.521195162484105,41.337151758443433,43.22834540704212,43.22834540704212]
[null,null,null,null,"Coincident",38.418635243975423,38.248484447197519,38.079040832379548,37.910301460326728,37.742263404060203,39.468989261966414,39.468989261966414]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",41.142547781513699,41.142547781513699,41.142547781513699,41.142547781513699,41.142547781513699,41.142547781513699,41.142547781513699]
[null,null,null,null,"Coincident",37.56458317588001,37.56458317588001,37.56458317588001,37.56458317588001,37.56458317588001,37.56458317588001,37.56458317588001]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",41.169852768611527,41.169852768611527,41.169852768611527,41.169852768611527,41.169852768611527,41.169852768611527,41.169852768611527]
[null,null,null,null,"Coincident",37.589513582825141,37.589513582825141,37.589513582825141,37.589513582825141,37.589513582825141,37.589513582825141,37.589513582825141]
[null,"Boambee South 66kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.531250521136,11.456992239612299,12.268930683784699,12.9810559169547,13.605638176062101,14.1534392933674,14.6338981276445]
[null,null,null,null,"Coincident",8.8776221306480672,9.6580028794219412,10.342449867578038,10.942756423489403,11.469266098169889,11.931050889294456,12.336067555784663]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.65291032415047,11.589346456826306,12.410664629548476,13.131016522545362,13.762814121792744,14.316943583095625,14.802952805431332]
[null,null,null,null,"Coincident",8.9801787793085381,9.7695746937535333,10.461928595299051,11.069170051979691,11.601762106257768,12.068881557934803,12.478577084524661]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4107435756014404,8.99159970680196,9.5056225861686006,9.9605020413725711,10.363043109236299,10.7192678396855,11.0345053861476]
[null,null,null,null,"Coincident",7.0900794879116669,7.5797289587621721,8.0130394075418572,8.3964931968322389,8.7358268291857364,9.0361167657106556,9.3018553703774511]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.5079067191957591,9.0954730546934588,9.6154340628818549,10.075568406363754,10.482759735554305,10.843099668699365,11.161978923022119]
[null,null,null,null,"Coincident",7.1719859692098833,7.6672920007936325,8.105608166960522,8.4934917162662593,8.8367454208643057,9.1405043864899529,9.4093128740953613]
[null,"Boundary Street","Substation Rating","MVA","Non-Coincident",24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004]
[null,null,null,null,"Coincident",24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.4700251095910097,4.4700253979646503,4.4700253982530205,4.47002539825331,4.47002539825331,4.47002539825331,4.47002539825331]
[null,null,null,null,"Coincident",3.7153215521337133,3.7153217918193473,3.7153217920590302,3.7153217920592709,3.7153217920592709,3.7153217920592709,3.7153217920592709]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7055812994950621,4.705581603065081,4.7055816033686479,4.7055816033689526,4.7055816033689526,4.7055816033689526,4.7055816033689526]
[null,null,null,null,"Coincident",3.9111072507892413,3.9111075031055496,3.9111075033578633,3.9111075033581164,3.9111075033581164,3.9111075033581164,3.9111075033581164]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.1973855352748997,4.2439643435934702,4.2686904943959796,4.2818162602877701,4.28878401404865,4.2924828147793992,4.2944463065036098]
[null,null,null,null,"Coincident",3.4887134992510114,3.5274281028999659,3.5479795760406341,3.5588892330806798,3.5646805754295658,3.5677548834558261,3.5693868660379247]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4185744816471049,4.4676078458907078,4.4936369866611114,4.5074544389142179,4.5147893712675806,4.5186830871019339,4.5207500486318226]
[null,null,null,null,"Coincident",3.6725576700112947,3.7133124108643161,3.7349468816596381,3.7464314431314287,3.7525279709109749,3.7557642852498403,3.7574822681539963]
[null,"Cartwrights Hill 33kV","Substation Rating","MVA","Non-Coincident",9.9,9.9,9.9,9.9,9.9,9.9,9.9]
[null,null,null,null,"Coincident",9.9,9.9,9.9,9.9,9.9,9.9,9.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.99316534052695,1.93723949091822,1.8853393382868802,1.8371751018559501,1.7924778600683702,1.7509980490828601,1.7125040693520499]
[null,null,null,null,"Coincident",0.75990418066158538,0.73858217286794725,0.71879498203153491,0.70043212779257835,0.6833910824724525,0.66757669861777036,0.65290067775137728]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0327436832697408,1.975707312421759,1.9227765769343559,1.8736559418451468,1.8280711456138103,1.7857676688025357,1.7465093129849341]
[null,null,null,null,"Coincident",0.77499362030935315,0.75324822078033704,0.73306811511397207,0.71434062913873753,0.69696119928088085,0.68083278874123687,0.66586534569719491]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8127010508272399,1.7596091354816299,1.71020499448661,1.66423247434739,1.6214532140387601,1.58164540913678,1.5446026617942301]
[null,null,null,null,"Coincident",0.69110127434239488,0.67085971805495026,0.65202414404572906,0.63449689252323049,0.61818708716330806,0.60301016392824025,0.58888743261416243]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8486959088659063,1.7945497457969919,1.7441645853223251,1.6972791874996416,1.653650458161849,1.6130521885080424,1.5752738822428844]
[null,null,null,null,"Coincident",0.7048244926573749,0.68418099919186348,0.66497140663599374,0.64709611596491501,0.63046244632064141,0.61498415447486932,0.60058098767004331]
[null,"Casino 132/66kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",33.192290773613799,33.192290774880796,33.192290774882103,33.192290774882103,33.192290774882103,33.192290774882103,33.192290774882103]
[null,null,null,null,"Coincident",27.163165899559566,27.163165900596422,27.163165900597491,27.163165900597491,27.163165900597491,27.163165900597491,27.163165900597491]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",34.022713368975189,34.022713370273884,34.022713370275227,34.022713370275227,34.022713370275227,34.022713370275227,34.022713370275227]
[null,null,null,null,"Coincident",27.842748603820397,27.842748604883191,27.842748604884292,27.842748604884292,27.842748604884292,27.842748604884292,27.842748604884292]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",28.930274192547298,28.9302741934459,28.930274193446799,28.930274193446799,28.930274193446799,28.930274193446799,28.930274193446799]
[null,null,null,null,"Coincident",23.675311920218849,23.675311920954226,23.675311920954961,23.675311920954961,23.675311920954961,23.675311920954961,23.675311920954961]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.654067363176846,29.65406736409793,29.65406736409885,29.65406736409885,29.65406736409885,29.65406736409885,29.65406736409885]
[null,null,null,null,"Coincident",24.267633616388363,24.267633617142138,24.267633617142891,24.267633617142891,24.267633617142891,24.267633617142891,24.267633617142891]
[null,"Casino 66/33kV","Substation Rating","MVA","Non-Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,null,null,"Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.1828743245847999,4.2830627081602497,4.3297169684229502,4.3514422415831895,4.3615589488512798,4.3662699490395598,4.3684636986644003]
[null,null,null,null,"Coincident",2.944836641871869,3.0153714942600494,3.0482171320822338,3.063512208025807,3.0706345951563652,3.0739512441631911,3.0754956927353971]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.285515055544761,4.388161894269925,4.4359609719486341,4.4582193469294005,4.468584301251628,4.4734109014951224,4.4756584820619336]
[null,null,null,null,"Coincident",3.0170980014118567,3.0893636609545156,3.1230152757230076,3.1386856672159174,3.1459828257989577,3.1493808598180939,3.1509632065718089]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7284453510906599,3.8958048723931,4.0060698508833497,4.0787180359811401,4.1265823612661494,4.1581178171334301,4.1788949819808501]
[null,null,null,null,"Coincident",2.6249085282280058,2.7427333569112058,2.8203623564402633,2.8715082960120193,2.9052058465478607,2.9274075095072947,2.9420350960922605]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8199351560630341,3.9914013997450182,4.1043720961491443,4.1788029460469565,4.227841781717153,4.2601510648597003,4.2814380665374259]
[null,null,null,null,"Coincident",2.6893193876355741,2.8100354402960752,2.8895693254700401,2.9419703007459344,2.9764947327393969,2.9992411873272316,3.0142277103905024]
[null,"Coleambally 132","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.347339577451999,12.347339474230699,12.347339435172699,12.347339420393501,12.347339414801199,12.3473394126851,12.3473394118844]
[null,null,null,null,"Coincident",10.612645720172655,10.612645631453049,10.612645597882359,10.612645585179509,10.612645580372877,10.612645578554073,10.612645577865864]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.558330836037317,13.558330722692371,13.558330679803676,13.558330663574978,13.558330657434199,13.558330655110559,13.558330654231328]
[null,null,null,null,"Coincident",11.65350323583224,11.653503138411274,11.653503101548068,11.653503087599359,11.653503082321308,11.65350308032412,11.653503079568413]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.353907296313301,11.353907241709098,11.353907222444201,11.353907215647299,11.3539072132493,11.3539072124033,11.353907212104799]
[null,null,null,null,"Coincident",9.7587820371845488,9.7587819902517623,9.7587819736934147,9.7587819678514176,9.7587819657903179,9.7587819650631733,9.7587819648066088]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.46746559770901,12.467465537749387,12.467465516595045,12.467465509131522,12.467465506498334,12.467465505569361,12.467465505241584]
[null,null,null,null,"Coincident",10.715895079013485,10.715895027477668,10.715895009295327,10.715895002880364,10.715895000617117,10.715894999818657,10.71589499953693]
[null,"Dubbo 132/66kV","Substation Rating","MVA","Non-Coincident",148.5,148.5,148.5,148.5,148.5,148.5,148.5]
[null,null,null,null,"Coincident",148.5,148.5,148.5,148.5,148.5,148.5,148.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",66.524805914284599,66.164612800565692,65.963219853521011,65.850616037472008,65.787656437471796,65.752454155957096,65.732771683008806]
[null,null,null,null,"Coincident",59.884485145919221,59.560245505206034,59.378955040994391,59.277591024115502,59.220915875963044,59.18922738810506,59.171509564765216]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",69.192565356734576,68.817927877984872,68.608458726451687,68.491339303188326,68.425854914651197,68.389240960939688,68.368769186882787]
[null,null,null,null,"Coincident",62.285956273999247,61.948714064526314,61.760153540055491,61.654724651292547,61.595776731960107,61.562817481090661,61.544389142479638]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",60.330177292915302,60.059351709001803,59.894070601019706,59.793201826877301,59.731643009168302,59.6940745141614,59.671146981281197]
[null,null,null,null,"Coincident",54.308187093447636,54.064394564719336,53.915611356413429,53.824811022255354,53.769396834208798,53.73557832169643,53.714939351265365]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",62.74952144470781,62.467835287827391,62.295926122379839,62.191012336441183,62.126984903980855,62.087909847535471,62.064062881047114]
[null,null,null,null,"Coincident",56.486039053024342,56.232470023461879,56.07772035191897,55.983278767771537,55.92564237521983,55.890467682034036,55.869001053295769]
[null,"Goulburn 132/33kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5780081487106106,9.7212682876322898,9.8001549195868893,9.843594083809279,9.8675139919304193,9.8806855622118892,9.8879385275159795]
[null,null,null,null,"Coincident",8.9062523628968471,9.0394649193041943,9.1128188193362387,9.153211367869412,9.1754536477794435,9.1877014269753925,9.1944457039038117]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.678991044617252,9.8237616044397793,9.9034799542650891,9.9473771064669041,9.9715492070642249,9.9848596479010343,9.9921890826995057]
[null,null,null,null,"Coincident",9.0001528003695146,9.1347698439633707,9.2088971291435868,9.2497155445648023,9.2721923293741835,9.2845692394074018,9.2913846226247756]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.6921049741775089,8.7870209317244505,8.8388535304812201,8.8671587634822409,8.8826159513226788,8.8910569578293597,8.8956665020479697]
[null,null,null,null,"Coincident",8.0824822095434694,8.1707412147618825,8.2189385223842102,8.2452585614135803,8.2596316558597547,8.2674806504500822,8.2717669032336953]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.7837476119983116,8.879664287869149,8.9320433682997233,8.9606470291526907,8.9762671852811557,8.9847971870432364,8.9894553306278908]
[null,null,null,null,"Coincident",8.1676974700612313,8.256887007995676,8.3055924696749894,8.3321900062508512,8.346714639167006,8.3546463873102024,8.358977830932238]
[null,"Goulburn 132/66kV","Substation Rating","MVA","Non-Coincident",144,144,144,144,144,144,144]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",6.8810000000000002,6.8810000000000002,6.8810000000000002,6.8810000000000002,6.8810000000000002,6.8810000000000002,6.8810000000000002]
[null,null,null,null,"Coincident",3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",41.310882764583198,42.829619267210504,44.346837033335198,45.862537581693701,47.3767224295039,48.8893930924663,50.400551084765702]
[null,null,null,null,"Coincident",36.029392162444481,37.353962091303295,38.677207450233254,39.999129563804232,41.319729755261683,42.639009346527693,43.956969658202404]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",41.970259707351232,43.513237275890376,45.054671866861,46.594565023240584,48.132918286463848,49.669733196423898,51.205011291473951]
[null,null,null,null,"Coincident",36.604469451139714,37.950181287692693,39.294547412409131,40.637569171000791,41.979247907833916,43.319584965930211,44.658581686968375]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",39.618550629116299,41.010469783492901,42.400997018715096,43.790133726702102,45.177881297981095,46.564241121688802,47.949214585572804]
[null,null,null,null,"Coincident",34.553420357985289,35.767386211904238,36.980138099969238,38.191677236146198,39.402004833186965,40.611122102630681,41.819030254804957]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",40.250915687485943,41.665051733276449,43.077773643021125,44.489082830856098,45.898980709503206,47.307468690271662,48.71454818305935]
[null,null,null,null,"Coincident",35.104939162549783,36.338281535192465,37.570390565462475,38.801267486702244,40.030913531020744,41.259329929294928,42.486517911170836]
[null,"Hawks Nest 132/33kV","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.964067303356799,13.7216877625885,14.2933738788804,14.724757445121901,15.050271352002001,15.295898009724601,15.481243255223301]
[null,null,null,null,"Coincident",11.177499724448973,11.830713123927895,12.323615641154833,12.695550588727009,12.976205688651902,13.187982736299656,13.347785704150125]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.014966664579244,13.775561683917861,14.349492347191669,14.782569606272752,15.109361541841034,15.355952575919043,15.542025521635642]
[null,null,null,null,"Coincident",11.221384686068324,11.877162723943314,12.372000468956776,12.745395702934811,13.027152707453048,13.239761231534439,13.400191615827197]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.7630094954682,11.477944452273199,12.0574430663609,12.5271622212758,12.907898394116101,13.216508404570702,13.466655738464301]
[null,null,null,null,"Coincident",9.2797679042199324,9.8961782556701792,10.395816636721058,10.800804176647686,11.12907140694109,11.395152122668732,11.610826855778408]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.805267090660458,11.523009016278984,12.104782850681122,12.576346211151245,12.958577225659548,13.268398896932581,13.519528356204638]
[null,null,null,null,"Coincident",9.3162020145623732,9.9350325087352367,10.43663256383814,10.84321016085125,11.172766229897279,11.439891628450706,11.656413141038628]
[null,"Hay 132","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.011871077801299,14.374513246871601,14.7367927737728,15.098710021147001,15.4602653512739,15.8214591260707,16.182291707092698]
[null,null,null,null,"Coincident",9.5591408780754836,9.8065416401311563,10.053695001424751,10.300601209356987,10.547260511081339,10.793673153503986,11.039839383284207]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.389529357595439,14.761945725771019,15.13398967757839,15.505661585433852,15.876961821381535,16.247890757093298,16.618448763869345]
[null,null,null,null,"Coincident",9.8167858906707828,10.070854780466066,10.324669601371529,10.578230607456019,10.831538052534475,11.084592190167871,11.337393273663633]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.656522580672299,12.8659426187794,13.062449318968099,13.2468389483848,13.4198586744493,13.5822095924596,13.7345495665098]
[null,null,null,null,"Coincident",8.6344986835387481,8.7773686568522518,8.9114289276154821,9.0372227230524693,9.1552597737042447,9.2660183789132269,9.3699473449465582]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.997650508516639,13.212714989889511,13.414518083539813,13.603877518193141,13.781560599476451,13.948287319125114,14.104733272471316]
[null,null,null,null,"Coincident",8.8672220579977221,9.0139427681654407,9.1516163301846394,9.2808006127399949,9.402019085005886,9.5157629378012452,9.6224930739506149]
[null,"Herons Creek","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.071874428390398,17.791369226015,19.509144528841901,21.225202056366001,22.939543526362598,24.652170654889201,26.363085156287301]
[null,null,null,null,"Coincident",12.769434477351274,14.135608426148904,15.500416200997673,16.863859168071617,18.225938692178502,19.586656136761281,20.946012863899497]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.760494314477445,18.553663052061154,20.345038620907197,22.134622814184421,23.922417423268392,25.70842423774328,27.492645045403719]
[null,null,null,null,"Coincident",13.316557126571119,14.74126653451434,16.164551233049554,17.586412646886252,19.006852199309133,20.425871312179591,21.843471405937201]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.721608731230999,12.5924480945773,13.462416618560301,14.331515174019399,15.199744630922901,16.067105858369601,16.933599724588799]
[null,null,null,null,"Coincident",9.3130589919369573,10.004958760075114,10.69616662844517,11.386683288946919,12.076509432788058,12.765645750485435,13.454092931865071]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.223835954646757,13.131987537290163,14.039230968350974,14.945567155980809,15.850997007422869,16.755521429013594,17.659141326182674]
[null,null,null,null,"Coincident",9.7120888406782448,10.43363393373739,11.154457481703513,11.874560206121739,12.593942827815429,13.312606066887513,14.030550642720479]
[null,"Hillston","Substation Rating","MVA","Non-Coincident",50.6,50.6,50.6,50.6,50.6,50.6,50.6]
[null,null,null,null,"Coincident",50.6,50.6,50.6,50.6,50.6,50.6,50.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.400618824693,11.5993223502955,11.7619606713649,11.895079715931901,12.0040373091357,12.093218816976,12.166213650165901]
[null,null,null,null,"Coincident",9.5790171698495659,9.7459716582614924,9.8826234746194732,9.9944726323844346,10.086020878329126,10.160952880527551,10.222284530255363]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.434590226522237,11.633885846064279,11.79700879448969,11.930524505292414,12.0398067687828,12.129254018411784,12.202466360567458]
[null,null,null,null,"Coincident",9.607560588975316,9.7750125659973133,9.9120715754941564,10.024254019788657,10.116075059894577,10.191230343407437,10.252744748312821]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.596211197450701,10.754488077761,10.883655522729699,10.9890671836559,11.0750920969916,11.1452957694259,11.202587958771401]
[null,null,null,null,"Coincident",8.9031385538377368,9.036125804564751,9.1446547530513769,9.2332236391303866,9.3055034104786483,9.3644898737553692,9.4126278629187432]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.62778563687292,10.786534148380083,10.916086484664225,11.021812249758442,11.108093498907417,11.178506363246369,11.235969271042848]
[null,null,null,null,"Coincident",8.9296679994761359,9.0630515237214624,9.1719038652252447,9.2607366676113259,9.3332318171942568,9.3923940474953174,9.4406754775541621]
[null,"Jindabyne 33kV","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.81760094535674899,0.82208296970709105,0.82578363012505995,0.82883914398635294,0.83136198150779106,0.83344500565643098,0.83516489033665509]
[null,null,null,null,"Coincident",0.10714109080374698,0.10772842987255772,0.10821337646676993,0.10861378095495464,0.10894438180063927,0.1092173480694814,0.10944272735963799]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.81760094535674899,0.82208296970709105,0.82578363012505995,0.82883914398635294,0.83136198150779106,0.83344500565643098,0.83516489033665509]
[null,null,null,null,"Coincident",0.10714109080374698,0.10772842987255772,0.10821337646676993,0.10861378095495464,0.10894438180063927,0.1092173480694814,0.10944272735963799]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.75758482237351299,0.76234717176302402,0.76615150939829502,0.76919055245444201,0.77161825040940002,0.77355758369676009,0.77510679355286405]
[null,null,null,null,"Coincident",9.9276382575663902E-2,9.9900456350625264E-2,0.10039898914506917,0.10079723524530218,0.10111536869232594,0.10136950524270519,0.1015725187480216]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.75758482237351299,0.76234717176302402,0.76615150939829502,0.76919055245444201,0.77161825040940002,0.77355758369676009,0.77510679355286405]
[null,null,null,null,"Coincident",9.9276382575663902E-2,9.9900456350625264E-2,0.10039898914506917,0.10079723524530218,0.10111536869232594,0.10136950524270519,0.1015725187480216]
[null,"Junee 66kV","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.2655216810001,10.837044525630398,10.408995847416,9.9813752178798403,9.5541822089732307,9.1274163930755208,8.7010773429937114]
[null,null,null,null,"Coincident",7.660554743080068,7.3691902774286699,7.0781171762428787,6.7873351481582906,6.4968439021017961,6.2066431472913539,5.9167325932357233]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.442551307415817,11.007340939604591,10.572565782161108,10.138225399875095,9.7043193579713822,9.2708472221095661,8.8378085583836139]
[null,null,null,null,"Coincident",7.7809348890427552,7.484991838931121,7.1893447318695527,6.8939932719150638,6.5989371634205396,6.3041761110345043,6.0097098197008565]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.3593094542105,10.0274086948475,9.6958398362439695,9.3646025464990004,9.0336964940437703,8.7031213476409999,8.3728767763846292]
[null,null,null,null,"Coincident",7.0443304288631392,6.8186379124962997,6.5931710886458985,6.36792973161932,6.1429136159497633,5.9181225163958793,5.6935562079415476]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.522098602776666,10.184982260052248,9.8482030336706607,9.5117605865154147,9.1756545818073167,8.8398846831039304,8.504450554299245]
[null,null,null,null,"Coincident",7.1550270498881323,6.925787936835528,6.6967780628960485,6.4679971988304814,6.2394451156289747,6.011121584510672,5.7830263769234858]
[null,"Lismore 132/66kV","Substation Rating","MVA","Non-Coincident",396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006]
[null,null,null,null,"Coincident",396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006,396.00000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",26.795999999999999,26.795999999999999,26.795999999999999,26.795999999999999,26.795999999999999,26.795999999999999,26.795999999999999]
[null,null,null,null,"Coincident",27.012,27.012,27.012,27.012,27.012,27.012,27.012]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",87.802192404144293,87.047098714054499,86.396955111996306,85.837174638599791,85.3551977685607,84.940210618610308,84.5829023216167]
[null,null,null,null,"Coincident",48.730861316507436,48.311778775568527,47.950944303897444,47.640262031964937,47.372761331031064,47.142440416499888,46.944131688764621]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",99.169204677409397,98.316355350385066,97.582043117662579,96.949792568779287,96.405418202195392,95.936706152016754,95.533140151359319]
[null,null,null,null,"Coincident",55.0396365703401,54.566298933304765,54.158750253755784,53.807846557944849,53.505714788385419,53.245576159847566,53.021594067013552]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",75.724351293560503,74.493981921227402,73.403331714230504,72.436534343643402,71.579525240470304,70.819836990102402,70.146417961517599]
[null,null,null,null,"Coincident",42.027570839960177,41.34470680650567,40.73938793545345,40.202808297778937,39.727161954445243,39.305529398824554,38.931776894572572]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",85.527746937452335,84.138091978130859,82.906244450778814,81.814283946147853,80.84632507364293,79.988286367217626,79.227685434020017]
[null,null,null,null,"Coincident",47.468527386402826,46.69725868289725,46.013574262556489,45.407528166698825,44.870303886933648,44.394086106236941,43.97194700494601]
[null,"Maclean 66/33kV","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.47075769025154801,0.46462136378182201,0.459794996746276,0.45599894403025304,0.45301325808538101,0.45066494492213599,0.44881794064422798]
[null,null,null,null,"Coincident",0.24300686325485002,0.23983926880404238,0.23734788026486006,0.23538834379339452,0.23384712165055549,0.23263491369823225,0.23168148324921953]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.49582117838994061,0.48935814935353938,0.48427482296193419,0.48027666558741927,0.47713201951122303,0.4746586804156756,0.47271334026186046]
[null,null,null,null,"Coincident",0.25594472865962214,0.25260848913388723,0.24998445722340584,0.24792059357869098,0.24629731562732116,0.2450205688256844,0.24401637703332149]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.41923302423871101,0.41385518312049496,0.409463046522064,0.40587594465809501,0.40294632270893099,0.40055367117839197,0.39859956875632996]
[null,null,null,null,"Coincident",0.21640963982692721,0.21363357832377403,0.21136634114449138,0.20951466587674814,0.20800238417613801,0.20676728859440141,0.20575857368671663]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.44155330099216089,0.43588913962922499,0.43126316242485907,0.42748508060053986,0.42439948340871203,0.42187944533835264,0.41982130505585674]
[null,null,null,null,"Coincident",0.22793144935474974,0.22500758828082679,0.22261964171468421,0.22066938188407498,0.2190765851855157,0.21777573220012186,0.21671331256355569]
[null,"Marulan South 33kV","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.074374715283561,7.9827254866985005,7.9094660592682402,7.8509064424523807,7.8040970577505409,7.7666801719287797,7.7367711407907596]
[null,null,null,null,"Coincident",4.1450511420062552,4.0980022059578172,4.0603938357693821,4.0303317424039884,4.0063017338452198,3.9870934470397739,3.971739383344874]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.8886870214197629,8.7877948362818632,8.707147090201488,8.6426816517836755,8.5911514732929106,8.5499610407066822,8.5170356407501338]
[null,null,null,null,"Coincident",4.5630855129044194,4.5112916239691243,4.4698903955423663,4.4367964968126117,4.4103430273202147,4.3891975571566739,4.3722950140492092]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5116356747932995,7.4308886563942096,7.3653056194245003,7.3120388261304994,7.2687753330242701,7.2336365585645002,7.2050967116431499]
[null,null,null,null,"Coincident",3.8561641154950332,3.8147119247519887,3.7810442969946383,3.7536993210479084,3.7314896270678024,3.713450828728722,3.6987996477710059]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.26919493911846,8.1803044677481171,8.1081072871497835,8.0494684611204654,8.0018417824939814,7.9631592120779784,7.9317410805361099]
[null,null,null,null,"Coincident",4.2450638141657739,4.1994311103516093,4.162368053899411,4.1322652977889405,4.1078157242192379,4.0879576871163659,4.0718289134813235]
[null,"Moruya North","Substation Rating","MVA","Non-Coincident",82.5,82.5,82.5,82.5,82.5,82.5,82.5]
[null,null,null,null,"Coincident",82.5,82.5,82.5,82.5,82.5,82.5,82.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.0988743308659,23.098874330894599,23.098874330894702,23.098874330894702,23.098874330894702,23.098874330894702,23.098874330894702]
[null,null,null,null,"Coincident",18.296681672392225,18.296681672414959,18.296681672415041,18.296681672415041,18.296681672415041,18.296681672415041,18.296681672415041]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.100645377393089,23.100645377421792,23.100645377421895,23.100645377421895,23.100645377421895,23.100645377421895,23.100645377421895]
[null,null,null,null,"Coincident",18.29808452320092,18.298084523223654,18.298084523223736,18.298084523223736,18.298084523223736,18.298084523223736,18.298084523223736]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.101680706593402,21.101680706593402,21.101680706593402,21.101680706593402,21.101680706593402,21.101680706593402,21.101680706593402]
[null,null,null,null,"Coincident",16.714699128220541,16.714699128220541,16.714699128220541,16.714699128220541,16.714699128220541,16.714699128220541,16.714699128220541]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.103298623458006,21.103298623458006,21.103298623458006,21.103298623458006,21.103298623458006,21.103298623458006,21.103298623458006]
[null,null,null,null,"Coincident",16.715980684603768,16.715980684603768,16.715980684603768,16.715980684603768,16.715980684603768,16.715980684603768,16.715980684603768]
[null,"Morven","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1902172526676296,8.1902172546148098,8.1902172549485002,8.1902172550056811,8.1902172550154795,8.1902172550171599,8.1902172550174406]
[null,null,null,null,"Coincident",6.4191357904260009,6.4191357919521153,6.4191357922136474,6.4191357922584631,6.4191357922661432,6.4191357922674603,6.4191357922676797]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3722910478513484,8.3722910498418148,8.3722910501829251,8.3722910502413761,8.372291050251393,8.3722910502531107,8.3722910502533967]
[null,null,null,null,"Coincident",6.561837306039866,6.561837307599907,6.5618373078672549,6.5618373079130663,6.5618373079209169,6.5618373079222634,6.5618373079224872]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3605270109390704,7.3605270141285803,7.3605270147178601,7.3605270148267401,7.3605270148468502,7.3605270148505699,7.3605270148512503]
[null,null,null,null,"Coincident",5.7688606925447692,5.7688606950445678,5.7688606955064197,5.768860695591755,5.7688606956075166,5.7688606956104325,5.7688606956109654]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.5241562586244655,7.5241562618848805,7.5241562624872609,7.5241562625985612,7.5241562626191181,7.5241562626229204,7.5241562626236158]
[null,null,null,null,"Coincident",5.8971061746576749,5.897106177213046,5.8971061776851661,5.8971061777723985,5.8971061777885101,5.8971061777914899,5.8971061777920353]
[null,"Nyngan 132","Substation Rating","MVA","Non-Coincident",82.5,82.5,82.5,82.5,82.5,82.5,82.5]
[null,null,null,null,"Coincident",82.5,82.5,82.5,82.5,82.5,82.5,82.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",36.2622498177778,37.403035514794205,38.376410271479202,39.206941737143197,39.915592244792599,40.5202478933181,41.036169986574507]
[null,null,null,null,"Coincident",32.185273950919417,33.197800762197495,34.06173869650231,34.798893254798614,35.427869968564792,35.964543997108471,36.422460811212169]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.411176321659063,37.556647145119307,38.534019483316975,39.367961883166416,40.079522768498073,40.686661695149979,41.204702644076129]
[null,null,null,null,"Coincident",32.317456602300886,33.334141789820023,34.201627856322176,34.941809856427497,35.573369733220645,36.112247844169481,36.572045290350225]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",34.274508504770999,35.499766839569205,36.568546741921097,37.500832160619595,38.314054883095203,39.023420473381798,39.642192584361297]
[null,null,null,null,"Coincident",30.42101500327631,31.508517167766779,32.457133817955103,33.284602101143321,34.006393943555651,34.636005342998843,35.185208715793991]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",34.41527149519532,35.645561879606269,36.71873118567899,37.654845434875433,38.471408005748302,39.183686910511135,39.805000274933278]
[null,null,null,null,"Coincident",30.545951967522146,31.637920426744323,32.590432978647129,33.421299615746292,34.14605580637641,34.778252975455906,35.329711887789863]
[null,"Oura 11/33kV","Substation Rating","MVA","Non-Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,null,null,"Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6484556799625401,1.6486170086599901,1.64871203625318,1.6487680104450801,1.6488009809755599,1.64882040163789,1.6488318410087499]
[null,null,null,null,"Coincident",1.2433267416666616,1.2434484217859247,1.2435200951401102,1.2435623129628146,1.2435871805663121,1.2436018283540018,1.2436104563540571]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.800129568191539,1.8003057406916601,1.8004095117437875,1.8004706361034655,1.8005066402420764,1.8005278477934346,1.8005403396972064]
[null,null,null,null,"Coincident",1.3577248438054828,1.3578577196742181,1.3579359876711616,1.3579820899424442,1.3580092456063118,1.3580252411323361,1.3580346629919606]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5158703118571499,1.5160358758006001,1.51613477565183,1.5161938536151198,1.5162291439184201,1.51625022463004,1.51626281722236]
[null,null,null,null,"Coincident",1.1433259131803928,1.1434507876801137,1.1435253816357023,1.1435699404385227,1.1435965577011813,1.1436124575599453,1.1436219553626275]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6553450621006651,1.6555258595304374,1.6556338591258484,1.6556983728339445,1.6557369101869432,1.6557599305282036,1.6557736817609792]
[null,null,null,null,"Coincident",1.2485229705674508,1.2486593347305841,1.2487407920525466,1.2487894506967887,1.2488185170054062,1.2488358798051704,1.2488462514976877]
[null,"Pinnacles Place","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.85934566726218,5.6309004115918597,5.5204814212147699,5.4671104137927893,5.4413135429510202,5.4288446281343008,5.4228177794649399]
[null,null,null,null,"Coincident",4.1238796485129718,3.9630970638769689,3.8853828184502781,3.8478196460711716,3.8296634906400144,3.8208877148159304,3.8166459444914533]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9882169062782102,5.7547471948380151,5.6418996342913408,5.5873547777325134,5.5609905270335203,5.5482473692222989,5.5420879652302979]
[null,null,null,null,"Coincident",4.2145808138028462,4.0502619553112131,3.9708384522871607,3.9324491104275756,3.913893626064648,3.9049248346432606,3.9005897702500634]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.3459034198968798,5.1285393407716899,5.0206581977018896,4.9671151234419302,4.9405408703368101,4.9273516588868498,4.9208056499366304]
[null,null,null,null,"Coincident",3.7625126708951648,3.6095291547953243,3.5336010775614475,3.4959168024224732,3.4772135157795732,3.4679307863133255,3.4633236245888308]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4634819408623532,5.2413371268590438,5.1310832313756851,5.0763625235176324,5.0492037927049216,5.0357244959591414,5.0290345132050316]
[null,null,null,null,"Coincident",3.8452658821318617,3.6889176259418495,3.6113195763347932,3.5728064681649028,3.5536918189125548,3.5442049238422113,3.539496431581254]
[null,"Quirindi 66/33kV","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6408249238817501,5.6408264346817791,5.6408274558691698,5.6408281461151804,5.6408286126696598,5.6408289280254706,5.6408291411823104]
[null,null,null,null,"Coincident",4.7424713248931747,4.7424725950843101,4.7424734536381532,4.7424740339560953,4.7424744262074547,4.7424746913399325,4.7424748705495716]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.8110942688063281,5.8110958252101357,5.8110968772222575,5.811097588303471,5.8110980689409839,5.8110983938158682,5.8110986134068874]
[null,null,null,null,"Coincident",4.8856237000705054,4.8856250086025952,4.8856258930720458,4.8856264909069917,4.8856268949985306,4.8856271681340813,4.8856273527531977]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.9328028777473705,4.93280286692739,4.9328028610900798,4.9328028579408905,4.93280285624191,4.9328028553253294,4.9328028548308405]
[null,null,null,null,"Coincident",4.1472083453653816,4.1472083362685828,4.1472083313609183,4.1472083287132673,4.147208327284865,4.1472083265142583,4.1472083260985215]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0817004460941888,5.0817004349476056,5.081700428934095,5.0817004256898466,5.0817004239395818,5.0817004229953344,5.0817004224859188]
[null,null,null,null,"Coincident",4.2723925972717804,4.2723925879003941,4.2723925828445903,4.2723925801170193,4.2723925786454995,4.2723925778516323,4.2723925774233464]
[null,"Snowy Adit 66kV","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.0746988265624,13.381196034776799,13.665908267493199,13.930383940634199,14.176061412993,14.404276808790101,14.616271284225]
[null,null,null,null,"Coincident",5.129640172954649,5.249889244310765,5.3615913436131653,5.4653539660421515,5.5617414276975881,5.6512779346486504,5.7344504338442759]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.563910474322944,13.881875786411364,14.177241001835236,14.451612473079596,14.706482377529156,14.943236832718997,15.163163434776418]
[null,null,null,null,"Coincident",5.3215742094260357,5.446322600202059,5.5622042197200248,5.6698492936048952,5.7698432527839394,5.8627299173700864,5.9490144542439483]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.6431183868603,11.88732670936,12.113582341819999,12.323205055312799,12.517417599479201,12.697352834946399,12.864060341413701]
[null,null,null,null,"Coincident",4.5679834471115246,4.6637945123055733,4.7525621387740467,4.8348041167010551,4.9110001715290066,4.9815947622439705,5.0469996739479761]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.078765066501989,12.332110850401886,12.566832214443098,12.784298311132419,12.985777641326381,13.172445453520643,13.345390599188264]
[null,null,null,null,"Coincident",4.7389021610909472,4.8382981569743402,4.9303871721331758,5.0157063707342866,5.094753427947051,5.1679894329312663,5.2358415784148624]
[null,"Steeple Flat 132/66kV","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.33,4.33,4.33,4.33,4.33,4.33,4.33]
[null,null,null,null,"Coincident",5.3999999999999999E-2,5.3999999999999999E-2,5.3999999999999999E-2,5.3999999999999999E-2,5.3999999999999999E-2,5.3999999999999999E-2,5.3999999999999999E-2]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0682751617884794,6.1148073836502901,6.1612930732902393,6.2077322772405594,6.2541250419869199,6.3004714139685305,6.3467714395781707]
[null,null,null,null,"Coincident",4.524388170886315,4.5590816922813771,4.5937405201550447,4.628364689200847,4.6629542340775956,4.697509189409466,4.7320295897860118]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0693268559239719,6.1158671422956372,6.162360888380932,6.2088081407201514,6.2552089458070226,6.3015633500888031,6.347871399966313]
[null,null,null,null,"Coincident",4.5251722936195709,4.559871827756643,4.5945366623595785,4.6291668321279182,4.6637623717264836,4.6983233157854469,4.7328496989003597]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7956188889808296,5.8091610622083198,5.82268969326259,5.8362047956857994,5.8497063830065796,5.8631944687400503,5.8766690663877794]
[null,null,null,null,"Coincident",4.3211009463423791,4.3311977278371216,4.3412844125503742,4.3513610105789091,4.3614275320094116,4.3714839869184914,4.3815303853726562]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7966233289962519,5.8101678492208348,5.8236988249252013,5.8372162696538563,5.8507201969377771,5.8642106202944255,5.8776875532277089]
[null,null,null,null,"Coincident",4.3218498373209489,4.3319483686911662,4.3420368015300204,4.352115145936029,4.3621834119976288,4.3722416097931749,4.3822897493909192]
[null,"Stroud 132/33kV","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",54.498596903699898,56.563245651471398,57.450939011069998,57.832601752263102,57.996697209821704,58.067249863473997,58.097583895941597]
[null,null,null,null,"Coincident",52.412526208821426,54.39814533945335,55.251860005861573,55.618913646913313,55.776727938632348,55.844580012240534,55.873752933417514]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",54.501313141583857,56.566064792502672,57.45380239519136,57.835484158650274,57.999587794810232,58.070143964842792,58.10047950917405]
[null,null,null,null,"Coincident",52.415138475877292,54.400856570780078,55.254613786762981,55.621685721955522,55.779507879219402,55.847363334609568,55.876537709779825]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",44.856581331499399,46.7498123512513,47.7519768191422,48.282463384291795,48.563271579773499,48.711914821336897,48.790597757298102]
[null,null,null,null,"Coincident",43.139583003020952,44.96034584976799,45.924149955251586,46.43433081455813,46.704390370978338,46.847343919084764,46.923015068023531]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",44.858817006406269,46.75214238575844,47.75435680203789,48.284869806908638,48.565691998014117,48.714342648032542,48.793029505591427]
[null,null,null,null,"Coincident",43.141733101854832,44.962586696351416,45.92643883832352,46.436645125304473,46.706718141630795,46.849678814615025,46.925353735042471]
[null,"Temora 132/66kV","Substation Rating","MVA","Non-Coincident",132,132,132,132,132,132,132]
[null,null,null,null,"Coincident",132,132,132,132,132,132,132]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.894570568554002,20.7217759319904,20.555913126548102,20.396704074830502,20.243881854796001,20.097190252250197,19.956383331289299]
[null,null,null,null,"Coincident",15.690392372424645,15.560635427258529,15.436083812816763,15.31652871200745,15.20176968464677,15.091614331411257,14.985877971270193]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.024060356741153,20.85019486108451,20.683304155141727,20.523108438188931,20.369339133990263,20.221738440516738,20.080058897727564]
[null,null,null,null,"Coincident",15.787630340451434,15.657069253401174,15.531745756037981,15.411449737169134,15.295979514424143,15.185141496124452,15.078749856716776]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.153936933795602,18.980952013765101,18.813562672536701,18.651587908771798,18.494852576018999,18.3431871933252,18.1964277619726]
[null,null,null,null,"Coincident",14.383295650030076,14.253395815004229,14.127697876670528,14.006065915412279,13.888368408232347,13.774478086535042,13.664271798508155]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.272639504320789,19.098582545954738,18.930155843835415,18.76717727490578,18.609470607280457,18.456865309683124,18.309196367047775]
[null,null,null,null,"Coincident",14.47243315592161,14.341728293481209,14.215251368120375,14.09286561788865,13.974438704702267,13.859842571244691,13.748953302495769]
[null,"Terranora 110/66kV","Substation Rating","MVA","Non-Coincident",330,330,330,330,330,330,330]
[null,null,null,null,"Coincident",330,330,330,330,330,330,330]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",24.073,24.073,24.073,24.073,24.073,24.073,24.073]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",94.186394895563396,94.186394895543103,94.186394895543103,94.186394895543103,94.186394895543103,94.186394895543103,94.186394895543103]
[null,null,null,null,"Coincident",58.501544249371292,58.501544249358687,58.501544249358687,58.501544249358687,58.501544249358687,58.501544249358687,58.501544249358687]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",94.791497586308807,94.791497586288386,94.791497586288386,94.791497586288386,94.791497586288386,94.791497586288386,94.791497586288386]
[null,null,null,null,"Coincident",58.87738878485127,58.87738878483858,58.87738878483858,58.87738878483858,58.87738878483858,58.87738878483858,58.87738878483858]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",82.167404038321095,81.691278142258,81.241698693805603,80.817185593085597,80.416341263338708,80.037846049839501,79.680453875345492]
[null,null,null,null,"Coincident",51.03624603674303,50.74051223986406,50.461267110815335,50.197591322250048,49.948616804010982,49.713523885280509,49.491538596070491]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",82.695290441981456,82.21610566399427,81.763637881889608,81.336397486852974,80.93297792336061,80.552051058534516,80.192362809679892]
[null,null,null,null,"Coincident",51.364129589740479,51.066495844185965,50.785456698292748,50.520086918474028,50.269512857635625,50.032909578965622,49.809498140087641]
[null,"Yanco 33/66kV","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.5451897360067,10.5696675270115,10.590564054705899,10.608403281685099,10.6236325113383,10.636633603599899,10.6477325497608]
[null,null,null,null,"Coincident",9.5389693413495724,9.5611114652737612,9.5800140494858699,9.5961510601502624,9.6099271190350279,9.6216876490579235,9.6317275354706471]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.56209423863694,10.586611268848696,10.607541294793597,10.625409119006886,10.640662761928995,10.653684695636205,10.664801434000875]
[null,null,null,null,"Coincident",9.5542608189196745,9.5764384378516834,9.5953713239163463,9.6115342030711144,9.625332345714396,9.6371117284953449,9.6471677093824706]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.7976804664411699,9.8062089989376506,9.8135128699629206,9.8197679357641992,9.8251248003696805,9.8297124417012203,9.8336413169924501]
[null,null,null,null,"Coincident",8.862787292162432,8.8705020333901654,8.8771089701572983,8.8827671785347917,8.8876128919374597,8.8917627812335471,8.8953167638443151]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.8133866717690541,9.8219288759588483,9.829244455479655,9.8355095484856534,9.8408750004313426,9.8454699959970782,9.8494051694853404]
[null,null,null,null,"Coincident",8.8769948137758234,8.8847219221459817,8.8913394501857947,8.897006728973663,8.9018602103138473,8.9060167521042271,8.9095764319390298]
[null,"<Enter substation name>"]
[]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,null,"FORECASTING ELEMENTS","UNIT","MAX DEMAND","2017-18","2018-19","2019-20","2020-21","2021-22","2022-23","2023-24"]
[null,"Adaminaby 11kV","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.64585650609565,1.64585650609565,1.64585650609565,1.64585650609565,1.64585650609565,1.64585650609565,1.64585650609565]
[null,null,null,null,"Coincident",0.43189142358538335,0.43189142358538335,0.43189142358538335,0.43189142358538335,0.43189142358538335,0.43189142358538335,0.43189142358538335]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6598637955092301,1.6598637955092301,1.6598637955092301,1.6598637955092301,1.6598637955092301,1.6598637955092301,1.6598637955092301]
[null,null,null,null,"Coincident",0.43556709527547172,0.43556709527547172,0.43556709527547172,0.43556709527547172,0.43556709527547172,0.43556709527547172,0.43556709527547172]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5147814931482,1.5145636142635999,1.51438897450645,1.5142489928609901,1.5141367912558901,1.5140468566066299,1.5139747699272099]
[null,null,null,null,"Coincident",0.397495852811939,0.39743867892023543,0.39739285146623154,0.39735611869401866,0.39732667571963071,0.39730307584712982,0.39728415948444512]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5276732505366952,1.5274535173637156,1.5272773913107602,1.5271362183321475,1.52702306181977,1.5269323617692394,1.5268596615861649]
[null,null,null,null,"Coincident",0.40087879624012568,0.40082113576210976,0.40077491828722078,0.40073787289566992,0.40070817934277653,0.40068437862029688,0.4006653012672915]
[null,"Adelong","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.74695384576889,1.74695384572228,1.74695384572224,1.74695384572224,1.74695384572224,1.74695384572224,1.74695384572224]
[null,null,null,null,"Coincident",1.5981197114767973,1.5981197114341581,1.5981197114341217,1.5981197114341217,1.5981197114341217,1.5981197114341217,1.5981197114341217]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7775651216161998,1.7775651215687731,1.7775651215687325,1.7775651215687325,1.7775651215687325,1.7775651215687325,1.7775651215687325]
[null,null,null,null,"Coincident",1.6261230175993513,1.6261230175559651,1.626123017555928,1.626123017555928,1.626123017555928,1.626123017555928,1.626123017555928]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.54491813328494,1.54491813323355,1.54491813323349,1.54491813323349,1.54491813323349,1.54491813323349,1.54491813323349]
[null,null,null,null,"Coincident",1.4132967092407245,1.4132967091937128,1.4132967091936579,1.4132967091936579,1.4132967091936579,1.4132967091936579,1.4132967091936579]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5719892063153105,1.5719892062630201,1.571989206262959,1.571989206262959,1.571989206262959,1.571989206262959,1.571989206262959]
[null,null,null,null,"Coincident",1.4380614249917705,1.438061424943935,1.438061424943879,1.438061424943879,1.438061424943879,1.438061424943879,1.438061424943879]
[null,"Alstonville","Substation Rating","MVA","Non-Coincident",44,44,44,44,44,44,44]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.8022464885956,11.802736700506902,11.802967582240001,11.803076323732101,11.8031275391831,11.803151660816701,11.803163021708601]
[null,null,null,null,"Coincident",7.9580862037387483,7.9584167466275115,7.9585724268818305,7.9586457497165037,7.9586802835634627,7.9586965484364045,7.9587042089235149]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.922142325940063,11.922637517781894,11.922870744980218,11.922980591147795,11.923032326882739,11.923056693561506,11.923068169865642]
[null,null,null,null,"Coincident",8.0389302540624445,8.0392641548472206,8.0394214166152338,8.0394954843168005,8.0395303689837903,8.0395467990871872,8.0395545373951194]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.8092429832815,11.121405002703598,11.317365577164201,11.440380371898,11.517603250862699,11.566080127554599,11.596511621501801]
[null,null,null,null,"Coincident",7.2885181258698122,7.4990045161087133,7.63113793203072,7.714085050765509,7.7661553348674213,7.798842600293959,7.8193621219269298]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.919051165968805,11.234384355112017,11.432335640170315,11.556600109009345,11.634607474363527,11.683576814564679,11.714317453847217]
[null,null,null,null,"Coincident",7.3625602147675382,7.5751848794469607,7.7086606030862708,7.7924503592177308,7.8450496112851225,7.878068937820756,7.8987969117369818]
[null,"Anona","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5289387664290299,1.5258375272354898,1.52313486905357,1.5207795649985001,1.5187269720258001,1.51693818475542,1.5153792980490701]
[null,null,null,null,"Coincident",1.459205003766848,1.4562452097918015,1.453665817844183,1.451417937459426,1.449458961729184,1.4477517597189233,1.446263972678554]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5289387664290299,1.5258375272354898,1.52313486905357,1.5207795649985001,1.5187269720258001,1.51693818475542,1.5153792980490701]
[null,null,null,null,"Coincident",1.459205003766848,1.4562452097918015,1.453665817844183,1.451417937459426,1.449458961729184,1.4477517597189233,1.446263972678554]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4327387674937699,1.43047774857414,1.4285193737044102,1.4268231330860301,1.42535393927646,1.4240814013908001,1.4229791964537202]
[null,null,null,null,"Coincident",1.3673926154024949,1.3652347198781103,1.3633656650330719,1.3617467886906833,1.3603446037206239,1.3591301053437042,1.3580781711559669]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4327387674937699,1.43047774857414,1.4285193737044102,1.4268231330860301,1.42535393927646,1.4240814013908001,1.4229791964537202]
[null,null,null,null,"Coincident",1.3673926154024949,1.3652347198781103,1.3633656650330719,1.3617467886906833,1.3603446037206239,1.3591301053437042,1.3580781711559669]
[null,"Ardlethan","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.84077539355220798,0.84170809055924889,0.84251822005065402,0.84322188886044902,0.84383308719248207,0.8443639667708881,0.84482508243825305]
[null,null,null,null,"Coincident",0.70856501225652924,0.70935104437794205,0.7100337824996914,0.71062680068583306,0.71114188920644084,0.71158928894942175,0.71197789502781539]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.85936747842191286,0.86032080017849522,0.86114884408125814,0.86186807313500446,0.86249278690926912,0.86303540583953187,0.86350671816784585]
[null,null,null,null,"Coincident",0.72423352604107161,0.72503693970816685,0.7257347752330997,0.72634090684350516,0.72686738552795915,0.72732467863135009,0.72772187796454835]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.75865201081839095,0.7588138357973,0.75894581643550496,0.75905345673293101,0.759141245622178,0.75921284417085799,0.759271238259416]
[null,null,null,null,"Coincident",0.63935538012459003,0.63949175842376893,0.63960298534982374,0.6396936994088338,0.63976768365701986,0.63982802346585832,0.63987723519159645]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.7754280995097067,0.77559350292795282,0.77572840205692895,0.77583842260663216,0.77592815277352833,0.77600133458249865,0.77606101994082821]
[null,null,null,null,"Coincident",0.65349345978336471,0.65363285381888914,0.65374654030841939,0.6538392603294223,0.65391488059292446,0.6539765546972901,0.65402685464300769]
[null,"Ariah Park","Substation Rating","MVA","Non-Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,null,null,"Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.98234117344834704,0.98029036611759901,0.97841071082598896,0.97668792392041093,0.97510891380335496,0.97366168144879306,0.972335229220612]
[null,null,null,null,"Coincident",0.78301175087484742,0.78137707823548419,0.77987882872634651,0.77850561702782262,0.77724700799277124,0.77609343734898928,0.77503613901953627]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.99760084216210776,0.99551817763010542,0.99360932380969369,0.99185977516577661,0.99025623673622265,0.98878652310236659,0.98743946579102926]
[null,null,null,null,"Coincident",0.79517504020882557,0.79351497459642373,0.79199345130850329,0.790598908166119,0.78932074792275597,0.78814925773499311,0.78707553535382035]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.90406154803868799,0.90167914396038895,0.89949770412752006,0.89750027649222897,0.89567133897210605,0.89399667882752099,0.89246328221391102]
[null,null,null,null,"Coincident",0.72061604945608038,0.7187170652344459,0.71697826707640189,0.71538614271856305,0.71392831970495052,0.71259346924018896,0.71137121815302995]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.91810522257132787,0.91568581027433682,0.91347048399746211,0.91144202836006949,0.90958468016002225,0.90788400587726892,0.90632678951043788]
[null,null,null,null,"Coincident",0.7318100851757865,0.72988160217012665,0.72811579355525857,0.72649893716856018,0.72501846836056139,0.72366288235459975,0.72242164484278582]
[null,"Ashford","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.81109050338148203,0.86579240306060201,0.91200349811417403,0.951041727473245,0.98402046017206202,1.0118802485967999,1.0354156530090699]
[null,null,null,null,"Coincident",0.55809975734682971,0.59573935096807151,0.62753654354844102,0.6543981899882837,0.67709038357220863,0.6962603049247057,0.7124546795805381]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.85452239111275285,0.91215344204644411,0.96083902679498656,1.0019676566552127,1.0367123188158136,1.0660639299138976,1.0908595969452985]
[null,null,null,null,"Coincident",0.58798461717798522,0.62763971782044481,0.66113957131542589,0.68943959239729491,0.71334689674876595,0.73354331991398047,0.75060486322608233]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.69489800063178997,0.737598983894168,0.77524693694904501,0.80843981123283093,0.83770479946773702,0.86350670890971404,0.88625534374627002]
[null,null,null,null,"Coincident",0.47814936054182067,0.5075312954773793,0.53343631270657177,0.55627585404775781,0.57641267326160217,0.59416659756304291,0.60981960734348428]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.732108067600025,0.77709558276400292,0.8167594904670662,0.85172976096417397,0.88256181684218071,0.90974535463446449,0.93371212252786417]
[null,null,null,null,"Coincident",0.50375307462705876,0.53470833941191098,0.56200050615806163,0.5860630483742777,0.60727814438672145,0.62598274736561543,0.64247393705397882]
[null,"Ashley","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.1332821914233104,6.13328216386995,6.1332821638423898,6.1332821638423702,6.1332821638423702,6.1332821638423702,6.1332821638423702]
[null,null,null,null,"Coincident",1.3839547047240273,1.3839546985067031,1.3839546985004842,1.3839546985004798,1.3839546985004798,1.3839546985004798,1.3839546985004798]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.2322968369645411,6.232296808966364,6.2322968089383588,6.2322968089383393,6.2322968089383393,6.2322968089383393,6.2322968089383393]
[null,null,null,null,"Coincident",1.4062970298048771,1.4062970234871819,1.4062970234808625,1.4062970234808581,1.4062970234808581,1.4062970234808581,1.4062970234808581]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8646672785373504,5.8646672785217699,5.8646672785217495,5.8646672785217495,5.8646672785217495,5.8646672785217495,5.8646672785217495]
[null,null,null,null,"Coincident",1.3233426440287912,1.3233426440252756,1.3233426440252709,1.3233426440252709,1.3233426440252709,1.3233426440252709,1.3233426440252709]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9593454514434745,5.9593454514276427,5.9593454514276223,5.9593454514276223,5.9593454514276223,5.9593454514276223,5.9593454514276223]
[null,null,null,null,"Coincident",1.3447064584985275,1.3447064584949553,1.3447064584949506,1.3447064584949506,1.3447064584949506,1.3447064584949506,1.3447064584949506]
[null,"Ashmont","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.417069321388698,22.387815806326099,22.367759063240701,22.3540077946382,22.344579674261201,22.3381155830991,22.333683684387299]
[null,null,null,null,"Coincident",19.517564216112554,19.49209445685921,19.47463192571729,19.462659296103915,19.454450643034367,19.448822640883581,19.444963980036047]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.449206586475807,23.418606167293046,23.397625962194933,23.383241551206005,23.373379336869561,23.366617622977316,23.361981668697414]
[null,null,null,null,"Coincident",20.416201101352488,20.389558651446261,20.371292102219915,20.358768223154264,20.350181623413462,20.344294494136623,20.340258171008752]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.4841338751073,20.474746019338902,20.468236774004399,20.4637234670395,20.460594081264098,20.4584242631223,20.4569197791416]
[null,null,null,null,"Coincident",17.834641655740139,17.826468059308581,17.820800743389931,17.816871203928216,17.81414658426662,17.812257418278296,17.81094752971595]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.427274015882031,21.417453920036266,21.41064497296194,21.405923862191806,21.402650391762457,21.400380669831698,21.398806915690884]
[null,null,null,null,"Coincident",18.655792627727404,18.647242698718834,18.641314445571112,18.637203980402518,18.63435391251905,18.632377764660419,18.631007565591869]
[null,"Attunga","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.60233639119601,3.6025831125397301,3.6027307750649502,3.6028191509671803,3.6028720438733899,3.6029037002350903,3.6029226465420403]
[null,null,null,null,"Coincident",2.6833825170669989,2.6835662999424525,2.6836762938451795,2.6837421251072331,2.6837815250644792,2.6838051059071093,2.6838192190224075]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.7920799036679913,3.7923396204039443,3.7924950606609342,3.7925880915293546,3.7926437704290752,3.792677094205644,3.7926970384590488]
[null,null,null,null,"Coincident",2.8247225721874911,2.8249160353383367,2.8250318228780773,2.8251011216272106,2.8251425968726775,2.8251674197736332,2.8251822762598384]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2292633257566798,3.2294855831851299,3.2296216481335098,3.2297049464525198,3.2297559412901502,3.22978716008899,3.2298062720902498]
[null,null,null,null,"Coincident",2.4054801690699765,2.4056457287604176,2.4057470836212689,2.4058091325885664,2.405847118673401,2.4058703735751963,2.4058846101162845]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3993562042628405,3.3995901685116889,3.3997334003202471,3.399821086157222,3.3998747670126361,3.3999076301788818,3.3999277488541044]
[null,null,null,null,"Coincident",2.5321824552797039,2.5323567353876117,2.5324634288468659,2.532528746078901,2.5325687329799775,2.5325932127720301,2.5326081991851508]
[null,"Ballina","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.015334366103499,24.568088297161101,24.134631853383997,23.714539868906197,23.307400286703501,22.912813754417598,22.530393232642101]
[null,null,null,null,"Coincident",19.781930620504365,19.428251929800943,19.085477966746183,18.753272513501056,18.431309718596012,18.11927377731185,17.816858621915376]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.215670206261262,24.764842357612562,24.327914568637151,23.904458268519104,23.494058100266731,23.096311513299828,22.710828368598637]
[null,null,null,null,"Coincident",19.940354634862988,19.583843500802583,19.238324425135385,18.903458497414608,18.57891725658224,18.264382368790244,17.959545315155424]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.991262643541699,22.5159427414155,22.052715572988102,21.601273483966601,21.161316647169102,20.7325528633923,20.314697367346998]
[null,null,null,null,"Coincident",18.18131054480801,17.805431286558061,17.439114867466724,17.082117996927195,16.734203573950793,16.395140529694601,16.064703673996789]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.175388662029899,22.696262150304065,22.229325217193427,21.7742677445491,21.330787504016794,20.898589956309635,20.477388055589518]
[null,null,null,null,"Coincident",18.326915959065385,17.948026463738561,17.578776391772223,17.218920504161542,16.868219801089502,16.526441363193413,16.19335819687123]
[null,"Banora Point","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.370688475537099,14.3876885520993,14.4017952433849,14.413500998844301,14.423214453835101,14.431274694644701,14.4379630956276]
[null,null,null,null,"Coincident",12.424226347726599,12.438923820258761,12.451119806961009,12.461240056637724,12.469637856341585,12.476606364246139,12.482388843482074]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.381307472415497,14.398320110920034,14.41243722612589,14.424151631371339,14.433872263968725,14.441938460767988,14.448631804040831]
[null,null,null,null,"Coincident",12.433407036670458,12.448115369671498,12.460320368408549,12.470448096286461,12.478852101413883,12.485825758589037,12.491612510698124]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.981732833401599,12.9817328340703,12.981732834070899,12.981732834070899,12.981732834070899,12.981732834070899,12.981732834070899]
[null,null,null,null,"Coincident",11.223400144151238,11.223400144729366,11.223400144729883,11.223400144729883,11.223400144729883,11.223400144729883,11.223400144729883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.991325483097453,12.99132548376665,12.991325483767248,12.991325483767248,12.991325483767248,12.991325483767248,12.991325483767248]
[null,null,null,null,"Coincident",11.231693501236991,11.231693501815547,11.231693501816064,11.231693501816064,11.231693501816064,11.231693501816064,11.231693501816064]
[null,"Barham","Substation Rating","MVA","Non-Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,null,null,"Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3848908183992998,6.3848908183948998,6.3848908183948998,6.3848908183948998,6.3848908183948998,6.3848908183948998,6.3848908183948998]
[null,null,null,null,"Coincident",5.0842649109475913,5.0842649109440874,5.0842649109440874,5.0842649109440874,5.0842649109440874,5.0842649109440874,5.0842649109440874]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6158942413557904,6.6158942413512314,6.6158942413512314,6.6158942413512314,6.6158942413512314,6.6158942413512314,6.6158942413512314]
[null,null,null,null,"Coincident",5.2682120810796116,5.2682120810759816,5.2682120810759816,5.2682120810759816,5.2682120810759816,5.2682120810759816,5.2682120810759816]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7935623780640801,5.7714115443268303,5.7500266111854694,5.7293810963987495,5.7094494333913897,5.6902069395934305,5.6716297858743605]
[null,null,null,null,"Coincident",4.6133922640139904,4.5957536371491434,4.5787248940921339,4.5622849471323379,4.5464134377005516,4.5310907111577325,4.5162977924555099]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.00317171650227,5.9802194722851576,5.9580608387163565,5.9366683754351239,5.9160155908752001,5.896076909458694,5.8768276399243415]
[null,null,null,null,"Coincident",4.7803034038814376,4.7620266168196634,4.7443817789778402,4.7273470396983397,4.7109013038450671,4.6950242056800713,4.6796960836434573]
[null,"Barraba","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.55705497158492,2.5471877601958299,2.5388276918003601,2.5317445615398499,2.52574332663194,2.5206587356255201,2.5163507779969101]
[null,null,null,null,"Coincident",2.0629736937300112,2.0550130523858212,2.0482683396716674,2.0425538315523375,2.0377121719546798,2.03361003977286,2.0301344777062309]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6169715444591155,2.6068731258817448,2.5983171654726824,2.5910680642435593,2.5849262091954133,2.579722476727055,2.5753135756067871]
[null,null,null,null,"Coincident",2.1113130196465395,2.1031658456104343,2.0962630916827192,2.0904146819672262,2.0854595732441727,2.0812613204452592,2.0777043194693547]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.24404076132079,2.23689656208537,2.2306425303688404,2.2251677512616999,2.22037512985673,2.2161796692761602,2.2125069632566703]
[null,null,null,null,"Coincident",1.8104409602869243,1.8046771831099706,1.7996315728065844,1.7952146457547529,1.7913480679954441,1.7879632659841551,1.7850002104428364]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2966228267446724,2.2893112255805206,2.2829106502224721,2.2773075868175794,2.2724026653436393,2.2681088972873171,2.2643501329076012]
[null,null,null,null,"Coincident",1.8528629726945123,1.8469641394553731,1.8418003010807111,1.8372798771801524,1.8333226982837292,1.8298585840407411,1.8268260985750582]
[null,"Batemans Bay","Substation Rating","MVA","Non-Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,null,null,"Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.1075217139432,20.513773970743202,19.968102419377399,19.466614295203399,19.005732033597301,18.582167747976399,18.1928997743547]
[null,null,null,null,"Coincident",15.143065724919875,14.717096195140307,14.325617731750032,13.965837567714139,13.635189068400241,13.331313421471542,13.052042809362407]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.132126803584704,20.53768692718954,19.991379285162875,19.489306575057061,19.02788706187237,18.603829026328675,18.214107282078885]
[null,null,null,null,"Coincident",15.160718033639887,14.734251950138528,14.342317139346839,13.982117578694551,13.65108364161701,13.34685376610412,13.067257607560006]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.743595083263298,18.234014296556499,17.762438257935699,17.326032557402101,16.922174176439302,16.548435722348497,16.202570838392798]
[null,null,null,null,"Coincident",13.447125442474148,13.081539399269465,12.74321891598815,12.430130515773712,12.140392379323544,11.872263034205378,11.624130887728743]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.76544453785479,18.255269731579684,17.783143975618295,17.34622955589316,16.941900396228782,16.567726274308754,16.22145821481265]
[null,null,null,null,"Coincident",13.462800789462614,13.096788581713998,12.758073717418583,12.444620349290936,12.154544464387087,11.8861025602361,11.637681165509965]
[null,"Batlow","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8426692031212202,1.7699367334690601,1.8052178394210101,1.7551000148415001,1.7050323080865701,1.65501466903839,1.60504704762926]
[null,null,null,null,"Coincident",1.5634768996180051,1.5017645011252632,1.5316999849632813,1.4891757701685455,1.446694079588605,1.4042548706992402,1.361858101018766]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8840310258624375,1.8096659530755488,1.8457390030443777,1.7944961992374937,1.7433046382344171,1.6921642687923384,1.6410750397197038]
[null,null,null,null,"Coincident",1.5985717795196439,1.5354741420034961,1.5660815783406841,1.5226028357166614,1.479167571835263,1.4357757432177416,1.3924273064288397]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8148609931199702,1.76703412570771,1.7192550851628701,1.6715238236585701,1.6238402934157801,1.5762044467032299,1.5286162358373898]
[null,null,null,null,"Coincident",1.5398820547684595,1.4993016824186631,1.4587618904412232,1.4182626382557566,1.3778038853224801,1.3373855911421344,1.2970077152559671]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8555986136164906,1.8066981913801616,1.7578466695660773,1.709043999273802,1.6602901316518248,1.6115850178974664,1.5629286092568599]
[null,null,null,null,"Coincident",1.574447308523083,1.5329560411710463,1.4915062650863686,1.4500979387777715,1.4087310207954877,1.3674054697311837,1.3261212442179418]
[null,"Beelbangera","Substation Rating","MVA","Non-Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,null,null,"Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.1943234288937,10.303036501491501,10.405072265932301,10.5008408517725,10.5907271978403,10.675092599485701,10.754276160795801]
[null,null,null,null,"Coincident",9.3093620471773288,9.4086378214975319,9.5018159396498021,9.5892709281589656,9.6713543096094039,9.748396015579468,9.8207057127910833]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.845093810814397,10.960746750316334,11.069296125381504,11.171178246820014,11.266802626624727,11.356553623992358,11.440791990243172]
[null,null,null,null,"Coincident",9.9036395524121303,10.009252749124359,10.108379036368923,10.201416849149846,10.288740150038629,10.370699932305534,10.447625630725978]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.3252764328198996,9.4128584842495204,9.4946803660543502,9.5711209178888996,9.6425340635644012,9.7092504497347605,9.7715789768081702]
[null,null,null,null,"Coincident",8.5157563529011711,8.5957354737599374,8.670454460891893,8.7402592671723109,8.8054730925583868,8.8663978805221308,8.9233157160647121]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.9205698574430627,10.013742844402227,10.10078795241162,10.182108204940246,10.258080119072483,10.329055448802096,10.395362813671957]
[null,null,null,null,"Coincident",9.0593728128629962,9.1444575244350634,9.2239463135192281,9.2982072174269064,9.3675840680837652,9.4323980839897192,9.4929493574776949]
[null,"Bellata","Substation Rating","MVA","Non-Coincident",5.83,5.83,5.83,5.83,5.83,5.83,5.83]
[null,null,null,null,"Coincident",5.83,5.83,5.83,5.83,5.83,5.83,5.83]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1702267497041801,1.1792014234805399,1.1862121523332501,1.1916887100634899,1.1959668222544799,1.1993087470218899,1.2019193520393201]
[null,null,null,null,"Coincident",0.91499210882219828,0.92200934346215035,0.92749098330583324,0.93177306548174088,0.93511809147469604,0.93773111907061335,0.93977233287025019]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.22223682746881,1.2316103756352303,1.2389326924369499,1.2446526527329782,1.2491209032435677,1.2526113580006404,1.2553379899077342]
[null,null,null,null,"Coincident",0.9556584247698513,0.96298753650491242,0.96871280478609234,0.97318520172537371,0.97667889554023801,0.97940805769597383,0.98153999210892784]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0332730672982899,1.0332730921173099,1.0332731054676501,1.0332731126489101,1.0332731165117599,1.03327311858962,1.03327311970731]
[null,null,null,null,"Coincident",0.80790898266121425,0.80790900206703231,0.8079090125055699,0.80790901812054683,0.80790902114088214,0.80790902276554644,0.80790902363946038]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0791963147337693,1.0791963406558569,1.0791963545995455,1.0791963620999725,1.0791963661345045,1.0791963683047141,1.0791963694720792]
[null,null,null,null,"Coincident",0.84381604855726811,0.84381606882556703,0.84381607972803963,0.84381608559257093,0.84381608874714331,0.84381609044401507,0.8438160913567696]
[null,"Bendemeer","Substation Rating","MVA","Non-Coincident",4.8,4.8,4.8,4.8,4.8,4.8,4.8]
[null,null,null,null,"Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.71205622654547807,0.71515156042519301,0.71806703752186696,0.72081310855379599,0.72339961699215705,0.72583583434557997,0.72813049339447]
[null,null,null,null,"Coincident",0.47470415103031871,0.47676770695012866,0.47871135834791129,0.48054207236919733,0.48226641132810466,0.48389055623038663,0.48542032892964665]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.71205622654547807,0.71515156042519301,0.71806703752186696,0.72081310855379599,0.72339961699215705,0.72583583434557997,0.72813049339447]
[null,null,null,null,"Coincident",0.47470415103031871,0.47676770695012866,0.47871135834791129,0.48054207236919733,0.48226641132810466,0.48389055623038663,0.48542032892964665]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.6826924019411319,0.68649697743860494,0.690297748360581,0.69409471851163596,0.69788789169253906,0.70167727170026106,0.70546286232797606]
[null,null,null,null,"Coincident",0.45512826796075456,0.45766465162573661,0.460198498907054,0.46272981234109062,0.46525859446169271,0.46778484780017404,0.47030857488531735]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6826924019411319,0.68649697743860494,0.690297748360581,0.69409471851163596,0.69788789169253906,0.70167727170026106,0.70546286232797606]
[null,null,null,null,"Coincident",0.45512826796075456,0.45766465162573661,0.460198498907054,0.46272981234109062,0.46525859446169271,0.46778484780017404,0.47030857488531735]
[null,"Bendick Murrell","Substation Rating","MVA","Non-Coincident",3.08,3.08,3.08,3.08,3.08,3.08,3.08]
[null,null,null,null,"Coincident",3.08,3.08,3.08,3.08,3.08,3.08,3.08]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.7612179483205801,1.77025771451836,1.77778778470851,1.7840602873184301,1.7892852437926599,1.79363760071547,1.79726308752611]
[null,null,null,null,"Coincident",1.5206312583573487,1.5284361703284615,1.5349376144681182,1.5403532778423574,1.5448644924514561,1.5486223067473324,1.5517525431705295]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.908243147742555,1.9180375470788535,1.9261962220776383,1.932992348664919,1.9386534807233957,1.9433691692515542,1.9472973090767427]
[null,null,null,null,"Coincident",1.6475724550561817,1.6560289154288528,1.6630730954190469,1.6689408544514976,1.6738286619906027,1.6779001759037062,1.681291722197608]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.59340247038484,1.5934024703423699,1.59340247034233,1.59340247034233,1.59340247034233,1.59340247034233,1.59340247034233]
[null,null,null,null,"Coincident",1.3757397861641438,1.3757397861274754,1.375739786127441,1.375739786127441,1.375739786127441,1.375739786127441,1.375739786127441]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7264185551863764,1.726418555140361,1.7264185551403177,1.7264185551403177,1.7264185551403177,1.7264185551403177,1.7264185551403177]
[null,null,null,null,"Coincident",1.4905855476477823,1.4905855476080527,1.4905855476080152,1.4905855476080152,1.4905855476080152,1.4905855476080152,1.4905855476080152]
[null,"Bermagui","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.20647293637224,3.2064729332307902,3.2064729324585102,3.20647293226865,3.2064729322219803,3.2064729322105001,3.2064729322076801]
[null,null,null,null,"Coincident",2.6295001320933298,2.6295001295171527,2.6295001288838367,2.6295001287281399,2.6295001286898678,2.6295001286804536,2.6295001286781408]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2321161721179692,3.232116168951396,3.23211616817294,3.2321161679815615,3.2321161679345183,3.2321161679229462,3.232116167920104]
[null,null,null,null,"Coincident",2.6505291234862787,2.6505291208894985,2.6505291202511181,2.6505291200941765,2.650529120055598,2.6505291200461083,2.6505291200437773]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0457389204020799,3.0457389185082904,3.0457389180798899,3.0457389179829804,3.0457389179610601,3.0457389179561001,3.0457389179549801]
[null,null,null,null,"Coincident",2.4976885981704493,2.4976885966174285,2.4976885962661144,2.4976885961866429,2.497688596168667,2.4976885961645992,2.4976885961636808]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0700967125012633,3.0700967105923285,3.0700967101605019,3.0700967100628174,3.0700967100407217,3.0700967100357222,3.0700967100345933]
[null,null,null,null,"Coincident",2.5176634486723124,2.5176634471068713,2.5176634467527474,2.5176634466726404,2.5176634466545207,2.5176634466504209,2.5176634466494949]
[null,"Bethungra","Substation Rating","MVA","Non-Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,null,null,"Coincident",6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005,6.6000000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.75793411102090202,0.74322674184736004,0.73018784348001997,0.71862813700718298,0.70837981617719092,0.69929411144227904,0.69123913034836004]
[null,null,null,null,"Coincident",0.67760957208118688,0.66446086431462359,0.65280380571990915,0.64246917683522609,0.6333069552236299,0.62518413767529846,0.61798280946905015]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.78985796624053239,0.77453112907190924,0.76094303797442298,0.74889644169090952,0.73821646604334978,0.72874807537530983,0.72035382197988063]
[null,null,null,null,"Coincident",0.70615019264438905,0.69244766702352756,0.68029961818909013,0.66952969922910122,0.65998156882679915,0.6515166217349917,0.64401197671570853]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.71425794375606699,0.69645387820230908,0.68023983209581007,0.665473806305247,0.65202648315003708,0.63978009386388102,0.62862738720121902]
[null,null,null,null,"Coincident",0.63856212906452725,0.62264490741456435,0.60814919771609111,0.59494804965876702,0.58292585042489731,0.5719773121772197,0.56200654997065502]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.74434217780014045,0.72578821274615635,0.70889123806723686,0.69350327369038656,0.67948955513054143,0.66672735325216947,0.65510489943387906]
[null,null,null,null,"Coincident",0.66545808830501685,0.64887044019968876,0.63376417751119818,0.62000700283732935,0.60747843379877209,0.59606874788033637,0.58567802150474513]
[null,"Bingara","Substation Rating","MVA","Non-Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,null,null,"Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7620796462055002,2.7620892517993303,2.7620907229368998,2.7620909482478799,2.76209098275522,2.7620909880401601,2.7620909888495699]
[null,null,null,null,"Coincident",2.2605786344933465,2.2605864960335498,2.260587700061885,2.2605878844639493,2.2605879127059136,2.2605879170312861,2.260587917693734]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.9073947541743812,2.9074048651257982,2.9074064136610325,2.9074066508257945,2.9074066871485922,2.9074066927115769,2.9074066935635701]
[null,null,null,null,"Coincident",2.3795093933492066,2.3795176684910113,2.3795189358641915,2.3795191299677882,2.3795191596955845,2.3795191642485176,2.3795191649458172]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4572188900967298,2.4572259019440397,2.45722692600217,2.4572270755626202,2.45722709740545,2.4572271005955297,2.4572271010614299]
[null,null,null,null,"Coincident",2.01107036535211,2.011076104083156,2.0110769422066808,2.0110770646119702,2.0110770824888751,2.011077085099743,2.0110770854810518]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5864950421469137,2.5865024228928362,2.5865035008274422,2.5865036582563814,2.586503681248379,2.5865036846062912,2.5865036850967029]
[null,null,null,null,"Coincident",2.1168743046684986,2.1168803453185436,2.1168812275363837,2.1168813563815081,2.1168813751989304,2.1168813779471582,2.1168813783485279]
[null,"Blayney","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.775929579643201,11.778354778777501,11.780327016010501,11.7819308924296,11.783235207916899,11.7842959123891,11.7851585058247]
[null,null,null,null,"Coincident",7.7186765311947019,7.7202661575180249,7.7215588844438567,7.7226101647857863,7.7234650942648573,7.7241603459357107,7.7247257433136678]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.866090758497611,11.868534525916601,11.870521863378649,11.872138019710572,11.873452321553611,11.874521147199175,11.875390344991612]
[null,null,null,null,"Coincident",7.7777737744774242,7.7793755716091999,7.7806781961641551,7.7817375255245755,7.7825990006821977,7.7832995754750884,7.7838693017592062]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.281280897803999,11.2731887942514,11.266713922952301,11.2615330749728,11.2573876356975,11.254070675452001,11.251416620105999]
[null,null,null,null,"Coincident",7.3944530254513596,7.3891489575765466,7.3849049242880618,7.3815090743519178,7.3787918956672671,7.3766177536576123,7.3748781207417462]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.367654850522946,11.359500790621953,11.352976345144839,11.347755830542152,11.343578652142616,11.34023629593632,11.337561920091872]
[null,null,null,null,"Coincident",7.4510678852167196,7.4457232072984212,7.4414466800109018,7.4380248301032577,7.4352868476228897,7.4330960595212838,7.4313431072871081]
[null,"Blue Cow","Substation Rating","MVA","Non-Coincident",9.6,9.6,9.6,9.6,9.6,9.6,9.6]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0062486907040498,5.0062476197098205,5.0062473759639694,5.0062473204902496,5.0062473078650802,5.0062473049917298,5.0062473043377906]
[null,null,null,null,"Coincident",7.2997981849400539E-2,7.2997966232833708E-2,7.2997962678684414E-2,7.2997961869801384E-2,7.2997961685709073E-2,7.2997961643811685E-2,7.2997961634276354E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.842193321560087,5.8421920717309801,5.8421917872843867,5.8421917225476516,5.8421917078143286,5.8421917044611851,5.8421917036980515]
[null,null,null,null,"Coincident",8.5187202713246812E-2,8.5187184489021822E-2,8.5187180341399812E-2,8.5187179397449297E-2,8.5187179182617215E-2,8.5187179133723784E-2,8.518717912259624E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.2868142315012197,4.2868141053225699,4.2868140819722003,4.2868140776510302,4.2868140768513605,4.2868140767033704,4.2868140766759897]
[null,null,null,null,"Coincident",6.2507639311635846E-2,6.250763747177783E-2,6.2507637131297381E-2,6.2507637068288782E-2,6.2507637056628498E-2,6.2507637054470599E-2,6.2507637054071349E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.002627520392533,5.0026273731445414,5.0026273458951209,5.0026273408524009,5.0026273399192025,5.0026273397465006,5.0026273397145475]
[null,null,null,null,"Coincident",7.2945180212685104E-2,7.2945178065607144E-2,7.2945177668273173E-2,7.2945177594743393E-2,7.294517758113607E-2,7.2945177578617848E-2,7.2945177578151929E-2]
[null,"Boambee South 11kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.1023073777293,12.0884827918954,12.076867780420899,12.067109188505599,12.058910305846,12.052021845149,12.046234362543801]
[null,null,null,null,"Coincident",9.1175379281159081,9.1071228740483647,9.0983724511456092,9.091020602515778,9.0848437949629783,9.0796542224532928,9.0752940958663313]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.208406604258526,12.194460820225117,12.182743981578732,12.172899837460704,12.164629076350044,12.15768022548701,12.151842004835851]
[null,null,null,null,"Coincident",9.1974701007034358,9.1869637393218131,9.1781366026922626,9.1707203014395677,9.1644893426837513,9.1592542739218121,9.1548559227183386]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.2730208915591188,9.1623362146392786,9.0726439719848493,8.9999627426019906,8.9410662210270004,8.8933400022620415,8.8546655288519194]
[null,null,null,null,"Coincident",6.9860330801534012,6.9026463582349864,6.8350747457535181,6.7803187521336765,6.7359477695983756,6.6999921789681274,6.6708559186533725]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.35431616141768,9.2426611275036485,9.1521825655735398,9.0788641500756686,9.0194512909801272,8.9713066631681926,8.9322931360894451]
[null,null,null,null,"Coincident",7.0472786495458823,6.9631608879651763,6.8949968846613761,6.8397608529471796,6.7950008762489977,6.7587300680130316,6.7293383742022597]
[null,"Bodalla","Substation Rating","MVA","Non-Coincident",8.4,8.4,8.4,8.4,8.4,8.4,8.4]
[null,null,null,null,"Coincident",7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3038617178591301,1.2790426234866099,1.2542483482084599,1.2294788672055799,1.2047341556837101,1.18001418887336,1.15531894202982]
[null,null,null,null,"Coincident",0.99127283949549416,0.97240389517772507,0.9535538198042719,0.934722594506186,0.91591020043340388,0.89711661875469273,0.87834183065766014]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.312310065923012,1.2873301566841473,1.262375227354519,1.2374452529542121,1.212540208528313,1.1876600691468373,1.1628048099047432]
[null,null,null,null,"Coincident",0.99769577366069173,0.97870456836462172,0.95973235427384607,0.94077911239715484,0.921844823762346,0.90292946941617014,0.88403303042434045]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.22352271166455,1.2075676933195301,1.19162862999286,1.1757055057295198,1.1597983045904401,1.1439070106525,1.12803160800849]
[null,null,null,null,"Coincident",0.93019437258298399,0.91806442343083072,0.90594660422783313,0.89384090284404105,0.88174730716163052,0.86966580507490288,0.85759638449025599]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2314505046127002,1.2153921060192245,1.199349765824347,1.1833234679696678,1.1673131964128403,1.1513189351275701,1.1353406681035774]
[null,null,null,null,"Coincident",0.93622154994313278,0.92401300500813621,0.91181666861807809,0.89963252856441267,0.8874605726507987,0.87530078869309869,0.86315316451935042]
[null,"Boggabri","Substation Rating","MVA","Non-Coincident",19.8,19.8,19.8,19.8,19.8,19.8,19.8]
[null,null,null,null,"Coincident",18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3821106794603901,6.4524958980133293,6.5179424485104196,6.5787968588543597,6.6353813423784205,6.68799550390899,6.7369179261201699]
[null,null,null,null,"Coincident",5.1923209846998146,5.2495845869249029,5.3028302159322314,5.3523397979044276,5.3983754773162467,5.4411810049431448,5.4809830284785512]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.4777438936964646,6.5491838048147635,6.6156110440367986,6.6773773318385148,6.7348097097829456,6.7882122721473799,6.8378677760488111]
[null,null,null,null,"Coincident",5.2701257063744702,5.3282473793248357,5.3822908714376068,5.432542333439355,5.479267837928302,5.522714788181605,5.5631132281119893]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8001913730251502,5.8493948837652301,5.8950993489788601,5.9375535988696599,5.97698876839556,6.0136195556438894,6.0476453907186096]
[null,null,null,null,"Coincident",4.7188864145458025,4.7589171244736068,4.7961011010202625,4.8306407860349898,4.8627242249705613,4.8925260906648829,4.9202086343175644]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8871047739431122,5.9370455783655025,5.9834349055523646,6.0265253143220923,6.0665514030916592,6.1037310871079233,6.1382667848501358]
[null,null,null,null,"Coincident",4.7895969205372344,4.8302274736283461,4.8679686362493015,4.9030258837543332,4.9355900793773477,4.9658385133544405,4.9939358681504409]
[null,"Bohnock","Substation Rating","MVA","Non-Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,null,null,"Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.8915179836883,7.4755623809877001,8.0590227338897904,8.6418996264389811,9.2241936420956296,9.8059053637366098,10.387035373655999]
[null,null,null,null,"Coincident",5.7373111043365581,6.223538436831749,6.7092795419944364,7.1945349060519632,7.679305014745438,8.1635903533302105,8.647391406576439]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.175446348919972,7.7835531910015572,8.391051926241051,8.9979431627453064,9.6042275080130661,10.209905568935545,10.814977951797154]
[null,null,null,null,"Coincident",5.9736865105294292,6.4799462556183443,6.9856997409621631,7.4909474728206389,7.9956899569472624,8.4999276985897492,9.0036612024906368]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8251969417921501,6.2198380892422902,6.6140845955449805,7.0079368553413595,7.4013952628779496,7.7944602120070101,8.1871320961869305]
[null,null,null,null,"Coincident",4.849579900712202,5.1781256641931863,5.5063428819106912,5.83423188241047,6.1617929939097564,6.4890265442975483,6.8159328611349439]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0651932167420712,6.4760934548764233,6.886582792772642,7.2966616413309557,7.7063304110407183,8.1155895119807795,8.5244393538198882]
[null,null,null,null,"Coincident",5.049381061578166,5.3914628067905692,5.7332024702577602,6.0746003940614779,6.4156569199413962,6.7563723892954428,7.0967471431801243]
[null,"Bombala","Substation Rating","MVA","Non-Coincident",34.799999999999997,34.799999999999997,34.799999999999997,34.799999999999997,34.799999999999997,34.799999999999997,34.799999999999997]
[null,null,null,null,"Coincident",31.900000000000002,31.900000000000002,31.900000000000002,31.900000000000002,31.900000000000002,31.900000000000002,31.900000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.3843854250030603,5.4990943184346701,5.6092614256420203,5.7150665741998496,5.8166824715863008,5.9142749870961699,6.0080034225920596]
[null,null,null,null,"Coincident",3.3528099216377893,3.4242381507930926,3.4928382492124452,3.5587221939608562,3.6219975284811796,3.6827675381390401,3.7411314188172193]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3903049340454992,5.5051399366387539,5.6154281598390758,5.7213496289208257,5.823077241234043,5.9207770484276301,6.0146085274981633]
[null,null,null,null,"Coincident",3.356495948376617,3.4280027046088284,3.4966782209024325,3.5626345974282714,3.6259794958607761,3.6868163151158857,3.7452443601307825]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.9249377332649003,4.9152413020582095,4.9088385709147397,4.9046107302565094,4.9018190096249601,4.8999755853536602,4.8987583385397606]
[null,null,null,null,"Coincident",3.0667158444604659,3.0606779611760881,3.0566910362424236,3.0540583966768766,3.0523200165474687,3.0511721323046537,3.0504141633123574]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.930352132707803,4.920645041396444,4.9142352711905914,4.9100027825105288,4.9072079927050227,4.9053625418019378,4.9041439567659477]
[null,null,null,null,"Coincident",3.0700873438497136,3.0640428226109782,3.0600515145144582,3.0574159806661867,3.0556756893888797,3.0545265431800983,3.0537677408885586]
[null,"Bomen","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.8259952118783,11.825995211881001,11.825995211881001,11.825995211881001,11.825995211881001,11.825995211881001,11.825995211881001]
[null,null,null,null,"Coincident",9.3936983243288648,9.3936983243310088,9.3936983243310088,9.3936983243310088,9.3936983243310088,9.3936983243310088,9.3936983243310088]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.938174421778211,11.938174421780937,11.938174421780937,11.938174421780937,11.938174421780937,11.938174421780937,11.938174421780937]
[null,null,null,null,"Coincident",9.4828052144621271,9.4828052144642925,9.4828052144642925,9.4828052144642925,9.4828052144642925,9.4828052144642925,9.4828052144642925]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.388811230733801,11.388811230741,11.3888112307411,11.3888112307411,11.3888112307411,11.3888112307411,11.3888112307411]
[null,null,null,null,"Coincident",9.0464316159020282,9.0464316159077462,9.0464316159078262,9.0464316159078262,9.0464316159078262,9.0464316159078262,9.0464316159078262]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.49684339400406,11.496843394011329,11.496843394011428,11.496843394011428,11.496843394011428,11.496843394011428,11.496843394011428]
[null,null,null,null,"Coincident",9.1322443980741479,9.1322443980799228,9.132244398080001,9.132244398080001,9.132244398080001,9.132244398080001,9.132244398080001]
[null,"Bonalbo","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0492173757529,1.0719144752362499,1.0804921657934301,1.0837338476369001,1.0849589444277301,1.08542193315375,1.0855969059085901]
[null,null,null,null,"Coincident",0.75648901700052351,0.7728536968788009,0.7790382386598399,0.78137550143099377,0.78225880005761106,0.78259261638044675,0.78271877228519038]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1654316305384875,1.1906427243219788,1.200170503906391,1.2037712435089079,1.2051320354510733,1.2056463061049492,1.205840659332112]
[null,null,null,null,"Coincident",0.84027985900894087,0.85845713665848,0.86532669560648878,0.86792284014748844,0.8689039754035951,0.86927476615717336,0.8694148954432156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.94218110322992199,0.99390668642158009,1.02639135890058,1.0467923651523299,1.05960459394585,1.0676509228686499,1.07270417396003]
[null,null,null,null,"Coincident",0.67931552897455194,0.71660983660490096,0.74003138729508899,0.75474057675559836,0.76397823387945296,0.76977966225639338,0.77342307213419093]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0465397207245632,1.1039945743637822,1.1400773401372168,1.1627380189727552,1.1769693661070413,1.1859069289544146,1.1915198922878913]
[null,null,null,null,"Coincident",0.75455841933118983,0.79598354891432577,0.82199933614909049,0.83833775662612442,0.84859860252231811,0.8550426133527127,0.85908957751164583]
[null,"Booral","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.42535389727249,2.43871972037218,2.4493921331916098,2.45791389758568,2.4647184008987302,2.47015169653988,2.4744901030577497]
[null,null,null,null,"Coincident",1.9266937654970921,1.9373115347495999,1.9457896670605714,1.9525593307981211,1.9579648075515554,1.9622810010974452,1.9657274180510995]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5531859402911259,2.5672562298504862,2.5784911487586895,2.5874620659769487,2.5946252112025099,2.6003448771267403,2.6049119460964065]
[null,null,null,null,"Coincident",2.0282431519976516,2.0394205472648927,2.0483455327033653,2.0554720020795041,2.0611623828783472,2.0657060681068553,2.0693341338173261]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.1016275812582599,2.1281539226146702,2.1360212755338397,2.1383546256601598,2.1390466656471698,2.1392519153172502,2.1393127895844399]
[null,null,null,null,"Coincident",1.6695265638390642,1.6905990088007328,1.6968488100513361,1.6987024163007822,1.6992521707633976,1.6994152204775688,1.6994635788104313]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2123971261393938,2.2403215795046174,2.2486035934750825,2.2510599264428182,2.2517884414718785,2.2520045091445131,2.2520685918844747]
[null,null,null,null,"Coincident",1.757521553671038,1.7797046545637347,1.7862838612933587,1.7882351647382881,1.7888138948634629,1.7889855383659881,1.7890364454998702]
[null,"Boorowa","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.50323053694349,3.60113686195047,3.6989011527887299,3.7965236155093498,3.8940044558645099,3.9913438793078799,4.0885420909950998]
[null,null,null,null,"Coincident",2.8225080155468878,2.9013898887752601,2.9801573268913937,3.0588104959080069,3.1373495615969986,3.215774689489761,3.2940860448775684]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6311712116966532,3.7326531510264416,3.833987868990381,3.935175579164695,4.0362164948157924,4.1371108289006679,4.2378587940674048]
[null,null,null,null,"Coincident",2.9255881800399575,3.0073508799739104,3.0889949655372737,3.1705206088056785,3.2519279816051405,3.3332172555123867,3.4143886018552552]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2092367452353803,3.2747935173910001,3.34028473277447,3.40571045694255,3.4710707553864699,3.5363656935319399,3.6015953367392699]
[null,null,null,null,"Coincident",2.5856409795735291,2.638459232021185,2.6912246662163977,2.7439373349774101,2.7965972910696677,2.8492045872058283,2.901759276045857]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.326440540503246,3.3943914964203339,3.4622745013815104,3.5300896233377195,3.5978369301719804,3.6655164896994008,3.7331283696672997]
[null,null,null,null,"Coincident",2.6800705776566436,2.7348177933244395,2.7895102617765724,2.8441480377602479,2.8987311759679462,2.953259731037432,3.0077337575518528]
[null,"Bootawa","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.2202622253411404,4.2202621783259202,4.2202621782789098,4.2202621782788601,4.2202621782788601,4.2202621782788601,4.2202621782788601]
[null,null,null,null,"Coincident",1.6687261350200939,1.6687261164298921,1.6687261164113036,1.6687261164112841,1.6687261164112841,1.6687261164112841,1.6687261164112841]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4194327640370874,4.4194327148030368,4.4194327147538077,4.4194327147537562,4.4194327147537562,4.4194327147537562,4.4194327147537562]
[null,null,null,null,"Coincident",1.7474797919024199,1.7474797724348743,1.7474797724154087,1.7474797724153883,1.7474797724153883,1.7474797724153883,1.7474797724153883]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8411698691651801,3.8411698424364897,3.8411698424097698,3.84116984240974,3.84116984240974,3.84116984240974,3.84116984240974]
[null,null,null,null,"Coincident",1.5188299227566402,1.5188299121878979,1.5188299121773325,1.5188299121773208,1.5188299121773208,1.5188299121773208,1.5188299121773208]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0224495696232312,4.0224495416331107,4.0224495416051296,4.0224495416050985,4.0224495416050985,4.0224495416050985,4.0224495416050985]
[null,null,null,null,"Coincident",1.5905093961520431,1.5905093850845209,1.5905093850734568,1.5905093850734446,1.5905093850734446,1.5905093850734446,1.5905093850734446]
[null,"Boronia St","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.2179761890457,23.217976316405899,23.217976316533299,23.217976316533402,23.217976316533402,23.217976316533402,23.217976316533402]
[null,null,null,null,"Coincident",15.465665347401249,15.465665432236817,15.465665432321678,15.465665432321748,15.465665432321748,15.465665432321748,15.465665432321748]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.309523578381704,23.309523706244079,23.30952370637198,23.309523706372083,23.309523706372083,23.309523706372083,23.309523706372083]
[null,null,null,null,"Coincident",15.526645739291171,15.526645824461243,15.526645824546438,15.526645824546506,15.526645824546506,15.526645824546506,15.526645824546506]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.920856239788101,19.920856445859002,19.920856446065098,19.920856446065301,19.920856446065301,19.920856446065301,19.920856446065301]
[null,null,null,null,"Coincident",13.269429408046774,13.269429545312121,13.269429545449404,13.269429545449539,13.269429545449539,13.269429545449539,13.269429545449539]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.999403240062435,19.999403446945863,19.999403447152773,19.999403447152975,19.999403447152975,19.999403447152975,19.999403447152975]
[null,null,null,null,"Coincident",13.321750144806691,13.321750282613269,13.321750282751093,13.321750282751228,13.321750282751228,13.321750282751228,13.321750282751228]
[null,"Borthwick St","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",17.288,17.288,17.288,17.288,17.288,17.288,17.288]
[null,null,null,null,"Coincident",17.408000000000001,17.408000000000001,17.408000000000001,17.408000000000001,17.408000000000001,17.408000000000001,17.408000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.270087342465001,25.941377372108303,27.4967811942937,28.944334286311602,30.291514950472902,31.545282948273801,32.712115455692903]
[null,null,null,null,"Coincident",21.059682356031356,22.509897044278762,23.859554751248293,25.115628035255344,26.28460598177405,27.372527727141886,28.385013657752555]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.562051120582709,26.253446399313077,27.827561385163278,29.292528220436733,30.655915169765677,31.924765719036451,33.105634963220837]
[null,null,null,null,"Coincident",21.31302567284207,22.780686122758475,24.146579913172296,25.417763480731967,26.600803973173392,27.701813176307329,28.726479088531615]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.557492137049202,21.415294207472499,22.167281318873698,22.8265063723113,23.4044121162941,23.911029768622001,24.3551531370478]
[null,null,null,null,"Coincident",17.838182794067247,18.582516296973623,19.235031859792787,19.807055768509535,20.308517144740726,20.748120294224091,21.133495795101378]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.804794216694226,21.672915456135087,22.433948806020826,23.101104190920182,23.68596201307346,24.198674163610107,24.648140237843524]
[null,null,null,null,"Coincident",18.05277218428331,18.80605985445829,19.466425035052335,20.045330264763358,20.552824110343288,20.997715588401018,21.387727071244196]
[null,"Bourke 22kV","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.0167688541959601,7.0715317087373197,7.11593390552303,7.1519355912625695,7.1811260698855701,7.2047939627838398,7.2239840953431003]
[null,null,null,null,"Coincident",4.6225335357034192,4.6586104162289779,4.6878618634357796,4.7115791901898687,4.7308094041475881,4.7464014281853002,4.759043576324002]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2083866973426405,7.2646450465040768,7.3102598032808386,7.3472446431636032,7.3772322716814323,7.4015465006188723,7.4212606880368739]
[null,null,null,null,"Coincident",4.7487682634520771,4.7858303515820779,4.8158806136478498,4.8402456264084543,4.8600009897901328,4.8760188095293246,4.8890061965107785]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4895804336124101,6.5242002073702601,6.5522847545758003,6.5750677397350001,6.5935499466570198,6.6085432396922297,6.6207062263413796]
[null,null,null,null,"Coincident",4.2752303532243916,4.2980372987743269,4.316538943048247,4.3315480042173142,4.3437237824260775,4.3536011207431917,4.3616138991100302]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6668015209041913,6.702366710780991,6.7312182064884842,6.7546233621320431,6.7736102914840837,6.7890130297401319,6.8015081700224371]
[null,null,null,null,"Coincident",4.3919807316767479,4.4154105020347743,4.4344173995447784,4.4498363365396907,4.4623446177006629,4.4724916918896138,4.4807232876837002]
[null,"Bourke 33kV","Substation Rating","MVA","Non-Coincident",9.6,9.6,9.6,9.6,9.6,9.6,9.6]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.40384185250395,1.4038418591257,1.4038418591323201,1.4038418591323301,1.4038418591323301,1.4038418591323301,1.4038418591323301]
[null,null,null,null,"Coincident",1.0781505427230336,1.0781505478085376,1.0781505478136217,1.0781505478136295,1.0781505478136295,1.0781505478136295,1.0781505478136295]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8886352389019809,1.888635247810442,1.8886352478193482,1.8886352478193615,1.8886352478193615,1.8886352478193615,1.8886352478193615]
[null,null,null,null,"Coincident",1.4504718634767213,1.4504718703184194,1.4504718703252595,1.4504718703252697,1.4504718703252697,1.4504718703252697,1.4504718703252697]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3331971168191701,1.3331971244279901,1.3331971244356,1.33319712443561,1.33319712443561,1.33319712443561,1.33319712443561]
[null,null,null,null,"Coincident",1.0238953857171227,1.0238953915606963,1.0238953915665407,1.0238953915665485,1.0238953915665485,1.0238953915665485,1.0238953915665485]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7935945211607236,1.7935945313971229,1.7935945314073607,1.7935945314073742,1.7935945314073742,1.7935945314073742,1.7935945314073742]
[null,null,null,null,"Coincident",1.3774805922514357,1.3774806001129904,1.377480600120853,1.3774806001208635,1.3774806001208635,1.3774806001208635,1.3774806001208635]
[null,"Bourkelands","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.727711006624601,12.7254364488224,12.723388346857501,12.7215441547007,12.7198835710143,12.7183883156693,12.7170419285134]
[null,null,null,null,"Coincident",11.928253715238307,11.926122027730592,11.924202571839484,11.922474217704595,11.920917939162722,11.919516604302514,11.91825478687233]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.077542112183215,13.075205036378351,13.073100640726842,13.071205759504211,13.069499533374596,13.06796317976533,13.06657978610394]
[null,null,null,null,"Coincident",12.256111110995764,12.25392083238733,12.251948618747706,12.250172759445745,12.248573705369248,12.247133853722859,12.245837354252332]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.504033611283699,11.455031122601801,11.4112553028038,11.3721486686199,11.337213198667399,11.306003991169201,11.278123598147801]
[null,null,null,null,"Coincident",10.781438358601827,10.735513830823693,10.694487672634581,10.657837417592509,10.625096326202423,10.595847442008219,10.569718281669278]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.82023098522817,11.769881624765338,11.724902592274285,11.684721081620914,11.648825382914765,11.616758365904941,11.588111658444991]
[null,null,null,null,"Coincident",11.077774636078477,11.030587836685559,10.98843404240629,10.950776426399337,10.91713542046906,10.887082607784599,10.860235267008976]
[null,"Brewarrina","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1594088367911302,3.1594088369593001,3.1594088369594702,3.1594088369594702,3.1594088369594702,3.1594088369594702,3.1594088369594702]
[null,null,null,null,"Coincident",2.8438831185307811,2.843883118682156,2.8438831186823093,2.8438831186823093,2.8438831186823093,2.8438831186823093,2.8438831186823093]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1625225774318575,3.1625225776001935,3.1625225776003636,3.1625225776003636,3.1625225776003636,3.1625225776003636,3.1625225776003636]
[null,null,null,null,"Coincident",2.8466858942717774,2.846685894423302,2.8466858944234548,2.8466858944234548,2.8466858944234548,2.8466858944234548,2.8466858944234548]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9050194096158304,2.9050194097822901,2.9050194097824602,2.9050194097824602,2.9050194097824602,2.9050194097824602,2.9050194097824602]
[null,null,null,null,"Coincident",2.6148992057645781,2.6148992059144138,2.614899205914567,2.614899205914567,2.614899205914567,2.614899205914567,2.614899205914567]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9078824379433104,2.907882438109934,2.9078824381101045,2.9078824381101045,2.9078824381101045,2.9078824381101045,2.9078824381101045]
[null,null,null,null,"Coincident",2.6174763074785385,2.6174763076285217,2.6174763076286749,2.6174763076286749,2.6174763076286749,2.6174763076286749,2.6174763076286749]
[null,"Brisbane Grove","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2800497087796598,2.3403687659309198,2.3986708619239496,2.4550234403247799,2.5094916895074699,2.56213861806369,2.6130251276907503]
[null,null,null,null,"Coincident",1.3671318732984701,1.4032995521351461,1.4382578486166904,1.4720472023214219,1.5047067006006392,1.5362741237946707,1.5667859889369873]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2852877619340597,2.3457453925674527,2.4041814283937453,2.4606634679198809,2.5152568492798859,2.5680247258176925,2.6190281391426158]
[null,null,null,null,"Coincident",1.3702726422886533,1.4065234106402151,1.4415620182721931,1.4754289976664332,1.5081635259712345,1.5398034703212746,1.5703854316421262]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2172757059291697,2.28220768665649,2.3470747354030901,2.41187691710094,2.4766142966170901,2.5412869387537298,2.6058949082482301]
[null,null,null,null,"Coincident",1.3294921938735125,1.3684258101481479,1.4073204928065131,1.4461762807822176,1.4849932129699452,1.5237713282254888,1.5625106653657748]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2223695457524397,2.2874506974233411,2.3524667679425786,2.4174178223912932,2.482303925785557,2.5471251430764323,2.6118815391500143]
[null,null,null,null,"Coincident",1.3325464916605536,1.3715695517533455,1.4105535887860488,1.4494986417817173,1.4884047497243886,1.5272719515591209,1.566100286192017]
[null,"Brogo","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.76346832153321309,0.79253553510643404,0.82075585570613596,0.84815395813325301,0.874753798271665,0.90057863403433203,0.92565104569915602]
[null,null,null,null,"Coincident",0.68788824379176161,0.71407792833119177,0.7395045586563177,0.76419036686898556,0.78815693732368108,0.81142522550008689,0.83401557632578194]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.80290140557223133,0.83346993864134322,0.86314783677560647,0.89196104922765351,0.91993476920104811,0.94709345587828608,0.97346085580700348]
[null,null,null,null,"Coincident",0.72341762223724726,0.7509600021043954,0.7776999160618091,0.80366074449779978,0.8288651865972142,0.85333528018875715,0.87709242101405771]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.71707036157703996,0.74781539723436796,0.77852968785603793,0.80921326418708706,0.839866156941805,0.87048839680376799,0.90108001442586894]
[null,null,null,null,"Coincident",0.64608348216697442,0.6737848916258008,0.70145859967516766,0.72910463401648595,0.75672302232346289,0.78431379224213249,0.81187697139088344]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.75410699431272643,0.78644000885622922,0.81874069038518771,0.85100907123261815,0.88324518369920102,0.91544906005331705,0.94762073253107892]
[null,null,null,null,"Coincident",0.67945364767344651,0.70858583294363275,0.73768888602854799,0.76676283606037909,0.79580771214217838,0.82482354334789554,0.85381035872240696]
[null,"Bulahdelah","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.8132143659365703,3.81321445101654,3.81321449080199,3.8132145094066301,3.8132145181066099,3.8132145221749401,3.8132145240773796]
[null,null,null,null,"Coincident",3.1709577291151674,3.1709577998651861,3.1709578329496049,3.1709578484206804,3.1709578556553297,3.1709578590384342,3.1709578606204474]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.8889475375066294,3.8889476242763483,3.8889476648519659,3.8889476838261072,3.8889476926988751,3.888947696848005,3.8889476987882285]
[null,null,null,null,"Coincident",3.2339352233483041,3.233935295503469,3.233935329244968,3.2339353450233097,3.2339353524016445,3.2339353558519397,3.2339353574653731]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.4122219970315002,3.41222201663658,3.4122220248055002,3.4122220282092699,3.4122220296275301,3.41222203021848,3.4122220304647097]
[null,null,null,null,"Coincident",2.8375041832420838,2.8375041995450956,2.8375042063381311,2.8375042091686065,2.8375042103479906,2.8375042108394073,2.8375042110441644]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4799911726238211,3.4799911926182716,3.4799912009494327,3.4799912044208035,3.4799912058672313,3.4799912064699181,3.4799912067210381]
[null,null,null,null,"Coincident",2.8938590509515607,2.893859067578362,2.8938590745063122,2.8938590773930031,2.8938590785958103,2.8938590790969867,2.8938590793058108]
[null,"Bulgary","Substation Rating","MVA","Non-Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,null,null,"Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.29685462971952803,0.31417764244311097,0.32867421506509903,0.34080551238259604,0.35095745508264503,0.35945299664656605,0.366562397142292]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.30066045830567573,0.3182055609359713,0.33288798705311301,0.34517481382339849,0.35545690963498655,0.364061368398445,0.37126191505437256]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.27518120654896,0.28954173978798797,0.301538339113051,0.31156013934641402,0.31993221856619697,0.326926142694618,0.33276877430738605]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.27870917073548507,0.29325381337501338,0.30540421525552591,0.31555450010726538,0.32403391367601991,0.33111750349839508,0.33703504064466017]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Bullocks Flat","Substation Rating","MVA","Non-Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,null,null,"Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.04519742014707,1.0679157568745299,1.09061137526526,1.1132842980375999,1.1359345478871701,1.1585621474868899,1.1811671194870101]
[null,null,null,null,"Coincident",0.19611621874776905,0.20037898691897357,0.20463749232200645,0.20889173921963639,0.21314173187036919,0.21738747452845111,0.22162897144387497]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0531327584779047,1.0760235771544884,1.0988915050123933,1.1217365649424407,1.1445587798125609,1.1673581724678099,1.190134765730404]
[null,null,null,null,"Coincident",0.19760517051700377,0.20190030243788118,0.20619113922683732,0.21047768517900456,0.21475994458522019,0.21903792173202938,0.22331162090169182]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.95345803028255294,0.97582407971662,0.99816776310125299,1.0204891028025,1.04278812116405,1.06506484050723,1.0873192831310801]
[null,null,null,null,"Coincident",0.1789026455953163,0.18309931213771719,0.18729178201357563,0.19148005941955801,0.19566414854813516,0.19984405358758217,0.2040197787219922]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.9606968656534618,0.9832327224042734,1.0057460432983343,1.0282368508714996,1.050705167637096,1.0731510160859183,1.0955744186863052]
[null,null,null,null,"Coincident",0.18026090863128943,0.18448943706717924,0.1887137369746332,0.1929338125821794,0.19714966811411885,0.20136130779052477,0.20556873582725679]
[null,"Bullocks Portal","Substation Rating","MVA","Non-Coincident",7.5,7.5,7.5,7.5,7.5,7.5,7.5]
[null,null,null,null,"Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3625358945796999,1.3910050765236599,1.4194457892856698,1.4478580613349199,1.47624192111212,1.5045973970295499,1.53292451747105]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3706301672207675,1.3992684730178599,1.427878140509149,1.4564591983329491,1.4850116750989246,1.5135355993881412,1.5420309997530561]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.23351880310023,1.25716271353397,1.2807829800572799,1.3043796263140701,1.3279526759246001,1.35150215248552,1.3750280795698799]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2408466375740927,1.2646310068816966,1.2883915918199964,1.3121284161733617,1.3358415037023701,1.3595308781438498,1.3831965632108891]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Bundarra","Substation Rating","MVA","Non-Coincident",3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.83703941095303303,0.84089025577732701,0.84294124255049807,0.84403361239027597,0.84461541617490499,0.84492528892265395,0.84509032930625694]
[null,null,null,null,"Coincident",0.61496773049610598,0.61779692261191377,0.61930377003710069,0.62010632747040684,0.62053377514890984,0.62076143675950091,0.62088269091888271]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2204452182376422,1.2260599420971003,1.2290503831291844,1.2306431128502209,1.2314914117924352,1.2319432217171575,1.2321838588297578]
[null,null,null,null,"Coincident",0.89665362972561469,0.90077873296929822,0.90297579168674769,0.90414596046138684,0.90476920050056464,0.90510114248607498,0.90527793709941395]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.79003779702639498,0.78912807595226997,0.78859142333862808,0.78827484715289298,0.78808809602408703,0.78797792985972703,0.78791294185217098]
[null,null,null,null,"Coincident",0.58043593250918823,0.57976756600574941,0.57937329061613496,0.57914070403069695,0.57900349911973747,0.57892256071326886,0.57887481442200317]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1519145203808889,1.1505881016719037,1.1498056353894281,1.1493440515177102,1.1490717590555282,1.1489111312920737,1.1488163755350247]
[null,null,null,null,"Coincident",0.84630454558595924,0.84533003388139871,0.84475516069427381,0.84441603784974639,0.84421598624487793,0.84409797401050313,0.84402835753593652]
[null,"Bungendore","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.1136186451744603,8.1431925892777404,8.1644232941236297,8.1796645087103403,8.1906059552503496,8.1984606607731205,8.2040994397612401]
[null,null,null,null,"Coincident",6.803731638623332,6.8285310762076987,6.8463342321837519,6.8591148592294076,6.8682898857190784,6.874876503948804,6.8796049414909719]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.1302257704556169,8.1598602471296591,8.1811344074287327,8.1964068180539975,8.2073706597768954,8.215241442476124,8.2208917630356666]
[null,null,null,null,"Coincident",6.8176576596311325,6.8425078572259066,6.8603474530760318,6.8731542397779135,6.8823480459047648,6.8889481457632069,6.8936862615707808]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.8993819120640003,7.9193981828876403,7.93473027838533,7.9464743816911598,7.9554701489350297,7.9623607412772897,7.9676388083437297]
[null,null,null,null,"Coincident",6.624081928307473,6.6408667121438505,6.6537235480127714,6.6635716479449343,6.6711151114582465,6.6768932658401727,6.6813192258786165]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9155505330941951,7.9356077736419204,7.950971251195126,7.9627393925785928,7.9717535725480486,7.9786582686996317,7.9839471390247461]
[null,null,null,null,"Coincident",6.6376402385099711,6.6544593777949066,6.6673425293058779,6.6772107865360972,6.6847696901691771,6.6905596713990123,6.6949946905855455]
[null,"Buronga Town","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.4384931042151,12.001371671792899,12.563687360803099,13.1254407341243,13.6866323540722,14.247262782400199,14.8073325802998]
[null,null,null,null,"Coincident",9.0718081892784888,9.5182241946384902,9.9641937839931156,10.409717403758393,10.854795499903922,11.299428517953343,11.743616902984659]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.930221503719311,12.517297609786533,13.103786639747668,13.689689180678851,14.275005819069126,14.859737140821057,15.443883731251166]
[null,null,null,null,"Coincident",9.461795373856086,9.9274023186019615,10.392543656403074,10.857219852866395,11.321431373133269,11.785178681879913,12.248462243317755]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.5264405549724,11.0362548164538,11.5403093266863,12.0386691578676,12.531398647026501,13.018561404328301,13.500220321287101]
[null,null,null,null,"Coincident",8.3484641517475939,8.7527951374972499,9.1525580950921555,9.5478046329470381,9.9385857764180727,10.324951974389847,10.7069531057885]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.97896080562197,11.510691428686899,12.036414695050235,12.556198474292811,13.070109869222444,13.57821522453637,14.080580135386604]
[null,null,null,null,"Coincident",8.7073555615036895,9.1290682973388861,9.5460166304485732,9.9582543878372025,10.365834788385609,10.768810449721151,11.167233395010854]
[null,"Burraga","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.502418384483581,0.502418384483581,0.502418384483581,0.502418384483581,0.502418384483581,0.502418384483581,0.502418384483581]
[null,null,null,null,"Coincident",0.16163870156541438,0.16163870156541438,0.16163870156541438,0.16163870156541438,0.16163870156541438,0.16163870156541438,0.16163870156541438]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.56007295319481165,0.56007295319481165,0.56007295319481165,0.56007295319481165,0.56007295319481165,0.56007295319481165,0.56007295319481165]
[null,null,null,null,"Coincident",0.18018740502374064,0.18018740502374064,0.18018740502374064,0.18018740502374064,0.18018740502374064,0.18018740502374064,0.18018740502374064]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.47611459470495598,0.47611459460912603,0.47611459460903,0.47611459460903,0.47611459460903,0.47611459460903,0.47611459460903]
[null,null,null,null,"Coincident",0.15317621182106167,0.15317621179023111,0.15317621179020022,0.15317621179020022,0.15317621179020022,0.15317621179020022,0.15317621179020022]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.53075069573667233,0.53075069562984545,0.53075069562973842,0.53075069562973842,0.53075069562973842,0.53075069562973842,0.53075069562973842]
[null,null,null,null,"Coincident",0.17075380989888844,0.17075380986451993,0.17075380986448552,0.17075380986448552,0.17075380986448552,0.17075380986448552,0.17075380986448552]
[null,"Burren Junction","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5349244856731499,2.5144471612850796,2.49574647017681,2.47866826985633,2.46307179138942,2.44882847909631,2.4358209309174401]
[null,null,null,null,"Coincident",2.1009079254060485,2.0839366217868864,2.0684377655558688,2.0542836056951894,2.0413574749939607,2.029552828405965,2.0187723648404665]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5371559332837781,2.5166605830819857,2.4979434300977408,2.4808501961502181,2.4652399883888827,2.4509841379687543,2.437965139483389]
[null,null,null,null,"Coincident",2.1027573161854556,2.0857710730384595,2.0702585734480836,2.0560919539396396,2.0431544446022301,2.0313394065999844,2.0205494531897985]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.25378166216607,2.23409785660645,2.2160214087610304,2.1994210635829199,2.1841762841666901,2.1701763765168298,2.1573196857866201]
[null,null,null,null,"Coincident",1.8679009110293618,1.8515872640800819,1.8366057714335478,1.8228476508479923,1.8102130031187842,1.7986100866994679,1.7879546515564289]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2557656248968505,2.2360644920436039,2.2179721318321231,2.2013571736741024,2.186098974557682,2.1720867430454542,2.159218734805799]
[null,null,null,null,"Coincident",1.869545190000339,1.8532171824463497,1.838222501866148,1.8244522702589505,1.8118065004806847,1.8001933702264925,1.7895285552989963]
[null,"Byabarra","Substation Rating","MVA","Non-Coincident",6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002]
[null,null,null,null,"Coincident",6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002,6.3250000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8556265764673501,1.9528563505104701,2.0374990608942403,2.11118418966905,2.1753302712151399,2.2311722008708896,2.2797850082710802]
[null,null,null,null,"Coincident",1.2789352895147676,1.3459480122210923,1.404285476602567,1.4550707545769483,1.4992815286700676,1.537768913673629,1.5712738417097696]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9896913405928582,2.0939457428065249,2.1847036948808656,2.2637124052070661,2.3324928940208212,2.3923692750163781,2.4444942462539681]
[null,null,null,null,"Coincident",1.3713354308443895,1.4431896690673409,1.5057418814488532,1.5601962792768882,1.6076011803973778,1.6488691906936275,1.6847947729342141]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4723460383270699,1.52123610294703,1.5623394169201699,1.59689618080883,1.6259490676694299,1.65037468337969,1.6709100162602999]
[null,null,null,null,"Coincident",1.0147706066910194,1.0484666259990425,1.0767958595975022,1.1006130787455353,1.120636914758403,1.1374715420999926,1.1516249079959175]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5787196626557458,1.6311419223113224,1.6752148564453657,1.7122682672663487,1.7434201585675655,1.7696104689908374,1.791629432572684]
[null,null,null,null,"Coincident",1.0880854555689257,1.1242159349875054,1.1545918907381476,1.1801298493429766,1.2016003615815445,1.2196512521370335,1.2348271662570907]
[null,"Byrock","Substation Rating","MVA","Non-Coincident",2.4,2.4,2.4,2.4,2.4,2.4,2.4]
[null,null,null,null,"Coincident",2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.107105839112639,0.115184492067641,0.123255066369688,0.131317570097433,0.13937201132145099,0.14741839810424401,0.15545673850025499]
[null,null,null,null,"Coincident",8.0605425311573664E-2,8.668523629832775E-2,9.275896747409508E-2,9.882662491868667E-2,0.10488821470583423,0.11094374290319392,0.11699321557235683]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11373094256290533,0.12230930600996931,0.13087909109358623,0.13944030639211957,0.14799296047535518,0.15653706190450653,0.16507261923222952]
[null,null,null,null,"Coincident",8.5591327908165857E-2,9.2047209677605754E-2,9.8496635565276214E-2,0.10493961202705904,0.11137614551238069,0.11780624246421624,0.12422990931910055]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.9731557952051103E-2,0.10708274261832701,0.11442657609993699,0.121763065748066,0.12909221890654601,0.13641404291186701,0.143728545093184]
[null,null,null,null,"Coincident",7.5055708561852882E-2,8.0588043413792484E-2,8.6114845930880396E-2,9.1636121645451721E-2,9.7151876084307809E-2,0.10266211476872464,0.10816684321445805]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.10590052029960066,0.11370641741946064,0.12150450864220114,0.12929480177371958,0.13707730461210557,0.14485202494765259,0.1526189705628655]
[null,null,null,null,"Coincident",7.9698329710008731E-2,8.5572870841449739E-2,9.1441537431759604E-2,9.7304335355479665E-2,0.10316127048127531,0.10901234867194472,0.11485757578442453]
[null,"Canowindra","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3921544622553705,6.4192730450797102,6.4444976530135003,6.46796056217564,6.4897848104571505,6.5100848427234599,6.5289671109554703]
[null,null,null,null,"Coincident",5.5997218703904847,5.6234785743675451,5.6455760986925494,5.6661303212718108,5.6852490270428362,5.7030324731911604,5.7195739148921891]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.633329598909901,6.6614713622529784,6.6876476912850942,6.7119958528855017,6.7346435271484637,6.755709476928943,6.7753041706269039]
[null,null,null,null,"Coincident",5.8109986308776334,5.8356516721322063,5.8585829331073915,5.8799126637674828,5.8997527157613199,5.9182071289647018,5.935372677058381]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7729741843873494,5.7935565975295304,5.8124807194907895,5.8298801560646494,5.8458777486455702,5.8605864414988602,5.8741100791560799]
[null,null,null,null,"Coincident",5.0573011006538513,5.075331921044417,5.0919100278861924,5.1071524639209338,5.1211668419491785,5.1340521045850824,5.1458992227990636]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.9907877316105882,6.0121467164597826,6.0317848430226242,6.0498407580214328,6.0664419376401248,6.0817055875160975,6.0957394702212593]
[null,null,null,null,"Coincident",5.2481123977298845,5.2668235185727266,5.2840271151780307,5.2998446462946154,5.3143877849396528,5.3277592068189525,5.3400533152255356]
[null,"Captains Flat","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.3803155977994801,3.3803155978970598,3.3803155978971597,3.3803155978971597,3.3803155978971597,3.3803155978971597,3.3803155978971597]
[null,null,null,null,"Coincident",2.5683255551956896,2.5683255552698294,2.5683255552699054,2.5683255552699054,2.5683255552699054,2.5683255552699054,2.5683255552699054]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.3845173573989822,3.3845173574966831,3.3845173574967831,3.3845173574967831,3.3845173574967831,3.3845173574967831,3.3845173574967831]
[null,null,null,null,"Coincident",2.5715180046117188,2.5715180046859509,2.5715180046860269,2.5715180046860269,2.5715180046860269,2.5715180046860269,2.5715180046860269]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2558423101593799,3.2558423102367802,3.2558423102368503,3.2558423102368503,3.2558423102368503,3.2558423102368503,3.2558423102368503]
[null,null,null,null,"Coincident",2.4737521592105916,2.4737521592693996,2.4737521592694529,2.4737521592694529,2.4737521592694529,2.4737521592694529,2.4737521592694529]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2598893484566567,3.2598893485341534,3.2598893485342235,3.2598893485342235,3.2598893485342235,3.2598893485342235,3.2598893485342235]
[null,null,null,null,"Coincident",2.4768270531313008,2.4768270531901817,2.476827053190235,2.476827053190235,2.476827053190235,2.476827053190235,2.476827053190235]
[null,"Carathool","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.72902009801088108,0.72902033074638495,0.72902039836177601,0.72902041800570994,0.72902042371275699,0.72902042537079403,0.72902042585249505]
[null,null,null,null,"Coincident",0.44976208322289501,0.44976222680687211,0.44976226852155082,0.44976228064069079,0.44976228416159975,0.44976228518451006,0.449762285481691]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.83408746991131133,0.83408773618897381,0.83408781354918737,0.83408783602423187,0.83408784255378632,0.83408784445078199,0.83408784500190636]
[null,null,null,null,"Coincident",0.51458240874427297,0.51458257302176891,0.51458262074842409,0.51458263461419107,0.51458263864253817,0.51458263981287178,0.5145826401528828]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.66328503374623304,0.66328536737195309,0.66328546846222003,0.66328549909307699,0.66328550837438105,0.66328551118666201,0.66328551203879793]
[null,null,null,null,"Coincident",0.40920745444773921,0.40920766027498495,0.40920772264167304,0.40920774153909173,0.40920774726510484,0.40920774900011508,0.40920774952583233]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.75887857843279494,0.75887896014110934,0.75887907580064362,0.75887911084606141,0.7588791214649997,0.75887912468259044,0.75887912565753735]
[null,null,null,null,"Coincident",0.46818299149836146,0.46818322698971093,0.46818329834477129,0.46818331996571172,0.46818332651696565,0.46818332850202798,0.46818332910351229]
[null,"Caroona","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1113666790462802,1.1315912531401999,1.14924284764617,1.16464879820693,1.17809479667467,1.1898301890531899,1.2000725994333601]
[null,null,null,null,"Coincident",0.79776321020648822,0.81228085002638106,0.82495154905294377,0.83601027594061805,0.84566210652389673,0.85408602679560663,0.861438252068501]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.263216779747653,1.286204711490049,1.3062681080176268,1.3237790300411441,1.3390622045371496,1.3524010465673881,1.3640429149995021]
[null,null,null,null,"Coincident",0.90676452011588948,0.92326575824780743,0.93766770129978161,0.95023742255428656,0.96120801810834999,0.97078292946668943,0.97913971621251383]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.99913462227032102,1.0168770147409301,1.0319758632620302,1.04482504507564,1.05575975132481,1.0650652310425301,1.0729842323219101]
[null,null,null,null,"Coincident",0.71720059519404233,0.72993647097740022,0.74077475333165532,0.74999817592063267,0.7578473462480072,0.76452702228300429,0.77021145389444035]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1356500459072558,1.1558166464580075,1.172978505965159,1.1875833185612223,1.2000120737830513,1.2105889952839846,1.2195899987183689]
[null,null,null,null,"Coincident",0.8151943398839212,0.82967036503173808,0.8419895216086537,0.85247317421473878,0.86139480543832891,0.86898715008008787,0.87544826640674989]
[null,"Cartwrights Hill 11kV","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3248766622696202,8.4363124793039095,8.5427898534226099,8.6445294152703411,8.7417419783208601,8.8346289757014489,8.9233828775803303]
[null,null,null,null,"Coincident",7.5223486015441354,7.6230418726203313,7.7192547006046839,7.8111864470839576,7.8990276028610609,7.9829601826690366,8.0631581023218395]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7164065247798952,8.83308331437056,8.9445684589752901,9.0510929657871468,9.1528775631139148,9.2501331577469106,9.3430612719786765]
[null,null,null,null,"Coincident",7.8761345173241741,7.98156352493793,8.0823013683478155,8.1785567853773689,8.2705292258616705,8.3584092649252657,8.4423789978708186]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6175617443771797,7.6590346966183001,7.6917667367314699,7.7176001146820301,7.7379888046026402,7.7540803384885306,7.7667803924797099]
[null,null,null,null,"Coincident",6.8832196871694533,6.9206945972431173,6.9502712295657236,6.9736142390039655,6.9920374348462211,7.0065777256317698,7.0180534792381941]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.9758256590796002,8.0192491386315279,8.0535206094996639,8.0805689650802215,8.1019165618153401,8.1187649016342807,8.132062255813171]
[null,null,null,null,"Coincident",7.2069465322721342,7.2461839364924359,7.2771515966051918,7.3015924583776721,7.3208821212713646,7.3361062609934287,7.3481217343355336]
[null,"Casino 66/11kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.296916512657898,26.296874056223203,26.296867512001299,26.296866503277002,26.296866347792498,26.296866323826201,26.296866320132001]
[null,null,null,null,"Coincident",28.538109368388689,28.538063293542763,28.538056191580054,28.538055096885763,28.538054928149869,28.53805490214101,28.538054898131964]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.541710073017853,26.541667221363369,26.541660616222405,26.541659598108065,26.541659441176183,26.541659416986786,26.541659413258198]
[null,null,null,null,"Coincident",28.803765815024441,28.803719311275543,28.803712143201857,28.803711038317246,28.803710868010619,28.803710841759642,28.803710837713282]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.864318371717303,22.864318369793999,22.864318369792102,22.864318369792102,22.864318369792102,22.864318369792102,22.864318369792102]
[null,null,null,null,"Coincident",24.812963071607548,24.812963069520329,24.812963069518272,24.812963069518272,24.812963069518272,24.812963069518272,24.812963069518272]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.077158454953757,23.077158453012551,23.077158453010636,23.077158453010636,23.077158453010636,23.077158453010636,23.077158453010636]
[null,null,null,null,"Coincident",25.043942759680679,25.043942757574033,25.043942757571955,25.043942757571955,25.043942757571955,25.043942757571955,25.043942757571955]
[null,"Clearwater Cr","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.561006443517599,16.584880748184698,16.606681748723599,16.6265894960327,16.6447684049419,16.661368612087202,16.6765272158651]
[null,null,null,null,"Coincident",10.896213585267654,10.91192153899255,10.926265374861135,10.939363556268244,10.951324258952427,10.962246264401299,10.972219775671991]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.616725717533171,16.640680346963638,16.662554696663229,16.682529423309074,16.700769494902453,16.717425553211982,16.732635157899786]
[null,null,null,null,"Coincident",10.932873743124629,10.948634546039628,10.963026641542909,10.976168891597746,10.988169835898436,10.999128588281527,11.009135655291074]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.0421863249388,14.0421863251205,14.042186325120699,14.042186325120699,14.042186325120699,14.042186325120699,14.042186325120699]
[null,null,null,null,"Coincident",9.2389711894924442,9.238971189611993,9.2389711896121245,9.2389711896121245,9.2389711896121245,9.2389711896121245,9.2389711896121245]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.089431063975978,14.089431064158289,14.089431064158489,14.089431064158489,14.089431064158489,14.089431064158489,14.089431064158489]
[null,null,null,null,"Coincident",9.2700555785412035,9.2700555786611538,9.270055578661287,9.270055578661287,9.270055578661287,9.270055578661287,9.270055578661287]
[null,"Clinton Street","Substation Rating","MVA","Non-Coincident",53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006]
[null,null,null,null,"Coincident",53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006,53.900000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.002434634879201,16.002434635872298,16.002434636018201,16.002434636039599,16.0024346360427,16.002434636043198,16.002434636043301]
[null,null,null,null,"Coincident",13.871686973051299,13.871686973912164,13.87168697403864,13.871686974057189,13.871686974059877,13.871686974060308,13.871686974060397]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.7611886803106,16.761188681350784,16.761188681503604,16.761188681526018,16.761188681529266,16.761188681529788,16.761188681529894]
[null,null,null,null,"Coincident",14.529411803548015,14.529411804449698,14.529411804582169,14.529411804601599,14.529411804604415,14.529411804604868,14.52941180460496]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.489595396362299,14.489595400311,14.489595401180601,14.489595401372,14.489595401414201,14.4895954014235,14.4895954014255]
[null,null,null,null,"Coincident",12.560284499860433,12.560284503283359,12.560284504037172,12.560284504203086,12.560284504239666,12.560284504247727,12.560284504249463]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.176618300970281,15.176618305106208,15.176618306017042,15.176618306217517,15.176618306261718,15.176618306271457,15.176618306273554]
[null,null,null,null,"Coincident",13.155829296229498,13.155829299814721,13.155829300604276,13.155829300778057,13.155829300816373,13.155829300824815,13.155829300826632]
[null,"Cobar CSA","Substation Rating","MVA","Non-Coincident",41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004]
[null,null,null,null,"Coincident",41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.9512986777743,20.5530080021102,21.1541156171217,21.754622124518299,22.354528125407398,22.9538342202957,23.552541009089097]
[null,null,null,null,"Coincident",13.460883962864314,13.866849485463698,14.272409042540438,14.677563040060178,15.082311883582328,15.486655978261016,15.890595728845016]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.610405808829132,21.231993082610686,21.852958769118395,22.47330348993971,23.093027866040096,23.712132517764477,24.330618064837115]
[null,null,null,null,"Coincident",13.905575045561054,14.324951964342166,14.743909506204455,15.162448090524958,15.580568136261068,15.998270061951507,16.41555428571624]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.715325130245301,18.153548709772799,18.591334065720797,19.028681636312797,19.4655918593343,19.902065172132701,20.3381020116183]
[null,null,null,null,"Coincident",11.952301441323938,12.247965239910744,12.543333374698983,12.838406141352401,13.133183835239228,13.427666751432115,13.721855184708806]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.30056508433946,18.753265730795174,19.205513676604461,19.657309374467886,20.108653276633547,20.559545834896955,21.009987500602101]
[null,null,null,null,"Coincident",12.347155292179743,12.65258658115355,12.957712438838403,13.262533170665536,13.567049081760908,13.871260476945126,14.175167660734163]
[null,"Cobar Elura","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.0636508343275,11.0636508342791,11.063650834279001,11.063650834279001,11.063650834279001,11.063650834279001,11.063650834279001]
[null,null,null,null,"Coincident",4.0949572049936744,4.0949572049757608,4.0949572049757235,4.0949572049757235,4.0949572049757235,4.0949572049757235,4.0949572049757235]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.080058791073325,11.080058791024854,11.080058791024754,11.080058791024754,11.080058791024754,11.080058791024754,11.080058791024754]
[null,null,null,null,"Coincident",4.101030234746843,4.1010302347289027,4.1010302347288663,4.1010302347288663,4.1010302347288663,4.1010302347288663,4.1010302347288663]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.5258341184077597,9.5260484867180502,9.5260560606955806,9.5260563282963986,9.5260563377511698,9.5260563380852314,9.52605633809703]
[null,null,null,null,"Coincident",3.5257695349276181,3.5258488784526345,3.5258516817871146,3.5258517808334342,3.5258517843329016,3.5258517844565467,3.5258517844609139]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.539961414769806,9.5401761009992008,9.5401836862093248,9.5401839542070075,9.5401839636758012,9.5401839640103585,9.5401839640221748]
[null,null,null,null,"Coincident",3.5309984304243334,3.5310778916198315,3.5310806991117993,3.5310807983050094,3.5310808018096664,3.5310808019334954,3.5310808019378688]
[null,"Cobar Peak","Substation Rating","MVA","Non-Coincident",48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006]
[null,null,null,null,"Coincident",48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006,48.400000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.6733223981512,14.027019516488702,14.346519413526101,14.6351284490952,14.895833307483201,15.1313319052769,15.344061310880202]
[null,null,null,null,"Coincident",9.4578819257911331,9.7025353820119111,9.9235345081563171,10.123166324158701,10.303496729331274,10.466391881421254,10.613537508632662]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.767326817807266,15.149323291591339,15.49438641966071,15.806087104155454,16.087650994386429,16.341991867620361,16.57174178244184]
[null,null,null,null,"Coincident",10.214608369160871,10.478836582313136,10.717517879162067,10.933122264423849,11.12788093030092,11.303809346080422,11.462728115313563]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.441373027685401,13.801113384293799,14.130913886998901,14.4332663186527,14.710455080274199,14.9645744506692,15.1975444095961]
[null,null,null,null,"Coincident",9.2974417858787071,9.5462753698220109,9.7743994586735372,9.983537626800409,10.175270001876044,10.351045203415742,10.512191287712341]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.516819146071517,14.905342378457895,15.261530265081696,15.588073956686166,15.887440629532367,16.161892125963533,16.413502043584568]
[null,null,null,null,"Coincident",10.041331391423412,10.310074184896484,10.556450513705967,10.782321855642923,10.989394764614859,11.179233764385216,11.353273169214839]
[null,"Cobar Town","Substation Rating","MVA","Non-Coincident",28.799999999999997,28.799999999999997,28.799999999999997,28.799999999999997,28.799999999999997,28.799999999999997,28.799999999999997]
[null,null,null,null,"Coincident",26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6654726457163296,6.6654726403968096,6.6654726392848698,6.6654726390524504,6.6654726390038608,6.6654726389937098,6.6654726389915808]
[null,null,null,null,"Coincident",5.0142295787102347,5.0142295747085246,5.0142295738720462,5.0142295736972038,5.0142295736606517,5.0142295736530151,5.0142295736514138]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.0170007023057508,7.0170006967056873,7.0170006955351045,7.0170006952904282,7.0170006952392763,7.0170006952285897,7.017000695226348]
[null,null,null,null,"Coincident",5.2786732982760176,5.2786732940632621,5.2786732931826688,5.2786732929986062,5.2786732929601259,5.278673292952087,5.2786732929504003]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3266856067779598,6.3266856033935399,6.3266856027339395,6.3266856026053899,6.3266856025803397,6.3266856025754592,6.3266856025745]
[null,null,null,null,"Coincident",4.759370533925142,4.7593705313791475,4.7593705308829506,4.7593705307862466,4.7593705307674021,4.7593705307637304,4.7593705307630092]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6603464908912891,6.6603464873283791,6.6603464866339923,6.6603464864986632,6.6603464864722923,6.6603464864671542,6.6603464864661444]
[null,null,null,null,"Coincident",5.0103733304717419,5.0103733277914744,5.0103733272691091,5.0103733271673052,5.0103733271474669,5.0103733271436015,5.0103733271428421]
[null,"Cobargo","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.2898758729865001,1.3072461384287601,1.32256232069322,1.33606732094424,1.3479753165942601,1.35847515796896,1.36773336330711]
[null,null,null,null,"Coincident",1.0262328017435871,1.0400526866993132,1.0522383310442065,1.0629829883677542,1.0724570594741285,1.0808107947888863,1.0881766771983998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3405434339094053,1.3585960200314877,1.374513836619252,1.3885493262276689,1.4009250793632757,1.4118373645735998,1.4214592410934745]
[null,null,null,null,"Coincident",1.066544210067736,1.0809069533539466,1.0935712614913491,1.1047379792557019,1.1145842009581322,1.1232660790049613,1.1309213003373517]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.21580904781563,1.23041550223981,1.2432290882500598,1.25446987137744,1.26433090522196,1.2729815470305199,1.2805703663044401]
[null,null,null,null,"Coincident",0.96730480169086419,0.97892578240783823,0.98912034651053371,0.99806357942479429,1.0059090757258604,1.0127915770316054,1.0188292861077271]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2635671928363506,1.2787474027938373,1.2920643187472327,1.3037466506126392,1.3139950353205589,1.3229854826329173,1.3308723980034827]
[null,null,null,null,"Coincident",1.0053014616773894,1.0173789256582129,1.0279739420126119,1.0372684736898161,1.0454221486072357,1.052575001162674,1.0588498772397883]
[null,"Coffs Harbour North","Substation Rating","MVA","Non-Coincident",78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009]
[null,null,null,null,"Coincident",78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009,78.100000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",29.758182204310497,30.6696780026661,31.437659686333099,32.084723411159999,32.6299075905373,33.089253058439901,33.476275035349801]
[null,null,null,null,"Coincident",22.926180434753849,23.628411404211167,24.220076799948455,24.718585062526962,25.138603690706699,25.492490800030737,25.790658732935128]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",30.145634653657833,31.068998155397264,31.846978984252221,32.502467498716697,33.054749992910239,33.520076152960414,33.9121371679364]
[null,null,null,null,"Coincident",23.22468001052221,23.936054048842266,24.535422946265189,25.04042180178482,25.465909085447024,25.824403815840071,26.126453904419414]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.838350796352501,25.600486349851501,26.242431395551801,26.7831402495178,27.238578089120299,27.622192346997501,27.945309765117702]
[null,null,null,null,"Coincident",19.135863479470338,19.72302492284399,20.217589672998304,20.634160438765637,20.98503704862889,21.280579620182973,21.529514456947382]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",25.161746889155545,25.93380547104756,26.584108661025468,27.131857560932936,27.593225215242121,27.981834142578588,28.30915855944011]
[null,null,null,null,"Coincident",19.385013011676072,19.979819315136794,20.480823313578941,20.902817843553876,21.258262877690385,21.557653422633734,21.809829398644151]
[null,"Coffs Harbour South","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.803907397022602,29.461373246117098,30.973800298294901,32.353880370176398,33.613194663756303,34.7623109522427,35.810872261517702]
[null,null,null,null,"Coincident",19.807249290361256,20.988012799406413,22.065451996286338,23.048608415061629,23.945732398093,24.764352330344039,25.511337815242523]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.726465322295951,30.438927335530877,32.001538037922316,33.427410371648364,34.728509813098405,35.915754783423139,36.999108272523571]
[null,null,null,null,"Coincident",20.464471117126674,21.684413390422058,22.797602960653762,23.813381367877394,24.740272708017251,25.586055164423641,26.357826279964502]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.9315939791163,24.546603965763101,25.08214895027,25.548496548939603,25.954587706688198,26.308208115310602,26.616137482912503]
[null,null,null,null,"Coincident",17.048648633854452,17.486776122470651,17.868293470477166,18.200515233803834,18.489810859820743,18.741726804142058,18.961092868804151]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.725665163953504,25.361081718972205,25.914396553692679,26.396217972891943,26.815783589845669,27.181137432400742,27.499284165297706]
[null,null,null,null,"Coincident",17.61433768207964,18.067002623332669,18.461179050079693,18.804424221603227,19.103318929098787,19.363593664420868,19.590238486654702]
[null,"Coleambally 33/11","Substation Rating","MVA","Non-Coincident",18,18,18,18,18,18,18]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5724184408505999,2.4691644530586201,2.3714828633369001,2.2790729412156603,2.19165018600886,2.10894545092727,2.0307041144613098]
[null,null,null,null,"Coincident",2.3454403431284883,2.2512970013181537,2.1622343753954087,2.0779782699319256,1.9982692872433723,1.9228620287866285,1.8515243396559]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8021987373100217,2.6897216264255119,2.5833146659443353,2.4826502627621569,2.3874185032776252,2.2973261992671787,2.2120959852519713]
[null,null,null,null,"Coincident",2.5549459075473728,2.4523932476232608,2.3553751365963058,2.2635928866360842,2.1767639294590113,2.0946209463906631,2.0169110453767973]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4664208485020001,2.3710097611110998,2.2804172121186697,2.1943998512712901,2.1127266182136002,2.0351781218126002,1.9615460508278899]
[null,null,null,null,"Coincident",2.2487954795165295,2.16180301748365,2.0792039286964341,2.0007763349826466,1.9263095636653413,1.8556035816526648,1.7884684581077819]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.6867329504379085,2.5827993040425925,2.4841146101510563,2.3904137813412745,2.3014451178797386,2.2169696316041394,2.1367604039519499]
[null,null,null,null,"Coincident",2.4496682783404458,2.3549052478035404,2.2649280269024334,2.1794949182817502,2.0983764310079969,2.0213546641096563,1.9482227212503072]
[null,"Colly Blue","Substation Rating","MVA","Non-Coincident",4.95,4.95,4.95,4.95,4.95,4.95,4.95]
[null,null,null,null,"Coincident",4.95,4.95,4.95,4.95,4.95,4.95,4.95]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1872039036625599,1.2383249172277202,1.28760894307961,1.3351219917220001,1.38092770163048,1.4250874244892,1.46766030736459]
[null,null,null,null,"Coincident",0.98405769751606853,1.0264312331390764,1.0672821138129978,1.1066650547760093,1.1446328051233325,1.1812362184588494,1.2165243210078156]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3128050526241002,1.3693344530889784,1.4238325203143434,1.476372248435919,1.5270240086107054,1.5758556432714059,1.6229325569937783]
[null,null,null,null,"Coincident",1.0881668375476672,1.1350233139219592,1.1801960448971696,1.223745534352128,1.2657301120131055,1.3062060115800707,1.345227446045441]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.05877264507578,1.0953820765217099,1.12916819935027,1.16034874629409,1.18912465860131,1.21568138098996,1.24019005673576]
[null,null,null,null,"Coincident",0.87760271684754165,0.90794779295865746,0.93595266569879787,0.96179781086566252,0.98564978601635722,1.0076623038380441,1.0279772227404966]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1707863103781853,1.2112688647461778,1.2486294163928469,1.2831087332525264,1.3149290153070603,1.3442953265408757,1.3713969164640143]
[null,null,null,null,"Coincident",0.97044937042386836,1.0040048271723148,1.0349724969364811,1.0635519490897205,1.0899273622738375,1.1142687113278096,1.1367328626808435]
[null,"Condobolin","Substation Rating","MVA","Non-Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,null,null,"Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.300233552935941,8.2239163431434203,8.1540252649125691,8.0900192192309603,8.03140266920059,7.9777218035749602,7.9285610233375499]
[null,null,null,null,"Coincident",8.2023686587512863,8.1269512761278655,8.0578842569950986,7.9946328822330317,7.9367074576305914,7.8836595226569344,7.8350783784653402]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.5142457940650242,8.4359608303532614,8.3642676888200072,8.2986113188198392,8.2384834065899302,8.183418439868225,8.1329901038822729]
[null,null,null,null,"Coincident",8.4138575630129484,8.336495627507686,8.2656477925149261,8.2007655517801137,8.1413465848745012,8.0869308682139103,8.0370971135410851]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.5487059711813895,7.4659727555945299,7.3900004790958,7.3202366393192699,7.2561738842635304,7.1973463226144201,7.1433261355873698]
[null,null,null,null,"Coincident",7.4597020526302744,7.3779443128944653,7.302867796587674,7.2339265156890482,7.1706191001914936,7.1124851519279844,7.0591018963623826]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.7433409139470157,7.6584745149056621,7.5805433782069773,7.5089807558293167,7.4432662142672159,7.3829218497199234,7.327508812573881]
[null,null,null,null,"Coincident",7.6520421288771558,7.5681763572409286,7.4911640769091239,7.4204452221702768,7.3555054957522747,7.2958726286361566,7.2411129455171022]
[null,"Coolamon","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8939723928308805,4.8448741948892904,4.7958250951456405,4.7468250445017404,4.6978739939084795,4.64897189436582,4.6001186969227001]
[null,null,null,null,"Coincident",4.0346240201236281,3.9941471328714426,3.953710722506508,3.9133147485519437,3.8729591705713302,3.8326439481687036,3.7923690409884774]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9271518666805818,4.8777207996004046,4.8283391635873061,4.779006909210227,4.729723987087521,4.6804903478869448,4.6313059423255662]
[null,null,null,null,"Coincident",4.0619774033109071,4.0212260964841304,3.9805155409641797,3.9398456959997539,3.8992165208802891,3.8586279749359496,3.818080017537552]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.49082321292979,4.44011385191566,4.3894552002625495,4.3388472072610806,4.2882898222526302,4.2377829946291801,4.1873266738333497]
[null,null,null,null,"Coincident",3.70226510299839,3.6604599619860632,3.6186966261147533,3.576975053579305,3.535295202616406,3.4936570315044633,3.4520604985636298]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.5212694720005011,4.4702163187083093,4.4192142185694152,4.3682631205306475,4.3173629735899368,4.2665137267961581,4.2157153292491696]
[null,null,null,null,"Coincident",3.7273652053916,3.6852766396944441,3.6432301625629897,3.6012257319086562,3.5592633056849925,3.5173428418875452,3.4754642985538919]
[null,"Cooma 11kV","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.214725880288601,14.512083841645799,14.709065310337101,14.839553489737801,14.925993930437199,14.983255437361601,15.0211876846839]
[null,null,null,null,"Coincident",8.8335396681168188,9.0183285532068655,9.1407398914361462,9.2218299186842163,9.2755471038257511,9.3111314546695656,9.3347039114474342]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.965684766712881,15.27875204286171,15.486139972122171,15.623521795390472,15.714528853669156,15.774815465533116,15.814751659920494]
[null,null,null,null,"Coincident",9.3002124107514472,9.494763626577905,9.62364191204321,9.7090158964407269,9.7655709412691447,9.8030352006464661,9.8278529818886433]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.783565471578001,14.1051206283321,14.331644152086001,14.491221461720301,14.603637679374501,14.6828306800627,14.738619172940901]
[null,null,null,null,"Coincident",8.5656011509943752,8.7654270397660827,8.9061968688639812,9.0053639232734266,9.0752233863648009,9.1244367527643941,9.1591057199336738]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.511746307751974,14.850289108479911,15.088779789010506,15.256787510863147,15.375142637106691,15.458519375709377,15.517255154721685]
[null,null,null,null,"Coincident",9.0181187975587047,9.2285014165955275,9.3767080654387893,9.4811140798799993,9.5546641934314049,9.6064774843838769,9.6429780006943915]
[null,"Coonabarabran","Substation Rating","MVA","Non-Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,null,null,"Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.9092868493389403,9.9232506469611312,9.93542399143106,9.9460364565779287,9.9552881800276296,9.9633536375443299,9.97038493342205]
[null,null,null,null,"Coincident",8.8811130947225116,8.8936280282187372,8.9045382834795053,8.9140496140743419,8.9223413916287857,8.9295699885455537,8.9358717269896939]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9816786749190776,9.9957444844031986,10.008006760664385,10.01869675467257,10.02801606614959,10.03614044548404,10.043223108160655]
[null,null,null,null,"Coincident",8.9459936456527256,8.958600006402655,8.9695899660163061,8.9791707811861627,8.9875231339286685,8.9948045390177231,9.0011523145134937]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.8922914782441396,8.90479841707978,8.9157167627928988,8.925248293623719,8.9335691585574803,8.9408331326739905,8.9471744590127091]
[null,null,null,null,"Coincident",7.9696397420155254,7.9808489783568382,7.9906344517778596,7.9991770042906065,8.0066345079077887,8.0131447822218451,8.0188281414020732]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9572536923255424,8.9698520000102739,8.9808501091806932,8.9904512721583973,8.9988329247766945,9.0061499655119484,9.0125376181097856]
[null,null,null,null,"Coincident",8.0278615675527494,8.0391526924390639,8.0490096531725328,8.0576146128979182,8.0651265969544426,8.0716844317690466,8.0774093104604905]
[null,"Coonamble","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3862688204069702,6.4310315549154806,6.46386029359397,6.4879367065980693,6.5055942129927402,6.5185441292458197,6.5280415252661497]
[null,null,null,null,"Coincident",6.1720143275117358,6.2152753061041661,6.2470026654082895,6.2702713329503679,6.287336443349071,6.2998518996979618,6.3090306652588817]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.4265741210506286,6.4716193640978075,6.5046552929556336,6.5288836580763503,6.5466526053019463,6.5596842516360114,6.5692415880397945]
[null,null,null,null,"Coincident",6.2109674157770485,6.2545014249601634,6.2864290233696778,6.3098445451496898,6.3270173576236548,6.3396118020710768,6.3488484970608807]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.8166190235310093,5.8456943267633701,5.8637142896181107,5.8748824985510097,5.8818042048705204,5.8860940617903994,5.8887527808321405]
[null,null,null,null,"Coincident",5.6214758508432059,5.6495756996239912,5.666991106342433,5.677784630305319,5.6844741186084633,5.6886200540704754,5.6911895750975301]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8533291253237651,5.8825879298886008,5.9007216211254168,5.9119603153497051,5.9189257062465517,5.9232426375000884,5.9259181363663744]
[null,null,null,null,"Coincident",5.6569543564622142,5.6852315502444393,5.7027568698436806,5.7136185143696956,5.7203502216656181,5.7245223231378537,5.7271080610390186]
[null,"Coopernook","Substation Rating","MVA","Non-Coincident",15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001]
[null,null,null,null,"Coincident",15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0764850307735903,3.07648503098399,3.0764850309842098,3.0764850309842098,3.0764850309842098,3.0764850309842098,3.0764850309842098]
[null,null,null,null,"Coincident",2.5278879566523211,2.5278879568252024,2.5278879568253831,2.5278879568253831,2.5278879568253831,2.5278879568253831,2.5278879568253831]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1810736815952709,3.1810736818128236,3.1810736818130509,3.1810736818130509,3.1810736818130509,3.1810736818130509,3.1810736818130509]
[null,null,null,null,"Coincident",2.6138264182960498,2.6138264184748086,2.6138264184749955,2.6138264184749955,2.6138264184749955,2.6138264184749955,2.6138264184749955]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.61571041507408,2.6157104152121802,2.6157104152123103,2.6157104152123103,2.6157104152123103,2.6157104152123103,2.6157104152123103]
[null,null,null,null,"Coincident",2.1492784103334803,2.1492784104469549,2.1492784104470619,2.1492784104470619,2.1492784104470619,2.1492784104470619,2.1492784104470619]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.7046345023087985,2.7046345024515936,2.7046345024517282,2.7046345024517282,2.7046345024517282,2.7046345024517282,2.7046345024517282]
[null,null,null,null,"Coincident",2.2223456045269856,2.2223456046443175,2.2223456046444281,2.2223456046444281,2.2223456046444281,2.2223456046444281,2.2223456046444281]
[null,"Cootamundra","Substation Rating","MVA","Non-Coincident",41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004]
[null,null,null,null,"Coincident",41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004,41.800000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.883543618851,11.9888388441308,12.094028774185301,12.199113514309801,12.3040931696942,12.4089678454232,12.5137376464764]
[null,null,null,null,"Coincident",11.684932861989981,11.788468278490731,11.891900159574961,11.995228608778161,12.09845372953218,12.201575625165431,12.30459439890298]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.883543618851,11.9888388441308,12.094028774185301,12.199113514309801,12.3040931696942,12.4089678454232,12.5137376464764]
[null,null,null,null,"Coincident",11.684932861989981,11.788468278490731,11.891900159574961,11.995228608778161,12.09845372953218,12.201575625165431,12.30459439890298]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.641484685441101,10.724613790590599,10.807659766635101,10.890622696703399,10.973502663841801,11.056299751012901,11.1390140410969]
[null,null,null,null,"Coincident",10.463632573706709,10.545372334480451,10.627030355493568,10.708606718485516,10.79010150511464,10.871514796956975,10.952846675507537]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.641484685441101,10.724613790590599,10.807659766635101,10.890622696703399,10.973502663841801,11.056299751012901,11.1390140410969]
[null,null,null,null,"Coincident",10.463632573706709,10.545372334480451,10.627030355493568,10.708606718485516,10.79010150511464,10.871514796956975,10.952846675507537]
[null,"Copeton","Substation Rating","MVA","Non-Coincident",4.95,4.95,4.95,4.95,4.95,4.95,4.95]
[null,null,null,null,"Coincident",4.95,4.95,4.95,4.95,4.95,4.95,4.95]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.92016961115455798,0.94117557531324803,0.95984576552724798,0.97643990993278995,0.99118885600113094,1.0042977819457699,1.0159490510348002]
[null,null,null,null,"Coincident",0.11361277852010358,0.11620637205398265,0.11851156900897654,0.12056043785904855,0.12238148120013963,0.12400003226065118,0.12543860732164369]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.96899493746071841,0.99111550379925728,1.0107763571674695,1.0282510071945301,1.0437825504011911,1.0575870520081987,1.0698565517019529]
[null,null,null,null,"Coincident",0.1196412116660683,0.12237242444868381,0.12479993797679981,0.12695752231687565,0.12887519244749399,0.13057962580917554,0.13209453342442479]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.88132922853093498,0.90040134682086903,0.91747782388278909,0.932767476789369,0.94645727270898306,0.95871461520496803,0.96968939130434295]
[null,null,null,null,"Coincident",0.10881718025739094,0.11117200302584199,0.1132804251936913,0.11516822927705474,0.11685849999774178,0.11837190657122564,0.1197269554569648]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.92809363657543376,0.94817774481544592,0.96616032066024338,0.98226126127207036,0.99667745452619461,1.0095851866240073,1.0211422977817164]
[null,null,null,null,"Coincident",0.11459115308737498,0.11707092563537648,0.11929122326519331,0.12127919654481685,0.1230591550996628,0.12465286487908661,0.1260798143179466]
[null,"Corowa","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.775030687987901,18.843048638355803,18.904349879847302,18.959597681171299,19.009389813873199,19.0542650201184,19.094708841788098]
[null,null,null,null,"Coincident",14.098307438423115,14.149382613295218,14.195414162498338,14.23690013934209,14.274289414838469,14.307986534407615,14.338356094988358]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.529707221195821,19.600459204430706,19.664224495604941,19.721693024013941,19.773486589081678,19.820165588121622,19.862235079737463]
[null,null,null,null,"Coincident",14.664999549799303,14.718127729885941,14.766009551962007,14.80916308896593,14.848055254618904,14.883106855349657,14.914697143346244]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.1161224847969,17.168359807551202,17.2148620684554,17.256258911845997,17.293110854297399,17.325916874061498,17.355121167272902]
[null,null,null,null,"Coincident",12.852621173011464,12.891846559546861,12.926765446322827,12.957850637862583,12.985523030148757,13.010157309588905,13.032087026299282]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.804117950341087,17.858454991721441,17.906826446110792,17.949887266875113,17.988220500975693,18.02234518347198,18.052723365297567]
[null,null,null,null,"Coincident",13.369241984485752,13.410044065047179,13.446366542840041,13.478701227122322,13.507485932108439,13.533110405008983,13.555921603238952]
[null,"Cowra","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",12.122999999999999,12.122999999999999,12.122999999999999,12.122999999999999,12.122999999999999,12.122999999999999,12.122999999999999]
[null,null,null,null,"Coincident",8.3160000000000007,8.3160000000000007,8.3160000000000007,8.3160000000000007,8.3160000000000007,8.3160000000000007,8.3160000000000007]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.313064026081701,21.302019387765998,21.292305081630197,21.283760868501499,21.276245810094998,21.2696359442123,21.263822239963702]
[null,null,null,null,"Coincident",18.382761914338108,18.373235787248213,18.364857086905602,18.357487605187817,18.351005781209341,18.345304696153779,18.340290309629552]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.458493834590453,21.447373833125027,21.437593241368376,21.42899072675484,21.421424389306356,21.414769420967794,21.408916046876577]
[null,null,null,null,"Coincident",18.508196790421277,18.498605661751281,18.490169789301227,18.482750021884787,18.476223969145074,18.470483982704575,18.465435380486575]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.3241920923879,19.293916702244001,19.266030516925799,19.240344990565802,19.2166864565332,19.194894953227902,19.174823142537999]
[null,null,null,null,"Coincident",16.667337084268571,16.641224213392853,16.617172059053321,16.595017998279026,16.574612241611124,16.555816820336801,16.538504653646427]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.456050822420487,19.42556884798698,19.397492381131318,19.371631589442256,19.347811621273774,19.325871423526937,19.305662652727431]
[null,null,null,null,"Coincident",16.781066749677063,16.754775697484643,16.730559423138924,16.708254194010227,16.687709198550522,16.668785526616723,16.651355230262613]
[null,"Crescent Head","Substation Rating","MVA","Non-Coincident",10.799999999999999,10.799999999999999,10.799999999999999,10.799999999999999,10.799999999999999,10.799999999999999,10.799999999999999]
[null,null,null,null,"Coincident",9.9,9.9,9.9,9.9,9.9,9.9,9.9]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9436617851190099,1.9786902754687401,2.0136837373281202,2.0486422057256402,2.0835657156547698,2.1184543020739603,2.1533079999067399]
[null,null,null,null,"Coincident",1.3132571955539554,1.3369245935309952,1.3605683241100579,1.3841884109585409,1.4077848777201805,1.4313577480150514,1.4549070454396331]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9837690917960691,2.0195203922641269,2.0552359414317167,2.0909157750501377,2.1265599288349479,2.162168438465963,2.1977413395873557]
[null,null,null,null,"Coincident",1.3403561535574497,1.3645119264133809,1.3886435434964561,1.4127510289624474,1.4368344069429779,1.460893701545521,1.4849289368534673]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.85941008215933,1.89732713326576,1.9352062673210901,1.97304752224236,2.0108509359087101,2.0486165461613899,2.0863443908038199]
[null,null,null,null,"Coincident",1.2563315740304044,1.2819506609419975,1.3075441287666836,1.3331120031235415,1.3586543096060437,1.3841710737820607,1.4096623211939037]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8977788616324593,1.9364783280791806,1.9751390950594621,2.0137612012727582,2.0523446853798424,2.0908895860028158,2.1293959417251691]
[null,null,null,null,"Coincident",1.2822558763516669,1.3084036110884198,1.3345251980904407,1.3606206635054561,1.3866900334550574,1.4127333340347068,1.4387505913137781]
[null,"Crookwell","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.0462563065922206,5.0723158456658801,5.0825502800353197,5.0865696775605906,5.0881482265925095,5.0887681744903004,5.0890116483312902]
[null,null,null,null,"Coincident",3.7135216698323865,3.7326987898945321,3.7402302729386538,3.7431881329645633,3.7443497814581734,3.7448059988622728,3.7449851703766828]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.079996423978546,5.1062302015081933,5.1165330650251093,5.1205793369174524,5.1221684403933789,5.1227925333669599,5.1230376351149509]
[null,null,null,null,"Coincident",3.7383508995512829,3.7576562410597276,3.7652380808646959,3.7682157176396296,3.7693851331102133,3.7698444008605168,3.7700247703457705]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8760874449040399,4.9100167530126004,4.9256332949942001,4.9328210744408896,4.9361293723621102,4.9376520728312396,4.9383529216586206]
[null,null,null,null,"Coincident",3.5882950231826221,3.6132634776661887,3.6247556341348877,3.6300450948977878,3.6324796593103534,3.6336002090496504,3.6341159611537113]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.9086897846944559,4.9428459498568138,4.9585669066615248,4.9658027448090696,4.9691331625659521,4.9706660440662169,4.9713715788865933]
[null,null,null,null,"Coincident",3.6122869665051973,3.6374223642698911,3.6489913592273067,3.6543161862134439,3.6567670285326543,3.6578950704557491,3.6584142709650194]
[null,"Cudgen 11kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.874792267981601,15.046115811440901,15.2039838754679,15.349453232080599,15.4834976560985,15.607014443610801,15.720830418494799]
[null,null,null,null,"Coincident",13.479433794755639,13.634686003992437,13.777744950902148,13.909568274972855,14.031038404205834,14.142968462106326,14.246107710748928]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.880436921999502,15.051825478946757,15.20975345040546,15.355278009415173,15.489373300321363,15.612936959717207,15.726796125241341]
[null,null,null,null,"Coincident",13.484548941156197,13.639860065165776,13.782973299775438,13.914846647876226,14.036362872331289,14.148335405208215,14.251513792909957]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.516488781406501,13.911837360181099,14.1669109170805,14.331480926743799,14.437659271570201,14.506164103848899,14.5503624952742]
[null,null,null,null,"Coincident",12.248548576957621,12.606810722568481,12.837956614294258,12.987088817950891,13.083306899100499,13.145385503943219,13.185437780325891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.521617989353297,13.917116594152022,14.17228694581345,14.336919406148297,14.44313804330349,14.511668871647867,14.555884035383212]
[null,null,null,null,"Coincident",12.253196629696292,12.611594727851786,12.842828334320931,12.992017130343857,13.088271724122924,13.150373886420425,13.190441361754367]
[null,"Cudgen 33kV","Substation Rating","MVA","Non-Coincident",96,96,96,96,96,96,96]
[null,null,null,null,"Coincident",88,88,88,88,88,88,88]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.127266361423501,12.1307783699817,12.1310878693274,12.131115144273799,12.1311175479063,12.1311177597289,12.131117778395899]
[null,null,null,null,"Coincident",8.2736019680620672,8.275997970594954,8.2762091207684048,8.2762277285934065,8.2762293684269839,8.2762295129390147,8.2762295256742267]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.188403819939769,12.191933533665077,12.192244593296737,12.192272005744931,12.192274421494917,12.192274634385385,12.192274653146489]
[null,null,null,null,"Coincident",8.3153118622812237,8.3177199438351419,8.317932158484675,8.317950860117719,8.3179525082182266,8.3179526534587893,8.3179526662582042]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.5925720098778,11.671193840003099,11.7050082690532,11.719551502276699,11.725806395189,11.7284965593871,11.7296535709482]
[null,null,null,null,"Coincident",7.9088166893835741,7.9624549710103789,7.9855242364491055,7.9954460868838151,7.9997133712632396,8.0015486857636784,8.0023380353865612]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.651013901828424,11.730032089940304,11.764016988426112,11.778633538775779,11.784919964619291,11.787623690802191,11.788786535231491]
[null,null,null,null,"Coincident",7.9486875834374917,8.002596272930349,8.0257818379716994,8.0357537076524022,8.0400425047877899,8.041887071700172,8.0426804006889228]
[null,"Culcairn","Substation Rating","MVA","Non-Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,null,null,"Coincident",16.5,16.5,16.5,16.5,16.5,16.5,16.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0520712515158595,3.9805638106031203,3.9091278771312798,3.83776337959292,3.7664702465521001,3.6952484066443096,3.62409778857644]
[null,null,null,null,"Coincident",3.5634391300095349,3.5005546452068614,3.4377330448889785,3.3749742661714208,3.3122782462325819,3.2496449223136721,3.1870742317186926]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.1722429724554226,4.098614845182281,4.0250603460363985,3.9515794013896706,3.8781719376875907,3.8048378814492017,3.7315771592670646]
[null,null,null,null,"Coincident",3.6691195551887392,3.6043701138514765,3.5396854219555385,3.4750654147515045,3.4105100275546754,3.3460191957450331,3.2815928547672124]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6783902525511998,3.6106899676220099,3.5430573829777501,3.4754924309181403,3.4079950438105797,3.3405651540901298,3.2732026942593997]
[null,null,null,null,"Coincident",3.2348196632729667,3.1752832362322967,3.1158063456186684,3.0563889318956585,2.9970309355863627,2.9377322972733788,2.8784929575987075]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.787479767394017,3.7177717044068781,3.6481333494827273,3.5785646329135066,3.509065485060844,3.4396358363560378,3.3702756172999355]
[null,null,null,null,"Coincident",3.3307542660317973,3.2694521753460486,3.2082113867509867,3.1470318389445247,3.0859134706858597,3.0248562207954568,2.9638600281549432]
[null,"Cumnock","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6923914233103101,1.6753969096352199,1.6584193904738098,1.64145884883156,1.62451526773095,1.6075886302114399,1.5906789193294602]
[null,null,null,null,"Coincident",1.3550931907737402,1.3414857300856087,1.3278918768581693,1.3143116174839566,1.3007449383691161,1.2871918259333899,1.273652266610108]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6933748000815534,1.6763704116164138,1.6593830275397443,1.6424126308471503,1.6254592045512466,1.608522731681638,1.5916031952849099]
[null,null,null,null,"Coincident",1.3558805778689018,1.3422652104633457,1.3286634584251988,1.3150753081390893,1.3015007460032639,1.287939758429574,1.2743923318434662]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.5401529652208001,1.5232993524340599,1.5064625932601099,1.4896426708453301,1.47283956835297,1.4560532689631001,1.4392837558726201]
[null,null,null,null,"Coincident",1.2331962731401873,1.2197016314085614,1.2062204843186699,1.1927528183758656,1.1792986200990077,1.165857876020425,1.152430572685921]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5410478826904226,1.5241844769851542,1.5073379346855948,1.4905082389283311,1.4736953728668296,1.4568993196713875,1.4401200625291408]
[null,null,null,null,"Coincident",1.2339128311141208,1.2204103482193738,1.2069213678075243,1.1934458763760836,1.1799838604360784,1.1665353065120114,1.1531002011418685]
[null,"Currabubula","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3627745863907401,1.3730413285410601,1.38104555555066,1.38728586519157,1.39215097763373,1.3959439495272701,1.3989010519491001]
[null,null,null,null,"Coincident",1.0862966716740443,1.0944805106876305,1.1008608506548441,1.1058351344878656,1.1097132193201014,1.1127366780673167,1.1150938474412635]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4337621590882701,1.4445637006926162,1.4529848716725586,1.4595502419938724,1.4646687804439857,1.4686593300372579,1.4717704693227338]
[null,null,null,null,"Coincident",1.1428823790402043,1.1514925180983637,1.1582052129919025,1.1634386096222575,1.1675187057274541,1.1706996578706861,1.1731796133120902]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.20889315872725,1.2190516444035899,1.22714784424098,1.2336004252550499,1.23874306038999,1.24284168326251,1.2461082400005201]
[null,null,null,null,"Coincident",0.96363450555160501,0.97173205102218996,0.97818570449092512,0.98332919436026256,0.98742849844657876,0.99069559810438601,0.99329944011007876]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2718649750831588,1.2825526210825979,1.2910705557984263,1.2978592548091168,1.3032697722403253,1.3075818943166229,1.3110186075399577]
[null,null,null,null,"Coincident",1.0138306826742383,1.0223500331179312,1.0291398604479574,1.0345512771370822,1.0388641159119247,1.0423014003360058,1.0450408777032014]
[null,"Dareton","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.1266830816095812,9.2394883394743097,9.1132399127528014,9.003757357609409,8.9088141556068603,8.82647947137621,8.7550788857167809]
[null,null,null,null,"Coincident",7.520120729550948,7.6130689726843421,7.5090439504093087,7.4188335174298796,7.3406030874779518,7.2727617085117444,7.2139297079351605]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.5982805564526164,9.7169147309437154,9.5841427470095404,9.4690029672114395,9.3691538235959797,9.2825647099271684,9.2074746857720449]
[null,null,null,null,"Coincident",7.9087032972657392,8.0064543977308524,7.8970541545363773,7.8021823334034224,7.7199095506173565,7.6485626458512241,7.5866906555364428]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.9381620184855084,8.7995127042612502,8.6792761073836182,8.575007007247061,8.4845849101017787,8.4061709251201986,8.3381703673493188]
[null,null,null,null,"Coincident",7.3647848707203707,7.2505418787469953,7.151470428961245,7.0655557308856043,6.991050559502817,6.9264397223921366,6.870409245652537]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.4000181605213164,9.2542045056606845,9.1277549971519409,9.0180980640108999,8.9230036415199887,8.8405378189782535,8.7690235102590943]
[null,null,null,null,"Coincident",7.7453408642545929,7.6251946645055773,7.5210039567013105,7.4306498413365976,7.3522948101117747,7.2843453770011637,7.2254196719394725]
[null,"Darlington Point","Substation Rating","MVA","Non-Coincident",29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002]
[null,null,null,null,"Coincident",29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002,29.150000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.3093726528952798,4.49360565720177,4.6716585059911901,4.8437385145725305,5.0100460437959198,5.1707747333421903,5.3261117271866496]
[null,null,null,null,"Coincident",3.2197378778801307,3.357387143817419,3.4904189207575254,3.6189881038573057,3.743244392265654,3.8633324634252633,3.9793921415273679]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.3006745335797945,5.5272873779148508,5.7462984213379151,5.9579626687110165,6.1625265706758947,6.3602283106080781,6.5512980819449727]
[null,null,null,null,"Coincident",3.9603868007597423,4.1297000668170476,4.2933336647862381,4.4514781209641674,4.6043175703816512,4.7520299712005478,4.894787311918801]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8458165649908,3.9882726928951904,4.1305863646716698,4.2727577227763804,4.4147869095229799,4.5566740670828407,4.6984193374851406]
[null,null,null,null,"Coincident",2.8733930117091302,2.9798287804147541,3.0861581133516673,3.1923811169556493,3.2984978975560226,3.4045085613758017,3.5104132145317597]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7304848220007099,4.9057106913225148,5.0807613347749898,5.255636927584022,5.430337644800237,5.6048636612992455,5.779215151781754]
[null,null,null,null,"Coincident",3.5343708676249528,3.665290473350125,3.7960791594695658,3.9267370569028945,4.0572642964387837,4.1876610087351445,4.317927324319208]
[null,"Deniliquin","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.231978531556802,23.198761154286903,23.169687100715297,23.144239559080201,23.121966181421602,23.102471042777498,23.085407603339803]
[null,null,null,null,"Coincident",22.69169996105548,22.659255080931391,22.630857168140523,22.606001429799267,22.584246037667612,22.565204274340811,22.548537659076086]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",24.69523299333121,24.659923436291404,24.629018168105308,24.601967825882731,24.578291570755326,24.557568540626853,24.539430369054031]
[null,null,null,null,"Coincident",24.12092524930025,24.086436844749741,24.056250303730764,24.029829039234293,24.006703394691247,23.986462295495997,23.968745941866729]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.3583147477521,21.3229022354455,21.291825782148699,21.264554462307199,21.2406223591551,21.219620604762198,21.201190394730997]
[null,null,null,null,"Coincident",20.861609753618328,20.827020788109557,20.796667043028961,20.770029939927962,20.746654397314284,20.726141055814239,20.708139455318648]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.703557440197724,22.665914488647008,22.632880700597983,22.603891710417631,22.57845225580731,22.556127716496249,22.536536688972774]
[null,null,null,null,"Coincident",22.175567732286147,22.138800198213357,22.106534637793377,22.078219810175359,22.053371970788536,22.031566606810287,22.012431184578059]
[null,"Dorrigo","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5447787819811301,2.4384535111585501,2.3339457936660502,2.2312245597486897,2.1302592707664401,2.03101991011517,1.9334769743028]
[null,null,null,null,"Coincident",1.9114498283574477,1.831586139575172,1.7530876625847469,1.6759310600815045,1.6000933936950623,1.5255521171698405,1.4522850696621254]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6785134026558142,2.5666004674506659,2.456600602642494,2.3484811056814285,2.2422098330439555,2.1377551906767782,2.035086124603998]
[null,null,null,null,"Coincident",2.0119013959137702,1.927840666429723,1.8452168941019633,1.7640055151908927,1.6841823858562142,1.6057237749790665,1.5286063571068316]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4551695157569102,2.3413075516344901,2.22762059831132,2.1141083867881498,2.0007706484792398,1.8876071152116598,1.77461751922466]
[null,null,null,null,"Coincident",1.8441419673534447,1.7586172713290593,1.673224030488345,1.5879620427789367,1.5028311064590685,1.4178310200970461,1.332961582570775]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5841949407591502,2.4643492397834499,2.3446877468712239,2.2252101788866261,2.1059162531290498,1.9868056873323927,1.8678781996643945]
[null,null,null,null,"Coincident",1.9410563350071544,1.8510370979004065,1.7611562242827772,1.6714135014835354,1.5818087171588695,1.4923416592913354,1.4030121161893592]
[null,"Dubbo Phillip St","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.8748731651268,24.7589328958279,24.669302220598201,24.600010869191902,24.5464433671352,24.505031600466499,24.473017144821302]
[null,null,null,null,"Coincident",16.702419472040592,16.624570511819705,16.564387325143301,16.517861129440117,16.481892829884131,16.454086589691975,16.432590244210914]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.743162129986274,26.618513879574223,26.522151270463578,26.447655620473192,26.390064798486243,26.345542698503724,26.311123717866547]
[null,null,null,null,"Coincident",17.956896058872601,17.87320005966016,17.808496665672902,17.758476004794673,17.719806217005999,17.689911520267337,17.666800638511841]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.6418327062391,22.419407467966202,22.241711099661,22.099748795589502,21.986334571261303,21.8957275163527,21.823341195784401]
[null,null,null,null,"Coincident",15.203027768823025,15.053678680442113,14.934363126051563,14.839041476124773,14.762888647676128,14.702049863568021,14.653445527692881]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.342403636126903,24.103272599379661,23.912229905173763,23.759605170610172,23.637672690033433,23.540260367829582,23.462437293351954]
[null,null,null,null,"Coincident",16.344888827747521,16.184322506141676,16.056045461490484,15.953564442931411,15.871691967669335,15.806283735981332,15.754028851065918]
[null,"Dubbo South","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.937387568215598,19.597508225953902,20.2569687630345,20.915769839577901,21.573912115044898,22.231396248236297,22.8882228972946]
[null,null,null,null,"Coincident",17.086658707453992,17.682266541105001,18.27727876692239,18.871695980513852,19.465518776891852,20.058747750473355,20.651383495081365]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.471752943505923,20.150500543410278,20.828569395714759,21.50596017916682,22.182673571835569,22.858710251111514,23.534070893708282]
[null,null,null,null,"Coincident",17.568801176143335,18.181215562567704,18.793017534605678,19.404207704671506,20.014786684567397,20.624755085483272,21.23411351799832]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.787914292894701,17.348955010662401,17.909434687712299,18.469353885085301,19.0287131632608,19.5875130821582,20.145754201136597]
[null,null,null,null,"Coincident",15.147250955254613,15.653461816227397,16.159166466339176,16.664365411800983,17.169059158317211,17.673248211086992,18.176933074803909]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.261626946720362,17.838498820323213,18.414793822052427,18.990512528780069,19.565655516800852,20.140223361833691,20.714216639021391]
[null,null,null,null,"Coincident",15.574668222402199,16.095163078763754,16.615137440268914,17.134591827412713,17.65352676016925,18.171942757993097,18.689840339819025]
[null,"Dubbo West","Substation Rating","MVA","Non-Coincident",50.6,50.6,50.6,50.6,50.6,50.6,50.6]
[null,null,null,null,"Coincident",50.6,50.6,50.6,50.6,50.6,50.6,50.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.495211315632801,18.523191512266102,19.462438036804599,20.320610243571501,21.104706343186201,21.821120471473101,22.475694832270499]
[null,null,null,null,"Coincident",16.76719211914353,17.752395506554116,18.652557650357593,19.47501918011989,20.226487093534757,20.913089450553542,21.540425346402284]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.222092982127556,19.292783149219158,20.271052985147779,21.164880070986467,21.981553375260059,22.727732693922469,23.409502959567039]
[null,null,null,null,"Coincident",17.463826434106643,18.489962524024079,19.427524122306778,20.284156843065052,21.066846342739485,21.781975286633106,22.435375398180632]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.5566973403731,16.428120238639703,17.209053261159799,17.908893013908401,18.536060345041101,19.098101669066001,19.601779769360402]
[null,null,null,null,"Coincident",14.909344525169017,15.744505352246373,16.49294181206082,17.163659494473979,17.764728835234447,18.303382223799275,18.7861010273324]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.203038666803426,17.110666976773043,17.924045786119557,18.652962105968701,19.306186649363678,19.891579365199494,20.416184013353984]
[null,null,null,null,"Coincident",15.528789983659459,16.398649625333853,17.178181722197806,17.876766023535673,18.502808271236709,19.063841342200295,19.56661588796084]
[null,"Dunedoo","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0112734357518205,6.0256617686639498,6.0386939777105502,6.0504978797797806,6.0611892448094302,6.0708729312316603,6.0796439144002496]
[null,null,null,null,"Coincident",5.6258546113421559,5.639320421861072,5.6515170577560125,5.6625641408071772,5.6725700182467014,5.6816328254032156,5.6898414481904505]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0763850627638076,6.0909292441456344,6.1041026126892461,6.1160343697424544,6.126841539215123,6.1366301153225695,6.1454961021523138]
[null,null,null,null,"Coincident",5.6867915410946397,5.700403207702335,5.7127319525115814,5.7238986929962135,5.7340129499607642,5.7431739216951438,5.7514714568885301]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.2081459382824296,5.2150369855187897,5.2211955131815602,5.2266993882345494,5.2316182003691498,5.2360141418799104,5.2399427940091696]
[null,null,null,null,"Coincident",4.8742204387454535,4.8806696595779444,4.886433327063874,4.8915843156485819,4.8961877532106106,4.9003018445231792,4.9039786071815374]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.264558420493036,5.2715241087022564,5.2777493429889075,5.2833128337395356,5.2882849244122818,5.2927284809429,5.2966996866067531]
[null,null,null,null,"Coincident",4.9270159780889573,4.9335350542134844,4.9393611513612123,4.944567933323321,4.9492212334165959,4.9533798868642762,4.9570964746946844]
[null,"Dungog","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5896942947916699,9.5902807690123204,9.5907477883384313,9.5911196837146999,9.5914158302832888,9.5916516567970991,9.5918394494326211]
[null,null,null,null,"Coincident",8.6771316353652459,8.677662300249537,8.6780848776586144,8.6784213831858246,8.6786893482199563,8.6789027333019551,8.6790726554463404]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.6301834230256045,9.6307723734284156,9.6312413645801964,9.6316148301545468,9.6319122270983843,9.6321490493071202,9.6323376348313285]
[null,null,null,null,"Coincident",8.7137677871222259,8.7143006925532855,8.7147250541475891,8.7150629804516306,8.7153320768743416,8.7155463629001755,8.7157170024813517]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.35773495826942,8.3577599720124507,8.3577652973062388,8.3577664310331699,8.3577666723976503,8.3577667237828699,8.3577667347225102]
[null,null,null,null,"Coincident",7.5624064935818787,7.5624291269979507,7.5624339455326997,7.5624349713733068,7.5624351897693582,7.5624352362647214,7.5624352461633375]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.3930225693306415,8.3930476886854475,8.3930530364634244,8.3930541749771219,8.3930544173606787,8.3930544689628555,8.3930544799486846]
[null,null,null,null,"Coincident",7.5943361085271741,7.5943588375049229,7.5943636763842486,7.5943647065561102,7.5943649258742623,7.5943649725659359,7.5943649825063453]
[null,"Dunoon","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.8711442868476595,7.0065372193017801,7.0702111839687305,7.1001564233761298,7.1142393749852602,7.1208624486340302,7.12397721503915]
[null,null,null,null,"Coincident",4.9412531654961933,5.0386184263822615,5.0844083510782845,5.1059429023606056,5.1160703900559739,5.1208332479244865,5.1230731731416794]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.8884786382370438,7.0242131366034526,7.0880477363599619,7.1180685208702812,7.1321870005983978,7.1388267827721403,7.1419494070322411]
[null,null,null,null,"Coincident",4.9537188357104798,5.0513297272476967,5.0972351696234011,5.1188240477344662,5.1289770848031369,5.1337519582906594,5.135997534335309]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.0237101114707601,6.0254061135491606,6.0259712260814,6.0261595231231002,6.0262222642125201,6.0262431697151495,6.0262501354858191]
[null,null,null,null,"Coincident",4.3318369421102272,4.3330565898557456,4.3334629798211166,4.3335983900693238,4.3336435091344701,4.3336585429304044,4.3336635522323386]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0389065770638188,6.0406068577739518,6.0411733959579896,6.0413621680307692,6.0414250674018435,6.0414460256443538,6.0414530089880962]
[null,null,null,null,"Coincident",4.342765192279531,4.3439879169219546,4.3443953321177924,4.3445310839755962,4.344576316865993,4.344591388588813,4.3445964105280899]
[null,"Eden South","Substation Rating","MVA","Non-Coincident",38.4,38.4,38.4,38.4,38.4,38.4,38.4]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8610712086487702,4.8288743563901395,4.7989375466393502,4.7711021368031394,4.7452206201285296,4.72115584402788,4.6987802832732699]
[null,null,null,null,"Coincident",4.0178662877430273,3.9912543247190682,3.9665103755980868,3.9435033160455668,3.9221112259363831,3.9022207432697527,3.8837264634358468]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.9188673843779274,4.8862877245340561,4.8559949781917497,4.827828616561308,4.801639379093964,4.7772884825131374,4.7546468853673893]
[null,null,null,null,"Coincident",4.0656370971089748,4.0387087285798469,4.0136705838854523,3.9903899796758324,3.968743546244756,3.9486165737629815,3.9299024044023874]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.7083822975657501,4.6800566257132008,4.6539781248372698,4.6299685192937208,4.6078636766457501,4.5875124856357798,4.5687758231713298]
[null,null,null,null,"Coincident",3.8916629053977632,3.8682506250321631,3.846695719743416,3.8268508377092258,3.8085803170237589,3.791759258297259,3.7762726708292962]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7643630637363836,4.7357006110719988,4.7093120473406431,4.6850169772725847,4.6626493169625576,4.6420561585010889,4.6230967246782502]
[null,null,null,null,"Coincident",3.9379332074576943,3.9142425645229912,3.8924313801055459,3.8723505504293354,3.8538628006231921,3.8368417462939997,3.8211710295482857]
[null,"Edrom","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0678114023081298,2.06784966203496,2.0678662935613903,2.0678735232960097,2.0678766660660299,2.0678780322300598,2.0678786261024]
[null,null,null,null,"Coincident",0.13234743882226341,0.13234988758371735,0.13235095206180481,0.1323514147910746,0.13235161593976857,0.13235170337922761,0.13235174138921396]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4254310774236076,2.4254759540164943,2.4254954618986075,2.4255039419867859,2.425507628286256,2.4255092307228665,2.4255099273030423]
[null,null,null,null,"Coincident",0.15523639669393038,0.15523926895884052,0.15524051753413692,0.15524106029057502,0.15524129622712757,0.15524139878888976,0.15524144337255058]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9642562900031801,1.9642852721261799,1.9642975828406299,1.96430281205349,1.96430503326227,1.9643059767634499,1.9643063775337299]
[null,null,null,null,"Coincident",0.12571953558349902,0.12572139054461703,0.1257221784750471,0.12572251316365959,0.12572265532908763,0.12572271571658938,0.12572274136734266]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3039665244522096,2.3040005189169537,2.3040149587200127,2.3040210923042297,2.3040236976621453,2.3040248043380638,2.3040252744199541]
[null,null,null,null,"Coincident",0.14746222421596075,0.14746439998515226,0.1474653241849849,0.14746571675664835,0.1474658835090161,0.14746595434029366,0.14746598442724171]
[null,"Egansford","Substation Rating","MVA","Non-Coincident",8.25,8.25,8.25,8.25,8.25,8.25,8.25]
[null,null,null,null,"Coincident",8.25,8.25,8.25,8.25,8.25,8.25,8.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.43855649369463,1.43855608651301,1.43855597046911,1.4385559373974099,1.43855592797221,1.43855592528609,1.4385559245205699]
[null,null,null,null,"Coincident",1.3045464781223164,1.3045461088720642,1.3045460036383372,1.3045459736474609,1.304545965100274,1.3045459626643818,1.3045459619701745]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6231621273911843,1.6231616679571701,1.623161537021705,1.6231614997060131,1.6231614890713055,1.6231614860404837,1.6231614851767269]
[null,null,null,null,"Coincident",1.4719550090600662,1.4719545924250381,1.4719544736869832,1.471954439847468,1.4719544302034462,1.4719544274549632,1.4719544266716704]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2923922367754301,1.29239177192245,1.29239163569923,1.29239159577959,1.2923915840812998,1.2923915806531701,1.2923915796485701]
[null,null,null,null,"Coincident",1.171998283159468,1.1719978616102826,1.1719977380770583,1.171997701876168,1.1719976912676426,1.1719976881588632,1.1719976872478477]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.458241050430072,1.4582405259239053,1.4582403722195685,1.4582403271771609,1.4582403139776645,1.4582403101096131,1.4582403089760958]
[null,null,null,null,"Coincident",1.3223973023862059,1.3223968267408799,1.3223966873550077,1.3223966465085659,1.3223966345386804,1.3223966310309607,1.3223966300030374]
[null,"Ellerslie","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.21942631590424,3.2625164079941902,3.2193271782098298,3.1761811376552402,3.1330782431412199,3.0900184515217002,3.0470017196938102]
[null,null,null,null,"Coincident",2.6475221005215572,2.6829575973857276,2.6474405738111466,2.6119590672601287,2.5765130422156739,2.5411024631962529,2.5057272947558591]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.2421052761694149,3.2854989125528014,3.242005440108398,3.1985554611364253,3.1551489321434394,3.1117858096794331,3.0684660503379009]
[null,null,null,null,"Coincident",2.6661723327763793,2.7018574518236669,2.666090231758361,2.6303587789131093,2.594663057520715,2.5590030318497021,2.5233786662043687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1483322573721897,3.1071584838039898,3.0660258840093602,3.0249344168145198,2.9838840410868701,2.9428747157349497,2.9019063997083898]
[null,null,null,null,"Coincident",2.5890573081299628,2.5551977117959304,2.5213719750582335,2.4875800640572696,2.4538219449673035,2.4200975839964287,2.3864069473865319]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.170510401911105,3.1290465833836194,3.0876242286746631,3.0462432963204105,3.0049037448985079,2.9636055330280286,2.9223486193694286]
[null,null,null,null,"Coincident",2.6072956903924402,2.573197573165396,2.5391335540555806,2.5051035989648707,2.4711076738292475,2.4371457446187619,2.4032177773374932]
[null,"Emmaville 66/11kV","Substation Rating","MVA","Non-Coincident",3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.926886591054074,0.92688659399258799,0.92688659500291892,0.92688659535029394,0.92688659546972996,0.926886595510795,0.92688659552491404]
[null,null,null,null,"Coincident",0.51916794027978697,0.51916794192570814,0.51916794249161491,0.51916794268618671,0.51916794275308531,0.51916794277608658,0.51916794278399503]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.97611002725233631,0.97611003034690369,0.97611003141088948,0.97611003177671229,0.97611003190249102,0.97611003194573687,0.97611003196060575]
[null,null,null,null,"Coincident",0.546738983200457,0.54673898493378681,0.54673898552974676,0.54673898573465152,0.54673898580510272,0.54673898582932556,0.54673898583765401]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.87366826974430301,0.87366828113153305,0.87366828630203996,0.87366828864976898,0.87366828971578403,0.87366829019982006,0.87366829041960292]
[null,null,null,null,"Coincident",0.48935928134976497,0.48935928772798298,0.48935929062408856,0.48935929193909911,0.4893592925361957,0.48935929280731411,0.48935929293041891]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.9200654824661948,0.92006549445815744,0.92006549990325037,0.92006550237565843,0.92006550349828553,0.92006550400802689,0.92006550423948152]
[null,null,null,null,"Coincident",0.51534729929719736,0.51534730601413836,0.51534730906404513,0.51534731044889093,0.51534731107769705,0.51534731136321354,0.51534731149285595]
[null,"Emmaville 66/22kV","Substation Rating","MVA","Non-Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,null,null,"Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.102653130698362,0.10265659812683001,0.102659038277699,0.102660755497338,0.10266196396494801,0.102662814405934,0.102663412891046]
[null,null,null,null,"Coincident",2.6569045592517226E-2,2.6569943044591298E-2,2.6570574613051508E-2,2.6571019069899247E-2,2.6571331849751252E-2,2.6571551963888801E-2,2.6571706865917789E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.10828898885435051,0.10829264665144028,0.10829522077137659,0.10829703226974087,0.10829830708459222,0.10829920421645586,0.10829983555957401]
[null,null,null,null,"Coincident",2.8027738291714253E-2,2.8028685015666899E-2,2.8029351258473941E-2,2.8029820116874112E-2,2.8030150068953284E-2,2.8030382267788579E-2,2.8030545674242686E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.1090373385902298E-2,9.1094113441703692E-2,9.1096723295124998E-2,9.1098544480487709E-2,9.1099815324320502E-2,9.1100702133582498E-2,9.1101320959158794E-2]
[null,null,null,null,"Coincident",2.3576331935174714E-2,2.3577299949617429E-2,2.3577975441091178E-2,2.3578446806714469E-2,2.3578775731000604E-2,2.3579005258103709E-2,2.3579165424723453E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.60914134933636E-2,9.6095358885561935E-2,9.6098112025053431E-2,9.6100033197063506E-2,9.6101373812714566E-2,9.6102309309543887E-2,9.6102962109857706E-2]
[null,null,null,null,"Coincident",2.4870718786517639E-2,2.4871739946851327E-2,2.4872452524131478E-2,2.4872949768651734E-2,2.4873296751526126E-2,2.4873538880117244E-2,2.4873707840198468E-2]
[null,"Euberta","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.47760322620788,1.4474344437967699,1.41729583016808,1.3871873551530101,1.3571089886129502,1.3270607004394401,1.2970424605541]
[null,null,null,null,"Coincident",0.96612518636669076,0.94639944402096499,0.92669342741759075,0.90700711683081425,0.88734049255462122,0.86769353490271084,0.84806622420845001]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6167809241238498,1.5837704981575331,1.5507930826171927,1.5178486444923831,1.4849371508056926,1.4520585686126997,1.4192128650018958]
[null,null,null,null,"Coincident",1.0571259888502096,1.0355422487953101,1.0139800924804723,0.99243949832194278,0.97092044475756822,0.94942291024676517,0.92794687327047032]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3516866996853201,1.31979116099883,1.2879275178510299,1.25609573834638,1.22429579062123,1.1925276428438101,1.1607912632141599]
[null,null,null,null,"Coincident",0.88379514979424778,0.862940374499235,0.84210645397951955,0.82129336738032543,0.80050109386772728,0.77972961262864504,0.75897890287079683]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4790041282271085,1.4441043001823932,1.4092393719657266,1.3744093086772791,1.3396140754521151,1.3048536374601813,1.2701279599062314]
[null,null,null,null,"Coincident",0.96704116076387858,0.9442220424269494,0.92142574320835968,0.89865224028899016,0.87590151087253676,0.85317353218550318,0.83046828147715135]
[null,"Eucumbene","Substation Rating","MVA","Non-Coincident",0.72,0.72,0.72,0.72,0.72,0.72,0.72]
[null,null,null,null,"Coincident",0.66,0.66,0.66,0.66,0.66,0.66,0.66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.19921064549884201,0.204910560946684,0.20948369658691701,0.213152798308748,0.216096578792036,0.21845842215065001,0.220353367810593]
[null,null,null,null,"Coincident",4.6407025371889336E-2,4.7734846584170709E-2,4.880017931854317E-2,4.9654913242378799E-2,5.0340680286781118E-2,5.0890882432821881E-2,5.1332318637694961E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.21166131084251963,0.21771747100585176,0.22257642762359933,0.22647484820304475,0.22960261496653825,0.23211207353506563,0.23412545329875506]
[null,null,null,null,"Coincident",4.9307464457632413E-2,5.0718274495681379E-2,5.185019052595212E-2,5.2758345320027475E-2,5.3486972804704935E-2,5.4071562584873251E-2,5.4540588552550895E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.18420091186314,0.188939612976915,0.192726165555237,0.19575188506869501,0.19816964591705499,0.20010160540433,0.201645375733396]
[null,null,null,null,"Coincident",4.2910439695390573E-2,4.4014341659394975E-2,4.4896436294117714E-2,4.5601291408048271E-2,4.6164519787495771E-2,4.6614578531690515E-2,4.69742068469843E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.19571346885458624,0.20074833878797219,0.20477155090243931,0.20798637788548846,0.21055524878687093,0.21260795574210062,0.21424821171673325]
[null,null,null,null,"Coincident",4.5592342176352475E-2,4.6765238013107162E-2,4.7702463562500068E-2,4.8451372121051293E-2,4.9049802274214252E-2,4.952798968992117E-2,4.9910094774920817E-2]
[null,"Eulomogo","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.936293715945698,19.8367347376184,19.7372753182695,19.6379153583399,19.538654758370299,19.439493419000598,19.3404312409704]
[null,null,null,null,"Coincident",18.88406876031755,18.789764441810448,18.695554427621921,18.601438623447535,18.507416935077394,18.413489268395551,18.319655529380519]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.796733827444577,20.692877935175638,20.589125898799043,20.485477614458773,20.381932978402919,20.278491886983048,20.175154236654734]
[null,null,null,null,"Coincident",19.699095387693326,19.600720943640965,19.502444874032726,19.404267080494044,19.306187464748977,19.208205928619581,19.110322374026449]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.7138653173593,17.4832719275411,17.252909131112798,17.0227766974809,16.792874396282603,16.563201997385498,16.333759270887299]
[null,null,null,null,"Coincident",16.778938725028183,16.560515908277711,16.342311514344065,16.124325324804328,15.906557121454103,15.689006686307224,15.471673801595498]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.478386570201494,18.237840889106234,17.997535753692155,17.757470923413464,17.517646157965018,17.278061217282016,17.038715861539707]
[null,null,null,null,"Coincident",17.503109030356736,17.2752591979595,17.04763721539474,16.820242854812523,16.593075888590857,16.366136089335406,16.13942322987922]
[null,"Ewingsdale","Substation Rating","MVA","Non-Coincident",108,108,108,108,108,108,108]
[null,null,null,null,"Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.385405683496,17.482809558907999,17.508338014899497,17.515028734981801,17.5167822971727,17.517241886024102,17.517362339072999]
[null,null,null,null,"Coincident",14.531632588876445,14.61304784923839,14.634385869747277,14.639978324002362,14.641444043120098,14.641828191551957,14.641928872518662]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.588082644891177,17.686622042928072,17.712448106578758,17.719216826268347,17.72099083127565,17.721455777958418,17.721577635234421]
[null,null,null,null,"Coincident",14.701040607926615,14.783404997568701,14.80499177414562,14.810649424557514,14.812132230851843,14.812520857639761,14.812622712333024]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.550951712504201,16.5509532123044,16.550953213804203,16.550953213805702,16.550953213805702,16.550953213805702,16.550953213805702]
[null,null,null,null,"Coincident",13.834152257411244,13.834153511022798,13.834153512276412,13.834153512277666,13.834153512277666,13.834153512277666,13.834153512277666]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.74390071020709,16.743902227491777,16.743902229009066,16.743902229010583,16.743902229010583,16.743902229010583,16.743902229010583]
[null,null,null,null,"Coincident",13.995429134928807,13.995430403154813,13.995430404423043,13.995430404424312,13.995430404424312,13.995430404424312,13.995430404424312]
[null,"Failford","Substation Rating","MVA","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.3120394494743399,4.3120409715609904,4.31204156372916,4.3120417941123295,4.3120418837429497,4.3120419186137697,4.3120419321802705]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.5085532937609782,4.5085548852141324,4.5085555043693564,4.5085557452518463,4.5085558389672293,4.508555875427227,4.5085558896119977]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.6876673293918798,3.6876673332315097,3.68766733402573,3.6876673341900101,3.6876673342239901,3.68766733423102,3.6876673342324797]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.8557264790913064,3.8557264831059208,3.8557264839363365,3.8557264841081031,3.8557264841436316,3.8557264841509822,3.8557264841525085]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Finley Town","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1.048,1.048,1.048,1.048,1.048,1.048,1.048]
[null,null,null,null,"Coincident",1.3520000000000001,1.3520000000000001,1.3520000000000001,1.3520000000000001,1.3520000000000001,1.3520000000000001,1.3520000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.8805154001102,14.5180303283244,14.168552611073501,13.831615494592599,13.5067689740319,13.1935791924413,12.891627861322]
[null,null,null,null,"Coincident",13.145721912538621,12.825495910749231,12.516760845996359,12.219104379390521,11.932128968342925,11.655451335617364,11.388701957434819]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.236188597620496,14.865039429123982,14.507208516179855,14.162217948702372,13.829606965852479,13.508931340656956,13.199762786710085]
[null,null,null,null,"Coincident",13.459930178885305,13.132050154172655,12.815935722192799,12.511164688356546,12.217330008035697,11.934039242924255,11.660914036907725]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.7893635221539,13.5389536616686,13.3098401520274,13.100211824299601,12.9084115421826,12.732923102147501,12.572359247673099]
[null,null,null,null,"Coincident",12.181778207211615,11.960561515344008,11.758158412819304,11.572968879580438,11.403528970836559,11.24849924440991,11.106654172288943]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.118956072121625,13.862560929986318,13.627971162811303,13.413332311213402,13.21694763011628,13.037264675784122,12.872863033572537]
[null,null,null,null,"Coincident",12.472946348221576,12.24644214809074,12.039201218600684,11.849585296109737,11.67609544470538,11.517360206942284,11.372124762310966]
[null,"Forbes Town","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.315383240249101,15.3153832534946,15.3153832589924,15.315383261274301,15.3153832622215,15.315383262614599,15.315383262777798]
[null,null,null,null,"Coincident",14.514796619845958,14.51479663239907,14.514796637609482,14.514796639772101,14.514796640669786,14.514796641042336,14.514796641197005]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.413173015358744,15.413173028688817,15.413173034221721,15.413173036518192,15.41317303747144,15.413173037867049,15.413173038031289]
[null,null,null,null,"Coincident",14.607474594334168,14.607474606967433,14.607474612211112,14.60747461438754,14.607474615290958,14.607474615665886,14.607474615821541]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.8930471472537,13.874259119593701,13.857865552792299,13.843561282150601,13.8310800350205,13.820189474164799,13.8106868728207]
[null,null,null,null,"Coincident",13.166810820793975,13.149004906564139,13.133468286666123,13.119911748386764,13.108082938045319,13.097761663453827,13.088755795059583]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.981755208606497,13.962847218097981,13.946348977245293,13.931953372851954,13.919392432100688,13.908432334265063,13.898869058157961]
[null,null,null,null,"Coincident",13.250881813264661,13.232962207048093,13.217326384763695,13.203683287055243,13.191778948946393,13.181391772306918,13.172328400823714]
[null,"Forest Hill","Substation Rating","MVA","Non-Coincident",22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002]
[null,null,null,null,"Coincident",22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002,22.990000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.5512057951184897,6.36264988921043,6.1791917709107702,6.0006936167003992,5.82702132924965,5.6580444366772795,5.4936359945329798]
[null,null,null,null,"Coincident",5.6170301972770975,5.4553616051913938,5.2980638767041164,5.1450188413756628,4.9961115236162454,4.8512300563101363,4.7102655967750788]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2901626462314892,7.0803381856716427,6.8761865282511625,6.677554304361121,6.4842922908853051,6.2962552990959049,6.1133020655799353]
[null,null,null,null,"Coincident",6.2506147734599065,6.0707104370749558,5.8956699849173599,5.7253619172675805,5.5596582896256104,5.3984346165922847,5.2415697783491595]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.03871358871677,5.9079174053726797,5.7869846374663103,5.6751714791647103,5.5717902154607604,5.4762049923316702,5.3878279058723599]
[null,null,null,null,"Coincident",5.1776173182964635,5.0654721446431212,4.9617839030561246,4.8659148514227599,4.7772753401299761,4.6953201853812683,4.6195453160039071]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.7198628180107818,6.5743132077702926,6.4397395773779582,6.3153142218785359,6.2002718540237014,6.0939048973167962,5.9955591340118932]
[null,null,null,null,"Coincident",5.7616374070330112,5.6368425858213307,5.5214586138761659,5.414775813639916,5.3161380247479277,5.2249385682661389,5.1406165152679675]
[null,"Forster","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.496069813214,16.496069902350797,16.496069936149699,16.496069948965602,16.496069953825202,16.496069955667799,16.496069956366501]
[null,null,null,null,"Coincident",11.330129644779358,11.330129706001911,11.330129729216283,11.330129738018735,11.330129741356494,11.330129742622059,11.330129743101955]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.245648088171478,17.245648181358632,17.24564821669335,17.245648230091607,17.245648235172027,17.245648237098351,17.245648237828799]
[null,null,null,null,"Coincident",11.844968580983133,11.844968644987624,11.844968669256856,11.844968678459288,11.844968681948716,11.844968683271787,11.844968683773487]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.999865525744401,14.0289004479925,14.054384872525,14.0767529673385,14.0963858087609,14.113617873696699,14.1287427379772]
[null,null,null,null,"Coincident",9.6156413747170326,9.6355836662459833,9.653087340584495,9.6684506008648707,9.6819351848372897,9.6937708239913789,9.7041591574003778]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.636016752627427,14.666371016220387,14.69301344815681,14.716397944944491,14.736922898947194,14.754937985636342,14.770750120873183]
[null,null,null,null,"Coincident",10.052574290004316,10.073422755467558,10.091721793439021,10.107783157344629,10.12188047824815,10.134253926594402,10.145114303897769]
[null,"Galloway St","Substation Rating","MVA","Non-Coincident",34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996]
[null,null,null,null,"Coincident",31.35,31.35,31.35,31.35,31.35,31.35,31.35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.975799264974299,10.6506715915892,10.360929251929099,10.1027210762987,9.8726150378073196,9.6675526348803302,9.4848082385581289]
[null,null,null,null,"Coincident",8.5059142318212366,8.2539500661653964,8.029408469605702,7.8293049014878004,7.6509796442213158,7.4920624510985947,7.3504410416744097]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.978440853245051,10.653234930119064,10.363422857043883,10.105152537448229,9.8749911184421695,9.6698793623496151,9.4870909842232454]
[null,null,null,null,"Coincident",8.5079613832609056,8.2559365764099599,8.0313409385514554,7.8311892107300345,7.6528210352307537,7.4938655948894723,7.3522101008902165]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.627226658248899,10.347842072389499,10.098996149024901,9.8773508016814908,9.6799328197642698,9.504093985106099,9.3474755480535503]
[null,null,null,null,"Coincident",8.2357809481495678,8.019266299180309,7.8264181949121969,7.6546497187519611,7.5016567219352455,7.3653869150521389,7.2440123380824142]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.629784354195529,10.350332527761914,10.101426713681704,9.8797280220910402,9.6822625268207716,9.506381372346798,9.3497252413262455]
[null,null,null,null,"Coincident",8.2377630855618769,8.0211963271704843,7.8283018093995391,7.6564919930525024,7.503462174816578,7.3671595713493829,7.24575578268845]
[null,"Ganmurra","Substation Rating","MVA","Non-Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,null,null,"Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.49758298896570896,0.47628761137889303,0.45524297061681002,0.43444611444463699,0.41389412538786202,0.39358412032301404,0.37351325007319702]
[null,null,null,null,"Coincident",0.32769924459868516,0.31367449032975603,0.29981486684278719,0.28611842984880009,0.27258325795133448,0.25920745237691034,0.24598913670865399]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.51429286546082598,0.49228234459684089,0.47053098082409089,0.44903572276553894,0.42779355497178273,0.40680149749804062,0.38605660548610288]
[null,null,null,null,"Coincident",0.33870406997699914,0.32420833515426273,0.30988327655019415,0.29572688458252844,0.28173717333029719,0.26791218025523938,0.25424996592648191]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.45415635523458703,0.43691436296644703,0.42030603145958101,0.40430807303619898,0.38889805586436998,0.374054372504809,0.35975620961361698]
[null,null,null,null,"Coincident",0.29909924141382316,0.28774397411782798,0.27680602445005986,0.26627005556301908,0.25612129425396007,0.24634551025036858,0.23692899625672906]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.46940787462679329,0.45158686023024558,0.43442078624740271,0.41788558295159367,0.40195806520309879,0.38661589993967194,0.37183757486183544]
[null,null,null,null,"Coincident",0.30914361892398884,0.29740701802476993,0.28610174915174091,0.27521196041401597,0.26472238249383184,0.2546183072363884,0.24488556702654457]
[null,"Geurie","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.5384513715180501,1.53845137147736,1.53845137147208,1.5384513714714001,1.5384513714713099,1.5384513714713,1.5384513714713]
[null,null,null,null,"Coincident",1.4707208079920981,1.4707208079531995,1.470720807948152,1.470720807947502,1.4707208079474159,1.4707208079474063,1.4707208079474063]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6072570233539378,1.6072570233114278,1.6072570233059118,1.6072570233052015,1.6072570233051073,1.6072570233050969,1.6072570233050969]
[null,null,null,null,"Coincident",1.5364972801874124,1.5364972801467738,1.5364972801415007,1.5364972801408217,1.5364972801407315,1.5364972801407215,1.5364972801407215]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.3751087627207501,1.37510876232219,1.37510876223502,1.3751087622159601,1.3751087622117899,1.37510876221088,1.3751087622106799]
[null,null,null,null,"Coincident",1.3145693832298995,1.314569382848886,1.3145693827655538,1.314569382747333,1.3145693827433462,1.3145693827424765,1.3145693827422853]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4366090847432016,1.4366090843268164,1.4366090842357477,1.4366090842158354,1.4366090842114787,1.4366090842105281,1.436609084210319]
[null,null,null,null,"Coincident",1.3733621439054506,1.3733621435073968,1.3733621434203376,1.3733621434013019,1.3733621433971368,1.3733621433962282,1.3733621433960281]
[null,"Gilgandra","Substation Rating","MVA","Non-Coincident",26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002]
[null,null,null,null,"Coincident",26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002,26.400000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.2159615692239001,7.2533136046994997,7.2836738265092702,7.3083510109411796,7.3284089484392094,7.3447123017567204,7.3579638800618907]
[null,null,null,null,"Coincident",7.0151344838781018,7.0514469766199523,7.0809622445316158,7.1049526394100528,7.1244523453976827,7.1403019608596479,7.1531847351153885]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.4082880372005651,7.4466356136010772,7.4778050240645912,7.5031399275926827,7.5237324677541118,7.5404703530920125,7.5540751246931981]
[null,null,null,null,"Coincident",7.202108323015481,7.239388649829821,7.2696905859040539,7.2943203949295965,7.3143398250791707,7.3306118791214061,7.3438380169672355]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4848621245702294,6.5230957363095801,6.5532327947958704,6.5769878692679704,6.5957124426510001,6.6104718006478995,6.6221056383874402]
[null,null,null,null,"Coincident",6.3043822333106547,6.341551767208931,6.3708500826450214,6.393944030762353,6.412147481428641,6.4264960724307807,6.4378061293821061]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6577026553532095,6.6969553046017367,6.7278956037868962,6.7522838204294349,6.7715074584247938,6.7866601964537123,6.7986041099745602]
[null,null,null,null,"Coincident",6.4724124474513163,6.51057265807402,6.5406518592550569,6.5643613285930096,6.5830499544279917,6.5977809773210732,6.6093924803492925]
[null,"Ginkgo","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.5887304898213497,8.5887300139536098,8.5887298023734608,8.5887297083007592,8.5887296664741903,8.5887296478772797,8.5887296396087205]
[null,null,null,null,"Coincident",8.4951746755572248,8.4951742048730434,8.4951739955976073,8.4951739025496256,8.4951738611786674,8.4951738427843306,8.4951738346058399]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9138489082509302,9.9138483589635964,9.9138481147396522,9.9138480061528771,9.9138479578730667,9.913847936406917,9.9138479268626387]
[null,null,null,null,"Coincident",9.8058587683574832,9.8058582250534574,9.8058579834898101,9.8058578760858541,9.8058578283319502,9.8058578070996276,9.8058577976593142]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.7969213967362601,7.7969210038929004,7.7969208254122693,7.7969207443231099,7.7969207074818492,7.7969206907437503,7.7969206831391205]
[null,null,null,null,"Coincident",7.7119906458075258,7.711990257243353,7.7119900807068857,7.7119900005010189,7.7119899640610647,7.7119899475052911,7.7119899399834981]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9998749836612841,8.9998745302078049,8.9998743241901629,8.9998742305901054,8.9998741880647639,8.9998741687442152,8.9998741599662999]
[null,null,null,null,"Coincident",8.9018406311606881,8.9018401826466125,8.9018399788730918,8.9018398862926063,8.9018398442304871,8.9018398251203941,8.9018398164380947]
[null,"Girilambone","Substation Rating","MVA","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0628152038957301,2.2496874096704302,2.4363727432393598,2.6228713914747201,2.8091835410618402,2.9953093784993796,3.1812490900994699]
[null,null,null,null,"Coincident",0.86258700282378198,0.94072950225167329,1.0187938591801384,1.0967801517516751,1.174688458030638,1.2525188560033247,1.330271423578034]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5162895139516612,2.7442423479970244,2.9719672292083468,3.1994643855384579,3.4267340447122328,3.6537764342268417,3.8805917813519222]
[null,null,null,null,"Coincident",1.0522118636595954,1.147532642531611,1.2427581006247566,1.337888333259809,1.4329234356622238,1.5278635029622396,1.6227086301949494]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8989134509929,2.0319760866495202,2.16038369277807,2.28429911975197,2.4038795208284802,2.5192765514551003,2.6306365616035903]
[null,null,null,null,"Coincident",0.79404983016429509,0.84969131460852099,0.90338625146036367,0.9552027382475381,1.0052064901911206,1.053460923547533,1.1000272360349541]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3163567902792721,2.4786709491865713,2.6353067506886614,2.7864628450021045,2.9323309328146694,3.0730960084058032,3.2089365942619663]
[null,null,null,null,"Coincident",0.96860797681928934,1.0364812810218635,1.1019801227491415,1.1651875695946672,1.2261837831363611,1.2850461205997981,1.3418492329649798]
[null,"Glen Innes","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.441652718028001,8.4416527180808405,8.4416527180808902,8.4416527180808902,8.4416527180808902,8.4416527180808902,8.4416527180808902]
[null,null,null,null,"Coincident",5.1047170553722259,5.1047170554041781,5.1047170554042083,5.1047170554042083,5.1047170554042083,5.1047170554042083,5.1047170554042083]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.5230898383666247,8.523089838419974,8.5230898384200255,8.5230898384200255,8.5230898384200255,8.5230898384200255,8.5230898384200255]
[null,null,null,null,"Coincident",5.1539625610828761,5.1539625611151365,5.1539625611151676,5.1539625611151676,5.1539625611151676,5.1539625611151676,5.1539625611151676]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.0910856317945008,8.0910856318277009,8.0910856318277293,8.0910856318277293,8.0910856318277293,8.0910856318277293,8.0910856318277293]
[null,null,null,null,"Coincident",4.892727076167497,4.8927270761875734,4.8927270761875912,4.8927270761875912,4.8927270761875912,4.8927270761875912,4.8927270761875912]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.1691408108306369,8.1691408108641568,8.169140810864187,8.169140810864187,8.169140810864187,8.169140810864187,8.169140810864187]
[null,null,null,null,"Coincident",4.9399275020787607,4.9399275020990308,4.9399275020990485,4.9399275020990485,4.9399275020990485,4.9399275020990485,4.9399275020990485]
[null,"Gloucester","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.9051754637788,10.9786880652339,11.046307469408301,11.108506109238601,11.1657185446923,11.218344498884701,11.2667516508037]
[null,null,null,null,"Coincident",9.231834343553869,9.2940668276666933,9.3513103942485714,9.4039649839170192,9.4523984757259445,9.4969492574065661,9.5379285895634656]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.9051754637788,10.9786880652339,11.046307469408301,11.108506109238601,11.1657185446923,11.218344498884701,11.2667516508037]
[null,null,null,null,"Coincident",9.231834343553869,9.2940668276666933,9.3513103942485714,9.4039649839170192,9.4523984757259445,9.4969492574065661,9.5379285895634656]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.0541972189512592,9.0975828057075709,9.1370645753876314,9.1729937918305211,9.2056901123009798,9.235444431435841,9.2625214692933096]
[null,null,null,null,"Coincident",7.6648788565443322,7.7016071559799988,7.7350306582874406,7.765446727739616,7.793125971895714,7.8183146491591504,7.8412368597044608]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.0541972189512592,9.0975828057075709,9.1370645753876314,9.1729937918305211,9.2056901123009798,9.235444431435841,9.2625214692933096]
[null,null,null,null,"Coincident",7.6648788565443322,7.7016071559799988,7.7350306582874406,7.765446727739616,7.793125971895714,7.8183146491591504,7.8412368597044608]
[null,"Goddard Lane","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.6222326689107,16.277987238391702,16.776751814996203,17.156110365364199,17.4446491198945,17.664110663031302,17.831032326619901]
[null,null,null,null,"Coincident",13.196532578952375,13.750466624319294,14.17178687500838,14.492241548494208,14.735978225264299,14.921363468539766,15.062366820516695]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.745327897356347,16.406249478508812,16.908944065682153,17.291291768011334,17.582104060816032,17.803294849020425,17.9715317702132]
[null,null,null,null,"Coincident",13.300514527430796,13.858813290652288,14.283453330106941,14.606433023036226,14.852090220550275,15.038936205024205,15.181050591524246]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.219066851436601,14.734236650796399,15.1322057182392,15.4396371298593,15.6771281325095,15.860590115273601,16.002314638493999]
[null,null,null,null,"Coincident",12.011239553531034,12.446417750209241,12.782593242869499,13.042289070298295,13.242904297334213,13.397879714987781,13.517598344683806]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.33110584864375,14.85033492336351,15.251439784153485,15.561293598553441,15.800655909219889,15.985563478870196,16.128404719075412]
[null,null,null,null,"Coincident",12.105881997290028,12.544489176282733,12.883313560426293,13.145055658569477,13.347251631310892,13.503448176241452,13.624110127701014]
[null,"Googong Dam","Substation Rating","MVA","Non-Coincident",21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998]
[null,null,null,null,"Coincident",19.8,19.8,19.8,19.8,19.8,19.8,19.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.34760228483308,1.3475903503390401,1.3475867040564402,1.3475855900270701,1.3475852496635901,1.3475851456741501,1.3475851139028001]
[null,null,null,null,"Coincident",0.26653132066014701,0.26652896023341455,0.26652823906476725,0.26652801872993803,0.26652795141220725,0.26652793084497978,0.26652792456118224]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3588115459823384,1.3587995122180154,1.3587958356058931,1.358794712310105,1.3587943691155053,1.3587942642610884,1.3587942322254667]
[null,null,null,null,"Coincident",0.26874830946415934,0.26874592940356312,0.26874520223628567,0.26874498006872682,0.26874491219105184,0.2687448914527476,0.26874488511668193]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0615177233568098,1.0615145559364201,1.0615136971824,1.0615134643562001,1.0615134012321401,1.0615133841178799,1.0615133794778502]
[null,null,null,null,"Coincident",0.20994897670827845,0.20994835024990191,0.20994818040391272,0.20994813435510795,0.20994812187031234,0.20994811848542169,0.20994811756770787]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0703473532183729,1.0703441594516028,1.0703432935545272,1.0703430587916953,1.0703429951425738,1.0703429778859583,1.0703429732073333]
[null,null,null,null,"Coincident",0.2116953175496597,0.21169468588044638,0.2116945146216902,0.21169446818985468,0.21169445560121142,0.21169445218816549,0.21169445126281822]
[null,"Googong Town","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.65,7.6,8.5500000000000007,9.5,10.45,11.4,12.35]
[null,null,null,null,"Coincident",5.5891050583657602,6.3875486381322961,7.1859922178988347,7.9844357976653706,8.7828793774319074,9.5813229571984451,10.379766536964981]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6551750972762651,7.605914396887159,8.5566536964980546,9.5073929961089494,10.458132295719844,11.408871595330739,12.359610894941634]
[null,null,null,null,"Coincident",5.5934545564656553,6.3925194931036051,7.1915844297415568,7.9906493663795075,8.7897143030174583,9.588779239655409,10.38784417629336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.39,7.34,8.2899999999999991,9.24,10.19,11.14,12.09]
[null,null,null,null,"Coincident",5.3705836575875487,6.1690272373540864,6.9674708171206232,7.7659143968871609,8.5643579766536977,9.3628015564202354,10.161245136186771]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.3949727626459136,7.3457120622568093,8.2964513618677032,9.2471906614785997,10.197929961089494,11.148669260700389,12.099408560311284]
[null,null,null,null,"Coincident",5.3747631001226361,6.1738280367605878,6.9728929733985376,7.7719579100364893,8.57102284667444,9.3700877833123908,10.169152719950342]
[null,"Goondiwindi 22kV","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.8979091894163,17.8979040523704,17.8979022995238,17.897901701423002,17.8979014973409,17.897901427704699,17.8979014039436]
[null,null,null,null,"Coincident",14.929557835171597,14.929553550099913,14.929552087961268,14.929551589054924,14.929551418819646,14.929551360732543,14.929551340912198]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.054375187990441,18.054370006035775,18.05436823786555,18.054367634536071,18.054367428669856,18.054367358424884,18.054367334456064]
[null,null,null,null,"Coincident",15.060074095491649,15.060069772959276,15.060068298038415,15.060067794770561,15.060067623047063,15.060067564452153,15.060067544458539]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.540238058038298,16.540245679160599,16.540245974695402,16.540245986155803,16.540245986600198,16.5402459866174,16.540245986618103]
[null,null,null,null,"Coincident",13.797055180110814,13.797061537277171,13.797061783797806,13.797061793357511,13.797061793728203,13.797061793742552,13.797061793743138]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.684835107728066,16.684842795475273,16.684843093593685,16.684843105154272,16.684843105602553,16.684843105619905,16.684843105620615]
[null,null,null,null,"Coincident",13.917670945521845,13.917677358263431,13.917677606939185,13.917677616582459,13.917677616956395,13.917677616970868,13.91767761697146]
[null,"Goondiwindi 33kV","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.91985466802128,5.9199636185128304,5.9200455949741295,5.9201072756523301,5.9201536853899794,5.9201886049760093,5.9202148791492801]
[null,null,null,null,"Coincident",4.5051435325679403,4.5052264463605756,4.5052888323050215,4.5053357726986736,4.505371091560562,4.5053976661567274,4.5054176613978987]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9370740860697193,5.9371833534717622,5.9372655683826583,5.9373274284749558,5.9373739732072499,5.9374089943658657,5.9374353449643191]
[null,null,null,null,"Coincident",4.5182478998549565,4.5183310548236575,4.5183936222336492,4.5184406991654935,4.518476120761366,4.5185027726565705,4.5185228260590371]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.2640610903074805,5.26416994885746,5.2642534506110694,5.2643175020140793,5.2643666337035402,5.2644043209796401,5.2644332296289207]
[null,null,null,null,"Coincident",4.0060697611632712,4.0061526049862879,4.0062161517127413,4.0062648962816887,4.0063022866105786,4.0063309674815972,4.0063529676187022]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2793729642688767,5.2794821394619138,5.2795658841018245,5.2796301218147939,5.2796793964163946,5.2797171933156184,5.2797461860531323]
[null,null,null,null,"Coincident",4.0177224441795145,4.0178055289750727,4.0178692605435042,4.0179181468985519,4.0179556459868184,4.0179844102835176,4.0180064744136743]
[null,"Goulburn North","Substation Rating","MVA","Non-Coincident",38.5,38.5,38.5,38.5,38.5,38.5,38.5]
[null,null,null,null,"Coincident",38.5,38.5,38.5,38.5,38.5,38.5,38.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.5729148731117295,8.9456941005105683,9.3026002660343199,9.6443092498683001,9.9714681529976303,10.2846965226351,10.584587525469701]
[null,null,null,null,"Coincident",6.9790855702802315,7.2825597287603703,7.5731118579507939,7.8512921821005923,8.117627496729682,8.3726221662318405,8.616759078999312]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.6672536791983301,9.044135075785503,9.4049687387869287,9.7504379859667019,10.081197039194178,10.39787226335679,10.701063352519352]
[null,null,null,null,"Coincident",7.0558854230749288,7.3626990979521043,7.6564485458351133,7.9376900457979822,8.2069561903691284,8.4647568941123037,8.7115803592616707]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6557036376715999,7.9894219420522807,8.3100039597113593,8.6179667795425594,8.9138071360632694,9.1980022106319108,9.4710104011267795]
[null,null,null,null,"Coincident",6.2323972159800771,6.5040724439642572,6.7650536115894164,7.0157616734188704,7.2566010138135821,7.4879600991915982,7.7102121046124186]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.7399491891112868,8.0773398251166828,8.4014496189459926,8.7128013496869539,9.0118972180655881,9.299219656480405,9.5752321071509954]
[null,null,null,null,"Coincident",6.300980296660966,6.5756451165203345,6.8394981955232756,7.0929651205374622,7.3364547258849706,7.5703597527793685,7.7950574828051886]
[null,"Grafton North","Substation Rating","MVA","Non-Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,null,null,"Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",22.0555090075365,22.346845597369601,22.4771089763147,22.5353527688432,22.561394925860498,22.5730389811783,22.578245309676799]
[null,null,null,null,"Coincident",17.676082671093216,17.909570351891901,18.013968135432638,18.060646817455346,18.081517944039366,18.090849911139014,18.095022451111717]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.429748761440976,22.726028775324966,22.858502474370251,22.917734552527293,22.944218595081214,22.956060227720634,22.961354897644185]
[null,null,null,null,"Coincident",17.976011946203787,18.213461465841554,18.319630679858328,18.36710140973025,18.388326679366418,18.39781699207802,18.402060332064092]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.877768423261401,18.119414792918199,18.242734911427402,18.305669238356099,18.337786702674599,18.354177304824301,18.362541970109501]
[null,null,null,null,"Coincident",14.327890257089337,14.521554398132899,14.620387601621099,14.670825447569753,14.696565545170115,14.709701566584453,14.716405311895736]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.181119919379505,18.426866565202289,18.552279189977686,18.61628139192182,18.64894382810828,18.6656125473902,18.674119145027849]
[null,null,null,null,"Coincident",14.571007118366541,14.767957369037386,14.868467582733711,14.919761262345002,14.945938120112098,14.959297034655751,14.96611452968801]
[null,"Grafton South","Substation Rating","MVA","Non-Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,null,null,"Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.980146127651199,19.980840859178798,19.9812899464936,19.981580244843602,19.981767899068799,19.9818892022322,19.981967614841697]
[null,null,null,null,"Coincident",15.08622369557469,15.086748260068202,15.087087348263386,15.087306541147091,15.087448231483121,15.087539822738076,15.087599029020147]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.881072757192555,20.881798814924156,20.88226815207689,20.882571540296823,20.882767656056163,20.882894428911801,20.882976377231572]
[null,null,null,null,"Coincident",15.766478013021908,15.767026230701843,15.767380608754411,15.767609685284848,15.767757764593014,15.767853485797776,15.767915361755822]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.026354054038102,17.0276303419996,17.0285489043425,17.029210006541401,17.0296858110644,17.030028254251601,17.030274715415501]
[null,null,null,null,"Coincident",12.85593129991136,12.856894974829657,12.857588545181684,12.858087717489761,12.858446978799638,12.858705544202119,12.85889163734814]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.794090970138704,17.79542480731952,17.796384788642559,17.797075700662269,17.797572959731323,17.797930844056165,17.798188418423354]
[null,null,null,null,"Coincident",13.435619295266672,13.436626423340448,13.437351267537801,13.437872948070902,13.438248408865958,13.43851863326508,13.438713117554475]
[null,"Grenfell","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8985456216051402,4.89289256129147,4.8876124216511494,4.88268060188022,4.8780741240387497,4.8737715259939094,4.8697527614252802]
[null,null,null,null,"Coincident",3.9840573612199788,3.9794596462458109,3.9751652330000695,3.9711541132963109,3.9674075988466622,3.9639082341908933,3.9606397153692985]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1558389380493841,5.1498889539651671,5.1443314780000904,5.1391406172069907,5.1342921867427398,5.129763597188215,5.1255337493014457]
[null,null,null,null,"Coincident",4.1933177030755884,4.1884784957432499,4.1839585208897319,4.1797367194100019,4.1757934214245207,4.1721102546349593,4.1686700587254224]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4983098055756701,4.4881560010135901,4.4786256407304901,4.4696804452059498,4.4612844852846703,4.4534040378639101,4.44600745044165]
[null,null,null,null,"Coincident",3.6585398357644139,3.6502816009872339,3.6425304223775057,3.6352551666526405,3.6284266121156876,3.6220173312838599,3.6160015807236139]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.7345809639304184,4.7238938365717145,4.7138628995473608,4.7044478627269468,4.6956109097967724,4.6873165463673487,4.6795314574070304]
[null,null,null,null,"Coincident",3.850702555151063,3.842010561299674,3.8338522564518946,3.8261948720672136,3.8190076515957054,3.8122617269416854,3.8059300025124361]
[null,"Gresford","Substation Rating","MVA","Non-Coincident",15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001]
[null,null,null,null,"Coincident",15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001,15.950000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4399998416741,2.3659823590178299,2.2920388938442202,2.21816937213578,2.1443737199490402,2.0706518634145001,2.0975214882934101]
[null,null,null,null,"Coincident",2.0287318231008609,1.9671901705294557,1.9057100596106253,1.8442914288027104,1.7829342166255966,1.7216383616606707,1.743979044694989]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4599920370214101,2.3853680904026811,2.3108187677305754,2.2363439943811372,2.1619436958050406,2.0876177975275332,2.1147075793016663]
[null,null,null,null,"Coincident",2.0453542843904113,1.9833083888599738,1.9213245392250704,1.8594026734397981,1.7975427295203048,1.7357446455447416,1.7582683774841399]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2063345743408198,2.1615228289827702,2.12130417569443,2.0852078340008902,2.05281127725108,2.0237352867212199,1.9976395126603901]
[null,null,null,null,"Coincident",1.8344514154975757,1.7971928008436531,1.7637531012114045,1.7337408873413565,1.7068048504963134,1.6826296902079279,1.6609324235190366]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.2244122278956997,2.179233316461755,2.1386851307040211,2.1022930327968394,2.0696310341072142,2.0403168087739494,2.014007218382539]
[null,null,null,null,"Coincident",1.8494820357572124,1.8119181417791648,1.7782044531916772,1.7479463335505518,1.7207895956622992,1.6964163556368652,1.6745413118896568]
[null,"Griffith","Substation Rating","MVA","Non-Coincident",110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001]
[null,null,null,null,"Coincident",110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001,110.00000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",30.507448920943599,30.975985801944898,31.444054146065099,31.911654421841298,32.378787097341601,32.845452640166499,33.311651517448503]
[null,null,null,null,"Coincident",24.392060526768116,24.766676575131342,25.140918007446125,25.514785198328692,25.888278522020276,26.261398352388248,26.634145062925796]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",31.876462004639702,32.366024344765663,32.855097122551392,33.343680827559467,33.831775948862401,34.319382975044135,34.806502394199612]
[null,null,null,null,"Coincident",25.486647297559305,25.878074134425393,26.26910954445453,26.65975391907374,27.050007649318228,27.439871125832553,27.829344738870304]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",27.8015217603315,28.184300615306899,28.566696691427403,28.948710371471702,29.330342037835997,29.711592072533897,30.0924608571971]
[null,null,null,null,"Coincident",22.228551566916529,22.534600264174763,22.840342912735803,23.145779818648215,23.450911287654748,23.75573762519225,24.060259136392215]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",29.049107133175536,29.449063080276254,29.848619071429955,30.247775506592415,30.646532785319756,31.044891306768335,31.442851469695469]
[null,null,null,null,"Coincident",23.226051489167684,23.545834034571673,23.865296797430329,24.184440097526053,24.503264254321717,24.82176958696056,25.139956414266763]
[null,"Gulargambone","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.55638531569091,1.5581986150762499,1.5597947024343499,1.56119959722188,1.5624362020693501,1.56352467614041,1.56448276376703]
[null,null,null,null,"Coincident",1.2673006135269325,1.2687771087112429,1.2700767370666191,1.2712206851675347,1.2722276016849869,1.2731139013976323,1.2738940327859121]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6381466455958733,1.6400552027350397,1.6417351370838091,1.6432138349746239,1.6445154021780588,1.645661056875741,1.6466694755596694]
[null,null,null,null,"Coincident",1.3338755050442948,1.3354295647035783,1.3367974662183364,1.3380015091538215,1.3390613218485508,1.339994181396007,1.3408152952962413]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.40859150200934,1.41076981555266,1.4127000221100701,1.4144103807339299,1.41592593180848,1.4172688636518702,1.4184588373625899]
[null,null,null,null,"Coincident",1.1469581836248661,1.1487318948402523,1.1503035827312766,1.1516962574831626,1.1529303084519331,1.1540238026733804,1.1549927493721652]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4825888041786861,1.4848815507036439,1.4869131564798297,1.4887133650876823,1.4903085323537659,1.491722012211443,1.4929744986124069]
[null,null,null,null,"Coincident",1.2072111463668853,1.2090780356573763,1.2107322887659402,1.2121981246680191,1.213497003830271,1.2146479424010626,1.2156677906149806]
[null,"Gulgong","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.8957759898073201,3.7456888084299997,3.6376601530177801,3.5599040762957204,3.5039373752002003,3.46365407177798,3.43465924980632]
[null,null,null,null,"Coincident",3.4953353741245556,3.3606754153272989,3.2637508535277076,3.193987200219397,3.1437732272845973,3.1076305805290678,3.081616090176146]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.9660660978792945,3.8132709465810057,3.7032931683538033,3.6241341662452875,3.5671576777598539,3.5261475569440126,3.4966295916562973]
[null,null,null,null,"Coincident",3.5584004738217181,3.4213108930231986,3.3226375556416574,3.2516151814152634,3.2004952155297541,3.1637004597841032,3.1372165991842449]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3510396720870701,3.15798397306932,3.00935024824817,2.8949170340689898,2.8068148182149897,2.73898485735912,2.68676252055283]
[null,null,null,null,"Coincident",3.0065916358091207,2.8333798249353497,2.7000239242073523,2.5973531180465894,2.5183067887866581,2.4574489616874335,2.4105944757939826]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4115012954762847,3.2149623607736872,3.0636468902340583,2.9471489980516452,2.8574571850827288,2.7884033922376608,2.7352388262817766]
[null,null,null,null,"Coincident",3.0608385051266174,2.8845014948220999,2.7487395007512792,2.6442162415542647,2.5637437073377574,2.5017878439923464,2.4540879791844699]
[null,"Gundagai South","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.4376840247868907,6.4723781577096497,6.5019173149941496,6.5270674409540899,6.5484806732175906,6.5667122525226294,6.9417164069403201]
[null,null,null,null,"Coincident",6.1568454599471938,6.1900260904270139,6.2182766267561496,6.2423295995701871,6.2628086975403132,6.2802449394931186,6.6388898522751383]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5673018239436747,6.6026944964554826,6.6328284018732271,6.6584849062081997,6.6803292773763348,6.6989279354593272,7.0814825090934814]
[null,null,null,null,"Coincident",6.2808087913555282,6.3146574882208473,6.3434768272948645,6.3680140881521377,6.3889055169538773,6.4066928241809,6.7725587754753098]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.9408569793378803,6.05285351487856,6.1647380538837098,6.2765107083498499,6.3881715901615195,6.4997208110913798,6.6111584828003096]
[null,null,null,null,"Coincident",5.6816920775546844,5.7888028581892268,5.8958065280431455,6.0027031942272053,6.109492963745077,6.2161759434934334,6.3227522402620409]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0604715493916634,6.1747230487351761,6.2888602965793554,6.4028834071756862,6.5167924946614164,6.6305876730596633,6.7442690562795109]
[null,null,null,null,"Coincident",5.7960885623376646,5.9053559358708902,6.0145140420305916,6.1235629900841291,6.2325028891896093,6.3413338483959869,6.4500559766431564]
[null,"Gunnedah 22kV","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",27.2204624588549,27.4819006803002,27.741637265931399,27.999683291269402,28.2560497597471,28.5107476031788,28.7637876822264]
[null,null,null,null,"Coincident",26.073399795365408,26.32382108338857,26.572612442054204,26.819784480163868,27.065347737468869,27.309312685119927,27.551689726113686]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",27.263322224059031,27.525172091000933,27.785317642831433,28.043769972510319,28.300540100795846,28.555638976714924,28.809077478030023]
[null,null,null,null,"Coincident",26.114453462068973,26.365269048962816,26.614452140106664,26.862013361006092,27.107963268007691,27.352312348749436,27.595071022607939]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",24.126857896348703,24.354649495914099,24.580041134054401,24.8030580962272,25.023725401488299,25.242067805298202,25.4581098022995]
[null,null,null,null,"Coincident",23.110158862596045,23.328351387960812,23.5442450856027,23.757864175457204,23.969232622284121,24.178374138355785,24.38531218611741]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.16484665080554,24.392996917843526,24.618743444616019,24.842111556393633,25.063126311625723,25.281812504751311,25.49819466898084]
[null,null,null,null,"Coincident",23.146546781580827,23.36508286027135,23.581316491637875,23.795271933751206,24.006973189104659,24.216444007306542,24.42370788774468]
[null,"Guyra","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.78834690962048,6.0791195336504398,6.2801906061515904,6.4192324995610299,6.5153808310062402,6.5818679983844603,6.6278442868913299]
[null,null,null,null,"Coincident",2.854454697424921,2.997845771855066,3.0970015889439222,3.1655684512931335,3.2129828617679443,3.2457702206122816,3.2684428825566574]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0986828006577714,6.4050448810172425,6.6168961592352895,6.7633926317424349,6.8646958508570775,6.9347476550224556,6.9831889119707728]
[null,null,null,null,"Coincident",3.0074931651917098,3.1585719953049347,3.2630439431178599,3.3352869428263241,3.3852434250795649,3.4197886423212291,3.4436768742472519]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.5127113424956899,5.78963765109566,5.9811339106205592,6.1135547614867001,6.2051246009583299,6.26844571274711,6.3122326541822202]
[null,null,null,null,"Coincident",2.7185282832618269,2.8550912112905404,2.9495253228037339,3.0148270964696535,3.0599836778742358,3.0912097339164615,3.1128027452920555]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8082693339597773,6.1000427438259486,6.3018058659383671,6.4413263159451812,6.5378055722448423,6.6045215762118676,6.6506561066388326]
[null,null,null,null,"Coincident",2.864279204944483,3.0081638050523205,3.1076608982074836,3.1764637550726924,3.2240413572186366,3.2569415641154591,3.2796922611878596]
[null,"Hallidays Point 11kV","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.4658398134228499,7.8483783517899202,8.2305343516186298,8.6123081954475094,8.99370026543256,9.374710943347619,9.7553406105847706]
[null,null,null,null,"Coincident",6.1141743309361098,6.4274555384531311,6.7404234647626398,7.0530784231458385,7.3654207265706537,7.6774506876920388,7.9891686188523083]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.4732317340301995,7.8561490234253561,8.2386833955311243,8.6208352332647848,9.0026049191607118,9.3839928353707354,9.7649993636645576]
[null,null,null,null,"Coincident",6.1202279688875318,6.4338193558179366,6.7470971513614151,7.0600616691093494,7.3727132223395362,7.6850521240164857,7.9970786867917658]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.0880521180629605,6.0880334954997197,6.0880273483164702,6.0880253191725,6.0880246493656793,6.08802442826694,6.0880243552837303]
[null,null,null,null,"Coincident",4.9858305181873463,4.9858152671772809,4.9858102329211258,4.9858085711469267,4.9858080226064052,4.9858078415368574,4.985807781767015]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.0940798924372803,6.0940612514358579,6.0940550981662884,6.0940530670132649,6.0940523965432689,6.0940521752256203,6.0940521021701501]
[null,null,null,null,"Coincident",4.990766984046938,4.9907517179368623,4.9907466786962953,4.9907450152767758,4.9907444661931439,4.99074428494432,4.9907442251152991]
[null,"Hammond Ave","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.112939472997002,18.769669039038501,18.479557216494999,18.234371901206099,18.027155806714301,17.852029046917,17.704022290625701]
[null,null,null,null,"Coincident",13.284170697544013,13.045585573232431,12.843947568911416,12.673535080270904,12.529512546510647,12.407793238282736,12.304923294193747]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.512820121545516,19.162367788436821,18.866186250457126,18.615871171479558,18.404319704798038,18.225528945416325,18.074425593869286]
[null,null,null,null,"Coincident",13.562101928450073,13.318525129551832,13.112668457764526,12.938690601453875,12.791654830285159,12.667388912417019,12.562366724816949]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.565395100289599,17.2404603361577,16.9661577414033,16.734597681371,16.539119904537802,16.374101976876499,16.234797566468501]
[null,null,null,null,"Coincident",12.208572481052343,11.982731297471307,11.792081267074632,11.631138814002536,11.495274827267407,11.38058151584324,11.283760010736971]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.932898047423315,17.601165002765253,17.321123453014216,17.084718696690462,16.885151136583094,16.71668070617994,16.574461770873334]
[null,null,null,null,"Coincident",12.464000061329678,12.233433831709181,12.038795024080802,11.874485335288405,11.73577880414995,11.61868588089102,11.519838677628274]
[null,"Hanwood","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.221399366481801,12.291425487273701,12.356151652132699,12.415978990416999,12.471278271843399,12.522392204269,12.5696375575652]
[null,null,null,null,"Coincident",10.510403455174348,10.570625919055383,10.62629042083412,10.67774193175862,10.725299313785323,10.769257295671339,10.809888299506071]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.308986061941585,12.379514036599161,12.444704072306315,12.504960173181653,12.560655766124942,12.612136015066259,12.659719960061082]
[null,null,null,null,"Coincident",10.585728013269764,10.646382071475278,10.702445502183432,10.754265748936222,10.80216395886745,10.846436972956983,10.88735916565253]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.632181738137501,11.7058834743279,11.7744826307257,11.838332473371599,11.897761810698499,11.953076686800999,12.0045619574746]
[null,null,null,null,"Coincident",10.00367629479825,10.067059787921993,10.126055062424102,10.180965927099574,10.232075157200709,10.27964595064886,10.323923283428156]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.715545707260818,11.789775639227248,11.858866422912566,11.923173856097428,11.98302910367517,12.038740403056405,12.090594651503165]
[null,null,null,null,"Coincident",10.075369308244303,10.139207049735433,10.198625123704806,10.253929516243788,10.305405029160646,10.353316746628508,10.397911400292722]
[null,"Harrington","Substation Rating","MVA","Non-Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,null,null,"Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0418830709292504,4.1182358260098502,4.1594779290972603,4.1817549388171704,4.1937879130088502,4.2002875496170704,4.2037983421581506]
[null,null,null,null,"Coincident",3.5366476870630938,3.6034563477586188,3.6395431879601028,3.659035571465024,3.6695644238827438,3.6752516059149367,3.6783235493883817]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.1348463815606227,4.2129552500080765,4.2551459214664966,4.2779353024099649,4.290245035008053,4.2968941632582629,4.3004857040277873]
[null,null,null,null,"Coincident",3.6179905838655451,3.686335843757067,3.7232526812831845,3.7431933896087193,3.7539644056320465,3.7597823928509801,3.7629249910243141]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.4018106688752399,3.4957724817410298,3.5609790233837999,3.6062303115755601,3.63763328175963,3.65942595498039,3.6745493844943198]
[null,null,null,null,"Coincident",2.976584335265835,3.0588009215234013,3.1158566454608247,3.1554515226286153,3.1829291215396762,3.2019977106078414,3.2152307114325298]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4800523142593702,3.5761752488210732,3.6428815409216271,3.6891736087417977,3.7212988472401012,3.7435927519449388,3.7590640203376888]
[null,null,null,null,"Coincident",3.0450457749769488,3.129153342718439,3.1875213483064235,3.2280269076490731,3.2561364913350888,3.2756436579518216,3.2891810177954777]
[null,"Hastings Point","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.9353966625556,15.4004263882585,16.8639910842357,18.326092215516898,19.7867312456669,21.2459096367866,22.703628849515297]
[null,null,null,null,"Coincident",8.5888423189865026,9.4917882208064714,10.393831176724621,11.294972089686839,12.195211861736148,13.094551394013312,13.992991586758272]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.095805923513142,15.577699491794149,17.05811116650688,18.537042429544872,20.014494761319913,21.490469640763024,22.964968545326812]
[null,null,null,null,"Coincident",8.68770781110209,9.601047452569583,10.51347375439561,11.424987629919798,12.335589991568513,13.245281750855485,14.154063818383243]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.986909530608701,11.161569261993799,11.325379547591599,11.479014329088201,11.6231056845204,11.7582464287453,11.8849925523756]
[null,null,null,null,"Coincident",6.7715929310377199,6.8792414557742978,6.9802031109963627,7.0748932690836366,7.1637015004748221,7.2469931764223725,7.3251109721883507]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.113378986820727,11.290049212711937,11.45574510569403,11.611148365143146,11.756898344896914,11.893594683657893,12.021799772003234]
[null,null,null,null,"Coincident",6.8495402075936678,6.9584278660782353,7.0605516830163504,7.156331812106715,7.2461623081028739,7.3304127480171912,7.4094297516198671]
[null,"Hay Town","Substation Rating","MVA","Non-Coincident",19.8,19.8,19.8,19.8,19.8,19.8,19.8]
[null,null,null,null,"Coincident",18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002,18.150000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6735320444520001,6.7448026356102,6.8050323223857303,6.8559315096960303,6.8989456345827298,6.93529621378726,6.9660155324293198]
[null,null,null,null,"Coincident",4.4410155990235118,4.4884438281796646,4.5285246994053896,4.5623964307939548,4.59102091305129,4.615211025304526,4.6356537192740825]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.7357586642023293,6.8076938101938378,6.8684851020971625,6.9198588933133491,6.9632740987036543,6.9999636249087835,7.030969382478145]
[null,null,null,null,"Coincident",4.4824253633199849,4.5302958318122899,4.570750432738631,4.6049379973824145,4.633829385494268,4.6582450558038486,4.6788783654377699]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.2602304322484796,6.2860140905419106,6.30871002490513,6.3286880059487105,6.3462735223760003,6.3617530839663496,6.3753788894989807]
[null,null,null,null,"Coincident",4.1659769995725187,4.1831351742719596,4.1982385704750635,4.2115332583345904,4.2232358398536824,4.23353697784641,4.2426045022872314]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.3186032663132856,6.3446273415088479,6.3675349016300755,6.3876991651731627,6.4054486558252774,6.4210725548948755,6.4348254127611169]
[null,null,null,null,"Coincident",4.2048221965258366,4.2221403607488934,4.2373845869182301,4.2508032396408346,4.2626149406015417,4.2730121304289792,4.2821642040098506]
[null,"Henty","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.5678034310492399,2.5462392775092098,2.52603998697395,2.5071191729772098,2.4893959167235198,2.4727944210221198,2.4572436861244999]
[null,null,null,null,"Coincident",2.1617321907902904,2.1435781824612419,2.1265731983362093,2.1106445130645346,2.0957240043114282,2.0817478614186218,2.0686563125048116]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6444394249216394,2.6222316900550271,2.6014295524766609,2.5819440475195528,2.563691841369919,2.5465948746727798,2.5305800286948821]
[null,null,null,null,"Coincident",2.2262490042363572,2.2075531902323715,2.1900406930152356,2.1736366167490191,2.1582708059904898,2.143877545654759,2.1303952799710402]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2918963867711701,2.2696373995031798,2.2474006712224601,2.2251861796700201,2.2029939026091303,2.1808238178253001,2.1586759031262601]
[null,null,null,null,"Coincident",1.9294569581654968,1.910717996791049,1.8919977743779781,1.8732962721873192,1.8546134714988494,1.8359493536110667,1.8173038998411772]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3602979456011624,2.3373746397209101,2.3144742571465411,2.2915967749547455,2.2687421702451389,2.2459104201402411,2.2231015017854547]
[null,null,null,null,"Coincident",1.9870415262967926,1.9677433013464407,1.9484643746210417,1.9292047268223671,1.9099643386714891,1.8907431909087611,1.8715412642938014]
[null,"Hillgrove","Substation Rating","MVA","Non-Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,null,null,"Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.55345788431990106,0.47479342614536102,0.44326792967656797,0.43063380048192196,0.425570558395791,0.423541418118071,0.42272822171216701]
[null,null,null,null,"Coincident",0.27075637506297323,0.2322730430063637,0.21685049797127071,0.21066977289763092,0.20819279115765318,0.20720011821603476,0.20680229551386589]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.66176043434509035,0.56770264334790654,0.5300081288650762,0.51490170964097437,0.50884767485885229,0.50642146540448496,0.50544913991771334]
[null,null,null,null,"Coincident",0.32373891752133921,0.27772503415581046,0.25928455225054092,0.25189436155098033,0.2489326754705177,0.24774575285974806,0.24727008283744253]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.52710274697133397,0.45218421537653397,0.42215993302530302,0.410127429030402,0.40530529371027701,0.40337277916006797,0.40259830639254002]
[null,null,null,null,"Coincident",0.2578632143456886,0.22121242191082241,0.20652428378216267,0.20063787895012475,0.19827884872157439,0.19733344592003327,0.19695456715606277]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.63024803270960938,0.54066918414086296,0.50476964653816814,0.49038258061045192,0.48461683319890675,0.48230615752808126,0.48138013325496515]
[null,null,null,null,"Coincident",0.30832277859175139,0.26450003252934307,0.24693766881003912,0.23989939195331464,0.2370787385433501,0.2359483360569031,0.23549531698804055]
[null,"Holbrook","Substation Rating","MVA","Non-Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,null,null,"Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.52812913073807,3.54597939943381,3.5627988949189699,3.5786471397379902,3.5935802192744899,3.6076509802319103,3.6209092176528803]
[null,null,null,null,"Coincident",3.0871129893958109,3.1027319745045832,3.1174490330540983,3.1313162472707412,3.1443826918651783,3.1566946077029212,3.1682955654462699]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5686498445793453,3.5867051243738879,3.6037177924834767,3.6197480550715189,3.6348526416646609,3.6490850059129922,3.662495514757333]
[null,null,null,null,"Coincident",3.1225686140069269,3.1383669838271513,3.1532530684230418,3.1672795481875786,3.1804960614565778,3.192949380173868,3.2046835754126661]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.15847202196694,3.1541949492179802,3.1501661112188901,3.1463711008050801,3.1427963469817302,3.1394290663937499,3.1362572176124299]
[null,null,null,null,"Coincident",2.763663019221072,2.7599205805657321,2.7563953473165284,2.7530747132044446,2.7499468036090136,2.7470004330945308,2.744225065410876]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1947472081166666,3.1904210130044039,3.1863459036287218,3.1825073073581294,3.1788914973343512,3.1754855433849167,3.1722772657847944]
[null,null,null,null,"Coincident",2.7954038071020828,2.7916183863788531,2.7880526656751314,2.7846938939383628,2.7815300601675568,2.7785498504618018,2.7757426075616949]
[null,"Ivanhoe","Substation Rating","MVA","Non-Coincident",2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002]
[null,null,null,null,"Coincident",2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002,2.2000000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.04133729215323,1.04819154839635,1.0539566082948599,1.0588055538922398,1.0628839631057201,1.0663142803527501,1.0691994926498301]
[null,null,null,null,"Coincident",0.79738412206505815,0.80263263773621774,0.80704712213091423,0.81076010951477429,0.81388307339460286,0.81650977324203822,0.81871906939594941]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0604906402180039,1.0674709670018976,1.0733420638201285,1.0782801962193964,1.0824336197359319,1.0859270309110292,1.0888653110044737]
[null,null,null,null,"Coincident",0.81205043215144357,0.81739548392884909,0.82189116406749452,0.82567244453973154,0.8288528491879209,0.83152786200447648,0.83377779380884687]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.96944563014735796,0.97907408371743498,0.98796581413524798,0.99617719192791609,1.00376027441981,1.0107631357581501,1.0172301716866801]
[null,null,null,null,"Coincident",0.74233445638582796,0.74970726062003024,0.75651593318584831,0.76280363873667156,0.76861023917334925,0.77397254635498247,0.77892455547353734]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.98727667271541208,0.99708222272095037,1.0061374990031762,1.0144999089140057,1.0222224672697389,1.0293541324468287,1.0359401167612659]
[null,null,null,null,"Coincident",0.75598823631935241,0.76349664876308987,0.77043055344773714,0.77683390895544879,0.78274731036821255,0.78820824662675859,0.79325133819763938]
[null,"Jelbart","Substation Rating","MVA","Non-Coincident",96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011]
[null,null,null,null,"Coincident",96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011,96.800000000000011]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",47.055792303556196,46.429621145157306,45.834056816830405,45.267603277062506,44.728837609855994,44.216406450401202,43.729022585461003]
[null,null,null,null,"Coincident",39.003906952370841,38.484882186176378,37.991227005611961,37.521701362192324,37.075125820178407,36.650378593865959,36.24639272969047]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",47.095616804837611,46.468915702028497,45.872847332621944,45.305914388967381,44.766692750817576,44.253827907976159,43.766031557805057]
[null,null,null,null,"Coincident",39.036916940437443,38.517452910521037,38.023379937153472,37.553456922365235,37.106503432231129,36.681396731651418,36.277068964071958]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",42.913385643152601,42.339864972661196,41.798110857036299,41.286363788626197,40.802961716591597,40.346334648901198,39.914999553315099]
[null,null,null,null,"Coincident",35.570322349247448,35.094938857183337,34.645886230875725,34.221706038336329,33.821020628204664,33.442528655415501,33.085000854693277]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",42.949704321425209,42.375698265956551,41.83348565018926,41.321305477355999,40.83749428998204,40.380480767312307,39.948780621979381]
[null,null,null,null,"Coincident",35.600426408251266,35.124640587173829,34.675207916327253,34.250668729415551,33.849644209137224,33.470831909065971,33.113001523568073]
[null,"Jerilderie","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5688014679473303,5.6960595084644803,5.8136661757484998,5.9223534393072095,6.0227977553709797,6.1156242770734695,6.2014107453283103]
[null,null,null,null,"Coincident",4.0986378804092354,4.1922997982298575,4.2788583053508962,4.3588521313301065,4.432779147953041,4.5010994679260738,4.5642383085616363]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6517147342478795,5.780867505590507,5.9002252054763114,6.0105307016257843,6.1124705219509483,6.2066791274210082,6.2937428608698651]
[null,null,null,null,"Coincident",4.1596620444064394,4.2547184841146128,4.3425657512305653,4.4237505963965775,4.4987783041558975,4.5681158377818623,4.6321947456002208]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.1080516441596604,5.2242114165870301,5.3323381496285398,5.43298736883684,5.5266761823456303,5.6138859376296599,5.6950646945362893]
[null,null,null,null,"Coincident",3.75952601010151,3.8450196026080543,3.9246008781266051,3.9986787034639142,4.0676336702063836,4.1318200500954294,4.1915676151787089]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.1841048575282604,5.3019941199006597,5.4117307398563428,5.5138785141061888,5.6089622499494434,5.6974704615899245,5.779857879988274]
[null,null,null,null,"Coincident",3.8155011751407995,3.9022676722468854,3.9830338245342682,4.0582145863821548,4.1281962159627899,4.1933382597301847,4.2539753996713694]
[null,"Jindabyne 11kV","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0.83499999999999996,0.83499999999999996,0.83499999999999996,0.83499999999999996,0.83499999999999996,0.83499999999999996,0.83499999999999996]
[null,null,null,null,"Coincident",0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002,0.33700000000000002]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.161585978322901,18.593152237782,18.810036769866901,18.919032547981399,18.973808605695602,19.001336428796701,19.0151705942388]
[null,null,null,null,"Coincident",4.2720072240820706,4.3735211656662409,4.4245372106836882,4.450175431489698,4.463059973321073,4.4695351269387977,4.472789229018777]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.171307711277574,18.603104984257836,18.820105612674048,18.929159735244216,18.983965114087425,19.011507672583626,19.025349243329547]
[null,null,null,null,"Coincident",4.2742939909680979,4.3758622720484137,4.4269056254940251,4.4525575702080911,4.4654490090183465,4.4719276287273253,4.4751834726987605]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.374638781807,16.683340643160797,16.826846856135198,16.893558579452801,16.9245708536656,16.9389875274377,16.9456894055789]
[null,null,null,null,"Coincident",3.8516776701719304,3.9242911843972323,3.9580470237418268,3.9737390984474126,3.9810338721323992,3.9844249930716802,3.9860014232286223]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.38340397806552,16.692271084737776,16.835854115291959,16.902601548792571,16.93363042359568,16.948054814483054,16.954760280079096]
[null,null,null,null,"Coincident",3.8537394384437973,3.9263918220274832,3.9601657305680251,3.9758662050994835,3.9831648836109439,3.9865578197866385,3.9881350937924065]
[null,"Jindabyne East","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.6922152771418997,4.6922155099392304,4.6922155954190004,4.6922156268059094,4.6922156383307305,4.6922156425624699,4.6922156441163096]
[null,null,null,null,"Coincident",1.3988529112606134,1.3988529806626346,1.3988530061460402,1.3988530155031702,1.3988530189389738,1.3988530202005487,1.3988530206637826]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.7627086521975519,4.7627088884923072,4.762708975256281,4.7627090071147302,4.7627090188126937,4.7627090231080089,4.7627090246851926]
[null,null,null,null,"Coincident",1.419868541852322,1.4198686122970026,1.4198686381632577,1.4198686476609643,1.4198686511483853,1.4198686524289137,1.4198686528991069]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.3435035540134601,4.3435041297104897,4.3435043578584498,4.3435044482731797,4.3435044841044199,4.3435044983042896,4.3435045039316797]
[null,null,null,null,"Coincident",1.2948942520180975,1.2948944236460851,1.2948944916620262,1.2948945186166523,1.2948945292987357,1.2948945335320301,1.2948945352096792]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.4087580675009859,4.408758651846985,4.4087588834225198,4.4087589751955933,4.4087590115651434,4.4087590259783447,4.4087590316902769]
[null,null,null,null,"Coincident",1.3143480623770547,1.3143482365834909,1.3143483056212677,1.3143483329808461,1.3143483438234114,1.3143483481203047,1.3143483498231578]
[null,"Johns River","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4100727377675901,1.5578656623198202,1.70104157828102,1.83974471967588,1.97411481469953,2.1042872264783199,2.2303930894333499]
[null,null,null,null,"Coincident",0.91766638489636809,1.0138490818271844,1.1070270588812985,1.1972941826462076,1.2847413873441385,1.3694567664382715,1.4515256613772594]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5197450618161807,1.679032991611362,1.8333448121473219,1.982835975650671,2.1276570780650492,2.2679540107599672,2.4038681075003887]
[null,null,null,null,"Coincident",0.98904043705497457,1.0927040104137433,1.1931291634609553,1.2904170635186905,1.3846657174709049,1.4759700704945815,1.564422101706602]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2429534605798001,1.34915583097648,1.45033570888556,1.54673061660239,1.63856684358503,1.7260599776744801,1.8094154111924599]
[null,null,null,null,"Coincident",0.80890622037733007,0.87802204873072498,0.94386927086203098,1.0066024647729839,1.0663688982061306,1.123308874359582,1.1775560612522356]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3396276186248959,1.4540901733857619,1.5631395973544371,1.6670318867825762,1.7660109314194214,1.8603090870491621,1.9501477209518736]
[null,null,null,null,"Coincident",0.87182114862890037,0.94631265252089247,1.0172813252624113,1.0848937675886605,1.1493087013999408,1.2106773423653276,1.2691437549051874]
[null,"Jugiong","Substation Rating","MVA","Non-Coincident",14.025,14.025,14.025,14.025,14.025,14.025,14.025]
[null,null,null,null,"Coincident",14.025,14.025,14.025,14.025,14.025,14.025,14.025]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0686458432074701,2.0686458432074701,2.0686458432074701,2.0686458432074701,2.0686458432074701,2.0686458432074701,2.0686458432074701]
[null,null,null,null,"Coincident",1.7653888609571602,1.7653888609571602,1.7653888609571602,1.7653888609571602,1.7653888609571602,1.7653888609571602,1.7653888609571602]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2105267884745792,2.2105267884745792,2.2105267884745792,2.2105267884745792,2.2105267884745792,2.2105267884745792,2.2105267884745792]
[null,null,null,null,"Coincident",1.8864705053474156,1.8864705053474156,1.8864705053474156,1.8864705053474156,1.8864705053474156,1.8864705053474156,1.8864705053474156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9393611059432301,1.9393615279120699,1.9393618042346199,1.9393619851819899,1.93936210367377,1.9393621812670598,1.9393622320783399]
[null,null,null,null,"Coincident",1.6550568600457931,1.6550572201553266,1.6550574559698588,1.6550576103909127,1.6550577115121701,1.6550577777305273,1.6550578210930333]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0723748781309594,2.0723753290411175,2.072375624315633,2.0723758176735294,2.0723759442922325,2.0723760272073659,2.0723760815036081]
[null,null,null,null,"Coincident",1.7685712310751118,1.7685716158832574,1.7685718678714564,1.7685720328836925,1.7685721409404915,1.7685722117005269,1.7685722580371104]
[null,"Junee 11kV","Substation Rating","MVA","Non-Coincident",36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004]
[null,null,null,null,"Coincident",36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004,36.300000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.7049316837572297,6.7120487976634005,6.7180050964384801,6.7229899112898002,6.7271616931362699,6.73065304924347,6.7335749583739002]
[null,null,null,null,"Coincident",6.4384399634171174,6.4452742031616754,6.4509937651014981,6.4557804553561837,6.4597864271133663,6.4631390170795804,6.4659447930967184]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.7049316837572297,6.7120487976634005,6.7180050964384801,6.7229899112898002,6.7271616931362699,6.73065304924347,6.7335749583739002]
[null,null,null,null,"Coincident",6.4384399634171174,6.4452742031616754,6.4509937651014981,6.4557804553561837,6.4597864271133663,6.4631390170795804,6.4659447930967184]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.23164423472197,6.2640724214093702,6.2910207078710503,6.3134151189499299,6.33202519452127,6.3474904332163797,6.3603422675348105]
[null,null,null,null,"Coincident",5.9839636212592531,6.01510292930248,6.0409801391957307,6.0624844703430174,6.0803548767740017,6.0952054398452997,6.107546469938038]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.23164423472197,6.2640724214093702,6.2910207078710503,6.3134151189499299,6.33202519452127,6.3474904332163797,6.3603422675348105]
[null,null,null,null,"Coincident",5.9839636212592531,6.01510292930248,6.0409801391957307,6.0624844703430174,6.0803548767740017,6.0952054398452997,6.107546469938038]
[null,"Junee Reefs","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.22503724720624299,0.22832626299856199,0.23134884200939101,0.23412656776493299,0.23667927535185002,0.23902519305495698,0.24118107252111901]
[null,null,null,null,"Coincident",0.18889136812130242,0.19165209640293804,0.19418918344829711,0.19652074599958105,0.19866343319688964,0.2006325454658188,0.20244214377420353]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.23786320430089933,0.24133967695184791,0.24453452730526304,0.24747056903650946,0.2501687677294166,0.25264839058658667,0.25492714401195998]
[null,null,null,null,"Coincident",0.19965719739246471,0.20257527288186197,0.20525696074327779,0.2077214102793499,0.20998621954489891,0.21206756101050281,0.21398029704630839]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.203399379987519,0.20593584771951201,0.20826575311158899,0.210405917982428,0.212371794232147,0.21417757540436599,0.21583629916300001]
[null,null,null,null,"Coincident",0.17072901325377243,0.17285806907026396,0.174813740953769,0.1766101487728152,0.17826026251610266,0.17977599593527094,0.18116829256168912]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.21499209076400971,0.21767312401440647,0.22013582194178316,0.22239796512132284,0.22447588613138852,0.22638458747404488,0.22813784989249741]
[null,null,null,null,"Coincident",0.18045968240295115,0.18271008336960542,0.18477721841745529,0.1866760121743746,0.18842017385121732,0.19002229622173716,0.191493946541889]
[null,"Kanangra Dr","Substation Rating","MVA","Non-Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,null,null,"Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.468891979936899,13.565622434669701,13.662256158947701,13.7587932495014,13.8552338029645,13.9515779158742,14.047825684670999]
[null,null,null,null,"Coincident",11.190770784517303,11.271140301802717,11.351429449570789,11.431638308191074,11.5117669579527,11.591815479064616,11.671783951655428]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.499866434786901,13.596819340862188,13.693675294031332,13.790434391247283,13.887096729365974,13.983662405146609,14.080131515251471]
[null,null,null,null,"Coincident",11.216506236618196,11.297060579944844,11.377534368928108,11.457927684122371,11.538240606001402,11.618473214958605,11.698625591306859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.981014993955899,10.9810152099957,10.981015210211702,10.981015210211899,10.981015210211899,10.981015210211899,10.981015210211899]
[null,null,null,null,"Coincident",9.123691983108758,9.1236921626077034,9.1236921627871705,9.123692162787334,9.123692162787334,9.123692162787334,9.123692162787334]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.006268069980573,11.006268286517201,11.0062682867337,11.006268286733897,11.006268286733897,11.006268286733897,11.006268286733897]
[null,null,null,null,"Coincident",9.1446737673429084,9.1446739472546472,9.1446739474345282,9.1446739474346916,9.1446739474346916,9.1446739474346916,9.1446739474346916]
[null,"Keepit Dam","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.266348528314997,0.26634852831104999,0.266348528311046,0.266348528311046,0.266348528311046,0.266348528311046,0.266348528311046]
[null,null,null,null,"Coincident",0.14243856079454187,0.14243856079243108,0.14243856079242895,0.14243856079242895,0.14243856079242895,0.14243856079242895,0.14243856079242895]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.28371908450945327,0.28371908450524885,0.28371908450524458,0.28371908450524458,0.28371908450524458,0.28371908450524458,0.28371908450524458]
[null,null,null,null,"Coincident",0.15172803215070763,0.15172803214845917,0.1517280321484569,0.1517280321484569,0.1517280321484569,0.1517280321484569,0.1517280321484569]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.23735912936971801,0.237359129366326,0.237359129366323,0.237359129366323,0.237359129366323,0.237359129366323,0.237359129366323]
[null,null,null,null,"Coincident",0.12693553440206659,0.1269355344002526,0.12693553440025099,0.12693553440025099,0.12693553440025099,0.12693553440025099,0.12693553440025099]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.25283907258948218,0.25283907258586896,0.25283907258586574,0.25283907258586574,0.25283907258586574,0.25283907258586574,0.25283907258586574]
[null,null,null,null,"Coincident",0.13521393881959265,0.13521393881766036,0.13521393881765864,0.13521393881765864,0.13521393881765864,0.13521393881765864,0.13521393881765864]
[null,"Kew","Substation Rating","MVA","Non-Coincident",13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001]
[null,null,null,null,"Coincident",13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2951047447774497,3.2561900091120202,3.22022342449264,3.1869816412179199,3.1562582303915301,3.1278624020147499,3.1016178201953699]
[null,null,null,null,"Coincident",2.4388656748012059,2.4100630052627636,2.3834424042615159,2.3588385599295894,2.3360986843016422,2.3150815645134357,2.2956566858808993]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5059914484432069,3.4645861696951896,3.4263177236601692,3.3909484662558671,3.3582587571365883,3.3280455957436939,3.3001213606878737]
[null,null,null,null,"Coincident",2.5949530779884835,2.5643070375995807,2.5359827181342527,2.5098042277650836,2.4856090000969475,2.4632467846422959,2.442578713777277]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0493987405018301,2.9589391655047996,2.8748742929099698,2.7967520730718203,2.7241524123091501,2.65668491389739,2.5939867787529001]
[null,null,null,null,"Coincident",2.2570068307477253,2.1900533438314045,2.1278328840560312,2.0700108677136022,2.0162763632439282,1.9663404192342759,1.9199345106147392]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2445602598939476,3.1483112720971071,3.0588662476562081,2.9757442057484171,2.8984981666969358,2.8267127483868233,2.7600019325930858]
[null,null,null,null,"Coincident",2.4014552679155798,2.3302167578366149,2.2640141886356173,2.202491563247273,2.1453180504915399,2.0921862060652696,2.0428103192940825]
[null,"Koolkhan 11kV","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4156592687713401,2.4156592862417803,2.4156592914706398,2.41565929303562,2.4156592935040098,2.4156592936441998,2.4156592936861596]
[null,null,null,null,"Coincident",1.2274463569859013,1.2274463658629926,1.2274463685198842,1.227446369315083,1.2274463695530815,1.227446369624315,1.2274463696456355]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4380783803144617,2.4380783979470406,2.438078403224428,2.4380784048039321,2.4380784052766691,2.4380784054181599,2.4380784054605091]
[null,null,null,null,"Coincident",1.2388379705078123,1.2388379794672897,1.2388379821488391,1.2388379829514178,1.2388379831916252,1.2388379832635197,1.2388379832850382]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0559006298513198,2.0498096604515701,2.04475968334014,2.0405727851385,2.03710145919701,2.0342234088571698,2.0318372388753803]
[null,null,null,null,"Coincident",1.0446455636599512,1.0415506163315402,1.0389846186809528,1.0368571692467088,1.0350933168541652,1.0336309200457545,1.0324184578044275]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.0749809141190818,2.0688334160010049,2.0637365713525777,2.0595108156270245,2.0560072732034791,2.0531025124196494,2.0506941970087946]
[null,null,null,null,"Coincident",1.0543406500976309,1.0512169793601394,1.0486271673462053,1.0464799736016668,1.0446997513493315,1.0432237824127684,1.0420000676216381]
[null,"Kooringal","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.016356482101401,19.016441356394999,19.0164940863115,19.016526845866601,19.016547198420202,19.016559842866499,19.016567698491198]
[null,null,null,null,"Coincident",18.092381001247976,18.092461751630335,18.092511919481382,18.092543087300143,18.092562450954503,18.092574481026624,18.092581954958614]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.783127801281847,19.78321609784901,19.783270953923992,19.783305034399181,19.783326207601807,19.78333936189334,19.783347534269971]
[null,null,null,null,"Coincident",18.821896082672719,18.821980089045638,18.822032279748402,18.822064704305777,18.822084848735088,18.822097363879852,18.822105139173285]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.296200192710799,17.296200273447202,17.2962003201547,17.296200347176001,17.2962003628083,17.296200371851899,17.2962003770838]
[null,null,null,null,"Coincident",16.455804457332206,16.455804534145752,16.455804578583805,16.455804604292183,16.45580461916493,16.455804627769115,16.455804632746805]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.993611931445116,17.993612015436945,17.993612064027769,17.993612092138612,17.993612108401233,17.993612117809487,17.993612123252344]
[null,null,null,null,"Coincident",17.119330033527639,17.119330113438433,17.119330159668305,17.119330186413286,17.119330201885731,17.119330210836853,17.11933021601525]
[null,"Kootingal","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.3421926244443902,6.3421926244682503,6.3421926244682698,6.3421926244682698,6.3421926244682698,6.3421926244682698,6.3421926244682698]
[null,null,null,null,"Coincident",5.9639884771151381,5.9639884771375753,5.9639884771375931,5.9639884771375931,5.9639884771375931,5.9639884771375931,5.9639884771375931]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.555538553707045,6.555538553731707,6.5555385537317274,6.5555385537317274,6.5555385537317274,6.5555385537317274,6.5555385537317274]
[null,null,null,null,"Coincident",6.1646119427061663,6.1646119427293575,6.1646119427293771,6.1646119427293771,6.1646119427293771,6.1646119427293771,6.1646119427293771]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7057880807723,5.7057880808497305,5.7057880808498105,5.7057880808498105,5.7057880808498105,5.7057880808498105,5.7057880808498105]
[null,null,null,null,"Coincident",5.3655346631115668,5.3655346631843797,5.3655346631844552,5.3655346631844552,5.3655346631844552,5.3655346631844552,5.3655346631844552]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8977259061193799,5.8977259061994145,5.897725906199498,5.897725906199498,5.897725906199498,5.897725906199498,5.897725906199498]
[null,null,null,null,"Coincident",5.5460266548370321,5.5460266549122936,5.5460266549123718,5.5460266549123718,5.5460266549123718,5.5460266549123718,5.5460266549123718]
[null,"Koraleigh","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.5498588437677903,4.5822362569178905,4.5972511172483701,4.6042141822004297,4.6074432680833199,4.6089407402038294,4.6096351852675594]
[null,null,null,null,"Coincident",3.8759258766571545,3.9035074913306707,3.9162983245603682,3.9222300082796338,3.9249807963724526,3.9262564603305563,3.9268480429894592]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.6472167362877856,4.6802869614168463,4.6956231097715158,4.7027351704072853,4.7060333522791105,4.7075628673123271,4.7082721721135128]
[null,null,null,null,"Coincident",3.9588629496241405,3.9870347557671324,4.0000992872827723,4.0061578971871858,4.0089675466514629,4.0102705072705822,4.0108747486169083]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.1775830489605195,4.19222127915108,4.2056699190190905,4.2180256418042203,4.2293772644992496,4.2398063862957693,4.2493879751460097]
[null,null,null,null,"Coincident",3.5587922169342701,3.5712622071322682,3.5827188111853068,3.5932443829254685,3.6029145836188325,3.611798925843495,3.6199612731688426]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.2669749829611003,4.2819264420430425,4.2956628559453192,4.3082829665218565,4.3198774912717006,4.3305297754461778,4.3403163911619727]
[null,null,null,null,"Coincident",3.6349432629457019,3.647680086029534,3.6593818385287871,3.6701326364830744,3.6800097601584647,3.6890842095633984,3.6974212148201016]
[null,"Koree Island","Substation Rating","MVA","Non-Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,null,null,"Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6237810894595501,2.8351824089389903,3.0336226759335401,3.2198965348755402,3.3947499104059102,3.5588829943931999,3.7129530498180201]
[null,null,null,null,"Coincident",1.8752317786431492,2.0263215452122783,2.1681479713289713,2.3012789940434009,2.4262477300842242,2.5435546106986693,2.653669385605232]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.7073819575060551,2.925519103341458,3.1302822219804418,3.3224912774083388,3.5029159614727647,3.6722787760772966,3.8312579264053586]
[null,null,null,null,"Coincident",1.9349818108057983,2.0908857120940421,2.237231117474257,2.3746040600300775,2.5035546430525937,2.6245992429023031,2.7382225768132415]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.80736450549808,1.8801983553019399,1.94565318043209,2.0044765729117602,2.05734038388271,2.1048483971503802,2.1475432252981399]
[null,null,null,null,"Coincident",1.2917340436353926,1.3437888245246217,1.3905697730735231,1.4326111976986993,1.4703932743632311,1.5043475309045364,1.5348617757277883]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8649521000360088,1.940106636230678,2.0076470317693866,2.0683446990094385,2.1228928961142666,2.1719146450987989,2.2159698476728353]
[null,null,null,null,"Coincident",1.3328922362022062,1.3866056253060435,1.4348771432940028,1.4782581231155694,1.5172440404581375,1.5522801728206121,1.5837666852485264]
[null,"Kyogle","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.9665496427753499,8.9761249369854603,8.9843309251085195,8.9913634234942688,8.9973902459565913,9.0025552082502198,9.0069815598909617]
[null,null,null,null,"Coincident",6.4659182682961687,6.4728231617305516,6.4787406272694907,6.4838118711253498,6.4881579064467854,6.4918824410091229,6.4950743519532432]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.4220217859840574,9.4320834746211748,9.4407063007863421,9.4480960276757493,9.4544289935101631,9.4598563194262759,9.4645075156224738]
[null,null,null,null,"Coincident",6.7943663078211731,6.8016219478343931,6.8078400017622629,6.8131688486426718,6.8177356487065319,6.8216493777536096,6.8250034276002705]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.7360286232272601,7.7360286350994603,7.73602863515901,7.7360286351593102,7.7360286351593102,7.7360286351593102,7.7360286351593102]
[null,null,null,null,"Coincident",5.5785704414507338,5.5785704500119619,5.5785704500549036,5.5785704500551203,5.5785704500551203,5.5785704500551203,5.5785704500551203]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.1289942206222694,8.12899423309754,8.1289942331601139,8.1289942331604301,8.1289942331604301,8.1289942331604301,8.1289942331604301]
[null,null,null,null,"Coincident",5.8619440395722346,5.8619440485683461,5.8619440486134691,5.8619440486136964,5.8619440486136964,5.8619440486136964,5.8619440486136964]
[null,"Kywong","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.40628859700196701,0.41333790483970101,0.41912623320731096,0.423879145984353,0.42778185820651699,0.43098645366271804,0.43361781140915501]
[null,null,null,null,"Coincident",0.33815324222523963,0.34402036800322944,0.34883798291788615,0.35279382336585902,0.35604204347623153,0.35870922230313179,0.3608992964523402]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.43783274273193334,0.44542935707880815,0.45166708982278536,0.45678901756698903,0.46099473539646391,0.46444813484771164,0.46728379055582847]
[null,null,null,null,"Coincident",0.3644073759383793,0.3707300239041012,0.37592167724380893,0.3801846481613449,0.38368505927407554,0.38655931720244324,0.38891942816447839]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.32738488238579599,0.32738756085634296,0.32738865683019097,0.32738910527965298,0.32738928877574602,0.32738936385849099,0.32738939458077199]
[null,null,null,null,"Coincident",0.27248182757575568,0.27248405686180099,0.27248496903879249,0.27248534228244409,0.27248549500590041,0.27248555749712916,0.27248558306722637]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.35280296331637018,0.35280584974270496,0.35280703080769021,0.35280751407465705,0.35280771181734116,0.35280779272949181,0.35280782583704307]
[null,null,null,null,"Coincident",0.29363724897138888,0.29363965133864883,0.29364063433683535,0.29364103655903134,0.29364120113989889,0.29364126848293109,0.29364129603828432]
[null,"Lake Cargelligo","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.1567742214892593,4.1883077913277607,4.2133712754476704,4.2332922117528993,4.2491257527473802,4.2617105538120708,4.2717131942759501]
[null,null,null,null,"Coincident",3.835654521942907,3.8647520560641411,3.8878793324274299,3.9062613337941317,3.920871699880383,3.9324842981451589,3.9417142132385274]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.1829240341559011,4.2146559782384792,4.2398771339998076,4.25992339073977,4.2758565388114684,4.2885205094852727,4.2985860754679228]
[null,null,null,null,"Coincident",3.8597842056491412,3.8890647891797938,3.9123375567129575,3.9308351972427618,3.9455374755464652,3.9572231273987151,3.9665111068799375]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8434826608625197,3.8637072898409399,3.8788862923857699,3.89027844788597,3.8988284963201401,3.9052454845911897,3.9100615670716303]
[null,null,null,null,"Coincident",3.5465654044748005,3.5652276376061209,3.5792340297379508,3.5897461168590463,3.5976356557639537,3.6035569179657503,3.6080009477734443]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.867661590535787,3.8880134504463815,3.9032879424385243,3.9147517647448407,3.9233556005999604,3.9298129574434246,3.9346593373727861]
[null,null,null,null,"Coincident",3.5688764601144261,3.5876560953162757,3.6017506001313708,3.6123288176445216,3.6202679887770643,3.6262265009927117,3.630698487706594]
[null,"Lake Cathie","Substation Rating","MVA","Non-Coincident",23.1,23.1,23.1,23.1,23.1,23.1,23.1]
[null,null,null,null,"Coincident",23.1,23.1,23.1,23.1,23.1,23.1,23.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.03437491459671,6.1328984573563705,6.2180503292545897,6.2916453410119306,6.35525199621308,6.4102259202504603,6.4577387522726806]
[null,null,null,null,"Coincident",4.2500216379635098,4.3194119550226153,4.3793845790644399,4.4312176847036486,4.4760159719743751,4.514734210398287,4.5481975876383895]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.1719131201973285,6.272682256158002,6.3597749480798633,6.4350473706712208,6.5001037775607289,6.5563306921686211,6.6049264581735363]
[null,null,null,null,"Coincident",4.3468900556740735,4.4178619482616206,4.4792014955080219,4.5322160047625539,4.5780353548827719,4.6176360769296281,4.6518621666170148]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8233144305733902,4.91074996665479,4.9878051574741402,5.0557123574332099,5.11555761584144,5.1682980462539403,5.2147771337218298]
[null,null,null,null,"Coincident",3.3970694540461039,3.4586504670809437,3.5129205833621646,3.5607477524201294,3.602896880832628,3.6400420654823979,3.6727773744824241]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.9332495972174017,5.0226780036306193,5.1014894712520409,5.170944442863008,5.2321537215006177,5.2860962356855392,5.3336346955621305]
[null,null,null,null,"Coincident",3.4744969993383243,3.5374815947079958,3.5929886600546452,3.6419059276073655,3.6850157380410389,3.7230075525598081,3.7564889795460985]
[null,"Laurieton","Substation Rating","MVA","Non-Coincident",48,48,48,48,48,48,48]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2329564268796087,9.2330053681910993,9.2330199651035887,9.2330243186823502,9.2330256171520197,9.2330260044250103,9.2330261199304893]
[null,null,null,null,"Coincident",8.0250904736219049,8.025133012374873,8.0251456997025219,8.0251494837411155,8.0251506123434933,8.0251509489529873,8.0251510493479064]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.3752415821644792,9.3752912776896569,9.3753060995489417,9.3753105202188483,9.375311838698682,9.3753122319397715,9.3753123492252559]
[null,null,null,null,"Coincident",8.1487617216406001,8.1488049159401541,8.1488177987868013,8.1488216411395999,8.1488227871343888,8.1488231289312267,8.1488232308732904]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.5682163174318511,8.5682278987742198,8.5682300725140585,8.5682304805103602,8.5682305570885084,8.5682305714617204,8.56823057415947]
[null,null,null,null,"Coincident",7.4473124279860414,7.447322494243914,7.4473243836126128,7.4473247382343706,7.4473248047944773,7.4473248172873694,7.4473248196321959]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.7002574462831621,8.7002692061006606,8.7002714133390775,8.7002718276228368,8.7002719053810971,8.7002719199758101,8.7002719227151335]
[null,null,null,null,"Coincident",7.5620797848627666,7.5620900062474465,7.5620919247324014,7.5620922848190837,7.5620923524049193,7.5620923650903356,7.5620923674712976]
[null,"Leeton","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.425752437158,21.4731700185337,21.517534684969601,21.559042994142498,21.5978788486367,21.634214310725,21.668210364690001]
[null,null,null,null,"Coincident",20.264400811692582,20.309248192307873,20.351208136779881,20.390466548663539,20.427197362372105,20.461563313794112,20.493716661294197]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.751826385010865,22.80217871603034,22.849289182341337,22.893366506888377,22.934605974279648,22.973190295996091,23.00929041989399]
[null,null,null,null,"Coincident",21.51859685750475,21.566219913944629,21.61077682621886,21.652465003749519,21.691469146027771,21.72796206092551,21.762105430320094]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.7742866250208,19.8131107971045,19.849509355498803,19.8836338450133,19.9156263424088,19.9456200479312,19.973739839888701]
[null,null,null,null,"Coincident",18.702450292469898,18.739170056995963,18.773595684680842,18.805870506068999,18.836128896857886,18.864496837368563,18.891092437062881]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.99814872310699,21.039375785044765,21.078027108198096,21.114263616726237,21.148236180747045,21.18008624448181,21.20994641515615]
[null,null,null,null,"Coincident",19.859974732584604,19.898967141828848,19.935523426448427,19.969795787943514,20.001926918737531,20.032050596274281,20.060292239998354]
[null,"Lennox Head","Substation Rating","MVA","Non-Coincident",38.4,38.4,38.4,38.4,38.4,38.4,38.4]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.1285167495302906,6.4016804948015498,6.6549409111698399,6.8897482002386896,7.1074468986396395,7.3092835770213593,7.4964139780728702]
[null,null,null,null,"Coincident",4.5339496955772685,4.7360394883171342,4.9234045612416377,5.097117790772197,5.2581738811252512,5.4074950601161156,5.5459363599535978]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.1327860053641681,6.4061400423423391,6.6595768853329682,6.8945477461810372,7.1123980981510577,7.3143753802794738,7.5016361403703788]
[null,null,null,null,"Coincident",4.5371081418995107,4.7393387147109474,4.9268343101522909,5.1006685520336204,5.2618368375036049,5.4112620368211788,5.5497997778288699]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.69447633825341,5.9244891155148496,6.1370968886378492,6.3336166895397703,6.5152658906919392,6.6831697463226902,6.8383683629797201]
[null,null,null,null,"Coincident",4.2128414289272884,4.3830076215094191,4.5402973846975945,4.6856850743930591,4.8200713172517169,4.9442885897559723,5.0591063751197938]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6984432322542835,5.9286162413354804,6.141372121580126,6.3380288223781829,6.5198045642486742,6.6878253852960956,6.8431321166286097]
[null,null,null,null,"Coincident",4.215776184363671,4.3860609183547759,4.5434602529558301,4.6889492228252392,4.8234290820146937,4.9477328869275192,5.0626306568161503]
[null,"Lightning Ridge","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.3953224448209096,3.3953225436381098,3.3953225437369303,3.3953225437370302,3.3953225437370302,3.3953225437370302,3.3953225437370302]
[null,null,null,null,"Coincident",3.0935160052812729,3.093516095314722,3.0935160954047585,3.0935160954048495,3.0935160954048495,3.0935160954048495,3.0935160954048495]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.4257126765801091,3.4257127762817845,3.4257127763814892,3.42571277638159,3.42571277638159,3.42571277638159,3.42571277638159]
[null,null,null,null,"Coincident",3.121204883106321,3.1212049739456256,3.1212049740364676,3.1212049740365595,3.1212049740365595,3.1212049740365595,3.1212049740365595]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.0826865399243504,3.0826865533296699,3.0826865533430801,3.0826865533430903,3.0826865533430903,3.0826865533430903,3.0826865533430903]
[null,null,null,null,"Coincident",2.8086699585977413,2.8086699708114766,2.8086699708236949,2.8086699708237042,2.8086699708237042,2.8086699708237042,2.8086699708237042]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.1102784873495994,3.1102785008749048,3.1102785008884348,3.110278500888445,3.110278500888445,3.110278500888445,3.110278500888445]
[null,null,null,null,"Coincident",2.8338092884740793,2.8338093007971352,2.8338093008094623,2.8338093008094716,2.8338093008094716,2.8338093008094716,2.8338093008094716]
[null,"Lismore East","Substation Rating","MVA","Non-Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,null,null,"Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.430425760845299,20.573611139547801,22.378173990848701,23.897616553613201,25.176987731999098,26.254218719333501,27.161247593891598]
[null,null,null,null,"Coincident",12.13152252131855,13.542238802454397,14.730062413029936,15.730210315700095,16.572335205548679,17.281404662385263,17.878441397291549]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",18.489728708088396,20.639810140690823,22.450179471828719,23.97451109268161,25.257998859717201,26.338696016159115,27.248643406338818]
[null,null,null,null,"Coincident",12.170557704194715,13.585813198601095,14.777458828365237,15.780824872551875,16.625659438702179,17.337010443948774,17.935968243427943]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.806726297730799,17.3862027715554,18.6952976204206,19.780295942159199,20.6795595510536,21.424883319836898,22.0426193371949]
[null,null,null,null,"Coincident",10.404515802159333,11.444180032532334,12.305870036204929,13.020052212274253,13.611977589661969,14.102574616773397,14.509189119555481]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.857587057426967,17.44214575839132,18.755452836738673,19.843942320269615,20.746099458757307,21.493821430203564,22.113545115503854]
[null,null,null,null,"Coincident",10.437994054898141,11.481003577116507,12.345466211084831,13.06194638658504,13.655776381906307,14.147951986202761,14.555874838489066]
[null,"Lismore South","Substation Rating","MVA","Non-Coincident",80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011]
[null,null,null,null,"Coincident",80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011,80.300000000000011]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.381574289077498,29.572035866794199,30.6166045266833,31.533159672726001,32.337389560138703,33.043059824061501,33.662249099639098]
[null,null,null,null,"Coincident",17.848889432316636,18.597558863323638,19.254477691184391,19.83089009501052,20.336662262276029,20.78045126383536,21.169853233045856]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",29.516297500410342,30.754354901060477,31.840686441758596,32.793886362614984,33.630270150695772,34.364153804752064,35.008098875623112]
[null,null,null,null,"Coincident",18.562505559775698,19.341107529842237,20.024290617547877,20.623748555327111,21.14974199051796,21.611274112169028,22.016244754508833]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",25.188391569772602,25.8774920050692,26.476777024211501,26.997952916393199,27.451200205938502,27.845372516212102,28.188169514165001]
[null,null,null,null,"Coincident",15.840728619475771,16.274097020822825,16.650981401377827,16.978743729837532,17.263786436566619,17.511677477130281,17.727259095396821]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.195448200220373,26.912099547630099,27.535344570347203,28.077357586503144,28.548726147782084,28.958657854105262,29.315160212669607]
[null,null,null,null,"Coincident",16.474056505584652,16.924751401193724,17.316703989391073,17.657570577611548,17.954009571673122,18.211811539472322,18.436012322542481]
[null,"Lismore Uni","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.674629560688203,18.674629560784897,18.674629560785,18.674629560785,18.674629560785,18.674629560785,18.674629560785]
[null,null,null,null,"Coincident",13.766512634841236,13.766512634912516,13.766512634912592,13.766512634912592,13.766512634912592,13.766512634912592,13.766512634912592]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.11819219052899,19.11819219062798,19.118192190628086,19.118192190628086,19.118192190628086,19.118192190628086,19.118192190628086]
[null,null,null,null,"Coincident",14.093496928061217,14.09349692813419,14.093496928134268,14.093496928134268,14.093496928134268,14.093496928134268,14.093496928134268]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.671915533688001,16.672014837723697,16.6720801786226,16.672123172173098,16.672151461428502,16.672170075429101,16.6721823232246]
[null,null,null,null,"Coincident",12.290157354696335,12.290230559375319,12.29027872720148,12.290310421070117,12.290331275266485,12.290344997084826,12.290354025881406]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.067909396622415,17.068011059342606,17.068077952228439,17.06812196696826,17.068150928154342,17.068169984277503,17.068182522984497]
[null,null,null,null,"Coincident",12.582075033689124,12.582149977136728,12.582199289052394,12.582231735718599,12.582253085246997,12.582267132988047,12.582276376237971]
[null,"Lockhart","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.27989826330673,3.2465799499482801,3.2132949549031999,3.1800432448531502,3.14682478651316,3.1136395466315099,3.0804874919897403]
[null,null,null,null,"Coincident",2.8099067179216872,2.7813627372796352,2.7528473006182343,2.7243603793934827,2.6959019450899637,2.6674719692207485,2.6390704233274014]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.27989826330673,3.2465799499482801,3.2132949549031999,3.1800432448531502,3.14682478651316,3.1136395466315099,3.0804874919897403]
[null,null,null,null,"Coincident",2.8099067179216872,2.7813627372796352,2.7528473006182343,2.7243603793934827,2.6959019450899637,2.6674719692207485,2.6390704233274014]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9873249122727996,2.9616779517188503,2.9360566381254598,2.9104609458456596,2.8848908492581398,2.8593463227672102,2.8338273408027699]
[null,null,null,null,"Coincident",2.5592575335392818,2.5372856426544224,2.5153357236604523,2.4934077545854731,2.47150171347957,2.4496175784147747,2.427755327485043]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.9873249122727996,2.9616779517188503,2.9360566381254598,2.9104609458456596,2.8848908492581398,2.8593463227672102,2.8338273408027699]
[null,null,null,null,"Coincident",2.5592575335392818,2.5372856426544224,2.5153357236604523,2.4934077545854731,2.47150171347957,2.4496175784147747,2.427755327485043]
[null,"Macksville","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.1335610362071,11.677631345817201,12.2211575851177,12.7641402981789,13.306580028527,13.8484773191448,14.3898327124719]
[null,null,null,null,"Coincident",9.101415915035318,9.5461801875515366,9.9904996957952452,10.434374884530712,10.87780619807741,11.320794080310604,11.763338974661494]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.177879094700739,11.724115121077249,12.269804911427391,12.814949011987183,13.359547968446378,13.903602325949162,14.447112629094361]
[null,null,null,null,"Coincident",9.1376448521728371,9.5841795455796532,10.03026770429307,10.475909774847775,10.921106203331894,11.365857435387566,11.810163916211119]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.5850603616996111,9.9052825827850786,10.206841681299901,10.4908253773369,10.758257996720801,11.010104165739,11.247272290537]
[null,null,null,null,"Coincident",7.8355541985932735,8.0973280919466362,8.3438453355869093,8.5759951142890003,8.7946147895523428,9.0004929199536274,9.1943721054681102]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.6232144854694823,9.9447113775320872,10.247470856924492,10.532584973499114,10.801082130494155,11.053930793971553,11.292042986062437]
[null,null,null,null,"Coincident",7.8667442687041786,8.1295601746427355,8.3770587005149721,8.6101325705691778,8.8296224794913378,9.0363201247806284,9.2309710623927881]
[null,"Maclean 66/11kV","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.9934608090969306,10.276502985978999,10.443575994635198,10.542195184640502,10.600407727262001,10.6347691950278,10.6550519453398]
[null,null,null,null,"Coincident",7.0512236165709306,7.2509335789394962,7.3688175799710285,7.4384016785026885,7.4794755029919697,7.5037203964916968,7.5180315756458489]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9945176471689603,10.277589756599346,10.444680433720928,10.543310052997592,10.601528751767846,10.63589385336061,10.656178748633513]
[null,null,null,null,"Coincident",7.0519693043476419,7.2517003866360863,7.3695968542497914,7.439188311505915,7.4802664796737597,7.5045139371427654,7.5188266297464894]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.1840385641899402,8.2929209769748304,8.3494946461445601,8.3788894764157309,8.3941625894973289,8.4020982700592395,8.4062215306966905]
[null,null,null,null,"Coincident",5.7745246721949322,5.8513503340076216,5.891267796010629,5.9120083107704904,5.9227847712696891,5.9283840585697174,5.9312933642986803]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.1849040505017214,8.2937979779241733,8.3503776299269372,8.3797755687884496,8.3950502970469802,8.4029868168306088,8.4071105135150823]
[null,null,null,null,"Coincident",5.7751353452778647,5.851969131631777,5.8918908150245901,5.9126335231553018,5.9234111232971083,5.9290110027383482,5.9319206161350078]
[null,"Madgwick Dr","Substation Rating","MVA","Non-Coincident",34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996]
[null,null,null,null,"Coincident",31.35,31.35,31.35,31.35,31.35,31.35,31.35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.887952086310401,12.887952834377,12.8879528351251,12.8879528351258,12.8879528351258,12.8879528351258,12.8879528351258]
[null,null,null,null,"Coincident",5.6987543238787497,5.6987546546564971,5.6987546549872894,5.6987546549875994,5.6987546549875994,5.6987546549875994,5.6987546549875994]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.057161253157879,13.057162011046033,13.057162011803955,13.057162011804666,13.057162011804666,13.057162011804666,13.057162011804666]
[null,null,null,null,"Coincident",5.7735747037772942,5.7735750388979064,5.7735750392330418,5.7735750392333562,5.7735750392333562,5.7735750392333562,5.7735750392333562]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",12.248627469603599,12.2486283561934,12.248628357080001,12.2486283570809,12.2486283570809,12.2486283570809,12.2486283570809]
[null,null,null,null,"Coincident",5.4160597654709797,5.4160601575004836,5.4160601578925185,5.4160601578929155,5.4160601578929155,5.4160601578929155,5.4160601578929155]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.409442782639895,12.409443680869956,12.409443681768197,12.409443681769108,12.409443681769108,12.409443681769108,12.409443681769108]
[null,null,null,null,"Coincident",5.4871685773577772,5.4871689745343346,5.4871689749315165,5.4871689749319188,5.4871689749319188,5.4871689749319188,5.4871689749319188]
[null,"Maher Street","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.227154534194799,17.303813241700098,17.373369493927399,17.436481335769699,17.4937458440372,17.545704776170901,17.592849695601]
[null,null,null,null,"Coincident",16.183084562425417,16.255097287657669,16.320438009446953,16.379724891177595,16.433518823186461,16.482328729130241,16.526616380716092]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.367867668250138,17.445152531802524,17.515276926506552,17.578904272232215,17.636636522773255,17.689019860700043,17.7365498645824]
[null,null,null,null,"Coincident",16.31526962775013,16.387870560178129,16.453744991566762,16.513516134521172,16.567749460786999,16.616958050960648,16.661607448547105]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.4250535313416,15.501646641752702,15.5712655721813,15.6345453560679,15.692063203930401,15.744343768425701,15.791863930001901]
[null,null,null,null,"Coincident",14.490201802169382,14.562152905888903,14.627552507200615,14.686997152669846,14.741029070358863,14.79014111579384,14.834781267577544]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.551046922824685,15.6282656534792,15.698453238346392,15.762249897883892,15.820237557323273,15.872945154737195,15.920853465781315]
[null,null,null,null,"Coincident",14.608559230532281,14.681098038116826,14.747031829961763,14.80696202528487,14.861435281121864,14.910948478692518,14.955953255733963]
[null,"Mallanganee","Substation Rating","MVA","Non-Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,null,null,"Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.65984829192292,1.67491922331234,1.68821616264561,1.6999479256710099,1.71029874853592,1.71943118103977,1.72748863932362]
[null,null,null,null,"Coincident",1.1975591016079039,1.2084325839273027,1.2180261538936508,1.2264904693719638,1.2339584543627149,1.2405473864464629,1.2463607385164115]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.68285816112412,1.69813801531793,1.7116192852531735,1.7235136814144014,1.7340079939472559,1.7432670260195273,1.7514361818977344]
[null,null,null,null,"Coincident",1.2141604250076354,1.2251846424316508,1.2349112045462405,1.2434928577312474,1.2510643686638994,1.2577446407009192,1.2636385811423478]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.48463954329213,1.50124615554508,1.51597274644966,1.5290321517255399,1.5406131121300801,1.5508830012297898,1.55999024436301]
[null,null,null,null,"Coincident",1.0711482527217953,1.0831297089471434,1.0937547540547328,1.1031769462670089,1.1115324596023579,1.118942051926975,1.1255128102051963]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5052205577549069,1.5220573813938461,1.5369881216367378,1.5502285646669147,1.5619700676857586,1.5723823244982558,1.581615818008874]
[null,null,null,null,"Coincident",1.0859971888023747,1.098144739568969,1.1089170757870603,1.1184698844005152,1.1269412271582822,1.1344535359486472,1.1411153822433275]
[null,"Mandurama","Substation Rating","MVA","Non-Coincident",7.15,7.15,7.15,7.15,7.15,7.15,7.15]
[null,null,null,null,"Coincident",7.15,7.15,7.15,7.15,7.15,7.15,7.15]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.9491379620923899,1.9500010011298199,1.9507384289567402,1.9513685276849801,1.9519069185523099,1.9523669491999598,1.95276002458368]
[null,null,null,null,"Coincident",1.2897451019980319,1.2903161751560159,1.2908041313429788,1.2912210678371254,1.2915773212155952,1.2918817236160995,1.2921418217008576]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0097816059611717,2.0106714967828512,2.0114318682450523,2.0120815712720237,2.0126367131260232,2.0131110567342265,2.0135163618954421]
[null,null,null,null,"Coincident",1.3298730170908717,1.3304618580815537,1.3309649960780146,1.3313949047417861,1.3317622422525395,1.3320761155428056,1.3323443060745477]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.8048309620981799,1.80439866745205,1.80401748976256,1.8036813846725099,1.8033850225435899,1.8031237039439501,1.80289328512909]
[null,null,null,null,"Coincident",1.1942571221596194,1.1939710726786132,1.1937188473012559,1.1934964464747984,1.1933003435761704,1.1931274289900808,1.1929749607997047]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8609847738023739,1.8605390291475346,1.8601459918542085,1.8597994295067555,1.8594938466455158,1.8592243976249407,1.8589868097759634]
[null,null,null,null,"Coincident",1.2314141141286523,1.2311191647733468,1.2308590918930127,1.2306297714965824,1.230427567236954,1.230249272749194,1.2300920608070574]
[null,"Manildra","Substation Rating","MVA","Non-Coincident",52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004]
[null,null,null,null,"Coincident",52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.3667120509458,11.377913932167999,11.3884067116184,11.398235276875601,11.407441674043302,11.416065287621999,11.424143008993299]
[null,null,null,null,"Coincident",10.998636957859489,11.009476101514736,11.019629105420931,11.029139403614117,11.038047680667637,11.046392045739246,11.0542081955996]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.858188042292262,11.869874272520045,11.88082074070288,11.891074275276772,11.900678740342599,11.909675223315153,11.9181022106924]
[null,null,null,null,"Coincident",11.474198050468853,11.485505859015886,11.49609786037689,11.506019366596776,11.515312821375961,11.524017981642992,11.532172087632075]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.914372361301,10.9310714436448,10.946975897140899,10.9621235343464,10.976550368501101,10.9902906991483,11.003377193681398]
[null,null,null,null,"Coincident",10.560944861346846,10.577103196616152,10.592492634584909,10.607149763369906,10.621109430035835,10.634404823443544,10.647067553156011]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.386290005748455,11.403711126093455,11.420303259282132,11.436105852817905,11.45115647708767,11.465490914684706,11.479143245481191]
[null,null,null,null,"Coincident",11.017580942389637,11.03443793473844,11.050492784063451,11.065783660485197,11.080346917792179,11.094217179871331,11.10742742302574]
[null,"Manilla","Substation Rating","MVA","Non-Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,null,null,"Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5993991705849906,5.8631140069032401,6.1181947128956198,6.3649239734786294,6.6035752183503504,6.8344129250100201,7.0576929118567007]
[null,null,null,null,"Coincident",5.2150226429769244,5.4606345025338037,5.6982049305406042,5.9279972067163573,6.1502659908956838,6.3652576052472778,6.5732103072525137]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.2219476570176875,6.5149826520169301,6.7984235628448495,7.0725845036948263,7.3377693045345973,7.5942718478159357,7.8423763941604152]
[null,null,null,null,"Coincident",5.7948356468707587,6.0677549525944166,6.3317387699437297,6.5870796504195024,6.8340605672681676,7.0729552290776763,7.3040283831062371]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8768440551540495,5.0744611967001205,5.2618159076025401,5.4394411248418599,5.6078421095160405,5.7674978840732303,5.9188625949077496]
[null,null,null,null,"Coincident",4.5420680682135952,4.7261195773856883,4.9006131310435954,5.0660450821595173,5.2228860076625496,5.3715820470111391,5.5125561712522586]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4190579235729466,5.638646396080552,5.8468314475507706,6.0442052675911766,6.2313292928861124,6.4087358042228759,6.5769294405829015]
[null,null,null,null,"Coincident",5.0470611067515572,5.2515757022245282,5.4454696762512231,5.6292945669732104,5.8035732706749368,5.9688015291804133,6.1254493400080383]
[null,"Marilba","Substation Rating","MVA","Non-Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,null,null,"Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4018949019650699,1.4019597447029,1.40199905268467,1.4020228813736402,1.4020373264403199,1.4020460831097201,1.40205139144512]
[null,null,null,null,"Coincident",0.98852762600205379,0.98857334899997662,0.98860106650279911,0.9886178689872831,0.98862805473476834,0.98863422938423873,0.98863797248665219]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.443979805626463,1.4440465949441479,1.4440870829520549,1.4441116269785861,1.4441265056863601,1.4441355252310926,1.444140992922792]
[null,null,null,null,"Coincident",1.0182032385237967,1.0182503341267271,1.0182788837093542,1.0182961906046466,1.0183066821284072,1.018313042140937,1.0183168976113348]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.25945051083982,1.25949942345013,1.2595282678442399,1.25954527775367,1.2595553087156,1.25956122410259,1.25956471248223]
[null,null,null,null,"Coincident",0.88808484987170744,0.88811933995115888,0.88813967919370329,0.88815167350609003,0.88815874670606332,0.88816291786286683,0.8881653776475763]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2972592319791074,1.2973096129466315,1.2973393232498374,1.2973568437969756,1.2973671758885166,1.2973732688555029,1.2973768619563464]
[null,null,null,null,"Coincident",0.9147451689138868,0.91478069438598342,0.91480164421286048,0.91481399859466506,0.91482128413219599,0.91482558050718232,0.9148281141346617]
[null,"Martins Creek","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.7309349609122302,3.7608089916332603,3.7888479561625799,3.81516457674913,3.8398646514745201,3.8630474795824497,3.8848062606815703]
[null,null,null,null,"Coincident",3.379552878069807,3.406613351533037,3.4320115866311882,3.4558496893523891,3.4782234936403955,3.4992229466661851,3.518932470433612]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.7794999642319147,3.8097628605902019,3.8381668039839916,3.8648259839503054,3.8898475757280169,3.9133321711237219,3.9353741829109627]
[null,null,null,null,"Coincident",3.4235439951656619,3.4509567106264996,3.4766855506225585,3.5008339502398247,3.523498990877675,3.5447717905354996,3.5647378701253203]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2733769122992298,3.2997284066757202,3.3246803442028399,3.3483070568841797,3.3706789288688701,3.3918626061264598,3.4119211949857498]
[null,null,null,null,"Coincident",2.9650879687978473,2.9889576608708857,3.0115596073445321,3.0329611395819174,3.053226012903425,3.0724145965142431,3.090584053344672]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3159859532709657,3.3426804609739493,3.3679571940125248,3.3918914519584762,3.4145545351405171,3.4360139570484733,3.4563336454564677]
[null,null,null,null,"Coincident",3.0036840602753077,3.0278644604381175,3.0507606129531522,3.07244072562548,3.0929693836686303,3.1124077421043976,3.130813707944105]
[null,"Marulan North","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6598194868907905,5.9940019285666102,6.3268570417333505,6.6583900983644897,6.9886063494939403,7.3175110252991802,7.6451093351841299]
[null,null,null,null,"Coincident",3.5292552547566132,3.7376391336176846,3.9451953392417729,4.1519271590376263,4.357837867356853,4.562930725545753,4.7672089819970003]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.6736437586260129,6.0086424505185692,6.3423105718640214,6.6746534075127943,7.0056762213246007,7.3353842562517793,7.6637827344223677]
[null,null,null,null,"Coincident",3.5378755621317377,3.7467684246049693,3.954831592225553,4.162068360431828,4.3684820115730982,4.5740758149615974,4.7788530269242919]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.2686087194468598,5.5331637948313102,5.7930995592495398,6.0484966690025903,6.2994343720778199,6.5459905327389798,6.7882416556870107]
[null,null,null,null,"Coincident",3.2853106095401392,3.450277423788489,3.6123638056239944,3.7716200493493162,3.9280955710945022,4.0818389241504551,4.2328978140347155]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.2814774476409116,5.5466787063991454,5.8072493713913849,6.0632702959240046,6.314820921549849,6.5619793027183713,6.8048221309954418]
[null,null,null,null,"Coincident",3.2933350751094186,3.4587048255419957,3.6211871080227884,3.7808323396997379,3.9376900574032101,4.0918089330169147,4.2432367885804902]
[null,"Mates Gully","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.67143262742250598,0.67957218848762202,0.68720723591235,0.69436904091774099,0.701086936443724,0.70738843728939793,0.713299352806682]
[null,null,null,null,"Coincident",0.44113942441935988,0.44648721530208091,0.45150353457046166,0.45620892779808897,0.46062266708421501,0.46476282998739404,0.46864637356658523]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.7113501159430512,0.71997358383978238,0.72806254414494387,0.73565012719181389,0.74276740979937217,0.7494435425550785,0.75570586920829863]
[null,null,null,null,"Coincident",0.46736570117599857,0.4730314247483936,0.47834597031474207,0.48333110490803621,0.48800724637733139,0.49239354701408355,0.49650797199508645]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.61252528276212903,0.62036991635623207,0.62773150658259902,0.63463979745569499,0.64112270146417705,0.64720641234943399,0.65291551093966205]
[null,null,null,null,"Coincident",0.40243658059524023,0.40759060053282931,0.41242725508704292,0.41696608643811667,0.42122543343149438,0.42522250567470432,0.4289734530716377]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6489406578043897,0.65725166443228844,0.66505091017516205,0.67236990736540847,0.67923822792317534,0.6856836228397204,0.69173213430345282]
[null,null,null,null,"Coincident",0.42636192608794504,0.43182235879621389,0.43694655836203478,0.44175522877209,0.44626779913854964,0.45050250220109678,0.45447644799510389]
[null,"Menindee","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.98447484455321799,0.98085114956942598,0.97782120262583994,0.97528771718569895,0.97316934726209692,0.9713980755341749,0.96991702942453195]
[null,null,null,null,"Coincident",0.66919233866236782,0.66672914832874031,0.66466955554948404,0.66294743023969582,0.66150747783139363,0.66030346385727068,0.65929672943915707]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.0492017166235248,1.0453397723406925,1.0421106136150255,1.0394105575520969,1.0371529098604531,1.0352651812426783,1.0336867598851056]
[null,null,null,null,"Coincident",0.71319013823507904,0.71056499901419301,0.70836999292389335,0.70653464198398108,0.70500001614056251,0.70371684112042088,0.7026439163163869]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.912910398710302,0.91105976405769007,0.90948056587996995,0.90813299201875697,0.90698306964863107,0.90600180880989101,0.90516447156116997]
[null,null,null,null,"Coincident",0.62054672913393816,0.61928876856943738,0.61821531572540911,0.61729930846662073,0.61651765391810454,0.61585064628540853,0.61528147006437972]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.97293207921935676,0.97095976975395382,0.96927674306401879,0.96784056943674512,0.96661504241450069,0.96556926601690385,0.96467687584196793]
[null,null,null,null,"Coincident",0.66134619594868271,0.66000552747856256,0.6588614976713002,0.65788526512084167,0.65705221865079011,0.65634135685772588,0.65573475865822006]
[null,"Merrywinebone","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0330916880335597,3.1059766779292901,3.17878878283513,3.2515280756360601,3.3241946291441899,3.3967885160988098,3.4693098091664702]
[null,null,null,null,"Coincident",1.3688037960628925,1.4016960595044774,1.4345554306826231,1.4673819424895889,1.500175627784748,1.5329365193946112,1.5656646501128622]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.0330916880335597,3.1059766779292901,3.17878878283513,3.2515280756360601,3.3241946291441899,3.3967885160988098,3.4693098091664702]
[null,null,null,null,"Coincident",1.3688037960628925,1.4016960595044774,1.4345554306826231,1.4673819424895889,1.500175627784748,1.5329365193946112,1.5656646501128622]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.88865875050816,2.95807302659933,3.0274178884144098,3.0966934053676702,3.1658996468039899,3.2350366819988601,3.30410458015854]
[null,null,null,null,"Coincident",1.303622662917044,1.3349486280995051,1.3662432673167841,1.3975066118948438,1.4287386931283312,1.459939542280579,1.4911091905836769]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.88865875050816,2.95807302659933,3.0274178884144098,3.0966934053676702,3.1658996468039899,3.2350366819988601,3.30410458015854]
[null,null,null,null,"Coincident",1.303622662917044,1.3349486280995051,1.3662432673167841,1.3975066118948438,1.4287386931283312,1.459939542280579,1.4911091905836769]
[null,"Miller St","Substation Rating","MVA","Non-Coincident",38.4,38.4,38.4,38.4,38.4,38.4,38.4]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.9560374776984,14.569094042792299,15.1531467750145,15.7095678516958,16.239664532173901,16.744682229077199,17.225807434304599]
[null,null,null,null,"Coincident",6.8965236294903773,7.1994720196864135,7.4880878588940263,7.7630492230642751,8.0250021082348404,8.2745619482374195,8.5123150606016154]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.295260870404501,14.923218737409076,15.521467787867044,16.091413552032641,16.63439506423331,17.151688008805866,17.64450771719682]
[null,null,null,null,"Coincident",7.0641544593166765,7.3744664855663826,7.6700975856832034,7.9517423173183195,8.2200623784568982,8.4756881620157447,8.7192202368921503]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.0859493583968,13.6246637858209,14.133086106096099,14.6129196553663,15.065771990567901,15.493160275129199,15.896516361829999]
[null,null,null,null,"Coincident",6.4665603763756447,6.7327718124093057,6.9840140830854445,7.2211289099875797,7.4449106843901234,7.6561091286587359,7.8554318079992038]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.404023893896518,13.955832620906913,14.476612943565444,14.96810960027411,15.431969222163458,15.869745849699859,16.282906139091999]
[null,null,null,null,"Coincident",6.623740274575141,6.8964223973386716,7.1537715056889093,7.3966497805734104,7.6258709221931831,7.842202876092558,8.0463704059600616]
[null,"Moama","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.5947789973157,15.719033248432,15.8357473959563,15.945378994955499,16.0483578347453,16.145087623795899,16.235947572391701]
[null,null,null,null,"Coincident",13.566020207150483,13.674109951914307,13.775640501596834,13.871009886929025,13.960591984997732,14.04473798495834,14.123777764802831]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.089796142116015,16.217994532782317,16.338413478180012,16.451525057313958,16.557772702083707,16.657572935672263,16.751317005443386]
[null,null,null,null,"Coincident",13.996639492643592,14.108160275246703,14.212913657572294,14.311310304838532,14.403735961922653,14.49055296559893,14.572101665008809]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.211869519048399,14.3254825406934,14.432891430047601,14.534434979768101,14.630433481864401,14.721189737974301,14.8069900144705]
[null,null,null,null,"Coincident",12.363016437102614,12.461849293130699,12.55528512596023,12.643618653973112,12.727128501693221,12.806078078633309,12.880716410149702]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.662989671043171,14.7802090530987,14.89102736824492,14.995794163262078,15.094839897026169,15.188476982853503,15.277000773924776]
[null,null,null,null,"Coincident",12.755449385262205,12.857419442414583,12.953821161403662,13.044958615707168,13.131119274085654,13.212574907326173,13.289582445470392]
[null,"Molong 11kV","Substation Rating","MVA","Non-Coincident",13.2,13.2,13.2,13.2,13.2,13.2,13.2]
[null,null,null,null,"Coincident",12.100000000000001,12.100000000000001,12.100000000000001,12.100000000000001,12.100000000000001,12.100000000000001,12.100000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.5459587871518501,3.5459587871817,3.5459587871843801,3.5459587871846203,3.5459587871846501,3.5459587871846501,3.5459587871846501]
[null,null,null,null,"Coincident",2.7917535632524544,2.7917535632759551,2.7917535632780655,2.7917535632782546,2.7917535632782777,2.7917535632782777,2.7917535632782777]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5808671897196667,3.5808671897498106,3.5808671897525168,3.5808671897527593,3.5808671897527895,3.5808671897527895,3.5808671897527895]
[null,null,null,null,"Coincident",2.8192371475539035,2.8192371475776361,2.8192371475797668,2.8192371475799578,2.8192371475799813,2.8192371475799813,2.8192371475799813]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3981923108521901,3.3981927263469802,3.39819283812494,3.39819286819586,3.3981928762856599,3.3981928784619999,3.3981928790474898]
[null,null,null,null,"Coincident",2.6754161742693801,2.6754165013907962,2.6754165893942212,2.6754166130692276,2.6754166194383733,2.6754166211518182,2.6754166216127779]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.4316460175393364,3.4316464371244897,3.4316465500028541,3.4316465803698093,3.4316465885392495,3.4316465907370151,3.4316465913282688]
[null,null,null,null,"Coincident",2.7017544682129646,2.7017547985547474,2.701754887424527,2.7017549113326038,2.7017549177644509,2.7017549194947641,2.7017549199602615]
[null,"Monteagle","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.83158907818043704,0.83045902996101906,0.82940941584641203,0.82843451073116703,0.82752899700902693,0.82668793556811004,0.82590673885059906]
[null,null,null,null,"Coincident",0.66115739431306841,0.66025894608208235,0.65942444722771287,0.65864934598767699,0.65792941458314869,0.65726072615839148,0.65663963336178377]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.86489182100509532,0.86371651761552404,0.86262486948454875,0.86161092223276858,0.86066914529914118,0.85979440177460686,0.85898192038289634]
[null,null,null,null,"Coincident",0.68763484002171893,0.68670041153177719,0.68583249340644348,0.68502635159849101,0.68427758901875191,0.6835821215522494,0.68293615578145472]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.76830122384231192,0.76829700617325103,0.76829412400611496,0.76829215446149501,0.76829080856244691,0.76828988883499694,0.76828926033423206]
[null,null,null,null,"Coincident",0.61084019563434699,0.61083684236389224,0.610834550888254,0.61083298499588834,0.61083191493480771,0.61083118370273615,0.61083068401131535]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.79906947073352352,0.79906508415898791,0.79906208656937516,0.79906003815017679,0.79905863835175583,0.79905768179187553,0.79905702812146873]
[null,null,null,null,"Coincident",0.63530258273866724,0.63529909517940741,0.6352967119367825,0.63529508333494633,0.63529397042100733,0.63529320990520144,0.63529269020258117]
[null,"Moonee","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6676957853408707,5.7499008332013704,5.82372058758052,5.8900103870323104,5.9495383216389399,6.0029941327567204,6.0509972049469996]
[null,null,null,null,"Coincident",4.2085241066607946,4.2695651255709715,4.3243796794247551,4.373602896334198,4.4178051184188227,4.4574985102752018,4.4931429933522722]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.7456915989006072,5.8290279088876282,5.9038635314463068,5.9710655758446816,6.031412702211953,6.0856041437579602,6.1342678086848021]
[null,null,null,null,"Coincident",4.2664395760185121,4.3283206089503885,4.3838894915269302,4.4337900921553102,4.4786006016998154,4.5188402328936679,4.5549752363800557]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8732078440662203,5.0156421687916799,5.0889957428619601,5.1267727803791106,5.1462279273390301,5.15624731393227,5.1614072907708799]
[null,null,null,null,"Coincident",3.6185803658633913,3.7243443856566656,3.7788127792466959,3.8068639624948091,3.8213103015504832,3.8287501557008534,3.8325816751997066]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.9402703373331871,5.0846647674447762,5.1590277943692353,5.1973246993751534,5.2170475777152552,5.2272048457753746,5.2324358314695623]
[null,null,null,null,"Coincident",3.6683773433752731,3.7755968313308395,3.8308147899702747,3.8592519986759304,3.8738971405626459,3.8814393780270122,3.8853236248584189]
[null,"Moree","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",23.038782997886798,23.057805832681399,23.073853276599902,23.0873907151101,23.0988107420219,23.1084445449432,23.116571509918298]
[null,null,null,null,"Coincident",21.822213598658458,21.840231927325288,21.855431981465916,21.868254571737953,21.879071560925038,21.888196648180525,21.895894466490272]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",23.612218053252246,23.631714366195613,23.648161230816708,23.662035616022496,23.673739887278501,23.683613475448528,23.691942720492452]
[null,null,null,null,"Coincident",22.365368255060712,22.38383505972984,22.399413443050811,22.412555187453655,22.423641411382608,22.432993621959501,22.440883038882294]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.356123870618202,20.3592466167587,20.3617289133967,20.3637021114479,20.365270622837603,20.3665174454656,20.367508555046101]
[null,null,null,null,"Coincident",19.281213039166417,19.284170887820949,19.286522106088626,19.288391108863195,19.289876794568954,19.29105777837831,19.291996552139377]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.862787569818135,20.865988041075717,20.868532122049729,20.870554432978714,20.872161984599654,20.873439840629146,20.874455618916201]
[null,null,null,null,"Coincident",19.761122219596718,19.764153689071723,19.766563429136216,19.768478951369282,19.770001615775911,19.771211994259293,19.772174134088946]
[null,"Morrow St","Substation Rating","MVA","Non-Coincident",44,44,44,44,44,44,44]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.6330388704702,15.949912471531599,16.238746664222202,16.502022590609702,16.742001842268099,16.960745887789798,17.1601337812039]
[null,null,null,null,"Coincident",9.5312544680359625,9.7244480595662743,9.900546399269377,10.061062206240674,10.207374342579412,10.340739658082668,10.462303786830867]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.65519910430864,16.992791363900977,17.300510869190578,17.581000990764956,17.836671193493324,18.069717734299136,18.282142528436466]
[null,null,null,null,"Coincident",10.154451875561394,10.360277355768687,10.547889817683146,10.718900888956412,10.874779588055759,11.016864943418847,11.146377495969812]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.472838767987199,14.856549237806,15.207061975905301,15.527249172329501,15.8197345219629,16.086914723749899,16.330979119851801]
[null,null,null,null,"Coincident",8.8238960009950436,9.0578391364401263,9.2715420593838598,9.4667559056367896,9.6450803068377802,9.807976498240679,9.9567792924452583]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",15.419139764355595,15.827938995662549,16.201369874329881,16.542492387443357,16.854101779168168,17.138751455687395,17.3987739084575]
[null,null,null,null,"Coincident",9.4008430472139537,9.650082464591982,9.8777582709589584,10.085736099466891,10.275720173054097,10.449267269279494,10.607799476951296]
[null,"Moruya Town","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.1314520768958598,7.1314520806765307,7.1314520820936895,7.1314520826249099,7.1314520828240298,7.1314520828986696,7.1314520829266499]
[null,null,null,null,"Coincident",6.5201847560190727,6.5201847594756854,6.5201847607713734,6.5201847612570614,6.5201847614391131,6.5201847615073554,6.5201847615329376]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.2975130324007207,7.2975130362694278,7.297513037719586,7.2975130382631761,7.2975130384669322,7.2975130385433102,7.2975130385719424]
[null,null,null,null,"Coincident",6.6720119153378024,6.6720119188749063,6.6720119202007648,6.6720119206977619,6.6720119208840529,6.6720119209538842,6.6720119209800623]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4681166005809203,6.4681166003492896,6.4681166002873294,6.4681166002707595,6.4681166002663302,6.46811660026514,6.4681166002648194]
[null,null,null,null,"Coincident",5.9137066062454133,5.913706606033637,5.9137066059769872,5.9137066059618375,5.9137066059577883,5.9137066059567003,5.9137066059564072]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.6187313157087333,6.6187313154717096,6.6187313154083061,6.6187313153913507,6.6187313153868184,6.6187313153855998,6.618731315385272]
[null,null,null,null,"Coincident",6.0514114886479851,6.0514114884312775,6.0514114883733088,6.0514114883578065,6.0514114883536632,6.0514114883525485,6.0514114883522492]
[null,"Mossy Point","Substation Rating","MVA","Non-Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,null,null,"Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.2569199878599902,7.3859051869142602,7.5098475737994805,7.6289443025671098,7.7433848193233894,7.8533511635795499,7.9590182578204702]
[null,null,null,null,"Coincident",5.076548080479208,5.1667791379753067,5.2534825172718627,5.3367961366624703,5.4168525223798305,5.4937790194040241,5.5676979940290634]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.3803053748668104,7.5114836377456902,7.6375333483161603,7.7586550127307063,7.8750412981426763,7.9868773391801806,8.0943410324381233]
[null,null,null,null,"Coincident",5.1628618128362564,5.2546270189750039,5.3428045677576774,5.4275347224261505,5.508952262483179,5.5871866980849365,5.6623624760516833]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.4563277814434494,6.5670467672681694,6.67421723906617,6.7779529257675302,6.8783639113203998,6.9755567515116903,7.0696345870436996]
[null,null,null,null,"Coincident",4.5164971448853848,4.5939501491766501,4.6689208052952704,4.7414886718394733,4.8117307575755959,4.8797216031595116,4.9455333602389082]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5661011430471232,6.6787026224004808,6.7876952543105702,6.8931947013774124,6.9953129192454941,7.09415827541069,7.1898356642194754]
[null,null,null,null,"Coincident",4.5932886417007186,4.6720585364806908,4.7483038770983574,4.8221055748426824,4.8935419478173614,4.9626888040517079,5.0296195219478737]
[null,"Moulamein","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.1083948634335203,3.1427155804467901,3.1754239015244496,3.2065955774339701,3.2363028001526399,3.2646143700604799,3.29159585527831]
[null,null,null,null,"Coincident",2.7144935859736252,2.744465121216618,2.7730285861797532,2.8002501323596927,2.8261928034390822,2.8509166812924849,2.8744790251328491]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1083948634335203,3.1427155804467901,3.1754239015244496,3.2065955774339701,3.2363028001526399,3.2646143700604799,3.29159585527831]
[null,null,null,null,"Coincident",2.7144935859736252,2.744465121216618,2.7730285861797532,2.8002501323596927,2.8261928034390822,2.8509166812924849,2.8744790251328491]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.75331519116778,2.7868247895255398,2.8185030506901096,2.8484500592963098,2.8767604302412702,2.9035236076116799,2.9288241472744296]
[null,null,null,null,"Coincident",2.4044102358131849,2.4336734387867658,2.461337374845082,2.4874894457215708,2.512212276546784,2.5355839768950483,2.5576783875647222]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.75331519116778,2.7868247895255398,2.8185030506901096,2.8484500592963098,2.8767604302412702,2.9035236076116799,2.9288241472744296]
[null,null,null,null,"Coincident",2.4044102358131849,2.4336734387867658,2.461337374845082,2.4874894457215708,2.512212276546784,2.5355839768950483,2.5576783875647222]
[null,"Mt Gipps 33kV","Substation Rating","MVA","Non-Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.1880687245611501,1.25765208933615,1.32716587074638,1.3966101383752001,1.46598496173639,1.53529041027422,1.60452655336351]
[null,null,null,null,"Coincident",1.0362422476958735,1.0969333683575355,1.1575637978985405,1.2181335970100047,1.2786428263223562,1.3390915464053965,1.3994798177683518]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.2209821566088672,1.2924932106671783,1.3639327536714361,1.43530085713269,1.5065975924904811,1.5778230311129158,1.6489772442967261]
[null,null,null,null,"Coincident",1.0649495843165813,1.1273220496971992,1.189632142612441,1.2518799254347679,1.3140654604742712,1.376188809978736,1.438250036133695]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.0968355495857098,1.1582421419223199,1.2195873276666001,1.2808711682251301,1.34209372494311,1.40325505910436,1.4643552319314599]
[null,null,null,null,"Coincident",0.95666800392819729,1.0102272837499411,1.0637330042918691,1.1171852191132501,1.1705839817198169,1.223929345563767,1.2772213640438828]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.1272215210219538,1.1903292790086397,1.2533739292373458,1.3163555348158174,1.3792741587887187,1.4421298641376352,1.5049227137812142]
[null,null,null,null,"Coincident",0.98317087088241906,1.0382139198502522,1.0932019257691237,1.1481349436820711,1.203013028577113,1.2578362353872492,1.3126046189905853]
[null,"Mt Gipps 6.6kV","Substation Rating","MVA","Non-Coincident",3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005]
[null,null,null,null,"Coincident",3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.97155229850841707,0.97155092171693691,0.97154995580115799,0.97154927814349901,0.97154880271912702,0.97154846917558801,0.97154823517140398]
[null,null,null,null,"Coincident",0.40097732020733923,0.40097675198043159,0.40097635332940562,0.40097607364775334,0.40097587743146013,0.4009757397719696,0.40097564319418294]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.99093488800484419,0.99093348374620238,0.9909324985602832,0.99093180738326947,0.99093132247412197,0.99093098227634779,0.99093074360375111]
[null,null,null,null,"Coincident",0.40897686774264769,0.4089762881795424,0.40897588157537873,0.40897559631404262,0.40897539618320994,0.40897525577739541,0.40897515727286982]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.88323870585074404,0.88319948910715507,0.883171357563722,0.88315117782253405,0.88313670218754303,0.88312631830766997,0.88311886958702401]
[null,null,null,null,"Coincident",0.36452869281371109,0.36451250734971113,0.36450089694961596,0.36449256840306582,0.36448659404498346,0.36448230842872664,0.36447923420611589]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.90085942816198072,0.90081942903946732,0.90079073626823503,0.9007701539386942,0.90075538951298018,0.90074479847340894,0.90073720114985734]
[null,null,null,null,"Coincident",0.37180108568780001,0.37178457732177517,0.37177273529275034,0.3717642405906581,0.37175814704338705,0.37175377592855158,0.37175064037481642]
[null,"Mudgee","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",26.7750854976452,27.3744756509886,27.9564287613922,28.521452095224397,29.070038161812299,29.602665142743,30.119797308675999]
[null,null,null,null,"Coincident",25.103159947589223,25.665122182657068,26.210736201844547,26.740477596117863,27.254808120880746,27.754176098468747,28.23901680893449]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.193688994662395,28.824836169572929,29.437622448281118,30.032581973254185,30.610233348057253,31.17108008939994,31.71561106603243]
[null,null,null,null,"Coincident",26.433181115624855,27.02491735802235,27.599439219752821,28.157247489648135,28.698828387938882,29.224653990073669,29.735182638209061]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.979063970763601,23.460782428925597,23.935508496839297,24.403343672632001,24.8643879811335,25.318739995262302,25.766496857100201]
[null,null,null,null,"Coincident",21.544174652764248,21.995813005366713,22.44089559586585,22.879517584507703,23.311772750238422,23.737753510755049,24.157550942264123]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",24.196545816338809,24.703786788308893,25.203664897665256,25.696287020131408,26.18175848007478,26.660183073026033,27.131663087870205]
[null,null,null,null,"Coincident",22.685632875388727,23.161200030998952,23.629864085669286,24.091725241446969,24.546882245895002,24.995432413205272,25.437471645004024]
[null,"Mullumbimby","Substation Rating","MVA","Non-Coincident",31.2,31.2,31.2,31.2,31.2,31.2,31.2]
[null,null,null,null,"Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3768307728566995,8.3802137995180495,8.3830761140805699,8.3854978640325815,8.3875468606407306,8.3892804777289598,8.3907472581992799]
[null,null,null,null,"Coincident",5.7401475928460819,5.7424657812962536,5.7444271564859326,5.7460866387572658,5.7474906951679703,5.7486786406124644,5.7496837386757109]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3936517181837207,8.3970415380712993,8.399909600253423,8.4023362131571453,8.4043893242163143,8.4061264224633554,8.4075961482759851]
[null,null,null,null,"Coincident",5.7516739936349293,5.7539968370819894,5.7559621507760657,5.7576249653411162,5.7590318411422032,5.7602221720193167,5.7612292883517666]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.0542821023443807,8.0788651224166088,8.0881444651281598,8.0916471348939307,8.0929692862433811,8.0934683581821503,8.0936567426663899]
[null,null,null,null,"Coincident",5.5191240309739351,5.5359693233427061,5.542327909086314,5.5447280818926785,5.5456340741577383,5.5459760586940936,5.5461051474596497]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.0704553595780038,8.0950877431443526,8.1043857190741999,8.1078954223133959,8.1092202285852348,8.109720302676493,8.1099090654428281]
[null,null,null,null,"Coincident",5.5302066093493849,5.5470857276064462,5.5534570815945195,5.5558620740249927,5.5567698855516294,5.5571125568039221,5.557241904783865]
[null,"Mulwala","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.3443190538904,14.3634808163867,14.380722234098998,14.396235759265899,14.4101945570353,14.4227544383692,14.4340555992377]
[null,null,null,null,"Coincident",13.825849690496772,13.844318859167904,13.86093709310747,13.875889888449061,13.889344151359326,13.901450061078748,13.912342746253206]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.861708272776962,14.881561186194626,14.899424489380131,14.915497576185206,14.929959857699453,14.942972764873634,14.954681550445146]
[null,null,null,null,"Coincident",14.324538094242856,14.343673432476749,14.360891074101332,14.376383205961647,14.390322754409112,14.402865315540854,14.414150891995323]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.0071641838554,13.0284317703818,13.047992637331198,13.065983748609201,13.0825310767953,13.0977504851947,13.1117485391055]
[null,null,null,null,"Coincident",12.5370257193787,12.557524597958363,12.576378445620433,12.593719275767906,12.609668507754508,12.624337817055133,12.637829917210123]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.476323193197777,13.498357886196025,13.518624299475903,13.537264337132079,13.554408515483928,13.570176876942313,13.584679830538599]
[null,null,null,null,"Coincident",12.989227174166533,13.010465432478098,13.029999324796051,13.047965626151402,13.064490135406198,13.079688556088977,13.09366730654323]
[null,"Mumbil","Substation Rating","MVA","Non-Coincident",5.83,5.83,5.83,5.83,5.83,5.83,5.83]
[null,null,null,null,"Coincident",5.83,5.83,5.83,5.83,5.83,5.83,5.83]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.32857603364145,1.28100054941978,1.2351663464209701,1.1910096930751599,1.14846919041269,1.1074856866901099,1.0680021951407501]
[null,null,null,null,"Coincident",1.1066281248207863,1.0670004576353671,1.0288231784786692,0.99204320258485224,0.95660938811111651,0.92247246502603231,0.88958496660045305]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.3980643976180132,1.3480005781560216,1.2997691139543075,1.2533029400978264,1.208537446273463,1.1654103869307324,1.1238617947304694]
[null,null,null,null,"Coincident",1.1645079720986886,1.1228076634601678,1.0826336023335255,1.0439299274663394,1.0066428221497152,0.97072043938726893,0.93611282980281885]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2011487171416799,1.16712845634578,1.13482963808338,1.1041651564849799,1.0750523132825298,1.04741259478243,1.02117146012404]
[null,null,null,null,"Coincident",1.0004884318424454,0.97215149330284722,0.94524841829427519,0.91970665259131434,0.89545731324938282,0.87243500283595066,0.85057763306194434]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2639722644082627,1.2281726457096889,1.1941845059612775,1.1619161834049594,1.131280654414403,1.1021952988030568,1.0745816770079673]
[null,null,null,null,"Coincident",1.0528168666070385,1.0229978243342999,0.99468764079678618,0.96780996697352983,0.94229231714298833,0.91806587339801848,0.89506530005269402]
[null,"Munga","Substation Rating","MVA","Non-Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,null,null,"Coincident",6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009,6.8750000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.6676965773886601,1.66949632864361,1.67101606115969,1.67229934234317,1.67338296105795,1.6742979822817798,1.6750706376712001]
[null,null,null,null,"Coincident",1.2418432503783763,1.2431834275896405,1.2443150900233606,1.2452706799655895,1.2460775920892808,1.246758958799612,1.2473343133894275]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7107398168929255,1.7125860197178824,1.7141449765218568,1.7154613791856355,1.7165729660934932,1.7175116040100853,1.7183042016308634]
[null,null,null,null,"Coincident",1.2738952178510747,1.2752699850288021,1.2764308556637221,1.2774111093771126,1.2782388478982849,1.2789378006796681,1.2795280051682871]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4254132198066201,1.4260683880292799,1.4266083187741001,1.42705328115036,1.4274199791355799,1.42772217864623,1.42797122431303]
[null,null,null,null,"Coincident",1.0614279659845014,1.0619158342491508,1.0623178914100384,1.0626492307742386,1.0629222908884386,1.0631473224845074,1.0633327732940521]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4622031271821894,1.4628752052930782,1.4634290716474572,1.4638855185002049,1.4642616809584095,1.4645716802367699,1.4648271537708624]
[null,null,null,null,"Coincident",1.0888234159577423,1.0893238760996233,1.0897363103536255,1.0900762015849961,1.0903563093792441,1.0905871490395718,1.0907773863334922]
[null,"Mungindi","Substation Rating","MVA","Non-Coincident",18.599999999999998,18.599999999999998,18.599999999999998,18.599999999999998,18.599999999999998,18.599999999999998,18.599999999999998]
[null,null,null,null,"Coincident",17.05,17.05,17.05,17.05,17.05,17.05,17.05]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.2690239048415197,6.4718934917580304,6.6640570327851902,6.8460795185671302,7.0184961234711301,7.1818137790834102,7.3365126646666106]
[null,null,null,null,"Coincident",2.3845078746165047,2.4616720607586289,2.5347640578141157,2.6039987676018876,2.669579750917443,2.7316998260332253,2.7905416356142436]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.5990961771406527,6.8126471119911223,7.014928313694436,7.2065345203878852,7.3880290840661074,7.5599456269234784,7.7227896102861209]
[null,null,null,null,"Coincident",2.5100553193920789,2.5912823004200822,2.6682226863031113,2.7411026937207059,2.8101366012093307,2.8755273791745664,2.9374672866555791]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.0863285251854204,6.2694169948282301,6.4426183564522894,6.6064665317467401,6.76146660966526,6.9080964034458106,7.0468079235486005]
[null,null,null,null,"Coincident",2.3150172205595658,2.3846573916997014,2.4505368678280206,2.5128587332669818,2.5718151054188643,2.6275877269992494,2.6803485262888622]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.4067816478343076,6.5995099638270567,6.7818306026885828,6.9543055977802499,7.1174666316468871,7.2718166750156588,7.4178315372861245]
[null,null,null,null,"Coincident",2.4369058919062478,2.5102127087444117,2.5795608250810984,2.6451640178928062,2.7072245198132245,2.7659336425485828,2.8214723666274746]
[null,"Murgha","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.55761371064779308,0.55761363630994798,0.55761359739154504,0.55761357701643199,0.55761356634936399,0.55761356076478896,0.55761355784107303]
[null,null,null,null,"Coincident",0.32140234710949189,0.32140230426198396,0.32140228182984892,0.32140227008586014,0.32140226393748067,0.32140226071859368,0.32140225903339631]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.64474085293651073,0.64474076698337734,0.64474072198397392,0.6447406984252495,0.64474068609145208,0.64474067963428727,0.64474067625374065]
[null,null,null,null,"Coincident",0.37162146384535,0.37162141430291895,0.37162138836576281,0.37162137478677582,0.37162136767771198,0.37162136395587397,0.37162136200736445]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.5231326128168019,0.52313257626299803,0.52313255765823397,0.52313254818898103,0.52313254336942205,0.52313254091641503,0.52313253966790896]
[null,null,null,null,"Coincident",0.30152782544301782,0.30152780437381138,0.30152779365023213,0.30152778819225995,0.30152778541431968,0.30152778400043367,0.30152778328080865]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.60487208356942723,0.60487204130409145,0.60487201979233307,0.60487200884350933,0.6048720032708943,0.60487200043460487,0.60487199899101973]
[null,null,null,null,"Coincident",0.34864154816848936,0.34864152380721941,0.34864151140808092,0.34864150509730057,0.34864150188530718,0.34864150025050145,0.34864149941843503]
[null,"Murrami","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.74592512646993203,0.73701258118429402,0.72861800470461502,0.72071129433011194,0.71326409683329905,0.70624970678615895,0.69964297079527293]
[null,null,null,null,"Coincident",0.456034101897132,0.45058526468717208,0.44545309657824389,0.44061919376863984,0.43606622202711676,0.43177785453285905,0.42773871332798558]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.79519514250404411,0.78569390375099835,0.77674484679723921,0.76831588059154776,0.76037677911261048,0.75289907297940739,0.74585594736085914]
[null,null,null,null,"Coincident",0.48615617007159684,0.48034742502749206,0.47487626578387282,0.46972307292693705,0.46486936726085865,0.46029774354194181,0.45599180806393536]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.67589637902816502,0.66797102858526403,0.66014585669145298,0.65241959706308295,0.64479099942266394,0.63725882929655198,0.62982186781517802]
[null,null,null,null,"Coincident",0.41322082773150487,0.40837552899682805,0.40359147613394514,0.39886789497865899,0.39420402115241204,0.38959909993859859,0.38505238616043141]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.72054084031573951,0.71209200282361462,0.70374996089687902,0.69551336461102831,0.68738088110495954,0.6793511943652949,0.67142300501341545]
[null,null,null,null,"Coincident",0.44051498378750281,0.43534964227926054,0.43024959206905966,0.42521400785743357,0.42024207477691844,0.41533298826019566,0.41048595390989145]
[null,"Murrumbateman","Substation Rating","MVA","Non-Coincident",15,15,15,15,15,15,15]
[null,null,null,null,"Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0295351758210503,6.0296878422937397,6.0297772097243501,6.0298295233562405,6.0298601465493,6.0298780726599501,6.0298885661915005]
[null,null,null,null,"Coincident",5.3950091177059143,5.3951457181217188,5.3952256808533248,5.3952724891914139,5.3952998897125068,5.3953159293453448,5.3953253185763117]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0295351758210503,6.0296878422937397,6.0297772097243501,6.0298295233562405,6.0298601465493,6.0298780726599501,6.0298885661915005]
[null,null,null,null,"Coincident",5.3950091177059143,5.3951457181217188,5.3952256808533248,5.3952724891914139,5.3952998897125068,5.3953159293453448,5.3953253185763117]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.7682243475808503,5.7683978788214798,5.76850445330229,5.7685699061851299,5.76861010417473,5.7686347918324401,5.7686499537957499]
[null,null,null,null,"Coincident",5.1611976778847355,5.1613529473372068,5.1614483063124705,5.1615068711751686,5.161542838876505,5.1615649284961123,5.1615784948702874]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7682243475808503,5.7683978788214798,5.76850445330229,5.7685699061851299,5.76861010417473,5.7686347918324401,5.7686499537957499]
[null,null,null,null,"Coincident",5.1611976778847355,5.1613529473372068,5.1614483063124705,5.1615068711751686,5.161542838876505,5.1615649284961123,5.1615784948702874]
[null,"Murrumburrah","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.1703707323182897,5.1703707323065702,5.1703707323058694,5.1703707323058294,5.1703707323058197,5.1703707323058197,5.1703707323058197]
[null,null,null,null,"Coincident",4.8010585371526968,4.8010585371418149,4.8010585371411638,4.8010585371411265,4.8010585371411176,4.8010585371411176,4.8010585371411176]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.4042684559231651,5.4042684559109153,5.4042684559101826,5.4042684559101408,5.4042684559101311,5.4042684559101311,5.4042684559101311]
[null,null,null,null,"Coincident",5.0182492805000818,5.0182492804887069,5.0182492804880265,5.0182492804879875,5.0182492804879786,5.0182492804879786,5.0182492804879786]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.7849265218814399,4.7849265209321006,4.7849265209311493,4.7849265209311493,4.7849265209311493,4.7849265209311493,4.7849265209311493]
[null,null,null,null,"Coincident",4.4431460560327656,4.4431460551512361,4.4431460551503523,4.4431460551503523,4.4431460551503523,4.4431460551503523,4.4431460551503523]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0013874835856003,5.0013874825933149,5.001387482592321,5.001387482592321,5.001387482592321,5.001387482592321,5.001387482592321]
[null,null,null,null,"Coincident",4.6441455204723425,4.6441455195509347,4.6441455195500119,4.6441455195500119,4.6441455195500119,4.6441455195500119,4.6441455195500119]
[null,"Murrurundi","Substation Rating","MVA","Non-Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.8027162387472697,2.8027162335950804,2.8027162313178802,2.8027162303113902,2.80271622986653,2.8027162296698998,2.8027162295829999]
[null,null,null,null,"Coincident",2.3309914633524831,2.3309914590674579,2.3309914571735328,2.3309914563364451,2.3309914559664593,2.3309914558029239,2.3309914557306501]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8717972728009,2.8717972675217198,2.8717972651883916,2.8717972641570935,2.8717972637012688,2.8717972634997917,2.87179726341075]
[null,null,null,null,"Coincident",2.3884454782942699,2.3884454739036278,2.3884454719630219,2.3884454711053014,2.3884454707261962,2.3884454705586298,2.3884454704845748]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4530634399850602,2.4530634370738,2.4530634358904901,2.4530634354095202,2.4530634352140201,2.4530634351345602,2.4530634351022598]
[null,null,null,null,"Coincident",2.040188677903068,2.0401886754818017,2.0401886744976543,2.0401886740976365,2.0401886739350408,2.040188673868955,2.0401886738420911]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5135262712522977,2.5135262682692812,2.5135262670568053,2.5135262665639804,2.5135262663636615,2.5135262662822431,2.5135262662491464]
[null,null,null,null,"Coincident",2.0904750185556082,2.090475016074663,2.0904750150662585,2.0904750146563811,2.0904750144897779,2.0904750144220632,2.0904750143945368]
[null,"Murwillumbah","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.527664220359199,18.3481993868104,18.183463257953001,18.032247046875302,17.8934411719815,17.766027115196501,17.649069948370499]
[null,null,null,null,"Coincident",13.443730283126888,13.313510046574612,13.193977003558228,13.084254054567653,12.98353608377589,12.891084051327338,12.806219570473909]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.141227254920274,18.955819255165547,18.785627716607202,18.629403822087049,18.486001245050883,18.354367738129213,18.233537412045902]
[null,null,null,null,"Coincident",13.888933512753209,13.754400896477833,13.630909391362223,13.517552851826023,13.413499499787124,13.317985821309916,13.230310964157587]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.700094251822897,17.642068930752199,17.5862213431116,17.532469756946899,17.480735507764599,17.430942883408399,17.3830190132552]
[null,null,null,null,"Coincident",12.843242962378037,12.801139610504404,12.760616428722077,12.721614112073095,12.684075581358432,12.647945899604039,12.613172191661123]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.286251438827168,18.226304548385716,18.168607509301147,18.113075882979878,18.05962839987119,18.008186840531316,17.958675921150032]
[null,null,null,null,"Coincident",13.268560424518929,13.225062775985259,13.183197626532927,13.142903707258084,13.104122048724159,13.066795894661588,13.030870618905553]
[null,"Nambucca Heads","Substation Rating","MVA","Non-Coincident",57,57,57,57,57,57,57]
[null,null,null,null,"Coincident",52.250000000000007,52.250000000000007,52.250000000000007,52.250000000000007,52.250000000000007,52.250000000000007,52.250000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.0488528605398812,9.1335747408914987,9.18070421039344,9.2069216041330009,9.2215059341023089,9.2296189709192689,9.2341321276108701]
[null,null,null,null,"Coincident",6.2726336478144038,6.3313625635775406,6.3640325495699832,6.3822063566440175,6.3923161639650363,6.397940093153446,6.4010685978333104]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0915310959391977,9.1766525606811076,9.2240043127888818,9.2503453588983984,9.2649984747654504,9.2731497761116728,9.2776842187680977]
[null,null,null,null,"Coincident",6.3022180536524637,6.3612239599391849,6.3940480314686754,6.4123075539398284,6.4224650434083337,6.4281154974366848,6.4312587574740769]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.5253147344551401,8.5902920223587902,8.6275168305846801,8.6488425336443111,8.6610598057449,8.6680589530725385,8.6720686913275689]
[null,null,null,null,"Coincident",5.9097188213491059,5.9547608536077501,5.9805649625052864,5.9953478664420352,6.0038168373982153,6.0086686222277388,6.0114481589806363]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.5655237415743724,8.6308074899798672,8.6682078662200297,8.6896341503576444,8.7019090443051876,8.7089412025859101,8.7129698524704899]
[null,null,null,null,"Coincident",5.9375915666449393,5.982846036268322,6.0087718483088732,6.0236244747025811,6.0321333889246782,6.0370080568332227,6.0398007030626113]
[null,"Nana Glen","Substation Rating","MVA","Non-Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,null,null,"Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.8653974361603893,5.8355572319684494,6.8047468679807102,7.7729673143569498,8.7402195402868088,9.7065045139907511,10.671823202720999]
[null,null,null,null,"Coincident",3.630941652655586,4.3549510801590534,5.0782364982350243,5.8007986308929125,6.5226382014181397,7.243755932372852,7.9641525455966153]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.1213015685948911,6.1424886245860417,7.1626544935212095,8.1818001965874334,9.1999267539505869,10.217035184756389,11.233126507131397]
[null,null,null,null,"Coincident",3.8219174127522568,4.5840073890394004,5.345335275350263,6.1059018337748086,6.8657078256409259,7.6247540115151864,8.3830411512035816]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.3600349631197299,3.8078337040546097,4.2303648113764503,4.6290540445839694,5.0052467128187503,5.3602122143825701,5.6951483201065098]
[null,null,null,null,"Coincident",2.5075219572603737,2.8417045439454838,3.1570304381294312,3.4545636535168485,3.735308165438008,4.0002112985931442,4.2501669236388633]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.5367619095755805,4.0081134126039588,4.4528682864041889,4.8725272808025766,5.2685064638403114,5.6421420000546929,5.9946946591395669]
[null,null,null,null,"Coincident",2.6394094832955699,2.9911689906829406,3.3230800046734528,3.6362625026432718,3.931773265770341,4.2106094449630778,4.4737119255768638]
[null,"Nangus","Substation Rating","MVA","Non-Coincident",4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,null,null,null,"Coincident",4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3059165062131699,1.2962875373799501,1.2869910220385299,1.27801548177143,1.2693498344694401,1.26098338064852,1.2529057902391301]
[null,null,null,null,"Coincident",0.97298985651430059,0.96581566968165022,0.95888918159064596,0.95220184009900066,0.94574538833899013,0.93951185452268526,0.93349354209917212]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4196273689624317,1.4091599710656368,1.3990539745858706,1.3892969016384216,1.3798767051548402,1.3707817540084002,1.3620008186531298]
[null,null,null,null,"Coincident",1.0577115944693161,1.0499127253002498,1.0423831228961151,1.035113490448734,1.0280948521351141,1.0213185420349837,1.0147761934309674]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.12069266943983,1.10814926439027,1.0956184027457601,1.08310007196289,1.07059425951081,1.05810095287118,1.0456201395381799]
[null,null,null,null,"Coincident",0.83498645927743154,0.8256408343302728,0.81630455500806165,0.80697761196516926,0.7976599958653251,0.78835169738157918,0.77905270719630981]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2182754243192409,1.2046398197276633,1.1910178507406781,1.1774095037226748,1.1638147650516975,1.1502336211193886,1.1366660583310018]
[null,null,null,null,"Coincident",0.90769174343354553,0.89753236119745095,0.88738313834359306,0.8772440647125852,0.86711513015521424,0.85699632453239893,0.8468876377151987]
[null,"Narooma","Substation Rating","MVA","Non-Coincident",34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996,34.199999999999996]
[null,null,null,null,"Coincident",31.35,31.35,31.35,31.35,31.35,31.35,31.35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.7966635832411102,7.8055130589579402,7.8072034349868797,7.8075263209081003,7.8075879967224404,7.8075997776822996,7.8076020280135898]
[null,null,null,null,"Coincident",6.1522060036493134,6.1591889646367877,6.1605228097415088,6.1607775931731421,6.1608262604410333,6.1608355565830566,6.1608373322787147]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.8826482932851247,7.8915953645433587,7.8933043827121274,7.8936308295478357,7.8936931855476109,7.8937050964325861,7.8937073715814252]
[null,null,null,null,"Coincident",6.2200549808056325,6.2271149526669687,6.2284635079465431,6.2287211012312955,6.2287703052211922,6.2287797038847712,6.2287814991635075]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.4384539282283502,7.4515660748961299,7.4551439696093507,7.45612026516973,7.4563866656922801,7.4564593580625997,7.4564791935368406]
[null,null,null,null,"Coincident",5.8695492535399891,5.8798958109602228,5.8827190628679249,5.8834894400098623,5.8836996518365892,5.8837570120692479,5.8837726638826693]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.5204881595846036,7.5337449122261111,7.5373622653866796,7.5383493279231866,7.5386186664167596,7.5386921604674804,7.5387122146952281]
[null,null,null,null,"Coincident",5.9342809795233356,5.9447416428980242,5.9475960307517726,5.9483749039195377,5.9485874340459803,5.9486454268701223,5.9486612512979722]
[null,"Narrabri","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.036225332122701,21.0966511407719,21.151314548631198,21.2007650769003,21.2454998426579,21.285968556288097,21.322578042336499]
[null,null,null,null,"Coincident",19.379983465606387,19.435651778434789,19.486011380680978,19.531568528177267,19.572781198560492,19.610063695236832,19.643790812298036]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.544168447148671,21.606053304319584,21.662036621108722,21.712681187517848,21.758496124071783,21.799941999913255,21.837435462820114]
[null,null,null,null,"Coincident",19.847934774135108,19.904947260444253,19.956522851435217,20.003180027051837,20.045387823311618,20.083570547438402,20.118112043345164]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.5966359402831,19.649824850560599,19.698191595270298,19.742173357288401,19.782167684006399,19.818536080729,19.851607278289002]
[null,null,null,null,"Coincident",18.053737042085185,18.102738238138997,18.147296931438781,18.187815884209147,18.224661343804474,18.258166353188372,18.288633761279975]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",20.06981856437001,20.124291780189239,20.173826393876556,20.21887014457614,20.259830178904497,20.297076731114984,20.330946469612872]
[null,null,null,null,"Coincident",18.489664652016867,18.53984903658338,18.585483649213693,18.626980977275387,18.664716111573561,18.699030136765515,18.730233214395184]
[null,"Narrandera","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.2179429573094,10.170820778231001,10.134853557908301,10.107400647982601,10.086446505387599,10.070452714817501,10.058245041053601]
[null,null,null,null,"Coincident",9.9857169810069148,9.9396657605439334,9.9045159770467492,9.8776869968920877,9.8572090848106075,9.8415787894807387,9.8296485628478383]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.486723022474315,10.438361307961404,10.401447980201764,10.373272929337363,10.351767594018376,10.335353091364679,10.322824298236199]
[null,null,null,null,"Coincident",10.248388408327171,10.201125823689555,10.16505143519718,10.137516726397877,10.116500148699776,10.100458702924573,10.088214655094468]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.4745634627983808,9.4368394267753395,9.4073115004673493,9.3841989567427806,9.3661079580099802,9.3519474986918496,9.3408636104520699]
[null,null,null,null,"Coincident",9.2592324750075079,9.222365803439537,9.1935089663658189,9.1709217077258991,9.1532418680552077,9.1394032373579446,9.128571255669069]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7237891431118904,9.6850727871177043,9.6547681371589373,9.6310476245863939,9.6124807473094851,9.5979478011616486,9.5865723544138781]
[null,null,null,null,"Coincident",9.5027939353138926,9.464957496501393,9.4353415885871428,9.4121601785730675,9.394015275779724,9.3798126238625201,9.3686957099953805]
[null,"Narromine","Substation Rating","MVA","Non-Coincident",52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004]
[null,null,null,null,"Coincident",52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004,52.800000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.448227809035599,15.4882594791299,15.523375533754701,15.5541795768913,15.5812010940775,15.604904553646501,15.6256973903945]
[null,null,null,null,"Coincident",13.548811054604888,13.583920682777949,13.614719088587082,13.641735660671264,13.665434782362778,13.686223813895122,13.704460094449136]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.505753002169785,15.545933739819414,15.581180557522632,15.612099306925391,15.639221445232288,15.663013170336113,15.683883434214557]
[null,null,null,null,"Coincident",13.599263312448917,13.634503679769955,13.6654167708533,13.692533945643902,13.716321316717112,13.737187761210265,13.755491948942622]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.7881459343829,13.802087579763599,13.8139652005567,13.824084370271001,13.832705423046701,13.840050151227,13.846307511371601]
[null,null,null,null,"Coincident",12.092842387332379,12.105069855841284,12.115487079220774,12.124362059586376,12.131923122032738,12.13836478871402,12.143852783281929]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.839489413236429,13.853482973688102,13.865404823660015,13.875561674537447,13.884214829877408,13.891586907920249,13.897867568850886]
[null,null,null,null,"Coincident",12.137872995533643,12.150145995963506,12.160602010380662,12.169510038871001,12.177099256752594,12.183564910529647,12.189073340965757]
[null,"Nericon","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8366277212150302,1.8365771883656201,1.83655031616123,1.83653602614242,1.8365284270398399,1.83652438601227,1.83652223708697]
[null,null,null,null,"Coincident",0.92680553435157398,0.92678003428753886,0.92676647394133405,0.92675926286182886,0.92675542817598255,0.92675338897845061,0.92675230458021474]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0016088110996035,2.0015537389717788,2.0015244528837712,2.0015088792173006,2.001500597500486,2.0014961934744027,2.0014938515148617]
[null,null,null,null,"Coincident",1.010058871651319,1.0100310809606599,1.0100163025120219,1.0100084436737238,1.0100042645246838,1.0100020421495666,1.0100008603417137]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6326215578022099,1.59601396658773,1.5676569708852601,1.5456910567512601,1.5286758063063601,1.5154954421322899,1.5052856600122]
[null,null,null,null,"Coincident",0.82385922731894867,0.80538617600596152,0.79107656919176927,0.7799920524160916,0.77140575694719893,0.76475463526358622,0.75960253913429376]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.7792771270631746,1.7393811392798908,1.7084768837256799,1.6845378095373706,1.6659941085901548,1.6516297751111482,1.6405028659313936]
[null,null,null,null,"Coincident",0.89786507600810128,0.87773262246356443,0.86213760843224529,0.85005738869653313,0.84069980116438459,0.83345122072980005,0.82783632072099389]
[null,"Nevertire","Substation Rating","MVA","Non-Coincident",40.799999999999997,40.799999999999997,40.799999999999997,40.799999999999997,40.799999999999997,40.799999999999997,40.799999999999997]
[null,null,null,null,"Coincident",37.400000000000006,37.400000000000006,37.400000000000006,37.400000000000006,37.400000000000006,37.400000000000006,37.400000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.5835239816014806,9.8961204504189695,10.1858138122189,10.454282116382499,10.703080466101799,10.933650026318301,11.147326371673399]
[null,null,null,null,"Coincident",6.0691537900225727,6.267118134569901,6.4505781611830573,6.6205965624354075,6.778158170258286,6.9241756605821303,7.0594948400133859]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.9044146751258069,10.227477992866998,10.526871325570726,10.804328909719198,11.061457918926845,11.299747773497021,11.520578767891699]
[null,null,null,null,"Coincident",6.2723707874991828,6.4769636870474514,6.666566612169226,6.8422778381898457,7.0051151727395693,7.1560218514065159,7.2958720014304479]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.8277209249285207,9.0978413430093799,9.3463312334360307,9.5749227115736097,9.7852091895764204,9.9786564833736584,10.1566130302372]
[null,null,null,null,"Coincident",5.5905109656582095,5.761575634803429,5.9189418983157349,6.0637066882373762,6.1968790971979457,6.3193874123618752,6.4320855861160888]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.1233046262139581,9.4024696429684838,9.6592798645620288,9.8955254037834166,10.112853025930558,10.312777627697827,10.49669279686459]
[null,null,null,null,"Coincident",5.777701287753656,5.954493814462011,6.1171292638742791,6.266741297244681,6.4043727952367702,6.5309831273926671,6.647454839482501]
[null,"North St","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.2487619720496,13.4903579940051,13.718231417687901,13.933161683511701,14.135883959855001,14.3270916577021,14.5074388024531]
[null,null,null,null,"Coincident",10.468415896631942,10.65931129064216,10.839363870342327,11.009189505081926,11.16936908297386,11.3204504978203,11.46295052318165]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.375391595286443,13.619296754752321,13.849348157467995,14.066332693618403,14.270992558208002,14.464027789736319,14.646098664677343]
[null,null,null,null,"Coincident",10.568471400963116,10.761191343702652,10.942964838185523,11.114413640145457,11.276124189734331,11.428649617438762,11.572511636061128]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.067960402814501,11.234526644664701,11.3950178270153,11.5496555214614,11.698653218365299,11.842216621597499,11.980543932528301]
[null,null,null,null,"Coincident",8.7452709067118892,8.8768820487722166,9.0036930253851768,9.1258789097850332,9.2436083898769024,9.3570440011242866,9.4663423509430302]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.173746261052838,11.341904517348912,11.503929649663799,11.660045347339729,11.810467141246948,11.955402701341823,12.095052123372778]
[null,null,null,null,"Coincident",8.8288568570336867,8.9617259180881064,9.089748934454267,9.2131026526893951,9.3319573729915817,9.446477184313224,9.5568201908996837]
[null,"Nundle","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.63006946376498,1.5610570184550399,1.49323556577651,1.4265845519953499,1.3610837780866201,1.3805679153633801,1.3558802433322201]
[null,null,null,null,"Coincident",1.3164859100770894,1.2607496890815399,1.2059753442839751,1.1521462759615824,1.0992461708637173,1.1149820598948614,1.0950436627258484]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.7477810079421159,1.6737849949465939,1.6010659792496837,1.5296019228788962,1.4593711681853072,1.4802623055542654,1.4537918726889663]
[null,null,null,null,"Coincident",1.4115527724454522,1.3517916943589476,1.2930619520456716,1.2353457470737705,1.1786255881704559,1.1954978065654898,1.174119606019165]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.4696987165341,1.43296558223116,1.3993682683018902,1.36863907721374,1.3405331641362801,1.3148265860603598,1.29131451745926]
[null,null,null,null,"Coincident",1.1869663811176614,1.1572997596528951,1.1301657071554261,1.1053480242315474,1.0826489679159559,1.0618876760903426,1.042898726405572]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.5758294730718021,1.5364437438596377,1.5004202807442566,1.4674720550599083,1.4373365410958612,1.4097736243373933,1.3845636882752088]
[null,null,null,null,"Coincident",1.272680302342218,1.2408713771899327,1.2117779043792436,1.1851680721974303,1.160829858146744,1.1385693395861789,1.1182091485896832]
[null,"Nymboida","Substation Rating","MVA","Non-Coincident",1.44,1.44,1.44,1.44,1.44,1.44,1.44]
[null,null,null,null,"Coincident",1.32,1.32,1.32,1.32,1.32,1.32,1.32]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.53328691924312399,0.542444472607571,0.54991506946325497,0.556009472101064,0.56098119581059203,0.56503705462283005,0.56834576437137896]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.5354547522481774,0.54464953143930916,0.55215049657489423,0.55826967320716592,0.56326160717567575,0.56733395321885782,0.570656113007035]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.51169183851184197,0.5204545579639801,0.52756853722125296,0.53334399324827197,0.53803277446532694,0.54183934302001102,0.54492969070115393]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.51377188663587392,0.52257022689879307,0.52971312477093291,0.53551205826147641,0.54021989956477956,0.54404194197537692,0.54714485204546759]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,"Nyngan Town","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.6860136507094801,9.5195857145375395,10.3523242063018,11.1842299595742,12.0153038070934,12.845546580765101,13.6749591116631]
[null,null,null,null,"Coincident",8.4324556941587527,9.2416945209414454,10.050124108897382,10.857745267265271,11.66455880447486,12.47056552814726,13.275766245095959]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.7411349456118135,9.5799968435801706,10.418019879650588,11.255204892684839,12.091552720706128,12.927064200899416,13.76174016961248]
[null,null,null,null,"Coincident",8.4859679145811349,9.3003421571956757,10.113902025567629,10.926648334071118,11.738581896266174,12.549703524899053,13.360014031903271]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.6881799319660704,8.3227644682283106,8.9567144199542916,9.5900304217285388,10.222713107501001,10.854763110587701,11.486181063671399]
[null,null,null,null,"Coincident",7.4637502601356109,8.0798103080947268,8.6952542960058867,9.3100828399291284,9.9242965553084357,10.537896056972373,11.150881959134731]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.7369689910596495,8.3755805899964813,9.0135535773343811,9.6508885916849341,10.287586271021125,10.923647252677991,11.559072173353284]
[null,null,null,null,"Coincident",7.5111150923486818,8.1310846468946689,8.7504342318861141,9.369164467292558,9.9872759724635856,10.604769366129453,11.221645266401737]
[null,"Oaks Estate","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",1E-3,1E-3,1E-3,1E-3,1E-3,1E-3,1E-3]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",18.775700500051698,18.775700500051698,18.775700500051698,18.775700500051698,18.775700500051698,18.775700500051698,18.775700500051698]
[null,null,null,null,"Coincident",16.745313734251962,16.745313734251962,16.745313734251962,16.745313734251962,16.745313734251962,16.745313734251962,16.745313734251962]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.385461779823125,19.385461779823125,19.385461779823125,19.385461779823125,19.385461779823125,19.385461779823125,19.385461779823125]
[null,null,null,null,"Coincident",17.28913599711472,17.28913599711472,17.28913599711472,17.28913599711472,17.28913599711472,17.28913599711472,17.28913599711472]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.179792212002699,18.179792212000201,18.179792212000201,18.179792212000201,18.179792212000201,18.179792212000201,18.179792212000201]
[null,null,null,null,"Coincident",16.213846413488401,16.213846413486174,16.213846413486174,16.213846413486174,16.213846413486174,16.213846413486174,16.213846413486174]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",18.770200722467532,18.770200722464953,18.770200722464953,18.770200722464953,18.770200722464953,18.770200722464953,18.770200722464953]
[null,null,null,null,"Coincident",16.740408697493667,16.740408697491368,16.740408697491368,16.740408697491368,16.740408697491368,16.740408697491368,16.740408697491368]
[null,"Oaky","Substation Rating","MVA","Non-Coincident",8.4,8.4,8.4,8.4,8.4,8.4,8.4]
[null,null,null,null,"Coincident",7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.40351336352241601,0.40351336330572796,0.40351336330551102,0.40351336330551102,0.40351336330551102,0.40351336330551102,0.40351336330551102]
[null,null,null,null,"Coincident",0.22247763826641312,0.22247763814694188,0.22247763814682225,0.22247763814682225,0.22247763814682225,0.22247763814682225,0.22247763814682225]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.42423432002762124,0.42423431979980591,0.42423431979957787,0.42423431979957787,0.42423431979957787,0.42423431979957787,0.42423431979957787]
[null,null,null,null,"Coincident",0.2339021656368506,0.23390216551124432,0.23390216551111859,0.23390216551111859,0.23390216551111859,0.23390216551111859,0.23390216551111859]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.38559994771776795,0.38559994771776795,0.38559994771776795,0.38559994771776795,0.38559994771776795,0.38559994771776795,0.38559994771776795]
[null,null,null,null,"Coincident",0.21260105225520176,0.21260105225520176,0.21260105225520176,0.21260105225520176,0.21260105225520176,0.21260105225520176,0.21260105225520176]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.40540102611408585,0.40540102611408585,0.40540102611408585,0.40540102611408585,0.40540102611408585,0.40540102611408585,0.40540102611408585]
[null,null,null,null,"Coincident",0.22351840358722569,0.22351840358722569,0.22351840358722569,0.22351840358722569,0.22351840358722569,0.22351840358722569,0.22351840358722569]
[null,"Oberon 132kV","Substation Rating","MVA","Non-Coincident",108,108,108,108,108,108,108]
[null,null,null,null,"Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.939542423409399,24.774902280339301,24.626829958776899,24.493658230399898,24.373887640921801,24.266169626905199,24.169291331538599]
[null,null,null,null,"Coincident",17.474645371504543,17.359285271258148,17.255533916694013,17.162223113817614,17.078302224591464,17.002826337219286,16.934945626860376]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.590555708795588,28.401813144780807,28.232063841177432,28.079396496510139,27.942092144545182,27.818604799497034,27.70754404891758]
[null,null,null,null,"Coincident",20.032838353781941,19.900590162669541,19.781650174430442,19.674679177826828,19.578472727130293,19.491947580599959,19.414129503663336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",23.2544732775062,23.054068851710198,22.8707958571344,22.7031898254446,22.549911477350499,22.4097360209092,22.281543364654297]
[null,null,null,null,"Coincident",16.293950663830874,16.153531236232315,16.025115464522742,15.907677224631248,15.80027810998028,15.702059933018008,15.612237867750968]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.658801610376493,26.429059067280289,26.218955903702646,26.026813261115127,25.851095797027931,25.690399416623251,25.54344005313974]
[null,null,null,null,"Coincident",18.679296366454274,18.518320298842649,18.371105157016139,18.2364745979242,18.113352837373309,18.000756053824453,17.897784527029884]
[null,"Oberon Town","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.2330126525185499,6.4568474593182197,6.6573146022001906,6.8368535932527701,6.9976492670213801,7.1416583680591206,7.2706333628188702]
[null,null,null,null,"Coincident",3.8134053375649013,3.9503492031669984,4.0729965512938469,4.1828398943045944,4.2812159308683571,4.3693218124332445,4.4482297115260687]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.3198536508120862,6.5468070198799513,6.7500671567414683,6.9321075618108035,7.0951435096827726,7.2411590071125396,7.3719309366651808]
[null,null,null,null,"Coincident",3.8665353318186795,4.0053871579307323,4.1297432813710859,4.2411170088194616,4.3408636624025734,4.4301970727945577,4.5102043504884675]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.9828669212133896,6.1627968947344796,6.3165678422139502,6.4479828801090298,6.5602922107598598,6.6562735075221795,6.7383006131490299]
[null,null,null,null,"Coincident",3.6603642449011904,3.7704467940094437,3.8645250487108336,3.9449257850614803,4.0136375019852641,4.0723596015195778,4.1225444190164646]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.066222782184667,6.2486596170574966,6.4045729671490115,6.5378189355616119,6.6516930078446377,6.7490115570871012,6.8321814994346317]
[null,null,null,null,"Coincident",3.7113620051923952,3.8229782714599416,3.9183672646455023,3.9998881784444342,4.0695572163981559,4.1290974573401229,4.1799814711797039]
[null,"Orange Industrial","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.2046258545972,12.3652558747198,12.525725264822301,12.6860341855347,12.8461827973263,13.0061712605062,13.165999735222901]
[null,null,null,null,"Coincident",9.621285782253695,9.7479154181983763,9.874418424507132,10.000794927809579,10.127045054608656,10.253168931281007,10.379166684076669]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.266725375566999,12.428172712616952,12.589458602329879,12.750583206153093,12.911546685372398,13.072349201112576,13.232990914336995]
[null,null,null,null,"Coincident",9.6702407641851096,9.7975147164592258,9.9246613947810847,10.051680926424623,10.17857343853645,10.305339058136237,10.431977912116409]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.722778988309599,11.876481869138301,12.030031047086201,12.183426675856101,12.3366689089973,12.4897578999053,12.642693801822499]
[null,null,null,null,"Coincident",9.2414309256551928,9.3625996824550235,9.4836472704980768,9.6045738109530454,9.7253794248676133,9.8460642331682209,9.966628356660614]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.782426778277255,11.936911729395112,12.091242195561879,12.245418331262426,12.399440290827343,12.553308228432636,12.707022298100432]
[null,null,null,null,"Coincident",9.2884531318576453,9.4102384189668378,9.5319019207889433,9.6534437591091855,9.774864055591161,9.89616293177661,10.017340509085956]
[null,"Orange North","Substation Rating","MVA","Non-Coincident",60,60,60,60,60,60,60]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.494148524777401,16.494149095917802,16.494149342009099,16.494149448044201,16.494149493732301,16.494149513418201,16.4941495219005]
[null,null,null,null,"Coincident",8.7631834183091897,8.7631837217506234,8.7631838524965779,8.7631839088320138,8.7631839331056653,8.7631839435645951,8.7631839480711591]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.766503894072088,16.766504474643298,16.766504724798111,16.766504832584094,16.766504879026606,16.766504899037564,16.766504907659925]
[null,null,null,null,"Coincident",8.9078832221520727,8.9078835306040069,8.9078836635088674,8.9078837207745298,8.9078837454489914,8.9078837560806221,8.9078837606616013]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.786187647637799,15.786188181481501,15.786188410405501,15.786188508573199,15.786188550669699,15.786188568721601,15.7861885764626]
[null,null,null,null,"Coincident",8.3870505727705549,8.3870508563966109,8.3870509780217422,8.387051030177302,8.3870510525427697,8.3870510621335725,8.3870510662462916]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.046852995719817,16.046853538378475,16.046853771082525,16.046853870871189,16.046853913662797,16.046853932012777,16.046853939881597]
[null,null,null,null,"Coincident",8.5255395801060203,8.5255398684153771,8.5255399920488131,8.5255400450655774,8.5255400678003497,8.5255400775495183,8.5255400817301474]
[null,"Orange South","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.9950405334565,20.725137224724801,19.456503819301901,18.189139047284399,16.9230416400389,15.6582103302006,14.3946438516722]
[null,null,null,null,"Coincident",17.793852162650403,16.766508216543045,15.740191614381853,14.714901328822799,13.690636333549293,12.667395603271023,11.645178113723082]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",22.541966893540444,21.240486302955286,19.940307192960784,18.64142826207625,17.343848210122587,16.047565738220829,14.752579548791035]
[null,null,null,null,"Coincident",18.236312215423983,17.183422443013459,16.131585560375406,15.080800514619966,14.031066253910273,12.982381727461251,11.934745885538726]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.2173276249755,20.022817134664603,18.829501154844099,17.6373784910034,16.446447949826602,15.256708339190901,14.068158468165901]
[null,null,null,null,"Coincident",17.164687215332115,16.198335594429373,15.232950325147604,14.268530441135102,13.305074977006663,12.342582968342287,11.381053451686629]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",21.744915457831961,20.520702395545619,19.297713546321649,18.075947685946883,16.855403591432559,15.636080041012663,14.417975814143254]
[null,null,null,null,"Coincident",17.591502518826612,16.601121700351918,15.611731262695768,14.623330215477258,13.635917569306022,12.649492335780888,11.664053527489333]
[null,"Orange West","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.847006819188699,14.8470068187743,14.847006818727799,14.847006818722601,14.847006818722001,14.8470068187219,14.8470068187219]
[null,null,null,null,"Coincident",10.911895382173393,10.911895381868828,10.911895381834652,10.911895381830831,10.911895381830391,10.911895381830316,10.911895381830316]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.963269094809858,14.963269094392214,14.963269094345348,14.963269094340109,14.963269094339505,14.963269094339402,14.963269094339402]
[null,null,null,null,"Coincident",10.997343028552315,10.997343028245366,10.997343028210921,10.997343028207071,10.997343028206627,10.997343028206553,10.997343028206553]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.2907152939145,14.290715293395801,14.2907152933316,14.2907152933237,14.2907152933227,14.2907152933226,14.2907152933226]
[null,null,null,null,"Coincident",10.503045638941886,10.503045638560666,10.50304563851348,10.503045638507674,10.50304563850694,10.503045638506867,10.503045638506867]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.402621424258379,14.402621423735619,14.402621423670915,14.402621423662954,14.402621423661945,14.402621423661845,14.402621423661845]
[null,null,null,null,"Coincident",10.585291710611907,10.5852917102277,10.585291710180146,10.585291710174294,10.585291710173554,10.585291710173481,10.585291710173481]
[null,"Oura 66/11kV","Substation Rating","MVA","Non-Coincident",15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001]
[null,null,null,null,"Coincident",15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001,15.180000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.13413863056644,4.1156397748802602,4.0984709821062193,4.0825366210669003,4.06774793644166,4.0540225543943205,4.0412840237461101]
[null,null,null,null,"Coincident",3.6535012209216662,3.6371530531714593,3.6219803144302052,3.6078984916579047,3.5948291482801431,3.5826994872918032,3.5714419457735094]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.3958068330837543,4.3761371017331152,4.3578816189503362,4.3409387006312512,4.3252139737323265,4.3106198506073081,4.297075041138938]
[null,null,null,null,"Coincident",3.8847477229874179,3.8673648062720889,3.8512317167471593,3.8362585921627348,3.8223620313413069,3.8094646296283341,3.7974945477438129]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.8142463213865199,3.7858346513622099,3.7588337236888201,3.7331734898975699,3.7087873796799298,3.6856121281843897,3.6635876118885098]
[null,null,null,null,"Coincident",3.3707997813736279,3.3456912689607243,3.3218294851561425,3.2991525253676355,3.2776015587902347,3.2571206757815969,3.2376567428156671]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.0556671028513973,4.0254571306195102,3.9967471929583187,3.9694628077168281,3.9435331910526794,3.9188910737977554,3.895472526941834]
[null,null,null,null,"Coincident",3.5841528395696809,3.5574550966306426,3.5320829933532605,3.5079707069255979,3.4850556828767991,3.4632784727921373,3.4425825800860439]
[null,"Owen St","Substation Rating","MVA","Non-Coincident",44,44,44,44,44,44,44]
[null,null,null,null,"Coincident",44,44,44,44,44,44,44]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.2511470014522,15.044665233886201,14.850489610602999,14.6678866954793,14.496166764584499,14.3346812009692,14.182820044723499]
[null,null,null,null,"Coincident",10.707028309747962,10.562068318832823,10.425747824685187,10.297551920371513,10.176996386990087,10.063625864689044,9.9570121326911192]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.33414085097519,15.126535448790433,14.931303158591735,14.74770655303552,14.575052154844363,14.412687817418442,14.260000261561705]
[null,null,null,null,"Coincident",10.76529392716631,10.619545091473025,10.482482767050124,10.353589244938192,10.232377671208084,10.118390208025986,10.011196304318373]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.256313101794801,14.023696918454199,13.805750618817399,13.601549050193901,13.4102254044252,13.230967538401201,13.0630145266217]
[null,null,null,null,"Coincident",10.008607743339777,9.8453001534190836,9.6922915174132918,9.5489323342686703,9.4146140635592861,9.2887665423150665,9.170855564756506]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.333893253911251,14.100011217417771,13.880878895352991,13.675566100520928,13.483201307757472,13.302967954423751,13.134100974207305]
[null,null,null,null,"Coincident",10.063072688494806,9.8988764096418933,9.7450351296578379,9.6008958130273534,9.4658466077629235,9.3393142481757252,9.2207616214397188]
[null,"Oxley Vale","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.987364236660401,20.9935084456882,20.994127505560702,20.994189878947399,20.994196163378898,20.9941967965669,20.9941968603638]
[null,null,null,null,"Coincident",19.68587509081555,19.691638279088703,19.692218949209369,19.692277454636049,19.692283349351179,19.692283943273303,19.692284003113965]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.952692137156141,21.95911895320091,21.959766487147636,21.959831729440104,21.959838302928247,21.959838965240156,21.959839031971438]
[null,null,null,null,"Coincident",20.591340124754574,20.597368394739423,20.597975773171921,20.598036969594954,20.598043135441461,20.598043756681431,20.598043819274505]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.217635405078799,18.218304947085997,18.218357259113802,18.218361346308097,18.218361665644903,18.218361690595,18.218361692544399]
[null,null,null,null,"Coincident",17.087905417296312,17.088533439003715,17.088582507006418,17.088586340741585,17.088586640275363,17.088586663678232,17.088586665506742]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.055567769489887,19.056268107530965,19.056322825685591,19.05632710087313,19.056327434898048,19.056327460995739,19.056327463034805]
[null,null,null,null,"Coincident",17.873875092875416,17.874532000862647,17.87458332578106,17.874587335851452,17.874587649162486,17.874587673641781,17.874587675554398]
[null,"Pacific Palms","Substation Rating","MVA","Non-Coincident",19.2,19.2,19.2,19.2,19.2,19.2,19.2]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.7064137895574705,4.6971094520188501,4.6887215193050098,4.6811597326737999,4.6743427231665997,4.6681971360338705,4.6626568413979106]
[null,null,null,null,"Coincident",3.2213556238445018,3.2149871697738703,3.2092459588586486,3.2040702125303491,3.1994042369285975,3.1951978236047696,3.1914057092516064]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.8325420173303524,4.8229883307848622,4.8143756080004545,4.806611171370915,4.7996114713128408,4.7933011872264792,4.7876124170048566]
[null,null,null,null,"Coincident",3.3076854482137943,3.3011463245289949,3.2952512536281477,3.2899368013251973,3.2851457812076434,3.2808266392795029,3.276932899212099]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.3985679611473998,4.3859394212275404,4.3745362838659503,4.36423964288349,4.3549421300885793,4.3465467956956498,4.33896609738163]
[null,null,null,null,"Coincident",3.0106472299446327,3.0020034897401384,2.9941984895187952,2.9871508426652285,2.9807870598639572,2.9750407827897392,2.9698520921563913]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.5164461602358541,4.5034791852716758,4.4917704527009139,4.4811978697513419,4.4716511908473828,4.4630308680246449,4.4552470128939108]
[null,null,null,null,"Coincident",3.091330233297374,3.0824548475805917,3.0744406794259334,3.0672041611200562,3.060669833891001,3.054769561062038,3.0494418175567355]
[null,"Pambula","Substation Rating","MVA","Non-Coincident",38.4,38.4,38.4,38.4,38.4,38.4,38.4]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.1438555286237,17.1438906764248,17.143902303481902,17.143906149766799,17.1439074221359,17.1439078430415,17.143907982279099]
[null,null,null,null,"Coincident",14.248448817122808,14.248478028850833,14.248487692227181,14.248490888917296,14.248491946397392,14.248492296216714,14.24849241193863]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.160787731614935,17.160822914129913,17.160834552670526,17.160838402754223,17.160839676379986,17.160840097701296,17.160840237076414]
[null,null,null,null,"Coincident",14.262521359164413,14.262550599743529,14.262560272663949,14.262563472511287,14.26256453103581,14.262564881200634,14.262564997036842]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.4217569717364,16.421806515752902,16.421826567190401,16.4218346824013,16.4218379667867,16.421839296042101,16.421839834017799]
[null,null,null,null,"Coincident",13.648304683176475,13.648345859759079,13.648362524731578,13.648369269373525,13.648371999062725,13.648373103821658,13.648373550939239]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.437975990967747,16.438025583916609,16.438045655157996,16.438053778383921,16.438057066013158,16.438058396581404,16.438058935088435]
[null,null,null,null,"Coincident",13.661784490270971,13.661825707521805,13.661842388953534,13.661849140256859,13.661851872642048,13.661852978492101,13.661853426051277]
[null,"Parkes Town","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.546586267170003,20.594275049815202,20.6370859055842,20.675517781384197,20.7100185885038,20.740990422876102,20.768794251379802]
[null,null,null,null,"Coincident",17.687666878148715,17.728720087196901,17.765574100110008,17.798658438686431,17.828358690369303,17.855021002145044,17.878956114777182]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.499559396843768,21.549460037354638,21.594256507408936,21.63447089561679,21.67057188788197,21.702980229786458,21.732073630247346]
[null,null,null,null,"Coincident",18.508040201596085,18.55099750335345,18.589560845669027,18.624179672031708,18.655257453851721,18.683156392791066,18.708201642109536]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.598016052860302,18.621478268342397,18.642151143009599,18.6603662918445,18.676415905283498,18.690557436262598,18.703017730038198]
[null,null,null,null,"Coincident",16.010227113156553,16.030424719039811,16.048221102135887,16.06390173543128,16.077718153026922,16.089891985013065,16.10061851265327]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.460612366094889,19.485162784776595,19.506794489967504,19.525854477315576,19.542648489369029,19.557445920012444,19.570484135833176]
[null,null,null,null,"Coincident",16.752798946765292,16.773933339686561,16.792555138483106,16.808963056690576,16.823420294836442,16.836158762456801,16.847382798173673]
[null,"Parsons Creek","Substation Rating","MVA","Non-Coincident",3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996,3.5999999999999996]
[null,null,null,null,"Coincident",3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003,3.3000000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.114564074531634,0.110755114597615,0.107330097824945,0.10425032274295999,0.10148098898924,9.899080407789429E-2,9.6751629805612291E-2]
[null,null,null,null,"Coincident",8.1972570570048475E-2,7.9247194065534876E-2,7.6796535512676165E-2,7.4592903341945516E-2,7.2611397294025173E-2,7.0829627055734715E-2,6.9227459257463972E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.11555169586380326,0.11170990006828409,0.10825535728895315,0.1051490324217786,0.10235582510121621,9.9844173078565787E-2,9.7585695579798598E-2]
[null,null,null,null,"Coincident",8.2679230661169584E-2,7.9930359531617062E-2,7.7458574611923375E-2,7.5235945612134689E-2,7.3237357615525397E-2,7.1440227288973798E-2,6.9824247699338662E-2]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.10832187383558499,0.10500312002928899,0.10201889660666799,9.9335482905046707E-2,9.6922557304548906E-2,9.4752854604581202E-2,9.2801857936770399E-2]
[null,null,null,null,"Coincident",7.7506168347875465E-2,7.5131542779577468E-2,7.2996279468564171E-2,7.1076250699300667E-2,6.9349760829978957E-2,6.7797301139484831E-2,6.6401329385792615E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.1092556830927883,0.10590831933988631,0.10289836985327719,0.1001918232749178,9.7758096591657087E-2,9.5569689558068965E-2,9.3601873953466697E-2]
[null,null,null,null,"Coincident",7.8174324971564041E-2,7.5779228493194517E-2,7.3625557739844888E-2,7.168897699843256E-2,6.9947603595754637E-2,6.8381760632066593E-2,6.6973754639118421E-2]
[null,"Paytens Bridge","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.6357886401733808,6.00862718231632,6.3405729720097099,6.6361111067257497,6.8992347605974,7.1334991383342707,7.3420695114988703]
[null,null,null,null,"Coincident",5.0431593192479331,5.3767921590212024,5.6738323089736378,5.9382932377710835,6.1737482187613848,6.3833786103857184,6.5700168412175461]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.9530196296099449,6.3468447536095898,6.6974753269290206,7.0096489071661896,7.2875834388743268,7.5350342444714382,7.7553447644141684]
[null,null,null,null,"Coincident",5.3270319984550847,5.6794445836423959,5.9932047255406085,6.2725518055878897,6.5212602318999133,6.7426904373208334,6.9398342840324725]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.1348310217049402,5.4192275776411796,5.66460694774847,5.8763220125671598,6.0589912754786299,6.2165996140311899,6.35258520890019]
[null,null,null,null,"Coincident",4.5948797183916374,4.8493706571057151,5.068947248088322,5.2583994916580359,5.4218602341396398,5.562895324720694,5.6845814034282114]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4238637781844146,5.7242686351042815,5.9834600810959619,6.2070923031714562,6.4000437740777372,6.5665236747797504,6.7101637165351917]
[null,null,null,null,"Coincident",4.8535193396536824,5.1223352322376456,5.3542714952487582,5.5543877517039428,5.7270494803087386,5.8760232471224985,6.0045588721160277]
[null,"Peak Hill","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.8532417598625599,1.8532581244844701,1.85326858328445,1.8532752676122499,1.8532795396356301,1.8532822699301801,1.85328401488982]
[null,null,null,null,"Coincident",1.7092126448297631,1.7092277376359488,1.7092373836052781,1.7092435484445587,1.7092474884574262,1.7092500065606062,1.709251615906535]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.9086375733367122,1.9086544271185166,1.9086651985456697,1.9086720826767463,1.9086764823964775,1.9086792943030928,1.9086810914218524]
[null,null,null,null,"Coincident",1.760303240191522,1.760318784141371,1.7603287184413052,1.760335067555673,1.7603391253406642,1.7603417187132329,1.7603433761646106]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.6277605992056499,1.62160843086039,1.6163300500970399,1.6118013535596201,1.6079158641931599,1.6045822277942401,1.60172206512434]
[null,null,null,null,"Coincident",1.5012552917673847,1.4955812538967836,1.490713095116672,1.4865363570601495,1.4829528377911914,1.4798782829167529,1.4772404046282634]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.6764164866819056,1.6700804220002383,1.6646442635510272,1.6599801983671085,1.6559785666554552,1.6525452835163503,1.6495996268536]
[null,null,null,null,"Coincident",1.5461297705973878,1.5402861283339153,1.5352724539380942,1.5309708677331431,1.5272802323990802,1.5241137750691556,1.5213970471579126]
[null,"Perisher","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.2223907955064011,8.8950233761518387,8.59667798648365,8.32478174307691,8.0769898557582795,7.8511654065065803,7.6453609210100204]
[null,null,null,null,"Coincident",0.50506890589611464,0.48714046326277854,0.47080142679380965,0.45591089122448442,0.44234044293260177,0.42997305251972506,0.41870206556817363]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.7079266497932739,9.3633241529900904,9.0492716232909594,8.7630607213811107,8.5022232097376875,8.2645096669399081,8.0478700890147845]
[null,null,null,null,"Coincident",0.53165952302952579,0.51278719264484318,0.49558794669157757,0.47991346159454806,0.46562856307489309,0.45261006042847912,0.44074568414876736]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.4780179663582196,8.1825926679524592,7.9126016817366995,7.66585526891717,7.4403522138238802,7.2342635932221304,7.0459179429870904]
[null,null,null,null,"Coincident",0.46430295065380878,0.448123834462752,0.43333764126909013,0.41982444891800541,0.40747465981909908,0.39618811206451005,0.38587326707433089]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9243644493071859,8.6133857463862658,8.329180408702566,8.0694434131808883,7.8320681851416882,7.6151295131073509,7.4168679345392103]
[null,null,null,null,"Coincident",0.48874734200441783,0.47171643573250055,0.4561517863767518,0.44192715818025446,0.4289271835130547,0.41704642719286861,0.40618853136205668]
[null,"Pindari","Substation Rating","MVA","Non-Coincident",0.33]
[null,null,null,null,"Coincident",0.36]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2]
[null,null,null,null,"Coincident",9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,null,null,"Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2]
[null,null,null,null,"Coincident",9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2,9.8000000000000004E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,null,null,null,"Coincident",0.1,0.1,0.1,0.1,0.1,0.1,0.1]
[null,"Prince St","Substation Rating","MVA","Non-Coincident",33,33,33,33,33,33,33]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.3868463849946,10.4673649339015,10.528158736822201,10.574059793457399,10.608716401516199,10.634883129914,10.654639756814101]
[null,null,null,null,"Coincident",6.0012415630378992,6.047763023391223,6.0828880539673857,6.1094084547373884,6.1294321143745281,6.1445505489993497,6.1559653987144278]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.616431249060996,10.698729533550809,10.760867087641238,10.807782714768528,10.843205352510955,10.869950455187107,10.890143771177732]
[null,null,null,null,"Coincident",6.133889546594304,6.1814392904858169,6.2173407044868663,6.244447296905431,6.2649135479707576,6.2803661517581508,6.2920333087302192]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.7202290495012296,8.7910211831099403,8.8489117765484693,8.8962520760680306,8.9349648241240907,8.9666223522187991,8.9925104416826507]
[null,null,null,null,"Coincident",5.0383147176104561,5.0792165157888212,5.1126641497072471,5.1400161064564953,5.1623832951143607,5.1806741666978153,5.1956316112117298]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.9129759648546543,8.9853328469701896,9.0445030207098682,9.0928897029164553,9.1324581352361172,9.1648154030800146,9.1912757079478684]
[null,null,null,null,"Coincident",5.1496787213409227,5.1914845892847188,5.2256715304193948,5.2536280590511435,5.2764896391515341,5.2951848016150587,5.3104728568589508]
[null,"Providence Portal","Substation Rating","MVA","Non-Coincident",0.55000000000000004]
[null,null,null,null,"Coincident",0.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998]
[null,null,null,null,"Coincident",0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,null,null,null,"Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998]
[null,null,null,null,"Coincident",0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998,0.28499999999999998]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,null,null,null,"Coincident",0.3,0.3,0.3,0.3,0.3,0.3,0.3]
[null,"Queanbeyan South","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",28.1286797789849,28.197465913784701,28.2606361664022,28.318649032328803,28.371925574270097,28.420852478257398,28.4657848602508]
[null,null,null,null,"Coincident",21.302881498757891,21.354975763043004,21.402816913652661,21.446752186048951,21.487100466471514,21.524154606442963,21.558183548312375]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",28.298437115928127,28.367638376896451,28.431189863682871,28.489552838811381,28.543150906112292,28.59237308527749,28.637576635401416]
[null,null,null,null,"Coincident",21.431444959996057,21.483853614563422,21.531983487800218,21.576183910743868,21.616775694121017,21.654053456821071,21.6882877642674]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",26.715149740456102,26.7647655256769,26.810405819950102,26.852389161583698,26.891008565835801,26.926533569962601,26.9592121144054]
[null,null,null,null,"Coincident",20.232363325053534,20.269939180064551,20.304504249883319,20.33629977526061,20.365547667404833,20.39245205677193,20.417200717757325]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",26.876376385702624,26.926291603518042,26.97220733819136,27.014444050417808,27.053296523810435,27.089035922290002,27.121911682625029]
[null,null,null,null,"Coincident",20.354466180399587,20.39226880670347,20.427042477645713,20.459029889871484,20.488454293829296,20.515521051907857,20.54041907172612]
[null,"Quira","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.36448386328418,1.4035232134909699,1.4385102729673098,1.46986567013239,1.49796637210894,1.52315021677266,1.54571997437428]
[null,null,null,null,"Coincident",1.3109212898086202,1.348428157206228,1.382041805831534,1.4121663524092956,1.4391639662843043,1.4633592235660156,1.485043009312349]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4307561999573308,1.471691672961922,1.5083780373895415,1.5412563513829987,1.5707218911800997,1.5971289032825766,1.620794863349212]
[null,null,null,null,"Coincident",1.3745921175904097,1.4139206758197043,1.4491669234800386,1.480754605054591,1.5090634802821452,1.5344338897804664,1.5571708467573269]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2466194946248099,1.28817964620488,1.3255433825184801,1.3591344243755399,1.3893337086112698,1.4164837080733601,1.4408923154111302]
[null,null,null,null,"Coincident",1.1976836661598307,1.2376123813172635,1.2735094107496243,1.3057818421811576,1.3347956588387717,1.3608798898589036,1.3843303416192096]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.307167214589954,1.3507459230997281,1.3899243984358782,1.4251469413279116,1.4568129905331748,1.4852816526437898,1.5108757745096084]
[null,null,null,null,"Coincident",1.2558545960531562,1.2977226300439171,1.335363161238462,1.3692030494194973,1.3996260534463769,1.4269771832452645,1.4515666123698434]
[null,"Quirindi 66/11kV","Substation Rating","MVA","Non-Coincident",29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005]
[null,null,null,null,"Coincident",29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005,29.260000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.6548450820145195,7.6548450823509198,7.6548450823512599,7.6548450823512599,7.6548450823512599,7.6548450823512599,7.6548450823512599]
[null,null,null,null,"Coincident",6.4162406899294355,6.4162406902114038,6.4162406902116889,6.4162406902116889,6.4162406902116889,6.4162406902116889,6.4162406902116889]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.9850011563506929,7.9850011567016024,7.9850011567019576,7.9850011567019576,7.9850011567019576,7.9850011567019576,7.9850011567019576]
[null,null,null,null,"Coincident",6.6929753351752712,6.6929753354694013,6.6929753354696997,6.6929753354696997,6.6929753354696997,6.6929753354696997,6.6929753354696997]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.6813789935743095,6.6813789938161099,6.6813789938163497,6.6813789938163497,6.6813789938163497,6.6813789938163497,6.6813789938163497]
[null,null,null,null,"Coincident",5.6002878313155069,5.6002878315181821,5.6002878315183828,5.6002878315183828,5.6002878315183828,5.6002878315183828,5.6002878315183828]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.9695491441177282,6.9695491443699575,6.9695491443702071,6.9695491443702071,6.9695491443702071,6.9695491443702071,6.9695491443702071]
[null,null,null,null,"Coincident",5.8418301519934293,5.8418301522048468,5.8418301522050555,5.8418301522050555,5.8418301522050555,5.8418301522050555,5.8418301522050555]
[null,"Raglan","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",21.464892940263301,21.526144080371999,21.585268902926,21.6423412224914,21.697432291180899,21.750610887608602,21.801943402756301]
[null,null,null,null,"Coincident",20.387203193469592,20.44537909225944,20.501535429705001,20.555742314358028,20.608067420970205,20.65857607498177,20.707331334076727]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.504404938312565,21.565768827873832,21.625002485812196,21.682179862569615,21.737372341417771,21.790648827576586,21.842075834238592]
[null,null,null,null,"Coincident",20.42473140919618,20.483014396617026,20.539274105139341,20.59358077236881,20.646002197630988,20.696603826615423,20.745448833081007]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",19.486328527875699,19.486328488560801,19.486328473728499,19.486328468132697,19.4863284660216,19.486328465225199,19.4863284649247]
[null,null,null,null,"Coincident",18.507976736623402,18.507976699282391,18.507976685194773,18.507976679879924,18.507976677874819,18.5079766771184,18.507976676832989]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.522198437729127,19.52219839834186,19.522198383482255,19.522198377876151,19.522198375761171,19.522198374963303,19.522198374662249]
[null,null,null,null,"Coincident",18.542045722792977,18.542045685383233,18.542045671269683,18.542045665945047,18.542045663936253,18.542045663178442,18.542045662892505]
[null,"Raleigh","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.454807332546299,13.6190806773518,13.683610321999501,13.7089587742592,13.7189161207698,13.722827552857199,13.724364036593801]
[null,null,null,null,"Coincident",10.918840526319194,11.052151573465707,11.104518648052046,11.125089415137145,11.13316999748421,11.136344201479575,11.137591088222477]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.556926801253432,13.722446949991511,13.787466362561146,13.813007204827874,13.823040125734321,13.826981244858985,13.828529390219494]
[null,null,null,null,"Coincident",11.001712481739059,11.136035334775535,11.188799865654063,11.209526761010171,11.217668673464441,11.220866969073873,11.222123319453717]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.9637007371091,11.3608323346739,11.6301696456703,11.8128360150543,11.936721570978399,12.020741585272201,12.077724522058201]
[null,null,null,null,"Coincident",8.8972585759150657,9.2195386706499338,9.4381111907813526,9.5863485387812037,9.686884101663443,9.7550679941874154,9.80131076705735]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.046913173130338,11.447058925171511,11.718440455934285,11.902493228863957,12.027319052964238,12.111976763436692,12.169392190044814]
[null,null,null,null,"Coincident",8.9647871028025996,9.2895132431207141,9.5097446877597918,9.6591071294786506,9.7604057384613636,9.82910713396452,9.8757008808231763]
[null,"Rappville","Substation Rating","MVA","Non-Coincident",12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002]
[null,null,null,null,"Coincident",12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002,12.375000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.44631625583003,1.5590370598580301,1.6471247768992301,1.7159625212751801,1.7697570253210999,1.8117957163296501,1.8446476139919901]
[null,null,null,null,"Coincident",0.7237683879385719,0.78017635147325881,0.8242573778069564,0.85870529545669338,0.88562524558262623,0.90666232893120868,0.92310213932257379]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4890344574790184,1.6050845679551029,1.6957740319131316,1.7666449586124218,1.822028329866449,1.8653086699765176,1.899130876852513]
[null,null,null,null,"Coincident",0.74514551332072387,0.80321953485010622,0.84860253242572736,0.8840678991199713,0.91178295325806258,0.93344138505997865,0.95036675947134186]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2987626283884699,1.38097555593427,1.44441064887653,1.4933568564465198,1.53112351090173,1.56026407683218,1.58274879503126]
[null,null,null,null,"Coincident",0.64992931530325948,0.69107046807512407,0.72281478040825498,0.74730853660150731,0.76620779912635084,0.78079037768901494,0.79204222401142366]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3371227060201969,1.4217638634935101,1.4870725667758369,1.5374644429238433,1.5763465681857476,1.6063478259369282,1.6294966497368248]
[null,null,null,null,"Coincident",0.66912553980588751,0.71148183211109817,0.74416374016714859,0.76938094063615103,0.78883840922712922,0.80385169686126434,0.8154358761974152]
[null,"Redcliff","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.463672022777323,0.45725913771988796,0.45210796720424296,0.44797027294594899,0.44464665674588,0.44197695136027199,0.43983250193624096]
[null,null,null,null,"Coincident",0.23934921546144219,0.23603886044336811,0.23337980714478282,0.23124391404385794,0.22952825105169269,0.22815013924384411,0.22704316650875403]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.48835826473074528,0.48160395292256719,0.47617853027298734,0.47182054210742308,0.46831997411892451,0.46550813164102717,0.46324951014117971]
[null,null,null,null,"Coincident",0.25209234498832456,0.24860574421697335,0.24580512095110227,0.24355551131934108,0.24174850515861152,0.2402970216572895,0.23913111287380343]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.41697377603406299,0.41221842930074598,0.40833897031644201,0.40517406923668398,0.402592111575789,0.40048572493220796,0.39876731383684]
[null,null,null,null,"Coincident",0.21524340753610197,0.21278867993996842,0.2107860888439041,0.20915235518467715,0.20781953907731701,0.20673221449046847,0.20584516431855399]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.43917376873958019,0.43416524382370236,0.4300792395694007,0.42674583681178518,0.42402641381246292,0.42180788158369126,0.41999798100870878]
[null,null,null,null,"Coincident",0.22670312599288514,0.22411770688121674,0.22200849635179712,0.22028778150237985,0.21888400527819268,0.2177387907249147,0.2168045133447733]
[null,"Ringwood Road","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1912485787430502,2.19124678006358,2.19124618028227,2.1912459802813102,2.1912459135897002,2.1912458913509498,2.1912458839352897]
[null,null,null,null,"Coincident",1.8953633251662356,1.8953617693632405,1.895361250570663,1.8953610775759202,1.8953610198897075,1.8953610006538653,1.8953609942395451]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.732088017658048,2.7320857750322336,2.7320850272141421,2.7320847778493591,2.7320846946970643,2.7320846669693912,2.7320846577234135]
[null,null,null,null,"Coincident",2.3631729781956441,2.3631710383925739,2.3631703915526865,2.363170175859739,2.3631701039355351,2.3631700799519417,2.3631700719544524]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0338329272803701,2.03383072967745,2.0338299831545399,2.0338297295616603,2.03382964341648,2.0338296141530701,2.0338296042123298]
[null,null,null,null,"Coincident",1.7592035779409068,1.7592016770812697,1.7592010313616746,1.7592008120115523,1.7592007374985934,1.7592007121866344,1.7592007035881967]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5358193609090613,2.5358166208983373,2.5358156901201871,2.5358153739360381,2.5358152665286826,2.5358152300425383,2.5358152176482451]
[null,null,null,null,"Coincident",2.1934065639739142,2.193404193948036,2.1934033888532665,2.1934031153636013,2.193403022459508,2.1934029909001036,2.1934029801794175]
[null,"Rocks Ferry","Substation Rating","MVA","Non-Coincident",34.1,34.1,34.1,34.1,34.1,34.1,34.1]
[null,null,null,null,"Coincident",34.1,34.1,34.1,34.1,34.1,34.1,34.1]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",16.112716181085901,16.350019884228999,16.561572461889298,16.750168309834098,16.918298588630002,17.068184129356599,17.201804768540601]
[null,null,null,null,"Coincident",14.991184933292505,15.211971029143264,15.408798415611047,15.584266983567977,15.740694495477738,15.880147200695532,16.004467128533864]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",16.615052910476443,16.859754892393241,17.077902921047755,17.272378511449908,17.445750489622419,17.600308924196668,17.738095375904912]
[null,null,null,null,"Coincident",15.458556338860911,15.686225753702592,15.889189512490319,16.070128561373476,16.231432922340609,16.375233262994694,16.503429040518856]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.375747880718899,11.434317551243899,11.4848244964471,11.528378634466101,11.5659370916434,11.5983252359094,11.6262548147003]
[null,null,null,null,"Coincident",10.583934968987593,10.638427877101556,10.685419268710977,10.725941805713115,10.760885993336489,10.791019749487901,10.817005280174207]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.73040291966756,11.79079858255799,11.842880153254482,11.887792153163309,11.926521548395208,11.959919438893857,11.988719761829035]
[null,null,null,null,"Coincident",10.913904119852702,10.970095921494567,11.018552336238841,11.060338220678831,11.096371842803791,11.127445061448009,11.154240727827748]
[null,"Russell Street","Substation Rating","MVA","Non-Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,null,null,"Coincident",99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014,99.000000000000014]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.399878141771403,24.399878144652899,24.399878144673799,24.399878144673998,24.399878144673998,24.399878144673998,24.399878144673998]
[null,null,null,null,"Coincident",18.974115765509076,18.974115767749819,18.974115767766072,18.974115767766225,18.974115767766225,18.974115767766225,18.974115767766225]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.925873810095183,25.92587381315689,25.925873813179098,25.925873813179312,25.925873813179312,25.925873813179312,25.925873813179312]
[null,null,null,null,"Coincident",20.160778186534543,20.160778188915423,20.160778188932692,20.160778188932856,20.160778188932856,20.160778188932856,20.160778188932856]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",21.319421271147,21.319421272107498,21.319421272108499,21.319421272108499,21.319421272108499,21.319421272108499,21.319421272108499]
[null,null,null,null,"Coincident",16.578655225326152,16.578655226073064,16.578655226073845,16.578655226073845,16.578655226073845,16.578655226073845,16.578655226073845]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.652761721534116,22.652761722554683,22.652761722555748,22.652761722555748,22.652761722555748,22.652761722555748,22.652761722555748]
[null,null,null,null,"Coincident",17.615502865035079,17.615502865828706,17.615502865829534,17.615502865829534,17.615502865829534,17.615502865829534,17.615502865829534]
[null,"Sawtell","Substation Rating","MVA","Non-Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,null,null,"Coincident",54.45,54.45,54.45,54.45,54.45,54.45,54.45]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.330030172932601,10.8220092025631,11.2249879455916,11.5550667854452,11.825433504295798,12.046890180205201,12.2282847672068]
[null,null,null,null,"Coincident",8.7375711604724025,9.1537075810726414,9.4945638403888371,9.7737583154779877,10.00244578355243,10.18976309360156,10.343194214858489]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.346327268089357,10.839082464771337,11.242696964212097,11.573296550488726,11.84408981137943,12.065895866764011,12.247576629584634]
[null,null,null,null,"Coincident",8.7513559245299426,9.1681488596544565,9.509542868309218,9.7891778124823503,10.018226067637366,10.205838897445421,10.359512078167935]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.5144659035437797,8.9236889424067112,9.2679056614456812,9.5574425115584791,9.8009855556246901,10.005841049113499,10.178154626671899]
[null,null,null,null,"Coincident",7.2018910380887542,7.5480289837395507,7.8391818677948253,8.0840842339145755,8.2900831170294023,8.4633584533069559,8.6091084773269415]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.5278986872545772,8.9377673337965806,9.2825271037783654,9.5725207395460643,9.8164480074816609,10.021626689713859,10.194212116504378]
[null,null,null,null,"Coincident",7.2132530478400785,7.5599370754425435,7.8515492946766292,8.0968380291900779,8.3031619049084231,8.4767106077295722,8.6226905731893009]
[null,"Shannon Creek","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.60753573285610696,0.63301401838492299,0.69196704602104708,0.71186247582044992,0.72625746373353395,0.73667270377142602,0.74420846730953305]
[null,null,null,null,"Coincident",0.29831562267165251,0.31082611415567374,0.3397735623411039,0.34954272851183626,0.35661103667941474,0.3617251865954566,0.36542543971737323]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.61454576054290821,0.64031802628936441,0.69995128116744376,0.72007627361837812,0.73463735754584392,0.74517277343032706,0.75279548808618146]
[null,null,null,null,"Coincident",0.30175772601017159,0.31441256931900841,0.34369402652196274,0.35357591384081899,0.36072577941033102,0.36589893874848112,0.36964188709872753]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.59663305296499503,0.63282801026866897,0.65901623430575895,0.67796426268614296,0.69167377498431803,0.701593051210881,0.70876996886622201]
[null,null,null,null,"Coincident",0.29296212728922189,0.31073477940115413,0.32359386889628933,0.33289783667793943,0.33962955874229972,0.34450017770995822,0.34802422830226026]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6035172804992065,0.6401298719256151,0.66662026777851768,0.68578692725559842,0.6996546262341371,0.70968835564792965,0.71694808389160147]
[null,null,null,null,"Coincident",0.29634245952717447,0.31432018070193662,0.32732764430663108,0.33673896556268484,0.3435483613431724,0.34847517976045772,0.35203989247497863]
[null,"Smithtown","Substation Rating","MVA","Non-Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,null,null,"Coincident",12.65,12.65,12.65,12.65,12.65,12.65,12.65]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.0733227366679099,3.9627281334711499,3.8778357762983302,3.8126724491734301,3.7626531147669002,3.7242583009220396,3.6947864627284197]
[null,null,null,null,"Coincident",3.3708290371585545,3.2793078089355183,3.2090561640032385,3.1551310396193655,3.1137381435153855,3.0819649790127306,3.0575759152473685]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.2510850124571515,4.1356639936716419,4.0470668825218521,3.9790597882622127,3.9268575797520606,3.8867871929342739,3.8560291858393221]
[null,null,null,null,"Coincident",3.5179340616506551,3.4224187914958319,3.3491013221522721,3.292822872620258,3.2496235654144239,3.2164638007339401,3.1910103834273595]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7907510187200701,3.6915635612580799,3.6122348250952201,3.5487888154663501,3.4980455875701799,3.4574618661922099,3.4250035755163597]
[null,null,null,null,"Coincident",3.1369902245930845,3.0549088420586115,2.9892613045012015,2.936757325471103,2.8947653800522422,2.8611808115560269,2.8343203451064203]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.9561816932826503,3.8526656349932638,3.7698749446501347,3.7036601126640654,3.6507024195131499,3.6083475999093499,3.5744728097337601]
[null,null,null,null,"Coincident",3.2738903814189677,3.1882269175463507,3.1197144816171241,3.0649191970844281,3.0210946976881279,2.9860444782447031,2.9580118047411696]
[null,"Snapper","Substation Rating","MVA","Non-Coincident",19.2,19.2,19.2,19.2,19.2,19.2,19.2]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.0671897409344204,6.0684640944425299,6.0694492579788006,6.0702108576346303,6.0707996269246092,6.0712547863698303,6.0716066561498803]
[null,null,null,null,"Coincident",4.3575969148650548,4.358512185221266,4.3592197526074195,4.3597667512101195,4.36018961902061,4.3605165251301852,4.3607692461976733]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.2656998157419128,6.2670158643380329,6.2680332610655558,6.2688197792110163,6.2694278122195852,6.2698978638536742,6.2702612463273013]
[null,null,null,null,"Coincident",4.5001714718653991,4.5011166886044727,4.5018474066189658,4.5024123022610159,4.5028490057226529,4.5031866077489608,4.5034475975009887]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.6632927176101306,5.6632927176237002,5.6632927176237198,5.6632927176237198,5.6632927176237198,5.6632927176237198,5.6632927176237198]
[null,null,null,null,"Coincident",4.0675086700741412,4.0675086700838872,4.0675086700839014,4.0675086700839014,4.0675086700839014,4.0675086700839014,4.0675086700839014]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.8485878392452042,5.848587839259217,5.8485878392592374,5.8485878392592374,5.8485878392592374,5.8485878392592374,5.8485878392592374]
[null,null,null,null,"Coincident",4.2005919400646698,4.2005919400747338,4.2005919400747489,4.2005919400747489,4.2005919400747489,4.2005919400747489,4.2005919400747489]
[null,"Snowy Adit 11kV","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.0295382312756299E-2,3.0295382310269001E-2,3.0295382310266499E-2,3.0295382310266499E-2,3.0295382310266499E-2,3.0295382310266499E-2,3.0295382310266499E-2]
[null,null,null,null,"Coincident",1.8934613945472687E-3,1.8934613943918125E-3,1.8934613943916562E-3,1.8934613943916562E-3,1.8934613943916562E-3,1.8934613943916562E-3,1.8934613943916562E-3]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.4377687414607129E-2,6.4377687409321621E-2,6.4377687409316306E-2,6.4377687409316306E-2,6.4377687409316306E-2,6.4377687409316306E-2,6.4377687409316306E-2]
[null,null,null,null,"Coincident",4.0236054634129456E-3,4.0236054630826013E-3,4.0236054630822691E-3,4.0236054630822691E-3,4.0236054630822691E-3,4.0236054630822691E-3,4.0236054630822691E-3]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6486225989380097E-2,2.6486225987185998E-2,2.6486225987183802E-2,2.6486225987183802E-2,2.6486225987183802E-2,2.6486225987183802E-2,2.6486225987183802E-2]
[null,null,null,null,"Coincident",1.6553891243362561E-3,1.6553891241991249E-3,1.6553891241989876E-3,1.6553891241989876E-3,1.6553891241989876E-3,1.6553891241989876E-3,1.6553891241989876E-3]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6283230227432708E-2,5.6283230222770243E-2,5.628323022276558E-2,5.628323022276558E-2,5.628323022276558E-2,5.628323022276558E-2,5.628323022276558E-2]
[null,null,null,null,"Coincident",3.5177018892145443E-3,3.5177018889231402E-3,3.5177018889228488E-3,3.5177018889228488E-3,3.5177018889228488E-3,3.5177018889228488E-3,3.5177018889228488E-3]
[null,"South West Rocks","Substation Rating","MVA","Non-Coincident",31.35,31.35,31.35,31.35,31.35,31.35,31.35]
[null,null,null,null,"Coincident",31.35,31.35,31.35,31.35,31.35,31.35,31.35]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.6865396743544094,6.7582527311119405,6.8191641852840803,6.8709010016620002,6.9148450874715204,6.9521702035654096,6.9838733159583199]
[null,null,null,null,"Coincident",5.6476443906949187,5.7082153081590947,5.7596628803321517,5.803361288632912,5.8404777317878409,5.8720036020893644,5.89878096580712]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.6906500414509855,6.7624071818456812,6.8233560796656905,6.875124699834223,6.9190957990667084,6.9564438597532483,6.9881664607660401]
[null,null,null,null,"Coincident",5.6511161253749229,5.7117242771513554,5.763203475310072,5.8069287460102803,5.8440680054818861,5.875613255448572,5.9024070798171451]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.1892096470948301,6.2560682567876906,6.3136577229749005,6.3632631011148799,6.4059912891555699,6.44279572693425,6.4744976713020996]
[null,null,null,null,"Coincident",5.2275850961169805,5.2840558074850392,5.3326975327293775,5.3745956667784514,5.4106851275855261,5.4417712179546092,5.4685475951246882]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.193014294180796,6.2599140033724687,6.3175388711064357,6.3671747427937584,6.4099291968175685,6.4467562591161682,6.4784776913858879]
[null,null,null,null,"Coincident",5.2307986108525677,5.2873040360435057,5.3359756624559669,5.377899552235208,5.4140111980496943,5.4451163977412733,5.4719092349557164]
[null,"Spring Ridge","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.94729550042729893,0.947295303255553,0.9472952457923679,0.94729522904545793,0.94729522416478507,0.94729522274237499,0.94729522232783203]
[null,null,null,null,"Coincident",0.44778948422329046,0.4477893910196023,0.44778936385657869,0.44778935594026309,0.44778935363315403,0.44778935296077643,0.44778935276482074]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.98639824412003696,0.98639803880937738,0.98639797897421,0.98639796153601611,0.9863979564538774,0.98639795497275262,0.98639795454109802]
[null,null,null,null,"Coincident",0.46627347092225446,0.46627337387127693,0.46627334558701006,0.4662733373439224,0.46627333494157985,0.46627333424144762,0.46627333403740318]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.82946497632145999,0.82946487345396391,0.82946484386504904,0.82946483535406301,0.82946483290595407,0.82946483220177702,0.82946483199922705]
[null,null,null,null,"Coincident",0.39209063461267418,0.39209058598689372,0.39209057200012304,0.39209056797695391,0.39209056681972532,0.39209056648685864,0.39209056639111267]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.86370387680876393,0.8637037696950729,0.86370373888477803,0.86370373002247303,0.86370372747331037,0.86370372674006601,0.86370372652915517]
[null,null,null,null,"Coincident",0.40827546773250489,0.40827541709953513,0.40827540253541439,0.40827539834617566,0.40827539714117866,0.40827539679457181,0.40827539669487362]
[null,"Stewart","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.403814873816401,19.403814931783199,19.403814952010201,19.4038149590682,19.403814961531101,19.403814962390502,19.403814962690298]
[null,null,null,null,"Coincident",15.896295124138121,15.896295171626583,15.896295188197263,15.896295193979427,15.896295195997123,15.896295196701175,15.896295196946777]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",19.433555369839112,19.433555427894756,19.433555448152763,19.43355545522158,19.433555457688254,19.433555458548973,19.433555458849227]
[null,null,null,null,"Coincident",15.920659596021082,15.920659643582329,15.920659660178409,15.920659665969435,15.920659667990222,15.920659668695354,15.920659668941333]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.424395329473501,17.466935159164201,17.504690837004699,17.538200402500301,17.567941385683,17.594337612181,17.617765242971]
[null,null,null,null,"Coincident",14.274684247308878,14.309534388463668,14.340465182303301,14.367917409922653,14.392282280904396,14.413907008273963,14.433099756479354]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.451101941722911,17.493706972800243,17.531520519291519,17.565081445362647,17.594868012962525,17.62130469732277,17.644768235967224]
[null,null,null,null,"Coincident",14.296563253722992,14.331466810172207,14.362445012068306,14.389939316097456,14.414341531454689,14.435999403343645,14.455221568540251]
[null,"Stroud 33/11kV","Substation Rating","MVA","Non-Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,null,null,"Coincident",14.3,14.3,14.3,14.3,14.3,14.3,14.3]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.2342527246431598,3.23501105203135,3.23558656810998,3.2360233435211296,3.2363548247201201,3.2366063951668202,3.236797319086]
[null,null,null,null,"Coincident",2.8913630900851199,2.892041020972743,2.8925555218757868,2.8929459911464264,2.8932423293071752,2.8934672287093162,2.8936379112192898]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.4040000684837732,3.4047981961197693,3.4054039177308675,3.4058636169739529,3.4062124957166273,3.4064772696507331,3.4066782140695198]
[null,null,null,null,"Coincident",3.0431141270035131,3.0438276385885272,3.0443691426880219,3.0447801054473231,3.0450919966955854,3.0453286997752356,3.0455083404295391]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.9367986758665903,2.9668602058964102,2.9968916743962,3.0268931114274902,3.0568645470217497,3.0868060111804199,3.1167175338749198]
[null,null,null,null,"Coincident",2.6254445825189427,2.6523190434098418,2.67916662983985,2.7059873686834282,2.7327812867881631,2.7595484109747979,2.7862887680372359]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.0909343656426533,3.1225736526719388,3.1541813004141948,3.185757340508709,3.217301804563129,3.2488147241534997,3.2802961308242682]
[null,null,null,null,"Coincident",2.7632390847505177,2.7915240316923735,2.8197806936872873,2.8480090990202069,2.8762092759477937,2.9043812526984576,2.9325250574723603]
[null,"Suffolk Park","Substation Rating","MVA","Non-Coincident",36,36,36,36,36,36,36]
[null,null,null,null,"Coincident",33,33,33,33,33,33,33]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.1701633108013,12.170163492620802,12.170163536452799,12.1701635470195,12.170163549566899,12.170163550181,12.170163550329001]
[null,null,null,null,"Coincident",8.8952830017129489,8.8952831346064762,8.8952831666436811,8.8952831743669787,8.8952831762288955,8.8952831766777489,8.8952831767859237]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.202248286802503,12.202248469101347,12.2022485130489,12.20224852364346,12.202248526197575,12.202248526813294,12.202248526961686]
[null,null,null,null,"Coincident",8.9187342023538285,8.9187343355977102,8.9187343677193773,8.9187343754630373,8.918734377329864,8.9187343777798986,8.9187343778883594]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.4673648342616,11.467365122839698,11.467365196312199,11.4673652150184,11.467365219781001,11.467365220993601,11.4673652213023]
[null,null,null,null,"Coincident",8.3816012061330234,8.3816014170573787,8.3816014707590973,8.3816014844316307,8.3816014879126577,8.3816014887989585,8.3816014890245896]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.497596977915562,11.497597267254458,11.497597340920658,11.497597359676176,11.497597364451332,11.497597365667129,11.497597365976642]
[null,null,null,null,"Coincident",8.4036981547673726,8.4036983662478022,8.4036984200910982,8.4036984337996774,8.4036984372898811,8.4036984381785196,8.403698438404744]
[null,"Sunset Strip 22","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.77634370688522902,0.77634370315726298,0.77634370202234693,0.77634370167684097,0.776343701571658,0.77634370153963594,0.77634370152988796]
[null,null,null,null,"Coincident",0.45667276875601709,0.45667276656309591,0.45667276589549821,0.4566727656922594,0.45667276563038706,0.45667276561155057,0.45667276560581649]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.79283466797919644,0.79283466417204151,0.79283466301301786,0.79283466266017266,0.79283466255275536,0.79283466252005319,0.79283466251009815]
[null,null,null,null,"Coincident",0.46637333410540971,0.46637333186590679,0.46637333118412816,0.46637333097657219,0.46637333091338551,0.46637333089414895,0.46637333088829303]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.70829754291255098,0.70829753961353692,0.708297538693204,0.70829753843645704,0.708297538364832,0.70829753834485099,0.708297538339276]
[null,null,null,null,"Coincident",0.41664561347797119,0.41664561153737467,0.41664561099600239,0.41664561084497476,0.41664561080284235,0.41664561079108881,0.41664561078780943]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.7233430789548112,0.72334307558571997,0.72334307464583747,0.72334307438363676,0.72334307431049027,0.72334307429008482,0.72334307428439149]
[null,null,null,null,"Coincident",0.42549592879694775,0.42549592681512943,0.42549592626225735,0.42549592610802162,0.42549592606499431,0.42549592605299108,0.42549592604964204]
[null,"Sunset Strip 33","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.0516150469570698,2.0864719207901299,2.12129393774936,2.15608113269163,2.1908335404389598,2.2255511957785403,2.26023413346278]
[null,null,null,null,"Coincident",1.6331583524551323,1.660905660472477,1.6886252211818067,1.7163170623304265,1.7439812116378992,1.7716176967960628,1.7992265454690675]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.0708790380083095,2.1060632064313514,2.1412121906859736,2.1763260259563402,2.211404747391438,2.2464483901050993,2.2814569891760454]
[null,null,null,null,"Coincident",1.6484931726659784,1.6765010187867722,1.704480857061448,1.7324327154978483,1.7603566220758136,1.7882526047471996,1.8161206914359131]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.9044824025699298,1.9362887033609799,1.96806319785123,1.99980591784699,2.0315168951227598,2.0631961614212502,2.0948437484534401]
[null,null,null,null,"Coincident",1.516035548420299,1.5413544920859965,1.5666481168080213,1.5919164479053243,1.6171595106715344,1.6423773303749754,1.6675699322587114]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.9223648664438258,1.9544698179465287,1.9865426644977202,2.0185834382023606,2.0505921711333022,2.0825688953313088,2.1145136428051154]
[null,null,null,null,"Coincident",1.5302706239923203,1.5558273042182593,1.5813584277639652,1.6068640201861255,1.6323441070158682,1.657798713758778,1.6832278658949433]
[null,"Sutton","Substation Rating","MVA","Non-Coincident",19.2,19.2,19.2,19.2,19.2,19.2,19.2]
[null,null,null,null,"Coincident",17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001,17.600000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.9058997727106699,3.9058997727106699,3.9058997727106699,3.9058997727106699,3.9058997727106699,3.9058997727106699,3.9058997727106699]
[null,null,null,null,"Coincident",2.6492468998243104,2.6492468998243104,2.6492468998243104,2.6492468998243104,2.6492468998243104,2.6492468998243104,2.6492468998243104]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.9797575650694079,3.9797575650694079,3.9797575650694079,3.9797575650694079,3.9797575650694079,3.9797575650694079,3.9797575650694079]
[null,null,null,null,"Coincident",2.6993422783082446,2.6993422783082446,2.6993422783082446,2.6993422783082446,2.6993422783082446,2.6993422783082446,2.6993422783082446]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.7220631959653403,3.7220631959653403,3.7220631959653403,3.7220631959653403,3.7220631959653403,3.7220631959653403,3.7220631959653403]
[null,null,null,null,"Coincident",2.5245564291625699,2.5245564291625699,2.5245564291625699,2.5245564291625699,2.5245564291625699,2.5245564291625699,2.5245564291625699]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.7924447691419934,3.7924447691419934,3.7924447691419934,3.7924447691419934,3.7924447691419934,3.7924447691419934,3.7924447691419934]
[null,null,null,null,"Coincident",2.5722939993495295,2.5722939993495295,2.5722939993495295,2.5722939993495295,2.5722939993495295,2.5722939993495295,2.5722939993495295]
[null,"Talbingo","Substation Rating","MVA","Non-Coincident",3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005]
[null,null,null,null,"Coincident",3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005,3.8500000000000005]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.24247988211175,1.26746441684355,1.2901137221502399,1.31064606491277,1.3292593112622602,1.3461328333767899,1.3614292380556701]
[null,null,null,null,"Coincident",0.43072635913207336,0.43938766450576405,0.44723942367874986,0.45435730250309364,0.46080989457091687,0.4666593822372872,0.47196213585929897]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.6041795811265036,1.6364373915246722,1.6656801612650871,1.6921896971429315,1.7162214663186066,1.7380070582042551,1.7577564162452093]
[null,null,null,null,"Coincident",0.55611558812385464,0.56729829572855306,0.57743578923856353,0.58662576167621627,0.5949567749904503,0.60250911351080849,0.6093555576316726]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1151963854056501,1.1363127270854401,1.15544561516239,1.1727813550228199,1.1884887524267,1.2027207572438998,1.2156159527946899]
[null,null,null,null,"Coincident",0.38660141360729205,0.39392174538961922,0.40055447992296189,0.40656420307457758,0.41200943417458935,0.41694319584455197,0.42141353030215917]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4398424442681836,1.467105987636979,1.4918086720207744,1.5141910383739072,1.5344710336886946,1.5528461332415682,1.5694952634971437]
[null,null,null,null,"Coincident",0.49914538067963699,0.50859674238081942,0.51716033963386843,0.52491955996962114,0.53194995834541414,0.53831999285707699,0.54409169134567648]
[null,"Tamworth East","Substation Rating","MVA","Non-Coincident",83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009]
[null,null,null,null,"Coincident",83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009,83.600000000000009]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",35.887292903059802,35.887294080989101,35.887294785433305,35.887295206716402,35.887295458658897,35.887295609329598,35.887295699436102]
[null,null,null,null,"Coincident",31.303861472505968,31.303862499993212,31.303863114467639,31.303863481945559,31.303863701710615,31.303863833138049,31.303863911736382]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",36.058494360749521,36.058495544298168,36.058496252102948,36.058496675395787,36.058496928540187,36.058497079929666,36.058497170466026]
[null,null,null,null,"Coincident",31.453197526632056,31.453198559020958,31.453199176426757,31.453199545657739,31.453199766471197,31.453199898525607,31.453199977498901]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",32.176106412677797,32.176106518080999,32.176106574600901,32.176106604908298,32.176106621159896,32.176106629874404,32.176106634547303]
[null,null,null,null,"Coincident",28.066658039319492,28.066658131260873,28.0666581805622,28.066658206998817,28.066658221174801,28.066658228776316,28.066658232852404]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",32.32960353868031,32.329603644586342,32.329603701375873,32.329603731827852,32.329603748156977,32.329603756913059,32.329603761608247]
[null,null,null,null,"Coincident",28.200550912816251,28.200551005196239,28.20055105473276,28.20055108129549,28.200551095539105,28.200551103176881,28.200551107272414]
[null,"Tamworth South","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",25.438739062423302,25.4387393461543,25.438739504753801,25.438739593407501,25.438739642963,25.438739670663399,25.4387396861474]
[null,null,null,null,"Coincident",23.666886590413718,23.666886854382359,23.666887001935127,23.666887084413943,23.666887130517814,23.666887156288833,23.666887170694348]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",26.407984551576163,26.407984846117643,26.407985010759969,26.407985102791478,26.407985154235099,26.407985182990913,26.407985199064875]
[null,null,null,null,"Coincident",24.568622443506182,24.568622717532335,24.568622870707035,24.56862295632839,24.568623004188872,24.568623030941794,24.568623045896178]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",22.273247179737599,22.310186672872401,22.3420346699058,22.369492949079699,22.393166560151702,22.413577156811503,22.431174491444597]
[null,null,null,null,"Coincident",20.721876729407615,20.75624332252308,20.785873051106392,20.811418813322906,20.833443516161037,20.852432479222642,20.868804128856418]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",23.121883753459773,23.160230684164681,23.193292126856193,23.2217965983419,23.246372201477548,23.267560465563982,23.285828279074682]
[null,null,null,null,"Coincident",21.511404288044663,21.547080288252712,21.577838943891084,21.60435802930316,21.627221898887072,21.646934363484899,21.663929791974951]
[null,"Tarcutta","Substation Rating","MVA","Non-Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,null,null,"Coincident",4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004,4.4000000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.0529968120903399,1.0536820944016698,1.0542403615388201,1.0546951554117399,1.0550656545027299,1.0553674826156401,1.0556133677256501]
[null,null,null,null,"Coincident",0.84054104001334673,0.84108805772513318,0.84153368722246658,0.84189672052944953,0.84219246662069047,0.84243339699485476,0.84262967159295277]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.1705694238222684,1.1713312214945106,1.1719518220828216,1.1724573960747551,1.1728692633306548,1.1732047921339388,1.1734781316049099]
[null,null,null,null,"Coincident",0.93439185153295667,0.9349999466386153,0.93549533300440701,0.93589890088239513,0.93622766857442086,0.93649550008732629,0.93671368977277336]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.97874996633713895,0.97898688494107799,0.97920360790789507,0.97940185677296998,0.97958320632295504,0.97974909710506408,0.97990084687004109]
[null,null,null,null,"Coincident",0.78127445892729508,0.78146357612828465,0.78163657242402984,0.78179482200780659,0.78193958193262325,0.78207200209659866,0.78219313437716309]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.0880325286901595,1.0882959004976724,1.0885368217193545,1.0887572061090314,1.0889588042865368,1.0891432176437295,1.089311911065129]
[null,null,null,null,"Coincident",0.86850784611408427,0.86871807924153088,0.86891039148019,0.86908631045921703,0.86924723358817579,0.8693944391573355,0.86952909649175336]
[null,"Tea Gardens","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.345211679893,11.6173364580258,11.884288618165199,12.146166482768701,12.403066505355,12.655083306029502,12.9023097063343]
[null,null,null,null,"Coincident",9.8595291980022495,10.096018588522423,10.328012727691185,10.555597062406132,10.778855415368035,10.997870015954209,11.212721530504808]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.346337196924734,11.618488971563302,11.885467615051921,12.147371459602308,12.404296968301958,12.656338770643194,12.903589697376594]
[null,null,null,null,"Coincident",9.860507325898876,10.097020177668108,10.329037332128456,10.556644244654388,10.779924746262417,10.998961074487537,11.213833903672516]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.117886066502701,10.293345994697599,10.459595845937299,10.617119066889,10.7663737275938,10.9077938535124,11.0417906876509]
[null,null,null,null,"Coincident",8.7929247958892525,8.9454078287252941,9.0898868661121774,9.2267820462249652,9.3564914537422315,9.4793922774572046,9.5958419071251875]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.118889825041043,10.294367159974851,10.460633504255346,10.618172352510713,10.767441820225505,10.908875975918502,11.042886103393721]
[null,null,null,null,"Coincident",8.7937971098570973,8.9462952699781439,9.0907886406028613,9.2276974015866919,9.3574196771007365,9.4803326933577452,9.5967938755683537]
[null,"Telegraph Point","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6109455331595299,2.61095058750786,2.6109507933971301,2.6109508017840399,2.61095080212568,2.6109508021396,2.6109508021401697]
[null,null,null,null,"Coincident",1.6967990108728128,1.6968022955883069,1.6968024293914465,1.6968024348419242,1.696802435063949,1.6968024350729953,1.6968024350733655]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.659335337561358,2.6593404855841536,2.6593406952892602,2.6593407038316084,2.6593407041795802,2.6593407041937582,2.6593407041943387]
[null,null,null,null,"Coincident",1.7282465348454754,1.7282498804380497,1.728250016721022,1.7282500222725157,1.7282500224986552,1.7282500225078692,1.7282500225082464]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.97610721806214,2.0059195163152901,2.0156118919754,2.0187630125344103,2.0197874838431602,2.0201205531252797,2.0202288383898299]
[null,null,null,null,"Coincident",1.284230839135468,1.3036052295795981,1.3099041022386462,1.311951949725223,1.312617732247791,1.3128341870229958,1.3129045593564848]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.012731284150318,2.0430961068674667,2.0529681155978285,2.0561776372630898,2.0572210955501644,2.0575603377520975,2.0576706299151852]
[null,null,null,null,"Coincident",1.3080320553321767,1.3277655198941272,1.334181132336542,1.3362669334832247,1.3369450552467426,1.3371655216737037,1.3372371982486677]
[null,"Temora 66/11kV","Substation Rating","MVA","Non-Coincident",24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004]
[null,null,null,null,"Coincident",24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004,24.750000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.0424132115667106,8.0511992631270299,8.0592455586057206,8.0666143829844597,8.0733627770582697,8.0795429789785302,8.0852028286194102]
[null,null,null,null,"Coincident",7.3877981827182575,7.3958690905469222,7.4032604549982777,7.4100294913461893,7.4162285975302709,7.4219057597593476,7.4271049239643414]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3250406525933442,8.3341354646219337,8.342464523972744,8.3500923044536819,8.3570778513941679,8.3634752387049076,8.3693339874546151]
[null,null,null,null,"Coincident",7.6474210645915601,7.6557756012224738,7.6634267138819387,7.6704336285097776,7.6768505844202242,7.6827272541591594,7.6881091280106348]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.3487211098337903,7.3532269914509598,7.3573201468789406,7.3610383806855602,7.3644160346456804,7.3674843049233596,7.3702715302010304]
[null,null,null,null,"Coincident",6.7505693915915046,6.7547085154026254,6.7584685070167012,6.7618840938855724,6.7649868225233574,6.7678053498714581,6.7703657079753645]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.6069707405669682,7.6116349684115114,7.6158719659940672,7.6197208664150793,7.6232172182921438,7.6263933140886255,7.6292784883683025]
[null,null,null,null,"Coincident",6.9877987035440752,6.9920832849361556,6.9959754106224565,6.9995110284510611,7.0027227935474343,7.0056403699186207,7.0082907044313476]
[null,"Terranora 11kV","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.03578999488946,5.9741927273928503,5.9164498962459104,5.8623203108865001,5.81157787320232,5.76401063312397,5.7194199033140602]
[null,null,null,null,"Coincident",4.5100594602864623,4.4640327861914217,4.4208862217651443,4.3804395447372331,4.3425238102088111,4.3069806449733203,4.2736615859950362]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.0459615317868138,5.9842604603341929,5.9264203207424488,5.8721995159941622,5.8213715669556105,5.7737241663783081,5.7290582920961874]
[null,null,null,null,"Coincident",4.5176598301217954,4.47155559169562,4.4283363165102827,4.3878214785841108,4.3498418483116241,4.3142387855951156,4.2808635772083745]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.6614961844030907,5.6118962026188601,5.5658330793257402,5.5230546094313802,5.4833265719976696,5.4464314478328397,5.4121672285290297]
[null,null,null,null,"Coincident",4.230379858719802,4.1933177894189457,4.158898529445624,4.1269336262586345,4.0972480654259638,4.0696793123847002,4.0440764225307912]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.6710369599076458,5.6213533920401932,5.575212642991608,5.5323620826525319,5.492567095374814,5.455609795402494,5.4212878339023511]
[null,null,null,null,"Coincident",4.2375089113971187,4.2003843849521765,4.1659071215073791,4.1338883509405671,4.1041527638847191,4.0765375518730469,4.0508915159290568]
[null,"Texas 66/22kV","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.4941496551692497,3.4941496596318,3.4941496608572704,3.4941496611937999,3.49414966128621,3.4941496613115901,3.4941496613185601]
[null,null,null,null,"Coincident",2.1612239057733986,2.161223908533604,2.1612239092915897,2.1612239094997423,2.1612239095569001,2.1612239095725987,2.1612239095769099]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6779049894106652,3.6779049941078985,3.677904995397816,3.6779049957520433,3.6779049958493131,3.6779049958760281,3.6779049958833645]
[null,null,null,null,"Coincident",2.2748814363226137,2.2748814392279768,2.2748814400258248,2.2748814402449238,2.2748814403050877,2.2748814403216118,2.2748814403261495]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.1795744966521502,3.1795745029626499,3.17957450487462,3.1795745054539104,3.17957450562943,3.1795745056826101,3.1795745056987199]
[null,null,null,null,"Coincident",1.9666508565784924,1.9666508604817032,1.9666508616643072,1.9666508620226135,1.9666508621311771,1.9666508621640704,1.9666508621740348]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3467865030163986,3.3467865096587639,3.3467865116712834,3.3467865122810383,3.3467865124657883,3.3467865125217653,3.3467865125387224]
[null,null,null,null,"Coincident",2.070075901625466,2.0700759057339444,2.0700759069787411,2.0700759073558905,2.0700759074701631,2.0700759075047865,2.070075907515275]
[null,"Texas 66/33kV","Substation Rating","MVA","Non-Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,null,null,"Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4812704508838803,2.47495647345889,2.4713816953546504,2.4693577669123301,2.4682118814279304,2.4675631166218701,2.4671958061189398]
[null,null,null,null,"Coincident",1.3346526272639843,1.3312563966935733,1.3293335563248383,1.3282449037710728,1.3276285424744827,1.3272795778331732,1.3270820048811465]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.6114483918682492,2.6048031564861449,2.6010408304050534,2.5989107181175877,2.5977047146348009,2.5970219128834309,2.5966353317181845]
[null,null,null,null,"Coincident",1.4046741482492171,1.4010997370606448,1.3990760163545992,1.3979302484840228,1.3972815502672615,1.3969142774651202,1.396706339000507]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2009725402103699,2.20097251884415,2.20097251882278,2.20097251882276,2.20097251882276,2.20097251882276,2.20097251882276]
[null,null,null,null,"Coincident",1.1838829508815714,1.1838829393888775,1.1838829393773829,1.183882939377372,1.183882939377372,1.183882939377372,1.183882939377372]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3164448674392131,2.3164448449520307,2.3164448449295394,2.3164448449295185,2.3164448449295185,2.3164448449295185,2.3164448449295185]
[null,null,null,null,"Coincident",1.2459944570486492,1.2459944449529998,1.2459944449409019,1.2459944449408908,1.2459944449408908,1.2459944449408908,1.2459944449408908]
[null,"Tharbogang","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",15.488197742282301,14.797733082695601,14.1280153473675,13.478421137460501,12.848345785882801,12.237202794441,11.6444232879056]
[null,null,null,null,"Coincident",14.895847013053624,14.231789379734174,13.587685198384401,12.962934912240765,12.356956979884229,11.769187333919239,11.19907885591865]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",15.524749329929806,14.832655198667814,14.161356953656838,13.510229724860631,12.878667418194873,12.266082151351599,11.671903706576302]
[null,null,null,null,"Coincident",14.931000674360199,14.265375888994324,13.619751645024582,12.993526970755111,12.386118952350119,11.796962191235354,11.225508277803931]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",14.4930058300934,13.9236008739021,13.373810981377899,12.842960445858299,12.330396837663001,11.835490202240601,11.357632285937299]
[null,null,null,null,"Coincident",13.938716511541205,13.391088617254633,12.862325602691202,12.351777603790698,11.858817143239991,11.382838359286858,10.923256261119402]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",14.527208800748165,13.956460069412108,13.405372692585427,12.873269368962291,12.359496129151898,11.863421531932847,11.384435888194666]
[null,null,null,null,"Coincident",13.971611379410465,13.422691103059218,12.892680226866363,12.38092735311595,11.886803523671041,11.409701446967553,10.949034751636377]
[null,"Thredbo","Substation Rating","MVA","Non-Coincident",38.4,38.4,38.4,38.4,38.4,38.4,38.4]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",19.698851330659799,19.6988595731335,19.698862464217399,19.698863478277801,19.698863833963902,19.698863958722399,19.698864002482001]
[null,null,null,null,"Coincident",1.1454991397939864,1.1454996190984077,1.1454997872165411,1.1454998461847163,1.1454998668680607,1.1454998741228366,1.1454998766674818]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",20.265600031954843,20.265608511569848,20.2656114858321,20.265612529067678,20.265612894987097,20.265613023334978,20.26561306835357]
[null,null,null,null,"Coincident",1.1784558913789067,1.1784563844732263,1.1784565574282273,1.1784566180929552,1.1784566393713727,1.1784566468348732,1.1784566494527293]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",17.3602056112437,17.360205617358499,17.360205617364603,17.360205617364699,17.360205617364699,17.360205617364699,17.360205617364699]
[null,null,null,null,"Coincident",1.0095055930177592,1.0095055933733381,1.0095055933736932,1.0095055933736987,1.0095055933736987,1.0095055933736987,1.0095055933736987]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",17.85966996168904,17.859669967979766,17.859669967986044,17.859669967986143,17.859669967986143,17.859669967986143,17.859669967986143]
[null,null,null,null,"Coincident",1.0385497222509399,1.0385497226167493,1.0385497226171143,1.0385497226171201,1.0385497226171201,1.0385497226171201,1.0385497226171201]
[null,"Trundle","Substation Rating","MVA","Non-Coincident",11,11,11,11,11,11,11]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.7493118462502899,2.8390465615507399,2.9078428019479703,2.9605862990097997,3.00102275987232,3.0320238777005302,3.05579127193087]
[null,null,null,null,"Coincident",2.1536613799292987,2.2239546757026059,2.2778459089688226,2.3191622961292682,2.3508380204453028,2.3751226101662959,2.3937406942244031]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8030014290989507,2.8944885172479355,2.9646282361790837,3.0184017278408679,3.0596278469295171,3.0912343661007244,3.1154658988329831]
[null,null,null,null,"Coincident",2.1957188792425826,2.2673848886032095,2.3223285298882579,2.3644517588023897,2.3967460584274698,2.4215048866360132,2.4404865515545033]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.50692113625577,2.5925575805649399,2.6580841527979602,2.7082232227143699,2.7465882133801802,2.7759440133828797,2.7984062368538898]
[null,null,null,null,"Coincident",1.9637856800588676,2.0308686132207305,2.0821985662669356,2.1214747868425756,2.1515278340627351,2.1745235712792934,2.1921192555458253]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5558772232939257,2.6431860078935845,2.7099922073662328,2.7611104116619973,2.8002246081145756,2.8301536790826924,2.8530545531962832]
[null,null,null,null,"Coincident",2.0021352161838193,2.0705281697795725,2.1228605132131948,2.1629037344117195,2.1935436686999217,2.2169884752136344,2.2349277745376925]
[null,"Tumbarumba","Substation Rating","MVA","Non-Coincident",30,30,30,30,30,30,30]
[null,null,null,null,"Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3753667026602603,8.3691423281398798,8.3650987420952205,8.3624718776533182,8.3607653684508811,8.3596567563688904,8.358936560575879]
[null,null,null,null,"Coincident",6.2044991301096752,6.1998880930448852,6.1968925912373471,6.1949466014409218,6.19368241382527,6.1928611503579454,6.1923276269517604]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3794074054476972,8.3731800279725359,8.3691344910963519,8.3665063593214661,8.3647990268122125,8.3636898798793808,8.3629693366272964]
[null,null,null,null,"Coincident",6.2074924959908042,6.2028792343272601,6.1998822873373287,6.1979353586964709,6.1966705611724286,6.1958489014858467,6.1953151206808412]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.2145697094703589,8.2214412067703204,8.2264435934388995,8.2300852848039199,8.2327364025356609,8.2346663917969796,8.2360714061817397]
[null,null,null,null,"Coincident",6.085380190033403,6.0904706177763002,6.0941764022315423,6.0968741791419223,6.0988381358550265,6.1002678782314614,6.1013087174970746]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2185328356117022,8.2254076480713803,8.2304124481456604,8.2340558964477761,8.2367082932135212,8.2386392135998001,8.2400449058349459]
[null,null,null,null,"Coincident",6.0883160868806021,6.0934089705046937,6.0971165428187968,6.0998156212739403,6.101780525499632,6.1032109576564917,6.1042522990758936]
[null,"Tumut","Substation Rating","MVA","Non-Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,null,null,"Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",20.225278885903602,20.1603240320221,20.097635329636301,20.037133717024201,19.978742890777099,19.922389209567299,19.8680016012732]
[null,null,null,null,"Coincident",19.226499681661448,19.164752474885205,19.105159510888829,19.047645632232879,18.992138303578226,18.93856752020595,18.886865719728842]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",21.803258815893493,21.733236172521487,21.665656486196237,21.600434526785829,21.537488037675772,21.476737632028609,21.418106692662914]
[null,null,null,null,"Coincident",20.726554676837022,20.659989941779681,20.595747523914941,20.53374640200628,20.473908381494251,20.416157995879047,20.360422411543755]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",18.518746796612199,18.488078432214397,18.457440736181002,18.4268336778436,18.396257226564501,18.365711351736802,18.335196022783798]
[null,null,null,null,"Coincident",17.60424078196468,17.575086904697635,17.545962181307864,17.516866582641445,17.48780007957366,17.458762643009056,17.429754243880893]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",19.963582783224258,19.93052166746919,19.897493612829887,19.86449858624518,19.831536554687016,19.798607485160545,19.765711344703455]
[null,null,null,null,"Coincident",18.977726843311945,18.946298375248485,18.914901335653102,18.883535693097269,18.852201416183952,18.820898473547675,18.789626833853898]
[null,"Tuncurry","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.3527732885727808,8.3527732167186297,8.3527731797695512,8.3527731607694697,8.3527731509991892,8.35277314597508,8.3527731433915591]
[null,null,null,null,"Coincident",6.2108971573019218,6.2108971038731111,6.2108970763987719,6.2108970622708233,6.2108970550059057,6.2108970512701136,6.2108970493490769]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",8.3826725746692023,8.3826725025578455,8.3826724654765048,8.3826724464084119,8.3826724366031584,8.3826724315610637,8.382672428968295]
[null,null,null,null,"Coincident",6.2331294608262704,6.2331294072062082,6.2331293796335228,6.2331293654550031,6.2331293581640805,6.2331293544149142,6.2331293524870013]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.1453394141380002,7.1453318005180799,7.1453309526739703,7.14533085825901,7.1453308477450603,7.1453308465742404,7.1453308464438594]
[null,null,null,null,"Coincident",5.3130818617980253,5.3130762005153969,5.3130755700813612,5.3130754998769412,5.3130754920590517,5.313075491188461,5.3130754910915137]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.1709166134726967,7.1709089725993369,7.1709081217203154,7.1709080269673908,7.1709080164158054,7.1709080152407942,7.1709080151099469]
[null,null,null,null,"Coincident",5.3321003780621909,5.3320946965146394,5.3320940638239254,5.3320939933682032,5.332093985522329,5.3320939846486226,5.332093984551328]
[null,"Tuross","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2320179871326498,2.2320180419523097,2.2320180662362499,2.2320180769935098,2.23201808175875,2.2320180838696402,2.23201808480473]
[null,null,null,null,"Coincident",1.432829961049348,1.4328299962404851,1.4328300118294084,1.4328300187349641,1.43283002179398,1.4328300231490527,1.4328300237493279]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.27687037635161,2.276870432272871,2.2768704570447968,2.2768704680182239,2.2768704728792213,2.2768704750325299,2.2768704759864105]
[null,null,null,null,"Coincident",1.461622671264077,1.46162270716238,1.4616227230645626,1.4616227301088853,1.4616227332293721,1.461622734611675,1.4616227352240128]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0493747583447899,2.0493747662330204,2.0493747690216302,2.0493747700074398,2.0493747703559402,2.0493747704791399,2.0493747705226903]
[null,null,null,null,"Coincident",1.3155832847686502,1.3155832898324502,1.3155832916225809,1.3155832922554151,1.3155832924791329,1.31558329255822,1.315583292586177]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.090556932882226,2.0905569409289706,2.0905569437736173,2.0905569447792369,2.0905569451347401,2.0905569452604156,2.0905569453048414]
[null,null,null,null,"Coincident",1.3420199236660835,1.3420199288316408,1.3420199306577441,1.3420199313032952,1.3420199315315082,1.3420199316121848,1.3420199316407038]
[null,"Tweed Heads","Substation Rating","MVA","Non-Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,null,null,"Coincident",55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007,55.000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.036395475252402,16.594911802775602,16.255791468230999,15.995300291611901,15.795207150079699,15.641508027492101,15.5234459085043]
[null,null,null,null,"Coincident",14.965058497637202,14.577251758003557,14.279362709139299,14.050542845108444,13.874777638650588,13.739765724663258,13.636057958570721]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.664171575405987,17.206419620205207,16.85480300137251,16.584712955366989,16.377246558603595,16.217883759335372,16.09547115571943]
[null,null,null,null,"Coincident",15.516507662800336,15.114410587926816,14.805544591172021,14.568292917602131,14.386050918796206,14.24606393523149,14.138534629714854]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",15.521986505334901,15.142549020839601,14.8519039043895,14.6292728065983,14.458739730697699,14.328113190808899,14.2280546371634]
[null,null,null,null,"Coincident",13.634775994094525,13.301471677467397,13.046164081676576,12.850601152494859,12.700802008635957,12.58605744229741,12.498164313104146]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.09395797483446,15.700538554746354,15.39918342290604,15.168348566136169,14.991531497269357,14.856091484958702,14.752345862139101]
[null,null,null,null,"Coincident",14.137205425981941,13.791619140181201,13.526903685371259,13.324134435275317,13.1688153255014,13.0498425234146,12.95871061017483]
[null,"Tweed Heads South","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",14.1250693939075,13.816664184851101,13.554504485432801,13.3316557592086,13.1422233068143,12.9811963418947,12.8443154479217]
[null,null,null,null,"Coincident",12.426388242527509,12.155071850594901,11.924439482309246,11.728390548729559,11.56173924716491,11.420077388535748,11.299657793837941]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.155676261499933,13.846602785468329,13.583875026029622,13.360543420658672,13.170700497078252,13.00932461132459,12.87214711736465]
[null,null,null,null,"Coincident",12.45331432756007,12.181410034453178,11.950277921057479,11.753804179387695,11.586791769910661,11.444822951674505,11.324142426110612]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",13.542822113013701,13.273683108283299,13.0448148903329,12.850191813531898,12.6846898388029,12.543951627849699,12.424271823093601]
[null,null,null,null,"Coincident",11.914162032250406,11.677389690060714,11.476045168960255,11.304827467592526,11.159228763930612,11.035415733276224,10.930128624433374]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",13.57216733969412,13.302445151854878,13.073081011438713,12.878036216161437,12.712175623935734,12.571132454778951,12.45119332216856]
[null,null,null,null,"Coincident",11.939978201334371,11.702692809649145,11.500912005729399,11.329323301758491,11.183409107947796,11.059327793369999,10.953812543446231]
[null,"Ulan Town","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.4027956347342601,2.4027956347347699,2.5747313667948002,2.6758543302477102,2.77658243278711,2.8769172162501402,2.9768602164534501]
[null,null,null,null,"Coincident",2.004601382462659,2.0046013824630839,2.1480437132214321,2.2324084546110354,2.3164437719240922,2.4001509514825927,2.4835312745857596]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.5293610449917372,2.5293610449922741,2.7103533593731326,2.8168028970759935,2.92283677487071,3.0284566158095076,3.1336640366069952]
[null,null,null,null,"Coincident",2.1101922170332204,2.110192217033668,2.2611902621350408,2.349998851328797,2.4384606642863829,2.5265770550858089,2.6143493725177485]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.2583758662435098,2.3554399948067997,2.4521251112331401,2.54843269547401,2.64436422170201,2.7399211583334702,2.8351049680509099]
[null,null,null,null,"Coincident",1.8841150358976446,1.9650935775150733,2.0457559173537421,2.1261032901057484,2.2061369256419932,2.2858580490310434,2.3652678805578704]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.3773340763778927,2.4795109831880331,2.5812889136886947,2.6826694257866603,2.7836540713054387,2.8842443960090582,2.9844419396257149]
[null,null,null,null,"Coincident",1.9833593449198061,2.0686033688752676,2.1535145353667029,2.2380941441226638,2.3223434897965554,2.4062638619864876,2.489856545255003]
[null,"Ulong","Substation Rating","MVA","Non-Coincident",3,3,3,3,3,3,3]
[null,null,null,null,"Coincident",2.75,2.75,2.75,2.75,2.75,2.75,2.75]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.41336522206320003,0.42658814288871999,0.43907443759368103,0.45086514234918701,0.46199900727200399,0.472512623776702,0.48244054483324]
[null,null,null,null,"Coincident",0.21738280070353572,0.22433654380796447,0.23090290587351617,0.23710346722995393,0.2429586060040784,0.24848756509238007,0.25370851540276657]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.44264995169165561,0.45680964619963743,0.47018052854037229,0.48280654207964707,0.49472918217410777,0.50598763254562362,0.51661889405848316]
[null,null,null,null,"Coincident",0.2327832171021513,0.24022959595784749,0.24726114988635381,0.25390098806913319,0.260170932314994,0.2660915887773988,0.27168241567653201]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.39595261519291103,0.40863324125654904,0.42069944635589096,0.432181001349209,0.44310623459191201,0.45350210183088097,0.46339425271218604]
[null,null,null,null,"Coincident",0.20822576221316574,0.21489432033382552,0.22123976334247125,0.22727774730353498,0.23302316969002457,0.23849020613994557,0.24369234543174906]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.42400375414390745,0.43758273518753071,0.45050376680617205,0.46279872896522922,0.47449795693357333,0.48563031612952645,0.49622327334029726]
[null,null,null,null,"Coincident",0.22297745108930284,0.23011844112041804,0.23691342505065724,0.24337916809343116,0.2495316231285549,0.2553859700626665,0.26095665328249962]
[null,"Union Rd","Substation Rating","MVA","Non-Coincident",135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001]
[null,null,null,null,"Coincident",135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001,135.30000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",51.447564563846598,51.588630929368598,51.687027843290906,51.755661869790501,51.803535623201704,51.836928626389302,51.860220985614099]
[null,null,null,null,"Coincident",45.836522721779197,45.962203922110923,46.049869342602413,46.111017914780824,46.153670398034649,46.183421449660372,46.204173467018286]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",51.450606878237743,51.591681585616882,51.690084318169284,51.758722403292225,51.806598987683088,51.839993965541694,51.863287702143246]
[null,null,null,null,"Coincident",45.839233231283366,45.964921863681653,46.052592468204161,46.11374465635901,46.156399661836474,46.186152472769045,46.206905717282439]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",47.355141765187504,47.323054461476104,47.290999245068299,47.258976083877002,47.226984945846901,47.195025798954795,47.163098611209598]
[null,null,null,null,"Coincident",42.190433112132581,42.16184535607227,42.133286187767922,42.104755578631959,42.076253500105139,42.047779923656819,42.019334820784962]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",47.357942077126623,47.32585287595581,47.293795763986047,47.261770709128356,47.229777679325522,47.197816642552461,47.165887566816188]
[null,null,null,null,"Coincident",42.192928012773912,42.164338566197401,42.135777709067362,42.107245412794541,42.078741648817989,42.050266388605394,42.021819603653014]
[null,"Upper Manilla","Substation Rating","MVA","Non-Coincident",1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001]
[null,null,null,null,"Coincident",1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001,1.6500000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.823030705478211,0.82303070471330209,0.82303070471253703,0.82303070471253603,0.82303070471253603,0.82303070471253603,0.82303070471253603]
[null,null,null,null,"Coincident",0.48667234829924155,0.48667234784693764,0.48667234784648522,0.48667234784648467,0.48667234784648467,0.48667234784648467,0.48667234784648467]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.89572353724949005,0.89572353641702185,0.89572353641618918,0.89572353641618807,0.89572353641618807,0.89572353641618807,0.89572353641618807]
[null,null,null,null,"Coincident",0.52965688205621042,0.52965688156395752,0.52965688156346513,0.52965688156346458,0.52965688156346458,0.52965688156346458,0.52965688156346458]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.7273843782405599,0.72738437795763,0.72738437795734701,0.72738437795734601,0.72738437795734601,0.72738437795734601,0.72738437795734601]
[null,null,null,null,"Coincident",0.43011501407937303,0.43011501391207163,0.43011501391190432,0.43011501391190371,0.43011501391190371,0.43011501391190371,0.43011501391190371]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.7916294056600105,0.79162940535209125,0.79162940535178328,0.79162940535178217,0.79162940535178217,0.79162940535178217,0.79162940535178217]
[null,null,null,null,"Coincident",0.46810421442470684,0.46810421424262882,0.46810421424244669,0.46810421424244608,0.46810421424244608,0.46810421424244608,0.46810421424244608]
[null,"Uralla","Substation Rating","MVA","Non-Coincident",12,12,12,12,12,12,12]
[null,null,null,null,"Coincident",11,11,11,11,11,11,11]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.35711980206302,3.3571304741043599,3.3571350684318699,3.3571370462957697,3.3571378977687298,3.3571382643289298,3.3571384221335601]
[null,null,null,null,"Coincident",1.8050168629253192,1.8050226009435359,1.8050250711677513,1.8050261346024521,1.8050265924124624,1.8050267895002583,1.8050268743468039]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.5331017338239854,3.533112965299174,3.5331178004636747,3.5331198820082084,3.5331207781158156,3.5331211638912881,3.5331213299681172]
[null,null,null,null,"Coincident",1.899636767226474,1.8996428060345316,1.8996454057491601,1.8996465249296499,1.8996470067382945,1.8996472141575331,1.8996473034517778]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2152771844771499,3.2152860578672997,3.2152898429844101,3.2152914575997102,3.2152921463452597,3.21529244014306,3.2152925654682298]
[null,null,null,null,"Coincident",1.7287525852946464,1.7287573562351537,1.7287593913725976,1.7287602595000449,1.7287606298166867,1.7287607877824474,1.7287608551658171]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.3838236539011879,3.3838329924389736,3.3838369759738529,3.3838386752281107,3.383839400078053,3.3838397092768835,3.3838398411716626]
[null,null,null,null,"Coincident",1.8193746772765769,1.8193796983122181,1.8193818401326045,1.8193827537677354,1.8193831434965642,1.8193833097429706,1.819383380658611]
[null,"Uranquinty","Substation Rating","MVA","Non-Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,null,null,"Coincident",35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003,35.200000000000003]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.5014365870294393,5.5014365923195498,5.5014365942263499,5.5014365949136401,5.5014365951613797,5.5014365952506692,5.5014365952828603]
[null,null,null,null,"Coincident",5.0638223130611886,5.0638223179304953,5.0638223196856176,5.0638223203182378,5.0638223205462705,5.0638223206284572,5.0638223206580877]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.5879175030755457,5.5879175084488146,5.5879175103855898,5.5879175110836838,5.5879175113353172,5.5879175114260109,5.5879175114587074]
[null,null,null,null,"Coincident",5.1434240653309002,5.1434240702767502,5.1434240720594637,5.1434240727020279,5.1434240729336445,5.1434240730171243,5.1434240730472194]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.0164808119737998,5.0164808148522599,5.0164808158584799,5.0164808162102199,5.0164808163331696,5.0164808163761503,5.01648081639118]
[null,null,null,null,"Coincident",4.617442565566793,4.6174425682162852,4.6174425691424652,4.6174425694662258,4.6174425695793948,4.6174425696189569,4.6174425696327912]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.0953383701923265,5.0953383731160358,5.0953383741380733,5.0953383744953422,5.0953383746202245,5.0953383746638812,5.0953383746791472]
[null,null,null,null,"Coincident",4.6900273634724829,4.6900273661636245,4.6900273671043635,4.6900273674332134,4.6900273675481614,4.6900273675883453,4.6900273676023971]
[null,"Urbenville","Substation Rating","MVA","Non-Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,null,null,"Coincident",11.55,11.55,11.55,11.55,11.55,11.55,11.55]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.83465952479331806,0.84178233243186196,0.84782334720289598,0.85294686889767801,0.85729224389705305,0.86097765502831203,0.86410333582878607]
[null,null,null,null,"Coincident",0.53003329901258656,0.53455649094743485,0.53839271265624222,0.54164629932934738,0.54440574000898967,0.54674608425966198,0.5487309833198456]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.84527652461945602,0.85248993548627883,0.85860779291095624,0.8637964866038127,0.86819713545347332,0.87192942559129438,0.87509486554089377]
[null,null,null,null,"Coincident",0.53677540555579939,0.54135613320019083,0.54524115224971692,0.54853612505467175,0.55133066625176541,0.55370078004770074,0.5557109273346772]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.74659692497701402,0.74988359569964202,0.75270422399864001,0.75512489362834589,0.75720231781722702,0.75898516798710791,0.76051521406304101]
[null,null,null,null,"Coincident",0.4741109631214111,0.47619809550789405,0.47798927727506596,0.47952647354676764,0.48084569888784773,0.48197786107987578,0.4829494852513832]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.7560937547467802,0.7594222324355473,0.76227873956809422,0.76473020049445983,0.76683404984425618,0.76863957814741346,0.77018908664897001]
[null,null,null,null,"Coincident",0.48014172879712369,0.48225540983431531,0.48406937571398551,0.48562612536292021,0.48696213145687112,0.48810869492922837,0.48909267831231074]
[null,"Walcha South 66/22kV","Substation Rating","MVA","Non-Coincident",21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998,21.599999999999998]
[null,null,null,null,"Coincident",19.8,19.8,19.8,19.8,19.8,19.8,19.8]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.4352163694784299,1.4756584175268499,1.51193644331219,1.54447918578917,1.5736712397942498,1.5998576012429901,1.6233477443416799]
[null,null,null,null,"Coincident",0.68681626990313227,0.70616962816921258,0.72353031250866984,0.73910349399947195,0.75307321875244826,0.76560458299482725,0.7768456842013276]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.8600404148440453,1.9124533091147975,1.9594696305325983,2.0016450247827642,2.039477926773348,2.0734154512109151,2.1038586766668175]
[null,null,null,null,"Coincident",0.89011388579445949,0.91519583810729943,0.93769528501123611,0.95787812822331553,0.97598289150317308,0.99222353956129605,1.0067920067249208]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.39624307205839,1.43575033021452,1.47129728361113,1.50328092294106,1.5320584435733899,1.5579512347345701,1.5812484688042401]
[null,null,null,null,"Coincident",0.66816577557412415,0.68707179438629395,0.70408262735718075,0.71938825257833994,0.73315960427002957,0.74555048178570704,0.75669926725322911]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.8095310213876736,1.860732427958018,1.9068012795600244,1.9482520761316138,1.9855477428711135,2.0191048002160028,2.0492980155702951]
[null,null,null,null,"Coincident",0.86594284514406494,0.89044504552463699,0.91249108505490628,0.93232717534152865,0.95017484713395828,0.96623342439427629,0.98068225036018486]
[null,"Walgett","Substation Rating","MVA","Non-Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,null,null,"Coincident",28.6,28.6,28.6,28.6,28.6,28.6,28.6]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.7652846685472596,5.7653108123226806,5.76533087532348,5.7653462718756101,5.7653580873472805,5.7653671546611402,5.7653741130106004]
[null,null,null,null,"Coincident",5.1647765192502151,5.1647999399076818,5.1648179131598964,5.1648317060175764,5.1648422907977141,5.164850413666298,5.1648566472387882]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.7652846685472596,5.7653108123226806,5.76533087532348,5.7653462718756101,5.7653580873472805,5.7653671546611402,5.7653741130106004]
[null,null,null,null,"Coincident",5.1647765192502151,5.1647999399076818,5.1648179131598964,5.1648317060175764,5.1648422907977141,5.164850413666298,5.1648566472387882]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.23148599178145,5.23148610072242,5.2314861687623697,5.2314862112572502,5.2314862377977596,5.2314862543738396,5.2314862647265699]
[null,null,null,null,"Coincident",4.6865779513967416,4.6865780489904934,4.686578109943448,4.6865781480120905,4.6865781717881587,4.6865781866376857,4.686578195912082]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.23148599178145,5.23148610072242,5.2314861687623697,5.2314862112572502,5.2314862377977596,5.2314862543738396,5.2314862647265699]
[null,null,null,null,"Coincident",4.6865779513967416,4.6865780489904934,4.686578109943448,4.6865781480120905,4.6865781717881587,4.6865781866376857,4.686578195912082]
[null,"Wallangra","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.18056850253579002,0.180568502828377,0.18056850290839402,0.18056850293027799,0.180568502936263,0.1805685029379,0.180568502938347]
[null,null,null,null,"Coincident",9.5191004054193645E-2,9.5191004208437874E-2,9.5191004250620756E-2,9.5191004262157417E-2,9.5191004265312559E-2,9.519100426617555E-2,9.5191004266411194E-2]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.19332605978016651,0.1933260600934254,0.19332606017909582,0.19332606020252593,0.19332606020893381,0.19332606021068646,0.19332606021116502]
[null,null,null,null,"Coincident",0.10191645542758779,0.1019164555927297,0.10191645563789291,0.10191645565024465,0.10191645565362271,0.10191645565454667,0.10191645565479895]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.15851546927691501,0.15851547254621301,0.15851547369268598,0.15851547409472999,0.15851547423571799,0.158515474285159,0.15851547430249702]
[null,null,null,null,"Coincident",8.3565220216634539E-2,8.3565221940123169E-2,8.3565222544513804E-2,8.3565222756460916E-2,8.3565222830786115E-2,8.3565222856850127E-2,8.3565222865990274E-2]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.16971493178017535,0.16971493528045636,0.16971493650793013,0.16971493693837941,0.16971493708932853,0.16971493714226266,0.16971493716082564]
[null,null,null,null,"Coincident",8.9469284688462006E-2,8.9469286533718842E-2,8.9469287180810986E-2,8.946928740773262E-2,8.9469287487309063E-2,8.946928751521456E-2,8.9469287525000482E-2]
[null,"Warialda","Substation Rating","MVA","Non-Coincident",13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001]
[null,null,null,null,"Coincident",13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001,13.200000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",3.62819442249807,3.8102009933379097,3.9920255576069099,4.1736682973116404,4.3551293942766698,4.5364090301447302,4.7175073863769201]
[null,null,null,null,"Coincident",2.6021797979756185,2.7327168548657945,2.8631233746990805,2.9933994880125323,3.1235453252126737,3.2535610165756119,3.3834466922471855]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.6443436558326305,3.8271603449403035,4.009794217358869,4.1922454559050149,4.3745142432126185,4.556600761732911,4.7385051937346807]
[null,null,null,null,"Coincident",2.6137622006372307,2.7448802830031789,2.8758672472867612,3.0067232246060596,3.1374483459480409,3.268042742168678,3.398506543993093]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",3.2208859592336099,3.32907365833116,3.4289442387981,3.52113709367904,3.6062424615597299,3.6848052054021001,3.7573283008747098]
[null,null,null,null,"Coincident",2.3100538170527107,2.3876471905597665,2.4592754377373911,2.5253971381074893,2.5864356170889811,2.6427816562186575,2.6947959950190423]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",3.2352222468859848,3.3438914936056308,3.4442066018788031,3.5368098107132191,3.6222939858693426,3.7012064155151654,3.7740523140833506]
[null,null,null,null,"Coincident",2.3203359557042802,2.3982747003100324,2.4702217675789515,2.5366377781880862,2.5979479417941249,2.6545447793175532,2.7067906359464269]
[null,"Warrawidgee","Substation Rating","MVA","Non-Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,null,null,"Coincident",6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007,6.0500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.28238958412679,1.28238164192699,1.28237869563448,1.28237760265775,1.28237719719966,1.2823770467881699,1.2823769909905001]
[null,null,null,null,"Coincident",0.61170668932678962,0.61170290085501344,0.61170149545773056,0.61170097410198554,0.6117007806963084,0.61170070894922324,0.61170068233343633]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.5896144684523525,1.5896046235223329,1.5896009713800665,1.5895996165565049,1.5895991139619314,1.5895989275160307,1.589598858350791]
[null,null,null,null,"Coincident",0.75825460206390294,0.75824990597963682,0.75824816388824556,0.75824751763016174,0.75824727788986246,0.75824718895417076,0.75824715596198156]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.1848428128717801,1.18483082047615,1.18482616833291,1.1848243636529001,1.1848236635734399,1.18482339199551,1.1848232866438]
[null,null,null,null,"Coincident",0.56517635779766195,0.56517063736081585,0.56516841826361264,0.5651675574215973,0.56516722347995096,0.5651670939358262,0.56516704368249704]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.4686982033351796,1.468683337895035,1.4686775712276392,1.4686753341964824,1.4686744663974511,1.4686741297570012,1.468673999165951]
[null,null,null,null,"Coincident",0.70057689699196801,0.70056980609752473,0.70056705536633912,0.70056598829051464,0.70056557434573608,0.70056541376644121,0.70056535147381194]
[null,"Wathagar","Substation Rating","MVA","Non-Coincident",6,6,6,6,6,6,6]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.56094025276174,5.70746326482874,5.8480561896263401,5.9829590299672599,6.11240207525739,6.23660629461732,6.3557837140934499]
[null,null,null,null,"Coincident",1.0808588096917184,1.1093379303469946,1.1366644424907533,1.1628849945570168,1.1880443470218589,1.2121854488129438,1.2353495106266141]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",5.8540924351004877,6.0083395979042189,6.1563440611921552,6.2983584798367618,6.4346252832488258,6.5653770892229018,6.6908371010335879]
[null,null,null,null,"Coincident",1.1378376845688272,1.1678181190292707,1.1965851837246724,1.224187986221793,1.2506736466032928,1.2760873779052964,1.300472563299486]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",5.4903346089899294,5.6435094363279203,5.7922072336228005,5.93655885656643,6.0766913361695893,6.2127279905506603,6.3447885334569403]
[null,null,null,null,"Coincident",1.0671354592121272,1.09690746790599,1.1258092932956991,1.1538663693044611,1.1811033864667653,1.2075443136563255,1.2332124191789546]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.7797647231861795,5.9410143603355499,6.0975509549928564,6.2495122610775784,6.3970320062050892,6.5402400093684214,6.6792622951804255]
[null,null,null,null,"Coincident",1.1233908898587222,1.1547323686285997,1.1851577912521325,1.214693932434797,1.243366784304651,1.2712015792856932,1.2982228123026742]
[null,"Wee Waa","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.1384223482775404,8.8695787468573606,8.6010039890386114,8.33269780597767,8.0646599290997898,7.7968900900987999,7.5293880209367998]
[null,null,null,null,"Coincident",8.2482943812580096,8.0056374890156405,7.7632232536655232,7.5210514325507463,7.2791217832570849,7.0374340636127286,6.7959880316880055]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.8880629467649488,9.5971656395094147,9.3065592295611488,9.0162434260228181,8.7262179382880269,8.4364824760409842,8.1470367492561753]
[null,null,null,null,"Coincident",8.9249162423204975,8.6623537853104899,8.4000538907575049,8.1380162960990603,7.8762407390352758,7.6147269575285677,7.3534746898033543]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.1394014245191606,7.9396079296650397,7.74001422830578,7.54062012064787,7.3414254070976304,7.1424298882609296,6.9436333649430697]
[null,null,null,null,"Coincident",7.3465830838207014,7.1662504729813952,6.9860981947529357,6.8061260688026959,6.6263339149784173,6.4467215533079525,6.2672888039991621]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.8070906079104141,8.5909077069478563,8.3749409888862676,8.1591902375427328,7.9436552369505531,7.728335771358954,7.513231625232951]
[null,null,null,null,"Coincident",7.9492360068201364,7.7541103998635243,7.5591799185138751,7.364444367645568,7.1699035523281403,6.9755572778260193,6.7814053495984048]
[null,"Wellington 11kV","Substation Rating","MVA","Non-Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,null,null,"Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",10.2523681906404,10.3606820745634,10.461509041944201,10.555366606487299,10.6427365101032,10.7240671955416,10.799776108108999]
[null,null,null,null,"Coincident",9.2615143136791165,9.3593600569912656,9.4504424668538611,9.5352290411652021,9.6141549632426155,9.6876253354846824,9.7560172586362697]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",10.792076190920048,10.906091964260945,11.012226692729476,11.111025133129619,11.202994387362699,11.2886065052256,11.368300907296039]
[null,null,null,null,"Coincident",9.7490615102732008,9.8520580762515788,9.9479352715114135,10.037185204104592,10.120265966388926,10.197603986275443,10.26959621595066]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",9.227906716043961,9.3241377537667702,9.41338443997574,9.4961536918487592,9.5729156350270213,9.6441062739075303,9.7101299681285713]
[null,null,null,null,"Coincident",8.3360632925726392,8.42299395256431,8.5036152730634509,8.5783851795572783,8.6477283617637379,8.7120386858500041,8.7716814315746809]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",9.7136847321934301,9.8149815908044928,9.9089264257386915,9.9960528394481152,10.076855706057916,10.151793982229085,10.221293314011763]
[null,null,null,null,"Coincident",8.7748926406979066,8.8663995285224733,8.9512649388608967,9.0299709034404767,9.1029644686126847,9.1706602345563351,9.233442710188065]
[null,"Wenna","Substation Rating","MVA","Non-Coincident",9,9,9,9,9,9,9]
[null,null,null,null,"Coincident",8.25,8.25,8.25,8.25,8.25,8.25,8.25]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.1660596282520901,2.2476651993299703,2.3175223202986901,2.3773223717606302,2.4285132325527901,2.4723343357889598,2.5098466780141]
[null,null,null,null,"Coincident",0.14160905956744846,0.14694413346157223,0.15151113663888208,0.15542064537961969,0.15876731670882754,0.16163218023222445,0.1640846000250078]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.2098466400920245,2.2931018721766403,2.3643711586015019,2.4253800713188016,2.477605758114072,2.5223127073081342,2.5605833635481479]
[null,null,null,null,"Coincident",0.14447169431999471,0.14991461701972011,0.15457394241179709,0.15856248208191734,0.16197680655197372,0.16489958344552103,0.16740157903626599]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0949642081829603,2.17565870904708,2.2447941976981403,2.30402643458959,2.35477400223713,2.3982522795620298,2.4355025496098603]
[null,null,null,null,"Coincident",0.13696110092206878,0.14223661237641125,0.14675643787101819,0.15062882497101834,0.15394651541507257,0.15678896623373267,0.15922425270567686]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1373140222838627,2.2196397668213645,2.290172833092468,2.3506024528372071,2.4023758852931061,2.4467330783316705,2.4847363645912206]
[null,null,null,null,"Coincident",0.13972977694070843,0.14511193314273005,0.14972312715271188,0.15367379476613138,0.15705855250088263,0.15995846361566188,0.1624429795345658]
[null,"Werris Creek","Substation Rating","MVA","Non-Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,null,null,"Coincident",15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001,15.675000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.6990803078344703,2.7182215730878303,2.7355953181081398,2.7513647571726403,2.7656780332175397,2.7786696095379897,2.79046153297752]
[null,null,null,null,"Coincident",1.9590265484779443,1.9729195203520846,1.9855296037358505,1.9969752616113465,2.0073640179911627,2.0167934680317798,2.0253521948724025]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.8404852799848799,2.8606293572228325,2.8789133137413381,2.8955089146229844,2.9105720640209056,2.9242442697699986,2.9366539727549266]
[null,null,null,null,"Coincident",2.061660061725163,2.0762808871927096,2.0895516135682826,2.1015969101164145,2.112529934038883,2.1224533935080143,2.1314605125387573]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.4043544593522204,2.4238774204110802,2.44184123493898,2.4583704198008198,2.47357954767135,2.4875740411999301,2.50045090375174]
[null,null,null,null,"Coincident",1.7451108083558371,1.7592808198624206,1.7723191831411793,1.7843162741039984,1.795355251044062,1.8055126310506566,1.8148588203903642]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.5303187273947647,2.5508644975033619,2.5697694373048074,2.587164587109696,2.6031705220617796,2.6178981879090655,2.6314496700285992]
[null,null,null,null,"Coincident",1.8365372637075577,1.8514496429297822,1.8651710868086135,1.8777967060551444,1.8894140156303088,1.9001035413580902,1.9099393780934153]
[null,"West Jemalong","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2230842014974899,2.2230841890344499,2.2230841848834202,2.2230841835008501,2.22308418304037,2.2230841828869901,2.22308418283591]
[null,null,null,null,"Coincident",1.6459701768383872,1.6459701676107601,1.6459701645373404,1.6459701635136863,1.645970163172747,1.6459701630591845,1.645970163021365]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.3300836459116039,2.3300836328487042,2.330083628497881,2.3300836270487664,2.3300836265661231,2.3300836264053606,2.3300836263518221]
[null,null,null,null,"Coincident",1.7251924997379309,1.7251924900661681,1.7251924868448212,1.7251924857718977,1.7251924854145488,1.7251924852955205,1.7251924852558804]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0306735404996701,2.03067353087209,2.0306735277448498,2.0306735267290499,2.0306735263991,2.0306735262919302,2.0306735262571101]
[null,null,null,null,"Coincident",1.5035094416602779,1.5035094345320237,1.5035094322166169,1.5035094314645192,1.5035094312202246,1.5035094311408761,1.5035094311150952]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1284120519215697,2.1284120418306034,2.1284120385528458,2.1284120374881543,2.1284120371423239,2.1284120370299959,2.1284120369934998]
[null,null,null,null,"Coincident",1.5758749754626675,1.5758749679913222,1.5758749655644726,1.5758749647761756,1.5758749645201229,1.5758749644369554,1.5758749644099337]
[null,"West Wyalong","Substation Rating","MVA","Non-Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,null,null,"Coincident",27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004,27.500000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",8.7274061837426711,8.5327686619964602,8.338325777771999,8.1440773364317707,7.9500231435328699,7.7561630048268695,7.5624967262595799]
[null,null,null,null,"Coincident",7.9227153160425363,7.746023909437926,7.5695091942399229,7.3931709937571259,7.2170091314747999,7.0410234310547581,6.8652137163351403]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.0291652591302221,8.8277979442059102,8.6266319965965277,8.4256672149347622,8.2249033980546464,8.0243403449914119,7.8239778549812442]
[null,null,null,null,"Coincident",8.1966513742474643,8.0138506799159615,7.8312327862787958,7.6487975105352737,7.466544670067484,7.2844740824401635,7.1025855654004735]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.9580244312950397,7.7915619942090899,7.62526601956022,7.4591363408859994,7.2931727918904494,7.1273752064439,6.9617434185827998]
[null,null,null,null,"Coincident",7.2242726784859954,7.073158536198985,6.9221955080542568,6.7713834429376734,6.6207221898862025,6.470211598087789,6.3198515168811751]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.2331813385984312,8.0609632909628797,7.8889174613749562,7.7170436776166218,7.545341767642042,7.3738115595774421,7.2024528817209088]
[null,null,null,null,"Coincident",7.4740593617124889,7.3177202920078175,7.1615375613728443,7.0055110134685066,6.8496404921120693,6.693925841276994,6.5383669050927553]
[null,"Whitbread St","Substation Rating","MVA","Non-Coincident",64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006]
[null,null,null,null,"Coincident",64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006,64.900000000000006]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",24.453896955721,24.528209452432399,24.5587213531076,24.5712492067528,24.576393006826997,24.578504995037601,24.5793721543629]
[null,null,null,null,"Coincident",19.904080258840391,19.964566401456299,19.98940135193428,19.999598311743039,20.003785072229423,20.005504110423036,20.006209928756991]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",25.876398568502339,25.955033879144505,25.987320680073768,26.000577288405683,26.006020307206231,26.008255151362505,26.009172753999191]
[null,null,null,null,"Coincident",21.061915605918095,21.125920273028395,21.152199891289687,21.162990015934287,21.167420323433031,21.169239359373726,21.169986235692022]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",20.938854097419199,20.994813432196597,21.024041495623603,21.039307575806401,21.047281186672897,21.051445875282401,21.0536211295688]
[null,null,null,null,"Coincident",17.043035440847291,17.088583154271351,17.112373134302551,17.124798854658962,17.131288920063543,17.134678739546576,17.136449272724921]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",22.156883018425329,22.216097549874046,22.24702583177497,22.263179951345524,22.271617393164522,22.276024344848679,22.278326135316046]
[null,null,null,null,"Coincident",18.034441654964954,18.082638913200686,18.107812774296882,18.12096130816964,18.127828905569299,18.131415913406009,18.133289439833494]
[null,"Whitton","Substation Rating","MVA","Non-Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,null,null,"Coincident",13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002,13.750000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",5.43416026642684,5.4341602638879802,5.43416026388544,5.43416026388544,5.43416026388544,5.43416026388544,5.43416026388544]
[null,null,null,null,"Coincident",3.1773505382932887,3.1773505368088188,3.1773505368073338,3.1773505368073338,3.1773505368073338,3.1773505368073338,3.1773505368073338]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.1005130335231144,6.100513030672932,6.100513030670081,6.100513030670081,6.100513030670081,6.100513030670081,6.100513030670081]
[null,null,null,null,"Coincident",3.5669666370872855,3.5669666354207852,3.5669666354191181,3.5669666354191181,3.5669666354191181,3.5669666354191181,3.5669666354191181]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.8778832156457499,4.87788321564536,4.87788321564536,4.87788321564536,4.87788321564536,4.87788321564536,4.87788321564536]
[null,null,null,null,"Coincident",2.8520956506781161,2.8520956506778878,2.8520956506778878,2.8520956506778878,2.8520956506778878,2.8520956506778878,2.8520956506778878]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",5.4760236493019825,5.4760236493015446,5.4760236493015446,5.4760236493015446,5.4760236493015446,5.4760236493015446,5.4760236493015446]
[null,null,null,null,"Coincident",3.201828035384219,3.2018280353839632,3.2018280353839632,3.2018280353839632,3.2018280353839632,3.2018280353839632,3.2018280353839632]
[null,"Widgelli","Substation Rating","MVA","Non-Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,null,null,"Coincident",1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.1000000000000001]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",0.63351765066176491,0.63351764097844399,0.63351763917650994,0.63351763884119494,0.63351763877879796,0.63351763876718603,0.63351763876502498]
[null,null,null,null,"Coincident",0.32478585209365335,0.32478584712929975,0.32478584620550122,0.32478584603359506,0.32478584600160598,0.32478584599565291,0.32478584599454496]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",0.76688978764318905,0.76688977592127427,0.76688977373998568,0.76688977333407804,0.7668897732585449,0.76688977324448837,0.76688977324187235]
[null,null,null,null,"Coincident",0.39316182095547508,0.39316181494599445,0.39316181382771198,0.39316181361961505,0.39316181358089147,0.39316181357368507,0.39316181357234392]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",0.56103887928895702,0.56103887928895402,0.56103887928895402,0.56103887928895402,0.56103887928895402,0.56103887928895402,0.56103887928895402]
[null,null,null,null,"Coincident",0.28762811940155109,0.28762811940154953,0.28762811940154953,0.28762811940154953,0.28762811940154953,0.28762811940154953,0.28762811940154953]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",0.6791523275603164,0.67915232756031274,0.67915232756031274,0.67915232756031274,0.67915232756031274,0.67915232756031274,0.67915232756031274]
[null,null,null,null,"Coincident",0.34818140769661449,0.3481814076966126,0.3481814076966126,0.3481814076966126,0.3481814076966126,0.3481814076966126,0.3481814076966126]
[null,"Wilcannia","Substation Rating","MVA","Non-Coincident",7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011]
[null,null,null,null,"Coincident",7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011,7.7000000000000011]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3744685258287701,1.37446594408196,1.37446514387911,1.3744648958591899,1.3744648189863402,1.3744647951598798,1.3744647877749601]
[null,null,null,null,"Coincident",0.69498866926602831,0.69498736382705595,0.69498695921108733,0.6949868338018611,0.69498679493173898,0.69498678288408589,0.69498677914996221]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4869074179275976,1.4869046249800613,1.4869037593163292,1.4869034910070504,1.4869034078455896,1.4869033820699971,1.4869033740809512]
[null,null,null,null,"Coincident",0.75184246731599957,0.75184105508512267,0.75184061736939922,0.75184048170102624,0.75184043965111969,0.75184042661790396,0.75184042257830885]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2742149835191001,1.2742091228475598,1.2742070740189599,1.2742063577702099,1.2742061073772399,1.27420601984252,1.27420598924131]
[null,null,null,null,"Coincident",0.64429629279491873,0.64429332939471118,0.64429229342143457,0.64429193125616391,0.64429180464702474,0.64429176038581581,0.64429174491256647]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.3784525985319462,1.3784462584260628,1.3784440419923023,1.3784432671505658,1.3784429962741087,1.3784429015785795,1.3784428684740266]
[null,null,null,null,"Coincident",0.69700318275557505,0.6969999769333477,0.6969988562119046,0.6969984644195738,0.69699832745312829,0.69699827957111526,0.69699826283207134]
[null,"Willbriggie","Substation Rating","MVA","Non-Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,null,null,"Coincident",8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007,8.8000000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",1.3678211365392301,1.38496080514025,1.4004792523112801,1.4145298275123401,1.4272513750554001,1.4387696061295501,1.4491983410478599]
[null,null,null,null,"Coincident",0.77702515268191008,0.78676177193413266,0.7955774156322295,0.80355919778870022,0.81078599240236338,0.81732921287171623,0.82325351768446497]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",1.4159838526145549,1.4337270306733574,1.4497919020405505,1.4643372158050281,1.4775067051629847,1.4894305077538299,1.5002264516481367]
[null,null,null,null,"Coincident",0.80438519326930114,0.81446465122758793,0.82359070491505448,0.83185353573900656,0.83933479495174246,0.8461084105080442,0.85224131760293209]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",1.2293846865236,1.23815491908681,1.2456500246356399,1.2520553972165001,1.2575294759512501,1.26220766408411,1.26620567822801]
[null,null,null,null,"Coincident",0.69838285009087131,0.7033650009835869,0.70762278394794564,0.71126151672862203,0.71437120464836268,0.71702876692102024,0.71929993927506675]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",1.2726728797110507,1.2817519232800074,1.2895109409960497,1.2961418548649684,1.3018086828509419,1.3066515959180576,1.3107903852078695]
[null,null,null,null,"Coincident",0.72297379551660623,0.72813137425765673,0.73253907915738037,0.73630593633174257,0.73952512030499518,0.74227625871401393,0.74462740192559718]
[null,"Wingham","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",13.5892104092114,13.5892106274745,13.5892106306102,13.5892106306553,13.5892106306559,13.5892106306559,13.5892106306559]
[null,null,null,null,"Coincident",11.328610791846888,11.328610973801368,11.328610976415437,11.328610976453033,11.328610976453534,11.328610976453534,11.328610976453534]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",14.592560288642645,14.592560523021048,14.592560526388271,14.592560526436699,14.592560526437344,14.592560526437344,14.592560526437344]
[null,null,null,null,"Coincident",12.165050874077,12.165051069465962,12.165051072273037,12.16505107231341,12.165051072313949,12.165051072313949,12.165051072313949]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.308136027417101,11.308158593932399,11.308162116981999,11.308162666995001,11.308162752862199,11.308162766267699,11.3081627683605]
[null,null,null,null,"Coincident",9.4269989188653742,9.4270177313836196,9.4270206683649818,9.4270211268819271,9.4270211984648977,9.4270212096403601,9.4270212113850178]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",12.143064369685625,12.143088602383852,12.143092385555363,12.143092976178194,12.143093068385335,12.143093082780622,12.143093085027942]
[null,null,null,null,"Coincident",10.123034813800858,10.123055015328275,10.123058169159609,10.123058661530834,10.123058738399084,10.123058750399679,10.123058752273151]
[null,"Woodburn","Substation Rating","MVA","Non-Coincident",24,24,24,24,24,24,24]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",6.7130716142421694,6.71307161432604,6.71307161432612,6.71307161432612,6.71307161432612,6.71307161432612,6.71307161432612]
[null,null,null,null,"Coincident",5.1584655562071413,5.1584655562715893,5.1584655562716506,5.1584655562716506,5.1584655562716506,5.1584655562716506,5.1584655562716506]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",6.9240819062103078,6.9240819062968146,6.9240819062968972,6.9240819062968972,6.9240819062968972,6.9240819062968972,6.9240819062968972]
[null,null,null,null,"Coincident",5.3206103068773949,5.3206103069438688,5.3206103069439319,5.3206103069439319,5.3206103069439319,5.3206103069439319,5.3206103069439319]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",6.3591528072921699,6.3591528073586696,6.35915280735873,6.35915280735873,6.35915280735873,6.35915280735873,6.35915280735873]
[null,null,null,null,"Coincident",4.8865068940245102,4.8865068940756098,4.886506894075656,4.886506894075656,4.886506894075656,4.886506894075656,4.886506894075656]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",6.5590384583985761,6.5590384584671657,6.5590384584672279,6.5590384584672279,6.5590384584672279,6.5590384584672279,6.5590384584672279]
[null,null,null,null,"Coincident",5.0401032364536427,5.0401032365063489,5.0401032365063969,5.0401032365063969,5.0401032365063969,5.0401032365063969,5.0401032365063969]
[null,"Woodlawn","Substation Rating","MVA","Non-Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,null,null,"Coincident",15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002,15.400000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",4.8650000000000002,4.8650000000000002,4.8650000000000002,4.8650000000000002,4.8650000000000002,4.8650000000000002,4.8650000000000002]
[null,null,null,null,"Coincident",3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001,3.3620000000000001]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",4.4692759982279906,4.6561978062955101,4.6561978062955101,4.6561978062955101,4.6561978062955101,4.6561978062955101,4.6561978062955101]
[null,null,null,null,"Coincident",2.2887944646983982,2.3845203943133919,2.3845203943133919,2.3845203943133919,2.3845203943133919,2.3845203943133919,2.3845203943133919]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",4.4703700682397978,4.6573376343998669,4.6573376343998669,4.6573376343998669,4.6573376343998669,4.6573376343998669,4.6573376343998669]
[null,null,null,null,"Coincident",2.2893547571010173,2.3851041202361127,2.3851041202361127,2.3851041202361127,2.3851041202361127,2.3851041202361127,2.3851041202361127]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",4.4344741012338202,4.4344741012338096,4.4344741012338096,4.4344741012338096,4.4344741012338096,4.4344741012338096,4.4344741012338096]
[null,null,null,null,"Coincident",2.2709718041079929,2.2709718041079876,2.2709718041079876,2.2709718041079876,2.2709718041079876,2.2709718041079876,2.2709718041079876]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",4.435559651809398,4.4355596518093874,4.4355596518093874,4.4355596518093874,4.4355596518093874,4.4355596518093874,4.4355596518093874]
[null,null,null,null,"Coincident",2.2715277335582034,2.2715277335581976,2.2715277335581976,2.2715277335581976,2.2715277335581976,2.2715277335581976,2.2715277335581976]
[null,"Woolgoolga","Substation Rating","MVA","Non-Coincident",72,72,72,72,72,72,72]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Winter","Winter","Winter","Winter","Winter","Winter","Winter"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.398229829465699,11.398230529381101,11.398230799667799,11.398230904044599,11.3982309443518,11.398230959917301,11.3982309659282]
[null,null,null,null,"Coincident",8.3619149066059144,8.3619154200745065,8.3619156183609427,8.3619156949333533,8.3619157245033282,8.3619157359224179,8.3619157403321047]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",11.398229829465699,11.398230529381101,11.398230799667799,11.398230904044599,11.3982309443518,11.398230959917301,11.3982309659282]
[null,null,null,null,"Coincident",8.3619149066059144,8.3619154200745065,8.3619156183609427,8.3619156949333533,8.3619157245033282,8.3619157359224179,8.3619157403321047]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.8361643549782,10.8361648980183,10.836165105833699,10.836165185362301,10.836165215797001,10.8361652274441,10.8361652319012]
[null,null,null,null,"Coincident",7.9495751187683616,7.949575517150846,7.9495756696073858,7.949575727950779,7.9495757502781377,7.9495757588226272,7.9495757620924232]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",10.8361643549782,10.8361648980183,10.836165105833699,10.836165185362301,10.836165215797001,10.8361652274441,10.8361652319012]
[null,null,null,null,"Coincident",7.9495751187683616,7.949575517150846,7.9495756696073858,7.949575727950779,7.9495757502781377,7.9495757588226272,7.9495757620924232]
[null,"Yallaroi","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.2879016507640397,2.2879016507812899,2.2879016507833501,2.2879016507835899,2.2879016507836201,2.2879016507836298,2.2879016507836298]
[null,null,null,null,"Coincident",1.8457187605387206,1.8457187605526368,1.8457187605542988,1.8457187605544922,1.8457187605545167,1.8457187605545244,1.8457187605545244]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",2.4083175271200417,2.4083175271381996,2.4083175271403685,2.4083175271406208,2.4083175271406527,2.4083175271406629,2.4083175271406629]
[null,null,null,null,"Coincident",1.942861853198653,1.9428618532133017,1.9428618532150514,1.9428618532152548,1.9428618532152806,1.9428618532152888,1.9428618532152888]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.0411262635555598,2.04112626444905,2.0411262646623398,2.0411262647132502,2.0411262647254098,2.0411262647283097,2.0411262647289998]
[null,null,null,null,"Coincident",1.6466376673204906,1.6466376680412957,1.646637668213363,1.6466376682544339,1.6466376682642434,1.6466376682665829,1.6466376682671395]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.1485539616374312,2.1485539625779473,2.1485539628024628,2.1485539628560528,2.1485539628688524,2.148553962871905,2.1485539628726311]
[null,null,null,null,"Coincident",1.7333028077057793,1.7333028084645217,1.7333028086456452,1.7333028086888778,1.7333028086992035,1.7333028087016662,1.733302808702252]
[null,"Yamba","Substation Rating","MVA","Non-Coincident",58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004]
[null,null,null,null,"Coincident",58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004,58.300000000000004]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",11.807243324085801,12.178979362344801,12.550343664565499,12.921336602484001,13.291958547464599,13.662209870500201,14.0320909422128]
[null,null,null,null,"Coincident",9.6560707280940594,9.9600798332751204,10.263784929350965,10.567186320330753,10.870284309919576,11.173079201518794,11.475571298226443]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",12.303991594784485,12.691367120525278,13.078355270740287,13.464956432805106,13.851170993707877,14.236999340049726,14.622441858045271]
[null,null,null,null,"Coincident",10.062315971311852,10.379115191266552,10.695597612001261,11.011763550315257,11.327613322690951,11.643147245294255,11.958365633974987]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",10.7867689940507,11.1025208494666,11.417956953027,11.733077620484,12.047883167273399,12.3623739085161,12.6765501590175]
[null,null,null,null,"Coincident",8.8215175613169787,9.0797422937744958,9.3377088014994865,9.5954173427168836,9.8528681753929455,10.110061557236405,10.366997745697976]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.240584393390387,11.569620398530533,11.89832736766545,12.2267056298314,12.554755513735033,12.882477347754858,13.209871459940603]
[null,null,null,null,"Coincident",9.1926519127691257,9.4617405434100768,9.7305600854203149,9.9991108078886803,10.267392979634455,10.535406869208559,10.803152744893042]
[null,"Yanco 33/11kV","Substation Rating","MVA","Non-Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,null,null,"Coincident",5.5,5.5,5.5,5.5,5.5,5.5,5.5]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",2.9435021284846798,3.0257888146385099,3.1003808093438101,3.1679976491289699,3.22929158610699,3.28485387979305,3.3352205005693101]
[null,null,null,null,"Coincident",2.1068538324106107,2.1657517072930101,2.2191419964968833,2.267539718604255,2.3114117324125671,2.3511812403932741,2.387231871028511]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",3.1497347616906133,3.2377867570654124,3.3176049424825491,3.3899592678577517,3.4555476844966524,3.5150028777403346,3.5688983700359502]
[null,null,null,null,"Coincident",2.2544677951909726,2.3174922727721383,2.3746232828756462,2.4264119281879926,2.4733577773586708,2.5159136839877076,2.5544901549859231]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",2.6612295877046699,2.7261390028903301,2.7851346019365399,2.83875518528128,2.88749046392432,2.93178553190493,2.9720449312976598]
[null,null,null,null,"Coincident",1.9048132160402056,1.9512730601898143,1.9935000056854695,2.0318797066623175,2.0667626807865953,2.0984675104956465,2.1272837525769077]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",2.8476851639132779,2.9171423725195895,2.9802714211805017,3.0376488606831535,3.089798712989082,3.1371972570702442,3.18027737871342]
[null,null,null,null,"Coincident",2.0382714668455706,2.0879864593113941,2.1331719806061078,2.1742407052182764,2.2115677093767396,2.2454938965813294,2.2763291110377106]
[null,"Yarrandale","Substation Rating","MVA","Non-Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,null,null,"Coincident",60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007,60.500000000000007]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",9.3374458112356802,9.2496446196366708,9.1619312292292605,9.07430555221225,8.9867675008722596,8.8993169875836191,8.811953924808261]
[null,null,null,null,"Coincident",7.1116593097201974,7.0447874719325796,6.9779825059827498,6.9112443449988641,6.8445729221759644,6.7779681707758952,6.7114300241272211]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",9.356748024798959,9.2687653320286856,9.1808706219511809,9.0930638065837481,9.0053447980316861,8.9177135084881858,8.8301698502342205]
[null,null,null,null,"Coincident",7.1263604142364159,7.0593503400916147,6.9924072760209564,6.9255311550143652,6.8587219101287831,6.7919794744880946,6.7253037812830394]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",8.3332879478097492,8.2272955149412095,8.1219689992271498,8.0173042169193103,7.9132970105545999,7.8099432487899803,7.7072388262383198]
[null,null,null,null,"Coincident",6.3468646579248666,6.2661378631238271,6.1859182494113751,6.1062026303280783,6.0269878394340264,5.948270730183066,5.8700481757977894]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",8.350514382843981,8.2443028441710631,8.138758599225552,8.0338774556106163,7.9296552472689248,7.8260878343171951,7.7231711028817065]
[null,null,null,null,"Coincident",6.359984791584659,6.2790911196884256,6.1987056773171352,6.1188252714243641,6.0394467290245872,5.9605668970671655,5.8821826423110668]
[null,"Yass","Substation Rating","MVA","Non-Coincident",22,22,22,22,22,22,22]
[null,null,null,null,"Coincident",22,22,22,22,22,22,22]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",12.5789212719846,12.7040159981165,12.821512906584299,12.9318734623517,13.0355311026089,13.1328929390819,13.224341356949301]
[null,null,null,null,"Coincident",11.380928769890829,11.494109712581597,11.600416439290559,11.700266465937254,11.794051949979483,11.882141230597911,11.964880275335084]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",13.197676079923658,13.328924192468296,13.45220075210494,13.567989923173398,13.676746463558992,13.778897510738128,13.874844259345535]
[null,null,null,null,"Coincident",11.940754548502358,12.059502840804651,12.171038775713994,12.275800406680695,12.37419918131528,12.466621557334499,12.553430520360248]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",11.273119062398701,11.373600241442,11.4678713547033,11.556316204576101,11.6392948732097,11.7171451884977,11.7901840994642]
[null,null,null,null,"Coincident",10.199488675503588,10.290400218447525,10.375693130445844,10.455714661283141,10.530790599570683,10.601226599116968,10.667309423324754]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",11.827641701463453,11.933065531096267,12.031973822961275,12.124769258620644,12.21182963259791,12.293509390478201,12.370141071949419]
[null,null,null,null,"Coincident",10.70119963465741,10.796583099563291,10.886071554107822,10.970029329228202,11.048798239017158,11.122698972337421,11.192032398430428]
[null,"Yenda","Substation Rating","MVA","Non-Coincident",20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002]
[null,null,null,null,"Coincident",20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002,20.900000000000002]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",7.6787580873172505,7.4874960887721596,7.31021826920158,7.14590217112268,6.9936000943412999,6.8524336300501201,6.7215885945679199]
[null,null,null,null,"Coincident",5.192932171738418,5.0635869606793227,4.9436988639173975,4.8325764216753662,4.7295787304670842,4.6341117466589843,4.5456248602977603]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",7.7426101258927922,7.5497577049942084,7.3710057472823962,7.2053232931191129,7.0517547617924539,6.9094144401637987,6.7774813742790228]
[null,null,null,null,"Coincident",5.2361135432023369,5.1056927733989506,4.9848077576962098,4.8727612865437786,4.7689071270788537,4.6726462959501989,4.5834236046557919]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",7.0053880970118394,6.7562336088242203,6.5113214721139601,6.2705794523963894,6.0339365451228399,5.8013229547385103,5.5726700740969601]
[null,null,null,null,"Coincident",4.7375506313411959,4.5690543272865725,4.4034270084532681,4.2406198246528701,4.0805847574687357,3.9232746060934125,3.76864297340722]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",7.0636407865640534,6.8124144761090673,6.5654657940326144,6.3227219051905106,6.0841112146019976,5.8495633463334693,5.6190091227417813]
[null,null,null,null,"Coincident",4.7769453175946435,4.6070478973199238,4.4400433190611954,4.275882326420593,4.1145165016885477,3.9558982515634371,3.7999807931144058]
[null,"Young","Substation Rating","MVA","Non-Coincident",66,66,66,66,66,66,66]
[null,null,null,null,"Coincident",66,66,66,66,66,66,66]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,null,null,"Coincident","Summer","Summer","Summer","Summer","Summer","Summer","Summer"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident",0,0,0,0,0,0,0]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident",17.601004468621902,17.468801033128997,17.3871827267299,17.336794112284302,17.305685742388199,17.286480398319199,17.274623613728998]
[null,null,null,null,"Coincident",17.297427510814479,17.167504281364938,17.087293703553275,17.037774177136647,17.007202355271779,16.988328259339013,16.976675977088536]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident",17.631146861595688,17.498717022665854,17.416958941797084,17.366484034923076,17.335322390754367,17.316084156799501,17.304207067012449]
[null,null,null,null,"Coincident",17.327050016643398,17.196904288696938,17.116556347204622,17.066952016706054,17.036327839427596,17.017421420884062,17.005749183654803]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident",16.257257614744699,16.134937110097301,16.054581748209401,16.001794325506001,15.967116963221601,15.944336547103299,15.9293715288799]
[null,null,null,null,"Coincident",15.97685720817846,15.856646451684613,15.777677035487992,15.725800074754154,15.691720817433925,15.669333311245005,15.654626405262521]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident",16.285098789864751,16.162568806677285,16.082075833160463,16.029198009977815,15.994461261384917,15.971641832933201,15.956651186544036]
[null,null,null,null,"Coincident",16.004218186883598,15.883801564874044,15.804696910533476,15.752731108521317,15.718593489170205,15.696167643521143,15.681435551399973]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,"<Enter substation name>","Substation Rating","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Raw Adjusted MD","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Date MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Half hour time period MD occurred",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Winter/Summer Peaking",null,"Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Adjustments - Embedded generation","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected 10% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 10% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MW","Non-Coincident"]
[null,null,null,null,"Coincident"]
[null,null,"Weather Corrected MD 50% POE","MVA","Non-Coincident"]
[null,null,null,null,"Coincident"]

{"sheet":"5.4.2 Expected Unserved Energy","index":30,"n_rows":722,"n_cols":13,"rows_kept":722,"cut":false,"hidden":false,"merged":[[16,2,16,3],[18,2,18,3],[20,2,20,3],[22,2,22,3],[24,2,24,3],[26,2,26,3],[8,5,8,6],[8,7,8,11],[9,2,9,3],[10,2,10,3],[12,2,12,3],[14,2,14,3],[40,7,40,11],[41,2,41,3],[42,2,42,3],[44,2,44,3],[46,2,46,3],[48,2,48,3],[28,2,28,3],[30,2,30,3],[32,2,32,3],[34,2,34,3],[36,2,36,3],[40,5,40,6],[62,2,62,3],[64,2,64,3],[66,2,66,3],[68,2,68,3],[70,2,70,3],[72,2,72,3],[50,2,50,3],[52,2,52,3],[54,2,54,3],[56,2,56,3],[58,2,58,3],[60,2,60,3],[86,2,86,3],[88,2,88,3],[90,2,90,3],[92,2,92,3],[94,2,94,3],[96,2,96,3],[74,2,74,3],[76,2,76,3],[78,2,78,3],[80,2,80,3],[82,2,82,3],[84,2,84,3],[110,2,110,3],[112,2,112,3],[114,2,114,3],[116,2,116,3],[118,2,118,3],[120,2,120,3],[98,2,98,3],[100,2,100,3],[102,2,102,3],[104,2,104,3],[106,2,106,3],[108,2,108,3],[134,2,134,3],[136,2,136,3],[138,2,138,3],[140,2,140,3],[142,2,142,3],[144,2,144,3],[122,2,122,3],[124,2,124,3],[126,2,126,3],[128,2,128,3],[130,2,130,3],[132,2,132,3],[158,2,158,3],[160,2,160,3],[162,2,162,3],[164,2,164,3],[166,2,166,3],[168,2,168,3],[146,2,146,3],[148,2,148,3],[150,2,150,3],[152,2,152,3],[154,2,154,3],[156,2,156,3],[182,2,182,3],[184,2,184,3],[186,2,186,3],[188,2,188,3],[190,2,190,3],[192,2,192,3],[170,2,170,3],[172,2,172,3],[174,2,174,3],[176,2,176,3],[178,2,178,3],[180,2,180,3],[206,2,206,3],[208,2,208,3],[210,2,210,3],[212,2,212,3],[214,2,214,3],[216,2,216,3],[194,2,194,3],[196,2,196,3],[198,2,198,3],[200,2,200,3],[202,2,202,3],[204,2,204,3],[230,2,230,3],[232,2,232,3],[234,2,234,3],[236,2,236,3],[238,2,238,3],[240,2,240,3],[218,2,218,3],[220,2,220,3],[222,2,222,3],[224,2,224,3],[226,2,226,3],[228,2,228,3],[254,2,254,3],[256,2,256,3],[258,2,258,3],[260,2,260,3],[262,2,262,3],[264,2,264,3],[242,2,242,3],[244,2,244,3],[246,2,246,3],[248,2,248,3],[250,2,250,3],[252,2,252,3],[278,2,278,3],[280,2,280,3],[282,2,282,3],[284,2,284,3],[286,2,286,3],[288,2,288,3],[266,2,266,3],[268,2,268,3],[270,2,270,3],[272,2,272,3],[274,2,274,3],[276,2,276,3],[302,2,302,3],[304,2,304,3],[306,2,306,3],[308,2,308,3],[310,2,310,3],[312,2,312,3],[290,2,290,3],[292,2,292,3],[294,2,294,3],[296,2,296,3],[298,2,298,3],[300,2,300,3],[326,2,326,3],[328,2,328,3],[330,2,330,3],[332,2,332,3],[334,2,334,3],[336,2,336,3],[314,2,314,3],[316,2,316,3],[318,2,318,3],[320,2,320,3],[322,2,322,3],[324,2,324,3],[350,2,350,3],[352,2,352,3],[354,2,354,3],[356,2,356,3],[358,2,358,3],[360,2,360,3],[338,2,338,3],[340,2,340,3],[342,2,342,3],[344,2,344,3],[346,2,346,3],[348,2,348,3],[374,2,374,3],[376,2,376,3],[378,2,378,3],[380,2,380,3],[382,2,382,3],[384,2,384,3],[362,2,362,3],[364,2,364,3],[366,2,366,3],[368,2,368,3],[370,2,370,3],[372,2,372,3],[398,2,398,3],[400,2,400,3],[402,2,402,3],[404,2,404,3],[406,2,406,3],[408,2,408,3],[386,2,386,3],[388,2,388,3],[390,2,390,3],[392,2,392,3],[394,2,394,3],[396,2,396,3],[422,2,422,3],[424,2,424,3],[426,2,426,3],[428,2,428,3],[430,2,430,3],[432,2,432,3],[410,2,410,3],[412,2,412,3],[414,2,414,3],[416,2,416,3],[418,2,418,3],[420,2,420,3],[446,2,446,3],[448,2,448,3],[450,2,450,3],[452,2,452,3],[454,2,454,3],[456,2,456,3],[434,2,434,3],[436,2,436,3],[438,2,438,3],[440,2,440,3],[442,2,442,3],[444,2,444,3],[470,2,470,3],[472,2,472,3],[474,2,474,3],[476,2,476,3],[478,2,478,3],[480,2,480,3],[458,2,458,3],[460,2,460,3],[462,2,462,3],[464,2,464,3],[466,2,466,3],[468,2,468,3],[494,2,494,3],[496,2,496,3],[498,2,498,3],[500,2,500,3],[502,2,502,3],[504,2,504,3],[482,2,482,3],[484,2,484,3],[486,2,486,3],[488,2,488,3],[490,2,490,3],[492,2,492,3],[518,2,518,3],[520,2,520,3],[522,2,522,3],[524,2,524,3],[526,2,526,3],[528,2,528,3],[506,2,506,3],[508,2,508,3],[510,2,510,3],[512,2,512,3],[514,2,514,3],[516,2,516,3],[542,2,542,3],[544,2,544,3],[546,2,546,3],[548,2,548,3],[550,2,550,3],[552,2,552,3],[530,2,530,3],[532,2,532,3],[534,2,534,3],[536,2,536,3],[538,2,538,3],[540,2,540,3],[566,2,566,3],[568,2,568,3],[570,2,570,3],[572,2,572,3],[574,2,574,3],[576,2,576,3],[554,2,554,3],[556,2,556,3],[558,2,558,3],[560,2,560,3],[562,2,562,3],[564,2,564,3],[590,2,590,3],[592,2,592,3],[594,2,594,3],[596,2,596,3],[598,2,598,3],[600,2,600,3],[578,2,578,3],[580,2,580,3],[582,2,582,3],[584,2,584,3],[586,2,586,3],[588,2,588,3],[614,2,614,3],[616,2,616,3],[618,2,618,3],[620,2,620,3],[622,2,622,3],[624,2,624,3],[602,2,602,3],[604,2,604,3],[606,2,606,3],[608,2,608,3],[610,2,610,3],[612,2,612,3],[638,2,638,3],[640,2,640,3],[642,2,642,3],[644,2,644,3],[646,2,646,3],[648,2,648,3],[626,2,626,3],[628,2,628,3],[630,2,630,3],[632,2,632,3],[634,2,634,3],[636,2,636,3],[662,2,662,3],[664,2,664,3],[666,2,666,3],[668,2,668,3],[670,2,670,3],[672,2,672,3],[650,2,650,3],[652,2,652,3],[654,2,654,3],[656,2,656,3],[658,2,658,3],[660,2,660,3],[686,2,686,3],[688,2,688,3],[690,2,690,3],[692,2,692,3],[694,2,694,3],[696,2,696,3],[674,2,674,3],[676,2,676,3],[678,2,678,3],[680,2,680,3],[682,2,682,3],[684,2,684,3],[710,2,710,3],[712,2,712,3],[714,2,714,3],[716,2,716,3],[718,2,718,3],[720,2,720,3],[698,2,698,3],[700,2,700,3],[702,2,702,3],[704,2,704,3],[706,2,706,3],[708,2,708,3]]}
[]
[null,"REGULATORY REPORTING STATEMENT"]
[null,"Australian Distribution Co."]
[null,"2019-20 to 2023-24"]
[null,"5.4 MAXIMUM DEMAND AND UTILISATION AT SPATIAL LEVEL"]
[]
[null,"5.4.2 - EXPECTED UNSERVED ENERGY"]
[null,"SUBTRANSMISSION SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","UNIT",null,"MAX DEMAND","2017-18","2018-19","2019-20","2020-21","2021-22","2022-23","2023-24"]
[null,"Ballina 132kV","MWh",null,"Non-Coincident",0.14714369612614067,0.14714369612614067,0.14714369612614067,0.14714369612614067,0.14714369612614067,0.14714369612614067,0.14714369612614067,"Andrew Mitchell provided this fc"]
[null,null,null,null,"Coincident",null,null,null,null,null,null,null,"Susan Hogan from AER advised coincident data not required"]
[null,"Casino 66/33kV","MWh",null,"Non-Coincident",0.16964426347462505,0.17725912169388608,0.18227617821519243,0.1855816706371419,0.18775949743760981,0.1891943606795711,0.19013972168012869]
[null,null,null,null,"Coincident"]
[null,"Casino 132/66kV","MWh",null,"Non-Coincident",0.27339109111957199,0.27339109112806376,0.27339109112807225,0.27339109112807225,0.27339109112807225,0.27339109112807225,0.27339109112807225]
[null,null,null,null,"Coincident"]
[null,"Dubbo 132/66kV","MWh",null,"Non-Coincident",3.1201754180496017E-3,5.6087365006703398E-4,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Goulburn 132/33kV","MWh",null,"Non-Coincident",8.2140392005977461E-2,8.3037347804796061E-2,8.3527165863047537E-2,8.3794650314907182E-2,8.3940720739999322E-2,8.402048825148746E-2,8.406404844435332E-2]
[null,null,null,null,"Coincident"]
[null,"Goulburn 132/66kV","MWh",null,"Non-Coincident",5.6798939454007921E-2,6.9939421826857667E-2,8.3066763717334874E-2,9.6180978265921355E-2,0.10928207859995918,0.12237007783366301,0.13544498906813385]
[null,null,null,null,"Coincident"]
[null,"Hawks Nest 132/33kV","MWh",null,"Non-Coincident",0.37670533234138703,0.401728055829562,0.42201050732263157,0.43845067774465302,0.45177644379406356,0.46257779415997458,0.4713329508462506]
[null,null,null,null,"Coincident"]
[null,"Herons Creek","MWh",null,"Non-Coincident",1.0051279487030582,1.0798024241100035,1.1544022250415458,1.2289274261721637,1.3033781021016388,1.3777543273551933,1.4520561763834896]
[null,null,null,null,"Coincident"]
[null,"Lismore 132/66kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Nyngan 132","MWh",null,"Non-Coincident",0.32389410537008595,0.33547279663392898,0.34557276671115439,0.35438286391785517,0.36206781864524967,0.36877132347345798,0.37461871992221424]
[null,null,null,null,"Coincident"]
[null,"Steeple Flat 132/66kV","MWh",null,"Non-Coincident",0.49813556108436347,0.49929564119726716,0.50045456123005727,0.50161232234281428,0.5027689256944593,0.50392437244275212,0.50507866374429733]
[null,null,null,null,"Coincident"]
[null,"Stroud 132/33kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Terranora 110/66kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Temora 132/66kV","MWh",null,"Non-Coincident",0.18100470402436847,0.17936999653008023,0.17778816725547186,0.17625750573789353,0.17477635684337958,0.17334311897692317,0.17195624235064108]
[null,null,null,null,"Coincident"]
[]
[null,"ZONE SUBSTATION"]
[null,null,null,null,null,null,null,"Forthcoming Period"]
[null,"SUBSTATION","UNIT",null,"MAX DEMAND","2017-18","2018-19","2019-20","2020-21","2021-22","2022-23","2023-24"]
[null,"Adaminaby 11kV","MWh",null,"Non-Coincident",6.8912644448993796E-2,6.890469834004348E-2,6.8898329175175049E-2,6.8893224002142997E-2,6.8889131975601661E-2,6.8885852031688052E-2,6.8883223008643676E-2,"Andrew Mitchell provided this fc"]
[null,null,null,null,"Coincident",null,null,null,null,null,null,null,"Susan Hogan from AER advised coincident data not required"]
[null,"Adaminaby 33kV","MWh",null,"Non-Coincident",9.7485103936551257E-2,9.5165725246073765E-2,9.3048997010428999E-2,9.1117213105554568E-2,8.9354214439833976E-2,8.7745253785649013E-2,8.6276872420960146E-2]
[null,null,null,null,"Coincident"]
[null,"Adelong","MWh",null,"Non-Coincident",7.0293775064464784E-2,7.0293775062126529E-2,7.0293775062123795E-2,7.0293775062123795E-2,7.0293775062123795E-2,7.0293775062123795E-2,7.0293775062123795E-2]
[null,null,null,null,"Coincident"]
[null,"Ashford","MWh",null,"Non-Coincident",6.5667861059704163E-3,6.970310397799888E-3,7.3260835541684765E-3,7.6397562161502532E-3,7.9163103549701151E-3,8.160138399196798E-3,8.375112998402252E-3]
[null,null,null,null,"Coincident"]
[null,"Ashley","MWh",null,"Non-Coincident",0.26684236117274052,0.26684236117273963,0.26684236117273963,0.26684236117273963,0.26684236117273963,0.26684236117273963,0.26684236117273963]
[null,null,null,null,"Coincident"]
[null,"Jelbart","MWh",null,"Non-Coincident",0.12203149432779208,0.11661172399164832,0.11149214759899304,0.10665613780251756,0.10208798822179059,9.7772862432116317E-2,9.3696745778827695E-2]
[null,null,null,null,"Coincident"]
[null,"Union Rd","MWh",null,"Non-Coincident",0.21125608968102191,0.2109528646609492,0.21064994286589545,0.21034732399263767,0.21004500773825321,0.20974299380012282,0.20944128187593072]
[null,null,null,null,"Coincident"]
[null,"Anona","MWh",null,"Non-Coincident",6.5189613920966533E-2,6.5086737560123384E-2,6.499763150355066E-2,6.4920452555414385E-2,6.4853604237078935E-2,6.4795703763281406E-2,6.4745553438644271E-2]
[null,null,null,null,"Coincident"]
[null,"Ariah Park","MWh",null,"Non-Coincident",4.1134800435760309E-2,4.1026401050197697E-2,4.0927145537802162E-2,4.0836262580396424E-2,4.0753045923230827E-2,4.0676848886652205E-2,4.0607079340732953E-2]
[null,null,null,null,"Coincident"]
[null,"Ardlethan","MWh",null,"Non-Coincident",3.4518666492236789E-2,3.4526029528777154E-2,3.4532034647815478E-2,3.4536932281348361E-2,3.4540926675809096E-2,3.454418440977404E-2,3.4546841340803429E-2]
[null,null,null,null,"Coincident"]
[null,"Ashmont","MWh",null,"Non-Coincident",0.19357506511976399,0.19348634988275265,0.19342483751434159,0.19338218676352328,0.19335261406794574,0.19333210928650574,0.19331789191288815]
[null,null,null,null,"Coincident"]
[null,"Attunga","MWh",null,"Non-Coincident",0.14693148132192893,0.14694159403492343,0.14694778499007471,0.14695157506358966,0.14695389532870184,0.14695531578404905,0.14695618538010638]
[null,null,null,null,"Coincident"]
[null,"Alstonville","MWh",null,"Non-Coincident",0.10214734619201019,0.105097277275549,0.1069491047042017,0.10811159451443611,0.10884135072065251,0.10929945720539097,0.10958703482319203]
[null,null,null,null,"Coincident"]
[null,"Ballina","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Barham","MWh",null,"Non-Coincident",0.26360708820191564,0.26259922526687079,0.26162621080893889,0.26068683988614311,0.25977994921930825,0.25890441575150114,0.25805915525728346]
[null,null,null,null,"Coincident"]
[null,"Batlow","MWh",null,"Non-Coincident",8.0400052719700812E-2,7.8226106374910592E-2,7.6054333976464952E-2,7.3884733350417994E-2,7.171730232499697E-2,6.9552038730601243E-2,6.7388940399800118E-2]
[null,null,null,null,"Coincident"]
[null,"Barraba","MWh",null,"Non-Coincident",0.10210385464009596,0.10177879357488435,0.10149423513178224,0.10124513268240734,0.10102706840848122,0.1008361749520653,0.10066906682817851]
[null,null,null,null,"Coincident"]
[null,"Boggabri","MWh",null,"Non-Coincident",0.26614746721131799,0.26822702037853813,0.27015868874856952,0.27195298896199799,0.27361968978179702,0.27516786527769677,0.27660594422841883]
[null,null,null,null,"Coincident"]
[null,"Bomen","MWh",null,"Non-Coincident",0.10762426613043442,0.10762426613050247,0.1076242661305034,0.1076242661305034,0.1076242661305034,0.1076242661305034,0.1076242661305034]
[null,null,null,null,"Coincident"]
[null,"Boambee South 11kV","MWh",null,"Non-Coincident",8.763004742523367E-2,8.6584077228341189E-2,8.5736485535256826E-2,8.504964791758883E-2,8.4493075788705158E-2,8.404206302137629E-2,8.3676589247650646E-2]
[null,null,null,null,"Coincident"]
[null,"Boambee South 66kV","MWh",null,"Non-Coincident",7.9481526789433612E-2,8.4970617229278525E-2,8.9828133439293273E-2,9.4126744290970801E-2,9.7930757382283046E-2,0.10129708108502798,0.10427607589909482]
[null,null,null,null,"Coincident"]
[null,"Batemans Bay","MWh",null,"Non-Coincident",0.17712697353683818,0.17231143510245892,0.16785504153749237,0.16373100766744986,0.15991454596735141,0.15638271757619332,0.15311429442281196]
[null,null,null,null,"Coincident"]
[null,"Blue Cow","MWh",null,"Non-Coincident",0.36759430953141037,0.3675943075291162,0.36759430715857588,0.36759430709000418,0.36759430707731405,0.36759430707496615,0.36759430707453139]
[null,null,null,null,"Coincident"]
[null,"Bundarra","MWh",null,"Non-Coincident",6.7667732512907156E-2,6.7621714551287362E-2,6.7594568143360567E-2,6.757855423406546E-2,6.7569107485471597E-2,6.7563534763823666E-2,6.7560247365386392E-2]
[null,null,null,null,"Coincident"]
[null,"Beelbangera","MWh",null,"Non-Coincident",8.8123862290148056E-2,8.8951512676157973E-2,8.9724729459213615E-2,9.0447092674050114E-2,9.1121946900683606E-2,9.1752416749993487E-2,9.2341421330837212E-2]
[null,null,null,null,"Coincident"]
[null,"Bega 132kV","MWh",null,"Non-Coincident",0.38879707653530449,0.38879707653530449,0.38879707653530449,0.38879707653530449,0.38879707653530449,0.38879707653530449,0.38879707653530449]
[null,null,null,null,"Coincident"]
[null,"Bermagui","MWh",null,"Non-Coincident",0.13858112079212723,0.13858112077263499,0.1385811207682256,0.13858112076722826,0.13858112076700255,0.13858112076695159,0.13858112076693976]
[null,null,null,null,"Coincident"]
[null,"Bethungra","MWh",null,"Non-Coincident",3.2498736440901052E-2,3.1688651458205069E-2,3.0950912360359358E-2,3.0279058186888742E-2,2.966720498332669E-2,2.9109994270806586E-2,2.8602546117655468E-2]
[null,null,null,null,"Coincident"]
[null,"Bullocks Flat","MWh",null,"Non-Coincident",9.2215375533220602E-3,9.4326853613068418E-3,9.6436220214836266E-3,9.8543477450002727E-3,1.0064862742793324E-2,1.0275167225588707E-2,1.0485261403901236E-2]
[null,null,null,null,"Coincident"]
[null,"Bingara","MWh",null,"Non-Coincident",0.11180345949940121,0.11180377853845382,0.11180382513309874,0.11180383193809923,0.11180383293194798,0.11180383307709661,0.11180383309829507]
[null,null,null,null,"Coincident"]
[null,"Burren Junction","MWh",null,"Non-Coincident",0.10254706562855619,0.10165145247559348,0.10082897409862689,0.10007365839302286,9.9380020929584409E-2,9.8743025131515769E-2,9.8158045703291216E-2]
[null,null,null,null,"Coincident"]
[null,"Bourke 22kV","MWh",null,"Non-Coincident",6.1653691959648968E-2,6.1919090930741313E-2,6.2134390140495752E-2,6.2309046995908834E-2,6.2450733615091576E-2,6.2565673838926042E-2,6.2658916624528091E-2]
[null,null,null,null,"Coincident"]
[null,"Bourke 33kV","MWh",null,"Non-Coincident",0.11432165341970016,0.11432165342035271,0.11432165342035357,0.11432165342035357,0.11432165342035357,0.11432165342035357,0.11432165342035357]
[null,null,null,null,"Coincident"]
[null,"Bulahdelah","MWh",null,"Non-Coincident",0.15525610086493327,0.15525610175696442,0.15525610212865026,0.1552561022835218,0.15525610234805262,0.15525610237494086,0.15525610238614429]
[null,null,null,null,"Coincident"]
[null,"Bendemeer","MWh",null,"Non-Coincident",3.1235612473456527E-2,3.1408547550406438E-2,3.1581309692279437E-2,3.1753899072010532E-2,3.192631586236188E-2,3.2098560235922911E-2,3.2270632365110324E-2]
[null,null,null,null,"Coincident"]
[null,"Bendick Murrell","MWh",null,"Non-Coincident",0.13663426183550004,0.13663426183185823,0.13663426183185481,0.13663426183185481,0.13663426183185481,0.13663426183185481,0.13663426183185481]
[null,null,null,null,"Coincident"]
[null,"Buronga Town","MWh",null,"Non-Coincident",9.9474863244489189E-2,0.10429260801548841,0.10905592313718553,0.11376542354184883,0.11842171721440044,0.12302540527090244,0.12757708203616311]
[null,null,null,null,"Coincident"]
[null,"Bohnock","MWh",null,"Non-Coincident",3.7546460851542833E-2,5.5502633060524213E-2,7.3440849097296618E-2,9.136112691803186E-2,0.10926348446094672,0.12714793964631896,0.14501451037650534]
[null,null,null,null,"Coincident"]
[null,"Blayney","MWh",null,"Non-Coincident",0.10653163410567575,0.10647044657189923,0.10642148755849297,0.10638231315734138,0.10635096788302141,0.10632588706000169,0.10630581871806005]
[null,null,null,null,"Coincident"]
[null,"Bodalla","MWh",null,"Non-Coincident",5.4944330046038624E-2,5.421910266467514E-2,5.3494600510693151E-2,5.2770822858865023E-2,5.2047768984688755E-2,5.1325438164386297E-2,5.060382967490442E-2]
[null,null,null,null,"Coincident"]
[null,"Bombala","MWh",null,"Non-Coincident",4.6449030304450079E-2,4.6388524495144287E-2,4.6348571400924014E-2,4.6322189640955871E-2,4.6304769281592092E-2,4.6293266299200747E-2,4.6285670669217939E-2]
[null,null,null,null,"Coincident"]
[null,"Bonalbo","MWh",null,"Non-Coincident",4.286924019696145E-2,4.5222754232181896E-2,4.6700806829976391E-2,4.7629052614431011E-2,4.8212009024536186E-2,4.857811699052357E-2,4.8808039915181366E-2]
[null,null,null,null,"Coincident"]
[null,"Boorowa","MWh",null,"Non-Coincident",0.14602027190820979,0.14900310504129052,0.15198295534123837,0.15495982579088605,0.15793371937008438,0.16090463905570329,0.1638725878216368]
[null,null,null,null,"Coincident"]
[null,"Bourkelands","MWh",null,"Non-Coincident",0.10871311762663095,0.10825004410858703,0.10783636261149591,0.10746680491845806,0.10713666472740692,0.10684173771654895,0.10657826800249673]
[null,null,null,null,"Coincident"]
[null,"Boronia St","MWh",null,"Non-Coincident",0.18825209146599758,0.1882520934133676,0.18825209341531521,0.18825209341531712,0.18825209341531712,0.18825209341531712,0.18825209341531712]
[null,null,null,null,"Coincident"]
[null,"Bullocks Portal","MWh",null,"Non-Coincident",0.10780170268553793,0.10982714053991176,0.11185055295643152,0.11387194196053448,0.11589130957563334,0.1179086578231172,0.1199239887223531]
[null,null,null,null,"Coincident"]
[null,"Banora Point","MWh",null,"Non-Coincident",0.12267737527564511,0.12267737528196435,0.12267737528196999,0.12267737528196999,0.12267737528196999,0.12267737528196999,0.12267737528196999]
[null,null,null,null,"Coincident"]
[null,"Brewarrina","MWh",null,"Non-Coincident",0.24910541437455747,0.24910541438883138,0.24910541438884598,0.24910541438884598,0.24910541438884598,0.24910541438884598,0.24910541438884598]
[null,null,null,null,"Coincident"]
[null,"Burraga","MWh",null,"Non-Coincident",4.0826826487732559E-2,4.0826826487724323E-2,4.0826826487724323E-2,4.0826826487724323E-2,4.0826826487724323E-2,4.0826826487724323E-2,4.0826826487724323E-2]
[null,null,null,null,"Coincident"]
[null,"Brisbane Grove","MWh",null,"Non-Coincident",0,0,0,0,1.8785557132947059E-3,4.8182183252944702E-3,7.7549412746824231E-3]
[null,null,null,null,"Coincident"]
[null,"Booral","MWh",null,"Non-Coincident",9.5624054947250833E-2,9.6831003478967503E-2,9.7188968036789711E-2,9.7295135467537278E-2,9.7326623286946232E-2,9.7335962146934893E-2,9.733873192609202E-2]
[null,null,null,null,"Coincident"]
[null,"Brogo","MWh",null,"Non-Coincident",6.1488783505231182E-2,6.4125170312847063E-2,6.6758920733655261E-2,6.9390037404042718E-2,7.2018522957759776E-2,7.4644380025923107E-2,7.7267611237018266E-2]
[null,null,null,null,"Coincident"]
[null,"Boundary Street","MWh",null,"Non-Coincident",0.19098104185500794,0.19310037763350293,0.19422541749501709,0.19482263984309353,0.19513967263921356,0.19530796807246267,0.19539730694591426]
[null,null,null,null,"Coincident"]
[null,"Bellata","MWh",null,"Non-Coincident",4.7013924562072193E-2,4.7013925691337596E-2,4.7013926298778083E-2,4.7013926625525407E-2,4.7013926801285078E-2,4.7013926895827715E-2,4.7013926946682612E-2]
[null,null,null,null,"Coincident"]
[null,"Russell Street","MWh",null,"Non-Coincident",1.2468531012339152E-2,1.2468531021415853E-2,1.2468531021425321E-2,1.2468531021425321E-2,1.2468531021425321E-2,1.2468531021425321E-2,1.2468531021425321E-2]
[null,null,null,null,"Coincident"]
[null,"Borthwick St","MWh",null,"Non-Coincident",0.19426830069511497,0.20237453026061511,0.20948080846335648,0.21571048521834182,0.22117169449897925,0.22595923131347792,0.23015619714510172]
[null,null,null,null,"Coincident"]
[null,"Bulgary","MWh",null,"Non-Coincident",2.3596788461573322E-2,2.4828204186819969E-2,2.5856912578944125E-2,2.6716281948955006E-2,2.7434187742051391E-2,2.8033916736063497E-2,2.8534922396858352E-2]
[null,null,null,null,"Coincident"]
[null,"Bungendore","MWh",null,"Non-Coincident",7.4838312828288206E-2,7.4983201130741375E-2,7.5094182906981471E-2,7.5179192907436035E-2,7.5244309005070384E-2,7.5294186738848246E-2,7.5332392166034393E-2]
[null,null,null,null,"Coincident"]
[null,"Bootawa","MWh",null,"Non-Coincident",0.1747732290470157,0.17477322783086027,0.17477322782964452,0.17477322782964319,0.17477322782964319,0.17477322782964319,0.17477322782964319]
[null,null,null,null,"Coincident"]
[null,"Byabarra","MWh",null,"Non-Coincident",6.6991744743881684E-2,6.9216242684089865E-2,7.1086443469867741E-2,7.2658776226801766E-2,7.3980682578959067E-2,7.5092048093775898E-2,7.602640573984365E-2]
[null,null,null,null,"Coincident"]
[null,"Byrock","MWh",null,"Non-Coincident",4.8722647891338792E-3,5.2064092125471331E-3,5.5402194915370037E-3,5.8736959602478439E-3,6.206838952489949E-3,6.5396488017398727E-3,6.8721258411405146E-3]
[null,null,null,null,"Coincident"]
[null,"Carathool","MWh",null,"Non-Coincident",3.0179469035453602E-2,3.0179484215423866E-2,3.0179488815031012E-2,3.0179490208735001E-2,3.0179490631034339E-2,3.0179490758993125E-2,3.0179490797765308E-2]
[null,null,null,null,"Coincident"]
[null,"Coonabarabran","MWh",null,"Non-Coincident",8.4032154469407122E-2,8.4150345041403937E-2,8.42535234083929E-2,8.4343596374744145E-2,8.44222285483682E-2,8.449087310376921E-2,8.4550798637670108E-2]
[null,null,null,null,"Coincident"]
[null,"Cobar CSA","MWh",null,"Non-Coincident",0,0,0,2.710414631559303E-4,4.3998430707091318E-3,8.5245158766540288E-3,1.2645064009792938E-2]
[null,null,null,null,"Coincident"]
[null,"Cobar Elura","MWh",null,"Non-Coincident",9.0019132418953346E-2,9.0021158199485571E-2,9.0021229773573255E-2,9.0021232302400972E-2,9.0021232391748571E-2,9.0021232394905448E-2,9.0021232395016929E-2]
[null,null,null,null,"Coincident"]
[null,"Colly Blue","MWh",null,"Non-Coincident",4.8174155350947989E-2,4.9839884481737803E-2,5.1377153070437297E-2,5.2795867956381096E-2,5.4105171966359604E-2,5.5313502835043181E-2,5.642864758147708E-2]
[null,null,null,null,"Coincident"]
[null,"Cobar Peak","MWh",null,"Non-Coincident",0.12702097511162705,0.1304205214815764,0.13353713623213961,0.13639436671126803,0.13901380050859119,0.14141522855882396,0.14361679467068314]
[null,null,null,null,"Coincident"]
[null,"Cobar Town","MWh",null,"Non-Coincident",0.28786419495440607,0.28786419492439425,0.28786419491854526,0.2878641949174055,0.2878641949171834,0.28786419491713977,0.28786419491713156]
[null,null,null,null,"Coincident"]
[null,"Coleambally 33/11","MWh",null,"Non-Coincident",0.10788094413055506,0.10375898315139948,9.9845193232843701E-2,9.6129061128718815E-2,9.2600604542473305E-2,8.9250345312668997E-2,8.6069283952683401E-2]
[null,null,null,null,"Coincident"]
[null,"Culcairn","MWh",null,"Non-Coincident",0.1673667564910796,0.16428639352680147,0.16120911092548762,0.15813490560677537,0.15506377449338141,0.15199571451110092,0.14893072258880269]
[null,null,null,null,"Coincident"]
[null,"Condobolin","MWh",null,"Non-Coincident",7.1335271427664132E-2,7.0553442540368314E-2,6.9835504527455308E-2,6.9176236241567102E-2,6.8570843206290366E-2,6.8014922748706269E-2,6.7504431981300655E-2]
[null,null,null,null,"Coincident"]
[null,"Captains Flat","MWh",null,"Non-Coincident",0.14814082511577351,0.1481408251157767,0.1481408251157767,0.1481408251157767,0.1481408251157767,0.1481408251157767,0.1481408251157767]
[null,null,null,null,"Coincident"]
[null,"Coffs Harbour North","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Crescent Head","MWh",null,"Non-Coincident",1.7929741409361433E-2,1.8287699226184301E-2,1.8645299085190303E-2,1.9002541344337313E-2,1.9359426361225136E-2,1.9715954493096099E-2,2.0072126096835216E-2]
[null,null,null,null,"Coincident"]
[null,"Cartwrights Hill 11kV","MWh",null,"Non-Coincident",8.1984584843643477E-3,8.5903778830429354E-3,8.8996956621123918E-3,9.1438210837451843E-3,9.3364942034949508E-3,9.4885591987166149E-3,9.6085747089332575E-3]
[null,null,null,null,"Coincident"]
[null,"Cartwrights Hill 33kV","MWh",null,"Non-Coincident",8.2477897812639422E-2,8.0062215664414169E-2,7.7814327249140766E-2,7.5722577582806247E-2,7.3776121238763592E-2,7.1964866115723489E-2,7.0279421111637472E-2]
[null,null,null,null,"Coincident"]
[null,"Coffs Harbour South","MWh",null,"Non-Coincident",3.7153563102649043E-2,4.2965407476461305E-2,4.8026307580051504E-2,5.2433292387479256E-2,5.6270853828203467E-2,5.9612566689685197E-2,6.2522499213523153E-2]
[null,null,null,null,"Coincident"]
[null,"Currabubula","MWh",null,"Non-Coincident",0.10366258836086169,0.10453367850760784,0.10522792764366405,0.10578123646562054,0.10622221742844165,0.10657367433976023,0.10685378158004462]
[null,null,null,null,"Coincident"]
[null,"Coolamon","MWh",null,"Non-Coincident",0.20433245618830545,0.20202518026216254,0.19972021161194603,0.19741754793037916,0.19511718691249466,0.19281912625562772,0.19052336365941744]
[null,null,null,null,"Coincident"]
[null,"Coleambally 132","MWh",null,"Non-Coincident",0.10729442395016069,0.10729442343415099,0.1072944232520977,0.10729442318786697,0.1072944231652059,0.10729442315721119,0.10729442315439036]
[null,null,null,null,"Coincident"]
[null,"Cumnock","MWh",null,"Non-Coincident",7.0076959917546408E-2,6.9310120535749725E-2,6.8544047993335008E-2,6.7778741523462527E-2,6.7014200360060144E-2,6.6250423737821057E-2,6.5487410892204223E-2]
[null,null,null,null,"Coincident"]
[null,"Caroona","MWh",null,"Non-Coincident",4.5460625313299613E-2,4.6267904170712325E-2,4.6954901778422375E-2,4.7539539550941624E-2,4.8037068685278857E-2,4.8460468012435129E-2,4.8820782570646912E-2]
[null,null,null,null,"Coincident"]
[null,"Coonamble","MWh",null,"Non-Coincident",0.26465616557066091,0.26597909186773339,0.26679900017762403,0.26730715368407099,0.26762209132160869,0.26781727981146319,0.26793825152786238]
[null,null,null,null,"Coincident"]
[null,"Coopernook","MWh",null,"Non-Coincident",0.11901482388587065,0.1190148238921542,0.11901482389216012,0.11901482389216012,0.11901482389216012,0.11901482389216012,0.11901482389216012]
[null,null,null,null,"Coincident"]
[null,"Cobargo","MWh",null,"Non-Coincident",5.5319311675611174E-2,5.5983905351911355E-2,5.6566923515377732E-2,5.7078379147673525E-2,5.7527056187599179E-2,5.7920660389888655E-2,5.8265951666852028E-2]
[null,null,null,null,"Coincident"]
[null,"Cooma 11kV","MWh",null,"Non-Coincident",0.64178298858911054,0.65208980891991308,0.65935057650827378,0.66446551441153978,0.66806879594285284,0.67060717236881107,0.67239536316763726]
[null,null,null,null,"Coincident"]
[null,"Cowra","MWh",null,"Non-Coincident",0.18261361527306566,0.1823275128362058,0.1820639883849488,0.18182126016084682,0.18159768701423876,0.18139175730800369,0.1812020786969841]
[null,null,null,null,"Coincident"]
[null,"Copeton","MWh",null,"Non-Coincident",4.0100479898157543E-2,4.0968261280349541E-2,4.1745240986666904E-2,4.2440920193916293E-2,4.3063805908258729E-2,4.3621514991826045E-2,4.4120867304347604E-2]
[null,null,null,null,"Coincident"]
[null,"Clearwater Cr","MWh",null,"Non-Coincident",0.13269866077067169,0.13269866077238873,0.13269866077239062,0.13269866077239062,0.13269866077239062,0.13269866077239062,0.13269866077239062]
[null,null,null,null,"Coincident"]
[null,"Corowa","MWh",null,"Non-Coincident",0.16174735748133071,0.16224100018135887,0.16268044654690353,0.16307164671694468,0.16341989757311043,0.16372991445988117,0.16400589503072893]
[null,null,null,null,"Coincident"]
[null,"Crookwell","MWh",null,"Non-Coincident",4.6399658315969074E-2,4.6547234637695188E-2,4.6615159153466409E-2,4.6646422568821948E-2,4.6660812088255219E-2,4.6667435109673971E-2,4.6670483468093188E-2]
[null,null,null,null,"Coincident"]
[null,"Casino 66/11kV","MWh",null,"Non-Coincident",0.21606780861272853,0.2160678085945533,0.21606780859453537,0.21606780859453537,0.21606780859453537,0.21606780859453537,0.21606780859453537]
[null,null,null,null,"Coincident"]
[null,"Clinton Street","MWh",null,"Non-Coincident",0.13692667649562373,0.13692667653293897,0.13692667654115667,0.13692667654296542,0.13692667654336421,0.13692667654345209,0.13692667654347099]
[null,null,null,null,"Coincident"]
[null,"Cootamundra","MWh",null,"Non-Coincident",0.48418755318757017,0.48796992747187229,0.49174851938189712,0.4955233327000047,0.49929437120480197,0.503061638671087,0.50682513886990899]
[null,null,null,null,"Coincident"]
[null,"Cudgen 11kV","MWh",null,"Non-Coincident",0.12773081898429145,0.13146686305371139,0.13387730816641075,0.13543249475772892,0.13643588011633839,0.1370832507813721,0.13750092558034119]
[null,null,null,null,"Coincident"]
[null,"Cudgen 33kV","MWh",null,"Non-Coincident",0.11029278178802929,0.11061232814255276,0.11074976169651482,0.11080887043453606,0.11083429248620809,0.1108452262454605,0.11084992874126735]
[null,null,null,null,"Coincident"]
[null,"Canowindra","MWh",null,"Non-Coincident",0.26267032538962437,0.26360682518759365,0.26446787273683092,0.26525954710094157,0.26598743756337345,0.26665668308819818,0.26727200860160166]
[null,null,null,null,"Coincident"]
[null,"Dubbo South","MWh",null,"Non-Coincident",0.15864579006785492,0.1639476248507597,0.16924415779888125,0.17453539421405609,0.17982133939281456,0.18510199862639501,0.19037737720074088]
[null,null,null,null,"Coincident"]
[null,"Dubbo West","MWh",null,"Non-Coincident",0.1470107898665258,0.15524573625514521,0.16262555331796011,0.16923903898143439,0.1751657702606384,0.18047706077267373,0.18523681882045578]
[null,null,null,null,"Coincident"]
[null,"Deniliquin","MWh",null,"Non-Coincident",0.20183607436625736,0.20150142612495997,0.20120775364130522,0.20095003966880307,0.20072388129401572,0.20052541471500276,0.20035124923020795]
[null,null,null,null,"Coincident"]
[null,"Dunedoo","MWh",null,"Non-Coincident",4.9216979116768964E-2,4.9282099513152572E-2,4.9340297599565743E-2,4.9392309218816495E-2,4.9438791993488468E-2,4.9480333640765158E-2,4.9517459403386657E-2]
[null,null,null,null,"Coincident"]
[null,"Dorrigo","MWh",null,"Non-Coincident",2.2125356362945933E-2,2.1051014654041977E-2,1.9978324255148016E-2,1.8907282628128817E-2,1.7837887238750186E-2,1.677013555667304E-2,1.5704025055447712E-2]
[null,null,null,null,"Coincident"]
[null,"Darlington Point","MWh",null,"Non-Coincident",0.17498465370708141,0.18146640752673118,0.187941679592561,0.19441047638632533,0.20087280438329561,0.20732867005226926,0.2137780798555739]
[null,null,null,null,"Coincident"]
[null,"Dareton","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Dungog","MWh",null,"Non-Coincident",7.8980595355646027E-2,7.8980831735517662E-2,7.8980882059543955E-2,7.898089277326345E-2,7.8980895054157799E-2,7.8980895539748117E-2,7.8980895643127727E-2]
[null,null,null,null,"Coincident"]
[null,"Dunoon","MWh",null,"Non-Coincident",5.6924060553398687E-2,5.694008777303957E-2,5.6945428086469234E-2,5.6947207493513299E-2,5.6947800396808322E-2,5.6947997953808165E-2,5.6948063780341E-2]
[null,null,null,null,"Coincident"]
[null,"Edrom","MWh",null,"Non-Coincident",8.9373661195144713E-2,8.9374979881741201E-2,8.9375540019248675E-2,8.9375777948433807E-2,8.9375879013433288E-2,8.9375921942736983E-2,8.9375940177784718E-2]
[null,null,null,null,"Coincident"]
[null,"Egansford","MWh",null,"Non-Coincident",5.880384677328207E-2,5.8803825622471474E-2,5.8803819424314965E-2,5.8803817607971348E-2,5.880381707569915E-2,5.8803816919719247E-2,5.8803816874009943E-2]
[null,null,null,null,"Coincident"]
[null,"Lismore East","MWh",null,"Non-Coincident",0.14937356351355607,0.16429961619119854,0.17667056251297469,0.18692379665340447,0.19542183775745653,0.20246514737245871,0.20830275273649182]
[null,null,null,null,"Coincident"]
[null,"Ellerslie","MWh",null,"Non-Coincident",0.26996949106966528,0.26643883998619217,0.26291171955380266,0.2593881262418451,0.25586805652319916,0.25235150687427194,0.24883847377499446]
[null,null,null,null,"Coincident"]
[null,"Emmaville 66/11kV","MWh",null,"Non-Coincident",7.4917055107028965E-2,7.491705555039993E-2,7.4917055751717698E-2,7.4917055843128494E-2,7.491705588463457E-2,7.4917055903480953E-2,7.4917055912038399E-2]
[null,null,null,null,"Coincident"]
[null,"Emmaville 66/22kV","MWh",null,"Non-Coincident",7.8109995178411223E-3,7.8113202276260925E-3,7.8115440225569694E-3,7.8117001892018213E-3,7.8118091640604834E-3,7.8118852079546997E-3,7.8119382722478667E-3]
[null,null,null,null,"Coincident"]
[null,"Eden South","MWh",null,"Non-Coincident",4.4226535112989747E-2,4.3980093279712203E-2,4.3753202507325666E-2,4.3544311744302344E-2,4.3351992989258119E-2,4.317493152896907E-2,4.3011916950840931E-2]
[null,null,null,null,"Coincident"]
[null,"Tamworth East","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Euberta","MWh",null,"Non-Coincident",6.1501744835682062E-2,6.0050497825446761E-2,5.8600702062221871E-2,5.7152356094760291E-2,5.5705458473265967E-2,5.4260007749393366E-2,5.2816002476244288E-2]
[null,null,null,null,"Coincident"]
[null,"Eucumbene","MWh",null,"Non-Coincident",1.620157181277046E-2,1.6526268696361573E-2,1.67857241446406E-2,1.6993047137387467E-2,1.7158712663421297E-2,1.7291090969138709E-2,1.7396870464994746E-2]
[null,null,null,null,"Coincident"]
[null,"Eulomogo","MWh",null,"Non-Coincident",0.1673960272490454,0.16521691971526342,0.16303999128901595,0.16086523979119452,0.15869266304487062,0.15652225887529297,0.15435402510988497]
[null,null,null,null,"Coincident"]
[null,"Ewingsdale","MWh",null,"Non-Coincident",0.15640650785627658,0.15640650787044971,0.1564065078704639,0.1564065078704639,0.1564065078704639,0.1564065078704639,0.1564065078704639]
[null,null,null,null,"Coincident"]
[null,"Forbes Town","MWh",null,"Non-Coincident",0.63213364520004334,0.63127878994151343,0.63053288265204965,0.62988203833785239,0.6293141415934328,0.62881862107449837,0.62838625271334192]
[null,null,null,null,"Coincident"]
[null,"Failford","MWh",null,"Non-Coincident",0.31621747349535367,0.31621747382460197,0.31621747389270638,0.31621747390679339,0.31621747390970717,0.31621747391031002,0.31621747391043514]
[null,null,null,null,"Coincident"]
[null,"Forest Hill","MWh",null,"Non-Coincident",5.7065843413373479E-2,5.5829819480771821E-2,5.468700482405664E-2,5.3630370478106516E-2,5.265341753610419E-2,5.1750137177534287E-2,5.0914973710493805E-2]
[null,null,null,null,"Coincident"]
[null,"Finley Town","MWh",null,"Non-Coincident",0.13030948528435435,0.12794311210276829,0.12577798943665894,0.12379700173963123,0.12198448907362558,0.1203261233152939,0.11880879489051079]
[null,null,null,null,"Coincident"]
[null,"Forster","MWh",null,"Non-Coincident",0.13229872921828459,0.13257310923352914,0.13281393704536126,0.13302531554134883,0.1332108458927905,0.13337368890643381,0.13351661887388455]
[null,null,null,null,"Coincident"]
[null,"Ganmurra","MWh",null,"Non-Coincident",3.8943907461365841E-2,3.7465406624372831E-2,3.6041242197659071E-2,3.4669417262854066E-2,3.3348008290369727E-2,3.2075162442287371E-2,3.084909497436766E-2]
[null,null,null,null,"Coincident"]
[null,"Goulburn North","MWh",null,"Non-Coincident",7.2346399375996628E-2,7.550003735239405E-2,7.8529537419272349E-2,8.1439786066677192E-2,8.4235477435797887E-2,8.6921120890471562E-2,8.9501048290648075E-2]
[null,null,null,null,"Coincident"]
[null,"Gundagai South","MWh",null,"Non-Coincident",0.27030899255987356,0.27540483492697448,0.28049558145170883,0.28558123722991818,0.29066180735234914,0.29573729690465783,0.3008077109674141]
[null,null,null,null,"Coincident"]
[null,"Gunnedah 22kV","MWh",null,"Non-Coincident",0.22799880712049525,0.23015143773638827,0.23228138871681411,0.23438889900934706,0.23647420504406444,0.23853754076006803,0.24057913763173031]
[null,null,null,null,"Coincident"]
[null,"Goondiwindi 22kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Goondiwindi 33kV","MWh",null,"Non-Coincident",4.9745377303405697E-2,4.9746406016703007E-2,4.9747195108274606E-2,4.9747800394033051E-2,4.974826468849846E-2,4.9748620833257602E-2,4.9748894019993301E-2]
[null,null,null,null,"Coincident"]
[null,"Goddard Lane","MWh",null,"Non-Coincident",0.13437018174607587,0.13923853635002598,0.14299934403736045,0.1459045708771704,0.14814886085221479,0.14988257658933554,0.1512218733337683]
[null,null,null,null,"Coincident"]
[null,"Googong Dam","MWh",null,"Non-Coincident",4.8298912295107119E-2,4.8298873221799196E-2,4.8298862628207109E-2,4.8298859756062379E-2,4.8298858977363537E-2,4.8298858766242188E-2,4.8298858709002725E-2]
[null,null,null,null,"Coincident"]
[null,"Griffith","MWh",null,"Non-Coincident",0.26272438063513265,0.26634164081465023,0.26995528373398897,0.2735653130104076,0.27717173225755021,0.28077454508544536,0.2843737551005126]
[null,null,null,null,"Coincident"]
[null,"Gulargambone","MWh",null,"Non-Coincident",0.12078672129730092,0.12097351168364059,0.12113902689593851,0.1212856901479345,0.12141564865257716,0.12153080505814788,0.12163284530384208]
[null,null,null,null,"Coincident"]
[null,"Gulgong","MWh",null,"Non-Coincident",0.28735165188146627,0.2707971256906942,0.25805178378728061,0.24823913567141589,0.24068437066193538,0.23486795151854456,0.23038988613740519]
[null,null,null,null,"Coincident"]
[null,"Gilgandra","MWh",null,"Non-Coincident",0.29506122666794549,0.29680085600208589,0.29817209216321211,0.29925294805169267,0.30010491614062051,0.30077646692947946,0.30130580654662853]
[null,null,null,null,"Coincident"]
[null,"Ginkgo","MWh",null,"Non-Coincident",0.66858600977013438,0.66858597608381631,0.66858596077910215,0.66858595382570674,0.66858595066656867,0.66858594923127668,0.66858594857917963]
[null,null,null,null,"Coincident"]
[null,"Gloucester","MWh",null,"Non-Coincident",8.556216371908941E-2,8.597215751393654E-2,8.634526023741311E-2,8.6684791332798425E-2,8.6993771561244257E-2,8.7274949877068714E-2,8.7530827884821777E-2]
[null,null,null,null,"Coincident"]
[null,"Galloway St","MWh",null,"Non-Coincident",9.7787107584080768E-2,9.5435513608285311E-2,9.3340965075890098E-2,9.1475365146772347E-2,8.9813688159252641E-2,8.8333643929106059E-2,8.7015378743006383E-2]
[null,null,null,null,"Coincident"]
[null,"Grenfell","MWh",null,"Non-Coincident",0.20467309615369297,0.20421109804611834,0.20377746665323732,0.20337046025687072,0.2029884440804525,0.20262988372280791,0.20229333899509508]
[null,null,null,null,"Coincident"]
[null,"Glen Innes","MWh",null,"Non-Coincident",7.6460759220771779E-2,7.6460759220772057E-2,7.6460759220772057E-2,7.6460759220772057E-2,7.6460759220772057E-2,7.6460759220772057E-2,7.6460759220772057E-2]
[null,null,null,null,"Coincident"]
[null,"Googong Town","MWh",null,"Non-Coincident",0.6294050000000001,0.71086749999999987,0.79233000000000009,0.87379250000000008,0.95525500000000019,1.0367175,1.11818]
[null,null,null,null,"Coincident"]
[null,"Girilambone","MWh",null,"Non-Coincident",0.17424194943019639,0.1852529016557195,0.19587864951873143,0.20613266891104221,0.21602796428727486,0.22557708515750788,0.23479214200294057]
[null,null,null,null,"Coincident"]
[null,"Grafton North","MWh",null,"Non-Coincident",0.81343846325839386,0.8244333730777782,0.8300444384699468,0.8329079503452026,0.83436929497169432,0.83511506736950569,0.83549565963998229]
[null,null,null,null,"Coincident"]
[null,"Gresford","MWh",null,"Non-Coincident",0.10038822313250731,9.8349288718716052E-2,9.6519339994096578E-2,9.4876956447040514E-2,9.3402913114924144E-2,9.2079955545815523E-2,9.089259782604775E-2]
[null,null,null,null,"Coincident"]
[null,"Geurie","MWh",null,"Non-Coincident",0.11791557640330433,0.11791557636912779,0.11791557636165298,0.11791557636001858,0.11791557635966099,0.11791557635958297,0.1179155763595658]
[null,null,null,null,"Coincident"]
[null,"Guyra","MWh",null,"Non-Coincident",5.4712075802853991E-2,5.6521715455364288E-2,5.7773092496049318E-2,5.8638427479056218E-2,5.9236811985460193E-2,5.9650598582021985E-2,5.9936734579297622E-2]
[null,null,null,null,"Coincident"]
[null,"Hammond Ave","MWh",null,"Non-Coincident",0.16599298369773674,0.16292235017669027,0.1603301906562612,0.15814194808895596,0.15629468309788225,0.15473526368148294,0.15341883700312733]
[null,null,null,null,"Coincident"]
[null,"Hanwood","MWh",null,"Non-Coincident",0.10992411742539938,0.11062059883239865,0.11126886086035787,0.11187224187336162,0.11243384911110081,0.11295657469026946,0.11344311049813498]
[null,null,null,null,"Coincident"]
[null,"Hay 132","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Hay Town","MWh",null,"Non-Coincident",0.28601364111965699,0.28704630613318344,0.28795530427066635,0.28875544526810804,0.28945976532046891,0.29007973947220361,0.29062546857295957]
[null,null,null,null,"Coincident"]
[null,"Henty","MWh",null,"Non-Coincident",2.1658420854987561E-2,2.144807342530505E-2,2.1237936343052249E-2,2.102800939788169E-2,2.0818292379656284E-2,2.0608785078449088E-2,2.0399487284543161E-2]
[null,null,null,null,"Coincident"]
[null,"Hillgrove","MWh",null,"Non-Coincident",4.5199060552791895E-2,3.8774796468537792E-2,3.6200214256919737E-2,3.5168427039356971E-2,3.4754928935656258E-2,3.4589215812975832E-2,3.4522804773160311E-2]
[null,null,null,null,"Coincident"]
[null,"Harrington","MWh",null,"Non-Coincident",0.15478238543382342,0.15905764791921687,0.1620245455639629,0.164083479176688,0.16551231432006316,0.16650388095160776,0.16719199699449155]
[null,null,null,null,"Coincident"]
[null,"Hillston","MWh",null,"Non-Coincident",0.10013419581590913,0.10162991233484145,0.10285054468979565,0.10384668488554825,0.10465962031657063,0.10532304502107476,0.10586445621038976]
[null,null,null,null,"Coincident"]
[null,"Hallidays Point 11kV","MWh",null,"Non-Coincident",5.753209251569498E-2,5.7531916532472353E-2,5.7531858441590651E-2,5.7531839266180135E-2,5.753183293650567E-2,5.7531830847122586E-2,5.7531830157431255E-2]
[null,null,null,null,"Coincident"]
[null,"Holbrook","MWh",null,"Non-Coincident",0.14371047699949577,0.14351587018941811,0.1433325580604595,0.14315988508663116,0.14299723378766874,0.14284402252091563,0.14269970340136556]
[null,null,null,null,"Coincident"]
[null,"Hastings Point","MWh",null,"Non-Coincident",0.10382629506425223,0.10547682952584141,0.10702483672474061,0.10847668540988351,0.10983834871871778,0.11111542875164311,0.11231317961994944]
[null,null,null,null,"Coincident"]
[null,"Ivanhoe","MWh",null,"Non-Coincident",4.4109776171704793E-2,4.4547870809143297E-2,4.495244454315378E-2,4.5326062232720184E-2,4.5671092486101357E-2,4.5989722676995831E-2,4.6283972811743943E-2]
[null,null,null,null,"Coincident"]
[null,"Jerilderie","MWh",null,"Non-Coincident",0.23770161945470988,0.24262138580809856,0.24720092528207624,0.25146376629672618,0.25543181016214955,0.25912544360140116,0.26256364349189115]
[null,null,null,null,"Coincident"]
[null,"Jugiong","MWh",null,"Non-Coincident",1.8326962451163525E-2,1.8326966438769063E-2,1.8326969050017159E-2,1.8326970759969807E-2,1.832697187971713E-2,1.8326972612973717E-2,1.8326973093140311E-2]
[null,null,null,null,"Coincident"]
[null,"Jindabyne 11kV","MWh",null,"Non-Coincident",0.15765756907786954,0.15901370279047763,0.15964412857582899,0.15993719456713992,0.16007343213428626,0.16013676488272061,0.16016620637311182]
[null,null,null,null,"Coincident"]
[null,"Jindabyne 33kV","MWh",null,"Non-Coincident",6.5371269978679314E-2,6.5697491930903795E-2,6.5958089872968403E-2,6.6166264972606054E-2,6.6332562801997189E-2,6.6465407547158101E-2,6.6571528753799583E-2]
[null,null,null,null,"Coincident"]
[null,"Johns River","MWh",null,"Non-Coincident",0.10658325924471787,0.11569011250623316,0.12436628703693677,0.13263215037365494,0.14050710683741632,0.14800964308558667,0.15515737150975345]
[null,null,null,null,"Coincident"]
[null,"Junee Reefs","MWh",null,"Non-Coincident",1.7441496833929756E-2,1.7658998941948157E-2,1.7858788329318757E-2,1.8042307466993202E-2,1.8210881355406605E-2,1.8365727090924384E-2,1.8507962653227253E-2]
[null,null,null,null,"Coincident"]
[null,"Jindabyne East","MWh",null,"Non-Coincident",4.1046114025764129E-2,4.1046116181762356E-2,4.1046117036181551E-2,4.1046117374786771E-2,4.1046117508975535E-2,4.1046117562154379E-2,4.1046117583229111E-2]
[null,null,null,null,"Coincident"]
[null,"Kew","MWh",null,"Non-Coincident",0.13874764269283327,0.13463173203046841,0.13080678032740362,0.12725221932476782,0.12394893476006634,0.12087916358233125,0.11802639843325696]
[null,null,null,null,"Coincident"]
[null,"Koree Island","MWh",null,"Non-Coincident",8.2235085000162647E-2,8.5549025166238274E-2,8.8527219709660113E-2,9.1203684067485094E-2,9.360898746666331E-2,9.5770602070342312E-2,9.7713216751065368E-2]
[null,null,null,null,"Coincident"]
[null,"Koolkhan 11kV","MWh",null,"Non-Coincident",0.1762934790097507,0.17577117838372217,0.17533814284641699,0.1749791163256264,0.17468145012614364,0.17443465730950231,0.17423004323356389]
[null,null,null,null,"Coincident"]
[null,"Kooringal","MWh",null,"Non-Coincident",0.78697710876834137,0.78697711244184765,0.78697711456703889,0.78697711579650798,0.7869771165077778,0.78697711691926142,0.78697711715731289]
[null,null,null,null,"Coincident"]
[null,"Koraleigh","MWh",null,"Non-Coincident",0.19008002872770363,0.19074606820137416,0.19135798131536863,0.19192016670209203,0.19243666553471586,0.1929111905764575,0.19334715286914345]
[null,null,null,null,"Coincident"]
[null,"Keepit Dam","MWh",null,"Non-Coincident",2.0353545343453319E-2,2.0353545343162454E-2,2.0353545343162197E-2,2.0353545343162197E-2,2.0353545343162197E-2,2.0353545343162197E-2,2.0353545343162197E-2]
[null,null,null,null,"Coincident"]
[null,"Kanangra Dr","MWh",null,"Non-Coincident",0.10377059169288326,0.10377059373445936,0.10377059373650058,0.10377059373650245,0.10377059373650245,0.10377059373650245,0.10377059373650245]
[null,null,null,null,"Coincident"]
[null,"Kootingal","MWh",null,"Non-Coincident",0.25961335767513966,0.25961335767866278,0.25961335767866639,0.25961335767866639,0.25961335767866639,0.25961335767866639,0.25961335767866639]
[null,null,null,null,"Coincident"]
[null,"Kyogle","MWh",null,"Non-Coincident",7.3105470489497615E-2,7.3105470601689912E-2,7.3105470602252656E-2,7.3105470602255487E-2,7.3105470602255487E-2,7.3105470602255487E-2,7.3105470602255487E-2]
[null,null,null,null,"Coincident"]
[null,"Kywong","MWh",null,"Non-Coincident",2.807325366458201E-2,2.8073483343431412E-2,2.8073577323188877E-2,2.8073615777730244E-2,2.8073631512520222E-2,2.8073637950865604E-2,2.80736405853012E-2]
[null,null,null,null,"Coincident"]
[null,"Lake Cargelligo","MWh",null,"Non-Coincident",0.17487846106924465,0.17579868168776278,0.17648932630355252,0.17700766937881166,0.17739669658256638,0.17768866954889914,0.17790780130175918]
[null,null,null,null,"Coincident"]
[null,"Leeton","MWh",null,"Non-Coincident",0.18686700860644656,0.18723389703263751,0.18757786340946372,0.18790033983537568,0.18820266893576318,0.18848610945294986,0.18875184148694826]
[null,null,null,null,"Coincident"]
[null,"Lightning Ridge","MWh",null,"Non-Coincident",0.14026223756655795,0.14026223817649999,0.14026223817711017,0.14026223817711062,0.14026223817711062,0.14026223817711062,0.14026223817711062]
[null,null,null,null,"Coincident"]
[null,"Lennox Head","MWh",null,"Non-Coincident",5.5986422141615332E-2,5.7995565597627682E-2,5.9852677716150826E-2,6.1569262667038827E-2,6.315595410274942E-2,6.462258103015836E-2,6.5978228697871275E-2]
[null,null,null,null,"Coincident"]
[null,"Lismore Uni","MWh",null,"Non-Coincident",0.15754960179335162,0.15755054021648895,0.15755115768798358,0.15755156397703579,0.15755183131049935,0.15755200721280502,0.15755212295447249]
[null,null,null,null,"Coincident"]
[null,"Lake Cathie","MWh",null,"Non-Coincident",0.21946080659108924,0.22343912348279296,0.22694513466507341,0.23003491226321107,0.23275787152078553,0.23515756110455432,0.23727235958434328]
[null,null,null,null,"Coincident"]
[null,"Lockhart","MWh",null,"Non-Coincident",0.1359232835084124,0.13475634680320769,0.13359057703470842,0.13242597303597753,0.13126253364124538,0.13010025768590808,0.12893914400652604]
[null,null,null,null,"Coincident"]
[null,"Laurieton","MWh",null,"Non-Coincident",8.0969753643416381E-2,8.0969774185257859E-2,8.0969778040822907E-2,8.0969778764486411E-2,8.0969778900313261E-2,8.0969778925806993E-2,8.0969778930592012E-2]
[null,null,null,null,"Coincident"]
[null,"Maher Street","MWh",null,"Non-Coincident",0.14576675587117813,0.14649056076456304,0.14714845965711329,0.14774645361484168,0.14828999727714229,0.14878404861162289,0.14923311413851797]
[null,null,null,null,"Coincident"]
[null,"Marilba","MWh",null,"Non-Coincident",5.7304998243211815E-2,5.7307223766980921E-2,5.7308536186912923E-2,5.7309310137791988E-2,5.7309766546559809E-2,5.7310035696667844E-2,5.7310194417941468E-2]
[null,null,null,null,"Coincident"]
[null,"Mumbil","MWh",null,"Non-Coincident",5.4652266629946447E-2,5.3104344763732991E-2,5.1634748532793789E-2,5.0239514620066587E-2,4.8914880254355107E-2,4.7657273062600571E-2,4.6463301435643825E-2]
[null,null,null,null,"Coincident"]
[null,"Murrumbateman","MWh",null,"Non-Coincident",0.49464011810894193,0.49464925687067135,0.49465486945537496,0.49465831643298314,0.49466043339963173,0.49466173353798559,0.4946625320199744]
[null,null,null,null,"Coincident"]
[null,"Martins Creek","MWh",null,"Non-Coincident",3.0933411821227722E-2,3.1182433443085557E-2,3.1418229252716839E-2,3.1641501687555501E-2,3.1852915877810827E-2,3.2053101627895049E-2,3.2242655292615337E-2]
[null,null,null,null,"Coincident"]
[null,"Macksville","MWh",null,"Non-Coincident",9.0578820418061326E-2,9.3604920407319006E-2,9.6454653888284059E-2,9.9138299815833705E-2,0.10166553806901157,0.10404548436623355,0.10628672314557465]
[null,null,null,null,"Coincident"]
[null,"Manildra","MWh",null,"Non-Coincident",0.10314081881429446,0.10329862514244338,0.10344892222798151,0.1035920673995735,0.10372840098233542,0.10385824710695145,0.10398191448028922]
[null,null,null,null,"Coincident"]
[null,"Murrurundi","MWh",null,"Non-Coincident",2.3181449507858821E-2,2.3181449480347411E-2,2.3181449469165134E-2,2.3181449464619967E-2,2.318144946277249E-2,2.3181449462021594E-2,2.3181449461716359E-2]
[null,null,null,null,"Coincident"]
[null,"Menindee","MWh",null,"Non-Coincident",4.1537423141318745E-2,4.1453219264624905E-2,4.1381365747538632E-2,4.1320051136853449E-2,4.1267729669012716E-2,4.1223082300850047E-2,4.118498345603324E-2]
[null,null,null,null,"Coincident"]
[null,"Munga","MWh",null,"Non-Coincident",6.4856301501201211E-2,6.4886111655332243E-2,6.4910678504221553E-2,6.4930924292341388E-2,6.4947609050668889E-2,6.4961359128403465E-2,6.4972690706242869E-2]
[null,null,null,null,"Coincident"]
[null,"Mallanganee","MWh",null,"Non-Coincident",1.4029843684110629E-2,1.4186776169901008E-2,1.4325942453949287E-2,1.4449353833806352E-2,1.4558793909629258E-2,1.4655844361621515E-2,1.4741907809230447E-2]
[null,null,null,null,"Coincident"]
[null,"Murgha","MWh",null,"Non-Coincident",4.4858621549040766E-2,4.4858618414552083E-2,4.4858616819193571E-2,4.4858616007205122E-2,4.4858615593927939E-2,4.4858615383582587E-2,4.4858615276523191E-2]
[null,null,null,null,"Coincident"]
[null,"Mungindi","MWh",null,"Non-Coincident",0.28525847326468451,0.29313913521857921,0.3005942271944767,0.30764673073976934,0.31431838635678438,0.32062976052146136,0.32660030908289472]
[null,null,null,null,"Coincident"]
[null,"Mates Gully","MWh",null,"Non-Coincident",5.2524042996852573E-2,5.3196720327546902E-2,5.3827976689457865E-2,5.4420362631825848E-2,5.4976271650553188E-2,5.5497949858963967E-2,5.598750506307603E-2]
[null,null,null,null,"Coincident"]
[null,"Manilla","MWh",null,"Non-Coincident",4.608617632120577E-2,4.7953658308816136E-2,4.9724160326844007E-2,5.1402718629755581E-2,5.2994107934926586E-2,5.4502855004492028E-2,5.5933251521878231E-2]
[null,null,null,null,"Coincident"]
[null,"Maclean 66/11kV","MWh",null,"Non-Coincident",7.7339164431594942E-2,7.8368103232412153E-2,7.8902724406066091E-2,7.918050555212866E-2,7.9324836470749768E-2,7.9399828652059815E-2,7.9438793465083729E-2]
[null,null,null,null,"Coincident"]
[null,"Maclean 66/33kV","MWh",null,"Non-Coincident",3.5949231828469472E-2,3.5488081952582448E-2,3.5111456239266987E-2,3.4803862254431647E-2,3.4552647172290833E-2,3.4347477303547112E-2,3.4179913020855296E-2]
[null,null,null,null,"Coincident"]
[null,"Molong 11kV","MWh",null,"Non-Coincident",3.2112921263978966E-2,3.2112922320280686E-2,3.211292260445088E-2,3.2112922680899485E-2,3.2112922701465901E-2,3.2112922706998781E-2,3.211292270848725E-2]
[null,null,null,null,"Coincident"]
[null,"Miller St","MWh",null,"Non-Coincident",0.1287530727760075,0.13355766370260816,0.13809209074321155,0.14237154531086668,0.14641036459997095,0.15022207961929351,0.15381946052408629]
[null,null,null,null,"Coincident"]
[null,"Moonee","MWh",null,"Non-Coincident",4.605181412642579E-2,4.739781849508138E-2,4.8091009770045524E-2,4.8448002774582596E-2,4.863185391335384E-2,4.872653711665996E-2,4.877529889778482E-2]
[null,null,null,null,"Coincident"]
[null,"Moama","MWh",null,"Non-Coincident",0.13430216695500738,0.13537581000955265,0.13639082401394984,0.13735041055880856,0.13825759640361859,0.13911524302385717,0.13992605563674623]
[null,null,null,null,"Coincident"]
[null,"Monteagle","MWh",null,"Non-Coincident",6.5881829944478248E-2,6.5881468279356273E-2,6.5881221133524362E-2,6.5881052245073193E-2,6.5880936834229825E-2,6.5880857967600986E-2,6.5880804073660398E-2]
[null,null,null,null,"Coincident"]
[null,"Moruya North","MWh",null,"Non-Coincident",0.19941088267730767,0.19941088267730767,0.19941088267730767,0.19941088267730767,0.19941088267730767,0.19941088267730767,0.19941088267730767]
[null,null,null,null,"Coincident"]
[null,"Moulamein","MWh",null,"Non-Coincident",0.12527584119813401,0.12680052792341207,0.1282418888064,0.12960447769798211,0.13089259957597779,0.13211032414633145,0.13326149870098655]
[null,null,null,null,"Coincident"]
[null,"Mossy Point","MWh",null,"Non-Coincident",0.29376291405567695,0.29880062791070172,0.30367688437751078,0.30839685812242262,0.31296555796507824,0.31738783219378192,0.32166837371048834]
[null,null,null,null,"Coincident"]
[null,"Moree","MWh",null,"Non-Coincident",0.19236537057734202,0.19239488052836973,0.19241833823159882,0.19243698495318268,0.19245180738581535,0.19246358985964993,0.19247295584518564]
[null,null,null,null,"Coincident"]
[null,"Murrumburrah","MWh",null,"Non-Coincident",4.5217555631779614E-2,4.5217555622808353E-2,4.5217555622799367E-2,4.5217555622799367E-2,4.5217555622799367E-2,4.5217555622799367E-2,4.5217555622799367E-2]
[null,null,null,null,"Coincident"]
[null,"Marulan North","MWh",null,"Non-Coincident",4.9788352398772821E-2,5.2288397861155883E-2,5.4744790834908158E-2,5.715829352207448E-2,5.9529654816135404E-2,6.1859610534383359E-2,6.4148883646242244E-2]
[null,null,null,null,"Coincident"]
[null,"Morrow St","MWh",null,"Non-Coincident",0.13676832635747904,0.14039439029726669,0.1437067356723051,0.14673250467851379,0.14949649123254941,0.15202134413943658,0.15432775268259952]
[null,null,null,null,"Coincident"]
[null,"Mt Gipps 33","MWh",null,"Non-Coincident",4.99060175061498E-2,5.2700017457465553E-2,5.5491223408830309E-2,5.8279638154243425E-2,6.1065264484911508E-2,6.3848105189248383E-2,6.6628163052881439E-2]
[null,null,null,null,"Coincident"]
[null,"Mt Gipps 6.6","MWh",null,"Non-Coincident",4.018736111620886E-2,4.0185576754375556E-2,4.0184296769149357E-2,4.0183378590925301E-2,4.0182719949533208E-2,4.0182247482998985E-2,4.0181908566209595E-2]
[null,null,null,null,"Coincident"]
[null,"Mandurama","MWh",null,"Non-Coincident",8.2119808775467193E-2,8.2100139369068278E-2,8.2082795784196486E-2,8.2067503002599199E-2,8.2054018525733338E-2,8.2042128529449726E-2,8.2031644473373591E-2]
[null,null,null,null,"Coincident"]
[null,"Mudgee","MWh",null,"Non-Coincident",0.21715215452371603,0.2217043939533469,0.22619055529513138,0.23061159770637241,0.23496846642171157,0.23926209295522877,0.2434933952995969]
[null,null,null,null,"Coincident"]
[null,"Mullumbimby","MWh",null,"Non-Coincident",7.6345275406836957E-2,7.6432965195461111E-2,7.6466065424747653E-2,7.6478559754999953E-2,7.6483275984821325E-2,7.6485056218197386E-2,7.648572820217471E-2]
[null,null,null,null,"Coincident"]
[null,"Marulan South 33kV","MWh",null,"Non-Coincident",0.64412275911352546,0.63719870228580344,0.6315749568656509,0.62700732934069037,0.62329748480683123,0.62028433489690593,0.61783704302340015]
[null,null,null,null,"Coincident"]
[null,"Murrami","MWh",null,"Non-Coincident",3.0753285245781511E-2,3.0392681800629515E-2,3.0036636479461115E-2,2.9685091666370275E-2,2.9337990473731212E-2,2.8995276732993118E-2,2.8656894985590604E-2]
[null,null,null,null,"Coincident"]
[null,"Morven","MWh",null,"Non-Coincident",0.63116519118802539,0.63116519146152583,0.63116519151205652,0.63116519152139305,0.63116519152311745,0.63116519152343642,0.63116519152349482]
[null,null,null,null,"Coincident"]
[null,"Mulwala","MWh",null,"Non-Coincident",0.12291770153743355,0.12311868023010801,0.12330353042277983,0.12347354642435696,0.1236299186757156,0.12377374208508993,0.12390602369454698]
[null,null,null,null,"Coincident"]
[null,"Merrywinebone","MWh",null,"Non-Coincident",0.25365476203089254,0.25960108393153564,0.26554145951027774,0.27147589471344213,0.27740439548140228,0.28332696774859484,0.28924361744352101]
[null,null,null,null,"Coincident"]
[null,"Murwillumbah","MWh",null,"Non-Coincident",0.16726589067972639,0.16671755139560829,0.16618979169240464,0.16568183920314819,0.16519295054837546,0.16472241024820938,0.16426952967526165]
[null,null,null,null,"Coincident"]
[null,"Moruya Town","MWh",null,"Non-Coincident",6.1123701875489697E-2,6.1123701873300795E-2,6.1123701872715271E-2,6.1123701872558681E-2,6.1123701872516825E-2,6.1123701872505577E-2,6.1123701872502545E-2]
[null,null,null,null,"Coincident"]
[null,"Nangus","MWh",null,"Non-Coincident",5.0991516459512269E-2,5.0420791529757286E-2,4.9850637324932091E-2,4.9281053274311495E-2,4.8712038807741859E-2,4.8143593355638697E-2,4.757571634898719E-2]
[null,null,null,null,"Coincident"]
[null,"Narooma","MWh",null,"Non-Coincident",7.0417299407768433E-2,7.0451110512808363E-2,7.0460336505853954E-2,7.0462853990792051E-2,7.0463540933691574E-2,7.0463728378923146E-2,7.0463779526864057E-2]
[null,null,null,null,"Coincident"]
[null,"Narrabri","MWh",null,"Non-Coincident",0.18569084483779769,0.18614791057530433,0.18656353822637539,0.18694148461386051,0.18728516596288908,0.18759768877983107,0.18788187793174535]
[null,null,null,null,"Coincident"]
[null,"Narrandera","MWh",null,"Non-Coincident",8.9534624723444714E-2,8.9178132583026953E-2,8.8899093679416452E-2,8.8680680141219284E-2,8.8509720203194309E-2,8.8375903862637994E-2,8.8271161118772062E-2]
[null,null,null,null,"Coincident"]
[null,"Nundle","MWh",null,"Non-Coincident",6.6871291602301555E-2,6.5199933991517786E-2,6.3671256207736004E-2,6.2273078013225173E-2,6.0994258968200744E-2,5.9824609665746376E-2,5.8754810544396338E-2]
[null,null,null,null,"Coincident"]
[null,"Nericon","MWh",null,"Non-Coincident",0.1399972985815395,0.13685819763489784,0.13442658525341106,0.13254300811642056,0.13108395039077039,0.12995373416284386,0.12907824534604614]
[null,null,null,null,"Coincident"]
[null,"Nana Glen","MWh",null,"Non-Coincident",0.15288159082194772,0.17325643353448475,0.19248159891762848,0.21062195902857064,0.22773872543325316,0.24388965575440696,0.2591292485648462]
[null,null,null,null,"Coincident"]
[null,"Nambucca Heads","MWh",null,"Non-Coincident",8.1178259611290576E-2,8.153003404902523E-2,8.1731561942938749E-2,8.1847015164289313E-2,8.1913157106535503E-2,8.1951049133045531E-2,8.1972757078477523E-2]
[null,null,null,null,"Coincident"]
[null,"Narromine","MWh",null,"Non-Coincident",0.13029797907991841,0.13042972762876601,0.13054197114526081,0.13063759729906096,0.13071906624779134,0.13078847392909518,0.13084760598246162]
[null,null,null,null,"Coincident"]
[null,"North St","MWh",null,"Non-Coincident",0.10459222580659704,0.10616627679208143,0.1076829184652946,0.10914424467781024,0.11055227291355207,0.11190894707409638,0.11321614016239245]
[null,null,null,null,"Coincident"]
[null,"Nevertire","MWh",null,"Non-Coincident",0.78013989516305438,0.80144790326713966,0.82104962251743707,0.83908168800617811,0.85566979344929128,0.87092956734283999,0.88496737895917132]
[null,null,null,null,"Coincident"]
[null,"Nymboida","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Nyngan Town","MWh",null,"Non-Coincident",0.3498121869044562,0.37868578330438812,0.4075305061079203,0.43634638418864852,0.46513344639129561,0.49389172153174044,0.52262123839704866]
[null,null,null,null,"Coincident"]
[null,"Oberon 132kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Oberon Town","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Oaks Estate","MWh",null,"Non-Coincident",0.82718054564600929,0.82718054564600929,0.82718054564600929,0.82718054564600929,0.82718054564600929,0.82718054564600929,0.82718054564600929]
[null,null,null,null,"Coincident"]
[null,"Oaky","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Owen St","MWh",null,"Non-Coincident",0.13472215881196087,0.13252393587939218,0.13046434334782445,0.12853463852433236,0.12672663007181814,0.12503264323789134,0.12344548727657507]
[null,null,null,null,"Coincident"]
[null,"Orange Industrial","MWh",null,"Non-Coincident",0.54037992504579269,0.54736641264242214,0.55434591375145259,0.5613184353593772,0.56828398444569117,0.57524256798292372,0.58219419293661534]
[null,null,null,null,"Coincident"]
[null,"Orange North","MWh",null,"Non-Coincident",0.1491794783150002,0.14917948047833199,0.14917948140601675,0.14917948180382867,0.14917948197441913,0.14917948204757156,0.1491794820789418]
[null,null,null,null,"Coincident"]
[null,"Orange South","MWh",null,"Non-Coincident",0.18921562192258051,0.17793878591327675,0.16667322673998214,0.15541893312586139,0.14417589380535403,0.13294409752416778,0.12172353303926245]
[null,null,null,null,"Coincident"]
[null,"Orange West","MWh",null,"Non-Coincident",0.13504725952259031,0.13504725952198363,0.13504725952190896,0.13504725952189953,0.13504725952189858,0.13504725952189858,0.13504725952189858]
[null,null,null,null,"Coincident"]
[null,"Oura 66/11kV","MWh",null,"Non-Coincident",0.17354820762308668,0.17225547663698057,0.17102693442784131,0.16985939379033943,0.16874982577543682,0.16769535183238976,0.1666932363409272]
[null,null,null,null,"Coincident"]
[null,"Oura 11/33kV","MWh",null,"Non-Coincident",6.8972099189500327E-2,6.8979632348927303E-2,6.8984132292158259E-2,6.8986820339487956E-2,6.8988426048288115E-2,6.8989385220666832E-2,6.8989958183617375E-2]
[null,null,null,null,"Coincident"]
[null,"Oxley Vale","MWh",null,"Non-Coincident",0.17215665457799464,0.1721629817499627,0.17216347609862542,0.17216351472261152,0.17216351774034433,0.17216351797612278,0.17216351799454457]
[null,null,null,null,"Coincident"]
[null,"Pambula","MWh",null,"Non-Coincident",0.29219219646675704,0.29219310880716326,0.29219347804925916,0.2921936274887949,0.29219368796991563,0.29219371244780989,0.29219372235449759]
[null,null,null,null,"Coincident"]
[null,"Parsons Creek","MWh",null,"Non-Coincident",9.0040175425115318E-3,8.7481203840217812E-3,8.5180176591077555E-3,8.3111092888650696E-3,8.1250572823428381E-3,7.9577593180780622E-3,7.8073249886111643E-3]
[null,null,null,null,"Coincident"]
[null,"Perisher","MWh",null,"Non-Coincident",8.3079663918368945E-3,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Dubbo Phillip St","MWh",null,"Non-Coincident",0.21396531907395952,0.21186340057228065,0.21018416989179645,0.20884262611832083,0.2077708616984193,0.20691462502953301,0.20623057430016262]
[null,null,null,null,"Coincident"]
[null,"Peak Hill","MWh",null,"Non-Coincident",7.4063107263857078E-2,7.3783183604147748E-2,7.3543017279415326E-2,7.3336961586962707E-2,7.316017182078878E-2,7.3008491364637926E-2,7.2878353963157477E-2]
[null,null,null,null,"Coincident"]
[null,"Parkes Town","MWh",null,"Non-Coincident",0.17575125169952988,0.17597296963583567,0.17616832830144072,0.17634046145793053,0.17649213030492905,0.17662576777268157,0.17674351754886097]
[null,null,null,null,"Coincident"]
[null,"Pinnacles Place","MWh",null,"Non-Coincident",0.24323860560530805,0.2333485400051119,0.22843994799543596,0.22600373811660784,0.22479460960032488,0.22419450047935169,0.2238966570721167]
[null,null,null,null,"Coincident"]
[null,"Pacific Palms","MWh",null,"Non-Coincident",4.1447127530600258E-2,4.1339367882533236E-2,4.1242064625248979E-2,4.1154203129337076E-2,4.1074867219323893E-2,4.1003229620256404E-2,4.093854333129459E-2]
[null,null,null,null,"Coincident"]
[null,"Providence Portal","MWh",null,"Non-Coincident",0.34790757854223503,0.35691168144523666,0.36431245339745627,0.37039539426106005,0.37539516587799365,0.37950464462881617,0.3828823620322]
[null,null,null,null,"Coincident"]
[null,"Prince St","MWh",null,"Non-Coincident",8.2406164517786623E-2,8.307515018038894E-2,8.3622216288383039E-2,8.4069582118842884E-2,8.4435417587972655E-2,8.4734581228467651E-2,8.4979223673901053E-2]
[null,null,null,null,"Coincident"]
[null,"Paytens Bridge","MWh",null,"Non-Coincident",0.23363481148757478,0.24657485478267371,0.25773961612255541,0.26737265157180579,0.27568410303427765,0.28285528243841918,0.28904262700495864]
[null,null,null,null,"Coincident"]
[null,"Quirindi 66/11kV","MWh",null,"Non-Coincident",0.30400274420763107,0.30400274421863299,0.30400274421864393,0.30400274421864393,0.30400274421864393,0.30400274421864393,0.30400274421864393]
[null,null,null,null,"Coincident"]
[null,"Quirindi 66/33kV","MWh",null,"Non-Coincident",4.6614987194712652E-2,4.6614987092463839E-2,4.6614987037301256E-2,4.6614987007541415E-2,4.661498699148605E-2,4.6614986982824361E-2,4.6614986978151446E-2]
[null,null,null,null,"Coincident"]
[null,"Queanbeyan South","MWh",null,"Non-Coincident",0.25292703421764673,0.2533583349985285,0.25375507757696597,0.25412003094714836,0.25445574223614659,0.25476455448113106,0.25504862298218323]
[null,null,null,null,"Coincident"]
[null,"Quira","MWh",null,"Non-Coincident",5.6721187005428858E-2,5.861217390232204E-2,6.0312223904590845E-2,6.1840616309087069E-2,6.3214683741812785E-2,6.4450008717337887E-2,6.5560600351206422E-2]
[null,null,null,null,"Coincident"]
[null,"Raglan","MWh",null,"Non-Coincident",0.18414580458842539,0.18414580421689961,0.18414580407673434,0.18414580402385403,0.18414580400390415,0.18414580399637812,0.18414580399353844]
[null,null,null,null,"Coincident"]
[null,"Redcliff","MWh",null,"Non-Coincident",1.8972306809549869E-2,1.8755938533183945E-2,1.8579423149398113E-2,1.8435420150269121E-2,1.8317941076698402E-2,1.8222100484415464E-2,1.8143912779576221E-2]
[null,null,null,null,"Coincident"]
[null,"Raleigh","MWh",null,"Non-Coincident",0.10360697196568101,0.10735986556266836,0.10990510315158435,0.11163130034226315,0.11280201884574588,0.11359600798082232,0.11413449673345001]
[null,null,null,null,"Coincident"]
[null,"Rocks Ferry","MWh",null,"Non-Coincident",0.10750081747279361,0.10805430085925485,0.10853159149142509,0.10894317809570467,0.10929810551603013,0.10960417347934384,0.10986810799891783]
[null,null,null,null,"Coincident"]
[null,"Rappville","MWh",null,"Non-Coincident",1.2273306838271041E-2,1.3050219003578853E-2,1.364968063188321E-2,1.4112222293419614E-2,1.4469117178021349E-2,1.4744495526064102E-2,1.4956976113045408E-2]
[null,null,null,null,"Coincident"]
[null,"Ringwood Road","MWh",null,"Non-Coincident",0.17440117351429174,0.17440098506984136,0.17440092105550181,0.1744008993099124,0.17440089192296315,0.17440088941362578,0.17440088856120731]
[null,null,null,null,"Coincident"]
[null,"Suffolk Park","MWh",null,"Non-Coincident",0.98332655928350432,0.98332656558377118,0.98332656718782796,0.98332656759622095,0.98332656770020144,0.98332656772667226,0.98332656773341232]
[null,null,null,null,"Coincident"]
[null,"Grafton South","MWh",null,"Non-Coincident",0.16089904581066006,0.16091110673189624,0.16091978714603664,0.16092603456181626,0.16093053091455858,0.16093376700267764,0.16093609606067649]
[null,null,null,null,"Coincident"]
[null,"Lismore South","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Smithtown","MWh",null,"Non-Coincident",0.17247917135176322,0.16796614203724264,0.16435668454183253,0.16146989110371895,0.1591610742344432,0.15731451491174556,0.15583766268599439]
[null,null,null,null,"Coincident"]
[null,"Snowy Adit 11kV","MWh",null,"Non-Coincident",2.2711938784011993E-3,2.2711938784010111E-3,2.2711938784010111E-3,2.2711938784010111E-3,2.2711938784010111E-3,2.2711938784010111E-3,2.2711938784010111E-3]
[null,null,null,null,"Coincident"]
[null,"Snowy Adit 66kV","MWh",null,"Non-Coincident",1.0193382653276202,1.0387396858110651,1.0567148334930727,1.0733685591553415,1.0887980055966537,1.1030931742762251,1.1163374503009442]
[null,null,null,null,"Coincident"]
[null,"Snapper","MWh",null,"Non-Coincident",0.48562735053623229,0.48562735053623401,0.48562735053623401,0.48562735053623401,0.48562735053623401,0.48562735053623401,0.48562735053623401]
[null,null,null,null,"Coincident"]
[null,"Spring Ridge","MWh",null,"Non-Coincident",7.11266217195652E-2,7.1126612898677402E-2,7.1126610361427964E-2,7.112660963161091E-2,7.1126609421685569E-2,7.1126609361302384E-2,7.1126609343933722E-2]
[null,null,null,null,"Coincident"]
[null,"Steeple Flat 22kV","MWh",null,"Non-Coincident",6.6151196060102072E-2,6.7742557134657516E-2,6.9332326848138406E-2,7.0920506791905771E-2,7.2507098555729427E-2,7.4092103727789196E-2,7.567552389467691E-2]
[null,null,null,null,"Coincident"]
[null,"Tamworth South","MWh",null,"Non-Coincident",0.2104821858485203,0.21083126405864419,0.21113222763060985,0.21139170836880319,0.21161542399343361,0.21180830413186871,0.21197459894415147]
[null,null,null,null,"Coincident"]
[null,"Sawtell","MWh",null,"Non-Coincident",8.0461702788488729E-2,8.4328860505743439E-2,8.7581708500661687E-2,9.0317831734227638E-2,9.2619313500653333E-2,9.4555197914122563E-2,9.6183561222049449E-2]
[null,null,null,null,"Coincident"]
[null,"Stroud 33/11kV","MWh",null,"Non-Coincident",0.13362433975192986,0.13499213936828666,0.13635857118502712,0.13772363656995082,0.13908733688948963,0.14044967350870913,0.14181064779130886]
[null,null,null,null,"Coincident"]
[null,"Sunset Strip 22","MWh",null,"Non-Coincident",6.073651430475125E-2,6.0736514021860796E-2,6.0736513942942251E-2,6.0736513920926195E-2,6.0736513914784351E-2,6.0736513913070972E-2,6.0736513912592917E-2]
[null,null,null,null,"Coincident"]
[null,"Sunset Strip 33","MWh",null,"Non-Coincident",8.6653949316931808E-2,8.8101136002924588E-2,8.9546875502230977E-2,9.0991169262038055E-2,9.2434018728085585E-2,9.3875425344666891E-2,9.5315390554631535E-2]
[null,null,null,null,"Coincident"]
[null,"Sutton","MWh",null,"Non-Coincident",0.31916691905402794,0.31916691905402794,0.31916691905402794,0.31916691905402794,0.31916691905402794,0.31916691905402794,0.31916691905402794]
[null,null,null,null,"Coincident"]
[null,"South West Rocks","MWh",null,"Non-Coincident",5.8488031165046146E-2,5.9119845026643678E-2,5.9664065482112817E-2,6.013283630553562E-2,6.0536617682520139E-2,6.0884419619528667E-2,6.1184002993804845E-2]
[null,null,null,null,"Coincident"]
[null,"Stewart","MWh",null,"Non-Coincident",0.16466053586352461,0.16506253725410172,0.16541932840969442,0.16573599380362786,0.16601704609470436,0.16626649043511046,0.16648788154607597]
[null,null,null,null,"Coincident"]
[null,"Talbingo","MWh",null,"Non-Coincident",9.5628090048534509E-2,9.7438816347576479E-2,9.9079461500174937E-2,0.10056600119320681,0.10191291052058954,0.10313330493366442,0.10423906795214467]
[null,null,null,null,"Coincident"]
[null,"Tarcutta","MWh",null,"Non-Coincident",4.4533123468339826E-2,4.4543903264819051E-2,4.4553764159809231E-2,4.456278448317013E-2,4.4571035887694455E-2,4.4578583918280422E-2,4.458548853258687E-2]
[null,null,null,null,"Coincident"]
[null,"Trundle","MWh",null,"Non-Coincident",0.11406491169963755,0.11796136991570476,0.12094282895230719,0.12322415663350385,0.1249697637087982,0.12630545260892104,0.12732748377685199]
[null,null,null,null,"Coincident"]
[null,"Tea Gardens","MWh",null,"Non-Coincident",9.5614023328450523E-2,9.7272119649892325E-2,9.8843180744107487E-2,0.10033177518210104,0.10174223172576141,0.10307865191569218,0.10434492199830102]
[null,null,null,null,"Coincident"]
[null,"Temora 66/11kV","MWh",null,"Non-Coincident",0.33436681049743749,0.33457182811101871,0.33475806668299185,0.33492724632119303,0.33508092957637847,0.3352205358740129,0.33534735462414694]
[null,null,null,null,"Coincident"]
[null,"Tharbogang","MWh",null,"Non-Coincident",0.13695890509438266,0.13157802825837484,0.12638251377402115,0.12136597621336094,0.11652225011591537,0.11184538241117369,0.10732962510210749]
[null,null,null,null,"Coincident"]
[null,"Tweed Heads","MWh",null,"Non-Coincident",0.70625038599273815,0.68898598044820181,0.67576162764972225,0.66563191270022271,0.65787265774674542,0.65192915018180497,0.64737648599093467]
[null,null,null,null,"Coincident"]
[null,"Thredbo","MWh",null,"Non-Coincident",6.1889355589811713E-2,6.1889355590089429E-2,6.1889355590093793E-2,6.1889355590093793E-2,6.1889355590093793E-2,6.1889355590093793E-2,6.1889355590093793E-2]
[null,null,null,null,"Coincident"]
[null,"Tumut","MWh",null,"Non-Coincident",0.84260297924585503,0.84120756866575519,0.83981355349623565,0.83842093234188386,0.8370297038086848,0.83563986650402466,0.83425141903666278]
[null,null,null,null,"Coincident"]
[null,"Terranora 11kV","MWh",null,"Non-Coincident",5.3032419114748229E-2,5.2597122599628246E-2,5.2192866059126541E-2,5.1817436105377979E-2,5.1468777182020344E-2,5.1144980309599332E-2,5.0844272633513043E-2]
[null,null,null,null,"Coincident"]
[null,"Telegraph Point","MWh",null,"Non-Coincident",1.8674213210687223E-2,1.8955939429179492E-2,1.9047532379167533E-2,1.9077310468450178E-2,1.9086991722317866E-2,1.9090139227033894E-2,1.9091162522783894E-2]
[null,null,null,null,"Coincident"]
[null,"Tweed Heads South","MWh",null,"Non-Coincident",0.12543630537327718,0.12327350071364591,0.12143431263787645,0.11987031897668741,0.11854034288317966,0.11740936872823454,0.11644762020854382]
[null,null,null,null,"Coincident"]
[null,"Tumbarumba","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Tuncurry","MWh",null,"Non-Coincident",6.7523457463604108E-2,6.7523385514895853E-2,6.752337750276903E-2,6.752337661054765E-2,6.7523376511190822E-2,6.7523376500126575E-2,6.7523376498894477E-2]
[null,null,null,null,"Coincident"]
[null,"Tuross","MWh",null,"Non-Coincident",0.17573388552806574,0.17573388620448152,0.17573388644360483,0.17573388652813796,0.17573388655802186,0.17573388656858627,0.1757338865723207]
[null,null,null,null,"Coincident"]
[null,"Texas 66/22kV","MWh",null,"Non-Coincident",0.14467063959767285,0.14467063988480058,0.14467063997179522,0.14467063999815294,0.14467064000613908,0.14467064000855878,0.14467064000929178]
[null,null,null,null,"Coincident"]
[null,"Texas 66/33kV","MWh",null,"Non-Coincident",0.10014425057957185,0.10014424960740884,0.1001442496064365,0.10014424960643559,0.10014424960643559,0.10014424960643559,0.10014424960643559]
[null,null,null,null,"Coincident"]
[null,"Urbenville","MWh",null,"Non-Coincident",7.0553409410327823E-3,7.086399979361618E-3,7.1130549167871485E-3,7.1359302447878692E-3,7.1555619033727954E-3,7.1724098374781695E-3,7.1868687728957378E-3]
[null,null,null,null,"Coincident"]
[null,"Ulong","MWh",null,"Non-Coincident",3.5040300437749083E-2,3.6074977525017655E-2,3.7059520865694674E-2,3.7996359616256456E-2,3.8887805231998043E-2,3.9736057170069956E-2,4.0543208316182487E-2]
[null,null,null,null,"Coincident"]
[null,"Ulan Town","MWh",null,"Non-Coincident",0.1027561019140797,0.10717251976370938,0.11157169256110788,0.11595368764406747,0.12031857208744147,0.12466641270417289,0.12899727604631642]
[null,null,null,null,"Coincident"]
[null,"Upper Manilla","MWh",null,"Non-Coincident",6.237321043412801E-2,6.2373210409866778E-2,6.2373210409842512E-2,6.2373210409842422E-2,6.2373210409842422E-2,6.2373210409842422E-2,6.2373210409842422E-2]
[null,null,null,null,"Coincident"]
[null,"Madgwick Dr","MWh",null,"Non-Coincident",0.11574953796602763,0.11574953797440601,0.11574953797441452,0.11574953797441452,0.11574953797441452,0.11574953797441452,0.11574953797441452]
[null,null,null,null,"Coincident"]
[null,"Uranquinty","MWh",null,"Non-Coincident",4.7405743673152416E-2,4.7405743700353858E-2,4.7405743709862641E-2,4.7405743713186579E-2,4.7405743714348449E-2,4.7405743714754624E-2,4.7405743714896656E-2]
[null,null,null,null,"Coincident"]
[null,"Uralla","MWh",null,"Non-Coincident",0.14629551563296214,0.14629568785579067,0.14629576132078681,0.14629579265870934,0.14629580602650924,0.14629581172880449,0.14629581416122947]
[null,null,null,null,"Coincident"]
[null,"Warrawidgee","MWh",null,"Non-Coincident",5.3910347985665998E-2,5.3909802331664827E-2,5.3909590659147411E-2,5.3909508546206963E-2,5.3909476692591517E-2,5.3909464335795715E-2,5.3909459542292905E-2]
[null,null,null,null,"Coincident"]
[null,"Willbriggie","MWh",null,"Non-Coincident",0.10541973686939869,0.10617178431169395,0.10681448961250613,0.10736375031131487,0.10783315256281971,0.10823430719521245,0.10857713690805186]
[null,null,null,null,"Coincident"]
[null,"Woodburn","MWh",null,"Non-Coincident",6.0093994029539431E-2,6.009399402954E-2,6.009399402954E-2,6.009399402954E-2,6.009399402954E-2,6.009399402954E-2,6.009399402954E-2]
[null,null,null,null,"Coincident"]
[null,"Werris Creek","MWh",null,"Non-Coincident",0.10939812790052603,0.11028642262870415,0.1111037761897236,0.1118558541009373,0.11254786941904645,0.11318461887459683,0.11377051612070418]
[null,null,null,null,"Coincident"]
[null,"Woolgoolga","MWh",null,"Non-Coincident",0.10240175828627293,0.10240176025012845,0.10240176100167375,0.10240176128928168,0.10240176139934674,0.10240176144146634,0.10240176145758616]
[null,null,null,null,"Coincident"]
[null,"Wingham","MWh",null,"Non-Coincident",3.5986885459091601E-2,3.5987098712661175E-2,3.5987132005479892E-2,3.5987137203102759E-2,3.5987138014547781E-2,3.5987138141229766E-2,3.5987138161006731E-2]
[null,null,null,null,"Coincident"]
[null,"Wellington 11kV","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Walgett","MWh",null,"Non-Coincident",0.23803261262605599,0.23803261758287014,0.23803262067868783,0.2380326226122049,0.23803262381979806,0.23803262457400973,0.23803262504505895]
[null,null,null,null,"Coincident"]
[null,"Whitton","MWh",null,"Non-Coincident",0.22194368631188163,0.2219436863118639,0.2219436863118639,0.2219436863118639,0.2219436863118639,0.2219436863118639,0.2219436863118639]
[null,null,null,null,"Coincident"]
[null,"Widgelli","MWh",null,"Non-Coincident",1.9636360775113496E-2,1.9636360775113392E-2,1.9636360775113392E-2,1.9636360775113392E-2,1.9636360775113392E-2,1.9636360775113392E-2,1.9636360775113392E-2]
[null,null,null,null,"Coincident"]
[null,"West Jemalong","MWh",null,"Non-Coincident",1.9189864957721882E-2,1.9189864866741253E-2,1.918986483718883E-2,1.9189864827589522E-2,1.9189864824471495E-2,1.918986482345874E-2,1.918986482312969E-2]
[null,null,null,null,"Coincident"]
[null,"Wilcannia","MWh",null,"Non-Coincident",1.2041331594255498E-2,1.2041276210909441E-2,1.2041256849479171E-2,1.2041250080928484E-2,1.2041247714714917E-2,1.2041246887511814E-2,1.204124659833038E-2]
[null,null,null,null,"Coincident"]
[null,"Wallangra","MWh",null,"Non-Coincident",1.3592701490495462E-2,1.3592701770837766E-2,1.3592701869147825E-2,1.3592701903623097E-2,1.359270191571282E-2,1.3592701919952386E-2,1.359270192143912E-2]
[null,null,null,null,"Coincident"]
[null,"Walcha South 66/22kV","MWh",null,"Non-Coincident",1.3567840620527214E-2,1.3903759330125179E-2,1.4206004721793019E-2,1.4477952291768535E-2,1.4722639168241689E-2,1.494279803020007E-2,1.5140887626166314E-2]
[null,null,null,null,"Coincident"]
[null,"Wenna","MWh",null,"Non-Coincident",0.18656273430078713,0.19249110245261555,0.19757026676605735,0.2019218706918339,0.20565013297244406,0.20884434362904555,0.21158100241290029]
[null,null,null,null,"Coincident"]
[null,"Woodlawn","MWh",null,"Non-Coincident",0.38025615418080011,0.38025615418079922,0.38025615418079922,0.38025615418079922,0.38025615418079922,0.38025615418079922,0.38025615418079922]
[null,null,null,null,"Coincident"]
[null,"Warialda","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"Whitbread St","MWh",null,"Non-Coincident",2.4622171220611444E-2,2.5150986934257855E-2,2.542719213364306E-2,2.5571456591370497E-2,2.5646807214058896E-2,2.5686163521418698E-2,2.5706719674425171E-2]
[null,null,null,null,"Coincident"]
[null,"Wathagar","MWh",null,"Non-Coincident",0.48393093416511918,0.49668177028315519,0.50905992195057148,0.52107628207654233,0.53274142518971912,0.54406561674393261,0.55505882215190228]
[null,null,null,null,"Coincident"]
[null,"Wee Waa","MWh",null,"Non-Coincident",0,0,0,0,0,0,0]
[null,null,null,null,"Coincident"]
[null,"West Wyalong","MWh",null,"Non-Coincident",0.36209011162392435,0.35451607073651359,0.34694960388999008,0.33939070351031297,0.33183936203101549,0.32429557189319747,0.31675932554551745]
[null,null,null,null,"Coincident"]
[null,"Yamba","MWh",null,"Non-Coincident",0.10193496699377913,0.10491882202745938,0.10789969320610517,0.1108775835135738,0.11385249593073363,0.11682443343547715,0.11979339900271538]
[null,null,null,null,"Coincident"]
[null,"Yanco 33/11kV","MWh",null,"Non-Coincident",0.22820043714567545,0.23376641949784582,0.2388252921160583,0.24342325713786978,0.24760230728151045,0.25140060936084774,0.25485285285877435]
[null,null,null,null,"Coincident"]
[null,"Yarrandale","MWh",null,"Non-Coincident",7.8749571106802127E-2,7.7747942616194429E-2,7.6752607042696569E-2,7.5763524849887479E-2,7.4780656749740979E-2,7.3803963701065317E-2,7.283340690795212E-2]
[null,null,null,null,"Coincident"]
[null,"Yass","MWh",null,"Non-Coincident",0.51292691733914086,0.51749881098561101,0.52178814663900019,0.52581238730821256,0.52958791673104144,0.53313010607664535,0.5364533765256212]
[null,null,null,null,"Coincident"]
[null,"Yenda","MWh",null,"Non-Coincident",6.6200917516761881E-2,6.3846407603388888E-2,6.1531987911476925E-2,5.9256975825145879E-2,5.7020700351410838E-2,5.4822501922278923E-2,5.266173220021627E-2]
[null,null,null,null,"Coincident"]
[null,"Yallaroi","MWh",null,"Non-Coincident",0.17502657709988928,0.17502657717650602,0.17502657719479564,0.17502657719916123,0.1750265772002039,0.17502657720045256,0.17502657720051176]
[null,null,null,null,"Coincident"]
[null,"Yanco 33/66kV","MWh",null,"Non-Coincident",0.8401510999973304,0.84088242165890359,0.84150872859932058,0.84204510049178005,0.84250445163170007,0.84289784187587968,0.84323474293210254]
[null,null,null,null,"Coincident"]
[null,"Young","MWh",null,"Non-Coincident",0.1536310844593374,0.1524751556904195,0.15171579752057884,0.15121695637603172,0.15088925530244415,0.15067398037012619,0.15053256094791506]
[null,null,null,null,"Coincident"]

{"sheet":"6.1 Telephone answering","index":31,"n_rows":1834,"n_cols":4,"rows_kept":1834,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"6.1 TELEPHONE ANSWERING"]
[]
[]
[null,"6.1.1 - TELEPHONE ANSWERING DATA"]
["C10 starts at first day of PRCP_y5 and goes for 5 full years","Date","Total number of calls \n(after removing excluded events)","Number of calls answered within 30 seconds \n(after excluding excluded events) "]
[null,{"$f":"IF(dms_RPT=\"calendar\",DATE(VALUE(PRCP_y3),1,1),(DATE(VALUE(LEFT(PRCP_y3,2)&RIGHT(PRCP_y3,2)),7,1)))","v":"2012-07-01"},1034,428]
[null,{"$f":"B9+1","v":"2012-07-02"},870,686]
[null,"2012-07-03",1169,744]
[null,"2012-07-04",937,612]
[null,"2012-07-05",1142,618]
[null,"2012-07-06",1206,695]
[null,"2012-07-07",391,348]
[null,{"$f":"B15+1","v":"2012-07-08"},391,311]
[null,"2012-07-09",878,730]
[null,"2012-07-10",1415,872]
[null,"2012-07-11",1114,643]
[null,"2012-07-12",1445,888]
[null,"2012-07-13",2544,846]
[null,"2012-07-14",1147,516]
[null,"2012-07-15",508,443]
[null,"2012-07-16",796,695]
[null,"2012-07-17",840,473]
[null,"2012-07-18",1220,551]
[null,"2012-07-19",903,335]
[null,"2012-07-20",1173,760]
[null,"2012-07-21",482,330]
[null,"2012-07-22",392,301]
[null,"2012-07-23",819,507]
[null,"2012-07-24",674,528]
[null,"2012-07-25",808,574]
[null,"2012-07-26",1729,754]
[null,"2012-07-27",1027,621]
[null,"2012-07-28",278,255]
[null,"2012-07-29",230,215]
[null,"2012-07-30",1597,769]
[null,"2012-07-31",1200,503]
[null,"2012-08-01",746,558]
[null,"2012-08-02",1095,543]
[null,"2012-08-03",789,486]
[null,"2012-08-04",283,265]
[null,"2012-08-05",358,312]
[null,"2012-08-06",864,575]
[null,"2012-08-07",677,494]
[null,"2012-08-08",919,506]
[null,"2012-08-09",885,536]
[null,"2012-08-10",1391,761]
[null,"2012-08-11",603,518]
[null,"2012-08-12",277,249]
[null,"2012-08-13",669,503]
[null,"2012-08-14",1681,553]
[null,"2012-08-15",1391,1021]
[null,"2012-08-16",891,484]
[null,"2012-08-17",1050,791]
[null,"2012-08-18",600,533]
[null,"2012-08-19",284,276]
[null,"2012-08-20",594,330]
[null,"2012-08-21",713,592]
[null,"2012-08-22",2042,682]
[null,"2012-08-23",1960,991]
[null,"2012-08-24",1074,588]
[null,"2012-08-25",242,226]
[null,"2012-08-26",303,297]
[null,"2012-08-27",996,668]
[null,"2012-08-28",614,551]
[null,"2012-08-29",593,332]
[null,"2012-08-30",943,648]
[null,"2012-08-31",632,479]
[null,"2012-09-01",404,384]
[null,"2012-09-02",535,426]
[null,"2012-09-03",500,372]
[null,"2012-09-04",752,396]
[null,"2012-09-05",2376,1187]
[null,"2012-09-06",2281,792]
[null,"2012-09-07",1298,742]
[null,"2012-09-08",525,440]
[null,"2012-09-09",316,297]
[null,{"$f":"B79+1","v":"2012-09-10"},678,504]
[null,"2012-09-11",601,451]
[null,"2012-09-12",558,343]
[null,"2012-09-13",2036.2,807]
[null,"2012-09-14",729,480]
[null,"2012-09-15",384,272]
[null,"2012-09-16",284,265]
[null,"2012-09-17",1252,714]
[null,"2012-09-18",1920,799]
[null,"2012-09-19",1637,567]
[null,"2012-09-20",923,630]
[null,"2012-09-21",888,761]
[null,"2012-09-22",752,481]
[null,"2012-09-23",699,400]
[null,"2012-09-24",2159.4,922]
[null,"2012-09-25",627,480]
[null,"2012-09-26",605,445]
[null,"2012-09-27",751,545]
[null,"2012-09-28",2801.4,1095]
[null,"2012-09-29",579,456]
[null,"2012-09-30",450,216]
[null,"2012-10-01",285,258]
[null,"2012-10-02",695,532]
[null,"2012-10-03",1254,726]
[null,"2012-10-04",1168,812]
[null,"2012-10-05",971,593]
[null,"2012-10-06",820,526]
[null,"2012-10-07",1078,602]
[null,"2012-10-08",1092,822]
[null,"2012-10-09",775,606]
[null,"2012-10-10",714,589]
[null,"2012-10-11",1962,1025]
[null,"2012-10-12",3918.6,1534]
[null,"2012-10-13",703,468]
[null,"2012-10-14",255,236]
[null,"2012-10-15",804,607]
[null,"2012-10-16",915,532]
[null,"2012-10-17",949,574]
[null,"2012-10-18",719,524]
[null,"2012-10-19",587,483]
[null,"2012-10-20",699,389]
[null,"2012-10-21",1100,657]
[null,"2012-10-22",1351,663]
[null,"2012-10-23",838,561]
[null,"2012-10-24",841,651]
[null,"2012-10-25",780,523]
[null,"2012-10-26",936,628]
[null,"2012-10-27",200,162]
[null,"2012-10-28",435,238]
[null,"2012-10-29",2934.6,815]
[null,"2012-10-30",856,588]
[null,"2012-10-31",651,372]
[null,"2012-11-01",845,628]
[null,"2012-11-02",1322,638]
[null,"2012-11-03",274,246]
[null,"2012-11-04",600,433]
[null,"2012-11-05",546,393]
[null,"2012-11-06",680,589]
[null,"2012-11-07",1754,851]
[null,"2012-11-08",1987,821]
[null,"2012-11-09",1194,714]
[null,"2012-11-10",442,356]
[null,"2012-11-11",668,533]
[null,"2012-11-12",832,386]
[null,{"$f":"B143+1","v":"2012-11-13"},1886.2,745]
[null,"2012-11-14",1515.4,598]
[null,"2012-11-15",743,512]
[null,"2012-11-16",1521,760]
[null,"2012-11-17",920,508]
[null,"2012-11-18",2882,1205]
[null,"2012-11-19",1160,443]
[null,"2012-11-20",924,488]
[null,"2012-11-21",953,481]
[null,"2012-11-22",926,472]
[null,"2012-11-23",539,442]
[null,"2012-11-24",559,424]
[null,"2012-11-25",1445,880]
[null,"2012-11-26",1325,645]
[null,"2012-11-27",5430.8,1869]
[null,"2012-11-28",3062.2,893]
[null,"2012-11-29",2537.4,968]
[null,"2012-11-30",1433,786]
[null,"2012-12-01",1368,763]
[null,"2012-12-02",1891,855]
[null,"2012-12-03",2486.8000000000002,907]
[null,"2012-12-04",1626,784]
[null,"2012-12-05",1288,633]
[null,"2012-12-06",1148,619]
[null,"2012-12-07",1037,683]
[null,"2012-12-08",648,401]
[null,"2012-12-09",1832,629]
[null,"2012-12-10",1173,959]
[null,"2012-12-11",808,678]
[null,"2012-12-12",926,644]
[null,"2012-12-13",932,750]
[null,"2012-12-14",572,545]
[null,"2012-12-15",639,528]
[null,"2012-12-16",742,531]
[null,"2012-12-17",755,558]
[null,"2012-12-18",1191,730]
[null,"2012-12-19",2296.8000000000002,998]
[null,"2012-12-20",1236,783]
[null,"2012-12-21",1640,894]
[null,"2012-12-22",932,716]
[null,"2012-12-23",2375,885]
[null,"2012-12-24",6230.4,1457]
[null,"2012-12-25",3768,1552]
[null,"2012-12-26",966,718]
[null,"2012-12-27",1407,896]
[null,"2012-12-28",2151.1999999999998,1123]
[null,"2012-12-29",666,512]
[null,"2012-12-30",321,295]
[null,"2012-12-31",2183.8000000000002,695]
[null,"2013-01-01",449,429]
[null,"2013-01-02",1436,920]
[null,"2013-01-03",785,509]
[null,"2013-01-04",961,735]
[null,"2013-01-05",2351.1999999999998,968]
[null,"2013-01-06",1349,808]
[null,"2013-01-07",1475,947]
[null,"2013-01-08",3507.8,1524]
[null,"2013-01-09",1945.6,824]
[null,"2013-01-10",932,548]
[null,"2013-01-11",1726,854]
[null,"2013-01-12",3889,1417]
[null,"2013-01-13",0,0]
[null,"2013-01-14",7731.8,1665]
[null,"2013-01-15",2089.1999999999998,1082]
[null,{"$f":"B207+1","v":"2013-01-16"},1824.4,620]
[null,"2013-01-17",1787,540]
[null,"2013-01-18",3149.4,759]
[null,"2013-01-19",2080,832]
[null,"2013-01-20",738,523]
[null,"2013-01-21",1608,896]
[null,"2013-01-22",1902,1017]
[null,"2013-01-23",2377,1480]
[null,"2013-01-24",1551,1098]
[null,"2013-01-25",996,793]
[null,"2013-01-26",3278.8,638]
[null,"2013-01-27",0,0]
[null,"2013-01-28",0,0]
[null,"2013-01-29",8392,1184]
[null,"2013-01-30",3346.6,1131]
[null,"2013-01-31",2551.8000000000002,1085]
[null,"2013-02-01",3780.2,1105]
[null,"2013-02-02",1610.2,597]
[null,"2013-02-03",559,374]
[null,"2013-02-04",1290,674]
[null,"2013-02-05",798,477]
[null,"2013-02-06",864,629]
[null,"2013-02-07",703,500]
[null,"2013-02-08",1021,763]
[null,"2013-02-09",1186,682]
[null,"2013-02-10",1246,845]
[null,"2013-02-11",3132,878]
[null,"2013-02-12",1565,636]
[null,"2013-02-13",944,562]
[null,"2013-02-14",674,486]
[null,"2013-02-15",1111,564]
[null,"2013-02-16",778,376]
[null,"2013-02-17",385,334]
[null,"2013-02-18",917,638]
[null,"2013-02-19",1043,681]
[null,"2013-02-20",2203,838]
[null,"2013-02-21",1515,860]
[null,"2013-02-22",0,0]
[null,"2013-02-23",0,0]
[null,"2013-02-24",3613,1979]
[null,"2013-02-25",2612.1999999999998,884]
[null,"2013-02-26",2315.6,1078]
[null,"2013-02-27",915,490]
[null,"2013-02-28",1722,947]
[null,"2013-03-01",1626,926]
[null,"2013-03-02",2321,940]
[null,"2013-03-03",1353,675]
[null,"2013-03-04",1310,578]
[null,"2013-03-05",993,526]
[null,"2013-03-06",916,615]
[null,"2013-03-07",1072,701]
[null,"2013-03-08",1088,603]
[null,"2013-03-09",441,368]
[null,"2013-03-10",375,274]
[null,"2013-03-11",786,522]
[null,"2013-03-12",854,594]
[null,"2013-03-13",928,601]
[null,"2013-03-14",1076,626]
[null,"2013-03-15",831,530]
[null,"2013-03-16",555,351]
[null,"2013-03-17",885,422]
[null,"2013-03-18",609,470]
[null,"2013-03-19",803,692]
[null,"2013-03-20",928,476]
[null,{"$f":"B271+1","v":"2013-03-21"},1252,752]
[null,"2013-03-22",4786.6000000000004,1128]
[null,"2013-03-23",3166.8,1048]
[null,"2013-03-24",1722,686]
[null,"2013-03-25",920,500]
[null,"2013-03-26",1023,501]
[null,"2013-03-27",1125,611]
[null,"2013-03-28",945,599]
[null,"2013-03-29",487,399]
[null,"2013-03-30",304,255]
[null,"2013-03-31",1048,380]
[null,"2013-04-01",638,536]
[null,"2013-04-02",1215,870]
[null,"2013-04-03",1186,753]
[null,"2013-04-04",1160,851]
[null,"2013-04-05",1095,614]
[null,"2013-04-06",572,345]
[null,"2013-04-07",311,267]
[null,"2013-04-08",1355,620]
[null,"2013-04-09",1181,669]
[null,"2013-04-10",840,696]
[null,"2013-04-11",981,526]
[null,"2013-04-12",521,424]
[null,"2013-04-13",407,321]
[null,"2013-04-14",184,165]
[null,"2013-04-15",1072,694]
[null,"2013-04-16",1188,798]
[null,"2013-04-17",696,588]
[null,"2013-04-18",549,489]
[null,"2013-04-19",1042,507]
[null,"2013-04-20",276,247]
[null,"2013-04-21",477,409]
[null,"2013-04-22",1036,742]
[null,"2013-04-23",1023,579]
[null,"2013-04-24",814,623]
[null,"2013-04-25",302,288]
[null,"2013-04-26",832,617]
[null,"2013-04-27",351,290]
[null,"2013-04-28",164,155]
[null,"2013-04-29",632,533]
[null,"2013-04-30",1027,633]
[null,"2013-05-01",578,427]
[null,"2013-05-02",986,520]
[null,"2013-05-03",710,520]
[null,"2013-05-04",252,220]
[null,"2013-05-05",213,188]
[null,"2013-05-06",804,709]
[null,"2013-05-07",1092,668]
[null,"2013-05-08",1194,619]
[null,"2013-05-09",839,498]
[null,"2013-05-10",742,436]
[null,"2013-05-11",397,263]
[null,"2013-05-12",303,255]
[null,"2013-05-13",1153,745]
[null,"2013-05-14",1166,622]
[null,"2013-05-15",852,740]
[null,"2013-05-16",1107,588]
[null,"2013-05-17",651,486]
[null,"2013-05-18",383,280]
[null,"2013-05-19",270,187]
[null,"2013-05-20",623,403]
[null,"2013-05-21",931,499]
[null,"2013-05-22",911,553]
[null,"2013-05-23",852,537]
[null,{"$f":"B335+1","v":"2013-05-24"},2687.8,908]
[null,"2013-05-25",1486,816]
[null,"2013-05-26",443,318]
[null,"2013-05-27",850,641]
[null,"2013-05-28",1176,614]
[null,"2013-05-29",625,554]
[null,"2013-05-30",784,559]
[null,"2013-05-31",739,523]
[null,"2013-06-01",344,241]
[null,"2013-06-02",1166,435]
[null,"2013-06-03",872,581]
[null,"2013-06-04",1452,552]
[null,"2013-06-05",673,389]
[null,"2013-06-06",792,507]
[null,"2013-06-07",696,509]
[null,"2013-06-08",294,260]
[null,"2013-06-09",536,340]
[null,"2013-06-10",394,323]
[null,"2013-06-11",938,715]
[null,"2013-06-12",1383,619]
[null,"2013-06-13",829,540]
[null,"2013-06-14",763,592]
[null,"2013-06-15",241,227]
[null,"2013-06-16",219,205]
[null,"2013-06-17",1147,609]
[null,"2013-06-18",954,477]
[null,"2013-06-19",726,506]
[null,"2013-06-20",973,628]
[null,"2013-06-21",786,657]
[null,"2013-06-22",612,321]
[null,"2013-06-23",509,296]
[null,"2013-06-24",916,592]
[null,"2013-06-25",1377,633]
[null,"2013-06-26",805,568]
[null,"2013-06-27",719,468]
[null,"2013-06-28",742,519]
[null,"2013-06-29",332,243]
[null,"2013-06-30",350,286]
[null,"2013-07-01",1920.6,815]
[null,"2013-07-02",1618.2,404]
[null,"2013-07-03",770.6,325]
[null,"2013-07-04",922.2,455]
[null,"2013-07-05",746.4,360]
[null,"2013-07-06",354.2,237]
[null,"2013-07-07",299.2,253]
[null,"2013-07-08",936.8,807]
[null,"2013-07-09",818,537]
[null,"2013-07-10",560.4,297]
[null,"2013-07-11",831.4,519]
[null,"2013-07-12",738.8,510]
[null,"2013-07-13",424.4,279]
[null,"2013-07-14",516.6,427]
[null,"2013-07-15",897.4,541]
[null,"2013-07-16",966.8,632]
[null,"2013-07-17",695.2,544]
[null,"2013-07-18",632.6,411]
[null,"2013-07-19",658.4,533]
[null,"2013-07-20",1129.5999999999999,583]
[null,"2013-07-21",349.6,270]
[null,"2013-07-22",862.4,623]
[null,"2013-07-23",816.8,528]
[null,"2013-07-24",993.6,586]
[null,"2013-07-25",1058.4000000000001,534]
[null,"2013-07-26",566,394]
[null,{"$f":"B399+1","v":"2013-07-27"},455,323]
[null,"2013-07-28",360,261]
[null,"2013-07-29",871.6,450]
[null,"2013-07-30",944.8,479]
[null,"2013-07-31",1102.5999999999999,611]
[null,"2013-08-01",521.79999999999995,230]
[null,"2013-08-02",658.4,368]
[null,"2013-08-03",314.2,289]
[null,"2013-08-04",381.6,321]
[null,"2013-08-05",578.4,443]
[null,"2013-08-06",775.4,413]
[null,"2013-08-07",1001.6,562]
[null,"2013-08-08",799.4,603]
[null,"2013-08-09",1192.2,633]
[null,"2013-08-10",251,198]
[null,"2013-08-11",622.4,275]
[null,"2013-08-12",1128.8,779]
[null,"2013-08-13",951,520]
[null,"2013-08-14",1208.4000000000001,693]
[null,"2013-08-15",657.4,498]
[null,"2013-08-16",935.4,535]
[null,"2013-08-17",391.6,334]
[null,"2013-08-18",221.2,190]
[null,"2013-08-19",961.4,580]
[null,"2013-08-20",1000.6,590]
[null,"2013-08-21",1522.4,616]
[null,"2013-08-22",612.4,561]
[null,"2013-08-23",594.79999999999995,415]
[null,"2013-08-24",214.2,178]
[null,"2013-08-25",318.60000000000002,195]
[null,"2013-08-26",884.2,586]
[null,"2013-08-27",777.2,382]
[null,"2013-08-28",1121,539]
[null,"2013-08-29",792.6,396]
[null,"2013-08-30",849.4,421]
[null,"2013-08-31",225.4,177]
[null,"2013-09-01",144.4,136]
[null,"2013-09-02",648.6,416]
[null,"2013-09-03",1036.8,434]
[null,"2013-09-04",534.79999999999995,375]
[null,"2013-09-05",612.20000000000005,329]
[null,"2013-09-06",782.8,508]
[null,"2013-09-07",199.2,152]
[null,"2013-09-08",385,221]
[null,"2013-09-09",1088.4000000000001,390]
[null,"2013-09-10",1290.4000000000001,395]
[null,"2013-09-11",762.8,415]
[null,"2013-09-12",1651.6,403]
[null,"2013-09-13",606.79999999999995,288]
[null,"2013-09-14",654.20000000000005,360]
[null,"2013-09-15",405.6,287]
[null,"2013-09-16",2291.1999999999998,675]
[null,"2013-09-17",1886.6,665]
[null,"2013-09-18",990.8,467]
[null,"2013-09-19",808.6,576]
[null,"2013-09-20",649.79999999999995,442]
[null,"2013-09-21",339.8,325]
[null,"2013-09-22",616.6,373]
[null,"2013-09-23",569.6,276]
[null,"2013-09-24",559.4,464]
[null,"2013-09-25",641.4,544]
[null,"2013-09-26",3387.6,1209]
[null,"2013-09-27",757.8,496]
[null,"2013-09-28",816,457]
[null,{"$f":"B463+1","v":"2013-09-29"},553.4,297]
[null,"2013-09-30",699.2,556]
[null,"2013-10-01",0,0]
[null,"2013-10-02",0,0]
[null,"2013-10-03",1001.6,594]
[null,"2013-10-04",780.8,532]
[null,"2013-10-05",452.2,321]
[null,"2013-10-06",631,368]
[null,"2013-10-07",454.6,375]
[null,"2013-10-08",1964.8,584]
[null,"2013-10-09",659,459]
[null,"2013-10-10",784.4,550]
[null,"2013-10-11",844.6,502]
[null,"2013-10-12",355.8,296]
[null,"2013-10-13",3168.2,1183]
[null,"2013-10-14",1661.6,608]
[null,"2013-10-15",1095.2,638]
[null,"2013-10-16",807.2,529]
[null,"2013-10-17",2913.4,946]
[null,"2013-10-18",858.4,586]
[null,"2013-10-19",637.4,408]
[null,"2013-10-20",620.20000000000005,410]
[null,"2013-10-21",3014.6,725]
[null,"2013-10-22",1388.4,916]
[null,"2013-10-23",1039,704]
[null,"2013-10-24",578.4,318]
[null,"2013-10-25",583.4,218]
[null,"2013-10-26",885.4,665]
[null,"2013-10-27",323,287]
[null,"2013-10-28",683.4,394]
[null,"2013-10-29",2450,796]
[null,"2013-10-30",785.8,285]
[null,"2013-10-31",726.6,250]
[null,"2013-11-01",538.4,342]
[null,"2013-11-02",268,243]
[null,"2013-11-03",702.2,491]
[null,"2013-11-04",927.4,460]
[null,"2013-11-05",416.2,231]
[null,"2013-11-06",850,322]
[null,"2013-11-07",830.2,458]
[null,"2013-11-08",1555.8,793]
[null,"2013-11-09",850.6,515]
[null,"2013-11-10",1519,542]
[null,"2013-11-11",2612,1012]
[null,"2013-11-12",2359.8000000000002,975]
[null,"2013-11-13",1943.6,1058]
[null,"2013-11-14",1366,612]
[null,"2013-11-15",882,422]
[null,"2013-11-16",1845.8,987]
[null,"2013-11-17",636.20000000000005,449]
[null,"2013-11-18",1806.8,716]
[null,"2013-11-19",892.6,654]
[null,"2013-11-20",1343.2,610]
[null,"2013-11-21",2469,670]
[null,"2013-11-22",1858.6,864]
[null,"2013-11-23",4515.8,1206]
[null,"2013-11-24",1884.8,932]
[null,"2013-11-25",1141,505]
[null,"2013-11-26",1116.2,602]
[null,"2013-11-27",939,577]
[null,"2013-11-28",1269.5999999999999,574]
[null,"2013-11-29",1268.4000000000001,622]
[null,"2013-11-30",345.6,271]
[null,"2013-12-01",704.8,437]
[null,{"$f":"B527+1","v":"2013-12-02"},761.6,440]
[null,"2013-12-03",976.4,621]
[null,"2013-12-04",1317.2,532]
[null,"2013-12-05",2993,1030]
[null,"2013-12-06",671.8,360]
[null,"2013-12-07",415.2,356]
[null,"2013-12-08",422.8,382]
[null,"2013-12-09",1870.6,954]
[null,"2013-12-10",1376.8,816]
[null,"2013-12-11",2262.8000000000002,1257]
[null,"2013-12-12",1407.4,717]
[null,"2013-12-13",820.6,614]
[null,"2013-12-14",669,503]
[null,"2013-12-15",735,502]
[null,"2013-12-16",2041.4,728]
[null,"2013-12-17",811.6,528]
[null,"2013-12-18",890.2,715]
[null,"2013-12-19",885.6,541]
[null,"2013-12-20",701.6,505]
[null,"2013-12-21",577.6,385]
[null,"2013-12-22",647.20000000000005,352]
[null,"2013-12-23",901.6,529]
[null,"2013-12-24",750,347]
[null,"2013-12-25",862.8,616]
[null,"2013-12-26",660.6,560]
[null,"2013-12-27",477.4,360]
[null,"2013-12-28",495.8,449]
[null,"2013-12-29",2236.8000000000002,717]
[null,"2013-12-30",688.4,491]
[null,"2013-12-31",466.2,372]
[null,"2014-01-01",375,347]
[null,"2014-01-02",666,513]
[null,"2014-01-03",1133.5999999999999,539]
[null,"2014-01-04",804.6,519]
[null,"2014-01-05",457.8,380]
[null,"2014-01-06",928.4,543]
[null,"2014-01-07",861.4,561]
[null,"2014-01-08",854.8,661]
[null,"2014-01-09",1178.5999999999999,756]
[null,"2014-01-10",783.6,618]
[null,"2014-01-11",390.00040000000001,349]
[null,"2014-01-12",301.00530000000003,273]
[null,"2014-01-13",825.98309999999992,597]
[null,"2014-01-14",1311.0284000000001,965]
[null,"2014-01-15",993.02440000000001,722]
[null,"2014-01-16",883.01679999999988,682]
[null,"2014-01-17",879.98659999999995,603]
[null,"2014-01-18",679.00080000000003,496]
[null,"2014-01-19",544.99810000000002,500]
[null,"2014-01-20",861.01020000000005,653]
[null,"2014-01-21",1569.9928999999997,943]
[null,"2014-01-22",1192.0225,792]
[null,"2014-01-23",1105.0181999999998,648]
[null,"2014-01-24",1192.0153,816]
[null,"2014-01-25",519.98579999999993,411]
[null,"2014-01-26",201,188]
[null,"2014-01-27",251.999,252]
[null,"2014-01-28",981.9751,618]
[null,"2014-01-29",885.01509999999996,667]
[null,"2014-01-30",843.99189999999999,479]
[null,"2014-01-31",702.9923,432]
[null,"2014-02-01",654.02499999999998,431]
[null,"2014-02-02",661.99489999999992,558]
[null,"2014-02-03",766.02440000000001,477]
[null,{"$f":"B591+1","v":"2014-02-04"},903.0299,714]
[null,"2014-02-05",827.01179999999999,697]
[null,"2014-02-06",858.98399999999992,759]
[null,"2014-02-07",522.00440000000003,478]
[null,"2014-02-08",312,306]
[null,"2014-02-09",545.01499999999999,428]
[null,"2014-02-10",1142.9851999999998,577]
[null,"2014-02-11",852.98779999999999,735]
[null,"2014-02-12",902.98620000000005,788]
[null,"2014-02-13",815.99490000000003,617]
[null,"2014-02-14",778.01,569]
[null,"2014-02-15",1312.0373999999999,832]
[null,"2014-02-16",1067.0085999999999,742]
[null,"2014-02-17",833.00599999999997,776]
[null,"2014-02-18",834.98009999999999,669]
[null,"2014-02-19",1562.0288999999998,853]
[null,"2014-02-20",848.98930000000007,635]
[null,"2014-02-21",691.01850000000002,572]
[null,"2014-02-22",454.99119999999999,350]
[null,"2014-02-23",491.01069999999999,404]
[null,"2014-02-24",902.98900000000003,764]
[null,"2014-02-25",756.98739999999998,669]
[null,"2014-02-26",1012.9734000000001,680]
[null,"2014-02-27",811.01689999999996,691]
[null,"2014-02-28",774.99029999999993,620]
[null,"2014-03-01",534.98670000000004,421]
[null,"2014-03-02",396,394]
[null,"2014-03-03",774.99549999999999,661]
[null,"2014-03-04",791.98860000000002,634]
[null,"2014-03-05",962.02539999999999,882]
[null,"2014-03-06",1032.9886000000001,890]
[null,"2014-03-07",870.01529999999991,675]
[null,"2014-03-08",813.00369999999998,666]
[null,"2014-03-09",539.01940000000002,433]
[null,"2014-03-10",644.99719999999991,570]
[null,"2014-03-11",645.99680000000001,598]
[null,"2014-03-12",669.99090000000001,584]
[null,"2014-03-13",710.00400000000002,604]
[null,"2014-03-14",1042.0263,653]
[null,"2014-03-15",677.98029999999994,626]
[null,"2014-03-16",0,0]
[null,"2014-03-17",0,0]
[null,"2014-03-18",1172.0071,770.98320000000001]
[null,"2014-03-19",851.00159999999994,627.99619999999993]
[null,"2014-03-20",938.00930000000005,787.99829999999997]
[null,"2014-03-21",764.98540000000003,708.01690000000008]
[null,"2014-03-22",393.00480000000005,324.99279999999999]
[null,"2014-03-23",371.0068,338.00169999999997]
[null,"2014-03-24",868.00819999999999,731.99060000000009]
[null,"2014-03-25",994.98899999999992,699.99360000000001]
[null,"2014-03-26",891.98859999999991,693.99090000000001]
[null,"2014-03-27",879.00879999999995,771.0127]
[null,"2014-03-28",1051.0039000000002,843.02929999999992]
[null,"2014-03-29",468.00339999999994,429.00819999999993]
[null,"2014-03-30",489.99619999999999,444.98399999999998]
[null,"2014-03-31",769.01830000000007,538.00659999999993]
[null,"2014-04-01",642.00549999999998,483.98149999999998]
[null,"2014-04-02",746.02480000000003,598.0159000000001]
[null,"2014-04-03",991.00240000000008,666.0068]
[null,"2014-04-04",910.99790000000007,778.01070000000004]
[null,"2014-04-05",349,253.9991]
[null,"2014-04-06",316.00540000000001,276.9984]
[null,"2014-04-07",810.98199999999997,675.98810000000014]
[null,"2014-04-08",773.00120000000004,620.97860000000003]
[null,{"$f":"B655+1","v":"2014-04-09"},777.00169999999991,552.0062999999999]
[null,"2014-04-10",727.99309999999991,453.00740000000002]
[null,"2014-04-11",629.0059,423.99770000000001]
[null,"2014-04-12",275.99180000000001,199.9999]
[null,"2014-04-13",431.01339999999999,299.99580000000003]
[null,"2014-04-14",908.99400000000003,557.0077]
[null,"2014-04-15",613.98469999999998,453.99759999999998]
[null,"2014-04-16",558.98790000000008,448.00319999999999]
[null,"2014-04-17",536.99980000000005,468.99590000000001]
[null,"2014-04-18",285.9923,255.00779999999997]
[null,"2014-04-19",640.00649999999996,525.00619999999992]
[null,"2014-04-20",644.97440000000006,593.98580000000004]
[null,"2014-04-21",193.99629999999999,168.00110000000001]
[null,"2014-04-22",588.01260000000002,519.98869999999999]
[null,"2014-04-23",522.98820000000001,270.98090000000002]
[null,"2014-04-24",616.00490000000002,425.99580000000003]
[null,"2014-04-25",784.02459999999996,501.98759999999999]
[null,"2014-04-26",253.00479999999999,227.00759999999997]
[null,"2014-04-27",523.00710000000004,487.01110000000006]
[null,"2014-04-28",652.01319999999998,482.99329999999998]
[null,"2014-04-29",785.99900000000002,591.99679999999989]
[null,"2014-04-30",574.98399999999992,403.00369999999998]
[null,"2014-05-01",845.00469999999996,519.01440000000002]
[null,"2014-05-02",640.01250000000005,488.00410000000005]
[null,"2014-05-03",519.0136,381.00760000000002]
[null,"2014-05-04",526.99279999999999,380.98769999999996]
[null,"2014-05-05",637.00420000000008,494.00930000000005]
[null,"2014-05-06",731.98230000000001,607.98710000000005]
[null,"2014-05-07",632.98739999999998,529.99090000000001]
[null,"2014-05-08",613.01440000000002,521.00760000000002]
[null,"2014-05-09",671.00480000000005,585.98130000000003]
[null,"2014-05-10",270.00569999999999,240.00500000000002]
[null,"2014-05-11",242.9983,205.99880000000002]
[null,"2014-05-12",867.98699999999997,682.00130000000001]
[null,"2014-05-13",641.99559999999997,593.99479999999994]
[null,"2014-05-14",565.99580000000003,505.99050000000005]
[null,"2014-05-15",663.98580000000004,515.98899999999992]
[null,"2014-05-16",556.99599999999998,401.99959999999999]
[null,"2014-05-17",224.00210000000001,167.0035]
[null,"2014-05-18",317,267.99450000000002]
[null,"2014-05-19",501.00560000000002,426.01070000000004]
[null,"2014-05-20",684.99929999999995,589.99549999999999]
[null,"2014-05-21",540,521.00669999999991]
[null,"2014-05-22",627.99549999999999,489.00549999999998]
[null,"2014-05-23",532.01120000000003,435.01860000000005]
[null,"2014-05-24",399.00130000000001,348.00900000000001]
[null,"2014-05-25",314.99299999999999,255.9933]
[null,"2014-05-26",511.00569999999999,428.00240000000002]
[null,"2014-05-27",1133.0266999999999,861.99649999999997]
[null,"2014-05-28",718.9914,563.98619999999994]
[null,"2014-05-29",619.99940000000004,507.01100000000002]
[null,"2014-05-30",475.995,383.99329999999998]
[null,"2014-05-31",391.012,344]
[null,"2014-06-01",457.0136,450.01589999999999]
[null,"2014-06-02",809.97990000000004,719.99419999999986]
[null,"2014-06-03",626.99789999999996,561.00739999999996]
[null,"2014-06-04",583,556.00009999999997]
[null,"2014-06-05",492.00839999999999,395.00780000000003]
[null,"2014-06-06",457.9984,367.00029999999998]
[null,"2014-06-07",312.00790000000001,227.99250000000001]
[null,"2014-06-08",231.00290000000001,177.99630000000002]
[null,"2014-06-09",189,186.9999]
[null,"2014-06-10",664.99689999999998,609.99630000000002]
[null,"2014-06-11",782.00689999999997,580.0172]
[null,{"$f":"B719+1","v":"2014-06-12"},618.01689999999996,420.00550000000004]
[null,"2014-06-13",565.99670000000003,396.00480000000005]
[null,"2014-06-14",428.99669999999998,356.9939]
[null,"2014-06-15",373.9923,299.99799999999999]
[null,"2014-06-16",567,502.01200000000006]
[null,"2014-06-17",737.99590000000001,619.01469999999995]
[null,"2014-06-18",555.00469999999996,441.01440000000002]
[null,"2014-06-19",610.98839999999996,508.00799999999998]
[null,"2014-06-20",533.99080000000004,410.00309999999996]
[null,"2014-06-21",341.99540000000002,317.99099999999999]
[null,"2014-06-22",174,173.00040000000001]
[null,"2014-06-23",663.00480000000005,556.99310000000003]
[null,"2014-06-24",1142.0092,927.02000000000021]
[null,"2014-06-25",806.98410000000001,573.98760000000004]
[null,"2014-06-26",618.00819999999999,513.99299999999994]
[null,"2014-06-27",604.99289999999996,390.99170000000004]
[null,"2014-06-28",951.00360000000001,701.00319999999999]
[null,"2014-06-29",417.00799999999998,399.99680000000006]
[null,"2014-06-30",596.00840000000005,472.00659999999993]
[null,"2014-07-01",650.99800000000005,603.98689999999999]
[null,"2014-07-02",963.00239999999997,907.00040000000001]
[null,"2014-07-03",512.0077,483.99689999999998]
[null,"2014-07-04",443.99160000000001,396.99770000000001]
[null,"2014-07-05",189.0001,138.9992]
[null,"2014-07-06",236.00409999999999,217.99760000000001]
[null,"2014-07-07",548.00639999999999,472.00849999999997]
[null,"2014-07-08",527,497.98570000000001]
[null,"2014-07-09",784.97760000000005,565.02380000000005]
[null,"2014-07-10",1182.0230999999999,848.01350000000002]
[null,"2014-07-11",535.99969999999996,413.99590000000001]
[null,"2014-07-12",261,238.00760000000002]
[null,"2014-07-13",401.99,346.00650000000002]
[null,"2014-07-14",629.99760000000003,488.98250000000002]
[null,"2014-07-15",687.9991,581.01819999999998]
[null,"2014-07-16",809.99480000000005,739.97630000000004]
[null,"2014-07-17",632.99810000000002,568.00200000000007]
[null,"2014-07-18",1116.9787000000001,689.99549999999999]
[null,"2014-07-19",473.00240000000002,385.00310000000002]
[null,"2014-07-20",935.99329999999998,583.01599999999996]
[null,"2014-07-21",608.99180000000001,481.00900000000001]
[null,"2014-07-22",743.00649999999996,595.98230000000001]
[null,"2014-07-23",601.98699999999997,510.99179999999996]
[null,"2014-07-24",534,440.00130000000001]
[null,"2014-07-25",573.01020000000005,422.98680000000002]
[null,"2014-07-26",1064.9919,644.02110000000005]
[null,"2014-07-27",262.99149999999997,209.9999]
[null,"2014-07-28",488.99419999999998,407.00139999999999]
[null,"2014-07-29",641.99569999999994,547.00440000000003]
[null,"2014-07-30",832.9855,675.99950000000001]
[null,"2014-07-31",1049.9979000000001,753.02260000000001]
[null,"2014-08-01",903.98739999999998,687.00540000000001]
[null,"2014-08-02",370,327.99639999999999]
[null,"2014-08-03",488.98969999999997,437.00060000000008]
[null,"2014-08-04",652.98130000000003,430.9889]
[null,"2014-08-05",630.99519999999995,553.00570000000005]
[null,"2014-08-06",608.00670000000002,527.01120000000003]
[null,"2014-08-07",593.99800000000005,510.99400000000003]
[null,"2014-08-08",466.00779999999997,400.99190000000004]
[null,"2014-08-09",299.99020000000002,207.0025]
[null,"2014-08-10",242.0016,234.99619999999999]
[null,"2014-08-11",471,393.99]
[null,"2014-08-12",497.00319999999999,457.0147]
[null,"2014-08-13",583.00360000000001,496.99309999999997]
[null,"2014-08-14",755.97820000000002,507.01230000000004]
[null,{"$f":"B783+1","v":"2014-08-15"},565.99570000000006,462.98700000000002]
[null,"2014-08-16",511.01530000000002,420.00649999999996]
[null,"2014-08-17",1095.0314000000001,817.01029999999992]
[null,"2014-08-18",1126.0009,771.01589999999999]
[null,"2014-08-19",894.98209999999995,627.00570000000005]
[null,"2014-08-20",673.01670000000001,491.99360000000001]
[null,"2014-08-21",862.97609999999997,746.98579999999993]
[null,"2014-08-22",429.99509999999998,259.99649999999997]
[null,"2014-08-23",402.00560000000002,322.0111]
[null,"2014-08-24",269.99860000000001,241.00239999999999]
[null,"2014-08-25",697.02139999999997,547.01690000000008]
[null,"2014-08-26",648.99080000000004,592.97949999999992]
[null,"2014-08-27",918.02559999999994,717.00429999999994]
[null,"2014-08-28",843.98289999999997,611.00670000000002]
[null,"2014-08-29",402.99860000000001,336.99590000000001]
[null,"2014-08-30",260.9984,207.00020000000001]
[null,"2014-08-31",169.99799999999999,161.00310000000002]
[null,"2014-09-01",605.99829999999997,494.01580000000001]
[null,"2014-09-02",723.98609999999996,645.01130000000001]
[null,"2014-09-03",935.02099999999996,746.00890000000004]
[null,"2014-09-04",548.98760000000004,490.99350000000004]
[null,"2014-09-05",448.98939999999993,324.00650000000002]
[null,"2014-09-06",163.00369999999998,145.9957]
[null,"2014-09-07",340.99289999999996,313.00099999999998]
[null,"2014-09-08",658.0104,546.99749999999995]
[null,"2014-09-09",766.98470000000009,635.01089999999999]
[null,"2014-09-10",999.00139999999999,730.01409999999998]
[null,"2014-09-11",445.9957,377.00600000000003]
[null,"2014-09-12",419,353.00569999999999]
[null,"2014-09-13",148.99700000000001,139.99809999999999]
[null,"2014-09-14",561.01819999999998,412.01730000000003]
[null,"2014-09-15",1052.0248000000001,534.00609999999995]
[null,"2014-09-16",615.99720000000002,421.00080000000003]
[null,"2014-09-17",527.99149999999997,427.98820000000001]
[null,"2014-09-18",663.00220000000002,493.99940000000004]
[null,"2014-09-19",390.00149999999996,287.00749999999999]
[null,"2014-09-20",339.99560000000002,274.9923]
[null,"2014-09-21",187,166.99680000000004]
[null,"2014-09-22",459.00399999999996,353.99240000000003]
[null,"2014-09-23",502.00969999999995,420.00069999999999]
[null,"2014-09-24",705.01639999999998,554.98760000000004]
[null,"2014-09-25",868.98529999999994,699.0077]
[null,"2014-09-26",464.0068,372.00220000000002]
[null,"2014-09-27",184,166.00300000000001]
[null,"2014-09-28",417.98910000000001,381.00819999999999]
[null,"2014-09-29",593.00639999999999,361.00470000000001]
[null,"2014-09-30",669.99549999999999,515.99390000000005]
[null,"2014-10-01",511.01240000000001,350.99779999999998]
[null,"2014-10-02",473.99419999999998,296.99869999999999]
[null,"2014-10-03",409.99860000000001,371.9991]
[null,"2014-10-04",328.99759999999998,253.00990000000002]
[null,"2014-10-05",189,187.005]
[null,"2014-10-06",399.02030000000002,310.00200000000001]
[null,"2014-10-07",756.00329999999997,530.98839999999996]
[null,"2014-10-08",643.97119999999995,372.99549999999999]
[null,"2014-10-09",512.9932,416.9907]
[null,"2014-10-10",437.99459999999999,341.9941]
[null,"2014-10-11",404.9982,321.00190000000003]
[null,"2014-10-12",545.0086,463.98569999999995]
[null,"2014-10-13",2236.9771999999998,1335.0037]
[null,"2014-10-14",943.96400000000006,797.98789999999997]
[null,"2014-10-15",949.00210000000004,820.00970000000007]
[null,"2014-10-16",561.01599999999996,475.99770000000001]
[null,"2014-10-17",594.00199999999995,416.98680000000002]
[null,{"$f":"B847+1","v":"2014-10-18"},352.99419999999998,283.99299999999999]
[null,"2014-10-19",151.99510000000001,146.9984]
[null,"2014-10-20",582.99839999999995,452.99290000000002]
[null,"2014-10-21",572.02390000000003,283.9984]
[null,"2014-10-22",775.01490000000001,492.00350000000003]
[null,"2014-10-23",790.99710000000005,466.98470000000003]
[null,"2014-10-24",683.00409999999999,424.99569999999994]
[null,"2014-10-25",677.97900000000004,445.00570000000005]
[null,"2014-10-26",473.0129,434.01220000000006]
[null,"2014-10-27",1483.0110999999999,971.01779999999985]
[null,"2014-10-28",700.00099999999998,531.99959999999987]
[null,"2014-10-29",797.00829999999996,549.98630000000003]
[null,"2014-10-30",561.00630000000001,456.99099999999999]
[null,"2014-10-31",843.99099999999999,567.00540000000001]
[null,"2014-11-01",1491.0488999999998,854.97700000000009]
[null,"2014-11-02",494.0179,397.99399999999997]
[null,"2014-11-03",535.98929999999996,396.99369999999999]
[null,"2014-11-04",740.02219999999988,638.00689999999997]
[null,"2014-11-05",0,0]
[null,"2014-11-06",0,0]
[null,"2014-11-07",827.02260000000001,607.97950000000003]
[null,"2014-11-08",297.99419999999998,225.0077]
[null,"2014-11-09",271.99900000000002,243.00050000000002]
[null,"2014-11-10",866.02300000000002,600.00839999999994]
[null,"2014-11-11",951.00970000000007,819.99700000000007]
[null,"2014-11-12",673.99199999999996,543.00610000000006]
[null,"2014-11-13",831.99680000000001,618.0059]
[null,"2014-11-14",921.98320000000001,662.00919999999996]
[null,"2014-11-15",780.01419999999996,541.01499999999999]
[null,"2014-11-16",924.01229999999987,667.02549999999997]
[null,"2014-11-17",866.01239999999996,610.99739999999997]
[null,"2014-11-18",722.98910000000001,518.98270000000002]
[null,"2014-11-19",843.01960000000008,673.9905]
[null,"2014-11-20",815.98399999999992,523.99290000000008]
[null,"2014-11-21",729.99270000000001,476.00509999999997]
[null,"2014-11-22",590.0068,422.0129]
[null,"2014-11-23",1391.9986000000001,976.00080000000003]
[null,"2014-11-24",2748,967]
[null,"2014-11-25",1253.0058000000001,1020.9683]
[null,"2014-11-26",682.99759999999992,568.98779999999999]
[null,"2014-11-27",987.03320000000008,670.02560000000017]
[null,"2014-11-28",715.99530000000004,398.00290000000001]
[null,"2014-11-29",732.98790000000008,522.99779999999998]
[null,"2014-11-30",823.01839999999993,535.00630000000001]
[null,"2014-12-01",1267.9871999999998,694.98700000000008]
[null,"2014-12-02",1463.0344,851.00210000000004]
[null,"2014-12-03",1718.0266999999999,926.9688000000001]
[null,"2014-12-04",2086.9834999999998,1069.0381]
[null,"2014-12-05",2379.9704000000002,897.00459999999998]
[null,"2014-12-06",2267.0499,884.95609999999999]
[null,"2014-12-07",1282.9772,856.98219999999992]
[null,"2014-12-08",1581.9433000000001,749.98910000000001]
[null,"2014-12-09",833.00909999999999,482.01210000000003]
[null,"2014-12-10",1656.0514000000001,964.97850000000005]
[null,"2014-12-11",0,0]
[null,"2014-12-12",0,0]
[null,"2014-12-13",428.99340000000001,321.00100000000003]
[null,"2014-12-14",416.00800000000004,367.00319999999999]
[null,"2014-12-15",1121.0368999999998,518.99290000000008]
[null,"2014-12-16",2235.9996000000001,1093.0160000000001]
[null,"2014-12-17",1088.0019,820.01289999999995]
[null,"2014-12-18",0,0]
[null,"2014-12-19",0,0]
[null,"2014-12-20",404.99649999999997,251.0042]
[null,{"$f":"B911+1","v":"2014-12-21"},698.97699999999998,499.00909999999999]
[null,"2014-12-22",787.01859999999988,560.98210000000006]
[null,"2014-12-23",1591.9911999999999,1084.0022000000001]
[null,"2014-12-24",832.01710000000003,669.00320000000011]
[null,"2014-12-25",746.97260000000006,607.99599999999998]
[null,"2014-12-26",513.99649999999997,424.99880000000002]
[null,"2014-12-27",619.01350000000002,361.99250000000001]
[null,"2014-12-28",635.97519999999997,444.99900000000002]
[null,"2014-12-29",1213.9969999999998,770.00040000000013]
[null,"2014-12-30",637.00279999999998,557.98540000000003]
[null,"2014-12-31",489.99279999999999,406.99760000000003]
[null,"2015-01-01",671.98169999999993,509.99599999999998]
[null,"2015-01-02",1510.0315000000001,1049.0378000000001]
[null,"2015-01-03",470.01600000000002,382.99220000000003]
[null,"2015-01-04",957.00119999999993,427.99619999999999]
[null,"2015-01-05",1099.9949999999999,668.01340000000005]
[null,"2015-01-06",1053.0084999999999,728.03290000000004]
[null,"2015-01-07",1026.9879000000001,624.01070000000004]
[null,"2015-01-08",1020.0329,600.98009999999999]
[null,"2015-01-09",935.00380000000007,479.99779999999998]
[null,"2015-01-10",605.99379999999996,477.01240000000007]
[null,"2015-01-11",582.00580000000002,492.98689999999999]
[null,"2015-01-12",982.97210000000007,652.98870000000011]
[null,"2015-01-13",658.99800000000005,448.99659999999994]
[null,"2015-01-14",857.98259999999993,697.02960000000007]
[null,"2015-01-15",760.00810000000001,369.01029999999997]
[null,"2015-01-16",798.01139999999998,379.00969999999995]
[null,"2015-01-17",395.00759999999997,368.0093]
[null,"2015-01-18",365.012,328.00319999999999]
[null,"2015-01-19",799.01620000000003,516.00339999999994]
[null,"2015-01-20",1684.9728000000002,1082.999]
[null,"2015-01-21",1180.0273,725.971]
[null,"2015-01-22",887.99530000000004,604.0073000000001]
[null,"2015-01-23",731.98979999999995,483.99009999999993]
[null,"2015-01-24",1415.0334,506.97109999999998]
[null,"2015-01-25",693.99990000000003,474.98779999999999]
[null,"2015-01-26",1851.9873,659.9516000000001]
[null,"2015-01-27",2108.9757,631.03340000000003]
[null,"2015-01-28",985.00980000000004,501.00409999999999]
[null,"2015-01-29",896.01799999999992,616.9842000000001]
[null,"2015-01-30",518.00080000000003,306.99640000000005]
[null,"2015-01-31",680.99,512.01880000000006]
[null,"2015-02-01",459.00080000000003,413.01210000000003]
[null,"2015-02-02",1239.9997000000001,576.00009999999997]
[null,"2015-02-03",695.00729999999999,289.99789999999996]
[null,"2015-02-04",460.99680000000001,363.99569999999994]
[null,"2015-02-05",579.00260000000003,428.01030000000003]
[null,"2015-02-06",446.00220000000002,352.99590000000001]
[null,"2015-02-07",299.00330000000002,216.00989999999999]
[null,"2015-02-08",399.99549999999999,279.99130000000002]
[null,"2015-02-09",880.01119999999992,582.02390000000003]
[null,"2015-02-10",739.0021999999999,575.0080999999999]
[null,"2015-02-11",1170.9863,537.0073000000001]
[null,"2015-02-12",1568.0673000000002,792.00970000000007]
[null,"2015-02-13",1246.9988000000001,689.98119999999994]
[null,"2015-02-14",831.00289999999995,550.00110000000006]
[null,"2015-02-15",711.9946000000001,623.01369999999997]
[null,"2015-02-16",0,0]
[null,"2015-02-17",1329.0309000000002,914.04070000000002]
[null,"2015-02-18",993.00610000000006,672.01210000000003]
[null,"2015-02-19",865.97900000000004,709.01689999999996]
[null,"2015-02-20",1034.011,788.98079999999993]
[null,"2015-02-21",1088.9765,789.98480000000018]
[null,"2015-02-22",587.98009999999999,512.9969000000001]
[null,{"$f":"B975+1","v":"2015-02-23"},972.00409999999988,741.00569999999993]
[null,"2015-02-24",1045.9937,798.99109999999996]
[null,"2015-02-25",1189.0160000000001,685.01649999999995]
[null,"2015-02-26",1060.9657000000002,742.01920000000007]
[null,"2015-02-27",1910.9704999999999,857.0517000000001]
[null,"2015-02-28",587.01639999999998,517.98750000000007]
[null,"2015-03-01",1204.0145,607.9849999999999]
[null,"2015-03-02",1413.9735000000001,726.00360000000001]
[null,"2015-03-03",692.98540000000003,485.00130000000001]
[null,"2015-03-04",647.99109999999996,458.01650000000001]
[null,"2015-03-05",632.99479999999994,480.99520000000001]
[null,"2015-03-06",450.99559999999997,312.00310000000002]
[null,"2015-03-07",529.99220000000003,422.00079999999997]
[null,"2015-03-08",194.00020000000001,175.00560000000002]
[null,"2015-03-09",831.00739999999996,572.00319999999999]
[null,"2015-03-10",870.03039999999987,573.00720000000001]
[null,"2015-03-11",886.00439999999992,618.98860000000002]
[null,"2015-03-12",957.98469999999998,506.99770000000001]
[null,"2015-03-13",684.98669999999993,528.99929999999995]
[null,"2015-03-14",436.99869999999999,411.99090000000001]
[null,"2015-03-15",728.9778,667.9976999999999]
[null,"2015-03-16",608.00520000000006,438.99510000000004]
[null,"2015-03-17",535.0068,457.00009999999997]
[null,"2015-03-18",1259.9932000000001,859.01610000000005]
[null,"2015-03-19",897.01919999999996,695.97219999999982]
[null,"2015-03-20",744.00700000000006,389.99709999999999]
[null,"2015-03-21",891.00249999999994,557.01940000000002]
[null,"2015-03-22",839.00639999999999,706.98660000000007]
[null,"2015-03-23",944.01519999999994,478.00270000000006]
[null,"2015-03-24",1428.0063,756.00589999999988]
[null,"2015-03-25",784.99770000000001,563.98680000000002]
[null,"2015-03-26",981.00150000000008,591.99120000000005]
[null,"2015-03-27",600.0127,289.00570000000005]
[null,"2015-03-28",443.00099999999998,309.9948]
[null,"2015-03-29",333,257.99830000000003]
[null,"2015-03-30",590.00660000000005,346.98509999999999]
[null,"2015-03-31",545.01249999999993,322.9948]
[null,"2015-04-01",750.00520000000006,447.0181]
[null,"2015-04-02",572.99389999999994,419.98270000000002]
[null,"2015-04-03",326.0043,302.99379999999996]
[null,"2015-04-04",530.98929999999996,433.012]
[null,"2015-04-05",384,346.99949999999995]
[null,"2015-04-06",1318.0309999999999,948.99329999999998]
[null,"2015-04-07",1705.0144999999998,747.95960000000002]
[null,"2015-04-08",953.99919999999997,537.01220000000012]
[null,"2015-04-09",684.01109999999994,486.99950000000001]
[null,"2015-04-10",458.99559999999997,404.00300000000004]
[null,"2015-04-11",203.00290000000001,196.9965]
[null,"2015-04-12",807.00319999999999,676.99680000000001]
[null,"2015-04-13",634.01199999999994,340.98810000000003]
[null,"2015-04-14",746.98689999999999,485.00689999999992]
[null,"2015-04-15",823.02440000000001,667.98849999999993]
[null,"2015-04-16",814.0204,733.99879999999996]
[null,"2015-04-17",647.98850000000004,455.99609999999996]
[null,"2015-04-18",328,313.99219999999997]
[null,"2015-04-19",448.99919999999997,335.99]
[null,"2015-04-20",891.99080000000004,597.01319999999998]
[null,"2015-04-21",0,0]
[null,"2015-04-22",1177.0219000000002,1070.0020999999999]
[null,"2015-04-23",666.00400000000002,482.00579999999997]
[null,"2015-04-24",782.00980000000004,520.99660000000006]
[null,"2015-04-25",800.97289999999998,609.0136]
[null,"2015-04-26",581.98610000000008,449.01589999999999]
[null,"2015-04-27",544.00150000000008,294.00570000000005]
[null,{"$f":"B1039+1","v":"2015-04-28"},681.00239999999997,279.99119999999994]
[null,"2015-04-29",474.0068,397.00749999999999]
[null,"2015-04-30",738.99579999999992,579.00990000000002]
[null,"2015-05-01",926.02210000000002,556.01429999999993]
[null,"2015-05-02",1144.9954999999998,869.99199999999996]
[null,"2015-05-03",448,435.99520000000001]
[null,"2015-05-04",647.98609999999996,469.00509999999997]
[null,"2015-05-05",788.98820000000001,573.99220000000014]
[null,"2015-05-06",685.99180000000001,544.00790000000006]
[null,"2015-05-07",508.99,441.00679999999994]
[null,"2015-05-08",470.00040000000001,389.00440000000003]
[null,"2015-05-09",319,305.9923]
[null,"2015-05-10",341.99739999999997,326.99879999999996]
[null,"2015-05-11",599.01679999999999,305.99899999999997]
[null,"2015-05-12",618.98260000000005,417.98459999999994]
[null,"2015-05-13",625.00540000000001,419.01179999999999]
[null,"2015-05-14",526.00139999999999,372.00599999999997]
[null,"2015-05-15",590.0068,380.99509999999998]
[null,"2015-05-16",289.99379999999996,248.99950000000001]
[null,"2015-05-17",426.00400000000002,345.00200000000001]
[null,"2015-05-18",649.99680000000001,280.99850000000004]
[null,"2015-05-19",1173.9808,704.98349999999994]
[null,"2015-05-20",894.98719999999992,580.99430000000007]
[null,"2015-05-21",659.01530000000002,403.97829999999999]
[null,"2015-05-22",823.99840000000006,395.0222]
[null,"2015-05-23",283.0009,256.00310000000002]
[null,"2015-05-24",319.00029999999998,311.00839999999999]
[null,"2015-05-25",660.01110000000006,429.01050000000004]
[null,"2015-05-26",579.01589999999999,468.00279999999998]
[null,"2015-05-27",599.00340000000006,493.99329999999998]
[null,"2015-05-28",556.99630000000002,393.00789999999995]
[null,"2015-05-29",511.00420000000003,303.99629999999996]
[null,"2015-05-30",460.00440000000003,405.99540000000002]
[null,"2015-05-31",347.99810000000002,306.00010000000003]
[null,"2015-06-01",801.00170000000003,609.99329999999998]
[null,"2015-06-02",883.01919999999996,787.02430000000004]
[null,"2015-06-03",538.00019999999995,415.00169999999997]
[null,"2015-06-04",709.99839999999995,467.00879999999995]
[null,"2015-06-05",757.00350000000003,540.98159999999996]
[null,"2015-06-06",370.00700000000001,315.00099999999998]
[null,"2015-06-07",194.0008,182.99790000000002]
[null,"2015-06-08",319.99950000000001,312.99639999999999]
[null,"2015-06-09",717.01859999999999,536.99489999999992]
[null,"2015-06-10",424.00020000000001,350.99020000000007]
[null,"2015-06-11",481.99990000000003,391.00730000000004]
[null,"2015-06-12",573.00329999999997,305.9889]
[null,"2015-06-13",248.00189999999998,213.00119999999998]
[null,"2015-06-14",244.0042,217.9939]
[null,"2015-06-15",922.00619999999992,480.9855]
[null,"2015-06-16",951.00259999999992,544.01620000000003]
[null,"2015-06-17",767.00299999999993,640.00559999999996]
[null,"2015-06-18",632.01049999999998,430.00330000000002]
[null,"2015-06-19",500.00289999999995,248.00130000000001]
[null,"2015-06-20",368.99869999999999,344.00240000000002]
[null,"2015-06-21",378.00919999999996,334.98970000000003]
[null,"2015-06-22",514.00279999999998,343.00240000000002]
[null,"2015-06-23",519.00350000000003,418.99770000000001]
[null,"2015-06-24",551.00009999999997,472.00689999999997]
[null,"2015-06-25",617.00969999999995,559.99829999999997]
[null,"2015-06-26",743.99379999999996,593.00369999999998]
[null,"2015-06-27",517.99160000000006,431.99519999999995]
[null,"2015-06-28",712.02340000000004,661.99940000000004]
[null,"2015-06-29",771.99479999999994,572.9973]
[null,"2015-06-30",710.0068,500.98699999999997]
[null,{"$f":"B1103+1","v":"2015-07-01"},593.01240000000007,367.98929999999996]
[null,"2015-07-02",652.01599999999996,420.00349999999997]
[null,"2015-07-03",585.01420000000007,379.99650000000003]
[null,"2015-07-04",518.00429999999994,362.98289999999997]
[null,"2015-07-05",230,221.0043]
[null,"2015-07-06",797.99829999999997,324.98770000000002]
[null,"2015-07-07",638.00459999999998,474.99779999999998]
[null,"2015-07-08",839.97680000000003,648.98569999999995]
[null,"2015-07-09",824.98489999999993,500.9742]
[null,"2015-07-10",583.00749999999994,381.99329999999998]
[null,"2015-07-11",1371.991,887.005]
[null,"2015-07-12",1128.0168000000001,877.00200000000007]
[null,"2015-07-13",1184.9712999999999,853.04050000000007]
[null,"2015-07-14",772.01070000000004,598.01689999999996]
[null,"2015-07-15",671.9914,564.01659999999993]
[null,"2015-07-16",761.98699999999997,651.00529999999992]
[null,"2015-07-17",1892.9872,1320.0000999999997]
[null,"2015-07-18",927.00159999999994,748.00099999999998]
[null,"2015-07-19",460,392.99470000000002]
[null,"2015-07-20",770.98749999999995,568.00350000000003]
[null,"2015-07-21",1121.9891000000002,845.03820000000007]
[null,"2015-07-22",955.9796,524.00170000000003]
[null,"2015-07-23",582.98720000000003,496.99560000000002]
[null,"2015-07-24",552.99520000000007,406.99250000000001]
[null,"2015-07-25",353.00640000000004,316.00209999999998]
[null,"2015-07-26",406.00379999999996,338.98789999999997]
[null,"2015-07-27",678.01210000000003,548.0172]
[null,"2015-07-28",587.99599999999998,534.98810000000003]
[null,"2015-07-29",593.99260000000004,540.01020000000005]
[null,"2015-07-30",591.00130000000001,447.01280000000003]
[null,"2015-07-31",540.00299999999993,429.01479999999998]
[null,"2015-08-01",208.9974,186.00560000000002]
[null,"2015-08-02",176,161.99970000000002]
[null,"2015-08-03",646.00520000000006,434.995]
[null,"2015-08-04",644.99959999999999,587.01080000000002]
[null,"2015-08-05",572.98910000000001,483.99309999999997]
[null,"2015-08-06",460.99930000000001,385.01100000000002]
[null,"2015-08-07",479.98560000000003,327.00079999999997]
[null,"2015-08-08",228.99979999999999,217.00170000000003]
[null,"2015-08-09",248.00040000000001,248]
[null,"2015-08-10",498.00689999999997,400.98869999999999]
[null,"2015-08-11",415.99900000000002,392.00010000000003]
[null,"2015-08-12",1061.019,609.99059999999997]
[null,"2015-08-13",526.00700000000006,447.00139999999999]
[null,"2015-08-14",486.99549999999999,376.99349999999998]
[null,"2015-08-15",442.00630000000001,375.9896]
[null,"2015-08-16",253,247.99520000000001]
[null,"2015-08-17",454.99889999999994,287.99960000000004]
[null,"2015-08-18",617.01350000000002,483.99430000000007]
[null,"2015-08-19",496.00350000000003,333.99799999999999]
[null,"2015-08-20",396.00099999999998,338.99150000000003]
[null,"2015-08-21",385.99299999999999,281.99299999999994]
[null,"2015-08-22",467.97839999999997,330.00209999999998]
[null,"2015-08-23",477.98440000000005,437.01089999999999]
[null,"2015-08-24",2159.0382,1062.9747]
[null,"2015-08-25",912.98440000000005,717.9851000000001]
[null,"2015-08-26",688.99110000000007,585.9991]
[null,"2015-08-27",667.01890000000003,529.98109999999997]
[null,"2015-08-28",538.01029999999992,435.99489999999997]
[null,"2015-08-29",473.99599999999998,404.99259999999998]
[null,"2015-08-30",169,162.00190000000001]
[null,"2015-08-31",483.00019999999995,334.00219999999996]
[null,"2015-09-01",434.00040000000001,367.00510000000003]
[null,"2015-09-02",686.01119999999992,490.01179999999999]
[null,{"$f":"B1167+1","v":"2015-09-03"},1110.9938,741.02769999999998]
[null,"2015-09-04",452.995,368.00170000000003]
[null,"2015-09-05",271.99360000000001,250.9992]
[null,"2015-09-06",137.001,137]
[null,"2015-09-07",418.00459999999998,333.00490000000002]
[null,"2015-09-08",448.99009999999998,390.9898]
[null,"2015-09-09",423.99259999999998,357.98770000000002]
[null,"2015-09-10",514.98969999999997,433.00460000000004]
[null,"2015-09-11",459.9984,281.99919999999997]
[null,"2015-09-12",213,211.999]
[null,"2015-09-13",342.99919999999997,339.00810000000001]
[null,"2015-09-14",550.00620000000004,391.98710000000005]
[null,"2015-09-15",633.01520000000005,349.99900000000002]
[null,"2015-09-16",531.99789999999996,478.00709999999998]
[null,"2015-09-17",745.97849999999994,644.01890000000003]
[null,"2015-09-18",568.98869999999999,288.00669999999997]
[null,"2015-09-19",217,209.0026]
[null,"2015-09-20",373.99520000000001,351.99509999999998]
[null,"2015-09-21",526.9873,404.00699999999995]
[null,"2015-09-22",703.00540000000001,488.98509999999999]
[null,"2015-09-23",581.9991,416.98610000000002]
[null,"2015-09-24",529.99810000000002,329.9819]
[null,"2015-09-25",441.00229999999999,238.00319999999999]
[null,"2015-09-26",219.00560000000002,207.99850000000001]
[null,"2015-09-27",175.00409999999999,174]
[null,"2015-09-28",491.0068,215.00219999999999]
[null,"2015-09-29",510.00080000000003,255.01309999999998]
[null,"2015-09-30",604.00239999999997,349.01589999999999]
[null,"2015-10-01",536.99710000000005,422.00639999999999]
[null,"2015-10-02",654.98019999999997,494.0018]
[null,"2015-10-03",244.99950000000001,225.00570000000002]
[null,"2015-10-04",368.00540000000001,344.00829999999996]
[null,"2015-10-05",272.00450000000001,262.99950000000001]
[null,"2015-10-06",614.00720000000001,410.99599999999998]
[null,"2015-10-07",760.99209999999994,506.00870000000003]
[null,"2015-10-08",645.00769999999989,399.01259999999991]
[null,"2015-10-09",707.00819999999999,468.98920000000004]
[null,"2015-10-10",581.98869999999999,536.99260000000004]
[null,"2015-10-11",625.02049999999997,577.98440000000005]
[null,"2015-10-12",797.00720000000001,224.99189999999999]
[null,"2015-10-13",960.01229999999998,621.98540000000003]
[null,"2015-10-14",727.99620000000004,406.99560000000002]
[null,"2015-10-15",648.99680000000012,505.98970000000003]
[null,"2015-10-16",578.99540000000002,279.99880000000002]
[null,"2015-10-17",514.99590000000001,361.99739999999997]
[null,"2015-10-18",483.99980000000005,391.99450000000002]
[null,"2015-10-19",1024.0129000000002,478.99879999999996]
[null,"2015-10-20",781.9828,550.0059]
[null,"2015-10-21",694.98910000000001,600.01919999999996]
[null,"2015-10-22",1421.961,1021.9881]
[null,"2015-10-23",717.02430000000004,521.00080000000003]
[null,"2015-10-24",764.99630000000002,329.9862]
[null,"2015-10-25",255.9992,245.00040000000001]
[null,"2015-10-26",1425.9816000000001,736.99400000000003]
[null,"2015-10-27",1474.0118,1156.0129999999999]
[null,"2015-10-28",660.01119999999992,560.98390000000006]
[null,"2015-10-29",792.99340000000007,640.0068]
[null,"2015-10-30",725.00930000000005,422.01579999999996]
[null,"2015-10-31",1110.9996000000001,917.01810000000012]
[null,"2015-11-01",1519.9725000000001,912.04179999999997]
[null,"2015-11-02",1049.0152,773.02149999999995]
[null,"2015-11-03",657.98410000000001,532.98339999999996]
[null,"2015-11-04",917.99869999999999,648.00449999999989]
[null,"2015-11-05",1249.0331999999999,671.02109999999993]
[null,{"$f":"B1231+1","v":"2015-11-06"},879.02250000000004,466.00429999999994]
[null,"2015-11-07",495.00740000000002,395.9991]
[null,"2015-11-08",384.99940000000004,365.99279999999999]
[null,"2015-11-09",737.01149999999996,472.99779999999998]
[null,"2015-11-10",562.01019999999994,459.00479999999999]
[null,"2015-11-11",751.01459999999997,539.00469999999996]
[null,"2015-11-12",1472.9939999999999,807.97919999999988]
[null,"2015-11-13",1514.0403999999999,733.98890000000006]
[null,"2015-11-14",1075.9782,691.9704999999999]
[null,"2015-11-15",681.97700000000009,588.98739999999998]
[null,"2015-11-16",687.02060000000006,410.99550000000005]
[null,"2015-11-17",594.99720000000002,550.99810000000002]
[null,"2015-11-18",645.01610000000005,577.98050000000001]
[null,"2015-11-19",1200.9769000000001,537.01139999999998]
[null,"2015-11-20",1111.9791,399.98080000000004]
[null,"2015-11-21",639.98860000000002,476.0027]
[null,"2015-11-22",480.00229999999999,409.01339999999999]
[null,"2015-11-23",973.00919999999985,756.02590000000009]
[null,"2015-11-24",724.98710000000005,671.01289999999995]
[null,"2015-11-25",647.98620000000005,570.01119999999992]
[null,"2015-11-26",1265.9766999999999,1037.0076999999999]
[null,"2015-11-27",542.99040000000002,456.98820000000001]
[null,"2015-11-28",306.99850000000004,288.00260000000003]
[null,"2015-11-29",0,0]
[null,"2015-11-30",2085.0061999999998,1281.9703999999999]
[null,"2015-12-01",1950.9916000000001,848.9697000000001]
[null,"2015-12-02",1221.9864,885.98469999999998]
[null,"2015-12-03",640.99260000000004,490.00669999999997]
[null,"2015-12-04",630.99479999999994,492.99050000000005]
[null,"2015-12-05",304.00040000000001,300.00049999999999]
[null,"2015-12-06",247.0001,233.995]
[null,"2015-12-07",599.99310000000003,504.00660000000005]
[null,"2015-12-08",893.01,690.00280000000009]
[null,"2015-12-09",1495.9519999999998,908.97730000000001]
[null,"2015-12-10",1840.0247999999999,1439.0048999999999]
[null,"2015-12-11",1270.0131000000001,690.98979999999995]
[null,"2015-12-12",599.99279999999999,493.98609999999996]
[null,"2015-12-13",546.00890000000004,430.01259999999996]
[null,"2015-12-14",569.00040000000001,517.01819999999998]
[null,"2015-12-15",909.97829999999999,816.98890000000006]
[null,"2015-12-16",1769.9805999999999,1219.0077000000001]
[null,"2015-12-17",887.98630000000003,680.02079999999989]
[null,"2015-12-18",490.00590000000005,435.00850000000003]
[null,"2015-12-19",470.00169999999997,459.99850000000004]
[null,"2015-12-20",1691.9934000000001,960.00450000000001]
[null,"2015-12-21",852.98019999999997,365.98430000000002]
[null,"2015-12-22",736.99459999999999,682.01620000000003]
[null,"2015-12-23",561.99739999999997,530.98660000000007]
[null,"2015-12-24",681.02140000000009,544.01309999999989]
[null,"2015-12-25",368.00040000000001,320.00600000000003]
[null,"2015-12-26",952.02480000000003,824.9969000000001]
[null,"2015-12-27",455.99900000000002,451.0093]
[null,"2015-12-28",435,429.99950000000001]
[null,"2015-12-29",411.0027,368.99660000000006]
[null,"2015-12-30",537.99180000000001,441.99720000000002]
[null,"2015-12-31",441,421.00010000000003]
[null,"2016-01-01",328.00029999999998,317.00229999999999]
[null,"2016-01-02",467.98430000000002,459.00240000000002]
[null,"2016-01-03",458.01699999999994,452.99459999999999]
[null,"2016-01-04",707.00300000000004,557.99420000000009]
[null,"2016-01-05",904.98270000000002,551.01260000000002]
[null,"2016-01-06",1673.0247999999999,892.01319999999998]
[null,"2016-01-07",977.02680000000009,752.00750000000005]
[null,"2016-01-08",474.99770000000001,392.00970000000007]
[null,{"$f":"B1295+1","v":"2016-01-09"},288.99279999999999,259.00650000000002]
[null,"2016-01-10",260.99790000000002,238.00720000000001]
[null,"2016-01-11",785.98509999999999,610.98559999999998]
[null,"2016-01-12",988.98910000000001,653.01599999999985]
[null,"2016-01-13",1210.0004000000001,702.99309999999991]
[null,"2016-01-14",1229.0351000000001,722.96170000000006]
[null,"2016-01-15",1150.9837,653.00120000000004]
[null,"2016-01-16",375.00200000000001,354.98940000000005]
[null,"2016-01-17",494.98680000000002,399.99470000000002]
[null,"2016-01-18",700.01110000000006,345.00170000000003]
[null,"2016-01-19",589.00920000000008,438.0068]
[null,"2016-01-20",813.98379999999997,560.9846]
[null,"2016-01-21",1073.9701,687.97289999999998]
[null,"2016-01-22",1354.9793,574.0249]
[null,"2016-01-23",1617.0045000000002,561.9849999999999]
[null,"2016-01-24",1195.0172,705.95849999999996]
[null,"2016-01-25",1456.0045,690.01560000000006]
[null,"2016-01-26",910.00000000000011,765.97280000000001]
[null,"2016-01-27",1475.9939999999999,1226.9884000000002]
[null,"2016-01-28",965.97679999999991,843.0098999999999]
[null,"2016-01-29",0,0]
[null,"2016-01-30",2007.9694000000002,1542.0187999999998]
[null,"2016-01-31",1849.9827000000002,1386.0462000000002]
[null,"2016-02-01",806.98709999999994,622.99509999999998]
[null,"2016-02-02",901.03229999999996,675.03409999999997]
[null,"2016-02-03",1158.9675999999999,710.01379999999995]
[null,"2016-02-04",697.00990000000002,634.01890000000003]
[null,"2016-02-05",564.0021999999999,420.988]
[null,"2016-02-06",590.99839999999995,500.00880000000006]
[null,"2016-02-07",352.00100000000003,351.00439999999998]
[null,"2016-02-08",688.99970000000008,566.99249999999995]
[null,"2016-02-09",822.98180000000002,723.00889999999993]
[null,"2016-02-10",621.99739999999986,508.00620000000004]
[null,"2016-02-11",1384.0070999999998,898.98329999999999]
[null,"2016-02-12",814.01339999999993,546.99649999999997]
[null,"2016-02-13",418.99430000000001,370.99039999999997]
[null,"2016-02-14",404.99880000000002,367.00530000000003]
[null,"2016-02-15",898.98039999999992,573.99360000000001]
[null,"2016-02-16",678.00870000000009,537.01670000000001]
[null,"2016-02-17",560.99860000000001,373.00990000000002]
[null,"2016-02-18",656.99839999999995,496.99590000000001]
[null,"2016-02-19",776.02319999999997,552.98759999999993]
[null,"2016-02-20",473.99199999999996,464.98840000000001]
[null,"2016-02-21",375.00559999999996,368.995]
[null,"2016-02-22",661.0009,494.00319999999999]
[null,"2016-02-23",697.00030000000004,581.99029999999993]
[null,"2016-02-24",704.00080000000003,619.99030000000005]
[null,"2016-02-25",811.98909999999989,689.01959999999997]
[null,"2016-02-26",593.01009999999997,515.01]
[null,"2016-02-27",287.99959999999999,277.99580000000003]
[null,"2016-02-28",436.0093,408.9873]
[null,"2016-02-29",829.01739999999995,535.99379999999996]
[null,"2016-03-01",1154.0399,655.03679999999997]
[null,"2016-03-02",639.97309999999993,533.01159999999993]
[null,"2016-03-03",1628.0526,714.00170000000003]
[null,"2016-03-04",1202.9737,797.98430000000008]
[null,"2016-03-05",419,409.99889999999999]
[null,"2016-03-06",315,314.01]
[null,"2016-03-07",891.00420000000008,633.00400000000002]
[null,"2016-03-08",618.98800000000006,564.0012999999999]
[null,"2016-03-09",625.00289999999995,570.02099999999996]
[null,"2016-03-10",642.01089999999999,480.98099999999999]
[null,"2016-03-11",1346.0233000000001,840.99990000000003]
[null,"2016-03-12",743.99099999999999,527.99029999999993]
[null,{"$f":"B1359+1","v":"2016-03-13"},1064.9877000000001,524.97419999999988]
[null,"2016-03-14",1834.9572999999998,850.98689999999999]
[null,"2016-03-15",764.99559999999997,642.99149999999997]
[null,"2016-03-16",742.00549999999998,588.00179999999989]
[null,"2016-03-17",544.98710000000005,466.00249999999994]
[null,"2016-03-18",1741.9953,858.97069999999997]
[null,"2016-03-19",685.00600000000009,533.99019999999996]
[null,"2016-03-20",318.0027,216.0035]
[null,"2016-03-21",760.99789999999996,683.98660000000007]
[null,"2016-03-22",528.00260000000003,429.01609999999999]
[null,"2016-03-23",560.00530000000003,436.99250000000006]
[null,"2016-03-24",625.99810000000002,402.01519999999999]
[null,"2016-03-25",359.99340000000001,284.99110000000002]
[null,"2016-03-26",439.00760000000002,423.0018]
[null,"2016-03-27",332.00120000000004,324.00319999999999]
[null,"2016-03-28",293.00639999999999,293]
[null,"2016-03-29",610.98479999999995,417.00450000000001]
[null,"2016-03-30",862.01369999999997,534.02530000000002]
[null,"2016-03-31",891.98799999999994,574.0104]
[null,"2016-04-01",373.00459999999998,280.00239999999997]
[null,"2016-04-02",414.00919999999996,372.99899999999997]
[null,"2016-04-03",299.0068,250.99730000000002]
[null,"2016-04-04",548.00450000000001,402.99819999999994]
[null,"2016-04-05",579.99610000000007,530.00510000000008]
[null,"2016-04-06",733.02020000000005,656.98170000000005]
[null,"2016-04-07",521.01049999999998,275.00229999999999]
[null,"2016-04-08",790.99649999999997,504.99809999999991]
[null,"2016-04-09",419.01119999999997,411.01159999999999]
[null,"2016-04-10",640.00390000000004,595.98270000000002]
[null,"2016-04-11",857.01330000000007,472.00260000000003]
[null,"2016-04-12",672.99700000000007,448.99790000000007]
[null,"2016-04-13",531.99099999999999,359.98699999999997]
[null,"2016-04-14",533.0059,385.98650000000004]
[null,"2016-04-15",383.00229999999999,335.99979999999999]
[null,"2016-04-16",287.99520000000001,278.99680000000001]
[null,"2016-04-17",677.01309999999989,478.99959999999999]
[null,"2016-04-18",910.02200000000005,645.03190000000006]
[null,"2016-04-19",627.99059999999997,586]
[null,"2016-04-20",507.99860000000001,461.01129999999995]
[null,"2016-04-21",726.00319999999999,582.98910000000012]
[null,"2016-04-22",690.97540000000004,490.00739999999996]
[null,"2016-04-23",629.01750000000004,526.99490000000003]
[null,"2016-04-24",598.99720000000002,436.00389999999993]
[null,"2016-04-25",604.99170000000004,562.01480000000004]
[null,"2016-04-26",749.00099999999998,645.00379999999996]
[null,"2016-04-27",527.99829999999997,499.99170000000004]
[null,"2016-04-28",848.00239999999997,618.98379999999997]
[null,"2016-04-29",673.00059999999996,470.9941]
[null,"2016-04-30",354.01260000000002,337.00260000000003]
[null,"2016-05-01",532.00170000000003,453.00740000000002]
[null,"2016-05-02",809.99770000000012,687.00760000000002]
[null,"2016-05-03",806.99150000000009,551.01480000000004]
[null,"2016-05-04",1197.9672999999998,432.00329999999997]
[null,"2016-05-05",521.98720000000003,425.99770000000001]
[null,"2016-05-06",598.99479999999994,509.98989999999998]
[null,"2016-05-07",282.9939,245.005]
[null,"2016-05-08",255.99950000000001,255.006]
[null,"2016-05-09",910.01729999999998,577.98739999999998]
[null,"2016-05-10",778.00099999999998,558.00509999999997]
[null,"2016-05-11",692.01389999999992,441.01239999999996]
[null,"2016-05-12",660.98360000000002,463.99429999999995]
[null,"2016-05-13",555.99119999999994,323.00490000000002]
[null,"2016-05-14",263,263]
[null,"2016-05-15",146,146]
[null,{"$f":"B1423+1","v":"2016-05-16"},1007.0057999999999,404.01569999999998]
[null,"2016-05-17",793.01530000000002,577.01609999999994]
[null,"2016-05-18",659.99360000000001,461.99260000000004]
[null,"2016-05-19",588.00879999999995,392.98669999999998]
[null,"2016-05-20",532.99279999999999,504.00620000000004]
[null,"2016-05-21",289.00040000000001,274.99950000000001]
[null,"2016-05-22",166,166]
[null,"2016-05-23",579.00649999999996,479.00819999999993]
[null,"2016-05-24",409.00290000000001,376.0059]
[null,"2016-05-25",555.99799999999993,447.00859999999994]
[null,"2016-05-26",782.99880000000007,517.00829999999996]
[null,"2016-05-27",543.0095,488.01580000000001]
[null,"2016-05-28",449.00119999999998,428.99319999999994]
[null,"2016-05-29",194,190.99439999999998]
[null,"2016-05-30",710.98520000000008,500.00389999999999]
[null,"2016-05-31",729.01580000000001,551.9855]
[null,"2016-06-01",518.98700000000008,345.99869999999999]
[null,"2016-06-02",459.99480000000005,264.00689999999997]
[null,"2016-06-03",879.00369999999998,526.00660000000005]
[null,"2016-06-04",0,0]
[null,"2016-06-05",0,0]
[null,"2016-06-06",1156.0307,664.99990000000003]
[null,"2016-06-07",990.98899999999992,387.99539999999996]
[null,"2016-06-08",954.02480000000003,538.99440000000004]
[null,"2016-06-09",715.98889999999994,507.02100000000007]
[null,"2016-06-10",458.00619999999992,202.99360000000001]
[null,"2016-06-11",383.99400000000003,373.01029999999997]
[null,"2016-06-12",247,243.99420000000001]
[null,"2016-06-13",343,322.98939999999999]
[null,"2016-06-14",707.99149999999997,439.99579999999997]
[null,"2016-06-15",593.00260000000003,368.00310000000002]
[null,"2016-06-16",859.01440000000002,250.99079999999998]
[null,"2016-06-17",762.99609999999996,475.00170000000003]
[null,"2016-06-18",356.99770000000001,296.00509999999997]
[null,"2016-06-19",792.00150000000008,474.01279999999997]
[null,"2016-06-20",1294.9905000000001,535.03240000000005]
[null,"2016-06-21",862.00749999999994,478.02869999999996]
[null,"2016-06-22",1011.0038,659.00620000000004]
[null,"2016-06-23",817.99289999999996,496.0059]
[null,"2016-06-24",0,0]
[null,"2016-06-25",1206.0066000000002,864.99920000000009]
[null,"2016-06-26",554.98919999999998,524.99750000000006]
[null,"2016-06-27",818.01419999999996,618.01370000000009]
[null,"2016-06-28",574.00559999999996,557.98709999999994]
[null,"2016-06-29",632.01109999999994,569.99950000000001]
[null,"2016-06-30",795.99240000000009,595.01469999999995]
[null,"2016-07-01",575.99959999999999,439.00209999999998]
[null,"2016-07-02",295.99400000000003,272.0025]
[null,"2016-07-03",220,217.00049999999999]
[null,"2016-07-04",612.98559999999998,443.00349999999997]
[null,"2016-07-05",945.99849999999992,758.01599999999996]
[null,"2016-07-06",920.0154,558.00319999999999]
[null,"2016-07-07",634.98849999999993,507.01060000000001]
[null,"2016-07-08",488.00850000000003,361.00580000000002]
[null,"2016-07-09",241,236.99610000000001]
[null,"2016-07-10",193.0017,189.00400000000002]
[null,"2016-07-11",528.99310000000003,349.99540000000002]
[null,"2016-07-12",1039.9803999999999,590.00420000000008]
[null,"2016-07-13",821.98419999999999,513.00099999999998]
[null,"2016-07-14",599.99040000000014,392.00409999999999]
[null,"2016-07-15",689.00260000000003,445.00689999999997]
[null,"2016-07-16",386.00040000000001,367.99720000000002]
[null,"2016-07-17",335,326.00750000000005]
[null,"2016-07-18",823.00830000000008,462.0030999999999]
[null,{"$f":"B1487+1","v":"2016-07-19"},812.98350000000005,518.99569999999994]
[null,"2016-07-20",605.99480000000005,423.00639999999999]
[null,"2016-07-21",582.99580000000003,477.98630000000003]
[null,"2016-07-22",1284.9938999999999,511.9905]
[null,"2016-07-23",1686.0133000000001,636.00970000000007]
[null,"2016-07-24",468.00599999999997,396.99590000000001]
[null,"2016-07-25",553.99350000000004,432.99220000000003]
[null,"2016-07-26",570.00659999999993,483.0059]
[null,"2016-07-27",479.99869999999999,425.00149999999996]
[null,"2016-07-28",463.00009999999997,414.00940000000003]
[null,"2016-07-29",413.99450000000002,338.00649999999996]
[null,"2016-07-30",400.0068,365.00399999999996]
[null,"2016-07-31",182,182]
[null,"2016-08-01",419.00220000000002,347.0104]
[null,"2016-08-02",693.98160000000007,611.00540000000001]
[null,"2016-08-03",0,0]
[null,"2016-08-04",0,0]
[null,"2016-08-05",686.0104,555.99310000000003]
[null,"2016-08-06",309.99869999999999,269.99950000000001]
[null,"2016-08-07",236.99930000000001,226.99280000000002]
[null,"2016-08-08",554.99990000000003,438.98869999999999]
[null,"2016-08-09",501.0104,399.00880000000001]
[null,"2016-08-10",554.00299999999993,437.01220000000001]
[null,"2016-08-11",804.98490000000004,621.01259999999991]
[null,"2016-08-12",547.00469999999996,411.99259999999998]
[null,"2016-08-13",270.00009999999997,240.99700000000001]
[null,"2016-08-14",198.0001,198]
[null,"2016-08-15",755.98719999999992,306.99380000000002]
[null,"2016-08-16",514.9991,327.99810000000002]
[null,"2016-08-17",558.99339999999995,444.01249999999999]
[null,"2016-08-18",467.99590000000001,400.99980000000005]
[null,"2016-08-19",772.01419999999996,431.98549999999994]
[null,"2016-08-20",309.00469999999996,284.99639999999999]
[null,"2016-08-21",265.00360000000001,248.99769999999998]
[null,"2016-08-22",546.99680000000001,418.99980000000005]
[null,"2016-08-23",564.99829999999997,371.9923]
[null,"2016-08-24",554.99559999999997,395.99390000000005]
[null,"2016-08-25",744.00379999999996,457.99210000000005]
[null,"2016-08-26",345.00459999999998,285.00330000000002]
[null,"2016-08-27",265.00080000000003,256.00059999999996]
[null,"2016-08-28",262.00450000000001,251.00130000000001]
[null,"2016-08-29",415.00559999999996,324.0025]
[null,"2016-08-30",403.0018,339.99310000000003]
[null,"2016-08-31",381.99270000000001,310.00889999999998]
[null,"2016-09-01",595.99549999999999,383.99419999999998]
[null,"2016-09-02",901.9953999999999,500.99060000000003]
[null,"2016-09-03",1699.9463000000001,861.02029999999991]
[null,"2016-09-04",293.99760000000003,293]
[null,"2016-09-05",595.00009999999997,352.01039999999995]
[null,"2016-09-06",522.9923,395.00660000000005]
[null,"2016-09-07",439.00200000000001,385.00219999999996]
[null,"2016-09-08",530.99,452.01650000000001]
[null,"2016-09-09",694.99270000000001,461.00870000000003]
[null,"2016-09-10",384.99369999999999,329.9932]
[null,"2016-09-11",184.00319999999999,183.00459999999998]
[null,"2016-09-12",503.0025,356.9914]
[null,"2016-09-13",379.99609999999996,312.0016]
[null,"2016-09-14",617.00459999999998,488.00729999999993]
[null,"2016-09-15",559.99609999999996,379.0025]
[null,"2016-09-16",629.0009,488.00050000000005]
[null,"2016-09-17",223.99969999999999,217.99350000000001]
[null,"2016-09-18",452.00079999999997,427.00600000000003]
[null,"2016-09-19",562.99080000000004,324.99740000000003]
[null,"2016-09-20",449.98770000000002,349.00679999999994]
[null,{"$f":"B1551+1","v":"2016-09-21"},557.01490000000001,452.98979999999995]
[null,"2016-09-22",405.99680000000001,366.00739999999996]
[null,"2016-09-23",357.99950000000001,308.99380000000002]
[null,"2016-09-24",223.99350000000001,221.9992]
[null,"2016-09-25",193,193]
[null,"2016-09-26",430.00409999999999,340.0061]
[null,"2016-09-27",627.0009,533.9846]
[null,"2016-09-28",479.99860000000001,382.99200000000002]
[null,"2016-09-29",824.02060000000006,673.99559999999997]
[null,"2016-09-30",591.99969999999996,441.00070000000005]
[null,"2016-10-01",527.9846,469.98270000000002]
[null,"2016-10-02",317.9966,303.0052]
[null,"2016-10-03",723.02269999999999,654.01070000000004]
[null,"2016-10-04",2244.9863,565.97460000000001]
[null,"2016-10-05",880.01429999999993,584.98009999999999]
[null,"2016-10-06",851.99180000000001,588.00530000000003]
[null,"2016-10-07",633.01480000000004,443.00130000000001]
[null,"2016-10-08",358.01260000000002,261.00599999999997]
[null,"2016-10-09",297,289.0086]
[null,"2016-10-10",710.99670000000003,330.0027]
[null,"2016-10-11",782.99759999999992,477.00700000000001]
[null,"2016-10-12",614.00199999999995,374.00990000000002]
[null,"2016-10-13",487.00470000000001,372.99680000000001]
[null,"2016-10-14",773.00440000000003,450.99689999999998]
[null,"2016-10-15",257,253.99179999999998]
[null,"2016-10-16",238.0001,238]
[null,"2016-10-17",845.98149999999987,562.98760000000004]
[null,"2016-10-18",523.0009,371.01819999999998]
[null,"2016-10-19",581.00440000000003,469.00919999999996]
[null,"2016-10-20",407.00780000000003,307.99930000000001]
[null,"2016-10-21",1062.9766999999999,577.01209999999992]
[null,"2016-10-22",975.00819999999999,638.98590000000013]
[null,"2016-10-23",398.00259999999997,383.00790000000001]
[null,"2016-10-24",527.98680000000002,410.012]
[null,"2016-10-25",795.00569999999993,423.00750000000005]
[null,"2016-10-26",577.0136,425.0016]
[null,"2016-10-27",652.98860000000002,583.00049999999999]
[null,"2016-10-28",693.98810000000003,582.00929999999994]
[null,"2016-10-29",944.99959999999987,722.00429999999994]
[null,"2016-10-30",591.01240000000007,554.00490000000002]
[null,"2016-10-31",703.00980000000004,497.00620000000004]
[null,"2016-11-01",404.00689999999997,290.99869999999999]
[null,"2016-11-02",549.01400000000001,427.99329999999998]
[null,"2016-11-03",578.005,414.99149999999997]
[null,"2016-11-04",534.99409999999989,318.98690000000005]
[null,"2016-11-05",1098.9845999999998,535.98539999999991]
[null,"2016-11-06",379.01,347.00939999999997]
[null,"2016-11-07",605.01749999999993,463.00389999999999]
[null,"2016-11-08",985.01009999999997,805.98910000000001]
[null,"2016-11-09",2446.9823999999999,982.00599999999997]
[null,"2016-11-10",1548.0364999999999,951.99720000000002]
[null,"2016-11-11",0,0]
[null,"2016-11-12",0,0]
[null,"2016-11-13",1059.9694,911.01169999999991]
[null,"2016-11-14",907.00859999999989,435.01129999999995]
[null,"2016-11-15",590.005,435.01069999999999]
[null,"2016-11-16",647.99860000000001,497.9941]
[null,"2016-11-17",780.99710000000005,619.98820000000001]
[null,"2016-11-18",590.98820000000001,439.00119999999998]
[null,"2016-11-19",424.99739999999997,399.99829999999997]
[null,"2016-11-20",554.01329999999996,502.9966]
[null,"2016-11-21",938.98799999999994,457.01659999999998]
[null,"2016-11-22",716.00920000000008,429.99059999999997]
[null,"2016-11-23",788.00440000000003,613.98990000000003]
[null,{"$f":"B1615+1","v":"2016-11-24"},706.99349999999993,460.0082000000001]
[null,"2016-11-25",543.00159999999994,431.00119999999993]
[null,"2016-11-26",292.00240000000002,274.99520000000001]
[null,"2016-11-27",279,269.00450000000001]
[null,"2016-11-28",806.01860000000011,591.0062999999999]
[null,"2016-11-29",647.99099999999999,603.01570000000004]
[null,"2016-11-30",937.00150000000008,821.00369999999998]
[null,"2016-12-01",827.0184999999999,664.00300000000004]
[null,"2016-12-02",680.99430000000007,482.00190000000003]
[null,"2016-12-03",1236.9935,621.01069999999993]
[null,"2016-12-04",743.99239999999998,607.98620000000005]
[null,"2016-12-05",0,0]
[null,"2016-12-06",0,0]
[null,"2016-12-07",1367.0104000000001,830.99879999999996]
[null,"2016-12-08",0,0]
[null,"2016-12-09",1119.0128999999999,633.99080000000004]
[null,"2016-12-10",399.00080000000003,348.00790000000001]
[null,"2016-12-11",291.00040000000001,266.99459999999999]
[null,"2016-12-12",861.98900000000003,485.01379999999995]
[null,"2016-12-13",1087.0162,602.97659999999996]
[null,"2016-12-14",772.99760000000003,511.99790000000007]
[null,"2016-12-15",836.01430000000005,630.01150000000007]
[null,"2016-12-16",776.99639999999999,582.99279999999999]
[null,"2016-12-17",635.995,554.98889999999994]
[null,"2016-12-18",790.01059999999995,582.00790000000006]
[null,"2016-12-19",567.00649999999996,443.01580000000007]
[null,"2016-12-20",1182.0432000000001,792.02449999999999]
[null,"2016-12-21",729.0018,639.99050000000011]
[null,"2016-12-22",593.00660000000005,522.99869999999999]
[null,"2016-12-23",913.00749999999994,664.00299999999993]
[null,"2016-12-24",1736.9945,998.0372000000001]
[null,"2016-12-25",379.00700000000001,362.01170000000002]
[null,"2016-12-26",302.99419999999998,303]
[null,"2016-12-27",515.00409999999999,497.99879999999996]
[null,"2016-12-28",565.98119999999994,546.01030000000003]
[null,"2016-12-29",524.99599999999998,489.00699999999995]
[null,"2016-12-30",1147.0023000000001,615.01100000000008]
[null,"2016-12-31",539.00639999999999,511.97940000000006]
[null,"2017-01-01",962.02380000000005,670.98040000000003]
[null,"2017-01-02",1079.9758000000002,769.97480000000007]
[null,"2017-01-03",751.01739999999995,541.99069999999995]
[null,"2017-01-04",752.99520000000007,654.99829999999997]
[null,"2017-01-05",540.99459999999999,501.00419999999997]
[null,"2017-01-06",471.99149999999997,395.00380000000001]
[null,"2017-01-07",377.99529999999999,349.00920000000002]
[null,"2017-01-08",502.99339999999995,345.01320000000004]
[null,"2017-01-09",655.99030000000005,481.99760000000003]
[null,"2017-01-10",808.99789999999996,595.02170000000001]
[null,"2017-01-11",1460.0115000000001,850.99860000000001]
[null,"2017-01-12",0,0]
[null,"2017-01-13",2113.0337,938.95349999999996]
[null,"2017-01-14",1150.9798000000001,851.98329999999999]
[null,"2017-01-15",988.98159999999996,700.01950000000011]
[null,"2017-01-16",802.97839999999997,421.98480000000006]
[null,"2017-01-17",967.01339999999982,411.9973]
[null,"2017-01-18",0,0]
[null,"2017-01-19",1153.9944,710.0258]
[null,"2017-01-20",1748.0470999999998,551.01650000000006]
[null,"2017-01-21",557.98860000000002,407.9914]
[null,"2017-01-22",370,356.0016]
[null,"2017-01-23",964.01050000000009,660.97749999999996]
[null,"2017-01-24",851.01319999999998,599.01530000000002]
[null,"2017-01-25",1191.9948000000002,759.03039999999999]
[null,"2017-01-26",718.99400000000003,626.00509999999997]
[null,{"$f":"B1679+1","v":"2017-01-27"},805.01330000000007,657.99399999999991]
[null,"2017-01-28",444.98599999999999,395.01320000000004]
[null,"2017-01-29",731.0139999999999,637.99060000000009]
[null,"2017-01-30",1194.0251999999998,633.99330000000009]
[null,"2017-01-31",1055.0171,560.98720000000003]
[null,"2017-02-01",936.97660000000019,617.98989999999992]
[null,"2017-02-02",815.98130000000003,550.01619999999991]
[null,"2017-02-03",735.99189999999999,470.01769999999999]
[null,"2017-02-04",1125.9834000000003,601.99620000000004]
[null,"2017-02-05",1257.9869000000001,859.96629999999993]
[null,"2017-02-06",1031.9960000000001,363.99939999999998]
[null,"2017-02-07",920.98630000000003,549.00779999999986]
[null,"2017-02-08",804.97770000000003,595.00810000000001]
[null,"2017-02-09",1145.9712999999999,598.02099999999996]
[null,"2017-02-10",987.00040000000001,604.97550000000001]
[null,"2017-02-11",1982.9538000000002,667.97329999999988]
[null,"2017-02-12",0,0]
[null,"2017-02-13",1494.9951999999998,627.96840000000009]
[null,"2017-02-14",832.01879999999994,686.00969999999995]
[null,"2017-02-15",710.98940000000005,513.99429999999995]
[null,"2017-02-16",605.99289999999996,449.00379999999996]
[null,"2017-02-17",0,0]
[null,"2017-02-18",0,0]
[null,"2017-02-19",1304.0214000000001,881.99839999999995]
[null,"2017-02-20",1099.9838000000002,460.01239999999996]
[null,"2017-02-21",843.01710000000014,614.99919999999997]
[null,"2017-02-22",768.98400000000004,485.99489999999997]
[null,"2017-02-23",641.01059999999995,336.01309999999995]
[null,"2017-02-24",819.99800000000005,586.99]
[null,"2017-02-25",521.9941,341.01339999999999]
[null,"2017-02-26",476,430.99329999999998]
[null,"2017-02-27",799.02080000000001,467.99860000000001]
[null,"2017-02-28",615.00410000000011,522.99710000000005]
[null,"2017-03-01",769.97900000000004,598.99170000000004]
[null,"2017-03-02",614.01170000000002,460.99449999999996]
[null,"2017-03-03",810.97930000000008,568.99250000000006]
[null,"2017-03-04",691.02580000000012,501.01210000000003]
[null,"2017-03-05",662.99200000000008,558.9851000000001]
[null,"2017-03-06",614.00549999999998,505.00810000000001]
[null,"2017-03-07",906.99340000000007,726.00360000000001]
[null,"2017-03-08",655.00019999999995,441.01010000000002]
[null,"2017-03-09",543.99240000000009,380.99789999999996]
[null,"2017-03-10",493.99919999999997,404.00990000000002]
[null,"2017-03-11",276.00040000000001,268.00990000000002]
[null,"2017-03-12",652.99980000000005,557.98809999999992]
[null,"2017-03-13",3101.0636000000004,1046.9630999999999]
[null,"2017-03-14",1744.9932000000001,1136.008]
[null,"2017-03-15",1120.0196000000001,767]
[null,"2017-03-16",943.02890000000002,598.99699999999996]
[null,"2017-03-17",772.02170000000001,541.98040000000003]
[null,"2017-03-18",957.00639999999999,815.9905]
[null,"2017-03-19",660.99850000000004,618.99210000000005]
[null,"2017-03-20",1559.9572000000001,730.02579999999989]
[null,"2017-03-21",1626.0480999999997,660.03039999999999]
[null,"2017-03-22",1568.0206000000001,1116.9846]
[null,"2017-03-23",1096.0220000000002,799.01679999999999]
[null,"2017-03-24",785.01920000000007,672.99300000000005]
[null,"2017-03-25",391.00790000000001,347.99760000000003]
[null,"2017-03-26",387.9973,355.9973]
[null,"2017-03-27",1087.9984999999999,535.00260000000003]
[null,"2017-03-28",876.01199999999994,575.00130000000001]
[null,"2017-03-29",1511.0253,479.00459999999998]
[null,"2017-03-30",0,0]
[null,"2017-03-31",0,0]
[null,{"$f":"B1743+1","v":"2017-04-01"},1487.9801999999997,1167.9631999999999]
[null,"2017-04-02",571.00800000000004,519.00569999999993]
[null,"2017-04-03",904.01700000000005,576.99389999999994]
[null,"2017-04-04",952.99890000000005,695.01940000000002]
[null,"2017-04-05",753.99099999999999,583.01949999999999]
[null,"2017-04-06",543.01080000000002,444.99419999999998]
[null,"2017-04-07",563.00760000000002,427.98739999999998]
[null,"2017-04-08",360.00049999999999,269.99430000000001]
[null,"2017-04-09",1162.0028,738.02570000000003]
[null,"2017-04-10",693.00459999999998,465.0068]
[null,"2017-04-11",478.00620000000004,348.00040000000001]
[null,"2017-04-12",436.00360000000001,329.00029999999998]
[null,"2017-04-13",488.00600000000009,374.99179999999996]
[null,"2017-04-14",1357.9666,579.01900000000001]
[null,"2017-04-15",380.00349999999997,327.995]
[null,"2017-04-16",167,167]
[null,"2017-04-17",280.00729999999999,254.99759999999998]
[null,"2017-04-18",639.00060000000008,459.98470000000003]
[null,"2017-04-19",663.99639999999999,484.99439999999993]
[null,"2017-04-20",844.98379999999997,508.99669999999998]
[null,"2017-04-21",630.99530000000004,436.98270000000002]
[null,"2017-04-22",390.98719999999997,378.00990000000002]
[null,"2017-04-23",346.99879999999996,332.00220000000002]
[null,"2017-04-24",360.00200000000001,285.99919999999997]
[null,"2017-04-25",605.99919999999997,517.98470000000009]
[null,"2017-04-26",1207.0174000000002,585.99480000000005]
[null,"2017-04-27",796.97730000000001,526.98750000000007]
[null,"2017-04-28",518.00459999999998,350.98759999999999]
[null,"2017-04-29",240.99939999999998,223.00069999999997]
[null,"2017-04-30",218,204.99539999999999]
[null,"2017-05-01",457.99450000000002,310.00540000000001]
[null,"2017-05-02",668.99170000000004,353.99059999999997]
[null,"2017-05-03",701.0136,356.98610000000002]
[null,"2017-05-04",452.99299999999994,378.98720000000003]
[null,"2017-05-05",708.99630000000002,506.99770000000001]
[null,"2017-05-06",355.00360000000001,293.00489999999996]
[null,"2017-05-07",310.99959999999999,280.99960000000004]
[null,"2017-05-08",648.99930000000006,362.99930000000001]
[null,"2017-05-09",483.99449999999996,348.00240000000002]
[null,"2017-05-10",520.00580000000002,374.00349999999997]
[null,"2017-05-11",461.00729999999999,301.0009]
[null,"2017-05-12",590.98859999999991,388.99779999999998]
[null,"2017-05-13",219,219]
[null,"2017-05-14",221,218.99599999999998]
[null,"2017-05-15",634.99670000000003,333.00909999999999]
[null,"2017-05-16",640.99760000000003,395.99419999999998]
[null,"2017-05-17",795.99380000000008,470.00700000000001]
[null,"2017-05-18",534.00960000000009,361.00290000000007]
[null,"2017-05-19",571.01670000000001,464.00409999999999]
[null,"2017-05-20",367.00149999999996,332.98890000000006]
[null,"2017-05-21",169,165.9991]
[null,"2017-05-22",538.98950000000002,484.0016]
[null,"2017-05-23",694.99080000000004,508.99189999999999]
[null,"2017-05-24",899.00520000000006,480.00009999999992]
[null,"2017-05-25",462.00400000000002,374.01529999999997]
[null,"2017-05-26",529.98910000000001,426.99760000000009]
[null,"2017-05-27",254,250.99279999999999]
[null,"2017-05-28",268,263.00300000000004]
[null,"2017-05-29",485.0009,321.99869999999999]
[null,"2017-05-30",607.01030000000003,428.99920000000003]
[null,"2017-05-31",641.00229999999999,496.99110000000002]
[null,"2017-06-01",523.00409999999999,422.9907]
[null,"2017-06-02",506.00389999999999,298.0061]
[null,"2017-06-03",260.99699999999996,245.00609999999998]
[null,{"$f":"B1807+1","v":"2017-06-04"},250.99789999999999,245.00289999999998]
[null,"2017-06-05",456.98869999999994,341.99279999999999]
[null,"2017-06-06",445,405.99810000000002]
[null,"2017-06-07",703.00919999999996,507.00019999999995]
[null,"2017-06-08",442.98910000000001,354.00599999999997]
[null,"2017-06-09",390.99209999999999,318.99470000000002]
[null,"2017-06-10",343.00119999999998,304.99470000000002]
[null,"2017-06-11",519.98739999999998,433.01400000000001]
[null,"2017-06-12",289.005,268.00440000000003]
[null,"2017-06-13",780.01740000000007,535.99379999999996]
[null,"2017-06-14",556.00070000000005,356.99430000000001]
[null,"2017-06-15",624.00520000000006,407.99139999999994]
[null,"2017-06-16",506.00209999999993,406.98609999999996]
[null,"2017-06-17",285,254.995]
[null,"2017-06-18",240.99119999999999,213.0052]
[null,"2017-06-19",505.00099999999998,463.99509999999998]
[null,"2017-06-20",410,362.98759999999999]
[null,"2017-06-21",475.98979999999995,385.00119999999998]
[null,"2017-06-22",920.03399999999999,400.01819999999998]
[null,"2017-06-23",450.00229999999999,321.99590000000001]
[null,"2017-06-24",262,241.99980000000002]
[null,"2017-06-25",342.00279999999998,263.00850000000003]
[null,"2017-06-26",469.99509999999998,328.00229999999999]
[null,"2017-06-27",476.00200000000001,399.00290000000001]
[null,"2017-06-28",593.00490000000002,460.99700000000001]
[null,"2017-06-29",538.00099999999998,471.01490000000001]
[null,"2017-06-30",660.00220000000013,529.00699999999995]

{"sheet":"6.2 Reliability & Cust serv","index":32,"n_rows":113,"n_cols":9,"rows_kept":113,"cut":false,"hidden":false,"merged":[[5,1,5,7],[105,1,105,8],[93,1,93,8],[108,3,108,8],[42,3,42,8],[68,3,68,8],[96,2,96,8],[12,1,12,7],[13,1,13,7],[16,3,16,8],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[7,1,7,7]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"6.2 RELIABILITY AND CUSTOMER SERVICE PERFORMANCE"]
[]
[null,"There are FIVE tables on this worksheet. Each table has been grouped for ease of navigation. See the Instructions sheet on how to group or ungroup tables. "]
[]
[null,"Instructions"]
[null,"This regulatory template requires the input of performance Historicals and proposed targets for the forthcoming regulatory control period under the STPIS."]
[null,{"$f":"CONCATENATE(\"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"\"whole network (system)\"\" cell. \",dms_TradingName,\" must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition.\")","v":"Performance targets for some parameters may cross feeder classifications in tables 6.2.1, 6.2.2 and 6.2.3. However, where a single target for the whole network is prescribed, this should be entered in the \"whole network (system)\" cell. Essential Energy must define each of the parameters which apply to it. If common definitions exist for the parameter, please attach a reference to the definition."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" should insert \"\"n/a\"\" against parameters which do not apply to it. Do not delete inapplicable fields.\")","v":"Essential Energy should insert \"n/a\" against parameters which do not apply to it. Do not delete inapplicable fields."}]
[null,{"$f":"CONCATENATE(\"If parts of this template are unsuitable to record any of the requested information \",dms_TradingName,\" must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column.\")","v":"If parts of this template are unsuitable to record any of the requested information Essential Energy must provide this information in an alternative format, within it's accompanying regulatory proposal and indicate the section of the regulatory proposal containing the information in the 'addressed at chapter/section of regulatory proposal' column."}]
[null,{"$f":"CONCATENATE(dms_TradingName,\" must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers \"&\"and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. \"&\"Table 6.2.3 is not compulsory - those businesses who want to \"&\" include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information \"&\"necessary to establish the MAIFI targets, including the estimated performance for \",CRCP_y4)","v":"Essential Energy must provide detail of historical unplanned minutes off supply, unplanned interruptions, momentary interruptions, customer numbers and customer service in accordance with tables 6.2.1, 6.2.2, 6.2.4 and 6.2.5. Table 6.2.3 is not compulsory - those businesses who want to  include MAIFI in the s-factor calcuation may make such a proposal and submit the relevant MAIFI information necessary to establish the MAIFI targets, including the estimated performance for 2017-18"}]
[null,"Definitions of parameters under the AER's STPIS apply. Where exclusions apply, data provided below must exclude all events outlined under clause 3.3 of the AER's STPIS."]
[]
[null,"6.2.1 - UNPLANNED MINUTES OFF SUPPLY (SAIDI)"]
[null,null,"Target","Proposed target"]
[null,"SAIDI",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},92.354177405772617,92.354177405772617]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},308.95276729929145,308.95276729929145]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},507.55168049117259,507.55168049117259]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"IFERROR((C20*(C$99/C$104))+(C21*(C$100/C$104))+(C22*(C$101/C$104))+(C23*(C$102/C$104))+(C24*(C$103/C$104)),\"\")","v":295.51890883504069},295.51890883504069,0,0,0,0,0]
[null,"TOTAL VALUE OF EXCLUDED EVENTS*   (*see 3.3 of STPIS)"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},23.884177405772622,23.884177405772622]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},96.012767299291468,96.012767299291468]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},88.121680491172569,88.121680491172569]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"IFERROR((C27*(C$99/C$104))+(C28*(C$100/C$104))+(C29*(C$101/C$104))+(C30*(C$102/C$104)+(C31*(C$103/C$104))),\"\")","v":80.064374504852765},80.064374504852765,0,0,0,0,0]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS AFTER REMOVING EXCLUDED EVENTS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},68.47,68.47,72.360404628804673,72.360404628804673,72.360404628804673,72.360404628804673,72.360404628804673]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},212.94,212.94,211.02484654704261,211.02484654704261,211.02484654704261,211.02484654704261,211.02484654704261]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},419.43,419.43,474.48789011352176,474.48789011352176,474.48789011352176,474.48789011352176,474.48789011352176]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"IFERROR(C25-C32,\"\")","v":215.45453433018793},215.45453433018793,0,0,0,0,0]
[]
[]
[null,"6.2.2 - UNPLANNED INTERRUPTIONS TO SUPPLY (SAIFI)"]
[null,null,"Target","Proposed target"]
[null,"SAIFI",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},1.0239996948050498,1.0239996948050498]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},2.2260966350157876,2.2260966350157876]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},3.1070126200242831,3.1070126200242831]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},0,0]
[null,"Total ",{"$f":"IFERROR((C46*(C$99/C$104))+(C47*(C$100/C$104))+(C48*(C$101/C$104))+(C49*(C$102/C$104))+(C50*(C$103/C$104)),\"\")","v":2.1172385652002563},2.1172385652002563,0,0,0,0,0]
[null,"TOTAL VALUE OF EXCLUDED EVENTS*   (*see 3.3 of STPIS)"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},0.16099969480505,0.16099969480505]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},0.30309663501578765,0.30309663501578765]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},0.30401262002428309,0.30401262002428309]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"IFERROR((C53*(C$99/C$104))+(C54*(C$100/C$104))+(C55*(C$101/C$104))+(C56*(C$102/C$104))+(C57*(C$103/C$104)),\"\")","v":0.27422927471978198},0.27422927471978198,0,0,0,0,0]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS AFTER REMOVING EXCLUDED EVENTS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},0.86299999999999999,0.86299999999999999,0.8650981594727305,0.8650981594727305,0.8650981594727305,0.8650981594727305,0.8650981594727305]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},1.923,1.923,1.8801159771369029,1.8801159771369029,1.8801159771369029,1.8801159771369029,1.8801159771369029]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},2.8029999999999999,2.8029999999999999,3.1047423999998509,3.1047423999998509,3.1047423999998509,3.1047423999998509,3.1047423999998509]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""},0,0,0,0,0,0,0]
[null,"Total ",{"$f":"IFERROR(C51-C58,\"\")","v":1.8430092904804742},1.8430092904804742,0,0,0,0,0]
[]
[]
[null,"6.2.3 - UNPLANNED MOMENTARY INTERRUPTIONS TO SUPPLY (MAIFI)"]
[null,null,"Target","Proposed target"]
[null,"MAIFI",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C72:C76)","v":0},0,0,0,0,0,0]
[null,"TOTAL VALUE OF EXCLUDED EVENTS*   (*see 3.3 of STPIS)"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C79:C83)","v":0},0,0,0,0,0,0]
[null,"TOTAL SUSTAINED CUSTOMERS INTERRUPTIONS AFTER REMOVING EXCLUDED EVENTS"]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"}]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"}]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"}]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"}]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C86:C90)","v":0},{"$f":"SUM(D86:D90)","v":0},{"$f":"SUM(E86:E90)","v":0},{"$f":"SUM(F86:F90)","v":0},{"$f":"SUM(G86:G90)","v":0},{"$f":"SUM(H86:H90)","v":0},{"$f":"SUM(I86:I90)","v":0}]
[]
[]
[null,"The number of distribution customers is calculated as the average of the number of customers at the beginning of the reporting period and the number of customers at the end of the reporting period."]
[]
[null,"6.2.4 - CUSTOMER NUMBERS"]
[null,null,"Forecast"]
[null,"Average customer numbers",{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,{"$f":"INDEX(dms_FeederName_1,MATCH(dms_TradingName,dms_TradingName_List))","v":"CBD"},0,0,0,0,0,0,0]
[null,{"$f":"INDEX(dms_FeederName_2,MATCH(dms_TradingName,dms_TradingName_List))","v":"Urban"},183057.38360212834,184846.40895684282,186579.75104434861,188174.02390480653,189759.85342916177,191325.88920862824,192683.87691141828]
[null,{"$f":"INDEX(dms_FeederName_3,MATCH(dms_TradingName,dms_TradingName_List))","v":"Short rural"},574620.72909060027,580236.51488114765,585677.5098002645,590681.96367925592,595659.91376008408,600575.73088623106,604838.48100599309]
[null,{"$f":"INDEX(dms_FeederName_4,MATCH(dms_TradingName,dms_TradingName_List))","v":"Long rural"},138994.69596256124,140353.09533632439,141669.21464116283,142879.73927098242,144083.85291146411,145272.93724529541,146304.05155577004]
[null,{"$f":"IF(ISBLANK(INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List))),\"\",INDEX(dms_FeederName_5,MATCH(dms_TradingName,dms_TradingName_List)))","v":""}]
[null,"Total ",{"$f":"SUM(C99:C103)","v":896672.80865528993},905436.01917431492,913926.47548577585,921735.72685504484,929503.62010071008,937174.55734015466,943826.40947318147]
[]
[null,"The AER's definition of calls answered within 30 seconds is as follows:\nCalls to the fault line answered in 30 seconds where the time to answer a call is measured from when the call enters the telephone system of the call centre (including that time when it may be ringing unanswered by any response) and the caller speaks with a human operator, but excluding the time that the caller is connected to an automated interactive service that provides substantive information. This measure does not apply to:\n- calls to payment lines and automated interactive services;\n- calls abandoned by the customer within 30 seconds of the call being queued for response by a human operator. Where the time in which a telephone call is abandoned is not measured, then an estimate of the number of calls abandoned within 30 seconds will be determined by taking 20 per cent of all calls abandoned. \nNote: Being placed in a queuing system (automated or otherwise) does not constitute a response. 'Calls answered within 30 seconds' and 'Calls received' should be calculated excluding calls abandoned within 30 seconds of being queued for a human operator; and calls to payment lines and automated interactive services. "]
[]
[null,"6.2.5 - CUSTOMER SERVICE"]
[null,null,"Target","Proposed target"]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"}]
[null,"Number of calls received",239605,239605,239605,239605,239605,239605,239605]
[null,"Number of calls answered within 30 seconds",164644,164644,164644,164644,164644,164644,164644]
[null,"Percentage of calls answered within 30 seconds",{"$f":"IFERROR((C112/C111),\"\")","v":0.68714759708687212},0.68714759708687212,0.68714759708687212,0.68714759708687212,0.68714759708687212,0.68714759708687212,0.68714759708687212]

{"sheet":"7.1  Policies and Procedure ","index":33,"n_rows":247,"n_cols":5,"rows_kept":247,"cut":false,"hidden":false,"merged":[[6,1,6,3]]}
[null,"REGULATORY REPORTING STATEMENT"]
[null,"Australian Distribution Co."]
[null,"2019-20 to 2023-24"]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"Instructions"]
[null,"List and provide a brief description of key internal plans, policies, procedures or strategies that are used to plan and conduct day to day operations and that have been relied upon in the development of the regulatory proposal. Identify any internal plans, policies, procedures and strategies that have changed in the current regulatory control period or that are expected to change before the next regulatory control period where the change has been identified as a step change."]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,"Document Name","Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"Essential Energy Statement of Corporate Intent (SCI)","This is summary document outlining our commitment to shareholders for the next budget period and the following three years.","Opex & Capex summary.  This document provides an all of business view, including both regulated and non regualted servcies.","No"]
[null,"Stakeholder Engagement Framework","Framework about how Essential Energy will engage with its stakeholders","This supports the Our Customer chapter of the proposal specifically and supports all other chapters in its approach to receiving stakeholder feedback.","No"]
[null,"Governance framework"]
[null,"CEOP2074 Regulatory Compliance","The purpose of this Procedure is to provide the business with a clear and accessible overview of Essential Energy’s regulatory compliance program. In practical terms, this Procedure seeks to outline the processes, through which regulatory compliance obligations are met, the method of reporting against these obligations and assurance activities in place to verify regulatory compliance.","Compliance","no"]
[null,"CECP2476 Ringfencing policy","The purpose of this policy is to outline Essential Energy’s approach to compliance with the obligations outlined in the Guideline. This policy is intended to be read in conjunction with the Ring-Fencing Procedure. ","Compliance","no"]
[null,"CEOP2477 Ringfencing procedure","The purpose of this procedure is to provide guidance to Essential Energy employees on how to adhere to the Ring-Fencing Policy.","Compliance","no"]
[null,"CECP0002 - Board Policy - Governance","This framework includes the processes by which the company is directed, controlled, held to account and is the main element to maintaining the integrity of the company and its culture of compliance.","Corporate governance","no"]
[null,"Board Policy - Delegation of Authority to the Chief Executive Officer CECP0001.01","This Delegations Policy sets the framework for managing delegated authority throughout the company by the board of directors to support effective decision making. ","Corporate governance","No"]
[null," CECP0002.03 Board Policy - Risk Management","To ensure that the requirements for the development, implementation, communication and review of the Risk Management Framework are continually aligned with the delivery of proactive, systematic risk management that is aimed at integrating risk management into all that we do as a company.","Comply with standards and NSW Govt guidelines","No"]
[null,"CECP0001.02 - Company Policy - Sub-Delegation of Authority by the Chief Executive Officer","The companys sub-delegations are a key element in effective governance and management of the organisation. This Policy and the Sub-delegation Schedules set the framework for managing sub-delegated authority throughout the company to ensure that responsibility and accountability are provided from the CEO to the employees of the company to discharge the responsibilities required of their positions and to enable the efficient delivery of outcomes.","Framework for sub delegations","No"]
[null,"CECP0002.01 - Board Policy (Governance) Preventing Fraud and Corruption","To outline the approach the company will take to promote an ethical framework in managing the risk of fraud and corrupt conduct, based on underlying principles including its commitment to preventing, detecting, investigating and responding to allegations of fraud and corruption.","Compliance","No"]
[null,"Operational Procedure: Management Representation Questionnaire Process CEOP8078.51","The purpose of this procedure is to provide the business with a clear and accessible overview of the process undertaken in Essential Energy in conducting the Management Representation Questionnaire. In practical terms, this procedure seeks to outline the actions through which representations from management will be obtained regarding effective systems, processes and internal controls and the annual financial statements and the method of reporting the representations made via the Management Representation Questionnaire.","Compliance","No"]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"Asset Capitalisation policy CEOP2416","Provides guidance in relation to the capitalisation of assets","Capex / Opex","No"]
[null,"Cost Allocation Methodology (CAM)","The purpose of the CAM is to establish a method for attributing or allocating costs to, or within, direct control services (standard and alternative), negotiated services (in the event they may arise) and unregulated distribution services. In addition, this CAM is also used to allocate all shared costs to other aspects of Essential Energy’s business not regulated under the NER (e.g. water services) in a consistent manner with the allocation of costs to the distribution business. ","Capex / Opex","No"]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"Asset Management Policy - CECP1004","Essential Energy Corporate Policy outlining Asset Management within Essential Energy. The Asset Management policy typically describes the mandated objectives and requirements used to guide decisions and achieve rational outcome(s) for Essential Energy. ","Capex / Opex","No"]
[]
[null,"Asset Management Strategies"]
[null,"Strategic Asset Management Plan (SAMP) -CEOM8018 \n","The Strategic Asset Management Plan (SAMP) is the overarching document that defines the asset management system and asset management objectives. ","Capex / Opex","No"]
[null,"Reliability Strategy - CEOP2463 (includes the latest Design, Reliability and Performance Licence Conditions for Distribution Network Service Providers)","This document provides direction for Essential Energy to achieve compliance with the Design Reliability and Performance Licence Conditions","Capex ","No"]
[null,"Power Quality Strategy - CEOP2090","This document provides direction for Essential Energy to move towards compliance with relevant the power quality requirements as stipulated in Supply Standards: Electricity Supply Standard (CEOP8026).","Capex / Opex","No"]
[null,"Distribution Growth Strategy - CEOP2091","This document outlines Essential Energy’s strategy for managing issues associated with growth in its Distribution network ","Capex ","No"]
[null,"Safety and Environment Strategy - OM8018.16  \n","This documents provides direction for Essential Energy to achieve compliance with Safety and Environment objectives.\n","Capex / Opex","No"]
[null,"Demand Management Strategy - CEOP1121 \n","This Strategy provides the long-term strategic direction for Essential Energy’s demand management and non-network alternative programs. \n","Capex / Opex","No"]
[null,"Asset Management Plans"]
[null,"IC ESS 15,17 & 46 – Poles","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS26 – LV Services ","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS13 – HV Regulators","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS14 – Poletop Reclosers ","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 12 – OH Switchgear","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_61 to 64 SCADA Field Assets","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_49 ZS RF Linking Equipment","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_50 Telecommunication into brownfield ZS","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 40 & 43 – Underground Cables","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 4009 – Subtransmission Terminations","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 42 – High Voltage Cast Iron Potheads","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 2006 – ZS Capacitor Banks","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 4004 – Outdoor Bus and Isolators","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 78 – ZS Circuit Breakers","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 80 – ZS Station Batteries","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC  ESS 4005 & 4019 - Distribution Poletops","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 1023 & 1024 – Low Clearances","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS23 – Low Voltage Spreaders ","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 30 – Distribution Transformers","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 32 – Distribution OH Substations","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_2007 IP Data Network Equipment","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_3000 RF Linking Equipment","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_48 RF Infrastructure Refurbishment","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 31 – Enclosed Substations","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 99 & 100 – Triangular and Potbelly Columns","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 41 – UG Low Voltage Switchgear and Pillars","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 70, 71, 72, 73 $ 74 – ZS Power Transformers","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 75, 76, 86, 88 & 89 – ZS Civil & Environment","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 85 – ZS Protection","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 81 & 82 – ZS Voltage & Current Transformers","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS2009 – Network Blackspots","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 38 – Two Pole Substations","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 16 – Bare OH Conductor","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 22 – Navigable Crossings","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 101 – LiDAR Data Capture","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_53, 55 and 56 Load Control","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 45 – Subtrans Poletops","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"ESS_54 Controlled Load Demand Management","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_65 & 68 Broken Hill asset refurbishment, and Legal and Safety ","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS_90 Minor Zone Substation Monitoring ","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 83 – ZS Surge Diverters","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 87 – ZS Earthing","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"IC ESS 79 – ZS Switchboards","This document provides analysis and option development for nvestment into the specified asset class","Capex","No"]
[null,"Public Lighting Equipment - CEOM8018.14","This asset management plan details the activities and resources, responsibilities and timescales required to deliver stakeholder requirements and defined service levels consistent with the Business Plan requirements","Capex","No"]
[null,"Vegetation Management Plan - CEOP8008","The purpose of the Vegetation Management Plan CEOP8008 is to ensure proper guidelines and methodology are in place to promote Best Practice in the maintenance of vegetation under or near powerlines with minimum danger to the public, vegetation management workers and electrical workers and ensure compliance with appropriate legislation","Opex","No"]
[null,"Network Management Plan Chapter 2: Customer Installation Safety Plan - CEOP8004","The purpose of the Customer Installation Safety Plan is to ensure the provision of safe electrical installations for connection to Essential Energy's transmission and distribution system and the safe connection of such installations","Capex / Opex","No"]
[null,"Network Management Plan Chapter 3: Public Electrical Safety Awareness Plan - CEOP8005","The purpose of the Customer Installation Safety Plan is to ensure the provision of safe electrical installations for connection to Essential Energy’s transmission and distribution system and the safe connection of such installations","Opex","No"]
[null,"Bush Fire Risk Management Plan - CEOP8022\n","The objective is to manage Essentials Energy’s assets in a manner that minimises the risk of Bush Fires.","Capex / Opex","No"]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"CECP2416 - Asset Capitalisation","The Asset Capitalisation procedure aims to:\n- achieve a consistent interpretation of capital expenditure across all areas of Essential Energy;\n- align the accounting for capital expenditures for both management decision making (Commercial and Decision Support) and external financial reporting (Financial Control); and\n- meet the requirements of NSW Treasury’s Guidelines for Capitalisation of Expenditure in the NSW Public Sector (TPP 06-6), Australian equivalents to International Financial Reporting Standards (AIFRS), and Australian Accounting Standards Boards (AASB) Interpretations.","Capex / Opex","Graciano to advise when updated policy is available."]
[null,"CEOP2513.06 Connection Policy","This connection policy sets out the circumstances in which Essential Energy requires a retail customer or real estate developer to pay the cost of connecting their premises or development to the Essential Energy network. The costs are also known as connection charges for the provision of connection services under Chapter 5A of the National Electricity Rules (NER)","Capex","no"]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"Electrical Safety Rules - CEOP8030","These Electrical Safety Rules provide a uniform set of safe work requirements which persons must comply with when involved with work on or near electrical apparatus.","Capex / Opex","No"]
[null,"The Network Planning Criteria and Guidelines - CEOP8003","This document forms the basis of transmission, subtransmission and distribution Network Planning best practice for Essential Energy. To be used by Essential Energy’s Network Planning and Design staff as the standard for planning Essential Energy’s electricity network","Capex / Opex","No"]
[null,"Distribution Planning Manual - CEOM7092","This manual sets out Essential Energy’s requirements for planning of the distribution network and to provide an educational resource to Distribution Planners & other employees at Essential Energy ","Capex / Opex","No"]
[null,"Network Investment Governance - CEOP0002.82","To provide guidance on the process to obtain endorsement for network investments to support investment decisions which are streamlined, consistent and relevant.","Capex / Opex","No"]
[null,"Standard Overhead Conductor: Current Rating Guide - CEOM7011","This manual is intended to be an easy ready-reference for Essential Energy staff who wishes to assess the thermal (load current) rating of bare overhead conductors across a range of variable conditions such as design temperature, ambient temperature and wind speed based on the ESAA Publication D (b) 5-1988","Capex / Opex","No"]
[null,"Supply Standards: Electricity Supply Standard - CEOP8026","This document provideS details of the objectives which Essential Energy has adopted in relation to the various system characteristics that influence the quality, reliability and security of electricity supply to its valued customers","Capex / Opex","No"]
[null,"Technology Guideline – Places in the Network - CEOM7621.01","The purpose of this manual is to outline the Telecommunications Infrastructure requirements for different locations within Essential Energy. ","Capex / Opex","No"]
[null,"Connection Policy - CEOP2513.06\n","The Guideline outlines the requirements charging customers for conenctions as approved by the AER.","Capex / Opex","No"]
[null,253.06,"The requirements for the design and construction of Subtransmission lines for use in the Essential Energy network are detailed within this design manual and associated construction manuals","Capex / Opex","No"]
[null,"Renewal and Refurbishment Guidelines - CEOM7094","This manual is required to ensure that a whole of network risk approach is taken and facilitate a reasonable compromise between AS/NZS7000, Essential Energy Overhead Design Manual and applicable standards. The manual also provides guidance to maximise the life and use of existing network assets and to ensure capital investment is prudent","Capex","No"]
[null,"Overhead design Manual - CEOM7097","This manual sets out Essential Energy’s requirements for the design of overhead feeders","Capex / Opex","No"]
[null,"Underground design manual - CEOM7098","This manual sets out Essential Energy’s requirements for the design of ungerground feeders (cables)","Capex / Opex","No"]
[null,"Network Planning: Easement Requirements - CEOP8046","This document provides guidelines for easement requirements for powerlines in Essential Energy’s New South Wales distribution area","Capex","No"]
[null,"Transmission & Zone Substation Design Guidelines - CEOP8032","The specific requirements in this guideline have been adopted by Essential Energy to standardise the design, procurement, construction and maintenance of its substations","Capex / Opex","No"]
[null,"Subtransmission design procedure - CEOP2291","This document outlines the process that shall apply to all internally designed Essential Energy Subtransmission power lines within the franchise area covered by Essential Energy","Capex / Opex","No"]
[null,"High voltage protection guideline - CEOP8002","This Operational Procedure sets out the general requirements for protection systems installed on Essential Energy’s high voltage transmission, subtransmission and distribution systems","Capex / Opex","No"]
[null,"SCADA & DSA Design Guidelines - CEOP8084","These guidelines are designed to cover all requirements that need to be satisfied to ensure Essential Energy’s minimum standards for SCADA & DSA Systems are met while maintaining the technical currency of these systems","Capex / Opex","No"]
[null,"CEOP2446 - Maintenance Strategy - Pole and Line Inspection","The purpose of this procedure is to document Essential Energy's criteria for the inspection, assessment and auditing of work processes used to inspect Essential Energy's overhead network, including the above ground components of underground distribution systems","Opex","No"]
[null,"Private Lines Management Plan - CEOP2339","This plan is intended to enhance the understanding of the responsibility associated with the management of overhead low voltage lines on private properties and address the issues and uncertainties that have existed associated with these assets","Capex / Opex","No"]
[null,"Sub-Transmission & Zone Substation: Maintenance - CEOP8011","This procedure documents Essential Energy’s network maintenance strategy and technical maintenance plans for each asset category within Sub-Transmission and Zone Substations","Capex / Opex","No"]
[null,"Distribution Substation & Switchgear maintenance - CEOP8009","This Procedural guideline outlines the schedule for periodic inspection/maintenance of distribution substations, regulators, reclosers and sectionalisers","Capex / Opex","No"]
[null,"Zone Substation: Field WORK Manual & General information - CEOM7772","These Zone Substation manuals provides practical “in the field” assistance to Construction and Maintenance personnel and those subcontractors. It will assist these personnel to carry out their duties in a reliable, consistent manner that complies with the organisation’s Safety, Environmental, Quality and Customer Service obligations","Capex / Opex","No"]
[null,"Zone Substation Inspection and Maintenance - CEOM7773","These Zone Substation manuals provides practical “in the field” assistance to Construction and Maintenance personnel and those subcontractors. It will assist these personnel to carry out their duties in a reliable, consistent manner that complies with the organisation’s Safety, Environmental, Quality and Customer Service obligations","Capex / Opex","No"]
[null,"Zone Substation: Reference Index for ZS activities - CEOM7776","The purpose of this document is to assist in locating forms used in relation to Zone Substation activities and guides.","Capex / Opex","No"]
[null,"Zone Substation Technical Guidelines (Parts 1 – 3) - CEOM7774","These Zone Substation manuals provides practical “in the field” assistance to Construction and Maintenance personnel and those subcontractors. It will assist these personnel to carry out their duties in a reliable, consistent manner that complies with the organisation’s Safety, Environmental, Quality and Customer Service obligations","Capex / Opex","No"]
[null,"Zone Substation: Technical Instructions & Manuals Catalogue - CEOM7775","This document provides an index and locations of specific technical manuals and instruction catalogues","Capex / Opex","No"]
[null,"Public Lighting Management Plan - CEOP1023 ","The purpose of this procedure is to document Essential Energy’s street lighting management and maintenance plans.","Capex / Opex","No"]
[null,"Metering Services Manual - CEOM8014","The main procedural guidelines used to manage and operate metering equipment","Capex / Opex","No"]
[null,"Asset Inspection: Critical Distribution Equipment - CEOP2034","This document details the strategy and process to provide a condition monitoring program that targets specific critical assets identified by the Regional Planning and Customer Connection Manager","Capex / Opex","No"]
[null,"Electricity Network Asset Inspection - CEOP8010","The purpose of this Guideline is to document Essential Energy’s criteria for the inspection, assessment and auditing of work processes used to inspect Essential Energy’s overhead network, including the above ground components of underground distribution systems","Capex / Opex","No"]
[null,"Asset Inspection Maunal - CEOM7005","The manual is to be used by Essential Energy asset inspectors, contractors and other personnel engaged by Essential Energy, in inspecting, treating and reporting of defects found on the electrical network","Capex / Opex","No"]
[null,"Operating agreement - CEOF6052","The Operating Agreement is used in situations where neither party involved in an isolation has complete operational control over all the isolation points and ensures that the isolation remains secured for the duration of the works.","Capex / Opex","No"]
[null,"Switching request and planned outage notification - CEOP2056","The purpose of this procedure is to explain how the forms are used & to ensure that all planned switching including live line work on Essential Energy Electrical System is formally notified to Network Operations prior to the switching taking place","Capex / Opex","No"]
[null,"System alteration notification - CEOP2057","This procedure ensures that alterations to the Essential Energy’s network system not captured by normal work packages and other planned work and maintenance programs are notified to network operations and asset management system as appropriate","Capex / Opex","No"]
[null,"Emergency communication - CEOP2060","To ensure the effective transmission of emergency information so that the safety and wellbeing of Essential Energy employees, customers and the public are maintained","Capex / Opex","No"]
[null,"Manual reclosing of overhead lines - CEOP2062","This procedure provides guidance to Network Operators in assessing the risks and benefits of attempting a manual reclose of an electrical distribution system protection device after an unplanned operation","Capex / Opex","No"]
[null,"Access permit - CEOP2045","This procedure is to ensure that the use of the Access Permit Form and the condition under which the Access Permit is issued provide a safe work and or test environment for employees working on or near Essential Energy’s High Voltage System","Capex / Opex","No"]
[null,"Authority for placing major electrical plant/equipment into service - CEOP2047","The purpose of this procedure is to ensure that Network Operations receives written notification that all construction and pre-commissioning checks on Electrical Plant/Equipment are complete and ready for service.","Capex / Opex","No"]
[null,"Low voltage back feed - CEOP2050","The purpose of this procedure is to explain the use of the form to provide Network Operations with relevant Low Voltage information where Low Voltage paralleling is required","Capex / Opex","No"]
[null,"High voltage live line work operational requirements - CEOP2061","This document is applicable to System Operations and covers the necessary steps to be considered for live line work, from the receipt of the request to undertake live line working techniques on the network, to the restoration of the network on conclusion of that work","Capex / Opex","No"]
[null,"Switching Log - CEOF6397","Authorised Field Officers use when no written instruction available in the field","Capex / Opex","No"]
[null,"Zone Substation: Emergency Response Plan - CEOP2153","The objectives of this plan are to provide the necessary information for the restoration of Zone Substation capacity and/or functionality within the shortest possible timeframe and facilitate the decision making process.","Capex / Opex","No"]
[null,"Operational Manual - CEOM7047","Operating notes directing and specifying the safe operating procedures and practices required to safeguard staff and equipment when operating specific electrical equipment","Capex / Opex","No"]
[null,"Corporate disposal procedure - CEOP8074 ","This Code of Practice prescribes the general guidelines and framework to be used in all disposal activities to promote fair and open competition, probity and accountability whilst achieving best value for the disposal or sale","Capex / Opex","No"]
[null,"Defined Distribution Capital Project Lifecycle - CEOF1113 ","This document shows the process flow for Network Services Project Process and associated Project Management Processes","Capex / Opex","No"]
[null,"The Project Management Manual  - CEOP1068","This guideline will ensure projects within Network Services of Essential Energy are undertaken with the use of a common process model that incorporates common process activities to facilitate the Network Services Project Management methodology","Capex / Opex","No"]
[null,"SSHE Manual - CECM1000","This manual is the driving mechanism for the HSE MS detailing how Essential Energy conforms to: AS/NZS 4801:2001 Occupational Health and Safety Management Systems Specification with guidance for use and AS/NZS ISO 14001:2004 Environmental Management Systems Requirements with guidance for use.","Capex / Opex","No"]
[null,"Asset Management - ISO5500X internation standards","The principles and practices set out in this international standard. ","Capex / Opex","No"]
[null,"Load Control Equipment - CEOM8018.08","Guidelines for use in the design and execution of Load Control facilities and relays","Capex / Opex","No"]
[null,"De-energisation and Re-energisation of Customers Electrical Supply - CEOP2381","General procedure for working on Customer Switchboards ","Capex / Opex","No"]
[null,"Health Safety & Environmental Manual (HSE): Hazardous Materials - Asbestos\nCECM1000.10a","General procedure for use when working with or near asbestos","Capex / Opex","No"]
[null,"Procurement and contracting out policies"]
[null,"Procurement Policy CECP0009.04","This  Policy governs the procurement of external goods and services; to establish a common approach, drive value for money and sustainable benefits and embed effective risks & compliance controls.","See Description","No"]
[null,"Probity in Procurement Policy CECP0009.05","This Policy is to promote and embed probity principles in the procurement of external goods and services","See Description","No"]
[null,"Source to Contract Procedure CEOP0009.06","The purpose of this procedure is to:\n• establish a common approach to procurement activity in the company;\n• drive value for money and sustainable benefits;\n• embed common effective risk and compliance controls; and\n• set out the business rules for the source to contract process within the company.","See Description","No"]
[null,"Category Management & Reporting  Procedure CEOP0009.08","The purpose of this prcedure is to set out how the company will develop Category Management Plans for key areas of external spend with the aim of identifying initiatives that deliver value and manage its risks","See Description","No"]
[null,"Benefits Management Procedure CEOP0009.07","The purpose of this procedure is to  outline a consistent and disciplined approach to the identification, calculation, validation and reporting of procurement benefits","See Description","No"]
[null,"Contract & Supplier Management Procedure CEOP0009.09","The purpose of this procedure is to achieve or exceed the standards of performance and/or delivery milestones set out in the contract through actively managing the contractor and supplier relationships","See Description","No"]
[null,"Procure to Pay Manual CEOM0009.30","This manual sets out the processes involved in the Procure to Pay process ( The process of completing of supplier due diligence, gaining the necessary approvals to purchase, dispatching approved purchase orders to suppliers, accepting/receipting of goods and services and processing payments in line with agreed payment terms and conditions.)\nThe Procure to Pay process is applicable to all expenditure levels, the difference being the type of requisition raised.","See Description","No"]
[null,"Information technology policies or strategies"]
[null,"CECP0002 - Governance","This framework includes the processes by which the company is directed, controlled, held to account and is the main element to maintaining the integrity of the company and its culture of compliance.","Provides governance model for technology investment.","No"]
[null,"CECP0002.17 Contracts Register Framework","To establish an accountability framework for the recording and production of contracts.","Evidence of contract management maturity.","No"]
[null,"CECP0002.30 - Investment Governance Framework","This framework provides the basis for making investment decisions in a transparent and efficient manner by taking into account a full life cycle approach to such investments, and thereby providing assurance to the board and other stakeholders that investment decisions are linked to organisational objectives and are designed to maximise value for customers and shareholders.","Provides governance model for technology investment.","No"]
[null,"CECP0002.33 Governance Procedure","To provide guidance on the process to obtain endorsement for non-system investments in order to support investment decisions which are: \n• streamlined – decision pathway flows are clear and efficient; \n• consistent – assessment of needs, outcomes and risks are aligned; and \n• relevant – appropriate information, both level and content, is submitted to the necessary forum to enable informed decisions.","Provides governance model for technology investment.","No"]
[null,"CECP0002.71 Intellectual Property Management","To articulate the principles that will govern the company’s management of intellectual property.","Evidence of technology IP processes.","No"]
[null,"CECP0010.02 Information Security Policy","This policy establishes the key requirements to enable strategic business outcomes while providing adequate protection against identified information security and cyber related threats.","Evidence of technology IP processes.","No"]
[null,"CECP1005.01 Acceptable Use Of Technology","The key purpose of this policy is to:\nensure safe, compliant, and appropriate use of technology resources by all employees, labour hire and ESPs as endorsed by the Executive Leadership Team; protect electronic information from common electronic security risks and to improve incident reporting; clearly inform all users of Essential Energy’s technology of what is acceptable use and the consequence of misuse; notify all users of Essential Energy’s technology that system activity is logged and monitored; and improve productivity, compliance, and security through efficient and responsible behaviour.","Evidence of prudent technology usage controls.","No"]
[null,"CECP7018 Software Asset Management","This policy is to provide guidance to Essential Energy employees and contractors of the responsibilities, risks and process surrounding Software Asset Management (SAM) based on the NSW Government Software Asset Management Standard.","Evidence of prudent technology asset management process.","No"]
[null,"CEOM7522.01 Information Technology Disaster Recovery Guideline","The fundamental purpose of this document is to outline the approach to IT Disaster Recovery adopted by Essential Energy in accordance with corporate and regulatory requirements and to define the key aspects of Essential Energy’s IT Disaster Recovery Policy and Framework.","Evidence of prudent disaster recovery management.","No"]
[null,"CEOM7621.01 Technology Guideline: Places In The Network","The Essential Energy Asset Management division provides Telecommunication infrastructure services to many different office types and locations in support of business services.","Evidence of prudent technology asset management process.","No"]
[null,"CEOP1005.02 Acceptable Use Of Technology","The purpose of this procedure is to provide guidance to Essential Energy employees (including agency employees, contractors or External Service Provider) on how to adhere to the Acceptable Use of Technology Policy.","Evidence of prudent technology usage controls.","No"]
[null,"CEOP2311 Operational Procedure Information Security Capacity Monitoring And Planning","This document outlines the process for capacity monitoring and planning for Essential Energy’s information systems.","Evidence of technology security processes.","No"]
[null,"CEOP2312 Operational Procedure: Information Security: E-Commerce Testing","To ensure that e-commerce applications are appropriately protected.","Evidence of technology security processes.","No"]
[null,"CEOP2313 Operational Procedure: Information Security: Forensics Plan","This document describes the Information System Forensics Framework that will be used when capturing IS evidence and the activities that will be initiated in response to the detection of all information security incidents.","Evidence of technology security processes.","No"]
[null,"CEOP2319 Secure Disposal Of ICT Equipment","This document outlines the process for the secure disposal of Essential Energy’s information technology (ICT) equipment containing security-classified material.","Evidence of prudent technology asset management process.","No"]
[null,"CEOP2322 User Access Review","To ensure that applicable controls are operating and being maintained in accordance with Essential Energy’s CEOP1003 Information Security Policy.","Evidence of technology security processes.","No"]
[null,"CEOP2325 - Operational Procedure Information Security System Monitoring","This document outlines the process for information system security monitoring of Essential Energy’s information systems.","Evidence of technology security processes.","No"]
[null,"CEOP2331 Operational Procedure: Information Security: Capacity Monitoring And Planning","The purpose of capacity monitoring and planning minimises the risk of systems failures by ensuring that information systems have enough capacity to meet the required load both now and into the future.","Evidence of technology security processes.","No"]
[null,"CEOP7003.01 - CONFIGURATION MANAGEMENT DATABASE (CMDB)","The purpose of this document is to clearly identify, define and communicate the responsibilities and accountabilities for all Essential Energy Essential Technology (eTech) employees, contractors, and vendors in relation to the Configuration Management Database (CMDB). This procedure is based on Information Technology Infrastructure Library (ITIL) Best Practice.","Evidence of prudent technology asset management process.","No"]
[null,"CEOP7009 ICT Change Management Procedure","To outline/describe the procedure for Information Communication and Technology (ICT) change management that is to be followed by the company. This procedure is based on Information Technology Infrastructure Library (ITIL) Best Practice.","Evidence of prudent technology asset management process.","No"]
[null,"CEOP7019 Software Asset Management","To provide guidance to Essential Energy employees (including agency employees, contractors, or External Service Providers) on how to adhere to Company Policy (Information & Communication Technology) - Software Asset Management Policy – CECP7018","Evidence of prudent technology asset management process.","No"]
[null,"CEOP9148.13 ICT Data Facility Procedures","The purpose of this document is to outline procedures which enable the management and control of Essential Energy’s Information Technology Data Facilities. Information Communication and Technology (ICT) Data Centre Systems team are responsible for the management of Servers and Storage and the Infrastructure that supports them, Telecommunications are responsible for communications equipment.","Evidence of prudent technology asset management process.","No"]
[null,"DFSI-2015-04-NSW Government Cloud Policy _ ARP","The policy provides guidance for NSW Government agencies to determine which cloud delivery model is best suited to their business needs.","NSW Government policy that EE are complying with in regard to technology spend on cloud based services.","No"]
[null,"NSW ICT Investment Policy And Guidelines","The Strategy recognises that opportunities for improved government performance will be provided by collaborative effort and more sustainable, consistent and standardised solutions.","NSW Government policy that EE are complying with in regard to technology spend on standardised solutions.","No"]
[null,"Preliminary Guidance On Funding As A Service Solutions","The purpose of this preliminary guidance is to provide support to agency Chief Financial Officers and Chief Information Officers for consideration in the preparation of ICT investment proposals for the 2015-16 financial year.","NSW Government policy that EE are complying with in regard to capitalisation of services based technology spend solutions.","No"]
[null,"Essential Energy 2016 Utilities IT Benchmarking Final Report 20170116","Benchmarking report presenting findings from KPMG benchmarking study of Australiasian utilities.","Benchmarks used as an efficiency measure supporting investment strategy.","No"]
[null,"ICT Systems SLA 2013 v1.5 Signed 05112013 ICT Management","Presents the ICT service level framework for providing ICT service levels to business users.","Evidence of technology service management.","No"]
[null,"Demand management policies or strategies"]
[null,"Demand Side Engagement","The objective of Essential Energy’s Demand Side Engagement Strategy is to identify non-network solutions that offer credible alternatives to network augmentation, leading to more efficient network investment and lower costs for customers.","Opex and Capex","No"]
[null,"CEOP1121 - Network Strategy – Demand Management ","Provides the long-term strategic direction for Essential Energy’s demand management program. \n","Opex and Capex","No"]
[null,"CECP0007.01 – Company Policy – Demand Management","Describes Essential Energy’s demand management policy\n","Opex and Capex","No"]
[null,"Demand Side Customer Engagement Strategy","Describes how Essential Energy engages with customers on Demand Management issues","Opex and Capex","No"]
[null,"Land and easement acquisition polices"]
[null,"CEOP 8046 - Easement Requirements","This document provides guidelines for easement requirements for powerlines in Essential Energy’s New South Wales distribution area. It outlines the need for easements, when they are required and how they are obtained. The document also describes the requirements for Essential Energy’s franchise areas in Queensland, Victoria, South Australia and ACT.","Opex and Capex","No"]
[null,"Asset security plans and policies"]
[null,"CEOM7031.6 Protective Security Manual","Covers corporate requirements and standards for security including access to sites, incident response and reporting,controls, responsibities.","Opex","No"]
[null,"CECP0002.03 Board Policy - Risk Management:","Ensure company operates within acceptable level of risk.","Opex","No"]
[null,"CECM1000.05  Emergency Preparedness","Discusses how Essential Energy prepares for possible emergencies","Opex","No"]
[null,"ENA 015-2006 National guidelines for prevention of unauthorised access to electricity infrastructure: ","Used in the design of company infrastructure including security fence specification.\n\n","Opex","No"]
[null,"HB167:2006 Security Risk Management","Standards Australia, guidance handbook  for applying risk management principles to security.","Opex","No"]
[null,"Protective Security Policy Framework (PSPF) ","Commonwealth Attorney-General's Department guidelines for enterprise security.  Company uses relevant sections for physical security.","Opex","No"]
[null,"Securing Government Business - Protective Security Guidance for Executives","Guidance notes for senior management for using the PSPF.","Opex","No"]
[null,"ISO31000:2009 Risk Management - Principles and Guidelines:","The standard with which the company's risk management framework is aligned.","Opex","No"]
[null,"Disaster recovery policy"]
[null,"CEOM7524-Business Impact Assessment: General Counsel & Company Secretary","This Manual forms the basis for implementing ‘Business Continuity’ measures which will allow General Counsel & Company Secretary to survive a range of potential disasters.","Opex","No"]
[null,"CEOM7531-Business Continuity Plan Volume 2: Business Impact Assessment - Engineering Services","This Business Impact Assessment (BIA) document forms the basis for implementing ‘Business Continuity’ measures which will allow Engineering Services to survive a range of potential disasters.","Opex","No"]
[null,"CEOM7532-Business Impact Assessment: Chief Financial Officer","Business Continuity Planning","Opex","No"]
[null,"CEOM7534-Business Impact Assessment: Network Services","This Manual forms the basis for implementing ‘Business Continuity’ measures which will allow Network Services to survive a range of potential disasters.","Opex","No"]
[null,"CEOM7542-Business Impact Assessment: Safety, Human Resources & Environment (SHRE)","Business Continuity Planning","Opex","No"]
[null,"CEOM7543-Business Impact Assessment: Customer & Stakeholder Engagement","Business Continuity Planning","Opex","No"]
[null,"CEOM7550-Recovery Action Plan: Customer Contact","This Manual contains information specific to Customer Contact's recovery which will be used 'on the day' of a business interruption.  To be used in conjunction with the Business Impact Assessment (BIA).","Opex","No"]
[null,"CEOM7551-Business Continuity Plan: Overarching Business Continuity Strategies","BCP overarching Business Continuity Strategies","Opex","No"]
[null,"CEOM7553-Recovery Action Plan: Southern Region","This recovery action plan forms part of Essential Energy’s Business Continuity processes, and is only invoked upon discovery of an actual or potential disruption at an Essential Energy depot.","Opex","No"]
[null,"CEOM7554-Recovery Action Plan: North Coast Region","Essential Energy has developed a Business Continuity response for a major event at a large depot which may impact: •\tPeople working in the complex. •\tAn entire depot complex, or buildings and infrastructure (including IT systems and communications) within the complex. •\tPlant and equipment stored in the complex. •\tStores and inventory located at the complex. •\tPlanned or fault and emergency work from the complex.","Opex","No"]
[null,"CEOM7559-Recovery Action Plan: Northern Region","This Manual forms part of Essential Energy’s Business Continuity processes, and is only invoked upon discovery of an actual or potential disruption at an Essential Energy depot.","Opex","No"]
[null,"CEOM7590-Business Continuity Plan: Warehouse – Grafton Wagga Dubbo","This procedure is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7589-Recovery Action Plan: Telecommunications","This Manual is to be invoked upon discovery of an actual or potential business disruption.","Opex","No"]
[null,"CEOM7586-Recovery Action Plan: HSE","Information for ‘the day’ of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7583-Recovery Action Plan: Network Revenue Services","Information for ‘the day’ of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7582-Recovery Action Plan: Property Services","This Procedure is to be invoked upon discovery of an actual or potential business disruption.","Opex","No"]
[null,"CEOM7581-Recovery Action Plan: Payroll","This procedure is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7580-Recovery Action Plan: Metering Services","This Manual contains information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7578-Recovery Action Plan: ICT Operations","This Procedure is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7574-Recovery Action Plan: Finance (excluding Billing, Accounts Payable & Payroll)","This Procedure is to be invoked upon discovery of an actual or potential business disruption. The associated CBA Payment Form is part of this Finance Recovery Action Plan.","Opex","No"]
[null,"CEOM7572-Operational Manual: Recovery Action Plan: Asset Management Stay @ Home Plan for: Asset Performance and Risk Commercial Services, Network Design, Engineering & Planning","This procedure is to be invoked upon discovery of an actual or potential business disruption.","Opex","No"]
[null,"CEOM7564-Recovery Action Plan: Legal Branch","This Manual is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7563-Recovery Action Plan: Customer Advocacy","This procedure is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7561-Recovery Action Plan: Network Asset Systems and Project Development","This Manual is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7602-Business Continuity Plan : ICT Incident Management","To provide ICT Incident Management information if required","Opex","No"]
[null,"CEOM7549.01-Recovery Action Plan: System Operations","Information specific to System Operations’ recovery, which will be used “on the day” of a business interruption. All the actions in this volume are based on Business Continuity activities undertaken before an incident occurs. The response to an incident will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7605-Recovery Action Plan: HR Operations","This Manual contains information for ‘the day’ of a Business Continuity event.","Opex","No"]
[null,"CEOM7607-Recovery Action Plan: Market Services","This Manual contains information for ‘the day’ of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7609-Business Continuity Plan Volume 4: SCADA Incident Mangement","Volume 4 contains the Business Continuity Incident Management (BCIM) response which will be used on the day of a business interruption. The BCIM process is an escalation of Essential Energys Incident Management process supported by IT, SCADA and Telecommunications.","Opex","No"]
[null,"CEOM7608-Recovery Action Plan: Accounts Payable","Information for ‘the day’ of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7611-Essential Water Emergency Response Plan","This Emergency Response Plan (ERP) has been prepared by the Manager Planning and Design Water and the Essential Water Emergency Management Committee in accordance with the organisation’s policies and is approved for issue by:","Opex","No"]
[null,"CECP0002.06-Company Policy - Business Continuity Management","To establish and maintain a whole of business approach to BCM that minimises the impacts of disruption-related risk on the Company’s essential service delivery. This excludes: •\tday to day operations and normal execution of critical business processes including any associated critical resource dependencies; and •\tminor localised business disruptions dealt with via business as usual work practices. ","Opex","No"]
[null,"CEOM7618-Recovery Action Plan: Finance Stay @ Home Plan for: Network Regulation, Transformation & Corporate Strategy & Planning","This Manual contains information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7619-Recovery Action Plan: Customer Connections","This Manual contains information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7622-Recovery Action Plan: Meter Reading","This Manual contains information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7624-Recovery Action Plan: Asset Operations","Information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOM7625-Recovery Action Plan: Vegetation Operations","Information for the day of a Business Continuity event. The response to a Business Continuity event will not work unless employees are familiar with their roles and responsibilities and measures to facilitate and support business recovery have been implemented.","Opex","No"]
[null,"CEOP0002.20-Company Procedure - Changes To Risk Based Management Plans","To outline the process for the management of changes to risk based management plans including changes to approved treatment action plans and strategic or operational initiatives.","Opex","No"]
[null,"CEOP0002.21-Company Procedure - Risk Management","To articulate the company’s risk management process, assessment methodology and reporting requirements. ","Opex","No"]
[null,"CEOM0002.24-Risk Assessment Training Manual","Guidance on the risk assessment process using the Bow-Tie methodology and facilitation of risk assessment workshops, in association with CEOP0002.21 Risk Management procedure and CEOF0002.23  Risk Management forms.","Opex","No"]
[null,"CEOF7630-Critical Processes - Mapping Form","Mapping to Individual Company Critical Processes","Opex","No"]
[null,"CEOP0002.34-Company Procedure: Business Continuity","To provide an overview of Business Continuity Management Framework (BCMF) and the detailed business continuity approach that minimises the impacts of disruptive events on the company’s essential service delivery.","Opex","No"]
[null,"CEOM7631-Recovery Action Plan: Fleet","This Manual contains information specific to Fleet’s recovery, which will be used ‘on the day’ of a business interruption. ","Opex","No"]
[null,"CEOM7632-Recovery Action Plan: System Control Engineering, Outage and Operational Technology","This document contains information specific to System Control Engineering’s recovery, which will be used ‘on the day’ of a business interruption. ","Opex","No"]
[null,"CEOM7633-Recovery Action Plan: Inventory & Logistics","This Manual contains information specific to Inventory & Logistics recovery, which will be used ‘on the day’ of a business interruption. ","Opex","No"]
[null,"CEOM7634-Recovery Action Plan: Essential Water","This document contains information specific to Essential Water’s recovery, which will be used ‘on the day’ of a business interruption. ","Opex","No"]
[null,"CEOM7636/7-Recovery Action Plan","This procedure is to be invoked upon discovery of an actual or potential business disruption","Opex","No"]
[null,"CEOM7639-Operational Manual: Controller of Premise Incident Management Plan","This document contains information specific to Controller of Premise’s recovery, which will be used ‘on the day’ of a business interruption. ","Opex","No"]
[null,"CEOM7807-Recovery Action Plan: Network Services Stay @ Home Plan for: Projects (excluding Zone Substations & Meter Reading) and Operational Performance","This Plan contains information for ‘the day’ of a Business Continuity event.  ","Opex","No"]
[null,"CEOM7777-Operational Manual: Recovery Action Plan: Company Secretariat Stay @ Home Plan for: Governance, Risk & Compliance (excluding Records), Internal Audit & Employee Relations.","This Manual is to be invoked upon discovery of an actual or potential business disruption. ","Opex","No"]
[null,"Self insurance guidelines or policy"]
[null,"Insurance Guidelines","This document describes Essential Energy's insurance practise, and discusses when we self insure and when transfer risk to third parties.","Opex","No"]

{"sheet":"7.1  Policies and Procedures","index":34,"n_rows":219,"n_cols":5,"rows_kept":219,"cut":false,"hidden":true,"merged":[[6,1,6,3]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.1  PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[]
[null,"Instructions"]
[null,"List and provide a brief description of key internal plans, policies, procedures or strategies that are used to plan and conduct day to day operations and that have been relied upon in the development of the regulatory proposal. Identify any internal plans, policies, procedures and strategies that have changed in the current regulatory control period or that are expected to change before the next regulatory control period where the change has been identified as a step change."]
[]
[null,"7.1.1 - PLANS, POLICIES, PROCEDURES AND STRATEGIES"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact"]
[null,null,"Description of the plan, policy, procedure or strategy.","Identify the element of the proposal/supporting documents that the policy, plan, procedure or strategy is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is this policy, plan or procedure identified in the response to section 4 'Step Changes' of the notice (yes or no)?"]
[null,"Corporate"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[null,"Governance framework"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Accounting policies, procedures and methodologies (including a capitalisation policy, depreciation policy and an approved expenditure allocation methodology)"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[null,"Asset management plan or equivalent documentation"]
[null,"Asset Management Policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Asset Management Strategies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[null,"Asset Management Plans"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Capital expenditure policies and procedures (including capex approval policies and procedures and replacement policy) "]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Internal standards for network planning, design, maintenance and operation"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Procurement and contracting out policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Information technology policies or strategies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Demand management policies or strategies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[null,"Self insurance guidelines or policy"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[null,"Land and easement acquisition polices"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[null,"Asset security plans and policies"]
[null,"<insert relevant policy, plan, strategy etc>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Disaster recovery policy"]
[null,"<insert relevant policy, plan, strategy etc>"]

{"sheet":"7.2 Contingent projects","index":35,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.2 CONTINGENT PROJECTS"]
[]
[null,"7.2.1 - PROPOSED CONTINGENT PROJECTS FOR THE FORTHCOMING REGULATORY CONTROL PERIOD"]
[null,"Proposed contingent project name","Proposed contingent capital expenditure  \n($0's, nominal)","Proposed trigger events",{"$f":"CONCATENATE(\"Proposed annual revenue requirement for \",  FRCP_y1, \" \n($0's, nominal)\")","v":"Proposed annual revenue requirement for 2019-20 \n($0's, nominal)"},{"$f":"CONCATENATE(\"5% of the annual revenue requirement for \",FRCP_y1,\"\")","v":"5% of the annual revenue requirement for 2019-20"}]
[null,"Essential Energy has no contingent projects",null,null,null,{"$f":"+E8*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},{"$f":"+E9*0.05","v":0}]
[null,null,null,null,{"$f":"+$E$8","v":0},0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]
[null,null,null,null,0,0]

{"sheet":"7.3 Obligations","index":36,"n_rows":360,"n_cols":6,"rows_kept":360,"cut":false,"hidden":false,"merged":[[6,1,6,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.3  OBLIGATIONS, REQUIREMENTS & STANDARDS"]
[]
[null,"Instructions"]
[null,"Outline those obligations and requirements that have been relied upon in the development of the regulatory proposal."]
[]
[null,"7.3.1 - OBLIGATIONS OR REQUIREMENTS"]
[null,null,"Brief description","Relevance to regulatory proposal","Expenditure impact","EE Additional Data \n(not required by the AER)"]
[null,null,"Description of relevant obligations or requirements within the instrument (e.g. safety obligations, reliability targets) ","Identify what element of the proposal/supporting documents the obligation or requirement is relevant to e.g. replacement capex, capacity utilisation thresholds, opex ","Is the obligation or requirement identified in the response to section 4 'Step Changes' of the notice (yes or no)?","Location (cut and paste location into browser)"]
[null,"LEGISLATION"]
[null,"Electricity (Consumer Safety) Act 2004 (NSW) No 4","Safety standards and requirements for customer electrical installations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2004/4/full "]
[null,"Electricity (Consumer Safety) Regulation 2015","Safety standards and requirements for customer electrical installations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2015/497"]
[null,"Electricity Supply (Corrosion Protection) Regulation 2014 No 522","Corrosion protection systems for cables and other metallic structures","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/522"]
[null,"Electricity Supply Act 1995 (NSW) No 94 ","General requirements relating to construction, operation, repair, maintenance and safety","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1995/94"]
[null,"Electricity Supply (General) Regulation 2014 No 523","Distributor service standards, consultation, ombudsman schemes","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/523"]
[null,"Electricity Supply (Safety and Network Management) Regulation 2014 No 523","Safety and network management and planning","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/524"]
[null,"Energy Services Corporations Act 1995 (NSW) No 95","General requirements relating to network management","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1995/95/full"]
[null,"Energy Services Corporations (Savings and Transitional) Regulation 1996 (NSW)","General requirements relating to network management","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/1996/65"]
[null,"Essential Services Act 1988 (NSW) No 41","General requirements relating to performance and maintenance of electricity supply","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1988/41"]
[null,"National Electricity (New South Wales) Act 1997 (NSW) No 20\n","Applied the National Electricity Law (as set out in the schedule to the National Electricity (South Australia) Act 1996) and the National Electricity Rules (as published by AEMC). The Rules are relevant to Essential Energy as a network operator as regards connection of customers Chapter 5 and 5A and economic regulation of its network Chapter 6 ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/20/full"]
[null,"National Electricity Law / National Electricity (NSW) Law No 20A","Compliance with National Electricity Law as a law in NSW - Distribution network economic regulation, planning and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/20a / http://www.legislation.sa.gov.au/LZ/C/A/NATIONAL%20ELECTRICITY%20(SOUTH%20AUSTRALIA)%20ACT%201996.aspx"]
[null,"Electricity Act 1994 (Qld)","Network operation and electrical safety management systems for EE's distribution system in QLD","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1994-064"]
[null,"Electricity Regulation 2006 (Qld)","Network operation and electrical safety management systems for EE's distribution system in QLD","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/sl-2006-0200"]
[null,"Electricity Safety Act 2002 (Qld)","Network operation and electrical safety management systems for EE's distribution system in QLD","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-2002-042"]
[null,"Electrical Safety Regulation 2013 (Qld)","Network operation and electrical safety management systems for EE's distribution system in QLD","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/sl-2013-0213"]
[null,"National Measurements Act 1960","Energy metering and accuracy","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00085"]
[null,"National Energy Retail Law (NSW) No 37A","Customer contracts, customer complaints and dispute resolution, RoLR, customer connection services","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2012/37a"]
[null,"National Energy Retail Law (Adoption) Act 2012 (NSW) No 37 and National Energy Retail Law (Adoption) Regulation 2013 (NSW)\n","Distributor liability, planned interruptions.  The National Energy Retail Law and National Energy Retails Rules are applied with changes and additions as a law of NSW from 1 July 2013 (these regulate the relationship between distributors and customers).","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2012/37/full and https://www.legislation.nsw.gov.au/#/view/regulation/2013/168/full"]
[null,"National Energy Retail Law (Queensland) Act 2014 (Qld)","Compliance with National Energy Retail Law as a law in Queensland","See Description in Column C","No","https://www.legislation.qld.gov.au/view/pdf/2015-07-01/act-2014-049 "]
[null,"National Energy Retail Law (Queensland) Regulation 2014 (Qld)","Model terms and conditions for certain deemed customer connection contracts; compliance with National Electricity Retail Rules in Queensland","See Description in Column C","No","https://www.legislation.qld.gov.au/view/pdf/2014-12-19/sl-2014-0339 "]
[null,"Marine Safety Act 1998 (NSW) No 121","Safety standards required for Marine operation on ports and waterways","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1998/121  "]
[null,"Rail Safety National Law (NSW) No 82a and the Rail Safety (Adoption of National Law) Act 2012 No 82  ","Applies a national law as a law in NSW that makes provision for a national system of rail safety; to repeal the Rail Safety Act 2008 and make consequential amendments to other legislation; to amend the Passenger Transport Act 1990 and the Transport Administration Act 1988 with respect to the regulation of transport safety; and for other purposes.","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2012/82a and https://www.legislation.nsw.gov.au/#/view/act/2012/82   "]
[null,"National Vocational Education and Training Regulator Act 2011 (Cth)","Requirements relating to registration as a Registered Training Organisation","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00245"]
[null,"ENVIRONMENT AND PLANNING",null,null,null,0]
[null,"Contaminated Land Management Act 1997 No 140 (NSW)","Remediation of sites","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/140"]
[null,"Dangerous Goods (Road and Rail Transport) Regulation 2014 No 398","Work Place Health & Safety","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/398"]
[null,"Dangerous Goods (Road and Rail Transport) Act 2008 No 95 (NSW)","Work Place Health & Safety / requirements relating to transportation of dangerous goods  by road or rail","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2008/95/full"]
[null,"Dividing Fences Act 1991 No 72 (NSW)","Obligations relating to fencing work for dividing fences between adjoining land","See Description in Column C","No","https://www.legislation.nsw.gov.au/inforce/d0d5ddf4-34ca-43e5-8b88-465e4671cdc9/1991-72.pdf"]
[null,"Encroachment of Buildings Act 1922 No 23 (NSW)","Rights and obligations relating to encroachment by buildings on adjoining land","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1922/23"]
[null,"Workers' Compensation (Dust Diseases) Act 1942 (NSW) No 14","Dust Diseases","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1942/14/full"]
[null,"Environment and Heritage Legislation Amendment Act (No.1) 2006","Environmental planning, assessment and consultation - Indigenous Heritage and environmental protection","See Description in Column C","No","https://www.legislation.gov.au/Details/C2008C00459"]
[null,"Environmental Planning and Assessment Act 1979 (NSW) No. 203","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1979/203/full"]
[null,"Environmental Planning and Assessment Amendment Act 2008 (NSW) No 36 ","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2008/36/full"]
[null,"Environmental Planning and Assessment Amendment (Part 3A Repeal) Act 2011 No 22","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2011/22/full"]
[null,"Environmental Planning and Assessment Regulation 2000 (NSW)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2000/557/full"]
[null,"Environmental Protection Act 1994 (Qld)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1994-062"]
[null,"Environment Protection and Biodiversity Conservation Act 1999 (Cth)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00777"]
[null,"Environment Protection and Biodiversity Conservation Regulations 2000 (Cth)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.gov.au/Details/F2016C00914"]
[null,"Environmentally Hazardous Chemicals Act 1985 No 14 (NSW)","Management of environmentally hazardous chemicals and chemical waste","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1985/14/full"]
[null,"Environmentally Hazardous Chemicals Regulation 2017 No 441","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/441/sec2"]
[null,"Fisheries Management Act 1994 No 38 (NSW)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1994/38/full"]
[null,"Forestry Act 2012 (NSW) No 96","Environmental planning, assessment and consultation - activities in and use of forestry areas","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2012/96/full"]
[null,"Heritage Act 1977 No 136","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1977/136/full"]
[null,"Heritage Regulation 2012","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2012/401/full"]
[null,"Land and Environment Court Act 1979 (NSW) No 204","Environmental planning, assessment and consultation \n(esp part 3 Jurisdiction of the Court and Class 3 relating to land tenure, rating and compensation matters) ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1979/204/full"]
[null,"Land and Environment Court Rules 2007","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2007/578/full"]
[null,"Local Government Act 1993 (NSW) No 30","Development of land for construction of zone substations or other electricity system infrastructure","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1993/30/full"]
[null,"Local Government and Environmental Planning and Assessment Amendment (Transfer of Functions) Act 2001 (NSW) No 93","Development of land for construction of zone substations or other electricity system infrastructure","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2001/93"]
[null,"Miscellaneous Acts (Planning) Repeal and Amendment Act 1979 (NSW) No 205","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1979/205/full"]
[null,"Miscellaneous Acts (Planning) Savings and Transitional Provisions Regulation 1980 (NSW)","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/1980/051/full"]
[null,"Coal Mine Subsidence Compensation Act 2017 No 37 ","Environmental planning, assessment and consultation - work and development within mine subsistence districts","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2017/37"]
[null,"National Environment Protection Council Act 1994 (Cth)","Implementation of miscellaneous national environmental protection measures","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00844"]
[null,"National Environment Protection Measures (Implementation) Act 1998 (Cth)","Implementation of miscellaneous national environmental protection measures","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00577"]
[null,"National Environment Protection (Movement of Controlled Waste between States and Territories) Measures (Cth)","Implementation of miscellaneous national environmental protection measures","See Description in Column C","No","https://www.legislation.gov.au/Details/F2012C00858"]
[null,"National Environment Protection Council (New South Wales) Act 1995 (NSW) No 4","General requirements relating to network management","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1995/4/full"]
[null,"National Greenhouse and Energy Reporting Act 2007 (Cth)","Reporting obligations relating to greenhouse gas and energy","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00054"]
[null,"National Parks and Wildlife Act 1974 No 80","Environmental planning, assessment and consultation - national parks, historic sites, nature reserves","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1974/80/full"]
[null,"National Parks and Wildlife Regulation 2009","Environmental planning, assessment and consultation - national parks, historic sites, nature reserves","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2009/427/full"]
[null,"Native Title Act 1993 (Cth)","Environmental planning, assessment and consultation - acts affected by native title","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00178"]
[null,"Native Title (New South Wales) Act 1994 (NSW) No 45","Electrical infrastructure construction dealings affected by native title","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1994/45/full"]
[null,"Local Land Services Act 2013 (NSW) No 51","Environmental planning, assessment and consultation - clearing of native vegetation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2016/63"]
[null,"Biodiversity Conservation (Savings and Transitional) Regulation 2017","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/433/whole"]
[null,"Vegetation Management Act 1999 (Qld) ","Vegetation Management in Qld","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1999-090"]
[null,"Biosecurity Act 2015, No 24","Identification and control of noxious weeds","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2015/24/full"]
[null,"Ozone Protection Act 1989 (NSW) No 208","Management of equipment with substances that deplete stratospheric ozone ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/208/full"]
[null,"Pesticides Act 1999 (NSW) No 80","Use and management of pesticides for treatment of termites","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1999/80/full"]
[null,"Pesticides Regulation 2017 No 448","Use and management of pesticides for treatment of termites","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/448/full"]
[null,"Biosecurity Regulation 2017 No 232 ","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/232"]
[null,"Property, Stock and Business Agents Act 2002 (NSW) No 66","Requirements relating to registration and conduct of property, stock and business agents","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2002/66/full"]
[null,"Protection of the Environment Operations Act 1997 (NSW) No 156","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/156/full"]
[null,"Protection of the Environment Operations (General) Regulation 2009","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2009/211/full"]
[null,"Protection of the Environment Administration Act 1991 (NSW) No 60","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1991/60/full"]
[null,"Protection of the Environment Administration Regulation 2012","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2012/409/full"]
[null,"Protection of the Environment Operations (Noise Control) Regulation 2017 No 449","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/449"]
[null,"Protection of the Environment Operations (Waste) Regulation 2014  No 666","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/666/part1/sec2"]
[null,"Protection of the Environment Operations (Clean Air) Regulation 2010","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2010/428/full"]
[null,"Radiation Control Act 1990 (NSW) No 13","Miscellaneous environmental obligations - sale, use, keeping and disposal of radioactive substances and radiation apparatus","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1990/13/full"]
[null,"Renewable Energy (Electricity) Act 2000 (Cth) and Renewable Energy (Electricity) Regulations 2001 (Cth)","Miscellaneous environmental obligations - Renewable Energy Target scheme (The legislation and accompanying regulations, under which the RET scheme is administered)","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00624 and https://www.legislation.gov.au/Details/F2017C01227"]
[null,"Retail Leases Act 1994 (NSW) No 46","Obligations relating to leasing of retail shops","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1994/46/full"]
[null,"Rural Fires Act 1997 No 65","Prevention and mitigation of bushfires","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/65/full"]
[null,"State Emergency and Rescue Management Act 1989 (NSW) No 165","Obligations relating to responding to emergencies in NSW","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/165/full"]
[null,"Telecommunications (Interception and Access) Act 1979 (Cth) ","Obligations relating to restrictions on interception of and access to telecommunications","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00308"]
[null,"Telecommunications Act 1997 (Cth) ","Obligations relating to supply of telecommunications services ","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00357"]
[null,"Trade Support Loans Act 2014 (Cth)","Qualification of apprentices for trade support loans and repayments of trade support loans","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00122"]
[null,"Utilities Act 2000 (ACT) and Utilities Exemption 2012 (No 1) DI2012-146 (ACT)","Obligations relating to provision of electricity distribution and connection services along the ACT-NSW border ","See Description in Column C","No","http://www.legislation.act.gov.au/a/2000-65/current/pdf/2000-65.pdf "]
[null,"Water Act 1912 (NSW) No 44","Environmental planning, assessment and consultation - licences and permits for works relating to water","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1912/44/full"]
[null,"Water NSW Act 2014 (NSW) No 74","Environmental planning, assessment and consultation - activities affecting water","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2014/74/full"]
[null,"Western Lands Act 1901 (NSW) No 70","Environmental planning, assessment and consultation - Use of, access to and leasing of land in the Western Division (NSW)","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1901/70/full"]
[null,"A New Tax System (Goods and Services Tax) Act 1999 (Cth )","Obligations relating to collection and payment of Goods and Services Tax","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00361"]
[null,"Bankruptcy Act 1966 (Cth)","Actions relating to bankruptcy","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00197"]
[null,"Corporations Act 2001 (Cth) \n","General provisions relating to regulation of corporations, including actions relating to insolvency","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00328"]
[null,"Soil Conservation Act 1938 (NSW) No 10","Environmental planning, assessment and consultation - construction and easement management","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1938/10"]
[null,"Roads Act 1993 (NSW) No 33","Carrying out of various activities on public roads","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1993/33/full"]
[null,"Road Transport Act 2013 (NSW) No 18","Registration of vehicles and traffic control/safety","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2013/18/full"]
[null,"Biodiversity Conservation Act 2016 No 63","Environmental planning, assessment and consultation - threatened species, populations and ecological communities of animals/plants","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2016/63"]
[null,"Nature Conservation Act 1992 (Qld) ","Environmental planning, assessment and consultation - nature conservation","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1992-020"]
[null,"Valuation of Land Act 1916 (NSW) No 2","General rules relating to valuation of land","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1916/2/full"]
[null,"Land Act 1994 (Qld)","Environmental planning, assessment and consultation - land in Queensland; general requirements relating to land transactions in Queensland","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1994-081"]
[null,"Land Title Act 1994 (Qld)","General requirements relating to land transactions in Queensland","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/act-1994-011"]
[null,"Biodiversity Conservation Regulation 2017","Environmental planning, assessment and consultation - threatened species, populations and ecological communities of animals/plants","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/432/full"]
[null,"Waste Avoidance and Resource Recovery Act 2001 (NSW) No 58","Miscellaneous environmental obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2001/58/full"]
[null,"Water Management Act 2000 (NSW) No 92","Environmental planning, assessment and consultation - protection of water sources/quality","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2000/92/full"]
[null,"Wilderness Act 1987 (NSW) No 196","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1987/196/full"]
[null,"GENERAL"]
[null,"Annual Reports (Statutory Bodies) Act 1984 (NSW) No 87","Preparation of annual report","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1984/87/full"]
[null,"Annual Reports (Statutory Bodies) Regulation 2015","Preparation of annual report","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2015/493/full"]
[null,"Multicultural NSW Act 2000 No 77","Active promotion of employee equal opportunity, employee development programs","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2000/77/full"]
[null,"Crimes Act 1900 (NSW) No 40","General criminal law obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1900/40/full"]
[null,"Defamation Act 2005 (NSW) No 77","General defamation law obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2005/77/full"]
[null,"Aboriginal Land Rights Act 1983 (NSW) No 42","Requirements relating to dealings affected by Aboriginal land claims","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1983/42/full"]
[null,"Building Energy Efficiency Disclosure Act 2010 (Cth)","Requirements relating to building energy efficiency disclosure and certificates","See Description in Column C","No","https://www.legislation.gov.au/Details/C2015C00369"]
[null,"Clean Energy Legislation (Carbon Tax Repeal) Act 2014 (Cth)","Transitional provisions relating to carbon tax repeal","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00166"]
[null,"Energy and Utilities Administration Act 1987 (NSW)  No 103","Promotion of customer awareness of safe, effective and efficient use of energy","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1987/103/full"]
[null,"Fair Trading Act 1987 No 68 (NSW)","Provision of safely designed and constructed infrastructure, other consumer protection requirements","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1987/68/full"]
[null,"Fair Trading Regulation 2012 (NSW)","Provision of safely designed and constructed infrastructure, other consumer protection requirements","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2012/427/full"]
[null,"Fines Act 1996 (NSW) No 99","Payment of any monetary penalty","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1996/99/full"]
[null,"Government Telecommunications Act 1991 (NSW) No 77","Government information ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1991/77/full"]
[null,"Government Information (Public Access) Act 2009 No 52","Government information ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2009/52/full"]
[null,"Government Information (Public Access) Regulation 2009","Government information ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2010/343/full"]
[null,"Home Building Act 1989 (NSW)  No 147","Residential building work and specialist work which includes electrical wiring. ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/147/full"]
[null,"Mutual Recognition (Automatic Licensed Occupations Recognition) Act 2014 (NSW) No 51","Occupation recognition","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2014/51/full"]
[null,"Independent Commission Against Corruption Act 1988 (NSW) No 35","Responding to an ICAC investigation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1988/35/full"]
[null,"Independent Commission Against Corruption Regulation 2017","Responding to an ICAC investigation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/479"]
[null,"Ombudsman Act 1974 (NSW) No 68","Requirements relating to Ombudsman investigations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1974/68/full"]
[null,"Independent Pricing and Regulatory Tribunal Act 1992 (NSW) No 39","Compliance with 2004 IPART Determination, NSW economic regulation framework, WAPC","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1992/39/full"]
[null,"Insurance Act 1973 (Cth)","Prudential standards relating to general insurance and regulation of insurance activities","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00065"]
[null,"Insurance Contracts Act 1984 (Cth)","Obligations relating to insurance contracts","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00820"]
[null,"Infrastructure NSW Act 2011 No 23","State infrastructure Act","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2011/23/full"]
[null,"Natural Resources Commission Act 2003 (NSW) No 102","General environmental requirements","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2003/102/full"]
[null,"Public Authorities (Financial Arrangements) Act 1987 (NSW) No 33","General requirements relating to financial arrangements or joint ventures","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1987/33/full"]
[null,"Public Authorities (Financial Arrangements) Regulation 2013 (NSW)","General requirements relating to financial arrangements or joint ventures","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2013/487/full"]
[null,"Public Finance and Audit Act 1983 (NSW) No 152","Financial, compliance and performance audits","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1983/152/full"]
[null,"Public Finance and Audit Regulation 2015 No 502","Financial, compliance and performance audits","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2015/502"]
[null,"Government Sector Employment Act 2013 No 40","Employment obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2013/40/full"]
[null,"Radiocommunications Act 1992 (Cth)","Obligations relating to licensing of radio communication devices","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00356"]
[null,"State Owned Corporations Act 1989 (NSW) No 134\n\n","Requirements and compliance relating to corporations law, corporate governance, SCI, reporting","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/134/full"]
[null,"Cybercrime Act 2001 (Cth)","Criminal law obligations relating to unauthorised access to or modification of data held in computer and unauthorised impairment of electronic communications","See Description in Column C","No","https://www.legislation.gov.au/Details/C2004C01213"]
[null,"Electronic Transactions Act 1999 (Cth)","Requirements relating to electronic transactions and contracts involving electronic communications","See Description in Column C","No","https://www.legislation.gov.au/Details/C2011C00445"]
[null,"Electronic Transactions Act 2000 (NSW) No 8","Requirements relating to electronic transactions and contracts involving electronic communications","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2000/8/full"]
[null,"Evidence Act 1995 (NSW) No 25 ","Evidentiary requirements for Court proceedings","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1995/25/full"]
[null,"State Records Act 1998 (NSW) No 17","Records management","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1998/17/full"]
[null,"State Records Regulation 2015","Records management","See Description in Column C","No","https://www.legislation.nsw.gov.au/regulations/2015-505.pdf"]
[null,"Spam Act 2003 (Cth)","Requirements relating to commercial electronic messages","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00614"]
[null,"Competition and Consumer Act 2010 (Cth)  ","General requirements relating to network management and consumer protection","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00375"]
[null,"Competition and Consumer Regulations 2010","General requirements relating to network management and consumer protection","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C01060"]
[null,"Superannuation Administration (Electricity Superannuation Scheme Transitional Provisions) Regulation 1997 (NSW)","Employment obligations","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/1997/294/full"]
[null,"PROPERTY",0,0,"No",0]
[null,"Access to Neighbouring Land Act 2000 (NSW) No 2","Neighbouring land access","See Description in Column C","No","https://www.legislation.nsw.gov.au/inforce/aeed5fdf-c5ef-ccce-d48d-c208e5b58abb/2000-2.pdf"]
[null,"Building and Construction Industry Long Service Payments Act 1986 (NSW) No 19 ","Requirements relating to long service payments/levies","See Description in Column C","No","https://legislation.nsw.gov.au/inforce/89778421-d2a1-e0fb-8080-ccf42c3467be/1986-19.pdf"]
[null,"Building and Construction Industry Long Service Levy","Long Service Levy","See Description in Column C","No","http://www.longservice.nsw.gov.au/bci"]
[null,"Building and Construction Industry Security of Payment Act 1999 (NSW) No 46","Payment for Security","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1999/46/full"]
[null,"Community Land Development Act 1989 (NSW) No 201","Development of land for electrical infrastructure, service centres, etc","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/201/full"]
[null,"Community Land Management Act 1989 (NSW) No 202","Management of schemes under the Community Land Development Act 1989 (NSW)","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/202"]
[null,"Community Land Development Regulation 2007 (NSW)","Development of land for electrical infrastructure, field and customer service centres","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2007/410/full"]
[null,"Contaminated Land Management Act 1997 (NSW) No 140","Remediation of sites","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/140/full"]
[null,"Contaminated Land Management Regulation 2013","Remediation of sites","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2013/491/full"]
[null,"Conveyancing Act 1919 (NSW) No 6","Application of general rules affecting property, sales, transactions, mortgages, leases etc","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1919/6/full"]
[null,"Conveyancing (General) Regulation 2013","Application of general rules affecting property, sales, transactions, mortgages, leases etc","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2013/495/full"]
[null,"Conveyancing (Sale of Land) Regulation 2017","Application of general rules affecting property, sales, transactions, mortgages, leases etc","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/372"]
[null,"Crown Lands Act 1989 (NSW) No 6","Creation of line easement/access over crown lands","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1989/6/full"]
[null,"Crown Lands Regulation 2006 (NSW)","Creation of line easement/access over crown lands","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2006/508/full"]
[null,"Duties Act 1997 (NSW) No 123","Payment of duties on land transactions","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/123/full"]
[null,"Land Acquisition (Just Terms Compensation) Act 1991 (NSW)","Compensation for acquisition of land for electricity system infrastructure","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1991/22/full"]
[null,"Land Tax Management Act 1956 (NSW) No 26","Payment of land taxes","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1956/26/full"]
[null,"Land Tax Act 1956 (NSW) No 27","Payment of land taxes","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1956/27/full"]
[null,"Real Property Act 1900 (NSW) No 25","Application of general requirements relating to land transactions","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1900/25/full"]
[null,"Real Property Regulation 2014","Application of general requirements relating to land transactions","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/536/full"]
[null,"Strata Schemes Development Act 2015 (NSW) No 51","Development of land","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2015/51/full"]
[null,"Strata Schemes Management Act 2015 (NSW) No 50","Development of land","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2015/50/full"]
[null,"EMPLOYMENT AND OCCUPATIONAL HEALTH AND SAFETY"]
[null,"Age Discrimination Act 2004 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2018C00022"]
[null,"Annual Holidays Act 1944 (NSW) No 31","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1944/31"]
[null,"Annual Holidays Regulation 2016","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2016/537/full"]
[null,"Anti-Discrimination Act 1977 (NSW) No 48","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1977/48/full"]
[null,"Anti-Discrimination Regulation 2014","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/554/full"]
[null,"Apprenticeship and Traineeship Act 2001 (NSW) No 80","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2001/80/full"]
[null,"Apprenticeship and Traineeship Regulation 2017","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/229/full"]
[null,"Contractors Debts Act 1997 (NSW) No 110","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/110/full"]
[null,"Disability Discrimination Act 1992 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00339"]
[null,"Disability Discrimination Regulations 1996 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2012C00527"]
[null,"Employees Liability Act 1991 (NSW) No 4","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1991/4/full"]
[null,"Employment Protection Act 1982 (NSW) No 122","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1982/122/full"]
[null,"Employment Protection Regulation 2017","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/478"]
[null,"Workplace Gender Equality Act 2012","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00895"]
[null,"Fringe Benefits Tax Act 1986 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2015C00611"]
[null,"Fringe Benefits Tax Regulations 1992 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2015C00695"]
[null,"Fringe Benefits Tax Assessment Act 1986 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00276"]
[null,"Fuel Tax Act 2006 (Cth) ","Requirements relating to fuel tax credits","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00004"]
[null,"Australian Human Rights Commission Act 1986","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00143"]
[null,"Australian Human Rights Commission Act 1986 (Cth)  ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00143"]
[null,"Australian Jobs Act 2013 (Cth)  ","Procurement of goods and services for major projects","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00165"]
[null,"Criminal Records Act 1991 (NSW) No 8  ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1991/8/full"]
[null,"Income Tax Act 1986 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00461"]
[null,"Income Tax Rates Act 1986 (Cth) ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00189"]
[null,"Income Tax Assessment (1936 Act) Regulation 2015","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C00433"]
[null,"Income Tax Assessment Act 1936 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00242"]
[null,"Income Tax Assessment Act 1997 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2018C00002"]
[null,"Income Tax Assessment Regulations 1997 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C01075"]
[null,"Independent Contractors Act 2006 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00818"]
[null,"Independent Contractors Regulation 2016","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2016L01896"]
[null,"Industrial Relations (Child Employment) Act 2006 (NSW) No 96","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2006/96/full"]
[null,"Industrial Relations Act 1996 (NSW) No 17","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1996/17/full"]
[null,"Industrial Relations (General) Regulation 2015","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2015/458/full"]
[null,"Jury Act 1977 (NSW) No 18 ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1977/18/full"]
[null,"Surveillance Devices Act 2007 (NSW) No 64","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2007/64/full"]
[null,"Long Service Leave Act 1955 (NSW) No 38","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1955/38/full"]
[null,"Long Service Leave Regulation 2016","Workplace and employment obligations, and related process","See Description in Column C","No","https://legislation.nsw.gov.au/#/view/regulation/2016/547/full"]
[null,"Work Health and Safety Act 2011 No 10","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2011/10/full"]
[null,"Work Health and Safety Act 2011 No 137 (Cth)","Handling of hazardous and dangerous materials","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00305"]
[null,"Work Health and Safety Regulation 2017 No 404","Workplace and employment obligations, and related process","See Description in Column C","No","https://legislation.nsw.gov.au/#/view/regulation/2017/404"]
[null,"Work Health and Safety Regulation 2011 (Cth)","Work Place Health & Safety","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C00580"]
[null,"Work Health and Safety Act 2011 (Qld)","Work Place Health & Safety","See Description in Column C","No","https://www.legislation.qld.gov.au/view/html/inforce/current/sl-2011-0240"]
[null,"Work Health and Safety (Transitional and Consequential Provisions) Act 2011","Workplace Health & Safety","See Description in Column C","No","https://www.legislation.gov.au/Details/C2011A00146"]
[null,"Payroll Tax Act 2007 (NSW) No 21","Payment of levied payroll taxes ","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2007/21/full"]
[null,"Personal Property Securities Act 2009 (Cth)","Requirements relating to security interests in personal property ","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00149"]
[null,"Public Interest Disclosures Act 1994 (NSW) No 92","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1994/92/full"]
[null,"Smoke-free Environment Act 2000 (NSW) No 69","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2000/69/full"]
[null,"Security Industry Act 1997 (NSW) No 157 ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1997/157/full"]
[null,"Government Sector Employment Act 2013 (NSW) No 40","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2013/40/full"]
[null,"Government Sector Employment Regulation 2014","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2014/60/full"]
[null,"Paid Parental Leave Act 2010 (Cth)","Parental leave pay payable to a person","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00081"]
[null,"Racial Discrimination Act 1975 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00089"]
[null,"Restraints of Trade Act 1976 (NSW) No 67","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1976/67/full"]
[null,"Sex Discrimination Act 1984 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00383"]
[null,"Sex Discrimination Regulations 1984 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2018C00017"]
[null,"Superannuation Contributions Tax (Assessment and Collection) Act 1997 (Cth) ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2016C00701"]
[null,"Superannuation Contributions Tax Imposition Act 1997 (Cth) ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2005C00530"]
[null,"Superannuation Guarantee (Administration) Act 1992 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00230"]
[null,"Superannuation Guarantee (Administration) Regulations 1993 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2015C00631"]
[null,"Superannuation Guarantee Charge Act 1992 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2004C00841"]
[null,"Superannuation Industry (Supervision) Act 1993 (Cth) ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00052"]
[null,"Taxation Administration Act 1953 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2018C00011"]
[null,"Taxation Administration Regulations 2017 ","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C01184 "]
[null,"Taxation Administration Act 1996 (NSW) No 97","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1996/97/full"]
[null,"Termination Payments Tax (Assessment and Collection) Act 1997 (Cth)","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2010C00873"]
[null,"Fair Work Act 2009","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00323"]
[null,"Fair Work Regulations 2009","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2018C00023"]
[null,"Workers Compensation Act 1987 (NSW) No 70","Workplace injury management, insurance","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1987/70/full"]
[null,"Workers Compensation Regulation 2016","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2016/559/full"]
[null,"Workplace Injury Management and Workers Compensation Act 1998 (NSW) No 86","Workplace injury management, insurance","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/1998/86/full"]
[null,"Workplace Surveillance Act 2005 (NSW) No 47","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2005/47/full"]
[null,"Workplace Surveillance Regulation 2017","Workplace and employment obligations, and related process","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/regulation/2017/417"]
[null,"Work Health and Safety (Mines and Petroleum Sites) Act 2013 ","The compliance requirement is the application of a health and safety management system and the general design requirements relating to electrical plant.","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2013/54"]
[null,"PRIVACY"]
[null,"Privacy Act 1988 (Cth)","Application of privacy laws and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/C2017C00283"]
[null,"Privacy Regulation 2013","Application of privacy laws and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2018C00011"]
[null,"Privacy (Credit Reporting) Code 2014 (Version 1.2)","Application of privacy laws and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2014L00459"]
[null,"Health Records and Information Privacy Act 2002 (NSW) No 71 ","Application of privacy laws and related process (to the extent collecting, holding or using health information)","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/act/2002/71/full"]
[null,"Privacy (Tax File Number) Rule 2015","Application of privacy laws and related process","See Description in Column C","No","https://www.legislation.gov.au/Details/F2015L00249"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"LICENSES"]
[null,"Reliability and Performance Licence Conditions for Electricity Distributors, 1 July 2014","Network reliability and security of supply standards and conditions, compliance reporting","See Description in Column C","No","https://www.ipart.nsw.gov.au/files/sharedassets/website/trimholdingbay/electricity_-_regulatory_instruments_-_dnsp_conditions_14_-_19_-_july_2014.pdf"]
[null,"Electricity distribution licence conditions via the Electricity Supply Act 1995 ","Investigations regarding expansion of distribution system; NEM registration requirements; separation of distribution system business and ring-fencing; requirements relating to customer connection contracts and provision of connection services; reporting and compliance systems; licence fees ","See Description in Column C","No","https://www.ipart.nsw.gov.au/files/sharedassets/website/trimholdingbay/website_document_-_electricity_-_regulatory_instruments_-_dnsp_conditions_1_-_13.pdf"]
[null,"IPART Electricity Networks Reporting Manuals (October 2017):\n- Incident Reporting\n- Electricity network safety management systems\n- Bushfire Preparedness\n- Compliance with reliability and performance standards\n- Compliance with other licence conditions","The IPART Reporting Manuals contain IPART's reporting requirements for holders of NSW electricity distribution licences in relation to matters such as incidents, performance, bushfire risk management and compliance with licence conditions. ","See Description in Column C","No","https://www.ipart.nsw.gov.au/Home/Industries/Energy/Energy-Networks-Safety-Reliability-and-Compliance/Electricity-networks/Reportinghttp://www.ipart.nsw.gov.au/Home/Industries/Electricity/Licensing/Licence_Compliance"]
[null,"RULES"]
[null,"NSW Service and Installation Rules","Customer electricity equipment and installation - safety and compliance","See Description in Column C","No","http://www.resourcesandenergy.nsw.gov.au/energy-supply-industry/pipelines-electricity-gas-networks/network-connections/rules"]
[null,"Wiring Rules, AS/NZS 3000:2007","Produced by the joint Standards Australia/Standards New Zealand Committee EL-001, the revised edition expands on issues relating to electrical installations, improves safeguards and, addresses the needs and expectations of stakeholders.","See Description in Column C","No","http://www.wiringrules.standards.org.au/"]
[null,"National Energy Retail Rules","Obligations in relation to the provision of customer connection services, re-energisation, de-energisation planned and unplanned interruptions, deemed connection contracts","See Description in Column C","No","http://www.aemc.gov.au/Energy-Rules/Retail-energy-rules/Current-rules"]
[null,"National Electricity Rules","The National Electricity Rules govern the operation of the National Electricity Market. The Rules have the force of law, and are made under the National Electricity Law. Copies of the National Electricity Rules are available for inspection at the AEMC's office in Sydney.","See Description in Column C","No","http://www.aemc.gov.au/energy-rules/national-electricity-rules/current-rules"]
[]
[]
[]
[]
[]
[null,"CODES"]
[null,"National Electricity Network Safety Code, ENA Doc 001-2008","Network safety, design, construction, maintenance and operational practices","See Description in Column C","No","https://infostore.saiglobal.com/store/details.aspx?ProductID=1021044"]
[null,"National guidelines for safe access to electrical and mechanical apparatus, ENA NENS 03-2006","Network operations and safety practices","See Description in Column C","No","https://infostore.saiglobal.com/en-au/standards/ena-nens-03-2006-589398/"]
[null,"National guidelines for safe approach distances to electrical and mechanical apparatus, ENA NENS 04-2006","Network operations and safety practices","See Description in Column C","No","https://infostore.saiglobal.com/en-au/Standards/ENA-NENS-04-2006-589399/"]
[null,"National guidelines for aerial surveillance of overhead electricity networks, ENA NENS 08-2006","Asset inspection and maintenance program","See Description in Column C","No","https://infostore.saiglobal.com/store/Details.aspx?ProductID=589402"]
[null,"Code of Practice - Electricity Service Standards","Published electricity supply standards","See Description in Column C","No","https://www.resourcesandenergy.nsw.gov.au/energy-supply-industry/pipelines-electricity-gas-networks/network-connections/electricity_connect_code_of_practice_electricity_service_standards.pdf"]
[null,"Code of Practice - Risk Management","Risk management","See Description in Column C","No",0]
[null,"AS/NZS 3835.1:2006 Earth potential rise - Protection of telecommunications network users, personnel and plant Code of practice","Line design and construction, safety standards","See Description in Column C","No","https://infostore.saiglobal.com/en-au/Standards/AS-NZS-3835-1-2006-375170/"]
[null,"Work Health and Safety (How to Safely Remove Asbestos) Code of Practice 2015 ","Asbestos Removal Safety","See Description in Column C","No","https://www.legislation.gov.au/Details/F2016L00418"]
[null,"Code for the Tendering and Performance of Building Work 2016","Building Codes","See Description in Column C","No","https://www.legislation.gov.au/Details/F2017C00668"]
[null,"NSW Public Lighting Code","The NSW Public Lighting Code is designed to help clarify the relationship between Public Lighting Service Providers and Public Lighting Customers.","See Description in Column C","No","https://www.resourcesandenergy.nsw.gov.au/energy-supply-industry/legislation-and-policy/electricity-legislation/code-review/electricity_legislation_nsw_public_lighting_code.pdf"]
[]
[]
[]
[]
[]
[null,"GUIDELINES"]
[null,"Guideline for the Fire Protection of Electricity Substations, ENA Doc 018-2015 ","Design and construction standards","See Description in Column C","No","ESAA Guideline"]
[null,"ENA EG1-2006 Substation Earthing Guide","Design and construction standards","See Description in Column C","No","ENA guideline - https://infostore.saiglobal.com/store/Details.aspx?ProductID=589392"]
[null,"ISSC3 Guide for the Management of Vegetation in the Vicinity of Electricity Assets, November 2016","Vegetation management program","See Description in Column C","No","https://www.resourcesandenergy.nsw.gov.au/energy-supply-industry/pipelines-electricity-gas-networks/electricity-networks/safety/ISSC3-guideline-for-managing-vegetation-near-power-lines.pdf"]
[null,"ISSC 14 - Guide to electrical workers' safety equipment, October 2010","Network operations and safety practices","See Description in Column C","No","https://www.resourcesandenergy.nsw.gov.au/energy-supply-industry/pipelines-electricity-gas-networks/electricity-networks/safety/ISSC14-Guide-to-Electrical-Workers-Safety-Equipment-Oct-10.pdf "]
[null,"ISSC 20 - Guideline for the Management of Activities within Electricity Easements and Close to Electricity Infrastructure, September 2012","Line design and construction, environmental planning and assessment","See Description in Column C","No","https://www.resourcesandenergy.nsw.gov.au/__data/assets/pdf_file/0004/466816/ISSC-20-Electricity-Easements.pdf"]
[null,"Joint use of poles, HB87-1997","Placement on poles of power lines and paired cable telecommunications lines","See Description in Column C","No","https://infostore.saiglobal.com/en-au/Standards/HB-87-1997-CJC-1--569149/"]
[null,"Risk Management Guidelines, SA/SNZ HB 436:2013","Risk management","See Description in Column C","No","https://infostore.saiglobal.com/en-au/standards/sa-snz-hb-436-2013-1694350/"]
[null,"NSW State Government's Total Asset Management Manual","Asset management planning, policies, strategies","See Description in Column C","No","ESAA Guideline"]
[null,"NSW Government Guide to Cost-Benefit Analysis TPP17-03, NSW Treasury, 2017","Expenditure appraisals","See Description in Column C","No","ESAA Guideline"]
[null,"NSW Government Guidelines for Financial Appraisal TPP07-4, NSW Treasury Policy and Guidelines Paper, 2007","Expenditure appraisals","See Description in Column C","No","https://www.treasury.nsw.gov.au/sites/default/files/pdf/TPP07-4_Commercial_Policy_Framework-_Guidelines_for_Financial_Appraisal.pdf"]
[null,"Connection charge guidelines for electricity retail customers under chapter 5A of the National Electricity Rules","Sets out the circumstances where a retail customer or real estate developer to pay a connection charge and the pioneer scheme.","See Description in Column C","No","https://www.aer.gov.au/system/files/AER%20-%20connection%20charge%20guideline%20-%2020%20June%202012.pdf"]
[null,"AER compliance procedures and guidelines National Energy Retail Law, Retail Rules and Retail Regulations","Sets out the manner in which regulated entities must submit information to the AER relating to compliance.","See Description in Column C","No","https://www.aer.gov.au/retail-markets/retail-guidelines-reviews/compliance-procedures-and-guidelines-december-2017 "]
[null,"Default agreements "]
[null,"Essential Energy Customer Connection Contracts and Connection Offers","Preparation and availability Customer Connection Contracts and Offers","See Description in Column C","No","http://www.essentialenergy.com.au/content/connection-offers-and-contracts"]
[null,"Other"]
[null,"Essential Energy Undertaking to the AER for the two years ending 30 June 2018 and 30 June 2019, 8 May 2017","Compliance with economic regulation framework","See Description in Column C","No","https://www.aer.gov.au/system/files/Essential%20Energy%20enforceable%20undertaking%20-%208%20May%202017.pdf"]
[null,"AER Final Decision Essential Energy Distribution Determination 2015-19, April 2015 (as applied by reference to Essential Energy's Undertaking referred to in the row above)","Compliance with economic regulation framework (although the Determination has been set aside and not yet remade, the Undertaking referred to in the row above provides for its application to some extent).","See Description in Column C","No","https://www.aer.gov.au/networks-pipelines/determinations-access-arrangements/essential-energy-determination-2014-19/final-decision"]
[null,"“Insulation of Overhead Service Lines”, Department of Energy, September 1996","Asset renewal program","See Description in Column C","No",0]
[null,"State Environmental Planning Policy 14 - Coastal Wetlands","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1985/532/full"]
[null,"State Environmental Planning Policy 19 - Bushland in Urban Areas","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1986/014/full"]
[null,"State Environmental Planning Policy 26 - Littoral Rainforests","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1988/111/full"]
[null,"State Environmental Planning Policy 44 - Koala Habitat","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1995/5/full"]
[null,"State Environmental Planning Policy 71 - Coastal Protection","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/2002/816/full"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DEFAULT AGREEMENTS "]
[null,"Essential Energy Customer Connection Contracts and Connection Offers","Preparation and availability Customer Connection Contracts and Offers","See Description in Column C","No","http://www.essentialenergy.com.au/content/connection-offers-and-contracts"]
[]
[]
[null,"OTHER"]
[null,"Essential Energy Undertaking to the AER for the two years ending 30 June 2018 and 30 June 2019, 8 May 2017","Compliance with economic regulation framework","See Description in Column C","No","https://www.aer.gov.au/system/files/Essential%20Energy%20enforceable%20undertaking%20-%208%20May%202017.pdf"]
[null,"AER Final Decision Essential Energy Distribution Determination 2015-19, April 2015 (as applied by reference to Essential Energy's Undertaking referred to in the row above)","Compliance with economic regulation framework (although the Determination has been set aside and not yet remade, the Undertaking referred to in the row above provides for its application to some extent).","See Description in Column C","No","https://www.aer.gov.au/networks-pipelines/determinations-access-arrangements/essential-energy-determination-2014-19/final-decision"]
[null,"“Insulation of Overhead Service Lines”, Department of Energy, September 1996","Asset renewal program","See Description in Column C","No",0]
[null,"State Environmental Planning Policy 14 - Coastal Wetlands","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1985/532/full"]
[null,"State Environmental Planning Policy 19 - Bushland in Urban Areas","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1986/014/full"]
[null,"State Environmental Planning Policy 26 - Littoral Rainforests","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1988/111/full"]
[null,"State Environmental Planning Policy 44 - Koala Habitat","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/1995/5/full"]
[null,"State Environmental Planning Policy 71 - Coastal Protection","Environmental planning, assessment and consultation","See Description in Column C","No","https://www.legislation.nsw.gov.au/#/view/EPI/2002/816/full"]

{"sheet":"7.4 Shared Assets","index":37,"n_rows":30,"n_cols":19,"rows_kept":30,"cut":false,"hidden":false,"merged":[[6,11,6,18],[32,2,32,8],[6,1,7,1],[6,2,7,2],[6,3,6,10],[25,1,26,1],[25,2,26,8],[27,2,27,8],[28,2,28,8],[29,2,29,8],[30,2,30,8],[31,2,31,8],[39,2,39,8],[40,2,40,8],[41,2,41,8],[33,2,33,8],[34,2,34,8],[35,2,35,8],[36,2,36,8],[37,2,37,8],[38,2,38,8]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.4 SHARED ASSETS"]
[]
[null,"7.4.1 - TOTAL UNREGULATED REVENUE EARNED WITH SHARED ASSETS "]
[null,"Name of shared asset unregulated service","Description of shared assets used to provide the service","Shared asset unregulated revenue  ($0's, nominal)",null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Shared asset unregulated revenue  ($0's, real \", dms_DollarReal,\")\")","v":"Shared asset unregulated revenue  ($0's, real June 2019)"}]
[null,null,null,{"$f":"PRCP_y1","v":"2009-10"},{"$f":"PRCP_y2","v":"2010-11"},{"$f":"PRCP_y3","v":"2011-12"},{"$f":"PRCP_y4","v":"2012-13"},{"$f":"PRCP_y5","v":"2013-14"},{"$f":"CRCP_y1","v":"2014-15"},{"$f":"CRCP_y2","v":"2015-16"},{"$f":"CRCP_y3","v":"2016-17"},{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CONCATENATE(\"Total \n\",CRCP_y5, \" to \", dms_MultiYear_FinalYear_Result)","v":"Total \n2018-19 to 2023-24"}]
[null,"Fibre Optic Income","Pole access for installation of fibre optic cable for telecommunication purposes",65314.684080573134,67475.339784601791,80140.395773831871,81443.217793062402,83433.027718839308,270026,1076721.1599999999,589307.83999999985,461250.01025000017,450000,2757753.7711933237,2724957.2442892375,2658494.8724773051,2612604.2686784267,2579199.8940284858,{"$f":"SUM(M9:R9)","v":13783010.050666779}]
[null,"NBN Income","Pole access for installation of fibre optic cable for telecommunication purposes",0,8736.409999999998,36204.576478791394,36630.990447414282,109550.88999999998,284892.17,905449.95000000007,358182.47999999975,717500.0307499998,717500.00000000047,717500.00000000047,717500.00000000047,717500.00000000047,717500.00000000047,717500.00000000047,{"$f":"SUM(M10:R10)","v":4305000.0000000028}]
[null,"Rental Income","Rental income from property leasing and tower access for a third party to install radio frequency equipment for use in telecommunications equipment. ",714214.82,805684.75,808684.75,808684.75,849118.98750000005,2108116.9900000002,1420452.3499999999,1143968.3999999997,1362767.0097500002,1133301.4300000006,1133301.4300000006,1133301.4300000006,1133301.4300000006,1133301.4300000006,1133301.4300000006,6799808.5800000038]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,"7.4.2 - SHARED ASSET UNREGULATED SERVICES - APPORTIONMENT METHODOLOGY"]
[null,"Name of shared asset unregulated service for which revenues were apportioned","Apportionment methodology"]
[]
[null,"Fibre Optic Income","Specific to the number of poles used, value per pole and annual escalation rates"]
[null,"NBN Income","Essential Energy and NBN Co have entered into a Facilities Access Agreement since June 2010. this agreement has been extended a number of times in order to expand the scope NBN Co is allowed to roll out its program."]
[null,"Rental Income","Each lease arrangement for Radio Towers are with individual access seekers. Price and terms vary. Each lease for Property Rentals vary on price and terms"]

{"sheet":"7.6 Indicative bill impact","index":38,"n_rows":57,"n_cols":13,"rows_kept":57,"cut":false,"hidden":false,"merged":[[21,2,21,3],[31,2,31,3],[6,1,6,2]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.6 INDICATIVE IMPACT ON DISTRIBUTION CHARGES & ELECTRICITY BILLS"]
[]
[null,"Instructions"]
[null,{"$f":"CONCATENATE(dms_TradingName,\" is required to populate all input cells (yellow) in table 7.6.1 presented below.\")","v":"Essential Energy is required to populate all input cells (yellow) in table 7.6.1 presented below."}]
[]
[null,"7.6.1 - INDICATIVE IMPACT OF THE REGULATORY PROPOSAL ON THE AVERAGE RESIDENTIAL ELECTRICITY BILLS"]
[]
[null,"Distribution costs as a proportion of a typical customer's electricity bill (per cent)",0.36599999999999999]
[null,"Source:","2017-18 forecast Australian Energy Market Commission, 2017 Residential Electricity Price Trends, 18 December 2017 pg 100, NUOS 47.9"]
[]
[null,"Typical electricity bill - Residential customer"]
[null,"Tariff type","Description of tariff type",{"$f":"CONCATENATE(\"Annual bill amount \n($\",  dms_CRCP_FinalYear_Result,\")\")","v":"Annual bill amount \n($2018-19)"}]
[null,"Regulated tariff","Origin Domestic standing offer - 5MWh/p.a.",1975.9811367499999]
[]
[]
[]
[]
[]
[null,"Souce: ","Origins Standing offer Price fact sheet (effective 21 Sept17) from their website escalated by CPI 1.95% to $18/19 - Domestic Anytime"]
[]
[null,"Typical electricity bill - Business customer"]
[null,"Tariff type","Description of tariff type",{"$f":"CONCATENATE(\"Annual bill amount \n($\",  dms_CRCP_FinalYear_Result,\")\")","v":"Annual bill amount \n($2018-19)"}]
[null,"Regulated tariff","Origin Sml Business standing offer - 23MWh/p.a.",9158.5870047500011]
[]
[]
[]
[]
[]
[null,"Souce:","Origins Standing offer Price fact sheet (effective 1 Jul 17) from their website escalated by CPI 1.95% to $18/19 - Business Anytime"]
[]
[null,"Indicative annual average distribution price impact"]
[null,null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},"Average"]
[null,"Forecast smoothed revenues ($ nominal)",null,963518472.14235032,985378746.67033458,1024436908.3226823,1065043246.2441199,1107259126.6039395,1151148347.9861445,1196777237.8048103]
[null,{"$f":"CONCATENATE(\"Forecast smoothed revenues ($ real \",dms_DollarReal,\")\")","v":"Forecast smoothed revenues ($ real June 2019)"},null,982307082.34912622,985378746.67033458,999450642.26603162,1013723494.3430054,1028200172.699934,1042883588.1182206,1057776692.9472566]
[]
[null,"Energy delivered forecast (MWh)",null,12306400,12287100,12288600,12272200,12248600,12279600,12307100]
[]
[null,"Annual price path ($/MWh, nominal)",null,{"$f":"+D36/D39","v":78.294096741723848},{"$f":"+E36/E39","v":80.196201436493112},83.364818475878636,86.785030087850586,90.398831425953944,93.744775724465342,97.242830382853015]
[null,{"$f":"CONCATENATE(\"Annual price path ($/MWh, \",dms_DollarReal,\")\")","v":"Annual price path ($/MWh, June 2019)"},null,{"$f":"+D37/D39","v":79.820831628187463},{"$f":"+E37/E39","v":80.196201436493112},81.331530220369416,82.603241011636499,83.944301609974531,84.928140014187804,85.948492573169673]
[]
[null,"Annual price path (per cent, nominal)",null,null,{"$f":"+E41/D41-1","v":2.4294356457600141E-2},{"$f":"+F41/E41-1","v":3.9510812016386287E-2},{"$f":"+G41/F41-1","v":4.1027038437822183E-2},4.1640837532062713E-2,3.7013136627237042E-2,3.7314662404966059E-2,{"$f":"+AVERAGE(F44:J44)","v":3.9301297403694854E-2}]
[null,{"$f":"CONCATENATE(\"Annual price path (per cent, \",dms_DollarReal,\")\")","v":"Annual price path (per cent, June 2019)"},null,null,{"$f":"+E42/D42-1","v":4.702654691123076E-3},{"$f":"+F42/E42-1","v":1.4156889772084291E-2},1.5636135061289913E-2,1.6234963445915129E-2,1.172013329486532E-2,1.2014304785332719E-2,{"$f":"+AVERAGE(F45:J45)","v":1.3952485271897474E-2}]
[]
[]
[null,"Distribution bill component - Residential customer",null,"Real"]
[null,"Tariff typea",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", IF(SUM(dms_SingleYear_Model)>0,\"\",dms_MultiYear_FinalYear_Result))","v":"Total 2019-20 to 2023-24"},"Annual average","Annual impact on customer bill (%)"]
[null,{"$f":"+B16","v":"Regulated tariff"},null,723.20909605049997,{"$f":"+D50*(1+IF($D$48=\"Nominal\",E$44,E$45))","v":726.61009869870475},736.89663777326564,748.41885312769887,760.56940585046073,769.48338066702468,778.72818852960654,{"$f":"+SUM(F50:J50)","v":3794.0964659480564},{"$f":"+AVERAGE(F50:J50)","v":758.81929318961124}]
[null,"Annual change",null,null,{"$f":"+E50-D50","v":3.4010026482047806},10.286539074560892,11.522215354433229,12.150552722761859,8.9139748165639503,9.2448078625818653,{"$f":"+SUM(F51:J51)","v":52.118089830901795},{"$f":"+AVERAGE(F51:J51)","v":10.423617966180359},{"$f":"+L51/D16","v":5.2751606644001834E-3}]
[]
[]
[null,"Distribution bill component - Business customer",null,"Real"]
[null,"Tariff typea",null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"CRCP_y5","v":"2018-19"},{"$f":"FRCP_y1","v":"2019-20"},{"$f":"FRCP_y2","v":"2020-21"},{"$f":"FRCP_y3","v":"2021-22"},{"$f":"FRCP_y4","v":"2022-23"},{"$f":"FRCP_y5","v":"2023-24"},{"$f":"CONCATENATE(\"Total \",FRCP_y1,\" to \", IF(SUM(dms_SingleYear_Model)>0,\"\",dms_MultiYear_FinalYear_Result))","v":"Total 2019-20 to 2023-24"},"Annual average","Annual impact on customer bill (%)"]
[null,{"$f":"+B26","v":"Regulated tariff"},null,{"$f":"+D26*$C$11","v":3352.0428437385003},{"$f":"+D56*(1+IF($D$54=\"Nominal\",E$44,E$45))","v":3367.8063437424526},3415.4840069245406,3468.8889761564883,3525.206261882327,3566.5221491634816,3609.3714332871714,{"$f":"+SUM(F56:J56)","v":17585.472827414007},{"$f":"+AVERAGE(F56:J56)","v":3517.0945654828015}]
[null,"Annual change",null,null,{"$f":"+E56-D56","v":15.763500003952231},47.677663182088054,53.404969231947689,56.317285725838701,41.315887281154573,42.849284123689813,{"$f":"+SUM(F57:J57)","v":241.56508954471883},{"$f":"+AVERAGE(F57:J57)","v":48.313017908943763},{"$f":"+L57/D26","v":5.2751606644001687E-3}]

{"sheet":"7.7 TSS-LRMC","index":39,"n_rows":150,"n_cols":22,"rows_kept":150,"cut":false,"hidden":false,"merged":[[8,1,9,1],[8,2,8,21],[19,1,20,1],[19,2,19,21],[30,1,31,1],[30,2,30,21],[107,2,107,21],[122,2,122,21],[137,2,137,21],[44,1,45,1],[44,2,44,21],[64,1,65,1],[64,2,64,21],[84,1,85,1],[84,2,84,21]]}
[null,{"$f":"SheetHeader","v":"REGULATORY REPORTING STATEMENT"}]
[null,{"$f":"dms_TradingName","v":"Essential Energy"}]
[null,{"$f":"dms_Reg_Year_Span","v":"2019-20 to 2023-24"}]
[null,"7.7 - TARIFF STRUCTURE STATEMENT - INPUTS TO LRMC CALCULATION"]
[]
[]
[null,"7.7.1 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - CAPEX"]
[null,"7.7.1.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C10,4)+1)&\"-\"&MID(C10,3,2)+2),VALUE(LEFT(C10,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[null,"Replacement expenditure",13561765.994975001,13365511.425000001,13779387.2179725,13752067.703457391,13279716.552837951,13177526.654668162,12918593.627224613,12918593.627224613,12918593.627224613,12918593.627224613,12918593.627224613,12918593.627224613,11415519.700774368,10948698.572812855,10465493.693049708,9938773.2945332043,9455813.2404466067,8994136.1685970929,8553923.1009294093,8130340.2294984991]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",33757306.839450434,20940326.079999998,23083648.416906182,19773925.03071003,16867023.238841377,17809753.968132693,17114701.715839066,17114701.715839066,17114701.715839066,17114701.715839066,17114701.715839066,17114701.715839066,15123412.056116391,14504962.045979474,13864806.652643424,13167001.398574587,12527170.353116315,11915535.247798391,11332335.90257957,10771168.432987383]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex",{"$f":"SUM(C11:C16)","v":47319072.834425434},{"$f":"SUM(D11:D16)","v":34305837.504999995},36863035.63487868,33525992.734167419,30146739.79167933,30987280.622800857,30033295.343063679,30033295.343063679,30033295.343063679,30033295.343063679,30033295.343063679,30033295.343063679,26538931.756890759,25453660.618792329,24330300.345693134,23105774.693107791,21982983.593562923,20909671.416395485,19886259.003508978,18901508.662485883]
[]
[null,"7.7.1.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C21,4)+1)&\"-\"&MID(C21,3,2)+2),VALUE(LEFT(C21,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[null,"Replacement expenditure",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex"]
[]
[null,"7.7.1.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C32,4)+1)&\"-\"&MID(C32,3,2)+2),VALUE(LEFT(C32,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[null,"Replacement expenditure",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Connections",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Augmentation Expenditure",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Non-network",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised network overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Capitalised corporate overheads",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Total capex"]
[]
[]
[]
[null,"7.7.2 - INPUTS TO LRMC CALCULATION - STANDARD CONTROL SERVICES - OPEX"]
[null,"7.7.2.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C46,4)+1)&\"-\"&MID(C46,3,2)+2),VALUE(LEFT(C46,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[null,"Opex related to asset growth",0,0,5392351.8207223685,4864053.9188415781,3579748.4157492598,5612264.4506340018,4366625.6347124316,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex",{"$f":"SUM(C47:C61)","v":0},{"$f":"SUM(D47:D61)","v":0},5392351.8207223685,4864053.9188415781,3579748.4157492598,5612264.4506340018,4366625.6347124316,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"7.7.2.2- SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C66,4)+1)&\"-\"&MID(C66,3,2)+2),VALUE(LEFT(C66,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[null,"7.7.2.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C86,4)+1)&\"-\"&MID(C86,3,2)+2),VALUE(LEFT(C86,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total opex"]
[]
[]
[]
[null,"7.7.3 - INPUTS TO LRMC CALCULATION - DEMAND"]
[null,"7.7.3.1 - SERIES A"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C109,4)+1)&\"-\"&MID(C109,3,2)+2),VALUE(LEFT(C109,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[null,"Peak system demand",2300.7851553344949,2302.0015741467187,2309.5082114349207,2309.0724788118901,2314.3192343276364,2311.6168530204386,2331.8399050079088,2344.8943901048838,2361.398507178832,2375.9592223733462,2391.1538180604625,2408.6518542709987,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[]
[null,"Total demand",{"$f":"SUM(C110:C119)","v":2300.7851553344949},{"$f":"SUM(D110:D119)","v":2302.0015741467187},2309.5082114349207,2309.0724788118901,2314.3192343276364,2311.6168530204386,2331.8399050079088,2344.8943901048838,2361.398507178832,2375.9592223733462,2391.1538180604625,2408.6518542709987,0,0,0,0,0,0,0,0]
[]
[null,"7.7.3.2 - SERIES B"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C124,4)+1)&\"-\"&MID(C124,3,2)+2),VALUE(LEFT(C124,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]
[]
[null,"7.7.3.3 - SERIES C"]
[null,null,{"$f":"CONCATENATE(\"Forecast \n($0's, real \", dms_DollarReal)","v":"Forecast \n($0's, real June 2019"}]
[null,null,{"$f":"CRCP_y4","v":"2017-18"},{"$f":"IF(dms_RPT=\"financial\",(VALUE(LEFT(C139,4)+1)&\"-\"&MID(C139,3,2)+2),VALUE(LEFT(C139,4)+1))","v":"2018-19"},"2019-20","2020-21","2021-22","2022-23","2023-24","2024-25","2025-26","2026-27","2027-28","2028-29","2029-30","2030-31","2031-32","2032-33","2033-34","2034-35","2035-36","2036-37"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Total demand"]

{"sheet":"Amendments","index":40,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,1,0,3]]}
[null,{"$f":"CONCATENATE(dms_TradingName,\" data amendments\")","v":"Essential Energy data amendments"}]
[null,{"$f":"INDEX(dms_TradingNameFull_List,MATCH(dms_TradingName,dms_TradingName_List))","v":"Essential Energy"},"Table","Comments"]