{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"MURRAYLINKV5_20211201204024"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"16.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (64-bit) NT 10.00"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"MURRAYLINK"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2015]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2015-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2015-12-31"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":544}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":9}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":553}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2015 Version: 5"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":9},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":40},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":544},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":544}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":593},null,{"$f":"SUM($P$46:$P$65)","v":544}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation",null,null,"2021-12-01T20:40:24"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":19428,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[1,"MURRAYLINKV5_20211201203644","2015-02-14T18:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.620619999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[2,"MURRAYLINKV5_20211201203644","2015-02-14T18:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-27.717400000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[3,"MURRAYLINKV5_20211201203644","2015-02-14T18:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-28.13334,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[4,"MURRAYLINKV5_20211201203644","2015-02-14T19:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-27.13081,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[5,"MURRAYLINKV5_20211201203644","2015-02-14T19:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-31.406079999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[6,"MURRAYLINKV5_20211201203644","2015-02-14T19:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-61.036729999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[7,"MURRAYLINKV5_20211201203644","2015-02-14T19:15:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,113.80301,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[8,"MURRAYLINKV5_20211201203644","2015-02-14T19:20:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-31.627880000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[9,"MURRAYLINKV5_20211201203644","2015-02-14T19:25:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-31.92445,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[10,"MURRAYLINKV5_20211201203644","2015-02-14T19:30:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.783380000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[11,"MURRAYLINKV5_20211201203644","2015-02-14T19:35:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-31.627590000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[12,"MURRAYLINKV5_20211201203644","2015-02-14T19:40:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-31.011240000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[13,"MURRAYLINKV5_20211201203644","2015-02-14T19:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.68967,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[14,"MURRAYLINKV5_20211201203644","2015-02-14T19:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-32.472430000000003,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[15,"MURRAYLINKV5_20211201203644","2015-02-14T19:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.74062,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[16,"MURRAYLINKV5_20211201203644","2015-02-14T20:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.727809999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[17,"MURRAYLINKV5_20211201203644","2015-02-14T20:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.686709999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[18,"MURRAYLINKV5_20211201203644","2015-02-14T20:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-33.838590000000003,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[19,"MURRAYLINKV5_20211201203644","2015-02-14T20:15:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.254580000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[20,"MURRAYLINKV5_20211201203644","2015-02-14T20:20:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.703330000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[21,"MURRAYLINKV5_20211201203644","2015-02-14T20:25:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.623560000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[22,"MURRAYLINKV5_20211201203644","2015-02-14T20:30:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.682289999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[23,"MURRAYLINKV5_20211201203644","2015-02-14T20:35:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.37059,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[24,"MURRAYLINKV5_20211201203644","2015-02-14T20:40:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.20186,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[25,"MURRAYLINKV5_20211201203644","2015-02-14T20:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.371130000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[26,"MURRAYLINKV5_20211201203644","2015-02-14T20:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.882840000000002,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[27,"MURRAYLINKV5_20211201203644","2015-02-14T20:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.9268,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[28,"MURRAYLINKV5_20211201203644","2015-02-14T21:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.85474,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[29,"MURRAYLINKV5_20211201203644","2015-02-14T21:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.54954,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[30,"MURRAYLINKV5_20211201203644","2015-02-14T21:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.317889999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[31,"MURRAYLINKV5_20211201203644","2015-02-14T21:15:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.30969,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[32,"MURRAYLINKV5_20211201203644","2015-02-14T21:20:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.387730000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[33,"MURRAYLINKV5_20211201203644","2015-02-14T21:25:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.400469999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[34,"MURRAYLINKV5_20211201203644","2015-02-14T21:30:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.396229999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[35,"MURRAYLINKV5_20211201203644","2015-02-14T21:35:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-25.20579,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[36,"MURRAYLINKV5_20211201203644","2015-02-14T21:40:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.286909999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[37,"MURRAYLINKV5_20211201203644","2015-02-14T21:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.554860000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[38,"MURRAYLINKV5_20211201203644","2015-02-14T21:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-16.51652,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[39,"MURRAYLINKV5_20211201203644","2015-02-18T15:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.876059999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[40,"MURRAYLINKV5_20211201203644","2015-02-18T16:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.346310000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[41,"MURRAYLINKV5_20211201203644","2015-02-18T16:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.11576,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[42,"MURRAYLINKV5_20211201203644","2015-02-18T18:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.61196,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[43,"MURRAYLINKV5_20211201203644","2015-02-18T18:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.02422,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[44,"MURRAYLINKV5_20211201203644","2015-02-20T17:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.783519999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","At 1735 hrs a runback of Murraylink occurred","UNPLANNED",0]
[45,"MURRAYLINKV5_20211201203644","2015-02-20T17:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.08414,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","At 1735 hrs a runback of Murraylink occurred","UNPLANNED",0]
[46,"MURRAYLINKV5_20211201203644","2015-03-25T06:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.06269,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[47,"MURRAYLINKV5_20211201203644","2015-03-25T06:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.92999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[48,"MURRAYLINKV5_20211201203644","2015-03-25T13:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.568429999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[49,"MURRAYLINKV5_20211201203644","2015-03-25T13:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.404059999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[50,"MURRAYLINKV5_20211201203644","2015-03-25T13:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.928269999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[51,"MURRAYLINKV5_20211201203644","2015-03-25T13:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.92395,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[52,"MURRAYLINKV5_20211201203644","2015-03-25T13:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.77962,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[53,"MURRAYLINKV5_20211201203644","2015-03-25T13:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.930160000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[54,"MURRAYLINKV5_20211201203644","2015-03-25T13:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.94528,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[55,"MURRAYLINKV5_20211201203644","2015-03-25T13:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.08877,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[56,"MURRAYLINKV5_20211201203644","2015-03-25T14:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.492349999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[57,"MURRAYLINKV5_20211201203644","2015-03-25T14:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.61914,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[58,"MURRAYLINKV5_20211201203644","2015-03-25T14:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.43427,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[59,"MURRAYLINKV5_20211201203644","2015-03-25T14:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.29529,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[60,"MURRAYLINKV5_20211201203644","2015-03-25T14:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.29208,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[61,"MURRAYLINKV5_20211201203644","2015-03-25T14:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-183.71155999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[62,"MURRAYLINKV5_20211201203644","2015-03-25T14:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.745380000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[63,"MURRAYLINKV5_20211201203644","2015-03-25T14:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-46.782049999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[64,"MURRAYLINKV5_20211201203644","2015-03-25T15:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.716259999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[65,"MURRAYLINKV5_20211201203644","2015-03-25T15:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.121729999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[66,"MURRAYLINKV5_20211201203644","2015-03-25T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.39358,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[67,"MURRAYLINKV5_20211201203644","2015-03-25T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.39588,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[68,"MURRAYLINKV5_20211201203644","2015-03-25T15:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.90264,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[69,"MURRAYLINKV5_20211201203644","2015-03-25T15:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.46529,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[70,"MURRAYLINKV5_20211201203644","2015-03-25T15:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-305.09604000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[71,"MURRAYLINKV5_20211201203644","2015-03-25T15:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.584619999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[72,"MURRAYLINKV5_20211201203644","2015-03-25T16:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.431340000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[73,"MURRAYLINKV5_20211201203644","2015-03-25T16:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.065530000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[74,"MURRAYLINKV5_20211201203644","2015-03-25T17:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.4305,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[75,"MURRAYLINKV5_20211201203644","2015-03-25T17:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.25507,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[76,"MURRAYLINKV5_20211201203644","2015-03-25T17:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.25568,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[77,"MURRAYLINKV5_20211201203644","2015-03-25T17:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.733879999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[78,"MURRAYLINKV5_20211201203644","2015-03-25T17:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.64555,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[79,"MURRAYLINKV5_20211201203644","2015-03-25T17:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.07582,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[80,"MURRAYLINKV5_20211201203644","2015-04-15T06:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.932130000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[81,"MURRAYLINKV5_20211201203644","2015-04-15T07:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.52637,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[82,"MURRAYLINKV5_20211201203644","2015-04-15T07:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.780940000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[83,"MURRAYLINKV5_20211201203644","2015-04-15T07:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.024380000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[84,"MURRAYLINKV5_20211201203644","2015-04-15T07:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.446389999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[85,"MURRAYLINKV5_20211201203644","2015-04-15T07:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.540889999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[86,"MURRAYLINKV5_20211201203644","2015-04-15T07:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.22096,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[87,"MURRAYLINKV5_20211201203644","2015-04-15T07:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.57235,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[88,"MURRAYLINKV5_20211201203644","2015-04-15T07:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.60779,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[89,"MURRAYLINKV5_20211201203644","2015-04-15T07:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.882960000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[90,"MURRAYLINKV5_20211201203644","2015-04-15T07:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.78191,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[91,"MURRAYLINKV5_20211201203644","2015-04-15T07:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.217829999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[92,"MURRAYLINKV5_20211201203644","2015-04-15T19:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.060700000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[93,"MURRAYLINKV5_20211201203644","2015-04-29T14:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.84483,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[94,"MURRAYLINKV5_20211201203644","2015-04-29T14:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.984480000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[95,"MURRAYLINKV5_20211201203644","2015-04-29T14:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.84479,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[96,"MURRAYLINKV5_20211201203644","2015-04-29T14:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.565940000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[97,"MURRAYLINKV5_20211201203644","2015-04-29T14:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.844709999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[98,"MURRAYLINKV5_20211201203644","2015-04-29T14:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.844749999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[99,"MURRAYLINKV5_20211201203644","2015-04-29T15:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.72354,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[100,"MURRAYLINKV5_20211201203644","2015-04-29T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.748279999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[101,"MURRAYLINKV5_20211201203644","2015-04-29T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-3063.7964099999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[102,"MURRAYLINKV5_20211201203644","2015-04-29T19:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.262450000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","Outage due to Murraylink runback scheme operation","UNPLANNED",0]
[103,"MURRAYLINKV5_20211201203644","2015-04-29T19:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.517510000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","Outage due to Murraylink runback scheme operation","UNPLANNED",0]
[104,"MURRAYLINKV5_20211201203644","2015-06-10T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13185.344709999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[105,"MURRAYLINKV5_20211201203644","2015-06-10T13:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-533.05286000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[106,"MURRAYLINKV5_20211201203644","2015-06-10T13:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-533.97450000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[107,"MURRAYLINKV5_20211201203644","2015-06-10T13:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-241.08466999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[108,"MURRAYLINKV5_20211201203644","2015-06-10T13:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13185.344709999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[109,"MURRAYLINKV5_20211201203644","2015-06-10T13:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-241.18281999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[110,"MURRAYLINKV5_20211201203644","2015-06-10T14:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-241.18281999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[111,"MURRAYLINKV5_20211201203644","2015-06-10T14:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-241.18281999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[112,"MURRAYLINKV5_20211201203644","2015-06-10T14:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13185.344709999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[113,"MURRAYLINKV5_20211201203644","2015-07-02T10:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.603100000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[114,"MURRAYLINKV5_20211201203644","2015-07-02T10:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-309.44162,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[115,"MURRAYLINKV5_20211201203644","2015-07-02T10:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.839,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[116,"MURRAYLINKV5_20211201203644","2015-07-02T11:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.972239999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[117,"MURRAYLINKV5_20211201203644","2015-07-02T11:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.365590000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[118,"MURRAYLINKV5_20211201203644","2015-07-02T11:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.771899999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[119,"MURRAYLINKV5_20211201203644","2015-07-02T11:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.175170000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[120,"MURRAYLINKV5_20211201203644","2015-07-02T11:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.997420000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[121,"MURRAYLINKV5_20211201203644","2015-07-02T11:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.20307,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[122,"MURRAYLINKV5_20211201203644","2015-07-02T11:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.96227,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[123,"MURRAYLINKV5_20211201203644","2015-07-02T11:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.745660000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[124,"MURRAYLINKV5_20211201203644","2015-07-02T11:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.789439999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[125,"MURRAYLINKV5_20211201203644","2015-07-02T11:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.943860000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[126,"MURRAYLINKV5_20211201203644","2015-07-02T11:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.864319999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[127,"MURRAYLINKV5_20211201203644","2015-07-02T12:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.53548,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[128,"MURRAYLINKV5_20211201203644","2015-07-02T12:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.937250000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[129,"MURRAYLINKV5_20211201203644","2015-07-02T12:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.1005,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[130,"MURRAYLINKV5_20211201203644","2015-07-02T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.72184,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[131,"MURRAYLINKV5_20211201203644","2015-07-02T12:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.77984,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[132,"MURRAYLINKV5_20211201203644","2015-07-02T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.875019999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[133,"MURRAYLINKV5_20211201203644","2015-07-02T12:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.42022,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[134,"MURRAYLINKV5_20211201203644","2015-07-02T12:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.963940000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[135,"MURRAYLINKV5_20211201203644","2015-07-02T12:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.42942,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[136,"MURRAYLINKV5_20211201203644","2015-07-02T12:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.194520000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[137,"MURRAYLINKV5_20211201203644","2015-07-02T12:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.20382,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[138,"MURRAYLINKV5_20211201203644","2015-07-02T12:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.988720000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[139,"MURRAYLINKV5_20211201203644","2015-07-02T13:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-311.23561999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[140,"MURRAYLINKV5_20211201203644","2015-07-19T12:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.435490000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","At 1146 hrs Murraylink runback scheme operated and Murraylink was reduced to zero MW.","UNPLANNED",0]
[141,"MURRAYLINKV5_20211201203644","2015-07-19T12:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.561109999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","At 1146 hrs Murraylink runback scheme operated and Murraylink was reduced to zero MW.","UNPLANNED",0]
[142,"MURRAYLINKV5_20211201203644","2015-07-19T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.757850000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","At 1146 hrs Murraylink runback scheme operated and Murraylink was reduced to zero MW.","UNPLANNED",0]
[143,"MURRAYLINKV5_20211201203644","2015-07-21T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413964.6875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[144,"MURRAYLINKV5_20211201203644","2015-07-21T12:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-56.030880000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[145,"MURRAYLINKV5_20211201203644","2015-07-21T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-57.131570000000004,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[146,"MURRAYLINKV5_20211201203644","2015-07-21T12:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413964.78125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[147,"MURRAYLINKV5_20211201203644","2015-07-21T12:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413944.78125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[148,"MURRAYLINKV5_20211201203644","2015-07-21T12:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413945.5,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[149,"MURRAYLINKV5_20211201203644","2015-07-21T12:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413945.5,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[150,"MURRAYLINKV5_20211201203644","2015-07-21T12:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413945.53125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[151,"MURRAYLINKV5_20211201203644","2015-07-21T12:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413955.34375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[152,"MURRAYLINKV5_20211201203644","2015-07-21T13:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413956.46875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[153,"MURRAYLINKV5_20211201203644","2015-07-21T13:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413958.09375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[154,"MURRAYLINKV5_20211201203644","2015-07-21T13:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.6875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[155,"MURRAYLINKV5_20211201203644","2015-07-21T13:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413953.4375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[156,"MURRAYLINKV5_20211201203644","2015-07-21T13:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413956.28125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[157,"MURRAYLINKV5_20211201203644","2015-07-21T13:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413955.25,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[158,"MURRAYLINKV5_20211201203644","2015-07-21T13:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413955.25,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[159,"MURRAYLINKV5_20211201203644","2015-07-21T13:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.46875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[160,"MURRAYLINKV5_20211201203644","2015-07-21T13:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413955.03125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[161,"MURRAYLINKV5_20211201203644","2015-07-21T13:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.53125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[162,"MURRAYLINKV5_20211201203644","2015-07-21T13:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.46875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[163,"MURRAYLINKV5_20211201203644","2015-07-21T13:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.84375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[164,"MURRAYLINKV5_20211201203644","2015-07-21T14:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.9375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[165,"MURRAYLINKV5_20211201203644","2015-07-21T14:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413953.4375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[166,"MURRAYLINKV5_20211201203644","2015-07-21T14:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413953.9375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[167,"MURRAYLINKV5_20211201203644","2015-07-21T14:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413955.78125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[168,"MURRAYLINKV5_20211201203644","2015-07-21T14:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413954.71875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[169,"MURRAYLINKV5_20211201203644","2015-07-21T14:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413953.96875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[170,"MURRAYLINKV5_20211201203644","2015-07-21T14:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413950.90625,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[171,"MURRAYLINKV5_20211201203644","2015-07-21T14:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413963.46875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[172,"MURRAYLINKV5_20211201203644","2015-07-21T14:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413945.28125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[173,"MURRAYLINKV5_20211201203644","2015-07-21T14:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413968.03125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[174,"MURRAYLINKV5_20211201203644","2015-07-21T14:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-59.647359999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[175,"MURRAYLINKV5_20211201203644","2015-07-21T14:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413965.21875,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[176,"MURRAYLINKV5_20211201203644","2015-07-21T15:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413965,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[177,"MURRAYLINKV5_20211201203644","2015-07-21T15:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413958.03125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[178,"MURRAYLINKV5_20211201203644","2015-07-21T15:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-61.964230000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[179,"MURRAYLINKV5_20211201203644","2015-07-21T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413970.34375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[180,"MURRAYLINKV5_20211201203644","2015-07-21T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413964.09375,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[181,"MURRAYLINKV5_20211201203644","2015-07-21T15:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-413970.3125,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage event originated from third party: the Berri converter station was tripped from Monash substation by ElectraNet technicians undertaking protection testing.","UNPLANNED",0]
[182,"MURRAYLINKV5_20211201203644","2015-07-30T05:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.50352,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[183,"MURRAYLINKV5_20211201203644","2015-07-30T05:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.283010000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[184,"MURRAYLINKV5_20211201203644","2015-07-30T05:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.406750000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[185,"MURRAYLINKV5_20211201203644","2015-07-30T05:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.797420000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[186,"MURRAYLINKV5_20211201203644","2015-07-30T05:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.15319,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[187,"MURRAYLINKV5_20211201203644","2015-07-30T05:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.75672,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[188,"MURRAYLINKV5_20211201203644","2015-07-30T06:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.28492,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[189,"MURRAYLINKV5_20211201203644","2015-07-30T16:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.39967,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[190,"MURRAYLINKV5_20211201203644","2015-07-30T17:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.715389999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[191,"MURRAYLINKV5_20211201203644","2015-07-30T17:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.65053,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[192,"MURRAYLINKV5_20211201203644","2015-07-30T17:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.27327,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[193,"MURRAYLINKV5_20211201203644","2015-07-30T17:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.794339999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[194,"MURRAYLINKV5_20211201203644","2015-07-30T17:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.99212,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[195,"MURRAYLINKV5_20211201203644","2015-07-30T17:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.399709999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[196,"MURRAYLINKV5_20211201203644","2015-07-30T19:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-54.42201,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[197,"MURRAYLINKV5_20211201203644","2015-07-30T19:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.063299999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[198,"MURRAYLINKV5_20211201203644","2015-07-30T19:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-56.36356,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[199,"MURRAYLINKV5_20211201203644","2015-07-30T19:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-56.276209999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[200,"MURRAYLINKV5_20211201203644","2015-07-30T20:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-54.25479,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[201,"MURRAYLINKV5_20211201203644","2015-07-30T20:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.738010000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[202,"MURRAYLINKV5_20211201203644","2015-07-30T20:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.688760000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[203,"MURRAYLINKV5_20211201203644","2015-07-30T20:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.13458,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[204,"MURRAYLINKV5_20211201203644","2015-07-30T20:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-54.320399999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[205,"MURRAYLINKV5_20211201203644","2015-07-30T20:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-54.00347,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[206,"MURRAYLINKV5_20211201203644","2015-07-30T20:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.143680000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[207,"MURRAYLINKV5_20211201203644","2015-07-30T20:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-55.738010000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[208,"MURRAYLINKV5_20211201203644","2015-07-30T21:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.126110000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[209,"MURRAYLINKV5_20211201203644","2015-07-30T21:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-56.742330000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[210,"MURRAYLINKV5_20211201203644","2015-07-30T21:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-56.742330000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[211,"MURRAYLINKV5_20211201203644","2015-07-30T21:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-57.870980000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[212,"MURRAYLINKV5_20211201203644","2015-07-30T21:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.03101,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[213,"MURRAYLINKV5_20211201203644","2015-07-30T21:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.81907,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[214,"MURRAYLINKV5_20211201203644","2015-07-30T22:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.966699999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[215,"MURRAYLINKV5_20211201203644","2015-07-31T08:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-201.68206000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[216,"MURRAYLINKV5_20211201203644","2015-07-31T08:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.5235,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[217,"MURRAYLINKV5_20211201203644","2015-07-31T08:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-303.95614,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[218,"MURRAYLINKV5_20211201203644","2015-07-31T08:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-314.54764,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[219,"MURRAYLINKV5_20211201203644","2015-07-31T08:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-314.87007,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[220,"MURRAYLINKV5_20211201203644","2015-07-31T08:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-305.71143999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[221,"MURRAYLINKV5_20211201203644","2015-07-31T09:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-302.14499000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[222,"MURRAYLINKV5_20211201203644","2015-07-31T09:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-314.26465999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[223,"MURRAYLINKV5_20211201203644","2015-07-31T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-317.05970000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[224,"MURRAYLINKV5_20211201203644","2015-07-31T10:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-53.177100000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[225,"MURRAYLINKV5_20211201203644","2015-07-31T10:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-53.617240000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[226,"MURRAYLINKV5_20211201203644","2015-07-31T11:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.551629999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[227,"MURRAYLINKV5_20211201203644","2015-07-31T11:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.012550000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[228,"MURRAYLINKV5_20211201203644","2015-07-31T11:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.029409999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[229,"MURRAYLINKV5_20211201203644","2015-07-31T11:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.493310000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[230,"MURRAYLINKV5_20211201203644","2015-07-31T11:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.234400000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[231,"MURRAYLINKV5_20211201203644","2015-07-31T11:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.441569999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[232,"MURRAYLINKV5_20211201203644","2015-07-31T11:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.498249999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[233,"MURRAYLINKV5_20211201203644","2015-07-31T11:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.10934,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[234,"MURRAYLINKV5_20211201203644","2015-07-31T11:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.399719999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[235,"MURRAYLINKV5_20211201203644","2015-07-31T11:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.750679999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[236,"MURRAYLINKV5_20211201203644","2015-07-31T12:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.399719999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[237,"MURRAYLINKV5_20211201203644","2015-07-31T12:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.112490000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[238,"MURRAYLINKV5_20211201203644","2015-07-31T12:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.399719999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[239,"MURRAYLINKV5_20211201203644","2015-07-31T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.196300000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[240,"MURRAYLINKV5_20211201203644","2015-07-31T12:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.34046,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[241,"MURRAYLINKV5_20211201203644","2015-07-31T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.78468,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[242,"MURRAYLINKV5_20211201203644","2015-07-31T16:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.675889999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[243,"MURRAYLINKV5_20211201203644","2015-08-18T10:20:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-17.515309999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[244,"MURRAYLINKV5_20211201203644","2015-08-18T10:25:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-17.31739,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[245,"MURRAYLINKV5_20211201203644","2015-08-18T10:30:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-13.598420000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[246,"MURRAYLINKV5_20211201203644","2015-09-03T11:40:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.28417,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[247,"MURRAYLINKV5_20211201203644","2015-09-03T11:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-22.2057,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[248,"MURRAYLINKV5_20211201203644","2015-09-03T11:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-24.762360000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[249,"MURRAYLINKV5_20211201203644","2015-09-03T11:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-13.36922,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[250,"MURRAYLINKV5_20211201203644","2015-09-03T12:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-13.86139,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[251,"MURRAYLINKV5_20211201203644","2015-09-03T12:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-23.341049999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[252,"MURRAYLINKV5_20211201203644","2015-09-03T12:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-28.472079999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[253,"MURRAYLINKV5_20211201203644","2015-09-03T12:15:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-23.841200000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[254,"MURRAYLINKV5_20211201203644","2015-09-15T05:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.167200000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[255,"MURRAYLINKV5_20211201203644","2015-09-15T05:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.042249999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[256,"MURRAYLINKV5_20211201203644","2015-09-15T05:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.93355,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[257,"MURRAYLINKV5_20211201203644","2015-09-15T05:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.676439999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[258,"MURRAYLINKV5_20211201203644","2015-09-15T05:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.535319999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[259,"MURRAYLINKV5_20211201203644","2015-09-15T06:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.011710000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[260,"MURRAYLINKV5_20211201203644","2015-09-15T06:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.46968,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[261,"MURRAYLINKV5_20211201203644","2015-09-15T06:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.371500000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[262,"MURRAYLINKV5_20211201203644","2015-09-15T06:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.839219999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[263,"MURRAYLINKV5_20211201203644","2015-09-15T06:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.323070000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[264,"MURRAYLINKV5_20211201203644","2015-09-15T06:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.85981,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[265,"MURRAYLINKV5_20211201203644","2015-09-15T06:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.89711,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[266,"MURRAYLINKV5_20211201203644","2015-09-15T06:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.3767,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[267,"MURRAYLINKV5_20211201203644","2015-09-15T07:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.718819999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[268,"MURRAYLINKV5_20211201203644","2015-09-15T07:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.186209999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[269,"MURRAYLINKV5_20211201203644","2015-09-15T07:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.617339999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[270,"MURRAYLINKV5_20211201203644","2015-09-15T07:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.226279999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[271,"MURRAYLINKV5_20211201203644","2015-09-15T07:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.164850000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[272,"MURRAYLINKV5_20211201203644","2015-09-15T07:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.271930000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[273,"MURRAYLINKV5_20211201203644","2015-09-15T07:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.477589999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[274,"MURRAYLINKV5_20211201203644","2015-09-15T07:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.839919999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[275,"MURRAYLINKV5_20211201203644","2015-09-15T07:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.941199999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[276,"MURRAYLINKV5_20211201203644","2015-09-15T07:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.390650000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[277,"MURRAYLINKV5_20211201203644","2015-09-15T07:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.838419999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[278,"MURRAYLINKV5_20211201203644","2015-09-15T07:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.000719999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[279,"MURRAYLINKV5_20211201203644","2015-09-15T08:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.32372,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[280,"MURRAYLINKV5_20211201203644","2015-09-15T08:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.44134,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[281,"MURRAYLINKV5_20211201203644","2015-09-15T08:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.31061,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[282,"MURRAYLINKV5_20211201203644","2015-09-15T08:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.435860000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[283,"MURRAYLINKV5_20211201203644","2015-09-15T08:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.887650000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[284,"MURRAYLINKV5_20211201203644","2015-09-15T08:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.217929999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[285,"MURRAYLINKV5_20211201203644","2015-09-15T08:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.261600000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[286,"MURRAYLINKV5_20211201203644","2015-09-15T08:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.460460000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[287,"MURRAYLINKV5_20211201203644","2015-09-15T08:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.113880000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[288,"MURRAYLINKV5_20211201203644","2015-09-15T08:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.781420000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[289,"MURRAYLINKV5_20211201203644","2015-09-15T08:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.881170000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[290,"MURRAYLINKV5_20211201203644","2015-09-15T08:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.580190000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[291,"MURRAYLINKV5_20211201203644","2015-09-15T09:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.681049999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[292,"MURRAYLINKV5_20211201203644","2015-09-15T09:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.140830000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[293,"MURRAYLINKV5_20211201203644","2015-09-15T09:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.661149999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[294,"MURRAYLINKV5_20211201203644","2015-09-15T09:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.525189999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[295,"MURRAYLINKV5_20211201203644","2015-09-15T09:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.248349999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[296,"MURRAYLINKV5_20211201203644","2015-09-15T09:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.569269999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[297,"MURRAYLINKV5_20211201203644","2015-09-15T09:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.09384,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[298,"MURRAYLINKV5_20211201203644","2015-09-15T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.42642,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[299,"MURRAYLINKV5_20211201203644","2015-09-15T09:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.553149999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[300,"MURRAYLINKV5_20211201203644","2015-09-15T09:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.276219999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[301,"MURRAYLINKV5_20211201203644","2015-09-15T09:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.429690000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[302,"MURRAYLINKV5_20211201203644","2015-09-15T09:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.907509999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[303,"MURRAYLINKV5_20211201203644","2015-09-15T10:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.70532,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[304,"MURRAYLINKV5_20211201203644","2015-09-15T10:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.577369999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[305,"MURRAYLINKV5_20211201203644","2015-09-15T10:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.425129999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[306,"MURRAYLINKV5_20211201203644","2015-09-15T10:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.97193,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[307,"MURRAYLINKV5_20211201203644","2015-09-15T10:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.072849999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[308,"MURRAYLINKV5_20211201203644","2015-09-15T10:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.676600000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[309,"MURRAYLINKV5_20211201203644","2015-09-15T10:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.336130000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[310,"MURRAYLINKV5_20211201203644","2015-09-15T10:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.317170000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[311,"MURRAYLINKV5_20211201203644","2015-09-15T10:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.429690000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[312,"MURRAYLINKV5_20211201203644","2015-09-15T10:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.189869999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[313,"MURRAYLINKV5_20211201203644","2015-09-15T10:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.002520000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[314,"MURRAYLINKV5_20211201203644","2015-09-15T10:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.539950000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[315,"MURRAYLINKV5_20211201203644","2015-09-15T11:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.568190000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[316,"MURRAYLINKV5_20211201203644","2015-09-15T11:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.64029,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[317,"MURRAYLINKV5_20211201203644","2015-09-15T11:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.682089999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[318,"MURRAYLINKV5_20211201203644","2015-09-15T11:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.006869999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[319,"MURRAYLINKV5_20211201203644","2015-09-15T11:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.892430000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[320,"MURRAYLINKV5_20211201203644","2015-09-15T11:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.485199999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[321,"MURRAYLINKV5_20211201203644","2015-09-15T11:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-30.287269999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[322,"MURRAYLINKV5_20211201203644","2015-09-15T11:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.25168,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[323,"MURRAYLINKV5_20211201203644","2015-09-15T11:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.1007,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[324,"MURRAYLINKV5_20211201203644","2015-09-15T11:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.702210000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[325,"MURRAYLINKV5_20211201203644","2015-09-15T11:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.244289999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[326,"MURRAYLINKV5_20211201203644","2015-09-15T11:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.410599999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[327,"MURRAYLINKV5_20211201203644","2015-09-15T12:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.08257,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[328,"MURRAYLINKV5_20211201203644","2015-09-15T12:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.35492,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[329,"MURRAYLINKV5_20211201203644","2015-09-15T12:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.77101,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[330,"MURRAYLINKV5_20211201203644","2015-09-15T12:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.057269999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[331,"MURRAYLINKV5_20211201203644","2015-09-15T12:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.17839,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[332,"MURRAYLINKV5_20211201203644","2015-09-15T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.124199999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[333,"MURRAYLINKV5_20211201203644","2015-09-15T12:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.405639999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[334,"MURRAYLINKV5_20211201203644","2015-09-15T12:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.076930000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[335,"MURRAYLINKV5_20211201203644","2015-09-15T12:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.026779999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[336,"MURRAYLINKV5_20211201203644","2015-09-15T12:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.652360000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[337,"MURRAYLINKV5_20211201203644","2015-09-15T12:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.01726,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[338,"MURRAYLINKV5_20211201203644","2015-09-15T12:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.013839999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[339,"MURRAYLINKV5_20211201203644","2015-09-15T13:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.87443,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[340,"MURRAYLINKV5_20211201203644","2015-09-15T13:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.686779999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[341,"MURRAYLINKV5_20211201203644","2015-09-15T13:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.182459999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[342,"MURRAYLINKV5_20211201203644","2015-09-15T13:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.373090000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[343,"MURRAYLINKV5_20211201203644","2015-09-15T13:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.06006,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[344,"MURRAYLINKV5_20211201203644","2015-09-15T13:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-259.46825000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[345,"MURRAYLINKV5_20211201203644","2015-09-15T13:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-257.75301999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[346,"MURRAYLINKV5_20211201203644","2015-09-15T13:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-309.20087999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[347,"MURRAYLINKV5_20211201203644","2015-09-15T14:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.31691,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[348,"MURRAYLINKV5_20211201203644","2015-09-15T14:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.67389,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[349,"MURRAYLINKV5_20211201203644","2015-09-15T14:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.899609999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[350,"MURRAYLINKV5_20211201203644","2015-09-15T14:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.084510000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[351,"MURRAYLINKV5_20211201203644","2015-09-15T14:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-308.74720000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[352,"MURRAYLINKV5_20211201203644","2015-09-15T14:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.96299,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[353,"MURRAYLINKV5_20211201203644","2015-09-15T14:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-308.73993000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[354,"MURRAYLINKV5_20211201203644","2015-09-15T14:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-306.77893,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[355,"MURRAYLINKV5_20211201203644","2015-09-15T15:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.506699999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[356,"MURRAYLINKV5_20211201203644","2015-09-15T15:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-308.45299,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[357,"MURRAYLINKV5_20211201203644","2015-09-15T15:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-307.06623000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[358,"MURRAYLINKV5_20211201203644","2015-09-15T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.394819999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[359,"MURRAYLINKV5_20211201203644","2015-09-15T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.38289,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[360,"MURRAYLINKV5_20211201203644","2015-09-15T15:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.752410000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[361,"MURRAYLINKV5_20211201203644","2015-09-15T15:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.391299999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[362,"MURRAYLINKV5_20211201203644","2015-09-15T15:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.010100000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[363,"MURRAYLINKV5_20211201203644","2015-09-15T15:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.596620000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[364,"MURRAYLINKV5_20211201203644","2015-09-15T15:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.481730000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[365,"MURRAYLINKV5_20211201203644","2015-09-15T15:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.578950000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[366,"MURRAYLINKV5_20211201203644","2015-09-15T15:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.120329999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[367,"MURRAYLINKV5_20211201203644","2015-09-15T16:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-306.48727000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[368,"MURRAYLINKV5_20211201203644","2015-09-15T16:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.906750000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[369,"MURRAYLINKV5_20211201203644","2015-09-15T16:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.231179999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[370,"MURRAYLINKV5_20211201203644","2015-09-15T16:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.869910000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[371,"MURRAYLINKV5_20211201203644","2015-09-15T16:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.98814,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[372,"MURRAYLINKV5_20211201203644","2015-09-15T16:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.21189,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[373,"MURRAYLINKV5_20211201203644","2015-09-15T16:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.18708,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[374,"MURRAYLINKV5_20211201203644","2015-09-15T16:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.08788,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[375,"MURRAYLINKV5_20211201203644","2015-09-15T16:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.290800000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[376,"MURRAYLINKV5_20211201203644","2015-09-15T16:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.18709,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[377,"MURRAYLINKV5_20211201203644","2015-09-15T16:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.16076,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[378,"MURRAYLINKV5_20211201203644","2015-09-15T16:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.714180000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[379,"MURRAYLINKV5_20211201203644","2015-09-15T17:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.003329999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[380,"MURRAYLINKV5_20211201203644","2015-09-15T17:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.014900000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[381,"MURRAYLINKV5_20211201203644","2015-09-15T17:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.87997,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[382,"MURRAYLINKV5_20211201203644","2015-09-15T17:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.275559999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[383,"MURRAYLINKV5_20211201203644","2015-09-15T17:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.62918,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[384,"MURRAYLINKV5_20211201203644","2015-09-15T17:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.57686,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[385,"MURRAYLINKV5_20211201203644","2015-09-15T17:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.26807,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[386,"MURRAYLINKV5_20211201203644","2015-09-15T17:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.760120000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[387,"MURRAYLINKV5_20211201203644","2015-09-15T17:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.456890000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[388,"MURRAYLINKV5_20211201203644","2015-09-15T17:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.07227,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[389,"MURRAYLINKV5_20211201203644","2015-09-15T18:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-26.769629999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[390,"MURRAYLINKV5_20211201203644","2015-09-15T18:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.036930000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[391,"MURRAYLINKV5_20211201203644","2015-09-15T18:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.666139999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[392,"MURRAYLINKV5_20211201203644","2015-09-15T18:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.85614,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[393,"MURRAYLINKV5_20211201203644","2015-09-15T18:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.254569999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[394,"MURRAYLINKV5_20211201203644","2015-09-15T18:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.254569999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[395,"MURRAYLINKV5_20211201203644","2015-09-15T18:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.254569999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[396,"MURRAYLINKV5_20211201203644","2015-09-15T18:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.549609999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[397,"MURRAYLINKV5_20211201203644","2015-09-15T19:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.352779999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[398,"MURRAYLINKV5_20211201203644","2015-09-15T19:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.574909999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[399,"MURRAYLINKV5_20211201203644","2015-09-15T19:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.29064,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[400,"MURRAYLINKV5_20211201203644","2015-09-15T19:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.830110000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[401,"MURRAYLINKV5_20211201203644","2015-09-15T19:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.898890000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[402,"MURRAYLINKV5_20211201203644","2015-09-15T19:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.3047,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[403,"MURRAYLINKV5_20211201203644","2015-09-17T06:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.678979999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[404,"MURRAYLINKV5_20211201203644","2015-09-17T08:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.23047,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[405,"MURRAYLINKV5_20211201203644","2015-09-17T08:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.60347,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[406,"MURRAYLINKV5_20211201203644","2015-09-17T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12062.28795,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[407,"MURRAYLINKV5_20211201203644","2015-09-17T17:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.985810000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[408,"MURRAYLINKV5_20211201203644","2015-09-17T17:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.941700000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[409,"MURRAYLINKV5_20211201203644","2015-09-17T17:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.18939,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[410,"MURRAYLINKV5_20211201203644","2015-09-17T17:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.505749999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[411,"MURRAYLINKV5_20211201203644","2015-09-17T17:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.295300000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[412,"MURRAYLINKV5_20211201203644","2015-09-17T17:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.376470000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[413,"MURRAYLINKV5_20211201203644","2015-09-17T17:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.652979999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[414,"MURRAYLINKV5_20211201203644","2015-09-17T17:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792919999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[415,"MURRAYLINKV5_20211201203644","2015-09-17T18:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792919999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[416,"MURRAYLINKV5_20211201203644","2015-09-17T18:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792919999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[417,"MURRAYLINKV5_20211201203644","2015-09-17T18:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.594670000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[418,"MURRAYLINKV5_20211201203644","2015-09-17T18:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.088340000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[419,"MURRAYLINKV5_20211201203644","2015-09-17T19:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.600770000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[420,"MURRAYLINKV5_20211201203644","2015-09-17T19:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.661940000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[421,"MURRAYLINKV5_20211201203644","2015-09-17T19:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.414849999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[422,"MURRAYLINKV5_20211201203644","2015-09-17T19:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.05644,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[423,"MURRAYLINKV5_20211201203644","2015-09-17T19:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.33192,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[424,"MURRAYLINKV5_20211201203644","2015-09-17T19:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.936389999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[425,"MURRAYLINKV5_20211201203644","2015-09-28T08:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-50.022930000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","Outage due to Murraylink runback scheme operation","UNPLANNED",0]
[426,"MURRAYLINKV5_20211201203644","2015-09-28T08:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-45.651269999999997,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","3","Outage due to Murraylink runback scheme operation","UNPLANNED",0]
[427,"MURRAYLINKV5_20211201203644","2015-10-13T01:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,12.014469999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[428,"MURRAYLINKV5_20211201203644","2015-10-13T01:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,11.67164,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[429,"MURRAYLINKV5_20211201203644","2015-10-13T01:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,11.99236,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[430,"MURRAYLINKV5_20211201203644","2015-10-13T02:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,11.996549999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[431,"MURRAYLINKV5_20211201203644","2015-11-03T09:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.242660000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[432,"MURRAYLINKV5_20211201203644","2015-11-03T10:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13070.623740000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[433,"MURRAYLINKV5_20211201203644","2015-11-03T10:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.53313,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[434,"MURRAYLINKV5_20211201203644","2015-11-03T11:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.518319999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[435,"MURRAYLINKV5_20211201203644","2015-11-03T11:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.632860000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[436,"MURRAYLINKV5_20211201203644","2015-11-03T11:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.527760000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[437,"MURRAYLINKV5_20211201203644","2015-11-03T12:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.24103,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[438,"MURRAYLINKV5_20211201203644","2015-11-03T12:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.67559,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[439,"MURRAYLINKV5_20211201203644","2015-11-03T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.007289999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[440,"MURRAYLINKV5_20211201203644","2015-11-03T12:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.78844,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[441,"MURRAYLINKV5_20211201203644","2015-11-03T12:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.67254,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[442,"MURRAYLINKV5_20211201203644","2015-11-03T13:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.68205,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[443,"MURRAYLINKV5_20211201203644","2015-11-03T13:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.69678,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[444,"MURRAYLINKV5_20211201203644","2015-11-03T13:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-66.736969999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[445,"MURRAYLINKV5_20211201203644","2015-11-03T13:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-66.593040000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[446,"MURRAYLINKV5_20211201203644","2015-11-03T14:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-68.794960000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[447,"MURRAYLINKV5_20211201203644","2015-11-03T14:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-59.92483,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[448,"MURRAYLINKV5_20211201203644","2015-11-03T14:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-58.417940000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[449,"MURRAYLINKV5_20211201203644","2015-11-03T14:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.64123,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[450,"MURRAYLINKV5_20211201203644","2015-11-03T14:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-63.104799999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[451,"MURRAYLINKV5_20211201203644","2015-11-03T14:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-65.122510000000005,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[452,"MURRAYLINKV5_20211201203644","2015-11-03T14:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-66.304609999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[453,"MURRAYLINKV5_20211201203644","2015-11-03T14:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-65.805030000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[454,"MURRAYLINKV5_20211201203644","2015-11-03T14:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.76445,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[455,"MURRAYLINKV5_20211201203644","2015-11-03T15:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-73.990269999999995,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[456,"MURRAYLINKV5_20211201203644","2015-11-12T08:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13220.64566,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[457,"MURRAYLINKV5_20211201203644","2015-11-12T09:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.25459,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[458,"MURRAYLINKV5_20211201203644","2015-11-12T09:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.0754,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[459,"MURRAYLINKV5_20211201203644","2015-11-25T17:25:00","VSML_000","I-ML_ZERO;I-VSML_000","2008-08-05",1,-11.254720000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Outage is not related to murraylink","UNPLANNED",0]
[460,"MURRAYLINKV5_20211201203644","2015-11-26T08:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.416869999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[461,"MURRAYLINKV5_20211201203644","2015-11-26T10:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.006530000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[462,"MURRAYLINKV5_20211201203644","2015-11-26T10:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.595859999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[463,"MURRAYLINKV5_20211201203644","2015-11-26T10:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.031690000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[464,"MURRAYLINKV5_20211201203644","2015-11-26T10:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-20.866769999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[465,"MURRAYLINKV5_20211201203644","2015-11-26T11:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.390899999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[466,"MURRAYLINKV5_20211201203644","2015-11-26T11:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.225819999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[467,"MURRAYLINKV5_20211201203644","2015-11-26T11:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.031099999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[468,"MURRAYLINKV5_20211201203644","2015-11-26T11:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-20.730740000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[469,"MURRAYLINKV5_20211201203644","2015-11-26T11:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.820920000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[470,"MURRAYLINKV5_20211201203644","2015-11-26T12:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.247890000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[471,"MURRAYLINKV5_20211201203644","2015-11-26T12:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.40316,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[472,"MURRAYLINKV5_20211201203644","2015-11-26T12:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.396429999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[473,"MURRAYLINKV5_20211201203644","2015-11-26T12:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-20.406659999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[474,"MURRAYLINKV5_20211201203644","2015-11-26T12:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.282530000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[475,"MURRAYLINKV5_20211201203644","2015-11-26T12:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-137.07602,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[476,"MURRAYLINKV5_20211201203644","2015-11-26T12:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-35.126800000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[477,"MURRAYLINKV5_20211201203644","2015-11-26T12:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-97.546440000000004,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[478,"MURRAYLINKV5_20211201203644","2015-11-26T12:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-124.46554999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[479,"MURRAYLINKV5_20211201203644","2015-11-26T12:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-107.48211999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[480,"MURRAYLINKV5_20211201203644","2015-11-26T13:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-99.881870000000006,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[481,"MURRAYLINKV5_20211201203644","2015-11-26T13:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-54.026539999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[482,"MURRAYLINKV5_20211201203644","2015-11-26T13:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-49.308520000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[483,"MURRAYLINKV5_20211201203644","2015-11-26T13:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-57.892620000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[484,"MURRAYLINKV5_20211201203644","2015-11-26T13:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-54.045270000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[485,"MURRAYLINKV5_20211201203644","2015-11-26T13:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-45.52496,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[486,"MURRAYLINKV5_20211201203644","2015-11-26T13:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.57424,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[487,"MURRAYLINKV5_20211201203644","2015-11-26T13:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.806229999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[488,"MURRAYLINKV5_20211201203644","2015-11-26T13:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-43.97081,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[489,"MURRAYLINKV5_20211201203644","2015-11-26T13:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.831429999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[490,"MURRAYLINKV5_20211201203644","2015-11-26T13:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-42.936450000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[491,"MURRAYLINKV5_20211201203644","2015-11-26T14:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.859819999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[492,"MURRAYLINKV5_20211201203644","2015-11-26T14:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-44.42709,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[493,"MURRAYLINKV5_20211201203644","2015-11-26T14:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-44.427680000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[494,"MURRAYLINKV5_20211201203644","2015-12-01T12:35:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,56.07855,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[495,"MURRAYLINKV5_20211201203644","2015-12-01T12:40:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,56.376820000000002,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[496,"MURRAYLINKV5_20211201203644","2015-12-01T12:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,56.09404,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[497,"MURRAYLINKV5_20211201203644","2015-12-01T12:50:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,57.18891,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[498,"MURRAYLINKV5_20211201203644","2015-12-01T12:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,66.036109999999994,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[499,"MURRAYLINKV5_20211201203644","2015-12-01T13:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,84.194810000000004,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[500,"MURRAYLINKV5_20211201203644","2015-12-01T13:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,82.501639999999995,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[501,"MURRAYLINKV5_20211201203644","2015-12-16T14:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-24.453299999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[502,"MURRAYLINKV5_20211201203644","2015-12-16T14:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-192.84943000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[503,"MURRAYLINKV5_20211201203644","2015-12-16T14:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-72.261679999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[504,"MURRAYLINKV5_20211201203644","2015-12-16T14:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-74.443889999999996,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[505,"MURRAYLINKV5_20211201203644","2015-12-16T14:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-60.212380000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[506,"MURRAYLINKV5_20211201203644","2015-12-16T14:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.200479999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[507,"MURRAYLINKV5_20211201203644","2015-12-16T15:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.698149999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[508,"MURRAYLINKV5_20211201203644","2015-12-16T15:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-166.12562,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[509,"MURRAYLINKV5_20211201203644","2015-12-16T15:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-218.49923000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[510,"MURRAYLINKV5_20211201203644","2015-12-16T15:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-194.94363000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[511,"MURRAYLINKV5_20211201203644","2015-12-16T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-61.0886,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[512,"MURRAYLINKV5_20211201203644","2015-12-16T15:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-63.89038,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[513,"MURRAYLINKV5_20211201203644","2015-12-16T15:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-292.33085,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[514,"MURRAYLINKV5_20211201203644","2015-12-16T15:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-278.87328000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[515,"MURRAYLINKV5_20211201203644","2015-12-16T15:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-38.4255,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[516,"MURRAYLINKV5_20211201203644","2015-12-16T15:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-36.099820000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[517,"MURRAYLINKV5_20211201203644","2015-12-16T15:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-34.064900000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[518,"MURRAYLINKV5_20211201203644","2015-12-16T16:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-82.182879999999997,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[519,"MURRAYLINKV5_20211201203644","2015-12-21T04:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-62.277540000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[520,"MURRAYLINKV5_20211201203644","2015-12-21T04:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-62.285130000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[521,"MURRAYLINKV5_20211201203644","2015-12-21T04:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-62.173850000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[522,"MURRAYLINKV5_20211201203644","2015-12-21T04:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-60.349600000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[523,"MURRAYLINKV5_20211201203644","2015-12-21T04:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-61.049239999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[524,"MURRAYLINKV5_20211201203644","2015-12-21T04:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-60.235489999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[525,"MURRAYLINKV5_20211201203644","2015-12-21T04:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-73.688079999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[526,"MURRAYLINKV5_20211201203644","2015-12-21T04:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-61.015689999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[527,"MURRAYLINKV5_20211201203644","2015-12-21T05:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-61.65513,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[528,"MURRAYLINKV5_20211201203644","2015-12-21T05:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-62.049970000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[529,"MURRAYLINKV5_20211201203644","2015-12-21T05:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-65.400530000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[530,"MURRAYLINKV5_20211201203644","2015-12-21T05:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.677820000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[531,"MURRAYLINKV5_20211201203644","2015-12-21T05:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-72.917599999999993,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[532,"MURRAYLINKV5_20211201203644","2015-12-21T05:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-72.621840000000006,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[533,"MURRAYLINKV5_20211201203644","2015-12-21T05:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-73.158510000000007,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[534,"MURRAYLINKV5_20211201203644","2015-12-21T05:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-89.576250000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[535,"MURRAYLINKV5_20211201203644","2015-12-21T05:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-65.610659999999996,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[536,"MURRAYLINKV5_20211201203644","2015-12-21T05:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-92.436869999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[537,"MURRAYLINKV5_20211201203644","2015-12-21T05:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-69.644120000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[538,"MURRAYLINKV5_20211201203644","2015-12-21T05:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-76.699730000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[539,"MURRAYLINKV5_20211201203644","2015-12-21T06:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-70.197509999999994,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[540,"MURRAYLINKV5_20211201203644","2015-12-21T06:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-65.797079999999994,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[541,"MURRAYLINKV5_20211201203644","2015-12-21T06:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-67.71087,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[542,"MURRAYLINKV5_20211201203644","2015-12-21T06:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-76.911580000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[543,"MURRAYLINKV5_20211201203644","2015-12-21T06:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.477689999999996,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[544,"MURRAYLINKV5_20211201203644","2015-12-21T06:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.520810000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[545,"MURRAYLINKV5_20211201203644","2015-12-21T06:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-80.108720000000005,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[546,"MURRAYLINKV5_20211201203644","2015-12-21T06:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-21.80453,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[547,"MURRAYLINKV5_20211201203644","2015-12-21T06:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-78.312309999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[548,"MURRAYLINKV5_20211201203644","2015-12-21T06:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-22.360939999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[549,"MURRAYLINKV5_20211201203644","2015-12-21T06:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-79.762219999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[550,"MURRAYLINKV5_20211201203644","2015-12-21T07:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-67.036360000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[551,"MURRAYLINKV5_20211201203644","2015-12-21T07:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-81.199340000000007,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[552,"MURRAYLINKV5_20211201203644","2015-12-21T07:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-66.971459999999993,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[553,"MURRAYLINKV5_20211201203644","2015-12-21T07:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-67.499600000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[554,"MURRAYLINKV5_20211201203644","2015-12-21T07:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-75.684209999999993,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[555,"MURRAYLINKV5_20211201203644","2015-12-21T07:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-78.550820000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[556,"MURRAYLINKV5_20211201203644","2015-12-21T07:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-78.612979999999993,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[557,"MURRAYLINKV5_20211201203644","2015-12-21T07:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-78.61421,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[558,"MURRAYLINKV5_20211201203644","2015-12-21T07:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.303319999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[559,"MURRAYLINKV5_20211201203644","2015-12-21T08:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-72.364410000000007,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[560,"MURRAYLINKV5_20211201203644","2015-12-21T08:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.012590000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[561,"MURRAYLINKV5_20211201203644","2015-12-21T08:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-67.754649999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[562,"MURRAYLINKV5_20211201203644","2015-12-21T08:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.422060000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[563,"MURRAYLINKV5_20211201203644","2015-12-21T08:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-880.62644999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[564,"MURRAYLINKV5_20211201203644","2015-12-21T08:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.222660000000005,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[565,"MURRAYLINKV5_20211201203644","2015-12-21T08:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.321759999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[566,"MURRAYLINKV5_20211201203644","2015-12-21T08:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-119.8171,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[567,"MURRAYLINKV5_20211201203644","2015-12-21T08:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-108.35097,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[568,"MURRAYLINKV5_20211201203644","2015-12-21T08:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-87.662959999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[569,"MURRAYLINKV5_20211201203644","2015-12-21T09:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.30381,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[570,"MURRAYLINKV5_20211201203644","2015-12-21T09:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-105.14211,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[571,"MURRAYLINKV5_20211201203644","2015-12-21T09:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-88.704750000000004,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[572,"MURRAYLINKV5_20211201203644","2015-12-21T09:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-88.991810000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[573,"MURRAYLINKV5_20211201203644","2015-12-21T09:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-76.753240000000005,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[574,"MURRAYLINKV5_20211201203644","2015-12-21T09:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.890510000000006,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[575,"MURRAYLINKV5_20211201203644","2015-12-21T09:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.648250000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[576,"MURRAYLINKV5_20211201203644","2015-12-21T09:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.340209999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[577,"MURRAYLINKV5_20211201203644","2015-12-21T09:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.87706,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[578,"MURRAYLINKV5_20211201203644","2015-12-21T09:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.351370000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[579,"MURRAYLINKV5_20211201203644","2015-12-21T09:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.092930000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[580,"MURRAYLINKV5_20211201203644","2015-12-21T09:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.02276,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[581,"MURRAYLINKV5_20211201203644","2015-12-21T10:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-104.62128,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[582,"MURRAYLINKV5_20211201203644","2015-12-21T10:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.77073,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[583,"MURRAYLINKV5_20211201203644","2015-12-21T10:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.908069999999995,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[584,"MURRAYLINKV5_20211201203644","2015-12-21T10:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-77.927769999999995,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[585,"MURRAYLINKV5_20211201203644","2015-12-21T10:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-76.867710000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[586,"MURRAYLINKV5_20211201203644","2015-12-21T10:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-75.680620000000005,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[587,"MURRAYLINKV5_20211201203644","2015-12-21T10:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-75.999279999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[588,"MURRAYLINKV5_20211201203644","2015-12-21T10:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-87.530559999999994,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[589,"MURRAYLINKV5_20211201203644","2015-12-21T10:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-104.53923,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[590,"MURRAYLINKV5_20211201203644","2015-12-21T10:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.264489999999995,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[591,"MURRAYLINKV5_20211201203644","2015-12-21T10:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.106049999999996,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[592,"MURRAYLINKV5_20211201203644","2015-12-21T10:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-104.68683,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[593,"MURRAYLINKV5_20211201203644","2015-12-21T11:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-86.303319999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[594,"MURRAYLINKV5_20211201203644","2015-01-01T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.49677,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[595,"MURRAYLINKV5_20211201203644","2015-01-01T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.4046,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[596,"MURRAYLINKV5_20211201203644","2015-01-01T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.187010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[597,"MURRAYLINKV5_20211201203644","2015-01-01T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.98856,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[598,"MURRAYLINKV5_20211201203644","2015-01-01T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.202,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[599,"MURRAYLINKV5_20211201203644","2015-01-01T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.39001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[600,"MURRAYLINKV5_20211201203644","2015-01-01T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.234640000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[601,"MURRAYLINKV5_20211201203644","2015-01-01T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.18985,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[602,"MURRAYLINKV5_20211201203644","2015-01-01T05:00:00","V>>V_NIL1A_R","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-30",1,-10.023389999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[603,"MURRAYLINKV5_20211201203644","2015-01-01T05:15:00","V>>V_NIL1A_R","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-30",1,-10.02852,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[604,"MURRAYLINKV5_20211201203644","2015-01-01T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.91356,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[605,"MURRAYLINKV5_20211201203644","2015-01-01T08:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.42362,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[606,"MURRAYLINKV5_20211201203644","2015-01-01T08:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.552949999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[607,"MURRAYLINKV5_20211201203644","2015-01-01T08:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.814730000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[608,"MURRAYLINKV5_20211201203644","2015-01-01T08:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.797040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[609,"MURRAYLINKV5_20211201203644","2015-01-01T08:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.05067,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[610,"MURRAYLINKV5_20211201203644","2015-01-01T08:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.03285,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[611,"MURRAYLINKV5_20211201203644","2015-01-01T08:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.030250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[612,"MURRAYLINKV5_20211201203644","2015-01-01T08:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.19487,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[613,"MURRAYLINKV5_20211201203644","2015-01-01T09:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.683009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[614,"MURRAYLINKV5_20211201203644","2015-01-01T09:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.99981,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[615,"MURRAYLINKV5_20211201203644","2015-01-01T09:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.214130000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[616,"MURRAYLINKV5_20211201203644","2015-01-01T09:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.221640000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[617,"MURRAYLINKV5_20211201203644","2015-01-01T09:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.453279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[618,"MURRAYLINKV5_20211201203644","2015-01-01T09:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.99381,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[619,"MURRAYLINKV5_20211201203644","2015-01-01T09:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.03627,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[620,"MURRAYLINKV5_20211201203644","2015-01-01T09:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.83639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[621,"MURRAYLINKV5_20211201203644","2015-01-01T09:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.917479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[622,"MURRAYLINKV5_20211201203644","2015-01-01T09:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.831110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[623,"MURRAYLINKV5_20211201203644","2015-01-01T09:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.842359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[624,"MURRAYLINKV5_20211201203644","2015-01-01T09:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.769220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[625,"MURRAYLINKV5_20211201203644","2015-01-01T10:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.32817,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[626,"MURRAYLINKV5_20211201203644","2015-01-01T10:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.61149,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[627,"MURRAYLINKV5_20211201203644","2015-01-01T10:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.581689999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[628,"MURRAYLINKV5_20211201203644","2015-01-01T10:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.424990000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[629,"MURRAYLINKV5_20211201203644","2015-01-01T10:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.32199,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[630,"MURRAYLINKV5_20211201203644","2015-01-01T10:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.012989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[631,"MURRAYLINKV5_20211201203644","2015-01-01T10:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.29552,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[632,"MURRAYLINKV5_20211201203644","2015-01-01T10:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.20064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[633,"MURRAYLINKV5_20211201203644","2015-01-01T10:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.07705,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[634,"MURRAYLINKV5_20211201203644","2015-01-01T10:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.974810000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[635,"MURRAYLINKV5_20211201203644","2015-01-01T10:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.44415,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[636,"MURRAYLINKV5_20211201203644","2015-01-01T10:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.963339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[637,"MURRAYLINKV5_20211201203644","2015-01-01T11:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-30.004999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[638,"MURRAYLINKV5_20211201203644","2015-01-01T11:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-29.61402,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[639,"MURRAYLINKV5_20211201203644","2015-01-01T11:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.466560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[640,"MURRAYLINKV5_20211201203644","2015-01-01T11:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.37969,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[641,"MURRAYLINKV5_20211201203644","2015-01-01T11:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.413309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[642,"MURRAYLINKV5_20211201203644","2015-01-01T11:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.866309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[643,"MURRAYLINKV5_20211201203644","2015-01-01T11:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.189710000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[644,"MURRAYLINKV5_20211201203644","2015-01-01T11:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.88645,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[645,"MURRAYLINKV5_20211201203644","2015-01-01T11:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.8658,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[646,"MURRAYLINKV5_20211201203644","2015-01-01T11:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.089829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[647,"MURRAYLINKV5_20211201203644","2015-01-01T11:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.60304,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[648,"MURRAYLINKV5_20211201203644","2015-01-01T11:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.62487,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[649,"MURRAYLINKV5_20211201203644","2015-01-01T12:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.082090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[650,"MURRAYLINKV5_20211201203644","2015-01-01T12:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.010390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[651,"MURRAYLINKV5_20211201203644","2015-01-01T12:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.500730000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[652,"MURRAYLINKV5_20211201203644","2015-01-01T12:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.505269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[653,"MURRAYLINKV5_20211201203644","2015-01-01T12:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.307469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[654,"MURRAYLINKV5_20211201203644","2015-01-01T12:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.3139,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[655,"MURRAYLINKV5_20211201203644","2015-01-01T12:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.955290000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[656,"MURRAYLINKV5_20211201203644","2015-01-01T12:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.64551,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[657,"MURRAYLINKV5_20211201203644","2015-01-01T12:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.56573,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[658,"MURRAYLINKV5_20211201203644","2015-01-01T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.78951,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[659,"MURRAYLINKV5_20211201203644","2015-01-01T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.57563,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[660,"MURRAYLINKV5_20211201203644","2015-01-01T12:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.919420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[661,"MURRAYLINKV5_20211201203644","2015-01-01T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.350149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[662,"MURRAYLINKV5_20211201203644","2015-01-01T13:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.163930000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[663,"MURRAYLINKV5_20211201203644","2015-01-01T13:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.648820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[664,"MURRAYLINKV5_20211201203644","2015-01-01T13:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.46331,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[665,"MURRAYLINKV5_20211201203644","2015-01-01T13:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.494199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[666,"MURRAYLINKV5_20211201203644","2015-01-01T13:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.34507,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[667,"MURRAYLINKV5_20211201203644","2015-01-01T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.545949999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[668,"MURRAYLINKV5_20211201203644","2015-01-01T13:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.462209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[669,"MURRAYLINKV5_20211201203644","2015-01-01T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.564819999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[670,"MURRAYLINKV5_20211201203644","2015-01-01T13:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.787210000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[671,"MURRAYLINKV5_20211201203644","2015-01-01T13:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.40549,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[672,"MURRAYLINKV5_20211201203644","2015-01-01T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.55635,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[673,"MURRAYLINKV5_20211201203644","2015-01-01T13:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.277899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[674,"MURRAYLINKV5_20211201203644","2015-01-01T14:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-89.827489999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[675,"MURRAYLINKV5_20211201203644","2015-01-01T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-132.84589,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[676,"MURRAYLINKV5_20211201203644","2015-01-01T14:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-89.187060000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[677,"MURRAYLINKV5_20211201203644","2015-01-01T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-131.50048000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[678,"MURRAYLINKV5_20211201203644","2015-01-01T14:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-96.807339999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[679,"MURRAYLINKV5_20211201203644","2015-01-01T14:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-135.41638,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[680,"MURRAYLINKV5_20211201203644","2015-01-01T14:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-19.759219999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[681,"MURRAYLINKV5_20211201203644","2015-01-01T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-33.495669999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[682,"MURRAYLINKV5_20211201203644","2015-01-01T14:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-72.878910000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[683,"MURRAYLINKV5_20211201203644","2015-01-01T14:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-143.21018000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[684,"MURRAYLINKV5_20211201203644","2015-01-01T14:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-78.670680000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[685,"MURRAYLINKV5_20211201203644","2015-01-01T14:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-138.13086999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[686,"MURRAYLINKV5_20211201203644","2015-01-01T14:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-74.812089999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[687,"MURRAYLINKV5_20211201203644","2015-01-01T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-143.00421,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[688,"MURRAYLINKV5_20211201203644","2015-01-01T14:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.141109999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[689,"MURRAYLINKV5_20211201203644","2015-01-01T14:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-62.40005,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[690,"MURRAYLINKV5_20211201203644","2015-01-01T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-23.859020000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[691,"MURRAYLINKV5_20211201203644","2015-01-01T14:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-70.241100000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[692,"MURRAYLINKV5_20211201203644","2015-01-01T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-143.20889,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[693,"MURRAYLINKV5_20211201203644","2015-01-01T14:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.22092,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[694,"MURRAYLINKV5_20211201203644","2015-01-01T15:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-70.948369999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[695,"MURRAYLINKV5_20211201203644","2015-01-01T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-144.47829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[696,"MURRAYLINKV5_20211201203644","2015-01-01T15:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-72.681079999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[697,"MURRAYLINKV5_20211201203644","2015-01-01T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-140.30537000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[698,"MURRAYLINKV5_20211201203644","2015-01-01T15:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-80.539590000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[699,"MURRAYLINKV5_20211201203644","2015-01-01T15:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-127.65430000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[700,"MURRAYLINKV5_20211201203644","2015-01-01T15:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-132.57839000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[701,"MURRAYLINKV5_20211201203644","2015-01-01T15:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-78.738630000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[702,"MURRAYLINKV5_20211201203644","2015-01-01T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-126.19268,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[703,"MURRAYLINKV5_20211201203644","2015-01-01T15:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-130.16943000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[704,"MURRAYLINKV5_20211201203644","2015-01-01T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-76.155749999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[705,"MURRAYLINKV5_20211201203644","2015-01-01T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-129.36295000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[706,"MURRAYLINKV5_20211201203644","2015-01-01T15:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-129.23502999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[707,"MURRAYLINKV5_20211201203644","2015-01-01T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-84.024349999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[708,"MURRAYLINKV5_20211201203644","2015-01-01T15:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-22.40043,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[709,"MURRAYLINKV5_20211201203644","2015-01-01T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-254.89388,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[710,"MURRAYLINKV5_20211201203644","2015-01-01T15:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-113.01741,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[711,"MURRAYLINKV5_20211201203644","2015-01-01T15:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-47.420450000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[712,"MURRAYLINKV5_20211201203644","2015-01-01T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-169.28625,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[713,"MURRAYLINKV5_20211201203644","2015-01-01T15:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-170.62305000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[714,"MURRAYLINKV5_20211201203644","2015-01-01T15:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-193.44408999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[715,"MURRAYLINKV5_20211201203644","2015-01-01T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-502.63024000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[716,"MURRAYLINKV5_20211201203644","2015-01-01T15:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-108.81918,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[717,"MURRAYLINKV5_20211201203644","2015-01-01T15:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-72.811300000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[718,"MURRAYLINKV5_20211201203644","2015-01-01T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-129.85682,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[719,"MURRAYLINKV5_20211201203644","2015-01-01T15:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-177.7987,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[720,"MURRAYLINKV5_20211201203644","2015-01-01T15:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-82.928659999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[721,"MURRAYLINKV5_20211201203644","2015-01-01T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-119.82073,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[722,"MURRAYLINKV5_20211201203644","2015-01-01T15:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-177.81344000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[723,"MURRAYLINKV5_20211201203644","2015-01-01T15:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-81.997739999999993,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[724,"MURRAYLINKV5_20211201203644","2015-01-01T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-120.62081999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[725,"MURRAYLINKV5_20211201203644","2015-01-01T15:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-179.00076999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[726,"MURRAYLINKV5_20211201203644","2015-01-01T16:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-78.773799999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[727,"MURRAYLINKV5_20211201203644","2015-01-01T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-121.40723,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[728,"MURRAYLINKV5_20211201203644","2015-01-01T16:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-180.1678,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[729,"MURRAYLINKV5_20211201203644","2015-01-01T16:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-79.036379999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[730,"MURRAYLINKV5_20211201203644","2015-01-01T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-120.73085,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[731,"MURRAYLINKV5_20211201203644","2015-01-01T16:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-179.16511,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[732,"MURRAYLINKV5_20211201203644","2015-01-01T16:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-15.963100000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[733,"MURRAYLINKV5_20211201203644","2015-01-01T16:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2014-12-18",1,-183.09215,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[734,"MURRAYLINKV5_20211201203644","2015-01-01T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-29.012869999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[735,"MURRAYLINKV5_20211201203644","2015-01-01T16:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-43.054569999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[736,"MURRAYLINKV5_20211201203644","2015-01-01T16:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-75.592680000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[737,"MURRAYLINKV5_20211201203644","2015-01-01T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-121.68304999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[738,"MURRAYLINKV5_20211201203644","2015-01-01T16:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-180.57713000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[739,"MURRAYLINKV5_20211201203644","2015-01-01T16:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-74.595910000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[740,"MURRAYLINKV5_20211201203644","2015-01-01T16:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-120.69435,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[741,"MURRAYLINKV5_20211201203644","2015-01-01T16:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-179.10989000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[742,"MURRAYLINKV5_20211201203644","2015-01-01T16:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-72.50967,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[743,"MURRAYLINKV5_20211201203644","2015-01-01T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-121.25315000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[744,"MURRAYLINKV5_20211201203644","2015-01-01T16:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-179.08249000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[745,"MURRAYLINKV5_20211201203644","2015-01-01T16:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-74.248159999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[746,"MURRAYLINKV5_20211201203644","2015-01-01T16:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-121.58656999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[747,"MURRAYLINKV5_20211201203644","2015-01-01T16:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-179.22835000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[748,"MURRAYLINKV5_20211201203644","2015-01-01T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-270.89908000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[749,"MURRAYLINKV5_20211201203644","2015-01-01T16:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-52.725110000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[750,"MURRAYLINKV5_20211201203644","2015-01-01T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-147.53518,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[751,"MURRAYLINKV5_20211201203644","2015-01-01T16:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-174.27195,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[752,"MURRAYLINKV5_20211201203644","2015-01-01T16:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.165059999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[753,"MURRAYLINKV5_20211201203644","2015-01-01T16:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.24305000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[754,"MURRAYLINKV5_20211201203644","2015-01-01T16:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.33094,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[755,"MURRAYLINKV5_20211201203644","2015-01-01T16:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.20449,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[756,"MURRAYLINKV5_20211201203644","2015-01-01T16:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.28169,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[757,"MURRAYLINKV5_20211201203644","2015-01-01T16:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.38874000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[758,"MURRAYLINKV5_20211201203644","2015-01-01T16:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.24765,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[759,"MURRAYLINKV5_20211201203644","2015-01-01T16:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.32398000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[760,"MURRAYLINKV5_20211201203644","2015-01-01T16:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.45201,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[761,"MURRAYLINKV5_20211201203644","2015-01-01T17:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.187069999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[762,"MURRAYLINKV5_20211201203644","2015-01-01T17:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.26463000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[763,"MURRAYLINKV5_20211201203644","2015-01-01T17:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.36321000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[764,"MURRAYLINKV5_20211201203644","2015-01-01T17:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-40.782269999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[765,"MURRAYLINKV5_20211201203644","2015-01-01T17:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-170.40898999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[766,"MURRAYLINKV5_20211201203644","2015-01-01T17:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-171.75641999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[767,"MURRAYLINKV5_20211201203644","2015-01-01T17:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-55.649329999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[768,"MURRAYLINKV5_20211201203644","2015-01-01T17:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-146.93153000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[769,"MURRAYLINKV5_20211201203644","2015-01-01T17:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-174.16481999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[770,"MURRAYLINKV5_20211201203644","2015-01-01T17:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.274380000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[771,"MURRAYLINKV5_20211201203644","2015-01-01T17:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.35006999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[772,"MURRAYLINKV5_20211201203644","2015-01-01T17:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.49176,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[773,"MURRAYLINKV5_20211201203644","2015-01-01T17:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-56.439039999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[774,"MURRAYLINKV5_20211201203644","2015-01-01T17:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-134.08488,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[775,"MURRAYLINKV5_20211201203644","2015-01-01T17:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-177.48650000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[776,"MURRAYLINKV5_20211201203644","2015-01-01T17:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-47.781959999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[777,"MURRAYLINKV5_20211201203644","2015-01-01T17:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-149.04660999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[778,"MURRAYLINKV5_20211201203644","2015-01-01T17:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-176.53378000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[779,"MURRAYLINKV5_20211201203644","2015-01-01T17:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-46.71031,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[780,"MURRAYLINKV5_20211201203644","2015-01-01T17:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-148.20733000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[781,"MURRAYLINKV5_20211201203644","2015-01-01T17:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-175.27822,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[782,"MURRAYLINKV5_20211201203644","2015-01-01T17:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-46.86759,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[783,"MURRAYLINKV5_20211201203644","2015-01-01T17:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-149.26424,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[784,"MURRAYLINKV5_20211201203644","2015-01-01T17:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-176.85936000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[785,"MURRAYLINKV5_20211201203644","2015-01-01T17:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-95.146050000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[786,"MURRAYLINKV5_20211201203644","2015-01-01T17:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-95.898300000000006,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[787,"MURRAYLINKV5_20211201203644","2015-01-01T17:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-38.508130000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[788,"MURRAYLINKV5_20211201203644","2015-01-01T17:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-44.108139999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[789,"MURRAYLINKV5_20211201203644","2015-01-01T17:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-38.160670000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[790,"MURRAYLINKV5_20211201203644","2015-01-01T17:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-38.520859999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[791,"MURRAYLINKV5_20211201203644","2015-01-01T17:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-44.074750000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[792,"MURRAYLINKV5_20211201203644","2015-01-01T17:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-38.131779999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[793,"MURRAYLINKV5_20211201203644","2015-01-01T17:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.420960000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[794,"MURRAYLINKV5_20211201203644","2015-01-01T17:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-68.168890000000005,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[795,"MURRAYLINKV5_20211201203644","2015-01-01T17:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-68.706699999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[796,"MURRAYLINKV5_20211201203644","2015-01-01T18:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-32.098170000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[797,"MURRAYLINKV5_20211201203644","2015-01-01T18:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-42.897950000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[798,"MURRAYLINKV5_20211201203644","2015-01-01T18:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-43.236109999999996,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[799,"MURRAYLINKV5_20211201203644","2015-01-01T18:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-63.036360000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[800,"MURRAYLINKV5_20211201203644","2015-01-01T18:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-28.3231,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[801,"MURRAYLINKV5_20211201203644","2015-01-01T18:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-45.03895,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[802,"MURRAYLINKV5_20211201203644","2015-01-01T18:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-64.356840000000005,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[803,"MURRAYLINKV5_20211201203644","2015-01-01T18:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-95.145390000000006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[804,"MURRAYLINKV5_20211201203644","2015-01-01T18:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.5091,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[805,"MURRAYLINKV5_20211201203644","2015-01-01T18:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-39.52572,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[806,"MURRAYLINKV5_20211201203644","2015-01-01T18:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-50.741779999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[807,"MURRAYLINKV5_20211201203644","2015-01-01T18:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-40.359189999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[808,"MURRAYLINKV5_20211201203644","2015-01-01T18:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-62.222050000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[809,"MURRAYLINKV5_20211201203644","2015-01-01T18:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-136.98237,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[810,"MURRAYLINKV5_20211201203644","2015-01-01T18:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-51.42812,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[811,"MURRAYLINKV5_20211201203644","2015-01-01T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.241770000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[812,"MURRAYLINKV5_20211201203644","2015-01-01T18:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-50.658459999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[813,"MURRAYLINKV5_20211201203644","2015-01-01T18:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-39.549390000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[814,"MURRAYLINKV5_20211201203644","2015-01-01T18:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-37.081380000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[815,"MURRAYLINKV5_20211201203644","2015-01-01T18:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-22.873750000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[816,"MURRAYLINKV5_20211201203644","2015-01-01T18:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-38.06653,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[817,"MURRAYLINKV5_20211201203644","2015-01-01T18:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-20.377210000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[818,"MURRAYLINKV5_20211201203644","2015-01-01T19:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-50.0886,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[819,"MURRAYLINKV5_20211201203644","2015-01-01T19:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-34.598579999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[820,"MURRAYLINKV5_20211201203644","2015-01-01T19:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-28.628499999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[821,"MURRAYLINKV5_20211201203644","2015-01-01T19:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-44.292560000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[822,"MURRAYLINKV5_20211201203644","2015-01-01T19:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-40.555370000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[823,"MURRAYLINKV5_20211201203644","2015-01-01T19:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-58.644869999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[824,"MURRAYLINKV5_20211201203644","2015-01-01T19:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-41.145620000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[825,"MURRAYLINKV5_20211201203644","2015-01-01T19:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-57.971539999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[826,"MURRAYLINKV5_20211201203644","2015-01-01T19:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.90821,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[827,"MURRAYLINKV5_20211201203644","2015-01-01T19:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-32.206180000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[828,"MURRAYLINKV5_20211201203644","2015-01-01T19:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-22.405449999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[829,"MURRAYLINKV5_20211201203644","2015-01-01T19:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-35.76491,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[830,"MURRAYLINKV5_20211201203644","2015-01-01T19:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-31.576239999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[831,"MURRAYLINKV5_20211201203644","2015-01-01T19:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.536899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[832,"MURRAYLINKV5_20211201203644","2015-01-01T19:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-52.496960000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[833,"MURRAYLINKV5_20211201203644","2015-01-01T19:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-52.543050000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[834,"MURRAYLINKV5_20211201203644","2015-01-01T19:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-18.102630000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[835,"MURRAYLINKV5_20211201203644","2015-01-01T19:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-84.973039999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[836,"MURRAYLINKV5_20211201203644","2015-01-01T19:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-20.70177,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[837,"MURRAYLINKV5_20211201203644","2015-01-01T19:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-84.939359999999994,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[838,"MURRAYLINKV5_20211201203644","2015-01-01T19:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-25.114070000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[839,"MURRAYLINKV5_20211201203644","2015-01-01T19:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-90.555400000000006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[840,"MURRAYLINKV5_20211201203644","2015-01-01T20:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-19.403569999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[841,"MURRAYLINKV5_20211201203644","2015-01-01T20:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-84.973060000000004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[842,"MURRAYLINKV5_20211201203644","2015-01-01T20:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-32.896059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[843,"MURRAYLINKV5_20211201203644","2015-01-01T20:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-94.557829999999996,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[844,"MURRAYLINKV5_20211201203644","2015-01-01T20:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-21.26249,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[845,"MURRAYLINKV5_20211201203644","2015-01-01T20:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-17.229140000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[846,"MURRAYLINKV5_20211201203644","2015-01-01T20:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-22.981539999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[847,"MURRAYLINKV5_20211201203644","2015-01-01T20:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.514099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[848,"MURRAYLINKV5_20211201203644","2015-01-01T20:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.035879999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[849,"MURRAYLINKV5_20211201203644","2015-01-01T20:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.328950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[850,"MURRAYLINKV5_20211201203644","2015-01-01T20:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-22.530550000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[851,"MURRAYLINKV5_20211201203644","2015-01-01T20:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.42938,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[852,"MURRAYLINKV5_20211201203644","2015-01-01T20:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.722629999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[853,"MURRAYLINKV5_20211201203644","2015-01-01T20:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-11.13571,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[854,"MURRAYLINKV5_20211201203644","2015-01-01T21:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.394,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[855,"MURRAYLINKV5_20211201203644","2015-01-01T21:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.06855,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[856,"MURRAYLINKV5_20211201203644","2015-01-01T21:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.53668,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[857,"MURRAYLINKV5_20211201203644","2015-01-01T21:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.732670000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[858,"MURRAYLINKV5_20211201203644","2015-01-01T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.604510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[859,"MURRAYLINKV5_20211201203644","2015-01-01T21:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.84168,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[860,"MURRAYLINKV5_20211201203644","2015-01-01T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.83211,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[861,"MURRAYLINKV5_20211201203644","2015-01-01T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.897320000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[862,"MURRAYLINKV5_20211201203644","2015-01-01T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.367650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[863,"MURRAYLINKV5_20211201203644","2015-01-01T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.01887,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[864,"MURRAYLINKV5_20211201203644","2015-01-01T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.042120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[865,"MURRAYLINKV5_20211201203644","2015-01-01T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.096069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[866,"MURRAYLINKV5_20211201203644","2015-01-01T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.970280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[867,"MURRAYLINKV5_20211201203644","2015-01-01T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.64874,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[868,"MURRAYLINKV5_20211201203644","2015-01-01T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.68695,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[869,"MURRAYLINKV5_20211201203644","2015-01-01T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.02971,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[870,"MURRAYLINKV5_20211201203644","2015-01-01T22:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.006500000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[871,"MURRAYLINKV5_20211201203644","2015-01-01T23:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.02169,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[872,"MURRAYLINKV5_20211201203644","2015-01-01T23:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.652419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[873,"MURRAYLINKV5_20211201203644","2015-01-01T23:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.45435,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[874,"MURRAYLINKV5_20211201203644","2015-01-01T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.19286,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[875,"MURRAYLINKV5_20211201203644","2015-01-01T23:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.0158,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[876,"MURRAYLINKV5_20211201203644","2015-01-01T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.891169999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[877,"MURRAYLINKV5_20211201203644","2015-01-01T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.864850000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[878,"MURRAYLINKV5_20211201203644","2015-01-01T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.80428,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[879,"MURRAYLINKV5_20211201203644","2015-01-02","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.08597,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[880,"MURRAYLINKV5_20211201203644","2015-01-02T00:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-14.929399999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[881,"MURRAYLINKV5_20211201203644","2015-01-02T00:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.87555,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[882,"MURRAYLINKV5_20211201203644","2015-01-02T00:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.17736,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[883,"MURRAYLINKV5_20211201203644","2015-01-02T00:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.916040000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[884,"MURRAYLINKV5_20211201203644","2015-01-02T00:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.1175,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[885,"MURRAYLINKV5_20211201203644","2015-01-02T00:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.063269999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[886,"MURRAYLINKV5_20211201203644","2015-01-02T00:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.21993,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[887,"MURRAYLINKV5_20211201203644","2015-01-02T00:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.74685,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[888,"MURRAYLINKV5_20211201203644","2015-01-02T00:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-15.976660000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[889,"MURRAYLINKV5_20211201203644","2015-01-02T00:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-20.397680000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[890,"MURRAYLINKV5_20211201203644","2015-01-02T00:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-14.72761,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[891,"MURRAYLINKV5_20211201203644","2015-01-02T00:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.39167,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[892,"MURRAYLINKV5_20211201203644","2015-01-02T00:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.36716,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[893,"MURRAYLINKV5_20211201203644","2015-01-02T01:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.427099999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[894,"MURRAYLINKV5_20211201203644","2015-01-02T01:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.76277,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[895,"MURRAYLINKV5_20211201203644","2015-01-02T01:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.366580000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[896,"MURRAYLINKV5_20211201203644","2015-01-02T01:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.947240000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[897,"MURRAYLINKV5_20211201203644","2015-01-02T01:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.422969999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[898,"MURRAYLINKV5_20211201203644","2015-01-02T01:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.884270000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[899,"MURRAYLINKV5_20211201203644","2015-01-02T01:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.48372,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[900,"MURRAYLINKV5_20211201203644","2015-01-02T01:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.38331,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[901,"MURRAYLINKV5_20211201203644","2015-01-02T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.91278,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[902,"MURRAYLINKV5_20211201203644","2015-01-02T01:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.21862,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[903,"MURRAYLINKV5_20211201203644","2015-01-02T01:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.75201,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[904,"MURRAYLINKV5_20211201203644","2015-01-02T01:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.81338,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[905,"MURRAYLINKV5_20211201203644","2015-01-02T01:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-15.78129,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[906,"MURRAYLINKV5_20211201203644","2015-01-02T01:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-20.492339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[907,"MURRAYLINKV5_20211201203644","2015-01-02T02:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.374549999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[908,"MURRAYLINKV5_20211201203644","2015-01-02T02:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.47109,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[909,"MURRAYLINKV5_20211201203644","2015-01-02T02:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.69994,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[910,"MURRAYLINKV5_20211201203644","2015-01-02T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.419549999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[911,"MURRAYLINKV5_20211201203644","2015-01-02T02:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.576589999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[912,"MURRAYLINKV5_20211201203644","2015-01-02T02:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.257,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[913,"MURRAYLINKV5_20211201203644","2015-01-02T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.365970000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[914,"MURRAYLINKV5_20211201203644","2015-01-02T02:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.19556,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[915,"MURRAYLINKV5_20211201203644","2015-01-02T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-14.58806,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[916,"MURRAYLINKV5_20211201203644","2015-01-02T02:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.363340000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[917,"MURRAYLINKV5_20211201203644","2015-01-02T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.45519,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[918,"MURRAYLINKV5_20211201203644","2015-01-02T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.941459999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[919,"MURRAYLINKV5_20211201203644","2015-01-02T02:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-14.12964,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[920,"MURRAYLINKV5_20211201203644","2015-01-02T02:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.413129999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[921,"MURRAYLINKV5_20211201203644","2015-01-02T02:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.831160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[922,"MURRAYLINKV5_20211201203644","2015-01-02T02:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.0739,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[923,"MURRAYLINKV5_20211201203644","2015-01-02T02:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.507009999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[924,"MURRAYLINKV5_20211201203644","2015-01-02T02:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-13.3071,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[925,"MURRAYLINKV5_20211201203644","2015-01-02T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.286940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[926,"MURRAYLINKV5_20211201203644","2015-01-02T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.18768,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[927,"MURRAYLINKV5_20211201203644","2015-01-02T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-13.30269,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[928,"MURRAYLINKV5_20211201203644","2015-01-02T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.28058,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[929,"MURRAYLINKV5_20211201203644","2015-01-02T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.29668,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[930,"MURRAYLINKV5_20211201203644","2015-01-02T03:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.71415,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[931,"MURRAYLINKV5_20211201203644","2015-01-02T03:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.867139999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[932,"MURRAYLINKV5_20211201203644","2015-01-02T03:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.03378,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[933,"MURRAYLINKV5_20211201203644","2015-01-02T03:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.098939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[934,"MURRAYLINKV5_20211201203644","2015-01-02T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.23901,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[935,"MURRAYLINKV5_20211201203644","2015-01-02T03:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-13.301539999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[936,"MURRAYLINKV5_20211201203644","2015-01-02T03:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.455719999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[937,"MURRAYLINKV5_20211201203644","2015-01-02T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.1782,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[938,"MURRAYLINKV5_20211201203644","2015-01-02T03:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.58961,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[939,"MURRAYLINKV5_20211201203644","2015-01-02T03:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.683479999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[940,"MURRAYLINKV5_20211201203644","2015-01-02T03:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.398910000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[941,"MURRAYLINKV5_20211201203644","2015-01-02T03:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-13.26253,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[942,"MURRAYLINKV5_20211201203644","2015-01-02T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.307749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[943,"MURRAYLINKV5_20211201203644","2015-01-02T03:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.974360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[944,"MURRAYLINKV5_20211201203644","2015-01-02T04:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.6067,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[945,"MURRAYLINKV5_20211201203644","2015-01-02T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-17.586659999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[946,"MURRAYLINKV5_20211201203644","2015-01-02T04:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.595969999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[947,"MURRAYLINKV5_20211201203644","2015-01-02T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.388590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[948,"MURRAYLINKV5_20211201203644","2015-01-02T06:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.589449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[949,"MURRAYLINKV5_20211201203644","2015-01-02T06:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.62791,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[950,"MURRAYLINKV5_20211201203644","2015-01-02T06:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.49066,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[951,"MURRAYLINKV5_20211201203644","2015-01-02T06:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.532080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[952,"MURRAYLINKV5_20211201203644","2015-01-02T06:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.24708,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[953,"MURRAYLINKV5_20211201203644","2015-01-02T07:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.2325,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[954,"MURRAYLINKV5_20211201203644","2015-01-02T07:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.52,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[955,"MURRAYLINKV5_20211201203644","2015-01-02T07:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.49539,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[956,"MURRAYLINKV5_20211201203644","2015-01-02T07:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.20806,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[957,"MURRAYLINKV5_20211201203644","2015-01-02T07:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.63672,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[958,"MURRAYLINKV5_20211201203644","2015-01-02T07:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.360760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[959,"MURRAYLINKV5_20211201203644","2015-01-02T07:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.33222,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[960,"MURRAYLINKV5_20211201203644","2015-01-02T07:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.581989999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[961,"MURRAYLINKV5_20211201203644","2015-01-02T08:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.511049999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[962,"MURRAYLINKV5_20211201203644","2015-01-02T08:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.6889,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[963,"MURRAYLINKV5_20211201203644","2015-01-02T08:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-106.24961999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[964,"MURRAYLINKV5_20211201203644","2015-01-02T08:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-143.18501000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[965,"MURRAYLINKV5_20211201203644","2015-01-02T08:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-102.21906,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[966,"MURRAYLINKV5_20211201203644","2015-01-02T08:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-140.78816,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[967,"MURRAYLINKV5_20211201203644","2015-01-02T08:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.64106,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[968,"MURRAYLINKV5_20211201203644","2015-01-02T08:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.729749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[969,"MURRAYLINKV5_20211201203644","2015-01-02T08:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-17.539280000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[970,"MURRAYLINKV5_20211201203644","2015-01-02T08:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-17.320209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[971,"MURRAYLINKV5_20211201203644","2015-01-02T08:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.91081,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[972,"MURRAYLINKV5_20211201203644","2015-01-02T09:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.147079999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[973,"MURRAYLINKV5_20211201203644","2015-01-02T09:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.488149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[974,"MURRAYLINKV5_20211201203644","2015-01-02T09:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.166239999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[975,"MURRAYLINKV5_20211201203644","2015-01-02T09:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.198360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[976,"MURRAYLINKV5_20211201203644","2015-01-02T09:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.414770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[977,"MURRAYLINKV5_20211201203644","2015-01-02T09:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-18.43759,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[978,"MURRAYLINKV5_20211201203644","2015-01-02T09:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-23.373950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[979,"MURRAYLINKV5_20211201203644","2015-01-02T09:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-71.853009999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[980,"MURRAYLINKV5_20211201203644","2015-01-02T09:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-139.54882000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[981,"MURRAYLINKV5_20211201203644","2015-01-02T09:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-34.6267,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[982,"MURRAYLINKV5_20211201203644","2015-01-02T09:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-33.67651,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[983,"MURRAYLINKV5_20211201203644","2015-01-02T09:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-44.473370000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[984,"MURRAYLINKV5_20211201203644","2015-01-02T09:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-74.943169999999995,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[985,"MURRAYLINKV5_20211201203644","2015-01-02T09:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-149.11535000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[986,"MURRAYLINKV5_20211201203644","2015-01-02T10:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-89.354929999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[987,"MURRAYLINKV5_20211201203644","2015-01-02T10:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-145.08797999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[988,"MURRAYLINKV5_20211201203644","2015-01-02T10:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-89.761870000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[989,"MURRAYLINKV5_20211201203644","2015-01-02T10:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-142.96686,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[990,"MURRAYLINKV5_20211201203644","2015-01-02T10:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-69.018860000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[991,"MURRAYLINKV5_20211201203644","2015-01-02T10:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-146.71414999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[992,"MURRAYLINKV5_20211201203644","2015-01-02T10:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-70.213409999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[993,"MURRAYLINKV5_20211201203644","2015-01-02T10:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-152.88704000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[994,"MURRAYLINKV5_20211201203644","2015-01-02T10:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-126.47637,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[995,"MURRAYLINKV5_20211201203644","2015-01-02T10:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-43.923490000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[996,"MURRAYLINKV5_20211201203644","2015-01-02T10:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-195.75456,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[997,"MURRAYLINKV5_20211201203644","2015-01-02T10:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-59.696980000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[998,"MURRAYLINKV5_20211201203644","2015-01-02T10:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-185.38920999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[999,"MURRAYLINKV5_20211201203644","2015-01-02T10:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.61797,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1000,"MURRAYLINKV5_20211201203644","2015-01-02T10:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-125.47577,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1001,"MURRAYLINKV5_20211201203644","2015-01-02T10:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-22.766680000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1002,"MURRAYLINKV5_20211201203644","2015-01-02T10:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-135.92643000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1003,"MURRAYLINKV5_20211201203644","2015-01-02T10:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-65.224500000000006,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1004,"MURRAYLINKV5_20211201203644","2015-01-02T10:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-178.61654999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1005,"MURRAYLINKV5_20211201203644","2015-01-02T10:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-60.363520000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1006,"MURRAYLINKV5_20211201203644","2015-01-02T10:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-176.41508999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1007,"MURRAYLINKV5_20211201203644","2015-01-02T10:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1105.5827300000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1008,"MURRAYLINKV5_20211201203644","2015-01-02T10:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-1102.1429499999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1009,"MURRAYLINKV5_20211201203644","2015-01-02T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-113.9932,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1010,"MURRAYLINKV5_20211201203644","2015-01-02T11:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-43.110849999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1011,"MURRAYLINKV5_20211201203644","2015-01-02T11:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-198.25994,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1012,"MURRAYLINKV5_20211201203644","2015-01-02T11:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2519.7524100000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1013,"MURRAYLINKV5_20211201203644","2015-01-02T11:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2588.73639,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1014,"MURRAYLINKV5_20211201203644","2015-01-02T11:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-40.908639999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1015,"MURRAYLINKV5_20211201203644","2015-01-02T11:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-136.45509000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1016,"MURRAYLINKV5_20211201203644","2015-01-02T11:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-189.14372,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1017,"MURRAYLINKV5_20211201203644","2015-01-02T11:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-59.96405,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1018,"MURRAYLINKV5_20211201203644","2015-01-02T11:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-258.96724999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1019,"MURRAYLINKV5_20211201203644","2015-01-02T11:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-310.02116999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1020,"MURRAYLINKV5_20211201203644","2015-01-02T11:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.629840000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1021,"MURRAYLINKV5_20211201203644","2015-01-02T11:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-162.68344999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1022,"MURRAYLINKV5_20211201203644","2015-01-02T11:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-213.80986999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1023,"MURRAYLINKV5_20211201203644","2015-01-02T11:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.540230000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1024,"MURRAYLINKV5_20211201203644","2015-01-02T11:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2616.9085700000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1025,"MURRAYLINKV5_20211201203644","2015-01-02T11:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2664.11742,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1026,"MURRAYLINKV5_20211201203644","2015-01-02T11:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.380179999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1027,"MURRAYLINKV5_20211201203644","2015-01-02T11:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-49.57658,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1028,"MURRAYLINKV5_20211201203644","2015-01-02T11:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-61.52861,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1029,"MURRAYLINKV5_20211201203644","2015-01-02T11:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-36.011899999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1030,"MURRAYLINKV5_20211201203644","2015-01-02T11:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-195.83493000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1031,"MURRAYLINKV5_20211201203644","2015-01-02T11:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-45.930050000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1032,"MURRAYLINKV5_20211201203644","2015-01-02T11:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-180.12006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1033,"MURRAYLINKV5_20211201203644","2015-01-02T11:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-349.29300000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1034,"MURRAYLINKV5_20211201203644","2015-01-02T11:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-307.28550000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1035,"MURRAYLINKV5_20211201203644","2015-01-02T11:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-163.61804000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1036,"MURRAYLINKV5_20211201203644","2015-01-02T11:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-34.074710000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1037,"MURRAYLINKV5_20211201203644","2015-01-02T11:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-196.90299999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1038,"MURRAYLINKV5_20211201203644","2015-01-02T11:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-64.280090000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1039,"MURRAYLINKV5_20211201203644","2015-01-02T11:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-85.013379999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1040,"MURRAYLINKV5_20211201203644","2015-01-02T12:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-63.359299999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1041,"MURRAYLINKV5_20211201203644","2015-01-02T12:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-76.422880000000006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1042,"MURRAYLINKV5_20211201203644","2015-01-02T12:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-6460.79846,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1043,"MURRAYLINKV5_20211201203644","2015-01-02T12:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-6881.4604300000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1044,"MURRAYLINKV5_20211201203644","2015-01-02T12:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3385.41705,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1045,"MURRAYLINKV5_20211201203644","2015-01-02T12:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-3510.82764,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1046,"MURRAYLINKV5_20211201203644","2015-01-02T12:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-45.463999999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1047,"MURRAYLINKV5_20211201203644","2015-01-02T12:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-179.5471,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1048,"MURRAYLINKV5_20211201203644","2015-01-02T12:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2696.43993,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1049,"MURRAYLINKV5_20211201203644","2015-01-02T12:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2752.73576,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1050,"MURRAYLINKV5_20211201203644","2015-01-02T12:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2655.2823199999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1051,"MURRAYLINKV5_20211201203644","2015-01-02T12:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2711.5778399999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1052,"MURRAYLINKV5_20211201203644","2015-01-02T12:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-49.075980000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1053,"MURRAYLINKV5_20211201203644","2015-01-02T12:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-184.08806999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1054,"MURRAYLINKV5_20211201203644","2015-01-02T12:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2592.86942,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1055,"MURRAYLINKV5_20211201203644","2015-01-02T12:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2641.0322299999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1056,"MURRAYLINKV5_20211201203644","2015-01-02T12:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2736.0615699999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1057,"MURRAYLINKV5_20211201203644","2015-01-02T12:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2792.3574899999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1058,"MURRAYLINKV5_20211201203644","2015-01-02T12:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2680.8038000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1059,"MURRAYLINKV5_20211201203644","2015-01-02T12:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2737.0992799999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1060,"MURRAYLINKV5_20211201203644","2015-01-02T12:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3469.6847699999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1061,"MURRAYLINKV5_20211201203644","2015-01-02T12:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-3595.8108000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1062,"MURRAYLINKV5_20211201203644","2015-01-02T12:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2711.7440200000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1063,"MURRAYLINKV5_20211201203644","2015-01-02T12:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2768.0400800000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1064,"MURRAYLINKV5_20211201203644","2015-01-02T13:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-6454.5820100000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1065,"MURRAYLINKV5_20211201203644","2015-01-02T13:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-6875.67605,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1066,"MURRAYLINKV5_20211201203644","2015-01-02T13:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1272.71516,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1067,"MURRAYLINKV5_20211201203644","2015-01-02T13:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-1262.45039,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1068,"MURRAYLINKV5_20211201203644","2015-01-02T13:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-84.811390000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1069,"MURRAYLINKV5_20211201203644","2015-01-02T13:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1163.5478599999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1070,"MURRAYLINKV5_20211201203644","2015-01-02T13:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-1174.4002399999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1071,"MURRAYLINKV5_20211201203644","2015-01-02T13:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-124.87309999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1072,"MURRAYLINKV5_20211201203644","2015-01-02T13:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-50.649479999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1073,"MURRAYLINKV5_20211201203644","2015-01-02T13:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-186.06623999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1074,"MURRAYLINKV5_20211201203644","2015-01-02T13:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2717.5677599999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1075,"MURRAYLINKV5_20211201203644","2015-01-02T13:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2773.6693500000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1076,"MURRAYLINKV5_20211201203644","2015-01-02T13:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2730.9843300000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1077,"MURRAYLINKV5_20211201203644","2015-01-02T13:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2787.08619,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1078,"MURRAYLINKV5_20211201203644","2015-01-02T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-52.893129999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1079,"MURRAYLINKV5_20211201203644","2015-01-02T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-186.47631000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1080,"MURRAYLINKV5_20211201203644","2015-01-02T13:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2381.6755400000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1081,"MURRAYLINKV5_20211201203644","2015-01-02T13:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2442.2254499999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1082,"MURRAYLINKV5_20211201203644","2015-01-02T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.241709999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1083,"MURRAYLINKV5_20211201203644","2015-01-02T13:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1168.7884200000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1084,"MURRAYLINKV5_20211201203644","2015-01-02T13:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-1195.76749,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1085,"MURRAYLINKV5_20211201203644","2015-01-02T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-137.4034,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1086,"MURRAYLINKV5_20211201203644","2015-01-02T13:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3522.0351000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1087,"MURRAYLINKV5_20211201203644","2015-01-02T13:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-3661.80654,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1088,"MURRAYLINKV5_20211201203644","2015-01-02T13:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-45.416139999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1089,"MURRAYLINKV5_20211201203644","2015-01-02T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-173.58743999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1090,"MURRAYLINKV5_20211201203644","2015-01-02T13:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-87.38682,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1091,"MURRAYLINKV5_20211201203644","2015-01-02T13:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3135.2277800000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1092,"MURRAYLINKV5_20211201203644","2015-01-02T13:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-3272.9837499999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1093,"MURRAYLINKV5_20211201203644","2015-01-02T14:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-41.158230000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1094,"MURRAYLINKV5_20211201203644","2015-01-02T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-143.24781999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1095,"MURRAYLINKV5_20211201203644","2015-01-02T14:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-95.91977,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1096,"MURRAYLINKV5_20211201203644","2015-01-02T14:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-63.733580000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1097,"MURRAYLINKV5_20211201203644","2015-01-02T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-171.42496,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1098,"MURRAYLINKV5_20211201203644","2015-01-02T14:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-93.993589999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1099,"MURRAYLINKV5_20211201203644","2015-01-02T14:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2776.6646999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1100,"MURRAYLINKV5_20211201203644","2015-01-02T14:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2832.7663200000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1101,"MURRAYLINKV5_20211201203644","2015-01-02T14:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2684.0842499999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1102,"MURRAYLINKV5_20211201203644","2015-01-02T14:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2731.8944799999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1103,"MURRAYLINKV5_20211201203644","2015-01-02T14:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-71.079089999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1104,"MURRAYLINKV5_20211201203644","2015-01-02T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-156.59078,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1105,"MURRAYLINKV5_20211201203644","2015-01-02T14:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2775.4095699999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1106,"MURRAYLINKV5_20211201203644","2015-01-02T14:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2841.7133399999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1107,"MURRAYLINKV5_20211201203644","2015-01-02T14:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2824.8334799999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1108,"MURRAYLINKV5_20211201203644","2015-01-02T14:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2891.1373199999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1109,"MURRAYLINKV5_20211201203644","2015-01-02T14:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2662.9313900000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1110,"MURRAYLINKV5_20211201203644","2015-01-02T14:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2716.8060799999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1111,"MURRAYLINKV5_20211201203644","2015-01-02T14:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-72.764830000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1112,"MURRAYLINKV5_20211201203644","2015-01-02T14:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-158.66905,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1113,"MURRAYLINKV5_20211201203644","2015-01-02T14:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-74.268839999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1114,"MURRAYLINKV5_20211201203644","2015-01-02T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-160.67676,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1115,"MURRAYLINKV5_20211201203644","2015-01-02T14:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2832.5618599999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1116,"MURRAYLINKV5_20211201203644","2015-01-02T14:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2898.8656299999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1117,"MURRAYLINKV5_20211201203644","2015-01-02T14:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-71.086650000000006,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1118,"MURRAYLINKV5_20211201203644","2015-01-02T14:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-161.75049000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1119,"MURRAYLINKV5_20211201203644","2015-01-02T15:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-73.245540000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1120,"MURRAYLINKV5_20211201203644","2015-01-02T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-159.30516,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1121,"MURRAYLINKV5_20211201203644","2015-01-02T15:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2739.92524,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1122,"MURRAYLINKV5_20211201203644","2015-01-02T15:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2798.1628799999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1123,"MURRAYLINKV5_20211201203644","2015-01-02T15:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-34.934139999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1124,"MURRAYLINKV5_20211201203644","2015-01-02T15:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-24.645209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1125,"MURRAYLINKV5_20211201203644","2015-01-02T15:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-60.594679999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1126,"MURRAYLINKV5_20211201203644","2015-01-02T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-27.57199,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1127,"MURRAYLINKV5_20211201203644","2015-01-02T15:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-34.86354,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1128,"MURRAYLINKV5_20211201203644","2015-01-02T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-58.76925,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1129,"MURRAYLINKV5_20211201203644","2015-01-02T15:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-39.737020000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1130,"MURRAYLINKV5_20211201203644","2015-01-02T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-54.434429999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1131,"MURRAYLINKV5_20211201203644","2015-01-02T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-61.486199999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1132,"MURRAYLINKV5_20211201203644","2015-01-02T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-62.094329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1133,"MURRAYLINKV5_20211201203644","2015-01-02T15:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.023489999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1134,"MURRAYLINKV5_20211201203644","2015-01-02T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-59.195659999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1135,"MURRAYLINKV5_20211201203644","2015-01-02T15:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-29.48133,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1136,"MURRAYLINKV5_20211201203644","2015-01-02T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-59.822049999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1137,"MURRAYLINKV5_20211201203644","2015-01-02T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-154.15405999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1138,"MURRAYLINKV5_20211201203644","2015-01-02T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-57.804729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1139,"MURRAYLINKV5_20211201203644","2015-01-02T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-61.298920000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1140,"MURRAYLINKV5_20211201203644","2015-01-02T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-61.235190000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1141,"MURRAYLINKV5_20211201203644","2015-01-02T16:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-31.61656,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1142,"MURRAYLINKV5_20211201203644","2015-01-02T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-58.931510000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1143,"MURRAYLINKV5_20211201203644","2015-01-02T16:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2330.8997599999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1144,"MURRAYLINKV5_20211201203644","2015-01-02T16:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2616.2100999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1145,"MURRAYLINKV5_20211201203644","2015-01-02T16:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2325.9697099999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1146,"MURRAYLINKV5_20211201203644","2015-01-02T16:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2610.00434,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1147,"MURRAYLINKV5_20211201203644","2015-01-02T16:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-237.35451,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1148,"MURRAYLINKV5_20211201203644","2015-01-02T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-35.978520000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1149,"MURRAYLINKV5_20211201203644","2015-01-02T16:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-57.192329999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1150,"MURRAYLINKV5_20211201203644","2015-01-02T16:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-241.95930999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1151,"MURRAYLINKV5_20211201203644","2015-01-02T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-46.525869999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1152,"MURRAYLINKV5_20211201203644","2015-01-02T16:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-23.122229999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1153,"MURRAYLINKV5_20211201203644","2015-01-02T16:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-269.80117000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1154,"MURRAYLINKV5_20211201203644","2015-01-02T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-41.6267,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1155,"MURRAYLINKV5_20211201203644","2015-01-02T16:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2719.6259399999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1156,"MURRAYLINKV5_20211201203644","2015-01-02T16:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-3016.9067100000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1157,"MURRAYLINKV5_20211201203644","2015-01-02T16:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-727.38248999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1158,"MURRAYLINKV5_20211201203644","2015-01-02T16:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-986.26716999999996,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1159,"MURRAYLINKV5_20211201203644","2015-01-02T16:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-80.98912,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1160,"MURRAYLINKV5_20211201203644","2015-01-02T17:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-241.76452,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1161,"MURRAYLINKV5_20211201203644","2015-01-02T17:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-219.83779999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1162,"MURRAYLINKV5_20211201203644","2015-01-02T17:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-35.824550000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1163,"MURRAYLINKV5_20211201203644","2015-01-02T17:10:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-319.02551,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1164,"MURRAYLINKV5_20211201203644","2015-01-02T17:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-254.35203000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1165,"MURRAYLINKV5_20211201203644","2015-01-02T17:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-37.177660000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1166,"MURRAYLINKV5_20211201203644","2015-01-02T17:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-28.68206,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1167,"MURRAYLINKV5_20211201203644","2015-01-02T17:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-249.68266,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1168,"MURRAYLINKV5_20211201203644","2015-01-02T17:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-57.150849999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1169,"MURRAYLINKV5_20211201203644","2015-01-02T17:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-48.293509999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1170,"MURRAYLINKV5_20211201203644","2015-01-02T17:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-52.800800000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1171,"MURRAYLINKV5_20211201203644","2015-01-02T17:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-48.059600000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1172,"MURRAYLINKV5_20211201203644","2015-01-02T18:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-62.364699999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1173,"MURRAYLINKV5_20211201203644","2015-01-02T18:05:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-281.42711000000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1174,"MURRAYLINKV5_20211201203644","2015-01-02T18:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-263.54939999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1175,"MURRAYLINKV5_20211201203644","2015-01-02T18:15:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-266.27104000000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1176,"MURRAYLINKV5_20211201203644","2015-01-02T18:20:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-268.72563000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1177,"MURRAYLINKV5_20211201203644","2015-01-02T18:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-272.44729000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1178,"MURRAYLINKV5_20211201203644","2015-01-02T18:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.87013000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1179,"MURRAYLINKV5_20211201203644","2015-01-02T18:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-276.57913000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1180,"MURRAYLINKV5_20211201203644","2015-01-02T18:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-265.16723999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1181,"MURRAYLINKV5_20211201203644","2015-01-02T18:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-266.26172000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1182,"MURRAYLINKV5_20211201203644","2015-01-02T18:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-242.78578999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1183,"MURRAYLINKV5_20211201203644","2015-01-02T19:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-34.896070000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1184,"MURRAYLINKV5_20211201203644","2015-01-02T19:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2150.6551199999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1185,"MURRAYLINKV5_20211201203644","2015-01-02T19:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.02084,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1186,"MURRAYLINKV5_20211201203644","2015-01-02T19:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-262.15384,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1187,"MURRAYLINKV5_20211201203644","2015-01-02T19:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-259.19103000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1188,"MURRAYLINKV5_20211201203644","2015-01-02T19:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-53.503610000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1189,"MURRAYLINKV5_20211201203644","2015-01-02T19:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.729340000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1190,"MURRAYLINKV5_20211201203644","2015-01-02T19:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-250.232,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1191,"MURRAYLINKV5_20211201203644","2015-01-02T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-29.765000000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1192,"MURRAYLINKV5_20211201203644","2015-01-02T20:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-11.249779999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1193,"MURRAYLINKV5_20211201203644","2015-01-02T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-21.368300000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1194,"MURRAYLINKV5_20211201203644","2015-01-02T21:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.41746,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1195,"MURRAYLINKV5_20211201203644","2015-01-02T22:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-13.35863,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1196,"MURRAYLINKV5_20211201203644","2015-01-02T22:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.42802,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1197,"MURRAYLINKV5_20211201203644","2015-01-02T22:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-15.924849999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1198,"MURRAYLINKV5_20211201203644","2015-01-02T23:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.28088,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1199,"MURRAYLINKV5_20211201203644","2015-01-03T05:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.06673,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1200,"MURRAYLINKV5_20211201203644","2015-01-03T05:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.3004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1201,"MURRAYLINKV5_20211201203644","2015-01-03T10:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-77.353309999999993,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1202,"MURRAYLINKV5_20211201203644","2015-01-03T10:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-81.878609999999995,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1203,"MURRAYLINKV5_20211201203644","2015-01-03T10:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-50.588349999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1204,"MURRAYLINKV5_20211201203644","2015-01-03T10:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-55.531089999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1205,"MURRAYLINKV5_20211201203644","2015-01-03T10:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-46.93441,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1206,"MURRAYLINKV5_20211201203644","2015-01-03T10:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-51.873420000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1207,"MURRAYLINKV5_20211201203644","2015-01-03T10:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-51.015700000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1208,"MURRAYLINKV5_20211201203644","2015-01-03T10:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-55.949509999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1209,"MURRAYLINKV5_20211201203644","2015-01-03T10:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-51.876510000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1210,"MURRAYLINKV5_20211201203644","2015-01-03T10:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-57.018140000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1211,"MURRAYLINKV5_20211201203644","2015-01-03T10:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-50.355060000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1212,"MURRAYLINKV5_20211201203644","2015-01-03T10:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-55.401310000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1213,"MURRAYLINKV5_20211201203644","2015-01-03T10:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-55.085990000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1214,"MURRAYLINKV5_20211201203644","2015-01-03T10:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-60.620489999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1215,"MURRAYLINKV5_20211201203644","2015-01-03T10:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-24.94885,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1216,"MURRAYLINKV5_20211201203644","2015-01-03T10:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.806090000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1217,"MURRAYLINKV5_20211201203644","2015-01-03T11:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-15.10074,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1218,"MURRAYLINKV5_20211201203644","2015-01-03T12:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-63.375109999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1219,"MURRAYLINKV5_20211201203644","2015-01-03T12:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-68.266109999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1220,"MURRAYLINKV5_20211201203644","2015-01-03T12:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-80.253339999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1221,"MURRAYLINKV5_20211201203644","2015-01-03T12:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-87.122540000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1222,"MURRAYLINKV5_20211201203644","2015-01-03T12:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-120.19009,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1223,"MURRAYLINKV5_20211201203644","2015-01-03T12:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-138.76521,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1224,"MURRAYLINKV5_20211201203644","2015-01-03T12:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-34.852170000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1225,"MURRAYLINKV5_20211201203644","2015-01-03T12:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-39.264499999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1226,"MURRAYLINKV5_20211201203644","2015-01-03T12:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-172.12296000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1227,"MURRAYLINKV5_20211201203644","2015-01-03T12:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-190.69816,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1228,"MURRAYLINKV5_20211201203644","2015-01-03T12:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-169.53053,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1229,"MURRAYLINKV5_20211201203644","2015-01-03T12:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-188.10572999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1230,"MURRAYLINKV5_20211201203644","2015-01-03T12:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-18.88897,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1231,"MURRAYLINKV5_20211201203644","2015-01-03T12:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.34337,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1232,"MURRAYLINKV5_20211201203644","2015-01-03T13:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-195.65393,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1233,"MURRAYLINKV5_20211201203644","2015-01-03T13:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-214.22913,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1234,"MURRAYLINKV5_20211201203644","2015-01-03T13:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-198.29487,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1235,"MURRAYLINKV5_20211201203644","2015-01-03T13:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-216.87007,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1236,"MURRAYLINKV5_20211201203644","2015-01-03T13:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-251.94654,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1237,"MURRAYLINKV5_20211201203644","2015-01-03T13:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-279.16493000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1238,"MURRAYLINKV5_20211201203644","2015-01-03T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-27.92033,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1239,"MURRAYLINKV5_20211201203644","2015-01-03T15:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-28.839569999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1240,"MURRAYLINKV5_20211201203644","2015-01-03T15:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-18.191590000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1241,"MURRAYLINKV5_20211201203644","2015-01-03T15:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-19.67943,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1242,"MURRAYLINKV5_20211201203644","2015-01-03T16:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-330.87130999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1243,"MURRAYLINKV5_20211201203644","2015-01-03T16:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-341.60590999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1244,"MURRAYLINKV5_20211201203644","2015-01-03T16:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2752.9460100000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1245,"MURRAYLINKV5_20211201203644","2015-01-03T16:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2755.05834,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1246,"MURRAYLINKV5_20211201203644","2015-01-03T16:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.747680000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1247,"MURRAYLINKV5_20211201203644","2015-01-03T16:55:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-14.96564,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1248,"MURRAYLINKV5_20211201203644","2015-01-03T17:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-208.86870999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1249,"MURRAYLINKV5_20211201203644","2015-01-03T17:00:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-212.36669000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1250,"MURRAYLINKV5_20211201203644","2015-01-03T17:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.210900000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1251,"MURRAYLINKV5_20211201203644","2015-01-03T17:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.965109999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1252,"MURRAYLINKV5_20211201203644","2015-01-03T17:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.18262,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1253,"MURRAYLINKV5_20211201203644","2015-01-04T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.01524,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1254,"MURRAYLINKV5_20211201203644","2015-01-04T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.188330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1255,"MURRAYLINKV5_20211201203644","2015-01-04T13:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-94.910349999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1256,"MURRAYLINKV5_20211201203644","2015-01-04T13:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-134.45624000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1257,"MURRAYLINKV5_20211201203644","2015-01-04T13:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-82.838160000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1258,"MURRAYLINKV5_20211201203644","2015-01-04T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-120.86793,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1259,"MURRAYLINKV5_20211201203644","2015-01-04T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.5167,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1260,"MURRAYLINKV5_20211201203644","2015-01-04T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.56162,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1261,"MURRAYLINKV5_20211201203644","2015-01-04T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.69054,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1262,"MURRAYLINKV5_20211201203644","2015-01-04T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.82089,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1263,"MURRAYLINKV5_20211201203644","2015-01-04T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.147080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1264,"MURRAYLINKV5_20211201203644","2015-01-04T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.882339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1265,"MURRAYLINKV5_20211201203644","2015-01-04T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.065329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1266,"MURRAYLINKV5_20211201203644","2015-01-04T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.105499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1267,"MURRAYLINKV5_20211201203644","2015-01-04T16:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.586130000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1268,"MURRAYLINKV5_20211201203644","2015-01-04T17:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.78952,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1269,"MURRAYLINKV5_20211201203644","2015-01-04T18:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.607430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1270,"MURRAYLINKV5_20211201203644","2015-01-04T18:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.38541,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1271,"MURRAYLINKV5_20211201203644","2015-01-04T18:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.2919,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1272,"MURRAYLINKV5_20211201203644","2015-01-04T22:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.5518,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1273,"MURRAYLINKV5_20211201203644","2015-01-05T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.01939,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1274,"MURRAYLINKV5_20211201203644","2015-01-05T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-12.05162,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1275,"MURRAYLINKV5_20211201203644","2015-01-05T13:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-19.91835,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1276,"MURRAYLINKV5_20211201203644","2015-01-05T13:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-20.399920000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1277,"MURRAYLINKV5_20211201203644","2015-01-05T14:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.97542,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1278,"MURRAYLINKV5_20211201203644","2015-01-05T14:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.778960000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1279,"MURRAYLINKV5_20211201203644","2015-01-05T14:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.12933,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1280,"MURRAYLINKV5_20211201203644","2015-01-05T14:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.97438,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1281,"MURRAYLINKV5_20211201203644","2015-01-05T14:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.93609,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1282,"MURRAYLINKV5_20211201203644","2015-01-05T14:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.99447,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1283,"MURRAYLINKV5_20211201203644","2015-01-05T14:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-19.045439999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1284,"MURRAYLINKV5_20211201203644","2015-01-05T14:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-20.978249999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1285,"MURRAYLINKV5_20211201203644","2015-01-05T14:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.463010000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1286,"MURRAYLINKV5_20211201203644","2015-01-05T14:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.14733,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1287,"MURRAYLINKV5_20211201203644","2015-01-05T14:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-19.789770000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1288,"MURRAYLINKV5_20211201203644","2015-01-05T14:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-19.20111,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1289,"MURRAYLINKV5_20211201203644","2015-01-05T15:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.714770000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1290,"MURRAYLINKV5_20211201203644","2015-01-05T15:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-20.132400000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1291,"MURRAYLINKV5_20211201203644","2015-01-05T15:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-26.180669999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1292,"MURRAYLINKV5_20211201203644","2015-01-05T15:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-127.96648999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1293,"MURRAYLINKV5_20211201203644","2015-01-05T15:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-27.693190000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1294,"MURRAYLINKV5_20211201203644","2015-01-05T16:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.16065,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1295,"MURRAYLINKV5_20211201203644","2015-01-05T16:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-118.95971,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1296,"MURRAYLINKV5_20211201203644","2015-01-05T17:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-132.84011000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1297,"MURRAYLINKV5_20211201203644","2015-01-05T17:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-251.50156999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1298,"MURRAYLINKV5_20211201203644","2015-01-05T17:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-278.28973000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1299,"MURRAYLINKV5_20211201203644","2015-01-05T17:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.97063000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1300,"MURRAYLINKV5_20211201203644","2015-01-05T17:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.83521000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1301,"MURRAYLINKV5_20211201203644","2015-01-05T17:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-270.58013999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1302,"MURRAYLINKV5_20211201203644","2015-01-05T17:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-120.61432000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1303,"MURRAYLINKV5_20211201203644","2015-01-05T17:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-279.96294,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1304,"MURRAYLINKV5_20211201203644","2015-01-05T17:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-394.04599999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1305,"MURRAYLINKV5_20211201203644","2015-01-05T17:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-173.78467000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1306,"MURRAYLINKV5_20211201203644","2015-01-05T18:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-161.53713999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1307,"MURRAYLINKV5_20211201203644","2015-01-05T18:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-246.12805,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1308,"MURRAYLINKV5_20211201203644","2015-01-05T18:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.470420000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1309,"MURRAYLINKV5_20211201203644","2015-01-05T18:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.554010000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1310,"MURRAYLINKV5_20211201203644","2015-01-05T18:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-24.182970000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1311,"MURRAYLINKV5_20211201203644","2015-01-05T21:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.825519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1312,"MURRAYLINKV5_20211201203644","2015-01-05T21:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.176729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1313,"MURRAYLINKV5_20211201203644","2015-01-06T01:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-14.569929999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1314,"MURRAYLINKV5_20211201203644","2015-01-06T01:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-16.680820000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1315,"MURRAYLINKV5_20211201203644","2015-01-06T10:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.171790000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1316,"MURRAYLINKV5_20211201203644","2015-01-06T10:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.171790000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1317,"MURRAYLINKV5_20211201203644","2015-01-06T10:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.12677,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1318,"MURRAYLINKV5_20211201203644","2015-01-06T10:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.391359999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1319,"MURRAYLINKV5_20211201203644","2015-01-06T11:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-13.139279999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1320,"MURRAYLINKV5_20211201203644","2015-01-06T11:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.212479999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1321,"MURRAYLINKV5_20211201203644","2015-01-06T11:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.6464,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1322,"MURRAYLINKV5_20211201203644","2015-01-06T11:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-18.192350000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1323,"MURRAYLINKV5_20211201203644","2015-01-06T11:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-13.787610000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1324,"MURRAYLINKV5_20211201203644","2015-01-06T11:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.355370000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1325,"MURRAYLINKV5_20211201203644","2015-01-06T11:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-55.553930000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1326,"MURRAYLINKV5_20211201203644","2015-01-06T11:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-45.713970000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1327,"MURRAYLINKV5_20211201203644","2015-01-06T11:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-58.919420000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1328,"MURRAYLINKV5_20211201203644","2015-01-06T11:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-184.55843999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1329,"MURRAYLINKV5_20211201203644","2015-01-06T11:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-169.29133999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1330,"MURRAYLINKV5_20211201203644","2015-01-06T12:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-193.12694999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1331,"MURRAYLINKV5_20211201203644","2015-01-06T12:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-274.83037999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1332,"MURRAYLINKV5_20211201203644","2015-01-06T12:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-71.074110000000005,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1333,"MURRAYLINKV5_20211201203644","2015-01-06T12:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-61.348379999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1334,"MURRAYLINKV5_20211201203644","2015-01-06T12:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-49.842979999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1335,"MURRAYLINKV5_20211201203644","2015-01-06T12:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-187.37564,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1336,"MURRAYLINKV5_20211201203644","2015-01-06T12:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-274.83037999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1337,"MURRAYLINKV5_20211201203644","2015-01-06T12:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-192.74288000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1338,"MURRAYLINKV5_20211201203644","2015-01-06T12:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-61.031230000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1339,"MURRAYLINKV5_20211201203644","2015-01-06T12:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-194.34132,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1340,"MURRAYLINKV5_20211201203644","2015-01-06T12:50:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-249.89053999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1341,"MURRAYLINKV5_20211201203644","2015-01-06T12:55:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-204.50299999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1342,"MURRAYLINKV5_20211201203644","2015-01-06T13:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-570.58855000000005,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1343,"MURRAYLINKV5_20211201203644","2015-01-06T13:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-193.19269,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1344,"MURRAYLINKV5_20211201203644","2015-01-06T13:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-143.68628000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1345,"MURRAYLINKV5_20211201203644","2015-01-06T13:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.55493999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1346,"MURRAYLINKV5_20211201203644","2015-01-06T13:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-262.26913000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1347,"MURRAYLINKV5_20211201203644","2015-01-06T13:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-189.61822000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1348,"MURRAYLINKV5_20211201203644","2015-01-06T13:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-190.95787999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1349,"MURRAYLINKV5_20211201203644","2015-01-06T13:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-259.17014,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1350,"MURRAYLINKV5_20211201203644","2015-01-06T13:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-260.76492000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1351,"MURRAYLINKV5_20211201203644","2015-01-06T13:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-183.74294,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1352,"MURRAYLINKV5_20211201203644","2015-01-06T13:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-183.97740999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1353,"MURRAYLINKV5_20211201203644","2015-01-06T13:55:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-267.14411000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1354,"MURRAYLINKV5_20211201203644","2015-01-06T14:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-261.81209999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1355,"MURRAYLINKV5_20211201203644","2015-01-06T14:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-182.54446999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1356,"MURRAYLINKV5_20211201203644","2015-01-06T14:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-32.243850000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1357,"MURRAYLINKV5_20211201203644","2015-01-06T14:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-83.188900000000004,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1358,"MURRAYLINKV5_20211201203644","2015-01-06T14:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-32.700000000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1359,"MURRAYLINKV5_20211201203644","2015-01-06T14:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-83.416330000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1360,"MURRAYLINKV5_20211201203644","2015-01-06T14:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-32.700000000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1361,"MURRAYLINKV5_20211201203644","2015-01-06T14:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-56.988259999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1362,"MURRAYLINKV5_20211201203644","2015-01-06T14:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-34.580539999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1363,"MURRAYLINKV5_20211201203644","2015-01-06T14:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-191.94613000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1364,"MURRAYLINKV5_20211201203644","2015-01-06T14:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-24.06165,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1365,"MURRAYLINKV5_20211201203644","2015-01-06T14:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-56.036520000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1366,"MURRAYLINKV5_20211201203644","2015-01-06T14:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-34.62368,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1367,"MURRAYLINKV5_20211201203644","2015-01-06T14:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-56.047840000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1368,"MURRAYLINKV5_20211201203644","2015-01-06T14:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-34.613729999999997,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1369,"MURRAYLINKV5_20211201203644","2015-01-06T14:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-45.096240000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1370,"MURRAYLINKV5_20211201203644","2015-01-06T14:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-43.80153,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1371,"MURRAYLINKV5_20211201203644","2015-01-06T14:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-32.645130000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1372,"MURRAYLINKV5_20211201203644","2015-01-06T14:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-114.39399,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1373,"MURRAYLINKV5_20211201203644","2015-01-06T14:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-33.092230000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1374,"MURRAYLINKV5_20211201203644","2015-01-06T15:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-538.97171000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1375,"MURRAYLINKV5_20211201203644","2015-01-06T15:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-576.69213000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1376,"MURRAYLINKV5_20211201203644","2015-01-06T15:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-151.21617000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1377,"MURRAYLINKV5_20211201203644","2015-01-06T15:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-62.942140000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1378,"MURRAYLINKV5_20211201203644","2015-01-06T15:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-62.016570000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1379,"MURRAYLINKV5_20211201203644","2015-01-06T15:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-61.462739999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1380,"MURRAYLINKV5_20211201203644","2015-01-06T15:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-191.11330000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1381,"MURRAYLINKV5_20211201203644","2015-01-06T15:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-167.95921000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1382,"MURRAYLINKV5_20211201203644","2015-01-06T15:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-144.03745000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1383,"MURRAYLINKV5_20211201203644","2015-01-06T15:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-38.057549999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1384,"MURRAYLINKV5_20211201203644","2015-01-06T15:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.09854,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1385,"MURRAYLINKV5_20211201203644","2015-01-06T15:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-37.53304,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1386,"MURRAYLINKV5_20211201203644","2015-01-06T16:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-47.837690000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1387,"MURRAYLINKV5_20211201203644","2015-01-06T16:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-160.63711000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1388,"MURRAYLINKV5_20211201203644","2015-01-06T16:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-176.58884,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1389,"MURRAYLINKV5_20211201203644","2015-01-06T16:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-148.76393999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1390,"MURRAYLINKV5_20211201203644","2015-01-06T16:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-186.40267,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1391,"MURRAYLINKV5_20211201203644","2015-01-06T16:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-40.004930000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1392,"MURRAYLINKV5_20211201203644","2015-01-06T16:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-114.46588,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1393,"MURRAYLINKV5_20211201203644","2015-01-06T16:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-33.03,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1394,"MURRAYLINKV5_20211201203644","2015-01-06T16:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-33.03,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1395,"MURRAYLINKV5_20211201203644","2015-01-06T16:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-49.866379999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1396,"MURRAYLINKV5_20211201203644","2015-01-06T16:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-46.968069999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1397,"MURRAYLINKV5_20211201203644","2015-01-06T16:40:00","V>>V_ROTS_TX_3A_R","V-ROTX_R","2014-03-04",1,-10.902749999999999,"Out= Rowville A1 or A2 500/220 kV txfmr, avoid overload of the South Morang F2 500/330 kV txfmr for trip of the remaining Rowville 500/220 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1398,"MURRAYLINKV5_20211201203644","2015-01-06T16:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-55.585009999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1399,"MURRAYLINKV5_20211201203644","2015-01-06T16:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-52.62623,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1400,"MURRAYLINKV5_20211201203644","2015-01-06T16:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-54.487749999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1401,"MURRAYLINKV5_20211201203644","2015-01-06T17:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.45533,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1402,"MURRAYLINKV5_20211201203644","2015-01-06T17:00:00","V>>V_ROTS_TX_3A_R","V-ROTX_R","2014-03-04",1,-14.906169999999999,"Out= Rowville A1 or A2 500/220 kV txfmr, avoid overload of the South Morang F2 500/330 kV txfmr for trip of the remaining Rowville 500/220 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1403,"MURRAYLINKV5_20211201203644","2015-01-06T17:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-281.72019999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1404,"MURRAYLINKV5_20211201203644","2015-01-06T17:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-16.37433,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1405,"MURRAYLINKV5_20211201203644","2015-01-06T17:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-62.39714,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1406,"MURRAYLINKV5_20211201203644","2015-01-06T17:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-28.282109999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1407,"MURRAYLINKV5_20211201203644","2015-01-06T17:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-21.320810000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1408,"MURRAYLINKV5_20211201203644","2015-01-06T17:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-34.411360000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1409,"MURRAYLINKV5_20211201203644","2015-01-06T17:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-11.617330000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1410,"MURRAYLINKV5_20211201203644","2015-01-06T17:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-39.92606,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1411,"MURRAYLINKV5_20211201203644","2015-01-06T17:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.04386,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1412,"MURRAYLINKV5_20211201203644","2015-01-06T17:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-39.726280000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1413,"MURRAYLINKV5_20211201203644","2015-01-06T17:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-164.55080000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1414,"MURRAYLINKV5_20211201203644","2015-01-06T17:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-20.200189999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1415,"MURRAYLINKV5_20211201203644","2015-01-06T17:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.63470999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1416,"MURRAYLINKV5_20211201203644","2015-01-06T17:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.404409999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1417,"MURRAYLINKV5_20211201203644","2015-01-06T17:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-20.537189999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1418,"MURRAYLINKV5_20211201203644","2015-01-06T17:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-20.582329999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1419,"MURRAYLINKV5_20211201203644","2015-01-06T17:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-21.95795,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1420,"MURRAYLINKV5_20211201203644","2015-01-06T18:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-138.15516,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1421,"MURRAYLINKV5_20211201203644","2015-01-06T18:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-277.87385,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1422,"MURRAYLINKV5_20211201203644","2015-01-06T18:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-266.67021999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1423,"MURRAYLINKV5_20211201203644","2015-01-06T18:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-147.1335,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1424,"MURRAYLINKV5_20211201203644","2015-01-06T18:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-267.50473,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1425,"MURRAYLINKV5_20211201203644","2015-01-06T18:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-139.72474,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1426,"MURRAYLINKV5_20211201203644","2015-01-06T18:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-38.179070000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1427,"MURRAYLINKV5_20211201203644","2015-01-06T18:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.55101,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1428,"MURRAYLINKV5_20211201203644","2015-01-06T18:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-22.440460000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1429,"MURRAYLINKV5_20211201203644","2015-01-06T18:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-21.36439,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1430,"MURRAYLINKV5_20211201203644","2015-01-06T18:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.41254,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1431,"MURRAYLINKV5_20211201203644","2015-01-06T18:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.412489999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1432,"MURRAYLINKV5_20211201203644","2015-01-06T19:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.412489999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1433,"MURRAYLINKV5_20211201203644","2015-01-06T19:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-22.390499999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1434,"MURRAYLINKV5_20211201203644","2015-01-06T19:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.281230000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1435,"MURRAYLINKV5_20211201203644","2015-01-06T19:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-23.412489999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1436,"MURRAYLINKV5_20211201203644","2015-01-06T19:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-11.28998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1437,"MURRAYLINKV5_20211201203644","2015-01-06T19:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.281269999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1438,"MURRAYLINKV5_20211201203644","2015-01-06T19:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.281269999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1439,"MURRAYLINKV5_20211201203644","2015-01-06T19:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-10.281269999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1440,"MURRAYLINKV5_20211201203644","2015-01-06T21:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.3003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1441,"MURRAYLINKV5_20211201203644","2015-01-06T21:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.350529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1442,"MURRAYLINKV5_20211201203644","2015-01-06T21:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.638369999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1443,"MURRAYLINKV5_20211201203644","2015-01-06T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.138639999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1444,"MURRAYLINKV5_20211201203644","2015-01-06T21:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.27345,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1445,"MURRAYLINKV5_20211201203644","2015-01-06T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.080490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1446,"MURRAYLINKV5_20211201203644","2015-01-06T21:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.563210000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1447,"MURRAYLINKV5_20211201203644","2015-01-06T21:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.084910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1448,"MURRAYLINKV5_20211201203644","2015-01-06T22:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.93066,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1449,"MURRAYLINKV5_20211201203644","2015-01-06T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.224989999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1450,"MURRAYLINKV5_20211201203644","2015-01-06T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.425370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1451,"MURRAYLINKV5_20211201203644","2015-01-06T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.72137,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1452,"MURRAYLINKV5_20211201203644","2015-01-06T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.086770000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1453,"MURRAYLINKV5_20211201203644","2015-01-06T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.60033,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1454,"MURRAYLINKV5_20211201203644","2015-01-06T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.65625,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1455,"MURRAYLINKV5_20211201203644","2015-01-06T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.72955,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1456,"MURRAYLINKV5_20211201203644","2015-01-06T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.3825,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1457,"MURRAYLINKV5_20211201203644","2015-01-06T22:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.833130000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1458,"MURRAYLINKV5_20211201203644","2015-01-06T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.311070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1459,"MURRAYLINKV5_20211201203644","2015-01-06T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.771509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1460,"MURRAYLINKV5_20211201203644","2015-01-06T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.063359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1461,"MURRAYLINKV5_20211201203644","2015-01-06T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.934090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1462,"MURRAYLINKV5_20211201203644","2015-01-06T23:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.72955,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1463,"MURRAYLINKV5_20211201203644","2015-01-06T23:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.43167,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1464,"MURRAYLINKV5_20211201203644","2015-01-06T23:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.52722,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1465,"MURRAYLINKV5_20211201203644","2015-01-06T23:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.7471,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1466,"MURRAYLINKV5_20211201203644","2015-01-06T23:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.340479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1467,"MURRAYLINKV5_20211201203644","2015-01-06T23:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.703489999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1468,"MURRAYLINKV5_20211201203644","2015-01-06T23:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.55104,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1469,"MURRAYLINKV5_20211201203644","2015-01-06T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-27.558900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1470,"MURRAYLINKV5_20211201203644","2015-01-06T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.166699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1471,"MURRAYLINKV5_20211201203644","2015-01-06T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.057919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1472,"MURRAYLINKV5_20211201203644","2015-01-07","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.318680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1473,"MURRAYLINKV5_20211201203644","2015-01-07T00:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.25872,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1474,"MURRAYLINKV5_20211201203644","2015-01-07T00:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.279039999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1475,"MURRAYLINKV5_20211201203644","2015-01-07T00:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-25.9678,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1476,"MURRAYLINKV5_20211201203644","2015-01-07T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.752410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1477,"MURRAYLINKV5_20211201203644","2015-01-07T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.4802,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1478,"MURRAYLINKV5_20211201203644","2015-01-07T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.01707,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1479,"MURRAYLINKV5_20211201203644","2015-01-07T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.035360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1480,"MURRAYLINKV5_20211201203644","2015-01-07T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.952100000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1481,"MURRAYLINKV5_20211201203644","2015-01-07T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.085979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1482,"MURRAYLINKV5_20211201203644","2015-01-07T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.736239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1483,"MURRAYLINKV5_20211201203644","2015-01-07T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.970880000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1484,"MURRAYLINKV5_20211201203644","2015-01-07T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.48884,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1485,"MURRAYLINKV5_20211201203644","2015-01-07T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.164639999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1486,"MURRAYLINKV5_20211201203644","2015-01-07T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.744769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1487,"MURRAYLINKV5_20211201203644","2015-01-07T01:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.99502,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1488,"MURRAYLINKV5_20211201203644","2015-01-07T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.083119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1489,"MURRAYLINKV5_20211201203644","2015-01-07T01:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.655709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1490,"MURRAYLINKV5_20211201203644","2015-01-07T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.419789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1491,"MURRAYLINKV5_20211201203644","2015-01-07T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.74784,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1492,"MURRAYLINKV5_20211201203644","2015-01-07T01:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.838380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1493,"MURRAYLINKV5_20211201203644","2015-01-07T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.924620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1494,"MURRAYLINKV5_20211201203644","2015-01-07T01:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.8643,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1495,"MURRAYLINKV5_20211201203644","2015-01-07T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.41527,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1496,"MURRAYLINKV5_20211201203644","2015-01-07T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.356590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1497,"MURRAYLINKV5_20211201203644","2015-01-07T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.8307,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1498,"MURRAYLINKV5_20211201203644","2015-01-07T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.117010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1499,"MURRAYLINKV5_20211201203644","2015-01-07T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.983650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1500,"MURRAYLINKV5_20211201203644","2015-01-07T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.9803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1501,"MURRAYLINKV5_20211201203644","2015-01-07T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.705030000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1502,"MURRAYLINKV5_20211201203644","2015-01-07T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.24789,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1503,"MURRAYLINKV5_20211201203644","2015-01-07T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.44469,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1504,"MURRAYLINKV5_20211201203644","2015-01-07T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.41686,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1505,"MURRAYLINKV5_20211201203644","2015-01-07T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.0238,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1506,"MURRAYLINKV5_20211201203644","2015-01-07T02:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.96153,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1507,"MURRAYLINKV5_20211201203644","2015-01-07T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.79833,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1508,"MURRAYLINKV5_20211201203644","2015-01-07T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.86131,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1509,"MURRAYLINKV5_20211201203644","2015-01-07T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.58445,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1510,"MURRAYLINKV5_20211201203644","2015-01-07T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.023630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1511,"MURRAYLINKV5_20211201203644","2015-01-07T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.83883,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1512,"MURRAYLINKV5_20211201203644","2015-01-07T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.008150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1513,"MURRAYLINKV5_20211201203644","2015-01-07T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.8483,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1514,"MURRAYLINKV5_20211201203644","2015-01-07T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.85901,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1515,"MURRAYLINKV5_20211201203644","2015-01-07T03:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.65544,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1516,"MURRAYLINKV5_20211201203644","2015-01-07T03:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.834059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1517,"MURRAYLINKV5_20211201203644","2015-01-07T03:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.62045,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1518,"MURRAYLINKV5_20211201203644","2015-01-07T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.80729,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1519,"MURRAYLINKV5_20211201203644","2015-01-07T03:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.095230000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1520,"MURRAYLINKV5_20211201203644","2015-01-07T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.99644,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1521,"MURRAYLINKV5_20211201203644","2015-01-07T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.954429999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1522,"MURRAYLINKV5_20211201203644","2015-01-07T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.278379999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1523,"MURRAYLINKV5_20211201203644","2015-01-07T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.825009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1524,"MURRAYLINKV5_20211201203644","2015-01-07T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.823910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1525,"MURRAYLINKV5_20211201203644","2015-01-07T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.722190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1526,"MURRAYLINKV5_20211201203644","2015-01-07T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.690239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1527,"MURRAYLINKV5_20211201203644","2015-01-07T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.609220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1528,"MURRAYLINKV5_20211201203644","2015-01-07T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.440329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1529,"MURRAYLINKV5_20211201203644","2015-01-07T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.90598,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1530,"MURRAYLINKV5_20211201203644","2015-01-07T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.615819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1531,"MURRAYLINKV5_20211201203644","2015-01-07T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.960049999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1532,"MURRAYLINKV5_20211201203644","2015-01-07T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.060870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1533,"MURRAYLINKV5_20211201203644","2015-01-07T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.734870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1534,"MURRAYLINKV5_20211201203644","2015-01-07T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.341189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1535,"MURRAYLINKV5_20211201203644","2015-01-07T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.803789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1536,"MURRAYLINKV5_20211201203644","2015-01-07T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-23.83644,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1537,"MURRAYLINKV5_20211201203644","2015-01-07T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.34216,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1538,"MURRAYLINKV5_20211201203644","2015-01-07T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.803470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1539,"MURRAYLINKV5_20211201203644","2015-01-07T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.831060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1540,"MURRAYLINKV5_20211201203644","2015-01-07T05:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.551490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1541,"MURRAYLINKV5_20211201203644","2015-01-07T05:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.746870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1542,"MURRAYLINKV5_20211201203644","2015-01-07T05:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.468530000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1543,"MURRAYLINKV5_20211201203644","2015-01-07T05:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.541869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1544,"MURRAYLINKV5_20211201203644","2015-01-07T06:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.279779999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1545,"MURRAYLINKV5_20211201203644","2015-01-07T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.25855,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1546,"MURRAYLINKV5_20211201203644","2015-01-07T06:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.604430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1547,"MURRAYLINKV5_20211201203644","2015-01-07T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.280639999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1548,"MURRAYLINKV5_20211201203644","2015-01-07T06:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.942489999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1549,"MURRAYLINKV5_20211201203644","2015-01-07T06:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.61665,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1550,"MURRAYLINKV5_20211201203644","2015-01-07T08:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.508849999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1551,"MURRAYLINKV5_20211201203644","2015-01-07T09:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-12.814170000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1552,"MURRAYLINKV5_20211201203644","2015-01-07T09:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-10.370710000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1553,"MURRAYLINKV5_20211201203644","2015-01-07T09:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-65.181920000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1554,"MURRAYLINKV5_20211201203644","2015-01-07T09:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-66.256770000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1555,"MURRAYLINKV5_20211201203644","2015-01-07T09:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-10.203239999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1556,"MURRAYLINKV5_20211201203644","2015-01-07T10:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-132.0763,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1557,"MURRAYLINKV5_20211201203644","2015-01-07T10:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-210.26913999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1558,"MURRAYLINKV5_20211201203644","2015-01-07T10:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-213.89512999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1559,"MURRAYLINKV5_20211201203644","2015-01-07T10:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-229.74831,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1560,"MURRAYLINKV5_20211201203644","2015-01-07T10:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-232.84363999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1561,"MURRAYLINKV5_20211201203644","2015-01-07T10:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-231.04526999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1562,"MURRAYLINKV5_20211201203644","2015-01-07T10:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-260.38166999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1563,"MURRAYLINKV5_20211201203644","2015-01-07T10:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-247.6121,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1564,"MURRAYLINKV5_20211201203644","2015-01-07T11:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-222.72318000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1565,"MURRAYLINKV5_20211201203644","2015-01-07T11:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-266.50486999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1566,"MURRAYLINKV5_20211201203644","2015-01-07T11:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-265.03771999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1567,"MURRAYLINKV5_20211201203644","2015-01-07T11:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-262.91037,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1568,"MURRAYLINKV5_20211201203644","2015-01-07T11:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-276.58863000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1569,"MURRAYLINKV5_20211201203644","2015-01-07T11:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-255.29546999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1570,"MURRAYLINKV5_20211201203644","2015-01-07T11:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-260.50389999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1571,"MURRAYLINKV5_20211201203644","2015-01-07T11:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-273.09985,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1572,"MURRAYLINKV5_20211201203644","2015-01-07T11:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-239.36256,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1573,"MURRAYLINKV5_20211201203644","2015-01-07T11:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-268.95711,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1574,"MURRAYLINKV5_20211201203644","2015-01-07T11:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-233.76971,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1575,"MURRAYLINKV5_20211201203644","2015-01-07T11:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-483.88670999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1576,"MURRAYLINKV5_20211201203644","2015-01-07T12:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-208.47309000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1577,"MURRAYLINKV5_20211201203644","2015-01-07T12:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-201.04504,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1578,"MURRAYLINKV5_20211201203644","2015-01-07T12:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-192.16471000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1579,"MURRAYLINKV5_20211201203644","2015-01-07T12:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-194.73145,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1580,"MURRAYLINKV5_20211201203644","2015-01-07T12:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12.587820000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1581,"MURRAYLINKV5_20211201203644","2015-01-07T12:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-132.34469000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1582,"MURRAYLINKV5_20211201203644","2015-01-07T12:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.658080000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1583,"MURRAYLINKV5_20211201203644","2015-01-07T12:50:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-96.410839999999993,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1584,"MURRAYLINKV5_20211201203644","2015-01-07T13:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-191.3733,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1585,"MURRAYLINKV5_20211201203644","2015-01-07T13:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-112.55267000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1586,"MURRAYLINKV5_20211201203644","2015-01-07T13:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-27.554569999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1587,"MURRAYLINKV5_20211201203644","2015-01-07T13:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-58.21163,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1588,"MURRAYLINKV5_20211201203644","2015-01-07T13:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-123.12679,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1589,"MURRAYLINKV5_20211201203644","2015-01-07T13:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-15.263059999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1590,"MURRAYLINKV5_20211201203644","2015-01-07T13:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-58.211210000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1591,"MURRAYLINKV5_20211201203644","2015-01-07T13:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-137.56028000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1592,"MURRAYLINKV5_20211201203644","2015-01-07T13:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-58.794930000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1593,"MURRAYLINKV5_20211201203644","2015-01-07T13:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-3001.3670499999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1594,"MURRAYLINKV5_20211201203644","2015-01-07T14:00:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-2244.2686899999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1595,"MURRAYLINKV5_20211201203644","2015-01-07T14:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-220.95648,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1596,"MURRAYLINKV5_20211201203644","2015-01-07T14:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-60.01455,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1597,"MURRAYLINKV5_20211201203644","2015-01-07T14:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-88.001270000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1598,"MURRAYLINKV5_20211201203644","2015-01-07T14:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-294.23505,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1599,"MURRAYLINKV5_20211201203644","2015-01-07T14:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-127.89922,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1600,"MURRAYLINKV5_20211201203644","2015-01-07T14:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-419.42734999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1601,"MURRAYLINKV5_20211201203644","2015-01-07T14:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-213.76936000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1602,"MURRAYLINKV5_20211201203644","2015-01-07T14:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-505.29748999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1603,"MURRAYLINKV5_20211201203644","2015-01-07T14:30:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-308.73144000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1604,"MURRAYLINKV5_20211201203644","2015-01-07T14:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1154.32728,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1605,"MURRAYLINKV5_20211201203644","2015-01-07T14:35:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-2860.7405100000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1606,"MURRAYLINKV5_20211201203644","2015-01-07T14:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-31.4831,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1607,"MURRAYLINKV5_20211201203644","2015-01-07T14:50:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-28.85821,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1608,"MURRAYLINKV5_20211201203644","2015-01-07T14:55:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-49.068089999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1609,"MURRAYLINKV5_20211201203644","2015-01-07T15:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-200.88076000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1610,"MURRAYLINKV5_20211201203644","2015-01-07T15:00:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-285.57337000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1611,"MURRAYLINKV5_20211201203644","2015-01-07T15:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2920.3674099999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1612,"MURRAYLINKV5_20211201203644","2015-01-07T15:05:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-637.95045000000005,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1613,"MURRAYLINKV5_20211201203644","2015-01-07T15:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2421.6479199999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1614,"MURRAYLINKV5_20211201203644","2015-01-07T15:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1575.1639299999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1615,"MURRAYLINKV5_20211201203644","2015-01-07T15:10:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-1659.41174,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1616,"MURRAYLINKV5_20211201203644","2015-01-07T15:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2895.9734899999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1617,"MURRAYLINKV5_20211201203644","2015-01-07T15:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2979.5057299999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1618,"MURRAYLINKV5_20211201203644","2015-01-07T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2615.6973400000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1619,"MURRAYLINKV5_20211201203644","2015-01-07T15:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2670.7565199999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1620,"MURRAYLINKV5_20211201203644","2015-01-07T15:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2445.3144499999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1621,"MURRAYLINKV5_20211201203644","2015-01-07T15:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2713.88904,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1622,"MURRAYLINKV5_20211201203644","2015-01-07T15:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-177.91073,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1623,"MURRAYLINKV5_20211201203644","2015-01-07T15:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-232.96991,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1624,"MURRAYLINKV5_20211201203644","2015-01-07T15:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2275.4250999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1625,"MURRAYLINKV5_20211201203644","2015-01-07T15:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2318.5675299999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1626,"MURRAYLINKV5_20211201203644","2015-01-07T15:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2223.8740899999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1627,"MURRAYLINKV5_20211201203644","2015-01-07T15:40:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-49.711320000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1628,"MURRAYLINKV5_20211201203644","2015-01-07T15:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-2217.4364300000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1629,"MURRAYLINKV5_20211201203644","2015-01-07T15:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2062.9523800000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1630,"MURRAYLINKV5_20211201203644","2015-01-07T15:45:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-2236.6969399999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1631,"MURRAYLINKV5_20211201203644","2015-01-07T15:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-35.169809999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1632,"MURRAYLINKV5_20211201203644","2015-01-07T15:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-29.216190000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1633,"MURRAYLINKV5_20211201203644","2015-01-07T16:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-28.993469999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1634,"MURRAYLINKV5_20211201203644","2015-01-07T16:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-255.42350999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1635,"MURRAYLINKV5_20211201203644","2015-01-07T16:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-39.604489999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1636,"MURRAYLINKV5_20211201203644","2015-01-07T16:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-33.294220000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1637,"MURRAYLINKV5_20211201203644","2015-01-07T16:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-32.716470000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1638,"MURRAYLINKV5_20211201203644","2015-01-07T16:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.483229999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1639,"MURRAYLINKV5_20211201203644","2015-01-07T16:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-17.853470000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1640,"MURRAYLINKV5_20211201203644","2015-01-07T16:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-13.157719999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1641,"MURRAYLINKV5_20211201203644","2015-01-07T16:35:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-2409.32908,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1642,"MURRAYLINKV5_20211201203644","2015-01-07T16:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2316.9053199999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1643,"MURRAYLINKV5_20211201203644","2015-01-07T16:40:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-02-03",1,-2373.0783000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1644,"MURRAYLINKV5_20211201203644","2015-01-07T16:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-333.88046000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1645,"MURRAYLINKV5_20211201203644","2015-01-07T16:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-336.85534000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1646,"MURRAYLINKV5_20211201203644","2015-01-07T16:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-1567.4225200000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1647,"MURRAYLINKV5_20211201203644","2015-01-07T16:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-1568.51785,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1648,"MURRAYLINKV5_20211201203644","2015-01-07T16:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-4427.2614000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1649,"MURRAYLINKV5_20211201203644","2015-01-07T16:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-4427.2614199999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1650,"MURRAYLINKV5_20211201203644","2015-01-07T17:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-4286.9197400000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1651,"MURRAYLINKV5_20211201203644","2015-01-07T17:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-4287.5016699999996,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1652,"MURRAYLINKV5_20211201203644","2015-01-07T17:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-30.31962,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1653,"MURRAYLINKV5_20211201203644","2015-01-07T18:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-29.728010000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1654,"MURRAYLINKV5_20211201203644","2015-01-07T19:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-13.717169999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1655,"MURRAYLINKV5_20211201203644","2015-01-07T19:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-15.23822,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1656,"MURRAYLINKV5_20211201203644","2015-01-07T20:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-13.263389999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1657,"MURRAYLINKV5_20211201203644","2015-01-07T20:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-11.06293,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1658,"MURRAYLINKV5_20211201203644","2015-01-07T20:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-21.38796,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1659,"MURRAYLINKV5_20211201203644","2015-01-08T02:40:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-19.68037,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1660,"MURRAYLINKV5_20211201203644","2015-01-08T09:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-17.20729,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1661,"MURRAYLINKV5_20211201203644","2015-01-08T09:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-23.434419999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1662,"MURRAYLINKV5_20211201203644","2015-01-08T09:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-25.78182,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1663,"MURRAYLINKV5_20211201203644","2015-01-08T09:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-17.571760000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1664,"MURRAYLINKV5_20211201203644","2015-01-08T10:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-49.493290000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1665,"MURRAYLINKV5_20211201203644","2015-01-08T12:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-27.544239999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1666,"MURRAYLINKV5_20211201203644","2015-01-08T12:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-19.41891,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1667,"MURRAYLINKV5_20211201203644","2015-01-08T12:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-11-25",1,-10.4201,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1668,"MURRAYLINKV5_20211201203644","2015-01-09T03:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.53176,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1669,"MURRAYLINKV5_20211201203644","2015-01-09T04:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.12969,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1670,"MURRAYLINKV5_20211201203644","2015-01-09T04:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.89678,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1671,"MURRAYLINKV5_20211201203644","2015-01-09T04:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.60515,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1672,"MURRAYLINKV5_20211201203644","2015-01-09T04:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.60473,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1673,"MURRAYLINKV5_20211201203644","2015-01-09T14:55:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.988939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1674,"MURRAYLINKV5_20211201203644","2015-01-09T21:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.77514,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1675,"MURRAYLINKV5_20211201203644","2015-01-09T22:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.883979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1676,"MURRAYLINKV5_20211201203644","2015-01-09T22:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.77844,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1677,"MURRAYLINKV5_20211201203644","2015-01-09T22:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.34704,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1678,"MURRAYLINKV5_20211201203644","2015-01-09T22:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.37121,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1679,"MURRAYLINKV5_20211201203644","2015-01-09T22:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.651389999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1680,"MURRAYLINKV5_20211201203644","2015-01-09T22:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.674390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1681,"MURRAYLINKV5_20211201203644","2015-01-09T22:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.8443,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1682,"MURRAYLINKV5_20211201203644","2015-01-09T23:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.569979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1683,"MURRAYLINKV5_20211201203644","2015-01-10T00:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.35647,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1684,"MURRAYLINKV5_20211201203644","2015-01-10T00:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.010479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1685,"MURRAYLINKV5_20211201203644","2015-01-10T00:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.85727,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1686,"MURRAYLINKV5_20211201203644","2015-01-10T00:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.1944,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1687,"MURRAYLINKV5_20211201203644","2015-01-10T00:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.7347,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1688,"MURRAYLINKV5_20211201203644","2015-01-10T00:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.01262,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1689,"MURRAYLINKV5_20211201203644","2015-01-10T00:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.255190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1690,"MURRAYLINKV5_20211201203644","2015-01-10T00:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.157879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1691,"MURRAYLINKV5_20211201203644","2015-01-10T00:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.57464,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1692,"MURRAYLINKV5_20211201203644","2015-01-10T00:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.038209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1693,"MURRAYLINKV5_20211201203644","2015-01-11T10:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-13.29388,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1694,"MURRAYLINKV5_20211201203644","2015-01-11T11:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.073359999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1695,"MURRAYLINKV5_20211201203644","2015-01-11T11:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.218159999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1696,"MURRAYLINKV5_20211201203644","2015-01-11T11:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.235749999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1697,"MURRAYLINKV5_20211201203644","2015-01-11T11:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.2624,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1698,"MURRAYLINKV5_20211201203644","2015-01-11T11:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.095459999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1699,"MURRAYLINKV5_20211201203644","2015-01-11T11:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.803430000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1700,"MURRAYLINKV5_20211201203644","2015-01-11T11:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.12077,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1701,"MURRAYLINKV5_20211201203644","2015-01-11T12:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.19544,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1702,"MURRAYLINKV5_20211201203644","2015-01-11T12:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.004250000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1703,"MURRAYLINKV5_20211201203644","2015-01-11T12:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.31246,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1704,"MURRAYLINKV5_20211201203644","2015-01-11T12:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.606490000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1705,"MURRAYLINKV5_20211201203644","2015-01-11T12:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.615959999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1706,"MURRAYLINKV5_20211201203644","2015-01-11T12:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.37698,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1707,"MURRAYLINKV5_20211201203644","2015-01-11T12:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.55761,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1708,"MURRAYLINKV5_20211201203644","2015-01-11T12:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.51158,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1709,"MURRAYLINKV5_20211201203644","2015-01-11T12:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.51746,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1710,"MURRAYLINKV5_20211201203644","2015-01-11T12:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.51338,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1711,"MURRAYLINKV5_20211201203644","2015-01-11T12:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.19617,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1712,"MURRAYLINKV5_20211201203644","2015-01-11T13:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.046860000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1713,"MURRAYLINKV5_20211201203644","2015-01-11T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.777240000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1714,"MURRAYLINKV5_20211201203644","2015-01-11T13:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.60689,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1715,"MURRAYLINKV5_20211201203644","2015-01-11T15:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.06559,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1716,"MURRAYLINKV5_20211201203644","2015-01-11T15:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.600250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1717,"MURRAYLINKV5_20211201203644","2015-01-12T00:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.54729,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1718,"MURRAYLINKV5_20211201203644","2015-01-12T00:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.4419,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1719,"MURRAYLINKV5_20211201203644","2015-01-12T05:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.012079999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1720,"MURRAYLINKV5_20211201203644","2015-01-12T05:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.055110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1721,"MURRAYLINKV5_20211201203644","2015-01-12T05:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.776249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1722,"MURRAYLINKV5_20211201203644","2015-01-13T00:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.90747,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1723,"MURRAYLINKV5_20211201203644","2015-01-13T00:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.05325,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1724,"MURRAYLINKV5_20211201203644","2015-01-13T05:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.711729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1725,"MURRAYLINKV5_20211201203644","2015-01-13T14:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.019399999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1726,"MURRAYLINKV5_20211201203644","2015-01-13T15:45:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-10.454639999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1727,"MURRAYLINKV5_20211201203644","2015-01-14T00:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.209619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1728,"MURRAYLINKV5_20211201203644","2015-01-14T00:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.85041,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1729,"MURRAYLINKV5_20211201203644","2015-01-15T23:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-16.03772,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1730,"MURRAYLINKV5_20211201203644","2015-01-15T23:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-11.79907,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1731,"MURRAYLINKV5_20211201203644","2015-01-16T13:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.37378,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1732,"MURRAYLINKV5_20211201203644","2015-01-16T14:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.48493,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1733,"MURRAYLINKV5_20211201203644","2015-01-16T14:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-11.392429999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1734,"MURRAYLINKV5_20211201203644","2015-01-16T14:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.932980000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1735,"MURRAYLINKV5_20211201203644","2015-01-16T15:25:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-15.85594,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1736,"MURRAYLINKV5_20211201203644","2015-01-16T17:10:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.774010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1737,"MURRAYLINKV5_20211201203644","2015-01-17T13:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2014-12-18",1,-11.12914,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1738,"MURRAYLINKV5_20211201203644","2015-01-17T13:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2014-12-18",1,-12.26224,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1739,"MURRAYLINKV5_20211201203644","2015-01-17T16:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-12-03",1,-11.57052,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1740,"MURRAYLINKV5_20211201203644","2015-01-17T18:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.18389,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1741,"MURRAYLINKV5_20211201203644","2015-01-17T19:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.29139,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1742,"MURRAYLINKV5_20211201203644","2015-01-17T19:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.646100000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1743,"MURRAYLINKV5_20211201203644","2015-01-17T19:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.28603,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1744,"MURRAYLINKV5_20211201203644","2015-01-17T19:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.39705,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1745,"MURRAYLINKV5_20211201203644","2015-01-17T21:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.152620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1746,"MURRAYLINKV5_20211201203644","2015-01-17T21:40:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.693669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1747,"MURRAYLINKV5_20211201203644","2015-01-17T22:05:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.285069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1748,"MURRAYLINKV5_20211201203644","2015-01-17T22:10:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.211510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1749,"MURRAYLINKV5_20211201203644","2015-01-17T22:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.10636,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1750,"MURRAYLINKV5_20211201203644","2015-01-17T22:40:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.06048,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1751,"MURRAYLINKV5_20211201203644","2015-01-17T23:05:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.63574,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1752,"MURRAYLINKV5_20211201203644","2015-01-17T23:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-01-31",1,-12727.303760000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1753,"MURRAYLINKV5_20211201203644","2015-01-18T00:30:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.305350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1754,"MURRAYLINKV5_20211201203644","2015-01-18T00:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.74672,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1755,"MURRAYLINKV5_20211201203644","2015-01-18T00:40:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.34112,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1756,"MURRAYLINKV5_20211201203644","2015-01-18T09:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.087630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1757,"MURRAYLINKV5_20211201203644","2015-01-18T09:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.454969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1758,"MURRAYLINKV5_20211201203644","2015-01-18T10:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.003119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1759,"MURRAYLINKV5_20211201203644","2015-01-18T10:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.48138,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1760,"MURRAYLINKV5_20211201203644","2015-01-18T10:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.88649,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1761,"MURRAYLINKV5_20211201203644","2015-01-18T12:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.275040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1762,"MURRAYLINKV5_20211201203644","2015-01-18T12:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.053789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1763,"MURRAYLINKV5_20211201203644","2015-01-18T13:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.31475,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1764,"MURRAYLINKV5_20211201203644","2015-01-18T13:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.73691,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1765,"MURRAYLINKV5_20211201203644","2015-01-18T13:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.396190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1766,"MURRAYLINKV5_20211201203644","2015-01-18T13:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.20515,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1767,"MURRAYLINKV5_20211201203644","2015-01-18T13:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.46303,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1768,"MURRAYLINKV5_20211201203644","2015-01-18T13:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.570550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1769,"MURRAYLINKV5_20211201203644","2015-01-18T13:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.49905,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1770,"MURRAYLINKV5_20211201203644","2015-01-18T13:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.13913,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1771,"MURRAYLINKV5_20211201203644","2015-01-18T13:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.31104,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1772,"MURRAYLINKV5_20211201203644","2015-01-18T14:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.84197,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1773,"MURRAYLINKV5_20211201203644","2015-01-18T14:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.2441,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1774,"MURRAYLINKV5_20211201203644","2015-01-18T14:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.857760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1775,"MURRAYLINKV5_20211201203644","2015-01-18T14:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.12297,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1776,"MURRAYLINKV5_20211201203644","2015-01-18T14:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.352029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1777,"MURRAYLINKV5_20211201203644","2015-01-18T15:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.92489,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1778,"MURRAYLINKV5_20211201203644","2015-01-18T15:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.35136,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1779,"MURRAYLINKV5_20211201203644","2015-01-18T15:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.51478,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1780,"MURRAYLINKV5_20211201203644","2015-01-18T15:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.66803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1781,"MURRAYLINKV5_20211201203644","2015-01-18T15:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.54941,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1782,"MURRAYLINKV5_20211201203644","2015-01-18T15:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.50539,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1783,"MURRAYLINKV5_20211201203644","2015-01-18T15:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.04067,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1784,"MURRAYLINKV5_20211201203644","2015-01-18T15:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.27487,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1785,"MURRAYLINKV5_20211201203644","2015-01-19T21:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.03633,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1786,"MURRAYLINKV5_20211201203644","2015-01-19T21:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.628259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1787,"MURRAYLINKV5_20211201203644","2015-01-19T22:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.17318,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1788,"MURRAYLINKV5_20211201203644","2015-01-19T22:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.043810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1789,"MURRAYLINKV5_20211201203644","2015-01-19T22:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.437709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1790,"MURRAYLINKV5_20211201203644","2015-01-19T22:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.05345,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1791,"MURRAYLINKV5_20211201203644","2015-01-19T22:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.797330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1792,"MURRAYLINKV5_20211201203644","2015-01-19T22:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.47039,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1793,"MURRAYLINKV5_20211201203644","2015-01-19T22:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.278359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1794,"MURRAYLINKV5_20211201203644","2015-01-21T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.497249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1795,"MURRAYLINKV5_20211201203644","2015-01-21T22:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.713889999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1796,"MURRAYLINKV5_20211201203644","2015-01-21T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.958769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1797,"MURRAYLINKV5_20211201203644","2015-01-21T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.862590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1798,"MURRAYLINKV5_20211201203644","2015-01-22T00:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.89791,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1799,"MURRAYLINKV5_20211201203644","2015-01-22T00:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.846769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1800,"MURRAYLINKV5_20211201203644","2015-01-22T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.63983,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1801,"MURRAYLINKV5_20211201203644","2015-01-22T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.45561,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1802,"MURRAYLINKV5_20211201203644","2015-01-22T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.61408,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1803,"MURRAYLINKV5_20211201203644","2015-01-22T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.40715,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1804,"MURRAYLINKV5_20211201203644","2015-01-22T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.33944,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1805,"MURRAYLINKV5_20211201203644","2015-01-22T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.324400000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1806,"MURRAYLINKV5_20211201203644","2015-01-22T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.315289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1807,"MURRAYLINKV5_20211201203644","2015-01-22T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.15132,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1808,"MURRAYLINKV5_20211201203644","2015-01-22T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.20025,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1809,"MURRAYLINKV5_20211201203644","2015-01-22T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.12331,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1810,"MURRAYLINKV5_20211201203644","2015-01-22T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.94947,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1811,"MURRAYLINKV5_20211201203644","2015-01-22T01:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.919930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1812,"MURRAYLINKV5_20211201203644","2015-01-22T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.28628,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1813,"MURRAYLINKV5_20211201203644","2015-01-22T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.333069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1814,"MURRAYLINKV5_20211201203644","2015-01-22T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.3489,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1815,"MURRAYLINKV5_20211201203644","2015-01-22T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.36764,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1816,"MURRAYLINKV5_20211201203644","2015-01-22T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.5037,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1817,"MURRAYLINKV5_20211201203644","2015-01-22T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.948130000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1818,"MURRAYLINKV5_20211201203644","2015-01-22T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.00446,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1819,"MURRAYLINKV5_20211201203644","2015-01-22T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.20528,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1820,"MURRAYLINKV5_20211201203644","2015-01-22T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.88701,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1821,"MURRAYLINKV5_20211201203644","2015-01-22T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.207850000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1822,"MURRAYLINKV5_20211201203644","2015-01-22T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.731,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1823,"MURRAYLINKV5_20211201203644","2015-01-22T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.06209,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1824,"MURRAYLINKV5_20211201203644","2015-01-22T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.90785,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1825,"MURRAYLINKV5_20211201203644","2015-01-22T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.252079999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1826,"MURRAYLINKV5_20211201203644","2015-01-22T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.44244,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1827,"MURRAYLINKV5_20211201203644","2015-01-22T05:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.737909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1828,"MURRAYLINKV5_20211201203644","2015-01-22T05:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.31199,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1829,"MURRAYLINKV5_20211201203644","2015-01-22T05:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.498189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1830,"MURRAYLINKV5_20211201203644","2015-01-22T05:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.33634,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1831,"MURRAYLINKV5_20211201203644","2015-01-22T06:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.20407,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1832,"MURRAYLINKV5_20211201203644","2015-01-22T18:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.610580000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1833,"MURRAYLINKV5_20211201203644","2015-01-22T18:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-13.924770000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1834,"MURRAYLINKV5_20211201203644","2015-01-22T18:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-11.8101,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1835,"MURRAYLINKV5_20211201203644","2015-01-22T18:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-11.27589,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1836,"MURRAYLINKV5_20211201203644","2015-01-22T18:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.43205,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1837,"MURRAYLINKV5_20211201203644","2015-01-22T18:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-17.38205,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1838,"MURRAYLINKV5_20211201203644","2015-01-22T19:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-16.80301,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1839,"MURRAYLINKV5_20211201203644","2015-01-22T19:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-28.434799999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1840,"MURRAYLINKV5_20211201203644","2015-01-22T19:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-27.08793,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1841,"MURRAYLINKV5_20211201203644","2015-01-22T19:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-28.434740000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1842,"MURRAYLINKV5_20211201203644","2015-01-22T19:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-28.434740000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1843,"MURRAYLINKV5_20211201203644","2015-01-22T19:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-28.780989999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1844,"MURRAYLINKV5_20211201203644","2015-01-22T19:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-30.723050000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1845,"MURRAYLINKV5_20211201203644","2015-01-22T19:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-29.99344,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1846,"MURRAYLINKV5_20211201203644","2015-01-22T19:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-29.99344,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1847,"MURRAYLINKV5_20211201203644","2015-01-22T19:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-29.99344,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1848,"MURRAYLINKV5_20211201203644","2015-01-22T19:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-27.041149999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1849,"MURRAYLINKV5_20211201203644","2015-01-22T19:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-25.893599999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1850,"MURRAYLINKV5_20211201203644","2015-01-22T20:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-30.745819999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1851,"MURRAYLINKV5_20211201203644","2015-01-22T20:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-15.249610000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1852,"MURRAYLINKV5_20211201203644","2015-01-22T20:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-14.258559999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1853,"MURRAYLINKV5_20211201203644","2015-01-22T20:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-19.276209999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1854,"MURRAYLINKV5_20211201203644","2015-01-22T20:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-20.227779999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1855,"MURRAYLINKV5_20211201203644","2015-01-22T20:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-20.31465,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1856,"MURRAYLINKV5_20211201203644","2015-01-22T21:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-11.806979999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1857,"MURRAYLINKV5_20211201203644","2015-01-23T11:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-39.470700000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1858,"MURRAYLINKV5_20211201203644","2015-01-23T11:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-34.23413,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1859,"MURRAYLINKV5_20211201203644","2015-01-23T11:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.731560000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1860,"MURRAYLINKV5_20211201203644","2015-01-23T11:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.731560000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1861,"MURRAYLINKV5_20211201203644","2015-01-23T11:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-33.478870000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1862,"MURRAYLINKV5_20211201203644","2015-01-23T12:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-41.305680000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1863,"MURRAYLINKV5_20211201203644","2015-01-23T12:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.731560000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1864,"MURRAYLINKV5_20211201203644","2015-01-23T12:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.751730000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1865,"MURRAYLINKV5_20211201203644","2015-01-23T12:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.504860000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1866,"MURRAYLINKV5_20211201203644","2015-01-23T12:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.814480000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1867,"MURRAYLINKV5_20211201203644","2015-01-23T12:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.683210000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1868,"MURRAYLINKV5_20211201203644","2015-01-23T12:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.714910000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1869,"MURRAYLINKV5_20211201203644","2015-01-23T12:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-43.875909999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1870,"MURRAYLINKV5_20211201203644","2015-01-23T12:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-51.359270000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1871,"MURRAYLINKV5_20211201203644","2015-01-23T12:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-44.193640000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1872,"MURRAYLINKV5_20211201203644","2015-01-23T12:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-50.93976,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1873,"MURRAYLINKV5_20211201203644","2015-01-23T12:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-44.678800000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1874,"MURRAYLINKV5_20211201203644","2015-01-23T13:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-46.768169999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1875,"MURRAYLINKV5_20211201203644","2015-01-23T13:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-44.671590000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1876,"MURRAYLINKV5_20211201203644","2015-01-23T13:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-50.892659999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1877,"MURRAYLINKV5_20211201203644","2015-01-23T13:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-50.191600000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1878,"MURRAYLINKV5_20211201203644","2015-01-23T13:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-56.156649999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1879,"MURRAYLINKV5_20211201203644","2015-01-23T13:25:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-54.361620000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1880,"MURRAYLINKV5_20211201203644","2015-01-23T13:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-51.146749999999997,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1881,"MURRAYLINKV5_20211201203644","2015-01-23T13:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-55.121850000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1882,"MURRAYLINKV5_20211201203644","2015-01-23T13:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-50.561860000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1883,"MURRAYLINKV5_20211201203644","2015-01-23T13:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-55.745939999999997,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1884,"MURRAYLINKV5_20211201203644","2015-01-23T13:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-55.36683,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1885,"MURRAYLINKV5_20211201203644","2015-01-23T13:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-53.112389999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1886,"MURRAYLINKV5_20211201203644","2015-01-23T14:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-55.317340000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1887,"MURRAYLINKV5_20211201203644","2015-01-23T14:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-46.516800000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1888,"MURRAYLINKV5_20211201203644","2015-01-23T14:10:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.097439999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1889,"MURRAYLINKV5_20211201203644","2015-01-23T14:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-49.581910000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1890,"MURRAYLINKV5_20211201203644","2015-01-23T14:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.504429999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1891,"MURRAYLINKV5_20211201203644","2015-01-23T15:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-500.81056000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1892,"MURRAYLINKV5_20211201203644","2015-01-23T15:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-479.01251000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1893,"MURRAYLINKV5_20211201203644","2015-01-23T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-46.93018,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1894,"MURRAYLINKV5_20211201203644","2015-01-23T15:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-24.357410000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1895,"MURRAYLINKV5_20211201203644","2015-01-23T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-48.015279999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1896,"MURRAYLINKV5_20211201203644","2015-01-23T15:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.649990000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1897,"MURRAYLINKV5_20211201203644","2015-01-23T15:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-82.518370000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1898,"MURRAYLINKV5_20211201203644","2015-01-23T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-126.53505,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1899,"MURRAYLINKV5_20211201203644","2015-01-23T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-84.416449999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1900,"MURRAYLINKV5_20211201203644","2015-01-23T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-128.73475999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1901,"MURRAYLINKV5_20211201203644","2015-01-23T15:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-111.47163,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1902,"MURRAYLINKV5_20211201203644","2015-01-23T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-156.87519,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1903,"MURRAYLINKV5_20211201203644","2015-01-23T15:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-109.56582,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1904,"MURRAYLINKV5_20211201203644","2015-01-23T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-156.49222,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1905,"MURRAYLINKV5_20211201203644","2015-01-23T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.859489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1906,"MURRAYLINKV5_20211201203644","2015-01-23T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.323090000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1907,"MURRAYLINKV5_20211201203644","2015-01-23T15:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-66.511430000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1908,"MURRAYLINKV5_20211201203644","2015-01-23T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-104.65640999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1909,"MURRAYLINKV5_20211201203644","2015-01-23T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-22.803159999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1910,"MURRAYLINKV5_20211201203644","2015-01-23T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-22.83718,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1911,"MURRAYLINKV5_20211201203644","2015-01-23T16:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-62.986629999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1912,"MURRAYLINKV5_20211201203644","2015-01-23T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-102.05228,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1913,"MURRAYLINKV5_20211201203644","2015-01-23T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.63359,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1914,"MURRAYLINKV5_20211201203644","2015-01-23T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-15.030250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1915,"MURRAYLINKV5_20211201203644","2015-01-23T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.27913,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1916,"MURRAYLINKV5_20211201203644","2015-01-23T16:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-254.43444,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1917,"MURRAYLINKV5_20211201203644","2015-01-23T16:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-259.21627000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1918,"MURRAYLINKV5_20211201203644","2015-01-23T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.111039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1919,"MURRAYLINKV5_20211201203644","2015-01-24T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.027609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1920,"MURRAYLINKV5_20211201203644","2015-01-24T03:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.428879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1921,"MURRAYLINKV5_20211201203644","2015-01-24T06:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.99094,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1922,"MURRAYLINKV5_20211201203644","2015-01-24T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.825799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1923,"MURRAYLINKV5_20211201203644","2015-01-24T06:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.8621,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1924,"MURRAYLINKV5_20211201203644","2015-01-24T06:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.05626,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1925,"MURRAYLINKV5_20211201203644","2015-01-24T06:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.07883,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1926,"MURRAYLINKV5_20211201203644","2015-01-24T06:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.884209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1927,"MURRAYLINKV5_20211201203644","2015-01-24T06:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.090109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1928,"MURRAYLINKV5_20211201203644","2015-01-24T06:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.50033,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1929,"MURRAYLINKV5_20211201203644","2015-01-24T06:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.317349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1930,"MURRAYLINKV5_20211201203644","2015-01-24T06:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.47467,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1931,"MURRAYLINKV5_20211201203644","2015-01-24T07:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.60069,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1932,"MURRAYLINKV5_20211201203644","2015-01-24T07:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.477259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1933,"MURRAYLINKV5_20211201203644","2015-01-24T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.33783,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1934,"MURRAYLINKV5_20211201203644","2015-01-24T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.245900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1935,"MURRAYLINKV5_20211201203644","2015-01-24T07:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.796580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1936,"MURRAYLINKV5_20211201203644","2015-01-24T07:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.56549,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1937,"MURRAYLINKV5_20211201203644","2015-01-24T07:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.101389999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1938,"MURRAYLINKV5_20211201203644","2015-01-24T07:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.845099999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1939,"MURRAYLINKV5_20211201203644","2015-01-24T07:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.36219,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1940,"MURRAYLINKV5_20211201203644","2015-01-24T07:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.333069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1941,"MURRAYLINKV5_20211201203644","2015-01-24T07:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.152729999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1942,"MURRAYLINKV5_20211201203644","2015-01-24T07:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.94792,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1943,"MURRAYLINKV5_20211201203644","2015-01-24T08:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.186779999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1944,"MURRAYLINKV5_20211201203644","2015-01-24T08:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.70224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1945,"MURRAYLINKV5_20211201203644","2015-01-24T08:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.554919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1946,"MURRAYLINKV5_20211201203644","2015-01-24T08:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.873609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1947,"MURRAYLINKV5_20211201203644","2015-01-24T08:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.83512,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1948,"MURRAYLINKV5_20211201203644","2015-01-24T09:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-22.611750000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1949,"MURRAYLINKV5_20211201203644","2015-01-24T09:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-21.52366,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1950,"MURRAYLINKV5_20211201203644","2015-01-24T09:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.06183,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1951,"MURRAYLINKV5_20211201203644","2015-01-24T09:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.91038,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1952,"MURRAYLINKV5_20211201203644","2015-01-24T09:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.056139999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1953,"MURRAYLINKV5_20211201203644","2015-01-24T09:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.003350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1954,"MURRAYLINKV5_20211201203644","2015-01-24T09:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.726929999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1955,"MURRAYLINKV5_20211201203644","2015-01-24T09:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.758410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1956,"MURRAYLINKV5_20211201203644","2015-01-24T09:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.162939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1957,"MURRAYLINKV5_20211201203644","2015-01-24T09:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.32912,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1958,"MURRAYLINKV5_20211201203644","2015-01-24T09:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.96434,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1959,"MURRAYLINKV5_20211201203644","2015-01-24T09:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.145040000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1960,"MURRAYLINKV5_20211201203644","2015-01-24T10:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.927099999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1961,"MURRAYLINKV5_20211201203644","2015-01-24T10:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.11253,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1962,"MURRAYLINKV5_20211201203644","2015-01-24T10:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.077400000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1963,"MURRAYLINKV5_20211201203644","2015-01-24T10:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.111190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1964,"MURRAYLINKV5_20211201203644","2015-01-24T10:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.932490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1965,"MURRAYLINKV5_20211201203644","2015-01-24T10:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.787430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1966,"MURRAYLINKV5_20211201203644","2015-01-24T10:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.53321,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1967,"MURRAYLINKV5_20211201203644","2015-01-24T10:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.18234,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1968,"MURRAYLINKV5_20211201203644","2015-01-24T10:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.05218,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1969,"MURRAYLINKV5_20211201203644","2015-01-24T10:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.62632,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1970,"MURRAYLINKV5_20211201203644","2015-01-24T11:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.193300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1971,"MURRAYLINKV5_20211201203644","2015-01-24T11:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.176670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1972,"MURRAYLINKV5_20211201203644","2015-01-24T11:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.017480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1973,"MURRAYLINKV5_20211201203644","2015-01-24T11:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.624599999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1974,"MURRAYLINKV5_20211201203644","2015-01-24T11:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.07931,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1975,"MURRAYLINKV5_20211201203644","2015-01-24T11:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.707380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1976,"MURRAYLINKV5_20211201203644","2015-01-24T12:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.55213,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1977,"MURRAYLINKV5_20211201203644","2015-01-24T13:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.32526,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1978,"MURRAYLINKV5_20211201203644","2015-01-24T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.17638,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1979,"MURRAYLINKV5_20211201203644","2015-01-24T13:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.199529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1980,"MURRAYLINKV5_20211201203644","2015-01-24T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.13635,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1981,"MURRAYLINKV5_20211201203644","2015-01-24T14:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.231210000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1982,"MURRAYLINKV5_20211201203644","2015-01-24T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.73155,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1983,"MURRAYLINKV5_20211201203644","2015-01-24T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.75099,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1984,"MURRAYLINKV5_20211201203644","2015-01-24T15:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-66.549750000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1985,"MURRAYLINKV5_20211201203644","2015-01-24T15:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-68.969089999999994,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1986,"MURRAYLINKV5_20211201203644","2015-01-24T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.06742,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1987,"MURRAYLINKV5_20211201203644","2015-01-24T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.8089,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1988,"MURRAYLINKV5_20211201203644","2015-01-24T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.62331,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1989,"MURRAYLINKV5_20211201203644","2015-01-24T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.63551,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1990,"MURRAYLINKV5_20211201203644","2015-01-24T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.89547,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1991,"MURRAYLINKV5_20211201203644","2015-01-24T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.82673,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1992,"MURRAYLINKV5_20211201203644","2015-01-24T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.878550000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1993,"MURRAYLINKV5_20211201203644","2015-01-24T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.898160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1994,"MURRAYLINKV5_20211201203644","2015-01-24T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.09253,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1995,"MURRAYLINKV5_20211201203644","2015-01-24T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.3931,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1996,"MURRAYLINKV5_20211201203644","2015-01-24T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.61933,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1997,"MURRAYLINKV5_20211201203644","2015-01-24T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.85717,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1998,"MURRAYLINKV5_20211201203644","2015-01-24T16:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.31714,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[1999,"MURRAYLINKV5_20211201203644","2015-01-24T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.794840000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2001,"MURRAYLINKV5_20211201203644","2015-01-24T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-15.539260000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2010,"MURRAYLINKV5_20211201203644","2015-01-24T17:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.135059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2023,"MURRAYLINKV5_20211201203644","2015-01-24T18:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-22.412310000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2029,"MURRAYLINKV5_20211201203644","2015-01-24T19:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.000959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2041,"MURRAYLINKV5_20211201203644","2015-01-24T20:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.324009999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2048,"MURRAYLINKV5_20211201203644","2015-01-24T20:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.136520000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2050,"MURRAYLINKV5_20211201203644","2015-01-24T20:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.084849999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2059,"MURRAYLINKV5_20211201203644","2015-01-24T23:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.14283,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2068,"MURRAYLINKV5_20211201203644","2015-01-25T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.92587,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2078,"MURRAYLINKV5_20211201203644","2015-01-25T10:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-15.738200000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2091,"MURRAYLINKV5_20211201203644","2015-01-25T11:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-22.427759999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2097,"MURRAYLINKV5_20211201203644","2015-01-25T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-35.642189999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2109,"MURRAYLINKV5_20211201203644","2015-01-25T13:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.715590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2116,"MURRAYLINKV5_20211201203644","2015-01-25T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.99052,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2125,"MURRAYLINKV5_20211201203644","2015-01-25T14:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.228960000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2129,"MURRAYLINKV5_20211201203644","2015-01-25T14:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-36.329500000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2136,"MURRAYLINKV5_20211201203644","2015-01-25T14:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-12.10183,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2147,"MURRAYLINKV5_20211201203644","2015-01-25T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-17.022970000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2155,"MURRAYLINKV5_20211201203644","2015-01-25T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.805249999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2165,"MURRAYLINKV5_20211201203644","2015-01-25T17:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-14.621980000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2174,"MURRAYLINKV5_20211201203644","2015-01-25T19:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.6625,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2183,"MURRAYLINKV5_20211201203644","2015-01-25T20:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.520020000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2193,"MURRAYLINKV5_20211201203644","2015-01-26T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.70002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2197,"MURRAYLINKV5_20211201203644","2015-01-26T14:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.18384,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2204,"MURRAYLINKV5_20211201203644","2015-01-26T15:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.27345,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2215,"MURRAYLINKV5_20211201203644","2015-01-26T16:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.145899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2223,"MURRAYLINKV5_20211201203644","2015-01-26T17:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.388299999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2232,"MURRAYLINKV5_20211201203644","2015-01-26T18:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.62227,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2244,"MURRAYLINKV5_20211201203644","2015-01-26T19:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.690989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2251,"MURRAYLINKV5_20211201203644","2015-01-26T20:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.535729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2253,"MURRAYLINKV5_20211201203644","2015-01-26T20:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.49034,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2262,"MURRAYLINKV5_20211201203644","2015-01-27T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.216089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2271,"MURRAYLINKV5_20211201203644","2015-01-27T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.18601,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2281,"MURRAYLINKV5_20211201203644","2015-01-28T02:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.19699,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2294,"MURRAYLINKV5_20211201203644","2015-01-28T02:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-30.48376,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2300,"MURRAYLINKV5_20211201203644","2015-01-28T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.97189,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2312,"MURRAYLINKV5_20211201203644","2015-01-29T06:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.31532,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2319,"MURRAYLINKV5_20211201203644","2015-01-29T13:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.2561,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2321,"MURRAYLINKV5_20211201203644","2015-01-29T13:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.235139999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2330,"MURRAYLINKV5_20211201203644","2015-01-29T20:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.74457,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2339,"MURRAYLINKV5_20211201203644","2015-01-30T14:50:00","V::N_NIL_S4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.14156,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2349,"MURRAYLINKV5_20211201203644","2015-01-30T21:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.13782,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2358,"MURRAYLINKV5_20211201203644","2015-02-02T21:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.454829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2368,"MURRAYLINKV5_20211201203644","2015-02-03T05:25:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-15.265040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2377,"MURRAYLINKV5_20211201203644","2015-02-03T21:45:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-12.629860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2386,"MURRAYLINKV5_20211201203644","2015-02-03T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.911910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2396,"MURRAYLINKV5_20211201203644","2015-02-03T23:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.58385,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2400,"MURRAYLINKV5_20211201203644","2015-02-03T23:50:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-13.375920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2407,"MURRAYLINKV5_20211201203644","2015-02-04T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.711930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2418,"MURRAYLINKV5_20211201203644","2015-02-04T05:15:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-14.415469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2426,"MURRAYLINKV5_20211201203644","2015-02-04T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.262119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2436,"MURRAYLINKV5_20211201203644","2015-02-05T01:05:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-12.17296,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2445,"MURRAYLINKV5_20211201203644","2015-02-05T04:50:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-14.07653,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2454,"MURRAYLINKV5_20211201203644","2015-02-05T15:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-14.57606,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2464,"MURRAYLINKV5_20211201203644","2015-02-06T17:05:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-15.51914,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2465,"MURRAYLINKV5_20211201203644","2015-02-06T17:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-16.236740000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2474,"MURRAYLINKV5_20211201203644","2015-02-06T18:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-13.75909,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2484,"MURRAYLINKV5_20211201203644","2015-02-07T01:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.475849999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2492,"MURRAYLINKV5_20211201203644","2015-02-07T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.88923,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2503,"MURRAYLINKV5_20211201203644","2015-02-07T14:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.734489999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2515,"MURRAYLINKV5_20211201203644","2015-02-07T17:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.912419999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2522,"MURRAYLINKV5_20211201203644","2015-02-07T17:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-32.204389999999997,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2524,"MURRAYLINKV5_20211201203644","2015-02-07T18:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-31.758109999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2533,"MURRAYLINKV5_20211201203644","2015-02-08T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.20443,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2542,"MURRAYLINKV5_20211201203644","2015-02-08T07:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.675319999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2552,"MURRAYLINKV5_20211201203644","2015-02-08T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.568199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2560,"MURRAYLINKV5_20211201203644","2015-02-08T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.067550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2571,"MURRAYLINKV5_20211201203644","2015-02-08T23:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.0816,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2583,"MURRAYLINKV5_20211201203644","2015-02-09T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.89461,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2590,"MURRAYLINKV5_20211201203644","2015-02-09T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.87209,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2599,"MURRAYLINKV5_20211201203644","2015-02-09T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.9109,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2607,"MURRAYLINKV5_20211201203644","2015-02-10T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.409610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2610,"MURRAYLINKV5_20211201203644","2015-02-10T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.008800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2621,"MURRAYLINKV5_20211201203644","2015-02-11T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.629670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2629,"MURRAYLINKV5_20211201203644","2015-02-11T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.250500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2639,"MURRAYLINKV5_20211201203644","2015-02-11T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.188829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2648,"MURRAYLINKV5_20211201203644","2015-02-11T14:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-39.404710000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2657,"MURRAYLINKV5_20211201203644","2015-02-11T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3162.7605400000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2667,"MURRAYLINKV5_20211201203644","2015-02-11T15:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-3184.8947199999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2675,"MURRAYLINKV5_20211201203644","2015-02-11T16:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2650.0134400000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2678,"MURRAYLINKV5_20211201203644","2015-02-11T16:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-966.57412999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2689,"MURRAYLINKV5_20211201203644","2015-02-11T16:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-178.76123999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2697,"MURRAYLINKV5_20211201203644","2015-02-11T17:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-514.23465999999996,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2706,"MURRAYLINKV5_20211201203644","2015-02-11T17:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-737.36519999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2713,"MURRAYLINKV5_20211201203644","2015-02-11T19:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.09957,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2725,"MURRAYLINKV5_20211201203644","2015-02-11T21:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.4008,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2727,"MURRAYLINKV5_20211201203644","2015-02-11T23:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-10.387359999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2736,"MURRAYLINKV5_20211201203644","2015-02-12T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.21749,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2745,"MURRAYLINKV5_20211201203644","2015-02-12T13:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-15.580360000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2755,"MURRAYLINKV5_20211201203644","2015-02-12T14:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-18.540579999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2763,"MURRAYLINKV5_20211201203644","2015-02-12T14:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-27.624169999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2774,"MURRAYLINKV5_20211201203644","2015-02-12T15:35:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-26.03745,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2781,"MURRAYLINKV5_20211201203644","2015-02-12T16:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-38.308970000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2793,"MURRAYLINKV5_20211201203644","2015-02-12T17:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-27.517219999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2795,"MURRAYLINKV5_20211201203644","2015-02-12T17:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-25.23479,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2804,"MURRAYLINKV5_20211201203644","2015-02-12T18:05:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-35.427169999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2813,"MURRAYLINKV5_20211201203644","2015-02-12T18:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-23.307780000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2823,"MURRAYLINKV5_20211201203644","2015-02-12T19:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-33.90061,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2832,"MURRAYLINKV5_20211201203644","2015-02-12T21:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.306330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2842,"MURRAYLINKV5_20211201203644","2015-02-12T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.772040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2851,"MURRAYLINKV5_20211201203644","2015-02-12T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.45013,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2860,"MURRAYLINKV5_20211201203644","2015-02-12T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.88359,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2870,"MURRAYLINKV5_20211201203644","2015-02-13T05:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-15.689249999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2878,"MURRAYLINKV5_20211201203644","2015-02-13T06:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.069879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2881,"MURRAYLINKV5_20211201203644","2015-02-13T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.568619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2896,"MURRAYLINKV5_20211201203644","2015-02-13T11:40:00","V::N_HYMLQE_R","V-HYML;V-HYML_P;V-HYML_R;V-HYMO;V-HYTR;V-HY_MO_ML;V-MLMO;V-MLTR","2013-08-21",1,-10.20317,"Out = one 500 kV line between Heywood and Moorabool, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2900,"MURRAYLINKV5_20211201203644","2015-02-13T15:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-14.69027,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2910,"MURRAYLINKV5_20211201203644","2015-02-13T23:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-102.07106,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2919,"MURRAYLINKV5_20211201203644","2015-02-13T23:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-118.19646,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2928,"MURRAYLINKV5_20211201203644","2015-02-14T07:45:00","V::N_DDSM_V4","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2014-02-21",1,-11.58536,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2938,"MURRAYLINKV5_20211201203644","2015-02-14T08:35:00","V::N_DDSM_V4","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2014-02-21",1,-12.905620000000001,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2939,"MURRAYLINKV5_20211201203644","2015-02-14T08:40:00","V::N_DDSM_V4","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2014-02-21",1,-12.90569,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2948,"MURRAYLINKV5_20211201203644","2015-02-14T14:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-17.257000000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2958,"MURRAYLINKV5_20211201203644","2015-02-14T16:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-26.785589999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2966,"MURRAYLINKV5_20211201203644","2015-02-14T17:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-18.513490000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2977,"MURRAYLINKV5_20211201203644","2015-02-14T18:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-34.978259999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2984,"MURRAYLINKV5_20211201203644","2015-02-14T20:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.973039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[2996,"MURRAYLINKV5_20211201203644","2015-02-14T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.04341,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3002,"MURRAYLINKV5_20211201203644","2015-02-14T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.809559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3007,"MURRAYLINKV5_20211201203644","2015-02-14T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.68516,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3016,"MURRAYLINKV5_20211201203644","2015-02-15T08:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.459680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3026,"MURRAYLINKV5_20211201203644","2015-02-15T09:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.48969,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3034,"MURRAYLINKV5_20211201203644","2015-02-15T10:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.12116,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3045,"MURRAYLINKV5_20211201203644","2015-02-15T11:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.372399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3052,"MURRAYLINKV5_20211201203644","2015-02-15T14:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-10.204560000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3064,"MURRAYLINKV5_20211201203644","2015-02-15T16:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-18.23366,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3073,"MURRAYLINKV5_20211201203644","2015-02-15T16:55:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-432.74243000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3081,"MURRAYLINKV5_20211201203644","2015-02-15T17:15:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-2573.2305700000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3084,"MURRAYLINKV5_20211201203644","2015-02-15T17:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-2874.7660500000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3099,"MURRAYLINKV5_20211201203644","2015-02-15T17:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-27.332280000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3103,"MURRAYLINKV5_20211201203644","2015-02-15T18:00:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-450.29489000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3108,"MURRAYLINKV5_20211201203644","2015-02-15T18:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-443.15442000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3122,"MURRAYLINKV5_20211201203644","2015-02-15T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.275359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3131,"MURRAYLINKV5_20211201203644","2015-02-15T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.8779,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3141,"MURRAYLINKV5_20211201203644","2015-02-16T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.84421,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3149,"MURRAYLINKV5_20211201203644","2015-02-16T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.7639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3152,"MURRAYLINKV5_20211201203644","2015-02-16T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.18638,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3167,"MURRAYLINKV5_20211201203644","2015-02-16T02:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.375590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3171,"MURRAYLINKV5_20211201203644","2015-02-16T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.42113,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3180,"MURRAYLINKV5_20211201203644","2015-02-16T03:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.415459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3187,"MURRAYLINKV5_20211201203644","2015-02-16T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.33512,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3199,"MURRAYLINKV5_20211201203644","2015-02-16T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-27.73987,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3205,"MURRAYLINKV5_20211201203644","2015-02-16T06:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.698630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3210,"MURRAYLINKV5_20211201203644","2015-02-16T14:05:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-27.87519,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3223,"MURRAYLINKV5_20211201203644","2015-02-17T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.296709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3229,"MURRAYLINKV5_20211201203644","2015-02-17T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.148009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3237,"MURRAYLINKV5_20211201203644","2015-02-17T01:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.391730000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3248,"MURRAYLINKV5_20211201203644","2015-02-17T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.45917,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3255,"MURRAYLINKV5_20211201203644","2015-02-17T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.54017,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3267,"MURRAYLINKV5_20211201203644","2015-02-17T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.15964,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3273,"MURRAYLINKV5_20211201203644","2015-02-17T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.612539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3278,"MURRAYLINKV5_20211201203644","2015-02-17T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-26.356290000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3287,"MURRAYLINKV5_20211201203644","2015-02-17T12:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-34.233939999999997,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3302,"MURRAYLINKV5_20211201203644","2015-02-17T15:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-33.496920000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3306,"MURRAYLINKV5_20211201203644","2015-02-17T15:55:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-34.233939999999997,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3311,"MURRAYLINKV5_20211201203644","2015-02-17T16:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-40.731369999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3325,"MURRAYLINKV5_20211201203644","2015-02-17T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.411390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3334,"MURRAYLINKV5_20211201203644","2015-02-17T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.361420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3344,"MURRAYLINKV5_20211201203644","2015-02-18T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.7758,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3352,"MURRAYLINKV5_20211201203644","2015-02-18T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.51967,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3355,"MURRAYLINKV5_20211201203644","2015-02-18T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.34815,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3370,"MURRAYLINKV5_20211201203644","2015-02-18T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.261189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3374,"MURRAYLINKV5_20211201203644","2015-02-18T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.11876,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3379,"MURRAYLINKV5_20211201203644","2015-02-18T14:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-41.835940000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3393,"MURRAYLINKV5_20211201203644","2015-02-18T17:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-23.07938,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3397,"MURRAYLINKV5_20211201203644","2015-02-18T18:00:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-22.977889999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3412,"MURRAYLINKV5_20211201203644","2015-02-18T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.490869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3413,"MURRAYLINKV5_20211201203644","2015-02-18T23:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.815160000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3426,"MURRAYLINKV5_20211201203644","2015-02-19T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.359209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3432,"MURRAYLINKV5_20211201203644","2015-02-19T01:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.7821,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3440,"MURRAYLINKV5_20211201203644","2015-02-19T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.18023,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3451,"MURRAYLINKV5_20211201203644","2015-02-19T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.94271,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3458,"MURRAYLINKV5_20211201203644","2015-02-19T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.94267,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3470,"MURRAYLINKV5_20211201203644","2015-02-19T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.1356,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3476,"MURRAYLINKV5_20211201203644","2015-02-19T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.42775,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3481,"MURRAYLINKV5_20211201203644","2015-02-19T16:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-153.10470000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3494,"MURRAYLINKV5_20211201203644","2015-02-19T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-250.92140000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3500,"MURRAYLINKV5_20211201203644","2015-02-19T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-153.51961,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3508,"MURRAYLINKV5_20211201203644","2015-02-19T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-146.88019,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3519,"MURRAYLINKV5_20211201203644","2015-02-19T23:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.576840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3528,"MURRAYLINKV5_20211201203644","2015-02-20T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.650589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3532,"MURRAYLINKV5_20211201203644","2015-02-20T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.161390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3547,"MURRAYLINKV5_20211201203644","2015-02-20T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.20241,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3555,"MURRAYLINKV5_20211201203644","2015-02-20T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.69624,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3558,"MURRAYLINKV5_20211201203644","2015-02-20T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.714119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3573,"MURRAYLINKV5_20211201203644","2015-02-20T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.63049,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3577,"MURRAYLINKV5_20211201203644","2015-02-20T04:45:00","#R011888_006_RAMP_V","#R011888_RAMP","2015-02-19",1,-17.730429999999998,"Soft Ramping constraint for constraint V::N_MLTR_Q4, Effective Date: 16/02/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[3582,"MURRAYLINKV5_20211201203644","2015-02-20T05:05:00","#R011888_006_RAMP_F","#R011888_RAMP","2015-02-19",1,-26.768529999999998,"Hard Ramping constraint for constraint V::N_MLTR_Q4, Effective Date: 16/02/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[3596,"MURRAYLINKV5_20211201203644","2015-02-20T13:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-262.06259,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3600,"MURRAYLINKV5_20211201203644","2015-02-20T15:30:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-14.04049,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3615,"MURRAYLINKV5_20211201203644","2015-02-21T00:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.683450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3623,"MURRAYLINKV5_20211201203644","2015-02-21T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.400029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3626,"MURRAYLINKV5_20211201203644","2015-02-21T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.143319999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3641,"MURRAYLINKV5_20211201203644","2015-02-21T08:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.8401,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3645,"MURRAYLINKV5_20211201203644","2015-02-21T08:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.599900000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3654,"MURRAYLINKV5_20211201203644","2015-02-21T15:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-161.42278999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3661,"MURRAYLINKV5_20211201203644","2015-02-21T16:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-183.32616999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3673,"MURRAYLINKV5_20211201203644","2015-02-21T17:10:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-175.16451000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3679,"MURRAYLINKV5_20211201203644","2015-02-21T17:50:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-13.872909999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3684,"MURRAYLINKV5_20211201203644","2015-02-22T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.163449999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3697,"MURRAYLINKV5_20211201203644","2015-02-22T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.216939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3703,"MURRAYLINKV5_20211201203644","2015-02-22T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.458130000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3715,"MURRAYLINKV5_20211201203644","2015-02-22T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.25196,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3722,"MURRAYLINKV5_20211201203644","2015-02-22T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.590949999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3729,"MURRAYLINKV5_20211201203644","2015-02-22T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.827170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3741,"MURRAYLINKV5_20211201203644","2015-02-22T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.1883,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3747,"MURRAYLINKV5_20211201203644","2015-02-22T07:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.86547,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3752,"MURRAYLINKV5_20211201203644","2015-02-22T16:10:00","V>>V_NIL_8","V-NIL","2015-01-21",1,-66.877340000000004,"Out = Nil, avoid O/L DDTS to WOTS 330kV line for trip of LowerTumut-Wagga (051) + 970,990,99M ex_Yass lines; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3761,"MURRAYLINKV5_20211201203644","2015-02-22T16:50:00","V>>V_NIL_8","V-NIL","2015-01-21",1,-82.021900000000002,"Out = Nil, avoid O/L DDTS to WOTS 330kV line for trip of LowerTumut-Wagga (051) + 970,990,99M ex_Yass lines; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3776,"MURRAYLINKV5_20211201203644","2015-02-22T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2013-08-21",1,-250.15549999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3780,"MURRAYLINKV5_20211201203644","2015-02-22T18:20:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-258.10275000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3785,"MURRAYLINKV5_20211201203644","2015-02-22T18:40:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-264.92367999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3799,"MURRAYLINKV5_20211201203644","2015-02-23T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.162000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3803,"MURRAYLINKV5_20211201203644","2015-02-23T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.27351,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3818,"MURRAYLINKV5_20211201203644","2015-02-27T16:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-11.26197,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3821,"MURRAYLINKV5_20211201203644","2015-02-27T16:45:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-12.264709999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3829,"MURRAYLINKV5_20211201203644","2015-02-27T17:25:00","V>>SML_NIL_7A","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-22",1,-23.32347,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3844,"MURRAYLINKV5_20211201203644","2015-03-03T05:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-12.915800000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3848,"MURRAYLINKV5_20211201203644","2015-03-03T06:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.491709999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3853,"MURRAYLINKV5_20211201203644","2015-03-03T06:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.37265,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3867,"MURRAYLINKV5_20211201203644","2015-03-05T02:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2014-06-11",1,-13.886279999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3871,"MURRAYLINKV5_20211201203644","2015-03-06T00:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.964549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3886,"MURRAYLINKV5_20211201203644","2015-03-07T01:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.1,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3887,"MURRAYLINKV5_20211201203644","2015-03-07T01:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.24352,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3900,"MURRAYLINKV5_20211201203644","2015-03-07T05:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.12804,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3906,"MURRAYLINKV5_20211201203644","2015-03-07T15:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.56817,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3918,"MURRAYLINKV5_20211201203644","2015-03-07T20:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.89368,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3925,"MURRAYLINKV5_20211201203644","2015-03-07T20:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.498249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3936,"MURRAYLINKV5_20211201203644","2015-03-07T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.73371,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3944,"MURRAYLINKV5_20211201203644","2015-03-07T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.25184,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3950,"MURRAYLINKV5_20211201203644","2015-03-07T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.00573,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3955,"MURRAYLINKV5_20211201203644","2015-03-07T23:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.22803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3968,"MURRAYLINKV5_20211201203644","2015-03-08T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.46571,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3974,"MURRAYLINKV5_20211201203644","2015-03-08T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.727679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3986,"MURRAYLINKV5_20211201203644","2015-03-08T07:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.01215,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[3993,"MURRAYLINKV5_20211201203644","2015-03-08T08:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.94232,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4002,"MURRAYLINKV5_20211201203644","2015-03-08T08:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.412459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4006,"MURRAYLINKV5_20211201203644","2015-03-08T09:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.81804,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4021,"MURRAYLINKV5_20211201203644","2015-03-08T17:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.989739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4024,"MURRAYLINKV5_20211201203644","2015-03-08T19:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.70759,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4032,"MURRAYLINKV5_20211201203644","2015-03-08T23:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.045500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4042,"MURRAYLINKV5_20211201203644","2015-03-09T03:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.13575,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4051,"MURRAYLINKV5_20211201203644","2015-03-09T05:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.22029,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4056,"MURRAYLINKV5_20211201203644","2015-03-09T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.00811,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4070,"MURRAYLINKV5_20211201203644","2015-03-09T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.85229,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4074,"MURRAYLINKV5_20211201203644","2015-03-09T07:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.170450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4089,"MURRAYLINKV5_20211201203644","2015-03-09T08:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.191739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4092,"MURRAYLINKV5_20211201203644","2015-03-09T14:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.93623,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4100,"MURRAYLINKV5_20211201203644","2015-03-09T21:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.24616,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4110,"MURRAYLINKV5_20211201203644","2015-03-10T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.08466,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4119,"MURRAYLINKV5_20211201203644","2015-03-10T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.75808,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4128,"MURRAYLINKV5_20211201203644","2015-03-11T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.748239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4139,"MURRAYLINKV5_20211201203644","2015-03-11T14:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2014-12-18",1,-19.065899999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4147,"MURRAYLINKV5_20211201203644","2015-03-12T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.207929999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4157,"MURRAYLINKV5_20211201203644","2015-03-14T00:40:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.14026,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4158,"MURRAYLINKV5_20211201203644","2015-03-14T00:45:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.52455,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4171,"MURRAYLINKV5_20211201203644","2015-03-16T06:40:00","V::N_ROSMQE_R","V-ROSM_R;V-X_MLTX+RO-SM-KT_R","2013-08-21",1,-11.85955,"Out = Rowville to South Morang 500kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4177,"MURRAYLINKV5_20211201203644","2015-03-16T08:55:00","V::N_ROSMQE_R","V-ROSM_R;V-X_MLTX+RO-SM-KT_R","2013-08-21",1,-11.84206,"Out = Rowville to South Morang 500kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4189,"MURRAYLINKV5_20211201203644","2015-03-17T12:25:00","S>V_NWRB2_RBNW1","S-NWRB2","2014-02-18",1,-45.595179999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4196,"MURRAYLINKV5_20211201203644","2015-03-17T13:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-16",1,-44.712890000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4207,"MURRAYLINKV5_20211201203644","2015-03-17T14:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2014-02-18",1,-47.541040000000002,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4215,"MURRAYLINKV5_20211201203644","2015-03-19T03:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-16",1,-43.461379999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4225,"MURRAYLINKV5_20211201203644","2015-03-22T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.136329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4226,"MURRAYLINKV5_20211201203644","2015-03-22T15:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.249930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4235,"MURRAYLINKV5_20211201203644","2015-03-23T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.788830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4245,"MURRAYLINKV5_20211201203644","2015-03-23T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-34.194929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4254,"MURRAYLINKV5_20211201203644","2015-03-23T06:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-126.94414999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4259,"MURRAYLINKV5_20211201203644","2015-03-23T16:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-16",1,-80.584670000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4273,"MURRAYLINKV5_20211201203644","2015-03-25T13:40:00","S>>X_BWPA+PARS_09","S-X_BWPA+PARS","2014-12-16",1,-93.700630000000004,"Out=Blyth West-Munno Para 275kV line AND Para-Roseworthy 132kV line , avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4277,"MURRAYLINKV5_20211201203644","2015-03-25T14:10:00","S>>X_BWPA+PARS_09","S-X_BWPA+PARS","2014-12-16",1,-93.263220000000004,"Out=Blyth West-Munno Para 275kV line AND Para-Roseworthy 132kV line , avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4292,"MURRAYLINKV5_20211201203644","2015-03-25T16:05:00","S>>X_BWPA+PARS_09","S-X_BWPA+PARS","2014-12-16",1,-94.391620000000003,"Out=Blyth West-Munno Para 275kV line AND Para-Roseworthy 132kV line , avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4295,"MURRAYLINKV5_20211201203644","2015-03-25T19:15:00","S>>X_BWPA+PARS_09","S-X_BWPA+PARS","2014-12-16",1,-20.952249999999999,"Out=Blyth West-Munno Para 275kV line AND Para-Roseworthy 132kV line , avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4303,"MURRAYLINKV5_20211201203644","2015-03-25T19:55:00","S>>X_BWPA+PARS_09","S-X_BWPA+PARS","2014-12-16",1,-29.966449999999998,"Out=Blyth West-Munno Para 275kV line AND Para-Roseworthy 132kV line , avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4313,"MURRAYLINKV5_20211201203644","2015-03-26T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.465540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4322,"MURRAYLINKV5_20211201203644","2015-04-01T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.559279999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4331,"MURRAYLINKV5_20211201203644","2015-04-01T05:50:00","#R012072_012_RAMP_F","#R012072_RAMP","2015-04-01",1,-16.795850000000002,"Hard Ramping constraint for constraint V>>N_DDMS_2, Effective Date: 27/02/2014, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[4341,"MURRAYLINKV5_20211201203644","2015-04-01T06:25:00","V>>N_DDMS_2","V-DDMS","2014-02-27",1,-276.35822000000002,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4350,"MURRAYLINKV5_20211201203644","2015-04-01T06:50:00","V>>N_DDMS_2","V-DDMS","2014-02-27",1,-261.70798000000002,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4360,"MURRAYLINKV5_20211201203644","2015-04-01T17:20:00","#R012075_012_RAMP_F","#R012075_RAMP","2015-04-01",1,-24.86016,"Hard Ramping constraint for constraint V::N_HWSM_V4, Effective Date: 21/02/2014, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[4361,"MURRAYLINKV5_20211201203644","2015-04-01T17:25:00","#R012075_012_RAMP_F","#R012075_RAMP","2015-04-01",1,-13.657999999999999,"Hard Ramping constraint for constraint V::N_HWSM_V4, Effective Date: 21/02/2014, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[4374,"MURRAYLINKV5_20211201203644","2015-04-01T19:30:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2014-02-21",1,-10.321899999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4380,"MURRAYLINKV5_20211201203644","2015-04-01T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.562200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4392,"MURRAYLINKV5_20211201203644","2015-04-02T05:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-16.911850000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4399,"MURRAYLINKV5_20211201203644","2015-04-02T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.52952,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4410,"MURRAYLINKV5_20211201203644","2015-04-03T08:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.92722,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4418,"MURRAYLINKV5_20211201203644","2015-04-03T09:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.8962,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4428,"MURRAYLINKV5_20211201203644","2015-04-03T17:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.665760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4429,"MURRAYLINKV5_20211201203644","2015-04-03T17:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.56448,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4437,"MURRAYLINKV5_20211201203644","2015-04-03T18:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.418240000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4448,"MURRAYLINKV5_20211201203644","2015-04-03T19:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.18928,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4460,"MURRAYLINKV5_20211201203644","2015-04-03T20:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.941050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4467,"MURRAYLINKV5_20211201203644","2015-04-03T21:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.39953,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4476,"MURRAYLINKV5_20211201203644","2015-04-03T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.867459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4480,"MURRAYLINKV5_20211201203644","2015-04-03T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.878349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4495,"MURRAYLINKV5_20211201203644","2015-04-04T00:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.768420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4498,"MURRAYLINKV5_20211201203644","2015-04-04T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.166729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4506,"MURRAYLINKV5_20211201203644","2015-04-04T06:35:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-13.14227,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4516,"MURRAYLINKV5_20211201203644","2015-04-04T07:25:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.378640000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4525,"MURRAYLINKV5_20211201203644","2015-04-04T08:10:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-19.833089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4534,"MURRAYLINKV5_20211201203644","2015-04-04T09:15:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.311809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4544,"MURRAYLINKV5_20211201203644","2015-04-05T07:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.73061,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4548,"MURRAYLINKV5_20211201203644","2015-04-05T08:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.382909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4563,"MURRAYLINKV5_20211201203644","2015-04-06T12:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-11.563980000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4566,"MURRAYLINKV5_20211201203644","2015-04-06T13:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-12.275790000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4574,"MURRAYLINKV5_20211201203644","2015-04-06T17:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.94035,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4583,"MURRAYLINKV5_20211201203644","2015-04-07T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.78267,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4595,"MURRAYLINKV5_20211201203644","2015-04-07T04:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-16.15372,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4602,"MURRAYLINKV5_20211201203644","2015-04-07T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.179360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4613,"MURRAYLINKV5_20211201203644","2015-04-07T09:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.87527,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4621,"MURRAYLINKV5_20211201203644","2015-04-07T09:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.028280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4631,"MURRAYLINKV5_20211201203644","2015-04-08T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.73319,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4632,"MURRAYLINKV5_20211201203644","2015-04-08T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.86792,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4640,"MURRAYLINKV5_20211201203644","2015-04-08T06:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.519549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4651,"MURRAYLINKV5_20211201203644","2015-04-08T17:15:00","V>SMLBAHO1","V-BAHO;V-BAHO_P;V-BAHO_R;V-BAWA;V-BEKG;V-HOWA","2013-08-21",1,-12.19271,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4663,"MURRAYLINKV5_20211201203644","2015-04-08T18:30:00","V>SMLBAHO1","V-BAHO;V-BAHO_P;V-BAHO_R;V-BAWA;V-BEKG;V-HOWA","2013-08-21",1,-11.61459,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4670,"MURRAYLINKV5_20211201203644","2015-04-08T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.271710000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4681,"MURRAYLINKV5_20211201203644","2015-04-09T01:15:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-18.35107,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4689,"MURRAYLINKV5_20211201203644","2015-04-09T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.0945,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4699,"MURRAYLINKV5_20211201203644","2015-04-09T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.72153,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4700,"MURRAYLINKV5_20211201203644","2015-04-09T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.01764,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4709,"MURRAYLINKV5_20211201203644","2015-04-09T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.56561,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4719,"MURRAYLINKV5_20211201203644","2015-04-09T06:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.47907,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4728,"MURRAYLINKV5_20211201203644","2015-04-10T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-20.28877,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4737,"MURRAYLINKV5_20211201203644","2015-04-10T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.479699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4747,"MURRAYLINKV5_20211201203644","2015-04-10T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.434670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4755,"MURRAYLINKV5_20211201203644","2015-04-10T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.988289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4766,"MURRAYLINKV5_20211201203644","2015-04-10T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.21433,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4769,"MURRAYLINKV5_20211201203644","2015-04-10T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.24178,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4777,"MURRAYLINKV5_20211201203644","2015-04-10T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.92146,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4787,"MURRAYLINKV5_20211201203644","2015-04-10T06:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-24.74615,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4796,"MURRAYLINKV5_20211201203644","2015-04-10T10:30:00","V::N_BUDPQF_R","N-BUDP;N-BUDP_P;N-BUDP_R;N-WAGGA_330_BUSB","2013-08-21",1,-20.013369999999998,"Out = Buronga to Darlington Point 220kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 3","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4805,"MURRAYLINKV5_20211201203644","2015-04-11T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-19.58052,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4815,"MURRAYLINKV5_20211201203644","2015-04-11T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.663869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4824,"MURRAYLINKV5_20211201203644","2015-04-11T06:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-18.15879,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4834,"MURRAYLINKV5_20211201203644","2015-04-11T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.629060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4835,"MURRAYLINKV5_20211201203644","2015-04-11T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-17.55621,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4843,"MURRAYLINKV5_20211201203644","2015-04-12T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.297940000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4854,"MURRAYLINKV5_20211201203644","2015-04-12T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.851649999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4861,"MURRAYLINKV5_20211201203644","2015-04-12T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.42093,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4873,"MURRAYLINKV5_20211201203644","2015-04-12T08:25:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.024229999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4884,"MURRAYLINKV5_20211201203644","2015-04-12T09:20:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.621930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4892,"MURRAYLINKV5_20211201203644","2015-04-12T10:00:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.45238,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4902,"MURRAYLINKV5_20211201203644","2015-04-14T01:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.13355,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4903,"MURRAYLINKV5_20211201203644","2015-04-14T01:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.69275,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4911,"MURRAYLINKV5_20211201203644","2015-04-15T01:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.37993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4922,"MURRAYLINKV5_20211201203644","2015-04-15T02:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.00197,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4929,"MURRAYLINKV5_20211201203644","2015-04-15T05:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.72993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4941,"MURRAYLINKV5_20211201203644","2015-04-16T01:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.72991,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4950,"MURRAYLINKV5_20211201203644","2015-04-16T06:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.444129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4958,"MURRAYLINKV5_20211201203644","2015-04-16T10:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-27.594190000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4969,"MURRAYLINKV5_20211201203644","2015-04-16T14:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-20.060649999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4976,"MURRAYLINKV5_20211201203644","2015-04-16T15:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-40.883270000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4980,"MURRAYLINKV5_20211201203644","2015-04-16T15:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-216.20468,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4990,"MURRAYLINKV5_20211201203644","2015-04-16T16:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-70.638490000000004,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[4999,"MURRAYLINKV5_20211201203644","2015-04-16T16:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-215.34591,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5008,"MURRAYLINKV5_20211201203644","2015-04-16T17:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-198.68167,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5018,"MURRAYLINKV5_20211201203644","2015-04-16T18:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-111.68776,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5026,"MURRAYLINKV5_20211201203644","2015-04-17T04:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.92515,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5037,"MURRAYLINKV5_20211201203644","2015-04-18T11:55:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.018330000000001,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5044,"MURRAYLINKV5_20211201203644","2015-04-18T12:55:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-12.5458,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5048,"MURRAYLINKV5_20211201203644","2015-04-18T13:10:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-20.587589999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5057,"MURRAYLINKV5_20211201203644","2015-04-18T14:20:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.193669999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5064,"MURRAYLINKV5_20211201203644","2015-04-18T15:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.15887,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5076,"MURRAYLINKV5_20211201203644","2015-04-19T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-13.385059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5082,"MURRAYLINKV5_20211201203644","2015-04-19T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-15.87058,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5095,"MURRAYLINKV5_20211201203644","2015-04-19T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-12.04275,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5105,"MURRAYLINKV5_20211201203644","2015-04-19T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-11.118550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5106,"MURRAYLINKV5_20211201203644","2015-04-19T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.32959,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5114,"MURRAYLINKV5_20211201203644","2015-04-19T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.319459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5125,"MURRAYLINKV5_20211201203644","2015-04-19T06:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-10.70805,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5132,"MURRAYLINKV5_20211201203644","2015-04-19T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.16267,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5144,"MURRAYLINKV5_20211201203644","2015-04-19T08:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-10-22",1,-14.24865,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5150,"MURRAYLINKV5_20211201203644","2015-04-19T10:20:00","V::N_NIL_S4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-15.312609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5163,"MURRAYLINKV5_20211201203644","2015-04-23T08:55:00","V>SMLBAHO1","V-BAHO;V-BAHO_P;V-BAHO_R;V-BAWA;V-BEKG;V-HOWA","2013-08-21",1,-13.640309999999999,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5173,"MURRAYLINKV5_20211201203644","2015-04-27T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.94525,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5174,"MURRAYLINKV5_20211201203644","2015-04-27T17:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-37.370080000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5183,"MURRAYLINKV5_20211201203644","2015-04-29T08:40:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2013-08-21",1,-240.98652999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5197,"MURRAYLINKV5_20211201203644","2015-04-29T12:40:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2013-08-21",1,-10.221640000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5202,"MURRAYLINKV5_20211201203644","2015-04-29T17:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-04-08",1,-37.376510000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5211,"MURRAYLINKV5_20211201203644","2015-05-01T08:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-750.06442000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5221,"MURRAYLINKV5_20211201203644","2015-05-01T09:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-48.537260000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5229,"MURRAYLINKV5_20211201203644","2015-05-01T09:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-47.450960000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5240,"MURRAYLINKV5_20211201203644","2015-05-01T10:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-33.125360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5247,"MURRAYLINKV5_20211201203644","2015-05-02T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.06237,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5251,"MURRAYLINKV5_20211201203644","2015-05-02T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.042870000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5265,"MURRAYLINKV5_20211201203644","2015-05-06T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-52.643909999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5270,"MURRAYLINKV5_20211201203644","2015-05-06T15:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-55.333359999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5279,"MURRAYLINKV5_20211201203644","2015-05-07T04:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.465669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5289,"MURRAYLINKV5_20211201203644","2015-05-07T06:45:00","V::N_HYSE_V3","I-HYSE","2015-04-20",1,-24.969909999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","",null,null,0]
[5298,"MURRAYLINKV5_20211201203644","2015-05-08T19:45:00","V::N_HYTR_Q1","V-HYTR","2015-02-16",1,-25.817039999999999,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5308,"MURRAYLINKV5_20211201203644","2015-05-08T22:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.66309,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5309,"MURRAYLINKV5_20211201203644","2015-05-08T22:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.299630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5317,"MURRAYLINKV5_20211201203644","2015-05-09T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.088089999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5328,"MURRAYLINKV5_20211201203644","2015-05-09T13:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.90657,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5335,"MURRAYLINKV5_20211201203644","2015-05-09T13:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-12.20069,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5347,"MURRAYLINKV5_20211201203644","2015-05-09T21:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.091989999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5353,"MURRAYLINKV5_20211201203644","2015-05-09T22:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.75689,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5366,"MURRAYLINKV5_20211201203644","2015-05-09T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.25046,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5371,"MURRAYLINKV5_20211201203644","2015-05-10T00:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-19.825690000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5377,"MURRAYLINKV5_20211201203644","2015-05-10T01:40:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-33.884819999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5385,"MURRAYLINKV5_20211201203644","2015-05-10T02:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-38.903060000000004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5396,"MURRAYLINKV5_20211201203644","2015-05-10T02:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5405,"MURRAYLINKV5_20211201203644","2015-05-10T02:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-39.330669999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5414,"MURRAYLINKV5_20211201203644","2015-05-10T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-38.048650000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5424,"MURRAYLINKV5_20211201203644","2015-05-10T03:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-32.534390000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5432,"MURRAYLINKV5_20211201203644","2015-05-10T03:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-20.981870000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5443,"MURRAYLINKV5_20211201203644","2015-05-10T04:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.42004,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5450,"MURRAYLINKV5_20211201203644","2015-05-10T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-32.737609999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5454,"MURRAYLINKV5_20211201203644","2015-05-10T04:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-40.368020000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5468,"MURRAYLINKV5_20211201203644","2015-05-10T05:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-39.886209999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5473,"MURRAYLINKV5_20211201203644","2015-05-10T05:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.292099999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5482,"MURRAYLINKV5_20211201203644","2015-05-10T05:40:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-16.456309999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5492,"MURRAYLINKV5_20211201203644","2015-05-10T06:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-32.635509999999996,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5500,"MURRAYLINKV5_20211201203644","2015-05-10T06:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.436219999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5511,"MURRAYLINKV5_20211201203644","2015-05-10T08:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.396839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5518,"MURRAYLINKV5_20211201203644","2015-05-10T08:40:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.251720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5522,"MURRAYLINKV5_20211201203644","2015-05-10T09:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.139419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5531,"MURRAYLINKV5_20211201203644","2015-05-10T09:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.170120000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5538,"MURRAYLINKV5_20211201203644","2015-05-10T10:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-17.259409999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5550,"MURRAYLINKV5_20211201203644","2015-05-10T11:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.06728,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5556,"MURRAYLINKV5_20211201203644","2015-05-10T11:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.39058,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5569,"MURRAYLINKV5_20211201203644","2015-05-10T13:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.46547,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5574,"MURRAYLINKV5_20211201203644","2015-05-10T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-41.032800000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5580,"MURRAYLINKV5_20211201203644","2015-05-10T13:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-40.925960000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5588,"MURRAYLINKV5_20211201203644","2015-05-10T14:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-23.381039999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5599,"MURRAYLINKV5_20211201203644","2015-05-10T14:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-25.546379999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5606,"MURRAYLINKV5_20211201203644","2015-05-10T14:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-23.437080000000002,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5618,"MURRAYLINKV5_20211201203644","2015-05-10T15:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-13.19351,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5624,"MURRAYLINKV5_20211201203644","2015-05-10T15:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.96133,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5637,"MURRAYLINKV5_20211201203644","2015-05-10T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-27.191559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5646,"MURRAYLINKV5_20211201203644","2015-05-11T01:55:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-32.80491,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5653,"MURRAYLINKV5_20211201203644","2015-05-11T02:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.0946,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5657,"MURRAYLINKV5_20211201203644","2015-05-11T02:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-32.53096,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5671,"MURRAYLINKV5_20211201203644","2015-05-11T03:15:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.432169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5676,"MURRAYLINKV5_20211201203644","2015-05-11T03:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.23969,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5689,"MURRAYLINKV5_20211201203644","2015-05-11T04:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-18.098279999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5695,"MURRAYLINKV5_20211201203644","2015-05-11T04:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.85933,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5703,"MURRAYLINKV5_20211201203644","2015-05-11T05:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-48.162219999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5714,"MURRAYLINKV5_20211201203644","2015-05-11T10:20:00","V::N_MLMO_Q4","V-MLMO","2015-02-16",1,-17.121639999999999,"Out = Moorabool to Mortlake (MLTS-MOPS) No. 2 500 kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5721,"MURRAYLINKV5_20211201203644","2015-05-11T21:45:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.069789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5725,"MURRAYLINKV5_20211201203644","2015-05-12","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.04602,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5739,"MURRAYLINKV5_20211201203644","2015-05-13T02:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.470099999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5744,"MURRAYLINKV5_20211201203644","2015-05-14T00:45:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-23.13804,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5757,"MURRAYLINKV5_20211201203644","2015-05-14T07:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-79.025899999999993,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5763,"MURRAYLINKV5_20211201203644","2015-05-14T22:30:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-22.841640000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5772,"MURRAYLINKV5_20211201203644","2015-05-14T23:55:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-17.553129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5777,"MURRAYLINKV5_20211201203644","2015-05-15T00:20:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-19.47606,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5783,"MURRAYLINKV5_20211201203644","2015-05-15T00:50:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-28.875419999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5795,"MURRAYLINKV5_20211201203644","2015-05-15T01:50:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-22.454709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5802,"MURRAYLINKV5_20211201203644","2015-05-15T02:25:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.41859,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5809,"MURRAYLINKV5_20211201203644","2015-05-15T04:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.288309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5821,"MURRAYLINKV5_20211201203644","2015-05-15T05:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-20.67597,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5827,"MURRAYLINKV5_20211201203644","2015-05-15T05:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-19.993939999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5840,"MURRAYLINKV5_20211201203644","2015-05-19T17:10:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-04-28",1,-16.019970000000001,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5845,"MURRAYLINKV5_20211201203644","2015-05-19T17:35:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-04-28",1,-22.968779999999999,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5851,"MURRAYLINKV5_20211201203644","2015-05-19T18:05:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-04-28",1,-21.402709999999999,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5863,"MURRAYLINKV5_20211201203644","2015-05-19T19:15:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-04-28",1,-10.47668,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5870,"MURRAYLINKV5_20211201203644","2015-05-21T06:15:00","#R012342_013_RAMP_F","#R012342_RAMP","2015-05-20",1,-11.727169999999999,"Hard Ramping constraint for constraint N^^V_LTWG, Effective Date: 24/09/2014, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[5879,"MURRAYLINKV5_20211201203644","2015-05-21T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11472.01554,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5892,"MURRAYLINKV5_20211201203644","2015-05-23T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-17.518899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5898,"MURRAYLINKV5_20211201203644","2015-05-23T15:30:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-11.251469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5901,"MURRAYLINKV5_20211201203644","2015-05-23T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-110.14617,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5917,"MURRAYLINKV5_20211201203644","2015-05-24T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.213520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5924,"MURRAYLINKV5_20211201203644","2015-05-24T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.23855,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5928,"MURRAYLINKV5_20211201203644","2015-05-24T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.06378,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5942,"MURRAYLINKV5_20211201203644","2015-05-24T05:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.9314,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5947,"MURRAYLINKV5_20211201203644","2015-05-24T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.94576,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5960,"MURRAYLINKV5_20211201203644","2015-05-25T08:25:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-23.67107,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5966,"MURRAYLINKV5_20211201203644","2015-05-25T08:55:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-13.533849999999999,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5969,"MURRAYLINKV5_20211201203644","2015-05-25T09:10:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-23.619610000000002,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5985,"MURRAYLINKV5_20211201203644","2015-05-26T05:35:00","#R012372_023_RAMP_F","#R012372_RAMP","2015-05-25",1,-21.144380000000002,"Hard Ramping constraint for constraint V::N_LTWG_V2, Effective Date: 20/04/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[5992,"MURRAYLINKV5_20211201203644","2015-05-26T10:40:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-23.22476,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[5996,"MURRAYLINKV5_20211201203644","2015-05-26T12:50:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-52.834620000000001,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6005,"MURRAYLINKV5_20211201203644","2015-05-26T13:40:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-22.336960000000001,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6016,"MURRAYLINKV5_20211201203644","2015-05-26T22:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.920529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6024,"MURRAYLINKV5_20211201203644","2015-05-26T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.76506,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6030,"MURRAYLINKV5_20211201203644","2015-05-27T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.37382,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6043,"MURRAYLINKV5_20211201203644","2015-05-27T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-16.340050000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6048,"MURRAYLINKV5_20211201203644","2015-05-27T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-15.78307,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6054,"MURRAYLINKV5_20211201203644","2015-05-27T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.31049,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6066,"MURRAYLINKV5_20211201203644","2015-05-27T08:05:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-10.635339999999999,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6073,"MURRAYLINKV5_20211201203644","2015-05-27T08:25:00","N^^V_LTWG","N^^V_LTWG","2014-09-24",1,-11.144299999999999,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6084,"MURRAYLINKV5_20211201203644","2015-05-28T00:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-16.213609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6092,"MURRAYLINKV5_20211201203644","2015-05-28T00:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-14.79072,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6098,"MURRAYLINKV5_20211201203644","2015-05-28T01:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.674200000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6111,"MURRAYLINKV5_20211201203644","2015-05-28T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.958209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6120,"MURRAYLINKV5_20211201203644","2015-05-28T13:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.45668,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6122,"MURRAYLINKV5_20211201203644","2015-05-28T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.928879999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6131,"MURRAYLINKV5_20211201203644","2015-05-28T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.289490000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6145,"MURRAYLINKV5_20211201203644","2015-05-28T22:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-17.780349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6150,"MURRAYLINKV5_20211201203644","2015-05-28T22:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.09144,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6163,"MURRAYLINKV5_20211201203644","2015-05-29T00:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-16.852509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6169,"MURRAYLINKV5_20211201203644","2015-05-29T01:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-15.2241,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6172,"MURRAYLINKV5_20211201203644","2015-05-29T01:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.816549999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6188,"MURRAYLINKV5_20211201203644","2015-05-29T22:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.75123,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6190,"MURRAYLINKV5_20211201203644","2015-05-29T22:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.61354,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6199,"MURRAYLINKV5_20211201203644","2015-05-30","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.18981,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6213,"MURRAYLINKV5_20211201203644","2015-05-30T01:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-22.888549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6218,"MURRAYLINKV5_20211201203644","2015-05-30T01:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-19.321570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6231,"MURRAYLINKV5_20211201203644","2015-05-30T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.740349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6237,"MURRAYLINKV5_20211201203644","2015-05-30T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.743230000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6246,"MURRAYLINKV5_20211201203644","2015-05-30T07:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.864470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6251,"MURRAYLINKV5_20211201203644","2015-05-30T08:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.00332,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6257,"MURRAYLINKV5_20211201203644","2015-05-30T10:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.30157,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6269,"MURRAYLINKV5_20211201203644","2015-05-30T11:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.13843,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6276,"MURRAYLINKV5_20211201203644","2015-05-30T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-17.06934,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6287,"MURRAYLINKV5_20211201203644","2015-05-30T13:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.939819999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6295,"MURRAYLINKV5_20211201203644","2015-05-30T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.323270000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6305,"MURRAYLINKV5_20211201203644","2015-05-30T16:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-16.20309,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6314,"MURRAYLINKV5_20211201203644","2015-05-30T17:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.56284,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6319,"MURRAYLINKV5_20211201203644","2015-05-30T19:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.7378,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6325,"MURRAYLINKV5_20211201203644","2015-05-30T20:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.146739999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6337,"MURRAYLINKV5_20211201203644","2015-05-30T21:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.757669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6344,"MURRAYLINKV5_20211201203644","2015-05-30T21:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.104839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6353,"MURRAYLINKV5_20211201203644","2015-05-30T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.10229,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6366,"MURRAYLINKV5_20211201203644","2015-05-31T00:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.6899,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6372,"MURRAYLINKV5_20211201203644","2015-05-31T00:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-10.445650000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6375,"MURRAYLINKV5_20211201203644","2015-05-31T00:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.32042,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6391,"MURRAYLINKV5_20211201203644","2015-05-31T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-16.19717,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6393,"MURRAYLINKV5_20211201203644","2015-05-31T01:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-16.189019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6402,"MURRAYLINKV5_20211201203644","2015-05-31T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.61069,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6411,"MURRAYLINKV5_20211201203644","2015-05-31T03:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-15.97165,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6421,"MURRAYLINKV5_20211201203644","2015-05-31T04:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-16.589200000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6434,"MURRAYLINKV5_20211201203644","2015-05-31T05:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.18511,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6440,"MURRAYLINKV5_20211201203644","2015-05-31T06:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.87072,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6443,"MURRAYLINKV5_20211201203644","2015-05-31T06:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-13.543229999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6459,"MURRAYLINKV5_20211201203644","2015-05-31T07:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.288040000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6460,"MURRAYLINKV5_20211201203644","2015-05-31T07:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.397550000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6472,"MURRAYLINKV5_20211201203644","2015-05-31T08:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.5571,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6479,"MURRAYLINKV5_20211201203644","2015-05-31T09:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.024419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6490,"MURRAYLINKV5_20211201203644","2015-05-31T10:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.31086,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6498,"MURRAYLINKV5_20211201203644","2015-05-31T11:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.177060000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6508,"MURRAYLINKV5_20211201203644","2015-05-31T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.75778,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6517,"MURRAYLINKV5_20211201203644","2015-05-31T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.572039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6522,"MURRAYLINKV5_20211201203644","2015-05-31T13:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.65962,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6528,"MURRAYLINKV5_20211201203644","2015-05-31T13:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.83464,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6540,"MURRAYLINKV5_20211201203644","2015-05-31T14:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.434609999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6547,"MURRAYLINKV5_20211201203644","2015-05-31T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.77618,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6558,"MURRAYLINKV5_20211201203644","2015-05-31T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.49009,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6566,"MURRAYLINKV5_20211201203644","2015-05-31T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-12.776870000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6576,"MURRAYLINKV5_20211201203644","2015-05-31T16:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.136240000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6585,"MURRAYLINKV5_20211201203644","2015-05-31T20:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.77425,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6594,"MURRAYLINKV5_20211201203644","2015-05-31T22:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.21527,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6596,"MURRAYLINKV5_20211201203644","2015-05-31T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.010400000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6605,"MURRAYLINKV5_20211201203644","2015-05-31T23:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.35195,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6614,"MURRAYLINKV5_20211201203644","2015-06-01T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.056889999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6624,"MURRAYLINKV5_20211201203644","2015-06-02T13:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-05-29",1,-12.41352,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6637,"MURRAYLINKV5_20211201203644","2015-06-04T03:40:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-14.34704,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6643,"MURRAYLINKV5_20211201203644","2015-06-04T05:25:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.01355,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6646,"MURRAYLINKV5_20211201203644","2015-06-04T05:50:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.6586,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6662,"MURRAYLINKV5_20211201203644","2015-06-07T00:05:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-16.095479999999998,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6664,"MURRAYLINKV5_20211201203644","2015-06-07T00:15:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-12.541270000000001,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6673,"MURRAYLINKV5_20211201203644","2015-06-07T01:05:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.151009999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6682,"MURRAYLINKV5_20211201203644","2015-06-07T01:50:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.130879999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6692,"MURRAYLINKV5_20211201203644","2015-06-07T08:40:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.31194,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6701,"MURRAYLINKV5_20211201203644","2015-06-07T09:30:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-12.036289999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6711,"MURRAYLINKV5_20211201203644","2015-06-07T10:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.71442,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6720,"MURRAYLINKV5_20211201203644","2015-06-07T23:25:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-66.784630000000007,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6729,"MURRAYLINKV5_20211201203644","2015-06-08T02:55:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-50.115130000000001,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6731,"MURRAYLINKV5_20211201203644","2015-06-08T03:05:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-50.384219999999999,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6743,"MURRAYLINKV5_20211201203644","2015-06-08T04:05:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-42.87209,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6750,"MURRAYLINKV5_20211201203644","2015-06-08T04:40:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-42.188890000000001,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6761,"MURRAYLINKV5_20211201203644","2015-06-08T05:35:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-49.764499999999998,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6769,"MURRAYLINKV5_20211201203644","2015-06-08T06:15:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-57.964100000000002,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6779,"MURRAYLINKV5_20211201203644","2015-06-08T07:10:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-68.005189999999999,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6788,"MURRAYLINKV5_20211201203644","2015-06-08T07:55:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-57.479869999999998,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6797,"MURRAYLINKV5_20211201203644","2015-06-08T08:40:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-60.943989999999999,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6799,"MURRAYLINKV5_20211201203644","2015-06-08T08:50:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-61.218400000000003,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6811,"MURRAYLINKV5_20211201203644","2015-06-08T11:10:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-59.157879999999999,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6818,"MURRAYLINKV5_20211201203644","2015-06-08T14:15:00","S::V_SA_PSS_2","S-NIL","2013-03-15",1,-56.646659999999997,"Out= Nil; Maintain maximum transfer limit on SA-VIC and Murray link combined to avoid oscillatory instability when both Northern Power Station and Play ford Power Station are out of service (Note: Both Para & South East SVCs assumed to be I/S).","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6827,"MURRAYLINKV5_20211201203644","2015-06-08T22:20:00","V>>V_NIL_2_P","V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL","2015-01-21",1,-10.852069999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6835,"MURRAYLINKV5_20211201203644","2015-06-09T12:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-217.94103000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6846,"MURRAYLINKV5_20211201203644","2015-06-09T14:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-219.46420000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6849,"MURRAYLINKV5_20211201203644","2015-06-09T16:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-251.60543999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6865,"MURRAYLINKV5_20211201203644","2015-06-10T00:40:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.318350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6867,"MURRAYLINKV5_20211201203644","2015-06-10T01:00:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.734920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6876,"MURRAYLINKV5_20211201203644","2015-06-10T01:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.585739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6885,"MURRAYLINKV5_20211201203644","2015-06-10T02:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.6395,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6895,"MURRAYLINKV5_20211201203644","2015-06-10T05:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.82701,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6903,"MURRAYLINKV5_20211201203644","2015-06-10T11:30:00","#R012470_002_RAMP_V","#R012470_RAMP","2015-06-10",1,-250.95353,"Soft Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[6914,"MURRAYLINKV5_20211201203644","2015-06-12T01:00:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.55119,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6917,"MURRAYLINKV5_20211201203644","2015-06-12T08:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11412.70347,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6933,"MURRAYLINKV5_20211201203644","2015-06-16T00:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-14.51543,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6934,"MURRAYLINKV5_20211201203644","2015-06-16T00:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-14.537610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6950,"MURRAYLINKV5_20211201203644","2015-06-18T13:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-05",1,-13.685230000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6953,"MURRAYLINKV5_20211201203644","2015-06-19T03:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.26182,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6964,"MURRAYLINKV5_20211201203644","2015-06-20T03:25:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-10.75254,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6972,"MURRAYLINKV5_20211201203644","2015-06-21T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.96171,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6982,"MURRAYLINKV5_20211201203644","2015-06-21T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.647779999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[6991,"MURRAYLINKV5_20211201203644","2015-06-22T01:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-10.729150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7000,"MURRAYLINKV5_20211201203644","2015-06-22T03:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-16.223669999999998,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7002,"MURRAYLINKV5_20211201203644","2015-06-22T04:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.485519999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7018,"MURRAYLINKV5_20211201203644","2015-06-23T01:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.60169,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7021,"MURRAYLINKV5_20211201203644","2015-06-23T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-11.5479,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7032,"MURRAYLINKV5_20211201203644","2015-06-23T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-01-21",1,-10.43018,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7040,"MURRAYLINKV5_20211201203644","2015-06-24T01:40:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-14.274699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7050,"MURRAYLINKV5_20211201203644","2015-06-24T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-12.063980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7059,"MURRAYLINKV5_20211201203644","2015-06-26T01:40:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-28.817129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7068,"MURRAYLINKV5_20211201203644","2015-06-26T02:30:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-16.444310000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7070,"MURRAYLINKV5_20211201203644","2015-06-26T03:05:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-13.559279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7079,"MURRAYLINKV5_20211201203644","2015-06-26T05:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.754250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7088,"MURRAYLINKV5_20211201203644","2015-06-26T22:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-17.908010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7098,"MURRAYLINKV5_20211201203644","2015-06-27T22:05:00","V::N_NIL_Q2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2014-12-04",1,-18.19342,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7106,"MURRAYLINKV5_20211201203644","2015-06-27T22:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-17.969809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7117,"MURRAYLINKV5_20211201203644","2015-06-27T23:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-18.176749999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7124,"MURRAYLINKV5_20211201203644","2015-06-28T02:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-13.009919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7136,"MURRAYLINKV5_20211201203644","2015-06-29T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-18",1,-179.46584999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7138,"MURRAYLINKV5_20211201203644","2015-06-30T22:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-04-20",1,-11.83362,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7147,"MURRAYLINKV5_20211201203644","2015-07-01T00:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.05641,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7156,"MURRAYLINKV5_20211201203644","2015-07-01T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.822199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7166,"MURRAYLINKV5_20211201203644","2015-07-01T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.2273,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7175,"MURRAYLINKV5_20211201203644","2015-07-01T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.05156,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7185,"MURRAYLINKV5_20211201203644","2015-07-01T05:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.627320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7194,"MURRAYLINKV5_20211201203644","2015-07-01T12:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.2751,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7203,"MURRAYLINKV5_20211201203644","2015-07-02T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.61082,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7205,"MURRAYLINKV5_20211201203644","2015-07-02T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.158939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7221,"MURRAYLINKV5_20211201203644","2015-07-02T10:15:00","#R012554_002_RAMP_V","#R012554_RAMP","2015-07-02",1,-15.51286,"Soft Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[7224,"MURRAYLINKV5_20211201203644","2015-07-02T10:25:00","#R012554_002_RAMP_F","#R012554_RAMP","2015-07-02",1,-308.06691999999998,"Hard Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[7230,"MURRAYLINKV5_20211201203644","2015-07-03T02:45:00","S>>RBTX1_RBTX2_WEWT","S-RB_TX1;S-X-RBTX1+6616+6573","2015-06-03",1,-16.274850000000001,"Out= Robertstown 275/132kV TX1, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown 132/275kV TX2, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7243,"MURRAYLINKV5_20211201203644","2015-07-03T04:50:00","S>>RBTX1_RBTX2_WEWT","S-RB_TX1;S-X-RBTX1+6616+6573","2015-06-03",1,-12.198230000000001,"Out= Robertstown 275/132kV TX1, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown 132/275kV TX2, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7253,"MURRAYLINKV5_20211201203644","2015-07-03T11:55:00","S>>RBTX1_RBTX2_WEWT","S-RB_TX1;S-X-RBTX1+6616+6573","2015-06-03",1,-27.14367,"Out= Robertstown 275/132kV TX1, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown 132/275kV TX2, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7262,"MURRAYLINKV5_20211201203644","2015-07-03T23:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.827390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7271,"MURRAYLINKV5_20211201203644","2015-07-04T00:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.501919999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7273,"MURRAYLINKV5_20211201203644","2015-07-04T00:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.187719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7289,"MURRAYLINKV5_20211201203644","2015-07-04T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.95101,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7292,"MURRAYLINKV5_20211201203644","2015-07-04T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.757569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7301,"MURRAYLINKV5_20211201203644","2015-07-04T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.78363,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7309,"MURRAYLINKV5_20211201203644","2015-07-04T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.63973,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7320,"MURRAYLINKV5_20211201203644","2015-07-04T05:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.77125,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7327,"MURRAYLINKV5_20211201203644","2015-07-04T07:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.843310000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7339,"MURRAYLINKV5_20211201203644","2015-07-04T23:00:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.247140000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7345,"MURRAYLINKV5_20211201203644","2015-07-05T00:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.656330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7350,"MURRAYLINKV5_20211201203644","2015-07-05T01:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.81531,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7359,"MURRAYLINKV5_20211201203644","2015-07-05T02:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.281469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7369,"MURRAYLINKV5_20211201203644","2015-07-05T03:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.64146,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7377,"MURRAYLINKV5_20211201203644","2015-07-05T10:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.04907,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7388,"MURRAYLINKV5_20211201203644","2015-07-06T20:25:00","S>>RBTX1_RBTX2_WEWT","S-RB_TX1;S-X-RBTX1+6616+6573","2015-06-03",1,-11.435460000000001,"Out= Robertstown 275/132kV TX1, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown 132/275kV TX2, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7395,"MURRAYLINKV5_20211201203644","2015-07-07T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.132770000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7407,"MURRAYLINKV5_20211201203644","2015-07-07T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.534660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7408,"MURRAYLINKV5_20211201203644","2015-07-07T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.534140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7424,"MURRAYLINKV5_20211201203644","2015-07-08T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.51566,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7427,"MURRAYLINKV5_20211201203644","2015-07-08T03:40:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-21.383150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7433,"MURRAYLINKV5_20211201203644","2015-07-08T04:10:00","V::N_NIL_Q4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.432,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7446,"MURRAYLINKV5_20211201203644","2015-07-08T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.894200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7456,"MURRAYLINKV5_20211201203644","2015-07-10","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.190659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7465,"MURRAYLINKV5_20211201203644","2015-07-10T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.45679,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7474,"MURRAYLINKV5_20211201203644","2015-07-10T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.739710000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7476,"MURRAYLINKV5_20211201203644","2015-07-11","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.516360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7492,"MURRAYLINKV5_20211201203644","2015-07-11T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-19.60641,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7495,"MURRAYLINKV5_20211201203644","2015-07-11T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.562480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7501,"MURRAYLINKV5_20211201203644","2015-07-11T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.668109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7514,"MURRAYLINKV5_20211201203644","2015-07-12T17:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-32.433239999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7523,"MURRAYLINKV5_20211201203644","2015-07-12T18:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.42886,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7530,"MURRAYLINKV5_20211201203644","2015-07-12T19:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-37.16048,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7542,"MURRAYLINKV5_20211201203644","2015-07-12T21:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-22.559729999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7548,"MURRAYLINKV5_20211201203644","2015-07-12T22:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-22.813120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7553,"MURRAYLINKV5_20211201203644","2015-07-12T22:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-22.817910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7562,"MURRAYLINKV5_20211201203644","2015-07-12T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.37079,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7572,"MURRAYLINKV5_20211201203644","2015-07-13T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.835129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7580,"MURRAYLINKV5_20211201203644","2015-07-13T05:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.24555,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7591,"MURRAYLINKV5_20211201203644","2015-07-13T17:50:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-16.9893,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7598,"MURRAYLINKV5_20211201203644","2015-07-13T19:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.844189999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7610,"MURRAYLINKV5_20211201203644","2015-07-13T22:35:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.595680000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7616,"MURRAYLINKV5_20211201203644","2015-07-14T01:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-29.34366,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7621,"MURRAYLINKV5_20211201203644","2015-07-14T02:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.674990000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7634,"MURRAYLINKV5_20211201203644","2015-07-14T03:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.956770000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7640,"MURRAYLINKV5_20211201203644","2015-07-14T03:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.38738,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7649,"MURRAYLINKV5_20211201203644","2015-07-14T04:25:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.12289,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7654,"MURRAYLINKV5_20211201203644","2015-07-14T04:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.88053,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7668,"MURRAYLINKV5_20211201203644","2015-07-14T05:50:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-68.572749999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7677,"MURRAYLINKV5_20211201203644","2015-07-14T06:40:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-82.455309999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7679,"MURRAYLINKV5_20211201203644","2015-07-14T06:50:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-106.46579,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7695,"MURRAYLINKV5_20211201203644","2015-07-14T12:50:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-77.936899999999994,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7698,"MURRAYLINKV5_20211201203644","2015-07-14T13:05:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-66.105530000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7704,"MURRAYLINKV5_20211201203644","2015-07-14T13:55:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-71.286510000000007,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7717,"MURRAYLINKV5_20211201203644","2015-07-14T15:30:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-72.911450000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7722,"MURRAYLINKV5_20211201203644","2015-07-14T17:05:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-83.476529999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7736,"MURRAYLINKV5_20211201203644","2015-07-14T18:55:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-15.15781,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7745,"MURRAYLINKV5_20211201203644","2015-07-15T00:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.34252,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7747,"MURRAYLINKV5_20211201203644","2015-07-15T00:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.37659,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7756,"MURRAYLINKV5_20211201203644","2015-07-15T03:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.228009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7769,"MURRAYLINKV5_20211201203644","2015-07-15T07:40:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-106.74654,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7775,"MURRAYLINKV5_20211201203644","2015-07-15T07:55:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-119.09562,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7783,"MURRAYLINKV5_20211201203644","2015-07-15T09:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-21.266369999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7794,"MURRAYLINKV5_20211201203644","2015-07-15T11:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.88597,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7801,"MURRAYLINKV5_20211201203644","2015-07-15T12:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-14.77312,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7813,"MURRAYLINKV5_20211201203644","2015-07-15T18:45:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-128.70097999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7819,"MURRAYLINKV5_20211201203644","2015-07-15T19:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-53.684420000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7824,"MURRAYLINKV5_20211201203644","2015-07-15T19:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-40.753239999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7837,"MURRAYLINKV5_20211201203644","2015-07-16T04:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.480029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7843,"MURRAYLINKV5_20211201203644","2015-07-16T05:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.810219999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7851,"MURRAYLINKV5_20211201203644","2015-07-16T08:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-33.472610000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7862,"MURRAYLINKV5_20211201203644","2015-07-16T09:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-275.57071000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7869,"MURRAYLINKV5_20211201203644","2015-07-16T09:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-274.07614000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7881,"MURRAYLINKV5_20211201203644","2015-07-16T10:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-33.723669999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7882,"MURRAYLINKV5_20211201203644","2015-07-16T10:55:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-34.182729999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7898,"MURRAYLINKV5_20211201203644","2015-07-16T13:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-51.052289999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7901,"MURRAYLINKV5_20211201203644","2015-07-16T13:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-51.052289999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7907,"MURRAYLINKV5_20211201203644","2015-07-16T13:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-50.975099999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7920,"MURRAYLINKV5_20211201203644","2015-07-16T14:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-51.018650000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7925,"MURRAYLINKV5_20211201203644","2015-07-16T15:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-66.516080000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7939,"MURRAYLINKV5_20211201203644","2015-07-16T16:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-55.585590000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7943,"MURRAYLINKV5_20211201203644","2015-07-16T16:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-55.24973,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7950,"MURRAYLINKV5_20211201203644","2015-07-16T17:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-50.082839999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7966,"MURRAYLINKV5_20211201203644","2015-07-16T19:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-20.411390000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7969,"MURRAYLINKV5_20211201203644","2015-07-16T19:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-20.411390000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7975,"MURRAYLINKV5_20211201203644","2015-07-16T20:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-294.63672000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7988,"MURRAYLINKV5_20211201203644","2015-07-16T21:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-50.082850000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[7997,"MURRAYLINKV5_20211201203644","2015-07-17T00:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-11.725210000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8004,"MURRAYLINKV5_20211201203644","2015-07-17T01:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.178719999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8016,"MURRAYLINKV5_20211201203644","2015-07-17T07:00:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.64734,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8022,"MURRAYLINKV5_20211201203644","2015-07-17T09:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-218.85914,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8027,"MURRAYLINKV5_20211201203644","2015-07-17T09:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-220.89783,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8040,"MURRAYLINKV5_20211201203644","2015-07-17T10:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-34.616349999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8046,"MURRAYLINKV5_20211201203644","2015-07-17T11:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-40.923090000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8058,"MURRAYLINKV5_20211201203644","2015-07-17T12:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-35.77704,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8065,"MURRAYLINKV5_20211201203644","2015-07-17T12:55:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-42.342509999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8072,"MURRAYLINKV5_20211201203644","2015-07-17T13:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-43.953449999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8084,"MURRAYLINKV5_20211201203644","2015-07-17T14:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-44.860759999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8090,"MURRAYLINKV5_20211201203644","2015-07-17T15:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-45.228569999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8095,"MURRAYLINKV5_20211201203644","2015-07-17T15:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-43.078809999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8108,"MURRAYLINKV5_20211201203644","2015-07-17T16:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-32.059220000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8114,"MURRAYLINKV5_20211201203644","2015-07-17T17:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-43.761389999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8123,"MURRAYLINKV5_20211201203644","2015-07-17T19:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-38.901119999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8128,"MURRAYLINKV5_20211201203644","2015-07-17T19:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-35.724919999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8142,"MURRAYLINKV5_20211201203644","2015-07-17T21:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-43.223379999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8146,"MURRAYLINKV5_20211201203644","2015-07-17T21:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.87734,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8153,"MURRAYLINKV5_20211201203644","2015-07-17T22:55:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-39.2746,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8164,"MURRAYLINKV5_20211201203644","2015-07-18T00:55:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.3043,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8172,"MURRAYLINKV5_20211201203644","2015-07-18T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.501339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8178,"MURRAYLINKV5_20211201203644","2015-07-18T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.427020000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8191,"MURRAYLINKV5_20211201203644","2015-07-18T02:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-46.923940000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8196,"MURRAYLINKV5_20211201203644","2015-07-18T02:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-47.501570000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8210,"MURRAYLINKV5_20211201203644","2015-07-18T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.45543,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8214,"MURRAYLINKV5_20211201203644","2015-07-18T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.39104,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8221,"MURRAYLINKV5_20211201203644","2015-07-18T03:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-17.999580000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8230,"MURRAYLINKV5_20211201203644","2015-07-18T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-24.567640000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8243,"MURRAYLINKV5_20211201203644","2015-07-18T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.4435,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8249,"MURRAYLINKV5_20211201203644","2015-07-18T05:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-23.859749999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8261,"MURRAYLINKV5_20211201203644","2015-07-18T05:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-55.390329999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8268,"MURRAYLINKV5_20211201203644","2015-07-18T06:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-57.883960000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8279,"MURRAYLINKV5_20211201203644","2015-07-18T07:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-46.378309999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8287,"MURRAYLINKV5_20211201203644","2015-07-18T09:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-15.496130000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8293,"MURRAYLINKV5_20211201203644","2015-07-18T09:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-18.42803,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8298,"MURRAYLINKV5_20211201203644","2015-07-18T10:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-11.48105,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8311,"MURRAYLINKV5_20211201203644","2015-07-18T11:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-21.534269999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8317,"MURRAYLINKV5_20211201203644","2015-07-18T11:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.75468,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8329,"MURRAYLINKV5_20211201203644","2015-07-18T13:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.82151,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8336,"MURRAYLINKV5_20211201203644","2015-07-18T13:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.3644,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8347,"MURRAYLINKV5_20211201203644","2015-07-18T14:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.976109999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8355,"MURRAYLINKV5_20211201203644","2015-07-18T15:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.08259,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8356,"MURRAYLINKV5_20211201203644","2015-07-18T15:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.12124,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8367,"MURRAYLINKV5_20211201203644","2015-07-18T16:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-23.489560000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8375,"MURRAYLINKV5_20211201203644","2015-07-18T17:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-32.718910000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8385,"MURRAYLINKV5_20211201203644","2015-07-18T23:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-214.88176999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8394,"MURRAYLINKV5_20211201203644","2015-07-19T01:00:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-20.873860000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8399,"MURRAYLINKV5_20211201203644","2015-07-19T01:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-16.66451,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8413,"MURRAYLINKV5_20211201203644","2015-07-19T02:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-19.653780000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8417,"MURRAYLINKV5_20211201203644","2015-07-19T02:55:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.339960000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8424,"MURRAYLINKV5_20211201203644","2015-07-19T03:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.345369999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8435,"MURRAYLINKV5_20211201203644","2015-07-19T04:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-24.827919999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8443,"MURRAYLINKV5_20211201203644","2015-07-19T05:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-23.965949999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8453,"MURRAYLINKV5_20211201203644","2015-07-19T06:05:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-18.81711,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8462,"MURRAYLINKV5_20211201203644","2015-07-19T06:50:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-13.659840000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8471,"MURRAYLINKV5_20211201203644","2015-07-19T07:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-14.88419,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8482,"MURRAYLINKV5_20211201203644","2015-07-19T09:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-22.08259,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8490,"MURRAYLINKV5_20211201203644","2015-07-19T10:45:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.17254,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8496,"MURRAYLINKV5_20211201203644","2015-07-19T11:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.47762,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8501,"MURRAYLINKV5_20211201203644","2015-07-19T11:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.47762,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8514,"MURRAYLINKV5_20211201203644","2015-07-19T16:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.57386,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8520,"MURRAYLINKV5_20211201203644","2015-07-19T17:15:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-21.477260000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8532,"MURRAYLINKV5_20211201203644","2015-07-19T21:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.072609999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8539,"MURRAYLINKV5_20211201203644","2015-07-19T22:20:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-12.360279999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8550,"MURRAYLINKV5_20211201203644","2015-07-20T00:30:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.22654,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8558,"MURRAYLINKV5_20211201203644","2015-07-20T09:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-05",1,-19.965389999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8559,"MURRAYLINKV5_20211201203644","2015-07-20T09:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-30.278220000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8569,"MURRAYLINKV5_20211201203644","2015-07-20T10:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-229.93260000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8578,"MURRAYLINKV5_20211201203644","2015-07-20T11:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-144.39321000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8588,"MURRAYLINKV5_20211201203644","2015-07-20T16:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-20.315079999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8597,"MURRAYLINKV5_20211201203644","2015-07-20T17:25:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-33.472729999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8602,"MURRAYLINKV5_20211201203644","2015-07-20T18:35:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-227.55328,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8616,"MURRAYLINKV5_20211201203644","2015-07-20T20:10:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-38.56561,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8620,"MURRAYLINKV5_20211201203644","2015-07-20T20:40:00","V>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-47.715000000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225; limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB - MWP #1132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8627,"MURRAYLINKV5_20211201203644","2015-07-20T22:05:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-63.10483,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8638,"MURRAYLINKV5_20211201203644","2015-07-21T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.30273,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8646,"MURRAYLINKV5_20211201203644","2015-07-21T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.13191,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8656,"MURRAYLINKV5_20211201203644","2015-07-21T03:50:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-13.220789999999999,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8665,"MURRAYLINKV5_20211201203644","2015-07-21T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.017150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8670,"MURRAYLINKV5_20211201203644","2015-07-21T04:55:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-10.802490000000001,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8684,"MURRAYLINKV5_20211201203644","2015-07-21T06:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.35538,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8688,"MURRAYLINKV5_20211201203644","2015-07-21T08:55:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-49.469430000000003,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8695,"MURRAYLINKV5_20211201203644","2015-07-21T09:35:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-51.28313,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8704,"MURRAYLINKV5_20211201203644","2015-07-21T10:40:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-27.852620000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8717,"MURRAYLINKV5_20211201203644","2015-07-21T11:40:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-41.411569999999998,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8723,"MURRAYLINKV5_20211201203644","2015-07-21T12:00:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-35.427259999999997,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8735,"MURRAYLINKV5_20211201203644","2015-07-21T13:00:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-414000,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8742,"MURRAYLINKV5_20211201203644","2015-07-21T13:35:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-414000,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8753,"MURRAYLINKV5_20211201203644","2015-07-21T14:30:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-414000,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8761,"MURRAYLINKV5_20211201203644","2015-07-21T15:05:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-414000,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8762,"MURRAYLINKV5_20211201203644","2015-07-21T15:10:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-414000,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8772,"MURRAYLINKV5_20211201203644","2015-07-21T16:00:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-40.791240000000002,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8785,"MURRAYLINKV5_20211201203644","2015-07-21T17:05:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-49.31006,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8791,"MURRAYLINKV5_20211201203644","2015-07-21T17:45:00","S>X_NWCB6225+6021_T1","S-NWCB6021+6225","2015-07-13",1,-65.08905,"Out = North West Bend 132 kV circuit breakers CB6021 and CB6225 (Note: this takes out North West Bend-Monash #1 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #1 O/L on trip NWB - MWP #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8803,"MURRAYLINKV5_20211201203644","2015-07-21T19:10:00","S>>BWPA_BRTW_WTTP","S-BWPA","2014-03-04",1,-30.37724,"Out= Blyth West- Para 275kV line with Bungama CB6539 OPEN, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8810,"MURRAYLINKV5_20211201203644","2015-07-21T20:05:00","S>>BWPA_BRTW_WTTP","S-BWPA","2014-03-04",1,-17.12604,"Out= Blyth West- Para 275kV line with Bungama CB6539 OPEN, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8819,"MURRAYLINKV5_20211201203644","2015-07-22T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.35848,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8823,"MURRAYLINKV5_20211201203644","2015-07-22T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.01174,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8830,"MURRAYLINKV5_20211201203644","2015-07-22T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.001939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8841,"MURRAYLINKV5_20211201203644","2015-07-22T08:00:00","#R012620_004_RAMP_V","#R012620_RAMP","2015-07-22",1,-36.297910000000002,"Soft Ramping constraint for constraint V>X_NWCB6022+6023_T1, Effective Date: 14/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[8849,"MURRAYLINKV5_20211201203644","2015-07-22T08:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-305.23984000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8859,"MURRAYLINKV5_20211201203644","2015-07-22T09:30:00","#R012621_004_RAMP_V","#R012621_RAMP","2015-07-22",1,-21.666260000000001,"Soft Ramping constraint for constraint V>X_NWCB6022+6023_T1, Effective Date: 14/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[8868,"MURRAYLINKV5_20211201203644","2015-07-22T10:35:00","#R012622_004_RAMP_V","#R012622_RAMP","2015-07-22",1,-21.098939999999999,"Soft Ramping constraint for constraint V>X_NWCB6022+6023_T1, Effective Date: 14/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[8877,"MURRAYLINKV5_20211201203644","2015-07-22T11:00:00","#R012622_004_RAMP_F","#R012622_RAMP","2015-07-22",1,-49.428849999999997,"Hard Ramping constraint for constraint V>X_NWCB6022+6023_T1, Effective Date: 14/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[8887,"MURRAYLINKV5_20211201203644","2015-07-22T11:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-52.276389999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8891,"MURRAYLINKV5_20211201203644","2015-07-22T12:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-22.93918,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8898,"MURRAYLINKV5_20211201203644","2015-07-22T12:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-22.303889999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8909,"MURRAYLINKV5_20211201203644","2015-07-22T13:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-21.555,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8917,"MURRAYLINKV5_20211201203644","2015-07-22T14:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.811630000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8927,"MURRAYLINKV5_20211201203644","2015-07-22T14:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.523599999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8936,"MURRAYLINKV5_20211201203644","2015-07-22T15:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-21.94689,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8945,"MURRAYLINKV5_20211201203644","2015-07-22T16:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-17.373519999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8956,"MURRAYLINKV5_20211201203644","2015-07-22T17:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-38.124630000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8964,"MURRAYLINKV5_20211201203644","2015-07-22T18:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-203.51297,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8965,"MURRAYLINKV5_20211201203644","2015-07-22T18:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-31.72007,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8975,"MURRAYLINKV5_20211201203644","2015-07-22T19:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-221.51981000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8983,"MURRAYLINKV5_20211201203644","2015-07-22T20:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-34.909230000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[8994,"MURRAYLINKV5_20211201203644","2015-07-22T21:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-49.805199999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9006,"MURRAYLINKV5_20211201203644","2015-07-22T22:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-51.477649999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9013,"MURRAYLINKV5_20211201203644","2015-07-22T22:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-24.65935,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9024,"MURRAYLINKV5_20211201203644","2015-07-23T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-19.424710000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9032,"MURRAYLINKV5_20211201203644","2015-07-23T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.173439999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9033,"MURRAYLINKV5_20211201203644","2015-07-23T00:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-52.210140000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9043,"MURRAYLINKV5_20211201203644","2015-07-23T01:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-22.80423,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9052,"MURRAYLINKV5_20211201203644","2015-07-23T01:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-20.294239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9062,"MURRAYLINKV5_20211201203644","2015-07-23T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-19.656600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9071,"MURRAYLINKV5_20211201203644","2015-07-23T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.053570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9080,"MURRAYLINKV5_20211201203644","2015-07-23T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.57156,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9090,"MURRAYLINKV5_20211201203644","2015-07-23T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.229889999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9098,"MURRAYLINKV5_20211201203644","2015-07-23T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.079599999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9101,"MURRAYLINKV5_20211201203644","2015-07-23T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.75863,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9112,"MURRAYLINKV5_20211201203644","2015-07-23T07:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-11.505089999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9120,"MURRAYLINKV5_20211201203644","2015-07-23T08:30:00","#R012631_002_RAMP_V","#R012631_RAMP","2015-07-23",1,-34.671700000000001,"Soft Ramping constraint for constraint V>S_CB6024+6023_TX1, Effective Date: 17/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[9130,"MURRAYLINKV5_20211201203644","2015-07-23T09:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-36.47428,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9139,"MURRAYLINKV5_20211201203644","2015-07-23T10:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-18.338809999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9148,"MURRAYLINKV5_20211201203644","2015-07-23T10:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-21.08455,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9158,"MURRAYLINKV5_20211201203644","2015-07-23T12:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-50.196550000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9166,"MURRAYLINKV5_20211201203644","2015-07-23T15:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-10.959860000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9169,"MURRAYLINKV5_20211201203644","2015-07-23T15:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.444990000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9178,"MURRAYLINKV5_20211201203644","2015-07-23T16:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-49.555349999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9186,"MURRAYLINKV5_20211201203644","2015-07-23T16:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-49.905929999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9197,"MURRAYLINKV5_20211201203644","2015-07-23T19:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-10.20012,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9204,"MURRAYLINKV5_20211201203644","2015-07-23T19:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-237.89852999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9216,"MURRAYLINKV5_20211201203644","2015-07-23T20:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-50.928739999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9227,"MURRAYLINKV5_20211201203644","2015-07-23T21:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-54.666469999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9235,"MURRAYLINKV5_20211201203644","2015-07-23T22:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-37.537529999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9236,"MURRAYLINKV5_20211201203644","2015-07-23T22:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.1076,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9246,"MURRAYLINKV5_20211201203644","2015-07-24","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.09206,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9254,"MURRAYLINKV5_20211201203644","2015-07-24T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.24188,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9265,"MURRAYLINKV5_20211201203644","2015-07-24T04:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.5166,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9272,"MURRAYLINKV5_20211201203644","2015-07-24T11:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.67952,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9284,"MURRAYLINKV5_20211201203644","2015-07-24T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.133570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9293,"MURRAYLINKV5_20211201203644","2015-07-24T12:30:00","S>NWCB6022+23+24_TX2","S-NW_CB22+23+24","2015-07-23",1,-46.921140000000001,"Out =North West Bend 132kV CB6022 & CB6023 & CB6024 (this offloads Monash-NWB #2 132kV line and NWB-MWP1 132kV line);  avoid O/L of North West Bend 132/66kV transformer #2  on trip of North West Bend 132/66kV transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9301,"MURRAYLINKV5_20211201203644","2015-07-24T12:50:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-50.027679999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9304,"MURRAYLINKV5_20211201203644","2015-07-24T12:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.077959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9319,"MURRAYLINKV5_20211201203644","2015-07-24T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.038040000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9323,"MURRAYLINKV5_20211201203644","2015-07-24T14:00:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-53.784990000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9333,"MURRAYLINKV5_20211201203644","2015-07-24T14:50:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-49.580820000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9342,"MURRAYLINKV5_20211201203644","2015-07-24T23:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.73832,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9351,"MURRAYLINKV5_20211201203644","2015-07-24T23:35:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-65.254390000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9361,"MURRAYLINKV5_20211201203644","2015-07-25T00:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.173439999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9369,"MURRAYLINKV5_20211201203644","2015-07-25T02:05:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.83404,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9372,"MURRAYLINKV5_20211201203644","2015-07-25T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.112209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9387,"MURRAYLINKV5_20211201203644","2015-07-25T03:30:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-15.877280000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9391,"MURRAYLINKV5_20211201203644","2015-07-25T03:55:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-16.65391,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9401,"MURRAYLINKV5_20211201203644","2015-07-25T05:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.155799999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9410,"MURRAYLINKV5_20211201203644","2015-07-25T05:35:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-12.30354,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9419,"MURRAYLINKV5_20211201203644","2015-07-25T09:35:00","#R012641_002_RAMP_F","#R012641_RAMP","2015-07-25",1,-358800,"Hard Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[9430,"MURRAYLINKV5_20211201203644","2015-07-25T10:05:00","#R012641_002_RAMP_F","#R012641_RAMP","2015-07-25",1,-358800,"Hard Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[9438,"MURRAYLINKV5_20211201203644","2015-07-25T11:25:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-47.924169999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9439,"MURRAYLINKV5_20211201203644","2015-07-25T11:35:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-46.260640000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9449,"MURRAYLINKV5_20211201203644","2015-07-25T12:35:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-46.708019999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9457,"MURRAYLINKV5_20211201203644","2015-07-25T13:15:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-44.130339999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9468,"MURRAYLINKV5_20211201203644","2015-07-25T14:10:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-43.957500000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9475,"MURRAYLINKV5_20211201203644","2015-07-25T14:45:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-43.960149999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9487,"MURRAYLINKV5_20211201203644","2015-07-25T15:45:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-45.581220000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9493,"MURRAYLINKV5_20211201203644","2015-07-25T16:15:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-45.980420000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9506,"MURRAYLINKV5_20211201203644","2015-07-25T17:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.575810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9507,"MURRAYLINKV5_20211201203644","2015-07-25T17:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.32555,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9517,"MURRAYLINKV5_20211201203644","2015-07-25T19:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.17747,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9526,"MURRAYLINKV5_20211201203644","2015-07-25T20:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.24471,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9536,"MURRAYLINKV5_20211201203644","2015-07-25T22:05:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-12.836980000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9545,"MURRAYLINKV5_20211201203644","2015-07-25T22:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.31203,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9554,"MURRAYLINKV5_20211201203644","2015-07-26T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.563289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9564,"MURRAYLINKV5_20211201203644","2015-07-26T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.5876,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9572,"MURRAYLINKV5_20211201203644","2015-07-26T02:00:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-11.22301,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9575,"MURRAYLINKV5_20211201203644","2015-07-26T02:10:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.27139,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9590,"MURRAYLINKV5_20211201203644","2015-07-26T04:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-33.976460000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9594,"MURRAYLINKV5_20211201203644","2015-07-26T04:25:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-42.425409999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9608,"MURRAYLINKV5_20211201203644","2015-07-26T05:30:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-19.782720000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9613,"MURRAYLINKV5_20211201203644","2015-07-26T05:55:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-14.06113,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9622,"MURRAYLINKV5_20211201203644","2015-07-26T07:55:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.693530000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9632,"MURRAYLINKV5_20211201203644","2015-07-26T08:25:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.54738,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9641,"MURRAYLINKV5_20211201203644","2015-07-26T08:55:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-11.22176,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9642,"MURRAYLINKV5_20211201203644","2015-07-26T08:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.709199999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9652,"MURRAYLINKV5_20211201203644","2015-07-26T09:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.868930000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9660,"MURRAYLINKV5_20211201203644","2015-07-26T09:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.704050000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9671,"MURRAYLINKV5_20211201203644","2015-07-26T10:25:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.000999999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9678,"MURRAYLINKV5_20211201203644","2015-07-26T13:10:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-19.579090000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9690,"MURRAYLINKV5_20211201203644","2015-07-26T15:30:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-10.540469999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9696,"MURRAYLINKV5_20211201203644","2015-07-26T18:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-13.64758,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9709,"MURRAYLINKV5_20211201203644","2015-07-26T19:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-46.593600000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9710,"MURRAYLINKV5_20211201203644","2015-07-26T19:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-46.945039999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9720,"MURRAYLINKV5_20211201203644","2015-07-26T20:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-49.699440000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9728,"MURRAYLINKV5_20211201203644","2015-07-26T20:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-49.156889999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9739,"MURRAYLINKV5_20211201203644","2015-07-26T21:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-52.31409,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9746,"MURRAYLINKV5_20211201203644","2015-07-26T22:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-23.4132,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9758,"MURRAYLINKV5_20211201203644","2015-07-26T22:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-32.77393,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9767,"MURRAYLINKV5_20211201203644","2015-07-27","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.78059,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9775,"MURRAYLINKV5_20211201203644","2015-07-27T00:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-29.465979999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9778,"MURRAYLINKV5_20211201203644","2015-07-27T00:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.419739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9793,"MURRAYLINKV5_20211201203644","2015-07-27T01:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-33.75121,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9797,"MURRAYLINKV5_20211201203644","2015-07-27T01:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-23.61693,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9811,"MURRAYLINKV5_20211201203644","2015-07-27T02:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-35.238869999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9816,"MURRAYLINKV5_20211201203644","2015-07-27T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.664720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9825,"MURRAYLINKV5_20211201203644","2015-07-27T02:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-37.890079999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9835,"MURRAYLINKV5_20211201203644","2015-07-27T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.54688,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9843,"MURRAYLINKV5_20211201203644","2015-07-27T03:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.237590000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9846,"MURRAYLINKV5_20211201203644","2015-07-27T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.172840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9861,"MURRAYLINKV5_20211201203644","2015-07-27T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.93207,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9865,"MURRAYLINKV5_20211201203644","2015-07-27T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.775230000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9874,"MURRAYLINKV5_20211201203644","2015-07-27T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.151859999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9881,"MURRAYLINKV5_20211201203644","2015-07-27T05:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-34.445889999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9893,"MURRAYLINKV5_20211201203644","2015-07-27T06:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-57.239730000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9899,"MURRAYLINKV5_20211201203644","2015-07-27T06:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-54.941020000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9912,"MURRAYLINKV5_20211201203644","2015-07-27T07:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-123.94428000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9917,"MURRAYLINKV5_20211201203644","2015-07-27T08:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-122.72487,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9923,"MURRAYLINKV5_20211201203644","2015-07-27T08:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-121.42688,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9931,"MURRAYLINKV5_20211201203644","2015-07-27T09:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-122.25712,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9942,"MURRAYLINKV5_20211201203644","2015-07-27T10:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-295.80721999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9949,"MURRAYLINKV5_20211201203644","2015-07-27T10:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-78.722499999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9961,"MURRAYLINKV5_20211201203644","2015-07-27T11:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-82.96593,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9967,"MURRAYLINKV5_20211201203644","2015-07-27T12:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.252279999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9980,"MURRAYLINKV5_20211201203644","2015-07-27T13:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-84.095889999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9985,"MURRAYLINKV5_20211201203644","2015-07-27T13:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-83.465729999999994,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[9991,"MURRAYLINKV5_20211201203644","2015-07-27T14:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-80.629289999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10000,"MURRAYLINKV5_20211201203644","2015-07-27T15:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-79.967519999999993,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10014,"MURRAYLINKV5_20211201203644","2015-07-27T16:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-80.092219999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10019,"MURRAYLINKV5_20211201203644","2015-07-27T16:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-78.722530000000006,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10023,"MURRAYLINKV5_20211201203644","2015-07-27T16:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-76.287279999999996,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10038,"MURRAYLINKV5_20211201203644","2015-07-27T19:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-32.258389999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10046,"MURRAYLINKV5_20211201203644","2015-07-27T20:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-72.687870000000004,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10049,"MURRAYLINKV5_20211201203644","2015-07-27T20:15:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-71.746629999999996,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10064,"MURRAYLINKV5_20211201203644","2015-07-27T21:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-79.781710000000004,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10068,"MURRAYLINKV5_20211201203644","2015-07-27T21:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-80.464939999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10082,"MURRAYLINKV5_20211201203644","2015-07-27T22:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.18994,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10087,"MURRAYLINKV5_20211201203644","2015-07-27T22:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-82.281949999999995,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10091,"MURRAYLINKV5_20211201203644","2015-07-27T23:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-83.601870000000005,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10106,"MURRAYLINKV5_20211201203644","2015-07-28T00:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-19.172989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10115,"MURRAYLINKV5_20211201203644","2015-07-28T00:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-237.31424999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10120,"MURRAYLINKV5_20211201203644","2015-07-28T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-19.529019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10126,"MURRAYLINKV5_20211201203644","2015-07-28T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.546519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10138,"MURRAYLINKV5_20211201203644","2015-07-28T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.418340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10145,"MURRAYLINKV5_20211201203644","2015-07-28T01:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-129.95925,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10152,"MURRAYLINKV5_20211201203644","2015-07-28T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.725630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10164,"MURRAYLINKV5_20211201203644","2015-07-28T02:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-59.95955,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10170,"MURRAYLINKV5_20211201203644","2015-07-28T03:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-58.73245,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10183,"MURRAYLINKV5_20211201203644","2015-07-28T03:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-62.048940000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10188,"MURRAYLINKV5_20211201203644","2015-07-28T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.515789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10194,"MURRAYLINKV5_20211201203644","2015-07-28T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.705760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10206,"MURRAYLINKV5_20211201203644","2015-07-28T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-21.815249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10213,"MURRAYLINKV5_20211201203644","2015-07-28T05:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-53.014859999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10220,"MURRAYLINKV5_20211201203644","2015-07-28T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.847479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10232,"MURRAYLINKV5_20211201203644","2015-07-28T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.881019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10241,"MURRAYLINKV5_20211201203644","2015-07-28T06:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-52.160330000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10244,"MURRAYLINKV5_20211201203644","2015-07-28T06:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-35.903979999999997,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10252,"MURRAYLINKV5_20211201203644","2015-07-28T07:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-62.289169999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10267,"MURRAYLINKV5_20211201203644","2015-07-28T09:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-69.544160000000005,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10271,"MURRAYLINKV5_20211201203644","2015-07-28T09:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-75.728700000000003,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10285,"MURRAYLINKV5_20211201203644","2015-07-28T10:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-295.80725999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10290,"MURRAYLINKV5_20211201203644","2015-07-28T11:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-82.334540000000004,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10294,"MURRAYLINKV5_20211201203644","2015-07-28T11:25:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-301.59064000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10309,"MURRAYLINKV5_20211201203644","2015-07-28T12:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.106539999999995,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10312,"MURRAYLINKV5_20211201203644","2015-07-28T12:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-301.92777999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10320,"MURRAYLINKV5_20211201203644","2015-07-28T13:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.050389999999993,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10335,"MURRAYLINKV5_20211201203644","2015-07-28T14:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.010210000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10339,"MURRAYLINKV5_20211201203644","2015-07-28T15:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.076539999999994,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10348,"MURRAYLINKV5_20211201203644","2015-07-28T15:55:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-81.259429999999995,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10359,"MURRAYLINKV5_20211201203644","2015-07-28T16:50:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-295.74027000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10367,"MURRAYLINKV5_20211201203644","2015-07-28T17:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-24.164760000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10373,"MURRAYLINKV5_20211201203644","2015-07-28T19:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-246.62952000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10386,"MURRAYLINKV5_20211201203644","2015-07-28T21:05:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-67.300430000000006,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10391,"MURRAYLINKV5_20211201203644","2015-07-28T21:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-78.722480000000004,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10397,"MURRAYLINKV5_20211201203644","2015-07-28T22:00:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-51.230730000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10409,"MURRAYLINKV5_20211201203644","2015-07-28T23:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.6546,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10416,"MURRAYLINKV5_20211201203644","2015-07-29T00:20:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-50.363050000000001,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10427,"MURRAYLINKV5_20211201203644","2015-07-29T04:45:00","S>X_NWCB6022+6023_T2","S-NWCB6022+6023","2015-07-14",1,-12.09094,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line); limit SA to Victoria flow on Murraylink to avoid North West Bend transformer #2 O/L on trip NWB 132/66kV Transformer #3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10435,"MURRAYLINKV5_20211201203644","2015-07-29T10:35:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-20.896350000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10441,"MURRAYLINKV5_20211201203644","2015-07-29T11:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-11.771979999999999,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10454,"MURRAYLINKV5_20211201203644","2015-07-29T12:45:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-12.48114,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10459,"MURRAYLINKV5_20211201203644","2015-07-29T13:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-50.816769999999998,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10465,"MURRAYLINKV5_20211201203644","2015-07-29T13:40:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-22.13026,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10474,"MURRAYLINKV5_20211201203644","2015-07-29T16:30:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-10.43038,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10488,"MURRAYLINKV5_20211201203644","2015-07-30T01:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.767010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10493,"MURRAYLINKV5_20211201203644","2015-07-30T02:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.02397,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10497,"MURRAYLINKV5_20211201203644","2015-07-30T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.83056,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10512,"MURRAYLINKV5_20211201203644","2015-07-30T04:40:00","#R012661_001_RAMP_V","#R012661_RAMP","2015-07-30",1,-11.64133,"Soft Ramping constraint for constraint SVML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[10515,"MURRAYLINKV5_20211201203644","2015-07-30T04:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.015739999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10523,"MURRAYLINKV5_20211201203644","2015-07-30T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.53247,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10533,"MURRAYLINKV5_20211201203644","2015-07-31T00:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-18",1,-10.42854,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10542,"MURRAYLINKV5_20211201203644","2015-07-31T00:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-18",1,-12.77417,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10556,"MURRAYLINKV5_20211201203644","2015-07-31T01:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.812569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10561,"MURRAYLINKV5_20211201203644","2015-07-31T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.46697,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10565,"MURRAYLINKV5_20211201203644","2015-07-31T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.88139,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10580,"MURRAYLINKV5_20211201203644","2015-07-31T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.401350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10589,"MURRAYLINKV5_20211201203644","2015-07-31T05:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11.512040000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10594,"MURRAYLINKV5_20211201203644","2015-07-31T06:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-10.70787,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10600,"MURRAYLINKV5_20211201203644","2015-07-31T08:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-05",1,-79.818539999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10612,"MURRAYLINKV5_20211201203644","2015-08-01T00:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.74006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10619,"MURRAYLINKV5_20211201203644","2015-08-01T01:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.11612,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10630,"MURRAYLINKV5_20211201203644","2015-08-01T01:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-24.402799999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10638,"MURRAYLINKV5_20211201203644","2015-08-01T02:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.222159999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10644,"MURRAYLINKV5_20211201203644","2015-08-01T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.29617,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10657,"MURRAYLINKV5_20211201203644","2015-08-01T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.1594,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10662,"MURRAYLINKV5_20211201203644","2015-08-01T03:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-19.37236,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10668,"MURRAYLINKV5_20211201203644","2015-08-01T03:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-22.005299999999998,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10680,"MURRAYLINKV5_20211201203644","2015-08-01T03:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-18.396190000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10687,"MURRAYLINKV5_20211201203644","2015-08-01T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.33888,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10696,"MURRAYLINKV5_20211201203644","2015-08-01T13:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11987.48718,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10700,"MURRAYLINKV5_20211201203644","2015-08-02T01:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.509080000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10715,"MURRAYLINKV5_20211201203644","2015-08-02T12:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-39.477460000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10718,"MURRAYLINKV5_20211201203644","2015-08-02T12:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-14.87547,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10726,"MURRAYLINKV5_20211201203644","2015-08-03T00:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.73227,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10736,"MURRAYLINKV5_20211201203644","2015-08-03T01:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.444559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10745,"MURRAYLINKV5_20211201203644","2015-08-03T02:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-11.148569999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10759,"MURRAYLINKV5_20211201203644","2015-08-03T03:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.004300000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10764,"MURRAYLINKV5_20211201203644","2015-08-03T03:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-30.101790000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10768,"MURRAYLINKV5_20211201203644","2015-08-03T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.66761,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10783,"MURRAYLINKV5_20211201203644","2015-08-03T05:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.140140000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10786,"MURRAYLINKV5_20211201203644","2015-08-03T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.42536,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10794,"MURRAYLINKV5_20211201203644","2015-08-03T05:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.466570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10804,"MURRAYLINKV5_20211201203644","2015-08-03T09:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-05",1,-38.560769999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10813,"MURRAYLINKV5_20211201203644","2015-08-03T20:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-03",1,-35.653910000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10822,"MURRAYLINKV5_20211201203644","2015-08-04T01:45:00","V>SML_NWRB_NWMWP1","S-NWRB","2015-03-23",1,-40.509039999999999,"Out=NWB - Robertstown 132kV #1 line, limit flow on ML to avoid OL North West Bend- MWP1 132 kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10833,"MURRAYLINKV5_20211201203644","2015-08-04T08:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-03",1,-42.245519999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10841,"MURRAYLINKV5_20211201203644","2015-08-04T08:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-03",1,-49.927390000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10851,"MURRAYLINKV5_20211201203644","2015-08-04T10:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-13.38456,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10860,"MURRAYLINKV5_20211201203644","2015-08-04T10:45:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-21.089490000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10865,"MURRAYLINKV5_20211201203644","2015-08-04T11:10:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-17.284790000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10871,"MURRAYLINKV5_20211201203644","2015-08-04T11:45:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-19.095130000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10883,"MURRAYLINKV5_20211201203644","2015-08-04T17:10:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-82.918729999999996,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10890,"MURRAYLINKV5_20211201203644","2015-08-04T23:25:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-11.90143,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10901,"MURRAYLINKV5_20211201203644","2015-08-05T00:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.6448,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10909,"MURRAYLINKV5_20211201203644","2015-08-05T01:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.39879,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10919,"MURRAYLINKV5_20211201203644","2015-08-05T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.565390000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10928,"MURRAYLINKV5_20211201203644","2015-08-05T02:00:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-17.915430000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10929,"MURRAYLINKV5_20211201203644","2015-08-05T02:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-18.152979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10939,"MURRAYLINKV5_20211201203644","2015-08-05T02:30:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-18.2196,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10948,"MURRAYLINKV5_20211201203644","2015-08-05T02:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-13.49701,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10957,"MURRAYLINKV5_20211201203644","2015-08-05T03:15:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-12.84582,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10967,"MURRAYLINKV5_20211201203644","2015-08-05T03:40:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-19.43366,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10971,"MURRAYLINKV5_20211201203644","2015-08-05T03:50:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-19.3339,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10986,"MURRAYLINKV5_20211201203644","2015-08-05T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.1609,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10989,"MURRAYLINKV5_20211201203644","2015-08-05T04:35:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-19.305289999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[10997,"MURRAYLINKV5_20211201203644","2015-08-05T04:55:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-20.468050000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11007,"MURRAYLINKV5_20211201203644","2015-08-05T05:20:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-23.63447,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11016,"MURRAYLINKV5_20211201203644","2015-08-05T05:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.828019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11025,"MURRAYLINKV5_20211201203644","2015-08-05T07:45:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-10.51498,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11035,"MURRAYLINKV5_20211201203644","2015-08-05T21:55:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-297.69792000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11039,"MURRAYLINKV5_20211201203644","2015-08-06T01:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-52.300699999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11054,"MURRAYLINKV5_20211201203644","2015-08-06T02:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.88294,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11063,"MURRAYLINKV5_20211201203644","2015-08-06T03:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.82413,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11072,"MURRAYLINKV5_20211201203644","2015-08-06T04:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-17.87828,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11074,"MURRAYLINKV5_20211201203644","2015-08-06T04:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.493729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11086,"MURRAYLINKV5_20211201203644","2015-08-06T06:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-30.316680000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11093,"MURRAYLINKV5_20211201203644","2015-08-06T08:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-35.961869999999998,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11104,"MURRAYLINKV5_20211201203644","2015-08-06T09:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-03",1,-42.568989999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11112,"MURRAYLINKV5_20211201203644","2015-08-06T10:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-42.06174,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11122,"MURRAYLINKV5_20211201203644","2015-08-06T11:25:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-21.946840000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11131,"MURRAYLINKV5_20211201203644","2015-08-06T12:20:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-45.67971,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11140,"MURRAYLINKV5_20211201203644","2015-08-06T13:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-76.786919999999995,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11142,"MURRAYLINKV5_20211201203644","2015-08-06T13:15:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-47.620980000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11154,"MURRAYLINKV5_20211201203644","2015-08-06T14:15:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-18.26051,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11161,"MURRAYLINKV5_20211201203644","2015-08-06T14:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-18.86984,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11170,"MURRAYLINKV5_20211201203644","2015-08-06T15:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-18.547219999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11178,"MURRAYLINKV5_20211201203644","2015-08-06T21:40:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-10.093070000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11189,"MURRAYLINKV5_20211201203644","2015-08-06T23:45:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-239.00897000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11192,"MURRAYLINKV5_20211201203644","2015-08-07T01:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-10.57939,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11200,"MURRAYLINKV5_20211201203644","2015-08-07T01:40:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-21.076070000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11210,"MURRAYLINKV5_20211201203644","2015-08-07T02:30:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-24.460730000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11219,"MURRAYLINKV5_20211201203644","2015-08-07T03:15:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-24.227509999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11228,"MURRAYLINKV5_20211201203644","2015-08-07T04:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-16.081060000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11238,"MURRAYLINKV5_20211201203644","2015-08-07T04:55:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-12.76108,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11246,"MURRAYLINKV5_20211201203644","2015-08-07T08:40:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-28.99203,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11257,"MURRAYLINKV5_20211201203644","2015-08-07T10:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-20.442350000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11260,"MURRAYLINKV5_20211201203644","2015-08-07T11:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-18.025680000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11268,"MURRAYLINKV5_20211201203644","2015-08-07T12:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-18.17595,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11278,"MURRAYLINKV5_20211201203644","2015-08-07T12:55:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-50.829680000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11287,"MURRAYLINKV5_20211201203644","2015-08-07T13:40:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-50.79618,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11296,"MURRAYLINKV5_20211201203644","2015-08-07T14:25:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-49.274569999999997,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11307,"MURRAYLINKV5_20211201203644","2015-08-07T15:20:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-21.338940000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11315,"MURRAYLINKV5_20211201203644","2015-08-07T16:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-47.817239999999998,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11325,"MURRAYLINKV5_20211201203644","2015-08-07T16:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-16.21012,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11334,"MURRAYLINKV5_20211201203644","2015-08-07T17:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-37.951120000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11343,"MURRAYLINKV5_20211201203644","2015-08-07T20:30:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-15.66539,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11345,"MURRAYLINKV5_20211201203644","2015-08-07T20:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-10.961209999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11352,"MURRAYLINKV5_20211201203644","2015-08-07T21:25:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-20.175149999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11364,"MURRAYLINKV5_20211201203644","2015-08-07T22:40:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-10.008089999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11375,"MURRAYLINKV5_20211201203644","2015-08-08T00:30:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-19.281140000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11383,"MURRAYLINKV5_20211201203644","2015-08-08T01:15:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-20.896039999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11393,"MURRAYLINKV5_20211201203644","2015-08-08T02:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-13.43272,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11402,"MURRAYLINKV5_20211201203644","2015-08-08T02:55:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-15.19028,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11403,"MURRAYLINKV5_20211201203644","2015-08-08T03:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-14.46152,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11413,"MURRAYLINKV5_20211201203644","2015-08-09T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.783440000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11422,"MURRAYLINKV5_20211201203644","2015-08-09T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.841329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11431,"MURRAYLINKV5_20211201203644","2015-08-09T04:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.240460000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11441,"MURRAYLINKV5_20211201203644","2015-08-09T04:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.22322,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11449,"MURRAYLINKV5_20211201203644","2015-08-09T05:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.90771,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11460,"MURRAYLINKV5_20211201203644","2015-08-09T05:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.697190000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11467,"MURRAYLINKV5_20211201203644","2015-08-09T05:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.03529,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11471,"MURRAYLINKV5_20211201203644","2015-08-09T06:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.4884,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11481,"MURRAYLINKV5_20211201203644","2015-08-09T06:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.64939,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11490,"MURRAYLINKV5_20211201203644","2015-08-09T11:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.19197,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11499,"MURRAYLINKV5_20211201203644","2015-08-09T12:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.29081,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11509,"MURRAYLINKV5_20211201203644","2015-08-09T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.39293,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11517,"MURRAYLINKV5_20211201203644","2015-08-09T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.12,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11528,"MURRAYLINKV5_20211201203644","2015-08-10T00:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.47683,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11537,"MURRAYLINKV5_20211201203644","2015-08-10T00:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.34595,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11546,"MURRAYLINKV5_20211201203644","2015-08-10T01:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-15.380940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11548,"MURRAYLINKV5_20211201203644","2015-08-10T01:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-16.82865,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11555,"MURRAYLINKV5_20211201203644","2015-08-10T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.493840000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11567,"MURRAYLINKV5_20211201203644","2015-08-10T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.930149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11573,"MURRAYLINKV5_20211201203644","2015-08-11T00:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.48278,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11586,"MURRAYLINKV5_20211201203644","2015-08-12T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-12.01953,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11596,"MURRAYLINKV5_20211201203644","2015-08-12T08:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-29.158719999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11605,"MURRAYLINKV5_20211201203644","2015-08-12T15:20:00","#R012713_003_RAMP_F","#R012713_RAMP","2015-08-12",1,-51.207180000000001,"Hard Ramping constraint for constraint S>>PATW_BWPA_TPRS, Effective Date: 30/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[11614,"MURRAYLINKV5_20211201203644","2015-08-12T15:40:00","#R012713_003_RAMP_F","#R012713_RAMP","2015-08-12",1,-57.870280000000001,"Hard Ramping constraint for constraint S>>PATW_BWPA_TPRS, Effective Date: 30/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[11616,"MURRAYLINKV5_20211201203644","2015-08-12T15:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-24.188140000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11623,"MURRAYLINKV5_20211201203644","2015-08-12T18:40:00","S>>NIL_RBTU_WEWT","S-NIL","2015-08-11",1,-31.90399,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11635,"MURRAYLINKV5_20211201203644","2015-08-13T01:50:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-11.682589999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11644,"MURRAYLINKV5_20211201203644","2015-08-14T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.162520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11652,"MURRAYLINKV5_20211201203644","2015-08-15T23:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-06-18",1,-12.514620000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11663,"MURRAYLINKV5_20211201203644","2015-08-16T15:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-14",1,-10.7491,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11670,"MURRAYLINKV5_20211201203644","2015-08-16T16:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-14",1,-10.678940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11674,"MURRAYLINKV5_20211201203644","2015-08-16T19:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-478.18693000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11684,"MURRAYLINKV5_20211201203644","2015-08-16T20:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.44665,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11693,"MURRAYLINKV5_20211201203644","2015-08-16T21:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.94248,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11702,"MURRAYLINKV5_20211201203644","2015-08-16T22:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-20.305520000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11712,"MURRAYLINKV5_20211201203644","2015-08-16T23:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-13",1,-34.107460000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11720,"MURRAYLINKV5_20211201203644","2015-08-17T00:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.80739,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11731,"MURRAYLINKV5_20211201203644","2015-08-17T01:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-20.547149999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11738,"MURRAYLINKV5_20211201203644","2015-08-17T01:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-14",1,-14.886990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11742,"MURRAYLINKV5_20211201203644","2015-08-17T01:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-16.64592,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11751,"MURRAYLINKV5_20211201203644","2015-08-17T02:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-16.85952,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11758,"MURRAYLINKV5_20211201203644","2015-08-17T04:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-12.910080000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11770,"MURRAYLINKV5_20211201203644","2015-08-18T02:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-13.21036,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11776,"MURRAYLINKV5_20211201203644","2015-08-18T08:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-55.659990000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11789,"MURRAYLINKV5_20211201203644","2015-08-19T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.91872,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11799,"MURRAYLINKV5_20211201203644","2015-08-20T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-14",1,-16.256329999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11808,"MURRAYLINKV5_20211201203644","2015-08-22T14:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-07-01",1,-10.88852,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11817,"MURRAYLINKV5_20211201203644","2015-08-24T14:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-14",1,-11.459009999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11819,"MURRAYLINKV5_20211201203644","2015-08-24T22:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.06987,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11826,"MURRAYLINKV5_20211201203644","2015-08-25T23:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.64151,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11838,"MURRAYLINKV5_20211201203644","2015-08-26T06:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11.5412,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11844,"MURRAYLINKV5_20211201203644","2015-08-26T14:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11.976179999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11857,"MURRAYLINKV5_20211201203644","2015-08-27T04:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-40.328800000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11867,"MURRAYLINKV5_20211201203644","2015-08-27T04:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-40.040869999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11876,"MURRAYLINKV5_20211201203644","2015-08-27T05:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-115.21014,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11877,"MURRAYLINKV5_20211201203644","2015-08-27T05:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-33.774120000000003,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11891,"MURRAYLINKV5_20211201203644","2015-08-27T10:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-14.998049999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11896,"MURRAYLINKV5_20211201203644","2015-08-28T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.493119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11905,"MURRAYLINKV5_20211201203644","2015-08-29T01:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.452390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11915,"MURRAYLINKV5_20211201203644","2015-08-29T03:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-19.57037,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11923,"MURRAYLINKV5_20211201203644","2015-08-29T03:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-24.539110000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11934,"MURRAYLINKV5_20211201203644","2015-08-29T04:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.353159999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11941,"MURRAYLINKV5_20211201203644","2015-08-29T05:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.6663,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11945,"MURRAYLINKV5_20211201203644","2015-08-29T05:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.4351,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11959,"MURRAYLINKV5_20211201203644","2015-08-31T05:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-14.854179999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11964,"MURRAYLINKV5_20211201203644","2015-08-31T08:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-14.78398,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11973,"MURRAYLINKV5_20211201203644","2015-09-01T08:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-11.557510000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11983,"MURRAYLINKV5_20211201203644","2015-09-01T15:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-07",1,-14.90607,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11992,"MURRAYLINKV5_20211201203644","2015-09-02T23:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.75163,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[11997,"MURRAYLINKV5_20211201203644","2015-09-03T11:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-20.389949999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12011,"MURRAYLINKV5_20211201203644","2015-09-03T21:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-19.33351,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12020,"MURRAYLINKV5_20211201203644","2015-09-04T00:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.75057,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12022,"MURRAYLINKV5_20211201203644","2015-09-04T00:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.613759999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12029,"MURRAYLINKV5_20211201203644","2015-09-04T04:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-29.678550000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12041,"MURRAYLINKV5_20211201203644","2015-09-04T05:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-47.90551,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12047,"MURRAYLINKV5_20211201203644","2015-09-04T06:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-28.826509999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12060,"MURRAYLINKV5_20211201203644","2015-09-04T07:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-169.00949,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12065,"MURRAYLINKV5_20211201203644","2015-09-04T08:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-249.72219999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12079,"MURRAYLINKV5_20211201203644","2015-09-04T09:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-32.053640000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12088,"MURRAYLINKV5_20211201203644","2015-09-04T10:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-249.01647,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12090,"MURRAYLINKV5_20211201203644","2015-09-04T10:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-194.44755000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12097,"MURRAYLINKV5_20211201203644","2015-09-04T10:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-122.33804000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12109,"MURRAYLINKV5_20211201203644","2015-09-04T11:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-189.57339999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12118,"MURRAYLINKV5_20211201203644","2015-09-04T12:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-136.95043000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12126,"MURRAYLINKV5_20211201203644","2015-09-04T13:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-56.323070000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12137,"MURRAYLINKV5_20211201203644","2015-09-04T14:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-94.815190000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12144,"MURRAYLINKV5_20211201203644","2015-09-04T14:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-88.885540000000006,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12148,"MURRAYLINKV5_20211201203644","2015-09-04T14:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-89.58869,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12162,"MURRAYLINKV5_20211201203644","2015-09-04T16:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-194.29957999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12167,"MURRAYLINKV5_20211201203644","2015-09-04T17:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-188.99538000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12180,"MURRAYLINKV5_20211201203644","2015-09-04T20:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-10.720039999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12186,"MURRAYLINKV5_20211201203644","2015-09-04T23:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.029529999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12194,"MURRAYLINKV5_20211201203644","2015-09-05T10:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-10.841049999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12205,"MURRAYLINKV5_20211201203644","2015-09-05T20:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-36.985309999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12212,"MURRAYLINKV5_20211201203644","2015-09-05T21:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.132809999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12216,"MURRAYLINKV5_20211201203644","2015-09-05T21:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.139620000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12225,"MURRAYLINKV5_20211201203644","2015-09-05T23:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.41892,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12232,"MURRAYLINKV5_20211201203644","2015-09-07T05:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.299250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12244,"MURRAYLINKV5_20211201203644","2015-09-07T19:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-18.799790000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12250,"MURRAYLINKV5_20211201203644","2015-09-07T19:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-12.717460000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12263,"MURRAYLINKV5_20211201203644","2015-09-07T21:10:00","S>>NIL_RBTU_WEWT","S-NIL","2015-08-11",1,-37.897069999999999,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12268,"MURRAYLINKV5_20211201203644","2015-09-07T21:45:00","S>>NIL_RBTU_WEWT","S-NIL","2015-08-11",1,-14.86661,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12282,"MURRAYLINKV5_20211201203644","2015-09-08T08:55:00","#R012837_002_RAMP_F","#R012837_RAMP","2015-09-08",1,-38.85,"Hard Ramping constraint for constraint V>S_CB6033+6225_TX1, Effective Date: 21/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12286,"MURRAYLINKV5_20211201203644","2015-09-08T09:05:00","#R012837_002_RAMP_F","#R012837_RAMP","2015-09-08",1,-38.37811,"Hard Ramping constraint for constraint V>S_CB6033+6225_TX1, Effective Date: 21/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12293,"MURRAYLINKV5_20211201203644","2015-09-08T09:25:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-224.79777999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12300,"MURRAYLINKV5_20211201203644","2015-09-08T10:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-230.33347000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12312,"MURRAYLINKV5_20211201203644","2015-09-08T11:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-47.964080000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12318,"MURRAYLINKV5_20211201203644","2015-09-08T11:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-43.551920000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12331,"MURRAYLINKV5_20211201203644","2015-09-08T17:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-12.520720000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12336,"MURRAYLINKV5_20211201203644","2015-09-08T17:25:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-228.74191999999999,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12350,"MURRAYLINKV5_20211201203644","2015-09-08T19:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-99.858840000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12351,"MURRAYLINKV5_20211201203644","2015-09-08T20:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-101.25433,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12365,"MURRAYLINKV5_20211201203644","2015-09-09T09:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-22.978739999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12370,"MURRAYLINKV5_20211201203644","2015-09-09T10:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-50.845880000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12383,"MURRAYLINKV5_20211201203644","2015-09-09T17:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-19.609190000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12389,"MURRAYLINKV5_20211201203644","2015-09-09T18:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-23.288679999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12401,"MURRAYLINKV5_20211201203644","2015-09-09T19:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.08606,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12408,"MURRAYLINKV5_20211201203644","2015-09-09T20:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-19.113679999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12415,"MURRAYLINKV5_20211201203644","2015-09-09T21:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-28.7775,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12419,"MURRAYLINKV5_20211201203644","2015-09-09T21:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-21.465530000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12433,"MURRAYLINKV5_20211201203644","2015-09-14T00:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.25834,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12438,"MURRAYLINKV5_20211201203644","2015-09-14T06:20:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.149900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12451,"MURRAYLINKV5_20211201203644","2015-09-15T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.529810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12457,"MURRAYLINKV5_20211201203644","2015-09-16T05:00:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.788679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12466,"MURRAYLINKV5_20211201203644","2015-09-16T08:25:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-04",1,-10.341480000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12471,"MURRAYLINKV5_20211201203644","2015-09-16T08:50:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-04",1,-13.31213,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12485,"MURRAYLINKV5_20211201203644","2015-09-17T02:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.28633,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12489,"MURRAYLINKV5_20211201203644","2015-09-17T05:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.989529999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12496,"MURRAYLINKV5_20211201203644","2015-09-17T05:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.296860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12507,"MURRAYLINKV5_20211201203644","2015-09-18T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.043019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12515,"MURRAYLINKV5_20211201203644","2015-09-18T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.86045,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12521,"MURRAYLINKV5_20211201203644","2015-09-18T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.12626,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12534,"MURRAYLINKV5_20211201203644","2015-09-18T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.52501,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12539,"MURRAYLINKV5_20211201203644","2015-09-18T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.864179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12553,"MURRAYLINKV5_20211201203644","2015-09-20T03:15:00","V::N_HWSM_V3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-33.429180000000002,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12557,"MURRAYLINKV5_20211201203644","2015-09-20T03:35:00","V::N_HWSM_V3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-39.226089999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12564,"MURRAYLINKV5_20211201203644","2015-09-20T04:10:00","V::N_HWSM_V3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-38.477780000000003,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12575,"MURRAYLINKV5_20211201203644","2015-09-20T05:05:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-41.585380000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12583,"MURRAYLINKV5_20211201203644","2015-09-20T05:45:00","V::N_HWSM_V3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-39.766330000000004,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12592,"MURRAYLINKV5_20211201203644","2015-09-20T06:30:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-28.421199999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12604,"MURRAYLINKV5_20211201203644","2015-09-20T07:30:00","V::N_HWSM_V3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-25.306909999999998,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12611,"MURRAYLINKV5_20211201203644","2015-09-20T08:05:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-24.78389,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12618,"MURRAYLINKV5_20211201203644","2015-09-21T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.53077,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12622,"MURRAYLINKV5_20211201203644","2015-09-21T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.566749999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12636,"MURRAYLINKV5_20211201203644","2015-09-21T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.760059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12641,"MURRAYLINKV5_20211201203644","2015-09-21T04:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.882580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12654,"MURRAYLINKV5_20211201203644","2015-09-21T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-29.536460000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12660,"MURRAYLINKV5_20211201203644","2015-09-22T04:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.26784,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12672,"MURRAYLINKV5_20211201203644","2015-09-27T04:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.782539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12679,"MURRAYLINKV5_20211201203644","2015-09-28T03:15:00","V>SML_NWRB_NWMWP1","S-NWRB","2015-03-23",1,-32.07141,"Out=NWB - Robertstown 132kV #1 line, limit flow on ML to avoid OL North West Bend- MWP1 132 kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12681,"MURRAYLINKV5_20211201203644","2015-09-28T03:25:00","V>SML_NWRB_NWMWP1","S-NWRB","2015-03-23",1,-32.540759999999999,"Out=NWB - Robertstown 132kV #1 line, limit flow on ML to avoid OL North West Bend- MWP1 132 kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12690,"MURRAYLINKV5_20211201203644","2015-09-29T01:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.581569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12699,"MURRAYLINKV5_20211201203644","2015-09-29T02:35:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.47889,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12710,"MURRAYLINKV5_20211201203644","2015-09-29T03:30:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.8673,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12718,"MURRAYLINKV5_20211201203644","2015-09-29T04:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.901009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12724,"MURRAYLINKV5_20211201203644","2015-09-29T04:45:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.74513,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12737,"MURRAYLINKV5_20211201203644","2015-09-30T02:10:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.808440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12742,"MURRAYLINKV5_20211201203644","2015-09-30T03:55:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.638950000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12756,"MURRAYLINKV5_20211201203644","2015-10-01T02:15:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.95327,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12760,"MURRAYLINKV5_20211201203644","2015-10-01T02:40:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.55054,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12767,"MURRAYLINKV5_20211201203644","2015-10-01T04:05:00","V>SML_NWRB_NWMWP1","S-NWRB","2015-03-23",1,-25.734950000000001,"Out=NWB - Robertstown 132kV #1 line, limit flow on ML to avoid OL North West Bend- MWP1 132 kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12778,"MURRAYLINKV5_20211201203644","2015-10-03T07:25:00","V::N_HWSM_S3","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-14.342090000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 220 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12786,"MURRAYLINKV5_20211201203644","2015-10-06T00:15:00","V::N_NIL_S3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.500109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 220 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12796,"MURRAYLINKV5_20211201203644","2015-10-06T05:10:00","#R012991_008_RAMP_F","#R012991_RAMP","2015-10-05",1,-41.151150000000001,"Hard Ramping constraint for constraint V::N_EPMB_S3, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12805,"MURRAYLINKV5_20211201203644","2015-10-07T05:05:00","#R012999_009_RAMP_V","#R012999_RAMP","2015-10-06",1,-27.92737,"Soft Ramping constraint for constraint V::N_MLSY_S3, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12814,"MURRAYLINKV5_20211201203644","2015-10-07T05:50:00","#R012999_005_RAMP_F","#R012999_RAMP","2015-10-06",1,-30.85172,"Hard Ramping constraint for constraint V::N_MLSY_Q3, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12816,"MURRAYLINKV5_20211201203644","2015-10-07T09:15:00","#R013004_001_RAMP_V","#R013004_RAMP","2015-10-07",1,-71.883679999999998,"Soft Ramping constraint for constraint S>VML_NWCB6023_TX2, Effective Date: 17/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12825,"MURRAYLINKV5_20211201203644","2015-10-07T10:00:00","#R013004_001_RAMP_V","#R013004_RAMP","2015-10-07",1,-70.890230000000003,"Soft Ramping constraint for constraint S>VML_NWCB6023_TX2, Effective Date: 17/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12839,"MURRAYLINKV5_20211201203644","2015-10-07T11:10:00","S>VML_NWCB6023_TX2","S-NW_CB6023","2015-07-17",1,-71.992339999999999,"Out= North West Bend_CB6023; limit SA to Victoria flow on Murraylink to avoid North West Bend transformer#2 O/L on trip NWB - Robertstown #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12844,"MURRAYLINKV5_20211201203644","2015-10-07T11:35:00","S>VML_NWCB6023_TX2","S-NW_CB6023","2015-07-17",1,-72.87218,"Out= North West Bend_CB6023; limit SA to Victoria flow on Murraylink to avoid North West Bend transformer#2 O/L on trip NWB - Robertstown #1 132kV line.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12857,"MURRAYLINKV5_20211201203644","2015-10-07T12:45:00","S>NWB6024_TX1","S-NW_CB6024","2015-07-27",1,-66.235799999999998,"Out= North West Bend 132kV CB6024, avoid O/L North West Bend 66/132kV #1 TX on trip of NorthWest Bend-Monash #1 132kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12863,"MURRAYLINKV5_20211201203644","2015-10-07T13:15:00","S>NWB6024_TX1","S-NW_CB6024","2015-07-27",1,-66.772469999999998,"Out= North West Bend 132kV CB6024, avoid O/L North West Bend 66/132kV #1 TX on trip of NorthWest Bend-Monash #1 132kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12875,"MURRAYLINKV5_20211201203644","2015-10-08T05:20:00","#R013011_005_RAMP_F","#R013011_RAMP","2015-10-07",1,-19.822620000000001,"Hard Ramping constraint for constraint V::N_MLSY_Q3, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12882,"MURRAYLINKV5_20211201203644","2015-10-10T05:40:00","#R013025_012_RAMP_F","#R013025_RAMP","2015-10-09",1,-12.322190000000001,"Hard Ramping constraint for constraint V::N_EPMB_V3, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[12884,"MURRAYLINKV5_20211201203644","2015-10-10T12:05:00","V>>V_NIL_ROYP56_P2_1","V-ROYP56_P2_N-2","2015-08-25",1,-34.134210000000003,"Out = Nil, loss of Yallourn to Rowville No. 5 and No. 6 220 kV lines declared credible, avoid overloading YPS - ROTS No. 7 or No. 8 220 kV line for loss of YPS - ROTS No. 5 & No. 6 220 kV lines, 3/5 parallel mode, option 2 (JLGA on HWPS B1/2/5 side)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12893,"MURRAYLINKV5_20211201203644","2015-10-10T13:50:00","V>>V_NIL_ROYP56_P2_1","V-ROYP56_P2_N-2","2015-08-25",1,-27.169090000000001,"Out = Nil, loss of Yallourn to Rowville No. 5 and No. 6 220 kV lines declared credible, avoid overloading YPS - ROTS No. 7 or No. 8 220 kV line for loss of YPS - ROTS No. 5 & No. 6 220 kV lines, 3/5 parallel mode, option 2 (JLGA on HWPS B1/2/5 side)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12907,"MURRAYLINKV5_20211201203644","2015-10-11T22:55:00","V::N_HYSE_V3","I-HYSE","2015-08-24",1,-11.182130000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12912,"MURRAYLINKV5_20211201203644","2015-10-12T00:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.69239,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12925,"MURRAYLINKV5_20211201203644","2015-10-12T01:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.084110000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12931,"MURRAYLINKV5_20211201203644","2015-10-12T04:20:00","V::N_HYSE_V3","I-HYSE","2015-08-24",1,-13.886340000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12940,"MURRAYLINKV5_20211201203644","2015-10-12T06:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-32.069409999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12945,"MURRAYLINKV5_20211201203644","2015-10-13T06:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-34.426819999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12959,"MURRAYLINKV5_20211201203644","2015-10-15T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.68041,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12963,"MURRAYLINKV5_20211201203644","2015-10-15T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.98348,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12970,"MURRAYLINKV5_20211201203644","2015-10-15T14:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-34.654159999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12981,"MURRAYLINKV5_20211201203644","2015-10-17T01:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.62237,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12989,"MURRAYLINKV5_20211201203644","2015-10-17T02:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.27112,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[12999,"MURRAYLINKV5_20211201203644","2015-10-17T05:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.43909,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13008,"MURRAYLINKV5_20211201203644","2015-10-19T00:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.78994,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13013,"MURRAYLINKV5_20211201203644","2015-10-19T00:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.845969999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13027,"MURRAYLINKV5_20211201203644","2015-10-19T02:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-52.23901,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13031,"MURRAYLINKV5_20211201203644","2015-10-19T04:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-66.185969999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13038,"MURRAYLINKV5_20211201203644","2015-10-19T04:55:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-13.97255,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13047,"MURRAYLINKV5_20211201203644","2015-10-19T06:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-147.29170999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13060,"MURRAYLINKV5_20211201203644","2015-10-19T22:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-55.237050000000004,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13066,"MURRAYLINKV5_20211201203644","2015-10-20T04:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.770580000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13078,"MURRAYLINKV5_20211201203644","2015-10-20T22:45:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-17.949619999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13085,"MURRAYLINKV5_20211201203644","2015-10-20T23:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-53.290889999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13087,"MURRAYLINKV5_20211201203644","2015-10-21T00:40:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-28.310680000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13096,"MURRAYLINKV5_20211201203644","2015-10-21T01:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-53.679679999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13105,"MURRAYLINKV5_20211201203644","2015-10-21T02:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-53.602339999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13115,"MURRAYLINKV5_20211201203644","2015-10-21T03:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-54.069249999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13128,"MURRAYLINKV5_20211201203644","2015-10-21T04:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-44.042029999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13134,"MURRAYLINKV5_20211201203644","2015-10-21T04:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-58.808549999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13146,"MURRAYLINKV5_20211201203644","2015-10-21T05:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-68.386380000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13153,"MURRAYLINKV5_20211201203644","2015-10-22T06:20:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-45.311369999999997,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13155,"MURRAYLINKV5_20211201203644","2015-10-22T06:30:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-40.342500000000001,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13164,"MURRAYLINKV5_20211201203644","2015-10-22T23:35:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-22.98096,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13173,"MURRAYLINKV5_20211201203644","2015-10-23T05:45:00","#R013123_018_RAMP_V","#R013123_RAMP","2015-10-23",1,-10.133599999999999,"Soft Ramping constraint for constraint N^^V_DDWG, Effective Date: 07/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13184,"MURRAYLINKV5_20211201203644","2015-10-23T06:30:00","#R013123_018_RAMP_V","#R013123_RAMP","2015-10-23",1,-25.496410000000001,"Soft Ramping constraint for constraint N^^V_DDWG, Effective Date: 07/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13192,"MURRAYLINKV5_20211201203644","2015-10-23T07:20:00","N^^V_DDWG","I-JNWO_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-07",1,-13.1053,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13202,"MURRAYLINKV5_20211201203644","2015-10-23T08:40:00","N^^V_DDWG","I-JNWO_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-07",1,-14.639519999999999,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13211,"MURRAYLINKV5_20211201203644","2015-10-23T09:40:00","N^^V_DDWG","I-JNWO_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-07",1,-23.01182,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13220,"MURRAYLINKV5_20211201203644","2015-10-24T01:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-58.368340000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13230,"MURRAYLINKV5_20211201203644","2015-10-24T02:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-54.052709999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13234,"MURRAYLINKV5_20211201203644","2015-10-24T02:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-54.356650000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13241,"MURRAYLINKV5_20211201203644","2015-10-24T03:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-62.6873,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13252,"MURRAYLINKV5_20211201203644","2015-10-24T04:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-54.37912,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13260,"MURRAYLINKV5_20211201203644","2015-10-24T05:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-60.549979999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13270,"MURRAYLINKV5_20211201203644","2015-10-24T20:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.465299999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13279,"MURRAYLINKV5_20211201203644","2015-10-24T21:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-20.91009,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13288,"MURRAYLINKV5_20211201203644","2015-10-24T22:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-21.907520000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13290,"MURRAYLINKV5_20211201203644","2015-10-24T22:30:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.153790000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13299,"MURRAYLINKV5_20211201203644","2015-10-24T23:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-72.810599999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13308,"MURRAYLINKV5_20211201203644","2015-10-24T23:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.85839,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13318,"MURRAYLINKV5_20211201203644","2015-10-25T00:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.619340000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13326,"MURRAYLINKV5_20211201203644","2015-10-25T01:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-64.462810000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13337,"MURRAYLINKV5_20211201203644","2015-10-25T02:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-49.325589999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13349,"MURRAYLINKV5_20211201203644","2015-10-25T03:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-59.424970000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13356,"MURRAYLINKV5_20211201203644","2015-10-25T03:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-59.824530000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13358,"MURRAYLINKV5_20211201203644","2015-10-25T04:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-49.950609999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13367,"MURRAYLINKV5_20211201203644","2015-10-25T04:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.71228,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13376,"MURRAYLINKV5_20211201203644","2015-10-25T05:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.400259999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13386,"MURRAYLINKV5_20211201203644","2015-10-25T05:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-63.642200000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13394,"MURRAYLINKV5_20211201203644","2015-10-25T06:05:00","#R013136_012_RAMP_F","#R013136_RAMP","2015-10-24",1,-13.2273,"Hard Ramping constraint for constraint V::N_BAHO_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13405,"MURRAYLINKV5_20211201203644","2015-10-25T06:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.067880000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13414,"MURRAYLINKV5_20211201203644","2015-10-25T07:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-57.826000000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13423,"MURRAYLINKV5_20211201203644","2015-10-25T07:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.90006,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13433,"MURRAYLINKV5_20211201203644","2015-10-25T10:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-21.177099999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13441,"MURRAYLINKV5_20211201203644","2015-10-25T11:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-60.867339999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13444,"MURRAYLINKV5_20211201203644","2015-10-25T11:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-61.740600000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13455,"MURRAYLINKV5_20211201203644","2015-10-25T12:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-19.77355,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13463,"MURRAYLINKV5_20211201203644","2015-10-25T13:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.590249999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13473,"MURRAYLINKV5_20211201203644","2015-10-25T14:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.894830000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13482,"MURRAYLINKV5_20211201203644","2015-10-25T14:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-72.512519999999995,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13491,"MURRAYLINKV5_20211201203644","2015-10-25T15:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.717359999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13501,"MURRAYLINKV5_20211201203644","2015-10-25T15:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.244779999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13509,"MURRAYLINKV5_20211201203644","2015-10-25T16:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.586510000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13512,"MURRAYLINKV5_20211201203644","2015-10-25T16:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-73.702929999999995,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13521,"MURRAYLINKV5_20211201203644","2015-10-25T16:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-27.453849999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13529,"MURRAYLINKV5_20211201203644","2015-10-25T18:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-28.295729999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13540,"MURRAYLINKV5_20211201203644","2015-10-25T19:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.532220000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13547,"MURRAYLINKV5_20211201203644","2015-10-25T20:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.64053,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13559,"MURRAYLINKV5_20211201203644","2015-10-25T21:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.984269999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13561,"MURRAYLINKV5_20211201203644","2015-10-25T21:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.947040000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13570,"MURRAYLINKV5_20211201203644","2015-10-25T22:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.246510000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13579,"MURRAYLINKV5_20211201203644","2015-10-26T00:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.509589999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13589,"MURRAYLINKV5_20211201203644","2015-10-26T01:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.887740000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13597,"MURRAYLINKV5_20211201203644","2015-10-26T02:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.429320000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13608,"MURRAYLINKV5_20211201203644","2015-10-26T03:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.517379999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13615,"MURRAYLINKV5_20211201203644","2015-10-26T03:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.115170000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13627,"MURRAYLINKV5_20211201203644","2015-10-26T04:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.511380000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13629,"MURRAYLINKV5_20211201203644","2015-10-26T04:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.649800000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13638,"MURRAYLINKV5_20211201203644","2015-10-26T05:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.27882,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13647,"MURRAYLINKV5_20211201203644","2015-10-26T06:35:00","#R013149_015_RAMP_F","#R013149_RAMP","2015-10-26",1,-26.145050000000001,"Hard Ramping constraint for constraint V::N_HYTR_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13658,"MURRAYLINKV5_20211201203644","2015-10-26T09:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.096880000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13666,"MURRAYLINKV5_20211201203644","2015-10-26T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.194750000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13676,"MURRAYLINKV5_20211201203644","2015-10-27T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.85675,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13685,"MURRAYLINKV5_20211201203644","2015-10-27T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.428249999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13694,"MURRAYLINKV5_20211201203644","2015-10-27T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.12322,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13704,"MURRAYLINKV5_20211201203644","2015-10-28T05:30:00","#R013180_004_RAMP_F","#R013180_RAMP","2015-10-27",1,-15.353429999999999,"Hard Ramping constraint for constraint V::N_BAHO_Q4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13712,"MURRAYLINKV5_20211201203644","2015-10-28T06:10:00","N^^V_LTUT_1","N-LTUT_64_15M","2015-08-07",1,-14.867139999999999,"Out = Lower Tumut to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13715,"MURRAYLINKV5_20211201203644","2015-10-28T07:20:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-16.514710000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13730,"MURRAYLINKV5_20211201203644","2015-10-28T15:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-1004.43377,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13734,"MURRAYLINKV5_20211201203644","2015-10-28T15:10:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-1004.34944,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13744,"MURRAYLINKV5_20211201203644","2015-10-28T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.05593,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13753,"MURRAYLINKV5_20211201203644","2015-10-29T01:10:00","V::N_HYMO_Q4","V-HYMO","2015-08-24",1,-14.174250000000001,"Out = Heywood to Mortlake (HYTS-MOPS) No. 2 500 kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13762,"MURRAYLINKV5_20211201203644","2015-10-29T06:50:00","#R013191_011_RAMP_F","#R013191_RAMP","2015-10-28",1,-74.400909999999996,"Hard Ramping constraint for constraint N^^V_MSUT_1, Effective Date: 07/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13764,"MURRAYLINKV5_20211201203644","2015-10-29T07:00:00","#R013191_011_RAMP_F","#R013191_RAMP","2015-10-28",1,-14.16883,"Hard Ramping constraint for constraint N^^V_MSUT_1, Effective Date: 07/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[13773,"MURRAYLINKV5_20211201203644","2015-10-29T09:05:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-22.784479999999999,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13782,"MURRAYLINKV5_20211201203644","2015-10-29T09:55:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-24.164490000000001,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13792,"MURRAYLINKV5_20211201203644","2015-10-29T10:50:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-15.45628,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13800,"MURRAYLINKV5_20211201203644","2015-10-29T11:30:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-51.353969999999997,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13811,"MURRAYLINKV5_20211201203644","2015-10-29T12:25:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-23.83325,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13818,"MURRAYLINKV5_20211201203644","2015-10-29T12:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-25.61778,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13830,"MURRAYLINKV5_20211201203644","2015-10-29T13:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.179939999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13832,"MURRAYLINKV5_20211201203644","2015-10-29T13:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-23.49267,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13841,"MURRAYLINKV5_20211201203644","2015-10-29T14:05:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-53.539529999999999,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13850,"MURRAYLINKV5_20211201203644","2015-10-29T14:40:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-26.077780000000001,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13860,"MURRAYLINKV5_20211201203644","2015-10-29T15:25:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-193.91956999999999,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13869,"MURRAYLINKV5_20211201203644","2015-10-29T15:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-18.440750000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13879,"MURRAYLINKV5_20211201203644","2015-10-29T16:20:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-75.214929999999995,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13888,"MURRAYLINKV5_20211201203644","2015-10-29T21:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.79467,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13897,"MURRAYLINKV5_20211201203644","2015-10-29T21:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-13.12229,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13907,"MURRAYLINKV5_20211201203644","2015-10-29T22:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-22.835419999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13915,"MURRAYLINKV5_20211201203644","2015-10-29T22:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.438839999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13918,"MURRAYLINKV5_20211201203644","2015-10-29T23:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.32696,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13933,"MURRAYLINKV5_20211201203644","2015-10-30T00:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.952529999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13937,"MURRAYLINKV5_20211201203644","2015-10-30T00:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-24.943439999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13947,"MURRAYLINKV5_20211201203644","2015-10-30T01:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.041899999999998,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13956,"MURRAYLINKV5_20211201203644","2015-10-30T01:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-28.94192,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13965,"MURRAYLINKV5_20211201203644","2015-10-30T01:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-13.772130000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13975,"MURRAYLINKV5_20211201203644","2015-10-30T02:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.188599999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13983,"MURRAYLINKV5_20211201203644","2015-10-30T02:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.050509999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13986,"MURRAYLINKV5_20211201203644","2015-10-30T02:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-28.499970000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[13995,"MURRAYLINKV5_20211201203644","2015-10-30T03:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-19.53454,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14003,"MURRAYLINKV5_20211201203644","2015-10-30T03:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11.4742,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14014,"MURRAYLINKV5_20211201203644","2015-10-30T04:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.61253,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14021,"MURRAYLINKV5_20211201203644","2015-10-30T04:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-24.538499999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14033,"MURRAYLINKV5_20211201203644","2015-10-30T05:05:00","#R013200_014_RAMP_F","#R013200_RAMP","2015-10-29",1,-24.964410000000001,"Hard Ramping constraint for constraint V::N_MLSY_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[14039,"MURRAYLINKV5_20211201203644","2015-10-30T05:30:00","#R013200_006_RAMP_F","#R013200_RAMP","2015-10-29",1,-26.790769999999998,"Hard Ramping constraint for constraint V::N_MLSY_Q4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[14044,"MURRAYLINKV5_20211201203644","2015-10-30T06:50:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-11.29997,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14053,"MURRAYLINKV5_20211201203644","2015-10-30T09:25:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-15.638500000000001,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14063,"MURRAYLINKV5_20211201203644","2015-10-30T10:25:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-12.68052,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14071,"MURRAYLINKV5_20211201203644","2015-10-30T11:15:00","N^^V_MSUT_1","I-MSUT;I-X_MSUT_LTUT;I-X_UTMS_DDMS","2015-08-07",1,-14.78572,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14082,"MURRAYLINKV5_20211201203644","2015-10-30T22:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.3172,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14089,"MURRAYLINKV5_20211201203644","2015-10-30T22:40:00","V>>V-MSUT_1","H-MSUT_P;H-MSUT_R;I-MSUT;I-MSUT_P;I-MSUT_R","2015-08-19",1,-18.05237,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14101,"MURRAYLINKV5_20211201203644","2015-10-30T23:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.815570000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14110,"MURRAYLINKV5_20211201203644","2015-10-31T00:30:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.284759999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14118,"MURRAYLINKV5_20211201203644","2015-10-31T01:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.03979,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14121,"MURRAYLINKV5_20211201203644","2015-10-31T01:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-85.080479999999994,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14136,"MURRAYLINKV5_20211201203644","2015-10-31T02:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-22.791609999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14140,"MURRAYLINKV5_20211201203644","2015-10-31T03:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-23.893640000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14145,"MURRAYLINKV5_20211201203644","2015-10-31T03:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-22.795010000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14159,"MURRAYLINKV5_20211201203644","2015-10-31T06:50:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-11.04884,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14168,"MURRAYLINKV5_20211201203644","2015-10-31T07:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-14.72518,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14178,"MURRAYLINKV5_20211201203644","2015-10-31T08:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-17.466239999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14186,"MURRAYLINKV5_20211201203644","2015-10-31T08:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.76995,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14189,"MURRAYLINKV5_20211201203644","2015-10-31T09:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-20.231390000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14204,"MURRAYLINKV5_20211201203644","2015-10-31T10:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.617640000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14208,"MURRAYLINKV5_20211201203644","2015-10-31T10:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.339860000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14213,"MURRAYLINKV5_20211201203644","2015-10-31T11:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.35529,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14227,"MURRAYLINKV5_20211201203644","2015-10-31T12:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.694470000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14236,"MURRAYLINKV5_20211201203644","2015-10-31T13:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.940720000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14242,"MURRAYLINKV5_20211201203644","2015-10-31T13:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.67103,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14247,"MURRAYLINKV5_20211201203644","2015-10-31T14:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.470739999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14260,"MURRAYLINKV5_20211201203644","2015-10-31T15:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.542249999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14266,"MURRAYLINKV5_20211201203644","2015-10-31T16:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.922260000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14274,"MURRAYLINKV5_20211201203644","2015-10-31T17:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-13.990500000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14285,"MURRAYLINKV5_20211201203644","2015-10-31T18:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.847770000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14292,"MURRAYLINKV5_20211201203644","2015-10-31T19:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.27037,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14304,"MURRAYLINKV5_20211201203644","2015-10-31T20:25:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.0992,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14310,"MURRAYLINKV5_20211201203644","2015-10-31T21:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.977460000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14315,"MURRAYLINKV5_20211201203644","2015-10-31T21:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.74263,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14328,"MURRAYLINKV5_20211201203644","2015-10-31T22:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.804939999999998,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14334,"MURRAYLINKV5_20211201203644","2015-10-31T23:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.373659999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14343,"MURRAYLINKV5_20211201203644","2015-11-01T01:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.39255,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14348,"MURRAYLINKV5_20211201203644","2015-11-01T10:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.93566,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14362,"MURRAYLINKV5_20211201203644","2015-11-01T12:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.190270000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14366,"MURRAYLINKV5_20211201203644","2015-11-01T13:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.769870000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14381,"MURRAYLINKV5_20211201203644","2015-11-01T14:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.387049999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14389,"MURRAYLINKV5_20211201203644","2015-11-01T14:50:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-19.031939999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14392,"MURRAYLINKV5_20211201203644","2015-11-01T15:00:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-20.926780000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14407,"MURRAYLINKV5_20211201203644","2015-11-01T15:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.49267,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14411,"MURRAYLINKV5_20211201203644","2015-11-01T15:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.68008,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14416,"MURRAYLINKV5_20211201203644","2015-11-01T16:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.32638,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14430,"MURRAYLINKV5_20211201203644","2015-11-01T17:25:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-30.181750000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14434,"MURRAYLINKV5_20211201203644","2015-11-01T17:45:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-34.245570000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14449,"MURRAYLINKV5_20211201203644","2015-11-01T19:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-21.068899999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14457,"MURRAYLINKV5_20211201203644","2015-11-01T19:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.974070000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14460,"MURRAYLINKV5_20211201203644","2015-11-01T19:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.34834,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14469,"MURRAYLINKV5_20211201203644","2015-11-01T20:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.740010000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14481,"MURRAYLINKV5_20211201203644","2015-11-01T22:00:00","F_S++ML_R6_1","F-SA_ISLE","2013-11-21",1,1461.93148,"Raise 6 sec Service Requirement for SA Generation Event, where Murraylink (Vic to SA transfer) is the largest generation risk in SA, Segment 1","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14488,"MURRAYLINKV5_20211201203644","2015-11-02T05:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.122389999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14495,"MURRAYLINKV5_20211201203644","2015-11-02T05:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.63593,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14507,"MURRAYLINKV5_20211201203644","2015-11-02T06:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-20.464659999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14513,"MURRAYLINKV5_20211201203644","2015-11-02T07:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-23.148489999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14518,"MURRAYLINKV5_20211201203644","2015-11-02T10:45:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-12.523400000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14531,"MURRAYLINKV5_20211201203644","2015-11-02T12:05:00","V>>V_EPMB_1B","V-EPMB;V-EPMB_P;V-EPMB_R;V-X_EPMB_DDSM","2015-09-04",1,-30.673120000000001,"Out = Eildon to Mt Beauty 220kV line, Mt Beauty 220kV Bustie CB closed, limit Vic interconnectors and Southern Hydro generation to avoid O/L of Mt Beauty to Dederang No.2 220kV line for loss of Mt Beauty to Dederang No.1 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14537,"MURRAYLINKV5_20211201203644","2015-11-02T12:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-28.726209999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14549,"MURRAYLINKV5_20211201203644","2015-11-02T13:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.76487,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14556,"MURRAYLINKV5_20211201203644","2015-11-02T14:20:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-19.64545,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14563,"MURRAYLINKV5_20211201203644","2015-11-02T15:15:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-17.77505,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14575,"MURRAYLINKV5_20211201203644","2015-11-02T21:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.150279999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14584,"MURRAYLINKV5_20211201203644","2015-11-02T21:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-15.492229999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14592,"MURRAYLINKV5_20211201203644","2015-11-02T22:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.524380000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14595,"MURRAYLINKV5_20211201203644","2015-11-02T22:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.11637,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14610,"MURRAYLINKV5_20211201203644","2015-11-03T00:15:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-11.56503,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14614,"MURRAYLINKV5_20211201203644","2015-11-03T00:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.623659999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14619,"MURRAYLINKV5_20211201203644","2015-11-03T01:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-12.729520000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14633,"MURRAYLINKV5_20211201203644","2015-11-03T02:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-43.68468,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14637,"MURRAYLINKV5_20211201203644","2015-11-03T03:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.71696,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14652,"MURRAYLINKV5_20211201203644","2015-11-03T05:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.43102,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14655,"MURRAYLINKV5_20211201203644","2015-11-03T05:45:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.34286,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14663,"MURRAYLINKV5_20211201203644","2015-11-03T06:25:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-10.43371,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14678,"MURRAYLINKV5_20211201203644","2015-11-03T07:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-24.164349999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14682,"MURRAYLINKV5_20211201203644","2015-11-03T07:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-28.173950000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14687,"MURRAYLINKV5_20211201203644","2015-11-03T08:15:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-29.469580000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14701,"MURRAYLINKV5_20211201203644","2015-11-03T09:15:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-30.28172,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14710,"MURRAYLINKV5_20211201203644","2015-11-03T10:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-29.646989999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14716,"MURRAYLINKV5_20211201203644","2015-11-03T10:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-23.088249999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14721,"MURRAYLINKV5_20211201203644","2015-11-03T10:55:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-25.916250000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14734,"MURRAYLINKV5_20211201203644","2015-11-03T12:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-12.749879999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14740,"MURRAYLINKV5_20211201203644","2015-11-03T12:30:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.368480000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14752,"MURRAYLINKV5_20211201203644","2015-11-03T13:30:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-19.996510000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14759,"MURRAYLINKV5_20211201203644","2015-11-03T14:35:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-14.11135,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14770,"MURRAYLINKV5_20211201203644","2015-11-03T16:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-20.294779999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14778,"MURRAYLINKV5_20211201203644","2015-11-03T16:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-21.969069999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14784,"MURRAYLINKV5_20211201203644","2015-11-03T17:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.378689999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14789,"MURRAYLINKV5_20211201203644","2015-11-03T17:35:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-25.536660000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14802,"MURRAYLINKV5_20211201203644","2015-11-03T18:40:00","V::N_HYSE_S4","I-HYSE","2015-08-24",1,-44.468060000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink VIC to TAS. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14808,"MURRAYLINKV5_20211201203644","2015-11-03T19:10:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-20.534649999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14817,"MURRAYLINKV5_20211201203644","2015-11-03T19:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.43084,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14822,"MURRAYLINKV5_20211201203644","2015-11-03T20:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.35703,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14836,"MURRAYLINKV5_20211201203644","2015-11-03T21:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-22.43817,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14840,"MURRAYLINKV5_20211201203644","2015-11-03T21:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.775650000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14855,"MURRAYLINKV5_20211201203644","2015-11-03T23:35:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.50168,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14858,"MURRAYLINKV5_20211201203644","2015-11-04T00:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.750969999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14866,"MURRAYLINKV5_20211201203644","2015-11-04T00:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-14.4735,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14881,"MURRAYLINKV5_20211201203644","2015-11-04T05:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.454429999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14885,"MURRAYLINKV5_20211201203644","2015-11-04T06:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.940110000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14890,"MURRAYLINKV5_20211201203644","2015-11-04T06:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.301939999999998,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14904,"MURRAYLINKV5_20211201203644","2015-11-04T16:10:00","V>X_NWCB6022+6023_T1","S-NWCB6022+6023","2015-07-14",1,-305.08129000000002,"Out = North West Bend 132 kV circuit breakers CB6022 and CB6023(Note: this takes out North West Bend-Monash #2 132kV line);  limit Victoria to SA on Murraylink to avoid North West Bend transformer#1 O/L on trip  NWB 132/66kV TX3.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14908,"MURRAYLINKV5_20211201203644","2015-11-04T17:10:00","V>NWB6024_TX1","S-NW_CB6024","2015-07-27",1,-35.485930000000003,"Out= North West Bend 132kV CB6024, avoid O/L North West Bend 132/66kV #1 TX on trip of Monash-NorthWest Bend #1 132kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14923,"MURRAYLINKV5_20211201203644","2015-11-05T00:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-21.18112,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14924,"MURRAYLINKV5_20211201203644","2015-11-05T00:40:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.601279999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14937,"MURRAYLINKV5_20211201203644","2015-11-06T00:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-16.281199999999998,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14943,"MURRAYLINKV5_20211201203644","2015-11-06T05:25:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-18.427769999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14955,"MURRAYLINKV5_20211201203644","2015-11-06T22:20:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.01885,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14962,"MURRAYLINKV5_20211201203644","2015-11-06T22:55:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-17.724930000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14973,"MURRAYLINKV5_20211201203644","2015-11-06T23:50:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.72772,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14981,"MURRAYLINKV5_20211201203644","2015-11-07T00:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-25.848040000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14987,"MURRAYLINKV5_20211201203644","2015-11-07T01:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-20.610769999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[14992,"MURRAYLINKV5_20211201203644","2015-11-07T01:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.19317,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15005,"MURRAYLINKV5_20211201203644","2015-11-07T02:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-17.056039999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15011,"MURRAYLINKV5_20211201203644","2015-11-07T05:40:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.9849,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15023,"MURRAYLINKV5_20211201203644","2015-11-07T06:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-24.98011,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15030,"MURRAYLINKV5_20211201203644","2015-11-07T07:05:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-25.007850000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15041,"MURRAYLINKV5_20211201203644","2015-11-07T08:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-21.176179999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15049,"MURRAYLINKV5_20211201203644","2015-11-07T08:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-20.481079999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15058,"MURRAYLINKV5_20211201203644","2015-11-07T09:20:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-20.29393,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15061,"MURRAYLINKV5_20211201203644","2015-11-07T09:35:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-20.237770000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15069,"MURRAYLINKV5_20211201203644","2015-11-07T10:15:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-14.949630000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15079,"MURRAYLINKV5_20211201203644","2015-11-07T11:05:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-17.152830000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15088,"MURRAYLINKV5_20211201203644","2015-11-07T11:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.064920000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15093,"MURRAYLINKV5_20211201203644","2015-11-07T12:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.808350000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15107,"MURRAYLINKV5_20211201203644","2015-11-07T13:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.675640000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15111,"MURRAYLINKV5_20211201203644","2015-11-07T13:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.832879999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15126,"MURRAYLINKV5_20211201203644","2015-11-07T15:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.995419999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15129,"MURRAYLINKV5_20211201203644","2015-11-07T15:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-18.995609999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15137,"MURRAYLINKV5_20211201203644","2015-11-07T15:55:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.30517,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15147,"MURRAYLINKV5_20211201203644","2015-11-07T16:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-16.487010000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15156,"MURRAYLINKV5_20211201203644","2015-11-07T16:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-19.859120000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15165,"MURRAYLINKV5_20211201203644","2015-11-07T17:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.983639999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15176,"MURRAYLINKV5_20211201203644","2015-11-07T22:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-16.189440000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15184,"MURRAYLINKV5_20211201203644","2015-11-08T00:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.158860000000001,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15194,"MURRAYLINKV5_20211201203644","2015-11-08T01:20:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-15.64723,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15195,"MURRAYLINKV5_20211201203644","2015-11-08T01:25:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-14.97617,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15208,"MURRAYLINKV5_20211201203644","2015-11-08T08:50:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.01972,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15214,"MURRAYLINKV5_20211201203644","2015-11-08T09:45:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-12.00657,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15226,"MURRAYLINKV5_20211201203644","2015-11-08T11:55:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-17.402950000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15233,"MURRAYLINKV5_20211201203644","2015-11-08T12:25:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.66628,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15244,"MURRAYLINKV5_20211201203644","2015-11-08T13:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-10.64165,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15252,"MURRAYLINKV5_20211201203644","2015-11-08T13:30:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-21.998190000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15262,"MURRAYLINKV5_20211201203644","2015-11-08T14:05:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-13.055059999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15263,"MURRAYLINKV5_20211201203644","2015-11-08T14:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-27.092300000000002,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15276,"MURRAYLINKV5_20211201203644","2015-11-08T14:40:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-27.072980000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15282,"MURRAYLINKV5_20211201203644","2015-11-08T15:00:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-12.54505,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15291,"MURRAYLINKV5_20211201203644","2015-11-08T15:40:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-68.715649999999997,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15300,"MURRAYLINKV5_20211201203644","2015-11-08T23:00:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-13.854279999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15310,"MURRAYLINKV5_20211201203644","2015-11-09T00:50:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-14.287269999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15314,"MURRAYLINKV5_20211201203644","2015-11-09T01:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.068719999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15329,"MURRAYLINKV5_20211201203644","2015-11-09T02:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-43.718919999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15332,"MURRAYLINKV5_20211201203644","2015-11-09T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-43.719299999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15340,"MURRAYLINKV5_20211201203644","2015-11-09T03:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-48.05836,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15350,"MURRAYLINKV5_20211201203644","2015-11-09T04:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-50.846800000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15359,"MURRAYLINKV5_20211201203644","2015-11-09T05:30:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-17.39507,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15368,"MURRAYLINKV5_20211201203644","2015-11-09T06:15:00","V::N_HYSE_V4","I-HYSE","2015-08-24",1,-11.639989999999999,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15378,"MURRAYLINKV5_20211201203644","2015-11-10T00:40:00","V::N_HYSE_Q4","I-HYSE","2015-08-24",1,-13.28037,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15382,"MURRAYLINKV5_20211201203644","2015-11-10T01:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-56.362639999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15397,"MURRAYLINKV5_20211201203644","2015-11-10T03:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-39.848019999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15398,"MURRAYLINKV5_20211201203644","2015-11-10T03:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-10.14,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15406,"MURRAYLINKV5_20211201203644","2015-11-10T03:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-51.655169999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15417,"MURRAYLINKV5_20211201203644","2015-11-10T05:40:00","#R013265_012_RAMP_F","#R013265_RAMP","2015-11-09",1,-24.785689999999999,"Hard Ramping constraint for constraint V::N_BAHO_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[15429,"MURRAYLINKV5_20211201203644","2015-11-10T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.068809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15436,"MURRAYLINKV5_20211201203644","2015-11-11T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.26946,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15447,"MURRAYLINKV5_20211201203644","2015-11-11T06:45:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-11.702109999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15455,"MURRAYLINKV5_20211201203644","2015-11-11T07:45:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-18.600300000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15465,"MURRAYLINKV5_20211201203644","2015-11-11T12:30:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-29.376950000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15466,"MURRAYLINKV5_20211201203644","2015-11-11T12:35:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-31.047139999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15474,"MURRAYLINKV5_20211201203644","2015-11-11T13:15:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-28.671990000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15485,"MURRAYLINKV5_20211201203644","2015-11-11T14:20:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-32.274889999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15497,"MURRAYLINKV5_20211201203644","2015-11-11T15:30:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-54.276069999999997,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15504,"MURRAYLINKV5_20211201203644","2015-11-11T16:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-09-16",1,-61.055250000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15515,"MURRAYLINKV5_20211201203644","2015-11-11T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.24804,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15523,"MURRAYLINKV5_20211201203644","2015-11-11T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.695709999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15532,"MURRAYLINKV5_20211201203644","2015-11-12T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.913320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15535,"MURRAYLINKV5_20211201203644","2015-11-12T01:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-11.37677,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15543,"MURRAYLINKV5_20211201203644","2015-11-12T01:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-16.321950000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15553,"MURRAYLINKV5_20211201203644","2015-11-12T02:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-21.088550000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15562,"MURRAYLINKV5_20211201203644","2015-11-12T03:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-15.455690000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15571,"MURRAYLINKV5_20211201203644","2015-11-12T04:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_4TH500;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2012-07-04",1,-13.84272,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15581,"MURRAYLINKV5_20211201203644","2015-11-12T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.792210000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15589,"MURRAYLINKV5_20211201203644","2015-11-13T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.596360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15600,"MURRAYLINKV5_20211201203644","2015-11-13T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.58849,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15603,"MURRAYLINKV5_20211201203644","2015-11-13T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.74873,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15611,"MURRAYLINKV5_20211201203644","2015-11-14T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.43103,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15621,"MURRAYLINKV5_20211201203644","2015-11-14T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.97723,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15630,"MURRAYLINKV5_20211201203644","2015-11-15T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.45621,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15639,"MURRAYLINKV5_20211201203644","2015-11-16T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.84529,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15650,"MURRAYLINKV5_20211201203644","2015-11-16T05:10:00","#R013291_013_RAMP_F","#R013291_RAMP","2015-11-15",1,-22.67831,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[15658,"MURRAYLINKV5_20211201203644","2015-11-17T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.32795,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15668,"MURRAYLINKV5_20211201203644","2015-11-18T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.330220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15669,"MURRAYLINKV5_20211201203644","2015-11-18T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.378589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15677,"MURRAYLINKV5_20211201203644","2015-11-18T09:10:00","S>>DVBL_BWPA_BRTW","S-DVBL","2015-07-30",1,-12.36107,"Out= Davenport-Belalie 275kV line, avoid O/L Brinkworth-Templers West 275kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15688,"MURRAYLINKV5_20211201203644","2015-11-18T12:55:00","S>>DVBL_BWPA_BRTW","S-DVBL","2015-07-30",1,-90.29419,"Out= Davenport-Belalie 275kV line, avoid O/L Brinkworth-Templers West 275kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15695,"MURRAYLINKV5_20211201203644","2015-11-18T16:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-36.883009999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15707,"MURRAYLINKV5_20211201203644","2015-11-19T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.685089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15718,"MURRAYLINKV5_20211201203644","2015-11-19T01:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.52168,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15726,"MURRAYLINKV5_20211201203644","2015-11-19T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.459160000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15736,"MURRAYLINKV5_20211201203644","2015-11-19T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.755179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15737,"MURRAYLINKV5_20211201203644","2015-11-19T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.058959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15745,"MURRAYLINKV5_20211201203644","2015-11-19T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.697859999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15756,"MURRAYLINKV5_20211201203644","2015-11-19T14:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.847490000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15765,"MURRAYLINKV5_20211201203644","2015-11-19T14:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.909739999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15774,"MURRAYLINKV5_20211201203644","2015-11-19T15:15:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-28.09177,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15784,"MURRAYLINKV5_20211201203644","2015-11-19T15:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-25.435300000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15792,"MURRAYLINKV5_20211201203644","2015-11-19T17:40:00","S>>DVBL_BWPA_BRTW","S-DVBL","2015-07-30",1,-90.925020000000004,"Out= Davenport-Belalie 275kV line, avoid O/L Brinkworth-Templers West 275kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15803,"MURRAYLINKV5_20211201203644","2015-11-20T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.795359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15806,"MURRAYLINKV5_20211201203644","2015-11-20T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.62079,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15814,"MURRAYLINKV5_20211201203644","2015-11-20T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-30.9573,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15824,"MURRAYLINKV5_20211201203644","2015-11-20T07:00:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-32.360680000000002,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15833,"MURRAYLINKV5_20211201203644","2015-11-20T13:15:00","V>>V_EPMB_1B","V-EPMB;V-EPMB_P;V-EPMB_R;V-X_EPMB_DDSM","2015-09-04",1,-30.303370000000001,"Out = Eildon to Mt Beauty 220kV line, Mt Beauty 220kV Bustie CB closed, limit Vic interconnectors and Southern Hydro generation to avoid O/L of Mt Beauty to Dederang No.2 220kV line for loss of Mt Beauty to Dederang No.1 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15842,"MURRAYLINKV5_20211201203644","2015-11-21T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.333399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15852,"MURRAYLINKV5_20211201203644","2015-11-21T01:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.41442,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15860,"MURRAYLINKV5_20211201203644","2015-11-21T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.22617,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15871,"MURRAYLINKV5_20211201203644","2015-11-21T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.96693,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15872,"MURRAYLINKV5_20211201203644","2015-11-21T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.14767,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15880,"MURRAYLINKV5_20211201203644","2015-11-21T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.799989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15891,"MURRAYLINKV5_20211201203644","2015-11-21T06:10:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-15.212949999999999,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15898,"MURRAYLINKV5_20211201203644","2015-11-21T11:25:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-19.038430000000002,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15910,"MURRAYLINKV5_20211201203644","2015-11-21T13:30:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-18.20241,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15921,"MURRAYLINKV5_20211201203644","2015-11-21T14:25:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-19.916329999999999,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15929,"MURRAYLINKV5_20211201203644","2015-11-21T15:05:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-20.408580000000001,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15939,"MURRAYLINKV5_20211201203644","2015-11-21T15:55:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-22.932569999999998,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15940,"MURRAYLINKV5_20211201203644","2015-11-21T16:00:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-22.641179999999999,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15948,"MURRAYLINKV5_20211201203644","2015-11-22T13:10:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-15.177339999999999,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15959,"MURRAYLINKV5_20211201203644","2015-11-22T14:05:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-15.661820000000001,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15966,"MURRAYLINKV5_20211201203644","2015-11-22T14:45:00","V::N_BAHO_V4","V-BAHO;V-BAWA;V-HOWA","2015-08-24",1,-15.48673,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15978,"MURRAYLINKV5_20211201203644","2015-11-24T23:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-60.476100000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15987,"MURRAYLINKV5_20211201203644","2015-11-25T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.976520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[15995,"MURRAYLINKV5_20211201203644","2015-11-25T10:35:00","S>>BRMN_BWPA_HUWT","S-BRMN","2015-07-30",1,-79.201160000000002,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16006,"MURRAYLINKV5_20211201203644","2015-11-25T13:20:00","S>>BRMN_BRTW_HUWT","S-BRMN","2013-11-12",1,-111.84238999999999,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Brinkworth - Templers West 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16013,"MURRAYLINKV5_20211201203644","2015-11-25T13:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-97.938339999999997,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16017,"MURRAYLINKV5_20211201203644","2015-11-25T14:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-214.83573000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16027,"MURRAYLINKV5_20211201203644","2015-11-25T16:30:00","S>>PATW_MKRB_WEMWP4","S-PATW","2015-04-21",1,-72.670779999999993,"Out= Para-Templers West 275kV line, avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Mokota-Robertstown 275kV line(This offloads Belalie-Mokota 275kV line and trips Hallet Hill WF), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16036,"MURRAYLINKV5_20211201203644","2015-11-25T17:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-14.155659999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16045,"MURRAYLINKV5_20211201203644","2015-11-25T18:05:00","S>>TPRS_TWPA_WEMWP4","S-TPRS","2015-01-09",1,-414000,"Out= Templers-Roseworthy 132kV line, avoid O/L Waterloo East-MWP4-Robertstown 132kV line on  trip of Templers West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16055,"MURRAYLINKV5_20211201203644","2015-11-25T23:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-14.111800000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16063,"MURRAYLINKV5_20211201203644","2015-11-26T00:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-12.92135,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16074,"MURRAYLINKV5_20211201203644","2015-11-26T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-28.382560000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16081,"MURRAYLINKV5_20211201203644","2015-11-26T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.11355,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16085,"MURRAYLINKV5_20211201203644","2015-11-26T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.74817,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16095,"MURRAYLINKV5_20211201203644","2015-11-26T03:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-14.933400000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16104,"MURRAYLINKV5_20211201203644","2015-11-26T03:40:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-13.466469999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16113,"MURRAYLINKV5_20211201203644","2015-11-26T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.838889999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16119,"MURRAYLINKV5_20211201203644","2015-11-26T04:20:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-67.419179999999997,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16132,"MURRAYLINKV5_20211201203644","2015-11-26T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.20448,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16142,"MURRAYLINKV5_20211201203644","2015-11-26T05:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-12.84507,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16143,"MURRAYLINKV5_20211201203644","2015-11-26T05:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-12.52534,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16151,"MURRAYLINKV5_20211201203644","2015-11-27T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.11482,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16162,"MURRAYLINKV5_20211201203644","2015-11-27T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.807379999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16169,"MURRAYLINKV5_20211201203644","2015-11-27T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.859390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16181,"MURRAYLINKV5_20211201203644","2015-11-28T06:55:00","N^^V_EPTT_1","V-EPTT_P;V-EPTT_R;V-X_EPTTSMRO;V-X_SMTXH1+EPTT","2015-08-07",1,-77.874269999999996,"Out = Eildon to Thomastown 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16187,"MURRAYLINKV5_20211201203644","2015-11-29T22:05:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-19.757200000000001,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16200,"MURRAYLINKV5_20211201203644","2015-11-29T23:25:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-12.125299999999999,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16210,"MURRAYLINKV5_20211201203644","2015-11-30T00:30:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-18.347860000000001,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16211,"MURRAYLINKV5_20211201203644","2015-11-30T00:35:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-16.274819999999998,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16220,"MURRAYLINKV5_20211201203644","2015-11-30T01:20:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-15.430070000000001,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16234,"MURRAYLINKV5_20211201203644","2015-11-30T02:30:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-20.333780000000001,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16239,"MURRAYLINKV5_20211201203644","2015-11-30T02:55:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-20.089479999999998,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16248,"MURRAYLINKV5_20211201203644","2015-11-30T03:40:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-23.22184,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16258,"MURRAYLINKV5_20211201203644","2015-11-30T04:30:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-23.547969999999999,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16266,"MURRAYLINKV5_20211201203644","2015-11-30T05:10:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-21.73978,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16277,"MURRAYLINKV5_20211201203644","2015-11-30T09:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-47.37491,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16284,"MURRAYLINKV5_20211201203644","2015-11-30T09:50:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-85.617679999999993,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16288,"MURRAYLINKV5_20211201203644","2015-11-30T10:00:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-86.433009999999996,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16302,"MURRAYLINKV5_20211201203644","2015-11-30T10:35:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-85.587440000000001,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16307,"MURRAYLINKV5_20211201203644","2015-11-30T10:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-50.881830000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16316,"MURRAYLINKV5_20211201203644","2015-11-30T11:10:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-99.934200000000004,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16326,"MURRAYLINKV5_20211201203644","2015-11-30T11:35:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-92.569360000000003,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16334,"MURRAYLINKV5_20211201203644","2015-11-30T11:55:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-91.104489999999998,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16345,"MURRAYLINKV5_20211201203644","2015-11-30T12:20:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-53.6753,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16346,"MURRAYLINKV5_20211201203644","2015-11-30T12:25:00","S>>PA6510_RBPA_TWPA","S-PA_CB6510","2015-08-13",1,-102.57649000000001,"Out= Para 275kV CB6510, avoid O/L Templers West-Para 275kV line on trip of Robertstown-Para 275kV line (this offloads Blyth West-Munno Para 275kV line& Munno Para-Para 275kV line & Munno Para TX), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16354,"MURRAYLINKV5_20211201203644","2015-11-30T12:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-95.351179999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16365,"MURRAYLINKV5_20211201203644","2015-11-30T13:40:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-87.004630000000006,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16372,"MURRAYLINKV5_20211201203644","2015-11-30T14:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-138.3723,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16384,"MURRAYLINKV5_20211201203644","2015-11-30T15:20:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-291.77551,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16390,"MURRAYLINKV5_20211201203644","2015-11-30T15:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-145.84505999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16403,"MURRAYLINKV5_20211201203644","2015-12-01T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.41855,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16408,"MURRAYLINKV5_20211201203644","2015-12-01T07:35:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-14.0458,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16414,"MURRAYLINKV5_20211201203644","2015-12-01T08:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-33.78801,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16422,"MURRAYLINKV5_20211201203644","2015-12-01T09:35:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-45.150669999999998,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16433,"MURRAYLINKV5_20211201203644","2015-12-01T10:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-34.010750000000002,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16440,"MURRAYLINKV5_20211201203644","2015-12-01T10:25:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-29.414739999999998,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16452,"MURRAYLINKV5_20211201203644","2015-12-01T10:55:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-66.772099999999995,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16461,"MURRAYLINKV5_20211201203644","2015-12-01T11:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-56.523789999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16469,"MURRAYLINKV5_20211201203644","2015-12-01T11:40:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-77.239019999999996,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16480,"MURRAYLINKV5_20211201203644","2015-12-01T12:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-54.74053,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16487,"MURRAYLINKV5_20211201203644","2015-12-01T12:25:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-69.883160000000004,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16491,"MURRAYLINKV5_20211201203644","2015-12-01T12:35:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-67.366799999999998,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16505,"MURRAYLINKV5_20211201203644","2015-12-01T13:35:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-20.596699999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16510,"MURRAYLINKV5_20211201203644","2015-12-01T14:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-19.5501,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16523,"MURRAYLINKV5_20211201203644","2015-12-01T16:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.004760000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16529,"MURRAYLINKV5_20211201203644","2015-12-01T16:35:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-119.82908999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16537,"MURRAYLINKV5_20211201203644","2015-12-01T18:10:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-51.298310000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16548,"MURRAYLINKV5_20211201203644","2015-12-01T18:50:00","S>>BGBW_TWPA_TPRS","S-BGBW","2015-03-31",1,-29.195080000000001,"Out= Bungama - Blyth West 275kV line, avoid O/L Templers-Roseworthy 132kV line on trip of Templers West- Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16555,"MURRAYLINKV5_20211201203644","2015-12-01T19:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-20.45628,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16559,"MURRAYLINKV5_20211201203644","2015-12-01T19:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-20.043040000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16573,"MURRAYLINKV5_20211201203644","2015-12-02T02:55:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-23.943999999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16578,"MURRAYLINKV5_20211201203644","2015-12-02T03:20:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-25.319959999999998,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16587,"MURRAYLINKV5_20211201203644","2015-12-02T04:05:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-21.855239999999998,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16593,"MURRAYLINKV5_20211201203644","2015-12-02T04:35:00","V::N_HWSM_V4","V-HWCB4;V-HWRO3;V-HWSM","2015-08-24",1,-27.43,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16606,"MURRAYLINKV5_20211201203644","2015-12-02T06:30:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-14.854179999999999,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16611,"MURRAYLINKV5_20211201203644","2015-12-02T06:55:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-60.339930000000003,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16617,"MURRAYLINKV5_20211201203644","2015-12-03T06:55:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-31.417929999999998,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16629,"MURRAYLINKV5_20211201203644","2015-12-03T15:05:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-15.43642,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16636,"MURRAYLINKV5_20211201203644","2015-12-03T15:40:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-15.448740000000001,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16643,"MURRAYLINKV5_20211201203644","2015-12-03T16:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.023869999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16655,"MURRAYLINKV5_20211201203644","2015-12-03T17:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.620450000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16661,"MURRAYLINKV5_20211201203644","2015-12-03T18:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.970829999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16674,"MURRAYLINKV5_20211201203644","2015-12-03T20:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.194410000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16679,"MURRAYLINKV5_20211201203644","2015-12-04T07:00:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-25.483219999999999,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16685,"MURRAYLINKV5_20211201203644","2015-12-04T07:40:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-18.3398,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16694,"MURRAYLINKV5_20211201203644","2015-12-04T08:25:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-32.103999999999999,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16708,"MURRAYLINKV5_20211201203644","2015-12-04T09:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-26.801539999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16713,"MURRAYLINKV5_20211201203644","2015-12-04T10:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-28.19763,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16726,"MURRAYLINKV5_20211201203644","2015-12-04T11:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.451079999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16732,"MURRAYLINKV5_20211201203644","2015-12-04T12:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-37.79448,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16735,"MURRAYLINKV5_20211201203644","2015-12-04T12:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-23.035959999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16751,"MURRAYLINKV5_20211201203644","2015-12-04T14:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-62.279089999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16758,"MURRAYLINKV5_20211201203644","2015-12-04T14:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-59.392220000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16762,"MURRAYLINKV5_20211201203644","2015-12-04T14:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-63.358699999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16776,"MURRAYLINKV5_20211201203644","2015-12-04T16:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-79.336740000000006,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16781,"MURRAYLINKV5_20211201203644","2015-12-04T16:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-78.634339999999995,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16794,"MURRAYLINKV5_20211201203644","2015-12-04T17:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.470649999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16800,"MURRAYLINKV5_20211201203644","2015-12-04T18:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-20.50123,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16803,"MURRAYLINKV5_20211201203644","2015-12-04T21:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-47.689039999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16819,"MURRAYLINKV5_20211201203644","2015-12-05T17:25:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-185.46520000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16820,"MURRAYLINKV5_20211201203644","2015-12-05T17:30:00","S>NWCB6024+25_TX3","S-NWBCB6024+6025","2015-07-27",1,-128.28041999999999,"Out= North West Bed 132kV CBs 6024 and 6025(this offloads NWB TX2), avoid O/L North West Bend #3 132/66kV TX on trip of North West Bend- Monash #1 132kV line (this splits NWB 132kV bus), Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16832,"MURRAYLINKV5_20211201203644","2015-12-05T18:45:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-32.535760000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16839,"MURRAYLINKV5_20211201203644","2015-12-05T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-26.982150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16846,"MURRAYLINKV5_20211201203644","2015-12-06T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.302199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16858,"MURRAYLINKV5_20211201203644","2015-12-06T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.092409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16864,"MURRAYLINKV5_20211201203644","2015-12-06T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.52305,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16877,"MURRAYLINKV5_20211201203644","2015-12-06T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.84592,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16882,"MURRAYLINKV5_20211201203644","2015-12-06T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.82807,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16888,"MURRAYLINKV5_20211201203644","2015-12-06T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.69237,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16900,"MURRAYLINKV5_20211201203644","2015-12-06T06:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.82141,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16907,"MURRAYLINKV5_20211201203644","2015-12-06T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.729780000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16918,"MURRAYLINKV5_20211201203644","2015-12-06T12:40:00","V>SML_NSWRB_10","@HWPS_20090217;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-15.9842,"Out = NSW Murraylink runback scheme, avoid O/L of Kerang to Wemen 220 kV line section for loss of Balranald to Darlington Point (X5/1) 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16926,"MURRAYLINKV5_20211201203644","2015-12-06T13:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.35524,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16935,"MURRAYLINKV5_20211201203644","2015-12-06T14:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.440349999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16938,"MURRAYLINKV5_20211201203644","2015-12-06T14:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.34984,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16954,"MURRAYLINKV5_20211201203644","2015-12-06T16:45:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-22.94303,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16961,"MURRAYLINKV5_20211201203644","2015-12-06T17:20:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-29.234179999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16965,"MURRAYLINKV5_20211201203644","2015-12-06T20:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-10.65734,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16979,"MURRAYLINKV5_20211201203644","2015-12-07T06:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.840070000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16984,"MURRAYLINKV5_20211201203644","2015-12-07T06:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-24.363890000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[16997,"MURRAYLINKV5_20211201203644","2015-12-07T07:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-82.159090000000006,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17003,"MURRAYLINKV5_20211201203644","2015-12-07T08:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-45.220129999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17006,"MURRAYLINKV5_20211201203644","2015-12-07T08:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-191.51275000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17022,"MURRAYLINKV5_20211201203644","2015-12-07T09:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-186.08327,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17029,"MURRAYLINKV5_20211201203644","2015-12-07T09:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-29.213899999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17033,"MURRAYLINKV5_20211201203644","2015-12-07T09:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-35.504950000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17042,"MURRAYLINKV5_20211201203644","2015-12-07T15:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-10.199199999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17053,"MURRAYLINKV5_20211201203644","2015-12-08T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.56775,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17061,"MURRAYLINKV5_20211201203644","2015-12-08T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.708490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17067,"MURRAYLINKV5_20211201203644","2015-12-08T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.91591,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17080,"MURRAYLINKV5_20211201203644","2015-12-08T05:50:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-14.89307,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17085,"MURRAYLINKV5_20211201203644","2015-12-08T06:20:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-18.219650000000001,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17091,"MURRAYLINKV5_20211201203644","2015-12-08T06:55:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-271.13139000000001,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17103,"MURRAYLINKV5_20211201203644","2015-12-08T08:15:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-270.45753999999999,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17110,"MURRAYLINKV5_20211201203644","2015-12-08T08:50:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-37.338540000000002,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17121,"MURRAYLINKV5_20211201203644","2015-12-08T12:40:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-45.938229999999997,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17129,"MURRAYLINKV5_20211201203644","2015-12-08T13:45:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-31.68797,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17135,"MURRAYLINKV5_20211201203644","2015-12-08T14:05:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-27.55275,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17148,"MURRAYLINKV5_20211201203644","2015-12-08T14:55:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-38.225929999999998,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17153,"MURRAYLINKV5_20211201203644","2015-12-08T15:25:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-15.22559,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17159,"MURRAYLINKV5_20211201203644","2015-12-08T23:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-79.353840000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17168,"MURRAYLINKV5_20211201203644","2015-12-09T02:50:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.08325,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17182,"MURRAYLINKV5_20211201203644","2015-12-09T06:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.969620000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17187,"MURRAYLINKV5_20211201203644","2015-12-09T22:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-24.963940000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17200,"MURRAYLINKV5_20211201203644","2015-12-09T23:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-39.096089999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17206,"MURRAYLINKV5_20211201203644","2015-12-10T00:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.762270000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17209,"MURRAYLINKV5_20211201203644","2015-12-10T00:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.29134,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17225,"MURRAYLINKV5_20211201203644","2015-12-11T01:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.062060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17227,"MURRAYLINKV5_20211201203644","2015-12-11T01:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.18295,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17236,"MURRAYLINKV5_20211201203644","2015-12-11T03:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.973000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17250,"MURRAYLINKV5_20211201203644","2015-12-12T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.93221,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17255,"MURRAYLINKV5_20211201203644","2015-12-12T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.403650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17268,"MURRAYLINKV5_20211201203644","2015-12-12T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.89803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17274,"MURRAYLINKV5_20211201203644","2015-12-12T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.34676,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17283,"MURRAYLINKV5_20211201203644","2015-12-12T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.167729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17288,"MURRAYLINKV5_20211201203644","2015-12-12T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.174849999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17294,"MURRAYLINKV5_20211201203644","2015-12-13T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.197290000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17306,"MURRAYLINKV5_20211201203644","2015-12-13T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.93333,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17313,"MURRAYLINKV5_20211201203644","2015-12-13T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.728770000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17324,"MURRAYLINKV5_20211201203644","2015-12-14T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.46224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17332,"MURRAYLINKV5_20211201203644","2015-12-14T14:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-28.50487,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17342,"MURRAYLINKV5_20211201203644","2015-12-14T22:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.662710000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17351,"MURRAYLINKV5_20211201203644","2015-12-15T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.57408,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17356,"MURRAYLINKV5_20211201203644","2015-12-15T03:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.08034,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17362,"MURRAYLINKV5_20211201203644","2015-12-15T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.779789999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17374,"MURRAYLINKV5_20211201203644","2015-12-15T14:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-30.26163,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17381,"MURRAYLINKV5_20211201203644","2015-12-16T10:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.746779999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17392,"MURRAYLINKV5_20211201203644","2015-12-16T11:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-167.81362999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17400,"MURRAYLINKV5_20211201203644","2015-12-16T12:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.948319999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17409,"MURRAYLINKV5_20211201203644","2015-12-16T12:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-159.08242000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17412,"MURRAYLINKV5_20211201203644","2015-12-16T12:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-196.23594,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17428,"MURRAYLINKV5_20211201203644","2015-12-16T14:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-38.505189999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17430,"MURRAYLINKV5_20211201203644","2015-12-16T14:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-124.90884,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17439,"MURRAYLINKV5_20211201203644","2015-12-16T16:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-161.09008,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17448,"MURRAYLINKV5_20211201203644","2015-12-16T16:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-162.14295000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17458,"MURRAYLINKV5_20211201203644","2015-12-16T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-29.845140000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17471,"MURRAYLINKV5_20211201203644","2015-12-16T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-27.538180000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17477,"MURRAYLINKV5_20211201203644","2015-12-16T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-145.98603,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17480,"MURRAYLINKV5_20211201203644","2015-12-16T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.95186,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17496,"MURRAYLINKV5_20211201203644","2015-12-16T20:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-21.629159999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17498,"MURRAYLINKV5_20211201203644","2015-12-16T21:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-25.878640000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17507,"MURRAYLINKV5_20211201203644","2015-12-17T09:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-17.68562,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17516,"MURRAYLINKV5_20211201203644","2015-12-17T10:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-206.78621000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17527,"MURRAYLINKV5_20211201203644","2015-12-17T10:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-194.08601999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17535,"MURRAYLINKV5_20211201203644","2015-12-17T11:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-210.66967,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17545,"MURRAYLINKV5_20211201203644","2015-12-17T11:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.65868,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17554,"MURRAYLINKV5_20211201203644","2015-12-17T12:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-177.09528,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17563,"MURRAYLINKV5_20211201203644","2015-12-17T13:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-182.28856999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17565,"MURRAYLINKV5_20211201203644","2015-12-17T13:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-197.95187000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17577,"MURRAYLINKV5_20211201203644","2015-12-17T14:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-97.950909999999993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17584,"MURRAYLINKV5_20211201203644","2015-12-17T14:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-236.67639,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17595,"MURRAYLINKV5_20211201203644","2015-12-17T15:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-29.19557,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17603,"MURRAYLINKV5_20211201203644","2015-12-17T16:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-807.50932999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17613,"MURRAYLINKV5_20211201203644","2015-12-17T17:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-511.45173999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17622,"MURRAYLINKV5_20211201203644","2015-12-17T18:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-258.97924999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17631,"MURRAYLINKV5_20211201203644","2015-12-17T19:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-239.88912999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17633,"MURRAYLINKV5_20211201203644","2015-12-17T19:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-141.58225999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17642,"MURRAYLINKV5_20211201203644","2015-12-17T20:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-126.4248,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17651,"MURRAYLINKV5_20211201203644","2015-12-17T20:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-21.380849999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17661,"MURRAYLINKV5_20211201203644","2015-12-17T21:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-23.845590000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17669,"MURRAYLINKV5_20211201203644","2015-12-17T22:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-40.870809999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17680,"MURRAYLINKV5_20211201203644","2015-12-17T23:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-27.824190000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17683,"MURRAYLINKV5_20211201203644","2015-12-17T23:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-43.070799999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17699,"MURRAYLINKV5_20211201203644","2015-12-18T07:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.42869,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17701,"MURRAYLINKV5_20211201203644","2015-12-18T08:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-19.45232,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17710,"MURRAYLINKV5_20211201203644","2015-12-18T08:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-23.82536,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17719,"MURRAYLINKV5_20211201203644","2015-12-18T09:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-26.259779999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17729,"MURRAYLINKV5_20211201203644","2015-12-18T10:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.085550000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17737,"MURRAYLINKV5_20211201203644","2015-12-18T11:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-22.80791,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17748,"MURRAYLINKV5_20211201203644","2015-12-18T12:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.783810000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17757,"MURRAYLINKV5_20211201203644","2015-12-18T14:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-21.51735,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17766,"MURRAYLINKV5_20211201203644","2015-12-18T15:15:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-204.69992999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17768,"MURRAYLINKV5_20211201203644","2015-12-18T15:25:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-50.516620000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17780,"MURRAYLINKV5_20211201203644","2015-12-18T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-27.605889999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17787,"MURRAYLINKV5_20211201203644","2015-12-18T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-36.245699999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17798,"MURRAYLINKV5_20211201203644","2015-12-18T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-34.494630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17806,"MURRAYLINKV5_20211201203644","2015-12-18T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.623150000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17816,"MURRAYLINKV5_20211201203644","2015-12-18T20:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-184.46977000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17825,"MURRAYLINKV5_20211201203644","2015-12-18T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-179.96108000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17834,"MURRAYLINKV5_20211201203644","2015-12-18T22:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-24.946400000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17836,"MURRAYLINKV5_20211201203644","2015-12-18T22:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-26.161760000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17852,"MURRAYLINKV5_20211201203644","2015-12-19","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.411110000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17855,"MURRAYLINKV5_20211201203644","2015-12-19T08:35:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-56.302010000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17866,"MURRAYLINKV5_20211201203644","2015-12-19T09:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-21.289639999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17874,"MURRAYLINKV5_20211201203644","2015-12-19T10:10:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-80.163049999999998,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17883,"MURRAYLINKV5_20211201203644","2015-12-19T10:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.665380000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17886,"MURRAYLINKV5_20211201203644","2015-12-19T11:15:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-11.49343,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17902,"MURRAYLINKV5_20211201203644","2015-12-19T14:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-19.972110000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17904,"MURRAYLINKV5_20211201203644","2015-12-19T14:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-52.449300000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17913,"MURRAYLINKV5_20211201203644","2015-12-19T16:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-39.333559999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17922,"MURRAYLINKV5_20211201203644","2015-12-19T17:10:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-21.116820000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17932,"MURRAYLINKV5_20211201203644","2015-12-19T18:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.664770000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17940,"MURRAYLINKV5_20211201203644","2015-12-19T18:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.10369,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17951,"MURRAYLINKV5_20211201203644","2015-12-20T13:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-20.695070000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17958,"MURRAYLINKV5_20211201203644","2015-12-20T14:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.86439,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17970,"MURRAYLINKV5_20211201203644","2015-12-20T14:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-41.754629999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17972,"MURRAYLINKV5_20211201203644","2015-12-20T14:35:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-50.40513,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17981,"MURRAYLINKV5_20211201203644","2015-12-20T15:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-16.569739999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[17990,"MURRAYLINKV5_20211201203644","2015-12-20T15:20:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-48.722929999999998,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18001,"MURRAYLINKV5_20211201203644","2015-12-20T15:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.395770000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18009,"MURRAYLINKV5_20211201203644","2015-12-20T16:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.520350000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18019,"MURRAYLINKV5_20211201203644","2015-12-20T19:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-67.253479999999996,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18028,"MURRAYLINKV5_20211201203644","2015-12-21T04:15:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-90.648880000000005,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18037,"MURRAYLINKV5_20211201203644","2015-12-21T05:05:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-89.334810000000004,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18039,"MURRAYLINKV5_20211201203644","2015-12-21T05:20:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-102.682,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18055,"MURRAYLINKV5_20211201203644","2015-12-21T06:45:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-114.0213,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18058,"MURRAYLINKV5_20211201203644","2015-12-21T07:05:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-99.172290000000004,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18069,"MURRAYLINKV5_20211201203644","2015-12-21T08:10:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-99.199910000000003,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18077,"MURRAYLINKV5_20211201203644","2015-12-21T09:05:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-150.33588,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18087,"MURRAYLINKV5_20211201203644","2015-12-21T10:10:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-109.96682,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18096,"MURRAYLINKV5_20211201203644","2015-12-21T10:55:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2015-07-30",1,-150.45774,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18105,"MURRAYLINKV5_20211201203644","2015-12-22T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.1044,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18107,"MURRAYLINKV5_20211201203644","2015-12-23T00:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.83638,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18116,"MURRAYLINKV5_20211201203644","2015-12-23T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.50639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18125,"MURRAYLINKV5_20211201203644","2015-12-23T04:40:00","#R013483_002_RAMP_V","#R013483_RAMP","2015-12-22",1,-12.00723,"Soft Ramping constraint for constraint V>>V_KTS_TX_A2_2B_R, Effective Date: 08/09/2015, Version: 1","SYSTEM NORMAL","RAMP",null,"","",null,null,0]
[18135,"MURRAYLINKV5_20211201203644","2015-12-23T05:35:00","V>>V_KTS_TX_A2_2B_R","V-KTTX_A2_OR_A4_R","2015-09-08",1,-10.815720000000001,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 220 kV network, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18143,"MURRAYLINKV5_20211201203644","2015-12-24T16:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-214.32918000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18154,"MURRAYLINKV5_20211201203644","2015-12-24T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-33.570390000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18161,"MURRAYLINKV5_20211201203644","2015-12-24T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-50.608379999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18173,"MURRAYLINKV5_20211201203644","2015-12-24T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-40.441400000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18175,"MURRAYLINKV5_20211201203644","2015-12-24T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-41.085569999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18184,"MURRAYLINKV5_20211201203644","2015-12-24T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-24.57,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18193,"MURRAYLINKV5_20211201203644","2015-12-24T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-53.629930000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18203,"MURRAYLINKV5_20211201203644","2015-12-24T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.474139999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18211,"MURRAYLINKV5_20211201203644","2015-12-24T22:55:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-24.664359999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18222,"MURRAYLINKV5_20211201203644","2015-12-24T23:35:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-277.39496000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18231,"MURRAYLINKV5_20211201203644","2015-12-25T00:05:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-55.95637,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18240,"MURRAYLINKV5_20211201203644","2015-12-25T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.89462,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18242,"MURRAYLINKV5_20211201203644","2015-12-25T00:35:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-99.084779999999995,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18258,"MURRAYLINKV5_20211201203644","2015-12-25T02:55:00","V>>V_NIL1A_R","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-32.985520000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18261,"MURRAYLINKV5_20211201203644","2015-12-25T03:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.440329999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18267,"MURRAYLINKV5_20211201203644","2015-12-25T04:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.22617,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18280,"MURRAYLINKV5_20211201203644","2015-12-25T05:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.15474,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18290,"MURRAYLINKV5_20211201203644","2015-12-25T05:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.93263,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18299,"MURRAYLINKV5_20211201203644","2015-12-25T06:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.328760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18308,"MURRAYLINKV5_20211201203644","2015-12-25T07:00:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-41.61768,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18310,"MURRAYLINKV5_20211201203644","2015-12-25T07:05:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-44.33231,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18326,"MURRAYLINKV5_20211201203644","2015-12-25T08:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.958310000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18329,"MURRAYLINKV5_20211201203644","2015-12-25T08:10:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-76.556849999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18338,"MURRAYLINKV5_20211201203644","2015-12-25T08:50:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-69.340159999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18346,"MURRAYLINKV5_20211201203644","2015-12-25T09:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.71848,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18357,"MURRAYLINKV5_20211201203644","2015-12-25T10:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-15.90828,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18364,"MURRAYLINKV5_20211201203644","2015-12-25T10:30:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-107.55361000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18376,"MURRAYLINKV5_20211201203644","2015-12-25T11:35:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-55.148879999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18382,"MURRAYLINKV5_20211201203644","2015-12-25T12:05:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-148.60297,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18387,"MURRAYLINKV5_20211201203644","2015-12-25T12:30:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-211.40064000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18396,"MURRAYLINKV5_20211201203644","2015-12-25T13:15:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-84.388050000000007,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18406,"MURRAYLINKV5_20211201203644","2015-12-25T14:05:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-82.680319999999995,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18414,"MURRAYLINKV5_20211201203644","2015-12-25T14:45:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-53.779179999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18425,"MURRAYLINKV5_20211201203644","2015-12-25T15:50:00","V>>SML_NIL_CONT_7B","V-NIL_BAHO_66_CONT","2015-08-13",1,-20.747420000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18432,"MURRAYLINKV5_20211201203644","2015-12-25T19:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-18.88946,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18444,"MURRAYLINKV5_20211201203644","2015-12-25T21:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-46.188600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18450,"MURRAYLINKV5_20211201203644","2015-12-25T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-14.810409999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18455,"MURRAYLINKV5_20211201203644","2015-12-25T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-29.930499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18464,"MURRAYLINKV5_20211201203644","2015-12-25T23:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL;S-NIL_2","2014-06-11",1,-14.94918,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18470,"MURRAYLINKV5_20211201203644","2015-12-25T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-15.90265,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18483,"MURRAYLINKV5_20211201203644","2015-12-26T07:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.935219999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18488,"MURRAYLINKV5_20211201203644","2015-12-26T08:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.84538,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18502,"MURRAYLINKV5_20211201203644","2015-12-26T08:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-18.29495,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18511,"MURRAYLINKV5_20211201203644","2015-12-26T09:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.85347,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18513,"MURRAYLINKV5_20211201203644","2015-12-26T09:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-20.707630000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18529,"MURRAYLINKV5_20211201203644","2015-12-26T10:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.384639999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18532,"MURRAYLINKV5_20211201203644","2015-12-26T10:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-18.789339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18538,"MURRAYLINKV5_20211201203644","2015-12-26T10:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-37.204360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18551,"MURRAYLINKV5_20211201203644","2015-12-26T11:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-38.535350000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18556,"MURRAYLINKV5_20211201203644","2015-12-26T11:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.2197,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18570,"MURRAYLINKV5_20211201203644","2015-12-26T11:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.388839999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18579,"MURRAYLINKV5_20211201203644","2015-12-26T12:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.899699999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18585,"MURRAYLINKV5_20211201203644","2015-12-26T12:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-44.54222,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18590,"MURRAYLINKV5_20211201203644","2015-12-26T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-41.135109999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18603,"MURRAYLINKV5_20211201203644","2015-12-26T13:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-37.047089999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18609,"MURRAYLINKV5_20211201203644","2015-12-26T13:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-36.92989,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18617,"MURRAYLINKV5_20211201203644","2015-12-26T14:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.50253,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18628,"MURRAYLINKV5_20211201203644","2015-12-26T14:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-18.194669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18635,"MURRAYLINKV5_20211201203644","2015-12-26T14:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-13.788029999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18647,"MURRAYLINKV5_20211201203644","2015-12-26T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-16.112459999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18653,"MURRAYLINKV5_20211201203644","2015-12-26T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-14.973420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18658,"MURRAYLINKV5_20211201203644","2015-12-26T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-14.00367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18671,"MURRAYLINKV5_20211201203644","2015-12-26T17:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-26.605370000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18677,"MURRAYLINKV5_20211201203644","2015-12-26T18:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-25.678149999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18685,"MURRAYLINKV5_20211201203644","2015-12-26T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.45688,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18696,"MURRAYLINKV5_20211201203644","2015-12-26T19:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-17.95139,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18705,"MURRAYLINKV5_20211201203644","2015-12-26T19:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.054869999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18709,"MURRAYLINKV5_20211201203644","2015-12-26T20:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-17.52467,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18716,"MURRAYLINKV5_20211201203644","2015-12-26T20:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-13.63232,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18732,"MURRAYLINKV5_20211201203644","2015-12-26T22:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.51695,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18735,"MURRAYLINKV5_20211201203644","2015-12-26T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-17.37125,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18741,"MURRAYLINKV5_20211201203644","2015-12-26T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.0571,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18754,"MURRAYLINKV5_20211201203644","2015-12-27T06:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-11.144159999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18759,"MURRAYLINKV5_20211201203644","2015-12-27T06:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-11.224349999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18773,"MURRAYLINKV5_20211201203644","2015-12-27T08:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-14.143660000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18777,"MURRAYLINKV5_20211201203644","2015-12-27T08:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-14.43173,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18784,"MURRAYLINKV5_20211201203644","2015-12-27T09:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-11.748849999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18800,"MURRAYLINKV5_20211201203644","2015-12-27T13:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-11.407679999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18803,"MURRAYLINKV5_20211201203644","2015-12-27T14:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.59121,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18812,"MURRAYLINKV5_20211201203644","2015-12-27T18:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.4069,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18820,"MURRAYLINKV5_20211201203644","2015-12-27T19:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.17792,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18831,"MURRAYLINKV5_20211201203644","2015-12-27T20:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.610569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18838,"MURRAYLINKV5_20211201203644","2015-12-27T23:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.78509,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18850,"MURRAYLINKV5_20211201203644","2015-12-28T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.776199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18856,"MURRAYLINKV5_20211201203644","2015-12-28T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.11778,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18861,"MURRAYLINKV5_20211201203644","2015-12-28T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.65607,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18874,"MURRAYLINKV5_20211201203644","2015-12-28T08:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.601419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18880,"MURRAYLINKV5_20211201203644","2015-12-28T08:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.909470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18892,"MURRAYLINKV5_20211201203644","2015-12-28T09:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.782539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18899,"MURRAYLINKV5_20211201203644","2015-12-28T10:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.2751,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18906,"MURRAYLINKV5_20211201203644","2015-12-28T11:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.259969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18918,"MURRAYLINKV5_20211201203644","2015-12-28T12:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.28886,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18924,"MURRAYLINKV5_20211201203644","2015-12-28T13:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.712059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18928,"MURRAYLINKV5_20211201203644","2015-12-28T13:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.71945,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18929,"MURRAYLINKV5_20211201203644","2015-12-28T14:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.04101,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18930,"MURRAYLINKV5_20211201203644","2015-12-28T14:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.884319999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18931,"MURRAYLINKV5_20211201203644","2015-12-28T14:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.04449,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18932,"MURRAYLINKV5_20211201203644","2015-12-28T14:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.779719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18933,"MURRAYLINKV5_20211201203644","2015-12-28T14:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.58329,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18934,"MURRAYLINKV5_20211201203644","2015-12-28T14:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.299250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18935,"MURRAYLINKV5_20211201203644","2015-12-28T14:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.757540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18936,"MURRAYLINKV5_20211201203644","2015-12-28T14:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.98067,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18937,"MURRAYLINKV5_20211201203644","2015-12-28T14:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.77872,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18938,"MURRAYLINKV5_20211201203644","2015-12-28T14:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.120380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18939,"MURRAYLINKV5_20211201203644","2015-12-28T14:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.799250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18940,"MURRAYLINKV5_20211201203644","2015-12-28T15:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.552809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18941,"MURRAYLINKV5_20211201203644","2015-12-28T15:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.40479,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18942,"MURRAYLINKV5_20211201203644","2015-12-28T15:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.793200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18943,"MURRAYLINKV5_20211201203644","2015-12-28T15:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.62773,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18944,"MURRAYLINKV5_20211201203644","2015-12-28T15:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.807370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18945,"MURRAYLINKV5_20211201203644","2015-12-28T15:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.520849999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18946,"MURRAYLINKV5_20211201203644","2015-12-28T15:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.74362,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18947,"MURRAYLINKV5_20211201203644","2015-12-28T15:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.40987,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18948,"MURRAYLINKV5_20211201203644","2015-12-28T15:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.273,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18949,"MURRAYLINKV5_20211201203644","2015-12-28T15:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.420809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18950,"MURRAYLINKV5_20211201203644","2015-12-28T15:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.57879,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18951,"MURRAYLINKV5_20211201203644","2015-12-28T16:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.036950000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18952,"MURRAYLINKV5_20211201203644","2015-12-28T16:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.057410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18953,"MURRAYLINKV5_20211201203644","2015-12-28T16:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.158620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18954,"MURRAYLINKV5_20211201203644","2015-12-28T16:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.367249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18955,"MURRAYLINKV5_20211201203644","2015-12-28T16:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.090979999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18956,"MURRAYLINKV5_20211201203644","2015-12-28T16:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.813759999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18957,"MURRAYLINKV5_20211201203644","2015-12-28T16:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.860009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18958,"MURRAYLINKV5_20211201203644","2015-12-28T16:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.211500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18959,"MURRAYLINKV5_20211201203644","2015-12-28T16:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.52383,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18960,"MURRAYLINKV5_20211201203644","2015-12-28T16:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.703679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18961,"MURRAYLINKV5_20211201203644","2015-12-28T16:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.8508,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18962,"MURRAYLINKV5_20211201203644","2015-12-28T16:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.49803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18963,"MURRAYLINKV5_20211201203644","2015-12-28T17:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-24.19781,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18964,"MURRAYLINKV5_20211201203644","2015-12-28T17:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.182729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18965,"MURRAYLINKV5_20211201203644","2015-12-28T17:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.368590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18966,"MURRAYLINKV5_20211201203644","2015-12-28T17:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.733409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18967,"MURRAYLINKV5_20211201203644","2015-12-28T17:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.64096,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18968,"MURRAYLINKV5_20211201203644","2015-12-28T17:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.446169999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18969,"MURRAYLINKV5_20211201203644","2015-12-28T17:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.452649999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18970,"MURRAYLINKV5_20211201203644","2015-12-28T17:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.612469999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18971,"MURRAYLINKV5_20211201203644","2015-12-28T17:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.89832,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18972,"MURRAYLINKV5_20211201203644","2015-12-28T17:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.922910000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18973,"MURRAYLINKV5_20211201203644","2015-12-28T17:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.52685,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18974,"MURRAYLINKV5_20211201203644","2015-12-28T17:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.014610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18975,"MURRAYLINKV5_20211201203644","2015-12-28T18:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.65612,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18976,"MURRAYLINKV5_20211201203644","2015-12-28T18:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.882989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18977,"MURRAYLINKV5_20211201203644","2015-12-28T18:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.869009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18978,"MURRAYLINKV5_20211201203644","2015-12-28T18:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.42831,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18979,"MURRAYLINKV5_20211201203644","2015-12-28T18:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.94049,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18980,"MURRAYLINKV5_20211201203644","2015-12-28T18:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.669359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18981,"MURRAYLINKV5_20211201203644","2015-12-28T18:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.535699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18982,"MURRAYLINKV5_20211201203644","2015-12-28T18:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.43432,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18983,"MURRAYLINKV5_20211201203644","2015-12-28T18:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.125229999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18984,"MURRAYLINKV5_20211201203644","2015-12-28T18:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.31854,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18985,"MURRAYLINKV5_20211201203644","2015-12-28T18:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.495529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18986,"MURRAYLINKV5_20211201203644","2015-12-28T18:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.041519999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18987,"MURRAYLINKV5_20211201203644","2015-12-28T19:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.545870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18988,"MURRAYLINKV5_20211201203644","2015-12-28T19:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.353459999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18989,"MURRAYLINKV5_20211201203644","2015-12-28T19:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.356269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18990,"MURRAYLINKV5_20211201203644","2015-12-28T19:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.1844,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18991,"MURRAYLINKV5_20211201203644","2015-12-28T19:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.212689999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18992,"MURRAYLINKV5_20211201203644","2015-12-28T19:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.91724,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18993,"MURRAYLINKV5_20211201203644","2015-12-28T19:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.565439999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18994,"MURRAYLINKV5_20211201203644","2015-12-28T19:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.881319999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18995,"MURRAYLINKV5_20211201203644","2015-12-28T19:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-28.51473,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18996,"MURRAYLINKV5_20211201203644","2015-12-28T19:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-28.49578,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18997,"MURRAYLINKV5_20211201203644","2015-12-28T19:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.26426,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18998,"MURRAYLINKV5_20211201203644","2015-12-28T19:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.618320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[18999,"MURRAYLINKV5_20211201203644","2015-12-28T20:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.83272,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19000,"MURRAYLINKV5_20211201203644","2015-12-28T20:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.51604,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19001,"MURRAYLINKV5_20211201203644","2015-12-28T20:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.84385,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19002,"MURRAYLINKV5_20211201203644","2015-12-28T20:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.377770000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19003,"MURRAYLINKV5_20211201203644","2015-12-28T20:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.865559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19004,"MURRAYLINKV5_20211201203644","2015-12-28T20:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.761379999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19005,"MURRAYLINKV5_20211201203644","2015-12-28T20:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.28093,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19006,"MURRAYLINKV5_20211201203644","2015-12-28T20:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.007239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19007,"MURRAYLINKV5_20211201203644","2015-12-28T20:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.82225,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19008,"MURRAYLINKV5_20211201203644","2015-12-28T20:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.82469,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19009,"MURRAYLINKV5_20211201203644","2015-12-28T20:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.495290000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19010,"MURRAYLINKV5_20211201203644","2015-12-28T20:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.282080000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19011,"MURRAYLINKV5_20211201203644","2015-12-28T21:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.65216,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19012,"MURRAYLINKV5_20211201203644","2015-12-28T21:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.19082,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19013,"MURRAYLINKV5_20211201203644","2015-12-28T21:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.18084,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19014,"MURRAYLINKV5_20211201203644","2015-12-28T21:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.209110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19015,"MURRAYLINKV5_20211201203644","2015-12-28T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.331329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19016,"MURRAYLINKV5_20211201203644","2015-12-28T21:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.999180000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19017,"MURRAYLINKV5_20211201203644","2015-12-28T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.52239,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19018,"MURRAYLINKV5_20211201203644","2015-12-28T21:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.75305,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19019,"MURRAYLINKV5_20211201203644","2015-12-28T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.9992,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19020,"MURRAYLINKV5_20211201203644","2015-12-28T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.884130000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19021,"MURRAYLINKV5_20211201203644","2015-12-28T22:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-12.893079999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19022,"MURRAYLINKV5_20211201203644","2015-12-28T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.321680000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19023,"MURRAYLINKV5_20211201203644","2015-12-28T22:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.807729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19024,"MURRAYLINKV5_20211201203644","2015-12-28T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.81451,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19025,"MURRAYLINKV5_20211201203644","2015-12-28T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.657069999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19026,"MURRAYLINKV5_20211201203644","2015-12-28T23:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-11.26061,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19027,"MURRAYLINKV5_20211201203644","2015-12-28T23:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.749359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19028,"MURRAYLINKV5_20211201203644","2015-12-28T23:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-10.302099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19029,"MURRAYLINKV5_20211201203644","2015-12-28T23:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.347529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19030,"MURRAYLINKV5_20211201203644","2015-12-28T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.09863,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19031,"MURRAYLINKV5_20211201203644","2015-12-28T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.755800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19032,"MURRAYLINKV5_20211201203644","2015-12-28T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.453720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19033,"MURRAYLINKV5_20211201203644","2015-12-29T00:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.09079,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19034,"MURRAYLINKV5_20211201203644","2015-12-29T00:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.063980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19035,"MURRAYLINKV5_20211201203644","2015-12-29T00:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.89495,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19036,"MURRAYLINKV5_20211201203644","2015-12-29T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.28898,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19037,"MURRAYLINKV5_20211201203644","2015-12-29T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.293430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19038,"MURRAYLINKV5_20211201203644","2015-12-29T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.7172,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19039,"MURRAYLINKV5_20211201203644","2015-12-29T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.14522,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19040,"MURRAYLINKV5_20211201203644","2015-12-29T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.571,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19041,"MURRAYLINKV5_20211201203644","2015-12-29T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.387040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19042,"MURRAYLINKV5_20211201203644","2015-12-29T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.31639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19043,"MURRAYLINKV5_20211201203644","2015-12-29T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.569520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19044,"MURRAYLINKV5_20211201203644","2015-12-29T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.34869,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19045,"MURRAYLINKV5_20211201203644","2015-12-29T01:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.53533,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19046,"MURRAYLINKV5_20211201203644","2015-12-29T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.44285,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19047,"MURRAYLINKV5_20211201203644","2015-12-29T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.14207,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19048,"MURRAYLINKV5_20211201203644","2015-12-29T05:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.17109,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19049,"MURRAYLINKV5_20211201203644","2015-12-29T13:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",1,-31.782769999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19050,"MURRAYLINKV5_20211201203644","2015-12-29T13:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",1,-29.350580000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19051,"MURRAYLINKV5_20211201203644","2015-12-29T13:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",1,-21.656770000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19052,"MURRAYLINKV5_20211201203644","2015-12-29T13:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-20.379629999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19053,"MURRAYLINKV5_20211201203644","2015-12-29T13:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-24.898820000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19054,"MURRAYLINKV5_20211201203644","2015-12-29T13:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.49973,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19055,"MURRAYLINKV5_20211201203644","2015-12-29T14:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.92253,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19056,"MURRAYLINKV5_20211201203644","2015-12-29T14:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.918150000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19057,"MURRAYLINKV5_20211201203644","2015-12-29T14:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-18.622450000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19058,"MURRAYLINKV5_20211201203644","2015-12-29T14:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-22.555869999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19059,"MURRAYLINKV5_20211201203644","2015-12-29T14:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-135.45806999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19060,"MURRAYLINKV5_20211201203644","2015-12-29T14:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-141.30359999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19061,"MURRAYLINKV5_20211201203644","2015-12-29T14:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-147.33058,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19062,"MURRAYLINKV5_20211201203644","2015-12-29T14:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-143.29040000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19063,"MURRAYLINKV5_20211201203644","2015-12-29T14:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-135.75118000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19064,"MURRAYLINKV5_20211201203644","2015-12-29T14:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-130.16102000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19065,"MURRAYLINKV5_20211201203644","2015-12-29T14:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-148.63086000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19066,"MURRAYLINKV5_20211201203644","2015-12-29T14:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-130.08123000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19067,"MURRAYLINKV5_20211201203644","2015-12-29T15:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-138.56227999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19068,"MURRAYLINKV5_20211201203644","2015-12-29T15:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-134.99995999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19069,"MURRAYLINKV5_20211201203644","2015-12-29T15:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-153.65648999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19070,"MURRAYLINKV5_20211201203644","2015-12-29T15:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-156.09123,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19071,"MURRAYLINKV5_20211201203644","2015-12-29T15:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-148.11264,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19072,"MURRAYLINKV5_20211201203644","2015-12-29T15:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-154.71933000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19073,"MURRAYLINKV5_20211201203644","2015-12-29T15:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-148.32052999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19074,"MURRAYLINKV5_20211201203644","2015-12-29T15:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-276.23421000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19075,"MURRAYLINKV5_20211201203644","2015-12-29T15:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-344.56441000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19076,"MURRAYLINKV5_20211201203644","2015-12-29T15:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-411.67104999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19077,"MURRAYLINKV5_20211201203644","2015-12-29T15:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-407.61342000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19078,"MURRAYLINKV5_20211201203644","2015-12-29T15:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-395.01315,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19079,"MURRAYLINKV5_20211201203644","2015-12-29T16:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-394.21616,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19080,"MURRAYLINKV5_20211201203644","2015-12-29T16:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-260.49331999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19081,"MURRAYLINKV5_20211201203644","2015-12-29T16:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-282.94520999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19082,"MURRAYLINKV5_20211201203644","2015-12-29T16:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-403.55579,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19083,"MURRAYLINKV5_20211201203644","2015-12-29T16:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-496.8349,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19084,"MURRAYLINKV5_20211201203644","2015-12-29T16:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-493.94967000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19085,"MURRAYLINKV5_20211201203644","2015-12-29T16:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-501.70420999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19086,"MURRAYLINKV5_20211201203644","2015-12-29T16:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-501.70420999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19087,"MURRAYLINKV5_20211201203644","2015-12-29T16:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-497.72584999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19088,"MURRAYLINKV5_20211201203644","2015-12-29T16:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-491.27591999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19089,"MURRAYLINKV5_20211201203644","2015-12-29T16:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-504.12437,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19090,"MURRAYLINKV5_20211201203644","2015-12-29T16:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-506.54451999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19091,"MURRAYLINKV5_20211201203644","2015-12-29T17:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-505.96832000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19092,"MURRAYLINKV5_20211201203644","2015-12-29T17:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-494.21494999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19093,"MURRAYLINKV5_20211201203644","2015-12-29T17:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-407.61342000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19094,"MURRAYLINKV5_20211201203644","2015-12-29T17:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-496.71816000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19095,"MURRAYLINKV5_20211201203644","2015-12-29T17:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-493.62317999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19096,"MURRAYLINKV5_20211201203644","2015-12-29T17:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-307.90571999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19097,"MURRAYLINKV5_20211201203644","2015-12-29T17:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-490.91653000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19098,"MURRAYLINKV5_20211201203644","2015-12-29T17:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-411.67104999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19099,"MURRAYLINKV5_20211201203644","2015-12-29T17:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-485.15255000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19100,"MURRAYLINKV5_20211201203644","2015-12-29T17:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-470.34697999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19101,"MURRAYLINKV5_20211201203644","2015-12-29T17:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-402.20130999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19102,"MURRAYLINKV5_20211201203644","2015-12-29T18:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-258.38285000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19103,"MURRAYLINKV5_20211201203644","2015-12-29T18:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-18.826339999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19104,"MURRAYLINKV5_20211201203644","2015-12-29T18:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-100.89327,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19105,"MURRAYLINKV5_20211201203644","2015-12-29T18:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-104.68593,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19106,"MURRAYLINKV5_20211201203644","2015-12-29T18:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-88.182990000000004,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19107,"MURRAYLINKV5_20211201203644","2015-12-29T18:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-104.95905,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19108,"MURRAYLINKV5_20211201203644","2015-12-29T18:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-49.463030000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19109,"MURRAYLINKV5_20211201203644","2015-12-29T18:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-48.64761,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19110,"MURRAYLINKV5_20211201203644","2015-12-29T18:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-38.088479999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19111,"MURRAYLINKV5_20211201203644","2015-12-29T18:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-48.044040000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19112,"MURRAYLINKV5_20211201203644","2015-12-29T18:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-33.491019999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19113,"MURRAYLINKV5_20211201203644","2015-12-29T18:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-49.314880000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19114,"MURRAYLINKV5_20211201203644","2015-12-29T19:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-42.488689999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19115,"MURRAYLINKV5_20211201203644","2015-12-29T19:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-30.61121,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19116,"MURRAYLINKV5_20211201203644","2015-12-29T19:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-42.807380000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19117,"MURRAYLINKV5_20211201203644","2015-12-29T19:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.79604,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19118,"MURRAYLINKV5_20211201203644","2015-12-29T19:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-11.613849999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19119,"MURRAYLINKV5_20211201203644","2015-12-29T19:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.44746,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19120,"MURRAYLINKV5_20211201203644","2015-12-29T20:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.92159,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19121,"MURRAYLINKV5_20211201203644","2015-12-29T20:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.11937,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19122,"MURRAYLINKV5_20211201203644","2015-12-29T20:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.684659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19123,"MURRAYLINKV5_20211201203644","2015-12-29T21:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.682829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19124,"MURRAYLINKV5_20211201203644","2015-12-29T21:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.81217,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19125,"MURRAYLINKV5_20211201203644","2015-12-29T21:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.516959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19126,"MURRAYLINKV5_20211201203644","2015-12-29T21:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.505509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19127,"MURRAYLINKV5_20211201203644","2015-12-29T21:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.386939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19128,"MURRAYLINKV5_20211201203644","2015-12-29T21:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.146280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19129,"MURRAYLINKV5_20211201203644","2015-12-29T21:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.09464,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19130,"MURRAYLINKV5_20211201203644","2015-12-29T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.16226,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19131,"MURRAYLINKV5_20211201203644","2015-12-29T21:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.13125,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19132,"MURRAYLINKV5_20211201203644","2015-12-29T21:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.48052,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19133,"MURRAYLINKV5_20211201203644","2015-12-29T21:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.67719,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19134,"MURRAYLINKV5_20211201203644","2015-12-29T22:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.404059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19135,"MURRAYLINKV5_20211201203644","2015-12-29T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-54.482170000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19136,"MURRAYLINKV5_20211201203644","2015-12-29T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-32.771030000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19137,"MURRAYLINKV5_20211201203644","2015-12-29T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-33.455289999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19138,"MURRAYLINKV5_20211201203644","2015-12-29T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-31.933509999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19139,"MURRAYLINKV5_20211201203644","2015-12-29T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.336690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19140,"MURRAYLINKV5_20211201203644","2015-12-29T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.079070000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19141,"MURRAYLINKV5_20211201203644","2015-12-29T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.793970000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19142,"MURRAYLINKV5_20211201203644","2015-12-29T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.64828,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19143,"MURRAYLINKV5_20211201203644","2015-12-29T22:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.777290000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19144,"MURRAYLINKV5_20211201203644","2015-12-29T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.954719999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19145,"MURRAYLINKV5_20211201203644","2015-12-29T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.96912,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19146,"MURRAYLINKV5_20211201203644","2015-12-29T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-22.469650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19147,"MURRAYLINKV5_20211201203644","2015-12-29T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.002929999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19148,"MURRAYLINKV5_20211201203644","2015-12-29T23:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.12627,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19149,"MURRAYLINKV5_20211201203644","2015-12-29T23:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.674040000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19150,"MURRAYLINKV5_20211201203644","2015-12-29T23:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.89892,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19151,"MURRAYLINKV5_20211201203644","2015-12-29T23:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.60909,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19152,"MURRAYLINKV5_20211201203644","2015-12-29T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.79522,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19153,"MURRAYLINKV5_20211201203644","2015-12-30","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.260280000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19154,"MURRAYLINKV5_20211201203644","2015-12-30T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.50595,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19155,"MURRAYLINKV5_20211201203644","2015-12-30T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.09003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19156,"MURRAYLINKV5_20211201203644","2015-12-30T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.49029,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19157,"MURRAYLINKV5_20211201203644","2015-12-30T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.028650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19158,"MURRAYLINKV5_20211201203644","2015-12-30T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.77159,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19159,"MURRAYLINKV5_20211201203644","2015-12-30T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.77731,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19160,"MURRAYLINKV5_20211201203644","2015-12-30T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.33089,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19161,"MURRAYLINKV5_20211201203644","2015-12-30T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.058260000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19162,"MURRAYLINKV5_20211201203644","2015-12-30T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.341139999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19163,"MURRAYLINKV5_20211201203644","2015-12-30T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.3292,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19164,"MURRAYLINKV5_20211201203644","2015-12-30T06:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.243410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19165,"MURRAYLINKV5_20211201203644","2015-12-30T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.90906,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19166,"MURRAYLINKV5_20211201203644","2015-12-30T06:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.187749999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19167,"MURRAYLINKV5_20211201203644","2015-12-30T06:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.19345,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19168,"MURRAYLINKV5_20211201203644","2015-12-30T06:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.205120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19169,"MURRAYLINKV5_20211201203644","2015-12-30T06:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.791700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19170,"MURRAYLINKV5_20211201203644","2015-12-30T06:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.513019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19171,"MURRAYLINKV5_20211201203644","2015-12-30T06:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.5261,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19172,"MURRAYLINKV5_20211201203644","2015-12-30T06:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.53702,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19173,"MURRAYLINKV5_20211201203644","2015-12-30T06:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.55259,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19174,"MURRAYLINKV5_20211201203644","2015-12-30T07:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.56635,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19175,"MURRAYLINKV5_20211201203644","2015-12-30T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.97959,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19176,"MURRAYLINKV5_20211201203644","2015-12-30T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.267670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19177,"MURRAYLINKV5_20211201203644","2015-12-30T07:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.09272,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19178,"MURRAYLINKV5_20211201203644","2015-12-30T07:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.72813,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19179,"MURRAYLINKV5_20211201203644","2015-12-30T12:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-31.980869999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19180,"MURRAYLINKV5_20211201203644","2015-12-30T13:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.206980000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19181,"MURRAYLINKV5_20211201203644","2015-12-30T13:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-24.831489999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19182,"MURRAYLINKV5_20211201203644","2015-12-30T13:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-25.056170000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19183,"MURRAYLINKV5_20211201203644","2015-12-30T13:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-29.621659999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19184,"MURRAYLINKV5_20211201203644","2015-12-30T13:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-11.578799999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19185,"MURRAYLINKV5_20211201203644","2015-12-30T13:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.66919,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19186,"MURRAYLINKV5_20211201203644","2015-12-30T13:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-533.78626999999994,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19187,"MURRAYLINKV5_20211201203644","2015-12-30T13:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-187.28384,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19188,"MURRAYLINKV5_20211201203644","2015-12-30T13:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-164.02885000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19189,"MURRAYLINKV5_20211201203644","2015-12-30T13:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-325.00126,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19190,"MURRAYLINKV5_20211201203644","2015-12-30T13:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-40.648060000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19191,"MURRAYLINKV5_20211201203644","2015-12-30T14:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.89978,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19192,"MURRAYLINKV5_20211201203644","2015-12-30T14:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-138.41248999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19193,"MURRAYLINKV5_20211201203644","2015-12-30T14:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-92.238780000000006,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19194,"MURRAYLINKV5_20211201203644","2015-12-30T14:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-493.65102000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19195,"MURRAYLINKV5_20211201203644","2015-12-30T14:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.21425,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19196,"MURRAYLINKV5_20211201203644","2015-12-30T14:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-503.21035999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19197,"MURRAYLINKV5_20211201203644","2015-12-30T14:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.21425,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19198,"MURRAYLINKV5_20211201203644","2015-12-30T14:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-355.31882000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19199,"MURRAYLINKV5_20211201203644","2015-12-30T14:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-62.167029999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19200,"MURRAYLINKV5_20211201203644","2015-12-30T14:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-346.58785,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19201,"MURRAYLINKV5_20211201203644","2015-12-30T14:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-16.73997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19202,"MURRAYLINKV5_20211201203644","2015-12-30T14:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-491.21980000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19203,"MURRAYLINKV5_20211201203644","2015-12-30T14:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-17.75057,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19204,"MURRAYLINKV5_20211201203644","2015-12-30T14:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-490.99488000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19205,"MURRAYLINKV5_20211201203644","2015-12-30T14:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-510.33228000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19206,"MURRAYLINKV5_20211201203644","2015-12-30T14:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-492.91496999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19207,"MURRAYLINKV5_20211201203644","2015-12-30T14:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-492.40847000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19208,"MURRAYLINKV5_20211201203644","2015-12-30T15:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-41.605690000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19209,"MURRAYLINKV5_20211201203644","2015-12-30T15:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-417.92140000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19210,"MURRAYLINKV5_20211201203644","2015-12-30T15:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-467.33327000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19211,"MURRAYLINKV5_20211201203644","2015-12-30T15:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-516.46321,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19212,"MURRAYLINKV5_20211201203644","2015-12-30T15:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-510.22545000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19213,"MURRAYLINKV5_20211201203644","2015-12-30T15:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-1898.3164200000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19214,"MURRAYLINKV5_20211201203644","2015-12-30T15:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-433.82184999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19215,"MURRAYLINKV5_20211201203644","2015-12-30T15:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-478.55916999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19216,"MURRAYLINKV5_20211201203644","2015-12-30T15:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-75.038089999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19217,"MURRAYLINKV5_20211201203644","2015-12-30T15:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.497159999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19218,"MURRAYLINKV5_20211201203644","2015-12-30T16:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-1765.5223699999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19219,"MURRAYLINKV5_20211201203644","2015-12-30T16:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-199.47187,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19220,"MURRAYLINKV5_20211201203644","2015-12-30T16:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2216.1375600000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19221,"MURRAYLINKV5_20211201203644","2015-12-30T16:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-661.03611000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19222,"MURRAYLINKV5_20211201203644","2015-12-30T16:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.34623,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19223,"MURRAYLINKV5_20211201203644","2015-12-30T16:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2237.4931700000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19224,"MURRAYLINKV5_20211201203644","2015-12-30T16:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.423590000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19225,"MURRAYLINKV5_20211201203644","2015-12-30T16:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.900880000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19226,"MURRAYLINKV5_20211201203644","2015-12-30T16:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-371.07844,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19227,"MURRAYLINKV5_20211201203644","2015-12-30T16:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-4453.1961000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19228,"MURRAYLINKV5_20211201203644","2015-12-30T16:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-527.59118000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19229,"MURRAYLINKV5_20211201203644","2015-12-30T16:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-434.54226999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19230,"MURRAYLINKV5_20211201203644","2015-12-30T16:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-137.37217000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19231,"MURRAYLINKV5_20211201203644","2015-12-30T16:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-1888.6385499999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19232,"MURRAYLINKV5_20211201203644","2015-12-30T17:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-1925.85481,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19233,"MURRAYLINKV5_20211201203644","2015-12-30T17:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-516.88845000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19234,"MURRAYLINKV5_20211201203644","2015-12-30T17:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-544.88954000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19235,"MURRAYLINKV5_20211201203644","2015-12-30T17:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-485.72313000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19236,"MURRAYLINKV5_20211201203644","2015-12-30T17:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-513.33160999999996,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19237,"MURRAYLINKV5_20211201203644","2015-12-30T17:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.70294,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19238,"MURRAYLINKV5_20211201203644","2015-12-30T17:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-475.30139000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19239,"MURRAYLINKV5_20211201203644","2015-12-30T17:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-465.42227000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19240,"MURRAYLINKV5_20211201203644","2015-12-30T17:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-4544.4625500000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19241,"MURRAYLINKV5_20211201203644","2015-12-30T17:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-505.46051999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19242,"MURRAYLINKV5_20211201203644","2015-12-30T17:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-22.23564,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19243,"MURRAYLINKV5_20211201203644","2015-12-30T17:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-496.84733,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19244,"MURRAYLINKV5_20211201203644","2015-12-30T17:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.80123,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19245,"MURRAYLINKV5_20211201203644","2015-12-30T17:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.46208,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19246,"MURRAYLINKV5_20211201203644","2015-12-30T17:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.974819999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19247,"MURRAYLINKV5_20211201203644","2015-12-30T17:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.06587,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19248,"MURRAYLINKV5_20211201203644","2015-12-30T18:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-232.84339,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19249,"MURRAYLINKV5_20211201203644","2015-12-30T18:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2205.7202400000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19250,"MURRAYLINKV5_20211201203644","2015-12-30T18:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-32.993220000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19251,"MURRAYLINKV5_20211201203644","2015-12-30T18:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-491.60820999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19252,"MURRAYLINKV5_20211201203644","2015-12-30T18:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.83559,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19253,"MURRAYLINKV5_20211201203644","2015-12-30T18:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.282730000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19254,"MURRAYLINKV5_20211201203644","2015-12-30T18:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.46467,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19255,"MURRAYLINKV5_20211201203644","2015-12-30T18:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-537.52867000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19256,"MURRAYLINKV5_20211201203644","2015-12-30T18:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.885910000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19257,"MURRAYLINKV5_20211201203644","2015-12-30T18:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.816000000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19258,"MURRAYLINKV5_20211201203644","2015-12-30T19:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-441.00977,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19259,"MURRAYLINKV5_20211201203644","2015-12-30T19:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-497.14594,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19260,"MURRAYLINKV5_20211201203644","2015-12-30T19:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-498.26294999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19261,"MURRAYLINKV5_20211201203644","2015-12-30T19:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-493.62151,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19262,"MURRAYLINKV5_20211201203644","2015-12-30T20:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.39123,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19263,"MURRAYLINKV5_20211201203644","2015-12-30T20:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.194850000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19264,"MURRAYLINKV5_20211201203644","2015-12-30T20:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-59.331429999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19265,"MURRAYLINKV5_20211201203644","2015-12-30T20:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-57.29233,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19266,"MURRAYLINKV5_20211201203644","2015-12-30T20:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-405.92187000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19267,"MURRAYLINKV5_20211201203644","2015-12-30T20:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-121.59778,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19268,"MURRAYLINKV5_20211201203644","2015-12-30T20:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-114.92759,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19269,"MURRAYLINKV5_20211201203644","2015-12-30T21:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.625879999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19270,"MURRAYLINKV5_20211201203644","2015-12-30T21:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-17.333729999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19271,"MURRAYLINKV5_20211201203644","2015-12-30T21:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-27.494140000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19272,"MURRAYLINKV5_20211201203644","2015-12-30T22:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.91329,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19273,"MURRAYLINKV5_20211201203644","2015-12-30T22:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-11.64175,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19274,"MURRAYLINKV5_20211201203644","2015-12-30T22:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-13.859,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19275,"MURRAYLINKV5_20211201203644","2015-12-30T22:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.507960000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19276,"MURRAYLINKV5_20211201203644","2015-12-30T22:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.334129999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19277,"MURRAYLINKV5_20211201203644","2015-12-30T23:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-27.582619999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19278,"MURRAYLINKV5_20211201203644","2015-12-30T23:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-20.621169999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19279,"MURRAYLINKV5_20211201203644","2015-12-30T23:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.907630000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19280,"MURRAYLINKV5_20211201203644","2015-12-30T23:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-18.709160000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19281,"MURRAYLINKV5_20211201203644","2015-12-30T23:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-30.999510000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19282,"MURRAYLINKV5_20211201203644","2015-12-30T23:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-28.510149999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19283,"MURRAYLINKV5_20211201203644","2015-12-31T00:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-13.44115,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19284,"MURRAYLINKV5_20211201203644","2015-12-31T00:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-11.870810000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19285,"MURRAYLINKV5_20211201203644","2015-12-31T01:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-28.073039999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19286,"MURRAYLINKV5_20211201203644","2015-12-31T01:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-28.72242,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19287,"MURRAYLINKV5_20211201203644","2015-12-31T01:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-95.166659999999993,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19288,"MURRAYLINKV5_20211201203644","2015-12-31T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-37.021099999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19289,"MURRAYLINKV5_20211201203644","2015-12-31T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.373360000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19290,"MURRAYLINKV5_20211201203644","2015-12-31T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.786720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19291,"MURRAYLINKV5_20211201203644","2015-12-31T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.134829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19292,"MURRAYLINKV5_20211201203644","2015-12-31T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.10952,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19293,"MURRAYLINKV5_20211201203644","2015-12-31T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.47932,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19294,"MURRAYLINKV5_20211201203644","2015-12-31T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.740500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19295,"MURRAYLINKV5_20211201203644","2015-12-31T02:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.44402,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19296,"MURRAYLINKV5_20211201203644","2015-12-31T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.44238,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19297,"MURRAYLINKV5_20211201203644","2015-12-31T02:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.168419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19298,"MURRAYLINKV5_20211201203644","2015-12-31T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.7989,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19299,"MURRAYLINKV5_20211201203644","2015-12-31T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.798629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19300,"MURRAYLINKV5_20211201203644","2015-12-31T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.53872,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19301,"MURRAYLINKV5_20211201203644","2015-12-31T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.272919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19302,"MURRAYLINKV5_20211201203644","2015-12-31T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.011189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19303,"MURRAYLINKV5_20211201203644","2015-12-31T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.63654,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19304,"MURRAYLINKV5_20211201203644","2015-12-31T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.27567,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19305,"MURRAYLINKV5_20211201203644","2015-12-31T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.29998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19306,"MURRAYLINKV5_20211201203644","2015-12-31T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.63862,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19307,"MURRAYLINKV5_20211201203644","2015-12-31T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.31583,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19308,"MURRAYLINKV5_20211201203644","2015-12-31T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.313800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19309,"MURRAYLINKV5_20211201203644","2015-12-31T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.33412,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19310,"MURRAYLINKV5_20211201203644","2015-12-31T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.33244,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19311,"MURRAYLINKV5_20211201203644","2015-12-31T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.94753,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19312,"MURRAYLINKV5_20211201203644","2015-12-31T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.58178,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19313,"MURRAYLINKV5_20211201203644","2015-12-31T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.948449999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19314,"MURRAYLINKV5_20211201203644","2015-12-31T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.620760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19315,"MURRAYLINKV5_20211201203644","2015-12-31T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.13555,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19316,"MURRAYLINKV5_20211201203644","2015-12-31T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.24602,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19317,"MURRAYLINKV5_20211201203644","2015-12-31T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.848850000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19318,"MURRAYLINKV5_20211201203644","2015-12-31T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.13921,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19319,"MURRAYLINKV5_20211201203644","2015-12-31T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.95637,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19320,"MURRAYLINKV5_20211201203644","2015-12-31T06:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.023720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19321,"MURRAYLINKV5_20211201203644","2015-12-31T11:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-69.018789999999996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19322,"MURRAYLINKV5_20211201203644","2015-12-31T11:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-60.103670000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19323,"MURRAYLINKV5_20211201203644","2015-12-31T11:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-84.712919999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19324,"MURRAYLINKV5_20211201203644","2015-12-31T11:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-105.98057,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19325,"MURRAYLINKV5_20211201203644","2015-12-31T11:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-105.98057,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19326,"MURRAYLINKV5_20211201203644","2015-12-31T11:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-105.98057,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19327,"MURRAYLINKV5_20211201203644","2015-12-31T11:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-55.6785,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19328,"MURRAYLINKV5_20211201203644","2015-12-31T11:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_2-5;V-NIL_PARALLEL_3-5;V-NIL_PARALLEL_6-2;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_6-2;V-NIL_PAR_6-2_BL;V-NIL_R2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-88.2393,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19329,"MURRAYLINKV5_20211201203644","2015-12-31T11:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-72.64076,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19330,"MURRAYLINKV5_20211201203644","2015-12-31T11:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-170.80306999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19331,"MURRAYLINKV5_20211201203644","2015-12-31T11:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-88.238420000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19332,"MURRAYLINKV5_20211201203644","2015-12-31T12:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-178.58054000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19333,"MURRAYLINKV5_20211201203644","2015-12-31T12:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-93.349630000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19334,"MURRAYLINKV5_20211201203644","2015-12-31T12:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-96.569659999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19335,"MURRAYLINKV5_20211201203644","2015-12-31T12:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-167.64654999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19336,"MURRAYLINKV5_20211201203644","2015-12-31T12:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-491.61901999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19337,"MURRAYLINKV5_20211201203644","2015-12-31T12:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-487.40620000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19338,"MURRAYLINKV5_20211201203644","2015-12-31T12:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-25.92952,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19339,"MURRAYLINKV5_20211201203644","2015-12-31T12:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-209.70672999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19340,"MURRAYLINKV5_20211201203644","2015-12-31T12:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-18.983750000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19341,"MURRAYLINKV5_20211201203644","2015-12-31T12:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-216.67176000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19342,"MURRAYLINKV5_20211201203644","2015-12-31T12:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-230.16207,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19343,"MURRAYLINKV5_20211201203644","2015-12-31T12:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-99.556479999999993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19344,"MURRAYLINKV5_20211201203644","2015-12-31T12:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-176.07686000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19345,"MURRAYLINKV5_20211201203644","2015-12-31T12:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-177.61680999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19346,"MURRAYLINKV5_20211201203644","2015-12-31T13:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-200.78514999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19347,"MURRAYLINKV5_20211201203644","2015-12-31T13:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-170.24719999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19348,"MURRAYLINKV5_20211201203644","2015-12-31T13:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-160.8706,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19349,"MURRAYLINKV5_20211201203644","2015-12-31T13:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-162.84007,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19350,"MURRAYLINKV5_20211201203644","2015-12-31T13:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-97.484120000000004,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19351,"MURRAYLINKV5_20211201203644","2015-12-31T13:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-174.37522999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19352,"MURRAYLINKV5_20211201203644","2015-12-31T14:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-166.96088,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19353,"MURRAYLINKV5_20211201203644","2015-12-31T14:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-160.96826999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19354,"MURRAYLINKV5_20211201203644","2015-12-31T14:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-13.73321,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19355,"MURRAYLINKV5_20211201203644","2015-12-31T14:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-159.96749,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19356,"MURRAYLINKV5_20211201203644","2015-12-31T14:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-13.918699999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19357,"MURRAYLINKV5_20211201203644","2015-12-31T14:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-189.19368,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19358,"MURRAYLINKV5_20211201203644","2015-12-31T14:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-179.34037000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19359,"MURRAYLINKV5_20211201203644","2015-12-31T14:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-15.267060000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19360,"MURRAYLINKV5_20211201203644","2015-12-31T14:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-47.201500000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19361,"MURRAYLINKV5_20211201203644","2015-12-31T14:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-192.11311000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19362,"MURRAYLINKV5_20211201203644","2015-12-31T14:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.253769999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19363,"MURRAYLINKV5_20211201203644","2015-12-31T14:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-181.19389000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19364,"MURRAYLINKV5_20211201203644","2015-12-31T14:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-200.06575000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19365,"MURRAYLINKV5_20211201203644","2015-12-31T14:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-103.34504,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19366,"MURRAYLINKV5_20211201203644","2015-12-31T14:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-28.297090000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19367,"MURRAYLINKV5_20211201203644","2015-12-31T14:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-59.8065,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19368,"MURRAYLINKV5_20211201203644","2015-12-31T15:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-222.01223999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19369,"MURRAYLINKV5_20211201203644","2015-12-31T15:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2802.9344799999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19370,"MURRAYLINKV5_20211201203644","2015-12-31T15:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-849.62589000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19371,"MURRAYLINKV5_20211201203644","2015-12-31T15:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-186.85239999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19372,"MURRAYLINKV5_20211201203644","2015-12-31T15:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-221.69871000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19373,"MURRAYLINKV5_20211201203644","2015-12-31T15:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-223.71505999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19374,"MURRAYLINKV5_20211201203644","2015-12-31T15:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2578.8959399999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19375,"MURRAYLINKV5_20211201203644","2015-12-31T15:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2580.5219000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19376,"MURRAYLINKV5_20211201203644","2015-12-31T15:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-137.38218000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19377,"MURRAYLINKV5_20211201203644","2015-12-31T15:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-173.15493000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19378,"MURRAYLINKV5_20211201203644","2015-12-31T15:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-216.13494,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19379,"MURRAYLINKV5_20211201203644","2015-12-31T15:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-139.4366,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19380,"MURRAYLINKV5_20211201203644","2015-12-31T15:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-247.74827999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19381,"MURRAYLINKV5_20211201203644","2015-12-31T15:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-2472.7518300000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19382,"MURRAYLINKV5_20211201203644","2015-12-31T15:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-182.33484999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19383,"MURRAYLINKV5_20211201203644","2015-12-31T15:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-152.30109999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19384,"MURRAYLINKV5_20211201203644","2015-12-31T15:55:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-191.39750000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19385,"MURRAYLINKV5_20211201203644","2015-12-31T15:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-646.19813999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19386,"MURRAYLINKV5_20211201203644","2015-12-31T16:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-461.04379999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19387,"MURRAYLINKV5_20211201203644","2015-12-31T16:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-226.33252999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19388,"MURRAYLINKV5_20211201203644","2015-12-31T16:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-679.99363000000005,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19389,"MURRAYLINKV5_20211201203644","2015-12-31T16:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-171.99373,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19390,"MURRAYLINKV5_20211201203644","2015-12-31T16:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-627.42729999999995,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19391,"MURRAYLINKV5_20211201203644","2015-12-31T16:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-401.91867000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19392,"MURRAYLINKV5_20211201203644","2015-12-31T16:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-221.82930999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19393,"MURRAYLINKV5_20211201203644","2015-12-31T16:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-247.24921000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19394,"MURRAYLINKV5_20211201203644","2015-12-31T16:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-54.872419999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19395,"MURRAYLINKV5_20211201203644","2015-12-31T16:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-163.21152000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19396,"MURRAYLINKV5_20211201203644","2015-12-31T16:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-74.467510000000004,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19397,"MURRAYLINKV5_20211201203644","2015-12-31T16:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-49.947090000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19398,"MURRAYLINKV5_20211201203644","2015-12-31T16:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-80.066890000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19399,"MURRAYLINKV5_20211201203644","2015-12-31T16:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-77.520269999999996,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19400,"MURRAYLINKV5_20211201203644","2015-12-31T17:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-49.755189999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19401,"MURRAYLINKV5_20211201203644","2015-12-31T17:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-35.549349999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19402,"MURRAYLINKV5_20211201203644","2015-12-31T17:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-359.91660999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19403,"MURRAYLINKV5_20211201203644","2015-12-31T17:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-25.785489999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19404,"MURRAYLINKV5_20211201203644","2015-12-31T17:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-118.31811999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19405,"MURRAYLINKV5_20211201203644","2015-12-31T17:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-22.333649999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19406,"MURRAYLINKV5_20211201203644","2015-12-31T17:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.674530000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19407,"MURRAYLINKV5_20211201203644","2015-12-31T17:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-462.41059000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19408,"MURRAYLINKV5_20211201203644","2015-12-31T17:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.80255,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19409,"MURRAYLINKV5_20211201203644","2015-12-31T17:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-136.55785,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19410,"MURRAYLINKV5_20211201203644","2015-12-31T17:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-23.085070000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19411,"MURRAYLINKV5_20211201203644","2015-12-31T17:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-59.429160000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19412,"MURRAYLINKV5_20211201203644","2015-12-31T17:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-84.991280000000003,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19413,"MURRAYLINKV5_20211201203644","2015-12-31T18:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-76.886619999999994,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19414,"MURRAYLINKV5_20211201203644","2015-12-31T18:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-19.785609999999998,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19415,"MURRAYLINKV5_20211201203644","2015-12-31T18:10:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-39.568399999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19416,"MURRAYLINKV5_20211201203644","2015-12-31T18:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-90.935310000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19417,"MURRAYLINKV5_20211201203644","2015-12-31T18:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-27.03642,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19418,"MURRAYLINKV5_20211201203644","2015-12-31T18:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-18.22991,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19419,"MURRAYLINKV5_20211201203644","2015-12-31T18:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.99274,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19420,"MURRAYLINKV5_20211201203644","2015-12-31T18:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.36294,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19421,"MURRAYLINKV5_20211201203644","2015-12-31T18:40:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-11.992520000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19422,"MURRAYLINKV5_20211201203644","2015-12-31T18:45:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-12.10981,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19423,"MURRAYLINKV5_20211201203644","2015-12-31T19:15:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-52.024650000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19424,"MURRAYLINKV5_20211201203644","2015-12-31T21:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-16.053619999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19425,"MURRAYLINKV5_20211201203644","2015-12-31T21:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-21.478960000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19426,"MURRAYLINKV5_20211201203644","2015-12-31T22:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-20.711950000000002,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[19427,"MURRAYLINKV5_20211201203644","2015-12-31T23:35:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.918290000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,"","",null,null,0]