{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"MURRAYLINKV3_20170131122207"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"14.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14]]}
[null,null,null,null,null,"This workbook has not been successfully validated. Please validate before submission."]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"MURRAYLINK"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,3]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2016]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2016-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2017-01-01"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":2956}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":202}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":3158}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2016 Version: 3"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":202},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":2956},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":2956}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":3158},null,{"$f":"SUM($P$46:$P$65)","v":2956}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":39759,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[null,null,"2016-01-01T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.874309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.36975,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.131720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.81561,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.554690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.55278,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.547969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.23671,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.51451,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T05:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.77154,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T05:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.78138,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T12:20:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.761089999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T14:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-14.840579999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T15:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-18.265419999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T15:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-14.465579999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T15:50:00","V>>BABE_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-27.153040000000001,"Out= Nil, avoid O/L Ballarat to Bendigo 220kV line on trip of both Dederang to Glenrowan 220kV No.1 and No.3 lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T15:55:00","V>>BABE_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-28.406230000000001,"Out= Nil, avoid O/L Ballarat to Bendigo 220kV line on trip of both Dederang to Glenrowan 220kV No.1 and No.3 lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T16:00:00","V>>BABE_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-23.123049999999999,"Out= Nil, avoid O/L Ballarat to Bendigo 220kV line on trip of both Dederang to Glenrowan 220kV No.1 and No.3 lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T16:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.160159999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T16:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.569230000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T16:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.653379999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.97419,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.985189999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.29223,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.843109999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.843139999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.613060000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.602550000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.910799999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-23.661960000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.49452,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-11.972849999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T17:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.1526,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T18:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.34042,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.033580000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T18:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.02412,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T18:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.186669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-01T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.926069999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T07:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.131959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T07:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.64752,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T08:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.604979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T08:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.447900000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T09:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.251340000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T09:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.499879999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T10:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.44448,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T11:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.807689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T11:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.815899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.86468,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.344580000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.71002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.63908,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.20144,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.19727,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.21041,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T12:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.326230000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.733689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.23413,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.096679999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T13:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.23455,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.23617,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.256159999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.968830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.072369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.081670000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.07982,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.49699,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.50095,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T14:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.50264,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.506640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.52867,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.69003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.69988,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.853260000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.871029999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.87824,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.453760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.57358,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.899979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.57024,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.56836,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.74377,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.09815,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.93947,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.7995,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.0793,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.91873,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.41682,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.91344,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.900779999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.580290000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.86293,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.6556,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.47465,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-23.286449999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T16:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.42299,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.329789999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.65231,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.25248,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.766439999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.300509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.194940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.19666,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-26.508510000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.74029,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.87175,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.595939999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-168.53567000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-202.38336000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-163.37694999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T17:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-197.22459000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-196.24402000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-200.6789,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-21.362159999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-48.970970000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-236.63930999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-276.31027,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-257.66505999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-260.53023999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-252.90342999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-255.76667,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-221.61448999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-260.4735,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-190.72187,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-229.31138000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-207.18758,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-243.67124999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-290.86063999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-329.81301000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-411.27192000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-450.17243999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-207.96003999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-246.91240999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-154.46633,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T18:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-188.67711,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-162.60202000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-196.81279000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-150.80544,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-194.34826000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-150.54795999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-194.03892999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-157.96448000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-201.70478,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-141.75852,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-147.46646000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-148.20171999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-182.41218000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-189.16828000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-193.66073,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.682550000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.807219999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-186.45419000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-191.12727000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-153.75854000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-186.34227000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-154.76777999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T19:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-188.97838999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.023389999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-26.60106,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.005569999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.662189999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-26.223310000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-26.9283,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.39228,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-78.579689999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.629709999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.321059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T20:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.07113,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T21:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.42404,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T21:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.012219999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T21:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-20.18909,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.62416,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.291740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.438040000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.470969999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.429959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.44896,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.45457,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.867509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.30247,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T22:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.39053,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T23:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.524039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T23:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.35107,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T23:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.516310000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T23:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.98943,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-02T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.94768,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.241239999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.461119999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.29236,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.44415,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.873150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.15422,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T02:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.483000000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.58315,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.2095,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.667579999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.80071,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.784649999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-13.55246,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.41334,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.6623,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.55555,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.667,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.40788,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.845140000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.73592,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.82333,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T03:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.021509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.78838,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.11476,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.678100000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.737830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.735749999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.074769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.583019999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.69983,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.765879999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.91647,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.445819999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.195180000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.525539999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T04:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.47813,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T07:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.650119999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T07:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.663729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T08:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.130470000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T08:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.34252,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T11:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.241619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.826750000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T17:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.333600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.93383,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-20.651800000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.04712,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-20.575130000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-23.351710000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-22.646280000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.37721,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.21932,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.22683,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.56171,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T18:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.51939,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.48437,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.327909999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.05578,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.355869999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.3466,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.60746,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T19:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.60802,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.912710000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T22:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.62635,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.884919999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.427569999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T22:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.4215,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-03T23:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.57606,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T13:50:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-15.472530000000001,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T14:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-10.63899,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T14:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.013339999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T14:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.425990000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-15.84468,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-15.887370000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.515910000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.41131,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.764699999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.625830000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.654509999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.935750000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.80275,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.864050000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T18:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.87382,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T19:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.310739999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-04T23:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.56732,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T05:25:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-39.822539999999996,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T05:55:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-35.074019999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T06:00:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-32.887079999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T06:30:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-79.215159999999997,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T07:05:00","V>>SML_NIL_MLTS_N-2","V-BAML+MLTG_N-2","2015-12-29",2,-27.520099999999999,"Out= Nil, avoid O/L Elaine to Ballarat 220kV line section on trip of Moorabool to Ballarat and Moorabool to Terang 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-10.718159999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.732939999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.180019999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.06448,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-268.38432,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T18:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-231.07767999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T19:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.23047,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T19:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.016950000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T19:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.720510000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T19:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.5875,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T19:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.23021,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-05T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.26975,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-11.43023,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-11.40282,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.90292,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-11.09117,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-11.93689,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.92675,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-15.85624,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.926539999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T16:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-15.042389999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.401450000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-15.680149999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-16.495799999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-16.484359999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-17.56063,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.732749999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.666319999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.419740000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.700589999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.719480000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.745190000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T17:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-30.612829999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.505859999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.555959999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-32.705190000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-33.697380000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.795280000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-33.737369999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-33.7303,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-33.274230000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.862010000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-20.634450000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.402349999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T18:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.15455,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T19:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.76108,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T19:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.060300000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T19:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.359529999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T19:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-17.608239999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-06T19:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-18.30883,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-09T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-2830.4859900000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-09T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-1258.99649,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-09T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-1247.49928,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T16:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.683779999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.184650000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.958179999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.630880000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.643509999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-51.953859999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-52.839509999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-53.110889999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-66.767189999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-71.490690000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T17:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-69.284689999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-67.413809999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.803329999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.892420000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.489540000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.567390000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.270050000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.343419999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.955880000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-204.05010999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-203.70201,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T18:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-218.01281,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-222.06433000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-227.99817999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-197.37597,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-224.98860999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-223.47587999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-215.29839000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-209.48384999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.294319999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.789950000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.862880000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.705730000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.688319999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.15231,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.57807,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.97753,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.59745,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.63687,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.185929999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.143940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.12772,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.216650000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.595109999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.64462,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.7165,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.450759999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.96405,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.735389999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.396719999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-10T21:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.197859999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T15:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.27338,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T15:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-88.850769999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T15:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-23.32677,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T15:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-16.727519999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T15:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-285.80592999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T16:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-293.56448,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T16:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-311.79356999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T16:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-309.36937999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T16:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-207.74927,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.161720000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-198.53529,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-187.64245,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-195.20842999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.375169999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.777749999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-57.770150000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:55:00","V>>N-NIL_HG","N-NIL;N-NIL_H","2015-09-24",1,-11.90742,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Nil trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.076650000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-45.747129999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-209.51201,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-62.011690000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.880229999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.885919999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.123739999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-62.991059999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.181579999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.674959999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.681669999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-193.16467,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.181750000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.123570000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.123570000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T19:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-17.096969999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.027360000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.0489,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.572179999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.572179999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.392659999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-40.544870000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.0489,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.0489,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.602880000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.995189999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.87054,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.23893,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.881790000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.55932,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.267099999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.964479999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-11T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.524080000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T09:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.472660000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T09:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.424109999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T10:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-15.857799999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T12:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-133.13643999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T12:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-13.613709999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T13:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-199.0881,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T13:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-197.29229000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T13:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.161549999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T14:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.443539999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T14:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.443539999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T14:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.443539999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T14:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.64798,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T14:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.818919999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-141.74651,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-140.12736000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-167.3373,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-108.65419,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-184.01562999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-142.84216000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-144.03835000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.590920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-167.96530000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T15:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-153.20568,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-153.20572000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:15:00","V>>SML_NIL_CONT_7A","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-241.55859000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-268.29021,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-254.59811999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-261.84035999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.83023,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.181069999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-169.56399999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-169.56399999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.680979999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.118470000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.118470000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-72.172479999999993,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-69.258049999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-185.56012999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-191.46682999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-72.581400000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-68.518749999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-70.488780000000006,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.019199999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-197.50308999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-198.26553000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-198.67225999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-195.37618000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-74.863299999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-76.634410000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-74.545559999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-76.634410000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-76.634410000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-69.274600000000007,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-193.24592999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-63.877899999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-186.08337,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-278.96841999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-187.06433999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-163.98632000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-169.74950999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-167.65917999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.008290000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.008290000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-43.181229999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.431910000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-140.93708000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-475.76161000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-487.70792999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-473.96132999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-473.96132999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.880519999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-279.71028999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-494.46269999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-58.122779999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.80274,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-45.24335,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.634050000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.76108,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.799619999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-58.03387,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-56.82705,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.601640000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-51.15278,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-49.896279999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-51.22092,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.730139999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.240479999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.950839999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.695959999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.695959999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-63.610599999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T21:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.62218,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.788499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.243320000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.14892,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.177219999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.45083,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.446090000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.139240000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T22:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.476479999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T23:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.110440000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T23:45:00","V^SML_NIL_3","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-5_BL;V-NIL_PAR_","2013-08-21",1,-254.95533,"Out = Nil, avoid voltage collapse for loss of Bendigo to Kerang 220kV line, swamped if Murraylink VFRB enabled and Murraylink > 25MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-12T23:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.429760000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-217.90468999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-475.47744,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-272.81024000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-213.79024999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-479.35518000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-474.68583000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-473.73768000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-263.64933000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-257.06292000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-257.32071999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-213.49986999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T00:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-201.58086,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.97561,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.166399999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.063079999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.019480000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.048760000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T01:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.246720000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T07:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-60.371119999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T07:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-61.851239999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T07:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-61.85134,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T07:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-37.84055,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T08:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-42.839419999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T08:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-45.102249999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.499580000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.64105,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.552379999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-47.463369999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-44.1813,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T09:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-47.865479999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.18477,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-56.709499999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-54.677410000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-46.220089999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-52.820799999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-50.298209999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-31.933910000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-33.480020000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T10:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-31.588609999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T14:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-16.526150000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T14:30:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-1821.25162,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T14:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-1839.7891999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T14:45:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-196.86845,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T14:55:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-182.10525000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:00:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-151.29886999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:15:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-148628.83119,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:15:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-147792.67647000001,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:20:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-59664.461510000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:20:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-59298.055039999999,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:25:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-59664.151660000003,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:25:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-59298.056360000002,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:30:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-59898.851609999998,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:30:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-59298.05646,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:35:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-27932.948649999998,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:35:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-39067.732750000003,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:40:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-41124.714469999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:40:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-52217.353000000003,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:45:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-80552.041769999996,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:45:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-98709.302420000007,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:50:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-59159.071040000003,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:50:00","V>>DDSH_DDGN_N-2","V-DDGN_N-2","2015-09-11",1,-59308.155630000001,"Out= Nil, avoid O/L Dederang to Shepparton 220kV line on trip of both Dederang to Glenrowan No.1 and No.3 220kV lines, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T15:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-101.9726,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T16:00:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-133.58099999999999,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T16:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-68.379580000000004,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T16:50:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-114.18797000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T16:55:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-119.88072,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-13T17:00:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-119.88072,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.31175,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.38627,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.125870000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T04:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.86215,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.09892,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.09717,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T08:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-35.017119999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T09:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-39.351939999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T09:55:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-45.489109999999997,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T09:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-136.05041,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T09:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-26.91995,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-20.059640000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-13.05111,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.197369999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-25.976849999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.786529999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-23.020250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:40:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.092549999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-27.682849999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-20.463159999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-25.412269999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-18.456150000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-24.522300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:55:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-20.06606,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-28.454529999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-19.52638,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-26.674520000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.61543,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:10:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-122.92086,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-145.7748,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-44.116779999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-52.097340000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:20:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-21.63683,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-27.017749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:25:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-24.845400000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-29.841280000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.214030000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-27.23434,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:35:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-21.504909999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-26.558769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:40:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.056660000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-27.39987,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-22.388919999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-26.97832,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:50:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-25.900980000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-32.223700000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:55:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-33.840800000000002,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T11:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-41.912950000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T12:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-60.775379999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T12:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-69.336519999999993,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T12:05:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-26.26951,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T12:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-32.824939999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T12:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-16.992249999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T15:15:00","V>>N-NIL_HG","N-NIL;N-NIL_H","2015-09-24",1,-11.35975,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Nil trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T15:20:00","V>>N-NIL_HG","N-NIL;N-NIL_H","2015-09-24",1,-28.983350000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Nil trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T16:40:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-23.662790000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-14T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-29.279800000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T02:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.75362,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:10:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2016-01-14",1,-88.432029999999997,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-49.808779999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:20:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2016-01-14",1,-88.852180000000004,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-50.1267,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:35:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2016-01-14",1,-88.473179999999999,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-15T22:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-49.803719999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T06:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.229570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T13:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.61623,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T13:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.14955,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T13:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.75325,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T13:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.645709999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T14:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.645709999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-17T14:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.576409999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.58985,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.19716,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.652850000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.528980000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.6281,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.848030000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.623259999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T13:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.029969999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T14:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.582930000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T14:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.654319999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T14:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.658860000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T14:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-10.35961,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-39.132890000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-39.819960000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-24.59234,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-33.473590000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.741300000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-55.031509999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T15:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.177869999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:05:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-43.56,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:20:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-46.278440000000003,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.179110000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.529780000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-38.644860000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-55.557360000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.537089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.12715,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.036370000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-68.39676,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-55.417110000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.450140000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-63.92353,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-53.27469,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.067660000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.114789999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.971339999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.862170000000006,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.904399999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.648759999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-75.248369999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-70.803799999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-69.731729999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-73.360330000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-72.784199999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.913039999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.222579999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-66.442480000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-53.438450000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.31569,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.039359999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.53379,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.979489999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.21528,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.246790000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.174029999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.71546,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.865870000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.49278,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-18T19:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.66581,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T10:55:00","S>>BRTW_BWPA_WTTP","S-BRTW;S-X_BRTW+PA6116","2016-01-14",1,-34.571919999999999,"Out= Brinkworth- Templers West 275kV line, avoid O/L Waterloo-Templers 132kV on trip of Blyth West-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T11:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.835889999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.351780000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.144580000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.970929999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.799320000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.762689999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.774789999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-48.366,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.790330000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.928359999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.46879,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.40128,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T12:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.374090000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.227879999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.0205,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.100250000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.449109999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.18974,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.90771,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.0609,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-48.907139999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T13:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-49.525410000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T14:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.534700000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T14:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-50.350259999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.559089999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.07667,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.181069999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.680979999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.953760000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-55.86927,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-45.532249999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.52974,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.46988,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T15:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.4026,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.9556,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.618849999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-59.206119999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-58.881279999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.817999999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.241040000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T20:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.47944,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T20:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.009170000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T20:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.861879999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.685939999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.28171,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.043019999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.953600000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.447320000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.869350000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.989450000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.124220000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.538640000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.787299999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.191610000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.78125,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T21:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.223129999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.944600000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.087879999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.81959,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.563189999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.58877,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.5791,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.96829,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.86008,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.358640000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.989470000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.989470000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T22:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.294289999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-38.713320000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.630129999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.652729999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.264479999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.719970000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.021470000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-19T23:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.626019999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.522120000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T00:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.50517,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T00:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.231580000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T00:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.296240000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T06:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.545900000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T06:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.64378,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.43609,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.442879999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.147120000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.074770000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.852920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.002420000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T07:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.992180000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.002420000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.463760000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.145949999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.10754,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.06532,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.32554,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.17061,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.1235,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T08:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.79693,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T09:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.045069999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T09:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.526479999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-50.741840000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-53.329520000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-14.374409999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.69309,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-23.95166,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T16:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-67.575909999999993,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-62.685169999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-12.177440000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-46.585380000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-38.65889,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.459289999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-32.823990000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.543880000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.38372,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-37.113140000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-30.521350000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-26.829470000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T17:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-23.38083,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-31.60896,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-32.492019999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-38.269799999999996,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-18.145900000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-51.632919999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.078150000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.730879999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-30.59151,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-27.22212,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T18:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-19.06353,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-10.41738,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-11.75395,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-10.686260000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:25:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-25.403369999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-13.248329999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T19:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-10.133190000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.483079999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T20:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.318390000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.395989999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.69065,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.60928,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.60928,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.635649999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.124220000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T21:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.77073,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T22:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.998139999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.258850000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-20T23:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.1675,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T00:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.97486,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T01:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.77952,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.503170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.48945,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.48523,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.56532,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.46017,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.53162,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.02805,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.16005,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.152089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T02:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.008100000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.009539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.0228,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.28776,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.292450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.003920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T03:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.28247,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T14:25:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-","2015-08-25",1,-27.034680000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T14:40:00","V>>SML_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_BATS_MLTS1_15M;V-NIL_PAR_2-5;V-NIL_PAR_2-5_BL;V-NIL_PAR_3-5;V-NIL_PAR_3-","2015-08-25",1,-11.28107,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T15:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.261310000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T15:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-174.69596000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T15:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.888290000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T15:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.95457,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T15:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.75393,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.239850000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.618269999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.754860000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-155.03054,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-162.04243,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-161.20116999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-161.20894000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-154.46905000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-40.181399999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-135.26695000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-157.72703000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-157.72703000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-185.44546,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-157.72703000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-142.84281999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-148.34082000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-118.98052,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-157.72703000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-175.95905999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-144.20153999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-145.09663,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-148.89017999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-152.79393999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-159.71208999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-59.24165,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.181609999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.911389999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-57.624899999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-57.136319999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-56.399940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-59.08173,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T20:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-52.492910000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T20:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.524810000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T20:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.253070000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-38.724780000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-169.21476000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-176.27877000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-177.19835,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-186.27934999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-179.57379,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.094939999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.19163,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T21:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.12669,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.871459999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.124269999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.836069999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.826589999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.29298,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.762659999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T22:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.516440000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T23:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.473199999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T23:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.60937,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T23:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.653309999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T23:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.1456,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-21T23:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.23296,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T00:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.299669999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T00:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.88165,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.41581,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.28294,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.30649,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.407879999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.148070000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.115279999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T01:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.562180000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T02:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.87947,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T02:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.474399999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T03:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.2113,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.949580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.9084,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.44806,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.058240000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.303650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.77291,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T04:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.83731,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.67521,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.81072,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.82497,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.85585,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.803550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T07:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.81087,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T07:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-17.17718,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T07:15:00","V:SS_720_HY_TEST_DYN","NULL","2015-12-18",1,-16.72174,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 720 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T07:20:00","V:SS_720_HY_TEST_DYN","NULL","2015-12-18",1,-18.643280000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 720 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T07:25:00","V:SS_720_HY_TEST_DYN","NULL","2015-12-18",1,-17.56542,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 720 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.914180000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.110700000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.007269999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-55.642380000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-41.030700000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.009450000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.814660000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.739289999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T08:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.066980000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T09:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.503489999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T09:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.263549999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T09:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.815200000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T09:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-18.95166,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T11:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.219580000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T14:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-10.451919999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.5959,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.5959,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.5959,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.5959,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.192920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.009329999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-45.336419999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-63.193959999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-65.19556,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-64.644030000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.046260000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.494579999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.354680000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.354680000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.354680000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.5959,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.5959,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.254290000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.689810000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.238440000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.401599999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-28.815329999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.10435,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.521640000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-29.278089999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.16151,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.139569999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-22T18:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.551310000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-23T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.17272,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-25T05:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.65063,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-25T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.479559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-25T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.02848,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-25T05:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.31579,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-25T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.058960000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-26T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.37355,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-26T02:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.20452,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-26T03:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.643610000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-26T05:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.95157,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-27T05:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.78281,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-27T05:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.105510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-27T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.268800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-28T15:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-26.135809999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T05:40:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.437049999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T05:45:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.06672,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T05:50:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.04504,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T05:55:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.06976,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T06:00:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.07503,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T06:05:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-12.249230000000001,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:05:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-13.81954,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:10:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-16.606829999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:15:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-13.846959999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:20:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-13.83337,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:25:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-13.82023,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:30:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-19.91798,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:35:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-20.537410000000001,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:40:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-17.066669999999998,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:45:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-21.997389999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:50:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-20.574439999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T14:55:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-16.622810000000001,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T15:00:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-17.162369999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-30T15:05:00","V>>N_SMHTX_2","V-SMTS_HTX_P;V-SMTS_HTX_R","2015-12-21",1,-15.27106,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L Thomastown to South Morang No. 2 or No. 1 220 kV line (flow TTS to SMTS) on trip of South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.62613,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T03:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.44952,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.46414,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T03:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.293329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.292289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.460940000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T05:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.191380000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T07:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.277340000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T10:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.33625,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T10:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.384,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.549250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T11:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.6861,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T11:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.287649999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T12:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.131539999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T12:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.754720000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T12:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.05002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T12:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.62682,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T12:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-13.56582,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T13:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.41944,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-01-31T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.420070000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.29072,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.970499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.78717,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.521100000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.747,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.74451,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T03:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.735279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-01T04:40:00","#R013544_012_RAMP_F","#R013544_RAMP","2016-01-31",1,-13.69242,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-01T04:45:00","#R013544_012_RAMP_F","#R013544_RAMP","2016-01-31",1,-15.846209999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-01T04:50:00","#R013544_012_RAMP_F","#R013544_RAMP","2016-01-31",1,-13.143879999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-01T04:55:00","#R013544_012_RAMP_F","#R013544_RAMP","2016-01-31",1,-10.09482,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-02T01:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.229990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-02T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-38.287570000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-02T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-38.637970000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-40.081899999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T02:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-39.293660000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T22:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.28223,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.51041,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.47588,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-03T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.13631,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T00:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.82381,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T01:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.181749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T01:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.144590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T02:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-38.283070000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T02:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-38.483690000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.492039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T02:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.501099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T03:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.569929999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-33.370919999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T05:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.403029999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-04T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.399179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T00:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.145239999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T00:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.78528,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T00:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.096830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T00:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.212949999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.059419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.101699999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.645569999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.09348,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.637639999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.028549999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.54818,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-31.897939999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-33.848329999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.04899,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.54425,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.43085,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T01:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.897349999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.961,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.35538,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.06222,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.470649999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.00329,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.626620000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.556850000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.783910000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.224409999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-31.568560000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-33.384810000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.229710000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.51182,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.93516,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.35718,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.977309999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.39066,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.71552,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.11778,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-38.503540000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-39.94209,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.998150000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.455829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-37.685490000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-39.339739999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.88883,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.340420000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.154489999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.75005,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.037799999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-34.060809999999996,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.94232,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.342649999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.65878,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.055910000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-31.25132,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-33.373950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.57851,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.972339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.33318,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.836729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.216519999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.70373,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.119249999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.571290000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.196429999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T03:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.755789999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T04:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.19022,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.71062,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.52237,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-05T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.53519,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T06:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.204050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T06:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.20623,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T07:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.20673,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T07:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.188420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T07:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.1944,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.19204,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T15:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.08311,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-06T15:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.70149,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-07T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.069419999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-07T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.47179,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-08T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.041679999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-08T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.40146,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-08T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.28858,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T14:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.960809999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T14:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.15011,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.832550000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-40.983310000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.086089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.086089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.505240000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.918000000000006,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.588329999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.537369999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.513500000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.56213,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.154,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.845109999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.931199999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.931199999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-63.405230000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.03454,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.03454,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.03454,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.617699999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.996459999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.637120000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.008049999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.79204,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.271940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.40395,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.798640000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.70288,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.328150000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.97067,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.867470000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.37471,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-09T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.289720000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T09:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.220849999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T09:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.47845,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T10:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.768330000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T10:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.407810000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T15:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.495660000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T15:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-199.83240000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T15:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-199.85494,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.96231,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.61806,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.191939999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.508430000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.066459999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.13794,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.9588,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.9588,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.9588,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-10T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.9588,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T14:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.89579,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T14:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.10464,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T14:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.241429999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T14:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.60122,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.440619999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.255469999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-11T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.344619999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T12:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.24363,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T15:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.446249999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T15:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.060370000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T15:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.01873,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T15:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.58582,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T16:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.88313,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.312059999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.207989999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.03134,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.301570000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.23939,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.193019999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.89687,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.243919999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.576659999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.81371,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-45.573799999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.76397,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.203939999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.770230000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.82347,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.73415,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.619489999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.21665,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.019120000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.625920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.339090000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.41123,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.893750000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.486000000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.91892,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.91888,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-12T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.91888,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-13T07:00:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-11.02746,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-13T07:10:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-11.81044,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T05:00:00","#R013592_013_RAMP_F","#R013592_RAMP","2016-02-13",1,-10.643090000000001,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-14T12:25:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2015-09-08",1,-10.859500000000001,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T13:45:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-12.8,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T14:00:00","V::N_EPMB_V4","V-EPMB;V-X_EPMB_DDSM","2015-08-24",1,-12.8,"Out = Eildon to Mt Beauty 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T16:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.819190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T17:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.782160000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T17:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.966619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T17:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.96238,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T18:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-24.269960000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T19:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-29.517189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T19:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.18886,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T19:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.0778,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T19:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.7697,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.76169,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.810029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.332929999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.799910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.06955,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T21:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.070399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T22:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.65034,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-31.925170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-14T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.191320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T00:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.550269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.628710000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.768050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.39899,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.50164,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.24225,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.04016,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.229810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.19773,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.17928,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.141629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.14181,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.14414,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T01:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.11979,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.27632,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.312390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.104799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.14024,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.83033,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.15639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.2948,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T04:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.42103,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T05:00:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-26.57084,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:05:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-27.324560000000002,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:10:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-41.458759999999998,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:15:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-41.501690000000004,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:20:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-41.230899999999998,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:25:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-39.254069999999999,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T05:40:00","#R013596_013_RAMP_F","#R013596_RAMP","2016-02-14",1,-10.420030000000001,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-15T08:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.95914,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.3751,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.37285,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.41122,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T13:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-16.835239999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T14:20:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-24.462820000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-27.97728,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-12.00873,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.507849999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.91916,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T21:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.27791,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.22644,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.79988,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.27577,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.25573,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.11703,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.078760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.02941,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.76468,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.074820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.55467,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-15T23:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.4422,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-16T05:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.486179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-17T03:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.53579,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-17T23:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.26107,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-18T05:00:00","#R013612_013_RAMP_F","#R013612_RAMP","2016-02-18",1,-24.553879999999999,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-18T06:25:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-10.10059,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-18T07:00:00","N^^V_EPMB_1","V-EPMB;V-X_EPMB_DDSM","2015-08-07",1,-42.749429999999997,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-19T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.27966,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-19T04:30:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-11.35084,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T04:35:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-11.641529999999999,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T04:40:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-15.51829,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T04:45:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-16.66639,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T04:50:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-17.017189999999999,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T04:55:00","#R013613_022_RAMP_F","#R013613_RAMP","2016-02-18",1,-17.019819999999999,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T05:00:00","#R013614_013_RAMP_F","#R013614_RAMP","2016-02-18",1,-17.66987,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T05:05:00","#R013614_013_RAMP_F","#R013614_RAMP","2016-02-18",1,-12.94731,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T05:15:00","#R013614_013_RAMP_F","#R013614_RAMP","2016-02-18",1,-17.929870000000001,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-19T14:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-170.50645,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-20T22:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.0543,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-20T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.305070000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-20T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.443619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-20T22:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.447749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-20T22:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.44036,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T00:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-730.79295000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T00:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-611.95596999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.68317,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-33.977249999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-35.253570000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T06:50:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2015-09-08",1,-10.051450000000001,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T07:15:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2015-09-08",1,-10.76224,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T15:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.74014,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.492940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.840630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.592510000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.28219,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.266079999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.597569999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.57926,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.40803,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.02012,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.36276,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T16:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.97789,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.031929999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.76179,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.82498,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.815720000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.80334,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.811870000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.448919999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.435460000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.4313,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.450710000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.815630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.857900000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.76341,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.867839999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.869479999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-21T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.601190000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T15:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-87.159109999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.479259999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-61.479259999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-58.079149999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-59.164140000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-48.740270000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-213.28684000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-179.54856000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-156.61526000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-41.661909999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T16:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.37598,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-66.070409999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-79.949349999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-81.017799999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-248.52879999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-72.328559999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-62.53051,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-68.501159999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.656009999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-79.949349999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.656009999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-77.61694,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-81.979709999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-81.017799999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-79.949349999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-78.88091,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-78.88091,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-78.88091,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-78.766300000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.804789999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.086089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.086089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.086089999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-69.558930000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-76.267489999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.517039999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-70.759900000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-68.863349999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.7087,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.46752,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.900569999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.14752,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.137880000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.137880000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.581849999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.84066,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.81007,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.99456,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.318290000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.44791,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.55125,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.55125,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.55125,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.06653,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.632059999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.757940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.171509999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.126799999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.96462,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.786829999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.716190000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.067969999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.564780000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.61051,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.564819999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.10219,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T21:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.02951,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-22T22:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.259880000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.33821,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-23.751999999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.494230000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.086310000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.31767,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.034410000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.789470000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T11:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-49.593649999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-63.102589999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.702539999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-66.893249999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-66.496200000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.18112,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.68121,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.971150000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.451219999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-184.77876000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T12:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-190.43208000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.916499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:20:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-18.246099999999998,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:25:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-47.403100000000002,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:30:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-45.582569999999997,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:35:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-77.438230000000004,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:40:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-85.973910000000004,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:45:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-33.736420000000003,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:50:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-20.99005,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T13:55:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-50.13776,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:00:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-18.291779999999999,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:05:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-50.662860000000002,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:10:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-51.764760000000003,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:15:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-51.116349999999997,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:20:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-19.117429999999999,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T14:25:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-17.593129999999999,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-23T16:05:00","N>>V_DBUSS_1","V-DBUSS_L","2015-09-02",1,-29.260929999999998,"Out = Dederang DBUSS-line control scheme, avoid overload of a Murray to Dederang 330 kV line (flow to South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-24T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.20665,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-24T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-11.25925,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-24T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.696200000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-24T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.26159,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-24T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.581900000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T00:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.065799999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T00:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.12839,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T00:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-12.98695,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T03:55:00","#R013635_002_RAMP_F","#R013635_RAMP","2016-02-25",1,-33.444360000000003,"Hard Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-02-25T06:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.44253,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.89654,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.21602,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.85501,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.08558,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.18571,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T06:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.75694,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.035440000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-17.32527,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-18.795259999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.789349999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.869260000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.538430000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.557849999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.213249999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.555399999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.557970000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T07:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.91525,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.69842,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.220949999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.21256,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T08:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.15559,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.771380000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.84892,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.467130000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.50046,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.87585,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.502089999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.48582,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.141400000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T09:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.100819999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.129570000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-34.874270000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.743870000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.493770000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-20.49155,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T10:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-19.792999999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T13:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.438750000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.034749999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:10:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-16.296389999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-28.005030000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:15:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-25.77336,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-24.157599999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-20.561959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-20.691099999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:25:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.7135,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.987780000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:30:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-33.043579999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.53608,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:40:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-34.403440000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.327249999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:45:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-32.543900000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T14:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.3209,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T14:50:00","V>>V_NIL_5","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-41.570030000000003,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T15:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.96543,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T15:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.157209999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T15:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.112220000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T16:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.89066,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T16:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.96232,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T16:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.58001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T16:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.729799999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T16:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.37682,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T17:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.47866,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T17:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.01938,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T17:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.155740000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T17:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.90169,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T17:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.84192,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T18:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-18.67004,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T18:50:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.730370000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T18:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.33975,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T18:55:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.160030000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T19:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-22.49277,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T19:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-22.945530000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T19:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.54687,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T19:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.258139999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-25T19:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.090389999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T19:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.384410000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T19:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.093299999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-25T19:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.85998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-02-28T22:35:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-17.594280000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T15:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.29759,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T15:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.32574,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.755190000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.324459999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-29.619039999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.65465,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-58.456020000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.096499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.096499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.096499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.77713,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.096499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.096499999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.056620000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T18:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-39.745899999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-37.347029999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.6252,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.76069,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T20:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.20147,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-02-29T20:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.64475,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T05:25:00","#R013647_013_RAMP_F","#R013647_RAMP","2016-03-01",1,-10.826549999999999,"Hard Ramping constraint for constraint V::N_EPMB_V4, Effective Date: 24/08/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-01T05:30:00","#R013649_024_RAMP_F","#R013649_RAMP","2016-03-01",1,-12.201510000000001,"Hard Ramping constraint for constraint V::N_JNWGVE_R, Effective Date: 01/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-01T05:35:00","#R013649_024_RAMP_F","#R013649_RAMP","2016-03-01",1,-19.3904,"Hard Ramping constraint for constraint V::N_JNWGVE_R, Effective Date: 01/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-01T05:40:00","#R013649_024_RAMP_F","#R013649_RAMP","2016-03-01",1,-19.926960000000001,"Hard Ramping constraint for constraint V::N_JNWGVE_R, Effective Date: 01/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-01T05:45:00","#R013649_024_RAMP_F","#R013649_RAMP","2016-03-01",1,-19.34675,"Hard Ramping constraint for constraint V::N_JNWGVE_R, Effective Date: 01/07/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-01T14:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-67.324789999999993,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T14:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-81.051400000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T14:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-36.747369999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T14:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.470410000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T14:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-55.180639999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T14:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-78.084789999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-48.603409999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-16.43608,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-54.064279999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:15:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-36.582610000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:20:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-73.642769999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-56.54325,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:30:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-35.563699999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:40:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.088469999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:45:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.69914,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T15:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.959109999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T17:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.60097,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T17:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.601189999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T17:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.601189999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.5098,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-31.402899999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-31.444089999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-31.17717,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.499650000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.620449999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:40:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.620449999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:45:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.620449999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:50:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.483249999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T18:55:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-40.32517,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:00:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-37.601529999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:05:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.073309999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:10:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.160810000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:15:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.932279999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:20:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-22.73845,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:25:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-36.582610000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-21.815259999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:35:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.670210000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-21.876359999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:45:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-35.644199999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:50:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.426250000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T19:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-44.393009999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-30.173449999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-19.545590000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.257829999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.4541,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.730429999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:30:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.71041,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T20:45:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-15.659549999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T21:00:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.29393,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T21:05:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-21.39996,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T21:10:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-19.693619999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T21:15:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.869770000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T21:35:00","V>SML_BUDP_5","I-JNWO_RADIAL;N-BUDP;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-12.23152,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T23:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-28.241330000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T23:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.45787,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T23:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.861460000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T23:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.019839999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-01T23:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.45617,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T11:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-49.990209999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T11:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-47.188920000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T11:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.637450000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T11:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-45.625480000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T11:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-50.280200000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-48.72869,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-47.177120000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.421390000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.421390000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-50.280259999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-36.012520000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.589749999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.92267,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.413720000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-19.467189999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T12:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-59.589660000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-61.449939999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-59.589709999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-62.69285,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-63.128489999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-61.14123,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.435919999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-13.952450000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-25.443619999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-40.142110000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.996600000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T13:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.266400000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-28.783629999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-17.7636,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.774319999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-23.278559999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.519349999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.658169999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.157019999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.579969999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-17.25535,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T14:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.26465,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.40015,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-13.51919,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-16.351330000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.95116,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.24677,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-205.52796000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-205.52796000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-76.447919999999996,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.275320000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-30.722840000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-30.722840000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T15:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.902569999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.77106,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-13.450229999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-12.579330000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-15.55761,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.38442,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.957840000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-14.73489,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.29562,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-28.796980000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.29562,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T16:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-41.314140000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-27.57958,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-13.87519,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.947980000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-28.202490000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-26.964269999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-27.95824,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-47.127189999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-40.854880000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-12.62513,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.59328,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.681380000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T17:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.135439999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-02T18:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.25024,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T13:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-46.823410000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-49.383580000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.455089999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.679960000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-45.325240000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.99727,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-48.286209999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-47.153579999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T14:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.35162,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T15:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.55716,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T15:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.288270000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T15:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.171379999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-48.149509999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.067689999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-79.949430000000007,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.901269999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-71.3874,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-67.813820000000007,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-65.395110000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.11863,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-24.386310000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-22.158660000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.031369999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-30.06954,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-26.060559999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.781230000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-54.661439999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.817449999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-25.33662,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.11233,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-27.211310000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-28.431249999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-38.455959999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.474739999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-35.827930000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.883659999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.637630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.931249999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-31.07461,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.5136,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.262099999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-10.77065,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-19.358360000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.637630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.439579999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.914999999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.958839999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T19:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.958839999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.958839999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.27843,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.56845,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.50187,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.36003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.838100000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-25.888179999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-03T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-23.784600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T00:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.22223,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T00:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.521409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T00:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.945499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.98737,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.13707,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.43533,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.41344,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T01:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-11.350709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T01:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.35216,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.143610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.145339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.727690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.789940000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.870340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.907500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.88735,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.880739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.64973,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.67559,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T03:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.75183,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T03:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-17.98939,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T03:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-16.721340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T03:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.452260000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T04:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.41536,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T04:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-20.001919999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T04:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-21.016780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T04:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.993069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T04:25:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.796110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T07:55:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-27.352789999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:00:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-27.352789999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:05:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-27.352789999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-22.66038,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:15:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-13.110010000000001,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:20:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-20.989909999999998,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:25:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-21.009879999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-03-04T08:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-16.403880000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T11:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-14.47072,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.52571,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.4948,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.88949,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.90602,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-17.76014,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.760809999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.14226,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T12:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.05899,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.983459999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.118969999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.139090000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-95.000339999999994,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-86.366339999999994,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-177.99799999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-55.763669999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-17.89593,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.41133,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-59.354759999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T13:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.515080000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.30707,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-38.523350000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-50.376950000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-42.462380000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-40.492910000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-89.039079999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-89.080269999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-90.951589999999996,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-91.158299999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-91.972840000000005,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-91.687799999999996,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T14:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-80.723780000000005,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-77.641440000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.664160000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-65.749920000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-65.688599999999994,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-75.571550000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-66.72448,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-65.14282,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-67.517480000000006,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-64.636790000000005,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-65.15701,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-243.35301999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T15:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-258.45636000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-259.89251000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-270.78681999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-263.53143,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-277.29946000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-274.99367000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-1227.29,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-1224.46261,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-10.09844,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T16:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-1233.27531,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T17:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-279.49419,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T17:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-277.18525,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T17:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-277.21744000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T17:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-96.232200000000006,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T17:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-94.899770000000004,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-95.450019999999995,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-92.338229999999996,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-49.120469999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-49.121720000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-48.637560000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-93.992999999999995,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-93.663749999999993,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-91.097040000000007,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-93.080669999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-93.171779999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-92.834900000000005,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T18:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-92.060789999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-48.045810000000003,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-48.076189999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-18.855149999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.243760000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.519290000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.519290000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.519290000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.519290000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-33.499789999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-34.149470000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-34.566189999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T19:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.313389999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-36.234229999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.73724,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-20.890339999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-32.843519999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:20:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-34.899909999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:25:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-35.449300000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:30:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-40.476529999999997,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-14.758470000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-17.758209999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:50:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-11.041270000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T20:55:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-15.503869999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T21:00:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-19.816210000000002,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T21:05:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-15.659420000000001,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T21:10:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-15.10807,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T21:15:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-21.548549999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T23:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-29.14141,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T23:40:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-29.858899999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-04T23:45:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-29.318079999999998,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-14.46109,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-36.444499999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-42.264220000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-44.974939999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.3916,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-13.686,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T14:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-15.401669999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T15:50:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-21.111630000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T15:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.66507,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.662400000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:05:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-39.119529999999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.602150000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:15:00","V>>SML_NIL_8","V+NIL_PAR_3-5;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL_BATS_BETS_15M;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-25",1,-19.583210000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.468409999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.065650000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-60.946689999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.702089999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-62.66086,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.882739999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.515720000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T16:55:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-22.2712,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-37.08155,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.637589999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.931199999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.931199999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-38.692639999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.243110000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-21.844919999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-34.787489999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.271979999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.34909,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-20.400829999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T17:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.137880000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-33.654519999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-32.692100000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.494630000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-16.664840000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.153960000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T18:30:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.33718,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T19:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.71434,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-05T20:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.588069999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-06T17:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-24.331579999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-06T18:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-335.29061000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-07T08:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-80.874129999999994,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-03-07T10:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.158709999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-03-07T16:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-21.072769999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-07T17:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-65.591099999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-07T18:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-41.121180000000003,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-07T20:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-34.767429999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-08T17:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.84526,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-08T18:30:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-121.17753,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-08T20:05:00","V>>V_NIL_8","V-NIL","2015-09-21",1,-200.51141999999999,"Out = Nil, avoid O/L DDTS to WOTS 330kV line for trip of LowerTumut-Wagga (051) + 970,990,99M ex_Yass lines; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-10T16:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.19603,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T02:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-18.600629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T04:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-13.65319,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T05:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.203290000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T21:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.342280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T22:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-15.43577,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-12T23:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-10.975580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-13T08:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-14.110989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-13T22:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-12.867039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T06:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.70815,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T11:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.34155,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T13:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-13.68125,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-15.260009999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-18.705649999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T17:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-28.47221,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-14T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.525499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T01:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.22565,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.48624,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-10.65888,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.494440000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T11:15:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-31.033560000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T12:45:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-47.94932,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T14:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-47.853960000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T14:50:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-22.71716,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T16:35:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-47.912500000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T18:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-57.281010000000002,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-15T19:25:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-36.123629999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-16T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-08-24",1,-19.032509999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-17T02:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.219659999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-17T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-11.22142,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-17T04:55:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-15.067119999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-17T05:10:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-21.747920000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-18T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2015-08-25",1,-14.116669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-18T03:45:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-10.797330000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-18T10:15:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-12.12994,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-18T23:35:00","V>SML_BUDP_2","I-JNWO_RADIAL;N-BUDP;N-BUDP_P;N-BUDP_R;N-DPWG_63_X5;N-JNWG_RADIAL;N-LTWG_RADIAL;N-WAGGA_330_BUSB;N-X_07+62_RADIAL;N-X_CNYS_JNWG_RADIAL;V-DDWO_RADIAL","2015-08-31",1,-24.195319999999999,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Horsham to Waubra 220 kV line section on trip of Bendigo to Kerang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-28T22:05:00","V::N_NIL_V","V-NIL","2016-03-23",1,-17.245830000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-30T05:45:00","#R013776_022_RAMP_F","#R013776_RAMP","2016-03-30",1,-41.619979999999998,"Hard Ramping constraint for constraint V::N_BUDP_V4, Effective Date: 24/03/2016, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-03-31T00:25:00","V::N_NIL_V4_-200","V-DSA_STAB-200","2016-03-24",1,-18.526879999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 200 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-31T00:50:00","V::N_NIL_V4_-200","V-DSA_STAB-200","2016-03-24",1,-12.86614,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 200 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-31T04:15:00","V::N_NIL_V4_-200","V-DSA_STAB-200","2016-03-24",1,-16.866320000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 200 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-31T17:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.609450000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-31T20:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.825060000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-03-31T20:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-16.842479999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T01:50:00","V::N_NIL_V","V-NIL","2016-03-23",1,-13.253819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T03:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.19562,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T06:25:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-10.338509999999999,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T08:25:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-10.62665,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T10:40:00","S>>V_NIL_WTTP_WEMW4","S-NIL;S-NIL_2","2016-01-12",1,-22.218730000000001,"Out= Nil, avoid O/L Waterloo East - Morgan Whyalla 4 132kV on trip of Waterloo - Templers 132 kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T11:35:00","S>>CNDV_MKRB_WEMWP4","S-DVCN","2016-03-24",1,-32.448619999999998,"Out= Canowie-Davenport 275kV line, avoid O/L Waterloo East-Morgan Whyalla 4- Robertstown 132kV line on trip of Mokota-Robertstown 275kV line (this trips Hallet 2 windfarm), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T12:25:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-11.16703,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.20241,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T14:25:00","S>>CNDV_MKRB_WEMWP4","S-DVCN","2016-03-24",1,-10.528359999999999,"Out= Canowie-Davenport 275kV line, avoid O/L Waterloo East-Morgan Whyalla 4- Robertstown 132kV line on trip of Mokota-Robertstown 275kV line (this trips Hallet 2 windfarm), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T15:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-40.773180000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T16:20:00","S>>CNDV_MKRB_WEMWP4","S-DVCN","2016-03-24",1,-10.618690000000001,"Out= Canowie-Davenport 275kV line, avoid O/L Waterloo East-Morgan Whyalla 4- Robertstown 132kV line on trip of Mokota-Robertstown 275kV line (this trips Hallet 2 windfarm), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T18:05:00","V::N_NIL_V","V-NIL","2016-04-01",1,-20.260459999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T18:45:00","V::N_NIL_V","V-NIL","2016-04-01",1,-18.1922,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T21:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-22.48509,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T22:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-39.906309999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-01T23:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-30.354790000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T01:30:00","V::N_NIL_V","V-NIL","2016-04-01",1,-15.18613,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T03:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-14.378590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T04:55:00","V::N_NIL_V","V-NIL","2016-04-01",1,-14.77121,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T05:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-17.146719999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T07:25:00","V::N_NIL_V","V-NIL","2016-04-01",1,-23.8735,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T10:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-23.31683,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T12:10:00","V::N_NIL_V","V-NIL","2016-04-01",1,-24.653639999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T13:00:00","V::N_NIL_V","V-NIL","2016-04-01",1,-24.40821,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T15:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-43.187660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T16:35:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-15.35181,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T17:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-52.29092,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T17:35:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-18.602209999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T18:20:00","V::N_NIL_V","V-NIL","2016-04-01",1,-80.090109999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T19:25:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-18.16554,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T20:30:00","V::N_NIL_V","V-NIL","2016-04-01",1,-29.729579999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T21:45:00","V::N_NIL_V","V-NIL","2016-04-01",1,-21.865269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-02T22:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-29.022829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T01:20:00","V::N_NIL_V","V-NIL","2016-04-01",1,-10.393140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T02:55:00","V::N_NIL_V","V-NIL","2016-04-01",1,-19.155329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T03:25:00","V::N_NIL_V","V-NIL","2016-04-01",1,-19.065930000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T05:00:00","V::N_NIL_V","V-NIL","2016-04-01",1,-14.54644,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T07:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-17.658200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T08:45:00","V::N_NIL_V","V-NIL","2016-04-01",1,-13.060140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T10:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-21.235479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T11:50:00","V::N_NIL_V","V-NIL","2016-04-01",1,-12.2294,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T14:55:00","V::N_NIL_V","V-NIL","2016-04-01",1,-25.021799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T16:30:00","V::N_NIL_V","V-NIL","2016-04-01",1,-20.061430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T16:55:00","V::N_NIL_V","V-NIL","2016-04-01",1,-31.79589,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T18:15:00","V::N_NIL_V","V-NIL","2016-04-01",1,-277.25761,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T19:50:00","V::N_NIL_V","V-NIL","2016-04-01",1,-35.614370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T20:35:00","S>>CNRB_MKRB_WEMWP4","S-CNRB;S-CNRB_BC-2CP","2016-03-23",1,-11.05475,"Out= Canowie-Robertstown 275kV line, avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Mokota-Robertstown 275kV line (this trips Hallet Hill WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T22:05:00","V::N_NIL_V","V-NIL","2016-04-01",1,-15.8,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-03T23:55:00","V::N_NIL_V","V-NIL","2016-04-01",1,-11.58933,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-04T02:00:00","V::N_NIL_V","V-NIL","2016-04-01",1,-17.580909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-04T03:40:00","V::N_NIL_V","V-NIL","2016-04-01",1,-16.714089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-04T04:00:00","V::N_NIL_V","V-NIL","2016-04-01",1,-17.320830000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-04T05:35:00","V::N_NIL_V","V-NIL","2016-04-01",1,-14.927429999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T00:25:00","V::N_NIL_V","V-NIL","2016-04-01",1,-14.286440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T01:20:00","V::N_NIL_V","V-NIL","2016-04-01",1,-19.41395,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-35.783650000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T03:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-18.21658,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-18.473420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T04:50:00","S>>X_DVCN+CNRB+CB_10","S-X_DVCN+CNRB+RBCB","2016-03-24",1,-36.839390000000002,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Robertstown 275/132kV TX1 on trip of Robertstown-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T05:15:00","S>>X_DVCN+CNRB+CB_10","S-X_DVCN+CNRB+RBCB","2016-03-24",1,-30.861270000000001,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Robertstown 275/132kV TX1 on trip of Robertstown-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T06:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-49.168289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T07:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.361969999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T07:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-26.34562,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T08:25:00","S>>X_DVCN+CNRB+CB_16","S-X_DVCN+CNRB+RBCB","2016-03-30",1,-23.64358,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Waterloo East-MWP4-RB 132kV line on trip of Mokota-Robertstown 275kV line(this offloads Belalie-Mokota 275kV line, RBTX1 and trips Hallet Hill WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T09:20:00","S>>X_DVCN+CNRB+CB_16","S-X_DVCN+CNRB+RBCB","2016-03-30",1,-16.406600000000001,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Waterloo East-MWP4-RB 132kV line on trip of Mokota-Robertstown 275kV line(this offloads Belalie-Mokota 275kV line, RBTX1 and trips Hallet Hill WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T10:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-53.160350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-21.756139999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T11:25:00","S>>X_DVCN+CNRB+CB_10","S-X_DVCN+CNRB+RBCB","2016-03-24",1,-23.283259999999999,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Robertstown 275/132kV TX1 on trip of Robertstown-Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T13:00:00","S>>X_DVCN+CNRB+CB_16","S-X_DVCN+CNRB+RBCB","2016-03-30",1,-15.414440000000001,"Out= Davenport-Canowie-Robertstown 275kV and Robertstown 275kV CBs 6616 and 6571, avoid O/L Waterloo East-MWP4-RB 132kV line on trip of Mokota-Robertstown 275kV line(this offloads Belalie-Mokota 275kV line, RBTX1 and trips Hallet Hill WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T13:50:00","V::N_NIL_V","V-NIL","2016-04-01",1,-42.727919999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T15:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-421.41021999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-05T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-12.90659,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-06T13:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2015-09-24",1,-10.82981,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-06T16:30:00","V>>N-NIL_HG","N-NIL;N-NIL_H","2015-09-24",1,-30.105650000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Nil trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-07T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-15.221349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-07T01:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-26.39575,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-07T04:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-10.86528,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-07T22:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-36.569969999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-08T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-05",1,-21.267399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-08T03:55:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-05",1,-23.544799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-08T12:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.286000000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-08T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-129.47810000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-27.14873,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-18.549250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T03:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-19.372579999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-19.345790000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T06:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-46.175669999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T08:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-22.82489,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T14:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-16.667619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T17:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.436019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-09T22:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-56.971249999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T00:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-22.11243,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T03:55:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-31.246919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T04:25:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-11.18342,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.62988,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-28.069680000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-10T22:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-21.798680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-11T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-08",1,-15.31813,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-11T03:20:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-17.388570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-11T04:05:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-11.22667,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-14T02:20:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-30.080249999999999,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-14T02:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.416180000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-16T05:15:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-11.611470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-16T22:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.98258,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-17T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.44774,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-17T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-13.23569,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-18T05:20:00","V::N_NIL_V4_-100","V-DSA_STAB-100","2016-04-08",2,-18.545670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 100 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-18T19:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-154.92454000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-19T03:15:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-19.796279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-19T05:00:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-19.495249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-19T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-50.466200000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-20T00:50:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-20.94922,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-20T06:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.470739999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-21T00:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-17.342289999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-22T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-24.413039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-22T05:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.066380000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T10:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.257149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T11:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.291069999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-13.928129999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-12.1591,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T17:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.11828,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-23T22:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-20.953800000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-24T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.82559,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-24T11:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.63706,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-24T17:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-14.18235,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-24T22:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-12.31691,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T03:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.753589999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-35.257959999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T04:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-34.539580000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T06:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.27877,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T06:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-13.020300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T08:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.65225,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.507650000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T11:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-16.586839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T12:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-12.241910000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T13:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.28604,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T16:35:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-32.147039999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T22:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-59.879710000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-25T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-125.22152,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T00:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-17.231300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-16.925419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.97369,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T04:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-16.713290000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T05:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-26.17944,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T06:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-26.937609999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T08:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.463800000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T10:20:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-33.255319999999998,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T18:25:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-12.637549999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T20:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-26.70468,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T21:45:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-55.3628,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T22:05:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-266.26844,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T22:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-73.442229999999995,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-26T23:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-48.926319999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T00:35:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-26.404150000000001,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T00:55:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-86.860259999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T01:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-102.57753,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T02:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-79.169089999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T03:30:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-89.225359999999995,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T03:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-109.54333,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T05:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-42.537999999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T06:10:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-281.86246999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T06:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-292.52483999999998,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T07:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-61.66319,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T08:35:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-68.682460000000006,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T09:20:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-73.601050000000001,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T10:15:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-68.682460000000006,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T11:45:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-33.020000000000003,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T12:05:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-71.150319999999994,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T13:20:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-64.759979999999999,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T14:00:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-64.452789999999993,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T14:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-24.55367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T15:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-75.546329999999998,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T16:35:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-27.405750000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T17:45:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-194.81613999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T20:05:00","S>NIL_NIL_NWMH2","S-NIL","2014-09-22",1,-39.295470000000002,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T20:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-43.376809999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T22:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-45.275300000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-27T23:30:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-34.735149999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-24.497910000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T02:05:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-51.094119999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T03:45:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-52.544989999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T05:10:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-283.17977999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T10:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-22.13449,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T13:50:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-10.09864,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-123.02267999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T22:35:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-60.305570000000003,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-28T22:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-283.47334999999998,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T00:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-30.923249999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T02:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.34131,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T02:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-29.056450000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T03:55:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-37.229329999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T04:20:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-63.202660000000002,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T05:30:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-126.14551,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T07:05:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-26.1692,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-29T22:55:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-14.292299999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T03:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-24.31739,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T04:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.82821,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T04:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.071300000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T06:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-13.148479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T07:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-17.0946,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T09:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-37.160640000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T12:10:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-15.17699,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T13:00:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-10.410880000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T14:05:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-52.590440000000001,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T15:25:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-51.929740000000002,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T16:35:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-53.85942,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T17:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-84.461529999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T18:30:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-75.700599999999994,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T21:00:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-53.269530000000003,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T21:55:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-49.174439999999997,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T22:00:00","S>>BRMN_BWPA_HUWT","S-BRMN","2016-04-14",1,-49.163339999999998,"Out= Brinkworth - Mintaro (or any line section between Brinkworth and Mintaro) 132kV line, avoid O/L Hummocks - Waterloo 132kV on trip of Blyth West-Munno Para 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-04-30T23:10:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-17.14499,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T01:55:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-18.89021,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T02:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-33.144849999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T03:30:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-30.194469999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T04:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-40.250819999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T05:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.682169999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T06:10:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-30.025739999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T06:25:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-18.805759999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T07:40:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-12.86083,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T08:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-15.27932,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T10:15:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-24.851839999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T10:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-27.481619999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-01T12:20:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-13.31517,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-02T12:10:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-11.173069999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-02T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.53383,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-02T14:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.971830000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-02T15:25:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-14.333740000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-02T16:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-34.622259999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T00:25:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-52.996189999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T01:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-29.987929999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T02:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-29.5442,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T03:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-30.161899999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T03:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-69.501450000000006,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T04:10:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-103.15819,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T04:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-70.60472,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T05:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-23.919149999999998,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T07:15:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-135.47333,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T07:40:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-133.11027999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T08:50:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-10.83168,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T13:05:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-11.070209999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-22.34168,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T15:15:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-16.37893,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T15:55:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-24.363620000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-03T22:35:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-16.169440000000002,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-04T02:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-19.557459999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-04T03:20:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-29.986280000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-04T05:05:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-19.588750000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T00:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-15.88208,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T01:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-35.221089999999997,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T02:40:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-23.462009999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T03:50:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-19.86861,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T05:45:00","V>>N_DDMS_2","V-DDMS","2015-10-23",1,-22.297170000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Dederang to Murray 330 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T10:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.857150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T10:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.22897,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T12:45:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-20.952030000000001,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T13:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-13.09375,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.913169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T16:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.84609,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T22:40:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-10.026529999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-05T23:20:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-10.286770000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-06T23:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-39.04457,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T00:40:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.838200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-17.33398,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T05:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-28.48075,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T07:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-13.85332,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T09:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-27.917619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T18:20:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-23.667670000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T19:35:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-11.293150000000001,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T22:25:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-35.6188,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-07T22:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.43268,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-08T01:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.793810000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-08T08:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-21.939050000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-08T09:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-20.029530000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-08T09:40:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-03-23",1,-54.497109999999999,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-10T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-34.897239999999996,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-10T04:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-12.885120000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-14T02:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-37.857579999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-14T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.394259999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-14T05:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.26031,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-14T21:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-12.94932,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-14T22:45:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.208729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-15T03:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.28708,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-15T04:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.11713,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-15T05:05:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.128880000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-16T03:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-15.23255,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-16T04:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-12.259969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-17T09:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-72.720359999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-17T11:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-32.08437,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-17T15:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-47.026119999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-17T16:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-25.997720000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-17T21:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-163.76312999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-18T07:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-247.99679,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-18T11:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-150.45235,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-18T15:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-34.447290000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T00:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2015-08-13",1,-125.32052,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T01:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-17.167310000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T03:10:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.88161,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T04:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.37603,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T05:50:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-16.074649999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-19T06:45:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-19.310230000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T00:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-36.004420000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T01:05:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-33.230550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T02:45:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-39.486870000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.19806,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T05:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-13.1076,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T07:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-23.351099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T08:30:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-23.69359,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T12:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-27.506499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T13:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-27.92661,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-128.47309000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T14:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-17.154820000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-40.56541,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T16:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-32.539020000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T17:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-115.30269,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T18:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-43.225389999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T20:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-23.563680000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T22:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-25.293220000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-21T23:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.75806,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T00:20:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-14.464840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.52985,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-12.93698,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T05:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.52374,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T07:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.50469,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T08:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-23.152339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T08:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-19.302420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T09:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-11.77684,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T09:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.772460000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.101610000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-24.510459999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T16:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-14.86735,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T17:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-155.20750000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T19:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-20.887689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T21:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-17.194510000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T22:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-167.09916999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-22T23:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-37.324919999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T05:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-34.97222,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T06:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-34.156260000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T11:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-22.792590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T13:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-40.526440000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-21.532769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-23T19:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.88603,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-24","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-16.843889999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-24T01:00:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-16.373349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-24T03:10:00","V::N_NIL_V4_-100","V-DSA_STAB-100","2016-04-08",2,-23.29448,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 100 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-24T03:50:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-11.46921,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-24T05:45:00","V::N_NIL_V4_-050","V-DSA_STAB-050","2016-04-08",2,-19.027090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 50 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T00:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.031829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T02:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.69627,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T03:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-10.601660000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-20.427779999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T04:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.002050000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-25T05:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.224679999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-28T03:15:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-20.395099999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-29T02:25:00","V::N_NIL_V4_-100","V-DSA_STAB-100","2016-04-08",2,-10.044409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV. Offset 100 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-05-29T06:25:00","#R014061_012_RAMP_F","#R014061_RAMP","2016-05-28",1,-10.49396,"Hard Ramping constraint for constraint V::N_MLSY_V4, Effective Date: 08/04/2016, Version: 2","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-05-29T08:55:00","V::N_MLSY_Q4","V-MLSY_NOEMTT_KTS_P;V-MLSY_NOEMTT_KTS_R;V-MLSY_P;V-MLSY_R","2016-04-08",2,-44.162379999999999,"Out = Moorabool to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-02T14:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-182.19820000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-04T02:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-34.14387,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-07T08:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-16.538689999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-07T13:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.98535,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-09T02:05:00","V::N_NIL_V3","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.558590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-10T01:10:00","V::N_NIL_V4","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.903119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-11T00:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-35.794080000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-11T07:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-15.73016,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-11T10:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-217.57758000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-11T11:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-50.34216,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-12T03:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.058579999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-12T03:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.962409999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-12T04:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.518549999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-13T07:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.39818,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-14T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-13.21569,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-15T04:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-20.810479999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-16T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-10.828250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-16T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.92563,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-16T14:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-56.38541,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-17T05:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-24.454450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-18T00:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-10.2674,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-19T20:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-132.40271999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-20T01:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-18.37734,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-21T05:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-03-21",1,-11.596450000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-22T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-29.238109999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-22T03:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-18.030809999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-22T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.37678,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-22T05:00:00","#R014165_001_RAMP_F","#R014165_RAMP","2016-06-21",1,-21.8185,"Hard Ramping constraint for constraint SVML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-06-22T05:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.31508,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-06-22T09:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-45.128860000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-06-22T10:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-46.830970000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-06-22T17:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.65082,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-06-22T19:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-49.512300000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-06-23T04:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.101579999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-06-23T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-16.428280000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-23T05:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.247529999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-06-24T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.256259999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-24T20:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-124.37088,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T02:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-62.112319999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T03:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-44.248690000000003,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T05:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-38.663699999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T06:10:00","#R014184_011_RAMP_F","#R014184_RAMP","2016-06-25",1,-115.11756,"Hard Ramping constraint for constraint V::N_EPMB_V2, Effective Date: 08/04/2016, Version: 2","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-06-25T09:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-135.12893,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T13:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-51.439439999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-25T15:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-20.870429999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-26T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-88.312460000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-27T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-101.88800000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T00:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-17.74258,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T14:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.05369,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T16:10:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-67.410150000000002,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T17:55:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-25.998819999999998,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T20:00:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-195.87559999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T20:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-226.5214,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T21:55:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-102.36046,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-28T23:45:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-12.278090000000001,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T01:05:00","V>SMLBAHO4","V-BAHO;V-BAWA;V-BEKG;V-HOWA","2015-11-24",1,-18.255199999999999,"Out = Ballarat to Horsham or Bendigo to Kerang line, avoid O/L Buronga to Redcliffs (0X1) line for trip of Bendigo to Kerang, or Ballarat to Horsham line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T08:00:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-101.5526,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T16:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-19.333919999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T19:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-290.13283999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T21:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-111.40835,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T21:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-75.35248,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T23:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-55.918810000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-29T23:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-2326.8621899999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T00:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-48.608409999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T02:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-36.148479999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T03:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.27364,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.69462,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T05:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.728199999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T05:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.1333,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T06:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-146.46348,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T07:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-50.13035,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T11:45:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-255.30533,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T20:15:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-37.915439999999997,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-06-30T22:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-119.8556,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T00:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-47.010809999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T02:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-49.896540000000002,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-17.208449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T11:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-220.25319999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T13:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-159.72995,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-01T21:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-21.486319999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T01:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-16.75686,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T03:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-27.580729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T05:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-26.76275,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T07:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-25.57591,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T10:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-261.03222,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-02T21:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-61.633620000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T00:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-18.029209999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T01:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-29.12097,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T02:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-32.472410000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T04:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-28.762329999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T07:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-25.139620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-03T23:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-246.69619,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T00:05:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-126.99611,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T07:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-10.498279999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T11:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-108.18164,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T13:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-65.662859999999995,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T16:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-102.26381000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-04T21:45:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-146.61554000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-05T18:10:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-517.70779000000005,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-05T19:35:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-307.78311000000002,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-05T21:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-352.39465999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-05T22:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-36.156619999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T00:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-211.16382999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T02:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-60.613030000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T05:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-214.20356000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T07:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-315.43423000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T09:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-144.75926000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T11:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-175.85539,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T13:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-123.11368,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T14:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-122.21192000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T15:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-38.4587,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2015-08-24",1,-9036.85,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-06T20:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-196.30054999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T00:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-97.413629999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T02:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-31.910499999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T03:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-28.47148,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T09:15:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-308.60942999999997,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T12:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-247.29937000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T13:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-265.47775999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T19:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-8988.8293200000007,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-07T22:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-254.34061,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T00:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-17.98179,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T01:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-175.35348999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T02:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-318.92381,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T04:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-449.50628999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T05:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-31.407920000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T06:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-38.4587,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T07:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-199.98751999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T11:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-31.853190000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T12:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-263.77463,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T14:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-152.25004000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T15:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-198.41934000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T17:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-199.76987,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T19:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-8977.8959300000006,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T20:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-125.32141,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-08T21:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-196.76092,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T00:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-44.48312,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T01:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-21.955390000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T03:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-42.278230000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T04:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-48.850070000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T07:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-27.138839999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T08:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-259.81887,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T10:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-124.48259,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T10:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-61.339750000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T13:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-48.202190000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-109.35915,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-09T19:50:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-76.945909999999998,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T03:55:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-12.791219999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T07:30:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-15.441560000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T11:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.35014,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T12:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-53.363759999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T19:20:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-73.358519999999999,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T20:00:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-101.48287000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T21:20:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-178.11552,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-10T22:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.481339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T00:10:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-255.87936999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-17.697759999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T09:15:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-87.262910000000005,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T10:05:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-125.63079,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T10:55:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-65.310689999999994,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T11:20:00","CA_SPS_46954420_01","CA_SPS_46954420","2016-07-11",1,-37.212220000000002,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T12:20:00","CA_SPS_46954420_01","CA_SPS_46954420","2016-07-11",1,-31.835360000000001,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T14:30:00","CA_SPS_46954420_01","CA_SPS_46954420","2016-07-11",1,-28.531829999999999,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T15:25:00","CA_SPS_46954420_01","CA_SPS_46954420","2016-07-11",1,-18.351700000000001,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T18:15:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-329.31022999999999,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T20:20:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-76.945840000000004,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T21:50:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-132.13166000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-11T23:35:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-15171.051369999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T00:05:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-808.28886999999997,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T00:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-93.881780000000006,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T07:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-44.502699999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T08:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-151.52196000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T11:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-454.3553,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T13:10:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-163.84107,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T15:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11978.982980000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T16:10:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-84.004949999999994,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T16:50:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-53.932110000000002,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T18:40:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-345.99007,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T19:15:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-550.79003999999998,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T20:20:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-320.29059000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-12T22:10:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-136.81907000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T00:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-127.36548000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T04:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.143789999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T06:05:00","#R014252_010_RAMP_F","#R014252_RAMP","2016-07-13",1,-42.688659999999999,"Hard Ramping constraint for constraint V::N_ROSM_V2, Effective Date: 08/04/2016, Version: 2","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-07-13T07:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-274.06281999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T09:45:00","NRM_SA1_VIC1","NRM_NIL_ALL","2012-06-12",1,-1119.2890199999999,"Negative Residue Management constraint for SA to VIC flow","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T10:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-1207.28306,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T11:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-1042.62363,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T17:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-113.89869,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T20:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-217.17364000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T22:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-125.10925,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-13T22:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-271.44655,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T01:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-301.84706999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T03:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-317.27019000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T04:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-102.47866,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T05:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-65.116159999999994,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T08:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-113.73094,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T11:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-51.354990000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T12:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-202.74718999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T14:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-212.15964,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T16:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-202.19879,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T17:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-243.68709999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T18:25:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-11835.12779,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-14T20:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-705.60443999999995,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-15T01:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-63.023319999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-15T19:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-105.75440999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T04:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-04-18",1,-23.756239999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T08:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-104.89528,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T10:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-27.855029999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T11:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-65.796610000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T12:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-62.278320000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T14:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-52.881959999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T16:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-28.19378,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-8994.2217199999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T20:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-112.06449000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-16T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-61.296720000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-17T01:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-71.927719999999994,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-17T09:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.185680000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-17T15:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-64.220359999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-17T19:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-21.459150000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T00:50:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-149.97642999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T03:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.195830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T05:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.336209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T06:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.31639,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T11:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-36.160989999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T16:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-192.30368000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T16:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-8975.1123700000007,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T18:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-263.33321999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T21:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-89.670689999999993,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-18T22:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-58.426679999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T00:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-54.78584,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T01:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-43.34552,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T07:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-1148.09151,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T08:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-93.624610000000004,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T09:10:00","N^^V_DDSM1","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2015-08-07",1,-200.93405999999999,"Out = Dederang to South Morang 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T10:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-54.552880000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T12:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-193.06691000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T14:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-41.404539999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T16:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-58.834589999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T17:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-151.29736,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-19T19:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-76.386870000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T00:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-21.37763,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T01:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.20899,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T03:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-39.441499999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T05:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-43.102040000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T07:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-28.998139999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T09:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-76.255650000000003,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T10:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-177.20031,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T12:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-181.24262999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T14:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-82.974350000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T16:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-154.54472000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T17:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-151.48925,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T18:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-98.750550000000004,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T19:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.2996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T21:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-181.18187,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-20T22:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-51.792340000000003,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-21T01:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-65.96387,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-21T03:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-80.255529999999993,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-21T19:05:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-40.064160000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-21T19:30:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-43.23601,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T00:40:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-69.050539999999998,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T02:50:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.74329,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T05:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-38.998399999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T08:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.765470000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T15:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-67.596649999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T18:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-52.964709999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T20:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-73.694779999999994,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-22T20:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-105.31647,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T04:35:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-47.599850000000004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T05:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-43.583500000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T09:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-22.921939999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T10:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-60.83905,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T16:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-25.536269999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T18:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-67.908370000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T19:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-32.618519999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T20:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-160.77421000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T22:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-35.820729999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-23T23:00:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-54.678139999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-24T01:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-37.862879999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-25T02:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-29.81917,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-25T05:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.067690000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-25T16:45:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-20.35652,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-25T21:20:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-47.898020000000002,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-25T21:30:00","S>>NIL_RBTU_WEWT","S-NIL","2016-05-31",1,-49.704050000000002,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-26T08:45:00","N^^V_DDSM1","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2015-08-07",1,-15.139609999999999,"Out = Dederang to South Morang 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-26T15:25:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-87.382170000000002,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-26T16:30:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-205.98004,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-26T18:30:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-35.01634,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-26T22:20:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-46.27308,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-27T03:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.83882,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-27T09:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-46.264679999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-27T09:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-44.696770000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-27T11:20:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-10.63761,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-27T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.01153,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.417350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T10:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-24.355129999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T14:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-24.355129999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T15:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.93281,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-40.182690000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T21:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-27.875330000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-28T22:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-32.803939999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-29T00:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-36.406649999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-29T01:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-43.210189999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-29T08:25:00","#R014336_002_RAMP_V","#R014336_RAMP","2016-07-29",1,-18.54393,"Soft Ramping constraint for constraint V>S_NWRB2_NWRB1, Effective Date: 20/03/2015, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-07-29T19:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-15.9961,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-29T20:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-47.442729999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-29T21:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-58.426679999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T11:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.481100000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T13:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-12.204700000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T14:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.39967,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T15:00:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-18.75187,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.806559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T19:30:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-57.505780000000001,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T20:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.623060000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-30T21:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.759359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-31T01:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-68.322959999999995,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-31T06:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-33.650799999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-31T07:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-24.973859999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-07-31T08:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-51.074689999999997,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-01T01:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-42.102150000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-01T09:10:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-12246.516729999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-01T19:55:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-15.51656,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-01T21:05:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-22.966989999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-02T02:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.42634,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-02T04:30:00","S>V_NWRB2_RBNW1","S-NWRB2","2015-03-20",1,-19.660799999999998,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-02T15:45:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-20.076640000000001,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-02T16:15:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-21.741099999999999,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T00:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-10.90875,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T04:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.343909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T09:35:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-69.8018,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T10:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-34.451459999999997,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T13:15:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-32.190170000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T14:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-22.022659999999998,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T20:45:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-20.0687,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-03T21:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-33.959110000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T01:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-40.922220000000003,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T09:50:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-30.61083,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T11:00:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-83.256839999999997,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T13:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-119.06773,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T14:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-86.704520000000002,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-04T15:05:00","V>S_CB6033+6225_TX1","S-NWCB6033+6225","2015-07-21",1,-42.438339999999997,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #1 on trip  of either Monash - North West Bend line #2 132kV line or NWB-MWP1 132kV line.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-05T12:05:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-29.452030000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-05T12:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-38.8949,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-05T14:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-30.761009999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-06T00:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-19.373049999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-06T02:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-30.21893,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-06T22:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.967220000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-07T14:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.55006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T06:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-27.224769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T11:25:00","CA_SPS_46BA5824_01","CA_SPS_46BA5824","2016-08-08",1,-10.825850000000001,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T13:05:00","CA_SPS_46BA5824_01","CA_SPS_46BA5824","2016-08-08",1,-24.60971,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T13:25:00","CA_SPS_46BA5824_01","CA_SPS_46BA5824","2016-08-08",1,-12.867100000000001,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T15:15:00","CA_SPS_46BA5824_01","CA_SPS_46BA5824","2016-08-08",1,-19.644590000000001,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-08T16:15:00","CA_SPS_46BA5824_01","CA_SPS_46BA5824","2016-08-08",1,-24.60971,"Constraint Automation, O/L SMTS     TRANSF F2TR_330 for CTG TVVP on trip of ROTS A1 500/220KV TRANS.  Generated by STNET[NORFL] Host NOREEMP4(SP)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T03:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-14.148479999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T04:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.11931,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T11:20:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-10.84146,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T13:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-12.98673,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T16:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.15995,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T20:00:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-44.352609999999999,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-09T23:45:00","V>>SML_NIL_CONT_7B","V-NIL;V-NIL_BAHO_66_CONT","2016-06-21",1,-75.714079999999996,"Out = Nil, 66 kV line limited cyclic ratings not available, avoid O/L Buangor to Arrarat 66kV line for loss of the Arrarat to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-16.530830000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T03:20:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-18.23461,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T04:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-21.592099999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T05:20:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-17.744579999999999,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T08:15:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-116.36367,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T08:35:00","S>>NIL_HUBG-T_WEWT","S-NIL","2016-05-31",1,-51.272210000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Hummocks-Snowtown-Bungama 132kV T line (this trips Snowtown WF), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T10:35:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-14.40099,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T11:50:00","S>NWCB6024+25_TX3","S-NWBCB6024+6025","2015-07-27",1,-56.713099999999997,"Out= North West Bed 132kV CBs 6024 and 6025(this offloads NWB TX2), avoid O/L North West Bend #3 132/66kV TX on trip of North West Bend- Monash #1 132kV line (this splits NWB 132kV bus), Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T12:30:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-12.799659999999999,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T13:40:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-12.81784,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-10T23:10:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-03-23",1,-12.664,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T08:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-43.355159999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T10:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.765470000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T11:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-27.983460000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T14:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-24.3552,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T18:50:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-153.28035,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T20:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-154.02960999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-11T21:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-50.954360000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-12T14:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.042759999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-13T01:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.073259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T01:45:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-10.68031,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T02:45:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-27.39828,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T04:00:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-12.00971,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T07:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.817029999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T08:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-49.979489999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T10:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-61.28295,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T11:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.143540000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T14:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-23.443180000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T19:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.99447,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T20:10:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-44.722279999999998,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T21:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-11.936769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-14T22:00:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-21.59835,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-15T00:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-12.246600000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-15T08:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.17779,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T10:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.638500000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T15:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.62463,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-15T16:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.706620000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T17:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.6143,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T20:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.112449999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T23:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-389.03874999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-15T23:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-389.03874999999999,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-16T00:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-116.71511,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T01:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-147.37803,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T02:20:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-237.01005000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-16T04:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.067119999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T04:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-36.886969999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-16T06:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-16.112390000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-16T11:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.78623,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T11:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.33705,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T19:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.104780000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T21:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-89.524789999999996,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-16T22:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.2536,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-16T23:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-18.77908,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-17T00:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-97.4101,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T02:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-61.952660000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T03:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-43.523009999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T04:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-32.946910000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T06:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.343450000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T08:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.98922,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T10:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-35.001710000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T11:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.7226,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.70241,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T17:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.29635,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T18:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.780329999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-17T19:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.074820000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T02:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-21.54335,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-18T03:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-24.857859999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T04:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-22.05433,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T05:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.74724,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-18T11:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.385910000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T13:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.9749,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T15:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.00062,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-18T21:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-25.21686,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-18T22:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.10303,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-18T23:50:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-187.27968000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-19T06:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.985139999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-19T19:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.26707,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-19T20:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.78567,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-19T23:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.604710000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-19T23:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-445.82389000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-20T01:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.806889999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T03:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.214829999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T04:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.81415,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-20T05:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.68633,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-20T05:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.651149999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T07:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.013339999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T17:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.549479999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T20:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.911370000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T20:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-25.210290000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-20T22:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-21.04908,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-20T23:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-241.79557,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-21T00:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-29.878779999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T02:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.51173,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T03:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.121390000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T05:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-32.441540000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T07:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-51.15155,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T07:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-51.115459999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.541460000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T16:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-23.301649999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T18:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-28.966280000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T19:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-71.332689999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T21:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-262.34183000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-21T22:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-63.984740000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T02:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-89.598939999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T02:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-95.900720000000007,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T03:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-22.902370000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T05:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-32.477789999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T07:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-84.838160000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T09:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-235.84705,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T10:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.47247,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T15:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-33.751890000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T16:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.10885,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T17:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-16.93234,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T19:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-48.200090000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-22T21:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.65644,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T02:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-40.323720000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T07:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.031090000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T09:05:00","N^^V_SMTXH1_1","V-SMTS_HTX_P;V-SMTS_HTX_R;V-SMTXH1T_P;V-SMTXH1T_R;V-SMTXH1_P;V-SMTXH1_R","2015-08-07",1,-31.55772,"Out = South Morang H1 or H2 500/330 kV txfmr, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-23T12:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-42.318019999999997,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T13:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-45.262210000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T14:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-20.797999999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-23T14:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-77.037520000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T15:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.70416,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T20:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.580109999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-23T20:40:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-33.841729999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-23T21:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-24.410399999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-24T06:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-11.56052,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-24T08:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.36182,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-24T15:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.425459999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-24T16:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.016019999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-24T19:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.062810000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T00:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.837109999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T00:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.96693,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T07:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.777900000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T09:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.223610000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T16:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.78314,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T18:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.196289999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-25T19:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.270479999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T05:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.858459999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T07:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-52.55744,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T08:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-209.70330000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.663489999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T11:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-27.187850000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"PLANNED",1]
[null,null,"2016-08-26T19:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-24.372679999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-26T21:55:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-47.829279999999997,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-26T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL_","2016-07-07",1,-207.66512,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-27T02:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.377759999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-27T02:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.825950000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-27T03:30:00","V:SS_PA_SVC_795","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_WEST_BUS_R;S-X_PA_W_BUS_R+BWPA","2016-07-06",1,-20.51238,"Out= one Para SVC, Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 795 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-27T04:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.01258,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-27T21:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.325810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-28T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.8184,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-28T07:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.171519999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-29T03:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.21359,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-29T22:40:00","V>>V_KTSY_1_R","V-KTSY_R;V-X_KTSY_KTA4","2016-07-01",1,-10.15536,"Out = Keilor to Sydenham 500 kV line, avoid overload of South Morang F2 500/330 txfmr for trip of South Morang to Keilor 500kV line, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-29T23:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-16.101120000000002,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-30T11:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-14.6393,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-31T15:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-64.871949999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-31T16:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-215.17625000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-08-31T21:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-13.86387,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-01T00:25:00","V::N_NIL_SD-100","V-DSA_STAB-100","2016-07-25",1,-18.15484,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise. Fixed 100 MW offset to manage DSA alarms","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-01T01:10:00","V::N_NIL_SD-100","V-DSA_STAB-100","2016-07-25",1,-45.404269999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise. Fixed 100 MW offset to manage DSA alarms","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-01T03:55:00","V::N_NIL_SD-050","V-DSA_STAB-050","2016-07-25",1,-11.97715,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise. Fixed 50 MW offset to manage DSA alarms","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-01T04:30:00","V::N_NIL_SD-050","V-DSA_STAB-050","2016-07-25",1,-11.26844,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise. Fixed 50 MW offset to manage DSA alarms","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-01T08:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.911020000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-03T15:35:00","V>>V_KTSY_1_R","V-KTSY_R;V-X_KTSY_KTA4","2016-07-01",1,-10.78219,"Out = Keilor to Sydenham 500 kV line, avoid overload of South Morang F2 500/330 txfmr for trip of South Morang to Keilor 500kV line, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T00:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-14.784409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T03:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.29467,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T07:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-16.542090000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T08:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-48.782069999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T10:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.404219999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T11:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-25.464829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T13:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-16.185780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T16:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.391300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T18:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-72.042820000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T20:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-34.473199999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T22:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-55.796390000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-04T23:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.85352,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T00:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-62.804340000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T02:15:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-07-28",1,-18.548100000000002,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T03:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-20.996220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T05:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.357939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T06:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-27.154299999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T11:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.4465,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T13:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.342739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T19:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-68.06841,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-05T22:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-36.157820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T01:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.541409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T01:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.71913,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T03:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-16.044910000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T04:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.949820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T09:20:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-10.78341,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T10:30:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-73.813919999999996,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T11:40:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-73.157579999999996,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T14:05:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-15.97128,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T15:40:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-12.57573,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T16:00:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-19.96828,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-06T17:45:00","V>S_NWRB2_NWRB1","S-NWRB2","2015-03-20",1,-10.03266,"Out = North West Bend-Robertstown 132kV No2 line, limit SA-V on ML to avoid O/L of  Robertstown-NWB1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-07T04:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.7746,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-07T22:35:00","V>>V_KTSY_1_R","V-KTSY_R;V-X_KTSY_KTA4","2016-07-01",1,-11.83263,"Out = Keilor to Sydenham 500 kV line, avoid overload of South Morang F2 500/330 txfmr for trip of South Morang to Keilor 500kV line, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-07T23:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.22452,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T00:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-38.80415,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T01:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-48.706139999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T02:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-88.983580000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T02:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-44.202289999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T03:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-45.321100000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T04:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-55.386119999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T05:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-72.048000000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T06:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-90.12039,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T12:55:00","S>>BRDV_RBTU_WEWT","NULL","2016-09-02",1,-46.686790000000002,"Out= Brinkworth - Davenport 275kV line, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-08T23:45:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-313.97681999999998,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-09T01:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-63.554760000000002,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-09T05:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-87.486459999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-09T13:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-61.915489999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-09T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2015-03-26",1,-65.754689999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T00:15:00","V:SS_PA_SVC_820","S-PA_EAST_BUS;S-PA_EAST_BUS_R;S-PA_VC1;S-PA_W_BUS_R","2016-09-01",1,-14.46697,"Out= one Para SVC(Note: both Black Range series caps I/S), Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 820 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T09:45:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-36.57929,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T11:20:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-26.697769999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T13:25:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-19.356960000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T19:35:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-24.394110000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-12T22:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-15.74399,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-13T00:30:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-19.29982,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-13T02:55:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-19.947230000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-13T10:15:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-23.723320000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-15T10:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-20.900020000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-15T18:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.177489999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-15T21:10:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-07-28",1,-45.799840000000003,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-16T01:25:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-07-28",1,-22.825299999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-16T02:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-22.856030000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-18T21:55:00","V:SS_PA_VC-POD_820","S-PA_SVC1-POD","2016-09-13",2,-44.253270000000001,"Out= one Para SVC(Note: both Black Range series caps I/S), Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 820 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-19T00:10:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-12.69603,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-19T03:05:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-19.649619999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-19T07:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-13.47791,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-22T06:05:00","#R014602_004_RAMP_V","#R014602_RAMP","2016-09-22",1,-70.144009999999994,"Soft Ramping constraint for constraint V::N_MLSY_Q4, Effective Date: 08/04/2016, Version: 2","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-09-22T08:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11.005599999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-22T12:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-19.611979999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-25T08:25:00","V>SMLMHNW2","S-MHNW_2;S-NWCB6022+6023","2015-07-14",1,-24.581499999999998,"Out = Monash-North West Bend # 2 132kV line, limit Murraylink (Vic to SA) to avoid overloading Monash-North West Bend # 1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-25T09:40:00","V>SMLMHNW2","S-MHNW_2;S-NWCB6022+6023","2015-07-14",1,-12.13944,"Out = Monash-North West Bend # 2 132kV line, limit Murraylink (Vic to SA) to avoid overloading Monash-North West Bend # 1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-25T19:55:00","V>SMLMHNW2","S-MHNW_2;S-NWCB6022+6023","2015-07-14",1,-35.492919999999998,"Out = Monash-North West Bend # 2 132kV line, limit Murraylink (Vic to SA) to avoid overloading Monash-North West Bend # 1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-25T20:05:00","V>SMLMHNW2","S-MHNW_2;S-NWCB6022+6023","2015-07-14",1,-25.704789999999999,"Out = Monash-North West Bend # 2 132kV line, limit Murraylink (Vic to SA) to avoid overloading Monash-North West Bend # 1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-26T07:50:00","N^^V_NIL_1","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2015-09-02",1,-17.069289999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T00:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.348980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T13:40:00","V>SMLMHNW2","S-MHNW_2;S-NWCB6022+6023","2015-07-14",1,-30.32816,"Out = Monash-North West Bend # 2 132kV line, limit Murraylink (Vic to SA) to avoid overloading Monash-North West Bend # 1 132kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T16:55:00","V::N_ESTN_HYSE_VD","SA_ESTN_ISLE","2015-07-01",1,-46.630830000000003,"SA / ESTN separation between Heywood and South East Sub, avoid transient instability for fault and trip of a Hazelwood to Sth Morang 500kV line, Basslink VIC to TAS, VIC accelerates, segment 1","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T18:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-1044.7809199999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-28T18:35:00","V::N_ESTN_HYSE_VD","SA_ESTN_ISLE","2015-07-01",1,-29.70262,"SA / ESTN separation between Heywood and South East Sub, avoid transient instability for fault and trip of a Hazelwood to Sth Morang 500kV line, Basslink VIC to TAS, VIC accelerates, segment 1","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T19:45:00","V::N_ESTN_HYSE_VE","SA_ESTN_ISLE","2015-07-01",1,-23.479150000000001,"SA / ESTN separation between Heywood and South East Sub, avoid transient instability for fault and trip of a Hazelwood to Sth Morang 500kV line, Basslink VIC to TAS, VIC accelerates, segment 2","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T19:55:00","V::N_ESTN_HYSE_VE","SA_ESTN_ISLE","2015-07-01",1,-22.763069999999999,"SA / ESTN separation between Heywood and South East Sub, avoid transient instability for fault and trip of a Hazelwood to Sth Morang 500kV line, Basslink VIC to TAS, VIC accelerates, segment 2","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-28T20:55:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13780.2448,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-28T22:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13785.10024,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-28T23:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-1429.3000199999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-28T23:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13376.44399,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-29T01:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-30.537939999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-29T02:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.808120000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-29T02:50:00","V>>N_SMHTX_1","V-SMTS_HTX_P;V-SMTS_HTX_R","2016-09-08",1,-11.900359999999999,"Out = South Morang H1 or H2 330/220 kV txfmr, avoid O/L of South Morang H2 or H1 330/220 kV txfmr (flow 220 kV to 330 kV) for trip of the South Morang F2 500/330 kV txfmr, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-29T03:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-46.506030000000003,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-29T04:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-91.35772,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-29T06:45:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-254.50187,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-09-29T08:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",6,-171.79133999999999,"V-S-MNSP1.ENERGY * 1 = 180 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T10:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",7,-45.879080000000002,"V-S-MNSP1.ENERGY * 1 = 130 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T12:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",9,-80.226020000000005,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T13:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",9,-78.693110000000004,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T14:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",9,-76.516369999999995,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T16:05:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",10,-228.37531999999999,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T17:50:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",12,-186.48822999999999,"V-S-MNSP1.ENERGY * 1 = 220 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T19:40:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",12,-33.60521,"V-S-MNSP1.ENERGY * 1 = 220 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T21:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",14,-75.954930000000004,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-29T23:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-29",14,993.26842999999997,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T00:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",1,-32.806399999999996,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T02:05:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",1,936.56313999999998,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T02:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",2,-42.270870000000002,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T04:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",2,960.09632999999997,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T06:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-33.806690000000003,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T08:00:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-103.83920999999999,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T10:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-10.40743,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T11:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-28.359909999999999,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T13:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-31.04214,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T14:25:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,76.882750000000001,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T15:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-37.727350000000001,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T16:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,-31.04214,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T18:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",3,12.03856,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-09-30T21:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-14.61032,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-09-30T22:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",6,-16.974550000000001,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T00:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-09-30",7,-30.29129,"V-S-MNSP1.ENERGY * 1 = 200 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T02:00:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",2,-55.375079999999997,"V-S-MNSP1. * 1 = 80 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T03:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-59.064070000000001,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T05:00:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-100.5955,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T06:25:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-76.254779999999997,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T07:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-59.175840000000001,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T07:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.091100000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T08:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-56.282820000000001,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T09:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-54.841030000000003,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T10:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,979.28502000000003,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T11:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-13.672129999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T12:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.889939999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T13:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-60.444290000000002,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T13:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",3,-60.606349999999999,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T14:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.61992,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T14:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",5,976.53413,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T15:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.566289999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T16:50:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",6,77.428569999999993,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T18:05:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",7,939.95477000000005,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T20:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",7,-14.16072,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T21:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",7,938.22320999999999,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-01T22:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.46269,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-01T23:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-148.19783000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T00:10:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-219.3914,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T01:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-01",9,71.24239,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T02:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",1,-85.122380000000007,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-33.303040000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T04:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",1,-80.695430000000002,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T05:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-29.238790000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T05:50:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",1,-51.94567,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T06:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-18.77374,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T07:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",3,934.11945000000003,"V-S-MNSP1. * 1 = 120 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T08:35:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",4,-52.186540000000001,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T10:25:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",4,946.39670000000001,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T11:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-35.136569999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T12:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",5,52.683030000000002,"V-S-MNSP1.ENERGY * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T13:00:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",5,55.200449999999996,"V-S-MNSP1.ENERGY * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.420000000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T14:00:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",5,51.60407,"V-S-MNSP1.ENERGY * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T15:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",6,-57.007019999999997,"V-S-MNSP1.ENERGY * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T15:50:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",7,-54.12218,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T17:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-200.74421000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-02T19:05:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,-35.661969999999997,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T20:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,-43.036340000000003,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T21:40:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,-46.479340000000001,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T22:15:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,941.14153999999996,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-02T22:40:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,76.158940000000001,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T00:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-02",9,90.378270000000001,"V-S-MNSP1.ENERGY * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T01:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-10.82877,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T02:15:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",1,-47.950949999999999,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T03:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-13.65537,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T04:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-12.021179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T05:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",1,-39.42465,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T07:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",2,87.883349999999993,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T08:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",2,-23.797999999999998,"V-S-MNSP1. * 1 = 150 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T09:55:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",3,946.72,"V-S-MNSP1. * 1 = 120 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T11:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",5,-56.497419999999998,"V-S-MNSP1. * 1 = 50 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T12:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.893650000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T13:20:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",10,946.19320000000005,"V-S-MNSP1. * 1 = 100 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T14:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.08272,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T15:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.445440000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T16:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.073090000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T16:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-27.953849999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T17:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.605309999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-03T18:30:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",13,-309.27965,"V-S-MNSP1. * 1 = 160 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T20:10:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",14,-18.892389999999999,"V-S-MNSP1. * 1 = 200 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T21:45:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",14,-58.070569999999996,"V-S-MNSP1. * 1 = 200 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T22:50:00","#V-S-MNSP1_E_E","#V-S-MNSP1_E","2016-10-03",14,-20.244150000000001,"V-S-MNSP1. * 1 = 200 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-03T23:35:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-564.19069000000002,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T00:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-22.3353,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T01:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-69.30104,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T01:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-66.996650000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T02:25:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-30.173010000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T03:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-77.401989999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T04:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-17.489350000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T06:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-116.24109,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T08:25:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-29.719080000000002,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T09:55:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-123.49243,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T11:05:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1018.82344,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T11:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.693159999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T12:35:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1010.14855,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T14:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1012.94754,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T14:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1015.77257,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.1441,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-04T16:35:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1025.24101,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T18:00:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-44.873869999999997,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T22:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-13.07658,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-04T22:40:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-12.955500000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T00:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.77239,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-05T10:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1029.3665699999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T11:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1022.12997,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T13:40:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1024.5266999999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T14:40:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1033.58151,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T15:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-119.73211999999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-05T20:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.363950000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-05T20:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.416,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-05T22:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-50.277619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T01:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-13.24141,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T04:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.044890000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T08:20:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1025.51675,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T09:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1012.0785100000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T10:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.363489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T11:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.53871,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T12:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1021.17993,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-19.061520000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T13:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1020.09813,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-21.065729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-10.5496,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T15:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1050.7573400000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T17:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1035.31798,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T18:20:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1021.70712,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T19:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1026.5010400000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T20:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.752330000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T20:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-18.368020000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T21:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-21.41356,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-06T22:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1019.13737,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T22:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1019.14058,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-06T23:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-250.7764,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-07T01:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.624829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-07T02:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-994.97807999999998,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T03:20:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1015.77034,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T04:20:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1012.73351,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T06:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-11921.50424,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-07T09:00:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1033.98317,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T14:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1041.6467399999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T18:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1032.52567,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-07T20:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1041.8970300000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-08T07:55:00","#R014657_002_RAMP_F","#R014657_RAMP","2016-10-08",1,-13764.03283,"Hard Ramping constraint for constraint VSML_ZERO, Effective Date: 21/08/2013, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-10-08T08:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-289.66888999999998,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","8(E)","AEMO restoration process: market suspension in SA from 28/9/16 1625 hrs until 11/10/16 23:30. ","UNPLANNED",0]
[null,null,"2016-10-08T17:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1027.6833899999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-08T18:40:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1043.6096,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-08T20:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1027.2737,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-08T22:05:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1038.38957,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T00:05:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1021.09339,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T01:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1009.24179,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T02:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-993.10478000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T03:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-998.48545999999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T04:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.630380000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T04:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-989.32596000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T05:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.84219,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T07:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1010.0938599999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T08:40:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1011.9411,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T09:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.7248,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T10:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-15.656560000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T11:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.95942,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T13:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-982.54841999999996,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.004379999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.68234,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.2911,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-09T17:55:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1306.32034,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T20:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1014.1248399999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T20:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1014.42698,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-09T23:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1020.0445,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T00:05:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1010.71496,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T02:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-991.18493999999998,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T02:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-992.28903000000003,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T03:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-987.40912000000003,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T04:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1013.81306,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T06:05:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1021.56765,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T06:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1043.7393099999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T09:25:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1027.08584,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T10:25:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1023.09998,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T12:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.429400000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T12:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1024.2399499999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T13:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-33.776699999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T14:15:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1022.65439,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.66113,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T15:25:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1035.87257,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T16:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.8353,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T17:50:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1044.85022,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T19:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-380.90645999999998,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T19:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1043.3269399999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T21:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.999180000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T21:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.02636,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-10T22:45:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1012.23168,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-10T23:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1033.05792,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T00:35:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-33.057049999999997,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T01:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1010.91062,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T03:10:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-1010.50892,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T03:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-15.03205,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T04:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-14.750069999999999,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T08:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.964919999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T10:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.28234,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T11:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-19.62424,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T13:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-15.87697,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T14:05:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-04-08",2,-13.670389999999999,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T14:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.44772,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T14:45:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-04-08",2,-28.518190000000001,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T15:30:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-35.652819999999998,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-10-11T16:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-19.97392,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T21:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.06385,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-11T22:45:00","V>>V_KTSY_1_R","V-KTSY_R;V-X_KTSY_KTA4","2016-07-01",1,-36.708889999999997,"Out = Keilor to Sydenham 500 kV line, avoid overload of South Morang F2 500/330 txfmr for trip of South Morang to Keilor 500kV line, radial mode, YWG1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T01:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-39.773719999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T02:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-22.61571,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T04:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-61.511150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T05:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-54.626460000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T14:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.34188,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T20:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-27.119450000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-12T21:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-27.920529999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-13T00:30:00","V::N_NIL_Q2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-08-12",1,-11.65006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-13T04:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-37.095669999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-13T11:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-37.274250000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-13T14:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.513170000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-13T18:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.160969999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T01:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-18.845189999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T09:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.74821,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T10:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.55963,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T11:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-48.759140000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T12:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-37.678600000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T13:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-48.33372,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T14:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-41.73254,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T15:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-21.889119999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T15:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.36307,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T16:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-20.462540000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T17:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-81.144080000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T17:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-19.348130000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T19:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-20.096810000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T21:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-23.145769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T22:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-28.69941,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T23:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-17.585529999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-14T23:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-13.63772,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T01:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-20.236070000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T01:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-53.00544,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T03:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-49.742530000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T04:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-39.23095,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T06:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-62.661630000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T07:20:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-19.628589999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T08:00:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-28.624860000000002,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T08:15:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-44.25403,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T09:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-44.837739999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T09:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-33.097850000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T10:45:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-28.965450000000001,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T11:30:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-35.751339999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T12:30:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-21.307200000000002,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T13:25:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-18.477219999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T14:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-32.200800000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T14:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-39.017389999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T16:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.847629999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T17:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.239649999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T19:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.109529999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-15T20:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-13.35065,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T02:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-47.700789999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T08:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.358219999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T10:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-17.15258,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T11:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-16.541789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T14:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-31.690539999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-16T15:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.2544,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T00:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-18.318200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T07:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.249739999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T09:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-20.17352,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T11:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-43.884300000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T11:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-30.53708,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T14:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.375210000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T15:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-24.469940000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T16:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.778120000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T19:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-13.75334,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-17T22:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-31.38768,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T04:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-13.32795,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T07:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-23.522220000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T09:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-25.57488,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T11:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-15.479010000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T12:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.679300000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T12:45:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-64.623779999999996,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T13:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.973949999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-18T16:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-79.866950000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T01:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-18.52224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T02:45:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.776969999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T03:50:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-19.36994,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T11:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.907719999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T13:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.398610000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T13:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-21.05265,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-19T16:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.960710000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T00:25:00","V::N_HYSE_Q1","I-HYSE","2016-04-08",2,-59.802790000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T01:45:00","V::N_HYSE_V1","I-HYSE","2016-04-08",2,-26.153580000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T03:50:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-16.521820000000002,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T05:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-71.638260000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T08:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.84327,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T09:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-67.537580000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T10:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.302040000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T10:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-15.51736,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T11:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-66.17192,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T12:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-65.915809999999993,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T12:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.50985,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T13:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-66.239450000000005,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T14:00:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-10.59238,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T14:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-65.939279999999997,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T14:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-100.41518000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T15:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.41559,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T16:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-68.943640000000002,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T17:05:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-64.038830000000004,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T18:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-25.074190000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T21:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.10167,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T23:00:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-53.89828,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-20T23:15:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-22.4236,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T00:15:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-22.028849999999998,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T01:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-75.968990000000005,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T02:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-51.910359999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T03:10:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-25.531690000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T04:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-16.68113,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T11:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-29.486989999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T13:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-21.542310000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T15:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-81.622969999999995,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-21T15:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-82.638570000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T00:55:00","V::N_HYSE_V1","I-HYSE","2016-04-08",2,-28.280830000000002,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T01:25:00","V::N_HYSE_V1","I-HYSE","2016-04-08",2,-24.84796,"Outage = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T07:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.236999999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T11:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.81142,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T12:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-14.654540000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T14:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-21.808910000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T19:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-72.258899999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-22T22:30:00","V::N_BYPASS_HW_SY_V2","NULL","2016-04-08",2,-34.474800000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T00:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-18.625979999999998,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T01:20:00","V::N_BYPASS_HW_SY_V2","NULL","2016-04-08",2,-41.329140000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T03:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-38.291609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T04:40:00","#R014729_010_RAMP_V","#R014729_RAMP","2016-10-22",1,-53.177990000000001,"Soft Ramping constraint for constraint V::N_HWSM_V2, Effective Date: 08/04/2016, Version: 2","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-10-23T05:55:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-47.198549999999997,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T08:55:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-24.34441,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T11:00:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-29.018879999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T11:20:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-29.795089999999998,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T14:05:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-35.855969999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-23T14:35:00","V::N_HWSM_V2","V-HWCB4;V-HWRO3;V-HWSM","2016-04-08",2,-32.776600000000002,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-24T18:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.084530000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-25T04:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-31.364740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-25T08:30:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.29124,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-25T11:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.77535,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-25T14:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.36173,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-25T14:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-13.864129999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-26T02:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-27.04729,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-26T04:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-23.008179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-14.70739,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T04:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-18.394100000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T09:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.617839999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T15:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-38.028849999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T17:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-40.874789999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T17:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-29.574480000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T18:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-21.585750000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-27T19:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-15.225020000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-28T12:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.042590000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-28T15:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.39132,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-28T16:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.24878,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-28T18:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-19.069790000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-28T23:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-30.17436,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T00:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.42939,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T06:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.84694,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T07:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.492609999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T10:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-15.87003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T11:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.88758,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T13:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-26.132629999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T15:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-29.131360000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T16:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-26.35688,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T17:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-20.907640000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T20:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-28.705539999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T22:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.46381,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-29T23:50:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-19.229659999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T00:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-11.68746,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-41.983199999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T04:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-45.94659,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T08:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-47.077800000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T09:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-26.61861,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T11:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-35.770110000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-43.576689999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T13:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-44.017240000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T15:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-25.40898,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T16:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-18.113890000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T19:45:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-12.99525,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T21:20:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-11.450670000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-30T23:25:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-18.886559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T06:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-26.024619999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T08:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-36.50956,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T08:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-18.927510000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T09:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.309480000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T10:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.788829999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T13:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-25.776700000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T14:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.335410000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T15:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-27.035959999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T17:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-32.786110000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T18:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-29.69772,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T18:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-20.934809999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T21:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.29401,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-10-31T23:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-14.17393,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T05:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-37.574509999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T06:10:00","V::N_NIL_Q2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-08-12",1,-42.488390000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T07:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-49.891460000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T08:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-142.24413999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T10:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-68.282520000000005,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T10:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-67.723709999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T11:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-37.28201,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T13:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-42.632440000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T15:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-68.776340000000005,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T16:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-64.032759999999996,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T18:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.529260000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T20:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-12.11177,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T21:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-35.56512,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T22:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-21.441759999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-01T23:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-15.770479999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-02T00:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.751710000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-02T02:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.890999999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-02T03:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-16.897290000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-02T14:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.576409999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-02T16:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.07206,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-03T01:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-51.141669999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-03T03:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-29.910869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-03T03:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-17.653359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-03T07:35:00","V>>V-MSUT_1","H-MSUT_P;H-MSUT_R;I-MSUT;I-MSUT_P;I-MSUT_R","2016-06-28",1,-10.62144,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-03T14:05:00","V>>V-MSUT_1","H-MSUT_P;H-MSUT_R;I-MSUT;I-MSUT_P;I-MSUT_R","2016-06-28",1,-10.609,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T02:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-15.7881,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T03:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-25.291609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T05:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-29.024920000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T10:10:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-11.79265,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T11:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-12.76535,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T11:30:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-24.09967,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T12:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-16.025269999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T13:30:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-19.445979999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T13:50:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-30.113189999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T15:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-44.379800000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T16:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-54.529780000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T18:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.080649999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T19:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-40.387099999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T20:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-34.119309999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T21:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-20.273510000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-04T22:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-32.8628,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T00:55:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-16.524699999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T01:50:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-13.886760000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T03:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-44.549289999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T04:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-11.125019999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T05:40:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-17.617819999999998,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T06:15:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-17.897819999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T07:25:00","V::N_MLSY_V1","V-MLSY_NOEMTT_KTS_P;V-MLSY_NOEMTT_KTS_R;V-MLSY_P;V-MLSY_R","2016-04-08",2,-39.228769999999997,"Out = Moorabool to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T08:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-35.766820000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T11:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-23.288309999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T12:10:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-22.422270000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T13:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-33.545259999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T15:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-14.03912,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T16:00:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-23.024290000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T16:40:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-18.000219999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T18:00:00","V::N_NIL_S1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-19.360040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T19:20:00","V::N_NIL_S1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-43.762819999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T21:05:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-45.915219999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-05T22:55:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-33.103490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T00:20:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-34.051229999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T01:45:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-36.126620000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T03:40:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-55.917659999999998,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T04:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-65.636989999999997,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T05:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-13.106870000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T06:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-18.577169999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T08:10:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-17.272580000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T10:00:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-17.074359999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T11:35:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-23.47607,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T13:55:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-23.084869999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T15:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-32.259369999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T16:20:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-28.387219999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-06T22:55:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-18.262630000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T00:15:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-15.15443,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T00:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-11.053739999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T01:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-54.789050000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T02:10:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-50.186579999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T03:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-50.52196,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T04:05:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-80.120069999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T04:55:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-18.684670000000001,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T11:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-41.992339999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T12:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-55.933549999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T13:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-55.9923,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T14:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-45.190669999999997,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T15:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-18.39048,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T17:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.29327,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T18:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-48.937750000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-07T22:05:00","V::N_NIL_S1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-247.65565000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T01:20:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-14.30654,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T02:15:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-22.4892,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T02:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-17.559349999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T03:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.8812,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T04:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-35.817369999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T10:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-19.37396,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T11:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-129.04445000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-08T14:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-225.00743,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-09T01:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-33.402180000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-09T03:45:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-35.105829999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-09T04:40:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-26.221820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-09T22:35:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-232.40091000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T00:50:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-25.645520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T02:15:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-15.12923,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T02:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-28.158480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T04:10:00","V::N_NIL_V1","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-12.82362,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T22:10:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-42.005110000000002,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T23:00:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-35.855029999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-10T23:20:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-21.947389999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-11T00:35:00","V::N_BUDP_V1","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-18.81391,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-11T02:25:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-15.848179999999999,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-11T04:40:00","V>>V_BTRT_2_P","V-BTRT_P","2016-04-05",1,-15.93844,"Out= Brunswick to Richmond 220kV line, avoid pre-contingent O/L South Morang 500/330kV (F2) transformer, Parallel Mode, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-11T07:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.28252,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-11T22:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-155.14111,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-11T23:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.18281,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T00:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.889749999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T01:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.34727,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T03:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-45.763959999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T05:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.106539999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T07:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.266690000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T08:00:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-34.946719999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-12T10:00:00","SVML_000","I-ML_ZERO;I-SVML_000","2008-08-05",1,-30.41358,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T11:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-36.335839999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T13:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-80.168660000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T14:25:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-67.179640000000006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-12T15:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-26.494789999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T20:00:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-401.75808000000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-12T22:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-35.887979999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T22:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-931.83132999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-12T23:30:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-2184.0888500000001,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-13T00:15:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-519.19204999999999,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-13T03:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.435580000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T04:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.69584,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T05:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.82391,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T07:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.303649999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T10:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-68.716470000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T11:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-52.599150000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T12:25:00","V>>V_NIL_2B_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-46.943219999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-13T13:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-62.80789,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T15:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-50.586309999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T16:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-55.457590000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T17:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.29786,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T18:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-384.42594000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T19:25:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-332.83674999999999,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-13T19:55:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-640.05633,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-13T20:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-411.07891999999998,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T22:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-573.28427999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-13T23:40:00","V>>SML_NIL_7B","@HWPS_20090217;V+NIL_PAR_3-5;V+NIL_PAR_6-2;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_3-4;V-NIL;V-NIL_PAR_2-5;V-NIL_PAR_3-5;V-NIL_PAR_6-2;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_H","2016-08-12",1,-1852.8316199999999,"Out = Nil, avoid O/L Buangor to Ararat 66kV line for loss of the Ararat to Horsham 220kV line, swamped if BATS-HOTS 66 kV tie opened, or with BGR tie splitting scheme in service","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T00:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-177.84523999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T01:45:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-10.448,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T04:10:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-16.057659999999998,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T07:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-58.31447,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T10:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-37.16339,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T12:25:00","V::N_BUDP_V2","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-10.51942,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T16:10:00","V>>N-NIL_HG","N-NIL;N-NIL_H","2016-07-01",1,-39.52187,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Nil trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T18:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.59722,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T20:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-210.16691,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T20:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-82.877870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T21:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-68.185069999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T22:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.48902,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-14T22:55:00","V::N_BUDP_V2","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-84.772909999999996,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-14T23:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-16.608409999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T00:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.864350000000002,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T01:35:00","V::N_BUDP_V3","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-59.301630000000003,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T02:35:00","V::N_BUDP_V3","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-36.726669999999999,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T03:15:00","V::N_BUDP_V3","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-24.68703,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T03:35:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-44.234430000000003,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T04:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.833220000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T05:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-70.138819999999996,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T06:25:00","V::N_DDWO_V4","V-DDWO_RADIAL","2016-04-08",2,-129.28465,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T08:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-32.299390000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T09:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-42.26614,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T10:50:00","V::N_DDWO_V2","V-DDWO_RADIAL","2016-04-08",2,-19.809989999999999,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T11:40:00","V::N_DDWO_V2","V-DDWO_RADIAL","2016-04-08",2,-19.809989999999999,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T15:30:00","V::N_DDWO_V2","V-DDWO_RADIAL","2016-04-08",2,-11.3,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T16:15:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.797319999999999,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T16:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-17.464939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-15T17:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.829980000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T19:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.82578,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T22:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-106.97026,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-15T22:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-17.371939999999999,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-16","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.511620000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-16T01:15:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-44.440150000000003,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T01:45:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-42.1387,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T03:20:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-35.232869999999998,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T04:30:00","V::N_BUDP_V4","N-BUDP;N-DPWG_63_X5","2016-04-08",2,-51.703850000000003,"Out = Buronga to Darlington Point 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T05:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.911300000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-16T09:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.572760000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-16T11:45:00","V::N_DDWO_S2","V-DDWO_RADIAL","2016-11-16",1,-10.280469999999999,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T14:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.221579999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T17:35:00","V::N_SMF2_V2","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-18.365210000000001,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T17:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.84665,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T19:10:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13.888070000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-16T21:10:00","V::N_SMF2_V2","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-28.875589999999999,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-16T23:05:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-56.968519999999998,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T01:10:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-29.001259999999998,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T02:00:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-18.38364,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T03:30:00","V>>V_SMTXF2_6","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-09-19",1,-23.89227,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T05:25:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-38.821440000000003,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T05:50:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-60.450090000000003,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T13:00:00","V::N_SMF2_V4","V-SMTXF2_P;V-SMTXF2_R;V-X_BTRT_SMF2_KTS_P;V-X_BTRT_SMF2_KTS_R","2016-04-08",2,-11.4322,"Out = South Morang F2 500/330 kV txfmr, prevent transient instability for fault and trip of Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T14:25:00","V>>V_BTRT_SMF2_KT_DR","V-BTRT_SM330B2_KTS_R;V-X_BTRT_SMF2_KTS_R","2016-10-11",1,-12.01728,"Out=Brunswick-Richmond 220kV cable and South Morang F2 500/330kV TX, with KTS 220kV bus #1 & #2 tied and both KTS-TTS lines bypass KTS to WMTS, avoid O/L Rowville-Thomastown 220kV line on trip of Rowville A1 500/220kV TX, Radial, YWPS1 on 500kV, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T16:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.56415,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-17T17:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-13.65316,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T19:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-37.888559999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T20:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-15.54921,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-17T20:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.512540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T21:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-58.694429999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T22:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-27.636109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-17T23:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-70.05829,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T00:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.263359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T02:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.188459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T02:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-10.05649,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T03:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-11.51892,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T04:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-28.57283,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T07:25:00","V::N_DDWO_SD","V-DDWO_RADIAL","2016-11-16",1,-10.37243,"Out = Dederang - Wodonga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T15:25:00","V:SS_PA_VC-POD_820","S-PA_SVC1-POD","2016-09-13",2,-27.19031,"Out= one Para SVC(Note: both Black Range series caps I/S), Oscillatory stability limit for Vic to SA on Heywood+ Murrylink upper transfer limit of 820 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T19:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-10.652089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T20:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-76.5505,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T21:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-32.20561,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-18T23:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-35.949480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T00:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-20.778390000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T02:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.2865,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T04:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-12.19304,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T05:55:00","V::N_KTSY_V2","V-KTSY_P;V-KTSY_R","2016-11-08",1,-10.6531,"Out = Keilor to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T08:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS","2016-06-21",1,-13.09449,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T14:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-15.49999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T17:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.78848,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-19T18:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-13.36961,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-20T00:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-11.496409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-20T06:20:00","V::N_KTSY_V2","V-KTSY_P;V-KTSY_R","2016-11-08",1,-15.01085,"Out = Keilor to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-20T08:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-82.865650000000002,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-20T13:30:00","V::N_KTSY_SD","V-KTSY_P;V-KTSY_R","2016-11-08",1,-15.379390000000001,"Out = Keilor to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-20T20:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-174.24879999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-20T21:10:00","I_CTRL_ISSUE_ML","I-CTRL_ISSUE_ML","2012-12-21",1,-223.13928999999999,"DC Link Control Issue Constraint for Murraylink","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-11-21T01:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-07-25",1,-14.376289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-22T10:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-147.7236,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-22T13:50:00","V>>N-CNUT_HB_15M","N-CNUT_01","2016-07-01",1,-64.24539,"Out = Upper Tumut -Canberra(01), avoid O/L Murray to Lower Tumut (66) on trip of Murray to Upper Tumut (65) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-23T02:30:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-10.06127,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-23T11:35:00","V>>N-CNUT_HB_15M","N-CNUT_01","2016-07-01",1,-41.18694,"Out = Upper Tumut -Canberra(01), avoid O/L Murray to Lower Tumut (66) on trip of Murray to Upper Tumut (65) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-23T22:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-16.717359999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-23T23:40:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-11.59863,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-24T00:30:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-37.03293,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-24T03:15:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-11.53304,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-24T04:05:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-23.630980000000001,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-24T22:15:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-40.053750000000001,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T00:25:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-32.166809999999998,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T01:50:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-20.55556,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T03:25:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-21.668990000000001,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T05:50:00","V::N_X_MLSM_EMTT_V2","V-X_MLSM_EMTT_KTS_P;V-X_MLSM_EMTT_KTS_R;V-X_MLSM_EMTT_P;V-X_MLSM_EMTT_R","2016-11-17",1,-30.92417,"Out = one Moorabool to Sydenham to South Morang 500kV line, EMTT scheme O/S, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T16:30:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-35.782919999999997,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T19:30:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-14.57658,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-25T22:40:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-20.92848,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T00:30:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-16.358260000000001,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T03:20:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-11.98152,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T07:25:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-10.797599999999999,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T09:00:00","V::N_HYSE_V2","I-HYSE","2016-11-21",1,-37.119160000000001,"Out = Heywood to South East 275kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T10:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.821539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T11:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-21.573149999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T13:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-41.430929999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T14:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.757429999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T16:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.911580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T18:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.575669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T20:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.443860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-26T22:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.870560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T00:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.61469,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T01:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.84028,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T04:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.400930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T11:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-16.412849999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T12:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.306950000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T15:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-22.688459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T16:40:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-171.60668999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-27T22:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.330939999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-28T01:10:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLEL","2012-07-04",1,-15.08723,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-28T03:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.60811,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-28T04:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.920739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-30T00:45:00","V::N_X_2SVC_V4","NULL","2016-11-24",1,-45.341450000000002,"Out = 2 SVCs at Rowville or South East, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-30T01:45:00","V::N_X_2SVC_V4","NULL","2016-11-24",1,-31.576779999999999,"Out = 2 SVCs at Rowville or South East, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-30T04:00:00","V::N_X_2SVC_V4","NULL","2016-11-24",1,-46.964910000000003,"Out = 2 SVCs at Rowville or South East, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-11-30T04:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-40.512259999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T00:35:00","F_S++ML_R6_1","F-SA_ISLE","2013-11-21",1,7762.06981,"Raise 6 sec Service Requirement for SA Generation Event, where Murraylink (Vic to SA transfer) is the largest generation risk in SA, Segment 1","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-01T01:35:00","F_S++ML_R6_1","F-SA_ISLE","2013-11-21",1,8880.4370999999992,"Raise 6 sec Service Requirement for SA Generation Event, where Murraylink (Vic to SA transfer) is the largest generation risk in SA, Segment 1","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-01T02:45:00","F_S++ML_R6_1","F-SA_ISLE","2013-11-21",1,976.60626000000002,"Raise 6 sec Service Requirement for SA Generation Event, where Murraylink (Vic to SA transfer) is the largest generation risk in SA, Segment 1","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-01T03:00:00","V::N_HYMO_V2","V-HYMO","2016-11-07",1,-34.116300000000003,"Out = Heywood to Mortlake (HYTS-MOPS) No.2 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T04:05:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-35.825699999999998,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T05:10:00","V::N_HYTR_Q4","V-HYTR","2016-11-24",1,-41.307569999999998,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T08:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-148.71736000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T10:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-1804132.5275900001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T14:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-11.720879999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T18:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-141.71655000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T21:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-14.40578,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-01T22:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.85981,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T00:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.784559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T02:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-38.804659999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T03:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-38.150390000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T03:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.822139999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T12:35:00","V::N_X_MLSM_EMTT_S2","V-X_MLSM_EMTT_KTS_P;V-X_MLSM_EMTT_KTS_R;V-X_MLSM_EMTT_P;V-X_MLSM_EMTT_R;V-X_MLSM_STAB","2016-11-17",1,-33.381349999999998,"Out = one Moorabool to Sydenham to South Morang 500kV line, EMTT scheme O/S, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T17:00:00","V::N_X_MLSM_EMTT_SD","V-X_MLSM_EMTT_KTS_P;V-X_MLSM_EMTT_KTS_R;V-X_MLSM_EMTT_P;V-X_MLSM_EMTT_R;V-X_MLSM_STAB","2016-11-17",1,-26.371970000000001,"Out = one Moorabool to Sydenham to South Morang 500kV line, EMTT scheme O/S, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T22:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-53.255299999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-02T23:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.43731,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T01:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.67679,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T03:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.108220000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T04:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.60716,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T05:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.173740000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T10:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.514140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T12:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-49.901400000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T12:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-47.37135,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T14:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.678649999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T16:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-41.698720000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-34.502020000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-12.4887,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-03T20:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.763629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-04T01:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-16.598230000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-04T03:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.94584,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-04T04:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-41.919170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-04T09:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-180.42160000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-04T20:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.314550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T00:50:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-822.33559000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T03:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.698630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T04:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.01455,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T05:10:00","#R014973_017_RAMP_V","#R014973_RAMP","2016-12-04",1,-20.23217,"Soft Ramping constraint for constraint V>>SML_ARWB_5, Effective Date: 24/08/2016, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-12-05T06:25:00","V::N_BAHO_V4","V-ARBA;V-ARHO;V-BAHO;V-BAWA;V-HOWA;V-X_BAHO","2016-11-24",1,-120.64532,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T07:00:00","V::N_BAHO_V4","V-ARBA;V-ARHO;V-BAHO;V-BAWA;V-HOWA;V-X_BAHO","2016-11-24",1,-283.74997000000002,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T10:00:00","V::N_BAHO_V4","V-ARBA;V-ARHO;V-BAHO;V-BAWA;V-HOWA;V-X_BAHO","2016-11-24",1,-125.52229,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T10:35:00","V::N_BAHO_V4","V-ARBA;V-ARHO;V-BAHO;V-BAWA;V-HOWA;V-X_BAHO","2016-11-24",1,-71.183679999999995,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T12:10:00","V::N_BAHO_V4","V-ARBA;V-ARHO;V-BAHO;V-BAWA;V-HOWA;V-X_BAHO","2016-11-24",1,-72.343580000000003,"Out = Ballarat to Waubra to Horsham 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T17:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-43.938040000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T20:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-55.355789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T22:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.80781,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-05T23:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.448459999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-06T00:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-43.200119999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-06T02:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-43.904269999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-06T03:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.542679999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-06T04:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.881129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-06T08:30:00","#R014980_016_RAMP_F","#R014980_RAMP","2016-12-05",1,-47.477690000000003,"Hard Ramping constraint for constraint V::N_JNWO_SD, Effective Date: 02/12/2016, Version: 1","SYSTEM NORMAL","RAMP",null,null,null,null,null,0]
[null,null,"2016-12-07T01:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-10.625500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-07T04:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-43.777610000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-07T22:35:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-22.658339999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-07T23:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.772290000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-08T01:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.8765,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-08T14:55:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-10.147080000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-08T17:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.934670000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T00:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.200890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T07:25:00","V>SMLHORC2","V-HORC;V-HORC_P;V-HORC_R","2015-08-13",1,-28.5611,"Out = Horsham to Redcliffs 220kV line, avoid overloading Bendigo to Kerang 220kV line for trip of Balranald to Darlington Point (X5/1) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T12:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.64358,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T14:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.166450000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T15:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.124890000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T19:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.68355,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-09T22:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-16.726430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T01:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.26751,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T01:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.535360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T03:00:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-44.014620000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T08:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-11.24968,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T10:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-10.904540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T11:30:00","V::N_KGRC_S2","V-KGRC","2016-12-02",1,-14.143269999999999,"Out = Kerang to Red Cliffs 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T13:55:00","V::N_KGRC_V2","V-KGRC","2016-12-02",1,-19.572189999999999,"Out = Kerang to Red Cliffs 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T14:25:00","V::N_KGRC_V2","V-KGRC","2016-12-02",1,-25.007259999999999,"Out = Kerang to Red Cliffs 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T16:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.98471,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T16:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.996690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T18:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.012329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T19:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-21.137060000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T21:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.456700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-10T22:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.755990000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.809699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T02:45:00","V::N_HWSM_S1","V-HWCB4;V-HWRO3;V-HWSM","2016-11-28",1,-16.25507,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T08:20:00","V::N_HWSM_S1","V-HWCB4;V-HWRO3;V-HWSM","2016-11-28",1,-23.548839999999998,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T08:45:00","V::N_HWSM_S1","V-HWCB4;V-HWRO3;V-HWSM","2016-11-28",1,-25.92313,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T10:20:00","V::N_HWSM_S1","V-HWCB4;V-HWRO3;V-HWSM","2016-11-28",1,-35.84881,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T11:20:00","V::N_HWSM_S1","V-HWCB4;V-HWRO3;V-HWSM","2016-11-28",1,-40.378590000000003,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T12:25:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-61.659669999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T12:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.700659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T14:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.299700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T15:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.155200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T16:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.00938,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T18:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.928129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T18:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.78354,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T20:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.182020000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T22:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.155569999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-11T22:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.009070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T05:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.11219,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T08:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-21.803249999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T11:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-38.61656,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T15:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-26.75929,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T17:15:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-176.37511000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T19:10:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-185.92077,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T20:55:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-44.08,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T21:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-23.22505,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-12T23:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.412680000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-13T05:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.06574,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-13T07:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.77572,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-13T18:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-28.060690000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-13T22:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.664580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T00:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-21.278510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T02:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.96261,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T03:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.802910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T06:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.158670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T07:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.839110000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T08:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.19444,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T08:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.455869999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T09:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.837240000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T11:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.32573,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.10337,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.289149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T18:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.1111,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T20:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.421720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T21:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.2821,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T22:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.488530000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-14T23:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.22513,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T01:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.42712,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T03:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-16.215399999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T05:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-14.30165,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T18:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-25.53941,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T20:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.859030000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T22:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.316510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-15T23:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.277049999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T03:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.28697,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T07:35:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-22.425740000000001,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T08:35:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-22.049759999999999,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T10:00:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-30.433890000000002,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T10:50:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-30.454709999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T11:50:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-32.812269999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T12:40:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-39.339660000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T13:35:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-59.13702,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T14:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-52.937840000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T14:55:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-156.84014999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T15:25:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-177.13643999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T16:30:00","V>>V_CBTS_TX_2A_R","V-CBTX_R","2016-11-21",1,-19.06362,"Out = Cranbourne A1 500/220kV txfmr, avoid pre-contingent O/L South Morang F2 500/330 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T18:10:00","V>>V_CBTS_TX_2A_R","V-CBTX_R","2016-11-21",1,-12.242900000000001,"Out = Cranbourne A1 500/220kV txfmr, avoid pre-contingent O/L South Morang F2 500/330 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-17T21:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.861459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T00:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.41526,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.55114,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T04:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.727309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T05:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.801449999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T06:45:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-16.98742,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T08:25:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-12.63588,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T10:30:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-10.392329999999999,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T14:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.60101,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T18:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-27.924569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-18T18:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-28.48424,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T00:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.94103,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T02:25:00","V>>V_CBTS_TX_2A_R","V-CBTX_R","2016-11-21",1,-15.28792,"Out = Cranbourne A1 500/220kV txfmr, avoid pre-contingent O/L South Morang F2 500/330 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T03:10:00","V>>V_CBTS_TX_2A_R","V-CBTX_R","2016-11-21",1,-12.498609999999999,"Out = Cranbourne A1 500/220kV txfmr, avoid pre-contingent O/L South Morang F2 500/330 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T05:05:00","V>>V_CBTS_TX_2A_R","V-CBTX_R","2016-11-21",1,-16.439630000000001,"Out = Cranbourne A1 500/220kV txfmr, avoid pre-contingent O/L South Morang F2 500/330 kV txfmr, radial mode, Yallourn W1 on 500 kV, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T19:15:00","S>>NIL_RBTU_WEWT","S-NIL","2016-11-21",1,-14.086130000000001,"Out= Nil, avoid O/L Waterloo East-Waterloo 132kV line on trip of Robertstown-Tungkillo 275kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-19T22:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.80978,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T02:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-13111.721,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-12-20T04:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.762799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T06:40:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-37.848799999999997,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","INCLUDED",null,"UNPLANNED",1]
[null,null,"2016-12-20T07:35:00","V::N_KTSY_MLSM_ET_V2","V-KTSY_MLSM_ET_KTS_P;V-KTSY_MLSM_ET_KTS_R;V-X_KTSY_MLSM_EMTT_P;V-X_KTSY_MLSM_EMTT_R;V-X_KTSY_MLSM_P;V-X_KTSY_MLSM_R","2016-11-17",1,-26.45064,"Out = Keilor to Sydenham & Moorabool to Sydenham to South Morang 500kV line, EMTT scheme O/S, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T08:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-31.298940000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T09:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-28.881509999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T11:20:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-38.488669999999999,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.26624,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.90056,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T15:40:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-10.8,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T18:05:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-24.920179999999998,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T18:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-19.740189999999998,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T19:55:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-23.10632,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T20:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-16.019369999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T21:10:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-13.970330000000001,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T22:00:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-19.8,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-20T23:50:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-34.30977,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T00:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-19.25432,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T01:35:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-20.255299999999998,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T01:50:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-26.210899999999999,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T04:05:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-26.75187,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T04:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-23.660299999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T05:30:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-18.95946,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T06:20:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-41.164650000000002,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T07:50:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-23.79935,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T08:15:00","V::N_SMSC_V4","V-SMSC","2016-11-24",1,-23.65737,"Out = 1 x South Morang Series Capacitor 330kV, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T09:50:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-20.006150000000002,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T11:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-18.54091,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T12:10:00","V::N_DDSM_V2","V-DDSM;V-X_DDMB_DDSM;V-X_DDSM_DDH1;V-X_DDSM_DDH2;V-X_EPMB_DDSM","2016-12-16",1,-64.82226,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T12:50:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-48.095179999999999,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T14:35:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-47.012920000000001,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T15:50:00","V>>V_DDSM_1","V-DDSM","2016-10-12",1,-72.57978,"Out= Dederang to South Morang 330kV line, avoid O/L Ballarat to Bendigo 220kV line on trip of the remaining South Morang to Dederang 330kV line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T17:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.37682,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T17:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.31091,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T19:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.452529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-21T22:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.40696,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T00:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.590769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T00:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.519410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T02:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.7928,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T04:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.304970000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T07:20:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-23.398849999999999,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T08:15:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-24.058509999999998,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T10:45:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-14.29013,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T11:30:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-205.11834999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T12:20:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-20.7818,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T12:35:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-18.661639999999998,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T13:25:00","V::N_HYTR_V4","V-HYTR","2016-11-24",1,-19.107289999999999,"Out = Heywood to Tarrone (HYTS-TRTS) No. 1 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T15:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-51.573830000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T16:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-46.478099999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T16:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-43.985720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T18:00:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-74.567920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T18:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-27.0502,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T19:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-13.753349999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T19:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.146160000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-22T20:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-11.729570000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T01:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.53764,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T04:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.769600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.861969999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T15:20:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-14.200279999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T19:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.48292,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T19:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.834400000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T21:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.151700000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-23T22:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-40.637360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.871659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T02:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.65099,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T05:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.44575,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T06:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.071439999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T08:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.265909999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T09:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.940460000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T10:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.442679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T12:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.480879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T15:40:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-197.60002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T16:35:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-37.362650000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-24T21:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.688210000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-25T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.45468,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-25T08:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.295960000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-25T08:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.940329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-25T13:25:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-19.519950000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-25T14:30:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-16.622129999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-25T18:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-246.77289999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-25T21:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.043959999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T12:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.024470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T13:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.523260000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T14:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.983359999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T15:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.558409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T18:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.022279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T19:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.999880000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T20:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.939170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T21:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-16.248180000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-26T23:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-16.733070000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T00:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.06893,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T07:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.03384,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T09:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-42.633339999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T10:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.335760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T11:20:00","S>V_NIL_NIL_RBNW","S-NIL;S-NIL_RBNW","2016-09-13",1,-10.73368,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T13:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.900230000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-20.797059999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T16:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-18.61618,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T17:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-18.91198,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T18:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.66986,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T20:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.70834,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T20:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-23.470300000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T21:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.606829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-27T23:45:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-383.74036999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T00:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-15.647080000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T01:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.707319999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T05:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.32321,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T06:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-29.505949999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T07:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-14.62994,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T09:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-14.898770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T10:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-16.732749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T12:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-18.135840000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-18.60989,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-28T23:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.22251,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-29T03:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.76666,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-29T07:05:00","V^SML_NSWRB_2","@HWPS_20090217;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-ML_VFRB;V-NIL;V-NIL_PARALLEL...","2016-07-07",1,-30.98967,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T00:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.513590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T01:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.91741,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T02:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.206430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T04:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.477129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.725519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.44436,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.139109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.0036,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.4704,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T06:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.076090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.58817,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.16371,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.46841,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.154780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.1637,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T07:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.53464,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.4306,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.984310000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43092,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.4306,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.4306,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.31175,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.316780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.305340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T08:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.84545,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.23358,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.466390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.866589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.11304,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.640840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.16367,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.430720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.842879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T09:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.454419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.663340000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.43018,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:15:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-10.03356,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.4918,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:20:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-16.64781,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.43018,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.43064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T10:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.29313,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T11:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.344279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T11:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.45115,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T11:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.045680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T11:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.50582,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.452,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.45205,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.482150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.82734,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.44946,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-13.53444,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T12:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.446730000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.44717,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.47946,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-14.704280000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.756880000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.45248,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.615600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.38382,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.867839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.85304,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T13:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.85585,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.867380000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-15.00088,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-18.9878,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.508699999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-15.70852,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.72584,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.141120000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-10.73695,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.1427,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.82282,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-16.873380000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.015919999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-32.995840000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.08634,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-33.405290000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-141.13237000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-31.30987,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-37.994039999999998,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-168.07971000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T14:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-30.308720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-17.143329999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-13.63795,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.89828,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-23.234200000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.93008,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:15:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-12.799149999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-60.775480000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-19.846769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.72894,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-133.93024,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-19.233560000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:25:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.13439,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:25:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-146.29560000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-16.18572,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-23.87378,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:30:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-176.32584,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:30:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-25.26643,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.22414,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:35:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-14.068250000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-21.578620000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:40:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-22.874890000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.90283,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:45:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-27.287299999999998,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.6492,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-24.13073,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:50:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-132.31601000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-27.476179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-37.420160000000003,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:55:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-132.75512000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T15:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-35.852719999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:00:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-32.26238,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-15.789400000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-89.973089999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.889290000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-15.039440000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:15:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-30.204689999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:15:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-131.57261,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:15:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-32.460630000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:20:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-28.990670000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.48038,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.37209,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-13.726330000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T16:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.192019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:00:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-28.447109999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.300330000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.762169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:25:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.698090000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.433,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.356159999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.303879999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-11.429399999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T17:55:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.05589,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.28365,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.35549,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:05:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-46.010640000000002,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.27947,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:10:00","V>>N-NIL_HA","N-NIL;N-NIL_H_15M","2016-07-01",1,-13.385540000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.53237,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.456440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.456440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.873620000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.873669999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.873620000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-15.80002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.006790000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.46392,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T18:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.117570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.313469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.09346,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.796419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-21.07978,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.128820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.903469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.81222,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.6419,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.701460000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.061959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.872229999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.01005,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T19:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.289819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.238390000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.688949999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-36.178939999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-36.650979999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-36.371899999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-37.192810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-37.414299999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-40.31306,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-40.32882,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-41.425579999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-41.402819999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T20:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-39.518169999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-39.007089999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.637999999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.328759999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.205220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-31.201339999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-32.443199999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-36.892130000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-38.20346,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.907510000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-35.127920000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-35.147120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T21:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-31.4999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-28.314340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-266.03451000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-38.353029999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-44.078440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-42.793729999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.098990000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.81307,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.859819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.899340000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.849910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.503409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.833449999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T22:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.852620000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.847380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.839019999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.733420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.872719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.729050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.947510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.800840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.93085,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.528759999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.754629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.039729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-30T23:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.003070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.878060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.014690000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.722369999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.284559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-35.076619999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.551600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.308579999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:30:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-20.52872,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T00:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.27957,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:35:00","VSML_220","@HWPS_20090217;I-VSML_220;PASA_NIL;V+NIL_PARALLEL_3-5;V+NIL_PARALLEL_6-2;V+NIL_PAR_3-5;V+NIL_PAR_3-5_BL;V+NIL_PAR_6-2;V+NIL_PAR_6-2_BL;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL;V-NIL_PARALLE...","2012-07-04",1,-20.548729999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.926519999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:40:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-20.79025,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T00:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.933340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:45:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-20.78566,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T00:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.152670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:50:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-21.320060000000002,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T00:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.65649,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T00:55:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-16.798719999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T01:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.210279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:00:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-16.419699999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T01:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.27216,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:05:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-15.047549999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[null,null,"2016-12-31T01:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.408719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.2308,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.838049999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.369520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.659940000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.13513,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.998570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T01:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.370660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.651969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.345829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-12.93266,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.62959,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.269410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.15081,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.14068,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.013369999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.553570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.533469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.322179999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T02:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.1632,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.147279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.023980000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.009840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.697949999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.39667,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.394259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.68318,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.685220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.684999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.669879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.377269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T03:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.812259999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.38354,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.14639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.792649999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.792300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.967790000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.797450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.947719999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.53068,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.127939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.254390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.15024,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T04:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.488890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.110019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.775320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-43.344160000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.48724,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-41.535739999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.517769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.345230000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.665870000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.334119999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.337029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.300059999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T05:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.927389999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.616099999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.11806,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.296479999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.140039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.134370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.77938,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.76699,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.495039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.264600000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.563870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.101939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T06:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.293289999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.33671,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.437999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-22.392859999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.35566,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.903379999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.734299999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.489190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.492930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.700320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-33.198509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.568999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T07:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.316680000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-27.453869999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.293959999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.978450000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-45.063299999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-45.086889999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-45.096490000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-45.096809999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.882869999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.83379,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.368409999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-38.080860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T08:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.596339999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.343789999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-55.574210000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-55.962569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-54.161000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-57.91733,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-40.465330000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-40.411499999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.982340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-40.461959999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-38.936880000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-48.81671,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T09:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.598260000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.598640000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.576920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.574060000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.593389999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.68665,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.055100000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-38.729730000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.95928,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.561570000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.141800000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.783550000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T10:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.936590000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.092170000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.113419999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.332999999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-38.452939999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.039000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.393389999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-38.435670000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.722070000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-37.946620000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.200900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.638669999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T11:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.635469999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.617109999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-43.173789999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-39.070610000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.617060000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-40.795659999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-46.685099999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-57.232880000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-63.887799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-46.078539999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-67.689779999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-35.120780000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T12:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-44.10333,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.816549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.424670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.698969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-20.700890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-21.9696,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.229430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.218910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T13:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-18.783380000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-12.760529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:10:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.624389999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:20:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-17.099689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.54655,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:35:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.79715,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:40:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.82109,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:45:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-14.70696,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:50:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.657629999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T14:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.350950000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.517440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:05:00","V>>V_NIL_2A_R","@HWPS_20090217;V+NIL_RADIAL;V+NIL_RADIAL_1-2;V+NIL_RADIAL_1-2_BL;V+NIL_RADIAL_3-4;V+NIL_RADIAL_BL;V-HW_BUS2_RADIAL;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_1-2_BL;V-NIL_RADIAL_3-4;V-NIL_RADIAL_BL;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BU...","2016-06-21",1,-10.04289,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.939109999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.788260000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.14817,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.488800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-10.86665,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-52.97945,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-52.861159999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.607890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.988350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T15:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.964379999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.969909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.681529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-16.590019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-13.931609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.38833,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.13344,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.326930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.8154,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.36135,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.725200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.51895,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T16:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.512319999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.558150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.419,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.582949999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.39254,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:20:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.688459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.380890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:30:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.102139999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:35:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.340389999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.448090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:45:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.217939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:50:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.306699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T17:55:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.974820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.025559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:05:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.96725,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.025289999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:15:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.02092,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.779910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:25:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.938220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.6509,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-70.764330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:40:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-44.335160000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-35.012230000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.99118,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T18:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.433250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:00:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-22.270630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.86472,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:10:00","V::N_NIL_S2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-18.147549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Basslink TAS to VIC. Yallourn W Unit 1 on 500 kV. Limit only applied during Heywood flow from SA to VIC","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.136600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.074849999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.790600000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.311340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.303280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.293280000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.546779999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.617330000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T19:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.97634,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-32.384180000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.757349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.242989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.810289999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-28.944769999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-34.166020000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-26.028320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.27224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-33.874360000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.97418,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.087150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T20:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-22.965630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.73536,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-31.031739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.128769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.56625,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.525770000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.962,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.061869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.062860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.81588,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.08053,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-24.804760000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T21:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.252199999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-25.073029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.644279999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-30.096679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-36.381790000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:20:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.2942,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:25:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.926359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:30:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.935279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:35:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.679320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:40:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-29.33287,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:45:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.822700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:50:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.813510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T22:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-19.065629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T23:00:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-23.32743,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T23:05:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.100110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T23:10:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-17.151520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T23:15:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-11.594239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2016-12-31T23:55:00","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-15.15132,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[null,null,"2017-01-01","V::N_NIL_V2","V-NIL;V-NIL_PAR_3-5;V-NIL_RADIAL;V-NIL_RADIAL_1-2;V-NIL_RADIAL_1-2_3-4;V-NIL_RADIAL_3-4;V-NIL_RAD_HW3-BUS1;V-NIL_RAD_HW4-BUS1;V-NIL_RAD_HWJL2OUT","2016-11-24",1,-14.97907,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]