{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Schema","Setup","Instructions","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":124,"n_cols":1,"rows_kept":124,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|9|(8\\([a-f]\\))|(99)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"SP AUSNET\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:positiveInteger\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_code\" type=\"extype\" xdb:SQLName=\"EXCLUSION_CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["DIRECTLINK",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"Instructions!$O$10 & \"V\" & TEXT(Instructions!$O$11,\"#\") & \"_\" &TEXT(Instructions!$O$17,\"YYYYMMDDHHMMSS\")","v":"TRANSGRIDV4_20140403131324"},"AERMIC_VER2",{"$f":"INFO(\"RELEASE\")","v":"12.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["ELECTRANET",3,"CATEGORY","DESCRIPTION"]
["MURRAYLINK",4,"ASSET CLASS","EQUIPMENTNAME"]
["POWERLINK",null,null,"EXCLUSION_DETAIL"]
["SP AUSNET",null,null,"TNSP_COMMENT"]
["TRANSEND"]
["TRANSGRID"]

{"sheet":"Instructions","index":2,"n_rows":67,"n_cols":15,"rows_kept":67,"cut":false,"hidden":false,"merged":[[57,6,57,22],[46,6,46,22],[47,6,47,22],[48,6,48,22],[49,6,49,22],[50,6,50,22],[56,6,56,22],[51,6,51,22],[52,6,52,22],[53,6,53,22],[54,6,54,22],[55,6,55,22],[64,6,64,22],[69,5,69,22],[58,6,58,22],[59,6,59,22],[60,6,60,22],[61,6,61,22],[62,6,62,22],[63,6,63,22],[45,6,45,22],[10,11,10,13],[40,6,40,22],[41,6,41,22],[42,6,42,22],[43,6,43,22],[11,11,11,13],[16,11,16,13],[34,6,34,22],[44,6,44,22],[35,6,35,22],[36,6,36,22],[37,6,37,22],[38,6,38,22],[39,6,39,22],[8,10,8,15],[0,5,0,22],[7,5,7,22],[33,6,33,22],[21,5,21,22],[22,5,22,22],[23,5,23,22],[24,5,24,22],[26,5,26,22],[29,6,29,22],[30,6,30,22],[31,6,31,22],[32,6,32,22],[13,11,13,13],[14,11,14,13],[9,11,9,13]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Market Impact Parameter Data Template"]
[null,null,null,null,null,null,null,null,null,null,"Please complete these details prior to data validation"]
[null,null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"TRANSGRID"]
[null,null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,4]
[null,null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2012]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,{"$f":"SUM(Data!$O:$O)","v":737}]
[null,null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"COUNTIFS(Data!$M$2:$M$1048576,\"<>99\",Data!$M$2:$M$1048576,\"<>\")","v":70}]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Last successful validation ",null,null,"2014-04-03T13:13:24"]
[]
[]
[]
[]
[null,null,null,null,null,"TEMPLATE INSTRUCTIONS"]
[null,null,null,null,null,"TNSP must provide performance data in this workbook in the Data tab. The data submitted must conform to the data field requirements detailed below and must be validated prior to the data being submitted to the AER for assessment. If the data does not conform to the field requirements set out below then the data will not be able to be validated. TNSP is able to provide additional tabs in the workbook for the AER reference.  "]
[null,null,null,null,null,"Please provide ALL binding constraints with a marginal cost greater than $10 and is used to manage TNSP's network. The data is submitted on a 5 minute resolution and  sourced from the MCC_Constraintsolution table (MCC table).   The TNSP is able to enter the exclusion clause number in the 'EXCLUSION CODE' field. Please use the code '99' for non-inclusion dispatch intervals."]
[null,null,null,null,null,"NOTE: All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and with no exclusion clause, will be used to calculate the TNSP's performance measure. "]
[]
[null,null,null,null,null,"When all data has been recorded in the Data tab, click the 'Validate Data' button to validate the data and resolve any issues prior to submission. If data is unable to be validated then an error message will appear indicating the row/s which need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,"Description of fields:"]
[null,null,null,null,null,"Settlementdate ","Settlement date/time of the binding network constraint as detailed in the MCC_Constraintsolution table (MCC table) published in the AEMO Market Management System"]
[null,null,null,null,null,"Constraint ID","Constraint identifier as detailed in the MCC table"]
[null,null,null,null,null,"Effective date","Effective date of the relevant binding network constraint, for the relevant settlement date/time"]
[null,null,null,null,null,"Version number","Version number of the relevant binding network constraint, for the relevant settlement date/time"]
[null,null,null,null,null,"Marginal value","Marginal value (up to 5 decimal places)* of the relevant binding network constraint, for the relevant settlement date time"]
[null,null,null,null,null,"Constraint description","Description of the binding network constraint "]
[null,null,null,null,null,"Network condition","Classification of the network constraint as \"System Normal\" or \"Outage\" constraint"]
[null,null,null,null,null,"Category","Additional categorisation of the network constraint as one of (note: this field cannot be empty):"]
[null,null,null,null,null,null,"NRM (negative residues management) "]
[null,null,null,null,null,null,"NSA (network support agreement)  - must have an associated exclusion code value of 7"]
[null,null,null,null,null,null,"RAMP( ramping constraint) - must have an associated weighting value of 0"]
[null,null,null,null,null,null,"FCAS (frequency control constraint)"]
[null,null,null,null,null,null,"RECLASS (reclassification) - must have an associated exclusion code value of 2"]
[null,null,null,null,null,null,"NC (non-conformance)"]
[null,null,null,null,null,null,"DIRECTION (AEMO direction)"]
[null,null,null,null,null,null,"MII (manifestly incorrect input) - must have an associated exclusion code value of 8(a)"]
[null,null,null,null,null,null,"OTHER (none of the above)"]
[null,null,null,null,null,"Outage equipment ","The equipment that the constraint is used to manage"]
[null,null,null,null,null,"Asset class","Identify whether the equipment is either a regulated asset or non-regulated asset (accepted values: Regulated | Non-Regulated). If the outage is related to non-regulated assets, TNSP must enter exclusion code 4.  If the equipment is in a adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) "]
[null,null,null,null,null,"Exclusion code ","Provide the relevant exclusion code under version 2, 3 or 4 of the scheme in the specified format. Valid exclusion codes are: "]
[null,null,null,null,null,null,"1 to 7"]
[null,null,null,null,null,null,"8(a)"]
[null,null,null,null,null,null,"8(b)"]
[null,null,null,null,null,null,"8(c) "]
[null,null,null,null,null,null,"8(d)"]
[null,null,null,null,null,null,"8(e)"]
[null,null,null,null,null,null,"8(f)"]
[null,null,null,null,null,null,"9 (only valid in version 4)"]
[null,null,null,null,null,null,"99(non-inclusion)"]
[null,null,null,null,null,"Exclusion detail","Free text for TNSP to provide details on the exclusion claim (i.e reference to supportive evidence, or outage details)"]
[null,null,null,null,null,"Weighting ","The following values are valid for weighting:"]
[null,null,null,null,null,null,"1 (the count is wholly attributed to TNSP)"]
[null,null,null,null,null,null,"0.5 (the count is shared with one other TNSP)"]
[null,null,null,null,null,null,"0.33 (count is shared with two other TNSPs)"]
[null,null,null,null,null,null," 0 (not included in the performance count)"]
[null,null,null,null,null,"TNSP comment ","Provide any further information that will assist the AER in its assessment of the TNSP data"]
[]
[null,null,null,null,null,"*This is to ensure consistency with the MCC table"]

{"sheet":"Data","index":3,"n_rows":1632,"n_cols":16,"rows_kept":1632,"cut":false,"hidden":false,"merged":[]}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","EXCLUSION CODE","EXCLUSION DETAIL","WEIGHTING","TNSP COMMENT"]
[1,"TRANSGRIDV4_19000100000000","2012-02-04T01:05:00","#BW04_E","2012-02-03",2,-1024.5038300000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[2,"TRANSGRIDV4_19000100000000","2012-02-04T01:10:00","#BW04_E","2012-02-03",2,-1024.51368,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[3,"TRANSGRIDV4_19000100000000","2012-02-04T01:15:00","#BW04_E","2012-02-03",2,-1024.32375,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[4,"TRANSGRIDV4_19000100000000","2012-02-04T01:20:00","#BW04_E","2012-02-03",2,-1024.32367,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[5,"TRANSGRIDV4_19000100000000","2012-02-04T01:25:00","#BW04_E","2012-02-03",2,-1023.80362,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[6,"TRANSGRIDV4_19000100000000","2012-02-04T01:30:00","#BW04_E","2012-02-03",2,-1020.21906,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[7,"TRANSGRIDV4_19000100000000","2012-02-04T01:35:00","#BW04_E","2012-02-03",2,-1024.5038300000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[8,"TRANSGRIDV4_19000100000000","2012-02-04T01:40:00","#BW04_E","2012-02-03",2,-1024.5038300000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[9,"TRANSGRIDV4_19000100000000","2012-02-04T01:45:00","#BW04_E","2012-02-03",2,-1024.3236199999999,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[10,"TRANSGRIDV4_19000100000000","2012-02-04T01:50:00","#BW04_E","2012-02-03",2,-1024.3238899999999,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[11,"TRANSGRIDV4_19000100000000","2012-02-04T02:00:00","#BW04_E","2012-02-03",2,-1021.75452,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[12,"TRANSGRIDV4_19000100000000","2012-02-04T02:05:00","#BW04_E","2012-02-03",2,-1019.97759,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[13,"TRANSGRIDV4_19000100000000","2012-02-04T02:10:00","#BW04_E","2012-02-03",2,-1018.62354,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[14,"TRANSGRIDV4_19000100000000","2012-02-04T02:20:00","#BW04_E","2012-02-03",2,-1018.1640200000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[15,"TRANSGRIDV4_19000100000000","2012-02-04T02:30:00","#BW04_E","2012-02-03",2,-1018.1640200000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[16,"TRANSGRIDV4_19000100000000","2012-02-04T02:35:00","#BW04_E","2012-02-03",2,-1024.32368,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[17,"TRANSGRIDV4_19000100000000","2012-02-04T02:40:00","#BW04_E","2012-02-03",2,-1019.07363,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[18,"TRANSGRIDV4_19000100000000","2012-02-04T02:45:00","#BW04_E","2012-02-03",2,-1018.30404,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[19,"TRANSGRIDV4_19000100000000","2012-02-04T02:50:00","#BW04_E","2012-02-03",2,-1018.16381,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[20,"TRANSGRIDV4_19000100000000","2012-02-04T02:55:00","#BW04_E","2012-02-03",2,-1018.1638,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[21,"TRANSGRIDV4_19000100000000","2012-02-04T03:05:00","#BW04_E","2012-02-03",2,-1018.16381,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[22,"TRANSGRIDV4_19000100000000","2012-02-04T03:10:00","#BW04_E","2012-02-03",2,-1018.1640200000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[23,"TRANSGRIDV4_19000100000000","2012-02-04T03:20:00","#BW04_E","2012-02-03",2,-1016.75207,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[24,"TRANSGRIDV4_19000100000000","2012-02-04T03:25:00","#BW04_E","2012-02-03",2,-1018.16366,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[25,"TRANSGRIDV4_19000100000000","2012-02-04T03:30:00","#BW04_E","2012-02-03",2,-1016.9064,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[26,"TRANSGRIDV4_19000100000000","2012-02-04T03:35:00","#BW04_E","2012-02-03",2,-1018.09426,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[27,"TRANSGRIDV4_19000100000000","2012-02-04T03:50:00","#BW04_E","2012-02-03",2,-1018.1638,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[28,"TRANSGRIDV4_19000100000000","2012-02-04T03:55:00","#BW04_E","2012-02-03",2,-1017.06816,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[29,"TRANSGRIDV4_19000100000000","2012-02-04T04:00:00","#BW04_E","2012-02-03",2,-1018.4008700000001,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[30,"TRANSGRIDV4_19000100000000","2012-02-04T04:05:00","#BW04_E","2012-02-03",2,-1018.16354,"NBAY4.ENERGY * 1 <= 0 (Wt = 20)","OUTAGE","DIRECTION","","REGULATED","8(a)","Transducer error at Baysater generator caused this constraint to be incorrectly invoked",0]
[31,"TRANSGRIDV4_19000100000000","2012-10-03T20:40:00","#MACARTH1_E","2012-10-02",1,-1033.0723,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[32,"TRANSGRIDV4_19000100000000","2012-10-03T20:45:00","#MACARTH1_E","2012-10-02",1,-1033.0420799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[33,"TRANSGRIDV4_19000100000000","2012-10-03T20:50:00","#MACARTH1_E","2012-10-02",1,-1032.3012799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[34,"TRANSGRIDV4_19000100000000","2012-10-03T20:55:00","#MACARTH1_E","2012-10-02",1,-1032.30826,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[35,"TRANSGRIDV4_19000100000000","2012-10-03T21:00:00","#MACARTH1_E","2012-10-02",1,-1031.7301399999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[36,"TRANSGRIDV4_19000100000000","2012-10-03T21:05:00","#MACARTH1_E","2012-10-02",1,-1033.19559,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[37,"TRANSGRIDV4_19000100000000","2012-10-03T21:45:00","#MACARTH1_E","2012-10-02",1,-1031.72,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[38,"TRANSGRIDV4_19000100000000","2012-10-03T21:50:00","#MACARTH1_E","2012-10-02",1,-1031.7300600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[39,"TRANSGRIDV4_19000100000000","2012-10-03T21:55:00","#MACARTH1_E","2012-10-02",1,-1031.7300600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[40,"TRANSGRIDV4_19000100000000","2012-10-03T22:00:00","#MACARTH1_E","2012-10-02",1,-1031.7300600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[41,"TRANSGRIDV4_19000100000000","2012-10-03T22:05:00","#MACARTH1_E","2012-10-02",1,-1038.3349499999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[42,"TRANSGRIDV4_19000100000000","2012-10-03T22:10:00","#MACARTH1_E","2012-10-02",1,-1034.1914999999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[43,"TRANSGRIDV4_19000100000000","2012-10-03T22:15:00","#MACARTH1_E","2012-10-02",1,-1032.4346800000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[44,"TRANSGRIDV4_19000100000000","2012-10-03T22:20:00","#MACARTH1_E","2012-10-02",1,-1031.73027,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[45,"TRANSGRIDV4_19000100000000","2012-10-03T22:25:00","#MACARTH1_E","2012-10-02",1,-1031.7301199999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[46,"TRANSGRIDV4_19000100000000","2012-10-03T22:30:00","#MACARTH1_E","2012-10-02",1,-1031.7300399999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[47,"TRANSGRIDV4_19000100000000","2012-10-03T22:35:00","#MACARTH1_E","2012-10-02",1,-1031.92039,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[48,"TRANSGRIDV4_19000100000000","2012-10-03T22:40:00","#MACARTH1_E","2012-10-02",1,-1031.8897999999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[49,"TRANSGRIDV4_19000100000000","2012-10-03T22:45:00","#MACARTH1_E","2012-10-02",1,-1031.7302,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[50,"TRANSGRIDV4_19000100000000","2012-10-03T22:50:00","#MACARTH1_E","2012-10-02",1,-1031.90445,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[51,"TRANSGRIDV4_19000100000000","2012-10-03T22:55:00","#MACARTH1_E","2012-10-02",1,-1031.7301199999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[52,"TRANSGRIDV4_19000100000000","2012-10-03T23:00:00","#MACARTH1_E","2012-10-02",1,-1031.7302,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[53,"TRANSGRIDV4_19000100000000","2012-10-03T23:05:00","#MACARTH1_E","2012-10-02",1,-1042.07005,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[54,"TRANSGRIDV4_19000100000000","2012-10-03T23:10:00","#MACARTH1_E","2012-10-02",1,-1040.07,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[55,"TRANSGRIDV4_19000100000000","2012-10-03T23:15:00","#MACARTH1_E","2012-10-02",1,-1035.0081700000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[56,"TRANSGRIDV4_19000100000000","2012-10-03T23:20:00","#MACARTH1_E","2012-10-02",1,-1033.2572,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[57,"TRANSGRIDV4_19000100000000","2012-10-03T23:25:00","#MACARTH1_E","2012-10-02",1,-1032.69517,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[58,"TRANSGRIDV4_19000100000000","2012-10-03T23:30:00","#MACARTH1_E","2012-10-02",1,-1032.7821100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[59,"TRANSGRIDV4_19000100000000","2012-10-03T23:35:00","#MACARTH1_E","2012-10-02",1,-1042.51088,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[60,"TRANSGRIDV4_19000100000000","2012-10-03T23:40:00","#MACARTH1_E","2012-10-02",1,-1033.6922500000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[61,"TRANSGRIDV4_19000100000000","2012-10-03T23:45:00","#MACARTH1_E","2012-10-02",1,-1033.2813799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[62,"TRANSGRIDV4_19000100000000","2012-10-03T23:50:00","#MACARTH1_E","2012-10-02",1,-1031.7298499999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[63,"TRANSGRIDV4_19000100000000","2012-10-03T23:55:00","#MACARTH1_E","2012-10-02",1,-1031.71983,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[64,"TRANSGRIDV4_19000100000000","2012-10-04","#MACARTH1_E","2012-10-02",1,-1031.72,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[65,"TRANSGRIDV4_19000100000000","2012-10-04T00:05:00","#MACARTH1_E","2012-10-02",1,-1030.9523899999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[66,"TRANSGRIDV4_19000100000000","2012-10-04T00:10:00","#MACARTH1_E","2012-10-02",1,-1030.19804,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[67,"TRANSGRIDV4_19000100000000","2012-10-04T00:15:00","#MACARTH1_E","2012-10-02",1,-1027.9924100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[68,"TRANSGRIDV4_19000100000000","2012-10-04T00:20:00","#MACARTH1_E","2012-10-02",1,-1027.12716,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[69,"TRANSGRIDV4_19000100000000","2012-10-04T00:25:00","#MACARTH1_E","2012-10-02",1,-1026.5336,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[70,"TRANSGRIDV4_19000100000000","2012-10-04T00:30:00","#MACARTH1_E","2012-10-02",1,-1026.9163000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[71,"TRANSGRIDV4_19000100000000","2012-10-04T00:35:00","#MACARTH1_E","2012-10-02",1,-1022.96001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[72,"TRANSGRIDV4_19000100000000","2012-10-04T00:40:00","#MACARTH1_E","2012-10-02",1,-1027.5730599999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[73,"TRANSGRIDV4_19000100000000","2012-10-04T00:45:00","#MACARTH1_E","2012-10-02",1,-1022.96007,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[74,"TRANSGRIDV4_19000100000000","2012-10-04T00:50:00","#MACARTH1_E","2012-10-02",1,-1022.47113,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[75,"TRANSGRIDV4_19000100000000","2012-10-04T00:55:00","#MACARTH1_E","2012-10-02",1,-1022.88582,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[76,"TRANSGRIDV4_19000100000000","2012-10-04T01:00:00","#MACARTH1_E","2012-10-02",1,-1026.6994999999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[77,"TRANSGRIDV4_19000100000000","2012-10-04T01:05:00","#MACARTH1_E","2012-10-02",1,-1026.9081699999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[78,"TRANSGRIDV4_19000100000000","2012-10-04T01:10:00","#MACARTH1_E","2012-10-02",1,-1027.16688,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[79,"TRANSGRIDV4_19000100000000","2012-10-04T01:15:00","#MACARTH1_E","2012-10-02",1,-1022.95984,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[80,"TRANSGRIDV4_19000100000000","2012-10-04T01:20:00","#MACARTH1_E","2012-10-02",1,-1022.68693,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[81,"TRANSGRIDV4_19000100000000","2012-10-04T01:25:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[82,"TRANSGRIDV4_19000100000000","2012-10-04T01:30:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[83,"TRANSGRIDV4_19000100000000","2012-10-04T01:35:00","#MACARTH1_E","2012-10-02",1,-1022.95984,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[84,"TRANSGRIDV4_19000100000000","2012-10-04T01:40:00","#MACARTH1_E","2012-10-02",1,-1022.96,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[85,"TRANSGRIDV4_19000100000000","2012-10-04T01:45:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[86,"TRANSGRIDV4_19000100000000","2012-10-04T01:50:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[87,"TRANSGRIDV4_19000100000000","2012-10-04T01:55:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[88,"TRANSGRIDV4_19000100000000","2012-10-04T02:00:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[89,"TRANSGRIDV4_19000100000000","2012-10-04T02:05:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[90,"TRANSGRIDV4_19000100000000","2012-10-04T02:10:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[91,"TRANSGRIDV4_19000100000000","2012-10-04T02:15:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[92,"TRANSGRIDV4_19000100000000","2012-10-04T02:20:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[93,"TRANSGRIDV4_19000100000000","2012-10-04T02:25:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[94,"TRANSGRIDV4_19000100000000","2012-10-04T02:30:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[95,"TRANSGRIDV4_19000100000000","2012-10-04T02:35:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[96,"TRANSGRIDV4_19000100000000","2012-10-04T02:40:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[97,"TRANSGRIDV4_19000100000000","2012-10-04T02:45:00","#MACARTH1_E","2012-10-02",1,-1021.73979,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[98,"TRANSGRIDV4_19000100000000","2012-10-04T02:50:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[99,"TRANSGRIDV4_19000100000000","2012-10-04T02:55:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[100,"TRANSGRIDV4_19000100000000","2012-10-04T03:00:00","#MACARTH1_E","2012-10-02",1,-1021.63568,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[101,"TRANSGRIDV4_19000100000000","2012-10-04T03:05:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[102,"TRANSGRIDV4_19000100000000","2012-10-04T03:10:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[103,"TRANSGRIDV4_19000100000000","2012-10-04T03:15:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[104,"TRANSGRIDV4_19000100000000","2012-10-04T03:20:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[105,"TRANSGRIDV4_19000100000000","2012-10-04T03:25:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[106,"TRANSGRIDV4_19000100000000","2012-10-04T03:30:00","#MACARTH1_E","2012-10-02",1,-1009.26707,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[107,"TRANSGRIDV4_19000100000000","2012-10-04T03:35:00","#MACARTH1_E","2012-10-02",1,-1017.43173,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[108,"TRANSGRIDV4_19000100000000","2012-10-04T03:40:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[109,"TRANSGRIDV4_19000100000000","2012-10-04T03:45:00","#MACARTH1_E","2012-10-02",1,-1020.5,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[110,"TRANSGRIDV4_19000100000000","2012-10-04T03:50:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[111,"TRANSGRIDV4_19000100000000","2012-10-04T03:55:00","#MACARTH1_E","2012-10-02",1,-1017.75,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[112,"TRANSGRIDV4_19000100000000","2012-10-04T04:00:00","#MACARTH1_E","2012-10-02",1,-1008.90458,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[113,"TRANSGRIDV4_19000100000000","2012-10-04T04:05:00","#MACARTH1_E","2012-10-02",1,-1008.19762,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[114,"TRANSGRIDV4_19000100000000","2012-10-04T04:10:00","#MACARTH1_E","2012-10-02",1,-1008.34677,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[115,"TRANSGRIDV4_19000100000000","2012-10-04T04:15:00","#MACARTH1_E","2012-10-02",1,-1008.5641900000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[116,"TRANSGRIDV4_19000100000000","2012-10-04T04:20:00","#MACARTH1_E","2012-10-02",1,-1008.55917,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[117,"TRANSGRIDV4_19000100000000","2012-10-04T04:25:00","#MACARTH1_E","2012-10-02",1,-1008.56811,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[118,"TRANSGRIDV4_19000100000000","2012-10-04T04:30:00","#MACARTH1_E","2012-10-02",1,-1008.36069,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[119,"TRANSGRIDV4_19000100000000","2012-10-04T04:35:00","#MACARTH1_E","2012-10-02",1,-1008.3680000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[120,"TRANSGRIDV4_19000100000000","2012-10-04T04:40:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[121,"TRANSGRIDV4_19000100000000","2012-10-04T04:45:00","#MACARTH1_E","2012-10-02",1,-1020.03759,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[122,"TRANSGRIDV4_19000100000000","2012-10-04T04:50:00","#MACARTH1_E","2012-10-02",1,-1021.74021,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[123,"TRANSGRIDV4_19000100000000","2012-10-04T04:55:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[124,"TRANSGRIDV4_19000100000000","2012-10-04T05:00:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[125,"TRANSGRIDV4_19000100000000","2012-10-04T05:05:00","#MACARTH1_E","2012-10-02",1,-1022.95994,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[126,"TRANSGRIDV4_19000100000000","2012-10-04T05:10:00","#MACARTH1_E","2012-10-02",1,-1021.79791,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[127,"TRANSGRIDV4_19000100000000","2012-10-04T05:15:00","#MACARTH1_E","2012-10-02",1,-1027.5934299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[128,"TRANSGRIDV4_19000100000000","2012-10-04T05:20:00","#MACARTH1_E","2012-10-02",1,-1028.1166499999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[129,"TRANSGRIDV4_19000100000000","2012-10-04T05:25:00","#MACARTH1_E","2012-10-02",1,-1027.6288500000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[130,"TRANSGRIDV4_19000100000000","2012-10-04T05:30:00","#MACARTH1_E","2012-10-02",1,-1028.2268099999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[131,"TRANSGRIDV4_19000100000000","2012-10-04T05:35:00","#MACARTH1_E","2012-10-02",1,-1022.95986,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[132,"TRANSGRIDV4_19000100000000","2012-10-04T05:40:00","#MACARTH1_E","2012-10-02",1,-1024.1881000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[133,"TRANSGRIDV4_19000100000000","2012-10-04T05:45:00","#MACARTH1_E","2012-10-02",1,-1023.26832,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[134,"TRANSGRIDV4_19000100000000","2012-10-04T05:50:00","#MACARTH1_E","2012-10-02",1,-1022.56727,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[135,"TRANSGRIDV4_19000100000000","2012-10-04T05:55:00","#MACARTH1_E","2012-10-02",1,-1022.77001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[136,"TRANSGRIDV4_19000100000000","2012-10-04T06:00:00","#MACARTH1_E","2012-10-02",1,-1022.91976,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[137,"TRANSGRIDV4_19000100000000","2012-10-04T06:05:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[138,"TRANSGRIDV4_19000100000000","2012-10-04T06:10:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[139,"TRANSGRIDV4_19000100000000","2012-10-04T06:15:00","#MACARTH1_E","2012-10-02",1,-1022.69457,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[140,"TRANSGRIDV4_19000100000000","2012-10-04T06:20:00","#MACARTH1_E","2012-10-02",1,-1022.95991,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[141,"TRANSGRIDV4_19000100000000","2012-10-04T06:25:00","#MACARTH1_E","2012-10-02",1,-1022.96014,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[142,"TRANSGRIDV4_19000100000000","2012-10-04T06:30:00","#MACARTH1_E","2012-10-02",1,-1022.96013,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[143,"TRANSGRIDV4_19000100000000","2012-10-04T06:35:00","#MACARTH1_E","2012-10-02",1,-1021.73958,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[144,"TRANSGRIDV4_19000100000000","2012-10-04T06:40:00","#MACARTH1_E","2012-10-02",1,-1021.73,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[145,"TRANSGRIDV4_19000100000000","2012-10-04T06:45:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[146,"TRANSGRIDV4_19000100000000","2012-10-04T06:50:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[147,"TRANSGRIDV4_19000100000000","2012-10-04T06:55:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[148,"TRANSGRIDV4_19000100000000","2012-10-04T07:00:00","#MACARTH1_E","2012-10-02",1,-1023.1727,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[149,"TRANSGRIDV4_19000100000000","2012-10-04T07:05:00","#MACARTH1_E","2012-10-02",1,-1021.74,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[150,"TRANSGRIDV4_19000100000000","2012-10-04T07:10:00","#MACARTH1_E","2012-10-02",1,-1022.96016,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[151,"TRANSGRIDV4_19000100000000","2012-10-04T07:15:00","#MACARTH1_E","2012-10-02",1,-1023.07707,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[152,"TRANSGRIDV4_19000100000000","2012-10-04T07:20:00","#MACARTH1_E","2012-10-02",1,-1025.64402,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[153,"TRANSGRIDV4_19000100000000","2012-10-04T07:25:00","#MACARTH1_E","2012-10-02",1,-1023.07707,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[154,"TRANSGRIDV4_19000100000000","2012-10-04T07:30:00","#MACARTH1_E","2012-10-02",1,-1031.7163,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[155,"TRANSGRIDV4_19000100000000","2012-10-04T07:35:00","#MACARTH1_E","2012-10-02",1,-1026.8667600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[156,"TRANSGRIDV4_19000100000000","2012-10-04T07:40:00","#MACARTH1_E","2012-10-02",1,-1032.0939900000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[157,"TRANSGRIDV4_19000100000000","2012-10-04T07:45:00","#MACARTH1_E","2012-10-02",1,-1032.4935700000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[158,"TRANSGRIDV4_19000100000000","2012-10-04T07:50:00","#MACARTH1_E","2012-10-02",1,-1032.5700200000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[159,"TRANSGRIDV4_19000100000000","2012-10-04T07:55:00","#MACARTH1_E","2012-10-02",1,-1033.26659,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[160,"TRANSGRIDV4_19000100000000","2012-10-04T08:00:00","#MACARTH1_E","2012-10-02",1,-1033.68462,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[161,"TRANSGRIDV4_19000100000000","2012-10-04T08:05:00","#MACARTH1_E","2012-10-02",1,-1033.2745600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[162,"TRANSGRIDV4_19000100000000","2012-10-04T08:10:00","#MACARTH1_E","2012-10-02",1,-1033.70921,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[163,"TRANSGRIDV4_19000100000000","2012-10-04T08:15:00","#MACARTH1_E","2012-10-02",1,-1033.95912,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[164,"TRANSGRIDV4_19000100000000","2012-10-04T08:20:00","#MACARTH1_E","2012-10-02",1,-1034.8828100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[165,"TRANSGRIDV4_19000100000000","2012-10-04T08:25:00","#MACARTH1_E","2012-10-02",1,-1034.4936399999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[166,"TRANSGRIDV4_19000100000000","2012-10-04T08:30:00","#MACARTH1_E","2012-10-02",1,-1034.8750299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[167,"TRANSGRIDV4_19000100000000","2012-10-04T08:35:00","#MACARTH1_E","2012-10-02",1,-1032.57,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[168,"TRANSGRIDV4_19000100000000","2012-10-04T08:40:00","#MACARTH1_E","2012-10-02",1,-1032.57,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[169,"TRANSGRIDV4_19000100000000","2012-10-04T08:45:00","#MACARTH1_E","2012-10-02",1,-1032.57,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[170,"TRANSGRIDV4_19000100000000","2012-10-04T08:50:00","#MACARTH1_E","2012-10-02",1,-1032.5798299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[171,"TRANSGRIDV4_19000100000000","2012-10-04T08:55:00","#MACARTH1_E","2012-10-02",1,-1032.5802699999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[172,"TRANSGRIDV4_19000100000000","2012-10-04T09:00:00","#MACARTH1_E","2012-10-02",1,-1033.7156299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[173,"TRANSGRIDV4_19000100000000","2012-10-04T09:05:00","#MACARTH1_E","2012-10-02",1,-1033.44084,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[174,"TRANSGRIDV4_19000100000000","2012-10-04T09:10:00","#MACARTH1_E","2012-10-02",1,-1033.6953599999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[175,"TRANSGRIDV4_19000100000000","2012-10-04T09:15:00","#MACARTH1_E","2012-10-02",1,-1034.59205,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[176,"TRANSGRIDV4_19000100000000","2012-10-04T09:20:00","#MACARTH1_E","2012-10-02",1,-1033.7652499999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[177,"TRANSGRIDV4_19000100000000","2012-10-04T09:25:00","#MACARTH1_E","2012-10-02",1,-1033.3775700000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[178,"TRANSGRIDV4_19000100000000","2012-10-04T09:30:00","#MACARTH1_E","2012-10-02",1,-1033.3979899999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[179,"TRANSGRIDV4_19000100000000","2012-10-04T09:35:00","#MACARTH1_E","2012-10-02",1,-1033.4129,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[180,"TRANSGRIDV4_19000100000000","2012-10-04T09:40:00","#MACARTH1_E","2012-10-02",1,-1033.0205800000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[181,"TRANSGRIDV4_19000100000000","2012-10-04T09:45:00","#MACARTH1_E","2012-10-02",1,-1033.04072,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[182,"TRANSGRIDV4_19000100000000","2012-10-04T09:50:00","#MACARTH1_E","2012-10-02",1,-1033.5882799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[183,"TRANSGRIDV4_19000100000000","2012-10-04T09:55:00","#MACARTH1_E","2012-10-02",1,-1033.57394,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[184,"TRANSGRIDV4_19000100000000","2012-10-04T10:00:00","#MACARTH1_E","2012-10-02",1,-1033.15689,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[185,"TRANSGRIDV4_19000100000000","2012-10-04T10:05:00","#MACARTH1_E","2012-10-02",1,-1032.6625799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[186,"TRANSGRIDV4_19000100000000","2012-10-04T10:10:00","#MACARTH1_E","2012-10-02",1,-1032.76729,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[187,"TRANSGRIDV4_19000100000000","2012-10-04T10:15:00","#MACARTH1_E","2012-10-02",1,-1032.7868000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[188,"TRANSGRIDV4_19000100000000","2012-10-04T10:20:00","#MACARTH1_E","2012-10-02",1,-1032.7976900000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[189,"TRANSGRIDV4_19000100000000","2012-10-04T10:25:00","#MACARTH1_E","2012-10-02",1,-1032.7847300000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[190,"TRANSGRIDV4_19000100000000","2012-10-04T10:30:00","#MACARTH1_E","2012-10-02",1,-1032.7963299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[191,"TRANSGRIDV4_19000100000000","2012-10-04T10:35:00","#MACARTH1_E","2012-10-02",1,-1032.5802000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[192,"TRANSGRIDV4_19000100000000","2012-10-04T10:40:00","#MACARTH1_E","2012-10-02",1,-1032.7832800000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[193,"TRANSGRIDV4_19000100000000","2012-10-04T10:45:00","#MACARTH1_E","2012-10-02",1,-1032.5798299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[194,"TRANSGRIDV4_19000100000000","2012-10-04T10:50:00","#MACARTH1_E","2012-10-02",1,-1032.5798299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[195,"TRANSGRIDV4_19000100000000","2012-10-04T10:55:00","#MACARTH1_E","2012-10-02",1,-1032.5801200000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[196,"TRANSGRIDV4_19000100000000","2012-10-04T11:00:00","#MACARTH1_E","2012-10-02",1,-1032.6088299999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[197,"TRANSGRIDV4_19000100000000","2012-10-04T11:05:00","#MACARTH1_E","2012-10-02",1,-1034.1375700000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[198,"TRANSGRIDV4_19000100000000","2012-10-04T11:10:00","#MACARTH1_E","2012-10-02",1,-1033.19238,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[199,"TRANSGRIDV4_19000100000000","2012-10-04T11:15:00","#MACARTH1_E","2012-10-02",1,-1033.17248,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[200,"TRANSGRIDV4_19000100000000","2012-10-04T11:20:00","#MACARTH1_E","2012-10-02",1,-1034.6592499999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[201,"TRANSGRIDV4_19000100000000","2012-10-04T11:25:00","#MACARTH1_E","2012-10-02",1,-1035.1147100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[202,"TRANSGRIDV4_19000100000000","2012-10-04T11:30:00","#MACARTH1_E","2012-10-02",1,-1035.08986,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[203,"TRANSGRIDV4_19000100000000","2012-10-04T11:35:00","#MACARTH1_E","2012-10-02",1,-1034.8833999999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[204,"TRANSGRIDV4_19000100000000","2012-10-04T11:40:00","#MACARTH1_E","2012-10-02",1,-1034.6509900000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[205,"TRANSGRIDV4_19000100000000","2012-10-04T11:45:00","#MACARTH1_E","2012-10-02",1,-1035.5802100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[206,"TRANSGRIDV4_19000100000000","2012-10-04T11:50:00","#MACARTH1_E","2012-10-02",1,-1035.7515000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[207,"TRANSGRIDV4_19000100000000","2012-10-04T11:55:00","#MACARTH1_E","2012-10-02",1,-1036.04982,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[208,"TRANSGRIDV4_19000100000000","2012-10-04T12:00:00","#MACARTH1_E","2012-10-02",1,-1035.3451399999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[209,"TRANSGRIDV4_19000100000000","2012-10-04T12:05:00","#MACARTH1_E","2012-10-02",1,-1034.9180200000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[210,"TRANSGRIDV4_19000100000000","2012-10-04T12:10:00","#MACARTH1_E","2012-10-02",1,-1034.65002,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[211,"TRANSGRIDV4_19000100000000","2012-10-04T12:15:00","#MACARTH1_E","2012-10-02",1,-1034.4169099999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[212,"TRANSGRIDV4_19000100000000","2012-10-04T12:20:00","#MACARTH1_E","2012-10-02",1,-1036.1908699999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[213,"TRANSGRIDV4_19000100000000","2012-10-04T12:25:00","#MACARTH1_E","2012-10-02",1,-1033.5812900000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[214,"TRANSGRIDV4_19000100000000","2012-10-04T12:30:00","#MACARTH1_E","2012-10-02",1,-1033.9052799999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[215,"TRANSGRIDV4_19000100000000","2012-10-04T12:35:00","#MACARTH1_E","2012-10-02",1,-1033.9198100000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[216,"TRANSGRIDV4_19000100000000","2012-10-04T12:40:00","#MACARTH1_E","2012-10-02",1,-1033.90753,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[217,"TRANSGRIDV4_19000100000000","2012-10-04T12:45:00","#MACARTH1_E","2012-10-02",1,-1034.50513,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[218,"TRANSGRIDV4_19000100000000","2012-10-04T12:50:00","#MACARTH1_E","2012-10-02",1,-1036.2924599999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[219,"TRANSGRIDV4_19000100000000","2012-10-04T12:55:00","#MACARTH1_E","2012-10-02",1,-1036.50305,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[220,"TRANSGRIDV4_19000100000000","2012-10-04T13:00:00","#MACARTH1_E","2012-10-02",1,-1035.70804,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[221,"TRANSGRIDV4_19000100000000","2012-10-04T13:05:00","#MACARTH1_E","2012-10-02",1,-1036.2617399999999,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[222,"TRANSGRIDV4_19000100000000","2012-10-04T13:10:00","#MACARTH1_E","2012-10-02",1,-1037.3427200000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[223,"TRANSGRIDV4_19000100000000","2012-10-04T13:15:00","#MACARTH1_E","2012-10-02",1,-1040.73587,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[224,"TRANSGRIDV4_19000100000000","2012-10-04T13:20:00","#MACARTH1_E","2012-10-02",1,-1040.6424,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[225,"TRANSGRIDV4_19000100000000","2012-10-04T13:25:00","#MACARTH1_E","2012-10-02",1,-1040.70551,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[226,"TRANSGRIDV4_19000100000000","2012-10-04T13:30:00","#MACARTH1_E","2012-10-02",1,-1039.9164000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[227,"TRANSGRIDV4_19000100000000","2012-10-04T13:35:00","#MACARTH1_E","2012-10-02",1,-1039.1920600000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[228,"TRANSGRIDV4_19000100000000","2012-10-04T13:40:00","#MACARTH1_E","2012-10-02",1,-1038.4614200000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[229,"TRANSGRIDV4_19000100000000","2012-10-04T13:45:00","#MACARTH1_E","2012-10-02",1,-1039.4245000000001,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[230,"TRANSGRIDV4_19000100000000","2012-10-04T13:50:00","#MACARTH1_E","2012-10-02",1,-1039.67975,"VTRT1M.ENERGY * 1 <= 168 (Wt = 360)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[231,"TRANSGRIDV4_19000100000000","2012-01-09T09:00:00","#N-Q-MNSP1_I_E","2012-01-09",1,11.409739999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[232,"TRANSGRIDV4_19000100000000","2012-01-09T09:05:00","#N-Q-MNSP1_I_E","2012-01-09",1,10.212020000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[233,"TRANSGRIDV4_19000100000000","2012-01-09T09:10:00","#N-Q-MNSP1_I_E","2012-01-09",1,10.220370000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[234,"TRANSGRIDV4_19000100000000","2012-01-09T09:35:00","#N-Q-MNSP1_I_E","2012-01-09",1,37.689639999999997,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[235,"TRANSGRIDV4_19000100000000","2012-01-09T09:40:00","#N-Q-MNSP1_I_E","2012-01-09",1,38.225279999999998,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[236,"TRANSGRIDV4_19000100000000","2012-01-09T09:50:00","#N-Q-MNSP1_I_E","2012-01-09",1,12.019869999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[237,"TRANSGRIDV4_19000100000000","2012-01-09T09:55:00","#N-Q-MNSP1_I_E","2012-01-09",1,38.7498,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[238,"TRANSGRIDV4_19000100000000","2012-01-09T10:00:00","#N-Q-MNSP1_I_E","2012-01-09",1,38.571710000000003,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[239,"TRANSGRIDV4_19000100000000","2012-01-09T10:05:00","#N-Q-MNSP1_I_E","2012-01-09",1,12.554349999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[240,"TRANSGRIDV4_19000100000000","2012-01-09T10:10:00","#N-Q-MNSP1_I_E","2012-01-09",1,12.3596,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[241,"TRANSGRIDV4_19000100000000","2012-01-09T10:15:00","#N-Q-MNSP1_I_E","2012-01-09",1,11.98208,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[242,"TRANSGRIDV4_19000100000000","2012-01-09T10:20:00","#N-Q-MNSP1_I_E","2012-01-09",1,38.99597,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[243,"TRANSGRIDV4_19000100000000","2012-01-09T10:25:00","#N-Q-MNSP1_I_E","2012-01-09",1,38.849679999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[244,"TRANSGRIDV4_19000100000000","2012-01-09T10:30:00","#N-Q-MNSP1_I_E","2012-01-09",1,40.720080000000003,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[245,"TRANSGRIDV4_19000100000000","2012-01-09T10:35:00","#N-Q-MNSP1_I_E","2012-01-09",1,189.18993,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[246,"TRANSGRIDV4_19000100000000","2012-01-09T10:40:00","#N-Q-MNSP1_I_E","2012-01-09",1,40.726129999999998,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[247,"TRANSGRIDV4_19000100000000","2012-01-09T10:45:00","#N-Q-MNSP1_I_E","2012-01-09",1,40.694029999999998,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[248,"TRANSGRIDV4_19000100000000","2012-01-09T10:50:00","#N-Q-MNSP1_I_E","2012-01-09",1,176.78852000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[249,"TRANSGRIDV4_19000100000000","2012-01-09T10:55:00","#N-Q-MNSP1_I_E","2012-01-09",1,176.75202999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[250,"TRANSGRIDV4_19000100000000","2012-01-09T11:00:00","#N-Q-MNSP1_I_E","2012-01-09",1,179.27914999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[251,"TRANSGRIDV4_19000100000000","2012-01-09T11:05:00","#N-Q-MNSP1_I_E","2012-01-09",1,41.227269999999997,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[252,"TRANSGRIDV4_19000100000000","2012-01-09T11:10:00","#N-Q-MNSP1_I_E","2012-01-09",1,40.786760000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[253,"TRANSGRIDV4_19000100000000","2012-01-09T11:15:00","#N-Q-MNSP1_I_E","2012-01-09",1,39.840229999999998,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[254,"TRANSGRIDV4_19000100000000","2012-01-09T11:20:00","#N-Q-MNSP1_I_E","2012-01-09",1,176.10051000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[255,"TRANSGRIDV4_19000100000000","2012-01-09T11:25:00","#N-Q-MNSP1_I_E","2012-01-09",1,163.99811,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[256,"TRANSGRIDV4_19000100000000","2012-01-09T11:30:00","#N-Q-MNSP1_I_E","2012-01-09",1,1513.8738499999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[257,"TRANSGRIDV4_19000100000000","2012-01-09T11:35:00","#N-Q-MNSP1_I_E","2012-01-09",1,199.45875000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[258,"TRANSGRIDV4_19000100000000","2012-01-09T11:40:00","#N-Q-MNSP1_I_E","2012-01-09",1,46.21611,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[259,"TRANSGRIDV4_19000100000000","2012-01-09T11:45:00","#N-Q-MNSP1_I_E","2012-01-09",1,164.07113000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[260,"TRANSGRIDV4_19000100000000","2012-01-09T11:50:00","#N-Q-MNSP1_I_E","2012-01-09",1,67.105729999999994,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[261,"TRANSGRIDV4_19000100000000","2012-01-09T11:55:00","#N-Q-MNSP1_I_E","2012-01-09",1,65.964200000000005,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[262,"TRANSGRIDV4_19000100000000","2012-01-09T12:00:00","#N-Q-MNSP1_I_E","2012-01-09",1,65.948509999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[263,"TRANSGRIDV4_19000100000000","2012-01-09T12:05:00","#N-Q-MNSP1_I_E","2012-01-09",1,65.799210000000002,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[264,"TRANSGRIDV4_19000100000000","2012-01-09T12:10:00","#N-Q-MNSP1_I_E","2012-01-09",1,44.796379999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[265,"TRANSGRIDV4_19000100000000","2012-01-09T12:15:00","#N-Q-MNSP1_I_E","2012-01-09",1,66.710080000000005,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[266,"TRANSGRIDV4_19000100000000","2012-01-09T12:20:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.19529,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[267,"TRANSGRIDV4_19000100000000","2012-01-09T12:25:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.73802000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[268,"TRANSGRIDV4_19000100000000","2012-01-09T12:30:00","#N-Q-MNSP1_I_E","2012-01-09",1,1511.70524,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[269,"TRANSGRIDV4_19000100000000","2012-01-09T12:35:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.72676000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[270,"TRANSGRIDV4_19000100000000","2012-01-09T12:40:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.65880999999999,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[271,"TRANSGRIDV4_19000100000000","2012-01-09T12:45:00","#N-Q-MNSP1_I_E","2012-01-09",1,45.883719999999997,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[272,"TRANSGRIDV4_19000100000000","2012-01-09T12:50:00","#N-Q-MNSP1_I_E","2012-01-09",1,46.196759999999998,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[273,"TRANSGRIDV4_19000100000000","2012-01-09T12:55:00","#N-Q-MNSP1_I_E","2012-01-09",1,45.618870000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[274,"TRANSGRIDV4_19000100000000","2012-01-09T13:00:00","#N-Q-MNSP1_I_E","2012-01-09",1,67.611850000000004,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[275,"TRANSGRIDV4_19000100000000","2012-01-09T13:05:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.47054,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[276,"TRANSGRIDV4_19000100000000","2012-01-09T13:10:00","#N-Q-MNSP1_I_E","2012-01-09",1,90.892390000000006,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[277,"TRANSGRIDV4_19000100000000","2012-01-09T13:15:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.99975000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[278,"TRANSGRIDV4_19000100000000","2012-01-09T13:20:00","#N-Q-MNSP1_I_E","2012-01-09",1,170.66371000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[279,"TRANSGRIDV4_19000100000000","2012-01-09T13:25:00","#N-Q-MNSP1_I_E","2012-01-09",1,83.449470000000005,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[280,"TRANSGRIDV4_19000100000000","2012-01-09T13:30:00","#N-Q-MNSP1_I_E","2012-01-09",1,169.95553000000001,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[281,"TRANSGRIDV4_19000100000000","2012-01-09T14:15:00","#N-Q-MNSP1_I_E","2012-01-09",2,47.48995,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[282,"TRANSGRIDV4_19000100000000","2012-01-09T14:20:00","#N-Q-MNSP1_I_E","2012-01-09",2,48.424680000000002,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[283,"TRANSGRIDV4_19000100000000","2012-01-09T14:25:00","#N-Q-MNSP1_I_E","2012-01-09",2,48.09751,"N-Q-MNSP1. * -1 <= 105 (Wt = 20)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[284,"TRANSGRIDV4_19000100000000","2012-01-12T15:15:00","#NSW1_E_20120112","2012-01-12",1,-18.63663,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[285,"TRANSGRIDV4_19000100000000","2012-01-12T15:20:00","#NSW1_E_20120112","2012-01-12",2,-21.5426,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[286,"TRANSGRIDV4_19000100000000","2012-01-12T15:25:00","#NSW1_E_20120112","2012-01-12",3,-128.1028,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[287,"TRANSGRIDV4_19000100000000","2012-01-12T15:30:00","#NSW1_E_20120112","2012-01-12",3,-22.60473,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[288,"TRANSGRIDV4_19000100000000","2012-01-12T15:35:00","#NSW1_E_20120112","2012-01-12",4,-41.936579999999999,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[289,"TRANSGRIDV4_19000100000000","2012-01-12T15:40:00","#NSW1_E_20120112","2012-01-12",5,-11.46734,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[290,"TRANSGRIDV4_19000100000000","2012-01-12T15:45:00","#NSW1_E_20120112","2012-01-12",6,-48.595350000000003,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[291,"TRANSGRIDV4_19000100000000","2012-01-12T15:50:00","#NSW1_E_20120112","2012-01-12",6,-135.29432,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[292,"TRANSGRIDV4_19000100000000","2012-01-12T15:55:00","#NSW1_E_20120112","2012-01-12",6,-400.64161999999999,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[293,"TRANSGRIDV4_19000100000000","2012-01-12T16:00:00","#NSW1_E_20120112","2012-01-12",7,-32.3399,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[294,"TRANSGRIDV4_19000100000000","2012-01-12T16:05:00","#NSW1_E_20120112","2012-01-12",7,-24.27093,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[295,"TRANSGRIDV4_19000100000000","2012-01-12T16:10:00","#NSW1_E_20120112","2012-01-12",7,-18.53227,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[296,"TRANSGRIDV4_19000100000000","2012-01-12T16:15:00","#NSW1_E_20120112","2012-01-12",8,-19.87913,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[297,"TRANSGRIDV4_19000100000000","2012-01-12T16:25:00","#NSW1_E_20120112","2012-01-12",9,-14.69656,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[298,"TRANSGRIDV4_19000100000000","2012-01-27T12:25:00","#NSW1_E_20120127","2012-01-27",1,-607.51774,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[299,"TRANSGRIDV4_19000100000000","2012-01-27T12:30:00","#NSW1_E_20120127","2012-01-27",1,-582.51405999999997,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[300,"TRANSGRIDV4_19000100000000","2012-01-27T12:55:00","#NSW1_E_20120127","2012-01-27",2,-18.970330000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[301,"TRANSGRIDV4_19000100000000","2012-01-27T13:00:00","#NSW1_E_20120127","2012-01-27",3,-29.08663,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[302,"TRANSGRIDV4_19000100000000","2012-01-27T13:05:00","#NSW1_E_20120127","2012-01-27",4,-89.572159999999997,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[303,"TRANSGRIDV4_19000100000000","2012-01-27T13:10:00","#NSW1_E_20120127","2012-01-27",5,-1011.52918,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[304,"TRANSGRIDV4_19000100000000","2012-01-27T13:15:00","#NSW1_E_20120127","2012-01-27",6,-86.079669999999993,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[305,"TRANSGRIDV4_19000100000000","2012-01-27T13:20:00","#NSW1_E_20120127","2012-01-27",6,-17.81766,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[306,"TRANSGRIDV4_19000100000000","2012-01-27T13:25:00","#NSW1_E_20120127","2012-01-27",7,-88.596279999999993,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[307,"TRANSGRIDV4_19000100000000","2012-01-27T13:30:00","#NSW1_E_20120127","2012-01-27",7,-46.254179999999998,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[308,"TRANSGRIDV4_19000100000000","2012-01-27T13:40:00","#NSW1_E_20120127","2012-01-27",8,-38.912570000000002,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[309,"TRANSGRIDV4_19000100000000","2012-01-27T13:45:00","#NSW1_E_20120127","2012-01-27",8,-906.13738000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[310,"TRANSGRIDV4_19000100000000","2012-01-27T13:50:00","#NSW1_E_20120127","2012-01-27",8,-921.66372000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[311,"TRANSGRIDV4_19000100000000","2012-01-27T13:55:00","#NSW1_E_20120127","2012-01-27",8,-137.20788999999999,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[312,"TRANSGRIDV4_19000100000000","2012-01-27T14:00:00","#NSW1_E_20120127","2012-01-27",8,-586.59379000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[313,"TRANSGRIDV4_19000100000000","2012-01-27T14:15:00","#NSW1_E_20120127","2012-01-27",10,-1042.5548799999999,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[314,"TRANSGRIDV4_19000100000000","2012-01-27T14:20:00","#NSW1_E_20120127","2012-01-27",10,-588.22394999999995,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[315,"TRANSGRIDV4_19000100000000","2012-01-27T14:25:00","#NSW1_E_20120127","2012-01-27",11,-24.221889999999998,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[316,"TRANSGRIDV4_19000100000000","2012-01-27T14:30:00","#NSW1_E_20120127","2012-01-27",11,-10.70349,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[317,"TRANSGRIDV4_19000100000000","2012-01-27T14:40:00","#NSW1_E_20120127","2012-01-27",11,-56.446649999999998,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[318,"TRANSGRIDV4_19000100000000","2012-01-27T14:45:00","#NSW1_E_20120127","2012-01-27",11,-1026.46678,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[319,"TRANSGRIDV4_19000100000000","2012-01-27T14:50:00","#NSW1_E_20120127","2012-01-27",12,-589.14382999999998,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[320,"TRANSGRIDV4_19000100000000","2012-01-27T14:55:00","#NSW1_E_20120127","2012-01-27",12,-23.588000000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[321,"TRANSGRIDV4_19000100000000","2012-01-27T15:00:00","#NSW1_E_20120127","2012-01-27",14,-20.73779,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[322,"TRANSGRIDV4_19000100000000","2012-01-27T15:10:00","#NSW1_E_20120127","2012-01-27",14,-56.942100000000003,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[323,"TRANSGRIDV4_19000100000000","2012-01-27T15:15:00","#NSW1_E_20120127","2012-01-27",14,-136.95876000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[324,"TRANSGRIDV4_19000100000000","2012-01-27T15:25:00","#NSW1_E_20120127","2012-01-27",14,-698.38978999999995,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[325,"TRANSGRIDV4_19000100000000","2012-01-27T15:30:00","#NSW1_E_20120127","2012-01-27",14,-19.539280000000002,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[326,"TRANSGRIDV4_19000100000000","2012-01-27T15:35:00","#NSW1_E_20120127","2012-01-27",14,-23.672809999999998,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[327,"TRANSGRIDV4_19000100000000","2012-01-27T15:40:00","#NSW1_E_20120127","2012-01-27",15,-29.781690000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[328,"TRANSGRIDV4_19000100000000","2012-01-27T15:45:00","#NSW1_E_20120127","2012-01-27",15,-27.95148,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[329,"TRANSGRIDV4_19000100000000","2012-01-27T15:50:00","#NSW1_E_20120127","2012-01-27",16,-19.19387,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[330,"TRANSGRIDV4_19000100000000","2012-01-27T15:55:00","#NSW1_E_20120127","2012-01-27",17,-18.973939999999999,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[331,"TRANSGRIDV4_19000100000000","2012-01-29T12:15:00","#NSW1_E_20120129","2012-01-29",1,-1083.48875,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[332,"TRANSGRIDV4_19000100000000","2012-01-29T12:20:00","#NSW1_E_20120129","2012-01-29",2,-620.74526000000003,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[333,"TRANSGRIDV4_19000100000000","2012-01-29T13:50:00","#NSW1_E_20120129","2012-01-29",3,-627.21470999999997,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[334,"TRANSGRIDV4_19000100000000","2012-01-29T13:55:00","#NSW1_E_20120129","2012-01-29",4,-46.756869999999999,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[335,"TRANSGRIDV4_19000100000000","2012-01-29T14:00:00","#NSW1_E_20120129","2012-01-29",4,-13.62712,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[336,"TRANSGRIDV4_19000100000000","2012-01-29T14:20:00","#NSW1_E_20120129","2012-01-29",5,-1064.8376800000001,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[337,"TRANSGRIDV4_19000100000000","2012-01-29T14:25:00","#NSW1_E_20120129","2012-01-29",5,-148.36908,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[338,"TRANSGRIDV4_19000100000000","2012-01-29T14:40:00","#NSW1_E_20120129","2012-01-29",6,-727.13296000000003,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[339,"TRANSGRIDV4_19000100000000","2012-01-29T14:45:00","#NSW1_E_20120129","2012-01-29",7,-921.00351999999998,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[340,"TRANSGRIDV4_19000100000000","2012-01-29T14:50:00","#NSW1_E_20120129","2012-01-29",8,-1062.4720299999999,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[341,"TRANSGRIDV4_19000100000000","2012-01-29T14:55:00","#NSW1_E_20120129","2012-01-29",8,-146.19828000000001,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[342,"TRANSGRIDV4_19000100000000","2012-01-29T16:10:00","#NSW1_E_20120129","2012-01-29",9,-23.517410000000002,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[343,"TRANSGRIDV4_19000100000000","2012-01-29T16:15:00","#NSW1_E_20120129","2012-01-29",9,-477.39609999999999,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[344,"TRANSGRIDV4_19000100000000","2012-01-31T14:45:00","#NSW1_E_20120131","2012-01-31",1,-160.66603000000001,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[345,"TRANSGRIDV4_19000100000000","2012-01-31T14:55:00","#NSW1_E_20120131","2012-01-31",2,-20.62818,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[346,"TRANSGRIDV4_19000100000000","2012-01-31T15:00:00","#NSW1_E_20120131","2012-01-31",2,-20.187360000000002,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[347,"TRANSGRIDV4_19000100000000","2012-01-31T15:05:00","#NSW1_E_20120131","2012-01-31",2,-14.404579999999999,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[348,"TRANSGRIDV4_19000100000000","2012-01-31T15:10:00","#NSW1_E_20120131","2012-01-31",2,-14.092180000000001,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[349,"TRANSGRIDV4_19000100000000","2012-01-31T15:15:00","#NSW1_E_20120131","2012-01-31",3,-17.007110000000001,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[350,"TRANSGRIDV4_19000100000000","2012-01-31T15:20:00","#NSW1_E_20120131","2012-01-31",4,-12.6534,"Multiple NSW1 LHS <= 750 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[351,"TRANSGRIDV4_19000100000000","2012-02-09T15:45:00","#NSW1_E_20120209","2012-02-09",1,-516.46822999999995,"Multiple NSW1 LHS <= 850 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[352,"TRANSGRIDV4_19000100000000","2012-02-09T15:50:00","#NSW1_E_20120209","2012-02-09",1,-20.026700000000002,"Multiple NSW1 LHS <= 850 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[353,"TRANSGRIDV4_19000100000000","2012-02-14T15:30:00","#NSW1_E_20120214","2012-02-14",1,-621.35907999999995,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[354,"TRANSGRIDV4_19000100000000","2012-02-14T15:40:00","#NSW1_E_20120214","2012-02-14",2,-571.04660999999999,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[355,"TRANSGRIDV4_19000100000000","2012-02-14T15:45:00","#NSW1_E_20120214","2012-02-14",2,-20.61429,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[356,"TRANSGRIDV4_19000100000000","2012-02-17T14:45:00","#NSW1_E_20120217","2012-02-17",1,-143.85035999999999,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[357,"TRANSGRIDV4_19000100000000","2012-02-17T14:55:00","#NSW1_E_20120217","2012-02-17",3,-173.94973999999999,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[358,"TRANSGRIDV4_19000100000000","2012-02-17T15:00:00","#NSW1_E_20120217","2012-02-17",4,-16.454270000000001,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[359,"TRANSGRIDV4_19000100000000","2012-02-17T15:05:00","#NSW1_E_20120217","2012-02-17",4,-14.43535,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[360,"TRANSGRIDV4_19000100000000","2012-02-17T15:40:00","#NSW1_E_20120217","2012-02-17",5,-565.73983999999996,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[361,"TRANSGRIDV4_19000100000000","2012-02-17T16:00:00","#NSW1_E_20120217","2012-02-17",9,-978.86131,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[362,"TRANSGRIDV4_19000100000000","2012-02-17T16:05:00","#NSW1_E_20120217","2012-02-17",10,-51.563450000000003,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[363,"TRANSGRIDV4_19000100000000","2012-02-17T16:10:00","#NSW1_E_20120217","2012-02-17",10,-47.17604,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[364,"TRANSGRIDV4_19000100000000","2012-02-17T16:15:00","#NSW1_E_20120217","2012-02-17",10,-21.615490000000001,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[365,"TRANSGRIDV4_19000100000000","2012-02-20T14:05:00","#NSW1_E_20120220","2012-02-20",1,-44.41104,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[366,"TRANSGRIDV4_19000100000000","2012-02-20T14:10:00","#NSW1_E_20120220","2012-02-20",2,-33.302700000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[367,"TRANSGRIDV4_19000100000000","2012-02-20T14:15:00","#NSW1_E_20120220","2012-02-20",2,-35.138730000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[368,"TRANSGRIDV4_19000100000000","2012-02-20T14:20:00","#NSW1_E_20120220","2012-02-20",3,-32.460299999999997,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[369,"TRANSGRIDV4_19000100000000","2012-02-20T14:25:00","#NSW1_E_20120220","2012-02-20",4,-45.27628,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[370,"TRANSGRIDV4_19000100000000","2012-02-20T14:30:00","#NSW1_E_20120220","2012-02-20",4,-20.29504,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[371,"TRANSGRIDV4_19000100000000","2012-02-20T14:35:00","#NSW1_E_20120220","2012-02-20",4,-42.627670000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[372,"TRANSGRIDV4_19000100000000","2012-02-20T14:40:00","#NSW1_E_20120220","2012-02-20",4,-42.272150000000003,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[373,"TRANSGRIDV4_19000100000000","2012-02-20T14:45:00","#NSW1_E_20120220","2012-02-20",4,-33.758780000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[374,"TRANSGRIDV4_19000100000000","2012-02-20T14:50:00","#NSW1_E_20120220","2012-02-20",4,-44.886189999999999,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[375,"TRANSGRIDV4_19000100000000","2012-02-20T14:55:00","#NSW1_E_20120220","2012-02-20",5,-178.85692,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[376,"TRANSGRIDV4_19000100000000","2012-02-20T15:00:00","#NSW1_E_20120220","2012-02-20",5,-154.43129999999999,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[377,"TRANSGRIDV4_19000100000000","2012-02-20T15:05:00","#NSW1_E_20120220","2012-02-20",5,-40.068010000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[378,"TRANSGRIDV4_19000100000000","2012-02-20T15:10:00","#NSW1_E_20120220","2012-02-20",5,-35.833680000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[379,"TRANSGRIDV4_19000100000000","2012-02-20T15:20:00","#NSW1_E_20120220","2012-02-20",5,-28.653390000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[380,"TRANSGRIDV4_19000100000000","2012-02-20T15:30:00","#NSW1_E_20120220","2012-02-20",5,-29.850480000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[381,"TRANSGRIDV4_19000100000000","2012-02-20T15:35:00","#NSW1_E_20120220","2012-02-20",5,-40.697119999999998,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[382,"TRANSGRIDV4_19000100000000","2012-02-20T16:05:00","#NSW1_E_20120220","2012-02-20",5,-29.367930000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[383,"TRANSGRIDV4_19000100000000","2012-02-20T16:35:00","#NSW1_E_20120220","2012-02-20",5,-19.946169999999999,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[384,"TRANSGRIDV4_19000100000000","2012-02-20T16:40:00","#NSW1_E_20120220","2012-02-20",5,-27.681539999999998,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[385,"TRANSGRIDV4_19000100000000","2012-02-20T16:50:00","#NSW1_E_20120220","2012-02-20",5,-34.056739999999998,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[386,"TRANSGRIDV4_19000100000000","2012-02-20T16:55:00","#NSW1_E_20120220","2012-02-20",5,-14.71278,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[387,"TRANSGRIDV4_19000100000000","2012-02-20T17:00:00","#NSW1_E_20120220","2012-02-20",5,-22.084340000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[388,"TRANSGRIDV4_19000100000000","2012-02-20T17:05:00","#NSW1_E_20120220","2012-02-20",5,-16.915890000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[389,"TRANSGRIDV4_19000100000000","2012-02-20T17:10:00","#NSW1_E_20120220","2012-02-20",5,-29.556519999999999,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[390,"TRANSGRIDV4_19000100000000","2012-02-20T17:15:00","#NSW1_E_20120220","2012-02-20",5,-29.34421,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[391,"TRANSGRIDV4_19000100000000","2012-02-20T17:20:00","#NSW1_E_20120220","2012-02-20",5,-13.90695,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[392,"TRANSGRIDV4_19000100000000","2012-02-20T17:25:00","#NSW1_E_20120220","2012-02-20",5,-27.419930000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[393,"TRANSGRIDV4_19000100000000","2012-02-20T17:30:00","#NSW1_E_20120220","2012-02-20",5,-34.949840000000002,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[394,"TRANSGRIDV4_19000100000000","2012-02-20T17:35:00","#NSW1_E_20120220","2012-02-20",5,-30.56,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[395,"TRANSGRIDV4_19000100000000","2012-02-20T17:40:00","#NSW1_E_20120220","2012-02-20",5,-16.66994,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[396,"TRANSGRIDV4_19000100000000","2012-02-20T17:45:00","#NSW1_E_20120220","2012-02-20",5,-16.707909999999998,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[397,"TRANSGRIDV4_19000100000000","2012-02-20T17:55:00","#NSW1_E_20120220","2012-02-20",6,-13.246309999999999,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[398,"TRANSGRIDV4_19000100000000","2012-02-20T18:05:00","#NSW1_E_20120220","2012-02-20",7,-10.488580000000001,"Multiple NSW1 LHS <= 150 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[399,"TRANSGRIDV4_19000100000000","2012-02-21T12:35:00","#NSW1_E_20120221","2012-02-21",1,-17.232800000000001,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[400,"TRANSGRIDV4_19000100000000","2012-02-21T12:55:00","#NSW1_E_20120221","2012-02-21",2,-18.694800000000001,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[401,"TRANSGRIDV4_19000100000000","2012-02-21T13:00:00","#NSW1_E_20120221","2012-02-21",2,-30.730640000000001,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[402,"TRANSGRIDV4_19000100000000","2012-02-21T13:05:00","#NSW1_E_20120221","2012-02-21",2,-47.820929999999997,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[403,"TRANSGRIDV4_19000100000000","2012-02-21T13:20:00","#NSW1_E_20120221","2012-02-21",3,-25.689499999999999,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[404,"TRANSGRIDV4_19000100000000","2012-02-21T13:25:00","#NSW1_E_20120221","2012-02-21",3,-24.672499999999999,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[405,"TRANSGRIDV4_19000100000000","2012-02-21T13:30:00","#NSW1_E_20120221","2012-02-21",3,-64.717299999999994,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[406,"TRANSGRIDV4_19000100000000","2012-02-21T13:35:00","#NSW1_E_20120221","2012-02-21",3,-61.796289999999999,"Multiple NSW1 LHS <= 100 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[407,"TRANSGRIDV4_19000100000000","2012-02-22T15:30:00","#NSW1_E_20120222","2012-02-22",1,-182.37631999999999,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[408,"TRANSGRIDV4_19000100000000","2012-02-22T15:35:00","#NSW1_E_20120222","2012-02-22",1,-16.455580000000001,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[409,"TRANSGRIDV4_19000100000000","2012-02-22T16:00:00","#NSW1_E_20120222","2012-02-22",2,-639.70902999999998,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[410,"TRANSGRIDV4_19000100000000","2012-02-22T16:05:00","#NSW1_E_20120222","2012-02-22",2,-748.75315000000001,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[411,"TRANSGRIDV4_19000100000000","2012-02-22T16:10:00","#NSW1_E_20120222","2012-02-22",3,-73.02225,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[412,"TRANSGRIDV4_19000100000000","2012-02-22T16:15:00","#NSW1_E_20120222","2012-02-22",3,-26.24372,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[413,"TRANSGRIDV4_19000100000000","2012-02-22T16:20:00","#NSW1_E_20120222","2012-02-22",3,-26.412240000000001,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[414,"TRANSGRIDV4_19000100000000","2012-02-22T16:25:00","#NSW1_E_20120222","2012-02-22",3,-26.738289999999999,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[415,"TRANSGRIDV4_19000100000000","2012-02-22T16:30:00","#NSW1_E_20120222","2012-02-22",3,-27.001999999999999,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[416,"TRANSGRIDV4_19000100000000","2012-02-22T16:35:00","#NSW1_E_20120222","2012-02-22",3,-10.669840000000001,"Multiple NSW1 LHS <= 500 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[417,"TRANSGRIDV4_19000100000000","2012-03-02T10:30:00","#NSW1_E_20120302","2012-03-02",1,-855.98717999999997,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[418,"TRANSGRIDV4_19000100000000","2012-03-02T10:35:00","#NSW1_E_20120302","2012-03-02",1,-12.97461,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[419,"TRANSGRIDV4_19000100000000","2012-03-02T11:00:00","#NSW1_E_20120302","2012-03-02",2,-129.13406000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[420,"TRANSGRIDV4_19000100000000","2012-03-02T11:30:00","#NSW1_E_20120302","2012-03-02",3,-283.46463999999997,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[421,"TRANSGRIDV4_19000100000000","2012-03-02T11:35:00","#NSW1_E_20120302","2012-03-02",3,-561.78889000000004,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[422,"TRANSGRIDV4_19000100000000","2012-03-02T13:20:00","#NSW1_E_20120302","2012-03-02",4,-30.055389999999999,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[423,"TRANSGRIDV4_19000100000000","2012-03-02T13:25:00","#NSW1_E_20120302","2012-03-02",4,-13.221270000000001,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[424,"TRANSGRIDV4_19000100000000","2012-03-02T13:30:00","#NSW1_E_20120302","2012-03-02",4,-12.62842,"Multiple NSW1 LHS <= 550 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[425,"TRANSGRIDV4_19000100000000","2012-03-03T14:25:00","#NSW1_E_20120303","2012-03-03",1,-985.18570999999997,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[426,"TRANSGRIDV4_19000100000000","2012-03-03T15:00:00","#NSW1_E_20120303","2012-03-03",2,-573.5761,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[427,"TRANSGRIDV4_19000100000000","2012-03-03T15:50:00","#NSW1_E_20120303","2012-03-03",3,-949.28988000000004,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[428,"TRANSGRIDV4_19000100000000","2012-03-03T16:20:00","#NSW1_E_20120303","2012-03-03",5,-21.71312,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[429,"TRANSGRIDV4_19000100000000","2012-03-03T16:25:00","#NSW1_E_20120303","2012-03-03",5,-19.193729999999999,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[430,"TRANSGRIDV4_19000100000000","2012-03-03T16:30:00","#NSW1_E_20120303","2012-03-03",5,-11.77646,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[431,"TRANSGRIDV4_19000100000000","2012-03-03T16:35:00","#NSW1_E_20120303","2012-03-03",5,-12.65541,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[432,"TRANSGRIDV4_19000100000000","2012-03-04T14:40:00","#NSW1_E_20120303","2012-03-04",1,-556.44090000000006,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[433,"TRANSGRIDV4_19000100000000","2012-03-04T14:55:00","#NSW1_E_20120303","2012-03-04",2,-872.67988000000003,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[434,"TRANSGRIDV4_19000100000000","2012-03-04T15:00:00","#NSW1_E_20120303","2012-03-04",3,-910.30721000000005,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[435,"TRANSGRIDV4_19000100000000","2012-03-04T15:05:00","#NSW1_E_20120303","2012-03-04",3,-957.28385000000003,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[436,"TRANSGRIDV4_19000100000000","2012-03-04T15:10:00","#NSW1_E_20120303","2012-03-04",3,-957.61266999999998,"Multiple NSW1 LHS <= 700 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[437,"TRANSGRIDV4_19000100000000","2012-03-05T12:35:00","#NSW1_E_20120305","2012-03-05",1,-15.469480000000001,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[438,"TRANSGRIDV4_19000100000000","2012-03-05T12:40:00","#NSW1_E_20120305","2012-03-05",1,-24.492899999999999,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[439,"TRANSGRIDV4_19000100000000","2012-03-05T13:05:00","#NSW1_E_20120305","2012-03-05",2,-24.16705,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[440,"TRANSGRIDV4_19000100000000","2012-03-05T13:10:00","#NSW1_E_20120305","2012-03-05",2,-14.313829999999999,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[441,"TRANSGRIDV4_19000100000000","2012-03-05T13:15:00","#NSW1_E_20120305","2012-03-05",2,-24.7547,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[442,"TRANSGRIDV4_19000100000000","2012-03-05T13:20:00","#NSW1_E_20120305","2012-03-05",2,-24.6294,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[443,"TRANSGRIDV4_19000100000000","2012-03-06T14:00:00","#NSW1_E_20120306","2012-03-06",1,-284.42156,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[444,"TRANSGRIDV4_19000100000000","2012-03-06T14:05:00","#NSW1_E_20120306","2012-03-06",1,-10.6046,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[445,"TRANSGRIDV4_19000100000000","2012-03-06T14:10:00","#NSW1_E_20120306","2012-03-06",1,-10.394170000000001,"Multiple NSW1 LHS <= 600 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[446,"TRANSGRIDV4_19000100000000","2012-03-08T14:30:00","#NSW1_E_20120308","2012-03-08",1,-994.52364,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[447,"TRANSGRIDV4_19000100000000","2012-03-08T14:35:00","#NSW1_E_20120308","2012-03-08",2,-13.72936,"Multiple NSW1 LHS <= 400 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[448,"TRANSGRIDV4_19000100000000","2012-03-09T13:50:00","#NSW1_E_20120309","2012-03-09",2,-288.37891000000002,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[449,"TRANSGRIDV4_19000100000000","2012-03-09T13:55:00","#NSW1_E_20120309","2012-03-09",2,-134.20069000000001,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[450,"TRANSGRIDV4_19000100000000","2012-03-09T14:00:00","#NSW1_E_20120309","2012-03-09",2,-546.34349999999995,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[451,"TRANSGRIDV4_19000100000000","2012-03-09T14:05:00","#NSW1_E_20120309","2012-03-09",2,-16.824760000000001,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[452,"TRANSGRIDV4_19000100000000","2012-03-09T15:00:00","#NSW1_E_20120309","2012-03-09",4,-1019.04884,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[453,"TRANSGRIDV4_19000100000000","2012-03-09T15:05:00","#NSW1_E_20120309","2012-03-09",4,-13.909269999999999,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[454,"TRANSGRIDV4_19000100000000","2012-03-09T15:10:00","#NSW1_E_20120309","2012-03-09",4,-41.01482,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[455,"TRANSGRIDV4_19000100000000","2012-03-09T15:15:00","#NSW1_E_20120309","2012-03-09",4,-578.36596999999995,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[456,"TRANSGRIDV4_19000100000000","2012-03-09T16:05:00","#NSW1_E_20120309","2012-03-09",5,-801.95465000000002,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[457,"TRANSGRIDV4_19000100000000","2012-03-09T16:10:00","#NSW1_E_20120309","2012-03-09",5,-946.40972999999997,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[458,"TRANSGRIDV4_19000100000000","2012-03-10T14:00:00","#NSW1_E_20120310","2012-03-10",3,-158.70429999999999,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[459,"TRANSGRIDV4_19000100000000","2012-03-10T14:05:00","#NSW1_E_20120310","2012-03-10",4,-14.76915,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[460,"TRANSGRIDV4_19000100000000","2012-03-10T14:10:00","#NSW1_E_20120310","2012-03-10",5,-122.84180000000001,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[461,"TRANSGRIDV4_19000100000000","2012-03-10T14:20:00","#NSW1_E_20120310","2012-03-10",6,-125.57850000000001,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[462,"TRANSGRIDV4_19000100000000","2012-03-10T14:25:00","#NSW1_E_20120310","2012-03-10",6,-10.55871,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[463,"TRANSGRIDV4_19000100000000","2012-03-10T14:30:00","#NSW1_E_20120310","2012-03-10",6,-40.110770000000002,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[464,"TRANSGRIDV4_19000100000000","2012-03-10T14:40:00","#NSW1_E_20120310","2012-03-10",6,-23.643630000000002,"Multiple NSW1 LHS <= 710 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[465,"TRANSGRIDV4_19000100000000","2012-03-11T14:40:00","#NSW1_E_20120311","2012-03-11",1,-171.20366000000001,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[466,"TRANSGRIDV4_19000100000000","2012-03-11T14:50:00","#NSW1_E_20120311","2012-03-11",1,-13.181340000000001,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[467,"TRANSGRIDV4_19000100000000","2012-03-11T15:00:00","#NSW1_E_20120311","2012-03-11",1,-10.17306,"Multiple NSW1 LHS <= 1000 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[468,"TRANSGRIDV4_19000100000000","2012-03-23T15:10:00","#NSW1_E_20120323","2012-03-23",2,-44.899990000000003,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[469,"TRANSGRIDV4_19000100000000","2012-03-23T15:15:00","#NSW1_E_20120323","2012-03-23",3,-47.924860000000002,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[470,"TRANSGRIDV4_19000100000000","2012-03-23T15:20:00","#NSW1_E_20120323","2012-03-23",3,-138.82201000000001,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[471,"TRANSGRIDV4_19000100000000","2012-03-23T15:25:00","#NSW1_E_20120323","2012-03-23",3,-128.75465,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[472,"TRANSGRIDV4_19000100000000","2012-03-23T15:30:00","#NSW1_E_20120323","2012-03-23",3,-34.145769999999999,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[473,"TRANSGRIDV4_19000100000000","2012-03-23T15:35:00","#NSW1_E_20120323","2012-03-23",3,-11.15699,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[474,"TRANSGRIDV4_19000100000000","2012-03-23T15:40:00","#NSW1_E_20120323","2012-03-23",4,-564.55785000000003,"Multiple NSW1 LHS <= 800 (Wt = 1)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[475,"TRANSGRIDV4_19000100000000","2012-02-03T13:05:00","#NSW1-QLD1_I_E","2012-02-03",2,-13.91006,"NSW1-QLD1.ENERGY * -1 <= 850 (Wt = 17)","SYSTEM NORMAL","DIRECTION","","REGULATED",null,null,0]
[476,"TRANSGRIDV4_19000100000000","2012-06-20T17:40:00","F_MAIN++RREG_0350","2008-07-02",1,21.280889999999999,"Mainland Raise Regulation Requirement greater than 350 MW, Basslink able transfer FCAS","SYSTEM NORMAL","FCAS","","REGULATED",null,null,0]
[477,"TRANSGRIDV4_19000100000000","2012-06-20T17:45:00","F_MAIN++RREG_0350","2008-07-02",1,33.770000000000003,"Mainland Raise Regulation Requirement greater than 350 MW, Basslink able transfer FCAS","SYSTEM NORMAL","FCAS","","REGULATED",null,null,0]
[478,"TRANSGRIDV4_19000100000000","2012-06-20T17:50:00","F_MAIN++RREG_0350","2008-07-02",1,29.82,"Mainland Raise Regulation Requirement greater than 350 MW, Basslink able transfer FCAS","SYSTEM NORMAL","FCAS","","REGULATED",null,null,0]
[479,"TRANSGRIDV4_19000100000000","2012-06-20T17:55:00","F_MAIN++RREG_0350","2008-07-02",1,29.02,"Mainland Raise Regulation Requirement greater than 350 MW, Basslink able transfer FCAS","SYSTEM NORMAL","FCAS","","REGULATED",null,null,0]
[480,"TRANSGRIDV4_19000100000000","2012-06-20T18:00:00","F_MAIN++RREG_0350","2008-07-02",1,21.189969999999999,"Mainland Raise Regulation Requirement greater than 350 MW, Basslink able transfer FCAS","SYSTEM NORMAL","FCAS","","REGULATED",null,null,0]
[481,"TRANSGRIDV4_19000100000000","2012-04-03T07:45:00","F_Q++ARTW_L5","2012-03-19",1,10.04975,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[482,"TRANSGRIDV4_19000100000000","2012-04-03T08:00:00","F_Q++ARTW_L5","2012-03-19",1,11.1647,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[483,"TRANSGRIDV4_19000100000000","2012-04-03T08:35:00","F_Q++ARTW_L5","2012-03-19",1,15.0815,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[484,"TRANSGRIDV4_19000100000000","2012-04-03T08:40:00","F_Q++ARTW_L5","2012-03-19",1,14.6,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[485,"TRANSGRIDV4_19000100000000","2012-04-03T09:35:00","F_Q++ARTW_L5","2012-03-19",1,10.520960000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[486,"TRANSGRIDV4_19000100000000","2012-04-03T09:40:00","F_Q++ARTW_L5","2012-03-19",1,14.6,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[487,"TRANSGRIDV4_19000100000000","2012-04-03T11:55:00","F_Q++ARTW_L5","2012-03-19",1,10.57741,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[488,"TRANSGRIDV4_19000100000000","2012-04-03T13:30:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[489,"TRANSGRIDV4_19000100000000","2012-04-03T14:55:00","F_Q++ARTW_L5","2012-03-19",1,36.33867,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[490,"TRANSGRIDV4_19000100000000","2012-04-03T15:00:00","F_Q++ARTW_L5","2012-03-19",1,53.81559,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[491,"TRANSGRIDV4_19000100000000","2012-04-03T15:05:00","F_Q++ARTW_L5","2012-03-19",1,10.084339999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[492,"TRANSGRIDV4_19000100000000","2012-04-04T08:10:00","F_Q++ARTW_L5","2012-03-19",1,12.88105,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[493,"TRANSGRIDV4_19000100000000","2012-04-04T09:40:00","F_Q++ARTW_L5","2012-03-19",1,10.780720000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[494,"TRANSGRIDV4_19000100000000","2012-04-04T09:45:00","F_Q++ARTW_L5","2012-03-19",1,10.48362,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[495,"TRANSGRIDV4_19000100000000","2012-04-04T14:45:00","F_Q++ARTW_L5","2012-03-19",1,40.923749999999998,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[496,"TRANSGRIDV4_19000100000000","2012-04-05T06:35:00","F_Q++ARTW_L5","2012-03-19",1,23.621169999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[497,"TRANSGRIDV4_19000100000000","2012-04-05T06:40:00","F_Q++ARTW_L5","2012-03-19",1,23.430980000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[498,"TRANSGRIDV4_19000100000000","2012-04-05T06:45:00","F_Q++ARTW_L5","2012-03-19",1,13.45,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[499,"TRANSGRIDV4_19000100000000","2012-04-05T06:50:00","F_Q++ARTW_L5","2012-03-19",1,11.0601,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[500,"TRANSGRIDV4_19000100000000","2012-04-05T06:55:00","F_Q++ARTW_L5","2012-03-19",1,13.45,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[501,"TRANSGRIDV4_19000100000000","2012-04-05T07:50:00","F_Q++ARTW_L5","2012-03-19",1,11.484540000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[502,"TRANSGRIDV4_19000100000000","2012-04-05T07:55:00","F_Q++ARTW_L5","2012-03-19",1,10.458500000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[503,"TRANSGRIDV4_19000100000000","2012-04-05T08:10:00","F_Q++ARTW_L5","2012-03-19",1,15.64029,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[504,"TRANSGRIDV4_19000100000000","2012-04-05T08:15:00","F_Q++ARTW_L5","2012-03-19",1,15.0596,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[505,"TRANSGRIDV4_19000100000000","2012-04-05T08:20:00","F_Q++ARTW_L5","2012-03-19",1,15.33806,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[506,"TRANSGRIDV4_19000100000000","2012-04-05T08:25:00","F_Q++ARTW_L5","2012-03-19",1,13.380050000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[507,"TRANSGRIDV4_19000100000000","2012-04-05T08:40:00","F_Q++ARTW_L5","2012-03-19",1,11.75005,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[508,"TRANSGRIDV4_19000100000000","2012-04-05T08:45:00","F_Q++ARTW_L5","2012-03-19",1,15.8653,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[509,"TRANSGRIDV4_19000100000000","2012-04-05T08:50:00","F_Q++ARTW_L5","2012-03-19",1,11.924300000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[510,"TRANSGRIDV4_19000100000000","2012-04-05T08:55:00","F_Q++ARTW_L5","2012-03-19",1,11.29809,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[511,"TRANSGRIDV4_19000100000000","2012-04-05T09:00:00","F_Q++ARTW_L5","2012-03-19",1,14.531779999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[512,"TRANSGRIDV4_19000100000000","2012-04-05T09:05:00","F_Q++ARTW_L5","2012-03-19",1,11.91352,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[513,"TRANSGRIDV4_19000100000000","2012-04-05T09:10:00","F_Q++ARTW_L5","2012-03-19",1,10.74178,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[514,"TRANSGRIDV4_19000100000000","2012-04-05T09:15:00","F_Q++ARTW_L5","2012-03-19",1,22.824000000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[515,"TRANSGRIDV4_19000100000000","2012-04-05T09:20:00","F_Q++ARTW_L5","2012-03-19",1,14.4299,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[516,"TRANSGRIDV4_19000100000000","2012-04-05T09:25:00","F_Q++ARTW_L5","2012-03-19",1,13.875909999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[517,"TRANSGRIDV4_19000100000000","2012-04-05T09:30:00","F_Q++ARTW_L5","2012-03-19",1,14.553089999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[518,"TRANSGRIDV4_19000100000000","2012-04-05T09:35:00","F_Q++ARTW_L5","2012-03-19",1,14.25989,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[519,"TRANSGRIDV4_19000100000000","2012-04-05T09:40:00","F_Q++ARTW_L5","2012-03-19",1,15.227589999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[520,"TRANSGRIDV4_19000100000000","2012-04-05T09:45:00","F_Q++ARTW_L5","2012-03-19",1,14.880039999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[521,"TRANSGRIDV4_19000100000000","2012-04-05T09:50:00","F_Q++ARTW_L5","2012-03-19",1,14.25,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[522,"TRANSGRIDV4_19000100000000","2012-04-05T09:55:00","F_Q++ARTW_L5","2012-03-19",1,14.83901,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[523,"TRANSGRIDV4_19000100000000","2012-04-05T10:00:00","F_Q++ARTW_L5","2012-03-19",1,15.33239,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[524,"TRANSGRIDV4_19000100000000","2012-04-05T10:05:00","F_Q++ARTW_L5","2012-03-19",1,14.094860000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[525,"TRANSGRIDV4_19000100000000","2012-04-05T10:10:00","F_Q++ARTW_L5","2012-03-19",1,15.409879999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[526,"TRANSGRIDV4_19000100000000","2012-04-05T10:15:00","F_Q++ARTW_L5","2012-03-19",1,14.96862,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[527,"TRANSGRIDV4_19000100000000","2012-04-05T10:20:00","F_Q++ARTW_L5","2012-03-19",1,15.387919999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[528,"TRANSGRIDV4_19000100000000","2012-04-05T10:25:00","F_Q++ARTW_L5","2012-03-19",1,15.4055,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[529,"TRANSGRIDV4_19000100000000","2012-04-05T10:30:00","F_Q++ARTW_L5","2012-03-19",1,14.260059999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[530,"TRANSGRIDV4_19000100000000","2012-04-05T10:35:00","F_Q++ARTW_L5","2012-03-19",1,10.33006,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[531,"TRANSGRIDV4_19000100000000","2012-04-05T11:55:00","F_Q++ARTW_L5","2012-03-19",1,14.26,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[532,"TRANSGRIDV4_19000100000000","2012-04-05T12:00:00","F_Q++ARTW_L5","2012-03-19",1,11.48005,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[533,"TRANSGRIDV4_19000100000000","2012-04-05T12:05:00","F_Q++ARTW_L5","2012-03-19",1,11.470050000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[534,"TRANSGRIDV4_19000100000000","2012-04-05T12:10:00","F_Q++ARTW_L5","2012-03-19",1,13.44769,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[535,"TRANSGRIDV4_19000100000000","2012-04-05T12:15:00","F_Q++ARTW_L5","2012-03-19",1,11.46992,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[536,"TRANSGRIDV4_19000100000000","2012-04-05T12:20:00","F_Q++ARTW_L5","2012-03-19",1,14.310969999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[537,"TRANSGRIDV4_19000100000000","2012-04-05T12:25:00","F_Q++ARTW_L5","2012-03-19",1,11.46992,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[538,"TRANSGRIDV4_19000100000000","2012-04-13T07:35:00","F_Q++ARTW_L5","2012-03-19",1,16.062049999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[539,"TRANSGRIDV4_19000100000000","2012-04-13T07:40:00","F_Q++ARTW_L5","2012-03-19",1,16.84,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[540,"TRANSGRIDV4_19000100000000","2012-04-13T07:45:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[541,"TRANSGRIDV4_19000100000000","2012-04-13T08:40:00","F_Q++ARTW_L5","2012-03-19",1,12.26709,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[542,"TRANSGRIDV4_19000100000000","2012-04-13T11:05:00","F_Q++ARTW_L5","2012-03-19",1,11.780290000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[543,"TRANSGRIDV4_19000100000000","2012-04-13T11:10:00","F_Q++ARTW_L5","2012-03-19",1,18.684539999999998,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[544,"TRANSGRIDV4_19000100000000","2012-04-13T11:20:00","F_Q++ARTW_L5","2012-03-19",1,10.23,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[545,"TRANSGRIDV4_19000100000000","2012-04-13T11:45:00","F_Q++ARTW_L5","2012-03-19",1,11.338990000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[546,"TRANSGRIDV4_19000100000000","2012-04-13T12:50:00","F_Q++ARTW_L5","2012-03-19",1,12.55997,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[547,"TRANSGRIDV4_19000100000000","2012-09-26T07:05:00","F_Q++ARTW_L5","2012-03-19",1,43.57,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[548,"TRANSGRIDV4_19000100000000","2012-09-26T07:10:00","F_Q++ARTW_L5","2012-03-19",1,45.328290000000003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[549,"TRANSGRIDV4_19000100000000","2012-09-26T07:15:00","F_Q++ARTW_L5","2012-03-19",1,17.45045,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[550,"TRANSGRIDV4_19000100000000","2012-09-26T07:40:00","F_Q++ARTW_L5","2012-03-19",1,23.77617,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[551,"TRANSGRIDV4_19000100000000","2012-09-26T09:25:00","F_Q++ARTW_L5","2012-03-19",1,10.258570000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[552,"TRANSGRIDV4_19000100000000","2012-09-26T14:25:00","F_Q++ARTW_L5","2012-03-19",1,14.6,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[553,"TRANSGRIDV4_19000100000000","2012-10-30T06:05:00","F_Q++ARTW_L5","2012-03-19",1,10.77,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[554,"TRANSGRIDV4_19000100000000","2012-10-30T06:20:00","F_Q++ARTW_L5","2012-03-19",1,12.9,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[555,"TRANSGRIDV4_19000100000000","2012-10-30T06:25:00","F_Q++ARTW_L5","2012-03-19",1,14.52,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[556,"TRANSGRIDV4_19000100000000","2012-10-30T06:30:00","F_Q++ARTW_L5","2012-03-19",1,14.52,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[557,"TRANSGRIDV4_19000100000000","2012-10-30T06:45:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[558,"TRANSGRIDV4_19000100000000","2012-10-30T06:50:00","F_Q++ARTW_L5","2012-03-19",1,14.52,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[559,"TRANSGRIDV4_19000100000000","2012-10-30T10:40:00","F_Q++ARTW_L5","2012-03-19",1,10.27004,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[560,"TRANSGRIDV4_19000100000000","2012-10-30T11:30:00","F_Q++ARTW_L5","2012-03-19",1,15.699820000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[561,"TRANSGRIDV4_19000100000000","2012-10-30T12:15:00","F_Q++ARTW_L5","2012-03-19",1,12.42618,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[562,"TRANSGRIDV4_19000100000000","2012-10-30T13:15:00","F_Q++ARTW_L5","2012-03-19",1,16.72,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[563,"TRANSGRIDV4_19000100000000","2012-10-30T13:20:00","F_Q++ARTW_L5","2012-03-19",1,29.452349999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[564,"TRANSGRIDV4_19000100000000","2012-10-30T13:30:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[565,"TRANSGRIDV4_19000100000000","2012-10-30T13:35:00","F_Q++ARTW_L5","2012-03-19",1,10.010059999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[566,"TRANSGRIDV4_19000100000000","2012-10-30T13:55:00","F_Q++ARTW_L5","2012-03-19",1,31.864260000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[567,"TRANSGRIDV4_19000100000000","2012-10-30T14:00:00","F_Q++ARTW_L5","2012-03-19",1,58.43,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[568,"TRANSGRIDV4_19000100000000","2012-10-30T14:10:00","F_Q++ARTW_L5","2012-03-19",1,19.399999999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[569,"TRANSGRIDV4_19000100000000","2012-10-30T14:15:00","F_Q++ARTW_L5","2012-03-19",1,49.005009999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[570,"TRANSGRIDV4_19000100000000","2012-10-30T14:20:00","F_Q++ARTW_L5","2012-03-19",1,16.72,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[571,"TRANSGRIDV4_19000100000000","2012-10-30T14:25:00","F_Q++ARTW_L5","2012-03-19",1,16.82,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[572,"TRANSGRIDV4_19000100000000","2012-10-30T14:30:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[573,"TRANSGRIDV4_19000100000000","2012-10-30T14:35:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[574,"TRANSGRIDV4_19000100000000","2012-10-30T14:40:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[575,"TRANSGRIDV4_19000100000000","2012-10-30T14:45:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[576,"TRANSGRIDV4_19000100000000","2012-10-30T14:50:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[577,"TRANSGRIDV4_19000100000000","2012-10-30T14:55:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[578,"TRANSGRIDV4_19000100000000","2012-10-30T15:00:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[579,"TRANSGRIDV4_19000100000000","2012-10-30T15:05:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[580,"TRANSGRIDV4_19000100000000","2012-10-30T15:10:00","F_Q++ARTW_L5","2012-03-19",1,28.79965,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[581,"TRANSGRIDV4_19000100000000","2012-10-30T15:15:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[582,"TRANSGRIDV4_19000100000000","2012-10-30T15:20:00","F_Q++ARTW_L5","2012-03-19",1,32.775019999999998,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[583,"TRANSGRIDV4_19000100000000","2012-10-30T15:25:00","F_Q++ARTW_L5","2012-03-19",1,20.375170000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[584,"TRANSGRIDV4_19000100000000","2012-10-30T15:30:00","F_Q++ARTW_L5","2012-03-19",1,21.868839999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[585,"TRANSGRIDV4_19000100000000","2012-10-30T15:35:00","F_Q++ARTW_L5","2012-03-19",1,17.90476,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[586,"TRANSGRIDV4_19000100000000","2012-10-30T15:40:00","F_Q++ARTW_L5","2012-03-19",1,41.500109999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[587,"TRANSGRIDV4_19000100000000","2012-10-30T15:45:00","F_Q++ARTW_L5","2012-03-19",1,14.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[588,"TRANSGRIDV4_19000100000000","2012-10-30T15:50:00","F_Q++ARTW_L5","2012-03-19",1,36.559849999999997,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[589,"TRANSGRIDV4_19000100000000","2012-10-30T15:55:00","F_Q++ARTW_L5","2012-03-19",1,50.659889999999997,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[590,"TRANSGRIDV4_19000100000000","2012-10-30T16:00:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[591,"TRANSGRIDV4_19000100000000","2012-10-30T16:05:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[592,"TRANSGRIDV4_19000100000000","2012-10-30T16:10:00","F_Q++ARTW_L5","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[593,"TRANSGRIDV4_19000100000000","2012-10-31T06:05:00","F_Q++ARTW_L5","2012-03-19",1,11.17774,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[594,"TRANSGRIDV4_19000100000000","2012-10-31T06:45:00","F_Q++ARTW_L5","2012-03-19",1,10.77004,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[595,"TRANSGRIDV4_19000100000000","2012-10-31T09:45:00","F_Q++ARTW_L5","2012-03-19",1,56.97289,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[596,"TRANSGRIDV4_19000100000000","2012-10-31T09:50:00","F_Q++ARTW_L5","2012-03-19",1,10.59004,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[597,"TRANSGRIDV4_19000100000000","2012-10-31T09:55:00","F_Q++ARTW_L5","2012-03-19",1,13.389620000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[598,"TRANSGRIDV4_19000100000000","2012-10-31T10:15:00","F_Q++ARTW_L5","2012-03-19",1,10.56476,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[599,"TRANSGRIDV4_19000100000000","2012-10-31T10:45:00","F_Q++ARTW_L5","2012-03-19",1,14.719709999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[600,"TRANSGRIDV4_19000100000000","2012-03-07T06:50:00","F_Q++ARTW_L6","2007-04-18",1,10.239789999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[601,"TRANSGRIDV4_19000100000000","2012-04-03T13:30:00","F_Q++ARTW_L6","2012-03-19",1,12.73423,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[602,"TRANSGRIDV4_19000100000000","2012-04-03T13:35:00","F_Q++ARTW_L6","2012-03-19",1,24.393509999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[603,"TRANSGRIDV4_19000100000000","2012-04-03T14:35:00","F_Q++ARTW_L6","2012-03-19",1,44.36956,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[604,"TRANSGRIDV4_19000100000000","2012-04-04T06:05:00","F_Q++ARTW_L6","2012-03-19",1,12.6074,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[605,"TRANSGRIDV4_19000100000000","2012-04-04T10:40:00","F_Q++ARTW_L6","2012-03-19",1,11.98563,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[606,"TRANSGRIDV4_19000100000000","2012-04-04T10:45:00","F_Q++ARTW_L6","2012-03-19",1,10.91056,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[607,"TRANSGRIDV4_19000100000000","2012-04-04T14:50:00","F_Q++ARTW_L6","2012-03-19",1,39.286140000000003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[608,"TRANSGRIDV4_19000100000000","2012-04-13T08:00:00","F_Q++ARTW_L6","2012-03-19",1,11.926640000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[609,"TRANSGRIDV4_19000100000000","2012-04-13T08:10:00","F_Q++ARTW_L6","2012-03-19",1,11.895110000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[610,"TRANSGRIDV4_19000100000000","2012-04-13T08:15:00","F_Q++ARTW_L6","2012-03-19",1,11.82971,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[611,"TRANSGRIDV4_19000100000000","2012-04-13T08:20:00","F_Q++ARTW_L6","2012-03-19",1,12.20368,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[612,"TRANSGRIDV4_19000100000000","2012-04-13T08:30:00","F_Q++ARTW_L6","2012-03-19",1,11.80428,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[613,"TRANSGRIDV4_19000100000000","2012-04-13T08:35:00","F_Q++ARTW_L6","2012-03-19",1,11.45546,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[614,"TRANSGRIDV4_19000100000000","2012-04-13T08:45:00","F_Q++ARTW_L6","2012-03-19",1,11.837249999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[615,"TRANSGRIDV4_19000100000000","2012-04-13T08:50:00","F_Q++ARTW_L6","2012-03-19",1,11.814870000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[616,"TRANSGRIDV4_19000100000000","2012-04-13T08:55:00","F_Q++ARTW_L6","2012-03-19",1,11.404439999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[617,"TRANSGRIDV4_19000100000000","2012-04-13T09:05:00","F_Q++ARTW_L6","2012-03-19",1,12.1151,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[618,"TRANSGRIDV4_19000100000000","2012-04-13T09:10:00","F_Q++ARTW_L6","2012-03-19",1,11.568149999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[619,"TRANSGRIDV4_19000100000000","2012-04-13T09:15:00","F_Q++ARTW_L6","2012-03-19",1,10.92047,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[620,"TRANSGRIDV4_19000100000000","2012-09-26T09:20:00","F_Q++ARTW_L6","2012-03-19",1,40.379600000000003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[621,"TRANSGRIDV4_19000100000000","2012-09-26T12:45:00","F_Q++ARTW_L6","2012-03-19",1,21.300139999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[622,"TRANSGRIDV4_19000100000000","2012-09-26T12:55:00","F_Q++ARTW_L6","2012-03-19",1,21.51014,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[623,"TRANSGRIDV4_19000100000000","2012-09-26T13:00:00","F_Q++ARTW_L6","2012-03-19",1,21.300139999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[624,"TRANSGRIDV4_19000100000000","2012-09-26T14:25:00","F_Q++ARTW_L6","2012-03-19",1,10.347619999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[625,"TRANSGRIDV4_19000100000000","2012-10-30T06:30:00","F_Q++ARTW_L6","2012-03-19",1,10.40911,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[626,"TRANSGRIDV4_19000100000000","2012-10-30T11:10:00","F_Q++ARTW_L6","2012-03-19",1,10.06053,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[627,"TRANSGRIDV4_19000100000000","2012-10-30T13:15:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[628,"TRANSGRIDV4_19000100000000","2012-10-30T13:20:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[629,"TRANSGRIDV4_19000100000000","2012-10-30T13:55:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[630,"TRANSGRIDV4_19000100000000","2012-10-30T14:00:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[631,"TRANSGRIDV4_19000100000000","2012-10-30T14:10:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[632,"TRANSGRIDV4_19000100000000","2012-10-30T14:20:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[633,"TRANSGRIDV4_19000100000000","2012-10-30T14:25:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[634,"TRANSGRIDV4_19000100000000","2012-10-30T14:30:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[635,"TRANSGRIDV4_19000100000000","2012-10-30T14:35:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[636,"TRANSGRIDV4_19000100000000","2012-10-30T14:40:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[637,"TRANSGRIDV4_19000100000000","2012-10-30T14:45:00","F_Q++ARTW_L6","2012-03-19",1,40.447270000000003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[638,"TRANSGRIDV4_19000100000000","2012-10-30T14:50:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[639,"TRANSGRIDV4_19000100000000","2012-10-30T14:55:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[640,"TRANSGRIDV4_19000100000000","2012-10-30T15:00:00","F_Q++ARTW_L6","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[641,"TRANSGRIDV4_19000100000000","2012-10-30T15:05:00","F_Q++ARTW_L6","2012-03-19",1,42.546320000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[642,"TRANSGRIDV4_19000100000000","2012-10-30T15:10:00","F_Q++ARTW_L6","2012-03-19",1,42.599299999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[643,"TRANSGRIDV4_19000100000000","2012-10-30T15:15:00","F_Q++ARTW_L6","2012-03-19",1,67.680030000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[644,"TRANSGRIDV4_19000100000000","2012-10-30T15:20:00","F_Q++ARTW_L6","2012-03-19",1,50.55003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[645,"TRANSGRIDV4_19000100000000","2012-10-30T15:25:00","F_Q++ARTW_L6","2012-03-19",1,32.190330000000003,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[646,"TRANSGRIDV4_19000100000000","2012-10-30T15:30:00","F_Q++ARTW_L6","2012-03-19",1,30.737660000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[647,"TRANSGRIDV4_19000100000000","2012-10-30T15:35:00","F_Q++ARTW_L6","2012-03-19",1,32.109110000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[648,"TRANSGRIDV4_19000100000000","2012-10-30T15:40:00","F_Q++ARTW_L6","2012-03-19",1,32.172820000000002,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[649,"TRANSGRIDV4_19000100000000","2012-10-30T15:45:00","F_Q++ARTW_L6","2012-03-19",1,13.527950000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[650,"TRANSGRIDV4_19000100000000","2012-10-30T15:50:00","F_Q++ARTW_L6","2012-03-19",1,25.685680000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[651,"TRANSGRIDV4_19000100000000","2012-10-30T15:55:00","F_Q++ARTW_L6","2012-03-19",1,26.963249999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[652,"TRANSGRIDV4_19000100000000","2012-10-30T16:00:00","F_Q++ARTW_L6","2012-03-19",1,61.53257,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[653,"TRANSGRIDV4_19000100000000","2012-10-30T16:05:00","F_Q++ARTW_L6","2012-03-19",1,19.276160000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[654,"TRANSGRIDV4_19000100000000","2012-10-30T16:10:00","F_Q++ARTW_L6","2012-03-19",1,60.113079999999997,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[655,"TRANSGRIDV4_19000100000000","2012-10-31T06:05:00","F_Q++ARTW_L6","2012-03-19",1,12.057779999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[656,"TRANSGRIDV4_19000100000000","2012-10-31T06:10:00","F_Q++ARTW_L6","2012-03-19",1,10.94129,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[657,"TRANSGRIDV4_19000100000000","2012-10-31T09:45:00","F_Q++ARTW_L6","2012-03-19",1,13.310040000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[658,"TRANSGRIDV4_19000100000000","2012-10-31T09:55:00","F_Q++ARTW_L6","2012-03-19",1,10.81962,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[659,"TRANSGRIDV4_19000100000000","2012-04-03T06:05:00","F_Q++ARTW_L60","2012-03-19",1,10.808870000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[660,"TRANSGRIDV4_19000100000000","2012-10-30T14:00:00","F_Q++ARTW_L60","2012-03-19",1,13.15006,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[661,"TRANSGRIDV4_19000100000000","2012-10-30T14:45:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[662,"TRANSGRIDV4_19000100000000","2012-10-30T14:55:00","F_Q++ARTW_L60","2012-03-19",1,10.59024,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[663,"TRANSGRIDV4_19000100000000","2012-10-30T15:00:00","F_Q++ARTW_L60","2012-03-19",1,12.58644,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[664,"TRANSGRIDV4_19000100000000","2012-10-30T15:05:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[665,"TRANSGRIDV4_19000100000000","2012-10-30T15:10:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[666,"TRANSGRIDV4_19000100000000","2012-10-30T15:15:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[667,"TRANSGRIDV4_19000100000000","2012-10-30T15:20:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[668,"TRANSGRIDV4_19000100000000","2012-10-30T15:25:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[669,"TRANSGRIDV4_19000100000000","2012-10-30T15:30:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[670,"TRANSGRIDV4_19000100000000","2012-10-30T15:35:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[671,"TRANSGRIDV4_19000100000000","2012-10-30T15:40:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[672,"TRANSGRIDV4_19000100000000","2012-10-30T15:50:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[673,"TRANSGRIDV4_19000100000000","2012-10-30T15:55:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[674,"TRANSGRIDV4_19000100000000","2012-10-30T16:00:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[675,"TRANSGRIDV4_19000100000000","2012-10-30T16:05:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[676,"TRANSGRIDV4_19000100000000","2012-10-30T16:10:00","F_Q++ARTW_L60","2012-03-19",1,15,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale To Tamworth (85 Or 86) Line","REGULATED",null,null,1]
[677,"TRANSGRIDV4_19000100000000","2012-09-06T09:25:00","F_Q++LDMU_L5","2012-03-19",1,11.75062,"Out = Liddell to Muswellbrook (83) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Liddell To Muswellbrook (83) Line","REGULATED",null,null,1]
[678,"TRANSGRIDV4_19000100000000","2012-09-06T09:30:00","F_Q++LDMU_L5","2012-03-19",1,14.95,"Out = Liddell to Muswellbrook (83) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Liddell To Muswellbrook (83) Line","REGULATED",null,null,1]
[679,"TRANSGRIDV4_19000100000000","2012-09-06T10:40:00","F_Q++LDMU_L6","2012-03-19",1,36.361640000000001,"Out = Liddell to Muswellbrook (83) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Liddell To Muswellbrook (83) Line","REGULATED",null,null,1]
[680,"TRANSGRIDV4_19000100000000","2012-12-03T13:30:00","N:Q_LDTW_1","2012-01-10",1,-45.159889999999997,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[681,"TRANSGRIDV4_19000100000000","2012-12-03T13:35:00","N:Q_LDTW_1","2012-01-10",1,-47.219549999999998,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[682,"TRANSGRIDV4_19000100000000","2012-12-03T13:40:00","N:Q_LDTW_1","2012-01-10",1,-21.519410000000001,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[683,"TRANSGRIDV4_19000100000000","2012-12-03T14:15:00","N:Q_LDTW_1","2012-01-10",1,-13.556710000000001,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[684,"TRANSGRIDV4_19000100000000","2012-12-03T14:20:00","N:Q_LDTW_1","2012-01-10",1,-25325.792839999998,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[685,"TRANSGRIDV4_19000100000000","2012-12-03T14:25:00","N:Q_LDTW_1","2012-01-10",1,-25772.689190000001,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[686,"TRANSGRIDV4_19000100000000","2012-12-03T14:30:00","N:Q_LDTW_1","2012-01-10",1,-25770.03731,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[687,"TRANSGRIDV4_19000100000000","2012-12-03T14:35:00","N:Q_LDTW_1","2012-01-10",1,-25780.80745,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[688,"TRANSGRIDV4_19000100000000","2012-12-03T17:45:00","N:Q_LDTW_1","2012-01-10",1,-92.442149999999998,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[689,"TRANSGRIDV4_19000100000000","2012-12-03T18:45:00","N:Q_LDTW_1","2012-01-10",1,-31.69801,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[690,"TRANSGRIDV4_19000100000000","2012-12-03T18:50:00","N:Q_LDTW_1","2012-01-10",1,-31.447790000000001,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[691,"TRANSGRIDV4_19000100000000","2012-12-03T18:55:00","N:Q_LDTW_1","2012-01-10",1,-33.27516,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[692,"TRANSGRIDV4_19000100000000","2012-12-03T19:00:00","N:Q_LDTW_1","2012-01-10",1,-32.69511,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[693,"TRANSGRIDV4_19000100000000","2012-12-03T19:05:00","N:Q_LDTW_1","2012-01-10",1,-33.160690000000002,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[694,"TRANSGRIDV4_19000100000000","2012-12-03T19:15:00","N:Q_LDTW_1","2012-01-10",1,-30.0304,"Out = Liddell to Tamworth (84), NSW to QLD Transient Stability limit on loss of largest Qld unit","OUTAGE","OTHER","Liddell To Tamworth (84)","REGULATED",null,null,1]
[695,"TRANSGRIDV4_19000100000000","2012-09-11T08:25:00","N^^Q_ARDM_B1","2008-01-03",1,-10.67802,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[696,"TRANSGRIDV4_19000100000000","2012-09-11T08:35:00","N^^Q_ARDM_B1","2008-01-03",1,-11.799630000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[697,"TRANSGRIDV4_19000100000000","2012-09-11T08:40:00","N^^Q_ARDM_B1","2008-01-03",1,-10.635490000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[698,"TRANSGRIDV4_19000100000000","2012-09-11T08:50:00","N^^Q_ARDM_B1","2008-01-03",1,-15.77643,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[699,"TRANSGRIDV4_19000100000000","2012-09-11T10:55:00","N^^Q_ARDM_B1","2008-01-03",1,-11.364739999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[700,"TRANSGRIDV4_19000100000000","2012-09-11T11:00:00","N^^Q_ARDM_B1","2008-01-03",1,-10.705270000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[701,"TRANSGRIDV4_19000100000000","2012-09-11T11:15:00","N^^Q_ARDM_B1","2008-01-03",1,-14.36135,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[702,"TRANSGRIDV4_19000100000000","2012-09-12T07:00:00","N^^Q_ARDM_B1","2008-01-03",1,-40.738579999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[703,"TRANSGRIDV4_19000100000000","2012-09-12T07:05:00","N^^Q_ARDM_B1","2008-01-03",1,-29.83333,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[704,"TRANSGRIDV4_19000100000000","2012-09-12T07:10:00","N^^Q_ARDM_B1","2008-01-03",1,-24.462199999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[705,"TRANSGRIDV4_19000100000000","2012-09-12T07:15:00","N^^Q_ARDM_B1","2008-01-03",1,-10.35094,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[706,"TRANSGRIDV4_19000100000000","2012-09-12T07:35:00","N^^Q_ARDM_B1","2008-01-03",1,-11.72096,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[707,"TRANSGRIDV4_19000100000000","2012-09-12T07:40:00","N^^Q_ARDM_B1","2008-01-03",1,-13.13236,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[708,"TRANSGRIDV4_19000100000000","2012-09-12T07:45:00","N^^Q_ARDM_B1","2008-01-03",1,-12.75038,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[709,"TRANSGRIDV4_19000100000000","2012-09-12T07:50:00","N^^Q_ARDM_B1","2008-01-03",1,-10.98071,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[710,"TRANSGRIDV4_19000100000000","2012-09-12T07:55:00","N^^Q_ARDM_B1","2008-01-03",1,-36.861750000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[711,"TRANSGRIDV4_19000100000000","2012-09-12T08:00:00","N^^Q_ARDM_B1","2008-01-03",1,-11.065950000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[712,"TRANSGRIDV4_19000100000000","2012-09-12T08:05:00","N^^Q_ARDM_B1","2008-01-03",1,-11.06245,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[713,"TRANSGRIDV4_19000100000000","2012-09-12T08:10:00","N^^Q_ARDM_B1","2008-01-03",1,-43.08117,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[714,"TRANSGRIDV4_19000100000000","2012-09-12T08:15:00","N^^Q_ARDM_B1","2008-01-03",1,-39.978209999999997,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[715,"TRANSGRIDV4_19000100000000","2012-09-12T08:20:00","N^^Q_ARDM_B1","2008-01-03",1,-32.315570000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[716,"TRANSGRIDV4_19000100000000","2012-09-12T08:25:00","N^^Q_ARDM_B1","2008-01-03",1,-11.09576,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[717,"TRANSGRIDV4_19000100000000","2012-09-12T08:30:00","N^^Q_ARDM_B1","2008-01-03",1,-10.35078,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[718,"TRANSGRIDV4_19000100000000","2012-09-12T08:40:00","N^^Q_ARDM_B1","2008-01-03",1,-11.141360000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[719,"TRANSGRIDV4_19000100000000","2012-09-12T08:45:00","N^^Q_ARDM_B1","2008-01-03",1,-11.13424,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[720,"TRANSGRIDV4_19000100000000","2012-09-12T08:50:00","N^^Q_ARDM_B1","2008-01-03",1,-11.64101,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[721,"TRANSGRIDV4_19000100000000","2012-09-12T08:55:00","N^^Q_ARDM_B1","2008-01-03",1,-10.16291,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[722,"TRANSGRIDV4_19000100000000","2012-09-12T09:00:00","N^^Q_ARDM_B1","2008-01-03",1,-19.10407,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[723,"TRANSGRIDV4_19000100000000","2012-09-12T09:15:00","N^^Q_ARDM_B1","2008-01-03",1,-41.824060000000003,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[724,"TRANSGRIDV4_19000100000000","2012-09-12T09:25:00","N^^Q_ARDM_B1","2008-01-03",1,-10.30179,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[725,"TRANSGRIDV4_19000100000000","2012-09-12T09:35:00","N^^Q_ARDM_B1","2008-01-03",1,-11.69012,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[726,"TRANSGRIDV4_19000100000000","2012-09-12T09:40:00","N^^Q_ARDM_B1","2008-01-03",1,-11.6785,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[727,"TRANSGRIDV4_19000100000000","2012-09-12T09:50:00","N^^Q_ARDM_B1","2008-01-03",1,-10.676,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[728,"TRANSGRIDV4_19000100000000","2012-09-12T11:30:00","N^^Q_ARDM_B1","2008-01-03",1,-12.00277,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[729,"TRANSGRIDV4_19000100000000","2012-09-12T11:35:00","N^^Q_ARDM_B1","2008-01-03",1,-10.918419999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[730,"TRANSGRIDV4_19000100000000","2012-09-12T11:50:00","N^^Q_ARDM_B1","2008-01-03",1,-10.60393,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[731,"TRANSGRIDV4_19000100000000","2012-09-12T11:55:00","N^^Q_ARDM_B1","2008-01-03",1,-11.46618,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[732,"TRANSGRIDV4_19000100000000","2012-09-12T12:00:00","N^^Q_ARDM_B1","2008-01-03",1,-11.14423,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[733,"TRANSGRIDV4_19000100000000","2012-09-12T12:05:00","N^^Q_ARDM_B1","2008-01-03",1,-228.25839999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[734,"TRANSGRIDV4_19000100000000","2012-09-12T12:30:00","N^^Q_ARDM_B1","2008-01-03",1,-11.171430000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[735,"TRANSGRIDV4_19000100000000","2012-09-12T12:35:00","N^^Q_ARDM_B1","2008-01-03",1,-10.900880000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[736,"TRANSGRIDV4_19000100000000","2012-09-12T12:40:00","N^^Q_ARDM_B1","2008-01-03",1,-11.180999999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[737,"TRANSGRIDV4_19000100000000","2012-09-12T12:45:00","N^^Q_ARDM_B1","2008-01-03",1,-11.29285,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[738,"TRANSGRIDV4_19000100000000","2012-09-12T12:50:00","N^^Q_ARDM_B1","2008-01-03",1,-11.14541,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[739,"TRANSGRIDV4_19000100000000","2012-09-12T12:55:00","N^^Q_ARDM_B1","2008-01-03",1,-14.08159,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[740,"TRANSGRIDV4_19000100000000","2012-09-12T13:15:00","N^^Q_ARDM_B1","2008-01-03",1,-10.681319999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[741,"TRANSGRIDV4_19000100000000","2012-09-12T13:20:00","N^^Q_ARDM_B1","2008-01-03",1,-10.271330000000001,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[742,"TRANSGRIDV4_19000100000000","2012-09-12T13:25:00","N^^Q_ARDM_B1","2008-01-03",1,-10.25469,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[743,"TRANSGRIDV4_19000100000000","2012-09-12T13:45:00","N^^Q_ARDM_B1","2008-01-03",1,-228.73943,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[744,"TRANSGRIDV4_19000100000000","2012-09-12T14:30:00","N^^Q_ARDM_B1","2008-01-03",1,-10.719799999999999,"Out= one Armidale - Dumaresq (8C or 8E) line, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","One Armidale To Dumaresq (8C Or 8E) Line","REGULATED",null,null,1]
[745,"TRANSGRIDV4_19000100000000","2012-12-12T14:20:00","N^^V_BUDP_1","2012-07-06",1,-25.695979999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[746,"TRANSGRIDV4_19000100000000","2012-12-12T14:45:00","N^^V_BUDP_1","2012-07-06",1,-25.435939999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[747,"TRANSGRIDV4_19000100000000","2012-12-12T14:50:00","N^^V_BUDP_1","2012-07-06",1,-50.726050000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[748,"TRANSGRIDV4_19000100000000","2012-12-12T14:55:00","N^^V_BUDP_1","2012-07-06",1,-50.726619999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[749,"TRANSGRIDV4_19000100000000","2012-12-12T15:00:00","N^^V_BUDP_1","2012-07-06",1,-53.187530000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[750,"TRANSGRIDV4_19000100000000","2012-12-12T15:05:00","N^^V_BUDP_1","2012-07-06",1,-59.427050000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[751,"TRANSGRIDV4_19000100000000","2012-12-12T15:10:00","N^^V_BUDP_1","2012-07-06",1,-34.685459999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[752,"TRANSGRIDV4_19000100000000","2012-12-12T15:20:00","N^^V_BUDP_1","2012-07-06",1,-50.726619999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[753,"TRANSGRIDV4_19000100000000","2012-12-12T15:30:00","N^^V_BUDP_1","2012-07-06",1,-50.400350000000003,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[754,"TRANSGRIDV4_19000100000000","2012-12-12T15:45:00","N^^V_BUDP_1","2012-07-06",1,-170.36892,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[755,"TRANSGRIDV4_19000100000000","2012-12-12T15:50:00","N^^V_BUDP_1","2012-07-06",1,-170.41093000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[756,"TRANSGRIDV4_19000100000000","2012-12-12T15:55:00","N^^V_BUDP_1","2012-07-06",1,-170.35337000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[757,"TRANSGRIDV4_19000100000000","2012-12-12T16:00:00","N^^V_BUDP_1","2012-07-06",1,-612.76603999999998,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[758,"TRANSGRIDV4_19000100000000","2012-12-12T16:05:00","N^^V_BUDP_1","2012-07-06",1,-207.75844000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[759,"TRANSGRIDV4_19000100000000","2012-12-12T16:10:00","N^^V_BUDP_1","2012-07-06",1,-216.38149999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[760,"TRANSGRIDV4_19000100000000","2012-12-12T16:15:00","N^^V_BUDP_1","2012-07-06",1,-352.48149000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[761,"TRANSGRIDV4_19000100000000","2012-12-12T16:20:00","N^^V_BUDP_1","2012-07-06",1,-635.31078000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[762,"TRANSGRIDV4_19000100000000","2012-12-12T16:25:00","N^^V_BUDP_1","2012-07-06",1,-178.33324999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[763,"TRANSGRIDV4_19000100000000","2012-12-12T17:20:00","N^^V_BUDP_1","2012-07-06",1,-24.851179999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[764,"TRANSGRIDV4_19000100000000","2012-12-12T17:30:00","N^^V_BUDP_1","2012-07-06",1,-13.3613,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[765,"TRANSGRIDV4_19000100000000","2012-12-12T17:35:00","N^^V_BUDP_1","2012-07-06",1,-119.74225,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[766,"TRANSGRIDV4_19000100000000","2012-12-12T17:40:00","N^^V_BUDP_1","2012-07-06",1,-119.74225,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[767,"TRANSGRIDV4_19000100000000","2012-12-12T17:45:00","N^^V_BUDP_1","2012-07-06",1,-119.74294,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[768,"TRANSGRIDV4_19000100000000","2012-12-12T17:50:00","N^^V_BUDP_1","2012-07-06",1,-50.726619999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[769,"TRANSGRIDV4_19000100000000","2012-12-12T18:05:00","N^^V_BUDP_1","2012-07-06",1,-194.02655999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[770,"TRANSGRIDV4_19000100000000","2012-12-12T18:10:00","N^^V_BUDP_1","2012-07-06",1,-167.46707000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[771,"TRANSGRIDV4_19000100000000","2012-12-12T18:15:00","N^^V_BUDP_1","2012-07-06",1,-29.016950000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[772,"TRANSGRIDV4_19000100000000","2012-12-12T18:20:00","N^^V_BUDP_1","2012-07-06",1,-32.443100000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[773,"TRANSGRIDV4_19000100000000","2012-12-12T18:25:00","N^^V_BUDP_1","2012-07-06",1,-30.977869999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[774,"TRANSGRIDV4_19000100000000","2012-12-12T18:30:00","N^^V_BUDP_1","2012-07-06",1,-31.019110000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[775,"TRANSGRIDV4_19000100000000","2012-12-12T18:35:00","N^^V_BUDP_1","2012-07-06",1,-33.095289999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[776,"TRANSGRIDV4_19000100000000","2012-12-12T19:05:00","N^^V_BUDP_1","2012-07-06",1,-28.950520000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[777,"TRANSGRIDV4_19000100000000","2012-12-12T19:10:00","N^^V_BUDP_1","2012-07-06",1,-32.354529999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[778,"TRANSGRIDV4_19000100000000","2012-12-12T19:15:00","N^^V_BUDP_1","2012-07-06",1,-32.364049999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[779,"TRANSGRIDV4_19000100000000","2012-12-12T19:20:00","N^^V_BUDP_1","2012-07-06",1,-32.449840000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[780,"TRANSGRIDV4_19000100000000","2012-12-12T19:25:00","N^^V_BUDP_1","2012-07-06",1,-18.318339999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[781,"TRANSGRIDV4_19000100000000","2012-12-12T19:30:00","N^^V_BUDP_1","2012-07-06",1,-10.030110000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[782,"TRANSGRIDV4_19000100000000","2012-12-12T19:35:00","N^^V_BUDP_1","2012-07-06",1,-35.207160000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[783,"TRANSGRIDV4_19000100000000","2012-12-12T19:40:00","N^^V_BUDP_1","2012-07-06",1,-30.085519999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[784,"TRANSGRIDV4_19000100000000","2012-12-12T19:45:00","N^^V_BUDP_1","2012-07-06",1,-64.423919999999995,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[785,"TRANSGRIDV4_19000100000000","2012-12-12T19:50:00","N^^V_BUDP_1","2012-07-06",1,-513.61833999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[786,"TRANSGRIDV4_19000100000000","2012-12-12T19:55:00","N^^V_BUDP_1","2012-07-06",1,-180.51464999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[787,"TRANSGRIDV4_19000100000000","2012-12-12T20:00:00","N^^V_BUDP_1","2012-07-06",1,-180.91369,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[788,"TRANSGRIDV4_19000100000000","2012-12-12T20:05:00","N^^V_BUDP_1","2012-07-06",1,-65.24512,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[789,"TRANSGRIDV4_19000100000000","2012-12-12T20:10:00","N^^V_BUDP_1","2012-07-06",1,-58.632040000000003,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[790,"TRANSGRIDV4_19000100000000","2012-12-12T20:15:00","N^^V_BUDP_1","2012-07-06",1,-56.913130000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[791,"TRANSGRIDV4_19000100000000","2012-12-12T20:20:00","N^^V_BUDP_1","2012-07-06",1,-36.823180000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[792,"TRANSGRIDV4_19000100000000","2012-12-12T20:25:00","N^^V_BUDP_1","2012-07-06",1,-10.718870000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[793,"TRANSGRIDV4_19000100000000","2012-12-12T20:30:00","N^^V_BUDP_1","2012-07-06",1,-10.09299,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[794,"TRANSGRIDV4_19000100000000","2012-12-13T09:30:00","N^^V_BUDP_1","2012-07-06",1,-15.48579,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[795,"TRANSGRIDV4_19000100000000","2012-12-13T09:50:00","N^^V_BUDP_1","2012-07-06",1,-12.16619,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[796,"TRANSGRIDV4_19000100000000","2012-12-13T09:55:00","N^^V_BUDP_1","2012-07-06",1,-13.85417,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[797,"TRANSGRIDV4_19000100000000","2012-12-13T10:00:00","N^^V_BUDP_1","2012-07-06",1,-17.25216,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[798,"TRANSGRIDV4_19000100000000","2012-12-13T10:05:00","N^^V_BUDP_1","2012-07-06",1,-17.268180000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[799,"TRANSGRIDV4_19000100000000","2012-12-13T10:10:00","N^^V_BUDP_1","2012-07-06",1,-12.24564,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[800,"TRANSGRIDV4_19000100000000","2012-12-13T10:15:00","N^^V_BUDP_1","2012-07-06",1,-22.216259999999998,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[801,"TRANSGRIDV4_19000100000000","2012-12-13T10:20:00","N^^V_BUDP_1","2012-07-06",1,-24.374269999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[802,"TRANSGRIDV4_19000100000000","2012-12-13T10:25:00","N^^V_BUDP_1","2012-07-06",1,-58.291930000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[803,"TRANSGRIDV4_19000100000000","2012-12-13T10:30:00","N^^V_BUDP_1","2012-07-06",1,-56.273820000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[804,"TRANSGRIDV4_19000100000000","2012-12-13T10:35:00","N^^V_BUDP_1","2012-07-06",1,-56.324849999999998,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[805,"TRANSGRIDV4_19000100000000","2012-12-13T10:40:00","N^^V_BUDP_1","2012-07-06",1,-60.366590000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[806,"TRANSGRIDV4_19000100000000","2012-12-13T10:45:00","N^^V_BUDP_1","2012-07-06",1,-121.52477,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[807,"TRANSGRIDV4_19000100000000","2012-12-13T10:50:00","N^^V_BUDP_1","2012-07-06",1,-89.149339999999995,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[808,"TRANSGRIDV4_19000100000000","2012-12-13T10:55:00","N^^V_BUDP_1","2012-07-06",1,-88.61121,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[809,"TRANSGRIDV4_19000100000000","2012-12-13T11:00:00","N^^V_BUDP_1","2012-07-06",1,-136.82871,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[810,"TRANSGRIDV4_19000100000000","2012-12-13T11:05:00","N^^V_BUDP_1","2012-07-06",1,-180.54423,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[811,"TRANSGRIDV4_19000100000000","2012-12-13T11:10:00","N^^V_BUDP_1","2012-07-06",1,-177.89331999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[812,"TRANSGRIDV4_19000100000000","2012-12-13T11:15:00","N^^V_BUDP_1","2012-07-06",1,-180.51427000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[813,"TRANSGRIDV4_19000100000000","2012-12-13T11:20:00","N^^V_BUDP_1","2012-07-06",1,-181.52314000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[814,"TRANSGRIDV4_19000100000000","2012-12-13T11:25:00","N^^V_BUDP_1","2012-07-06",1,-181.51545999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[815,"TRANSGRIDV4_19000100000000","2012-12-13T11:30:00","N^^V_BUDP_1","2012-07-06",1,-174.73174,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[816,"TRANSGRIDV4_19000100000000","2012-12-13T11:35:00","N^^V_BUDP_1","2012-07-06",1,-11.40687,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[817,"TRANSGRIDV4_19000100000000","2012-12-13T11:40:00","N^^V_BUDP_1","2012-07-06",1,-180.50050999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[818,"TRANSGRIDV4_19000100000000","2012-12-13T11:45:00","N^^V_BUDP_1","2012-07-06",1,-180.42690999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[819,"TRANSGRIDV4_19000100000000","2012-12-13T11:50:00","N^^V_BUDP_1","2012-07-06",1,-237.60334,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[820,"TRANSGRIDV4_19000100000000","2012-12-13T11:55:00","N^^V_BUDP_1","2012-07-06",1,-240.52525,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[821,"TRANSGRIDV4_19000100000000","2012-12-13T12:00:00","N^^V_BUDP_1","2012-07-06",1,-248.77979999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[822,"TRANSGRIDV4_19000100000000","2012-12-13T12:05:00","N^^V_BUDP_1","2012-07-06",1,-179.06021999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[823,"TRANSGRIDV4_19000100000000","2012-12-13T12:10:00","N^^V_BUDP_1","2012-07-06",1,-242.31007,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[824,"TRANSGRIDV4_19000100000000","2012-12-13T12:15:00","N^^V_BUDP_1","2012-07-06",1,-246.41304,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[825,"TRANSGRIDV4_19000100000000","2012-12-13T12:20:00","N^^V_BUDP_1","2012-07-06",1,-479.63958000000002,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[826,"TRANSGRIDV4_19000100000000","2012-12-13T12:25:00","N^^V_BUDP_1","2012-07-06",1,-253.88040000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[827,"TRANSGRIDV4_19000100000000","2012-12-13T12:30:00","N^^V_BUDP_1","2012-07-06",1,-179.73455999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[828,"TRANSGRIDV4_19000100000000","2012-12-13T12:35:00","N^^V_BUDP_1","2012-07-06",1,-175.11401000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[829,"TRANSGRIDV4_19000100000000","2012-12-13T12:40:00","N^^V_BUDP_1","2012-07-06",1,-782.24911999999995,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[830,"TRANSGRIDV4_19000100000000","2012-12-13T12:45:00","N^^V_BUDP_1","2012-07-06",1,-807.64242999999999,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[831,"TRANSGRIDV4_19000100000000","2012-12-13T12:50:00","N^^V_BUDP_1","2012-07-06",1,-112.14875000000001,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[832,"TRANSGRIDV4_19000100000000","2012-12-13T12:55:00","N^^V_BUDP_1","2012-07-06",1,-943.71484999999996,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[833,"TRANSGRIDV4_19000100000000","2012-12-13T13:00:00","N^^V_BUDP_1","2012-07-06",1,-945.49221999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[834,"TRANSGRIDV4_19000100000000","2012-12-13T13:15:00","N^^V_BUDP_1","2012-07-06",1,-950.32345999999995,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[835,"TRANSGRIDV4_19000100000000","2012-12-14T10:00:00","N^^V_BUDP_1","2012-07-06",1,-36.837539999999997,"Out = Buronga to Darlington Point 220 kV line (X5/1 or X5/3), avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line (X5/1 Or X5/3)","REGULATED",null,null,1]
[836,"TRANSGRIDV4_19000100000000","2012-12-12T13:35:00","N^^V_BUDP_2","2012-07-06",1,-34.088279999999997,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[837,"TRANSGRIDV4_19000100000000","2012-12-12T13:40:00","N^^V_BUDP_2","2012-07-06",1,-34.749470000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[838,"TRANSGRIDV4_19000100000000","2012-12-12T13:45:00","N^^V_BUDP_2","2012-07-06",1,-38.198279999999997,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[839,"TRANSGRIDV4_19000100000000","2012-12-12T13:50:00","N^^V_BUDP_2","2012-07-06",1,-121.01161,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[840,"TRANSGRIDV4_19000100000000","2012-12-12T13:55:00","N^^V_BUDP_2","2012-07-06",1,-384.28014000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[841,"TRANSGRIDV4_19000100000000","2012-12-12T14:00:00","N^^V_BUDP_2","2012-07-06",1,-393.03413999999998,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[842,"TRANSGRIDV4_19000100000000","2012-12-12T14:05:00","N^^V_BUDP_2","2012-07-06",1,-540.52075000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[843,"TRANSGRIDV4_19000100000000","2012-12-12T15:15:00","N^^V_BUDP_2","2012-07-06",1,-59.95984,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[844,"TRANSGRIDV4_19000100000000","2012-12-12T15:20:00","N^^V_BUDP_2","2012-07-06",1,-153.58913000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[845,"TRANSGRIDV4_19000100000000","2012-12-12T15:25:00","N^^V_BUDP_2","2012-07-06",1,-203.21507,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[846,"TRANSGRIDV4_19000100000000","2012-12-12T15:30:00","N^^V_BUDP_2","2012-07-06",1,-156.56524999999999,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[847,"TRANSGRIDV4_19000100000000","2012-12-12T15:35:00","N^^V_BUDP_2","2012-07-06",1,-209.78608,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[848,"TRANSGRIDV4_19000100000000","2012-12-12T15:40:00","N^^V_BUDP_2","2012-07-06",1,-206.96941000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[849,"TRANSGRIDV4_19000100000000","2012-12-12T16:30:00","N^^V_BUDP_2","2012-07-06",1,-180.02748,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[850,"TRANSGRIDV4_19000100000000","2012-12-12T16:35:00","N^^V_BUDP_2","2012-07-06",1,-558.12647000000004,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[851,"TRANSGRIDV4_19000100000000","2012-12-12T16:40:00","N^^V_BUDP_2","2012-07-06",1,-175.45787000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[852,"TRANSGRIDV4_19000100000000","2012-12-12T16:45:00","N^^V_BUDP_2","2012-07-06",1,-81.859650000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[853,"TRANSGRIDV4_19000100000000","2012-12-12T16:55:00","N^^V_BUDP_2","2012-07-06",1,-82.1571,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[854,"TRANSGRIDV4_19000100000000","2012-12-12T17:00:00","N^^V_BUDP_2","2012-07-06",1,-61.007910000000003,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[855,"TRANSGRIDV4_19000100000000","2012-12-12T17:05:00","N^^V_BUDP_2","2012-07-06",1,-171.74572000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[856,"TRANSGRIDV4_19000100000000","2012-12-12T17:10:00","N^^V_BUDP_2","2012-07-06",1,-13.52275,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[857,"TRANSGRIDV4_19000100000000","2012-12-12T17:15:00","N^^V_BUDP_2","2012-07-06",1,-13.48002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[858,"TRANSGRIDV4_19000100000000","2012-12-12T17:25:00","N^^V_BUDP_2","2012-07-06",1,-13.541180000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[859,"TRANSGRIDV4_19000100000000","2012-12-13T12:50:00","N^^V_BUDP_2","2012-07-06",1,-592.32793000000004,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[860,"TRANSGRIDV4_19000100000000","2012-12-13T13:05:00","N^^V_BUDP_2","2012-07-06",1,-591.58290999999997,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[861,"TRANSGRIDV4_19000100000000","2012-12-13T13:10:00","N^^V_BUDP_2","2012-07-06",1,-656.03669000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[862,"TRANSGRIDV4_19000100000000","2012-12-13T13:20:00","N^^V_BUDP_2","2012-07-06",1,-683.07929000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[863,"TRANSGRIDV4_19000100000000","2012-12-13T13:25:00","N^^V_BUDP_2","2012-07-06",1,-679.78402000000006,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[864,"TRANSGRIDV4_19000100000000","2012-12-13T13:30:00","N^^V_BUDP_2","2012-07-06",1,-646.08166000000006,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[865,"TRANSGRIDV4_19000100000000","2012-12-13T13:35:00","N^^V_BUDP_2","2012-07-06",1,-584.07276000000002,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[866,"TRANSGRIDV4_19000100000000","2012-12-13T13:50:00","N^^V_BUDP_2","2012-07-06",1,-141.53745000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[867,"TRANSGRIDV4_19000100000000","2012-12-13T13:55:00","N^^V_BUDP_2","2012-07-06",1,-13282.11815,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[868,"TRANSGRIDV4_19000100000000","2012-12-13T14:00:00","N^^V_BUDP_2","2012-07-06",1,-13339.75332,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[869,"TRANSGRIDV4_19000100000000","2012-12-13T14:05:00","N^^V_BUDP_2","2012-07-06",1,-13340.333130000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[870,"TRANSGRIDV4_19000100000000","2012-12-13T14:10:00","N^^V_BUDP_2","2012-07-06",1,-13339.66791,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[871,"TRANSGRIDV4_19000100000000","2012-12-13T14:15:00","N^^V_BUDP_2","2012-07-06",1,-75.823650000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[872,"TRANSGRIDV4_19000100000000","2012-12-13T14:20:00","N^^V_BUDP_2","2012-07-06",1,-313.03654999999998,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[873,"TRANSGRIDV4_19000100000000","2012-12-13T14:25:00","N^^V_BUDP_2","2012-07-06",1,-122.32037,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[874,"TRANSGRIDV4_19000100000000","2012-12-13T14:35:00","N^^V_BUDP_2","2012-07-06",1,-12238.79523,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[875,"TRANSGRIDV4_19000100000000","2012-12-13T15:10:00","N^^V_BUDP_2","2012-07-06",1,-185.28012000000001,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[876,"TRANSGRIDV4_19000100000000","2012-12-13T15:15:00","N^^V_BUDP_2","2012-07-06",1,-12.11735,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[877,"TRANSGRIDV4_19000100000000","2012-12-13T15:20:00","N^^V_BUDP_2","2012-07-06",1,-180.87836999999999,"Out = Buronga to Darlington Point 220 kV line, avoid voltage collapse for loss of a Dederang to Murray 330 kV line ","OUTAGE","OTHER","Buronga To Darlington Point 220 Kv Line","REGULATED",null,null,1]
[878,"TRANSGRIDV4_19000100000000","2012-11-29T08:25:00","N^^V_MSUT_1","2012-07-06",1,-33.905180000000001,"Outage = Murray to Upper Tumut 330kV line, limit NSW to VIC, VIC and NSW gen to avoid voltage collapse for trip of the largest Vic generating unit","OUTAGE","OTHER","Murray To Upper Tumut 330 Kv Line","REGULATED",null,null,1]
[879,"TRANSGRIDV4_19000100000000","2012-11-29T08:30:00","N^^V_MSUT_1","2012-07-06",1,-33.286639999999998,"Outage = Murray to Upper Tumut 330kV line, limit NSW to VIC, VIC and NSW gen to avoid voltage collapse for trip of the largest Vic generating unit","OUTAGE","OTHER","Murray To Upper Tumut 330 Kv Line","REGULATED",null,null,1]
[880,"TRANSGRIDV4_19000100000000","2012-11-29T08:35:00","N^^V_MSUT_1","2012-07-06",1,-33.232779999999998,"Outage = Murray to Upper Tumut 330kV line, limit NSW to VIC, VIC and NSW gen to avoid voltage collapse for trip of the largest Vic generating unit","OUTAGE","OTHER","Murray To Upper Tumut 330 Kv Line","REGULATED",null,null,1]
[881,"TRANSGRIDV4_19000100000000","2012-11-29T08:40:00","N^^V_MSUT_1","2012-07-06",1,-33.21875,"Outage = Murray to Upper Tumut 330kV line, limit NSW to VIC, VIC and NSW gen to avoid voltage collapse for trip of the largest Vic generating unit","OUTAGE","OTHER","Murray To Upper Tumut 330 Kv Line","REGULATED",null,null,1]
[882,"TRANSGRIDV4_19000100000000","2012-11-29T08:45:00","N^^V_MSUT_1","2012-07-06",1,-35.595689999999998,"Outage = Murray to Upper Tumut 330kV line, limit NSW to VIC, VIC and NSW gen to avoid voltage collapse for trip of the largest Vic generating unit","OUTAGE","OTHER","Murray To Upper Tumut 330 Kv Line","REGULATED",null,null,1]
[883,"TRANSGRIDV4_19000100000000","2012-11-26T10:40:00","N^^V_MSUT2_A","2012-05-14",1,-10.41445,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[884,"TRANSGRIDV4_19000100000000","2012-11-26T10:45:00","N^^V_MSUT2_A","2012-05-14",1,-10.2273,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[885,"TRANSGRIDV4_19000100000000","2012-11-29T11:10:00","N^^V_MSUT2_A","2012-05-14",1,-26.044029999999999,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[886,"TRANSGRIDV4_19000100000000","2012-11-29T11:15:00","N^^V_MSUT2_A","2012-05-14",1,-26.007259999999999,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[887,"TRANSGRIDV4_19000100000000","2012-11-29T11:20:00","N^^V_MSUT2_A","2012-05-14",1,-25.267949999999999,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[888,"TRANSGRIDV4_19000100000000","2012-11-29T11:25:00","N^^V_MSUT2_A","2012-05-14",1,-25.269659999999998,"Out = Murray to Upper Tumut or Murray to Lower Tumut 330kV line, avoid voltage collapse for trip of Murray to Lower Tumut or Murray to Upper Tumut 330kV line, linear approx. first segment","OUTAGE","OTHER","Murray To Upper Tumut Or Murray To Lower Tumut 330Kv Line","REGULATED",null,null,1]
[889,"TRANSGRIDV4_19000100000000","2012-08-08T16:05:00","N^N_KKLS_1","2012-02-14",1,-144.52751000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[890,"TRANSGRIDV4_19000100000000","2012-10-26T12:45:00","N^N_KKLS_1","2012-02-14",1,-18.97007,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[891,"TRANSGRIDV4_19000100000000","2012-10-26T12:50:00","N^N_KKLS_1","2012-02-14",1,-19.224489999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[892,"TRANSGRIDV4_19000100000000","2012-10-26T12:55:00","N^N_KKLS_1","2012-02-14",1,-19.581140000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[893,"TRANSGRIDV4_19000100000000","2012-10-26T13:00:00","N^N_KKLS_1","2012-02-14",1,-20.2941,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[894,"TRANSGRIDV4_19000100000000","2012-10-26T13:15:00","N^N_KKLS_1","2012-02-14",1,-18.156330000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[895,"TRANSGRIDV4_19000100000000","2012-10-26T13:30:00","N^N_KKLS_1","2012-02-14",1,-17.288430000000002,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[896,"TRANSGRIDV4_19000100000000","2012-11-27T13:50:00","N^N_KKLS_1","2012-02-14",1,-11.957190000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[897,"TRANSGRIDV4_19000100000000","2012-11-27T13:55:00","N^N_KKLS_1","2012-02-14",1,-12.210889999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[898,"TRANSGRIDV4_19000100000000","2012-11-27T14:30:00","N^N_KKLS_1","2012-02-14",1,-13.63697,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[899,"TRANSGRIDV4_19000100000000","2012-11-27T14:45:00","N^N_KKLS_1","2012-02-14",1,-15.41086,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[900,"TRANSGRIDV4_19000100000000","2012-11-27T14:50:00","N^N_KKLS_1","2012-02-14",1,-14.58587,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[901,"TRANSGRIDV4_19000100000000","2012-11-27T14:55:00","N^N_KKLS_1","2012-02-14",1,-15.170489999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[902,"TRANSGRIDV4_19000100000000","2012-11-27T15:00:00","N^N_KKLS_1","2012-02-14",1,-10.163539999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[903,"TRANSGRIDV4_19000100000000","2012-11-27T15:10:00","N^N_KKLS_1","2012-02-14",1,-10.49175,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[904,"TRANSGRIDV4_19000100000000","2012-11-27T15:15:00","N^N_KKLS_1","2012-02-14",1,-10.418060000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[905,"TRANSGRIDV4_19000100000000","2012-11-27T15:25:00","N^N_KKLS_1","2012-02-14",1,-12.975529999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[906,"TRANSGRIDV4_19000100000000","2012-11-27T15:30:00","N^N_KKLS_1","2012-02-14",1,-12.96271,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[907,"TRANSGRIDV4_19000100000000","2012-11-27T15:40:00","N^N_KKLS_1","2012-02-14",1,-14.911659999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[908,"TRANSGRIDV4_19000100000000","2012-11-27T15:45:00","N^N_KKLS_1","2012-02-14",1,-12.867179999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[909,"TRANSGRIDV4_19000100000000","2012-11-27T15:50:00","N^N_KKLS_1","2012-02-14",1,-104.2634,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[910,"TRANSGRIDV4_19000100000000","2012-11-28T14:20:00","N^N_KKLS_1","2012-02-14",1,-11.50224,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[911,"TRANSGRIDV4_19000100000000","2012-11-28T14:50:00","N^N_KKLS_1","2012-02-14",1,-12.79607,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[912,"TRANSGRIDV4_19000100000000","2012-11-28T15:30:00","N^N_KKLS_1","2012-02-14",1,-10.03112,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[913,"TRANSGRIDV4_19000100000000","2012-11-28T15:45:00","N^N_KKLS_1","2012-02-14",1,-10.253550000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[914,"TRANSGRIDV4_19000100000000","2012-11-30T09:30:00","N^N_KKLS_1","2012-02-14",1,-258000,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[915,"TRANSGRIDV4_19000100000000","2012-11-30T09:35:00","N^N_KKLS_1","2012-02-14",1,-258000,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[916,"TRANSGRIDV4_19000100000000","2012-11-30T09:40:00","N^N_KKLS_1","2012-02-14",1,-257992.31585000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[917,"TRANSGRIDV4_19000100000000","2012-11-30T09:45:00","N^N_KKLS_1","2012-02-14",1,-258000,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[918,"TRANSGRIDV4_19000100000000","2012-11-30T09:50:00","N^N_KKLS_1","2012-02-14",1,-258000,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[919,"TRANSGRIDV4_19000100000000","2012-03-28T15:20:00","N_GG_ZERO","2010-02-25",2,-28.38599,"Redbank unit upper limit of 0 MW","OUTAGE","OTHER","","REGULATED",null,null,1]
[920,"TRANSGRIDV4_19000100000000","2012-10-16T14:55:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-10.77783,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[921,"TRANSGRIDV4_19000100000000","2012-10-16T15:00:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-17.662050000000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[922,"TRANSGRIDV4_19000100000000","2012-10-16T15:05:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-243.48500999999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[923,"TRANSGRIDV4_19000100000000","2012-10-16T15:10:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-44.716259999999998,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[924,"TRANSGRIDV4_19000100000000","2012-10-16T15:15:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-269.68869000000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[925,"TRANSGRIDV4_19000100000000","2012-10-16T15:20:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-271.17473000000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[926,"TRANSGRIDV4_19000100000000","2012-10-16T15:25:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-318.63790999999998,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[927,"TRANSGRIDV4_19000100000000","2012-10-16T15:30:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-287.91618,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[928,"TRANSGRIDV4_19000100000000","2012-10-16T15:35:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-284.16268000000002,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[929,"TRANSGRIDV4_19000100000000","2012-10-16T15:45:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-10.378769999999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[930,"TRANSGRIDV4_19000100000000","2012-10-16T15:50:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1272.6074100000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[931,"TRANSGRIDV4_19000100000000","2012-10-16T15:55:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1274.6085,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[932,"TRANSGRIDV4_19000100000000","2012-10-16T16:00:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1275.3923199999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[933,"TRANSGRIDV4_19000100000000","2012-10-16T16:05:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1274.29907,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[934,"TRANSGRIDV4_19000100000000","2012-10-16T16:10:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1285.33743,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[935,"TRANSGRIDV4_19000100000000","2012-10-16T16:15:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1287.49387,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[936,"TRANSGRIDV4_19000100000000","2012-10-16T16:20:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1281.37535,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[937,"TRANSGRIDV4_19000100000000","2012-10-16T16:25:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1303.0353399999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[938,"TRANSGRIDV4_19000100000000","2012-10-16T16:30:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1303.0051800000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[939,"TRANSGRIDV4_19000100000000","2012-10-16T16:35:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1287.3541499999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[940,"TRANSGRIDV4_19000100000000","2012-10-16T16:40:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1283.26199,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[941,"TRANSGRIDV4_19000100000000","2012-10-16T16:45:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1287.3996400000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[942,"TRANSGRIDV4_19000100000000","2012-10-16T16:50:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1287.4211700000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[943,"TRANSGRIDV4_19000100000000","2012-10-16T16:55:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1281.35871,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[944,"TRANSGRIDV4_19000100000000","2012-10-16T17:00:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1288.1193699999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[945,"TRANSGRIDV4_19000100000000","2012-10-16T17:05:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1258.1543099999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[946,"TRANSGRIDV4_19000100000000","2012-10-16T17:10:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1255.4032099999999,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[947,"TRANSGRIDV4_19000100000000","2012-10-16T17:15:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1276.5676100000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[948,"TRANSGRIDV4_19000100000000","2012-10-16T17:20:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1279.9461100000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[949,"TRANSGRIDV4_19000100000000","2012-10-16T17:25:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1261.07537,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[950,"TRANSGRIDV4_19000100000000","2012-10-16T17:30:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-1262.54458,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[951,"TRANSGRIDV4_19000100000000","2012-10-16T17:35:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-22.711600000000001,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[952,"TRANSGRIDV4_19000100000000","2012-10-16T17:40:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-10.72653,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[953,"TRANSGRIDV4_19000100000000","2012-10-16T17:45:00","N>>N-X_DTMN_LDTM_02","2012-10-11",1,-15.50766,"Out = Dapto-Marulan and Liddell-Tomago(8+82), avoid Marulan to Avon(16) O/L on KangarooValley-Dapto(18) trip; Feedback","OUTAGE","OTHER","Dapto To Marulan And Liddell To Tomago (8 & 82)","REGULATED",null,null,1]
[954,"TRANSGRIDV4_19000100000000","2012-11-27T07:10:00","N>>V-MSUT_5","2008-07-01",1,-12.41418,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[955,"TRANSGRIDV4_19000100000000","2012-11-27T07:15:00","N>>V-MSUT_5","2008-07-01",1,-12.95,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[956,"TRANSGRIDV4_19000100000000","2012-11-27T07:20:00","N>>V-MSUT_5","2008-07-01",1,-13.584149999999999,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[957,"TRANSGRIDV4_19000100000000","2012-11-27T07:25:00","N>>V-MSUT_5","2008-07-01",1,-13.83602,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[958,"TRANSGRIDV4_19000100000000","2012-11-27T07:30:00","N>>V-MSUT_5","2008-07-01",1,-12.66991,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[959,"TRANSGRIDV4_19000100000000","2012-11-27T07:35:00","N>>V-MSUT_5","2008-07-01",1,-15.23809,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[960,"TRANSGRIDV4_19000100000000","2012-11-27T07:55:00","N>>V-MSUT_5","2008-07-01",1,-10.797610000000001,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[961,"TRANSGRIDV4_19000100000000","2012-11-27T08:05:00","N>>V-MSUT_5","2008-07-01",1,-11.70562,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[962,"TRANSGRIDV4_19000100000000","2012-11-27T08:10:00","N>>V-MSUT_5","2008-07-01",1,-11.13302,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[963,"TRANSGRIDV4_19000100000000","2012-11-27T08:15:00","N>>V-MSUT_5","2008-07-01",1,-27.547419999999999,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[964,"TRANSGRIDV4_19000100000000","2012-11-27T08:20:00","N>>V-MSUT_5","2008-07-01",1,-25.42596,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[965,"TRANSGRIDV4_19000100000000","2012-11-27T08:25:00","N>>V-MSUT_5","2008-07-01",1,-23.10772,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[966,"TRANSGRIDV4_19000100000000","2012-11-27T10:30:00","N>>V-MSUT_5","2008-07-01",1,-14.5716,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[967,"TRANSGRIDV4_19000100000000","2012-11-27T11:00:00","N>>V-MSUT_5","2008-07-01",1,-17.011140000000001,"Out= Murray-UpperTumut(65), avoid LowerTumut to Murray (66) O/L on LowerTumut-Wagga(051)+ 970,990,99M trips; Feedback","OUTAGE","OTHER","Murray To Uppertumut (65)","REGULATED",null,null,1]
[968,"TRANSGRIDV4_19000100000000","2012-03-06T14:00:00","N>N-CHKK_TE_1","2010-11-22",2,-250000,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour To Koolkhan (96H)","REGULATED",null,null,1]
[969,"TRANSGRIDV4_19000100000000","2012-12-05T08:35:00","N>N-CHKK_TE_1","2012-03-07",1,-258000,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour To Koolkhan (96H)","REGULATED",null,null,1]
[970,"TRANSGRIDV4_19000100000000","2012-12-05T08:55:00","N>N-CHKK_TE_1","2012-03-07",1,-258000,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour To Koolkhan (96H)","REGULATED",null,null,1]
[971,"TRANSGRIDV4_19000100000000","2012-12-06T11:45:00","N>N-CHKK_TE_1","2012-03-07",1,-258000,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour To Koolkhan (96H)","REGULATED",null,null,1]
[972,"TRANSGRIDV4_19000100000000","2012-12-06T13:05:00","N>N-CHKK_TE_1","2012-03-07",1,-258000,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour To Koolkhan (96H)","REGULATED",null,null,1]
[973,"TRANSGRIDV4_19000100000000","2012-03-05T11:55:00","N>N-GITN_TE_C1","2010-11-22",2,-158.00971999999999,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[974,"TRANSGRIDV4_19000100000000","2012-03-05T12:00:00","N>N-GITN_TE_C1","2010-11-22",2,-1413.76893,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[975,"TRANSGRIDV4_19000100000000","2012-03-05T12:05:00","N>N-GITN_TE_C1","2010-11-22",2,-150.41266999999999,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[976,"TRANSGRIDV4_19000100000000","2012-03-05T12:25:00","N>N-GITN_TE_C1","2010-11-22",2,-1360.9344699999999,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[977,"TRANSGRIDV4_19000100000000","2012-03-05T12:30:00","N>N-GITN_TE_C1","2010-11-22",2,-148.85568000000001,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[978,"TRANSGRIDV4_19000100000000","2012-03-05T12:40:00","N>N-GITN_TE_C1","2010-11-22",2,-144.42032,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[979,"TRANSGRIDV4_19000100000000","2012-03-05T12:55:00","N>N-GITN_TE_C1","2010-11-22",2,-135.50228999999999,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[980,"TRANSGRIDV4_19000100000000","2012-03-05T13:00:00","N>N-GITN_TE_C1","2010-11-22",2,-138.45475999999999,"Out= Glen Innes to Tenterfield (96R), avoid O/L Koolkhan to Lismore (967) on trip of Coffs Harbour to Lismore (89), Feedback, TG formulation in PD/ST","OUTAGE","OTHER","Glen Innes To Tenterfield (96R)","REGULATED",null,null,1]
[981,"TRANSGRIDV4_19000100000000","2012-11-27T15:20:00","N>N-KKLS_TE_2","2012-03-08",1,-11.90579,"Out= Koolkhan to Lismore (967), avoid O/L Tenterfield to Lismore (96L) on trip of Coffs Harbour to Lismore (89), TG formulation","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[982,"TRANSGRIDV4_19000100000000","2012-11-30T09:30:00","N>N-KKLS_TE_2","2012-03-08",1,-257992.20516000001,"Out= Koolkhan to Lismore (967), avoid O/L Tenterfield to Lismore (96L) on trip of Coffs Harbour to Lismore (89), TG formulation","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[983,"TRANSGRIDV4_19000100000000","2012-11-30T09:35:00","N>N-KKLS_TE_2","2012-03-08",1,-257991.41016,"Out= Koolkhan to Lismore (967), avoid O/L Tenterfield to Lismore (96L) on trip of Coffs Harbour to Lismore (89), TG formulation","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[984,"TRANSGRIDV4_19000100000000","2012-11-30T09:40:00","N>N-KKLS_TE_2","2012-03-08",1,-258000,"Out= Koolkhan to Lismore (967), avoid O/L Tenterfield to Lismore (96L) on trip of Coffs Harbour to Lismore (89), TG formulation","OUTAGE","OTHER","Koolkhan To Lismore (967)","REGULATED",null,null,1]
[985,"TRANSGRIDV4_19000100000000","2012-02-28T13:55:00","N>Q_LSLS_9U8","2012-02-10",1,-151.24524,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[986,"TRANSGRIDV4_19000100000000","2012-02-28T14:20:00","N>Q_LSLS_9U8","2012-02-10",1,-151.59636,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[987,"TRANSGRIDV4_19000100000000","2012-02-28T14:30:00","N>Q_LSLS_9U8","2012-02-10",1,-151.34524999999999,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[988,"TRANSGRIDV4_19000100000000","2012-02-28T15:10:00","N>Q_LSLS_9U8","2012-02-10",1,-148.98463000000001,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[989,"TRANSGRIDV4_19000100000000","2012-03-08T14:20:00","N>Q_LSLS_9U8","2012-02-10",1,-233.49327,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[990,"TRANSGRIDV4_19000100000000","2012-03-08T14:25:00","N>Q_LSLS_9U8","2012-02-10",1,-1257.9781499999999,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[991,"TRANSGRIDV4_19000100000000","2012-03-08T14:30:00","N>Q_LSLS_9U8","2012-02-10",1,-152.93084999999999,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd","OUTAGE","OTHER","One Of Lismore330 To Lismore132 (9U8","REGULATED",null,null,1]
[992,"TRANSGRIDV4_19000100000000","2012-08-04T16:40:00","NQTE_ROC","2010-11-08",2,-158.13171,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[993,"TRANSGRIDV4_19000100000000","2012-08-04T17:00:00","NQTE_ROC","2010-11-08",2,-141.15923000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[994,"TRANSGRIDV4_19000100000000","2012-08-11T16:15:00","NQTE_ROC","2010-11-08",2,-129.71252999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[995,"TRANSGRIDV4_19000100000000","2012-08-24T14:35:00","NQTE_ROC","2010-11-08",2,-126.97029000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[996,"TRANSGRIDV4_19000100000000","2012-08-24T16:10:00","NQTE_ROC","2010-11-08",2,-14.16872,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[997,"TRANSGRIDV4_19000100000000","2012-08-25T09:10:00","NQTE_ROC","2010-11-08",2,-10.70299,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[998,"TRANSGRIDV4_19000100000000","2012-08-25T12:40:00","NQTE_ROC","2010-11-08",2,-304.74194,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[999,"TRANSGRIDV4_19000100000000","2012-08-25T12:45:00","NQTE_ROC","2010-11-08",2,-121.51739000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1000,"TRANSGRIDV4_19000100000000","2012-08-25T13:45:00","NQTE_ROC","2010-11-08",2,-859.25147000000004,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1001,"TRANSGRIDV4_19000100000000","2012-08-25T16:55:00","NQTE_ROC","2010-11-08",2,-882.48198000000002,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1002,"TRANSGRIDV4_19000100000000","2012-08-26T08:45:00","NQTE_ROC","2010-11-08",2,-271.15710000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1003,"TRANSGRIDV4_19000100000000","2012-08-26T10:30:00","NQTE_ROC","2010-11-08",2,-918.65674999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1004,"TRANSGRIDV4_19000100000000","2012-08-26T10:45:00","NQTE_ROC","2010-11-08",2,-1288.96578,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1005,"TRANSGRIDV4_19000100000000","2012-08-26T14:55:00","NQTE_ROC","2010-11-08",2,-14.171340000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1006,"TRANSGRIDV4_19000100000000","2012-08-27T14:50:00","NQTE_ROC","2010-11-08",2,-11.14677,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1007,"TRANSGRIDV4_19000100000000","2012-08-30T11:35:00","NQTE_ROC","2010-11-08",2,-124.17049,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1008,"TRANSGRIDV4_19000100000000","2012-08-30T12:30:00","NQTE_ROC","2010-11-08",2,-15.154350000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1009,"TRANSGRIDV4_19000100000000","2012-08-30T14:45:00","NQTE_ROC","2010-11-08",2,-18.130749999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1010,"TRANSGRIDV4_19000100000000","2012-08-30T15:35:00","NQTE_ROC","2010-11-08",2,-10.132860000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1011,"TRANSGRIDV4_19000100000000","2012-08-30T16:00:00","NQTE_ROC","2010-11-08",2,-12.21341,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1012,"TRANSGRIDV4_19000100000000","2012-08-31T09:30:00","NQTE_ROC","2010-11-08",2,-24.811969999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1013,"TRANSGRIDV4_19000100000000","2012-08-31T10:00:00","NQTE_ROC","2010-11-08",2,-1381.32195,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1014,"TRANSGRIDV4_19000100000000","2012-08-31T11:35:00","NQTE_ROC","2010-11-08",2,-16.988620000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1015,"TRANSGRIDV4_19000100000000","2012-08-31T12:00:00","NQTE_ROC","2010-11-08",2,-122.27879,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1016,"TRANSGRIDV4_19000100000000","2012-08-31T12:30:00","NQTE_ROC","2010-11-08",2,-1338.7128499999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1017,"TRANSGRIDV4_19000100000000","2012-08-31T16:00:00","NQTE_ROC","2010-11-08",2,-53.77581,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1018,"TRANSGRIDV4_19000100000000","2012-09-01T07:35:00","NQTE_ROC","2010-11-08",2,-15.179729999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1019,"TRANSGRIDV4_19000100000000","2012-09-01T11:35:00","NQTE_ROC","2010-11-08",2,-93.748620000000003,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1020,"TRANSGRIDV4_19000100000000","2012-09-02T09:45:00","NQTE_ROC","2010-11-08",2,-116.25579999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1021,"TRANSGRIDV4_19000100000000","2012-09-03T09:10:00","NQTE_ROC","2010-11-08",2,-15.46869,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1022,"TRANSGRIDV4_19000100000000","2012-09-03T09:25:00","NQTE_ROC","2010-11-08",2,-10.70294,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1023,"TRANSGRIDV4_19000100000000","2012-09-03T12:55:00","NQTE_ROC","2010-11-08",2,-99.071759999999998,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1024,"TRANSGRIDV4_19000100000000","2012-09-03T13:05:00","NQTE_ROC","2010-11-08",2,-113.03128,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1025,"TRANSGRIDV4_19000100000000","2012-09-03T13:25:00","NQTE_ROC","2010-11-08",2,-14.207240000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1026,"TRANSGRIDV4_19000100000000","2012-09-04T10:10:00","NQTE_ROC","2010-11-08",2,-873.86414000000002,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1027,"TRANSGRIDV4_19000100000000","2012-09-04T10:25:00","NQTE_ROC","2010-11-08",2,-10.82535,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1028,"TRANSGRIDV4_19000100000000","2012-09-05T07:55:00","NQTE_ROC","2010-11-08",2,-38.72589,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1029,"TRANSGRIDV4_19000100000000","2012-09-05T08:50:00","NQTE_ROC","2010-11-08",2,-35.154829999999997,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1030,"TRANSGRIDV4_19000100000000","2012-09-05T11:15:00","NQTE_ROC","2010-11-08",2,-37.231949999999998,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1031,"TRANSGRIDV4_19000100000000","2012-09-05T13:30:00","NQTE_ROC","2010-11-08",2,-35.561430000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1032,"TRANSGRIDV4_19000100000000","2012-09-05T14:50:00","NQTE_ROC","2010-11-08",2,-36.220730000000003,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1033,"TRANSGRIDV4_19000100000000","2012-09-05T15:30:00","NQTE_ROC","2010-11-08",2,-36.895690000000002,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1034,"TRANSGRIDV4_19000100000000","2012-09-05T15:50:00","NQTE_ROC","2010-11-08",2,-45.985230000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1035,"TRANSGRIDV4_19000100000000","2012-09-05T16:25:00","NQTE_ROC","2010-11-08",2,-50.987189999999998,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1036,"TRANSGRIDV4_19000100000000","2012-09-06T07:05:00","NQTE_ROC","2010-11-08",2,-18.240600000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1037,"TRANSGRIDV4_19000100000000","2012-09-06T07:40:00","NQTE_ROC","2010-11-08",2,-16.566579999999998,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1038,"TRANSGRIDV4_19000100000000","2012-09-06T11:20:00","NQTE_ROC","2010-11-08",2,-15.040139999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1039,"TRANSGRIDV4_19000100000000","2012-09-07T07:35:00","NQTE_ROC","2010-11-08",2,-16.642109999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1040,"TRANSGRIDV4_19000100000000","2012-09-07T08:20:00","NQTE_ROC","2010-11-08",2,-25.368559999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1041,"TRANSGRIDV4_19000100000000","2012-09-07T09:00:00","NQTE_ROC","2010-11-08",2,-14.81433,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1042,"TRANSGRIDV4_19000100000000","2012-09-07T13:05:00","NQTE_ROC","2010-11-08",2,-15.50113,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1043,"TRANSGRIDV4_19000100000000","2012-09-08T07:35:00","NQTE_ROC","2010-11-08",2,-17.32105,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1044,"TRANSGRIDV4_19000100000000","2012-09-08T10:05:00","NQTE_ROC","2010-11-08",2,-17.1614,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1045,"TRANSGRIDV4_19000100000000","2012-09-08T12:05:00","NQTE_ROC","2010-11-08",2,-15.31728,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1046,"TRANSGRIDV4_19000100000000","2012-09-08T13:00:00","NQTE_ROC","2010-11-08",2,-14.738899999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1047,"TRANSGRIDV4_19000100000000","2012-09-08T14:00:00","NQTE_ROC","2010-11-08",2,-18.52788,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1048,"TRANSGRIDV4_19000100000000","2012-09-09T12:20:00","NQTE_ROC","2010-11-08",2,-13.68563,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1049,"TRANSGRIDV4_19000100000000","2012-10-21T13:00:00","NQTE_ROC","2010-11-08",2,-154.48076,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1050,"TRANSGRIDV4_19000100000000","2012-10-21T13:55:00","NQTE_ROC","2010-11-08",2,-150.05598000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1051,"TRANSGRIDV4_19000100000000","2012-10-21T14:30:00","NQTE_ROC","2010-11-08",2,-117.6718,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1052,"TRANSGRIDV4_19000100000000","2012-10-26T15:50:00","NQTE_ROC","2010-11-08",2,-10.592969999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1053,"TRANSGRIDV4_19000100000000","2012-10-27T11:00:00","NQTE_ROC","2010-11-08",2,-128.97728000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1054,"TRANSGRIDV4_19000100000000","2012-10-27T12:00:00","NQTE_ROC","2010-11-08",2,-122.33986,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1055,"TRANSGRIDV4_19000100000000","2012-10-27T12:05:00","NQTE_ROC","2010-11-08",2,-105.11295,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1056,"TRANSGRIDV4_19000100000000","2012-10-27T12:20:00","NQTE_ROC","2010-11-08",2,-110.63055,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1057,"TRANSGRIDV4_19000100000000","2012-10-27T12:50:00","NQTE_ROC","2010-11-08",2,-134.09280000000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1058,"TRANSGRIDV4_19000100000000","2012-10-27T13:20:00","NQTE_ROC","2010-11-08",2,-19.512429999999998,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1059,"TRANSGRIDV4_19000100000000","2012-10-27T13:25:00","NQTE_ROC","2010-11-08",2,-104.56735,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1060,"TRANSGRIDV4_19000100000000","2012-10-27T14:40:00","NQTE_ROC","2010-11-08",2,-18447.263490000001,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1061,"TRANSGRIDV4_19000100000000","2012-10-27T14:55:00","NQTE_ROC","2010-11-08",2,-100.47960999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1062,"TRANSGRIDV4_19000100000000","2012-12-02T15:35:00","NQTE_ROC","2010-11-08",2,-15.320679999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1063,"TRANSGRIDV4_19000100000000","2012-12-03T08:35:00","NQTE_ROC","2010-11-08",2,-29847.35094,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1064,"TRANSGRIDV4_19000100000000","2012-12-03T11:30:00","NQTE_ROC","2010-11-08",2,-14.92351,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1065,"TRANSGRIDV4_19000100000000","2012-12-05T08:10:00","NQTE_ROC","2010-11-08",2,-14.13607,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1066,"TRANSGRIDV4_19000100000000","2012-12-05T08:40:00","NQTE_ROC","2010-11-08",2,-70.249660000000006,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1067,"TRANSGRIDV4_19000100000000","2012-12-05T09:00:00","NQTE_ROC","2010-11-08",2,-121.13661999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1068,"TRANSGRIDV4_19000100000000","2012-12-05T11:05:00","NQTE_ROC","2010-11-08",2,-16.551369999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1069,"TRANSGRIDV4_19000100000000","2012-12-05T13:25:00","NQTE_ROC","2010-11-08",2,-18.616209999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1070,"TRANSGRIDV4_19000100000000","2012-12-05T18:15:00","NQTE_ROC","2010-11-08",2,-13.71068,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1071,"TRANSGRIDV4_19000100000000","2012-12-06T08:15:00","NQTE_ROC","2010-11-08",2,-15.78009,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1072,"TRANSGRIDV4_19000100000000","2012-12-06T11:30:00","NQTE_ROC","2010-11-08",2,-10.65826,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1073,"TRANSGRIDV4_19000100000000","2012-12-06T13:15:00","NQTE_ROC","2010-11-08",2,-16.638719999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1074,"TRANSGRIDV4_19000100000000","2012-12-06T14:35:00","NQTE_ROC","2010-11-08",2,-13.68093,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1075,"TRANSGRIDV4_19000100000000","2012-12-09T13:35:00","NQTE_ROC","2010-11-08",2,-17.270579999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1076,"TRANSGRIDV4_19000100000000","2012-12-09T14:55:00","NQTE_ROC","2010-11-08",2,-16.345739999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1077,"TRANSGRIDV4_19000100000000","2012-12-09T16:35:00","NQTE_ROC","2010-11-08",2,-17.155989999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1078,"TRANSGRIDV4_19000100000000","2012-12-09T18:10:00","NQTE_ROC","2010-11-08",2,-11.00421,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1079,"TRANSGRIDV4_19000100000000","2012-12-09T18:45:00","NQTE_ROC","2010-11-08",2,-17.265499999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1080,"TRANSGRIDV4_19000100000000","2012-12-09T18:55:00","NQTE_ROC","2010-11-08",2,-14.003439999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1081,"TRANSGRIDV4_19000100000000","2012-12-29T09:05:00","NQTE_ROC","2010-11-08",2,-128.40541999999999,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1082,"TRANSGRIDV4_19000100000000","2012-10-16T15:50:00","NRM_NSW1_VIC1","2012-06-12",1,-1028.73245,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1083,"TRANSGRIDV4_19000100000000","2012-10-16T15:55:00","NRM_NSW1_VIC1","2012-06-12",1,-1030.11374,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1084,"TRANSGRIDV4_19000100000000","2012-10-16T16:00:00","NRM_NSW1_VIC1","2012-06-12",1,-1029.7644,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1085,"TRANSGRIDV4_19000100000000","2012-10-16T16:05:00","NRM_NSW1_VIC1","2012-06-12",1,-1035.64806,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1086,"TRANSGRIDV4_19000100000000","2012-10-16T16:10:00","NRM_NSW1_VIC1","2012-06-12",1,-1050.61538,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1087,"TRANSGRIDV4_19000100000000","2012-10-16T16:15:00","NRM_NSW1_VIC1","2012-06-12",1,-1053.38247,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1088,"TRANSGRIDV4_19000100000000","2012-10-16T16:20:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.7247600000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1089,"TRANSGRIDV4_19000100000000","2012-10-16T16:25:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.75701,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1090,"TRANSGRIDV4_19000100000000","2012-10-16T16:30:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.6576600000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1091,"TRANSGRIDV4_19000100000000","2012-10-16T16:35:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.5892699999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1092,"TRANSGRIDV4_19000100000000","2012-10-16T16:40:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.53288,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1093,"TRANSGRIDV4_19000100000000","2012-10-16T16:45:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.5306700000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1094,"TRANSGRIDV4_19000100000000","2012-10-16T16:50:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.5402999999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1095,"TRANSGRIDV4_19000100000000","2012-10-16T16:55:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.39228,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1096,"TRANSGRIDV4_19000100000000","2012-10-16T17:00:00","NRM_NSW1_VIC1","2012-06-12",1,-1054.4044899999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1097,"TRANSGRIDV4_19000100000000","2012-10-16T17:05:00","NRM_NSW1_VIC1","2012-06-12",1,-1035.6047100000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1098,"TRANSGRIDV4_19000100000000","2012-10-16T17:10:00","NRM_NSW1_VIC1","2012-06-12",1,-1035.6885600000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1099,"TRANSGRIDV4_19000100000000","2012-10-16T17:15:00","NRM_NSW1_VIC1","2012-06-12",1,-1045.7016799999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1100,"TRANSGRIDV4_19000100000000","2012-10-16T17:20:00","NRM_NSW1_VIC1","2012-06-12",1,-1045.7216000000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1101,"TRANSGRIDV4_19000100000000","2012-10-16T17:25:00","NRM_NSW1_VIC1","2012-06-12",1,-1035.4945600000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1102,"TRANSGRIDV4_19000100000000","2012-10-16T17:30:00","NRM_NSW1_VIC1","2012-06-12",1,-1035.47569,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1103,"TRANSGRIDV4_19000100000000","2012-08-25T09:40:00","NRM_QLD1_NSW1","2012-06-12",1,-1041.1415999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1104,"TRANSGRIDV4_19000100000000","2012-08-25T09:50:00","NRM_QLD1_NSW1","2012-06-12",1,-578.78692999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1105,"TRANSGRIDV4_19000100000000","2012-08-25T09:55:00","NRM_QLD1_NSW1","2012-06-12",1,-569.54241999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1106,"TRANSGRIDV4_19000100000000","2012-08-25T10:00:00","NRM_QLD1_NSW1","2012-06-12",1,-588.22874000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1107,"TRANSGRIDV4_19000100000000","2012-08-25T10:05:00","NRM_QLD1_NSW1","2012-06-12",1,-1089.2705599999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1108,"TRANSGRIDV4_19000100000000","2012-08-25T10:10:00","NRM_QLD1_NSW1","2012-06-12",1,-42.699750000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1109,"TRANSGRIDV4_19000100000000","2012-08-25T10:15:00","NRM_QLD1_NSW1","2012-06-12",1,-480.30721999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1110,"TRANSGRIDV4_19000100000000","2012-08-25T10:20:00","NRM_QLD1_NSW1","2012-06-12",1,-38.09299,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1111,"TRANSGRIDV4_19000100000000","2012-08-25T10:25:00","NRM_QLD1_NSW1","2012-06-12",1,-38.077570000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1112,"TRANSGRIDV4_19000100000000","2012-08-25T10:30:00","NRM_QLD1_NSW1","2012-06-12",1,-37.71575,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1113,"TRANSGRIDV4_19000100000000","2012-08-25T10:35:00","NRM_QLD1_NSW1","2012-06-12",1,-494.35816999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1114,"TRANSGRIDV4_19000100000000","2012-08-25T10:40:00","NRM_QLD1_NSW1","2012-06-12",1,-494.48243000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1115,"TRANSGRIDV4_19000100000000","2012-08-25T10:45:00","NRM_QLD1_NSW1","2012-06-12",1,-1057.44183,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1116,"TRANSGRIDV4_19000100000000","2012-08-25T10:50:00","NRM_QLD1_NSW1","2012-06-12",1,-520.90612999999996,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1117,"TRANSGRIDV4_19000100000000","2012-08-25T10:55:00","NRM_QLD1_NSW1","2012-06-12",1,-490.97548,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1118,"TRANSGRIDV4_19000100000000","2012-08-25T11:00:00","NRM_QLD1_NSW1","2012-06-12",1,-1033.9297099999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1119,"TRANSGRIDV4_19000100000000","2012-08-25T11:25:00","NRM_QLD1_NSW1","2012-06-12",1,-1088.3497600000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1120,"TRANSGRIDV4_19000100000000","2012-08-25T11:30:00","NRM_QLD1_NSW1","2012-06-12",1,-497.71575000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1121,"TRANSGRIDV4_19000100000000","2012-08-25T11:35:00","NRM_QLD1_NSW1","2012-06-12",1,-464.87382000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1122,"TRANSGRIDV4_19000100000000","2012-08-25T11:40:00","NRM_QLD1_NSW1","2012-06-12",1,-496.69905,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1123,"TRANSGRIDV4_19000100000000","2012-08-25T11:50:00","NRM_QLD1_NSW1","2012-06-12",1,-721.95995000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1124,"TRANSGRIDV4_19000100000000","2012-08-25T11:55:00","NRM_QLD1_NSW1","2012-06-12",1,-21.236930000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1125,"TRANSGRIDV4_19000100000000","2012-08-25T12:00:00","NRM_QLD1_NSW1","2012-06-12",1,-41.626240000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1126,"TRANSGRIDV4_19000100000000","2012-08-26T09:10:00","NRM_QLD1_NSW1","2012-06-12",1,-593.52904999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1127,"TRANSGRIDV4_19000100000000","2012-08-26T09:25:00","NRM_QLD1_NSW1","2012-06-12",1,-1038.9347399999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1128,"TRANSGRIDV4_19000100000000","2012-08-26T09:30:00","NRM_QLD1_NSW1","2012-06-12",1,-565.07898999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1129,"TRANSGRIDV4_19000100000000","2012-08-26T09:35:00","NRM_QLD1_NSW1","2012-06-12",1,-594.85036000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1130,"TRANSGRIDV4_19000100000000","2012-08-26T09:40:00","NRM_QLD1_NSW1","2012-06-12",1,-587.03877,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1131,"TRANSGRIDV4_19000100000000","2012-08-26T09:45:00","NRM_QLD1_NSW1","2012-06-12",1,-47.406120000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1132,"TRANSGRIDV4_19000100000000","2012-08-26T09:50:00","NRM_QLD1_NSW1","2012-06-12",1,-476.00515000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1133,"TRANSGRIDV4_19000100000000","2012-08-26T09:55:00","NRM_QLD1_NSW1","2012-06-12",1,-43.954009999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1134,"TRANSGRIDV4_19000100000000","2012-08-26T10:00:00","NRM_QLD1_NSW1","2012-06-12",1,-47.29016,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1135,"TRANSGRIDV4_19000100000000","2012-08-26T10:50:00","NRM_QLD1_NSW1","2012-06-12",1,-1095.4633799999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1136,"TRANSGRIDV4_19000100000000","2012-08-26T10:55:00","NRM_QLD1_NSW1","2012-06-12",1,-1119.5019400000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1137,"TRANSGRIDV4_19000100000000","2012-08-26T11:00:00","NRM_QLD1_NSW1","2012-06-12",1,-1116.27981,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1138,"TRANSGRIDV4_19000100000000","2012-08-26T11:05:00","NRM_QLD1_NSW1","2012-06-12",1,-602.89724999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1139,"TRANSGRIDV4_19000100000000","2012-08-26T11:10:00","NRM_QLD1_NSW1","2012-06-12",1,-593.81392000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1140,"TRANSGRIDV4_19000100000000","2012-08-26T11:15:00","NRM_QLD1_NSW1","2012-06-12",1,-447.34307000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1141,"TRANSGRIDV4_19000100000000","2012-08-30T13:10:00","NRM_QLD1_NSW1","2012-06-12",1,-605.56705999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1142,"TRANSGRIDV4_19000100000000","2012-08-30T13:15:00","NRM_QLD1_NSW1","2012-06-12",1,-1081.7374299999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1143,"TRANSGRIDV4_19000100000000","2012-08-30T13:20:00","NRM_QLD1_NSW1","2012-06-12",1,-1090.0785599999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1144,"TRANSGRIDV4_19000100000000","2012-08-30T13:25:00","NRM_QLD1_NSW1","2012-06-12",1,-1087.69228,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1145,"TRANSGRIDV4_19000100000000","2012-08-30T13:30:00","NRM_QLD1_NSW1","2012-06-12",1,-1085.0323100000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1146,"TRANSGRIDV4_19000100000000","2012-08-30T13:35:00","NRM_QLD1_NSW1","2012-06-12",1,-10.82443,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1147,"TRANSGRIDV4_19000100000000","2012-08-30T13:45:00","NRM_QLD1_NSW1","2012-06-12",1,-11.57701,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1148,"TRANSGRIDV4_19000100000000","2012-08-30T13:50:00","NRM_QLD1_NSW1","2012-06-12",1,-12.96316,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1149,"TRANSGRIDV4_19000100000000","2012-08-30T13:55:00","NRM_QLD1_NSW1","2012-06-12",1,-13.30931,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1150,"TRANSGRIDV4_19000100000000","2012-08-30T14:00:00","NRM_QLD1_NSW1","2012-06-12",1,-11.94689,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1151,"TRANSGRIDV4_19000100000000","2012-08-30T14:05:00","NRM_QLD1_NSW1","2012-06-12",1,-12.671580000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1152,"TRANSGRIDV4_19000100000000","2012-08-30T14:10:00","NRM_QLD1_NSW1","2012-06-12",1,-12.82823,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1153,"TRANSGRIDV4_19000100000000","2012-08-30T14:15:00","NRM_QLD1_NSW1","2012-06-12",1,-12.33494,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1154,"TRANSGRIDV4_19000100000000","2012-08-30T14:20:00","NRM_QLD1_NSW1","2012-06-12",1,-11.718109999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1155,"TRANSGRIDV4_19000100000000","2012-08-31T10:05:00","NRM_QLD1_NSW1","2012-06-12",1,-43.417859999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1156,"TRANSGRIDV4_19000100000000","2012-08-31T10:10:00","NRM_QLD1_NSW1","2012-06-12",1,-22.20823,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1157,"TRANSGRIDV4_19000100000000","2012-08-31T10:25:00","NRM_QLD1_NSW1","2012-06-12",1,-18.25648,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1158,"TRANSGRIDV4_19000100000000","2012-08-31T12:35:00","NRM_QLD1_NSW1","2012-06-12",1,-22.180009999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1159,"TRANSGRIDV4_19000100000000","2012-09-01T09:10:00","NRM_QLD1_NSW1","2012-06-12",1,-1066.30052,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1160,"TRANSGRIDV4_19000100000000","2012-09-01T09:15:00","NRM_QLD1_NSW1","2012-06-12",1,-1066.6656,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1161,"TRANSGRIDV4_19000100000000","2012-09-01T09:20:00","NRM_QLD1_NSW1","2012-06-12",1,-30.20758,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1162,"TRANSGRIDV4_19000100000000","2012-09-01T09:35:00","NRM_QLD1_NSW1","2012-06-12",1,-506.72403000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1163,"TRANSGRIDV4_19000100000000","2012-09-01T09:40:00","NRM_QLD1_NSW1","2012-06-12",1,-47.821620000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1164,"TRANSGRIDV4_19000100000000","2012-09-01T09:45:00","NRM_QLD1_NSW1","2012-06-12",1,-12.231249999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1165,"TRANSGRIDV4_19000100000000","2012-09-01T10:00:00","NRM_QLD1_NSW1","2012-06-12",1,-11.20097,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1166,"TRANSGRIDV4_19000100000000","2012-09-01T11:45:00","NRM_QLD1_NSW1","2012-06-12",1,-41.619959999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1167,"TRANSGRIDV4_19000100000000","2012-09-01T11:50:00","NRM_QLD1_NSW1","2012-06-12",1,-1062.3143299999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1168,"TRANSGRIDV4_19000100000000","2012-09-01T11:55:00","NRM_QLD1_NSW1","2012-06-12",1,-1101.57232,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1169,"TRANSGRIDV4_19000100000000","2012-09-01T12:00:00","NRM_QLD1_NSW1","2012-06-12",1,-1095.84707,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1170,"TRANSGRIDV4_19000100000000","2012-09-01T12:05:00","NRM_QLD1_NSW1","2012-06-12",1,-23.874659999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1171,"TRANSGRIDV4_19000100000000","2012-09-01T12:10:00","NRM_QLD1_NSW1","2012-06-12",1,-20.95007,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1172,"TRANSGRIDV4_19000100000000","2012-09-01T12:15:00","NRM_QLD1_NSW1","2012-06-12",1,-21.128080000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1173,"TRANSGRIDV4_19000100000000","2012-09-01T12:25:00","NRM_QLD1_NSW1","2012-06-12",1,-14.287990000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1174,"TRANSGRIDV4_19000100000000","2012-09-03T09:55:00","NRM_QLD1_NSW1","2012-06-12",1,-579.41629999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1175,"TRANSGRIDV4_19000100000000","2012-09-03T10:00:00","NRM_QLD1_NSW1","2012-06-12",1,-593.38220000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1176,"TRANSGRIDV4_19000100000000","2012-09-03T10:05:00","NRM_QLD1_NSW1","2012-06-12",1,-480.9796,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1177,"TRANSGRIDV4_19000100000000","2012-09-03T10:10:00","NRM_QLD1_NSW1","2012-06-12",1,-15.284689999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1178,"TRANSGRIDV4_19000100000000","2012-09-03T10:15:00","NRM_QLD1_NSW1","2012-06-12",1,-17.440390000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1179,"TRANSGRIDV4_19000100000000","2012-09-03T10:35:00","NRM_QLD1_NSW1","2012-06-12",1,-18.249510000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1180,"TRANSGRIDV4_19000100000000","2012-09-03T10:40:00","NRM_QLD1_NSW1","2012-06-12",1,-21.058859999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1181,"TRANSGRIDV4_19000100000000","2012-09-03T10:45:00","NRM_QLD1_NSW1","2012-06-12",1,-19.085650000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1182,"TRANSGRIDV4_19000100000000","2012-09-03T10:50:00","NRM_QLD1_NSW1","2012-06-12",1,-20.9695,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1183,"TRANSGRIDV4_19000100000000","2012-09-03T10:55:00","NRM_QLD1_NSW1","2012-06-12",1,-14.63017,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1184,"TRANSGRIDV4_19000100000000","2012-09-03T12:05:00","NRM_QLD1_NSW1","2012-06-12",1,-487.19324999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1185,"TRANSGRIDV4_19000100000000","2012-09-03T12:20:00","NRM_QLD1_NSW1","2012-06-12",1,-863.53794000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1186,"TRANSGRIDV4_19000100000000","2012-09-03T12:25:00","NRM_QLD1_NSW1","2012-06-12",1,-1091.3316400000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1187,"TRANSGRIDV4_19000100000000","2012-09-03T12:30:00","NRM_QLD1_NSW1","2012-06-12",1,-1076.29261,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1188,"TRANSGRIDV4_19000100000000","2012-09-03T12:35:00","NRM_QLD1_NSW1","2012-06-12",1,-56.956440000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1189,"TRANSGRIDV4_19000100000000","2012-09-03T12:40:00","NRM_QLD1_NSW1","2012-06-12",1,-56.139189999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1190,"TRANSGRIDV4_19000100000000","2012-09-03T12:45:00","NRM_QLD1_NSW1","2012-06-12",1,-41.860340000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1191,"TRANSGRIDV4_19000100000000","2012-09-03T12:50:00","NRM_QLD1_NSW1","2012-06-12",1,-64.962159999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1192,"TRANSGRIDV4_19000100000000","2012-09-03T12:55:00","NRM_QLD1_NSW1","2012-06-12",1,-602.67074000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1193,"TRANSGRIDV4_19000100000000","2012-09-03T13:05:00","NRM_QLD1_NSW1","2012-06-12",1,-537.17791999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1194,"TRANSGRIDV4_19000100000000","2012-09-03T13:10:00","NRM_QLD1_NSW1","2012-06-12",1,-37.426969999999997,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1195,"TRANSGRIDV4_19000100000000","2012-09-03T13:15:00","NRM_QLD1_NSW1","2012-06-12",1,-41.001339999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1196,"TRANSGRIDV4_19000100000000","2012-09-03T13:20:00","NRM_QLD1_NSW1","2012-06-12",1,-42.511000000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1197,"TRANSGRIDV4_19000100000000","2012-09-03T13:25:00","NRM_QLD1_NSW1","2012-06-12",1,-33.44726,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1198,"TRANSGRIDV4_19000100000000","2012-09-03T13:30:00","NRM_QLD1_NSW1","2012-06-12",1,-35.869520000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1199,"TRANSGRIDV4_19000100000000","2012-09-03T16:35:00","NRM_QLD1_NSW1","2012-06-12",1,-51.298490000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1200,"TRANSGRIDV4_19000100000000","2012-09-03T16:45:00","NRM_QLD1_NSW1","2012-06-12",1,-15.844569999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1201,"TRANSGRIDV4_19000100000000","2012-09-03T16:50:00","NRM_QLD1_NSW1","2012-06-12",1,-17.79008,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1202,"TRANSGRIDV4_19000100000000","2012-09-03T16:55:00","NRM_QLD1_NSW1","2012-06-12",1,-15.37993,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1203,"TRANSGRIDV4_19000100000000","2012-09-03T17:00:00","NRM_QLD1_NSW1","2012-06-12",1,-19.147680000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1204,"TRANSGRIDV4_19000100000000","2012-09-06T09:35:00","NRM_QLD1_NSW1","2012-06-12",1,-1035.6104800000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1205,"TRANSGRIDV4_19000100000000","2012-09-06T09:45:00","NRM_QLD1_NSW1","2012-06-12",1,-46.00929,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1206,"TRANSGRIDV4_19000100000000","2012-09-06T09:50:00","NRM_QLD1_NSW1","2012-06-12",1,-45.872630000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1207,"TRANSGRIDV4_19000100000000","2012-09-06T09:55:00","NRM_QLD1_NSW1","2012-06-12",1,-36.242040000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1208,"TRANSGRIDV4_19000100000000","2012-09-06T10:00:00","NRM_QLD1_NSW1","2012-06-12",1,-12.678979999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1209,"TRANSGRIDV4_19000100000000","2012-09-06T10:05:00","NRM_QLD1_NSW1","2012-06-12",1,-12.25662,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1210,"TRANSGRIDV4_19000100000000","2012-09-06T10:10:00","NRM_QLD1_NSW1","2012-06-12",1,-10.170669999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1211,"TRANSGRIDV4_19000100000000","2012-09-06T10:25:00","NRM_QLD1_NSW1","2012-06-12",1,-10.51661,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1212,"TRANSGRIDV4_19000100000000","2012-09-06T10:30:00","NRM_QLD1_NSW1","2012-06-12",1,-50.269539999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1213,"TRANSGRIDV4_19000100000000","2012-09-08T13:10:00","NRM_QLD1_NSW1","2012-06-12",1,-474.45195000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1214,"TRANSGRIDV4_19000100000000","2012-09-08T13:15:00","NRM_QLD1_NSW1","2012-06-12",1,-167.35471000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1215,"TRANSGRIDV4_19000100000000","2012-09-08T13:20:00","NRM_QLD1_NSW1","2012-06-12",1,-161.69149999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1216,"TRANSGRIDV4_19000100000000","2012-09-08T13:25:00","NRM_QLD1_NSW1","2012-06-12",1,-165.59470999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1217,"TRANSGRIDV4_19000100000000","2012-09-08T13:35:00","NRM_QLD1_NSW1","2012-06-12",1,-43.80462,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1218,"TRANSGRIDV4_19000100000000","2012-09-08T13:45:00","NRM_QLD1_NSW1","2012-06-12",1,-21.472750000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1219,"TRANSGRIDV4_19000100000000","2012-09-08T13:50:00","NRM_QLD1_NSW1","2012-06-12",1,-20.864809999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1220,"TRANSGRIDV4_19000100000000","2012-09-08T13:55:00","NRM_QLD1_NSW1","2012-06-12",1,-20.844439999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1221,"TRANSGRIDV4_19000100000000","2012-09-08T14:00:00","NRM_QLD1_NSW1","2012-06-12",1,-12.66441,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1222,"TRANSGRIDV4_19000100000000","2012-09-08T14:10:00","NRM_QLD1_NSW1","2012-06-12",1,-1033.9810600000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1223,"TRANSGRIDV4_19000100000000","2012-09-08T14:15:00","NRM_QLD1_NSW1","2012-06-12",1,-11.93515,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1224,"TRANSGRIDV4_19000100000000","2012-09-08T14:25:00","NRM_QLD1_NSW1","2012-06-12",1,-171.20841999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1225,"TRANSGRIDV4_19000100000000","2012-09-08T14:30:00","NRM_QLD1_NSW1","2012-06-12",1,-47.512810000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1226,"TRANSGRIDV4_19000100000000","2012-09-08T14:35:00","NRM_QLD1_NSW1","2012-06-12",1,-46.806429999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1227,"TRANSGRIDV4_19000100000000","2012-09-08T14:40:00","NRM_QLD1_NSW1","2012-06-12",1,-22.69041,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1228,"TRANSGRIDV4_19000100000000","2012-09-08T14:45:00","NRM_QLD1_NSW1","2012-06-12",1,-23.098939999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1229,"TRANSGRIDV4_19000100000000","2012-09-08T14:50:00","NRM_QLD1_NSW1","2012-06-12",1,-23.064,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1230,"TRANSGRIDV4_19000100000000","2012-09-08T14:55:00","NRM_QLD1_NSW1","2012-06-12",1,-24.354620000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1231,"TRANSGRIDV4_19000100000000","2012-09-08T15:00:00","NRM_QLD1_NSW1","2012-06-12",1,-24.535119999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1232,"TRANSGRIDV4_19000100000000","2012-09-08T15:05:00","NRM_QLD1_NSW1","2012-06-12",1,-22.916920000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1233,"TRANSGRIDV4_19000100000000","2012-09-08T15:10:00","NRM_QLD1_NSW1","2012-06-12",1,-23.643419999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1234,"TRANSGRIDV4_19000100000000","2012-09-08T15:15:00","NRM_QLD1_NSW1","2012-06-12",1,-23.42822,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1235,"TRANSGRIDV4_19000100000000","2012-09-08T15:20:00","NRM_QLD1_NSW1","2012-06-12",1,-23.184270000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1236,"TRANSGRIDV4_19000100000000","2012-10-21T13:15:00","NRM_QLD1_NSW1","2012-06-12",1,-161.62036000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1237,"TRANSGRIDV4_19000100000000","2012-10-21T13:20:00","NRM_QLD1_NSW1","2012-06-12",1,-56.693179999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1238,"TRANSGRIDV4_19000100000000","2012-10-21T13:25:00","NRM_QLD1_NSW1","2012-06-12",1,-30.072410000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1239,"TRANSGRIDV4_19000100000000","2012-10-21T13:30:00","NRM_QLD1_NSW1","2012-06-12",1,-31.64,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1240,"TRANSGRIDV4_19000100000000","2012-10-21T13:40:00","NRM_QLD1_NSW1","2012-06-12",1,-26.09581,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1241,"TRANSGRIDV4_19000100000000","2012-10-21T13:45:00","NRM_QLD1_NSW1","2012-06-12",1,-20.130569999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1242,"TRANSGRIDV4_19000100000000","2012-10-21T13:50:00","NRM_QLD1_NSW1","2012-06-12",1,-26.65091,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1243,"TRANSGRIDV4_19000100000000","2012-10-21T13:55:00","NRM_QLD1_NSW1","2012-06-12",1,-25.243659999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1244,"TRANSGRIDV4_19000100000000","2012-10-21T14:00:00","NRM_QLD1_NSW1","2012-06-12",1,-121.79210999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1245,"TRANSGRIDV4_19000100000000","2012-10-27T12:15:00","NRM_QLD1_NSW1","2012-06-12",1,-40.945869999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1246,"TRANSGRIDV4_19000100000000","2012-10-27T12:20:00","NRM_QLD1_NSW1","2012-06-12",1,-20.890969999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1247,"TRANSGRIDV4_19000100000000","2012-10-27T12:25:00","NRM_QLD1_NSW1","2012-06-12",1,-573.49203,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1248,"TRANSGRIDV4_19000100000000","2012-10-27T12:35:00","NRM_QLD1_NSW1","2012-06-12",1,-576.11377000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1249,"TRANSGRIDV4_19000100000000","2012-10-27T12:45:00","NRM_QLD1_NSW1","2012-06-12",1,-20.682130000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1250,"TRANSGRIDV4_19000100000000","2012-10-27T12:50:00","NRM_QLD1_NSW1","2012-06-12",1,-705.97008000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1251,"TRANSGRIDV4_19000100000000","2012-10-27T12:55:00","NRM_QLD1_NSW1","2012-06-12",1,-703.07743000000005,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1252,"TRANSGRIDV4_19000100000000","2012-10-27T13:00:00","NRM_QLD1_NSW1","2012-06-12",1,-27.124210000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1253,"TRANSGRIDV4_19000100000000","2012-10-27T13:20:00","NRM_QLD1_NSW1","2012-06-12",1,-147.71044000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1254,"TRANSGRIDV4_19000100000000","2012-10-27T14:45:00","NRM_QLD1_NSW1","2012-06-12",1,-34.204500000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1255,"TRANSGRIDV4_19000100000000","2012-10-27T14:50:00","NRM_QLD1_NSW1","2012-06-12",1,-53.800220000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1256,"TRANSGRIDV4_19000100000000","2012-10-27T14:55:00","NRM_QLD1_NSW1","2012-06-12",1,-708.75197000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1257,"TRANSGRIDV4_19000100000000","2012-10-27T15:00:00","NRM_QLD1_NSW1","2012-06-12",1,-26.135739999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1258,"TRANSGRIDV4_19000100000000","2012-12-03T09:00:00","NRM_QLD1_NSW1","2012-06-12",1,-12.27571,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1259,"TRANSGRIDV4_19000100000000","2012-12-03T09:05:00","NRM_QLD1_NSW1","2012-06-12",1,-10.414630000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1260,"TRANSGRIDV4_19000100000000","2012-12-03T14:20:00","NRM_QLD1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1261,"TRANSGRIDV4_19000100000000","2012-12-03T14:25:00","NRM_QLD1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1262,"TRANSGRIDV4_19000100000000","2012-12-03T14:30:00","NRM_QLD1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1263,"TRANSGRIDV4_19000100000000","2012-12-03T14:35:00","NRM_QLD1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1264,"TRANSGRIDV4_19000100000000","2012-12-03T14:40:00","NRM_QLD1_NSW1","2012-06-12",1,-16.376650000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1265,"TRANSGRIDV4_19000100000000","2012-12-03T14:45:00","NRM_QLD1_NSW1","2012-06-12",1,-15.63978,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1266,"TRANSGRIDV4_19000100000000","2012-12-03T14:50:00","NRM_QLD1_NSW1","2012-06-12",1,-16.07,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1267,"TRANSGRIDV4_19000100000000","2012-12-03T14:55:00","NRM_QLD1_NSW1","2012-06-12",1,-34.27505,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1268,"TRANSGRIDV4_19000100000000","2012-12-03T15:00:00","NRM_QLD1_NSW1","2012-06-12",1,-53.673839999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1269,"TRANSGRIDV4_19000100000000","2012-12-05T11:40:00","NRM_QLD1_NSW1","2012-06-12",1,-14.171329999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1270,"TRANSGRIDV4_19000100000000","2012-12-05T11:45:00","NRM_QLD1_NSW1","2012-06-12",1,-477.89057000000003,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1271,"TRANSGRIDV4_19000100000000","2012-12-05T11:50:00","NRM_QLD1_NSW1","2012-06-12",1,-1039.95758,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1272,"TRANSGRIDV4_19000100000000","2012-12-05T11:55:00","NRM_QLD1_NSW1","2012-06-12",1,-17.825849999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1273,"TRANSGRIDV4_19000100000000","2012-12-05T12:00:00","NRM_QLD1_NSW1","2012-06-12",1,-12.446020000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1274,"TRANSGRIDV4_19000100000000","2012-12-05T12:05:00","NRM_QLD1_NSW1","2012-06-12",1,-10.27975,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1275,"TRANSGRIDV4_19000100000000","2012-12-05T12:10:00","NRM_QLD1_NSW1","2012-06-12",1,-13.77787,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1276,"TRANSGRIDV4_19000100000000","2012-12-05T12:15:00","NRM_QLD1_NSW1","2012-06-12",1,-10.34131,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1277,"TRANSGRIDV4_19000100000000","2012-12-05T12:20:00","NRM_QLD1_NSW1","2012-06-12",1,-48.08943,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1278,"TRANSGRIDV4_19000100000000","2012-12-05T12:30:00","NRM_QLD1_NSW1","2012-06-12",1,-19.985440000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1279,"TRANSGRIDV4_19000100000000","2012-12-05T12:35:00","NRM_QLD1_NSW1","2012-06-12",1,-14.65488,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1280,"TRANSGRIDV4_19000100000000","2012-12-05T12:45:00","NRM_QLD1_NSW1","2012-06-12",1,-13.93239,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1281,"TRANSGRIDV4_19000100000000","2012-12-05T12:50:00","NRM_QLD1_NSW1","2012-06-12",1,-11.349539999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1282,"TRANSGRIDV4_19000100000000","2012-12-05T12:55:00","NRM_QLD1_NSW1","2012-06-12",1,-14.519270000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1283,"TRANSGRIDV4_19000100000000","2012-12-05T13:00:00","NRM_QLD1_NSW1","2012-06-12",1,-11.03275,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1284,"TRANSGRIDV4_19000100000000","2012-12-05T14:35:00","NRM_QLD1_NSW1","2012-06-12",1,-1063.43,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1285,"TRANSGRIDV4_19000100000000","2012-12-05T14:45:00","NRM_QLD1_NSW1","2012-06-12",1,-745.70659999999998,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1286,"TRANSGRIDV4_19000100000000","2012-12-05T14:50:00","NRM_QLD1_NSW1","2012-06-12",1,-250.56057000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1287,"TRANSGRIDV4_19000100000000","2012-12-05T14:55:00","NRM_QLD1_NSW1","2012-06-12",1,-146.47807,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1288,"TRANSGRIDV4_19000100000000","2012-12-05T15:00:00","NRM_QLD1_NSW1","2012-06-12",1,-25.82892,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1289,"TRANSGRIDV4_19000100000000","2012-12-05T15:05:00","NRM_QLD1_NSW1","2012-06-12",1,-27.748809999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1290,"TRANSGRIDV4_19000100000000","2012-12-05T15:10:00","NRM_QLD1_NSW1","2012-06-12",1,-27.098510000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1291,"TRANSGRIDV4_19000100000000","2012-12-05T15:15:00","NRM_QLD1_NSW1","2012-06-12",1,-26.350570000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1292,"TRANSGRIDV4_19000100000000","2012-12-05T15:20:00","NRM_QLD1_NSW1","2012-06-12",1,-19.48114,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1293,"TRANSGRIDV4_19000100000000","2012-09-11T09:10:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1294,"TRANSGRIDV4_19000100000000","2012-09-11T09:15:00","NRM_VIC1_NSW1","2012-06-12",1,-46.206420000000001,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1295,"TRANSGRIDV4_19000100000000","2012-09-11T09:20:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1296,"TRANSGRIDV4_19000100000000","2012-09-11T09:25:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1297,"TRANSGRIDV4_19000100000000","2012-09-11T09:30:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1298,"TRANSGRIDV4_19000100000000","2012-09-11T09:35:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1299,"TRANSGRIDV4_19000100000000","2012-09-11T09:45:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1300,"TRANSGRIDV4_19000100000000","2012-09-11T09:50:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1301,"TRANSGRIDV4_19000100000000","2012-09-11T09:55:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1302,"TRANSGRIDV4_19000100000000","2012-09-11T10:00:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1303,"TRANSGRIDV4_19000100000000","2012-09-11T10:05:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1304,"TRANSGRIDV4_19000100000000","2012-09-11T10:10:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1305,"TRANSGRIDV4_19000100000000","2012-09-11T10:15:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1306,"TRANSGRIDV4_19000100000000","2012-09-11T10:20:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1307,"TRANSGRIDV4_19000100000000","2012-09-11T10:25:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1308,"TRANSGRIDV4_19000100000000","2012-09-11T10:30:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1309,"TRANSGRIDV4_19000100000000","2012-09-11T10:35:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1310,"TRANSGRIDV4_19000100000000","2012-09-11T10:40:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1311,"TRANSGRIDV4_19000100000000","2012-09-11T10:45:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1312,"TRANSGRIDV4_19000100000000","2012-09-11T10:50:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1313,"TRANSGRIDV4_19000100000000","2012-09-11T10:55:00","NRM_VIC1_NSW1","2012-06-12",1,-46.920029999999997,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1314,"TRANSGRIDV4_19000100000000","2012-09-11T11:05:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1315,"TRANSGRIDV4_19000100000000","2012-09-11T11:10:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1316,"TRANSGRIDV4_19000100000000","2012-09-11T11:15:00","NRM_VIC1_NSW1","2012-06-12",1,-44.375169999999997,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1317,"TRANSGRIDV4_19000100000000","2012-09-11T11:25:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1318,"TRANSGRIDV4_19000100000000","2012-09-11T11:30:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1319,"TRANSGRIDV4_19000100000000","2012-09-11T11:35:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1320,"TRANSGRIDV4_19000100000000","2012-09-11T11:40:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1321,"TRANSGRIDV4_19000100000000","2012-09-11T11:50:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1322,"TRANSGRIDV4_19000100000000","2012-09-11T11:55:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1323,"TRANSGRIDV4_19000100000000","2012-09-11T12:00:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1324,"TRANSGRIDV4_19000100000000","2012-09-11T12:05:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1325,"TRANSGRIDV4_19000100000000","2012-09-11T12:10:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1326,"TRANSGRIDV4_19000100000000","2012-09-11T12:15:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1327,"TRANSGRIDV4_19000100000000","2012-09-11T12:20:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1328,"TRANSGRIDV4_19000100000000","2012-09-11T12:25:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1329,"TRANSGRIDV4_19000100000000","2012-09-11T12:30:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1330,"TRANSGRIDV4_19000100000000","2012-09-11T12:35:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1331,"TRANSGRIDV4_19000100000000","2012-09-11T12:40:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1332,"TRANSGRIDV4_19000100000000","2012-09-11T12:45:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1333,"TRANSGRIDV4_19000100000000","2012-09-11T12:50:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1334,"TRANSGRIDV4_19000100000000","2012-09-11T12:55:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1335,"TRANSGRIDV4_19000100000000","2012-09-11T13:00:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1336,"TRANSGRIDV4_19000100000000","2012-09-11T13:05:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1337,"TRANSGRIDV4_19000100000000","2012-09-11T13:10:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1338,"TRANSGRIDV4_19000100000000","2012-09-11T13:15:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1339,"TRANSGRIDV4_19000100000000","2012-09-11T13:20:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1340,"TRANSGRIDV4_19000100000000","2012-09-11T13:25:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1341,"TRANSGRIDV4_19000100000000","2012-09-11T13:30:00","NRM_VIC1_NSW1","2012-06-12",1,-51.009120000000003,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1342,"TRANSGRIDV4_19000100000000","2012-09-11T13:35:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1343,"TRANSGRIDV4_19000100000000","2012-09-11T13:40:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1344,"TRANSGRIDV4_19000100000000","2012-09-11T14:40:00","NRM_VIC1_NSW1","2012-06-12",1,-25800,"Negative Residue Management constraint for VIC to NSW flow","SYSTEM NORMAL","NRM","","REGULATED",null,null,0]
[1345,"TRANSGRIDV4_19000100000000","2012-06-19T21:35:00","NV_0000","2009-04-20",1,-29.55245,"Discretionary NSW to Vic transfer upper limit of    0 MW","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1346,"TRANSGRIDV4_19000100000000","2012-06-19T21:40:00","NV_0000","2009-04-20",1,-16.283840000000001,"Discretionary NSW to Vic transfer upper limit of    0 MW","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1347,"TRANSGRIDV4_19000100000000","2012-06-19T21:45:00","NV_0000","2009-04-20",1,-13.63519,"Discretionary NSW to Vic transfer upper limit of    0 MW","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1348,"TRANSGRIDV4_19000100000000","2012-06-19T21:50:00","NV_0000","2009-04-20",1,-18.37227,"Discretionary NSW to Vic transfer upper limit of    0 MW","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1349,"TRANSGRIDV4_19000100000000","2012-08-25T12:10:00","QNTE_ROC","2010-11-08",3,-355.28537999999998,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1350,"TRANSGRIDV4_19000100000000","2012-08-25T12:55:00","QNTE_ROC","2010-11-08",3,-833.34824000000003,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1351,"TRANSGRIDV4_19000100000000","2012-09-03T11:30:00","QNTE_ROC","2010-11-08",3,-20.531289999999998,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1352,"TRANSGRIDV4_19000100000000","2012-09-03T15:05:00","QNTE_ROC","2010-11-08",3,-23.489889999999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1353,"TRANSGRIDV4_19000100000000","2012-09-07T10:00:00","QNTE_ROC","2010-11-08",3,-26.081009999999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1354,"TRANSGRIDV4_19000100000000","2012-09-09T12:35:00","QNTE_ROC","2010-11-08",3,-22.560459999999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1355,"TRANSGRIDV4_19000100000000","2012-10-27T11:25:00","QNTE_ROC","2010-11-08",3,-11.92348,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1356,"TRANSGRIDV4_19000100000000","2012-12-05T08:35:00","QNTE_ROC","2010-11-08",3,-257975.52874000001,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1357,"TRANSGRIDV4_19000100000000","2012-12-05T08:55:00","QNTE_ROC","2010-11-08",3,-257854.63834999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1358,"TRANSGRIDV4_19000100000000","2012-12-06T11:45:00","QNTE_ROC","2010-11-08",3,-257979.33663999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1359,"TRANSGRIDV4_19000100000000","2012-12-06T13:05:00","QNTE_ROC","2010-11-08",3,-258005.02262999999,"Out=Nil, Rate of Change (Qld to NSW) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER","","REGULATED",null,null,0]
[1360,"TRANSGRIDV4_19000100000000","2012-05-20T17:20:00","V::N_LTMSQE_R","2012-02-16",1,-13.69631,"Out = Lower Tumut to Murray 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Lower Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1361,"TRANSGRIDV4_19000100000000","2012-05-20T17:25:00","V::N_LTMSQE_R","2012-02-16",1,-14.43253,"Out = Lower Tumut to Murray 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Lower Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1362,"TRANSGRIDV4_19000100000000","2012-05-20T17:30:00","V::N_LTMSQE_R","2012-02-16",1,-14.89481,"Out = Lower Tumut to Murray 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Lower Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1363,"TRANSGRIDV4_19000100000000","2012-05-20T17:40:00","V::N_LTMSQE_R","2012-02-16",1,-11.348420000000001,"Out = Lower Tumut to Murray 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Lower Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1364,"TRANSGRIDV4_19000100000000","2012-05-01T06:45:00","V::N_MSUTQD_R","2012-02-16",1,-10.698180000000001,"Outage = Upper Tumut to Murray 330kV line, limit Vic generators and interconnectors avoid avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Radial","OUTAGE","OTHER","Upper Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1365,"TRANSGRIDV4_19000100000000","2012-05-01T06:50:00","V::N_MSUTQD_R","2012-02-16",1,-15.72678,"Outage = Upper Tumut to Murray 330kV line, limit Vic generators and interconnectors avoid avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Radial","OUTAGE","OTHER","Upper Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1366,"TRANSGRIDV4_19000100000000","2012-05-19T17:25:00","V::N_MSUTQE_R","2012-02-16",1,-12.27642,"Outage = Upper Tumut to Murray 330kV line, limit Vic generators and interconnectors avoid avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Radial","OUTAGE","OTHER","Upper Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1367,"TRANSGRIDV4_19000100000000","2012-05-19T17:30:00","V::N_MSUTQE_R","2012-02-16",1,-10.76427,"Outage = Upper Tumut to Murray 330kV line, limit Vic generators and interconnectors avoid avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Radial","OUTAGE","OTHER","Upper Tumut To Murray 330Kv Line","REGULATED",null,null,1]
[1368,"TRANSGRIDV4_19000100000000","2012-03-31T06:25:00","V>>N_DDMS_2","2012-02-28",1,-13.959379999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1369,"TRANSGRIDV4_19000100000000","2012-03-31T06:30:00","V>>N_DDMS_2","2012-02-28",1,-14.112159999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1370,"TRANSGRIDV4_19000100000000","2012-03-31T06:35:00","V>>N_DDMS_2","2012-02-28",1,-16.353010000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1371,"TRANSGRIDV4_19000100000000","2012-03-31T06:40:00","V>>N_DDMS_2","2012-02-28",1,-12.99713,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1372,"TRANSGRIDV4_19000100000000","2012-03-31T06:45:00","V>>N_DDMS_2","2012-02-28",1,-11.05832,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1373,"TRANSGRIDV4_19000100000000","2012-03-31T06:50:00","V>>N_DDMS_2","2012-02-28",1,-16.044450000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1374,"TRANSGRIDV4_19000100000000","2012-03-31T06:55:00","V>>N_DDMS_2","2012-02-28",1,-15.40211,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1375,"TRANSGRIDV4_19000100000000","2012-03-31T07:00:00","V>>N_DDMS_2","2012-02-28",1,-11.56892,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1376,"TRANSGRIDV4_19000100000000","2012-03-31T07:05:00","V>>N_DDMS_2","2012-02-28",1,-13.424569999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1377,"TRANSGRIDV4_19000100000000","2012-03-31T07:10:00","V>>N_DDMS_2","2012-02-28",1,-13.56521,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1378,"TRANSGRIDV4_19000100000000","2012-03-31T08:10:00","V>>N_DDMS_2","2012-02-28",1,-23.953340000000001,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1379,"TRANSGRIDV4_19000100000000","2012-04-01T07:10:00","V>>N_DDMS_2","2012-02-28",1,-13.65185,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1380,"TRANSGRIDV4_19000100000000","2012-04-01T07:15:00","V>>N_DDMS_2","2012-02-28",1,-14.296849999999999,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1381,"TRANSGRIDV4_19000100000000","2012-04-01T07:20:00","V>>N_DDMS_2","2012-02-28",1,-11.63565,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1382,"TRANSGRIDV4_19000100000000","2012-04-01T07:30:00","V>>N_DDMS_2","2012-02-28",1,-13.04875,"Out = Dederang to Murray 330 kV line, avoid O/L Dederang to Wodonga 330 kV line (flow North) for trip the remaining Murray to Dederang 330 kV line, feedback","OUTAGE","OTHER","Dederang To Murray 330 Kv Line","REGULATED",null,null,1]
[1383,"TRANSGRIDV4_19000100000000","2012-10-05T11:35:00","V>>N-LTMS_1","2010-12-07",2,-10.18805,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1384,"TRANSGRIDV4_19000100000000","2012-10-05T11:50:00","V>>N-LTMS_1","2010-12-07",2,-11.523770000000001,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1385,"TRANSGRIDV4_19000100000000","2012-10-05T12:05:00","V>>N-LTMS_1","2010-12-07",2,-11.4474,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1386,"TRANSGRIDV4_19000100000000","2012-10-05T12:10:00","V>>N-LTMS_1","2010-12-07",2,-28.931899999999999,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1387,"TRANSGRIDV4_19000100000000","2012-10-05T12:15:00","V>>N-LTMS_1","2010-12-07",2,-20.844259999999998,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1388,"TRANSGRIDV4_19000100000000","2012-10-05T12:25:00","V>>N-LTMS_1","2010-12-07",2,-13.92759,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1389,"TRANSGRIDV4_19000100000000","2012-10-05T12:35:00","V>>N-LTMS_1","2010-12-07",2,-23.605090000000001,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1390,"TRANSGRIDV4_19000100000000","2012-10-05T12:45:00","V>>N-LTMS_1","2010-12-07",2,-28.617149999999999,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1391,"TRANSGRIDV4_19000100000000","2012-10-05T12:50:00","V>>N-LTMS_1","2010-12-07",2,-31.282250000000001,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1392,"TRANSGRIDV4_19000100000000","2012-10-05T13:00:00","V>>N-LTMS_1","2010-12-07",2,-20.270350000000001,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1393,"TRANSGRIDV4_19000100000000","2012-10-05T13:05:00","V>>N-LTMS_1","2010-12-07",2,-30.93655,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1394,"TRANSGRIDV4_19000100000000","2012-10-05T13:10:00","V>>N-LTMS_1","2010-12-07",2,-23.911239999999999,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1395,"TRANSGRIDV4_19000100000000","2012-10-05T13:15:00","V>>N-LTMS_1","2010-12-07",2,-27.019870000000001,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1396,"TRANSGRIDV4_19000100000000","2012-10-05T13:20:00","V>>N-LTMS_1","2010-12-07",2,-31.339110000000002,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1397,"TRANSGRIDV4_19000100000000","2012-10-05T13:35:00","V>>N-LTMS_1","2010-12-07",2,-19.983239999999999,"Out= Lower Tumut-Murray(66), avoid Murray to Upper Tumut (65) O/L on Nil trip; Feedback","OUTAGE","OTHER","","REGULATED",null,null,1]
[1398,"TRANSGRIDV4_19000100000000","2012-10-05T13:45:00","V>>N-LTMS_4","2009-09-22",1,-91.367949999999993,"Out= LowerTumut-Murray(66), avoid Murray to UpperTumut (65) O/L(15m rating) on Dederang-Wodonga(DDWO) trip; Feedback","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1399,"TRANSGRIDV4_19000100000000","2012-10-05T10:35:00","V>>V_LTMS_1","2011-01-04",2,-10.357889999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1400,"TRANSGRIDV4_19000100000000","2012-10-05T10:40:00","V>>V_LTMS_1","2011-01-04",2,-14.40666,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1401,"TRANSGRIDV4_19000100000000","2012-10-05T10:45:00","V>>V_LTMS_1","2011-01-04",2,-23.981639999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1402,"TRANSGRIDV4_19000100000000","2012-10-05T10:55:00","V>>V_LTMS_1","2011-01-04",2,-13.14364,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1403,"TRANSGRIDV4_19000100000000","2012-10-05T11:00:00","V>>V_LTMS_1","2011-01-04",2,-24.808409999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1404,"TRANSGRIDV4_19000100000000","2012-10-05T13:40:00","V>>V_LTMS_1","2011-01-04",2,-38.768979999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1405,"TRANSGRIDV4_19000100000000","2012-10-05T13:50:00","V>>V_LTMS_1","2011-01-04",2,-29.162369999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1406,"TRANSGRIDV4_19000100000000","2012-10-05T13:55:00","V>>V_LTMS_1","2011-01-04",2,-29.132529999999999,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1407,"TRANSGRIDV4_19000100000000","2012-10-05T14:00:00","V>>V_LTMS_1","2011-01-04",2,-81.738060000000004,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1408,"TRANSGRIDV4_19000100000000","2012-10-05T14:05:00","V>>V_LTMS_1","2011-01-04",2,-88.608680000000007,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1409,"TRANSGRIDV4_19000100000000","2012-10-05T14:10:00","V>>V_LTMS_1","2011-01-04",2,-89.278440000000003,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1410,"TRANSGRIDV4_19000100000000","2012-10-05T14:15:00","V>>V_LTMS_1","2011-01-04",2,-95.185879999999997,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1411,"TRANSGRIDV4_19000100000000","2012-10-05T14:20:00","V>>V_LTMS_1","2011-01-04",2,-95.213790000000003,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1412,"TRANSGRIDV4_19000100000000","2012-10-05T14:25:00","V>>V_LTMS_1","2011-01-04",2,-95.258830000000003,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1413,"TRANSGRIDV4_19000100000000","2012-10-05T14:30:00","V>>V_LTMS_1","2011-01-04",2,-95.207629999999995,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1414,"TRANSGRIDV4_19000100000000","2012-10-05T14:35:00","V>>V_LTMS_1","2011-01-04",2,-95.237470000000002,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1415,"TRANSGRIDV4_19000100000000","2012-10-05T14:40:00","V>>V_LTMS_1","2011-01-04",2,-95.150689999999997,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1416,"TRANSGRIDV4_19000100000000","2012-10-05T14:45:00","V>>V_LTMS_1","2011-01-04",2,-95.124930000000006,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1417,"TRANSGRIDV4_19000100000000","2012-10-05T14:50:00","V>>V_LTMS_1","2011-01-04",2,-94.573660000000004,"Out= LowerTumut-Murray(66), avoid Dederang->Wodonga line OL(15 min rating) on Murray-UpperTumut(65) trip; Fb,CoOp","OUTAGE","OTHER","Lowertumut To Murray (66)","REGULATED",null,null,1]
[1418,"TRANSGRIDV4_19000100000000","2012-09-11T08:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-31.111460000000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1419,"TRANSGRIDV4_19000100000000","2012-09-11T08:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-87.413259999999994,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1420,"TRANSGRIDV4_19000100000000","2012-09-11T08:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25.453279999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1421,"TRANSGRIDV4_19000100000000","2012-09-11T08:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-91.281949999999995,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1422,"TRANSGRIDV4_19000100000000","2012-09-11T08:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-21.487269999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1423,"TRANSGRIDV4_19000100000000","2012-09-11T08:45:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-24.663209999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1424,"TRANSGRIDV4_19000100000000","2012-09-11T08:50:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-46.113300000000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1425,"TRANSGRIDV4_19000100000000","2012-09-11T08:55:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-26.81277,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1426,"TRANSGRIDV4_19000100000000","2012-09-11T09:00:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-13199.45883,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1427,"TRANSGRIDV4_19000100000000","2012-09-11T09:05:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-99.071809999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1428,"TRANSGRIDV4_19000100000000","2012-09-11T09:10:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-39039.539550000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1429,"TRANSGRIDV4_19000100000000","2012-09-11T09:15:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-76.169889999999995,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1430,"TRANSGRIDV4_19000100000000","2012-09-11T09:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.414219999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1431,"TRANSGRIDV4_19000100000000","2012-09-11T09:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25803.995299999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1432,"TRANSGRIDV4_19000100000000","2012-09-11T09:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25804.47882,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1433,"TRANSGRIDV4_19000100000000","2012-09-11T09:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25803.949540000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1434,"TRANSGRIDV4_19000100000000","2012-09-11T09:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-13.786899999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1435,"TRANSGRIDV4_19000100000000","2012-09-11T09:45:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25819.61419,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1436,"TRANSGRIDV4_19000100000000","2012-09-11T09:50:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.14343,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1437,"TRANSGRIDV4_19000100000000","2012-09-11T09:55:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.118880000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1438,"TRANSGRIDV4_19000100000000","2012-09-11T10:00:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25812.254870000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1439,"TRANSGRIDV4_19000100000000","2012-09-11T10:05:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25812.67671,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1440,"TRANSGRIDV4_19000100000000","2012-09-11T10:10:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25811.069149999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1441,"TRANSGRIDV4_19000100000000","2012-09-11T10:15:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25810.551739999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1442,"TRANSGRIDV4_19000100000000","2012-09-11T10:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25815.634030000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1443,"TRANSGRIDV4_19000100000000","2012-09-11T10:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25812.9895,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1444,"TRANSGRIDV4_19000100000000","2012-09-11T10:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25802.19932,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1445,"TRANSGRIDV4_19000100000000","2012-09-11T10:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25814.794430000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1446,"TRANSGRIDV4_19000100000000","2012-09-11T10:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25819.592560000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1447,"TRANSGRIDV4_19000100000000","2012-09-11T10:45:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.999360000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1448,"TRANSGRIDV4_19000100000000","2012-09-11T10:50:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25820.212769999998,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1449,"TRANSGRIDV4_19000100000000","2012-09-11T10:55:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-60.718319999999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1450,"TRANSGRIDV4_19000100000000","2012-09-11T11:00:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-13.68342,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1451,"TRANSGRIDV4_19000100000000","2012-09-11T11:05:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25819.157029999998,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1452,"TRANSGRIDV4_19000100000000","2012-09-11T11:10:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.034759999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1453,"TRANSGRIDV4_19000100000000","2012-09-11T11:15:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-59.678040000000003,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1454,"TRANSGRIDV4_19000100000000","2012-09-11T11:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-11.666460000000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1455,"TRANSGRIDV4_19000100000000","2012-09-11T11:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25811.066269999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1456,"TRANSGRIDV4_19000100000000","2012-09-11T11:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25812.41778,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1457,"TRANSGRIDV4_19000100000000","2012-09-11T11:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25818.335620000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1458,"TRANSGRIDV4_19000100000000","2012-09-11T11:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.099539999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1459,"TRANSGRIDV4_19000100000000","2012-09-11T11:50:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25811.776020000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1460,"TRANSGRIDV4_19000100000000","2012-09-11T11:55:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.065190000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1461,"TRANSGRIDV4_19000100000000","2012-09-11T12:00:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25816.187119999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1462,"TRANSGRIDV4_19000100000000","2012-09-11T12:05:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25849.054230000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1463,"TRANSGRIDV4_19000100000000","2012-09-11T12:10:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25816.073499999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1464,"TRANSGRIDV4_19000100000000","2012-09-11T12:15:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25827.439780000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1465,"TRANSGRIDV4_19000100000000","2012-09-11T12:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25819.287779999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1466,"TRANSGRIDV4_19000100000000","2012-09-11T12:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.40481,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1467,"TRANSGRIDV4_19000100000000","2012-09-11T12:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.265050000002,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1468,"TRANSGRIDV4_19000100000000","2012-09-11T12:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25818.148829999998,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1469,"TRANSGRIDV4_19000100000000","2012-09-11T12:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.318520000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1470,"TRANSGRIDV4_19000100000000","2012-09-11T12:45:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.521420000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1471,"TRANSGRIDV4_19000100000000","2012-09-11T12:50:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25812.255359999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1472,"TRANSGRIDV4_19000100000000","2012-09-11T12:55:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25815.315129999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1473,"TRANSGRIDV4_19000100000000","2012-09-11T13:00:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25815.308239999998,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1474,"TRANSGRIDV4_19000100000000","2012-09-11T13:05:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25814.982090000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1475,"TRANSGRIDV4_19000100000000","2012-09-11T13:10:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25826.105459999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1476,"TRANSGRIDV4_19000100000000","2012-09-11T13:15:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25818.412110000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1477,"TRANSGRIDV4_19000100000000","2012-09-11T13:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25799.849409999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1478,"TRANSGRIDV4_19000100000000","2012-09-11T13:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25799.20652,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1479,"TRANSGRIDV4_19000100000000","2012-09-11T13:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-64.31353,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1480,"TRANSGRIDV4_19000100000000","2012-09-11T13:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.56061,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1481,"TRANSGRIDV4_19000100000000","2012-09-11T13:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25813.18651,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1482,"TRANSGRIDV4_19000100000000","2012-09-11T14:20:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-10.39714,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1483,"TRANSGRIDV4_19000100000000","2012-09-11T14:25:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-24.297370000000001,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1484,"TRANSGRIDV4_19000100000000","2012-09-11T14:30:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-22.20157,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1485,"TRANSGRIDV4_19000100000000","2012-09-11T14:35:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-18.08672,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1486,"TRANSGRIDV4_19000100000000","2012-09-11T14:40:00","V>>V-LTWG_RADIAL_2","2010-06-28",2,-25817.478599999999,"Outage = Lower Tumut to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload Murray to Dederang No.1 330kV line for loss of the parallel No.2 line, 15 min line ratings; Feedback","OUTAGE","OTHER","Lower Tumut To Wagga 330Kv Line","REGULATED",null,null,1]
[1487,"TRANSGRIDV4_19000100000000","2012-12-13T12:40:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1488,"TRANSGRIDV4_19000100000000","2012-12-13T12:45:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1489,"TRANSGRIDV4_19000100000000","2012-12-13T12:50:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1490,"TRANSGRIDV4_19000100000000","2012-12-13T12:55:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1491,"TRANSGRIDV4_19000100000000","2012-12-13T13:00:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1492,"TRANSGRIDV4_19000100000000","2012-12-13T13:05:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1493,"TRANSGRIDV4_19000100000000","2012-12-13T13:10:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1494,"TRANSGRIDV4_19000100000000","2012-12-13T13:15:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1495,"TRANSGRIDV4_19000100000000","2012-12-13T13:20:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1496,"TRANSGRIDV4_19000100000000","2012-12-13T13:25:00","V>SML_BUDP_1","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV kV line, avoid O/L Bendigo to Kerang 220 kV line on trip of Ballarat to Waubra to Horsham 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1497,"TRANSGRIDV4_19000100000000","2012-11-23T13:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1498,"TRANSGRIDV4_19000100000000","2012-11-23T13:50:00","V>SML_BUDP_2","2012-09-28",1,-11806.182150000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1499,"TRANSGRIDV4_19000100000000","2012-12-12T13:05:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1500,"TRANSGRIDV4_19000100000000","2012-12-12T13:10:00","V>SML_BUDP_2","2012-09-28",1,-14.909509999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1501,"TRANSGRIDV4_19000100000000","2012-12-12T13:15:00","V>SML_BUDP_2","2012-09-28",1,-10.75595,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1502,"TRANSGRIDV4_19000100000000","2012-12-12T13:30:00","V>SML_BUDP_2","2012-09-28",1,-11.449909999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1503,"TRANSGRIDV4_19000100000000","2012-12-12T13:35:00","V>SML_BUDP_2","2012-09-28",1,-13.860250000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1504,"TRANSGRIDV4_19000100000000","2012-12-12T13:40:00","V>SML_BUDP_2","2012-09-28",1,-17.506900000000002,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1505,"TRANSGRIDV4_19000100000000","2012-12-12T13:45:00","V>SML_BUDP_2","2012-09-28",1,-351.81155999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1506,"TRANSGRIDV4_19000100000000","2012-12-12T13:50:00","V>SML_BUDP_2","2012-09-28",1,-180.65586999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1507,"TRANSGRIDV4_19000100000000","2012-12-12T13:55:00","V>SML_BUDP_2","2012-09-28",1,-57.238059999999997,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1508,"TRANSGRIDV4_19000100000000","2012-12-12T14:00:00","V>SML_BUDP_2","2012-09-28",1,-40.34572,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1509,"TRANSGRIDV4_19000100000000","2012-12-12T14:05:00","V>SML_BUDP_2","2012-09-28",1,-19.51191,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1510,"TRANSGRIDV4_19000100000000","2012-12-12T14:10:00","V>SML_BUDP_2","2012-09-28",1,-15.602410000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1511,"TRANSGRIDV4_19000100000000","2012-12-12T14:15:00","V>SML_BUDP_2","2012-09-28",1,-14.91963,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1512,"TRANSGRIDV4_19000100000000","2012-12-12T14:20:00","V>SML_BUDP_2","2012-09-28",1,-17.114370000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1513,"TRANSGRIDV4_19000100000000","2012-12-12T14:25:00","V>SML_BUDP_2","2012-09-28",1,-68.365589999999997,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1514,"TRANSGRIDV4_19000100000000","2012-12-12T14:30:00","V>SML_BUDP_2","2012-09-28",1,-12.50845,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1515,"TRANSGRIDV4_19000100000000","2012-12-12T14:35:00","V>SML_BUDP_2","2012-09-28",1,-422.31049999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1516,"TRANSGRIDV4_19000100000000","2012-12-12T14:40:00","V>SML_BUDP_2","2012-09-28",1,-333.55606999999998,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1517,"TRANSGRIDV4_19000100000000","2012-12-12T14:45:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1518,"TRANSGRIDV4_19000100000000","2012-12-12T14:50:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1519,"TRANSGRIDV4_19000100000000","2012-12-12T14:55:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1520,"TRANSGRIDV4_19000100000000","2012-12-12T15:00:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1521,"TRANSGRIDV4_19000100000000","2012-12-12T15:05:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1522,"TRANSGRIDV4_19000100000000","2012-12-12T15:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1523,"TRANSGRIDV4_19000100000000","2012-12-12T15:15:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1524,"TRANSGRIDV4_19000100000000","2012-12-12T15:20:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1525,"TRANSGRIDV4_19000100000000","2012-12-12T15:25:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1526,"TRANSGRIDV4_19000100000000","2012-12-12T15:30:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1527,"TRANSGRIDV4_19000100000000","2012-12-12T15:35:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1528,"TRANSGRIDV4_19000100000000","2012-12-12T15:40:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1529,"TRANSGRIDV4_19000100000000","2012-12-12T15:45:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1530,"TRANSGRIDV4_19000100000000","2012-12-12T15:50:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1531,"TRANSGRIDV4_19000100000000","2012-12-12T15:55:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1532,"TRANSGRIDV4_19000100000000","2012-12-12T16:00:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1533,"TRANSGRIDV4_19000100000000","2012-12-12T16:05:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1534,"TRANSGRIDV4_19000100000000","2012-12-12T16:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1535,"TRANSGRIDV4_19000100000000","2012-12-12T16:15:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1536,"TRANSGRIDV4_19000100000000","2012-12-12T16:20:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1537,"TRANSGRIDV4_19000100000000","2012-12-12T16:25:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1538,"TRANSGRIDV4_19000100000000","2012-12-12T16:30:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1539,"TRANSGRIDV4_19000100000000","2012-12-12T16:35:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1540,"TRANSGRIDV4_19000100000000","2012-12-12T16:40:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1541,"TRANSGRIDV4_19000100000000","2012-12-12T16:45:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1542,"TRANSGRIDV4_19000100000000","2012-12-12T16:50:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1543,"TRANSGRIDV4_19000100000000","2012-12-12T16:55:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1544,"TRANSGRIDV4_19000100000000","2012-12-12T17:00:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1545,"TRANSGRIDV4_19000100000000","2012-12-12T17:05:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,0]
[1546,"TRANSGRIDV4_19000100000000","2012-12-12T17:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1547,"TRANSGRIDV4_19000100000000","2012-12-12T17:15:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1548,"TRANSGRIDV4_19000100000000","2012-12-12T17:20:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1549,"TRANSGRIDV4_19000100000000","2012-12-12T17:25:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1550,"TRANSGRIDV4_19000100000000","2012-12-12T17:30:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1551,"TRANSGRIDV4_19000100000000","2012-12-12T17:35:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1552,"TRANSGRIDV4_19000100000000","2012-12-12T17:40:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1553,"TRANSGRIDV4_19000100000000","2012-12-12T17:45:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1554,"TRANSGRIDV4_19000100000000","2012-12-12T17:50:00","V>SML_BUDP_2","2012-09-28",1,-18.295590000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1555,"TRANSGRIDV4_19000100000000","2012-12-12T17:55:00","V>SML_BUDP_2","2012-09-28",1,-11.96954,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1556,"TRANSGRIDV4_19000100000000","2012-12-12T18:00:00","V>SML_BUDP_2","2012-09-28",1,-11.664239999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1557,"TRANSGRIDV4_19000100000000","2012-12-12T18:05:00","V>SML_BUDP_2","2012-09-28",1,-57.366520000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1558,"TRANSGRIDV4_19000100000000","2012-12-12T18:10:00","V>SML_BUDP_2","2012-09-28",1,-53.076839999999997,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1559,"TRANSGRIDV4_19000100000000","2012-12-12T18:15:00","V>SML_BUDP_2","2012-09-28",1,-18.250450000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1560,"TRANSGRIDV4_19000100000000","2012-12-12T18:20:00","V>SML_BUDP_2","2012-09-28",1,-17.766729999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1561,"TRANSGRIDV4_19000100000000","2012-12-12T18:25:00","V>SML_BUDP_2","2012-09-28",1,-17.344110000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1562,"TRANSGRIDV4_19000100000000","2012-12-12T18:30:00","V>SML_BUDP_2","2012-09-28",1,-17.768360000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1563,"TRANSGRIDV4_19000100000000","2012-12-12T18:35:00","V>SML_BUDP_2","2012-09-28",1,-13.69237,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1564,"TRANSGRIDV4_19000100000000","2012-12-12T18:40:00","V>SML_BUDP_2","2012-09-28",1,-10.81522,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1565,"TRANSGRIDV4_19000100000000","2012-12-12T18:45:00","V>SML_BUDP_2","2012-09-28",1,-10.372960000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1566,"TRANSGRIDV4_19000100000000","2012-12-12T19:05:00","V>SML_BUDP_2","2012-09-28",1,-12.15338,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1567,"TRANSGRIDV4_19000100000000","2012-12-12T19:50:00","V>SML_BUDP_2","2012-09-28",1,-32.78539,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1568,"TRANSGRIDV4_19000100000000","2012-12-12T19:55:00","V>SML_BUDP_2","2012-09-28",1,-12.47946,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1569,"TRANSGRIDV4_19000100000000","2012-12-12T20:00:00","V>SML_BUDP_2","2012-09-28",1,-12.42329,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1570,"TRANSGRIDV4_19000100000000","2012-12-12T23:35:00","V>SML_BUDP_2","2012-09-28",1,-11.47856,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1571,"TRANSGRIDV4_19000100000000","2012-12-12T23:40:00","V>SML_BUDP_2","2012-09-28",1,-10.42301,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1572,"TRANSGRIDV4_19000100000000","2012-12-13T07:20:00","V>SML_BUDP_2","2012-09-28",1,-25660.350729999998,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1573,"TRANSGRIDV4_19000100000000","2012-12-13T07:25:00","V>SML_BUDP_2","2012-09-28",1,-37958.31826,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1574,"TRANSGRIDV4_19000100000000","2012-12-13T08:25:00","V>SML_BUDP_2","2012-09-28",1,-12.158759999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1575,"TRANSGRIDV4_19000100000000","2012-12-13T08:30:00","V>SML_BUDP_2","2012-09-28",1,-22.61543,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1576,"TRANSGRIDV4_19000100000000","2012-12-13T08:35:00","V>SML_BUDP_2","2012-09-28",1,-24.68844,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1577,"TRANSGRIDV4_19000100000000","2012-12-13T08:40:00","V>SML_BUDP_2","2012-09-28",1,-24.0275,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1578,"TRANSGRIDV4_19000100000000","2012-12-13T08:45:00","V>SML_BUDP_2","2012-09-28",1,-23.472829999999998,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1579,"TRANSGRIDV4_19000100000000","2012-12-13T08:50:00","V>SML_BUDP_2","2012-09-28",1,-23.171859999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1580,"TRANSGRIDV4_19000100000000","2012-12-13T08:55:00","V>SML_BUDP_2","2012-09-28",1,-23.184059999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1581,"TRANSGRIDV4_19000100000000","2012-12-13T09:10:00","V>SML_BUDP_2","2012-09-28",1,-13.583259999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1582,"TRANSGRIDV4_19000100000000","2012-12-13T11:00:00","V>SML_BUDP_2","2012-09-28",1,-19.377369999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1583,"TRANSGRIDV4_19000100000000","2012-12-13T11:05:00","V>SML_BUDP_2","2012-09-28",1,-27.733730000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1584,"TRANSGRIDV4_19000100000000","2012-12-13T11:10:00","V>SML_BUDP_2","2012-09-28",1,-20.95411,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1585,"TRANSGRIDV4_19000100000000","2012-12-13T11:15:00","V>SML_BUDP_2","2012-09-28",1,-28.751339999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1586,"TRANSGRIDV4_19000100000000","2012-12-13T11:20:00","V>SML_BUDP_2","2012-09-28",1,-26.523019999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1587,"TRANSGRIDV4_19000100000000","2012-12-13T11:25:00","V>SML_BUDP_2","2012-09-28",1,-25.270879999999998,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1588,"TRANSGRIDV4_19000100000000","2012-12-13T11:30:00","V>SML_BUDP_2","2012-09-28",1,-25.264410000000002,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1589,"TRANSGRIDV4_19000100000000","2012-12-13T11:40:00","V>SML_BUDP_2","2012-09-28",1,-34.326999999999998,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1590,"TRANSGRIDV4_19000100000000","2012-12-13T11:45:00","V>SML_BUDP_2","2012-09-28",1,-27.581710000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1591,"TRANSGRIDV4_19000100000000","2012-12-13T11:50:00","V>SML_BUDP_2","2012-09-28",1,-33.172150000000002,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1592,"TRANSGRIDV4_19000100000000","2012-12-13T11:55:00","V>SML_BUDP_2","2012-09-28",1,-37.583350000000003,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1593,"TRANSGRIDV4_19000100000000","2012-12-13T12:00:00","V>SML_BUDP_2","2012-09-28",1,-20.3291,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1594,"TRANSGRIDV4_19000100000000","2012-12-13T12:05:00","V>SML_BUDP_2","2012-09-28",1,-30.786110000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1595,"TRANSGRIDV4_19000100000000","2012-12-13T12:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1596,"TRANSGRIDV4_19000100000000","2012-12-13T12:15:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1597,"TRANSGRIDV4_19000100000000","2012-12-13T12:20:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1598,"TRANSGRIDV4_19000100000000","2012-12-13T12:25:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1599,"TRANSGRIDV4_19000100000000","2012-12-13T12:30:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1600,"TRANSGRIDV4_19000100000000","2012-12-13T12:35:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1601,"TRANSGRIDV4_19000100000000","2012-12-13T12:40:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1602,"TRANSGRIDV4_19000100000000","2012-12-13T12:45:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1603,"TRANSGRIDV4_19000100000000","2012-12-13T12:50:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1604,"TRANSGRIDV4_19000100000000","2012-12-13T12:55:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1605,"TRANSGRIDV4_19000100000000","2012-12-13T13:00:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1606,"TRANSGRIDV4_19000100000000","2012-12-13T13:05:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1607,"TRANSGRIDV4_19000100000000","2012-12-13T13:10:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1608,"TRANSGRIDV4_19000100000000","2012-12-13T13:15:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1609,"TRANSGRIDV4_19000100000000","2012-12-13T13:20:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1610,"TRANSGRIDV4_19000100000000","2012-12-13T13:25:00","V>SML_BUDP_2","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1611,"TRANSGRIDV4_19000100000000","2012-12-13T15:50:00","V>SML_BUDP_2","2012-09-28",1,-11.60083,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1612,"TRANSGRIDV4_19000100000000","2012-12-13T15:55:00","V>SML_BUDP_2","2012-09-28",1,-10.583780000000001,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1613,"TRANSGRIDV4_19000100000000","2012-12-13T23:35:00","V>SML_BUDP_2","2012-09-28",1,-11.208,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1614,"TRANSGRIDV4_19000100000000","2012-12-13T23:40:00","V>SML_BUDP_2","2012-09-28",1,-12.50981,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1615,"TRANSGRIDV4_19000100000000","2012-12-13T23:45:00","V>SML_BUDP_2","2012-09-28",1,-11.64869,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1616,"TRANSGRIDV4_19000100000000","2012-12-13T23:50:00","V>SML_BUDP_2","2012-09-28",1,-10.3009,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1617,"TRANSGRIDV4_19000100000000","2012-12-23T20:55:00","V>SML_BUDP_2","2012-09-28",1,-10.035019999999999,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Bendigo to Kerang line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1618,"TRANSGRIDV4_19000100000000","2012-12-12T13:05:00","V>SML_BUDP_3","2012-09-28",1,-8244.3767000000007,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1619,"TRANSGRIDV4_19000100000000","2012-12-13T12:20:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED",null,null,1]
[1620,"TRANSGRIDV4_19000100000000","2012-12-13T12:35:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1621,"TRANSGRIDV4_19000100000000","2012-12-13T12:40:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1622,"TRANSGRIDV4_19000100000000","2012-12-13T12:45:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1623,"TRANSGRIDV4_19000100000000","2012-12-13T12:50:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1624,"TRANSGRIDV4_19000100000000","2012-12-13T12:55:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1625,"TRANSGRIDV4_19000100000000","2012-12-13T13:00:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1626,"TRANSGRIDV4_19000100000000","2012-12-13T13:05:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1627,"TRANSGRIDV4_19000100000000","2012-12-13T13:10:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1628,"TRANSGRIDV4_19000100000000","2012-12-13T13:15:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1629,"TRANSGRIDV4_19000100000000","2012-12-13T13:20:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1630,"TRANSGRIDV4_19000100000000","2012-12-13T13:25:00","V>SML_BUDP_3","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt (X5) line, limit Murraylink from Vic to SA to avoid O/L Kerang to Red Cliffs line on loss of Ballarat to Horsham line","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]
[1631,"TRANSGRIDV4_19000100000000","2012-12-13T13:00:00","V>SML_BUDP_4","2012-09-28",1,-258000,"Out = Buronga to Balranald to Darlington Pt. (X5) 220 kV line, avoid O/L Ballarat to Bendigo 220 kV line on trip of Shepparton to Fosterville to Bendigo 220 kV line, feedback","OUTAGE","OTHER","Buronga To Balranald To Darlington Pt. (X5) 220 Kv Line","REGULATED","8(b)","Special exclusion, refer to 2012 MIC submission",0]