{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"TRANSGRIDV5_20161215153009"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"14.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"TRANSGRID"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2014]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2014-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2015-01-01"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":749.5}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":9031}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":9800}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2014 Version: 5"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":4},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":127},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":6},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":185},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":8709},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":769},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":749.5}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":9800},null,{"$f":"SUM($P$46:$P$65)","v":749.5}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation",null,null,"2016-12-15T15:30:09"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":23554,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[1,"TRANSGRIDV5_20161215152814","2014-01-01T05:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-43.506909999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2,"TRANSGRIDV5_20161215152814","2014-01-01T04:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-24.704219999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3,"TRANSGRIDV5_20161215152814","2014-01-01T04:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-23.722639999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4,"TRANSGRIDV5_20161215152814","2014-01-01T04:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-23.698720000000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[5,"TRANSGRIDV5_20161215152814","2014-01-01T05:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-23.21162,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6,"TRANSGRIDV5_20161215152814","2014-01-01T03:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-23.183160000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[7,"TRANSGRIDV5_20161215152814","2014-01-01T03:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-23.18281,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[8,"TRANSGRIDV5_20161215152814","2014-01-01T04:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-22.8904,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[9,"TRANSGRIDV5_20161215152814","2014-01-01T04:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-22.58971,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[10,"TRANSGRIDV5_20161215152814","2014-01-01T03:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-22.499960000000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[11,"TRANSGRIDV5_20161215152814","2014-01-01T04:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-22.374569999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[12,"TRANSGRIDV5_20161215152814","2014-01-01T04:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-22.009170000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[13,"TRANSGRIDV5_20161215152814","2014-01-01T05:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-21.0396,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[14,"TRANSGRIDV5_20161215152814","2014-01-01T03:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-20.096209999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[15,"TRANSGRIDV5_20161215152814","2014-01-01T03:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-20.042079999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[16,"TRANSGRIDV5_20161215152814","2014-01-01T03:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-18.17334,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[17,"TRANSGRIDV5_20161215152814","2014-01-01T02:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-15.774559999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[18,"TRANSGRIDV5_20161215152814","2014-01-01T04:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-15.542479999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[19,"TRANSGRIDV5_20161215152814","2014-01-01T02:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-13.543480000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[20,"TRANSGRIDV5_20161215152814","2014-01-01T02:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-11.69219,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[21,"TRANSGRIDV5_20161215152814","2014-01-01T16:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-21.373760000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[22,"TRANSGRIDV5_20161215152814","2014-01-01T13:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.872029999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[23,"TRANSGRIDV5_20161215152814","2014-01-01T13:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.815339999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[24,"TRANSGRIDV5_20161215152814","2014-01-01T16:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.750489999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[25,"TRANSGRIDV5_20161215152814","2014-01-01T16:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.750489999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[26,"TRANSGRIDV5_20161215152814","2014-01-01T16:55:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.691020000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[27,"TRANSGRIDV5_20161215152814","2014-01-01T13:55:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.681100000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[28,"TRANSGRIDV5_20161215152814","2014-01-01T10:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.4222,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[29,"TRANSGRIDV5_20161215152814","2014-01-01T18:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.028089999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[30,"TRANSGRIDV5_20161215152814","2014-01-01T13:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-18.588909999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[31,"TRANSGRIDV5_20161215152814","2014-01-01T16:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-18.50141,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[32,"TRANSGRIDV5_20161215152814","2014-01-01T16:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-18.491140000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[33,"TRANSGRIDV5_20161215152814","2014-01-01T18:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-17.6845,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[34,"TRANSGRIDV5_20161215152814","2014-01-01T17:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-16.910299999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[35,"TRANSGRIDV5_20161215152814","2014-01-01T11:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-15.88429,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[36,"TRANSGRIDV5_20161215152814","2014-01-01T10:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-14.76911,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[37,"TRANSGRIDV5_20161215152814","2014-01-01T16:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-14.759069999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[38,"TRANSGRIDV5_20161215152814","2014-01-01T10:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-14.39926,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[39,"TRANSGRIDV5_20161215152814","2014-01-01T10:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-14.24579,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[40,"TRANSGRIDV5_20161215152814","2014-01-01T18:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-13.14386,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[41,"TRANSGRIDV5_20161215152814","2014-01-01T13:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.60066,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[42,"TRANSGRIDV5_20161215152814","2014-01-01T13:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.50375,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[43,"TRANSGRIDV5_20161215152814","2014-01-01T14:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.50371,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[44,"TRANSGRIDV5_20161215152814","2014-01-01T16:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.339639999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[45,"TRANSGRIDV5_20161215152814","2014-01-01T16:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.316649999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[46,"TRANSGRIDV5_20161215152814","2014-01-01T18:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.92398,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[47,"TRANSGRIDV5_20161215152814","2014-01-01T16:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.917909999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[48,"TRANSGRIDV5_20161215152814","2014-01-01T16:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.88363,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[49,"TRANSGRIDV5_20161215152814","2014-01-01T17:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.411630000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[50,"TRANSGRIDV5_20161215152814","2014-01-01T13:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.20515,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[51,"TRANSGRIDV5_20161215152814","2014-01-01T13:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-11.153689999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[52,"TRANSGRIDV5_20161215152814","2014-01-01T14:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-10.73062,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[53,"TRANSGRIDV5_20161215152814","2014-01-01T11:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-10.45326,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[54,"TRANSGRIDV5_20161215152814","2014-01-01T17:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-10.300890000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[55,"TRANSGRIDV5_20161215152814","2014-01-01T02:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-20.533290000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[56,"TRANSGRIDV5_20161215152814","2014-01-01T02:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-14.947760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[57,"TRANSGRIDV5_20161215152814","2014-01-01T05:05:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-78.814210000000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[58,"TRANSGRIDV5_20161215152814","2014-01-01T04:05:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-48.348410000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[59,"TRANSGRIDV5_20161215152814","2014-01-01T04:50:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-46.1706,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[60,"TRANSGRIDV5_20161215152814","2014-01-01T04:55:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-46.169730000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[61,"TRANSGRIDV5_20161215152814","2014-01-01T05:00:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-45.142850000000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[62,"TRANSGRIDV5_20161215152814","2014-01-01T03:50:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-45.12717,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[63,"TRANSGRIDV5_20161215152814","2014-01-01T03:55:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-45.126159999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[64,"TRANSGRIDV5_20161215152814","2014-01-01T04:30:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-44.429400000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[65,"TRANSGRIDV5_20161215152814","2014-01-01T03:45:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-43.93609,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[66,"TRANSGRIDV5_20161215152814","2014-01-01T04:10:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-43.79439,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[67,"TRANSGRIDV5_20161215152814","2014-01-01T04:15:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-43.342950000000002,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[68,"TRANSGRIDV5_20161215152814","2014-01-01T05:10:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-42.614260000000002,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[69,"TRANSGRIDV5_20161215152814","2014-01-01T04:20:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-42.607320000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[70,"TRANSGRIDV5_20161215152814","2014-01-01T03:35:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-38.592179999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[71,"TRANSGRIDV5_20161215152814","2014-01-01T03:40:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-38.467979999999997,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[72,"TRANSGRIDV5_20161215152814","2014-01-01T03:30:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-34.907049999999998,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[73,"TRANSGRIDV5_20161215152814","2014-01-01T04:00:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-29.084029999999998,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[74,"TRANSGRIDV5_20161215152814","2014-01-01T02:30:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-28.23912,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[75,"TRANSGRIDV5_20161215152814","2014-01-01T03:25:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-10.41269,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[76,"TRANSGRIDV5_20161215152814","2014-01-01T02:35:00","V>>V_NIL1A_R","V-NIL","2013-12-03",1,-10.35913,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[77,"TRANSGRIDV5_20161215152814","2014-01-02T15:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.671009999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[78,"TRANSGRIDV5_20161215152814","2014-01-02T15:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.034079999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[79,"TRANSGRIDV5_20161215152814","2014-01-02T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.002980000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[80,"TRANSGRIDV5_20161215152814","2014-01-02T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.965610000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[81,"TRANSGRIDV5_20161215152814","2014-01-02T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.963249999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[82,"TRANSGRIDV5_20161215152814","2014-01-02T17:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.842980000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[83,"TRANSGRIDV5_20161215152814","2014-01-02T15:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.339479999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[84,"TRANSGRIDV5_20161215152814","2014-01-02T16:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.933800000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[85,"TRANSGRIDV5_20161215152814","2014-01-02T16:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.653040000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[86,"TRANSGRIDV5_20161215152814","2014-01-02T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.647179999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[87,"TRANSGRIDV5_20161215152814","2014-01-02T16:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.615089999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[88,"TRANSGRIDV5_20161215152814","2014-01-02T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.031189999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[89,"TRANSGRIDV5_20161215152814","2014-01-02T17:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.160019999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[90,"TRANSGRIDV5_20161215152814","2014-01-02T15:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.68178,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[91,"TRANSGRIDV5_20161215152814","2014-01-02T16:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.680289999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[92,"TRANSGRIDV5_20161215152814","2014-01-02T15:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.656750000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[93,"TRANSGRIDV5_20161215152814","2014-01-02T15:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.63716,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[94,"TRANSGRIDV5_20161215152814","2014-01-02T16:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.3582,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[95,"TRANSGRIDV5_20161215152814","2014-01-02T15:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.27197,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[96,"TRANSGRIDV5_20161215152814","2014-01-02T15:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.235889999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[97,"TRANSGRIDV5_20161215152814","2014-01-02T16:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.20065,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[98,"TRANSGRIDV5_20161215152814","2014-01-02T16:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.180429999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[99,"TRANSGRIDV5_20161215152814","2014-01-02T16:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-15.176740000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[100,"TRANSGRIDV5_20161215152814","2014-01-02T15:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-14.440619999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[101,"TRANSGRIDV5_20161215152814","2014-01-03T15:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-222.84636,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[102,"TRANSGRIDV5_20161215152814","2014-01-03T17:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-218.72209000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[103,"TRANSGRIDV5_20161215152814","2014-01-03T17:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-211.27249,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[104,"TRANSGRIDV5_20161215152814","2014-01-03T17:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-211.08393000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[105,"TRANSGRIDV5_20161215152814","2014-01-03T12:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-210.63699,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[106,"TRANSGRIDV5_20161215152814","2014-01-03T17:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-210.46915999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[107,"TRANSGRIDV5_20161215152814","2014-01-03T17:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-210.38363000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[108,"TRANSGRIDV5_20161215152814","2014-01-03T14:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-210.02207000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[109,"TRANSGRIDV5_20161215152814","2014-01-03T16:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-208.9478,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[110,"TRANSGRIDV5_20161215152814","2014-01-03T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-208.71628000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[111,"TRANSGRIDV5_20161215152814","2014-01-03T14:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-208.05517,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[112,"TRANSGRIDV5_20161215152814","2014-01-03T13:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-200.09630000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[113,"TRANSGRIDV5_20161215152814","2014-01-03T14:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-197.08798999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[114,"TRANSGRIDV5_20161215152814","2014-01-03T17:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-161.21790999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[115,"TRANSGRIDV5_20161215152814","2014-01-03T17:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-160.24518,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[116,"TRANSGRIDV5_20161215152814","2014-01-03T13:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-127.69068,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[117,"TRANSGRIDV5_20161215152814","2014-01-03T15:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-126.27742000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[118,"TRANSGRIDV5_20161215152814","2014-01-03T16:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-91.677539999999993,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[119,"TRANSGRIDV5_20161215152814","2014-01-03T13:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-87.196100000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[120,"TRANSGRIDV5_20161215152814","2014-01-03T19:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-86.971860000000007,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[121,"TRANSGRIDV5_20161215152814","2014-01-03T16:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-86.733400000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[122,"TRANSGRIDV5_20161215152814","2014-01-03T17:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-86.591009999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[123,"TRANSGRIDV5_20161215152814","2014-01-03T17:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.440290000000005,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[124,"TRANSGRIDV5_20161215152814","2014-01-03T15:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.114649999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[125,"TRANSGRIDV5_20161215152814","2014-01-03T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.067390000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[126,"TRANSGRIDV5_20161215152814","2014-01-03T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.027720000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[127,"TRANSGRIDV5_20161215152814","2014-01-03T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.025090000000006,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[128,"TRANSGRIDV5_20161215152814","2014-01-03T15:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.999049999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[129,"TRANSGRIDV5_20161215152814","2014-01-03T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.985349999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[130,"TRANSGRIDV5_20161215152814","2014-01-03T16:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.881299999999996,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[131,"TRANSGRIDV5_20161215152814","2014-01-03T16:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.825249999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[132,"TRANSGRIDV5_20161215152814","2014-01-03T16:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.808980000000005,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[133,"TRANSGRIDV5_20161215152814","2014-01-03T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.450860000000006,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[134,"TRANSGRIDV5_20161215152814","2014-01-03T15:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.302959999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[135,"TRANSGRIDV5_20161215152814","2014-01-03T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.275810000000007,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[136,"TRANSGRIDV5_20161215152814","2014-01-03T15:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.240260000000006,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[137,"TRANSGRIDV5_20161215152814","2014-01-03T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.04898,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[138,"TRANSGRIDV5_20161215152814","2014-01-03T19:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.297289999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[139,"TRANSGRIDV5_20161215152814","2014-01-03T19:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.245780000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[140,"TRANSGRIDV5_20161215152814","2014-01-03T18:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.124519999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[141,"TRANSGRIDV5_20161215152814","2014-01-03T18:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.930019999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[142,"TRANSGRIDV5_20161215152814","2014-01-03T19:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.410209999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[143,"TRANSGRIDV5_20161215152814","2014-01-03T19:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.37283,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[144,"TRANSGRIDV5_20161215152814","2014-01-03T18:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.25385,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[145,"TRANSGRIDV5_20161215152814","2014-01-03T19:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.214170000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[146,"TRANSGRIDV5_20161215152814","2014-01-03T18:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.125599999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[147,"TRANSGRIDV5_20161215152814","2014-01-03T18:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.057789999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[148,"TRANSGRIDV5_20161215152814","2014-01-03T17:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.033819999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[149,"TRANSGRIDV5_20161215152814","2014-01-03T19:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.692950000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[150,"TRANSGRIDV5_20161215152814","2014-01-03T13:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.614100000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[151,"TRANSGRIDV5_20161215152814","2014-01-03T15:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.471719999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[152,"TRANSGRIDV5_20161215152814","2014-01-03T17:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.436369999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[153,"TRANSGRIDV5_20161215152814","2014-01-03T17:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.346589999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[154,"TRANSGRIDV5_20161215152814","2014-01-03T16:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.157310000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[155,"TRANSGRIDV5_20161215152814","2014-01-03T16:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.127490000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[156,"TRANSGRIDV5_20161215152814","2014-01-03T16:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.108339999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[157,"TRANSGRIDV5_20161215152814","2014-01-03T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.826340000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[158,"TRANSGRIDV5_20161215152814","2014-01-03T13:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.168750000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[159,"TRANSGRIDV5_20161215152814","2014-01-03T14:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.139139999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[160,"TRANSGRIDV5_20161215152814","2014-01-03T18:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.995240000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[161,"TRANSGRIDV5_20161215152814","2014-01-03T19:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.789769999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[162,"TRANSGRIDV5_20161215152814","2014-01-03T20:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.745750000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[163,"TRANSGRIDV5_20161215152814","2014-01-03T13:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.538379999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[164,"TRANSGRIDV5_20161215152814","2014-01-03T13:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.511470000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[165,"TRANSGRIDV5_20161215152814","2014-01-03T13:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.478079999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[166,"TRANSGRIDV5_20161215152814","2014-01-03T13:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.44932,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[167,"TRANSGRIDV5_20161215152814","2014-01-03T19:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.43873,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[168,"TRANSGRIDV5_20161215152814","2014-01-03T18:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.416260000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[169,"TRANSGRIDV5_20161215152814","2014-01-03T18:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.411050000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[170,"TRANSGRIDV5_20161215152814","2014-01-03T18:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.385779999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[171,"TRANSGRIDV5_20161215152814","2014-01-03T18:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.356589999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[172,"TRANSGRIDV5_20161215152814","2014-01-03T12:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.97139,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[173,"TRANSGRIDV5_20161215152814","2014-01-03T12:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.951860000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[174,"TRANSGRIDV5_20161215152814","2014-01-03T12:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.945250000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[175,"TRANSGRIDV5_20161215152814","2014-01-03T13:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.85107,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[176,"TRANSGRIDV5_20161215152814","2014-01-03T12:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.213050000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[177,"TRANSGRIDV5_20161215152814","2014-01-03T21:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-29.77055,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[178,"TRANSGRIDV5_20161215152814","2014-01-03T18:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-29.27826,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[179,"TRANSGRIDV5_20161215152814","2014-01-03T18:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.74539,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[180,"TRANSGRIDV5_20161215152814","2014-01-03T19:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.54842,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[181,"TRANSGRIDV5_20161215152814","2014-01-03T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.418579999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[182,"TRANSGRIDV5_20161215152814","2014-01-03T19:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.412179999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[183,"TRANSGRIDV5_20161215152814","2014-01-03T23:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-24.423410000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[184,"TRANSGRIDV5_20161215152814","2014-01-03T23:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.805150000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[185,"TRANSGRIDV5_20161215152814","2014-01-03T22:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.58991,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[186,"TRANSGRIDV5_20161215152814","2014-01-03T12:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.38287,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[187,"TRANSGRIDV5_20161215152814","2014-01-03T22:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.295190000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[188,"TRANSGRIDV5_20161215152814","2014-01-03T12:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.95194,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[189,"TRANSGRIDV5_20161215152814","2014-01-03T12:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.692419999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[190,"TRANSGRIDV5_20161215152814","2014-01-03T23:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.475580000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[191,"TRANSGRIDV5_20161215152814","2014-01-03T22:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.388390000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[192,"TRANSGRIDV5_20161215152814","2014-01-03T12:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.21555,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[193,"TRANSGRIDV5_20161215152814","2014-01-03T12:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.155169999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[194,"TRANSGRIDV5_20161215152814","2014-01-03T12:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.11148,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[195,"TRANSGRIDV5_20161215152814","2014-01-03T13:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.091930000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[196,"TRANSGRIDV5_20161215152814","2014-01-03T13:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.04813,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[197,"TRANSGRIDV5_20161215152814","2014-01-03T21:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.89622,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[198,"TRANSGRIDV5_20161215152814","2014-01-03T12:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.587209999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[199,"TRANSGRIDV5_20161215152814","2014-01-03T21:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.874680000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[200,"TRANSGRIDV5_20161215152814","2014-01-03T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.32892,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[201,"TRANSGRIDV5_20161215152814","2014-01-03T14:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.26491,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[202,"TRANSGRIDV5_20161215152814","2014-01-03T14:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.440079999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[203,"TRANSGRIDV5_20161215152814","2014-01-03T14:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.418800000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[204,"TRANSGRIDV5_20161215152814","2014-01-03T17:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.19190999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[205,"TRANSGRIDV5_20161215152814","2014-01-03T15:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-113.34390999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[206,"TRANSGRIDV5_20161215152814","2014-01-03T17:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-111.97681,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[207,"TRANSGRIDV5_20161215152814","2014-01-03T17:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-111.858,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[208,"TRANSGRIDV5_20161215152814","2014-01-03T16:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-111.34856000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[209,"TRANSGRIDV5_20161215152814","2014-01-03T16:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-111.1258,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[210,"TRANSGRIDV5_20161215152814","2014-01-03T14:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-108.59384,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[211,"TRANSGRIDV5_20161215152814","2014-01-03T17:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-108.36597,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[212,"TRANSGRIDV5_20161215152814","2014-01-03T17:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-108.31207999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[213,"TRANSGRIDV5_20161215152814","2014-01-03T14:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-107.99731,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[214,"TRANSGRIDV5_20161215152814","2014-01-03T12:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-104.85459,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[215,"TRANSGRIDV5_20161215152814","2014-01-03T14:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-102.79866,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[216,"TRANSGRIDV5_20161215152814","2014-01-03T13:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-99.961539999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[217,"TRANSGRIDV5_20161215152814","2014-01-03T17:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-86.289460000000005,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[218,"TRANSGRIDV5_20161215152814","2014-01-03T17:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-85.782349999999994,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[219,"TRANSGRIDV5_20161215152814","2014-01-03T13:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-69.207710000000006,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[220,"TRANSGRIDV5_20161215152814","2014-01-03T15:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-68.363630000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[221,"TRANSGRIDV5_20161215152814","2014-01-03T16:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-54.331359999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[222,"TRANSGRIDV5_20161215152814","2014-01-03T16:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-51.53539,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[223,"TRANSGRIDV5_20161215152814","2014-01-03T16:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-51.035249999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[224,"TRANSGRIDV5_20161215152814","2014-01-03T16:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-51.015059999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[225,"TRANSGRIDV5_20161215152814","2014-01-03T16:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-50.760860000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[226,"TRANSGRIDV5_20161215152814","2014-01-03T17:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-50.244340000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[227,"TRANSGRIDV5_20161215152814","2014-01-03T19:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-50.004429999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[228,"TRANSGRIDV5_20161215152814","2014-01-03T13:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-49.863160000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[229,"TRANSGRIDV5_20161215152814","2014-01-03T15:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-49.367040000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[230,"TRANSGRIDV5_20161215152814","2014-01-03T15:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-49.33746,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[231,"TRANSGRIDV5_20161215152814","2014-01-03T17:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-49.076180000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[232,"TRANSGRIDV5_20161215152814","2014-01-03T14:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.99183,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[233,"TRANSGRIDV5_20161215152814","2014-01-03T16:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.97298,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[234,"TRANSGRIDV5_20161215152814","2014-01-03T16:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.897419999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[235,"TRANSGRIDV5_20161215152814","2014-01-03T15:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.888809999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[236,"TRANSGRIDV5_20161215152814","2014-01-03T15:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.882390000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[237,"TRANSGRIDV5_20161215152814","2014-01-03T15:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.870629999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[238,"TRANSGRIDV5_20161215152814","2014-01-03T15:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.845849999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[239,"TRANSGRIDV5_20161215152814","2014-01-03T15:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.816079999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[240,"TRANSGRIDV5_20161215152814","2014-01-03T15:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.63944,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[241,"TRANSGRIDV5_20161215152814","2014-01-03T16:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.108319999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[242,"TRANSGRIDV5_20161215152814","2014-01-03T16:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.096249999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[243,"TRANSGRIDV5_20161215152814","2014-01-03T16:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.067520000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[244,"TRANSGRIDV5_20161215152814","2014-01-03T19:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.83878,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[245,"TRANSGRIDV5_20161215152814","2014-01-03T19:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.835479999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[246,"TRANSGRIDV5_20161215152814","2014-01-03T17:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.60445,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[247,"TRANSGRIDV5_20161215152814","2014-01-03T18:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.589350000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[248,"TRANSGRIDV5_20161215152814","2014-01-03T18:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.54663,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[249,"TRANSGRIDV5_20161215152814","2014-01-03T19:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.49033,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[250,"TRANSGRIDV5_20161215152814","2014-01-03T18:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.445650000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[251,"TRANSGRIDV5_20161215152814","2014-01-03T17:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.413139999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[252,"TRANSGRIDV5_20161215152814","2014-01-03T19:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.410649999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[253,"TRANSGRIDV5_20161215152814","2014-01-03T19:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.367229999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[254,"TRANSGRIDV5_20161215152814","2014-01-03T17:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.356529999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[255,"TRANSGRIDV5_20161215152814","2014-01-03T15:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.33426,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[256,"TRANSGRIDV5_20161215152814","2014-01-03T13:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.24456,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[257,"TRANSGRIDV5_20161215152814","2014-01-03T19:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.194890000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[258,"TRANSGRIDV5_20161215152814","2014-01-03T18:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.184980000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[259,"TRANSGRIDV5_20161215152814","2014-01-03T18:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.029699999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[260,"TRANSGRIDV5_20161215152814","2014-01-03T14:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-33.636450000000004,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[261,"TRANSGRIDV5_20161215152814","2014-01-03T14:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-33.454689999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[262,"TRANSGRIDV5_20161215152814","2014-01-03T13:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-33.436030000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[263,"TRANSGRIDV5_20161215152814","2014-01-03T19:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-26.102499999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[264,"TRANSGRIDV5_20161215152814","2014-01-03T20:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.948979999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[265,"TRANSGRIDV5_20161215152814","2014-01-03T18:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.936640000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[266,"TRANSGRIDV5_20161215152814","2014-01-03T18:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.918130000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[267,"TRANSGRIDV5_20161215152814","2014-01-03T18:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.89902,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[268,"TRANSGRIDV5_20161215152814","2014-01-03T18:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.89217,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[269,"TRANSGRIDV5_20161215152814","2014-01-03T13:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.8782,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[270,"TRANSGRIDV5_20161215152814","2014-01-03T19:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.87473,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[271,"TRANSGRIDV5_20161215152814","2014-01-03T13:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.86008,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[272,"TRANSGRIDV5_20161215152814","2014-01-03T13:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.63072,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[273,"TRANSGRIDV5_20161215152814","2014-01-03T18:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-25.534269999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[274,"TRANSGRIDV5_20161215152814","2014-01-03T13:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.412299999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[275,"TRANSGRIDV5_20161215152814","2014-01-03T13:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.405470000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[276,"TRANSGRIDV5_20161215152814","2014-01-03T12:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.146319999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[277,"TRANSGRIDV5_20161215152814","2014-01-03T12:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.134029999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[278,"TRANSGRIDV5_20161215152814","2014-01-03T12:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.13043,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[279,"TRANSGRIDV5_20161215152814","2014-01-03T12:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-23.50572,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[280,"TRANSGRIDV5_20161215152814","2014-01-03T18:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.450990000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[281,"TRANSGRIDV5_20161215152814","2014-01-03T21:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.303979999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[282,"TRANSGRIDV5_20161215152814","2014-01-03T18:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.166830000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[283,"TRANSGRIDV5_20161215152814","2014-01-03T19:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.109179999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[284,"TRANSGRIDV5_20161215152814","2014-01-03T19:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.105149999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[285,"TRANSGRIDV5_20161215152814","2014-01-03T19:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.023350000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[286,"TRANSGRIDV5_20161215152814","2014-01-03T21:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.543939999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[287,"TRANSGRIDV5_20161215152814","2014-01-03T14:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.303319999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[288,"TRANSGRIDV5_20161215152814","2014-01-03T14:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.262989999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[289,"TRANSGRIDV5_20161215152814","2014-01-03T22:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.14068,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[290,"TRANSGRIDV5_20161215152814","2014-01-03T23:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.029399999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[291,"TRANSGRIDV5_20161215152814","2014-01-03T22:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.931529999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[292,"TRANSGRIDV5_20161215152814","2014-01-03T12:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.906300000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[293,"TRANSGRIDV5_20161215152814","2014-01-03T12:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.781839999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[294,"TRANSGRIDV5_20161215152814","2014-01-03T12:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.756219999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[295,"TRANSGRIDV5_20161215152814","2014-01-03T13:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.709510000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[296,"TRANSGRIDV5_20161215152814","2014-01-03T23:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.689900000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[297,"TRANSGRIDV5_20161215152814","2014-01-03T13:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.681920000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[298,"TRANSGRIDV5_20161215152814","2014-01-03T12:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.603840000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[299,"TRANSGRIDV5_20161215152814","2014-01-03T12:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.591809999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[300,"TRANSGRIDV5_20161215152814","2014-01-03T12:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.53491,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[301,"TRANSGRIDV5_20161215152814","2014-01-03T22:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.426919999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[302,"TRANSGRIDV5_20161215152814","2014-01-03T14:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.416920000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[303,"TRANSGRIDV5_20161215152814","2014-01-03T23:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.371839999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[304,"TRANSGRIDV5_20161215152814","2014-01-03T12:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.371320000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[305,"TRANSGRIDV5_20161215152814","2014-01-03T14:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.33746,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[306,"TRANSGRIDV5_20161215152814","2014-01-03T21:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.024699999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[307,"TRANSGRIDV5_20161215152814","2014-01-03T15:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-14.199389999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[308,"TRANSGRIDV5_20161215152814","2014-01-03T15:10:00","N>>N-NIL__3_15M","N-NIL","2013-12-11",1,-39.661070000000002,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[309,"TRANSGRIDV5_20161215152814","2014-01-03T14:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-11.940619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[310,"TRANSGRIDV5_20161215152814","2014-01-03T14:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-12.179539999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[311,"TRANSGRIDV5_20161215152814","2014-01-03T14:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-11.80823,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[312,"TRANSGRIDV5_20161215152814","2014-01-03T14:15:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-11.766640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[313,"TRANSGRIDV5_20161215152814","2014-01-04T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11809.527050000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[314,"TRANSGRIDV5_20161215152814","2014-01-04T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10800.9467,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[315,"TRANSGRIDV5_20161215152814","2014-01-04T17:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10795.527700000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[316,"TRANSGRIDV5_20161215152814","2014-01-04T16:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1302.2427,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[317,"TRANSGRIDV5_20161215152814","2014-01-04T16:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1211.7348199999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[318,"TRANSGRIDV5_20161215152814","2014-01-04T17:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-351.90967999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[319,"TRANSGRIDV5_20161215152814","2014-01-04T12:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-220.96518,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[320,"TRANSGRIDV5_20161215152814","2014-01-04T13:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-219.32550000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[321,"TRANSGRIDV5_20161215152814","2014-01-04T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-216.43729999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[322,"TRANSGRIDV5_20161215152814","2014-01-04T13:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-211.11181999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[323,"TRANSGRIDV5_20161215152814","2014-01-04T11:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-210.17053999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[324,"TRANSGRIDV5_20161215152814","2014-01-04T11:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.98307,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[325,"TRANSGRIDV5_20161215152814","2014-01-04T12:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.55270999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[326,"TRANSGRIDV5_20161215152814","2014-01-04T13:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.53775999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[327,"TRANSGRIDV5_20161215152814","2014-01-04T17:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-208.98581999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[328,"TRANSGRIDV5_20161215152814","2014-01-04T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-206.82044999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[329,"TRANSGRIDV5_20161215152814","2014-01-04T15:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-206.55327,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[330,"TRANSGRIDV5_20161215152814","2014-01-04T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-206.47545,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[331,"TRANSGRIDV5_20161215152814","2014-01-04T15:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-206.27149,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[332,"TRANSGRIDV5_20161215152814","2014-01-04T17:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-167.53152,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[333,"TRANSGRIDV5_20161215152814","2014-01-04T13:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-128.79208,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[334,"TRANSGRIDV5_20161215152814","2014-01-04T12:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-127.90385999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[335,"TRANSGRIDV5_20161215152814","2014-01-04T13:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-127.47418999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[336,"TRANSGRIDV5_20161215152814","2014-01-04T12:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-96.476939999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[337,"TRANSGRIDV5_20161215152814","2014-01-04T16:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.778120000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[338,"TRANSGRIDV5_20161215152814","2014-01-04T09:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.267030000000005,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[339,"TRANSGRIDV5_20161215152814","2014-01-04T16:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.120350000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[340,"TRANSGRIDV5_20161215152814","2014-01-04T18:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-82.773989999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[341,"TRANSGRIDV5_20161215152814","2014-01-04T13:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-81.788730000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[342,"TRANSGRIDV5_20161215152814","2014-01-04T15:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-80.356679999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[343,"TRANSGRIDV5_20161215152814","2014-01-04T19:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.086129999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[344,"TRANSGRIDV5_20161215152814","2014-01-04T18:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.076920000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[345,"TRANSGRIDV5_20161215152814","2014-01-04T18:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.051630000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[346,"TRANSGRIDV5_20161215152814","2014-01-04T18:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.013370000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[347,"TRANSGRIDV5_20161215152814","2014-01-04T18:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.997329999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[348,"TRANSGRIDV5_20161215152814","2014-01-04T18:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.9925,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[349,"TRANSGRIDV5_20161215152814","2014-01-04T18:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.983440000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[350,"TRANSGRIDV5_20161215152814","2014-01-04T18:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.955359999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[351,"TRANSGRIDV5_20161215152814","2014-01-04T18:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.029170000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[352,"TRANSGRIDV5_20161215152814","2014-01-04T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.832039999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[353,"TRANSGRIDV5_20161215152814","2014-01-04T15:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.816940000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[354,"TRANSGRIDV5_20161215152814","2014-01-04T15:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.782170000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[355,"TRANSGRIDV5_20161215152814","2014-01-04T15:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.745440000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[356,"TRANSGRIDV5_20161215152814","2014-01-04T16:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.900359999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[357,"TRANSGRIDV5_20161215152814","2014-01-04T18:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.807139999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[358,"TRANSGRIDV5_20161215152814","2014-01-04T18:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.24729,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[359,"TRANSGRIDV5_20161215152814","2014-01-04T17:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.690730000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[360,"TRANSGRIDV5_20161215152814","2014-01-04T17:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.461399999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[361,"TRANSGRIDV5_20161215152814","2014-01-04T13:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.212670000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[362,"TRANSGRIDV5_20161215152814","2014-01-04T20:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.008710000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[363,"TRANSGRIDV5_20161215152814","2014-01-04T14:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.861660000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[364,"TRANSGRIDV5_20161215152814","2014-01-04T13:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.521320000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[365,"TRANSGRIDV5_20161215152814","2014-01-04T14:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.274940000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[366,"TRANSGRIDV5_20161215152814","2014-01-04T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.245989999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[367,"TRANSGRIDV5_20161215152814","2014-01-04T15:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.186349999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[368,"TRANSGRIDV5_20161215152814","2014-01-04T14:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.160339999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[369,"TRANSGRIDV5_20161215152814","2014-01-04T16:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.959449999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[370,"TRANSGRIDV5_20161215152814","2014-01-04T14:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.631909999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[371,"TRANSGRIDV5_20161215152814","2014-01-04T15:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.49485,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[372,"TRANSGRIDV5_20161215152814","2014-01-04T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.482509999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[373,"TRANSGRIDV5_20161215152814","2014-01-04T16:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.275919999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[374,"TRANSGRIDV5_20161215152814","2014-01-04T10:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-29.92633,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[375,"TRANSGRIDV5_20161215152814","2014-01-04T10:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-29.901140000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[376,"TRANSGRIDV5_20161215152814","2014-01-04T17:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.949639999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[377,"TRANSGRIDV5_20161215152814","2014-01-04T19:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.942869999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[378,"TRANSGRIDV5_20161215152814","2014-01-04T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-26.965959999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[379,"TRANSGRIDV5_20161215152814","2014-01-04T14:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-26.663129999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[380,"TRANSGRIDV5_20161215152814","2014-01-04T09:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.988099999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[381,"TRANSGRIDV5_20161215152814","2014-01-04T10:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.95797,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[382,"TRANSGRIDV5_20161215152814","2014-01-04T11:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.277439999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[383,"TRANSGRIDV5_20161215152814","2014-01-04T11:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.127690000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[384,"TRANSGRIDV5_20161215152814","2014-01-04T20:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.402010000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[385,"TRANSGRIDV5_20161215152814","2014-01-04T14:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.048480000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[386,"TRANSGRIDV5_20161215152814","2014-01-04T16:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-5930.5807000000004,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[387,"TRANSGRIDV5_20161215152814","2014-01-04T17:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-5442.3161799999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[388,"TRANSGRIDV5_20161215152814","2014-01-04T15:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-5428.0161200000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[389,"TRANSGRIDV5_20161215152814","2014-01-04T16:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-665.38316999999995,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[390,"TRANSGRIDV5_20161215152814","2014-01-04T16:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-619.46636999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[391,"TRANSGRIDV5_20161215152814","2014-01-04T17:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-187.67490000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[392,"TRANSGRIDV5_20161215152814","2014-01-04T15:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-119.26533999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[393,"TRANSGRIDV5_20161215152814","2014-01-04T13:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-115.96796999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[394,"TRANSGRIDV5_20161215152814","2014-01-04T12:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.93497000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[395,"TRANSGRIDV5_20161215152814","2014-01-04T15:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.43639,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[396,"TRANSGRIDV5_20161215152814","2014-01-04T15:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.29884,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[397,"TRANSGRIDV5_20161215152814","2014-01-04T15:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.26006,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[398,"TRANSGRIDV5_20161215152814","2014-01-04T15:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.25068,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[399,"TRANSGRIDV5_20161215152814","2014-01-04T17:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-112.67861000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[400,"TRANSGRIDV5_20161215152814","2014-01-04T13:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.98981000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[401,"TRANSGRIDV5_20161215152814","2014-01-04T12:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.98042,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[402,"TRANSGRIDV5_20161215152814","2014-01-04T11:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.35131,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[403,"TRANSGRIDV5_20161215152814","2014-01-04T11:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.24506,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[404,"TRANSGRIDV5_20161215152814","2014-01-04T13:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.22112,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[405,"TRANSGRIDV5_20161215152814","2014-01-04T17:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-98.106039999999993,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[406,"TRANSGRIDV5_20161215152814","2014-01-04T12:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-71.154229999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[407,"TRANSGRIDV5_20161215152814","2014-01-04T13:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-70.594650000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[408,"TRANSGRIDV5_20161215152814","2014-01-04T13:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-70.207250000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[409,"TRANSGRIDV5_20161215152814","2014-01-04T12:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-53.522759999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[410,"TRANSGRIDV5_20161215152814","2014-01-04T16:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-53.338349999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[411,"TRANSGRIDV5_20161215152814","2014-01-04T16:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-53.18159,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[412,"TRANSGRIDV5_20161215152814","2014-01-04T15:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-50.885640000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[413,"TRANSGRIDV5_20161215152814","2014-01-04T18:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.883319999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[414,"TRANSGRIDV5_20161215152814","2014-01-04T13:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-48.265239999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[415,"TRANSGRIDV5_20161215152814","2014-01-04T09:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-47.963009999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[416,"TRANSGRIDV5_20161215152814","2014-01-04T15:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-37.016379999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[417,"TRANSGRIDV5_20161215152814","2014-01-04T15:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-37.008769999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[418,"TRANSGRIDV5_20161215152814","2014-01-04T15:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-37.003869999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[419,"TRANSGRIDV5_20161215152814","2014-01-04T16:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-36.964469999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[420,"TRANSGRIDV5_20161215152814","2014-01-04T14:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-36.954219999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[421,"TRANSGRIDV5_20161215152814","2014-01-04T18:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.49053,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[422,"TRANSGRIDV5_20161215152814","2014-01-04T18:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.467129999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[423,"TRANSGRIDV5_20161215152814","2014-01-04T18:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.453989999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[424,"TRANSGRIDV5_20161215152814","2014-01-04T18:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.453949999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[425,"TRANSGRIDV5_20161215152814","2014-01-04T18:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.442419999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[426,"TRANSGRIDV5_20161215152814","2014-01-04T18:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.429879999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[427,"TRANSGRIDV5_20161215152814","2014-01-04T18:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.41395,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[428,"TRANSGRIDV5_20161215152814","2014-01-04T19:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-35.408149999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[429,"TRANSGRIDV5_20161215152814","2014-01-04T18:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-34.596739999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[430,"TRANSGRIDV5_20161215152814","2014-01-04T16:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.283919999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[431,"TRANSGRIDV5_20161215152814","2014-01-04T17:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.272259999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[432,"TRANSGRIDV5_20161215152814","2014-01-04T14:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.137689999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[433,"TRANSGRIDV5_20161215152814","2014-01-04T16:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.12612,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[434,"TRANSGRIDV5_20161215152814","2014-01-04T15:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.121300000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[435,"TRANSGRIDV5_20161215152814","2014-01-04T14:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.085129999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[436,"TRANSGRIDV5_20161215152814","2014-01-04T14:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.083729999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[437,"TRANSGRIDV5_20161215152814","2014-01-04T14:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.988320000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[438,"TRANSGRIDV5_20161215152814","2014-01-04T14:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.944659999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[439,"TRANSGRIDV5_20161215152814","2014-01-04T15:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.936879999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[440,"TRANSGRIDV5_20161215152814","2014-01-04T13:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.803999999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[441,"TRANSGRIDV5_20161215152814","2014-01-04T14:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.715499999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[442,"TRANSGRIDV5_20161215152814","2014-01-04T17:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.644659999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[443,"TRANSGRIDV5_20161215152814","2014-01-04T13:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.57161,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[444,"TRANSGRIDV5_20161215152814","2014-01-04T18:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-26.87255,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[445,"TRANSGRIDV5_20161215152814","2014-01-04T18:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-26.519850000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[446,"TRANSGRIDV5_20161215152814","2014-01-04T20:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.728899999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[447,"TRANSGRIDV5_20161215152814","2014-01-04T17:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.449809999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[448,"TRANSGRIDV5_20161215152814","2014-01-04T16:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.364460000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[449,"TRANSGRIDV5_20161215152814","2014-01-04T14:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-23.91553,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[450,"TRANSGRIDV5_20161215152814","2014-01-04T19:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.83963,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[451,"TRANSGRIDV5_20161215152814","2014-01-04T10:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.637789999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[452,"TRANSGRIDV5_20161215152814","2014-01-04T10:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-22.622070000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[453,"TRANSGRIDV5_20161215152814","2014-01-04T14:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-19.91058,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[454,"TRANSGRIDV5_20161215152814","2014-01-04T11:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-19.09037,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[455,"TRANSGRIDV5_20161215152814","2014-01-04T11:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.571380000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[456,"TRANSGRIDV5_20161215152814","2014-01-04T10:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.52731,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[457,"TRANSGRIDV5_20161215152814","2014-01-04T09:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.272130000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[458,"TRANSGRIDV5_20161215152814","2014-01-04T20:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.32347,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[459,"TRANSGRIDV5_20161215152814","2014-01-04T14:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.344480000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[460,"TRANSGRIDV5_20161215152814","2014-01-04T16:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.334009999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[461,"TRANSGRIDV5_20161215152814","2014-01-04T16:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.25395,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[462,"TRANSGRIDV5_20161215152814","2014-01-04T14:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.12679,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[463,"TRANSGRIDV5_20161215152814","2014-01-04T16:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.109669999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[464,"TRANSGRIDV5_20161215152814","2014-01-04T13:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.917310000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[465,"TRANSGRIDV5_20161215152814","2014-01-04T18:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.86964,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[466,"TRANSGRIDV5_20161215152814","2014-01-04T13:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.61876,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[467,"TRANSGRIDV5_20161215152814","2014-01-04T13:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.503909999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[468,"TRANSGRIDV5_20161215152814","2014-01-04T19:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.165789999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[469,"TRANSGRIDV5_20161215152814","2014-01-04T11:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.926399999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[470,"TRANSGRIDV5_20161215152814","2014-01-04T11:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.864979999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[471,"TRANSGRIDV5_20161215152814","2014-01-04T09:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.82605,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[472,"TRANSGRIDV5_20161215152814","2014-01-04T13:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.781549999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[473,"TRANSGRIDV5_20161215152814","2014-01-04T20:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.774039999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[474,"TRANSGRIDV5_20161215152814","2014-01-04T11:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.749029999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[475,"TRANSGRIDV5_20161215152814","2014-01-04T20:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.516450000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[476,"TRANSGRIDV5_20161215152814","2014-01-04T21:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.21832,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[477,"TRANSGRIDV5_20161215152814","2014-01-04T20:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.179500000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[478,"TRANSGRIDV5_20161215152814","2014-01-04T20:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.939780000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[479,"TRANSGRIDV5_20161215152814","2014-01-04T19:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.604559999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[480,"TRANSGRIDV5_20161215152814","2014-01-04T17:35:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-18.60614,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[481,"TRANSGRIDV5_20161215152814","2014-01-05T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.67232000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[482,"TRANSGRIDV5_20161215152814","2014-01-05T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.67061000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[483,"TRANSGRIDV5_20161215152814","2014-01-05T15:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.63059000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[484,"TRANSGRIDV5_20161215152814","2014-01-05T19:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-54.655650000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[485,"TRANSGRIDV5_20161215152814","2014-01-05T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.867329999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[486,"TRANSGRIDV5_20161215152814","2014-01-05T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.749040000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[487,"TRANSGRIDV5_20161215152814","2014-01-05T15:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-103.87218,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[488,"TRANSGRIDV5_20161215152814","2014-01-05T14:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-103.59838999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[489,"TRANSGRIDV5_20161215152814","2014-01-05T15:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-103.59764,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[490,"TRANSGRIDV5_20161215152814","2014-01-05T19:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-33.567219999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[491,"TRANSGRIDV5_20161215152814","2014-01-05T15:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-17.752649999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[492,"TRANSGRIDV5_20161215152814","2014-01-05T14:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-16.96303,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[493,"TRANSGRIDV5_20161215152814","2014-01-05T18:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-12.114240000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[494,"TRANSGRIDV5_20161215152814","2014-01-05T18:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.55119,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[495,"TRANSGRIDV5_20161215152814","2014-01-05T15:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.924810000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[496,"TRANSGRIDV5_20161215152814","2014-01-05T16:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.33751,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[497,"TRANSGRIDV5_20161215152814","2014-01-05T15:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-81.799840000000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[498,"TRANSGRIDV5_20161215152814","2014-01-05T08:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-79.813879999999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[499,"TRANSGRIDV5_20161215152814","2014-01-05T15:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-70.846630000000005,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[500,"TRANSGRIDV5_20161215152814","2014-01-05T08:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-29.390149999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[501,"TRANSGRIDV5_20161215152814","2014-01-06T09:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11860.56935,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[502,"TRANSGRIDV5_20161215152814","2014-01-06T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1323.37832,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[503,"TRANSGRIDV5_20161215152814","2014-01-06T15:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1313.28557,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[504,"TRANSGRIDV5_20161215152814","2014-01-06T15:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1311.0125800000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[505,"TRANSGRIDV5_20161215152814","2014-01-06T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-219.88452000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[506,"TRANSGRIDV5_20161215152814","2014-01-06T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-218.16987,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[507,"TRANSGRIDV5_20161215152814","2014-01-06T13:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-218.03892999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[508,"TRANSGRIDV5_20161215152814","2014-01-06T13:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-217.98568,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[509,"TRANSGRIDV5_20161215152814","2014-01-06T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-216.70003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[510,"TRANSGRIDV5_20161215152814","2014-01-06T08:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-213.00315000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[511,"TRANSGRIDV5_20161215152814","2014-01-06T12:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.61684,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[512,"TRANSGRIDV5_20161215152814","2014-01-06T13:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-209.31589,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[513,"TRANSGRIDV5_20161215152814","2014-01-06T14:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-208.32863,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[514,"TRANSGRIDV5_20161215152814","2014-01-06T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-207.34869,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[515,"TRANSGRIDV5_20161215152814","2014-01-06T14:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-93.266710000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[516,"TRANSGRIDV5_20161215152814","2014-01-06T13:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-93.248980000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[517,"TRANSGRIDV5_20161215152814","2014-01-06T08:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.935200000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[518,"TRANSGRIDV5_20161215152814","2014-01-06T13:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.371989999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[519,"TRANSGRIDV5_20161215152814","2014-01-06T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.040930000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[520,"TRANSGRIDV5_20161215152814","2014-01-06T14:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.669170000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[521,"TRANSGRIDV5_20161215152814","2014-01-06T11:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.783740000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[522,"TRANSGRIDV5_20161215152814","2014-01-06T12:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.203589999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[523,"TRANSGRIDV5_20161215152814","2014-01-06T12:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.011330000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[524,"TRANSGRIDV5_20161215152814","2014-01-06T09:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-5760.4751900000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[525,"TRANSGRIDV5_20161215152814","2014-01-06T15:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-657.81658000000004,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[526,"TRANSGRIDV5_20161215152814","2014-01-06T15:05:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-656.90504999999996,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[527,"TRANSGRIDV5_20161215152814","2014-01-06T15:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-651.44759999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[528,"TRANSGRIDV5_20161215152814","2014-01-06T14:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-117.50785,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[529,"TRANSGRIDV5_20161215152814","2014-01-06T15:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-116.05875,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[530,"TRANSGRIDV5_20161215152814","2014-01-06T13:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-115.34251,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[531,"TRANSGRIDV5_20161215152814","2014-01-06T13:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-115.30896,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[532,"TRANSGRIDV5_20161215152814","2014-01-06T14:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.89221999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[533,"TRANSGRIDV5_20161215152814","2014-01-06T12:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.41794,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[534,"TRANSGRIDV5_20161215152814","2014-01-06T13:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-114.08487,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[535,"TRANSGRIDV5_20161215152814","2014-01-06T14:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-113.09262,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[536,"TRANSGRIDV5_20161215152814","2014-01-06T14:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.27803,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[537,"TRANSGRIDV5_20161215152814","2014-01-06T08:25:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-104.92014,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[538,"TRANSGRIDV5_20161215152814","2014-01-06T13:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-54.59554,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[539,"TRANSGRIDV5_20161215152814","2014-01-06T14:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-54.584359999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[540,"TRANSGRIDV5_20161215152814","2014-01-06T15:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-27.085640000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[541,"TRANSGRIDV5_20161215152814","2014-01-06T13:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-26.927949999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[542,"TRANSGRIDV5_20161215152814","2014-01-06T14:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-26.365559999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[543,"TRANSGRIDV5_20161215152814","2014-01-06T08:20:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-24.533270000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[544,"TRANSGRIDV5_20161215152814","2014-01-06T12:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-19.92267,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[545,"TRANSGRIDV5_20161215152814","2014-01-06T12:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.539159999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[546,"TRANSGRIDV5_20161215152814","2014-01-06T11:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-18.173660000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[547,"TRANSGRIDV5_20161215152814","2014-01-06T14:40:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.779439999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[548,"TRANSGRIDV5_20161215152814","2014-01-06T14:45:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.18511,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[549,"TRANSGRIDV5_20161215152814","2014-01-09T09:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-15.35571,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[550,"TRANSGRIDV5_20161215152814","2014-01-09T13:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-14.37093,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[551,"TRANSGRIDV5_20161215152814","2014-01-09T13:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-13.376110000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[552,"TRANSGRIDV5_20161215152814","2014-01-09T12:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-13.15014,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[553,"TRANSGRIDV5_20161215152814","2014-01-09T11:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-11.312469999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[554,"TRANSGRIDV5_20161215152814","2014-01-09T07:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-10.888500000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[555,"TRANSGRIDV5_20161215152814","2014-01-10T14:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-52.617570000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[556,"TRANSGRIDV5_20161215152814","2014-01-10T15:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-30.661580000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[557,"TRANSGRIDV5_20161215152814","2014-01-10T15:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27.267029999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[558,"TRANSGRIDV5_20161215152814","2014-01-10T16:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-21.596550000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[559,"TRANSGRIDV5_20161215152814","2014-01-10T16:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-19.497250000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[560,"TRANSGRIDV5_20161215152814","2014-01-10T14:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-19.249939999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[561,"TRANSGRIDV5_20161215152814","2014-01-10T15:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-16.591930000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[562,"TRANSGRIDV5_20161215152814","2014-01-10T13:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-16.474730000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[563,"TRANSGRIDV5_20161215152814","2014-01-10T11:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-13.93731,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[564,"TRANSGRIDV5_20161215152814","2014-01-10T14:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-13.451090000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[565,"TRANSGRIDV5_20161215152814","2014-01-10T14:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-13.24921,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[566,"TRANSGRIDV5_20161215152814","2014-01-10T14:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-13.23842,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[567,"TRANSGRIDV5_20161215152814","2014-01-10T14:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-12.17864,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[568,"TRANSGRIDV5_20161215152814","2014-01-10T14:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-12.03294,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[569,"TRANSGRIDV5_20161215152814","2014-01-10T11:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.95149,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[570,"TRANSGRIDV5_20161215152814","2014-01-10T11:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.441420000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[571,"TRANSGRIDV5_20161215152814","2014-01-10T14:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.39485,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[572,"TRANSGRIDV5_20161215152814","2014-01-10T11:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.319279999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[573,"TRANSGRIDV5_20161215152814","2014-01-10T10:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-10.778650000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[574,"TRANSGRIDV5_20161215152814","2014-01-10T10:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-10.23964,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[575,"TRANSGRIDV5_20161215152814","2014-01-10T17:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-12.94333,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[576,"TRANSGRIDV5_20161215152814","2014-01-10T16:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-46.334780000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[577,"TRANSGRIDV5_20161215152814","2014-01-10T16:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-43.051479999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[578,"TRANSGRIDV5_20161215152814","2014-01-10T16:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-41.363160000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[579,"TRANSGRIDV5_20161215152814","2014-01-10T16:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-41.040669999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[580,"TRANSGRIDV5_20161215152814","2014-01-10T16:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-38.311190000000003,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[581,"TRANSGRIDV5_20161215152814","2014-01-10T16:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-36.240279999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[582,"TRANSGRIDV5_20161215152814","2014-01-10T16:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-33.426990000000004,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[583,"TRANSGRIDV5_20161215152814","2014-01-10T16:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-33.129370000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[584,"TRANSGRIDV5_20161215152814","2014-01-10T15:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-30.744700000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[585,"TRANSGRIDV5_20161215152814","2014-01-10T16:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-26.01914,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[586,"TRANSGRIDV5_20161215152814","2014-01-10T14:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-25.963380000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[587,"TRANSGRIDV5_20161215152814","2014-01-10T14:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-23.86542,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[588,"TRANSGRIDV5_20161215152814","2014-01-10T21:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-18.5946,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[589,"TRANSGRIDV5_20161215152814","2014-01-10T14:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-18.495550000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[590,"TRANSGRIDV5_20161215152814","2014-01-10T20:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-17.793389999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[591,"TRANSGRIDV5_20161215152814","2014-01-10T20:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-17.037240000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[592,"TRANSGRIDV5_20161215152814","2014-01-10T21:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-16.262640000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[593,"TRANSGRIDV5_20161215152814","2014-01-10T20:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-16.110959999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[594,"TRANSGRIDV5_20161215152814","2014-01-10T20:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-12.35643,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[595,"TRANSGRIDV5_20161215152814","2014-01-10T20:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-12.18308,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[596,"TRANSGRIDV5_20161215152814","2014-01-10T20:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-11.822789999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[597,"TRANSGRIDV5_20161215152814","2014-01-10T17:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-11.55594,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[598,"TRANSGRIDV5_20161215152814","2014-01-10T11:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-21.596050000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[599,"TRANSGRIDV5_20161215152814","2014-01-10T10:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-21.179849999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[600,"TRANSGRIDV5_20161215152814","2014-01-10T10:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-16.99559,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[601,"TRANSGRIDV5_20161215152814","2014-01-10T10:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-12.27183,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[602,"TRANSGRIDV5_20161215152814","2014-01-10T09:25:00","VSML_220","V-NIL","2012-07-04",1,-16.724720000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[603,"TRANSGRIDV5_20161215152814","2014-01-10T09:30:00","VSML_220","V-NIL","2012-07-04",1,-16.667190000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[604,"TRANSGRIDV5_20161215152814","2014-01-10T09:35:00","VSML_220","V-NIL","2012-07-04",1,-16.640609999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[605,"TRANSGRIDV5_20161215152814","2014-01-10T10:00:00","VSML_220","V-NIL","2012-07-04",1,-16.539339999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[606,"TRANSGRIDV5_20161215152814","2014-01-10T09:10:00","VSML_220","V-NIL","2012-07-04",1,-16.108440000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[607,"TRANSGRIDV5_20161215152814","2014-01-10T09:20:00","VSML_220","V-NIL","2012-07-04",1,-16.05911,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[608,"TRANSGRIDV5_20161215152814","2014-01-10T09:15:00","VSML_220","V-NIL","2012-07-04",1,-16.029309999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[609,"TRANSGRIDV5_20161215152814","2014-01-10T09:40:00","VSML_220","V-NIL","2012-07-04",1,-15.962149999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[610,"TRANSGRIDV5_20161215152814","2014-01-10T09:45:00","VSML_220","V-NIL","2012-07-04",1,-15.926920000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[611,"TRANSGRIDV5_20161215152814","2014-01-10T09:50:00","VSML_220","V-NIL","2012-07-04",1,-15.91376,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[612,"TRANSGRIDV5_20161215152814","2014-01-10T08:50:00","VSML_220","V-NIL","2012-07-04",1,-15.381769999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[613,"TRANSGRIDV5_20161215152814","2014-01-10T09:55:00","VSML_220","V-NIL","2012-07-04",1,-15.21625,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[614,"TRANSGRIDV5_20161215152814","2014-01-10T10:10:00","VSML_220","V-NIL","2012-07-04",1,-15.15361,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[615,"TRANSGRIDV5_20161215152814","2014-01-10T08:45:00","VSML_220","V-NIL","2012-07-04",1,-14.78558,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[616,"TRANSGRIDV5_20161215152814","2014-01-10T10:15:00","VSML_220","V-NIL","2012-07-04",1,-14.3962,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[617,"TRANSGRIDV5_20161215152814","2014-01-10T10:20:00","VSML_220","V-NIL","2012-07-04",1,-13.62396,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[618,"TRANSGRIDV5_20161215152814","2014-01-10T10:25:00","VSML_220","V-NIL","2012-07-04",1,-13.604609999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[619,"TRANSGRIDV5_20161215152814","2014-01-12T18:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-55.105649999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[620,"TRANSGRIDV5_20161215152814","2014-01-12T18:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-55.105649999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[621,"TRANSGRIDV5_20161215152814","2014-01-12T18:55:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-54.694229999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[622,"TRANSGRIDV5_20161215152814","2014-01-12T18:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-54.526090000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[623,"TRANSGRIDV5_20161215152814","2014-01-12T16:55:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844990000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[624,"TRANSGRIDV5_20161215152814","2014-01-12T17:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844729999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[625,"TRANSGRIDV5_20161215152814","2014-01-12T17:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[626,"TRANSGRIDV5_20161215152814","2014-01-12T17:55:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[627,"TRANSGRIDV5_20161215152814","2014-01-12T18:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[628,"TRANSGRIDV5_20161215152814","2014-01-12T18:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[629,"TRANSGRIDV5_20161215152814","2014-01-12T18:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[630,"TRANSGRIDV5_20161215152814","2014-01-12T18:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844610000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[631,"TRANSGRIDV5_20161215152814","2014-01-12T17:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-53.844540000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[632,"TRANSGRIDV5_20161215152814","2014-01-12T17:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.672780000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[633,"TRANSGRIDV5_20161215152814","2014-01-12T18:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583950000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[634,"TRANSGRIDV5_20161215152814","2014-01-12T17:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583620000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[635,"TRANSGRIDV5_20161215152814","2014-01-12T17:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583559999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[636,"TRANSGRIDV5_20161215152814","2014-01-12T17:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583559999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[637,"TRANSGRIDV5_20161215152814","2014-01-12T18:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583559999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[638,"TRANSGRIDV5_20161215152814","2014-01-12T18:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583559999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[639,"TRANSGRIDV5_20161215152814","2014-01-12T18:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583559999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[640,"TRANSGRIDV5_20161215152814","2014-01-12T17:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-52.583359999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[641,"TRANSGRIDV5_20161215152814","2014-01-12T16:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.777880000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[642,"TRANSGRIDV5_20161215152814","2014-01-12T16:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.547629999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[643,"TRANSGRIDV5_20161215152814","2014-01-12T16:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.322519999999997,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[644,"TRANSGRIDV5_20161215152814","2014-01-12T16:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.322450000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[645,"TRANSGRIDV5_20161215152814","2014-01-12T17:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.322450000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[646,"TRANSGRIDV5_20161215152814","2014-01-12T17:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.322450000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[647,"TRANSGRIDV5_20161215152814","2014-01-12T17:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-51.305950000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[648,"TRANSGRIDV5_20161215152814","2014-01-12T16:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-47.57123,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[649,"TRANSGRIDV5_20161215152814","2014-01-12T19:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-32.41281,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[650,"TRANSGRIDV5_20161215152814","2014-01-12T19:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-25.875910000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[651,"TRANSGRIDV5_20161215152814","2014-01-12T19:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.735759999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[652,"TRANSGRIDV5_20161215152814","2014-01-12T19:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.735759999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[653,"TRANSGRIDV5_20161215152814","2014-01-12T19:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.735759999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[654,"TRANSGRIDV5_20161215152814","2014-01-12T19:30:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.735759999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[655,"TRANSGRIDV5_20161215152814","2014-01-12T19:35:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.735759999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[656,"TRANSGRIDV5_20161215152814","2014-01-12T19:40:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.71152,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[657,"TRANSGRIDV5_20161215152814","2014-01-12T19:45:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.687750000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[658,"TRANSGRIDV5_20161215152814","2014-01-12T19:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-23.59562,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[659,"TRANSGRIDV5_20161215152814","2014-01-12T19:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-21.883990000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[660,"TRANSGRIDV5_20161215152814","2014-01-12T16:25:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-21.470659999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[661,"TRANSGRIDV5_20161215152814","2014-01-12T16:15:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-20.2987,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[662,"TRANSGRIDV5_20161215152814","2014-01-12T16:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-19.601469999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[663,"TRANSGRIDV5_20161215152814","2014-01-12T16:00:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-16.6373,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[664,"TRANSGRIDV5_20161215152814","2014-01-12T16:20:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-16.609190000000002,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[665,"TRANSGRIDV5_20161215152814","2014-01-12T16:10:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-15.610860000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[666,"TRANSGRIDV5_20161215152814","2014-01-12T15:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-25.659949999999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[667,"TRANSGRIDV5_20161215152814","2014-01-12T15:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-24.800650000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[668,"TRANSGRIDV5_20161215152814","2014-01-12T15:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-24.036560000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[669,"TRANSGRIDV5_20161215152814","2014-01-12T15:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-23.279409999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[670,"TRANSGRIDV5_20161215152814","2014-01-12T15:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-22.21237,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[671,"TRANSGRIDV5_20161215152814","2014-01-12T15:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-19.126740000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[672,"TRANSGRIDV5_20161215152814","2014-01-12T15:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-17.95478,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[673,"TRANSGRIDV5_20161215152814","2014-01-12T15:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-16.846070000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[674,"TRANSGRIDV5_20161215152814","2014-01-13T15:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-476.00495999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[675,"TRANSGRIDV5_20161215152814","2014-01-13T16:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-197.47389999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[676,"TRANSGRIDV5_20161215152814","2014-01-13T16:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-196.09531000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[677,"TRANSGRIDV5_20161215152814","2014-01-13T13:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-183.73633000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[678,"TRANSGRIDV5_20161215152814","2014-01-13T17:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.287939999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[679,"TRANSGRIDV5_20161215152814","2014-01-13T17:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27.057189999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[680,"TRANSGRIDV5_20161215152814","2014-01-13T17:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-25.81683,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[681,"TRANSGRIDV5_20161215152814","2014-01-13T17:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-25.369499999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[682,"TRANSGRIDV5_20161215152814","2014-01-13T14:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.86721,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[683,"TRANSGRIDV5_20161215152814","2014-01-13T18:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.72017,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[684,"TRANSGRIDV5_20161215152814","2014-01-13T17:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.317530000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[685,"TRANSGRIDV5_20161215152814","2014-01-13T17:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.303090000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[686,"TRANSGRIDV5_20161215152814","2014-01-13T14:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.048660000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[687,"TRANSGRIDV5_20161215152814","2014-01-13T17:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-22.917359999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[688,"TRANSGRIDV5_20161215152814","2014-01-13T14:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-22.171990000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[689,"TRANSGRIDV5_20161215152814","2014-01-13T14:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-21.507860000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[690,"TRANSGRIDV5_20161215152814","2014-01-13T17:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-20.671220000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[691,"TRANSGRIDV5_20161215152814","2014-01-13T15:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-19.352869999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[692,"TRANSGRIDV5_20161215152814","2014-01-13T18:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.446859999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[693,"TRANSGRIDV5_20161215152814","2014-01-13T18:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.39141,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[694,"TRANSGRIDV5_20161215152814","2014-01-13T18:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.02885,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[695,"TRANSGRIDV5_20161215152814","2014-01-13T18:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.956810000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[696,"TRANSGRIDV5_20161215152814","2014-01-13T18:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.769869999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[697,"TRANSGRIDV5_20161215152814","2014-01-13T18:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.41583,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[698,"TRANSGRIDV5_20161215152814","2014-01-13T19:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-11.75484,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[699,"TRANSGRIDV5_20161215152814","2014-01-13T18:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-11.28506,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[700,"TRANSGRIDV5_20161215152814","2014-01-13T13:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.85582,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[701,"TRANSGRIDV5_20161215152814","2014-01-13T15:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.214370000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[702,"TRANSGRIDV5_20161215152814","2014-01-13T18:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.036060000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[703,"TRANSGRIDV5_20161215152814","2014-01-13T15:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-17.257300000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[704,"TRANSGRIDV5_20161215152814","2014-01-13T16:35:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-13551.3007,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[705,"TRANSGRIDV5_20161215152814","2014-01-13T16:45:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-13543.382449999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[706,"TRANSGRIDV5_20161215152814","2014-01-13T16:40:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-13511.96019,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[707,"TRANSGRIDV5_20161215152814","2014-01-13T16:30:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-319.86658999999997,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[708,"TRANSGRIDV5_20161215152814","2014-01-13T16:25:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-158.57981000000001,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[709,"TRANSGRIDV5_20161215152814","2014-01-13T16:20:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-28.80322,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[710,"TRANSGRIDV5_20161215152814","2014-01-13T16:15:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-24.97043,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[711,"TRANSGRIDV5_20161215152814","2014-01-13T16:50:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-20.730599999999999,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[712,"TRANSGRIDV5_20161215152814","2014-01-13T16:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-73371.617440000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[713,"TRANSGRIDV5_20161215152814","2014-01-13T16:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-73370.215590000007,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[714,"TRANSGRIDV5_20161215152814","2014-01-13T16:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-72299.898289999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[715,"TRANSGRIDV5_20161215152814","2014-01-13T16:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-2818.8423200000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[716,"TRANSGRIDV5_20161215152814","2014-01-13T15:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-2484.5502200000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[717,"TRANSGRIDV5_20161215152814","2014-01-13T16:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-1938.9066700000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[718,"TRANSGRIDV5_20161215152814","2014-01-13T13:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-1148.4338,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[719,"TRANSGRIDV5_20161215152814","2014-01-13T16:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-386.83904000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[720,"TRANSGRIDV5_20161215152814","2014-01-13T16:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36.975099999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[721,"TRANSGRIDV5_20161215152814","2014-01-13T21:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-31.237120000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[722,"TRANSGRIDV5_20161215152814","2014-01-13T21:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-30.491409999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[723,"TRANSGRIDV5_20161215152814","2014-01-13T16:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-73638.80429,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[724,"TRANSGRIDV5_20161215152814","2014-01-13T16:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-73637.113800000006,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[725,"TRANSGRIDV5_20161215152814","2014-01-13T16:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-72362.479879999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[726,"TRANSGRIDV5_20161215152814","2014-01-13T16:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-3124.92094,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[727,"TRANSGRIDV5_20161215152814","2014-01-13T15:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-2768.1964200000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[728,"TRANSGRIDV5_20161215152814","2014-01-13T16:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-2245.86303,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[729,"TRANSGRIDV5_20161215152814","2014-01-13T13:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-1357.2222300000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[730,"TRANSGRIDV5_20161215152814","2014-01-13T16:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-653.73690999999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[731,"TRANSGRIDV5_20161215152814","2014-01-13T16:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-300.62178,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[732,"TRANSGRIDV5_20161215152814","2014-01-13T15:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-271.23975999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[733,"TRANSGRIDV5_20161215152814","2014-01-13T14:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-269.2133,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[734,"TRANSGRIDV5_20161215152814","2014-01-13T17:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-268.93011000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[735,"TRANSGRIDV5_20161215152814","2014-01-13T14:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-264.95663000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[736,"TRANSGRIDV5_20161215152814","2014-01-13T15:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-264.86603000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[737,"TRANSGRIDV5_20161215152814","2014-01-13T16:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-263.64677,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[738,"TRANSGRIDV5_20161215152814","2014-01-13T16:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-263.13393000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[739,"TRANSGRIDV5_20161215152814","2014-01-13T14:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-262.93101000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[740,"TRANSGRIDV5_20161215152814","2014-01-13T14:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-262.63074999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[741,"TRANSGRIDV5_20161215152814","2014-01-13T15:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-260.80142999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[742,"TRANSGRIDV5_20161215152814","2014-01-13T17:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-256.73750999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[743,"TRANSGRIDV5_20161215152814","2014-01-13T15:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-256.73701999999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[744,"TRANSGRIDV5_20161215152814","2014-01-13T15:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-255.02809999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[745,"TRANSGRIDV5_20161215152814","2014-01-13T18:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-254.70518999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[746,"TRANSGRIDV5_20161215152814","2014-01-13T17:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-253.80192,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[747,"TRANSGRIDV5_20161215152814","2014-01-13T17:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-252.67294000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[748,"TRANSGRIDV5_20161215152814","2014-01-13T17:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-252.67294000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[749,"TRANSGRIDV5_20161215152814","2014-01-13T17:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-251.71717000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[750,"TRANSGRIDV5_20161215152814","2014-01-13T17:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-250.81720999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[751,"TRANSGRIDV5_20161215152814","2014-01-13T17:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-249.63242,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[752,"TRANSGRIDV5_20161215152814","2014-01-13T15:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-247.60992999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[753,"TRANSGRIDV5_20161215152814","2014-01-13T15:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-244.40246999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[754,"TRANSGRIDV5_20161215152814","2014-01-13T16:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-244.20455000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[755,"TRANSGRIDV5_20161215152814","2014-01-13T13:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-201.15593000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[756,"TRANSGRIDV5_20161215152814","2014-01-13T12:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-159.47689,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[757,"TRANSGRIDV5_20161215152814","2014-01-13T13:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-158.85136,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[758,"TRANSGRIDV5_20161215152814","2014-01-13T14:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-157.04855000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[759,"TRANSGRIDV5_20161215152814","2014-01-13T13:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-155.43818999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[760,"TRANSGRIDV5_20161215152814","2014-01-13T14:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-153.82782,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[761,"TRANSGRIDV5_20161215152814","2014-01-13T14:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-153.82782,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[762,"TRANSGRIDV5_20161215152814","2014-01-13T14:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-152.21745000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[763,"TRANSGRIDV5_20161215152814","2014-01-13T16:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-151.88293999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[764,"TRANSGRIDV5_20161215152814","2014-01-13T12:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-150.62836999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[765,"TRANSGRIDV5_20161215152814","2014-01-13T14:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-150.60708,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[766,"TRANSGRIDV5_20161215152814","2014-01-13T14:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-148.99671000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[767,"TRANSGRIDV5_20161215152814","2014-01-13T13:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-148.02538000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[768,"TRANSGRIDV5_20161215152814","2014-01-13T15:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-147.38633999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[769,"TRANSGRIDV5_20161215152814","2014-01-13T11:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-146.60449,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[770,"TRANSGRIDV5_20161215152814","2014-01-13T16:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-146.07516000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[771,"TRANSGRIDV5_20161215152814","2014-01-13T14:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-145.77597,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[772,"TRANSGRIDV5_20161215152814","2014-01-13T13:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-144.51132999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[773,"TRANSGRIDV5_20161215152814","2014-01-13T13:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-144.51132999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[774,"TRANSGRIDV5_20161215152814","2014-01-13T13:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-142.69638,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[775,"TRANSGRIDV5_20161215152814","2014-01-13T12:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-142.55527000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[776,"TRANSGRIDV5_20161215152814","2014-01-13T14:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-140.22971999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[777,"TRANSGRIDV5_20161215152814","2014-01-13T13:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-139.69648000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[778,"TRANSGRIDV5_20161215152814","2014-01-13T12:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-137.71164999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[779,"TRANSGRIDV5_20161215152814","2014-01-13T12:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-136.41152,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[780,"TRANSGRIDV5_20161215152814","2014-01-13T12:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-134.24602999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[781,"TRANSGRIDV5_20161215152814","2014-01-13T12:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-130.76799,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[782,"TRANSGRIDV5_20161215152814","2014-01-13T12:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-129.82114000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[783,"TRANSGRIDV5_20161215152814","2014-01-13T15:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-79.773009999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[784,"TRANSGRIDV5_20161215152814","2014-01-13T13:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-62.645760000000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[785,"TRANSGRIDV5_20161215152814","2014-01-13T13:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-33.272799999999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[786,"TRANSGRIDV5_20161215152814","2014-01-13T11:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-22.26566,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[787,"TRANSGRIDV5_20161215152814","2014-01-13T11:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-16.22353,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[788,"TRANSGRIDV5_20161215152814","2014-01-13T18:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-252.67293000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[789,"TRANSGRIDV5_20161215152814","2014-01-13T18:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-252.67271,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[790,"TRANSGRIDV5_20161215152814","2014-01-13T18:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-250.64089999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[791,"TRANSGRIDV5_20161215152814","2014-01-13T19:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-250.64080000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[792,"TRANSGRIDV5_20161215152814","2014-01-13T19:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-250.64080000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[793,"TRANSGRIDV5_20161215152814","2014-01-13T19:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-250.15978000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[794,"TRANSGRIDV5_20161215152814","2014-01-13T17:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-249.63242,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[795,"TRANSGRIDV5_20161215152814","2014-01-13T17:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-249.63242,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[796,"TRANSGRIDV5_20161215152814","2014-01-13T18:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-249.63242,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[797,"TRANSGRIDV5_20161215152814","2014-01-13T19:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-249.63242,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[798,"TRANSGRIDV5_20161215152814","2014-01-13T19:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-248.60865000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[799,"TRANSGRIDV5_20161215152814","2014-01-13T19:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-248.60840999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[800,"TRANSGRIDV5_20161215152814","2014-01-13T18:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-247.54767000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[801,"TRANSGRIDV5_20161215152814","2014-01-13T19:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.57661999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[802,"TRANSGRIDV5_20161215152814","2014-01-13T18:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.55081999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[803,"TRANSGRIDV5_20161215152814","2014-01-13T18:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.55081999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[804,"TRANSGRIDV5_20161215152814","2014-01-13T18:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.55070000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[805,"TRANSGRIDV5_20161215152814","2014-01-13T18:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.55070000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[806,"TRANSGRIDV5_20161215152814","2014-01-13T18:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.54071999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[807,"TRANSGRIDV5_20161215152814","2014-01-13T17:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-246.54064,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[808,"TRANSGRIDV5_20161215152814","2014-01-13T17:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-244.40246999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[809,"TRANSGRIDV5_20161215152814","2014-01-13T18:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-244.40246999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[810,"TRANSGRIDV5_20161215152814","2014-01-13T20:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-242.51192,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[811,"TRANSGRIDV5_20161215152814","2014-01-13T19:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-241.29340999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[812,"TRANSGRIDV5_20161215152814","2014-01-13T20:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-229.09868,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[813,"TRANSGRIDV5_20161215152814","2014-01-13T19:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-178.71732,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[814,"TRANSGRIDV5_20161215152814","2014-01-13T20:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-152.82432,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[815,"TRANSGRIDV5_20161215152814","2014-01-13T19:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-149.77790999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[816,"TRANSGRIDV5_20161215152814","2014-01-13T19:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-148.43879999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[817,"TRANSGRIDV5_20161215152814","2014-01-13T19:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-146.47964999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[818,"TRANSGRIDV5_20161215152814","2014-01-13T20:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-145.45257000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[819,"TRANSGRIDV5_20161215152814","2014-01-13T20:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-143.66437999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[820,"TRANSGRIDV5_20161215152814","2014-01-13T20:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-142.18681000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[821,"TRANSGRIDV5_20161215152814","2014-01-13T20:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-142.11528000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[822,"TRANSGRIDV5_20161215152814","2014-01-13T20:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-142.11528000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[823,"TRANSGRIDV5_20161215152814","2014-01-13T12:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-141.83671000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[824,"TRANSGRIDV5_20161215152814","2014-01-13T12:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-141.42654999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[825,"TRANSGRIDV5_20161215152814","2014-01-13T20:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-140.57076000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[826,"TRANSGRIDV5_20161215152814","2014-01-13T20:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-140.48903000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[827,"TRANSGRIDV5_20161215152814","2014-01-13T20:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-140.48903000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[828,"TRANSGRIDV5_20161215152814","2014-01-13T12:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-139.39036999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[829,"TRANSGRIDV5_20161215152814","2014-01-13T20:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-139.33450999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[830,"TRANSGRIDV5_20161215152814","2014-01-13T12:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-138.54364000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[831,"TRANSGRIDV5_20161215152814","2014-01-13T11:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-137.60607999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[832,"TRANSGRIDV5_20161215152814","2014-01-13T11:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-136.58349999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[833,"TRANSGRIDV5_20161215152814","2014-01-13T11:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-136.58349999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[834,"TRANSGRIDV5_20161215152814","2014-01-13T13:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-136.07500999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[835,"TRANSGRIDV5_20161215152814","2014-01-13T11:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-135.89272,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[836,"TRANSGRIDV5_20161215152814","2014-01-13T11:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-135.51025000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[837,"TRANSGRIDV5_20161215152814","2014-01-13T11:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-135.24999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[838,"TRANSGRIDV5_20161215152814","2014-01-13T10:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-128.21940000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[839,"TRANSGRIDV5_20161215152814","2014-01-13T11:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-122.03228,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[840,"TRANSGRIDV5_20161215152814","2014-01-13T11:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-121.11514,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[841,"TRANSGRIDV5_20161215152814","2014-01-13T11:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-114.1306,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[842,"TRANSGRIDV5_20161215152814","2014-01-13T10:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-111.54752000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[843,"TRANSGRIDV5_20161215152814","2014-01-13T21:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-89.053120000000007,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[844,"TRANSGRIDV5_20161215152814","2014-01-13T11:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-87.401499999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[845,"TRANSGRIDV5_20161215152814","2014-01-13T13:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-76.132189999999994,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[846,"TRANSGRIDV5_20161215152814","2014-01-13T11:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-48.710470000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[847,"TRANSGRIDV5_20161215152814","2014-01-13T21:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-45.64743,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[848,"TRANSGRIDV5_20161215152814","2014-01-13T10:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-21.585000000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[849,"TRANSGRIDV5_20161215152814","2014-01-13T10:25:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-21.30951,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[850,"TRANSGRIDV5_20161215152814","2014-01-13T10:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-20.359729999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[851,"TRANSGRIDV5_20161215152814","2014-01-13T10:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-20.20664,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[852,"TRANSGRIDV5_20161215152814","2014-01-13T10:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-19.145910000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[853,"TRANSGRIDV5_20161215152814","2014-01-13T10:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-18.85014,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[854,"TRANSGRIDV5_20161215152814","2014-01-13T10:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-18.492180000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[855,"TRANSGRIDV5_20161215152814","2014-01-13T10:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-17.909210000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[856,"TRANSGRIDV5_20161215152814","2014-01-13T10:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-17.615919999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[857,"TRANSGRIDV5_20161215152814","2014-01-13T10:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-15.060029999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[858,"TRANSGRIDV5_20161215152814","2014-01-13T09:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-13.635759999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[859,"TRANSGRIDV5_20161215152814","2014-01-13T09:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-13.035080000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[860,"TRANSGRIDV5_20161215152814","2014-01-13T09:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-11.01116,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[861,"TRANSGRIDV5_20161215152814","2014-01-13T08:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-10.68647,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[862,"TRANSGRIDV5_20161215152814","2014-01-13T08:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-10.669,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[863,"TRANSGRIDV5_20161215152814","2014-01-13T08:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-10.01473,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[864,"TRANSGRIDV5_20161215152814","2014-01-13T15:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-251.71717000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[865,"TRANSGRIDV5_20161215152814","2014-01-13T15:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-246.54071999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[866,"TRANSGRIDV5_20161215152814","2014-01-13T15:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-166.953,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[867,"TRANSGRIDV5_20161215152814","2014-01-13T13:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-111.47698,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[868,"TRANSGRIDV5_20161215152814","2014-01-14T18:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-36693.694230000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[869,"TRANSGRIDV5_20161215152814","2014-01-14T17:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27232.356810000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[870,"TRANSGRIDV5_20161215152814","2014-01-14T18:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27231.336429999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[871,"TRANSGRIDV5_20161215152814","2014-01-14T17:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27228.851770000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[872,"TRANSGRIDV5_20161215152814","2014-01-14T18:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27220.40897,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[873,"TRANSGRIDV5_20161215152814","2014-01-14T12:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27215.052189999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[874,"TRANSGRIDV5_20161215152814","2014-01-14T12:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27211.4303,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[875,"TRANSGRIDV5_20161215152814","2014-01-14T12:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27207.46271,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[876,"TRANSGRIDV5_20161215152814","2014-01-14T14:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1541.45426,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[877,"TRANSGRIDV5_20161215152814","2014-01-14T13:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1146.5591300000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[878,"TRANSGRIDV5_20161215152814","2014-01-14T13:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1144.5864300000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[879,"TRANSGRIDV5_20161215152814","2014-01-14T12:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1143.1144099999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[880,"TRANSGRIDV5_20161215152814","2014-01-14T13:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1139.65987,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[881,"TRANSGRIDV5_20161215152814","2014-01-14T13:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1139.33277,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[882,"TRANSGRIDV5_20161215152814","2014-01-14T13:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1139.2837,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[883,"TRANSGRIDV5_20161215152814","2014-01-14T12:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1077.82509,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[884,"TRANSGRIDV5_20161215152814","2014-01-14T12:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-956.06764999999996,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[885,"TRANSGRIDV5_20161215152814","2014-01-14T11:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-605.68682999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[886,"TRANSGRIDV5_20161215152814","2014-01-14T21:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-216.74644000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[887,"TRANSGRIDV5_20161215152814","2014-01-14T10:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-193.34602000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[888,"TRANSGRIDV5_20161215152814","2014-01-14T10:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-191.38046,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[889,"TRANSGRIDV5_20161215152814","2014-01-14T10:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-191.02341000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[890,"TRANSGRIDV5_20161215152814","2014-01-14T10:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-189.01883000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[891,"TRANSGRIDV5_20161215152814","2014-01-14T11:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-184.74825000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[892,"TRANSGRIDV5_20161215152814","2014-01-14T10:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-183.62183999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[893,"TRANSGRIDV5_20161215152814","2014-01-14T10:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-178.43268,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[894,"TRANSGRIDV5_20161215152814","2014-01-14T10:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-173.18799000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[895,"TRANSGRIDV5_20161215152814","2014-01-14T09:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-166.89971,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[896,"TRANSGRIDV5_20161215152814","2014-01-14T10:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-165.2039,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[897,"TRANSGRIDV5_20161215152814","2014-01-14T10:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-164.73213000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[898,"TRANSGRIDV5_20161215152814","2014-01-14T20:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-160.16202000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[899,"TRANSGRIDV5_20161215152814","2014-01-14T20:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-158.56605999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[900,"TRANSGRIDV5_20161215152814","2014-01-14T20:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-148.04649000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[901,"TRANSGRIDV5_20161215152814","2014-01-14T23:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-138.10659999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[902,"TRANSGRIDV5_20161215152814","2014-01-14T16:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-133.56994,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[903,"TRANSGRIDV5_20161215152814","2014-01-14T23:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-129.18625,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[904,"TRANSGRIDV5_20161215152814","2014-01-14T23:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-128.44908000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[905,"TRANSGRIDV5_20161215152814","2014-01-14T23:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-125.61261,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[906,"TRANSGRIDV5_20161215152814","2014-01-14T23:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-124.34647,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[907,"TRANSGRIDV5_20161215152814","2014-01-14T23:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-122.9859,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[908,"TRANSGRIDV5_20161215152814","2014-01-14T20:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-122.35017000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[909,"TRANSGRIDV5_20161215152814","2014-01-14T23:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-121.28292,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[910,"TRANSGRIDV5_20161215152814","2014-01-14T20:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-118.37327000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[911,"TRANSGRIDV5_20161215152814","2014-01-14T21:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-116.01125,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[912,"TRANSGRIDV5_20161215152814","2014-01-14T22:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-113.86962,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[913,"TRANSGRIDV5_20161215152814","2014-01-14T20:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-113.24525,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[914,"TRANSGRIDV5_20161215152814","2014-01-14T21:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-112.56732,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[915,"TRANSGRIDV5_20161215152814","2014-01-14T21:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-108.721,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[916,"TRANSGRIDV5_20161215152814","2014-01-14T09:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-82.236750000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[917,"TRANSGRIDV5_20161215152814","2014-01-14T21:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-40.98265,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[918,"TRANSGRIDV5_20161215152814","2014-01-14T23:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-36.951549999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[919,"TRANSGRIDV5_20161215152814","2014-01-14T19:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-31.719729999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[920,"TRANSGRIDV5_20161215152814","2014-01-14T23:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.253350000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[921,"TRANSGRIDV5_20161215152814","2014-01-14T23:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.92417,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[922,"TRANSGRIDV5_20161215152814","2014-01-14T21:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-21.632290000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[923,"TRANSGRIDV5_20161215152814","2014-01-14T21:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-19.02957,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[924,"TRANSGRIDV5_20161215152814","2014-01-14T22:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-17.523900000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[925,"TRANSGRIDV5_20161215152814","2014-01-14T21:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.862869999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[926,"TRANSGRIDV5_20161215152814","2014-01-14T22:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.25559,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[927,"TRANSGRIDV5_20161215152814","2014-01-14T09:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.18379,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[928,"TRANSGRIDV5_20161215152814","2014-01-14T20:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.090159999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[929,"TRANSGRIDV5_20161215152814","2014-01-14T21:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.94279,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[930,"TRANSGRIDV5_20161215152814","2014-01-14T20:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.81062,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[931,"TRANSGRIDV5_20161215152814","2014-01-14T22:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.62391,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[932,"TRANSGRIDV5_20161215152814","2014-01-14T23:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.255929999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[933,"TRANSGRIDV5_20161215152814","2014-01-14T22:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.01962,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[934,"TRANSGRIDV5_20161215152814","2014-01-14T21:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-11.712479999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[935,"TRANSGRIDV5_20161215152814","2014-01-14T20:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.904809999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[936,"TRANSGRIDV5_20161215152814","2014-01-14T20:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.52238,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[937,"TRANSGRIDV5_20161215152814","2014-01-14T18:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-19418.52679,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[938,"TRANSGRIDV5_20161215152814","2014-01-14T12:05:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-19389.895830000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[939,"TRANSGRIDV5_20161215152814","2014-01-14T17:05:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-6089.6340700000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[940,"TRANSGRIDV5_20161215152814","2014-01-14T19:55:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-13.3002,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[941,"TRANSGRIDV5_20161215152814","2014-01-14T19:50:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-12.632630000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[942,"TRANSGRIDV5_20161215152814","2014-01-14T20:00:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-11.429970000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[943,"TRANSGRIDV5_20161215152814","2014-01-14T14:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.37994,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[944,"TRANSGRIDV5_20161215152814","2014-01-14T22:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.33234,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[945,"TRANSGRIDV5_20161215152814","2014-01-14T15:30:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-3811.5478400000002,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[946,"TRANSGRIDV5_20161215152814","2014-01-14T15:40:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-3803.5695500000002,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[947,"TRANSGRIDV5_20161215152814","2014-01-14T15:45:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-3800.66329,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[948,"TRANSGRIDV5_20161215152814","2014-01-14T15:05:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-3799.1914499999998,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[949,"TRANSGRIDV5_20161215152814","2014-01-14T15:15:00","NRM_NSW1_VIC1","NRM_NIL_ALL","2012-06-12",1,-719.48343,"Negative Residue Management constraint for NSW to VIC flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[950,"TRANSGRIDV5_20161215152814","2014-01-14T14:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-412502.68550999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[951,"TRANSGRIDV5_20161215152814","2014-01-14T12:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-385134.06816000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[952,"TRANSGRIDV5_20161215152814","2014-01-14T12:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-385071.98423,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[953,"TRANSGRIDV5_20161215152814","2014-01-14T17:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-346438.58046000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[954,"TRANSGRIDV5_20161215152814","2014-01-14T12:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-319276.58403000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[955,"TRANSGRIDV5_20161215152814","2014-01-14T17:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-318682.76416000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[956,"TRANSGRIDV5_20161215152814","2014-01-14T15:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-305478.30352999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[957,"TRANSGRIDV5_20161215152814","2014-01-14T16:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-301041.26130000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[958,"TRANSGRIDV5_20161215152814","2014-01-14T16:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-300926.87656,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[959,"TRANSGRIDV5_20161215152814","2014-01-14T15:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-298675.21755,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[960,"TRANSGRIDV5_20161215152814","2014-01-14T15:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-298603.34445999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[961,"TRANSGRIDV5_20161215152814","2014-01-14T15:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-298419.71687,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[962,"TRANSGRIDV5_20161215152814","2014-01-14T15:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-297822.69750000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[963,"TRANSGRIDV5_20161215152814","2014-01-14T16:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-279347.37244000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[964,"TRANSGRIDV5_20161215152814","2014-01-14T16:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-278666.16769999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[965,"TRANSGRIDV5_20161215152814","2014-01-14T16:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-278548.79599999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[966,"TRANSGRIDV5_20161215152814","2014-01-14T16:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-278303.05421999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[967,"TRANSGRIDV5_20161215152814","2014-01-14T16:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-277205.78717999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[968,"TRANSGRIDV5_20161215152814","2014-01-14T15:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-254274.57769999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[969,"TRANSGRIDV5_20161215152814","2014-01-14T15:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-253952.33074999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[970,"TRANSGRIDV5_20161215152814","2014-01-14T14:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-247263.37323,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[971,"TRANSGRIDV5_20161215152814","2014-01-14T14:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-247259.84028,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[972,"TRANSGRIDV5_20161215152814","2014-01-14T14:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-247227.12195,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[973,"TRANSGRIDV5_20161215152814","2014-01-14T14:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-247188.08395999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[974,"TRANSGRIDV5_20161215152814","2014-01-14T12:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-243588.91198,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[975,"TRANSGRIDV5_20161215152814","2014-01-14T14:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-237001.69461999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[976,"TRANSGRIDV5_20161215152814","2014-01-14T13:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-148339.88333000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[977,"TRANSGRIDV5_20161215152814","2014-01-14T18:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-147653.66359000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[978,"TRANSGRIDV5_20161215152814","2014-01-14T17:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-147546.25562000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[979,"TRANSGRIDV5_20161215152814","2014-01-14T18:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-147528.15653000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[980,"TRANSGRIDV5_20161215152814","2014-01-14T18:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-132587.59302999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[981,"TRANSGRIDV5_20161215152814","2014-01-14T13:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-116185.72181,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[982,"TRANSGRIDV5_20161215152814","2014-01-14T13:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-116176.05727,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[983,"TRANSGRIDV5_20161215152814","2014-01-14T18:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-109195.19769,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[984,"TRANSGRIDV5_20161215152814","2014-01-14T14:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-94811.831090000007,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[985,"TRANSGRIDV5_20161215152814","2014-01-14T13:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-82438.850590000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[986,"TRANSGRIDV5_20161215152814","2014-01-14T13:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-82438.816949999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[987,"TRANSGRIDV5_20161215152814","2014-01-14T13:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-82253.026410000006,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[988,"TRANSGRIDV5_20161215152814","2014-01-14T13:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-82174.144709999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[989,"TRANSGRIDV5_20161215152814","2014-01-14T12:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-82145.911439999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[990,"TRANSGRIDV5_20161215152814","2014-01-14T12:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-81811.806719999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[991,"TRANSGRIDV5_20161215152814","2014-01-14T16:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-80748.457949999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[992,"TRANSGRIDV5_20161215152814","2014-01-14T15:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-80419.091990000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[993,"TRANSGRIDV5_20161215152814","2014-01-14T14:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-78599.584239999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[994,"TRANSGRIDV5_20161215152814","2014-01-14T14:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-77569.977429999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[995,"TRANSGRIDV5_20161215152814","2014-01-14T14:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-77327.503219999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[996,"TRANSGRIDV5_20161215152814","2014-01-14T14:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-76902.449380000005,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[997,"TRANSGRIDV5_20161215152814","2014-01-14T15:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-74356.007310000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[998,"TRANSGRIDV5_20161215152814","2014-01-14T13:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-71886.489140000005,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[999,"TRANSGRIDV5_20161215152814","2014-01-14T14:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-70340.989369999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1000,"TRANSGRIDV5_20161215152814","2014-01-14T13:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69192.571760000006,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1001,"TRANSGRIDV5_20161215152814","2014-01-14T12:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69131.990269999995,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1002,"TRANSGRIDV5_20161215152814","2014-01-14T13:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69119.566680000004,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1003,"TRANSGRIDV5_20161215152814","2014-01-14T12:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69084.889989999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1004,"TRANSGRIDV5_20161215152814","2014-01-14T12:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-68930.225229999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1005,"TRANSGRIDV5_20161215152814","2014-01-14T12:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-68906.608789999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1006,"TRANSGRIDV5_20161215152814","2014-01-14T13:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-68876.046040000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1007,"TRANSGRIDV5_20161215152814","2014-01-14T16:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-66993.687909999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1008,"TRANSGRIDV5_20161215152814","2014-01-14T17:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-65008.079409999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1009,"TRANSGRIDV5_20161215152814","2014-01-14T17:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-64510.63003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1010,"TRANSGRIDV5_20161215152814","2014-01-14T17:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-64173.785329999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1011,"TRANSGRIDV5_20161215152814","2014-01-14T17:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-64137.418089999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1012,"TRANSGRIDV5_20161215152814","2014-01-14T17:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-63958.089039999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1013,"TRANSGRIDV5_20161215152814","2014-01-14T17:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-63954.131280000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1014,"TRANSGRIDV5_20161215152814","2014-01-14T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-50979.23719,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1015,"TRANSGRIDV5_20161215152814","2014-01-14T12:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-48424.722130000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1016,"TRANSGRIDV5_20161215152814","2014-01-14T15:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-47380.467320000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1017,"TRANSGRIDV5_20161215152814","2014-01-14T17:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-46960.971140000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1018,"TRANSGRIDV5_20161215152814","2014-01-14T17:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-46756.377229999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1019,"TRANSGRIDV5_20161215152814","2014-01-14T16:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-46238.196210000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1020,"TRANSGRIDV5_20161215152814","2014-01-14T16:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-41556.6325,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1021,"TRANSGRIDV5_20161215152814","2014-01-14T16:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-38164.930569999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1022,"TRANSGRIDV5_20161215152814","2014-01-14T18:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37389.726920000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1023,"TRANSGRIDV5_20161215152814","2014-01-14T15:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36958.686679999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1024,"TRANSGRIDV5_20161215152814","2014-01-14T15:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36865.494429999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1025,"TRANSGRIDV5_20161215152814","2014-01-14T18:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36747.088000000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1026,"TRANSGRIDV5_20161215152814","2014-01-14T18:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36673.286070000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1027,"TRANSGRIDV5_20161215152814","2014-01-14T18:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36639.566980000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1028,"TRANSGRIDV5_20161215152814","2014-01-14T17:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36613.469149999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1029,"TRANSGRIDV5_20161215152814","2014-01-14T18:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36567.51195,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1030,"TRANSGRIDV5_20161215152814","2014-01-14T12:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-11188.10565,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1031,"TRANSGRIDV5_20161215152814","2014-01-14T11:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-7328.03946,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1032,"TRANSGRIDV5_20161215152814","2014-01-14T18:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-5506.2761799999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1033,"TRANSGRIDV5_20161215152814","2014-01-14T18:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-299.88675999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1034,"TRANSGRIDV5_20161215152814","2014-01-14T11:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-112.52278,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1035,"TRANSGRIDV5_20161215152814","2014-01-14T19:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-90.172020000000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1036,"TRANSGRIDV5_20161215152814","2014-01-14T11:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-64.181839999999994,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1037,"TRANSGRIDV5_20161215152814","2014-01-14T19:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-48.888869999999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1038,"TRANSGRIDV5_20161215152814","2014-01-14T11:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-30.396809999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1039,"TRANSGRIDV5_20161215152814","2014-01-14T09:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-181.94818000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1040,"TRANSGRIDV5_20161215152814","2014-01-14T09:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-181.93010000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1041,"TRANSGRIDV5_20161215152814","2014-01-14T09:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-180.21091999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1042,"TRANSGRIDV5_20161215152814","2014-01-14T08:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-100.22716,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1043,"TRANSGRIDV5_20161215152814","2014-01-14T08:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-98.168059999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1044,"TRANSGRIDV5_20161215152814","2014-01-14T09:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-97.121219999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1045,"TRANSGRIDV5_20161215152814","2014-01-14T08:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.912909999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1046,"TRANSGRIDV5_20161215152814","2014-01-14T08:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.750960000000006,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1047,"TRANSGRIDV5_20161215152814","2014-01-14T08:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.422269999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1048,"TRANSGRIDV5_20161215152814","2014-01-14T08:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.075749999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1049,"TRANSGRIDV5_20161215152814","2014-01-14T08:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-95.381150000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1050,"TRANSGRIDV5_20161215152814","2014-01-14T08:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-95.210049999999995,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1051,"TRANSGRIDV5_20161215152814","2014-01-14T08:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-94.980180000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1052,"TRANSGRIDV5_20161215152814","2014-01-14T08:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-94.171099999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1053,"TRANSGRIDV5_20161215152814","2014-01-14T08:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-92.66319,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1054,"TRANSGRIDV5_20161215152814","2014-01-14T09:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-84.175110000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1055,"TRANSGRIDV5_20161215152814","2014-01-14T15:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-205118.96189000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1056,"TRANSGRIDV5_20161215152814","2014-01-14T16:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-201938.37111000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1057,"TRANSGRIDV5_20161215152814","2014-01-14T16:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-201937.30545000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1058,"TRANSGRIDV5_20161215152814","2014-01-14T16:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-186730.5392,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1059,"TRANSGRIDV5_20161215152814","2014-01-14T16:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-186285.00899999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1060,"TRANSGRIDV5_20161215152814","2014-01-14T16:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-186260.36408999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1061,"TRANSGRIDV5_20161215152814","2014-01-14T16:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-186160.83650999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1062,"TRANSGRIDV5_20161215152814","2014-01-14T16:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-185483.50086,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1063,"TRANSGRIDV5_20161215152814","2014-01-14T15:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169557.18218999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1064,"TRANSGRIDV5_20161215152814","2014-01-14T15:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169516.47399,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1065,"TRANSGRIDV5_20161215152814","2014-01-14T15:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169466.19375000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1066,"TRANSGRIDV5_20161215152814","2014-01-14T15:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169412.57191999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1067,"TRANSGRIDV5_20161215152814","2014-01-14T15:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169207.76196999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1068,"TRANSGRIDV5_20161215152814","2014-01-14T15:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-169073.81567000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1069,"TRANSGRIDV5_20161215152814","2014-01-14T14:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-164552.74411999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1070,"TRANSGRIDV5_20161215152814","2014-01-14T14:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-164552.50380000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1071,"TRANSGRIDV5_20161215152814","2014-01-14T14:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-164552.1833,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1072,"TRANSGRIDV5_20161215152814","2014-01-14T17:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-164381.71853000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1073,"TRANSGRIDV5_20161215152814","2014-01-14T13:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-159946.68633,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1074,"TRANSGRIDV5_20161215152814","2014-01-14T14:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-157548.30660000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1075,"TRANSGRIDV5_20161215152814","2014-01-14T17:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-147818.92301,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1076,"TRANSGRIDV5_20161215152814","2014-01-14T18:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-147802.399,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1077,"TRANSGRIDV5_20161215152814","2014-01-14T18:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-147703.27051999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1078,"TRANSGRIDV5_20161215152814","2014-01-14T18:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-134515.12770000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1079,"TRANSGRIDV5_20161215152814","2014-01-14T13:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-124438.20073,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1080,"TRANSGRIDV5_20161215152814","2014-01-14T13:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-124426.70813,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1081,"TRANSGRIDV5_20161215152814","2014-01-14T18:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-105414.43992,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1082,"TRANSGRIDV5_20161215152814","2014-01-14T17:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-71499.600149999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1083,"TRANSGRIDV5_20161215152814","2014-01-14T17:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-71021.258489999993,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1084,"TRANSGRIDV5_20161215152814","2014-01-14T17:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-70721.17916,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1085,"TRANSGRIDV5_20161215152814","2014-01-14T17:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-70648.987580000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1086,"TRANSGRIDV5_20161215152814","2014-01-14T17:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-70533.374060000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1087,"TRANSGRIDV5_20161215152814","2014-01-14T15:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-51017.47118,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1088,"TRANSGRIDV5_20161215152814","2014-01-14T16:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-45609.54047,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1089,"TRANSGRIDV5_20161215152814","2014-01-14T16:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-44466.178489999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1090,"TRANSGRIDV5_20161215152814","2014-01-14T16:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-40791.08943,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1091,"TRANSGRIDV5_20161215152814","2014-01-14T15:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39513.628660000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1092,"TRANSGRIDV5_20161215152814","2014-01-14T18:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39456.553599999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1093,"TRANSGRIDV5_20161215152814","2014-01-14T15:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39432.803950000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1094,"TRANSGRIDV5_20161215152814","2014-01-14T17:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39404.633000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1095,"TRANSGRIDV5_20161215152814","2014-01-14T18:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39391.086029999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1096,"TRANSGRIDV5_20161215152814","2014-01-14T18:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39304.720020000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1097,"TRANSGRIDV5_20161215152814","2014-01-14T18:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39274.894269999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1098,"TRANSGRIDV5_20161215152814","2014-01-14T18:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39188.629869999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1099,"TRANSGRIDV5_20161215152814","2014-01-14T16:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-36082.554830000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1100,"TRANSGRIDV5_20161215152814","2014-01-14T17:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-34742.365689999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1101,"TRANSGRIDV5_20161215152814","2014-01-14T14:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-11510.85541,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1102,"TRANSGRIDV5_20161215152814","2014-01-14T16:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-11425.72661,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1103,"TRANSGRIDV5_20161215152814","2014-01-14T15:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-10469.58711,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1104,"TRANSGRIDV5_20161215152814","2014-01-14T14:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-10176.561890000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1105,"TRANSGRIDV5_20161215152814","2014-01-14T18:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-5451.6214600000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1106,"TRANSGRIDV5_20161215152814","2014-01-14T18:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-4552.1429099999996,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1107,"TRANSGRIDV5_20161215152814","2014-01-14T17:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-4471.6063100000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1108,"TRANSGRIDV5_20161215152814","2014-01-14T15:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-4206.7792799999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1109,"TRANSGRIDV5_20161215152814","2014-01-14T17:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-3244.4178400000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1110,"TRANSGRIDV5_20161215152814","2014-01-14T18:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-299.88675999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1111,"TRANSGRIDV5_20161215152814","2014-01-14T19:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-208.18924999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1112,"TRANSGRIDV5_20161215152814","2014-01-14T19:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-54.792470000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1113,"TRANSGRIDV5_20161215152814","2014-01-14T14:00:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-294976.19284999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1114,"TRANSGRIDV5_20161215152814","2014-01-14T14:55:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-164552.86558000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1115,"TRANSGRIDV5_20161215152814","2014-01-14T12:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-387531.94097,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1116,"TRANSGRIDV5_20161215152814","2014-01-14T12:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-387468.18436000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1117,"TRANSGRIDV5_20161215152814","2014-01-14T17:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-347632.52781,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1118,"TRANSGRIDV5_20161215152814","2014-01-14T12:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-319638.68511000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1119,"TRANSGRIDV5_20161215152814","2014-01-14T12:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-240436.33,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1120,"TRANSGRIDV5_20161215152814","2014-01-14T17:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-172305.5435,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1121,"TRANSGRIDV5_20161215152814","2014-01-14T14:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-150082.70850000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1122,"TRANSGRIDV5_20161215152814","2014-01-14T15:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-148654.36316000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1123,"TRANSGRIDV5_20161215152814","2014-01-14T15:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-148618.74531999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1124,"TRANSGRIDV5_20161215152814","2014-01-14T15:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-148527.65207000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1125,"TRANSGRIDV5_20161215152814","2014-01-14T15:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-148230.70462,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1126,"TRANSGRIDV5_20161215152814","2014-01-14T15:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-124023.36517999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1127,"TRANSGRIDV5_20161215152814","2014-01-14T16:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-122407.04631999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1128,"TRANSGRIDV5_20161215152814","2014-01-14T16:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-122291.71217,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1129,"TRANSGRIDV5_20161215152814","2014-01-14T16:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-114153.97249,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1130,"TRANSGRIDV5_20161215152814","2014-01-14T16:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-113869.55364,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1131,"TRANSGRIDV5_20161215152814","2014-01-14T16:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-113862.7687,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1132,"TRANSGRIDV5_20161215152814","2014-01-14T16:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-113528.38845,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1133,"TRANSGRIDV5_20161215152814","2014-01-14T16:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-113122.98957999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1134,"TRANSGRIDV5_20161215152814","2014-01-14T15:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-104334.75771999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1135,"TRANSGRIDV5_20161215152814","2014-01-14T15:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-104242.66968000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1136,"TRANSGRIDV5_20161215152814","2014-01-14T14:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101699.9332,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1137,"TRANSGRIDV5_20161215152814","2014-01-14T14:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101695.89893,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1138,"TRANSGRIDV5_20161215152814","2014-01-14T14:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101661.95852,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1139,"TRANSGRIDV5_20161215152814","2014-01-14T14:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101624.35739,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1140,"TRANSGRIDV5_20161215152814","2014-01-14T14:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-97704.647830000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1141,"TRANSGRIDV5_20161215152814","2014-01-14T14:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-97259.283989999996,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1142,"TRANSGRIDV5_20161215152814","2014-01-14T13:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84650.898929999996,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1143,"TRANSGRIDV5_20161215152814","2014-01-14T13:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84639.120150000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1144,"TRANSGRIDV5_20161215152814","2014-01-14T13:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84607.330440000005,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1145,"TRANSGRIDV5_20161215152814","2014-01-14T13:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84607.30287,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1146,"TRANSGRIDV5_20161215152814","2014-01-14T13:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84573.262229999993,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1147,"TRANSGRIDV5_20161215152814","2014-01-14T12:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84542.468489999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1148,"TRANSGRIDV5_20161215152814","2014-01-14T12:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-84208.995769999994,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1149,"TRANSGRIDV5_20161215152814","2014-01-14T14:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-80018.682990000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1150,"TRANSGRIDV5_20161215152814","2014-01-14T14:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-79779.895999999993,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1151,"TRANSGRIDV5_20161215152814","2014-01-14T14:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-79349.983420000004,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1152,"TRANSGRIDV5_20161215152814","2014-01-14T15:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-72561.174939999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1153,"TRANSGRIDV5_20161215152814","2014-01-14T12:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71529.863549999995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1154,"TRANSGRIDV5_20161215152814","2014-01-14T12:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71480.683879999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1155,"TRANSGRIDV5_20161215152814","2014-01-14T13:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71361.051739999995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1156,"TRANSGRIDV5_20161215152814","2014-01-14T12:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71326.019159999996,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1157,"TRANSGRIDV5_20161215152814","2014-01-14T12:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71304.481650000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1158,"TRANSGRIDV5_20161215152814","2014-01-14T13:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71286.730880000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1159,"TRANSGRIDV5_20161215152814","2014-01-14T13:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71256.184389999995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1160,"TRANSGRIDV5_20161215152814","2014-01-14T14:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-69979.985350000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1161,"TRANSGRIDV5_20161215152814","2014-01-14T14:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-62852.485569999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1162,"TRANSGRIDV5_20161215152814","2014-01-14T13:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-53134.648950000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1163,"TRANSGRIDV5_20161215152814","2014-01-14T12:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-50050.303999999996,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1164,"TRANSGRIDV5_20161215152814","2014-01-14T17:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-45426.521670000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1165,"TRANSGRIDV5_20161215152814","2014-01-14T15:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-44800.08296,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1166,"TRANSGRIDV5_20161215152814","2014-01-14T17:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-44174.28037,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1167,"TRANSGRIDV5_20161215152814","2014-01-14T16:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-41062.393190000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1168,"TRANSGRIDV5_20161215152814","2014-01-14T16:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-36713.737139999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1169,"TRANSGRIDV5_20161215152814","2014-01-14T16:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-35703.59592,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1170,"TRANSGRIDV5_20161215152814","2014-01-14T17:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-34005.878060000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1171,"TRANSGRIDV5_20161215152814","2014-01-14T15:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-29258.52764,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1172,"TRANSGRIDV5_20161215152814","2014-01-14T12:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-11459.277050000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1173,"TRANSGRIDV5_20161215152814","2014-01-14T11:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-7624.0855199999996,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1174,"TRANSGRIDV5_20161215152814","2014-01-14T11:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-382.60739000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1175,"TRANSGRIDV5_20161215152814","2014-01-14T11:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-334.25353000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1176,"TRANSGRIDV5_20161215152814","2014-01-14T11:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-296.07233000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1177,"TRANSGRIDV5_20161215152814","2014-01-14T11:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-263.22930000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1178,"TRANSGRIDV5_20161215152814","2014-01-14T11:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-263.18524000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1179,"TRANSGRIDV5_20161215152814","2014-01-14T11:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-262.67052999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1180,"TRANSGRIDV5_20161215152814","2014-01-14T11:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-259.70505000000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1181,"TRANSGRIDV5_20161215152814","2014-01-14T11:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-250.20447999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1182,"TRANSGRIDV5_20161215152814","2014-01-14T11:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-250.20447999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1183,"TRANSGRIDV5_20161215152814","2014-01-14T11:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-247.87656999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1184,"TRANSGRIDV5_20161215152814","2014-01-14T10:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-238.56493,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1185,"TRANSGRIDV5_20161215152814","2014-01-14T09:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-211.33600000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1186,"TRANSGRIDV5_20161215152814","2014-01-14T10:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-52.076779999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1187,"TRANSGRIDV5_20161215152814","2014-01-14T11:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-49.451749999999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1188,"TRANSGRIDV5_20161215152814","2014-01-14T10:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-47.333159999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1189,"TRANSGRIDV5_20161215152814","2014-01-14T10:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-35.902769999999997,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1190,"TRANSGRIDV5_20161215152814","2014-01-14T09:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-26.78811,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1191,"TRANSGRIDV5_20161215152814","2014-01-14T09:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-24.780100000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1192,"TRANSGRIDV5_20161215152814","2014-01-14T10:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-23.946729999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1193,"TRANSGRIDV5_20161215152814","2014-01-14T09:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-23.785419999999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1194,"TRANSGRIDV5_20161215152814","2014-01-14T13:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-24584.63825,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1195,"TRANSGRIDV5_20161215152814","2014-01-14T13:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-24582.787530000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1196,"TRANSGRIDV5_20161215152814","2014-01-14T13:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-21116.00347,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1197,"TRANSGRIDV5_20161215152814","2014-01-14T18:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-10952.745800000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1198,"TRANSGRIDV5_20161215152814","2014-01-14T16:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8828.2673699999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1199,"TRANSGRIDV5_20161215152814","2014-01-14T14:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8800.7179500000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1200,"TRANSGRIDV5_20161215152814","2014-01-14T16:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8042.3307100000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1201,"TRANSGRIDV5_20161215152814","2014-01-14T18:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8033.5834199999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1202,"TRANSGRIDV5_20161215152814","2014-01-14T18:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8032.2797300000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1203,"TRANSGRIDV5_20161215152814","2014-01-14T18:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8019.1617999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1204,"TRANSGRIDV5_20161215152814","2014-01-14T18:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8017.5957600000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1205,"TRANSGRIDV5_20161215152814","2014-01-14T15:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8007.5054899999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1206,"TRANSGRIDV5_20161215152814","2014-01-14T15:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7821.9628899999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1207,"TRANSGRIDV5_20161215152814","2014-01-14T14:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7784.0610399999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1208,"TRANSGRIDV5_20161215152814","2014-01-14T15:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7778.8296099999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1209,"TRANSGRIDV5_20161215152814","2014-01-14T17:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7775.5164999999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1210,"TRANSGRIDV5_20161215152814","2014-01-14T14:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7447.81927,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1211,"TRANSGRIDV5_20161215152814","2014-01-14T14:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7427.4026899999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1212,"TRANSGRIDV5_20161215152814","2014-01-14T14:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7420.9173700000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1213,"TRANSGRIDV5_20161215152814","2014-01-14T14:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7420.4685200000004,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1214,"TRANSGRIDV5_20161215152814","2014-01-14T18:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6739.1662999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1215,"TRANSGRIDV5_20161215152814","2014-01-14T13:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1302900000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1216,"TRANSGRIDV5_20161215152814","2014-01-14T12:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1301000000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1217,"TRANSGRIDV5_20161215152814","2014-01-14T13:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1287599999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1218,"TRANSGRIDV5_20161215152814","2014-01-14T12:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1275299999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1219,"TRANSGRIDV5_20161215152814","2014-01-14T12:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1275299999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1220,"TRANSGRIDV5_20161215152814","2014-01-14T12:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1274000000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1221,"TRANSGRIDV5_20161215152814","2014-01-14T12:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1274000000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1222,"TRANSGRIDV5_20161215152814","2014-01-14T13:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.12565,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1223,"TRANSGRIDV5_20161215152814","2014-01-14T13:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.11006,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1224,"TRANSGRIDV5_20161215152814","2014-01-14T13:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6557.1100299999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1225,"TRANSGRIDV5_20161215152814","2014-01-14T12:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6555.02027,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1226,"TRANSGRIDV5_20161215152814","2014-01-14T13:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6554.55663,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1227,"TRANSGRIDV5_20161215152814","2014-01-14T12:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6549.7256200000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1228,"TRANSGRIDV5_20161215152814","2014-01-14T13:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6549.7085100000004,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1229,"TRANSGRIDV5_20161215152814","2014-01-14T13:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6547.7188999999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1230,"TRANSGRIDV5_20161215152814","2014-01-14T12:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6547.7178999999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1231,"TRANSGRIDV5_20161215152814","2014-01-14T13:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-5942.3233099999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1232,"TRANSGRIDV5_20161215152814","2014-01-14T16:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-5735.6394600000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1233,"TRANSGRIDV5_20161215152814","2014-01-14T17:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-5047.0119299999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1234,"TRANSGRIDV5_20161215152814","2014-01-14T15:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-4967.0818099999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1235,"TRANSGRIDV5_20161215152814","2014-01-14T17:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-4894.3886199999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1236,"TRANSGRIDV5_20161215152814","2014-01-14T12:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-4400.1465200000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1237,"TRANSGRIDV5_20161215152814","2014-01-14T17:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-2866.6042200000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1238,"TRANSGRIDV5_20161215152814","2014-01-14T12:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-1243.10627,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1239,"TRANSGRIDV5_20161215152814","2014-01-14T19:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-289.22273000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1240,"TRANSGRIDV5_20161215152814","2014-01-14T12:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-283.56272999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1241,"TRANSGRIDV5_20161215152814","2014-01-14T19:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-13.39343,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1242,"TRANSGRIDV5_20161215152814","2014-01-14T14:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-67962.842149999997,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1243,"TRANSGRIDV5_20161215152814","2014-01-14T15:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-49272.199979999998,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1244,"TRANSGRIDV5_20161215152814","2014-01-14T16:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-48508.17181,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1245,"TRANSGRIDV5_20161215152814","2014-01-14T16:25:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-48507.914100000002,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1246,"TRANSGRIDV5_20161215152814","2014-01-14T16:35:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-44855.053319999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1247,"TRANSGRIDV5_20161215152814","2014-01-14T16:20:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-44748.032859999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1248,"TRANSGRIDV5_20161215152814","2014-01-14T16:50:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-44742.111210000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1249,"TRANSGRIDV5_20161215152814","2014-01-14T16:40:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-44718.203410000002,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1250,"TRANSGRIDV5_20161215152814","2014-01-14T16:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-44555.498670000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1251,"TRANSGRIDV5_20161215152814","2014-01-14T15:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40729.795400000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1252,"TRANSGRIDV5_20161215152814","2014-01-14T15:40:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40720.024360000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1253,"TRANSGRIDV5_20161215152814","2014-01-14T15:35:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40707.946400000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1254,"TRANSGRIDV5_20161215152814","2014-01-14T15:45:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40695.065739999998,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1255,"TRANSGRIDV5_20161215152814","2014-01-14T15:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40645.872969999997,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1256,"TRANSGRIDV5_20161215152814","2014-01-14T15:05:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-40613.697310000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1257,"TRANSGRIDV5_20161215152814","2014-01-14T14:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-39527.694190000002,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1258,"TRANSGRIDV5_20161215152814","2014-01-14T14:45:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-39527.667329999997,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1259,"TRANSGRIDV5_20161215152814","2014-01-14T14:50:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-39527.613819999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1260,"TRANSGRIDV5_20161215152814","2014-01-14T14:40:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-39527.542939999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1261,"TRANSGRIDV5_20161215152814","2014-01-14T17:05:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-39488.001830000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1262,"TRANSGRIDV5_20161215152814","2014-01-14T14:35:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-37846.06093,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1263,"TRANSGRIDV5_20161215152814","2014-01-14T17:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13440.96385,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1264,"TRANSGRIDV5_20161215152814","2014-01-14T17:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13225.717930000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1265,"TRANSGRIDV5_20161215152814","2014-01-14T17:20:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13174.263650000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1266,"TRANSGRIDV5_20161215152814","2014-01-14T17:25:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13161.885050000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1267,"TRANSGRIDV5_20161215152814","2014-01-14T17:15:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13098.190629999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1268,"TRANSGRIDV5_20161215152814","2014-01-14T16:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-12265.365100000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1269,"TRANSGRIDV5_20161215152814","2014-01-14T15:50:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-12256.32069,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1270,"TRANSGRIDV5_20161215152814","2014-01-14T16:45:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-9912.7180800000006,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1271,"TRANSGRIDV5_20161215152814","2014-01-14T13:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-9898.7512000000006,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1272,"TRANSGRIDV5_20161215152814","2014-01-14T17:35:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-9430.8088499999994,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1273,"TRANSGRIDV5_20161215152814","2014-01-14T12:40:00","V>>V_NIL_4A","V-NIL","2013-12-03",1,-566.56739000000005,"Out = Nil, avoid pre-contingent O/L of the Dederang H1 330/220kV transformer, DBUSS-Transformer control scheme armed, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1274,"TRANSGRIDV5_20161215152814","2014-01-14T12:05:00","V>>V_NIL_4A","V-NIL","2013-12-03",1,-352.584,"Out = Nil, avoid pre-contingent O/L of the Dederang H1 330/220kV transformer, DBUSS-Transformer control scheme armed, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1275,"TRANSGRIDV5_20161215152814","2014-01-15T07:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-206.56451999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1276,"TRANSGRIDV5_20161215152814","2014-01-15T08:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-192.05663000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1277,"TRANSGRIDV5_20161215152814","2014-01-15T20:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-183.61107999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1278,"TRANSGRIDV5_20161215152814","2014-01-15T08:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-182.44324,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1279,"TRANSGRIDV5_20161215152814","2014-01-15T20:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-182.37718000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1280,"TRANSGRIDV5_20161215152814","2014-01-15T08:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-181.17522,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1281,"TRANSGRIDV5_20161215152814","2014-01-15T08:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-181.00023999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1282,"TRANSGRIDV5_20161215152814","2014-01-15T20:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-180.13489000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1283,"TRANSGRIDV5_20161215152814","2014-01-15T08:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-178.54334,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1284,"TRANSGRIDV5_20161215152814","2014-01-15T07:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-177.43894,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1285,"TRANSGRIDV5_20161215152814","2014-01-15T07:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-173.26365000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1286,"TRANSGRIDV5_20161215152814","2014-01-15T08:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-173.00709000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1287,"TRANSGRIDV5_20161215152814","2014-01-15T08:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-170.09378000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1288,"TRANSGRIDV5_20161215152814","2014-01-15T20:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-167.65179000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1289,"TRANSGRIDV5_20161215152814","2014-01-15T08:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-166.28639000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1290,"TRANSGRIDV5_20161215152814","2014-01-15T20:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-164.6336,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1291,"TRANSGRIDV5_20161215152814","2014-01-15T08:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-135.50050999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1292,"TRANSGRIDV5_20161215152814","2014-01-15T06:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-110.33665000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1293,"TRANSGRIDV5_20161215152814","2014-01-15T06:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-108.82579,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1294,"TRANSGRIDV5_20161215152814","2014-01-15T06:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-105.1653,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1295,"TRANSGRIDV5_20161215152814","2014-01-15T05:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-81.252610000000004,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1296,"TRANSGRIDV5_20161215152814","2014-01-15T05:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-68.768180000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1297,"TRANSGRIDV5_20161215152814","2014-01-15T05:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-68.768180000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1298,"TRANSGRIDV5_20161215152814","2014-01-15T23:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-35.425759999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1299,"TRANSGRIDV5_20161215152814","2014-01-15T06:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-30.362120000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1300,"TRANSGRIDV5_20161215152814","2014-01-15T07:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-30.352499999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1301,"TRANSGRIDV5_20161215152814","2014-01-15T07:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.856719999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1302,"TRANSGRIDV5_20161215152814","2014-01-15T06:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.8306,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1303,"TRANSGRIDV5_20161215152814","2014-01-15T23:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.008800000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1304,"TRANSGRIDV5_20161215152814","2014-01-15T23:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.931609999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1305,"TRANSGRIDV5_20161215152814","2014-01-15T23:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.884540000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1306,"TRANSGRIDV5_20161215152814","2014-01-15T06:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.29881,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1307,"TRANSGRIDV5_20161215152814","2014-01-15T23:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.276340000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1308,"TRANSGRIDV5_20161215152814","2014-01-15T06:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-28.184989999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1309,"TRANSGRIDV5_20161215152814","2014-01-15T06:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-27.3431,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1310,"TRANSGRIDV5_20161215152814","2014-01-15T23:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-26.72531,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1311,"TRANSGRIDV5_20161215152814","2014-01-15T23:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-26.440860000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1312,"TRANSGRIDV5_20161215152814","2014-01-15T07:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-26.221920000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1313,"TRANSGRIDV5_20161215152814","2014-01-15T05:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-25.524260000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1314,"TRANSGRIDV5_20161215152814","2014-01-15T06:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.360980000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1315,"TRANSGRIDV5_20161215152814","2014-01-15T07:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-21.638670000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1316,"TRANSGRIDV5_20161215152814","2014-01-15T00:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-19.43431,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1317,"TRANSGRIDV5_20161215152814","2014-01-15T00:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-18.849419999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1318,"TRANSGRIDV5_20161215152814","2014-01-15T00:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.0602,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1319,"TRANSGRIDV5_20161215152814","2014-01-15T07:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.297459999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1320,"TRANSGRIDV5_20161215152814","2014-01-15T16:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-258.02350000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1321,"TRANSGRIDV5_20161215152814","2014-01-15T16:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-52.392800000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1322,"TRANSGRIDV5_20161215152814","2014-01-15T18:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.058440000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1323,"TRANSGRIDV5_20161215152814","2014-01-15T16:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.290120000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1324,"TRANSGRIDV5_20161215152814","2014-01-15T16:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.14462,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1325,"TRANSGRIDV5_20161215152814","2014-01-15T16:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.694949999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1326,"TRANSGRIDV5_20161215152814","2014-01-15T16:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.86243,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1327,"TRANSGRIDV5_20161215152814","2014-01-15T16:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.72283,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1328,"TRANSGRIDV5_20161215152814","2014-01-15T16:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.89587,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1329,"TRANSGRIDV5_20161215152814","2014-01-15T17:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.20614,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1330,"TRANSGRIDV5_20161215152814","2014-01-15T16:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.33929,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1331,"TRANSGRIDV5_20161215152814","2014-01-15T17:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.38672,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1332,"TRANSGRIDV5_20161215152814","2014-01-15T22:15:00","N>>N-NIL_DPTX","N-NIL","2013-10-01",1,-25.6569,"Out=Nil, avoid Darlington Point Tx3 or Tx4 O/L on trip of the other","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1333,"TRANSGRIDV5_20161215152814","2014-01-15T09:55:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-188.67105000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1334,"TRANSGRIDV5_20161215152814","2014-01-15T10:00:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-188.43906000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1335,"TRANSGRIDV5_20161215152814","2014-01-15T09:20:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-179.30372,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1336,"TRANSGRIDV5_20161215152814","2014-01-15T09:15:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-178.30858000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1337,"TRANSGRIDV5_20161215152814","2014-01-15T09:40:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-177.27212,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1338,"TRANSGRIDV5_20161215152814","2014-01-15T09:45:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-174.62952999999999,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1339,"TRANSGRIDV5_20161215152814","2014-01-15T09:10:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-174.51524000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1340,"TRANSGRIDV5_20161215152814","2014-01-15T09:30:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-174.27535,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1341,"TRANSGRIDV5_20161215152814","2014-01-15T09:05:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-172.67157,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1342,"TRANSGRIDV5_20161215152814","2014-01-15T09:35:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-172.31835000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1343,"TRANSGRIDV5_20161215152814","2014-01-15T08:55:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-171.51535999999999,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1344,"TRANSGRIDV5_20161215152814","2014-01-15T09:00:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-169.18754999999999,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1345,"TRANSGRIDV5_20161215152814","2014-01-15T09:50:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-159.43110999999999,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1346,"TRANSGRIDV5_20161215152814","2014-01-15T08:45:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-135.65951000000001,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1347,"TRANSGRIDV5_20161215152814","2014-01-15T08:50:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-129.77804,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1348,"TRANSGRIDV5_20161215152814","2014-01-15T09:25:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-85.638750000000002,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1349,"TRANSGRIDV5_20161215152814","2014-01-15T10:10:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-10.162409999999999,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1350,"TRANSGRIDV5_20161215152814","2014-01-15T15:15:00","NRM_VIC1_SA1","NRM_NIL_ALL","2012-06-12",1,-54.993740000000003,"Negative Residue Management constraint for VIC to SA flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[1351,"TRANSGRIDV5_20161215152814","2014-01-15T15:05:00","NRM_VIC1_SA1","NRM_NIL_ALL","2012-06-12",1,-54.46837,"Negative Residue Management constraint for VIC to SA flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[1352,"TRANSGRIDV5_20161215152814","2014-01-15T16:25:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-239.48586,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED",null,"UNPLANNED",1]
[1353,"TRANSGRIDV5_20161215152814","2014-01-15T16:20:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-13.134829999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED",null,"UNPLANNED",1]
[1354,"TRANSGRIDV5_20161215152814","2014-01-15T14:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-335031.64061,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1355,"TRANSGRIDV5_20161215152814","2014-01-15T12:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-320299.21957000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1356,"TRANSGRIDV5_20161215152814","2014-01-15T15:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-133648.53868999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1357,"TRANSGRIDV5_20161215152814","2014-01-15T13:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-119079.8383,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1358,"TRANSGRIDV5_20161215152814","2014-01-15T13:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-118578.29790000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1359,"TRANSGRIDV5_20161215152814","2014-01-15T13:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-101573.66833,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1360,"TRANSGRIDV5_20161215152814","2014-01-15T12:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-99729.012069999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1361,"TRANSGRIDV5_20161215152814","2014-01-15T12:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-99646.716709999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1362,"TRANSGRIDV5_20161215152814","2014-01-15T12:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-99404.86593,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1363,"TRANSGRIDV5_20161215152814","2014-01-15T12:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-99369.151329999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1364,"TRANSGRIDV5_20161215152814","2014-01-15T12:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-98986.276580000005,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1365,"TRANSGRIDV5_20161215152814","2014-01-15T11:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-98541.501149999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1366,"TRANSGRIDV5_20161215152814","2014-01-15T11:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-98497.9709,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1367,"TRANSGRIDV5_20161215152814","2014-01-15T11:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-94482.643400000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1368,"TRANSGRIDV5_20161215152814","2014-01-15T11:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-94433.326449999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1369,"TRANSGRIDV5_20161215152814","2014-01-15T15:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-67190.59809,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1370,"TRANSGRIDV5_20161215152814","2014-01-15T15:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-67004.815340000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1371,"TRANSGRIDV5_20161215152814","2014-01-15T14:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-66221.758650000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1372,"TRANSGRIDV5_20161215152814","2014-01-15T15:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-65981.694449999995,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1373,"TRANSGRIDV5_20161215152814","2014-01-15T15:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-65520.100250000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1374,"TRANSGRIDV5_20161215152814","2014-01-15T13:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-51788.647709999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1375,"TRANSGRIDV5_20161215152814","2014-01-15T14:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-38983.10557,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1376,"TRANSGRIDV5_20161215152814","2014-01-15T14:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-38738.982450000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1377,"TRANSGRIDV5_20161215152814","2014-01-15T14:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-38597.060559999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1378,"TRANSGRIDV5_20161215152814","2014-01-15T14:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-38584.104740000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1379,"TRANSGRIDV5_20161215152814","2014-01-15T12:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37982.247300000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1380,"TRANSGRIDV5_20161215152814","2014-01-15T12:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37570.328589999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1381,"TRANSGRIDV5_20161215152814","2014-01-15T12:40:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37479.917710000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1382,"TRANSGRIDV5_20161215152814","2014-01-15T12:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37413.426440000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1383,"TRANSGRIDV5_20161215152814","2014-01-15T12:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37373.277979999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1384,"TRANSGRIDV5_20161215152814","2014-01-15T13:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37334.783060000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1385,"TRANSGRIDV5_20161215152814","2014-01-15T14:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37330.098769999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1386,"TRANSGRIDV5_20161215152814","2014-01-15T12:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37310.395629999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1387,"TRANSGRIDV5_20161215152814","2014-01-15T14:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37223.375749999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1388,"TRANSGRIDV5_20161215152814","2014-01-15T14:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37191.122089999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1389,"TRANSGRIDV5_20161215152814","2014-01-15T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37177.741770000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1390,"TRANSGRIDV5_20161215152814","2014-01-15T13:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37131.018550000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1391,"TRANSGRIDV5_20161215152814","2014-01-15T13:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37124.501149999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1392,"TRANSGRIDV5_20161215152814","2014-01-15T13:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37120.979200000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1393,"TRANSGRIDV5_20161215152814","2014-01-15T14:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37026.212059999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1394,"TRANSGRIDV5_20161215152814","2014-01-15T14:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-37020.311670000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1395,"TRANSGRIDV5_20161215152814","2014-01-15T14:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36992.14834,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1396,"TRANSGRIDV5_20161215152814","2014-01-15T13:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36958.202080000003,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1397,"TRANSGRIDV5_20161215152814","2014-01-15T13:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-36882.565949999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1398,"TRANSGRIDV5_20161215152814","2014-01-15T15:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-3086.7989600000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1399,"TRANSGRIDV5_20161215152814","2014-01-15T15:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-2802.34744,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1400,"TRANSGRIDV5_20161215152814","2014-01-15T15:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-2578.7351399999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1401,"TRANSGRIDV5_20161215152814","2014-01-15T18:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-214.76186999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1402,"TRANSGRIDV5_20161215152814","2014-01-15T18:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-214.69422,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1403,"TRANSGRIDV5_20161215152814","2014-01-15T18:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-213.40807000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1404,"TRANSGRIDV5_20161215152814","2014-01-15T18:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-212.64589000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1405,"TRANSGRIDV5_20161215152814","2014-01-15T18:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-211.34755000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1406,"TRANSGRIDV5_20161215152814","2014-01-15T18:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-209.59404000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1407,"TRANSGRIDV5_20161215152814","2014-01-15T17:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-208.12299999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1408,"TRANSGRIDV5_20161215152814","2014-01-15T17:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-206.79035999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1409,"TRANSGRIDV5_20161215152814","2014-01-15T17:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-206.42318,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1410,"TRANSGRIDV5_20161215152814","2014-01-15T18:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-206.15878000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1411,"TRANSGRIDV5_20161215152814","2014-01-15T18:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-205.66032000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1412,"TRANSGRIDV5_20161215152814","2014-01-15T17:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-205.47881000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1413,"TRANSGRIDV5_20161215152814","2014-01-15T20:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-205.24757,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1414,"TRANSGRIDV5_20161215152814","2014-01-15T17:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-205.06171000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1415,"TRANSGRIDV5_20161215152814","2014-01-15T20:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-202.92214999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1416,"TRANSGRIDV5_20161215152814","2014-01-15T17:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-201.02762000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1417,"TRANSGRIDV5_20161215152814","2014-01-15T20:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-199.48935,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1418,"TRANSGRIDV5_20161215152814","2014-01-15T19:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-197.70868999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1419,"TRANSGRIDV5_20161215152814","2014-01-15T19:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-197.20097000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1420,"TRANSGRIDV5_20161215152814","2014-01-15T19:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-195.18398999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1421,"TRANSGRIDV5_20161215152814","2014-01-15T19:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-194.04709,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1422,"TRANSGRIDV5_20161215152814","2014-01-15T20:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-192.87746999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1423,"TRANSGRIDV5_20161215152814","2014-01-15T19:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-189.99369999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1424,"TRANSGRIDV5_20161215152814","2014-01-15T18:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-181.9074,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1425,"TRANSGRIDV5_20161215152814","2014-01-15T17:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-167.73098999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1426,"TRANSGRIDV5_20161215152814","2014-01-15T17:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-165.39458999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1427,"TRANSGRIDV5_20161215152814","2014-01-15T18:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-153.47650999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1428,"TRANSGRIDV5_20161215152814","2014-01-15T17:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-150.60157000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1429,"TRANSGRIDV5_20161215152814","2014-01-15T15:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-119.84275,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1430,"TRANSGRIDV5_20161215152814","2014-01-15T20:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-115.60442999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1431,"TRANSGRIDV5_20161215152814","2014-01-15T17:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-108.57738000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1432,"TRANSGRIDV5_20161215152814","2014-01-15T17:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-106.59444000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1433,"TRANSGRIDV5_20161215152814","2014-01-15T19:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-106.12281,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1434,"TRANSGRIDV5_20161215152814","2014-01-15T10:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.802989999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1435,"TRANSGRIDV5_20161215152814","2014-01-15T10:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-90.853480000000005,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1436,"TRANSGRIDV5_20161215152814","2014-01-15T19:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-89.08211,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1437,"TRANSGRIDV5_20161215152814","2014-01-15T16:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-55.596820000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1438,"TRANSGRIDV5_20161215152814","2014-01-15T10:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-53.364319999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1439,"TRANSGRIDV5_20161215152814","2014-01-15T10:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-50.885480000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1440,"TRANSGRIDV5_20161215152814","2014-01-15T10:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-40.955550000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1441,"TRANSGRIDV5_20161215152814","2014-01-15T21:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-39.276940000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1442,"TRANSGRIDV5_20161215152814","2014-01-15T21:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-37.553440000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1443,"TRANSGRIDV5_20161215152814","2014-01-15T21:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-36.694519999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1444,"TRANSGRIDV5_20161215152814","2014-01-15T17:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-35.991289999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1445,"TRANSGRIDV5_20161215152814","2014-01-15T20:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-35.911819999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1446,"TRANSGRIDV5_20161215152814","2014-01-15T20:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-35.300190000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1447,"TRANSGRIDV5_20161215152814","2014-01-15T21:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-32.373449999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1448,"TRANSGRIDV5_20161215152814","2014-01-15T21:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-30.05312,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1449,"TRANSGRIDV5_20161215152814","2014-01-15T21:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-29.527439999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1450,"TRANSGRIDV5_20161215152814","2014-01-15T21:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-29.07076,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1451,"TRANSGRIDV5_20161215152814","2014-01-15T22:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.65699,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1452,"TRANSGRIDV5_20161215152814","2014-01-15T19:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.630780000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1453,"TRANSGRIDV5_20161215152814","2014-01-15T21:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.18798,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1454,"TRANSGRIDV5_20161215152814","2014-01-15T21:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.048120000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1455,"TRANSGRIDV5_20161215152814","2014-01-15T21:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.335760000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1456,"TRANSGRIDV5_20161215152814","2014-01-15T21:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.280390000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1457,"TRANSGRIDV5_20161215152814","2014-01-15T21:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.241219999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1458,"TRANSGRIDV5_20161215152814","2014-01-15T23:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-23.358599999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1459,"TRANSGRIDV5_20161215152814","2014-01-15T23:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-22.95345,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1460,"TRANSGRIDV5_20161215152814","2014-01-15T18:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-14.756970000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1461,"TRANSGRIDV5_20161215152814","2014-01-15T14:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-358067.89682000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1462,"TRANSGRIDV5_20161215152814","2014-01-15T12:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-215631.29329,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1463,"TRANSGRIDV5_20161215152814","2014-01-15T15:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-153004.1183,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1464,"TRANSGRIDV5_20161215152814","2014-01-15T13:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-133260.89713,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1465,"TRANSGRIDV5_20161215152814","2014-01-15T13:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-132779.57917000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1466,"TRANSGRIDV5_20161215152814","2014-01-15T13:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-113714.20217,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1467,"TRANSGRIDV5_20161215152814","2014-01-15T11:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-101098.78494,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1468,"TRANSGRIDV5_20161215152814","2014-01-15T11:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-101043.71995,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1469,"TRANSGRIDV5_20161215152814","2014-01-15T15:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-73802.557180000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1470,"TRANSGRIDV5_20161215152814","2014-01-15T15:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-73568.004740000004,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1471,"TRANSGRIDV5_20161215152814","2014-01-15T14:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-72749.416490000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1472,"TRANSGRIDV5_20161215152814","2014-01-15T15:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-72452.696939999994,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1473,"TRANSGRIDV5_20161215152814","2014-01-15T15:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-71981.958880000006,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1474,"TRANSGRIDV5_20161215152814","2014-01-15T14:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-46941.824379999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1475,"TRANSGRIDV5_20161215152814","2014-01-15T14:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-41303.429089999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1476,"TRANSGRIDV5_20161215152814","2014-01-15T14:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-41244.295259999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1477,"TRANSGRIDV5_20161215152814","2014-01-15T12:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-40753.674220000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1478,"TRANSGRIDV5_20161215152814","2014-01-15T12:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-40314.688439999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1479,"TRANSGRIDV5_20161215152814","2014-01-15T12:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-40176.074000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1480,"TRANSGRIDV5_20161215152814","2014-01-15T12:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-40108.517749999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1481,"TRANSGRIDV5_20161215152814","2014-01-15T12:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39932.280630000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1482,"TRANSGRIDV5_20161215152814","2014-01-15T13:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39857.137219999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1483,"TRANSGRIDV5_20161215152814","2014-01-15T13:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39852.719080000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1484,"TRANSGRIDV5_20161215152814","2014-01-15T14:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39846.831440000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1485,"TRANSGRIDV5_20161215152814","2014-01-15T13:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39760.888469999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1486,"TRANSGRIDV5_20161215152814","2014-01-15T13:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39739.699390000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1487,"TRANSGRIDV5_20161215152814","2014-01-15T13:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39711.355219999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1488,"TRANSGRIDV5_20161215152814","2014-01-15T12:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39679.96572,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1489,"TRANSGRIDV5_20161215152814","2014-01-15T13:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39650.660609999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1490,"TRANSGRIDV5_20161215152814","2014-01-15T14:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39230.053679999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1491,"TRANSGRIDV5_20161215152814","2014-01-15T13:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39164.766960000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1492,"TRANSGRIDV5_20161215152814","2014-01-15T14:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39060.524689999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1493,"TRANSGRIDV5_20161215152814","2014-01-15T14:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-39054.361530000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1494,"TRANSGRIDV5_20161215152814","2014-01-15T13:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-13296.712729999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1495,"TRANSGRIDV5_20161215152814","2014-01-15T15:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-5705.1653900000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1496,"TRANSGRIDV5_20161215152814","2014-01-15T13:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-91.088949999999997,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1497,"TRANSGRIDV5_20161215152814","2014-01-15T14:35:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-41651.245589999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1498,"TRANSGRIDV5_20161215152814","2014-01-15T14:30:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-39384.782050000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1499,"TRANSGRIDV5_20161215152814","2014-01-15T14:15:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-39025.486989999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1500,"TRANSGRIDV5_20161215152814","2014-01-15T19:00:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-254.70777000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1501,"TRANSGRIDV5_20161215152814","2014-01-15T18:55:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-250.59143,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1502,"TRANSGRIDV5_20161215152814","2014-01-15T19:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-249.9076,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1503,"TRANSGRIDV5_20161215152814","2014-01-15T19:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-247.69538,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1504,"TRANSGRIDV5_20161215152814","2014-01-15T19:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-247.69538,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1505,"TRANSGRIDV5_20161215152814","2014-01-15T19:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-144.85006000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1506,"TRANSGRIDV5_20161215152814","2014-01-15T18:50:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-73.091890000000006,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1507,"TRANSGRIDV5_20161215152814","2014-01-15T12:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-129564.11199999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1508,"TRANSGRIDV5_20161215152814","2014-01-15T12:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-103057.45829,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1509,"TRANSGRIDV5_20161215152814","2014-01-15T12:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-102959.24482000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1510,"TRANSGRIDV5_20161215152814","2014-01-15T12:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-102727.78764,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1511,"TRANSGRIDV5_20161215152814","2014-01-15T12:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-102692.19532,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1512,"TRANSGRIDV5_20161215152814","2014-01-15T12:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-102300.8563,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1513,"TRANSGRIDV5_20161215152814","2014-01-15T11:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101848.02938000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1514,"TRANSGRIDV5_20161215152814","2014-01-15T11:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-101804.42594,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1515,"TRANSGRIDV5_20161215152814","2014-01-15T13:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-40730.114249999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1516,"TRANSGRIDV5_20161215152814","2014-01-15T11:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-239.23934,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1517,"TRANSGRIDV5_20161215152814","2014-01-15T11:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-236.37640999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1518,"TRANSGRIDV5_20161215152814","2014-01-15T11:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-229.51817,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1519,"TRANSGRIDV5_20161215152814","2014-01-15T11:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-216.17195000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1520,"TRANSGRIDV5_20161215152814","2014-01-15T11:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-195.45903999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1521,"TRANSGRIDV5_20161215152814","2014-01-15T10:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-147.68136999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1522,"TRANSGRIDV5_20161215152814","2014-01-15T10:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-138.90273999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1523,"TRANSGRIDV5_20161215152814","2014-01-15T11:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-137.00452999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1524,"TRANSGRIDV5_20161215152814","2014-01-15T11:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-126.36897999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1525,"TRANSGRIDV5_20161215152814","2014-01-15T11:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-114.05479,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1526,"TRANSGRIDV5_20161215152814","2014-01-15T10:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-85.512919999999994,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1527,"TRANSGRIDV5_20161215152814","2014-01-15T10:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-58.886270000000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1528,"TRANSGRIDV5_20161215152814","2014-01-15T14:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-70882.839000000007,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1529,"TRANSGRIDV5_20161215152814","2014-01-15T13:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-38672.435279999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1530,"TRANSGRIDV5_20161215152814","2014-01-15T13:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-38595.756350000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1531,"TRANSGRIDV5_20161215152814","2014-01-15T13:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-32909.356890000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1532,"TRANSGRIDV5_20161215152814","2014-01-15T11:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-20215.55343,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1533,"TRANSGRIDV5_20161215152814","2014-01-15T11:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-20203.951539999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1534,"TRANSGRIDV5_20161215152814","2014-01-15T14:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-19377.524959999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1535,"TRANSGRIDV5_20161215152814","2014-01-15T15:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-13916.85692,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1536,"TRANSGRIDV5_20161215152814","2014-01-15T15:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-11893.962949999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1537,"TRANSGRIDV5_20161215152814","2014-01-15T15:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-10452.61767,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1538,"TRANSGRIDV5_20161215152814","2014-01-15T15:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-10368.5321,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1539,"TRANSGRIDV5_20161215152814","2014-01-15T12:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-10027.60698,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1540,"TRANSGRIDV5_20161215152814","2014-01-15T12:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-10011.981030000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1541,"TRANSGRIDV5_20161215152814","2014-01-15T12:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-9997.6947199999995,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1542,"TRANSGRIDV5_20161215152814","2014-01-15T12:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-9997.0178300000007,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1543,"TRANSGRIDV5_20161215152814","2014-01-15T12:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-9950.8265800000008,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1544,"TRANSGRIDV5_20161215152814","2014-01-15T11:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-9906.2452499999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1545,"TRANSGRIDV5_20161215152814","2014-01-15T11:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-9905.8402800000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1546,"TRANSGRIDV5_20161215152814","2014-01-15T14:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8672.61643,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1547,"TRANSGRIDV5_20161215152814","2014-01-15T13:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8357.7950799999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1548,"TRANSGRIDV5_20161215152814","2014-01-15T13:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8342.7378599999993,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1549,"TRANSGRIDV5_20161215152814","2014-01-15T12:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8329.8195699999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1550,"TRANSGRIDV5_20161215152814","2014-01-15T12:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8259.4311500000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1551,"TRANSGRIDV5_20161215152814","2014-01-15T14:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8237.0768100000005,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1552,"TRANSGRIDV5_20161215152814","2014-01-15T13:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8169.3387899999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1553,"TRANSGRIDV5_20161215152814","2014-01-15T12:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8141.8967599999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1554,"TRANSGRIDV5_20161215152814","2014-01-15T14:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8141.7066199999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1555,"TRANSGRIDV5_20161215152814","2014-01-15T12:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-8125.8629700000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1556,"TRANSGRIDV5_20161215152814","2014-01-15T14:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7991.9457499999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1557,"TRANSGRIDV5_20161215152814","2014-01-15T13:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7972.9952599999997,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1558,"TRANSGRIDV5_20161215152814","2014-01-15T12:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7864.1384799999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1559,"TRANSGRIDV5_20161215152814","2014-01-15T13:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7773.5933100000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1560,"TRANSGRIDV5_20161215152814","2014-01-15T13:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7670.0796700000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1561,"TRANSGRIDV5_20161215152814","2014-01-15T12:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-7436.7663700000003,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1562,"TRANSGRIDV5_20161215152814","2014-01-15T14:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6777.43487,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1563,"TRANSGRIDV5_20161215152814","2014-01-15T14:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6763.0441700000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1564,"TRANSGRIDV5_20161215152814","2014-01-15T13:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6743.5820299999996,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1565,"TRANSGRIDV5_20161215152814","2014-01-15T14:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6726.0763100000004,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1566,"TRANSGRIDV5_20161215152814","2014-01-15T14:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6724.8896100000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1567,"TRANSGRIDV5_20161215152814","2014-01-15T14:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6722.4464200000002,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1568,"TRANSGRIDV5_20161215152814","2014-01-15T13:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-6674.0466800000004,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1569,"TRANSGRIDV5_20161215152814","2014-01-15T10:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-528.03552999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1570,"TRANSGRIDV5_20161215152814","2014-01-15T11:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-523.76306,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1571,"TRANSGRIDV5_20161215152814","2014-01-15T11:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-521.78581999999994,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1572,"TRANSGRIDV5_20161215152814","2014-01-15T11:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-521.68588,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1573,"TRANSGRIDV5_20161215152814","2014-01-15T11:30:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-520.81700000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1574,"TRANSGRIDV5_20161215152814","2014-01-15T11:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-511.56779999999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1575,"TRANSGRIDV5_20161215152814","2014-01-15T10:25:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-498.83382,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1576,"TRANSGRIDV5_20161215152814","2014-01-15T15:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-492.95652999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1577,"TRANSGRIDV5_20161215152814","2014-01-15T10:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-392.11410000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1578,"TRANSGRIDV5_20161215152814","2014-01-15T10:45:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-332.45751999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1579,"TRANSGRIDV5_20161215152814","2014-01-15T11:05:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-327.68792999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1580,"TRANSGRIDV5_20161215152814","2014-01-15T11:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-325.04437999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1581,"TRANSGRIDV5_20161215152814","2014-01-15T13:10:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-233.91479000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1582,"TRANSGRIDV5_20161215152814","2014-01-15T11:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-230.58283,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1583,"TRANSGRIDV5_20161215152814","2014-01-15T10:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-228.89547999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1584,"TRANSGRIDV5_20161215152814","2014-01-15T10:40:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-227.05681999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1585,"TRANSGRIDV5_20161215152814","2014-01-15T10:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-227.03674000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1586,"TRANSGRIDV5_20161215152814","2014-01-15T10:20:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-213.61878999999999,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1587,"TRANSGRIDV5_20161215152814","2014-01-15T10:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-206.42687000000001,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1588,"TRANSGRIDV5_20161215152814","2014-01-15T16:35:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-192.47529,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1589,"TRANSGRIDV5_20161215152814","2014-01-15T17:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-102.85271,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1590,"TRANSGRIDV5_20161215152814","2014-01-15T15:55:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-35.780169999999998,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1591,"TRANSGRIDV5_20161215152814","2014-01-15T12:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-51797.390579999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1592,"TRANSGRIDV5_20161215152814","2014-01-15T15:10:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-36751.915500000003,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1593,"TRANSGRIDV5_20161215152814","2014-01-15T15:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13755.497939999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1594,"TRANSGRIDV5_20161215152814","2014-01-15T15:05:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13668.7096,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1595,"TRANSGRIDV5_20161215152814","2014-01-15T14:50:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13578.87428,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1596,"TRANSGRIDV5_20161215152814","2014-01-15T15:15:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13477.46919,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1597,"TRANSGRIDV5_20161215152814","2014-01-15T15:20:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13444.40681,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1598,"TRANSGRIDV5_20161215152814","2014-01-15T22:40:00","V>SMLKGRC1","V-KGRC","2013-08-21",1,-52.30894,"Out = Kerang to Redcliffs 220kV line, avoid overloading Darlington Pt to Balranald (X5/1) 220kV line for trip of Ballarat to Waubra to Horsham 220 kV line","OUTAGE","OTHER","Kerang - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1599,"TRANSGRIDV5_20161215152814","2014-01-15T22:35:00","V>SMLKGRC1","V-KGRC","2013-08-21",1,-52.298369999999998,"Out = Kerang to Redcliffs 220kV line, avoid overloading Darlington Pt to Balranald (X5/1) 220kV line for trip of Ballarat to Waubra to Horsham 220 kV line","OUTAGE","OTHER","Kerang - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1600,"TRANSGRIDV5_20161215152814","2014-01-15T22:30:00","V>SMLKGRC1","V-KGRC","2013-08-21",1,-52.04157,"Out = Kerang to Redcliffs 220kV line, avoid overloading Darlington Pt to Balranald (X5/1) 220kV line for trip of Ballarat to Waubra to Horsham 220 kV line","OUTAGE","OTHER","Kerang - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1601,"TRANSGRIDV5_20161215152814","2014-01-15T22:25:00","V>SMLKGRC1","V-KGRC","2013-08-21",1,-48.082479999999997,"Out = Kerang to Redcliffs 220kV line, avoid overloading Darlington Pt to Balranald (X5/1) 220kV line for trip of Ballarat to Waubra to Horsham 220 kV line","OUTAGE","OTHER","Kerang - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1602,"TRANSGRIDV5_20161215152814","2014-01-16T14:30:00","#V-S-MNSP1_I_E","#V-S-MNSP1_E","2014-01-16",1,152.06128000000001,"V-S-MNSP1.ENERGY * -1 >= 20 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1603,"TRANSGRIDV5_20161215152814","2014-01-16T14:35:00","#V-S-MNSP1_I_E","#V-S-MNSP1_E","2014-01-16",1,59.48113,"V-S-MNSP1.ENERGY * -1 >= 20 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1604,"TRANSGRIDV5_20161215152814","2014-01-16T14:15:00","#V-S-MNSP1_I_E","#V-S-MNSP1_E","2014-01-16",1,15.528639999999999,"V-S-MNSP1.ENERGY * -1 >= 20 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1605,"TRANSGRIDV5_20161215152814","2014-01-16T14:20:00","#V-S-MNSP1_I_E","#V-S-MNSP1_E","2014-01-16",1,14.192360000000001,"V-S-MNSP1.ENERGY * -1 >= 20 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1606,"TRANSGRIDV5_20161215152814","2014-01-16T14:25:00","#V-S-MNSP1_I_E","#V-S-MNSP1_E","2014-01-16",1,14.182499999999999,"V-S-MNSP1.ENERGY * -1 >= 20 (Wt = 35)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1607,"TRANSGRIDV5_20161215152814","2014-01-16T07:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-217.78645,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1608,"TRANSGRIDV5_20161215152814","2014-01-16T08:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-193.64142000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1609,"TRANSGRIDV5_20161215152814","2014-01-16T08:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-191.93074999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1610,"TRANSGRIDV5_20161215152814","2014-01-16T08:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-186.99558999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1611,"TRANSGRIDV5_20161215152814","2014-01-16T19:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-154.31612999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1612,"TRANSGRIDV5_20161215152814","2014-01-16T08:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-139.54221000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1613,"TRANSGRIDV5_20161215152814","2014-01-16T08:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-135.94191000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1614,"TRANSGRIDV5_20161215152814","2014-01-16T08:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-135.81457,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1615,"TRANSGRIDV5_20161215152814","2014-01-16T08:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-129.72820999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1616,"TRANSGRIDV5_20161215152814","2014-01-16T07:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-128.25744,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1617,"TRANSGRIDV5_20161215152814","2014-01-16T20:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-94.730980000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1618,"TRANSGRIDV5_20161215152814","2014-01-16T19:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-60.807409999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1619,"TRANSGRIDV5_20161215152814","2014-01-16T19:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-49.96011,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1620,"TRANSGRIDV5_20161215152814","2014-01-16T20:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-46.222149999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1621,"TRANSGRIDV5_20161215152814","2014-01-16T19:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-34.835850000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1622,"TRANSGRIDV5_20161215152814","2014-01-16T19:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-33.602449999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1623,"TRANSGRIDV5_20161215152814","2014-01-16T19:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-26.000039999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1624,"TRANSGRIDV5_20161215152814","2014-01-16T19:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-24.324159999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1625,"TRANSGRIDV5_20161215152814","2014-01-16T07:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.734159999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1626,"TRANSGRIDV5_20161215152814","2014-01-16T08:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-21.514510000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1627,"TRANSGRIDV5_20161215152814","2014-01-16T08:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-20.891680000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1628,"TRANSGRIDV5_20161215152814","2014-01-16T07:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-20.377880000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1629,"TRANSGRIDV5_20161215152814","2014-01-16T08:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.34768,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1630,"TRANSGRIDV5_20161215152814","2014-01-16T23:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.83976,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1631,"TRANSGRIDV5_20161215152814","2014-01-16T06:55:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-11.598979999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1632,"TRANSGRIDV5_20161215152814","2014-01-16T15:55:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-529.38019999999995,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1633,"TRANSGRIDV5_20161215152814","2014-01-16T17:00:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-515.56712000000005,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1634,"TRANSGRIDV5_20161215152814","2014-01-16T17:20:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-427.97618999999997,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1635,"TRANSGRIDV5_20161215152814","2014-01-16T15:45:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-379.55642999999998,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1636,"TRANSGRIDV5_20161215152814","2014-01-16T17:05:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-361.27269000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1637,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-264.59820999999999,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1638,"TRANSGRIDV5_20161215152814","2014-01-16T17:25:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-191.15512000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1639,"TRANSGRIDV5_20161215152814","2014-01-16T17:30:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-183.58761999999999,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1640,"TRANSGRIDV5_20161215152814","2014-01-16T15:50:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-161.49437,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1641,"TRANSGRIDV5_20161215152814","2014-01-16T20:35:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-138.17958999999999,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1642,"TRANSGRIDV5_20161215152814","2014-01-16T14:40:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-123.40236,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1643,"TRANSGRIDV5_20161215152814","2014-01-16T15:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-109.52381,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1644,"TRANSGRIDV5_20161215152814","2014-01-16T20:30:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-73.628420000000006,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1645,"TRANSGRIDV5_20161215152814","2014-01-16T16:40:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-70.499510000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1646,"TRANSGRIDV5_20161215152814","2014-01-16T17:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-16.582229999999999,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1647,"TRANSGRIDV5_20161215152814","2014-01-16T15:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-253.91596999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1648,"TRANSGRIDV5_20161215152814","2014-01-16T12:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-209.83471,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1649,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-184.36538999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1650,"TRANSGRIDV5_20161215152814","2014-01-16T15:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-172.14491000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1651,"TRANSGRIDV5_20161215152814","2014-01-16T15:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-169.22962999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1652,"TRANSGRIDV5_20161215152814","2014-01-16T14:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-167.69553999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1653,"TRANSGRIDV5_20161215152814","2014-01-16T14:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-167.68538000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1654,"TRANSGRIDV5_20161215152814","2014-01-16T14:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-167.23937000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1655,"TRANSGRIDV5_20161215152814","2014-01-16T11:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-163.74463,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1656,"TRANSGRIDV5_20161215152814","2014-01-16T11:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-162.42153999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1657,"TRANSGRIDV5_20161215152814","2014-01-16T10:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-161.44210000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1658,"TRANSGRIDV5_20161215152814","2014-01-16T11:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-156.03143,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1659,"TRANSGRIDV5_20161215152814","2014-01-16T14:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-155.46136000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1660,"TRANSGRIDV5_20161215152814","2014-01-16T14:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-154.35227,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1661,"TRANSGRIDV5_20161215152814","2014-01-16T14:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-148.84897000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1662,"TRANSGRIDV5_20161215152814","2014-01-16T11:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-145.66732999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1663,"TRANSGRIDV5_20161215152814","2014-01-16T11:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-128.08031,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1664,"TRANSGRIDV5_20161215152814","2014-01-16T11:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-117.42592999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1665,"TRANSGRIDV5_20161215152814","2014-01-16T10:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-115.18221,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1666,"TRANSGRIDV5_20161215152814","2014-01-16T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-110.04262,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1667,"TRANSGRIDV5_20161215152814","2014-01-16T11:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-109.59629,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1668,"TRANSGRIDV5_20161215152814","2014-01-16T10:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-108.39069000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1669,"TRANSGRIDV5_20161215152814","2014-01-16T10:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-93.896330000000006,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1670,"TRANSGRIDV5_20161215152814","2014-01-16T10:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-91.491299999999995,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1671,"TRANSGRIDV5_20161215152814","2014-01-16T10:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-90.429640000000006,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1672,"TRANSGRIDV5_20161215152814","2014-01-16T13:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-87.73854,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1673,"TRANSGRIDV5_20161215152814","2014-01-16T11:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-84.87294,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1674,"TRANSGRIDV5_20161215152814","2014-01-16T13:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-80.650329999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1675,"TRANSGRIDV5_20161215152814","2014-01-16T13:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-80.650329999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1676,"TRANSGRIDV5_20161215152814","2014-01-16T09:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-61.727420000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1677,"TRANSGRIDV5_20161215152814","2014-01-16T09:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-57.525509999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1678,"TRANSGRIDV5_20161215152814","2014-01-16T15:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-52.392899999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1679,"TRANSGRIDV5_20161215152814","2014-01-16T14:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-47.25752,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1680,"TRANSGRIDV5_20161215152814","2014-01-16T10:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-39.4298,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1681,"TRANSGRIDV5_20161215152814","2014-01-16T15:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.53378,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1682,"TRANSGRIDV5_20161215152814","2014-01-16T14:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.136429999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1683,"TRANSGRIDV5_20161215152814","2014-01-16T11:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-33.815640000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1684,"TRANSGRIDV5_20161215152814","2014-01-16T15:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-32.944099999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1685,"TRANSGRIDV5_20161215152814","2014-01-16T15:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-32.452849999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1686,"TRANSGRIDV5_20161215152814","2014-01-16T14:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-30.272580000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1687,"TRANSGRIDV5_20161215152814","2014-01-16T11:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.11299,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1688,"TRANSGRIDV5_20161215152814","2014-01-16T09:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.903130000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1689,"TRANSGRIDV5_20161215152814","2014-01-16T12:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.991779999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1690,"TRANSGRIDV5_20161215152814","2014-01-16T12:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.970289999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1691,"TRANSGRIDV5_20161215152814","2014-01-16T10:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.36347,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1692,"TRANSGRIDV5_20161215152814","2014-01-16T14:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.8592,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1693,"TRANSGRIDV5_20161215152814","2014-01-16T14:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.84727,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1694,"TRANSGRIDV5_20161215152814","2014-01-16T14:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.812480000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1695,"TRANSGRIDV5_20161215152814","2014-01-16T13:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.197990000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1696,"TRANSGRIDV5_20161215152814","2014-01-16T09:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.43477,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1697,"TRANSGRIDV5_20161215152814","2014-01-16T09:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.432869999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1698,"TRANSGRIDV5_20161215152814","2014-01-16T17:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.63359,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1699,"TRANSGRIDV5_20161215152814","2014-01-16T09:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.83272,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1700,"TRANSGRIDV5_20161215152814","2014-01-16T13:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.663209999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1701,"TRANSGRIDV5_20161215152814","2014-01-16T12:55:00","N>>N-NIL_DPTX","N-NIL","2013-10-01",1,-119.92592,"Out=Nil, avoid Darlington Point Tx3 or Tx4 O/L on trip of the other","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1702,"TRANSGRIDV5_20161215152814","2014-01-16T09:30:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-108.85898,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1703,"TRANSGRIDV5_20161215152814","2014-01-16T10:40:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-104.5197,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1704,"TRANSGRIDV5_20161215152814","2014-01-16T09:35:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-78.869470000000007,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1705,"TRANSGRIDV5_20161215152814","2014-01-16T09:40:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-73.538880000000006,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1706,"TRANSGRIDV5_20161215152814","2014-01-16T10:55:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-28.870349999999998,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1707,"TRANSGRIDV5_20161215152814","2014-01-16T09:45:00","N>>V-NIL_O","N-NIL","2013-08-21",1,-23.1495,"Out = Nil, avoid overloading Upper Tumut to Murray (65) line on trip of Lower Tumut to Wagga (051) + 970,990,99M (out of Yass) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1708,"TRANSGRIDV5_20161215152814","2014-01-16T15:10:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-227.63103000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1709,"TRANSGRIDV5_20161215152814","2014-01-16T12:45:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-190.53595000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1710,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-162.66012000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1711,"TRANSGRIDV5_20161215152814","2014-01-16T15:15:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-148.77781999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1712,"TRANSGRIDV5_20161215152814","2014-01-16T15:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-148.66318000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1713,"TRANSGRIDV5_20161215152814","2014-01-16T11:20:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-145.27537000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1714,"TRANSGRIDV5_20161215152814","2014-01-16T10:35:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-144.42314999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1715,"TRANSGRIDV5_20161215152814","2014-01-16T14:55:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-144.3434,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1716,"TRANSGRIDV5_20161215152814","2014-01-16T14:45:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-144.28370000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1717,"TRANSGRIDV5_20161215152814","2014-01-16T14:50:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-143.93409,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1718,"TRANSGRIDV5_20161215152814","2014-01-16T11:30:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-143.01263,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1719,"TRANSGRIDV5_20161215152814","2014-01-16T11:05:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-139.75717,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1720,"TRANSGRIDV5_20161215152814","2014-01-16T14:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-133.97211999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1721,"TRANSGRIDV5_20161215152814","2014-01-16T14:15:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-132.99421000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1722,"TRANSGRIDV5_20161215152814","2014-01-16T14:20:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-126.53992,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1723,"TRANSGRIDV5_20161215152814","2014-01-16T11:55:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-123.32653000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1724,"TRANSGRIDV5_20161215152814","2014-01-16T11:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-109.10926000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1725,"TRANSGRIDV5_20161215152814","2014-01-16T11:15:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-103.01624,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1726,"TRANSGRIDV5_20161215152814","2014-01-16T10:15:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-100.48157,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1727,"TRANSGRIDV5_20161215152814","2014-01-16T10:50:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-95.521069999999995,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1728,"TRANSGRIDV5_20161215152814","2014-01-16T11:10:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-95.209940000000003,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1729,"TRANSGRIDV5_20161215152814","2014-01-16T10:45:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-93.979200000000006,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1730,"TRANSGRIDV5_20161215152814","2014-01-16T10:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-76.685670000000002,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1731,"TRANSGRIDV5_20161215152814","2014-01-16T10:30:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-74.289789999999996,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1732,"TRANSGRIDV5_20161215152814","2014-01-16T13:45:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-74.28049,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1733,"TRANSGRIDV5_20161215152814","2014-01-16T10:20:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-73.42389,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1734,"TRANSGRIDV5_20161215152814","2014-01-16T11:00:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-68.137,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1735,"TRANSGRIDV5_20161215152814","2014-01-16T13:30:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-66.50694,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1736,"TRANSGRIDV5_20161215152814","2014-01-16T13:50:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-66.505589999999998,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1737,"TRANSGRIDV5_20161215152814","2014-01-16T09:50:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-43.668759999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1738,"TRANSGRIDV5_20161215152814","2014-01-16T09:45:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-42.13026,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1739,"TRANSGRIDV5_20161215152814","2014-01-16T14:00:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-30.061990000000002,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1740,"TRANSGRIDV5_20161215152814","2014-01-16T10:10:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-28.924759999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1741,"TRANSGRIDV5_20161215152814","2014-01-16T14:40:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-17.477,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1742,"TRANSGRIDV5_20161215152814","2014-01-16T14:05:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-16.172930000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1743,"TRANSGRIDV5_20161215152814","2014-01-16T09:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-10.822369999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1744,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-142642.61249,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1745,"TRANSGRIDV5_20161215152814","2014-01-16T12:45:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-78521.219339999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1746,"TRANSGRIDV5_20161215152814","2014-01-16T11:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-1004.03011,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1747,"TRANSGRIDV5_20161215152814","2014-01-16T19:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-9321.1163199999992,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1748,"TRANSGRIDV5_20161215152814","2014-01-16T12:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-218.17865,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1749,"TRANSGRIDV5_20161215152814","2014-01-16T12:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-215.02065999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1750,"TRANSGRIDV5_20161215152814","2014-01-16T22:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-195.24997999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1751,"TRANSGRIDV5_20161215152814","2014-01-16T19:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-192.79740000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1752,"TRANSGRIDV5_20161215152814","2014-01-16T19:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-190.87039999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1753,"TRANSGRIDV5_20161215152814","2014-01-16T19:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-185.28689,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1754,"TRANSGRIDV5_20161215152814","2014-01-16T23:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-179.11659,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1755,"TRANSGRIDV5_20161215152814","2014-01-16T20:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-174.87045000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1756,"TRANSGRIDV5_20161215152814","2014-01-16T19:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-151.60237000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1757,"TRANSGRIDV5_20161215152814","2014-01-16T14:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-149.93436,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1758,"TRANSGRIDV5_20161215152814","2014-01-16T19:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-128.46698000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1759,"TRANSGRIDV5_20161215152814","2014-01-16T19:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-128.46695,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1760,"TRANSGRIDV5_20161215152814","2014-01-16T19:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-124.88585999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1761,"TRANSGRIDV5_20161215152814","2014-01-16T19:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-121.30452,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1762,"TRANSGRIDV5_20161215152814","2014-01-16T19:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-121.30449,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1763,"TRANSGRIDV5_20161215152814","2014-01-16T11:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-121.04263,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1764,"TRANSGRIDV5_20161215152814","2014-01-16T20:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-110.67856,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1765,"TRANSGRIDV5_20161215152814","2014-01-16T08:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-106.61978000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1766,"TRANSGRIDV5_20161215152814","2014-01-16T13:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-106.37477,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1767,"TRANSGRIDV5_20161215152814","2014-01-16T20:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-102.04588,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1768,"TRANSGRIDV5_20161215152814","2014-01-16T20:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-98.728759999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1769,"TRANSGRIDV5_20161215152814","2014-01-16T20:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-97.703389999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1770,"TRANSGRIDV5_20161215152814","2014-01-16T20:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-96.758679999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1771,"TRANSGRIDV5_20161215152814","2014-01-16T08:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-94.875230000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1772,"TRANSGRIDV5_20161215152814","2014-01-16T12:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-93.265569999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1773,"TRANSGRIDV5_20161215152814","2014-01-16T12:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-88.180999999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1774,"TRANSGRIDV5_20161215152814","2014-01-16T12:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-85.8506,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1775,"TRANSGRIDV5_20161215152814","2014-01-16T12:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-85.56277,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1776,"TRANSGRIDV5_20161215152814","2014-01-16T12:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-84.893100000000004,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1777,"TRANSGRIDV5_20161215152814","2014-01-16T11:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-58.338239999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1778,"TRANSGRIDV5_20161215152814","2014-01-16T12:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-39.099330000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1779,"TRANSGRIDV5_20161215152814","2014-01-16T22:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-29.697939999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1780,"TRANSGRIDV5_20161215152814","2014-01-16T22:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-29.30059,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1781,"TRANSGRIDV5_20161215152814","2014-01-16T22:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-28.568619999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1782,"TRANSGRIDV5_20161215152814","2014-01-16T21:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.891169999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1783,"TRANSGRIDV5_20161215152814","2014-01-16T23:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-25.25741,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1784,"TRANSGRIDV5_20161215152814","2014-01-16T21:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-23.930599999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1785,"TRANSGRIDV5_20161215152814","2014-01-16T21:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-21.30424,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1786,"TRANSGRIDV5_20161215152814","2014-01-16T21:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-20.181640000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1787,"TRANSGRIDV5_20161215152814","2014-01-16T21:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-20.00019,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1788,"TRANSGRIDV5_20161215152814","2014-01-16T20:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-19.494700000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1789,"TRANSGRIDV5_20161215152814","2014-01-16T21:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-19.390029999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1790,"TRANSGRIDV5_20161215152814","2014-01-16T21:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-18.867360000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1791,"TRANSGRIDV5_20161215152814","2014-01-16T20:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-18.663350000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1792,"TRANSGRIDV5_20161215152814","2014-01-16T22:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-17.83764,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1793,"TRANSGRIDV5_20161215152814","2014-01-16T21:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-17.716100000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1794,"TRANSGRIDV5_20161215152814","2014-01-16T22:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-15.333629999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1795,"TRANSGRIDV5_20161215152814","2014-01-16T12:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-86217.620259999996,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1796,"TRANSGRIDV5_20161215152814","2014-01-16T08:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-243.88791000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1797,"TRANSGRIDV5_20161215152814","2014-01-16T08:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-241.87096,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1798,"TRANSGRIDV5_20161215152814","2014-01-16T08:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-235.02809999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1799,"TRANSGRIDV5_20161215152814","2014-01-16T09:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-142.08501000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1800,"TRANSGRIDV5_20161215152814","2014-01-16T08:45:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-132.21208999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1801,"TRANSGRIDV5_20161215152814","2014-01-16T08:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-123.09491,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1802,"TRANSGRIDV5_20161215152814","2014-01-16T08:20:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-52.2515,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1803,"TRANSGRIDV5_20161215152814","2014-01-16T08:30:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-50.34984,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1804,"TRANSGRIDV5_20161215152814","2014-01-16T08:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-35.894469999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1805,"TRANSGRIDV5_20161215152814","2014-01-16T08:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2013-12-05",1,-30.307089999999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1806,"TRANSGRIDV5_20161215152814","2014-01-16T13:50:00","V>>SML_NIL_1_5M","V-NIL","2013-12-05",1,-186.65665000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1807,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-148713.33001999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1808,"TRANSGRIDV5_20161215152814","2014-01-16T11:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-1106.6374499999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1809,"TRANSGRIDV5_20161215152814","2014-01-16T10:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-239.80293,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1810,"TRANSGRIDV5_20161215152814","2014-01-16T10:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-197.01988,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1811,"TRANSGRIDV5_20161215152814","2014-01-16T09:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-195.96854999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1812,"TRANSGRIDV5_20161215152814","2014-01-16T10:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-184.36542,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1813,"TRANSGRIDV5_20161215152814","2014-01-16T09:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-183.52856,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1814,"TRANSGRIDV5_20161215152814","2014-01-16T09:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-179.34805,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1815,"TRANSGRIDV5_20161215152814","2014-01-16T09:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-168.84401,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1816,"TRANSGRIDV5_20161215152814","2014-01-16T09:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-152.75909999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1817,"TRANSGRIDV5_20161215152814","2014-01-16T11:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-106.80405,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1818,"TRANSGRIDV5_20161215152814","2014-01-16T11:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-95.995260000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1819,"TRANSGRIDV5_20161215152814","2014-01-16T11:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-92.72842,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1820,"TRANSGRIDV5_20161215152814","2014-01-16T10:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-82.889240000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1821,"TRANSGRIDV5_20161215152814","2014-01-16T10:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-74.842510000000004,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1822,"TRANSGRIDV5_20161215152814","2014-01-16T10:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-71.921480000000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1823,"TRANSGRIDV5_20161215152814","2014-01-16T10:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-69.509240000000005,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1824,"TRANSGRIDV5_20161215152814","2014-01-16T10:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-68.813109999999995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1825,"TRANSGRIDV5_20161215152814","2014-01-16T10:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-67.908010000000004,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1826,"TRANSGRIDV5_20161215152814","2014-01-16T10:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-67.313869999999994,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1827,"TRANSGRIDV5_20161215152814","2014-01-16T10:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-61.889679999999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1828,"TRANSGRIDV5_20161215152814","2014-01-16T11:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-47.95635,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1829,"TRANSGRIDV5_20161215152814","2014-01-16T11:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-46.807099999999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1830,"TRANSGRIDV5_20161215152814","2014-01-16T11:05:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-18.544219999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1831,"TRANSGRIDV5_20161215152814","2014-01-16T09:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-14.09487,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1832,"TRANSGRIDV5_20161215152814","2014-01-16T10:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-11.14157,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1833,"TRANSGRIDV5_20161215152814","2014-01-16T12:50:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-115.20075,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1834,"TRANSGRIDV5_20161215152814","2014-01-16T13:00:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-112.82402,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1835,"TRANSGRIDV5_20161215152814","2014-01-16T12:45:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-15966.415230000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1836,"TRANSGRIDV5_20161215152814","2014-01-16T11:35:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-12565.855020000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1837,"TRANSGRIDV5_20161215152814","2014-01-16T16:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-10993.17438,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1838,"TRANSGRIDV5_20161215152814","2014-01-16T15:55:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-8439.4449600000007,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1839,"TRANSGRIDV5_20161215152814","2014-01-16T12:10:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-202.64815999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1840,"TRANSGRIDV5_20161215152814","2014-01-16T12:00:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-197.87246999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1841,"TRANSGRIDV5_20161215152814","2014-01-16T12:05:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-192.30556999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1842,"TRANSGRIDV5_20161215152814","2014-01-16T12:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-191.44126,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1843,"TRANSGRIDV5_20161215152814","2014-01-16T12:25:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-189.12862000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1844,"TRANSGRIDV5_20161215152814","2014-01-16T15:15:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-142.1711,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1845,"TRANSGRIDV5_20161215152814","2014-01-16T11:40:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-134.21413000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1846,"TRANSGRIDV5_20161215152814","2014-01-16T16:05:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-27.548929999999999,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1847,"TRANSGRIDV5_20161215152814","2014-01-16T16:15:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-17.25639,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1848,"TRANSGRIDV5_20161215152814","2014-01-16T13:30:00","V>>V_NIL_3","V-NIL","2013-12-03",1,-13.086740000000001,"Out = Nil, avoid O/L either Dederang to South Morang 330 kV line (flow South) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1849,"TRANSGRIDV5_20161215152814","2014-01-16T16:30:00","V>SMLHORC1","V-HORC","2013-08-21",1,-7123.5528599999998,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1850,"TRANSGRIDV5_20161215152814","2014-01-16T15:55:00","V>SMLHORC1","V-HORC","2013-08-21",1,-5106.9400599999999,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1851,"TRANSGRIDV5_20161215152814","2014-01-16T13:05:00","V>SMLHORC1","V-HORC","2013-08-21",1,-140.28514000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1852,"TRANSGRIDV5_20161215152814","2014-01-16T15:15:00","V>SMLHORC1","V-HORC","2013-08-21",1,-103.54779000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1853,"TRANSGRIDV5_20161215152814","2014-01-16T13:00:00","V>SMLHORC1","V-HORC","2013-08-21",1,-65.841809999999995,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1854,"TRANSGRIDV5_20161215152814","2014-01-16T15:30:00","V>SMLHORC1","V-HORC","2013-08-21",1,-43.532789999999999,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1855,"TRANSGRIDV5_20161215152814","2014-01-16T15:10:00","V>SMLHORC1","V-HORC","2013-08-21",1,-42.104419999999998,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1856,"TRANSGRIDV5_20161215152814","2014-01-16T15:25:00","V>SMLHORC1","V-HORC","2013-08-21",1,-37.63411,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1857,"TRANSGRIDV5_20161215152814","2014-01-16T15:20:00","V>SMLHORC1","V-HORC","2013-08-21",1,-36.083469999999998,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1858,"TRANSGRIDV5_20161215152814","2014-01-16T15:05:00","V>SMLHORC1","V-HORC","2013-08-21",1,-32.673360000000002,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1859,"TRANSGRIDV5_20161215152814","2014-01-16T16:05:00","V>SMLHORC1","V-HORC","2013-08-21",1,-30.120290000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1860,"TRANSGRIDV5_20161215152814","2014-01-16T16:15:00","V>SMLHORC1","V-HORC","2013-08-21",1,-24.463650000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1861,"TRANSGRIDV5_20161215152814","2014-01-16T16:45:00","V>SMLHORC1","V-HORC","2013-08-21",1,-19.176580000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1862,"TRANSGRIDV5_20161215152814","2014-01-16T16:35:00","V>SMLHORC1","V-HORC","2013-08-21",1,-18.560749999999999,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1863,"TRANSGRIDV5_20161215152814","2014-01-16T16:25:00","V>SMLHORC1","V-HORC","2013-08-21",1,-17.853809999999999,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1864,"TRANSGRIDV5_20161215152814","2014-01-16T16:40:00","V>SMLHORC1","V-HORC","2013-08-21",1,-16.039580000000001,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1865,"TRANSGRIDV5_20161215152814","2014-01-16T16:50:00","V>SMLHORC1","V-HORC","2013-08-21",1,-15.90293,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1866,"TRANSGRIDV5_20161215152814","2014-01-16T16:20:00","V>SMLHORC1","V-HORC","2013-08-21",1,-15.44867,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1867,"TRANSGRIDV5_20161215152814","2014-01-16T16:55:00","V>SMLHORC1","V-HORC","2013-08-21",1,-14.938789999999999,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1868,"TRANSGRIDV5_20161215152814","2014-01-16T15:35:00","V>SMLHORC1","V-HORC","2013-08-21",1,-12.98204,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1869,"TRANSGRIDV5_20161215152814","2014-01-16T15:40:00","V>SMLHORC1","V-HORC","2013-08-21",1,-12.9473,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1870,"TRANSGRIDV5_20161215152814","2014-01-16T16:10:00","V>SMLHORC1","V-HORC","2013-08-21",1,-12.94177,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1871,"TRANSGRIDV5_20161215152814","2014-01-16T16:00:00","V>SMLHORC1","V-HORC","2013-08-21",1,-12.01811,"Out = Horsham to Red Cliffs 220kV line, avoid overloading Balranald to Darlington Pt (X5/1) 220kV line for trip of Bendigo to Kerang line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[1872,"TRANSGRIDV5_20161215152814","2014-01-16T14:10:00","VSML_000","I-VSML_000","2008-08-05",1,-162.22361000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1873,"TRANSGRIDV5_20161215152814","2014-01-16T14:00:00","VSML_000","I-VSML_000","2008-08-05",1,-120.35776,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1874,"TRANSGRIDV5_20161215152814","2014-01-16T13:20:00","VSML_000","I-VSML_000","2008-08-05",1,-117.99863000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1875,"TRANSGRIDV5_20161215152814","2014-01-16T13:15:00","VSML_000","I-VSML_000","2008-08-05",1,-115.33629999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1876,"TRANSGRIDV5_20161215152814","2014-01-16T13:25:00","VSML_000","I-VSML_000","2008-08-05",1,-101.31516000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1877,"TRANSGRIDV5_20161215152814","2014-01-16T13:40:00","VSML_000","I-VSML_000","2008-08-05",1,-19.500920000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1878,"TRANSGRIDV5_20161215152814","2014-01-17T10:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-234.71600000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1879,"TRANSGRIDV5_20161215152814","2014-01-17T10:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-197.53443999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1880,"TRANSGRIDV5_20161215152814","2014-01-17T10:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-188.00827000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1881,"TRANSGRIDV5_20161215152814","2014-01-17T10:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-76.314160000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1882,"TRANSGRIDV5_20161215152814","2014-01-17T10:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-71.738069999999993,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1883,"TRANSGRIDV5_20161215152814","2014-01-17T10:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.69614,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1884,"TRANSGRIDV5_20161215152814","2014-01-17T14:20:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-566.90956000000006,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1885,"TRANSGRIDV5_20161215152814","2014-01-17T14:45:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-530.65476000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1886,"TRANSGRIDV5_20161215152814","2014-01-17T14:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-529.60407999999995,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1887,"TRANSGRIDV5_20161215152814","2014-01-17T12:50:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-125.79091,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1888,"TRANSGRIDV5_20161215152814","2014-01-17T12:55:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-106.77815,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1889,"TRANSGRIDV5_20161215152814","2014-01-17T14:30:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-104.94247,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1890,"TRANSGRIDV5_20161215152814","2014-01-17T13:00:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-101.65819,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1891,"TRANSGRIDV5_20161215152814","2014-01-17T14:40:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-79.757869999999997,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1892,"TRANSGRIDV5_20161215152814","2014-01-17T14:50:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-79.734049999999996,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1893,"TRANSGRIDV5_20161215152814","2014-01-17T14:10:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-78.481290000000001,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1894,"TRANSGRIDV5_20161215152814","2014-01-17T12:15:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-71.949079999999995,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1895,"TRANSGRIDV5_20161215152814","2014-01-17T11:05:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-26.693090000000002,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1896,"TRANSGRIDV5_20161215152814","2014-01-17T11:10:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-26.45233,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1897,"TRANSGRIDV5_20161215152814","2014-01-17T12:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-72.219110000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1898,"TRANSGRIDV5_20161215152814","2014-01-17T12:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-58.884300000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1899,"TRANSGRIDV5_20161215152814","2014-01-17T11:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.632449999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1900,"TRANSGRIDV5_20161215152814","2014-01-17T12:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.849830000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1901,"TRANSGRIDV5_20161215152814","2014-01-17T15:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.739649999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1902,"TRANSGRIDV5_20161215152814","2014-01-17T12:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.01402,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1903,"TRANSGRIDV5_20161215152814","2014-01-17T15:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.9847,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1904,"TRANSGRIDV5_20161215152814","2014-01-17T15:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.2242,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1905,"TRANSGRIDV5_20161215152814","2014-01-17T13:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.891959999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1906,"TRANSGRIDV5_20161215152814","2014-01-17T10:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.7926,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1907,"TRANSGRIDV5_20161215152814","2014-01-17T15:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.765930000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1908,"TRANSGRIDV5_20161215152814","2014-01-17T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.736459999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1909,"TRANSGRIDV5_20161215152814","2014-01-17T14:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.700839999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1910,"TRANSGRIDV5_20161215152814","2014-01-17T14:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.684979999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1911,"TRANSGRIDV5_20161215152814","2014-01-17T13:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.47578,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1912,"TRANSGRIDV5_20161215152814","2014-01-17T13:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.316090000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1913,"TRANSGRIDV5_20161215152814","2014-01-17T14:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.176299999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1914,"TRANSGRIDV5_20161215152814","2014-01-17T14:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.16751,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1915,"TRANSGRIDV5_20161215152814","2014-01-17T13:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.033429999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1916,"TRANSGRIDV5_20161215152814","2014-01-17T13:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.02885,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1917,"TRANSGRIDV5_20161215152814","2014-01-17T13:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.01722,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1918,"TRANSGRIDV5_20161215152814","2014-01-17T13:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.7614,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1919,"TRANSGRIDV5_20161215152814","2014-01-17T14:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.69224,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1920,"TRANSGRIDV5_20161215152814","2014-01-17T13:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.435029999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1921,"TRANSGRIDV5_20161215152814","2014-01-17T13:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.38453,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1922,"TRANSGRIDV5_20161215152814","2014-01-17T15:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.35487,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1923,"TRANSGRIDV5_20161215152814","2014-01-17T12:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.227880000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1924,"TRANSGRIDV5_20161215152814","2014-01-17T10:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.07127,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[1925,"TRANSGRIDV5_20161215152814","2014-01-17T20:55:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,12351.986349999999,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1926,"TRANSGRIDV5_20161215152814","2014-01-17T20:45:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,12348.30761,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1927,"TRANSGRIDV5_20161215152814","2014-01-17T20:50:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,12347.87371,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1928,"TRANSGRIDV5_20161215152814","2014-01-17T20:40:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,12347.45199,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1929,"TRANSGRIDV5_20161215152814","2014-01-17T20:35:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,12347.3,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1930,"TRANSGRIDV5_20161215152814","2014-01-17T12:05:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-58.232430000000001,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1931,"TRANSGRIDV5_20161215152814","2014-01-17T12:00:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-43.649439999999998,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1932,"TRANSGRIDV5_20161215152814","2014-01-17T11:25:00","Q:N_BI_POT_-050","Q-MIBCK_9903_9904","2014-01-08",1,-14.911519999999999,"Nominated Offset -50MW, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1933,"TRANSGRIDV5_20161215152814","2014-01-17T15:45:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-6810.6544800000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1934,"TRANSGRIDV5_20161215152814","2014-01-17T16:35:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-870.82042000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1935,"TRANSGRIDV5_20161215152814","2014-01-17T16:40:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-645.16616999999997,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1936,"TRANSGRIDV5_20161215152814","2014-01-17T16:25:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-534.96339999999998,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1937,"TRANSGRIDV5_20161215152814","2014-01-17T17:10:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-350.99,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1938,"TRANSGRIDV5_20161215152814","2014-01-17T17:15:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-350.99,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1939,"TRANSGRIDV5_20161215152814","2014-01-17T17:05:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-350.98991999999998,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1940,"TRANSGRIDV5_20161215152814","2014-01-17T17:20:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-330.92630000000003,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1941,"TRANSGRIDV5_20161215152814","2014-01-17T15:10:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-304.92392000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1942,"TRANSGRIDV5_20161215152814","2014-01-17T23:50:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-292.67955000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1943,"TRANSGRIDV5_20161215152814","2014-01-17T23:45:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-283.43365,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1944,"TRANSGRIDV5_20161215152814","2014-01-17T17:25:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-83.852930000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1945,"TRANSGRIDV5_20161215152814","2014-01-17T17:35:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-69.708060000000003,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1946,"TRANSGRIDV5_20161215152814","2014-01-17T17:30:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-54.02984,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1947,"TRANSGRIDV5_20161215152814","2014-01-17T12:50:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-38.147840000000002,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East to Waterloo line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1948,"TRANSGRIDV5_20161215152814","2014-01-17T15:30:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-28.471889999999998,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1949,"TRANSGRIDV5_20161215152814","2014-01-17T15:25:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-21.477450000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1950,"TRANSGRIDV5_20161215152814","2014-01-17T15:15:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-13.12604,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1951,"TRANSGRIDV5_20161215152814","2014-01-17T14:45:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-11.045590000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1952,"TRANSGRIDV5_20161215152814","2014-01-17T15:35:00","S>RBTU2_DVBG_WEWT","S-RBPA+RBTU","2014-01-17",1,-10.15319,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines; avoid O/L Waterloo East-Waterloo 132kV line on trip of Davenport - Bungama 275KV line.","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1953,"TRANSGRIDV5_20161215152814","2014-01-17T12:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-341582.33695999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1954,"TRANSGRIDV5_20161215152814","2014-01-17T11:25:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69801.93475,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1955,"TRANSGRIDV5_20161215152814","2014-01-17T11:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-69166.344809999995,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1956,"TRANSGRIDV5_20161215152814","2014-01-17T14:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-3727.20001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1957,"TRANSGRIDV5_20161215152814","2014-01-17T16:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-1033.5021400000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1958,"TRANSGRIDV5_20161215152814","2014-01-17T14:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-595.03652999999997,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1959,"TRANSGRIDV5_20161215152814","2014-01-17T16:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-189.57817,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1960,"TRANSGRIDV5_20161215152814","2014-01-17T19:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-98.323179999999994,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1961,"TRANSGRIDV5_20161215152814","2014-01-17T16:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-94.486069999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1962,"TRANSGRIDV5_20161215152814","2014-01-17T16:55:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-93.031499999999994,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1963,"TRANSGRIDV5_20161215152814","2014-01-17T17:00:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-91.341579999999993,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1964,"TRANSGRIDV5_20161215152814","2014-01-17T14:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-24.858139999999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1965,"TRANSGRIDV5_20161215152814","2014-01-17T17:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-13.502660000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1966,"TRANSGRIDV5_20161215152814","2014-01-17T11:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-225.96540999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1967,"TRANSGRIDV5_20161215152814","2014-01-17T11:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-220.15593000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1968,"TRANSGRIDV5_20161215152814","2014-01-17T11:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-209.96023,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1969,"TRANSGRIDV5_20161215152814","2014-01-17T12:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-205.75242,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1970,"TRANSGRIDV5_20161215152814","2014-01-17T11:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-201.51517000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1971,"TRANSGRIDV5_20161215152814","2014-01-17T08:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-199.36607000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1972,"TRANSGRIDV5_20161215152814","2014-01-17T08:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-197.79247000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1973,"TRANSGRIDV5_20161215152814","2014-01-17T12:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-115.65,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1974,"TRANSGRIDV5_20161215152814","2014-01-17T12:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-111.14273,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1975,"TRANSGRIDV5_20161215152814","2014-01-17T11:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-109.77576999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1976,"TRANSGRIDV5_20161215152814","2014-01-17T08:15:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-31.665949999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1977,"TRANSGRIDV5_20161215152814","2014-01-17T08:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-27.9267,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1978,"TRANSGRIDV5_20161215152814","2014-01-17T08:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-27.540959999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1979,"TRANSGRIDV5_20161215152814","2014-01-17T08:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-27.294219999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1980,"TRANSGRIDV5_20161215152814","2014-01-17T08:25:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.981940000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1981,"TRANSGRIDV5_20161215152814","2014-01-17T08:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.276299999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1982,"TRANSGRIDV5_20161215152814","2014-01-17T12:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-24.223960000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1983,"TRANSGRIDV5_20161215152814","2014-01-17T08:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-23.88598,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1984,"TRANSGRIDV5_20161215152814","2014-01-17T09:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-20.295159999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1985,"TRANSGRIDV5_20161215152814","2014-01-17T08:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-19.288920000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1986,"TRANSGRIDV5_20161215152814","2014-01-17T08:45:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-18.809650000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1987,"TRANSGRIDV5_20161215152814","2014-01-17T09:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-15.165179999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1988,"TRANSGRIDV5_20161215152814","2014-01-17T10:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.720829999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[1989,"TRANSGRIDV5_20161215152814","2014-01-17T19:55:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-118.1349,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1990,"TRANSGRIDV5_20161215152814","2014-01-17T18:05:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-47.524979999999999,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1991,"TRANSGRIDV5_20161215152814","2014-01-17T18:10:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-46.885939999999998,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1992,"TRANSGRIDV5_20161215152814","2014-01-17T17:55:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-40.446689999999997,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1993,"TRANSGRIDV5_20161215152814","2014-01-17T17:50:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-24.969950000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1994,"TRANSGRIDV5_20161215152814","2014-01-17T18:00:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-21.914449999999999,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1995,"TRANSGRIDV5_20161215152814","2014-01-17T17:15:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-19.36994,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1996,"TRANSGRIDV5_20161215152814","2014-01-17T18:20:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-14.28354,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1997,"TRANSGRIDV5_20161215152814","2014-01-17T18:25:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-14.28354,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1998,"TRANSGRIDV5_20161215152814","2014-01-17T18:35:00","V>>S_RBTU2_BRPA_WTTP","S-RBPA+RBTU","2014-01-17",1,-14.28342,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[1999,"TRANSGRIDV5_20161215152814","2014-01-17T20:05:00","V>>S_RBTU2_BUPA_BRPA","S-RBPA+RBTU","2014-01-17",1,-11.492240000000001,"Out = Robertstown - Para and Robertstown - Tungkillo 275kV lines , avoid O/L Brinkworth - Templers West line on trip of Bungama - Blyth West 275kV line, Feedback","OUTAGE","OTHER","Robertstown - Para and Robertstown - Tungkillo 275kV Lines","REGULATED",99,"Non Inclusion",null,0]
[2005,"TRANSGRIDV5_20161215152814","2014-01-17T17:45:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-88.997720000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2012,"TRANSGRIDV5_20161215152814","2014-01-17T17:10:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-25.38551,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2022,"TRANSGRIDV5_20161215152814","2014-01-17T10:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-44.580680000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2038,"TRANSGRIDV5_20161215152814","2014-01-17T12:15:00","V>>V_NIL_1B","V-NIL","2013-12-03",1,-75.745720000000006,"Out = Nil, avoid O/L Dederang to Murray No.2 330kV line (flow MSS to DDTS) for loss of the parallel No.1 line, DBUSS-Line control scheme enabled, 15 min line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2049,"TRANSGRIDV5_20161215152814","2014-01-17T17:30:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-432.40053,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2060,"TRANSGRIDV5_20161215152814","2014-01-18T16:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-29.876200000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2066,"TRANSGRIDV5_20161215152814","2014-01-18T16:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-26.68995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2075,"TRANSGRIDV5_20161215152814","2014-01-18T15:05:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-10.89317,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2093,"TRANSGRIDV5_20161215152814","2014-01-20T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-53.912419999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2101,"TRANSGRIDV5_20161215152814","2014-01-20T15:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.227240000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2114,"TRANSGRIDV5_20161215152814","2014-01-20T15:30:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-110.91363,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2116,"TRANSGRIDV5_20161215152814","2014-01-20T12:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-105.70323,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2131,"TRANSGRIDV5_20161215152814","2014-01-20T16:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-19.900700000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2138,"TRANSGRIDV5_20161215152814","2014-01-20T18:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.87242,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2148,"TRANSGRIDV5_20161215152814","2014-01-20T14:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.46242,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2164,"TRANSGRIDV5_20161215152814","2014-01-20T19:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-10.03834,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2175,"TRANSGRIDV5_20161215152814","2014-01-21T16:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.09243,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2179,"TRANSGRIDV5_20161215152814","2014-01-21T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.305860000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2196,"TRANSGRIDV5_20161215152814","2014-01-21T16:15:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-28.329529999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2208,"TRANSGRIDV5_20161215152814","2014-01-21T14:35:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-13.05667,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2211,"TRANSGRIDV5_20161215152814","2014-01-22T15:45:00","#R009795_018_RAMP_F","#R009795_RAMP","2014-01-22",1,-29.83071,"Hard Ramping constraint for constraint V>SMLBAHO4, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Horsham - Warbura 220kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[2225,"TRANSGRIDV5_20161215152814","2014-01-22T10:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-96.451340000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2237,"TRANSGRIDV5_20161215152814","2014-01-22T14:30:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-565.07397000000003,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2246,"TRANSGRIDV5_20161215152814","2014-01-22T10:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-16.382639999999999,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2252,"TRANSGRIDV5_20161215152814","2014-01-22T12:40:00","N>>N-NIL__2_OPENED","N-NIL_RBKU_OPENED","2014-01-07",1,-51.723619999999997,"Out= NIL, avoid O/L Liddell to Tamworth (84) on trip of Liddell to Muswellbrook (83) line, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2263,"TRANSGRIDV5_20161215152814","2014-01-22T17:05:00","V>SMLBAHO1","V-BAHO","2013-08-21",1,-25.06803,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","OUTAGE","OTHER","Horsham - Redcliffs 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[2274,"TRANSGRIDV5_20161215152814","2014-01-23T15:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-37.134720000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2290,"TRANSGRIDV5_20161215152814","2014-01-23T10:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-23.40483,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[2300,"TRANSGRIDV5_20161215152814","2014-01-23T16:55:00","V>>V_BAELML_1","V-BA_EL_ML","2013-12-03",1,-102.64718999999999,"Out = Moorabool to Elaine to Ballarat 220 kV line, avoid O/L Moorabool to Ballarat No. 1 220 kV line on trip of Moorabool to Terang 220 kV line, feedback","OUTAGE","OTHER"," Moorabool - Elaine - Ballarat 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[2307,"TRANSGRIDV5_20161215152814","2014-01-23T17:00:00","V>>V_BAELML_1","V-BA_EL_ML","2013-12-03",1,-95.049980000000005,"Out = Moorabool to Elaine to Ballarat 220 kV line, avoid O/L Moorabool to Ballarat No. 1 220 kV line on trip of Moorabool to Terang 220 kV line, feedback","OUTAGE","OTHER"," Moorabool - Elaine - Ballarat 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[2315,"TRANSGRIDV5_20161215152814","2014-01-23T18:10:00","V>>V_BAELML_1","V-BA_EL_ML","2013-12-03",1,-56.240070000000003,"Out = Moorabool to Elaine to Ballarat 220 kV line, avoid O/L Moorabool to Ballarat No. 1 220 kV line on trip of Moorabool to Terang 220 kV line, feedback","OUTAGE","OTHER"," Moorabool - Elaine - Ballarat 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[2328,"TRANSGRIDV5_20161215152814","2014-01-24T08:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-30.670649999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2341,"TRANSGRIDV5_20161215152814","2014-01-26T18:35:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-21.658049999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2355,"TRANSGRIDV5_20161215152814","2014-01-26T17:20:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-20.231739999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2363,"TRANSGRIDV5_20161215152814","2014-01-26T19:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-19.068539999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2372,"TRANSGRIDV5_20161215152814","2014-01-27T17:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-87.619649999999993,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2378,"TRANSGRIDV5_20161215152814","2014-01-27T18:05:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-30.844370000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2399,"TRANSGRIDV5_20161215152814","2014-01-27T15:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-18.73996,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2405,"TRANSGRIDV5_20161215152814","2014-01-27T18:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-22.195060000000002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2410,"TRANSGRIDV5_20161215152814","2014-01-27T19:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-43.928629999999998,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2422,"TRANSGRIDV5_20161215152814","2014-01-27T18:15:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-30.418050000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2436,"TRANSGRIDV5_20161215152814","2014-01-28T15:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-215.99409,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2449,"TRANSGRIDV5_20161215152814","2014-01-28T16:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-110.31957,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2462,"TRANSGRIDV5_20161215152814","2014-01-28T12:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-39.556939999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2470,"TRANSGRIDV5_20161215152814","2014-01-28T17:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-37.893590000000003,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2477,"TRANSGRIDV5_20161215152814","2014-01-28T10:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.894269999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2487,"TRANSGRIDV5_20161215152814","2014-01-28T09:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-18.690390000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2499,"TRANSGRIDV5_20161215152814","2014-01-28T12:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.500260000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2514,"TRANSGRIDV5_20161215152814","2014-01-28T15:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-51.967190000000002,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2525,"TRANSGRIDV5_20161215152814","2014-01-28T13:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-2464.1480299999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2531,"TRANSGRIDV5_20161215152814","2014-01-28T14:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-117.66262999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2540,"TRANSGRIDV5_20161215152814","2014-01-28T12:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2013-12-03",1,-42.924840000000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2552,"TRANSGRIDV5_20161215152814","2014-01-28T16:55:00","V>>V_NIL_4A","V-NIL","2013-12-03",1,-8939.0691000000006,"Out = Nil, avoid pre-contingent O/L of the Dederang H1 330/220kV transformer, DBUSS-Transformer control scheme armed, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2566,"TRANSGRIDV5_20161215152814","2014-01-29T16:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-26.781500000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2569,"TRANSGRIDV5_20161215152814","2014-01-29T19:05:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-24.594660000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2581,"TRANSGRIDV5_20161215152814","2014-01-29T17:50:00","V>>SML_NIL_7B","V-NIL","2013-12-03",1,-20.452680000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2598,"TRANSGRIDV5_20161215152814","2014-01-30T15:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-766.83064000000002,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2602,"TRANSGRIDV5_20161215152814","2014-01-30T13:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-196.17986999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2613,"TRANSGRIDV5_20161215152814","2014-01-30T15:10:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-4240.3305899999996,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2629,"TRANSGRIDV5_20161215152814","2014-01-30T15:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-30",1,-4240.39786,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2635,"TRANSGRIDV5_20161215152814","2014-01-30T15:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-30",1,-256.37212,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2646,"TRANSGRIDV5_20161215152814","2014-01-30T13:50:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-30",1,-21.588349999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2661,"TRANSGRIDV5_20161215152814","2014-01-30T12:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-30",1,-11.18496,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2663,"TRANSGRIDV5_20161215152814","2014-01-30T17:40:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-44.008620000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2676,"TRANSGRIDV5_20161215152814","2014-01-30T18:05:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-20.855219999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2684,"TRANSGRIDV5_20161215152814","2014-01-30T17:30:00","V>>SML_NIL_7A","V-NIL","2013-08-21",1,-18.07696,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2702,"TRANSGRIDV5_20161215152814","2014-01-31T13:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-22680.1459,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2711,"TRANSGRIDV5_20161215152814","2014-01-31T16:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-65.118639999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2724,"TRANSGRIDV5_20161215152814","2014-01-31T15:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.256600000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2728,"TRANSGRIDV5_20161215152814","2014-01-31T11:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.025639999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2739,"TRANSGRIDV5_20161215152814","2014-01-31T13:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-266744.96179999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2755,"TRANSGRIDV5_20161215152814","2014-01-31T18:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-12.57719,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2765,"TRANSGRIDV5_20161215152814","2014-01-31T18:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-10.42831,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2776,"TRANSGRIDV5_20161215152814","2014-01-31T17:25:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-23.067080000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2780,"TRANSGRIDV5_20161215152814","2014-01-31T16:40:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-20.068200000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2797,"TRANSGRIDV5_20161215152814","2014-01-31T14:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-380.23975999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2805,"TRANSGRIDV5_20161215152814","2014-01-31T13:10:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-63.915750000000003,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2812,"TRANSGRIDV5_20161215152814","2014-01-31T12:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-56.164850000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2826,"TRANSGRIDV5_20161215152814","2014-02-01T15:30:00","#R009821_005_RAMP_F","#R009821_RAMP","2014-02-01",1,-20.90192,"Hard Ramping constraint for constraint N^^V_SMTXH1_1, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","South Morang F1 Transformer 500kV","REGULATED",10,"Ramping Constraint","PLANNED",0]
[2838,"TRANSGRIDV5_20161215152814","2014-02-01T14:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13462.19233,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2843,"TRANSGRIDV5_20161215152814","2014-02-01T14:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-1832.0420200000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2860,"TRANSGRIDV5_20161215152814","2014-02-01T15:05:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-140752.41821999999,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2870,"TRANSGRIDV5_20161215152814","2014-02-01T14:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-73374.879660000006,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2875,"TRANSGRIDV5_20161215152814","2014-02-01T12:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-2714.6449400000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2887,"TRANSGRIDV5_20161215152814","2014-02-01T13:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-34.504379999999998,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2901,"TRANSGRIDV5_20161215152814","2014-02-01T18:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-18.94753,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2908,"TRANSGRIDV5_20161215152814","2014-02-01T15:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-140918.74337000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2916,"TRANSGRIDV5_20161215152814","2014-02-01T17:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-73545.380569999994,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2935,"TRANSGRIDV5_20161215152814","2014-02-01T13:40:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-124.79573000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2938,"TRANSGRIDV5_20161215152814","2014-02-01T13:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-106.80401000000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2952,"TRANSGRIDV5_20161215152814","2014-02-01T11:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-38.341250000000002,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2964,"TRANSGRIDV5_20161215152814","2014-02-01T16:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-2359.04144,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2974,"TRANSGRIDV5_20161215152814","2014-02-01T14:55:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-151.00837999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2985,"TRANSGRIDV5_20161215152814","2014-02-01T17:40:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-56.90166,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[2996,"TRANSGRIDV5_20161215152814","2014-02-01T18:20:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-01-31",1,-49.422730000000001,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3002,"TRANSGRIDV5_20161215152814","2014-02-02T17:50:00","CA_SPS_42008454_01","CA_SPS_42008454","2014-02-02",1,-1194.6591100000001,"Constraint Automation, O/L DDTS_WOTS_330 @DDTS for CTG LXPE on trip of LOWER TUMUT-WAGGA 051 330KV LINE.  Generated by STNET[NORFL] Host NOREEMP3(SP)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3011,"TRANSGRIDV5_20161215152814","2014-02-02T12:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-32464.87802,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3029,"TRANSGRIDV5_20161215152814","2014-02-02T17:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-208.75592,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3037,"TRANSGRIDV5_20161215152814","2014-02-02T16:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-197.25385,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3050,"TRANSGRIDV5_20161215152814","2014-02-02T15:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-101.72269,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3052,"TRANSGRIDV5_20161215152814","2014-02-02T18:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-94.575370000000007,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3067,"TRANSGRIDV5_20161215152814","2014-02-02T19:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-22.27957,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3074,"TRANSGRIDV5_20161215152814","2014-02-02T18:10:00","N^^V_NIL_2","V-NIL","2013-08-21",1,-28.468299999999999,"Out = Nil, avoid voltage collapse for loss of a Dederang to Murray 330kV line ","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3084,"TRANSGRIDV5_20161215152814","2014-02-02T12:30:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-177067.09815000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3100,"TRANSGRIDV5_20161215152814","2014-02-02T11:20:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-101.29246000000001,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3111,"TRANSGRIDV5_20161215152814","2014-02-02T18:35:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-109.06444,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3115,"TRANSGRIDV5_20161215152814","2014-02-02T19:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-26.644449999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3132,"TRANSGRIDV5_20161215152814","2014-02-02T11:05:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-665.65106000000003,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3141,"TRANSGRIDV5_20161215152814","2014-02-02T11:10:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-90.322109999999995,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3149,"TRANSGRIDV5_20161215152814","2014-02-02T09:15:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-63.524079999999998,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3167,"TRANSGRIDV5_20161215152814","2014-02-02T08:25:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-01-31",1,-20.83961,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3173,"TRANSGRIDV5_20161215152814","2014-02-02T13:15:00","V>>SML_NIL_1_5M","V-NIL","2014-01-31",1,-277812.58191000001,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3182,"TRANSGRIDV5_20161215152814","2014-02-02T12:55:00","V>>SML_NIL_1_5M","V-NIL","2014-01-31",1,-147.50914,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 5 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3199,"TRANSGRIDV5_20161215152814","2014-02-02T20:30:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-17.172370000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3209,"TRANSGRIDV5_20161215152814","2014-02-03T12:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-248.72566,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3210,"TRANSGRIDV5_20161215152814","2014-02-03T13:35:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-228.73362,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3226,"TRANSGRIDV5_20161215152814","2014-02-03T17:15:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-73.56429,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3236,"TRANSGRIDV5_20161215152814","2014-02-03T02:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.3505,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3243,"TRANSGRIDV5_20161215152814","2014-02-03T12:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-284.25545,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3262,"TRANSGRIDV5_20161215152814","2014-02-03T11:45:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-22.05247,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3264,"TRANSGRIDV5_20161215152814","2014-02-03T10:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-17.91328,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3277,"TRANSGRIDV5_20161215152814","2014-02-05T16:10:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-11.18843,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3291,"TRANSGRIDV5_20161215152814","2014-02-05T18:55:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-38.29007,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3299,"TRANSGRIDV5_20161215152814","2014-02-05T18:15:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-36.48742,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3308,"TRANSGRIDV5_20161215152814","2014-02-05T19:25:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-24.175650000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3325,"TRANSGRIDV5_20161215152814","2014-02-06T15:40:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-49.073099999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3335,"TRANSGRIDV5_20161215152814","2014-02-06T20:15:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-16.006,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3340,"TRANSGRIDV5_20161215152814","2014-02-06T20:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.61429,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3356,"TRANSGRIDV5_20161215152814","2014-02-06T16:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-11.286199999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3366,"TRANSGRIDV5_20161215152814","2014-02-07T10:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-43.003189999999996,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3372,"TRANSGRIDV5_20161215152814","2014-02-07T15:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-31.946380000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3385,"TRANSGRIDV5_20161215152814","2014-02-07T12:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-17.317329999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3398,"TRANSGRIDV5_20161215152814","2014-02-07T16:10:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.007440000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3406,"TRANSGRIDV5_20161215152814","2014-02-07T13:00:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-02-03",1,-10.92048,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3413,"TRANSGRIDV5_20161215152814","2014-02-08T17:35:00","CA_MQS_42084A52_01","CA_MQS_42084A52","2014-02-08",1,-18.701609999999999,"Constraint Automation, O/L ROBNWB_1      @R_TOWN for CTG LS5K on trip of R_TOWN-N_W_B132KV 2LN VIA1 2&3MWPS.  Generated by STNET[MANFR] Host MANEEMP1(MQ)","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3423,"TRANSGRIDV5_20161215152814","2014-02-08T18:25:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-257.16287999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3435,"TRANSGRIDV5_20161215152814","2014-02-08T16:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-38.157940000000004,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3450,"TRANSGRIDV5_20161215152814","2014-02-08T15:50:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-29.993449999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3461,"TRANSGRIDV5_20161215152814","2014-02-08T14:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-4452.4667200000004,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3467,"TRANSGRIDV5_20161215152814","2014-02-08T18:50:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-38.319029999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3476,"TRANSGRIDV5_20161215152814","2014-02-08T18:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-25.69238,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3488,"TRANSGRIDV5_20161215152814","2014-02-08T15:35:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2014-02-03",1,-177120.57506999999,"Out = Nil, avoid O/L Ballarat to Moorabool No.1 220 kV line for loss of Ballarat to Elaine To Moorabool 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3502,"TRANSGRIDV5_20161215152814","2014-02-08T12:50:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-60.026949999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3505,"TRANSGRIDV5_20161215152814","2014-02-08T13:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-55.090989999999998,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3517,"TRANSGRIDV5_20161215152814","2014-02-08T13:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-30.094989999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3532,"TRANSGRIDV5_20161215152814","2014-02-09T23:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-23.28679,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3539,"TRANSGRIDV5_20161215152814","2014-02-09T12:50:00","S>V_NIL_NIL_RBNW","S-NIL","2011-01-27",2,-92.86788,"Out = Nil, avoid overloading North West Bend to Robertstown 132kV line for no contingencies","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3549,"TRANSGRIDV5_20161215152814","2014-02-09T12:35:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-99.591449999999995,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3565,"TRANSGRIDV5_20161215152814","2014-02-10T17:20:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-19.40645,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3571,"TRANSGRIDV5_20161215152814","2014-02-11T19:05:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-109.71210000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3582,"TRANSGRIDV5_20161215152814","2014-02-11T20:00:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-98.790459999999996,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3597,"TRANSGRIDV5_20161215152814","2014-02-12T13:05:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-59.00244,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3609,"TRANSGRIDV5_20161215152814","2014-02-12T12:30:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-48.801470000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3612,"TRANSGRIDV5_20161215152814","2014-02-12T13:25:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-38.777340000000002,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3630,"TRANSGRIDV5_20161215152814","2014-02-12T17:45:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-26.69538,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3638,"TRANSGRIDV5_20161215152814","2014-02-12T16:00:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-245.22696999999999,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3647,"TRANSGRIDV5_20161215152814","2014-02-12T15:15:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-59.100320000000004,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3660,"TRANSGRIDV5_20161215152814","2014-02-12T15:25:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-53.359650000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3664,"TRANSGRIDV5_20161215152814","2014-02-12T15:30:00","V>>SML_NIL_8","V-NIL_BATS_BETS_15M","2014-02-03",1,-48.896430000000002,"Out = Nil, avoid O/L Ballarat to Bendigo 220 kV line (flow North) for loss of Shepparton to Bendigo 220 kV line, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3675,"TRANSGRIDV5_20161215152814","2014-02-13T17:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-9707.74395,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3691,"TRANSGRIDV5_20161215152814","2014-02-13T16:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-30.892230000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3701,"TRANSGRIDV5_20161215152814","2014-02-13T17:05:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-84.065950000000001,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3712,"TRANSGRIDV5_20161215152814","2014-02-13T16:35:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-20.972760000000001,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3716,"TRANSGRIDV5_20161215152814","2014-02-13T16:45:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-12.31415,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3729,"TRANSGRIDV5_20161215152814","2014-02-16T19:00:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-4765.7689899999996,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3742,"TRANSGRIDV5_20161215152814","2014-02-17T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.804559999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3748,"TRANSGRIDV5_20161215152814","2014-02-17T17:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-3758.6576599999999,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3762,"TRANSGRIDV5_20161215152814","2014-02-19T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10730.357120000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3774,"TRANSGRIDV5_20161215152814","2014-02-20T11:50:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-26.08709,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED",null,"PLANNED",1]
[3779,"TRANSGRIDV5_20161215152814","2014-02-20T22:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.599080000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3796,"TRANSGRIDV5_20161215152814","2014-02-21T09:30:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-12300.532639999999,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED",null,"PLANNED",1]
[3806,"TRANSGRIDV5_20161215152814","2014-02-21T13:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-4620.4211299999997,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3811,"TRANSGRIDV5_20161215152814","2014-02-21T16:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-119.58622,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3823,"TRANSGRIDV5_20161215152814","2014-02-23T09:30:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2013-08-21",1,13052.91,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3837,"TRANSGRIDV5_20161215152814","2014-02-26T17:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-13.069509999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3844,"TRANSGRIDV5_20161215152814","2014-03-08T02:30:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-24.438829999999999,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[3852,"TRANSGRIDV5_20161215152814","2014-03-08T03:50:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-16.884840000000001,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[3871,"TRANSGRIDV5_20161215152814","2014-03-11T12:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2013-08-21",1,13035.255010000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3874,"TRANSGRIDV5_20161215152814","2014-03-11T11:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2013-08-21",1,13033.567870000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3888,"TRANSGRIDV5_20161215152814","2014-03-15T12:35:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-13.58474,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[3900,"TRANSGRIDV5_20161215152814","2014-03-18T18:00:00","#R010022_003_RAMP_F","#R010022_RAMP","2014-03-18",1,-68.129519999999999,"Hard Ramping constraint for constraint N^Q_AR_330_BS5_1, Effective Date: 10/03/2014, Version: 1","OUTAGE","RAMP","Armidale No.5 Bus Section 330kV","REGULATED",10,"Ramping Constraint","PLANNED",0]
[3905,"TRANSGRIDV5_20161215152814","2014-03-18T05:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.96997,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[3915,"TRANSGRIDV5_20161215152814","2014-03-19T03:15:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13057.545910000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3926,"TRANSGRIDV5_20161215152814","2014-03-19T04:10:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13054.96587,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3941,"TRANSGRIDV5_20161215152814","2014-03-19T21:50:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13052.91,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3947,"TRANSGRIDV5_20161215152814","2014-03-19T21:30:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13052.54845,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3965,"TRANSGRIDV5_20161215152814","2014-03-19T05:10:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13050.5735,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3973,"TRANSGRIDV5_20161215152814","2014-03-19T20:20:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13049.05092,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3986,"TRANSGRIDV5_20161215152814","2014-03-19T09:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13046.57012,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[3999,"TRANSGRIDV5_20161215152814","2014-03-19T08:55:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13045.14803,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4003,"TRANSGRIDV5_20161215152814","2014-03-19T17:10:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13044.85385,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4010,"TRANSGRIDV5_20161215152814","2014-03-19T07:20:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13044.31328,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4030,"TRANSGRIDV5_20161215152814","2014-03-19T05:55:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13042.85,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4036,"TRANSGRIDV5_20161215152814","2014-03-19T17:20:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13042.85,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4047,"TRANSGRIDV5_20161215152814","2014-03-19T14:05:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13042.551939999999,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4062,"TRANSGRIDV5_20161215152814","2014-03-19T15:05:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13041.88437,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4068,"TRANSGRIDV5_20161215152814","2014-03-19T15:15:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13041.64797,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4077,"TRANSGRIDV5_20161215152814","2014-03-19T10:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13041.41149,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4085,"TRANSGRIDV5_20161215152814","2014-03-19T12:25:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13040.94061,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4103,"TRANSGRIDV5_20161215152814","2014-03-19T16:20:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13039.919029999999,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4112,"TRANSGRIDV5_20161215152814","2014-03-19T13:15:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13039.6705,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4125,"TRANSGRIDV5_20161215152814","2014-03-19T13:35:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13039.130590000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4129,"TRANSGRIDV5_20161215152814","2014-03-19T11:00:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13038.948340000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4140,"TRANSGRIDV5_20161215152814","2014-03-19T13:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-03-19",1,13037.85,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4157,"TRANSGRIDV5_20161215152814","2014-03-21T04:55:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-03-21",1,18.979330000000001,"NSW1-QLD1 >= MIN(-200, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[4162,"TRANSGRIDV5_20161215152814","2014-03-21T04:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-15.714980000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4172,"TRANSGRIDV5_20161215152814","2014-03-22T05:45:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-03-22",1,14.6258,"NSW1-QLD1 >= MIN(-171, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[4179,"TRANSGRIDV5_20161215152814","2014-03-24T07:00:00","N^^V_MSDD1","V-DDMS","2013-08-21",1,-87.767200000000003,"Out = Murray to Dederang No. 1 or No. 2 330 kV line, avoid voltage collapse for trip of the largest Vic generating unit or Basslink","OUTAGE","OTHER","Murray - Dederang 67 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[4198,"TRANSGRIDV5_20161215152814","2014-03-28T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.450740000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4200,"TRANSGRIDV5_20161215152814","2014-03-28T07:00:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-209.97657000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4213,"TRANSGRIDV5_20161215152814","2014-03-28T07:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-10.95251,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4227,"TRANSGRIDV5_20161215152814","2014-03-29T18:25:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-13.85439,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4235,"TRANSGRIDV5_20161215152814","2014-03-31T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.729039999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4244,"TRANSGRIDV5_20161215152814","2014-03-31T16:15:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-11.586550000000001,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4261,"TRANSGRIDV5_20161215152814","2014-04-11T09:20:00","NSA_V_BDL01_30","NSA-V_BDL01_30","2013-08-21",1,391950.94803000003,"Bairnsdale Unit 1 >= 30 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4271,"TRANSGRIDV5_20161215152814","2014-04-21T13:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-41.908340000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4276,"TRANSGRIDV5_20161215152814","2014-04-21T14:25:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-17.583580000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4292,"TRANSGRIDV5_20161215152814","2014-04-21T14:15:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-17.22231,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4302,"TRANSGRIDV5_20161215152814","2014-04-22T02:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-16.075970000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4309,"TRANSGRIDV5_20161215152814","2014-04-22T02:10:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-16.302230000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4317,"TRANSGRIDV5_20161215152814","2014-04-23T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.480250000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4326,"TRANSGRIDV5_20161215152814","2014-04-24T16:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.979950000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4339,"TRANSGRIDV5_20161215152814","2014-04-24T03:25:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-22.285889999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4349,"TRANSGRIDV5_20161215152814","2014-04-24T03:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-23.40804,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4359,"TRANSGRIDV5_20161215152814","2014-04-25T14:35:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-38.608980000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4371,"TRANSGRIDV5_20161215152814","2014-04-29T17:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-115.27983999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4386,"TRANSGRIDV5_20161215152814","2014-04-29T13:40:00","N^Q_TW_330_BUS3_1","N-TW_330_BUS3","2014-03-10",1,-12.10238,"Out= Tamworth No.3 330kV bus, NSW to Qld voltage stability limit for trip of the largest Qld generator","OUTAGE","OTHER","Tamworth330 Bus Section No.3 330kV","REGULATED","INCLUDED",null,"PLANNED",1]
[4397,"TRANSGRIDV5_20161215152814","2014-05-01T08:00:00","#R010344_002_RAMP_F","#R010344_RAMP","2014-04-30",1,-10.034700000000001,"Hard Ramping constraint for constraint N>N-LSTN_TE_C1, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Lismore330 - Tenterfield 96L Line 132kV","REGULATED",10,"Ramping Constraint","PLANNED",0]
[4403,"TRANSGRIDV5_20161215152814","2014-05-01T17:55:00","N>N-LS_TX_TE_B","N-LS_TX","2013-08-21",1,-432.54892999999998,"Out= Lismore No.1 or No.2 330/132 Transformer, avoid O/L Koolkhan to Lismore (967) on trip of remaining Lismore 330/132kV transformer, Feedback. DS only","OUTAGE","OTHER","Lismore330 No.2 Transformer 330kV","REGULATED","INCLUDED",null,"UNPLANNED",1]
[4412,"TRANSGRIDV5_20161215152814","2014-05-03T04:15:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-64.307050000000004,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4424,"TRANSGRIDV5_20161215152814","2014-05-06T08:30:00","NSA_Q_GSTONE34_400","NSA-Q_GSTONE34_400","2013-08-21",1,13041.99483,"Gladstone 3 + 4 >= 400 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4438,"TRANSGRIDV5_20161215152814","2014-05-09T06:15:00","S>V_NIL_NIL_RBNW","S-NIL","2014-02-11",1,-34.546120000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4451,"TRANSGRIDV5_20161215152814","2014-05-13T08:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-13.94927,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4460,"TRANSGRIDV5_20161215152814","2014-05-13T23:25:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,15.68088,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4468,"TRANSGRIDV5_20161215152814","2014-05-13T12:40:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,13.42014,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4475,"TRANSGRIDV5_20161215152814","2014-05-13T23:45:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,10.42009,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4485,"TRANSGRIDV5_20161215152814","2014-05-14T23:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-31.918209999999998,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4501,"TRANSGRIDV5_20161215152814","2014-05-14T15:35:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-14.74982,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4506,"TRANSGRIDV5_20161215152814","2014-05-14T22:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-12.02955,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4516,"TRANSGRIDV5_20161215152814","2014-05-14T02:35:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,17.258579999999998,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4533,"TRANSGRIDV5_20161215152814","2014-05-14T02:45:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,16.824000000000002,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4545,"TRANSGRIDV5_20161215152814","2014-05-14T02:15:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,15.8437,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4548,"TRANSGRIDV5_20161215152814","2014-05-14T01:25:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,15.24616,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4566,"TRANSGRIDV5_20161215152814","2014-05-14T01:05:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,10.470750000000001,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4574,"TRANSGRIDV5_20161215152814","2014-05-15T18:20:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-177.68513999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4583,"TRANSGRIDV5_20161215152814","2014-05-15T09:45:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-16.393239999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4596,"TRANSGRIDV5_20161215152814","2014-05-21T16:30:00","N^^V_NIL_1","V-NIL","2013-08-21",1,-82.545699999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4600,"TRANSGRIDV5_20161215152814","2014-05-21T03:20:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,13.736179999999999,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4611,"TRANSGRIDV5_20161215152814","2014-05-21T03:10:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,13.17953,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4627,"TRANSGRIDV5_20161215152814","2014-05-21T04:35:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,11.41155,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4637,"TRANSGRIDV5_20161215152814","2014-05-21T04:55:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,10.47174,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4648,"TRANSGRIDV5_20161215152814","2014-05-22T09:00:00","CA_SPS_428FB629_01","CA_SPS_428FB629","2014-05-22",1,-231556.78547999999,"Constraint Automation, O/L 94E           @MT_PIPER for CTG LNWT on trip of MT_PIPER-WWANG 70 330KV LINE.  Generated by STNET[NORFL] Host NOREEMP4(SP)","OUTAGE","OTHER","Mount Piper 330 - Wallerwang 330 71 330kV Line","REGULATED","8(B)","Constraint applied by AEMO doesn't accurately reflect network capability advised by the TNSP","PLANNED",0,"Incorrect constraint formulation of prior constraint N>>N-MPWW_ONE_9 led to price spike causing the penalty with this automated constraint"]
[4652,"TRANSGRIDV5_20161215152814","2014-05-23T06:20:00","#R010528_008_RAMP_F","#R010528_RAMP","2014-05-23",1,-10.143509999999999,"Hard Ramping constraint for constraint V::N_ROSMVB_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Rowville - South Morang 500kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[4665,"TRANSGRIDV5_20161215152814","2014-05-27T07:25:00","#R010552_001_RAMP_V","#R010552_RAMP","2014-05-26",1,-13.016769999999999,"Soft Ramping constraint for constraint N^N-967_LS_SVC, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Lismore No.1 SVC 132kV","REGULATED",10,"Ramping Constraint","PLANNED",0]
[4678,"TRANSGRIDV5_20161215152814","2014-06-03T11:50:00","N^^V_EPMB_1","V-EPMB","2013-08-21",1,-13.839919999999999,"Out = Eildon to Mt Beauty 220 kV line, avoid voltage collapse for trip of the largest Vic generating unit of Basslink","OUTAGE","OTHER","Eildon - Mount Beauty 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[4692,"TRANSGRIDV5_20161215152814","2014-06-03T23:45:00","N^^V_NIL_1","V-NIL","2014-05-28",1,-45.947839999999999,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4700,"TRANSGRIDV5_20161215152814","2014-06-03T09:40:00","N^^V_NIL_1","V-NIL","2014-05-28",1,-11.65667,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4709,"TRANSGRIDV5_20161215152814","2014-06-04T07:45:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-252.49071000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4715,"TRANSGRIDV5_20161215152814","2014-06-04T23:15:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-191.27289999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4732,"TRANSGRIDV5_20161215152814","2014-06-04T22:40:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-88.799700000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4742,"TRANSGRIDV5_20161215152814","2014-06-04T12:10:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-37.42286,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4747,"TRANSGRIDV5_20161215152814","2014-06-04T11:15:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-34.822069999999997,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4759,"TRANSGRIDV5_20161215152814","2014-06-04T15:35:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-17.00553,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4773,"TRANSGRIDV5_20161215152814","2014-06-04T12:40:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-11.423870000000001,"Out = Nil, avoid voltage collapse for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4780,"TRANSGRIDV5_20161215152814","2014-06-04T11:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.2475,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4799,"TRANSGRIDV5_20161215152814","2014-06-05T00:05:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-86.875929999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4807,"TRANSGRIDV5_20161215152814","2014-06-05T13:25:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-84.826679999999996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4810,"TRANSGRIDV5_20161215152814","2014-06-05T13:40:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-84.653310000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4824,"TRANSGRIDV5_20161215152814","2014-06-05T15:05:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-40.663609999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4836,"TRANSGRIDV5_20161215152814","2014-06-05T12:10:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-30.584,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4851,"TRANSGRIDV5_20161215152814","2014-06-05T12:25:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-16.10285,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4862,"TRANSGRIDV5_20161215152814","2014-06-05T03:20:00","Q:N_AR_2L-G_-150","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.790430000000001,"Nominated Offset -150MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4872,"TRANSGRIDV5_20161215152814","2014-06-08T03:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.18178,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4877,"TRANSGRIDV5_20161215152814","2014-06-08T05:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.432499999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4889,"TRANSGRIDV5_20161215152814","2014-06-11T16:30:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-39.357590000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4903,"TRANSGRIDV5_20161215152814","2014-06-15T12:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.106529999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4906,"TRANSGRIDV5_20161215152814","2014-06-15T10:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.756769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4925,"TRANSGRIDV5_20161215152814","2014-06-15T13:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.52599,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4935,"TRANSGRIDV5_20161215152814","2014-06-15T11:15:00","Q:N_AR_2L-G_-150","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.94739,"Nominated Offset -150MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4939,"TRANSGRIDV5_20161215152814","2014-06-15T10:45:00","Q:N_AR_2L-G_-150","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.992710000000001,"Nominated Offset -150MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4957,"TRANSGRIDV5_20161215152814","2014-06-17T04:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.11899,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4966,"TRANSGRIDV5_20161215152814","2014-06-18T07:25:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-11.989549999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,"REGULATED",null,null,null,0]
[4972,"TRANSGRIDV5_20161215152814","2014-06-20T17:55:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-89.54025,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[4983,"TRANSGRIDV5_20161215152814","2014-06-22T19:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.531180000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[4998,"TRANSGRIDV5_20161215152814","2014-06-23T23:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.634930000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5004,"TRANSGRIDV5_20161215152814","2014-06-23T01:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.740320000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5013,"TRANSGRIDV5_20161215152814","2014-06-23T02:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.348280000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5021,"TRANSGRIDV5_20161215152814","2014-06-23T02:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.24553,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5039,"TRANSGRIDV5_20161215152814","2014-06-23T03:05:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-11.2174,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[5048,"TRANSGRIDV5_20161215152814","2014-06-27T05:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.928319999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[5061,"TRANSGRIDV5_20161215152814","2014-06-28T13:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.504239999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5065,"TRANSGRIDV5_20161215152814","2014-06-28T14:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.504239999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5076,"TRANSGRIDV5_20161215152814","2014-06-28T13:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.850669999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5086,"TRANSGRIDV5_20161215152814","2014-06-28T02:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-16.068660000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[5102,"TRANSGRIDV5_20161215152814","2014-06-29T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.15033,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5113,"TRANSGRIDV5_20161215152814","2014-06-29T09:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.632110000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5117,"TRANSGRIDV5_20161215152814","2014-06-29T09:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.632009999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5134,"TRANSGRIDV5_20161215152814","2014-06-30T04:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.47147,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5146,"TRANSGRIDV5_20161215152814","2014-06-30T03:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.81331,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5149,"TRANSGRIDV5_20161215152814","2014-06-30T03:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.35427,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5163,"TRANSGRIDV5_20161215152814","2014-07-01T11:20:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-07-01",1,17.011579999999999,"NSW1-QLD1 >= MIN(-304, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[5171,"TRANSGRIDV5_20161215152814","2014-07-01T17:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.24,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5180,"TRANSGRIDV5_20161215152814","2014-07-01T22:25:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.05,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5197,"TRANSGRIDV5_20161215152814","2014-07-01T17:05:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,13.62992,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5207,"TRANSGRIDV5_20161215152814","2014-07-01T23:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,274.42631999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5212,"TRANSGRIDV5_20161215152814","2014-07-01T20:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,67.770030000000006,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5228,"TRANSGRIDV5_20161215152814","2014-07-01T19:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,21.8842,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5238,"TRANSGRIDV5_20161215152814","2014-07-01T20:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.9848,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5245,"TRANSGRIDV5_20161215152814","2014-07-01T20:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-86.096130000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5253,"TRANSGRIDV5_20161215152814","2014-07-01T21:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-73.032409999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5272,"TRANSGRIDV5_20161215152814","2014-07-01T22:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-33.991720000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5275,"TRANSGRIDV5_20161215152814","2014-07-01T11:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-33.022120000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5289,"TRANSGRIDV5_20161215152814","2014-07-01T14:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.708279999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5301,"TRANSGRIDV5_20161215152814","2014-07-01T23:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.605080000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5307,"TRANSGRIDV5_20161215152814","2014-07-01T11:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-24.077279999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5322,"TRANSGRIDV5_20161215152814","2014-07-01T13:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.225519999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5333,"TRANSGRIDV5_20161215152814","2014-07-01T14:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.419180000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5339,"TRANSGRIDV5_20161215152814","2014-07-01T12:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.905270000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5348,"TRANSGRIDV5_20161215152814","2014-07-01T20:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.515979999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5360,"TRANSGRIDV5_20161215152814","2014-07-01T08:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.01689,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5374,"TRANSGRIDV5_20161215152814","2014-07-01T11:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.72841,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5387,"TRANSGRIDV5_20161215152814","2014-07-01T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.27009,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5396,"TRANSGRIDV5_20161215152814","2014-07-02T17:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,21.44651,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5404,"TRANSGRIDV5_20161215152814","2014-07-02T02:50:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.03,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5411,"TRANSGRIDV5_20161215152814","2014-07-02T04:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5421,"TRANSGRIDV5_20161215152814","2014-07-02T09:25:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,11.901529999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5437,"TRANSGRIDV5_20161215152814","2014-07-02T03:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5442,"TRANSGRIDV5_20161215152814","2014-07-02T10:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5452,"TRANSGRIDV5_20161215152814","2014-07-02T04:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.93146,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5469,"TRANSGRIDV5_20161215152814","2014-07-02T04:15:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,15.43,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5478,"TRANSGRIDV5_20161215152814","2014-07-02T23:35:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,12,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5486,"TRANSGRIDV5_20161215152814","2014-07-02T03:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-52.38955,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5500,"TRANSGRIDV5_20161215152814","2014-07-02T14:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-36.981520000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5510,"TRANSGRIDV5_20161215152814","2014-07-02T17:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-31.609020000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5519,"TRANSGRIDV5_20161215152814","2014-07-02T22:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-28.651409999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5532,"TRANSGRIDV5_20161215152814","2014-07-02T10:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.512280000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5546,"TRANSGRIDV5_20161215152814","2014-07-02T11:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.750610000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5547,"TRANSGRIDV5_20161215152814","2014-07-02T22:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.73762,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5563,"TRANSGRIDV5_20161215152814","2014-07-02T23:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.635670000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5573,"TRANSGRIDV5_20161215152814","2014-07-02T11:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.573879999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5584,"TRANSGRIDV5_20161215152814","2014-07-02T13:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.311769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5599,"TRANSGRIDV5_20161215152814","2014-07-02T04:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.41544,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5601,"TRANSGRIDV5_20161215152814","2014-07-02T04:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.3477,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5614,"TRANSGRIDV5_20161215152814","2014-07-02T02:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.12114,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5628,"TRANSGRIDV5_20161215152814","2014-07-02T04:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.505510000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5636,"TRANSGRIDV5_20161215152814","2014-07-02T23:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.622769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5645,"TRANSGRIDV5_20161215152814","2014-07-02T00:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.725359999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5662,"TRANSGRIDV5_20161215152814","2014-07-02T17:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.87086,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5666,"TRANSGRIDV5_20161215152814","2014-07-02T02:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.47331,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5677,"TRANSGRIDV5_20161215152814","2014-07-02T21:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.10891,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5693,"TRANSGRIDV5_20161215152814","2014-07-02T15:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.57075,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5703,"TRANSGRIDV5_20161215152814","2014-07-03T13:40:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,21.194089999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5709,"TRANSGRIDV5_20161215152814","2014-07-03T20:05:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.07,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5716,"TRANSGRIDV5_20161215152814","2014-07-03T19:55:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,14.53486,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5735,"TRANSGRIDV5_20161215152814","2014-07-03T22:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.151949999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5743,"TRANSGRIDV5_20161215152814","2014-07-03T13:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,21.684090000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5757,"TRANSGRIDV5_20161215152814","2014-07-03T15:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.835529999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5760,"TRANSGRIDV5_20161215152814","2014-07-03T16:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.678349999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5772,"TRANSGRIDV5_20161215152814","2014-07-03T13:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.756119999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5787,"TRANSGRIDV5_20161215152814","2014-07-03T12:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.16508,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5798,"TRANSGRIDV5_20161215152814","2014-07-03T10:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.22481,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[5808,"TRANSGRIDV5_20161215152814","2014-07-03T19:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-106.02762,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5813,"TRANSGRIDV5_20161215152814","2014-07-03T20:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-52.917409999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5825,"TRANSGRIDV5_20161215152814","2014-07-03T14:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.111469999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5839,"TRANSGRIDV5_20161215152814","2014-07-03T20:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-29.164560000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5842,"TRANSGRIDV5_20161215152814","2014-07-03T21:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-28.46491,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5861,"TRANSGRIDV5_20161215152814","2014-07-03T17:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-27.749870000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5869,"TRANSGRIDV5_20161215152814","2014-07-03T20:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.90653,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5876,"TRANSGRIDV5_20161215152814","2014-07-03T02:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.08878,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5890,"TRANSGRIDV5_20161215152814","2014-07-03T21:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.917680000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5902,"TRANSGRIDV5_20161215152814","2014-07-03T22:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.498069999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5908,"TRANSGRIDV5_20161215152814","2014-07-03T14:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.397079999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5919,"TRANSGRIDV5_20161215152814","2014-07-03T14:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.89293,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5934,"TRANSGRIDV5_20161215152814","2014-07-03T15:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.486750000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5940,"TRANSGRIDV5_20161215152814","2014-07-03T15:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.419049999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5949,"TRANSGRIDV5_20161215152814","2014-07-03T02:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.321110000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5967,"TRANSGRIDV5_20161215152814","2014-07-03T03:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.41544,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5975,"TRANSGRIDV5_20161215152814","2014-07-03T00:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.75507,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5984,"TRANSGRIDV5_20161215152814","2014-07-03T00:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.622769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[5997,"TRANSGRIDV5_20161215152814","2014-07-03T01:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.55979,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6001,"TRANSGRIDV5_20161215152814","2014-07-03T08:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.19969,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6012,"TRANSGRIDV5_20161215152814","2014-07-03T08:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.539940000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6022,"TRANSGRIDV5_20161215152814","2014-07-03T00:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.891529999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6038,"TRANSGRIDV5_20161215152814","2014-07-03T17:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.1195,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6049,"TRANSGRIDV5_20161215152814","2014-07-03T16:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.70567,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6053,"TRANSGRIDV5_20161215152814","2014-07-03T17:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.22654,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6066,"TRANSGRIDV5_20161215152814","2014-07-03T23:05:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-16.133610000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6075,"TRANSGRIDV5_20161215152814","2014-07-04T22:05:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,22.926839999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6085,"TRANSGRIDV5_20161215152814","2014-07-04T09:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.057359999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6099,"TRANSGRIDV5_20161215152814","2014-07-04T06:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,13.05983,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6107,"TRANSGRIDV5_20161215152814","2014-07-04T12:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.02112,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6116,"TRANSGRIDV5_20161215152814","2014-07-04T03:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.01,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6133,"TRANSGRIDV5_20161215152814","2014-07-04T09:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.71918,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6143,"TRANSGRIDV5_20161215152814","2014-07-04T03:55:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,15.35,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6148,"TRANSGRIDV5_20161215152814","2014-07-04T02:40:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,12.819929999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6164,"TRANSGRIDV5_20161215152814","2014-07-04T02:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-36.420909999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6174,"TRANSGRIDV5_20161215152814","2014-07-04T01:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.539290000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6181,"TRANSGRIDV5_20161215152814","2014-07-04T10:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-32.759860000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6189,"TRANSGRIDV5_20161215152814","2014-07-04T10:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-30.472729999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6208,"TRANSGRIDV5_20161215152814","2014-07-04T10:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.40024,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6211,"TRANSGRIDV5_20161215152814","2014-07-04T06:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.13946,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6225,"TRANSGRIDV5_20161215152814","2014-07-04T15:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.187180000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6237,"TRANSGRIDV5_20161215152814","2014-07-04T08:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.711849999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6246,"TRANSGRIDV5_20161215152814","2014-07-04T10:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.42435,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6252,"TRANSGRIDV5_20161215152814","2014-07-04T13:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.290590000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6263,"TRANSGRIDV5_20161215152814","2014-07-04T11:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.78838,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6278,"TRANSGRIDV5_20161215152814","2014-07-04T05:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.768820000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6284,"TRANSGRIDV5_20161215152814","2014-07-04T19:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.69134,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6296,"TRANSGRIDV5_20161215152814","2014-07-04T03:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.449680000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6310,"TRANSGRIDV5_20161215152814","2014-07-04T23:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.00637,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6323,"TRANSGRIDV5_20161215152814","2014-07-04T20:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.50798,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6332,"TRANSGRIDV5_20161215152814","2014-07-04T22:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.989339999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6340,"TRANSGRIDV5_20161215152814","2014-07-04T19:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.54477,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6347,"TRANSGRIDV5_20161215152814","2014-07-04T08:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.05067,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6367,"TRANSGRIDV5_20161215152814","2014-07-04T15:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.622990000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6373,"TRANSGRIDV5_20161215152814","2014-07-04T14:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.272449999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6388,"TRANSGRIDV5_20161215152814","2014-07-04T07:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.94069,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6399,"TRANSGRIDV5_20161215152814","2014-07-04T20:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.699159999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6405,"TRANSGRIDV5_20161215152814","2014-07-04T07:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.57624,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6414,"TRANSGRIDV5_20161215152814","2014-07-04T14:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.31931,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6422,"TRANSGRIDV5_20161215152814","2014-07-04T18:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.66188,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6436,"TRANSGRIDV5_20161215152814","2014-07-04T01:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.59266,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6449,"TRANSGRIDV5_20161215152814","2014-07-04T06:10:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.578060000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6462,"TRANSGRIDV5_20161215152814","2014-07-05T12:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,528.35360000000003,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6470,"TRANSGRIDV5_20161215152814","2014-07-05T12:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,22.772040000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6477,"TRANSGRIDV5_20161215152814","2014-07-05T00:50:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,16.900020000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6494,"TRANSGRIDV5_20161215152814","2014-07-05T22:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.02,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6499,"TRANSGRIDV5_20161215152814","2014-07-05T16:30:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,14.21,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6509,"TRANSGRIDV5_20161215152814","2014-07-05T12:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,13.33966,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6520,"TRANSGRIDV5_20161215152814","2014-07-05T11:05:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.92999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6535,"TRANSGRIDV5_20161215152814","2014-07-05T15:40:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.16511,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6537,"TRANSGRIDV5_20161215152814","2014-07-05T09:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.09013,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6550,"TRANSGRIDV5_20161215152814","2014-07-05T09:50:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,11.335789999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6564,"TRANSGRIDV5_20161215152814","2014-07-05T02:30:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.35844,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6572,"TRANSGRIDV5_20161215152814","2014-07-05T12:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,532.30359999999996,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6581,"TRANSGRIDV5_20161215152814","2014-07-05T10:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,27.304870000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6598,"TRANSGRIDV5_20161215152814","2014-07-05T11:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,18.129370000000002,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6602,"TRANSGRIDV5_20161215152814","2014-07-05T11:05:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.85999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6613,"TRANSGRIDV5_20161215152814","2014-07-05T10:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.21322,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6629,"TRANSGRIDV5_20161215152814","2014-07-05T16:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,16.473199999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6639,"TRANSGRIDV5_20161215152814","2014-07-05T03:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.5,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6646,"TRANSGRIDV5_20161215152814","2014-07-05T07:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.33508,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6661,"TRANSGRIDV5_20161215152814","2014-07-05T11:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.60853,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6663,"TRANSGRIDV5_20161215152814","2014-07-05T03:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.5306,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6676,"TRANSGRIDV5_20161215152814","2014-07-05T14:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,13.37865,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6693,"TRANSGRIDV5_20161215152814","2014-07-05T16:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.914669999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6696,"TRANSGRIDV5_20161215152814","2014-07-05T23:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.855869999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6708,"TRANSGRIDV5_20161215152814","2014-07-05T06:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.723549999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[6723,"TRANSGRIDV5_20161215152814","2014-07-05T12:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-1023.54445,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6734,"TRANSGRIDV5_20161215152814","2014-07-05T11:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-51.814079999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6744,"TRANSGRIDV5_20161215152814","2014-07-05T00:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-37.841990000000003,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6749,"TRANSGRIDV5_20161215152814","2014-07-05T00:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-37.152720000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6761,"TRANSGRIDV5_20161215152814","2014-07-05T12:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.15137,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6775,"TRANSGRIDV5_20161215152814","2014-07-05T12:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-32.2376,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6788,"TRANSGRIDV5_20161215152814","2014-07-05T03:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-31.020949999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6797,"TRANSGRIDV5_20161215152814","2014-07-05T04:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-29.80997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6805,"TRANSGRIDV5_20161215152814","2014-07-05T03:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-28.946750000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6812,"TRANSGRIDV5_20161215152814","2014-07-05T02:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-27.55864,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6826,"TRANSGRIDV5_20161215152814","2014-07-05T22:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-24.3873,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6838,"TRANSGRIDV5_20161215152814","2014-07-05T08:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.981950000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6843,"TRANSGRIDV5_20161215152814","2014-07-05T00:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.971869999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6853,"TRANSGRIDV5_20161215152814","2014-07-05T21:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.00704,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6870,"TRANSGRIDV5_20161215152814","2014-07-05T22:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.59599,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6876,"TRANSGRIDV5_20161215152814","2014-07-05T07:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.546659999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6885,"TRANSGRIDV5_20161215152814","2014-07-05T01:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.15157,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6903,"TRANSGRIDV5_20161215152814","2014-07-05T16:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.66893,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6907,"TRANSGRIDV5_20161215152814","2014-07-05T02:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.357790000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6920,"TRANSGRIDV5_20161215152814","2014-07-05T14:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.526029999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6933,"TRANSGRIDV5_20161215152814","2014-07-05T15:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.72566,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6937,"TRANSGRIDV5_20161215152814","2014-07-05T13:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.36908,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6948,"TRANSGRIDV5_20161215152814","2014-07-05T21:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.71064,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6958,"TRANSGRIDV5_20161215152814","2014-07-05T08:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.8254,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[6974,"TRANSGRIDV5_20161215152814","2014-07-05T06:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-65.403869999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6985,"TRANSGRIDV5_20161215152814","2014-07-05T19:35:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-12.30697,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[6989,"TRANSGRIDV5_20161215152814","2014-07-06T11:20:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,23.590050000000002,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7002,"TRANSGRIDV5_20161215152814","2014-07-06T09:55:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,14.45045,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7011,"TRANSGRIDV5_20161215152814","2014-07-06T13:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,14.13631,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7029,"TRANSGRIDV5_20161215152814","2014-07-06T12:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.83568,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7037,"TRANSGRIDV5_20161215152814","2014-07-06T02:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.373900000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7050,"TRANSGRIDV5_20161215152814","2014-07-06T10:50:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.52997,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7052,"TRANSGRIDV5_20161215152814","2014-07-06T15:05:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.349299999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7069,"TRANSGRIDV5_20161215152814","2014-07-06T12:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,16.15474,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7079,"TRANSGRIDV5_20161215152814","2014-07-06T14:05:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.46565,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7084,"TRANSGRIDV5_20161215152814","2014-07-06T03:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.064260000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7100,"TRANSGRIDV5_20161215152814","2014-07-06T12:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,13.06799,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7110,"TRANSGRIDV5_20161215152814","2014-07-06T15:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.53387,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7117,"TRANSGRIDV5_20161215152814","2014-07-06T07:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.9649,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7136,"TRANSGRIDV5_20161215152814","2014-07-06T10:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.0046,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink outage of line 8M"]
[7144,"TRANSGRIDV5_20161215152814","2014-07-06T14:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-35.03969,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7147,"TRANSGRIDV5_20161215152814","2014-07-06T11:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-34.91527,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7161,"TRANSGRIDV5_20161215152814","2014-07-06T10:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-32.464480000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7173,"TRANSGRIDV5_20161215152814","2014-07-06T09:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-31.512930000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7182,"TRANSGRIDV5_20161215152814","2014-07-06T00:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-29.460180000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7199,"TRANSGRIDV5_20161215152814","2014-07-06T15:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-25.18648,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7209,"TRANSGRIDV5_20161215152814","2014-07-06T01:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.619150000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7214,"TRANSGRIDV5_20161215152814","2014-07-06T13:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.507850000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7226,"TRANSGRIDV5_20161215152814","2014-07-06T15:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.50751,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7236,"TRANSGRIDV5_20161215152814","2014-07-06T09:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.101980000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7243,"TRANSGRIDV5_20161215152814","2014-07-06T00:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.861260000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7262,"TRANSGRIDV5_20161215152814","2014-07-06T07:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.031179999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7268,"TRANSGRIDV5_20161215152814","2014-07-06T07:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.731179999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7276,"TRANSGRIDV5_20161215152814","2014-07-06T07:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.502549999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7294,"TRANSGRIDV5_20161215152814","2014-07-06T04:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.266400000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7303,"TRANSGRIDV5_20161215152814","2014-07-07T15:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.32663,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7309,"TRANSGRIDV5_20161215152814","2014-07-07T13:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.28825,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7324,"TRANSGRIDV5_20161215152814","2014-07-07T13:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.52918,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7335,"TRANSGRIDV5_20161215152814","2014-07-07T12:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.099399999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7341,"TRANSGRIDV5_20161215152814","2014-07-07T23:30:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.77445,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[7350,"TRANSGRIDV5_20161215152814","2014-07-07T22:45:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.124689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,null,null,0]
[7358,"TRANSGRIDV5_20161215152814","2014-07-08T09:15:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1052.97298,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7372,"TRANSGRIDV5_20161215152814","2014-07-08T08:35:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1052.5216499999999,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7385,"TRANSGRIDV5_20161215152814","2014-07-08T14:50:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1049.72298,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7398,"TRANSGRIDV5_20161215152814","2014-07-08T09:55:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1049.7226800000001,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7406,"TRANSGRIDV5_20161215152814","2014-07-08T11:00:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1049.6029799999999,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7413,"TRANSGRIDV5_20161215152814","2014-07-08T12:35:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1049.6029799999999,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7423,"TRANSGRIDV5_20161215152814","2014-07-08T14:15:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1049.6029799999999,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7439,"TRANSGRIDV5_20161215152814","2014-07-08T16:35:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1044.8239900000001,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7450,"TRANSGRIDV5_20161215152814","2014-07-08T14:35:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1043.28298,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7461,"TRANSGRIDV5_20161215152814","2014-07-08T16:25:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1043.27298,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","PLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[7471,"TRANSGRIDV5_20161215152814","2014-07-08T12:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.551210000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7483,"TRANSGRIDV5_20161215152814","2014-07-08T12:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.56391,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7486,"TRANSGRIDV5_20161215152814","2014-07-08T12:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.5379,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7500,"TRANSGRIDV5_20161215152814","2014-07-08T14:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.612159999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7508,"TRANSGRIDV5_20161215152814","2014-07-08T04:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.46543,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7517,"TRANSGRIDV5_20161215152814","2014-07-08T04:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.11431,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7534,"TRANSGRIDV5_20161215152814","2014-07-08T03:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.493080000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7538,"TRANSGRIDV5_20161215152814","2014-07-08T03:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.42882,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7549,"TRANSGRIDV5_20161215152814","2014-07-08T11:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.337580000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7565,"TRANSGRIDV5_20161215152814","2014-07-08T10:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.57587,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7575,"TRANSGRIDV5_20161215152814","2014-07-08T10:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.386430000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7582,"TRANSGRIDV5_20161215152814","2014-07-08T03:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.020759999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7597,"TRANSGRIDV5_20161215152814","2014-07-08T14:45:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-11.970929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7609,"TRANSGRIDV5_20161215152814","2014-07-08T00:15:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.362920000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7612,"TRANSGRIDV5_20161215152814","2014-07-08T00:40:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.08624,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7630,"TRANSGRIDV5_20161215152814","2014-07-09T12:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.803900000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7638,"TRANSGRIDV5_20161215152814","2014-07-09T10:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.012,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7647,"TRANSGRIDV5_20161215152814","2014-07-10T12:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.71264,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7653,"TRANSGRIDV5_20161215152814","2014-07-10T12:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.56603,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7670,"TRANSGRIDV5_20161215152814","2014-07-10T12:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.189769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7680,"TRANSGRIDV5_20161215152814","2014-07-11T11:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.572880000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7685,"TRANSGRIDV5_20161215152814","2014-07-11T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.86946,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7697,"TRANSGRIDV5_20161215152814","2014-07-11T22:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.08413,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7711,"TRANSGRIDV5_20161215152814","2014-07-11T10:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.5184,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7724,"TRANSGRIDV5_20161215152814","2014-07-11T23:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.058439999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7733,"TRANSGRIDV5_20161215152814","2014-07-11T15:30:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-18.092870000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7741,"TRANSGRIDV5_20161215152814","2014-07-11T15:05:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-12.694369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7748,"TRANSGRIDV5_20161215152814","2014-07-11T15:15:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.239179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7762,"TRANSGRIDV5_20161215152814","2014-07-12T15:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.58202,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7774,"TRANSGRIDV5_20161215152814","2014-07-12T13:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.09235,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7779,"TRANSGRIDV5_20161215152814","2014-07-12T13:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.307970000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7789,"TRANSGRIDV5_20161215152814","2014-07-12T13:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.505420000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7806,"TRANSGRIDV5_20161215152814","2014-07-12T15:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.66422,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7811,"TRANSGRIDV5_20161215152814","2014-07-12T10:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.94772,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7823,"TRANSGRIDV5_20161215152814","2014-07-12T23:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.72869,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7837,"TRANSGRIDV5_20161215152814","2014-07-12T21:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.48091,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7843,"TRANSGRIDV5_20161215152814","2014-07-12T22:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.81671,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7856,"TRANSGRIDV5_20161215152814","2014-07-12T23:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.864330000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7869,"TRANSGRIDV5_20161215152814","2014-07-12T11:45:00","V::N_LTWGQC_R","N-LTWG_RADIAL","2013-08-21",1,-12.236610000000001,"Out = Lower Tumut to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink TAS to VIC, QLD accelerates, segment 3","OUTAGE","OTHER","Wagga330 330kV Bus A","REGULATED","INCLUDED","","PLANNED",1]
[7883,"TRANSGRIDV5_20161215152814","2014-07-12T12:50:00","V::N_LTWGQC_R","N-LTWG_RADIAL","2013-08-21",1,-11.322010000000001,"Out = Lower Tumut to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink TAS to VIC, QLD accelerates, segment 3","OUTAGE","OTHER","Wagga330 330kV Bus A","REGULATED","INCLUDED","","PLANNED",1]
[7884,"TRANSGRIDV5_20161215152814","2014-07-12T13:20:00","V::N_LTWGQC_R","N-LTWG_RADIAL","2013-08-21",1,-10.827970000000001,"Out = Lower Tumut to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink TAS to VIC, QLD accelerates, segment 3","OUTAGE","OTHER","Wagga330 330kV Bus A","REGULATED","INCLUDED","","PLANNED",1]
[7904,"TRANSGRIDV5_20161215152814","2014-07-13T11:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.561,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7910,"TRANSGRIDV5_20161215152814","2014-07-13T01:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.73481,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7921,"TRANSGRIDV5_20161215152814","2014-07-13T10:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.990010000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7936,"TRANSGRIDV5_20161215152814","2014-07-13","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.6343,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7938,"TRANSGRIDV5_20161215152814","2014-07-13T15:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.169919999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7947,"TRANSGRIDV5_20161215152814","2014-07-13T08:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.70025,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7965,"TRANSGRIDV5_20161215152814","2014-07-13T22:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.284520000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[7973,"TRANSGRIDV5_20161215152814","2014-07-13T10:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.37928,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7986,"TRANSGRIDV5_20161215152814","2014-07-13T01:35:00","V::N_NIL_V1","V-NIL","2013-10-21",1,-11.42854,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink TAS to VIC, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[7999,"TRANSGRIDV5_20161215152814","2014-07-14T13:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.551210000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8003,"TRANSGRIDV5_20161215152814","2014-07-14T10:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.68802,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8014,"TRANSGRIDV5_20161215152814","2014-07-14T13:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.663449999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8030,"TRANSGRIDV5_20161215152814","2014-07-14T12:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.635300000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8036,"TRANSGRIDV5_20161215152814","2014-07-14T14:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.6111,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8046,"TRANSGRIDV5_20161215152814","2014-07-14T21:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.88523,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8053,"TRANSGRIDV5_20161215152814","2014-07-14T23:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.72869,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8072,"TRANSGRIDV5_20161215152814","2014-07-14T15:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.15366,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8080,"TRANSGRIDV5_20161215152814","2014-07-14T09:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.88682,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8094,"TRANSGRIDV5_20161215152814","2014-07-14T05:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.14991,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8097,"TRANSGRIDV5_20161215152814","2014-07-14T06:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.49208,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8109,"TRANSGRIDV5_20161215152814","2014-07-15T06:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-24.802689999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8118,"TRANSGRIDV5_20161215152814","2014-07-15T11:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.38522,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8135,"TRANSGRIDV5_20161215152814","2014-07-15T03:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.311150000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8145,"TRANSGRIDV5_20161215152814","2014-07-15T00:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.84051,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8150,"TRANSGRIDV5_20161215152814","2014-07-15T01:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.84028,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8162,"TRANSGRIDV5_20161215152814","2014-07-15T15:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.662890000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8172,"TRANSGRIDV5_20161215152814","2014-07-15T11:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.474349999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8179,"TRANSGRIDV5_20161215152814","2014-07-15T12:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.66239,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8198,"TRANSGRIDV5_20161215152814","2014-07-15T15:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.72869,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8200,"TRANSGRIDV5_20161215152814","2014-07-15T13:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.50116,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8213,"TRANSGRIDV5_20161215152814","2014-07-15T16:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.529529999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8227,"TRANSGRIDV5_20161215152814","2014-07-15T06:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.285769999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8239,"TRANSGRIDV5_20161215152814","2014-07-15T11:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.29448,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8245,"TRANSGRIDV5_20161215152814","2014-07-15T00:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.30681,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8260,"TRANSGRIDV5_20161215152814","2014-07-16T10:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.627459999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8271,"TRANSGRIDV5_20161215152814","2014-07-16T09:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.747689999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8277,"TRANSGRIDV5_20161215152814","2014-07-16T23:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.852259999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8286,"TRANSGRIDV5_20161215152814","2014-07-16T22:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.87318,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8304,"TRANSGRIDV5_20161215152814","2014-07-16T16:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.29166,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8308,"TRANSGRIDV5_20161215152814","2014-07-16T11:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-10.358890000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8321,"TRANSGRIDV5_20161215152814","2014-07-17T01:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-19.09637,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8334,"TRANSGRIDV5_20161215152814","2014-07-17T06:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.17292,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8342,"TRANSGRIDV5_20161215152814","2014-07-17T01:15:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-21.61233,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8349,"TRANSGRIDV5_20161215152814","2014-07-17T00:40:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-12.80002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8359,"TRANSGRIDV5_20161215152814","2014-07-18T14:00:00","N^^V_NIL_1","V-NIL","2014-06-04",1,-24.07403,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8375,"TRANSGRIDV5_20161215152814","2014-07-18T10:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.115320000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8386,"TRANSGRIDV5_20161215152814","2014-07-18T09:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.78965,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8397,"TRANSGRIDV5_20161215152814","2014-07-19T11:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.46608,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8403,"TRANSGRIDV5_20161215152814","2014-07-19T18:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-201.18668,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8412,"TRANSGRIDV5_20161215152814","2014-07-20T10:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.18116,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8424,"TRANSGRIDV5_20161215152814","2014-07-20T12:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.573790000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8438,"TRANSGRIDV5_20161215152814","2014-07-20T10:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.465439999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8444,"TRANSGRIDV5_20161215152814","2014-07-20T06:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.116860000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8453,"TRANSGRIDV5_20161215152814","2014-07-21T10:45:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-91.047809999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8470,"TRANSGRIDV5_20161215152814","2014-07-21T13:25:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-34.886780000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8474,"TRANSGRIDV5_20161215152814","2014-07-21T23:50:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-30.136099999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8485,"TRANSGRIDV5_20161215152814","2014-07-21T14:30:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-22.315719999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8501,"TRANSGRIDV5_20161215152814","2014-07-21T14:25:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-20.447890000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8511,"TRANSGRIDV5_20161215152814","2014-07-21T10:00:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-18.261520000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8518,"TRANSGRIDV5_20161215152814","2014-07-21T09:10:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-17.888290000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8533,"TRANSGRIDV5_20161215152814","2014-07-21T23:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.614360000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8545,"TRANSGRIDV5_20161215152814","2014-07-21T23:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.834580000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8548,"TRANSGRIDV5_20161215152814","2014-07-21T03:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.69253,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8566,"TRANSGRIDV5_20161215152814","2014-07-21T23:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.35965,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8574,"TRANSGRIDV5_20161215152814","2014-07-22T09:55:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-176.55547000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8583,"TRANSGRIDV5_20161215152814","2014-07-22T10:45:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-66.218860000000006,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8589,"TRANSGRIDV5_20161215152814","2014-07-22T05:35:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-21.844159999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8600,"TRANSGRIDV5_20161215152814","2014-07-22","N^^V_NIL_1","V-NIL","2014-07-21",1,-16.591059999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8611,"TRANSGRIDV5_20161215152814","2014-07-22T10:00:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-12.458500000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8621,"TRANSGRIDV5_20161215152814","2014-07-22T01:35:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-10.33142,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8633,"TRANSGRIDV5_20161215152814","2014-07-22T03:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.034230000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8647,"TRANSGRIDV5_20161215152814","2014-07-22T00:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.09182,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8660,"TRANSGRIDV5_20161215152814","2014-07-22T00:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.938140000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8669,"TRANSGRIDV5_20161215152814","2014-07-22T09:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.8917,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8677,"TRANSGRIDV5_20161215152814","2014-07-22T23:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.007110000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8684,"TRANSGRIDV5_20161215152814","2014-07-22T03:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.336639999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8698,"TRANSGRIDV5_20161215152814","2014-07-22T01:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.589779999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8710,"TRANSGRIDV5_20161215152814","2014-07-22T07:30:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-22.299679999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8725,"TRANSGRIDV5_20161215152814","2014-07-23T00:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.77427,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8736,"TRANSGRIDV5_20161215152814","2014-07-27T13:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.812750000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8742,"TRANSGRIDV5_20161215152814","2014-07-27T03:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.273620000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8747,"TRANSGRIDV5_20161215152814","2014-07-28T06:15:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,11.757619999999999,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8759,"TRANSGRIDV5_20161215152814","2014-07-29T02:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-15.94495,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8773,"TRANSGRIDV5_20161215152814","2014-07-29T03:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-15.567170000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8780,"TRANSGRIDV5_20161215152814","2014-07-29T03:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.32095,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8799,"TRANSGRIDV5_20161215152814","2014-07-29T03:05:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-14.134729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8807,"TRANSGRIDV5_20161215152814","2014-07-29T04:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-13.82879,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8814,"TRANSGRIDV5_20161215152814","2014-07-29T03:10:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-13.19187,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8831,"TRANSGRIDV5_20161215152814","2014-07-31T03:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8840,"TRANSGRIDV5_20161215152814","2014-07-31T03:35:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-18.157990000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8846,"TRANSGRIDV5_20161215152814","2014-07-31T04:45:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2013-12-03",1,-12.337020000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8857,"TRANSGRIDV5_20161215152814","2014-08-01T08:30:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-56.922960000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8872,"TRANSGRIDV5_20161215152814","2014-08-01T10:50:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-11.956950000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8874,"TRANSGRIDV5_20161215152814","2014-08-01T10:45:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-11.111219999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[8894,"TRANSGRIDV5_20161215152814","2014-08-02T08:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.056360000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8901,"TRANSGRIDV5_20161215152814","2014-08-02T08:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.235580000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8909,"TRANSGRIDV5_20161215152814","2014-08-02T02:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.946960000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8922,"TRANSGRIDV5_20161215152814","2014-08-02T13:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.967449999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8935,"TRANSGRIDV5_20161215152814","2014-08-02T04:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.41301,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8939,"TRANSGRIDV5_20161215152814","2014-08-02T03:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.41276,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8950,"TRANSGRIDV5_20161215152814","2014-08-02T01:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.034940000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8966,"TRANSGRIDV5_20161215152814","2014-08-02T13:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.580719999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8972,"TRANSGRIDV5_20161215152814","2014-08-02T05:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.146789999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8983,"TRANSGRIDV5_20161215152814","2014-08-02T10:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.59779,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[8998,"TRANSGRIDV5_20161215152814","2014-08-02T05:30:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,36.552630000000001,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9000,"TRANSGRIDV5_20161215152814","2014-08-02T05:40:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,33.419939999999997,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9013,"TRANSGRIDV5_20161215152814","2014-08-02T10:50:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,20.190159999999999,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9030,"TRANSGRIDV5_20161215152814","2014-08-02T12:15:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,18.340160000000001,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9033,"TRANSGRIDV5_20161215152814","2014-08-02T12:05:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,18.330380000000002,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9045,"TRANSGRIDV5_20161215152814","2014-08-02T09:30:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,15.97016,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9054,"TRANSGRIDV5_20161215152814","2014-08-02T11:35:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,15.51796,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9071,"TRANSGRIDV5_20161215152814","2014-08-02T10:25:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,14.57016,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9081,"TRANSGRIDV5_20161215152814","2014-08-02T14:20:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,13.88016,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9086,"TRANSGRIDV5_20161215152814","2014-08-02T08:50:00","NSA_Q_GSTONE34_290","NSA-Q_GSTONE34_290","2013-08-21",1,13.440160000000001,"Gladstone 3 + 4 >= 290 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9098,"TRANSGRIDV5_20161215152814","2014-08-02T08:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.533249999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9108,"TRANSGRIDV5_20161215152814","2014-08-02T09:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.77534,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9125,"TRANSGRIDV5_20161215152814","2014-08-02T02:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.00714,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9134,"TRANSGRIDV5_20161215152814","2014-08-02T02:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.906499999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9146,"TRANSGRIDV5_20161215152814","2014-08-02T11:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.453200000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9149,"TRANSGRIDV5_20161215152814","2014-08-02T12:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.42675,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9163,"TRANSGRIDV5_20161215152814","2014-08-02T12:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.36834,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9175,"TRANSGRIDV5_20161215152814","2014-08-02T09:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.48474,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9180,"TRANSGRIDV5_20161215152814","2014-08-02T10:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.36163,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9197,"TRANSGRIDV5_20161215152814","2014-08-02T11:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.174329999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9207,"TRANSGRIDV5_20161215152814","2014-08-02T01:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.50568,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9212,"TRANSGRIDV5_20161215152814","2014-08-02T05:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.151350000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9222,"TRANSGRIDV5_20161215152814","2014-08-02T04:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.469099999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9240,"TRANSGRIDV5_20161215152814","2014-08-03T22:20:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.66525,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9244,"TRANSGRIDV5_20161215152814","2014-08-03T21:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-31.146640000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9257,"TRANSGRIDV5_20161215152814","2014-08-03T20:45:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-21.882159999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9270,"TRANSGRIDV5_20161215152814","2014-08-04T03:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.25952,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9278,"TRANSGRIDV5_20161215152814","2014-08-04T03:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.30339,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9285,"TRANSGRIDV5_20161215152814","2014-08-04T01:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.10843,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9295,"TRANSGRIDV5_20161215152814","2014-08-04T01:50:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-34.114840000000001,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9311,"TRANSGRIDV5_20161215152814","2014-08-04T12:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.60571,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9322,"TRANSGRIDV5_20161215152814","2014-08-04T11:35:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-10.188639999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9333,"TRANSGRIDV5_20161215152814","2014-08-05T16:25:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-21.377880000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9339,"TRANSGRIDV5_20161215152814","2014-08-05T11:35:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-20.421130000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9348,"TRANSGRIDV5_20161215152814","2014-08-05T11:05:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-18.083089999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9360,"TRANSGRIDV5_20161215152814","2014-08-05T14:30:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-15.362959999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9374,"TRANSGRIDV5_20161215152814","2014-08-05T11:30:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-12.860250000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9387,"TRANSGRIDV5_20161215152814","2014-08-05T10:40:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-10.04508,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9389,"TRANSGRIDV5_20161215152814","2014-08-05T08:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-236.22676000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9406,"TRANSGRIDV5_20161215152814","2014-08-05T09:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-23.719760000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9420,"TRANSGRIDV5_20161215152814","2014-08-05T08:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-253.57337999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9421,"TRANSGRIDV5_20161215152814","2014-08-05T08:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-215.59905000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9437,"TRANSGRIDV5_20161215152814","2014-08-05T09:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-27.17427,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9447,"TRANSGRIDV5_20161215152814","2014-08-05T00:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.90906,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9454,"TRANSGRIDV5_20161215152814","2014-08-05T04:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.098280000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9469,"TRANSGRIDV5_20161215152814","2014-08-06T01:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.378820000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9481,"TRANSGRIDV5_20161215152814","2014-08-06T01:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.8066,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9484,"TRANSGRIDV5_20161215152814","2014-08-06T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.226430000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9502,"TRANSGRIDV5_20161215152814","2014-08-06T01:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.96838,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9510,"TRANSGRIDV5_20161215152814","2014-08-06T10:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.48812,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9519,"TRANSGRIDV5_20161215152814","2014-08-06T23:40:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-220.08687,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9536,"TRANSGRIDV5_20161215152814","2014-08-07T21:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.276210000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9546,"TRANSGRIDV5_20161215152814","2014-08-07T23:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.26985,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9547,"TRANSGRIDV5_20161215152814","2014-08-07T21:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.172079999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9563,"TRANSGRIDV5_20161215152814","2014-08-07T21:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.915389999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9573,"TRANSGRIDV5_20161215152814","2014-08-07T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.535780000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9580,"TRANSGRIDV5_20161215152814","2014-08-07T00:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.271319999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9599,"TRANSGRIDV5_20161215152814","2014-08-07T01:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.087020000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9605,"TRANSGRIDV5_20161215152814","2014-08-07T01:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.049580000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9613,"TRANSGRIDV5_20161215152814","2014-08-08T01:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.505409999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9631,"TRANSGRIDV5_20161215152814","2014-08-08T20:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.145300000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9634,"TRANSGRIDV5_20161215152814","2014-08-08T00:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.238250000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9646,"TRANSGRIDV5_20161215152814","2014-08-08T01:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.610049999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9661,"TRANSGRIDV5_20161215152814","2014-08-08T01:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.752330000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9672,"TRANSGRIDV5_20161215152814","2014-08-08T21:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.3424,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9678,"TRANSGRIDV5_20161215152814","2014-08-08T22:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.43519,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9694,"TRANSGRIDV5_20161215152814","2014-08-08T20:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.365030000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9695,"TRANSGRIDV5_20161215152814","2014-08-08T22:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.302440000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9709,"TRANSGRIDV5_20161215152814","2014-08-08T04:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.027609999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9716,"TRANSGRIDV5_20161215152814","2014-08-09T08:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.215809999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9735,"TRANSGRIDV5_20161215152814","2014-08-09T09:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.57963,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9743,"TRANSGRIDV5_20161215152814","2014-08-09T08:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.24119,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9750,"TRANSGRIDV5_20161215152814","2014-08-09T23:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.182550000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9760,"TRANSGRIDV5_20161215152814","2014-08-09T00:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.100709999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9772,"TRANSGRIDV5_20161215152814","2014-08-10T08:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.195819999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9787,"TRANSGRIDV5_20161215152814","2014-08-11T09:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-55.231499999999997,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9798,"TRANSGRIDV5_20161215152814","2014-08-11T08:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-24.034980000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9808,"TRANSGRIDV5_20161215152814","2014-08-11T10:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.173649999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9820,"TRANSGRIDV5_20161215152814","2014-08-11T10:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.54813,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9830,"TRANSGRIDV5_20161215152814","2014-08-11T16:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.11022,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9837,"TRANSGRIDV5_20161215152814","2014-08-11T11:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.149570000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9845,"TRANSGRIDV5_20161215152814","2014-08-11T22:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.136279999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9858,"TRANSGRIDV5_20161215152814","2014-08-11T22:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.895630000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[9871,"TRANSGRIDV5_20161215152814","2014-08-11T08:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-67.311149999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9875,"TRANSGRIDV5_20161215152814","2014-08-11T09:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-44.521369999999997,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9886,"TRANSGRIDV5_20161215152814","2014-08-11T08:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.09273,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9902,"TRANSGRIDV5_20161215152814","2014-08-11T19:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.28509,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9908,"TRANSGRIDV5_20161215152814","2014-08-11T11:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.404730000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9919,"TRANSGRIDV5_20161215152814","2014-08-11T07:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.482799999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9934,"TRANSGRIDV5_20161215152814","2014-08-11T10:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.52502,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9946,"TRANSGRIDV5_20161215152814","2014-08-11T06:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.49358,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9949,"TRANSGRIDV5_20161215152814","2014-08-11T08:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.39705,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9967,"TRANSGRIDV5_20161215152814","2014-08-11T23:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.202059999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9975,"TRANSGRIDV5_20161215152814","2014-08-11T01:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.860609999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9984,"TRANSGRIDV5_20161215152814","2014-08-11T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.53717,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[9997,"TRANSGRIDV5_20161215152814","2014-08-12T08:00:00","#R010876_002_RAMP_F","#R010876_RAMP","2014-08-12",1,-33.759,"Hard Ramping constraint for constraint N_X_MBTE_3B, Effective Date: 25/11/2013, Version: 1","OUTAGE","RAMP","Terranora Interconnector","REGULATED",10,"Ramping Constraint","PLANNED",0]
[10007,"TRANSGRIDV5_20161215152814","2014-08-12T19:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.602650000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10017,"TRANSGRIDV5_20161215152814","2014-08-12T09:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.87472,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10022,"TRANSGRIDV5_20161215152814","2014-08-12T09:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.841740000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10034,"TRANSGRIDV5_20161215152814","2014-08-12T17:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.474399999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10044,"TRANSGRIDV5_20161215152814","2014-08-12T10:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.88246,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10061,"TRANSGRIDV5_20161215152814","2014-08-12T11:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.68661,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10070,"TRANSGRIDV5_20161215152814","2014-08-12T13:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.877800000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10082,"TRANSGRIDV5_20161215152814","2014-08-12T14:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.55883,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10085,"TRANSGRIDV5_20161215152814","2014-08-12T17:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.33564,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10099,"TRANSGRIDV5_20161215152814","2014-08-12T15:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.432510000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10111,"TRANSGRIDV5_20161215152814","2014-08-12T16:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.057320000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10116,"TRANSGRIDV5_20161215152814","2014-08-12T12:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.80429,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10133,"TRANSGRIDV5_20161215152814","2014-08-12T03:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-21.642029999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10143,"TRANSGRIDV5_20161215152814","2014-08-12T06:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.697659999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10148,"TRANSGRIDV5_20161215152814","2014-08-12T22:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.912130000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10160,"TRANSGRIDV5_20161215152814","2014-08-12T00:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-15.653219999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10174,"TRANSGRIDV5_20161215152814","2014-08-12T21:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.1915,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10180,"TRANSGRIDV5_20161215152814","2014-08-12T00:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.93385,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10193,"TRANSGRIDV5_20161215152814","2014-08-12T22:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.58736,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10206,"TRANSGRIDV5_20161215152814","2014-08-12T03:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.928459999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10214,"TRANSGRIDV5_20161215152814","2014-08-12T02:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.0191,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10221,"TRANSGRIDV5_20161215152814","2014-08-12T08:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.74841,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10241,"TRANSGRIDV5_20161215152814","2014-08-12T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.18496,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10247,"TRANSGRIDV5_20161215152814","2014-08-12T02:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.25928,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10258,"TRANSGRIDV5_20161215152814","2014-08-12T05:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.17456,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10269,"TRANSGRIDV5_20161215152814","2014-08-12T09:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.620419999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10275,"TRANSGRIDV5_20161215152814","2014-08-12T02:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.961309999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10284,"TRANSGRIDV5_20161215152814","2014-08-12T10:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.871119999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10296,"TRANSGRIDV5_20161215152814","2014-08-12T19:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.053430000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10310,"TRANSGRIDV5_20161215152814","2014-08-12T19:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.34469,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10323,"TRANSGRIDV5_20161215152814","2014-08-12T23:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-224.48129,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10336,"TRANSGRIDV5_20161215152814","2014-08-12T23:20:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-209.80833000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10340,"TRANSGRIDV5_20161215152814","2014-08-12T23:00:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-57.888350000000003,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10347,"TRANSGRIDV5_20161215152814","2014-08-13T09:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.100090000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10367,"TRANSGRIDV5_20161215152814","2014-08-13T09:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.47335,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10373,"TRANSGRIDV5_20161215152814","2014-08-13T01:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.084479999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10383,"TRANSGRIDV5_20161215152814","2014-08-13T01:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.4474,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10390,"TRANSGRIDV5_20161215152814","2014-08-13T06:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.06596,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10405,"TRANSGRIDV5_20161215152814","2014-08-13T02:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.524179999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10417,"TRANSGRIDV5_20161215152814","2014-08-13T06:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.86918,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10431,"TRANSGRIDV5_20161215152814","2014-08-13T00:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.28166,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10438,"TRANSGRIDV5_20161215152814","2014-08-13T08:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.56305,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10446,"TRANSGRIDV5_20161215152814","2014-08-13T21:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.1563,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10455,"TRANSGRIDV5_20161215152814","2014-08-13T01:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.26859,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10472,"TRANSGRIDV5_20161215152814","2014-08-13T22:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.118550000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10482,"TRANSGRIDV5_20161215152814","2014-08-13T01:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-81.631820000000005,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10494,"TRANSGRIDV5_20161215152814","2014-08-13T00:15:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-89.647859999999994,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10499,"TRANSGRIDV5_20161215152814","2014-08-14T06:45:00","#R010888_001_RAMP_F","#R010888_RAMP","2014-08-14",1,-12.73976,"Hard Ramping constraint for constraint Q>N-MUTE_758, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","758 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[10509,"TRANSGRIDV5_20161215152814","2014-08-14T07:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.646940000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10516,"TRANSGRIDV5_20161215152814","2014-08-14T08:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.96439,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10535,"TRANSGRIDV5_20161215152814","2014-08-14T10:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.462769999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10537,"TRANSGRIDV5_20161215152814","2014-08-14T11:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.123809999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10550,"TRANSGRIDV5_20161215152814","2014-08-14T09:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.578709999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10564,"TRANSGRIDV5_20161215152814","2014-08-14T22:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.95749,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10572,"TRANSGRIDV5_20161215152814","2014-08-14T22:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.39991,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10582,"TRANSGRIDV5_20161215152814","2014-08-14T00:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.65409,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10597,"TRANSGRIDV5_20161215152814","2014-08-14T10:40:00","Q>NIL_MUTE_757","Q-NIL","2013-08-21",1,-18.462240000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10608,"TRANSGRIDV5_20161215152814","2014-08-14T10:25:00","Q>NIL_MUTE_757","Q-NIL","2013-08-21",1,-14.510020000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10614,"TRANSGRIDV5_20161215152814","2014-08-14T10:30:00","Q>NIL_MUTE_757","Q-NIL","2013-08-21",1,-14.28988,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10630,"TRANSGRIDV5_20161215152814","2014-08-15T08:10:00","#R010894_001_RAMP_F","#R010894_RAMP","2014-08-15",1,-25.290369999999999,"Hard Ramping constraint for constraint Q>N-MUTE_757, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","757 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[10641,"TRANSGRIDV5_20161215152814","2014-08-15T02:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.60266,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10645,"TRANSGRIDV5_20161215152814","2014-08-15T08:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-20.843589999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10662,"TRANSGRIDV5_20161215152814","2014-08-15T04:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.965909999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10671,"TRANSGRIDV5_20161215152814","2014-08-15T09:20:00","Q>NIL_MUTE_758","Q-NIL","2013-08-21",1,-14.247629999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10679,"TRANSGRIDV5_20161215152814","2014-08-16T07:10:00","#R010896_005_RAMP_F","#R010896_RAMP","2014-08-15",1,-10.633330000000001,"Hard Ramping constraint for constraint V::N_HORCQE_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Horsham - Redcliffs 220kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[10686,"TRANSGRIDV5_20161215152814","2014-08-17T13:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.51885,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10696,"TRANSGRIDV5_20161215152814","2014-08-17T12:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.354979999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10708,"TRANSGRIDV5_20161215152814","2014-08-17T11:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.124969999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10723,"TRANSGRIDV5_20161215152814","2014-08-18T12:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-23.261119999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10734,"TRANSGRIDV5_20161215152814","2014-08-18T15:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.44361,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10740,"TRANSGRIDV5_20161215152814","2014-08-18T15:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.115130000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10749,"TRANSGRIDV5_20161215152814","2014-08-18T12:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.270879999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10761,"TRANSGRIDV5_20161215152814","2014-08-18T12:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.086200000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10775,"TRANSGRIDV5_20161215152814","2014-08-18T10:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.39462,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10781,"TRANSGRIDV5_20161215152814","2014-08-18T16:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.55833,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10794,"TRANSGRIDV5_20161215152814","2014-08-18T09:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.855169999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10807,"TRANSGRIDV5_20161215152814","2014-08-18T11:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-26.207139999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10811,"TRANSGRIDV5_20161215152814","2014-08-18T10:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-25.078420000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10822,"TRANSGRIDV5_20161215152814","2014-08-18T13:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.61889,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10838,"TRANSGRIDV5_20161215152814","2014-08-18T12:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-22.229179999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10844,"TRANSGRIDV5_20161215152814","2014-08-18T16:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-21.492529999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10855,"TRANSGRIDV5_20161215152814","2014-08-18T10:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.926549999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10870,"TRANSGRIDV5_20161215152814","2014-08-18T15:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.916879999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10876,"TRANSGRIDV5_20161215152814","2014-08-18T09:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.47514,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10885,"TRANSGRIDV5_20161215152814","2014-08-18T14:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.25027,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10903,"TRANSGRIDV5_20161215152814","2014-08-18T06:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.256,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10911,"TRANSGRIDV5_20161215152814","2014-08-19T13:10:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-16.821249999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10920,"TRANSGRIDV5_20161215152814","2014-08-19T08:50:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-12.954739999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10933,"TRANSGRIDV5_20161215152814","2014-08-19T16:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.970660000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10937,"TRANSGRIDV5_20161215152814","2014-08-19T15:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.46654,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10948,"TRANSGRIDV5_20161215152814","2014-08-19T13:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.929729999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10958,"TRANSGRIDV5_20161215152814","2014-08-19T22:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.002459999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[10970,"TRANSGRIDV5_20161215152814","2014-08-19T23:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.546980000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10980,"TRANSGRIDV5_20161215152814","2014-08-19T15:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.961490000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[10997,"TRANSGRIDV5_20161215152814","2014-08-19T14:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.041060000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11006,"TRANSGRIDV5_20161215152814","2014-08-19T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.817909999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11018,"TRANSGRIDV5_20161215152814","2014-08-19T21:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.07776,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11021,"TRANSGRIDV5_20161215152814","2014-08-19T22:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.738899999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11035,"TRANSGRIDV5_20161215152814","2014-08-19T13:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.565799999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11047,"TRANSGRIDV5_20161215152814","2014-08-19T13:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.205629999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11062,"TRANSGRIDV5_20161215152814","2014-08-19T02:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.96964,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11069,"TRANSGRIDV5_20161215152814","2014-08-19T15:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.738770000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11079,"TRANSGRIDV5_20161215152814","2014-08-19T22:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.207079999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11084,"TRANSGRIDV5_20161215152814","2014-08-20T09:40:00","N^^V_NIL_1","V-NIL","2014-07-21",1,-96.150360000000006,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11096,"TRANSGRIDV5_20161215152814","2014-08-20T03:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.99891,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11110,"TRANSGRIDV5_20161215152814","2014-08-20T00:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.88223,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11117,"TRANSGRIDV5_20161215152814","2014-08-20T23:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.418799999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11136,"TRANSGRIDV5_20161215152814","2014-08-20T12:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.53073,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11144,"TRANSGRIDV5_20161215152814","2014-08-20T23:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.616109999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11147,"TRANSGRIDV5_20161215152814","2014-08-20T00:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.057200000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11168,"TRANSGRIDV5_20161215152814","2014-08-20T03:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.724959999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11177,"TRANSGRIDV5_20161215152814","2014-08-20T01:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.3749,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11183,"TRANSGRIDV5_20161215152814","2014-08-20T23:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.739890000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11194,"TRANSGRIDV5_20161215152814","2014-08-20T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.31898,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11205,"TRANSGRIDV5_20161215152814","2014-08-20T12:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.20027,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11211,"TRANSGRIDV5_20161215152814","2014-08-20T11:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.19426,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11231,"TRANSGRIDV5_20161215152814","2014-08-20T14:30:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.22672,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11232,"TRANSGRIDV5_20161215152814","2014-08-20T13:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.15236,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11246,"TRANSGRIDV5_20161215152814","2014-08-21T03:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.609439999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11259,"TRANSGRIDV5_20161215152814","2014-08-21T10:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.88475,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11272,"TRANSGRIDV5_20161215152814","2014-08-21T09:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.70656,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11276,"TRANSGRIDV5_20161215152814","2014-08-21T01:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.222799999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11294,"TRANSGRIDV5_20161215152814","2014-08-21T09:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.08681,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11303,"TRANSGRIDV5_20161215152814","2014-08-22T01:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.363200000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11309,"TRANSGRIDV5_20161215152814","2014-08-22T05:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.118370000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11320,"TRANSGRIDV5_20161215152814","2014-08-22T01:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-20.551559999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11335,"TRANSGRIDV5_20161215152814","2014-08-22T05:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.29846,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11341,"TRANSGRIDV5_20161215152814","2014-08-22T00:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.07075,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11350,"TRANSGRIDV5_20161215152814","2014-08-23T06:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.138590000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11367,"TRANSGRIDV5_20161215152814","2014-08-23T06:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.09686,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11374,"TRANSGRIDV5_20161215152814","2014-08-23T23:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.08498,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11382,"TRANSGRIDV5_20161215152814","2014-08-23T07:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.32103,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11391,"TRANSGRIDV5_20161215152814","2014-08-23T07:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.013500000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11408,"TRANSGRIDV5_20161215152814","2014-08-23T16:20:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-24.096240000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11418,"TRANSGRIDV5_20161215152814","2014-08-23T12:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-15.38363,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11430,"TRANSGRIDV5_20161215152814","2014-08-23T13:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-10.768980000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11435,"TRANSGRIDV5_20161215152814","2014-08-23T09:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-10.27567,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11445,"TRANSGRIDV5_20161215152814","2014-08-23T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-10.14123,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11462,"TRANSGRIDV5_20161215152814","2014-08-24T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.5687,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11471,"TRANSGRIDV5_20161215152814","2014-08-24T01:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.359450000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11483,"TRANSGRIDV5_20161215152814","2014-08-25T09:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.518700000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11486,"TRANSGRIDV5_20161215152814","2014-08-25T11:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.02622,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11500,"TRANSGRIDV5_20161215152814","2014-08-25T05:45:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-10.412660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11508,"TRANSGRIDV5_20161215152814","2014-08-25T02:45:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-11.412509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11517,"TRANSGRIDV5_20161215152814","2014-08-26T08:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-81.381050000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11534,"TRANSGRIDV5_20161215152814","2014-08-26T09:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-28.49869,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11544,"TRANSGRIDV5_20161215152814","2014-08-26T13:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.784700000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11549,"TRANSGRIDV5_20161215152814","2014-08-26T12:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.843229999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11566,"TRANSGRIDV5_20161215152814","2014-08-26T14:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.525700000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11577,"TRANSGRIDV5_20161215152814","2014-08-26T14:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.670179999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11581,"TRANSGRIDV5_20161215152814","2014-08-26T15:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.651,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11598,"TRANSGRIDV5_20161215152814","2014-08-26T23:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.31964,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11607,"TRANSGRIDV5_20161215152814","2014-08-26T21:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.038080000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11615,"TRANSGRIDV5_20161215152814","2014-08-26T09:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-40.353430000000003,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11622,"TRANSGRIDV5_20161215152814","2014-08-26T10:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.56399,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11632,"TRANSGRIDV5_20161215152814","2014-08-26T08:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-20.721520000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11644,"TRANSGRIDV5_20161215152814","2014-08-26T23:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.510859999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11659,"TRANSGRIDV5_20161215152814","2014-08-26T11:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.06977,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11670,"TRANSGRIDV5_20161215152814","2014-08-26T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.77824,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11676,"TRANSGRIDV5_20161215152814","2014-08-26T14:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.42347,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11685,"TRANSGRIDV5_20161215152814","2014-08-26T21:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.73878,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11697,"TRANSGRIDV5_20161215152814","2014-08-26T04:40:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-12.504300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11711,"TRANSGRIDV5_20161215152814","2014-08-26T01:55:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-10.56701,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11724,"TRANSGRIDV5_20161215152814","2014-08-26T18:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-21.853760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11733,"TRANSGRIDV5_20161215152814","2014-08-27T11:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.57109,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11743,"TRANSGRIDV5_20161215152814","2014-08-27T02:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.42324,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11757,"TRANSGRIDV5_20161215152814","2014-08-27T00:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.897550000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11758,"TRANSGRIDV5_20161215152814","2014-08-27T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.45806,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11774,"TRANSGRIDV5_20161215152814","2014-08-28T22:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.456109999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11780,"TRANSGRIDV5_20161215152814","2014-08-28T17:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.948,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11791,"TRANSGRIDV5_20161215152814","2014-08-28T10:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.60704,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11806,"TRANSGRIDV5_20161215152814","2014-08-29T12:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.450489999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11812,"TRANSGRIDV5_20161215152814","2014-08-29T12:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.234089999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11821,"TRANSGRIDV5_20161215152814","2014-08-29T10:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.524260000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11839,"TRANSGRIDV5_20161215152814","2014-08-29T11:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.34595,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11847,"TRANSGRIDV5_20161215152814","2014-08-29T09:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.86839,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11856,"TRANSGRIDV5_20161215152814","2014-08-29T11:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-27.331019999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11869,"TRANSGRIDV5_20161215152814","2014-08-29T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-22.608779999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11883,"TRANSGRIDV5_20161215152814","2014-08-29T11:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.716390000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11884,"TRANSGRIDV5_20161215152814","2014-08-29T11:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.595120000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11900,"TRANSGRIDV5_20161215152814","2014-08-29T12:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.9941,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11910,"TRANSGRIDV5_20161215152814","2014-08-29T17:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.0448,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11921,"TRANSGRIDV5_20161215152814","2014-08-29T13:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.884219999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11936,"TRANSGRIDV5_20161215152814","2014-08-29T05:00:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-13.99586,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11942,"TRANSGRIDV5_20161215152814","2014-08-29T05:20:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-10.466229999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11954,"TRANSGRIDV5_20161215152814","2014-08-30T12:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.77915,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11968,"TRANSGRIDV5_20161215152814","2014-08-30T11:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.954319999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11971,"TRANSGRIDV5_20161215152814","2014-08-30T14:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.99184,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[11983,"TRANSGRIDV5_20161215152814","2014-08-30T12:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.423909999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[11998,"TRANSGRIDV5_20161215152814","2014-08-30T14:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.636369999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12005,"TRANSGRIDV5_20161215152814","2014-08-30T11:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.836320000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12015,"TRANSGRIDV5_20161215152814","2014-08-30T15:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.66253,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12031,"TRANSGRIDV5_20161215152814","2014-09-01T10:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.588750000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12032,"TRANSGRIDV5_20161215152814","2014-09-01T11:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.729430000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12046,"TRANSGRIDV5_20161215152814","2014-09-01T12:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.507370000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12053,"TRANSGRIDV5_20161215152814","2014-09-01T10:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.214870000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12072,"TRANSGRIDV5_20161215152814","2014-09-01T08:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.29518,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12080,"TRANSGRIDV5_20161215152814","2014-09-01T14:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.1655,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[12094,"TRANSGRIDV5_20161215152814","2014-09-01T09:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.16639,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12097,"TRANSGRIDV5_20161215152814","2014-09-01T09:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-22.962599999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12109,"TRANSGRIDV5_20161215152814","2014-09-01T09:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-21.72945,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12124,"TRANSGRIDV5_20161215152814","2014-09-01T13:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.7713,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12135,"TRANSGRIDV5_20161215152814","2014-09-01T14:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.432600000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12141,"TRANSGRIDV5_20161215152814","2014-09-01T14:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.045070000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12157,"TRANSGRIDV5_20161215152814","2014-09-02T12:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-22.248000000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12167,"TRANSGRIDV5_20161215152814","2014-09-02T11:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.80364,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12178,"TRANSGRIDV5_20161215152814","2014-09-02T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.747730000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12182,"TRANSGRIDV5_20161215152814","2014-09-02T12:40:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-25.321860000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12195,"TRANSGRIDV5_20161215152814","2014-09-02T11:20:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-15.79257,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12208,"TRANSGRIDV5_20161215152814","2014-09-03T10:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.02899,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12212,"TRANSGRIDV5_20161215152814","2014-09-03T11:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.50886,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12230,"TRANSGRIDV5_20161215152814","2014-09-04T10:40:00","Q>N-MUTE_758","I-MUTE_758","2013-08-21",1,-21.223040000000001,"Out= 758 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","758 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12239,"TRANSGRIDV5_20161215152814","2014-09-04T12:25:00","Q>N-MUTE_758","I-MUTE_758","2013-08-21",1,-12.17586,"Out= 758 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","758 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12245,"TRANSGRIDV5_20161215152814","2014-09-04T17:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.49788,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12256,"TRANSGRIDV5_20161215152814","2014-09-04T18:10:00","V>>V_NIL_2_P","V-NIL_PAR_3-5","2013-12-03",1,-11.065630000000001,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12271,"TRANSGRIDV5_20161215152814","2014-09-05T10:40:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-22.750879999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[12277,"TRANSGRIDV5_20161215152814","2014-09-05T10:30:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-15.70843,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[12286,"TRANSGRIDV5_20161215152814","2014-09-05T11:50:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-12.183540000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[12304,"TRANSGRIDV5_20161215152814","2014-09-05T10:30:00","Q>N-MUTE_758","I-MUTE_758","2013-08-21",1,-18.110939999999999,"Out= 758 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","758 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12308,"TRANSGRIDV5_20161215152814","2014-09-05T10:25:00","Q>N-MUTE_758","I-MUTE_758","2013-08-21",1,-14.86238,"Out= 758 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","758 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12321,"TRANSGRIDV5_20161215152814","2014-09-06T12:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.582549999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12334,"TRANSGRIDV5_20161215152814","2014-09-06T10:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.29937,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12344,"TRANSGRIDV5_20161215152814","2014-09-06T12:20:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-17.180620000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12354,"TRANSGRIDV5_20161215152814","2014-09-06T11:50:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-23.955939999999998,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12366,"TRANSGRIDV5_20161215152814","2014-09-06T11:25:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-19.118040000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12371,"TRANSGRIDV5_20161215152814","2014-09-06T12:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.838270000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12381,"TRANSGRIDV5_20161215152814","2014-09-06T12:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-10.424340000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12398,"TRANSGRIDV5_20161215152814","2014-09-06T08:45:00","V::N_JNWGQE_R","N-JNWG_RADIAL","2013-08-21",1,-11.36985,"Out = Jindera to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Jindera - Wagga330 62 330 kV Line","REGULATED","INCLUDED","","PLANNED",1]
[12407,"TRANSGRIDV5_20161215152814","2014-09-07T08:40:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-11.56019,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12419,"TRANSGRIDV5_20161215152814","2014-09-07T10:55:00","V::N_HWSM_S4","V-HWSM","2014-02-21",1,-20.410340000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 500 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12422,"TRANSGRIDV5_20161215152814","2014-09-07T10:45:00","V::N_HWSM_S4","V-HWSM","2014-02-21",1,-19.25188,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 500 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12436,"TRANSGRIDV5_20161215152814","2014-09-07T09:55:00","V::N_HWSM_S4","V-HWSM","2014-02-21",1,-13.291,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 500 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12444,"TRANSGRIDV5_20161215152814","2014-09-07T08:15:00","V::N_HWSM_S4","V-HWSM","2014-02-21",1,-11.796110000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 500 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12453,"TRANSGRIDV5_20161215152814","2014-09-07T12:15:00","V::N_HWSM_S4","V-HWSM","2014-02-21",1,-10.823309999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 500 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12470,"TRANSGRIDV5_20161215152814","2014-09-08T17:25:00","NSA_V_BDL01_20","NSA-V_BDL01_20","2013-08-21",1,118.84276,"Bairnsdale Unit 1 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12480,"TRANSGRIDV5_20161215152814","2014-09-08T22:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2013-12-03",1,-10.18563,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12485,"TRANSGRIDV5_20161215152814","2014-09-09T06:55:00","#R011047_012_RAMP_F","#R011047_RAMP","2014-09-08",1,-32.780180000000001,"Hard Ramping constraint for constraint V::N_HWSM_V4, Effective Date: 21/02/2014, Version: 1","OUTAGE","RAMP","Hazelwood - South Morang 500kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[12501,"TRANSGRIDV5_20161215152814","2014-09-09T06:00:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-25.782540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12511,"TRANSGRIDV5_20161215152814","2014-09-09T01:00:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-16.482240000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12517,"TRANSGRIDV5_20161215152814","2014-09-09T01:05:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-15.805669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12534,"TRANSGRIDV5_20161215152814","2014-09-10T06:05:00","#R011056_012_RAMP_V","#R011056_RAMP","2014-09-09",1,-18.343440000000001,"Soft Ramping constraint for constraint V::N_SMCSVE_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","South Morang 330kV Series Capacitor","REGULATED",10,"Ramping Constraint","PLANNED",0]
[12543,"TRANSGRIDV5_20161215152814","2014-09-10T07:55:00","#R011057_011_RAMP_F","#R011057_RAMP","2014-09-09",1,-10.70365,"Hard Ramping constraint for constraint V::N_ROSMVE_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Rowville - South Morang 500kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[12551,"TRANSGRIDV5_20161215152814","2014-09-10T09:45:00","Q>N-MUTE_757","I-MUTE_757","2013-08-21",1,-10.95576,"Out= 757 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","757 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12558,"TRANSGRIDV5_20161215152814","2014-09-10T06:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-14.0427,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12578,"TRANSGRIDV5_20161215152814","2014-09-10T09:45:00","V::N_ROSMQE_R","V-ROSM_R","2013-08-21",1,-28.93732,"Out = Rowville to South Morang 500kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Rowville - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12580,"TRANSGRIDV5_20161215152814","2014-09-10T10:40:00","V::N_ROSMQE_R","V-ROSM_R","2013-08-21",1,-25.51567,"Out = Rowville to South Morang 500kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Rowville - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12595,"TRANSGRIDV5_20161215152814","2014-09-10T10:55:00","V::N_ROSMQE_R","V-ROSM_R","2013-08-21",1,-13.302070000000001,"Out = Rowville to South Morang 500kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Rowville - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[12606,"TRANSGRIDV5_20161215152814","2014-09-10T11:50:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-18.103899999999999,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12612,"TRANSGRIDV5_20161215152814","2014-09-10T12:50:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-14.7182,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12621,"TRANSGRIDV5_20161215152814","2014-09-10T13:30:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-10.571719999999999,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12633,"TRANSGRIDV5_20161215152814","2014-09-11T07:05:00","#R011063_012_RAMP_F","#R011063_RAMP","2014-09-10",1,-213.67289,"Hard Ramping constraint for constraint V::N_HWSM_V4, Effective Date: 21/02/2014, Version: 1","OUTAGE","RAMP","Hazelwood - South Morang 500kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[12647,"TRANSGRIDV5_20161215152814","2014-09-11T06:00:00","#R011065_011_RAMP_F","#R011065_RAMP","2014-09-10",1,-56.872039999999998,"Hard Ramping constraint for constraint V::N_SMCSVD_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","South Morang 330kV Series Capacitor","REGULATED",10,"Ramping Constraint","PLANNED",0]
[12660,"TRANSGRIDV5_20161215152814","2014-09-11T11:35:00","Q>N-MUTE_757","I-MUTE_757","2013-08-21",1,-17.06615,"Out= 757 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","757 T174 Terranora to H4 Mudgeeraba 110kV Line","REGULATED",99,"Non Inclusion",null,0]
[12669,"TRANSGRIDV5_20161215152814","2014-09-11T18:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-13.02406,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12677,"TRANSGRIDV5_20161215152814","2014-09-11T06:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-37.79721,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12684,"TRANSGRIDV5_20161215152814","2014-09-11T07:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-35.246029999999998,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12704,"TRANSGRIDV5_20161215152814","2014-09-11T05:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.36525,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12710,"TRANSGRIDV5_20161215152814","2014-09-11T10:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.704700000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12716,"TRANSGRIDV5_20161215152814","2014-09-11T00:20:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-24.298380000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12727,"TRANSGRIDV5_20161215152814","2014-09-11T10:45:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-38.123449999999998,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12742,"TRANSGRIDV5_20161215152814","2014-09-11T12:20:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-17.369240000000001,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12748,"TRANSGRIDV5_20161215152814","2014-09-11T09:30:00","V::N_SMCSQE_R","V-SMSC","2013-08-21",1,-10.719200000000001,"Out = South Morang 330kV series capacitor, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","South Morang 330kV Series Capacitor","REGULATED",99,"Non Inclusion",null,0]
[12768,"TRANSGRIDV5_20161215152814","2014-09-11T01:05:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2014-03-04",1,-12.90897,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A2 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[12775,"TRANSGRIDV5_20161215152814","2014-09-11T05:05:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2014-03-04",1,-11.224159999999999,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A2 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[12783,"TRANSGRIDV5_20161215152814","2014-09-12T23:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-237.93759,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12792,"TRANSGRIDV5_20161215152814","2014-09-12T01:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-28.590399999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12805,"TRANSGRIDV5_20161215152814","2014-09-12T23:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.408429999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12819,"TRANSGRIDV5_20161215152814","2014-09-12T23:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-22.433620000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12831,"TRANSGRIDV5_20161215152814","2014-09-12T01:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-19.15222,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12836,"TRANSGRIDV5_20161215152814","2014-09-12T22:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.09036,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12846,"TRANSGRIDV5_20161215152814","2014-09-12T21:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.617519999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12857,"TRANSGRIDV5_20161215152814","2014-09-12T21:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.82882,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12872,"TRANSGRIDV5_20161215152814","2014-09-12T14:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.131309999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12874,"TRANSGRIDV5_20161215152814","2014-09-12T04:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.81724,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12894,"TRANSGRIDV5_20161215152814","2014-09-12T04:25:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-13.60905,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12901,"TRANSGRIDV5_20161215152814","2014-09-12T23:05:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-37.928019999999997,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12909,"TRANSGRIDV5_20161215152814","2014-09-12T01:50:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-27.443359999999998,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12919,"TRANSGRIDV5_20161215152814","2014-09-12T23:20:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-25.042549999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12934,"TRANSGRIDV5_20161215152814","2014-09-12T12:00:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-19.371780000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12941,"TRANSGRIDV5_20161215152814","2014-09-12T22:00:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-17.712959999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12951,"TRANSGRIDV5_20161215152814","2014-09-12T00:45:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.3124,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12967,"TRANSGRIDV5_20161215152814","2014-09-12T21:40:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-12.030950000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12978,"TRANSGRIDV5_20161215152814","2014-09-13T23:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-46.83043,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12982,"TRANSGRIDV5_20161215152814","2014-09-13T06:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-36.675289999999997,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[12999,"TRANSGRIDV5_20161215152814","2014-09-13T01:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-28.601469999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13008,"TRANSGRIDV5_20161215152814","2014-09-13T22:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-27.777429999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13016,"TRANSGRIDV5_20161215152814","2014-09-13T03:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.60041,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13030,"TRANSGRIDV5_20161215152814","2014-09-13T12:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-24.980920000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13033,"TRANSGRIDV5_20161215152814","2014-09-13T03:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-24.602650000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13045,"TRANSGRIDV5_20161215152814","2014-09-13T22:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.81418,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13060,"TRANSGRIDV5_20161215152814","2014-09-13T23:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-22.402629999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13071,"TRANSGRIDV5_20161215152814","2014-09-13T11:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.426970000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13081,"TRANSGRIDV5_20161215152814","2014-09-13T07:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.565819999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13086,"TRANSGRIDV5_20161215152814","2014-09-13T09:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.174569999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13098,"TRANSGRIDV5_20161215152814","2014-09-13T12:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.915800000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13108,"TRANSGRIDV5_20161215152814","2014-09-13T09:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.07245,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13118,"TRANSGRIDV5_20161215152814","2014-09-13T11:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.029309999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13131,"TRANSGRIDV5_20161215152814","2014-09-13T21:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.151230000000002,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13144,"TRANSGRIDV5_20161215152814","2014-09-13T14:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.450099999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13148,"TRANSGRIDV5_20161215152814","2014-09-13T06:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.398040000000002,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13166,"TRANSGRIDV5_20161215152814","2014-09-13T13:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.321,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13175,"TRANSGRIDV5_20161215152814","2014-09-13T14:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.403130000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13181,"TRANSGRIDV5_20161215152814","2014-09-13T13:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.38716,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13192,"TRANSGRIDV5_20161215152814","2014-09-13T21:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.859260000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13207,"TRANSGRIDV5_20161215152814","2014-09-13T00:35:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-26.994150000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13213,"TRANSGRIDV5_20161215152814","2014-09-13T03:00:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-23.441420000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13222,"TRANSGRIDV5_20161215152814","2014-09-13T11:20:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-19.862459999999999,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13240,"TRANSGRIDV5_20161215152814","2014-09-13T06:30:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-10.73976,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13244,"TRANSGRIDV5_20161215152814","2014-09-13T04:05:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-40.306620000000002,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13257,"TRANSGRIDV5_20161215152814","2014-09-13T01:50:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-28.447620000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13270,"TRANSGRIDV5_20161215152814","2014-09-13T08:00:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-25.844889999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13274,"TRANSGRIDV5_20161215152814","2014-09-13T05:30:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-25.415839999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13285,"TRANSGRIDV5_20161215152814","2014-09-13T03:45:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-24.412040000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13295,"TRANSGRIDV5_20161215152814","2014-09-13T06:25:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-23.8584,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13311,"TRANSGRIDV5_20161215152814","2014-09-13T02:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-21.24689,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13317,"TRANSGRIDV5_20161215152814","2014-09-13T13:00:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-21.24155,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13328,"TRANSGRIDV5_20161215152814","2014-09-13T03:35:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-20.29665,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13343,"TRANSGRIDV5_20161215152814","2014-09-13T22:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-18.209869999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13355,"TRANSGRIDV5_20161215152814","2014-09-13T02:50:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-17.805440000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13358,"TRANSGRIDV5_20161215152814","2014-09-13T07:25:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-17.49147,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13372,"TRANSGRIDV5_20161215152814","2014-09-13T06:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.296150000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13380,"TRANSGRIDV5_20161215152814","2014-09-13T07:20:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.008189999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13399,"TRANSGRIDV5_20161215152814","2014-09-13T14:10:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-13.2539,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13406,"TRANSGRIDV5_20161215152814","2014-09-13T15:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-13.2539,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13416,"TRANSGRIDV5_20161215152814","2014-09-13T08:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-10.59937,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13421,"TRANSGRIDV5_20161215152814","2014-09-13T20:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-10.413040000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13437,"TRANSGRIDV5_20161215152814","2014-09-14T00:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.65738,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13447,"TRANSGRIDV5_20161215152814","2014-09-14T22:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.503830000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13454,"TRANSGRIDV5_20161215152814","2014-09-14T10:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.381319999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13469,"TRANSGRIDV5_20161215152814","2014-09-14T23:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.044809999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13481,"TRANSGRIDV5_20161215152814","2014-09-14T06:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.268450000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13484,"TRANSGRIDV5_20161215152814","2014-09-14T05:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.24943,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13505,"TRANSGRIDV5_20161215152814","2014-09-14T23:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.466439999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13514,"TRANSGRIDV5_20161215152814","2014-09-14T06:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.35801,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13516,"TRANSGRIDV5_20161215152814","2014-09-14T02:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.315149999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13531,"TRANSGRIDV5_20161215152814","2014-09-14T09:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.489140000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13542,"TRANSGRIDV5_20161215152814","2014-09-14T06:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.460380000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13548,"TRANSGRIDV5_20161215152814","2014-09-14T11:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.24286,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13568,"TRANSGRIDV5_20161215152814","2014-09-14T21:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.660640000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13569,"TRANSGRIDV5_20161215152814","2014-09-14T21:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.453530000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13583,"TRANSGRIDV5_20161215152814","2014-09-14T03:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.24447,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13596,"TRANSGRIDV5_20161215152814","2014-09-14T11:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.021750000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13605,"TRANSGRIDV5_20161215152814","2014-09-14T07:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.68622,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13613,"TRANSGRIDV5_20161215152814","2014-09-14T14:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.4795,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13631,"TRANSGRIDV5_20161215152814","2014-09-14T04:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.13387,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13640,"TRANSGRIDV5_20161215152814","2014-09-14T00:35:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-21.24155,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13646,"TRANSGRIDV5_20161215152814","2014-09-14T04:30:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-18.209900000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13661,"TRANSGRIDV5_20161215152814","2014-09-14T10:15:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-12.87021,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13672,"TRANSGRIDV5_20161215152814","2014-09-14T14:05:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-10.55198,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13678,"TRANSGRIDV5_20161215152814","2014-09-14T08:30:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-27.550719999999998,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13694,"TRANSGRIDV5_20161215152814","2014-09-14T23:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-21.241389999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13704,"TRANSGRIDV5_20161215152814","2014-09-14T04:45:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-20.314640000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13711,"TRANSGRIDV5_20161215152814","2014-09-14T05:35:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-18.770869999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13719,"TRANSGRIDV5_20161215152814","2014-09-14T05:55:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-18.209900000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13728,"TRANSGRIDV5_20161215152814","2014-09-14T03:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-17.020879999999998,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13741,"TRANSGRIDV5_20161215152814","2014-09-14T02:30:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.28548,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13755,"TRANSGRIDV5_20161215152814","2014-09-14T08:50:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-15.388579999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13767,"TRANSGRIDV5_20161215152814","2014-09-14T09:45:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-15.388450000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13772,"TRANSGRIDV5_20161215152814","2014-09-14T12:10:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-15.169549999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13782,"TRANSGRIDV5_20161215152814","2014-09-14T21:20:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-14.431559999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13793,"TRANSGRIDV5_20161215152814","2014-09-14T03:20:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-13.32822,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13808,"TRANSGRIDV5_20161215152814","2014-09-14T03:40:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-13.151719999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13820,"TRANSGRIDV5_20161215152814","2014-09-14T13:25:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-11.82827,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13830,"TRANSGRIDV5_20161215152814","2014-09-14T14:40:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-11.41319,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13837,"TRANSGRIDV5_20161215152814","2014-09-14T16:10:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-10.7471,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13845,"TRANSGRIDV5_20161215152814","2014-09-15T14:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-24.996680000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13854,"TRANSGRIDV5_20161215152814","2014-09-15T10:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.537459999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13871,"TRANSGRIDV5_20161215152814","2014-09-15T04:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.79973,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13875,"TRANSGRIDV5_20161215152814","2014-09-15T04:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.698450000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13886,"TRANSGRIDV5_20161215152814","2014-09-15T10:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.098310000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13903,"TRANSGRIDV5_20161215152814","2014-09-15T13:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.745100000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13914,"TRANSGRIDV5_20161215152814","2014-09-15T00:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.962949999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13918,"TRANSGRIDV5_20161215152814","2014-09-15T00:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.55218,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13935,"TRANSGRIDV5_20161215152814","2014-09-15T11:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.609220000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13944,"TRANSGRIDV5_20161215152814","2014-09-15T09:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.758240000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13952,"TRANSGRIDV5_20161215152814","2014-09-15T00:55:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-18.209900000000001,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13966,"TRANSGRIDV5_20161215152814","2014-09-15T12:10:00","Q>NIL_MUTE_757","Q-NIL","2014-09-02",1,-11.64574,"Out= Nil, ECS for managing 757 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13969,"TRANSGRIDV5_20161215152814","2014-09-15T13:40:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-24.52214,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13981,"TRANSGRIDV5_20161215152814","2014-09-15T00:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-18.806460000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[13996,"TRANSGRIDV5_20161215152814","2014-09-15T10:35:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-17.204229999999999,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14007,"TRANSGRIDV5_20161215152814","2014-09-15T04:40:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-15.949870000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14017,"TRANSGRIDV5_20161215152814","2014-09-15T13:10:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-14.43169,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14022,"TRANSGRIDV5_20161215152814","2014-09-15T13:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-14.36834,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14034,"TRANSGRIDV5_20161215152814","2014-09-15T04:30:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-13.253740000000001,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14044,"TRANSGRIDV5_20161215152814","2014-09-15T01:30:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-11.27928,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14061,"TRANSGRIDV5_20161215152814","2014-09-15T18:25:00","V>>V_KTS_TX_A2_2_P","V-KTTX_A2_OR_A4_P","2014-03-04",1,-34.809899999999999,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, parallel mode, feedback","OUTAGE","OTHER","Keilor A2 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[14070,"TRANSGRIDV5_20161215152814","2014-09-16T18:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12705.564469999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14078,"TRANSGRIDV5_20161215152814","2014-09-16T00:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.70426,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14085,"TRANSGRIDV5_20161215152814","2014-09-16T01:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.152329999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14102,"TRANSGRIDV5_20161215152814","2014-09-16T01:15:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-11.27928,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14111,"TRANSGRIDV5_20161215152814","2014-09-17T06:50:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-10.92188,"DC Link Control Issue Constraint for Terranora","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14117,"TRANSGRIDV5_20161215152814","2014-09-18T01:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.636189999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14128,"TRANSGRIDV5_20161215152814","2014-09-18T01:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.99173,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14143,"TRANSGRIDV5_20161215152814","2014-09-18T01:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.497490000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14149,"TRANSGRIDV5_20161215152814","2014-09-19T06:50:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-100.1,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14158,"TRANSGRIDV5_20161215152814","2014-09-19T09:35:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-92.117009999999993,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14176,"TRANSGRIDV5_20161215152814","2014-09-19T07:10:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-87.662679999999995,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14180,"TRANSGRIDV5_20161215152814","2014-09-19T05:45:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-86.760199999999998,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14193,"TRANSGRIDV5_20161215152814","2014-09-19T05:35:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-82.860299999999995,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14206,"TRANSGRIDV5_20161215152814","2014-09-19T04:50:00","N_GUNNING1_ZERO","N-GUNNING1_ZERO","2013-08-21",1,-76.554019999999994,"Gunning unit upper limit of 0 MW","OUTAGE","OTHER","Goulburn - Yass 971 132kV Line","REGULATED",99,"Non Inclusion","UNPLANNED",0,"Forced outage on Essential Energy's part of the line"]
[14220,"TRANSGRIDV5_20161215152814","2014-09-19T01:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.06578,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14221,"TRANSGRIDV5_20161215152814","2014-09-19T01:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.993840000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14241,"TRANSGRIDV5_20161215152814","2014-09-19T03:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.23359,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14247,"TRANSGRIDV5_20161215152814","2014-09-19T10:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.99494,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14258,"TRANSGRIDV5_20161215152814","2014-09-19T01:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.315239999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14269,"TRANSGRIDV5_20161215152814","2014-09-19T01:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.255019999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14279,"TRANSGRIDV5_20161215152814","2014-09-19T01:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.338900000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14291,"TRANSGRIDV5_20161215152814","2014-09-19T00:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.13916,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14305,"TRANSGRIDV5_20161215152814","2014-09-19T11:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.60018,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14308,"TRANSGRIDV5_20161215152814","2014-09-19T04:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.42975,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14316,"TRANSGRIDV5_20161215152814","2014-09-20T03:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.40593,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14335,"TRANSGRIDV5_20161215152814","2014-09-20T01:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.02702,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14342,"TRANSGRIDV5_20161215152814","2014-09-21T06:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-32.771650000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14352,"TRANSGRIDV5_20161215152814","2014-09-21T05:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.461740000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14368,"TRANSGRIDV5_20161215152814","2014-09-21T22:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.695639999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14373,"TRANSGRIDV5_20161215152814","2014-09-21T08:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.60502,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14383,"TRANSGRIDV5_20161215152814","2014-09-22T04:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.049939999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14390,"TRANSGRIDV5_20161215152814","2014-09-22T01:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.43375,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14405,"TRANSGRIDV5_20161215152814","2014-09-23T18:25:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-897.27806999999996,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14417,"TRANSGRIDV5_20161215152814","2014-09-23T18:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-892.07264999999995,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14431,"TRANSGRIDV5_20161215152814","2014-09-23T17:10:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.42939000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14434,"TRANSGRIDV5_20161215152814","2014-09-23T15:20:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.17146000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14446,"TRANSGRIDV5_20161215152814","2014-09-23T17:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.77,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14455,"TRANSGRIDV5_20161215152814","2014-09-23T16:15:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.54876000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14472,"TRANSGRIDV5_20161215152814","2014-09-23T14:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-888.77,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14478,"TRANSGRIDV5_20161215152814","2014-09-23T20:55:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-888.77,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14494,"TRANSGRIDV5_20161215152814","2014-09-23T11:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-887.86596999999995,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14504,"TRANSGRIDV5_20161215152814","2014-09-23T12:00:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-887.63508000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14515,"TRANSGRIDV5_20161215152814","2014-09-23T12:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-887.41063999999994,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14519,"TRANSGRIDV5_20161215152814","2014-09-23T21:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-887.30032000000006,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14532,"TRANSGRIDV5_20161215152814","2014-09-23T12:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-886.57,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14541,"TRANSGRIDV5_20161215152814","2014-09-23T21:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-886.55,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14549,"TRANSGRIDV5_20161215152814","2014-09-23T22:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-883.59770000000003,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14567,"TRANSGRIDV5_20161215152814","2014-09-23T07:25:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-27.78,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14576,"TRANSGRIDV5_20161215152814","2014-09-23T23:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.3725,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14582,"TRANSGRIDV5_20161215152814","2014-09-23T00:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.097799999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14597,"TRANSGRIDV5_20161215152814","2014-09-24T04:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.57086,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14608,"TRANSGRIDV5_20161215152814","2014-09-24T04:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.76056,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14614,"TRANSGRIDV5_20161215152814","2014-09-24T02:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.34281,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14630,"TRANSGRIDV5_20161215152814","2014-09-24T08:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-27.788129999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14641,"TRANSGRIDV5_20161215152814","2014-09-24T12:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.064969999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14645,"TRANSGRIDV5_20161215152814","2014-09-24T15:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.56073,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14658,"TRANSGRIDV5_20161215152814","2014-09-24T12:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.40747,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14671,"TRANSGRIDV5_20161215152814","2014-09-24T15:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.795500000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[14677,"TRANSGRIDV5_20161215152814","2014-09-24T18:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-895.10333000000003,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14691,"TRANSGRIDV5_20161215152814","2014-09-24T09:00:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.96082999999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14703,"TRANSGRIDV5_20161215152814","2014-09-24T09:20:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.43691999999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14708,"TRANSGRIDV5_20161215152814","2014-09-24T19:00:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.02,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14718,"TRANSGRIDV5_20161215152814","2014-09-24T07:15:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.78084999999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14729,"TRANSGRIDV5_20161215152814","2014-09-24T17:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.73721,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14744,"TRANSGRIDV5_20161215152814","2014-09-24T15:00:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.46843000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14756,"TRANSGRIDV5_20161215152814","2014-09-24T19:20:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.27877999999998,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14766,"TRANSGRIDV5_20161215152814","2014-09-24T09:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.01089000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14773,"TRANSGRIDV5_20161215152814","2014-09-24T17:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-888.79390000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14781,"TRANSGRIDV5_20161215152814","2014-09-24T11:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-888.09613000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14790,"TRANSGRIDV5_20161215152814","2014-09-24T20:20:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-887.61267999999995,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14807,"TRANSGRIDV5_20161215152814","2014-09-24T13:50:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-886.55,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14811,"TRANSGRIDV5_20161215152814","2014-09-24T20:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-886.55,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14822,"TRANSGRIDV5_20161215152814","2014-09-24T13:00:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-882.56822,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14838,"TRANSGRIDV5_20161215152814","2014-09-24T23:25:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-881.20316000000003,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14844,"TRANSGRIDV5_20161215152814","2014-09-24T06:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-880.02678000000003,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14855,"TRANSGRIDV5_20161215152814","2014-09-24T13:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.74477999999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14870,"TRANSGRIDV5_20161215152814","2014-09-24T12:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.42038000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14880,"TRANSGRIDV5_20161215152814","2014-09-24T12:10:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.42,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14888,"TRANSGRIDV5_20161215152814","2014-09-24T21:55:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-877.71073000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14902,"TRANSGRIDV5_20161215152814","2014-09-24T05:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-877.37005999999997,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14915,"TRANSGRIDV5_20161215152814","2014-09-24T01:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-876.58,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14917,"TRANSGRIDV5_20161215152814","2014-09-24T02:10:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-876.58,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14932,"TRANSGRIDV5_20161215152814","2014-09-24T00:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-873.27,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14943,"TRANSGRIDV5_20161215152814","2014-09-24T03:15:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-872.71,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14953,"TRANSGRIDV5_20161215152814","2014-09-24T03:10:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-865.79012999999998,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14958,"TRANSGRIDV5_20161215152814","2014-09-24T02:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-858.83965999999998,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14970,"TRANSGRIDV5_20161215152814","2014-09-24T03:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.73423,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14980,"TRANSGRIDV5_20161215152814","2014-09-24T02:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.632379999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[14997,"TRANSGRIDV5_20161215152814","2014-09-24T05:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.931509999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15006,"TRANSGRIDV5_20161215152814","2014-09-24T15:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.08042,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15014,"TRANSGRIDV5_20161215152814","2014-09-24T00:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.519780000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15021,"TRANSGRIDV5_20161215152814","2014-09-24T00:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.258979999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15035,"TRANSGRIDV5_20161215152814","2014-09-24T00:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.686579999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15047,"TRANSGRIDV5_20161215152814","2014-09-24T11:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.16633,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15053,"TRANSGRIDV5_20161215152814","2014-09-25T05:55:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,11.99,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8M 330kV Line","REGULATED",3,"3rd Party Outage","UNPLANNED",0,"Auto reclose failure at Powerlink's Bulli Creek substation"]
[15064,"TRANSGRIDV5_20161215152814","2014-09-25T10:15:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-892.62630999999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15079,"TRANSGRIDV5_20161215152814","2014-09-25T09:10:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-890.92559000000006,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15085,"TRANSGRIDV5_20161215152814","2014-09-25T09:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-889.56583000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15105,"TRANSGRIDV5_20161215152814","2014-09-25T08:05:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-884.76422000000002,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15112,"TRANSGRIDV5_20161215152814","2014-09-25T06:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-883.12597000000005,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15116,"TRANSGRIDV5_20161215152814","2014-09-25T05:25:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-881.73024999999996,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15129,"TRANSGRIDV5_20161215152814","2014-09-25T01:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.42025000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15142,"TRANSGRIDV5_20161215152814","2014-09-25T00:40:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.42012,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15156,"TRANSGRIDV5_20161215152814","2014-09-25T06:15:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-879.26697000000001,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15168,"TRANSGRIDV5_20161215152814","2014-09-25T01:30:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-877.56431999999995,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15177,"TRANSGRIDV5_20161215152814","2014-09-25T01:25:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-876.59,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15183,"TRANSGRIDV5_20161215152814","2014-09-25T03:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2013-08-21",1,-876.57,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15194,"TRANSGRIDV5_20161215152814","2014-09-25T01:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.467090000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15205,"TRANSGRIDV5_20161215152814","2014-09-26T23:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.559850000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15211,"TRANSGRIDV5_20161215152814","2014-09-26T02:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.079610000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15231,"TRANSGRIDV5_20161215152814","2014-09-26T23:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.87086,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15238,"TRANSGRIDV5_20161215152814","2014-09-26T01:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.469340000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15246,"TRANSGRIDV5_20161215152814","2014-09-26T04:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.14292,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15263,"TRANSGRIDV5_20161215152814","2014-09-26T01:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.28641,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15271,"TRANSGRIDV5_20161215152814","2014-09-26T00:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.77178,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15278,"TRANSGRIDV5_20161215152814","2014-09-26T02:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.2905,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15288,"TRANSGRIDV5_20161215152814","2014-09-27T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-32.653889999999997,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15304,"TRANSGRIDV5_20161215152814","2014-09-27T03:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-24.379200000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15309,"TRANSGRIDV5_20161215152814","2014-09-27T00:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.765699999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15319,"TRANSGRIDV5_20161215152814","2014-09-27T03:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.917649999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15336,"TRANSGRIDV5_20161215152814","2014-09-27T04:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.07583,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15341,"TRANSGRIDV5_20161215152814","2014-09-27T00:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.80397,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15353,"TRANSGRIDV5_20161215152814","2014-09-27T02:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.993840000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15367,"TRANSGRIDV5_20161215152814","2014-09-27T06:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.7813,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15370,"TRANSGRIDV5_20161215152814","2014-09-27T05:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.685460000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15382,"TRANSGRIDV5_20161215152814","2014-09-27T11:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.363200000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15391,"TRANSGRIDV5_20161215152814","2014-09-27T08:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.391690000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15408,"TRANSGRIDV5_20161215152814","2014-09-27T07:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-30.55932,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15418,"TRANSGRIDV5_20161215152814","2014-09-27T01:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.228010000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15423,"TRANSGRIDV5_20161215152814","2014-09-27T00:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.214169999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15435,"TRANSGRIDV5_20161215152814","2014-09-27T03:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.53717,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15445,"TRANSGRIDV5_20161215152814","2014-09-27T02:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.677489999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15455,"TRANSGRIDV5_20161215152814","2014-09-27T03:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.632269999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15468,"TRANSGRIDV5_20161215152814","2014-09-27T07:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.52933,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15477,"TRANSGRIDV5_20161215152814","2014-09-27T08:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.94786,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15485,"TRANSGRIDV5_20161215152814","2014-09-27T12:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.05705,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15503,"TRANSGRIDV5_20161215152814","2014-09-27T09:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.210089999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15512,"TRANSGRIDV5_20161215152814","2014-09-27T09:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.376659999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15518,"TRANSGRIDV5_20161215152814","2014-09-27T12:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.332700000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15533,"TRANSGRIDV5_20161215152814","2014-09-27T11:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.559850000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15544,"TRANSGRIDV5_20161215152814","2014-09-28T12:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.827059999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15550,"TRANSGRIDV5_20161215152814","2014-09-28T01:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-17.135400000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15566,"TRANSGRIDV5_20161215152814","2014-09-28T18:00:00","V::N_HWSM_V4","V-HWSM","2014-02-21",1,-10.179180000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[15577,"TRANSGRIDV5_20161215152814","2014-09-28T01:30:00","V>>V_MLTS_TX_2A_R","V-MLTX_R","2014-03-04",1,-34.670999999999999,"Out = Moorabool A1 or A2 500/220kV transformer, avoid O/L South Morang 500/330kV (F2) transformer for NIL trip, Yallourn unit 1 in 500kV mode, radial mode at Hazelwood","OUTAGE","OTHER","Moorabool 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[15581,"TRANSGRIDV5_20161215152814","2014-09-28T09:40:00","V>>V_MLTS_TX_2A_R","V-MLTX_R","2014-03-04",1,-13.00942,"Out = Moorabool A1 or A2 500/220kV transformer, avoid O/L South Morang 500/330kV (F2) transformer for NIL trip, Yallourn unit 1 in 500kV mode, radial mode at Hazelwood","OUTAGE","OTHER","Moorabool 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[15594,"TRANSGRIDV5_20161215152814","2014-09-28T01:35:00","V>>V_MLTS_TX_2A_R","V-MLTX_R","2014-03-04",1,-11.005000000000001,"Out = Moorabool A1 or A2 500/220kV transformer, avoid O/L South Morang 500/330kV (F2) transformer for NIL trip, Yallourn unit 1 in 500kV mode, radial mode at Hazelwood","OUTAGE","OTHER","Moorabool 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[15607,"TRANSGRIDV5_20161215152814","2014-09-29T23:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.694470000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15615,"TRANSGRIDV5_20161215152814","2014-09-29T22:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.81865,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15622,"TRANSGRIDV5_20161215152814","2014-09-29T22:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.605,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15632,"TRANSGRIDV5_20161215152814","2014-09-29T01:20:00","V>>V_MLTS_TX_2A_R","V-MLTX_R","2014-03-04",1,-11.21599,"Out = Moorabool A1 or A2 500/220kV transformer, avoid O/L South Morang 500/330kV (F2) transformer for NIL trip, Yallourn unit 1 in 500kV mode, radial mode at Hazelwood","OUTAGE","OTHER","Moorabool 500kV Transformer","REGULATED",99,"Non Inclusion",null,0]
[15648,"TRANSGRIDV5_20161215152814","2014-09-30T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.932200000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15654,"TRANSGRIDV5_20161215152814","2014-09-30T23:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.065939999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15665,"TRANSGRIDV5_20161215152814","2014-09-30","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.34281,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15680,"TRANSGRIDV5_20161215152814","2014-09-30T01:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.662320000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15692,"TRANSGRIDV5_20161215152814","2014-09-30T01:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.52101,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15702,"TRANSGRIDV5_20161215152814","2014-09-30T00:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.3691,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15709,"TRANSGRIDV5_20161215152814","2014-09-30T15:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.40753,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15717,"TRANSGRIDV5_20161215152814","2014-10-01T06:55:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-10-01",1,22.938960000000002,"NSW1-QLD1 >= MIN(-402, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[15736,"TRANSGRIDV5_20161215152814","2014-10-01T00:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.20533,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15743,"TRANSGRIDV5_20161215152814","2014-10-02T06:50:00","#R011210_002_RAMP_F","#R011210_RAMP","2014-10-02",1,-30.140889999999999,"Hard Ramping constraint for constraint N_X_MBTE_3B, Effective Date: 25/11/2013, Version: 1","OUTAGE","RAMP","Terranora Interconnector","REGULATED",10,"Ramping Constraint","PLANNED",0]
[15757,"TRANSGRIDV5_20161215152814","2014-10-02T08:45:00","F_Q++ARTW_L60","F-N-ARTW_85","2013-08-21",1,10.505979999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[15758,"TRANSGRIDV5_20161215152814","2014-10-02T09:35:00","F_Q++ARTW_L60","F-N-ARTW_85","2013-08-21",1,10.431150000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[15774,"TRANSGRIDV5_20161215152814","2014-10-02T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.46861,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15780,"TRANSGRIDV5_20161215152814","2014-10-02T01:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.44852,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15791,"TRANSGRIDV5_20161215152814","2014-10-02T01:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.79946,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15806,"TRANSGRIDV5_20161215152814","2014-10-02T23:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-19.97167,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15818,"TRANSGRIDV5_20161215152814","2014-10-02T21:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.92812,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15821,"TRANSGRIDV5_20161215152814","2014-10-02T21:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.528970000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15838,"TRANSGRIDV5_20161215152814","2014-10-02T21:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.89959,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15851,"TRANSGRIDV5_20161215152814","2014-10-02T01:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.042259999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15853,"TRANSGRIDV5_20161215152814","2014-10-02T01:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.023949999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15868,"TRANSGRIDV5_20161215152814","2014-10-02T01:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.49568,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15879,"TRANSGRIDV5_20161215152814","2014-10-02T04:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.004300000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15889,"TRANSGRIDV5_20161215152814","2014-10-02T23:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.418189999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15905,"TRANSGRIDV5_20161215152814","2014-10-02T02:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.90743,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15906,"TRANSGRIDV5_20161215152814","2014-10-02T03:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.90742,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15916,"TRANSGRIDV5_20161215152814","2014-10-02T22:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.10286,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[15933,"TRANSGRIDV5_20161215152814","2014-10-03T06:45:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-10-03",1,27.75207,"NSW1-QLD1 >= MIN(-443, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[15942,"TRANSGRIDV5_20161215152814","2014-10-03T09:25:00","F_Q++ARTW_L6","F-N-ARTW_85","2013-08-21",1,10.97531,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[15950,"TRANSGRIDV5_20161215152814","2014-10-03T09:30:00","F_Q++ARTW_L60","F-N-ARTW_85","2013-08-21",1,11.966229999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[15968,"TRANSGRIDV5_20161215152814","2014-10-03T03:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-30.006329999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15971,"TRANSGRIDV5_20161215152814","2014-10-03T03:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-28.924109999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15983,"TRANSGRIDV5_20161215152814","2014-10-03T02:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-27.699929999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[15998,"TRANSGRIDV5_20161215152814","2014-10-03T01:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-23.533190000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16009,"TRANSGRIDV5_20161215152814","2014-10-03T01:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.96556,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16015,"TRANSGRIDV5_20161215152814","2014-10-03T04:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-22.29053,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16031,"TRANSGRIDV5_20161215152814","2014-10-03T05:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.369289999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16041,"TRANSGRIDV5_20161215152814","2014-10-03","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.603020000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16048,"TRANSGRIDV5_20161215152814","2014-10-03T03:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.754239999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16063,"TRANSGRIDV5_20161215152814","2014-10-03T02:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.664719999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16065,"TRANSGRIDV5_20161215152814","2014-10-03T02:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.658049999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16078,"TRANSGRIDV5_20161215152814","2014-10-03T00:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-19.17558,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16092,"TRANSGRIDV5_20161215152814","2014-10-03T01:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.684560000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16104,"TRANSGRIDV5_20161215152814","2014-10-03T05:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.073350000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16113,"TRANSGRIDV5_20161215152814","2014-10-03T05:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.02017,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16119,"TRANSGRIDV5_20161215152814","2014-10-03T06:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.469749999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16130,"TRANSGRIDV5_20161215152814","2014-10-03T05:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.79565,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16141,"TRANSGRIDV5_20161215152814","2014-10-03T23:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.73678,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16157,"TRANSGRIDV5_20161215152814","2014-10-04T03:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.20063,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16167,"TRANSGRIDV5_20161215152814","2014-10-04T01:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.07493,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16174,"TRANSGRIDV5_20161215152814","2014-10-04T23:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.581160000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16182,"TRANSGRIDV5_20161215152814","2014-10-04T09:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.4457,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16195,"TRANSGRIDV5_20161215152814","2014-10-04T15:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.050190000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16208,"TRANSGRIDV5_20161215152814","2014-10-04T09:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.807829999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16212,"TRANSGRIDV5_20161215152814","2014-10-04T10:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.79922,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16223,"TRANSGRIDV5_20161215152814","2014-10-04","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.264239999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16240,"TRANSGRIDV5_20161215152814","2014-10-04T12:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.0192,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16245,"TRANSGRIDV5_20161215152814","2014-10-04T11:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.007849999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16255,"TRANSGRIDV5_20161215152814","2014-10-04T10:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.28444,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16272,"TRANSGRIDV5_20161215152814","2014-10-04T09:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.10435,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16277,"TRANSGRIDV5_20161215152814","2014-10-04T00:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.07865,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16289,"TRANSGRIDV5_20161215152814","2014-10-04T01:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.017910000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16303,"TRANSGRIDV5_20161215152814","2014-10-04","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.558479999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16306,"TRANSGRIDV5_20161215152814","2014-10-04T02:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.533799999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16318,"TRANSGRIDV5_20161215152814","2014-10-04T23:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.978059999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16327,"TRANSGRIDV5_20161215152814","2014-10-04T16:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.815720000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16344,"TRANSGRIDV5_20161215152814","2014-10-04T08:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.7799,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16354,"TRANSGRIDV5_20161215152814","2014-10-04T14:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.71706,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16359,"TRANSGRIDV5_20161215152814","2014-10-04T03:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.66366,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16371,"TRANSGRIDV5_20161215152814","2014-10-04T01:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.98457,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16381,"TRANSGRIDV5_20161215152814","2014-10-04T08:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.298209999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16398,"TRANSGRIDV5_20161215152814","2014-10-04T08:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.70645,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16407,"TRANSGRIDV5_20161215152814","2014-10-04T14:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.647919999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16419,"TRANSGRIDV5_20161215152814","2014-10-05T00:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.08588,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16422,"TRANSGRIDV5_20161215152814","2014-10-05T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.077279999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16439,"TRANSGRIDV5_20161215152814","2014-10-05T23:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.220050000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16448,"TRANSGRIDV5_20161215152814","2014-10-05T09:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.82067,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16454,"TRANSGRIDV5_20161215152814","2014-10-05T02:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.47358,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16469,"TRANSGRIDV5_20161215152814","2014-10-05T01:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.8689,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16480,"TRANSGRIDV5_20161215152814","2014-10-05T01:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-19.488099999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16486,"TRANSGRIDV5_20161215152814","2014-10-05T01:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.556480000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16502,"TRANSGRIDV5_20161215152814","2014-10-05T09:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.786160000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16513,"TRANSGRIDV5_20161215152814","2014-10-05T21:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.83432,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16517,"TRANSGRIDV5_20161215152814","2014-10-05T00:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.798310000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16530,"TRANSGRIDV5_20161215152814","2014-10-05T11:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.6881,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16543,"TRANSGRIDV5_20161215152814","2014-10-05T12:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.62227,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16551,"TRANSGRIDV5_20161215152814","2014-10-05T14:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.272270000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16558,"TRANSGRIDV5_20161215152814","2014-10-05T22:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.28288,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16578,"TRANSGRIDV5_20161215152814","2014-10-05T08:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.607710000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16584,"TRANSGRIDV5_20161215152814","2014-10-05T16:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.515940000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16595,"TRANSGRIDV5_20161215152814","2014-10-06T11:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.022939999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16606,"TRANSGRIDV5_20161215152814","2014-10-06T12:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.4839,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16616,"TRANSGRIDV5_20161215152814","2014-10-06T10:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.97894,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16628,"TRANSGRIDV5_20161215152814","2014-10-06T08:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.90814,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16638,"TRANSGRIDV5_20161215152814","2014-10-06T01:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.4781,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16645,"TRANSGRIDV5_20161215152814","2014-10-06T23:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.50806,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16653,"TRANSGRIDV5_20161215152814","2014-10-06T13:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.34281,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16672,"TRANSGRIDV5_20161215152814","2014-10-06T06:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.359629999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16679,"TRANSGRIDV5_20161215152814","2014-10-06T11:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.767389999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16693,"TRANSGRIDV5_20161215152814","2014-10-06T15:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.096170000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16705,"TRANSGRIDV5_20161215152814","2014-10-06T12:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.03454,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16710,"TRANSGRIDV5_20161215152814","2014-10-06T12:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.020659999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16716,"TRANSGRIDV5_20161215152814","2014-10-06T11:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.978249999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16727,"TRANSGRIDV5_20161215152814","2014-10-06T08:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.50304,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16742,"TRANSGRIDV5_20161215152814","2014-10-06T06:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.06033,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16754,"TRANSGRIDV5_20161215152814","2014-10-06T05:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.65391,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16768,"TRANSGRIDV5_20161215152814","2014-10-06T15:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.56893,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16775,"TRANSGRIDV5_20161215152814","2014-10-06T07:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.19821,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16783,"TRANSGRIDV5_20161215152814","2014-10-06T15:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.49175,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16792,"TRANSGRIDV5_20161215152814","2014-10-07T08:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.180430000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16809,"TRANSGRIDV5_20161215152814","2014-10-07T10:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.49525,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16815,"TRANSGRIDV5_20161215152814","2014-10-07T05:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.011240000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16825,"TRANSGRIDV5_20161215152814","2014-10-07T10:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.87791,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16841,"TRANSGRIDV5_20161215152814","2014-10-07T23:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.608239999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16852,"TRANSGRIDV5_20161215152814","2014-10-07T08:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.731300000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16863,"TRANSGRIDV5_20161215152814","2014-10-07T11:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.65504,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16869,"TRANSGRIDV5_20161215152814","2014-10-07T22:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.65504,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16878,"TRANSGRIDV5_20161215152814","2014-10-07T05:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.25329,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16886,"TRANSGRIDV5_20161215152814","2014-10-07T12:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.95195,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16904,"TRANSGRIDV5_20161215152814","2014-10-07T12:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.82001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16907,"TRANSGRIDV5_20161215152814","2014-10-07T11:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.81296,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16919,"TRANSGRIDV5_20161215152814","2014-10-07T08:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.46416,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16934,"TRANSGRIDV5_20161215152814","2014-10-07T13:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.59714,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16945,"TRANSGRIDV5_20161215152814","2014-10-07T06:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.25606,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16951,"TRANSGRIDV5_20161215152814","2014-10-08T06:30:00","N^^V_NIL_1","V-NIL","2014-09-24",1,-13.95257,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[16967,"TRANSGRIDV5_20161215152814","2014-10-08T01:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.472539999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16978,"TRANSGRIDV5_20161215152814","2014-10-08T04:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.66995,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16982,"TRANSGRIDV5_20161215152814","2014-10-08T01:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.02542,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[16999,"TRANSGRIDV5_20161215152814","2014-10-08T04:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.41301,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17008,"TRANSGRIDV5_20161215152814","2014-10-08T02:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.10243,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17014,"TRANSGRIDV5_20161215152814","2014-10-08T03:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.891,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17028,"TRANSGRIDV5_20161215152814","2014-10-08T01:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.78096,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17040,"TRANSGRIDV5_20161215152814","2014-10-08T00:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-20.437370000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17049,"TRANSGRIDV5_20161215152814","2014-10-08T01:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.083300000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17055,"TRANSGRIDV5_20161215152814","2014-10-08T01:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.024819999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17066,"TRANSGRIDV5_20161215152814","2014-10-08T02:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.208489999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17077,"TRANSGRIDV5_20161215152814","2014-10-08T02:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.88936,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17093,"TRANSGRIDV5_20161215152814","2014-10-08T05:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.155469999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17103,"TRANSGRIDV5_20161215152814","2014-10-09T23:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.725759999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17110,"TRANSGRIDV5_20161215152814","2014-10-09T01:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.016579999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17118,"TRANSGRIDV5_20161215152814","2014-10-09T04:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.49776,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17131,"TRANSGRIDV5_20161215152814","2014-10-09T02:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.66066,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17144,"TRANSGRIDV5_20161215152814","2014-10-09T21:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.83806,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17148,"TRANSGRIDV5_20161215152814","2014-10-09T22:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.00779,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17159,"TRANSGRIDV5_20161215152814","2014-10-09T01:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.238160000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17175,"TRANSGRIDV5_20161215152814","2014-10-09T02:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.796299999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17181,"TRANSGRIDV5_20161215152814","2014-10-09T03:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.313379999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17192,"TRANSGRIDV5_20161215152814","2014-10-09T04:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.352969999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17207,"TRANSGRIDV5_20161215152814","2014-10-09T05:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.69548,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17213,"TRANSGRIDV5_20161215152814","2014-10-09T22:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.59951,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17225,"TRANSGRIDV5_20161215152814","2014-10-10T03:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.867059999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17239,"TRANSGRIDV5_20161215152814","2014-10-10T01:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.218699999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17252,"TRANSGRIDV5_20161215152814","2014-10-10T02:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.86591,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17254,"TRANSGRIDV5_20161215152814","2014-10-10T00:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.20321,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17273,"TRANSGRIDV5_20161215152814","2014-10-10T03:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.6654,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17280,"TRANSGRIDV5_20161215152814","2014-10-10T22:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.70776,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17290,"TRANSGRIDV5_20161215152814","2014-10-10T01:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-23.819870000000002,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17302,"TRANSGRIDV5_20161215152814","2014-10-10T03:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-19.480239999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17307,"TRANSGRIDV5_20161215152814","2014-10-10T23:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.84178,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17317,"TRANSGRIDV5_20161215152814","2014-10-10T04:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.737590000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17334,"TRANSGRIDV5_20161215152814","2014-10-10T02:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.33173,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17343,"TRANSGRIDV5_20161215152814","2014-10-10T21:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.139609999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17355,"TRANSGRIDV5_20161215152814","2014-10-10T02:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.15335,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17358,"TRANSGRIDV5_20161215152814","2014-10-10T23:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.667730000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17372,"TRANSGRIDV5_20161215152814","2014-10-10T10:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.75916,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17384,"TRANSGRIDV5_20161215152814","2014-10-10T11:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.720470000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17390,"TRANSGRIDV5_20161215152814","2014-10-10T02:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.98082,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17405,"TRANSGRIDV5_20161215152814","2014-10-10T08:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.67604,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17416,"TRANSGRIDV5_20161215152814","2014-10-10T09:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.59482,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17422,"TRANSGRIDV5_20161215152814","2014-10-10T11:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.578200000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17438,"TRANSGRIDV5_20161215152814","2014-10-11T05:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.858450000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17449,"TRANSGRIDV5_20161215152814","2014-10-11T12:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.72907,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17453,"TRANSGRIDV5_20161215152814","2014-10-11T01:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.23631,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17466,"TRANSGRIDV5_20161215152814","2014-10-11T10:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.227219999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17479,"TRANSGRIDV5_20161215152814","2014-10-11T01:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.016579999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17487,"TRANSGRIDV5_20161215152814","2014-10-11T13:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.82629,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17505,"TRANSGRIDV5_20161215152814","2014-10-11T11:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.48419,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17514,"TRANSGRIDV5_20161215152814","2014-10-11T10:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.419140000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17520,"TRANSGRIDV5_20161215152814","2014-10-11T11:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.33386,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17531,"TRANSGRIDV5_20161215152814","2014-10-11T04:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.805110000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17542,"TRANSGRIDV5_20161215152814","2014-10-11T05:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.67426,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17548,"TRANSGRIDV5_20161215152814","2014-10-11T04:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.552,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17568,"TRANSGRIDV5_20161215152814","2014-10-11T06:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.484959999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17569,"TRANSGRIDV5_20161215152814","2014-10-11T00:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-25.21668,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17583,"TRANSGRIDV5_20161215152814","2014-10-11T00:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.82028,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17600,"TRANSGRIDV5_20161215152814","2014-10-11T01:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.769559999999998,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17608,"TRANSGRIDV5_20161215152814","2014-10-11T02:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-18.718730000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17615,"TRANSGRIDV5_20161215152814","2014-10-11T00:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.357479999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17629,"TRANSGRIDV5_20161215152814","2014-10-11T11:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.144690000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17641,"TRANSGRIDV5_20161215152814","2014-10-11T13:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.104939999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17646,"TRANSGRIDV5_20161215152814","2014-10-11T10:50:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.077940000000002,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17663,"TRANSGRIDV5_20161215152814","2014-10-11T23:35:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-16.688179999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17673,"TRANSGRIDV5_20161215152814","2014-10-11T04:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.611090000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17678,"TRANSGRIDV5_20161215152814","2014-10-11T13:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-15.0312,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17690,"TRANSGRIDV5_20161215152814","2014-10-11T05:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.36134,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17704,"TRANSGRIDV5_20161215152814","2014-10-11T06:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.778269999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17711,"TRANSGRIDV5_20161215152814","2014-10-11T23:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.77056,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17719,"TRANSGRIDV5_20161215152814","2014-10-11T07:45:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.752280000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17728,"TRANSGRIDV5_20161215152814","2014-10-11T22:15:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.58268,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17745,"TRANSGRIDV5_20161215152814","2014-10-11T04:10:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.428839999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17755,"TRANSGRIDV5_20161215152814","2014-10-11T23:35:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-182.08010999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17767,"TRANSGRIDV5_20161215152814","2014-10-12T06:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.416699999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17772,"TRANSGRIDV5_20161215152814","2014-10-12T00:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.71973,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17782,"TRANSGRIDV5_20161215152814","2014-10-12T09:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.745050000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17799,"TRANSGRIDV5_20161215152814","2014-10-12T15:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.580450000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17805,"TRANSGRIDV5_20161215152814","2014-10-12T04:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.361520000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17814,"TRANSGRIDV5_20161215152814","2014-10-12T11:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.95289,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17822,"TRANSGRIDV5_20161215152814","2014-10-12T14:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.88396,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17840,"TRANSGRIDV5_20161215152814","2014-10-12T10:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.426360000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[17843,"TRANSGRIDV5_20161215152814","2014-10-12T07:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-21.389849999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17855,"TRANSGRIDV5_20161215152814","2014-10-12T09:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-17.096920000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17870,"TRANSGRIDV5_20161215152814","2014-10-12T07:25:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.70866,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17881,"TRANSGRIDV5_20161215152814","2014-10-12T15:05:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-14.013500000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17887,"TRANSGRIDV5_20161215152814","2014-10-12T07:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-13.37541,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17903,"TRANSGRIDV5_20161215152814","2014-10-12T10:40:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.78243,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17914,"TRANSGRIDV5_20161215152814","2014-10-12T14:00:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.730930000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17918,"TRANSGRIDV5_20161215152814","2014-10-12T13:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-12.72357,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17935,"TRANSGRIDV5_20161215152814","2014-10-12T21:55:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-11.68571,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17944,"TRANSGRIDV5_20161215152814","2014-10-12T08:30:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.82978,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17952,"TRANSGRIDV5_20161215152814","2014-10-12T16:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.582129999999999,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17959,"TRANSGRIDV5_20161215152814","2014-10-12T08:20:00","Q:N_AR_2L-G_-200","Q-X_BC_CB8L2_CB99012","2014-01-08",1,-10.493930000000001,"Nominated Offset -200MW, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17969,"TRANSGRIDV5_20161215152814","2014-10-12T01:10:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-12.359540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[17981,"TRANSGRIDV5_20161215152814","2014-10-13T22:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.198399999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[17991,"TRANSGRIDV5_20161215152814","2014-10-13T14:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,12.709820000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18002,"TRANSGRIDV5_20161215152814","2014-10-13T13:15:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.32724,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18013,"TRANSGRIDV5_20161215152814","2014-10-13T06:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-30.211210000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18029,"TRANSGRIDV5_20161215152814","2014-10-13T07:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.838059999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18039,"TRANSGRIDV5_20161215152814","2014-10-13T07:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.375070000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18046,"TRANSGRIDV5_20161215152814","2014-10-13T10:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.4391,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18054,"TRANSGRIDV5_20161215152814","2014-10-13T09:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.67516,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18067,"TRANSGRIDV5_20161215152814","2014-10-13T22:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.82382,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18080,"TRANSGRIDV5_20161215152814","2014-10-13T21:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.22316,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18094,"TRANSGRIDV5_20161215152814","2014-10-13T10:35:00","V::N_JNWGQE_R","N-JNWG_RADIAL","2013-08-21",1,-10.78694,"Out = Jindera to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Jindera - Wagga330 62 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[18095,"TRANSGRIDV5_20161215152814","2014-10-13T10:50:00","V::N_JNWGVD_R","N-JNWG_RADIAL","2013-08-21",1,-20.28716,"Out = Jindera to Wagga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, VIC accelerates, segment 1","OUTAGE","OTHER","Jindera - Wagga330 62 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[18111,"TRANSGRIDV5_20161215152814","2014-10-13T10:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.011979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[18117,"TRANSGRIDV5_20161215152814","2014-10-14T01:50:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,18.22138,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18128,"TRANSGRIDV5_20161215152814","2014-10-14T23:40:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,14.70673,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18143,"TRANSGRIDV5_20161215152814","2014-10-14T05:20:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.24995,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18149,"TRANSGRIDV5_20161215152814","2014-10-14T04:35:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.93858,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18158,"TRANSGRIDV5_20161215152814","2014-10-14T22:55:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.026300000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18176,"TRANSGRIDV5_20161215152814","2014-10-14T12:05:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.37994,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18184,"TRANSGRIDV5_20161215152814","2014-10-14T10:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,13.65456,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18190,"TRANSGRIDV5_20161215152814","2014-10-14T05:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,12.66976,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18209,"TRANSGRIDV5_20161215152814","2014-10-14T15:05:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.00666,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18216,"TRANSGRIDV5_20161215152814","2014-10-14T02:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.43069,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18226,"TRANSGRIDV5_20161215152814","2014-10-14T23:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-33.738500000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18238,"TRANSGRIDV5_20161215152814","2014-10-14T02:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-28.905270000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18243,"TRANSGRIDV5_20161215152814","2014-10-14T04:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-27.043839999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18253,"TRANSGRIDV5_20161215152814","2014-10-14T23:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-24.679290000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18270,"TRANSGRIDV5_20161215152814","2014-10-14T03:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.591080000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18279,"TRANSGRIDV5_20161215152814","2014-10-14T02:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.869700000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18291,"TRANSGRIDV5_20161215152814","2014-10-14T13:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.31128,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18305,"TRANSGRIDV5_20161215152814","2014-10-14T04:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.14508,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18308,"TRANSGRIDV5_20161215152814","2014-10-14T04:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.01286,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18320,"TRANSGRIDV5_20161215152814","2014-10-14T00:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.12434,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18335,"TRANSGRIDV5_20161215152814","2014-10-14T12:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.282819999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18342,"TRANSGRIDV5_20161215152814","2014-10-14T22:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.066229999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18352,"TRANSGRIDV5_20161215152814","2014-10-14T20:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.81916,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18368,"TRANSGRIDV5_20161215152814","2014-10-14T03:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.573370000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18374,"TRANSGRIDV5_20161215152814","2014-10-14T03:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.4231,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18385,"TRANSGRIDV5_20161215152814","2014-10-14T21:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.839040000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18400,"TRANSGRIDV5_20161215152814","2014-10-14T12:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.403779999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18402,"TRANSGRIDV5_20161215152814","2014-10-14T06:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.3657,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18415,"TRANSGRIDV5_20161215152814","2014-10-15T02:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,21.659330000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18423,"TRANSGRIDV5_20161215152814","2014-10-15T08:25:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,20.450949999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18441,"TRANSGRIDV5_20161215152814","2014-10-15T05:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,18.618790000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18450,"TRANSGRIDV5_20161215152814","2014-10-15T23:30:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,16.0746,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18456,"TRANSGRIDV5_20161215152814","2014-10-15T01:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,15.32945,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18467,"TRANSGRIDV5_20161215152814","2014-10-15T10:00:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,13.99996,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18478,"TRANSGRIDV5_20161215152814","2014-10-15T07:20:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.31494,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18494,"TRANSGRIDV5_20161215152814","2014-10-15T04:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.74587,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18504,"TRANSGRIDV5_20161215152814","2014-10-15T19:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,27.665569999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18515,"TRANSGRIDV5_20161215152814","2014-10-15T08:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,23.93186,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18519,"TRANSGRIDV5_20161215152814","2014-10-15T07:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,23.200859999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18532,"TRANSGRIDV5_20161215152814","2014-10-15T08:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,20.439959999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18545,"TRANSGRIDV5_20161215152814","2014-10-15T05:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.900020000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18549,"TRANSGRIDV5_20161215152814","2014-10-15T08:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,17.453250000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18567,"TRANSGRIDV5_20161215152814","2014-10-15T18:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,15.585290000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18577,"TRANSGRIDV5_20161215152814","2014-10-15T23:25:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.795019999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18582,"TRANSGRIDV5_20161215152814","2014-10-15T19:20:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.28548,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18599,"TRANSGRIDV5_20161215152814","2014-10-15T20:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,13.014860000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18609,"TRANSGRIDV5_20161215152814","2014-10-15T13:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,12.6806,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18614,"TRANSGRIDV5_20161215152814","2014-10-15T14:10:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,12.309810000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18626,"TRANSGRIDV5_20161215152814","2014-10-15T11:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.69008,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18640,"TRANSGRIDV5_20161215152814","2014-10-15T11:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.171860000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18647,"TRANSGRIDV5_20161215152814","2014-10-15T22:20:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.677989999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18655,"TRANSGRIDV5_20161215152814","2014-10-15T18:30:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.29677,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18664,"TRANSGRIDV5_20161215152814","2014-10-15T11:50:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.046279999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18681,"TRANSGRIDV5_20161215152814","2014-10-15T08:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-43.556260000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18691,"TRANSGRIDV5_20161215152814","2014-10-15T09:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-37.890770000000003,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18703,"TRANSGRIDV5_20161215152814","2014-10-15T09:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-35.256990000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18708,"TRANSGRIDV5_20161215152814","2014-10-15T06:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-33.093170000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18718,"TRANSGRIDV5_20161215152814","2014-10-15T07:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-30.145869999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18729,"TRANSGRIDV5_20161215152814","2014-10-15T02:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-28.633749999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18744,"TRANSGRIDV5_20161215152814","2014-10-15T10:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-24.982589999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18756,"TRANSGRIDV5_20161215152814","2014-10-15T21:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-22.864350000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18759,"TRANSGRIDV5_20161215152814","2014-10-15T11:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-22.50684,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18776,"TRANSGRIDV5_20161215152814","2014-10-15T12:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.62002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18789,"TRANSGRIDV5_20161215152814","2014-10-15T12:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.97823,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18791,"TRANSGRIDV5_20161215152814","2014-10-15T22:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.904150000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18806,"TRANSGRIDV5_20161215152814","2014-10-15T21:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.05219,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18813,"TRANSGRIDV5_20161215152814","2014-10-15T06:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.397469999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18823,"TRANSGRIDV5_20161215152814","2014-10-15T13:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.616070000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18839,"TRANSGRIDV5_20161215152814","2014-10-15T22:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.092749999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18850,"TRANSGRIDV5_20161215152814","2014-10-15T04:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.984369999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18854,"TRANSGRIDV5_20161215152814","2014-10-15T22:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.803899999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18871,"TRANSGRIDV5_20161215152814","2014-10-15T01:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.336919999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18880,"TRANSGRIDV5_20161215152814","2014-10-15T03:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.974539999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18888,"TRANSGRIDV5_20161215152814","2014-10-15T05:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.594250000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18895,"TRANSGRIDV5_20161215152814","2014-10-15T20:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.058439999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18915,"TRANSGRIDV5_20161215152814","2014-10-15T16:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.823589999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18917,"TRANSGRIDV5_20161215152814","2014-10-15T04:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.585039999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[18932,"TRANSGRIDV5_20161215152814","2014-10-16T04:10:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,17.834849999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18943,"TRANSGRIDV5_20161215152814","2014-10-16T04:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.489789999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18953,"TRANSGRIDV5_20161215152814","2014-10-16T06:45:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,10.3001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18958,"TRANSGRIDV5_20161215152814","2014-10-16T06:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,20.960059999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18975,"TRANSGRIDV5_20161215152814","2014-10-16T02:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.040039999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18982,"TRANSGRIDV5_20161215152814","2014-10-16T22:00:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.171099999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[18990,"TRANSGRIDV5_20161215152814","2014-10-16T05:30:00","F_Q++ARDM_L60","F-I-BCDM_ONE","2013-08-21",1,15,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19003,"TRANSGRIDV5_20161215152814","2014-10-16T04:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-28.88899,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19016,"TRANSGRIDV5_20161215152814","2014-10-16T04:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.490269999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19030,"TRANSGRIDV5_20161215152814","2014-10-16T22:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.068110000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19042,"TRANSGRIDV5_20161215152814","2014-10-16T03:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.483630000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19047,"TRANSGRIDV5_20161215152814","2014-10-16T04:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.9907,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19053,"TRANSGRIDV5_20161215152814","2014-10-16T03:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.62799,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19064,"TRANSGRIDV5_20161215152814","2014-10-16T05:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.85272,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19079,"TRANSGRIDV5_20161215152814","2014-10-16T00:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.68751,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19085,"TRANSGRIDV5_20161215152814","2014-10-16T07:00:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-31.959379999999999,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19105,"TRANSGRIDV5_20161215152814","2014-10-16T08:00:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-19.348369999999999,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19112,"TRANSGRIDV5_20161215152814","2014-10-16T10:40:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-18.912980000000001,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19120,"TRANSGRIDV5_20161215152814","2014-10-16T09:30:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-18.707989999999999,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19129,"TRANSGRIDV5_20161215152814","2014-10-16T09:50:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-18.14594,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19142,"TRANSGRIDV5_20161215152814","2014-10-16T11:10:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-17.230730000000001,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19152,"TRANSGRIDV5_20161215152814","2014-10-16T13:15:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-15.62838,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19162,"TRANSGRIDV5_20161215152814","2014-10-16T12:00:00","N>N-X_9U6_9G2_2","N-X_9U6_9G2","2013-03-04",1,-13.14049,"Out = one of Lismore 132 to Dunoon 132kV line (9U6 or 9U7) and one 132kV line between Mullumbimby and Ballina (9G2, 9G3, 9G4 or 9G5), avoid O/L remaining 132kV line, Qld to NSW limit","OUTAGE","OTHER","Lismore132 - Dunoon 9U7 132kV Line","REGULATED",99,"Non Inclusion",null,0]
[19174,"TRANSGRIDV5_20161215152814","2014-10-17T05:15:00","F_Q++ARDM_L5","F-I-BCDM_ONE","2013-08-21",1,12.910640000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19189,"TRANSGRIDV5_20161215152814","2014-10-17T06:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,24.78979,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19200,"TRANSGRIDV5_20161215152814","2014-10-17T10:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,14.83827,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19206,"TRANSGRIDV5_20161215152814","2014-10-17T11:40:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,13.24248,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19215,"TRANSGRIDV5_20161215152814","2014-10-17T02:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,12.14996,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19227,"TRANSGRIDV5_20161215152814","2014-10-17T09:20:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,11.710140000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19241,"TRANSGRIDV5_20161215152814","2014-10-17T10:45:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.767160000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19244,"TRANSGRIDV5_20161215152814","2014-10-17T12:35:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.561590000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19256,"TRANSGRIDV5_20161215152814","2014-10-17T09:55:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.46176,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19271,"TRANSGRIDV5_20161215152814","2014-10-17T09:05:00","F_Q++ARDM_L6","F-I-BCDM_ONE","2013-08-21",1,10.00051,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Bulli Creek - Dumaresq 8L 330kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Powerlink's outage"]
[19278,"TRANSGRIDV5_20161215152814","2014-10-17T02:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-28.905550000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19288,"TRANSGRIDV5_20161215152814","2014-10-17T05:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-22.40325,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19304,"TRANSGRIDV5_20161215152814","2014-10-17T05:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-19.393149999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19309,"TRANSGRIDV5_20161215152814","2014-10-17T00:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.860589999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19319,"TRANSGRIDV5_20161215152814","2014-10-17T00:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.48115,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19336,"TRANSGRIDV5_20161215152814","2014-10-17T08:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.068049999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19345,"TRANSGRIDV5_20161215152814","2014-10-17T02:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.72907,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19351,"TRANSGRIDV5_20161215152814","2014-10-17T12:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.439540000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19359,"TRANSGRIDV5_20161215152814","2014-10-17T03:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.741160000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19377,"TRANSGRIDV5_20161215152814","2014-10-17T09:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.82376,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19386,"TRANSGRIDV5_20161215152814","2014-10-17T09:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.205730000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19392,"TRANSGRIDV5_20161215152814","2014-10-18T10:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.539849999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19403,"TRANSGRIDV5_20161215152814","2014-10-18T09:50:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.26249,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19414,"TRANSGRIDV5_20161215152814","2014-10-18T06:55:00","V::N_BUDPQE_R","N-BUDP","2013-08-21",1,-16.32442,"Out = Buronga to Darlington Point 220kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Darlington Point - Wagga330 63 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[19430,"TRANSGRIDV5_20161215152814","2014-10-18T07:50:00","V::N_BUDPQE_R","N-BUDP","2013-08-21",1,-10.817349999999999,"Out = Buronga to Darlington Point 220kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Darlington Point - Wagga330 63 330kV Line","REGULATED","INCLUDED",null,"PLANNED",1]
[19440,"TRANSGRIDV5_20161215152814","2014-10-18T23:10:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-10.046469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19451,"TRANSGRIDV5_20161215152814","2014-10-18T08:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.20642,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19455,"TRANSGRIDV5_20161215152814","2014-10-18T10:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.612,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19468,"TRANSGRIDV5_20161215152814","2014-10-18T10:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.979749999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19481,"TRANSGRIDV5_20161215152814","2014-10-19T16:45:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-11.75041,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19485,"TRANSGRIDV5_20161215152814","2014-10-19T00:45:00","V::N_NIL_V4","V-NIL","2014-06-24",1,-11.43069,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19503,"TRANSGRIDV5_20161215152814","2014-10-20T09:05:00","V::N_HWSM_V4","V-HWSM","2014-02-21",1,-20.166989999999998,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19512,"TRANSGRIDV5_20161215152814","2014-10-21T16:55:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-253.01364000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19518,"TRANSGRIDV5_20161215152814","2014-10-21T16:20:00","V^SML_NSWRB_2","V-NIL","2013-08-21",1,-37.173549999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19533,"TRANSGRIDV5_20161215152814","2014-10-22T05:50:00","#R011347_019_RAMP_V","#R011347_RAMP","2014-10-21",1,-13.941369999999999,"Soft Ramping constraint for constraint V::N_JNWOQF_R, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Jindera - Wodonga O60 330 kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[19544,"TRANSGRIDV5_20161215152814","2014-10-22T06:50:00","V::N_JNWOQE_R","I-JNWO_RADIAL","2013-08-21",1,-11.69267,"Out = Jindera to Wodonga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Jindera - Wodonga O60 330 kV Line","REGULATED","INCLUDED","","PLANNED",0.5,"Shared outage between TG & SPAusnet"]
[19550,"TRANSGRIDV5_20161215152814","2014-10-23T16:50:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-45.852130000000002,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19562,"TRANSGRIDV5_20161215152814","2014-10-23T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.632339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19576,"TRANSGRIDV5_20161215152814","2014-10-23T23:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.728859999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19583,"TRANSGRIDV5_20161215152814","2014-10-23T23:45:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-11.940659999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19591,"TRANSGRIDV5_20161215152814","2014-10-24T05:40:00","#R011378_012_RAMP_F","#R011378_RAMP","2014-10-24",1,-20.985869999999998,"Hard Ramping constraint for constraint V::N_HWSM_V4, Effective Date: 21/02/2014, Version: 1","OUTAGE","RAMP","Hazelwood - South Morang 500kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[19610,"TRANSGRIDV5_20161215152814","2014-10-24T05:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.38602,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[19617,"TRANSGRIDV5_20161215152814","2014-10-24T05:35:00","Q:N_30+38+KCTX_AR","N-X_30+38+KCTX","2014-10-10",1,-11.59798,"Out= Liverpool-SydneyWest & Regentville-SydneyWest & one KempsCreek Tie Tx (30+38+KCTX), limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Liverpool - Sydney West 30 330kV Line + Regentville - Sydney West 38 330kV Line + Kemps Creek 500kV No.3 Transformer","REGULATED","INCLUDED","","PLANNED",1]
[19627,"TRANSGRIDV5_20161215152814","2014-10-24T07:20:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-15.3583,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19639,"TRANSGRIDV5_20161215152814","2014-10-24T12:50:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-12.35167,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19644,"TRANSGRIDV5_20161215152814","2014-10-24T09:05:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-11.892939999999999,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19654,"TRANSGRIDV5_20161215152814","2014-10-24T11:40:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-11.03758,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19665,"TRANSGRIDV5_20161215152814","2014-10-24T11:05:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-10.81268,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19680,"TRANSGRIDV5_20161215152814","2014-10-24T09:40:00","V::N_HWSM_Q4","V-HWSM","2014-02-21",1,-10.297610000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[19692,"TRANSGRIDV5_20161215152814","2014-10-24T13:55:00","V::N_JNWOQE_R","I-JNWO_RADIAL","2013-08-21",1,-17.19106,"Out = Jindera to Wodonga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Jindera - Wodonga O60 330 kV Line","REGULATED","INCLUDED",null,"PLANNED",0.5,"Shared outage between TG & SP Ausnet"]
[19695,"TRANSGRIDV5_20161215152814","2014-10-24T20:20:00","V::N_JNWOQF_R","I-JNWO_RADIAL","2013-08-21",1,-16.929729999999999,"Out = Jindera to Wodonga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 3","OUTAGE","OTHER","Jindera - Wodonga O60 330 kV Line","REGULATED","INCLUDED",null,"PLANNED",0.5,"Shared outage between TG & SP Ausnet"]
[19709,"TRANSGRIDV5_20161215152814","2014-10-24T22:15:00","V::N_JNWOQF_R","I-JNWO_RADIAL","2013-08-21",1,-14.605040000000001,"Out = Jindera to Wodonga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 3","OUTAGE","OTHER","Jindera - Wodonga O60 330 kV Line","REGULATED","8(B)","Constraint applied by AEMO doesn't accurately reflect network capability advised by the TNSP","PLANNED",0,"Outage ended at 2203 hrs hence exclusion claimed for 2215 penalty period"]
[19717,"TRANSGRIDV5_20161215152814","2014-10-24T19:40:00","V::N_JNWOQF_R","I-JNWO_RADIAL","2013-08-21",1,-11.86369,"Out = Jindera to Wodonga 330kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 3","OUTAGE","OTHER","Jindera - Wodonga O60 330 kV Line","REGULATED","INCLUDED",null,"PLANNED",0.5,"Shared outage between TG & SP Ausnet"]
[19736,"TRANSGRIDV5_20161215152814","2014-10-24T00:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.93111,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19743,"TRANSGRIDV5_20161215152814","2014-10-24T01:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.77548,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19749,"TRANSGRIDV5_20161215152814","2014-10-24T01:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.714700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19759,"TRANSGRIDV5_20161215152814","2014-10-24T01:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.43479,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19775,"TRANSGRIDV5_20161215152814","2014-10-24T14:35:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-25.800260000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19786,"TRANSGRIDV5_20161215152814","2014-10-25T19:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.26464,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19790,"TRANSGRIDV5_20161215152814","2014-10-25T18:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.72418,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19807,"TRANSGRIDV5_20161215152814","2014-10-25T05:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.547470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19816,"TRANSGRIDV5_20161215152814","2014-10-25T01:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.3629,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19824,"TRANSGRIDV5_20161215152814","2014-10-25T08:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.10689,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19842,"TRANSGRIDV5_20161215152814","2014-10-26T14:35:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,10.67475,"DC Link Control Issue Constraint for Terranora","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19851,"TRANSGRIDV5_20161215152814","2014-10-26T20:50:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-32.425319999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19853,"TRANSGRIDV5_20161215152814","2014-10-26T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-13.92436,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19868,"TRANSGRIDV5_20161215152814","2014-10-26T15:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.255979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19879,"TRANSGRIDV5_20161215152814","2014-10-27T14:00:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-150.42242999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19889,"TRANSGRIDV5_20161215152814","2014-10-27T13:50:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-98.415239999999997,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19905,"TRANSGRIDV5_20161215152814","2014-10-27T14:55:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-52.346049999999998,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19906,"TRANSGRIDV5_20161215152814","2014-10-27T15:05:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-52.120220000000003,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19920,"TRANSGRIDV5_20161215152814","2014-10-27T13:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-23.171189999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19937,"TRANSGRIDV5_20161215152814","2014-10-27T08:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-18.605309999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19939,"TRANSGRIDV5_20161215152814","2014-10-27T08:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-18.515239999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19952,"TRANSGRIDV5_20161215152814","2014-10-27T12:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-15.76632,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19966,"TRANSGRIDV5_20161215152814","2014-10-27T11:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.91419,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19978,"TRANSGRIDV5_20161215152814","2014-10-27T09:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.70758,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[19983,"TRANSGRIDV5_20161215152814","2014-10-27T14:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.938140000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20000,"TRANSGRIDV5_20161215152814","2014-10-27T05:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-30.795999999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20010,"TRANSGRIDV5_20161215152814","2014-10-27T03:15:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-29.961010000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20015,"TRANSGRIDV5_20161215152814","2014-10-27T04:15:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-26.25517,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20031,"TRANSGRIDV5_20161215152814","2014-10-27T02:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-12.89414,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20041,"TRANSGRIDV5_20161215152814","2014-10-27T23:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.985620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20048,"TRANSGRIDV5_20161215152814","2014-10-27T05:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-32.897289999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20056,"TRANSGRIDV5_20161215152814","2014-10-27T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-30.03633,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20065,"TRANSGRIDV5_20161215152814","2014-10-27T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-27.39151,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20078,"TRANSGRIDV5_20161215152814","2014-10-27T05:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-22.68253,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20092,"TRANSGRIDV5_20161215152814","2014-10-27T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-18.046779999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20104,"TRANSGRIDV5_20161215152814","2014-10-27T04:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.926770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20113,"TRANSGRIDV5_20161215152814","2014-10-27T08:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.690249999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20119,"TRANSGRIDV5_20161215152814","2014-10-27T07:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.42464,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20136,"TRANSGRIDV5_20161215152814","2014-10-27T07:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.42681,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20142,"TRANSGRIDV5_20161215152814","2014-10-27T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.579660000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20151,"TRANSGRIDV5_20161215152814","2014-10-27T08:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.927820000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20163,"TRANSGRIDV5_20161215152814","2014-10-27T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.13547,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20177,"TRANSGRIDV5_20161215152814","2014-10-27T05:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.772740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20180,"TRANSGRIDV5_20161215152814","2014-10-27T10:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.063789999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20192,"TRANSGRIDV5_20161215152814","2014-10-28T04:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-21.30949,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20207,"TRANSGRIDV5_20161215152814","2014-10-28T06:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.8744,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20214,"TRANSGRIDV5_20161215152814","2014-10-28T07:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.09314,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20224,"TRANSGRIDV5_20161215152814","2014-10-28T11:40:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-56.088859999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20240,"TRANSGRIDV5_20161215152814","2014-10-28T11:40:00","V>>SML_NIL_5","V-NIL","2014-01-30",1,-54.106650000000002,"Out = NIL, prevent pre-contingent overload of the Ballarat to Bendigo 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20245,"TRANSGRIDV5_20161215152814","2014-10-29T05:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-15.63884,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20255,"TRANSGRIDV5_20161215152814","2014-10-29T00:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.18838,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20272,"TRANSGRIDV5_20161215152814","2014-10-29T00:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.3756,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20281,"TRANSGRIDV5_20161215152814","2014-10-29T00:15:00","V::N_NIL_V3","V-NIL","2014-10-22",1,-11.19317,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20289,"TRANSGRIDV5_20161215152814","2014-10-29T00:25:00","V::N_NIL_V3","V-NIL","2014-10-22",1,-10.268409999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20303,"TRANSGRIDV5_20161215152814","2014-10-30T10:15:00","#R011425_002_RAMP_V","#R011425_RAMP","2014-10-30",1,-20.850850000000001,"Soft Ramping constraint for constraint N_X_MBTE_3B, Effective Date: 25/11/2013, Version: 1","OUTAGE","RAMP","Terranora Interconnector","REGULATED",10,"Ramping Constraint","PLANNED",0]
[20306,"TRANSGRIDV5_20161215152814","2014-10-30T06:00:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,15.0923,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumaresq 8E 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20318,"TRANSGRIDV5_20161215152814","2014-10-30T05:50:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,10.569750000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumaresq 8E 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20328,"TRANSGRIDV5_20161215152814","2014-10-30T11:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-24.521930000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20339,"TRANSGRIDV5_20161215152814","2014-10-30T11:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.189330000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20350,"TRANSGRIDV5_20161215152814","2014-10-30T15:25:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.807090000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20366,"TRANSGRIDV5_20161215152814","2014-10-30T14:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.891500000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20376,"TRANSGRIDV5_20161215152814","2014-10-30T15:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.474270000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20387,"TRANSGRIDV5_20161215152814","2014-10-30T13:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.387119999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20391,"TRANSGRIDV5_20161215152814","2014-10-30T04:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-27.73893,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20404,"TRANSGRIDV5_20161215152814","2014-10-30T09:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.253489999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20417,"TRANSGRIDV5_20161215152814","2014-10-30T08:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.758579999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20431,"TRANSGRIDV5_20161215152814","2014-10-30T10:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.05307,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20439,"TRANSGRIDV5_20161215152814","2014-10-30T09:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.71674,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20448,"TRANSGRIDV5_20161215152814","2014-10-30T08:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.363250000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20454,"TRANSGRIDV5_20161215152814","2014-10-30T07:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.33447,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20469,"TRANSGRIDV5_20161215152814","2014-10-30T14:40:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-12.12466,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20480,"TRANSGRIDV5_20161215152814","2014-10-31T15:50:00","V::N_HWSM_S3","V-HWSM","2014-02-21",1,-13.996790000000001,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, SA accelerates, Basslink VIC to TAS, YWG1 220 kV. Limit only applied during Heywood flow from SA to VIC","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[20486,"TRANSGRIDV5_20161215152814","2014-10-31T16:20:00","V::N_HWSM_V3","V-HWSM","2014-02-21",1,-12.50032,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[20495,"TRANSGRIDV5_20161215152814","2014-10-31T13:10:00","V::N_HWSM_V3","V-HWSM","2014-02-21",1,-10.24498,"Out = Hazelwood to South Morang 500 kV line, prevent transient instability for fault and trip of a Hazelwood to South Morang 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","OUTAGE","OTHER","Hazelwood - South Morang 500kV Line","REGULATED",99,"Non Inclusion",null,0]
[20513,"TRANSGRIDV5_20161215152814","2014-10-31T14:55:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-16.987880000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20517,"TRANSGRIDV5_20161215152814","2014-10-31T15:15:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-14.17163,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20527,"TRANSGRIDV5_20161215152814","2014-11-01T06:00:00","#N-Q-MNSP1_RAMP_I_F","#N-Q-MNSP1_RAMP_I","2014-11-01",1,15.79148,"N-Q-MNSP1 >= MIN(-65, InitialFlow + 80) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[20546,"TRANSGRIDV5_20161215152814","2014-11-01T11:20:00","F_Q++ARTW_L6","F-N-ARTW_85","2013-08-21",1,19.263120000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[20553,"TRANSGRIDV5_20161215152814","2014-11-01T06:05:00","F_Q++ARTW_L6","F-N-ARTW_85","2013-08-21",1,12.66905,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[20563,"TRANSGRIDV5_20161215152814","2014-11-01T12:40:00","F_Q++ARTW_L6","F-N-ARTW_85","2013-08-21",1,10.139519999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Tamworth330 85 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[20575,"TRANSGRIDV5_20161215152814","2014-11-01T12:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-26.00901,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20580,"TRANSGRIDV5_20161215152814","2014-11-01T09:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-25.798690000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20590,"TRANSGRIDV5_20161215152814","2014-11-01T01:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-23.58577,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20601,"TRANSGRIDV5_20161215152814","2014-11-01T09:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-21.150379999999998,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20616,"TRANSGRIDV5_20161215152814","2014-11-01T10:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-17.64931,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20628,"TRANSGRIDV5_20161215152814","2014-11-01T13:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-16.74737,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20642,"TRANSGRIDV5_20161215152814","2014-11-01T11:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42014,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20645,"TRANSGRIDV5_20161215152814","2014-11-01T13:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20653,"TRANSGRIDV5_20161215152814","2014-11-01T11:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-28.573450000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20672,"TRANSGRIDV5_20161215152814","2014-11-01T01:10:00","V>>V_NIL_2_P","V-NIL_PAR_3-5","2013-12-03",1,-14.015890000000001,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, parallel mode at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20679,"TRANSGRIDV5_20161215152814","2014-11-01T11:45:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-42.727539999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20693,"TRANSGRIDV5_20161215152814","2014-11-01T11:05:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-29.863019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20705,"TRANSGRIDV5_20161215152814","2014-11-01T11:50:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-29.084420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20711,"TRANSGRIDV5_20161215152814","2014-11-01T13:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-25.873860000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20722,"TRANSGRIDV5_20161215152814","2014-11-01T13:35:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-23.898150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20737,"TRANSGRIDV5_20161215152814","2014-11-01T13:55:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-20.349689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20743,"TRANSGRIDV5_20161215152814","2014-11-01T09:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-17.331720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20752,"TRANSGRIDV5_20161215152814","2014-11-01T15:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.458500000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20760,"TRANSGRIDV5_20161215152814","2014-11-02T18:55:00","V::N_NIL_V3","V-NIL","2014-10-22",1,-25.665959999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20778,"TRANSGRIDV5_20161215152814","2014-11-02T17:40:00","V::N_NIL_V3","V-NIL","2014-10-22",1,-14.58225,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20787,"TRANSGRIDV5_20161215152814","2014-11-02T17:05:00","V::N_NIL_V3","V-NIL","2014-10-22",1,-10.91811,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20800,"TRANSGRIDV5_20161215152814","2014-11-03T04:35:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2014-11-03",1,36.067270000000001,"NSW1-QLD1 >= MIN(-331, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[20804,"TRANSGRIDV5_20161215152814","2014-11-03T09:25:00","N^^Q_ARTW_B1","N-ARTW_86","2014-06-26",1,-1319.1684499999999,"Out = Armidale to Tamworth (85 or 86), avoid Voltage Collapse on loss of Kogan Creek generators","OUTAGE","OTHER","Armidale - Tamworth330 86 Line 330kV","REGULATED","INCLUDED","","PLANNED",1]
[20815,"TRANSGRIDV5_20161215152814","2014-11-03T21:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.6881,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20825,"TRANSGRIDV5_20161215152814","2014-11-03T22:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.176550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20841,"TRANSGRIDV5_20161215152814","2014-11-03T11:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.21664,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20852,"TRANSGRIDV5_20161215152814","2014-11-03T04:40:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.862489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20856,"TRANSGRIDV5_20161215152814","2014-11-04T04:50:00","#N-Q-MNSP1_RAMP_I_F","#N-Q-MNSP1_RAMP_I","2014-11-04",2,22.266850000000002,"N-Q-MNSP1 >= MIN(-73, InitialFlow + 80) (Wt=35)","SYSTEM NORMAL","OTHER",null,null,null,null,null,0]
[20869,"TRANSGRIDV5_20161215152814","2014-11-04T05:45:00","#R011444_018_RAMP_F","#R011444_RAMP","2014-11-03",1,-34.67362,"Hard Ramping constraint for constraint V>>V-MSUT_1, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Murray - Upper Tumut 65 330kV Line","REGULATED",10,"Ramping Constraint","PLANNED",0]
[20878,"TRANSGRIDV5_20161215152814","2014-11-04T05:10:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,16.191659999999999,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20886,"TRANSGRIDV5_20161215152814","2014-11-04T23:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.08525,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20904,"TRANSGRIDV5_20161215152814","2014-11-04T21:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.359489999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20914,"TRANSGRIDV5_20161215152814","2014-11-04T18:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.71064,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20919,"TRANSGRIDV5_20161215152814","2014-11-04T04:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.06747,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[20936,"TRANSGRIDV5_20161215152814","2014-11-04T07:05:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-32.488430000000001,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20946,"TRANSGRIDV5_20161215152814","2014-11-04T10:45:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-16.47587,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20951,"TRANSGRIDV5_20161215152814","2014-11-04T10:55:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-16.41133,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20967,"TRANSGRIDV5_20161215152814","2014-11-04T10:15:00","V>>V-MSUT_1","I-MSUT","2013-08-21",1,-15.21781,"Out= Murray-UpperTumut(65), avoid Dederang to Wodonga (DDWO) O/L on Murray-LowerTumut(66) trip; Feedback","OUTAGE","OTHER","Murray - Upper Tumut 65 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[20977,"TRANSGRIDV5_20161215152814","2014-11-05T00:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-27.91788,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20984,"TRANSGRIDV5_20161215152814","2014-11-05T01:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.190339999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[20992,"TRANSGRIDV5_20161215152814","2014-11-05T02:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.05725,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21001,"TRANSGRIDV5_20161215152814","2014-11-05T02:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.62434,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21014,"TRANSGRIDV5_20161215152814","2014-11-05T02:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.599130000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21028,"TRANSGRIDV5_20161215152814","2014-11-05T06:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.496840000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21040,"TRANSGRIDV5_20161215152814","2014-11-05T06:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.83976,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21049,"TRANSGRIDV5_20161215152814","2014-11-05T11:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.32532,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21055,"TRANSGRIDV5_20161215152814","2014-11-05T10:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.126989999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21066,"TRANSGRIDV5_20161215152814","2014-11-05T01:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.327449999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21081,"TRANSGRIDV5_20161215152814","2014-11-05T01:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.56005,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21093,"TRANSGRIDV5_20161215152814","2014-11-05T03:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.76257,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21103,"TRANSGRIDV5_20161215152814","2014-11-05T03:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.1389,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21113,"TRANSGRIDV5_20161215152814","2014-11-05T01:00:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-18.270530000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21126,"TRANSGRIDV5_20161215152814","2014-11-06T00:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.627649999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21128,"TRANSGRIDV5_20161215152814","2014-11-06T04:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.575949999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21143,"TRANSGRIDV5_20161215152814","2014-11-06T03:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.59629,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21150,"TRANSGRIDV5_20161215152814","2014-11-06T03:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.59947,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21160,"TRANSGRIDV5_20161215152814","2014-11-06T02:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.19336,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21176,"TRANSGRIDV5_20161215152814","2014-11-06T06:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.97603,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21181,"TRANSGRIDV5_20161215152814","2014-11-06T00:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.1732,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21191,"TRANSGRIDV5_20161215152814","2014-11-06T01:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.50325,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21208,"TRANSGRIDV5_20161215152814","2014-11-06T02:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.45322,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21217,"TRANSGRIDV5_20161215152814","2014-11-06T02:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.536479999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21225,"TRANSGRIDV5_20161215152814","2014-11-06T04:15:00","V::N_NIL_Q4","V-NIL","2014-06-24",1,-10.75459,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, QLD accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21239,"TRANSGRIDV5_20161215152814","2014-11-07T01:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.48821,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21252,"TRANSGRIDV5_20161215152814","2014-11-07T10:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-61.71557,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21254,"TRANSGRIDV5_20161215152814","2014-11-07T10:40:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-61.455460000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21273,"TRANSGRIDV5_20161215152814","2014-11-08T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.15213,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21280,"TRANSGRIDV5_20161215152814","2014-11-08T09:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.055099999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21290,"TRANSGRIDV5_20161215152814","2014-11-08T14:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.620990000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21295,"TRANSGRIDV5_20161215152814","2014-11-08T07:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.76976,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21312,"TRANSGRIDV5_20161215152814","2014-11-08T10:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.02055,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21323,"TRANSGRIDV5_20161215152814","2014-11-09T07:50:00","#R011476_002_RAMP_F","#R011476_RAMP","2014-11-08",1,-13.77821,"Hard Ramping constraint for constraint N_X_MBTE_3B, Effective Date: 25/11/2013, Version: 1","OUTAGE","RAMP","Terranora Interconnector","REGULATED",10,"Ramping Constraint","PLANNED",0]
[21327,"TRANSGRIDV5_20161215152814","2014-11-09T00:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.95284,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21340,"TRANSGRIDV5_20161215152814","2014-11-09T11:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.956160000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21353,"TRANSGRIDV5_20161215152814","2014-11-09T11:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.33832,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21367,"TRANSGRIDV5_20161215152814","2014-11-09T12:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-11.32582,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21375,"TRANSGRIDV5_20161215152814","2014-11-09T09:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.03683,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21384,"TRANSGRIDV5_20161215152814","2014-11-09T23:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.94598,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21390,"TRANSGRIDV5_20161215152814","2014-11-09T14:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.397019999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21405,"TRANSGRIDV5_20161215152814","2014-11-10T05:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.626919999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21416,"TRANSGRIDV5_20161215152814","2014-11-10T05:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.537710000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21422,"TRANSGRIDV5_20161215152814","2014-11-10T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.62411,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21442,"TRANSGRIDV5_20161215152814","2014-11-11T02:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.80814,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21449,"TRANSGRIDV5_20161215152814","2014-11-11T01:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.473710000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21453,"TRANSGRIDV5_20161215152814","2014-11-11T05:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.599080000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21466,"TRANSGRIDV5_20161215152814","2014-11-11T04:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.18647,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21479,"TRANSGRIDV5_20161215152814","2014-11-12T05:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.69384,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21489,"TRANSGRIDV5_20161215152814","2014-11-12T00:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.23292,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21499,"TRANSGRIDV5_20161215152814","2014-11-12T00:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.030609999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21511,"TRANSGRIDV5_20161215152814","2014-11-12T00:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.60641,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21526,"TRANSGRIDV5_20161215152814","2014-11-12T01:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.23588,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21537,"TRANSGRIDV5_20161215152814","2014-11-12T17:35:00","V>>SML_BESH_1","V-BESH","2013-12-03",1,-17.977049999999998,"Out = Bendigo to Shepparton 220 kV line, avoid O/L Waubra to Horsham 220 kV line section for trip of the Ballarat to Bendigo 220 kV line, feedback","OUTAGE","OTHER","Bendigo - Shepparton 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[21547,"TRANSGRIDV5_20161215152814","2014-11-12T14:40:00","V>>SML_BESH_3","V-BESH","2013-12-05",1,-15.82394,"Out = Bendigo to Shepparton 220 kV line, avoid O/L Moorabool to Ballarat No. 1 220 kV line (flow from MLTS to BATS) for trip of the Moorabool to Elaine to Ballarat 220 kV line and Mt Mercer Wind Farm, feedback","OUTAGE","OTHER","Bendigo - Shepparton 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[21552,"TRANSGRIDV5_20161215152814","2014-11-12T14:45:00","V>>SML_BESH_3","V-BESH","2013-12-05",1,-10.90868,"Out = Bendigo to Shepparton 220 kV line, avoid O/L Moorabool to Ballarat No. 1 220 kV line (flow from MLTS to BATS) for trip of the Moorabool to Elaine to Ballarat 220 kV line and Mt Mercer Wind Farm, feedback","OUTAGE","OTHER","Bendigo - Shepparton 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[21564,"TRANSGRIDV5_20161215152814","2014-11-14T09:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2014-10-15",1,-887.32997,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21578,"TRANSGRIDV5_20161215152814","2014-11-14T09:55:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2014-10-15",1,-886.19691,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21581,"TRANSGRIDV5_20161215152814","2014-11-14T08:35:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2014-10-15",1,-884.42341999999996,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21600,"TRANSGRIDV5_20161215152814","2014-11-14T07:20:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2014-10-15",1,-882.26,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21608,"TRANSGRIDV5_20161215152814","2014-11-14T15:00:00","V>>V_EPTT_2A_R","V-EPTT_R","2014-02-28",1,-17.653980000000001,"Out = Eildon to Thomastown 220kV line, avoid pre-contingent O/L the South Morang 500/330kV (F2) transformer, Yallourn unit 1 in 500kV mode, radial mode, feedback","OUTAGE","OTHER","Eildon - Thomastown 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[21615,"TRANSGRIDV5_20161215152814","2014-11-14T15:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.91672,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21629,"TRANSGRIDV5_20161215152814","2014-11-15T15:15:00","NSA_V_BDL02_20","NSA-V_BDL02_20","2013-08-21",1,336474.85029999999,"Bairnsdale Unit 2 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21641,"TRANSGRIDV5_20161215152814","2014-11-18T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-133.32131999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21646,"TRANSGRIDV5_20161215152814","2014-11-18T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.082569999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21656,"TRANSGRIDV5_20161215152814","2014-11-18T05:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.167950000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21673,"TRANSGRIDV5_20161215152814","2014-11-18T01:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.31616,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21678,"TRANSGRIDV5_20161215152814","2014-11-18T16:30:00","N>Q_LSLS_9U8","N-LSLS_9U8","2013-08-21",1,-41.897530000000003,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd, Swamp out when all 3 directlink cable O/S.","OUTAGE","OTHER","Lismore330 - Lismore132 9U9 132kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Essential Energy's outage"]
[21688,"TRANSGRIDV5_20161215152814","2014-11-18T05:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.96808,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21696,"TRANSGRIDV5_20161215152814","2014-11-18T04:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.17394,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21714,"TRANSGRIDV5_20161215152814","2014-11-19T13:55:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-224.01542000000001,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[21723,"TRANSGRIDV5_20161215152814","2014-11-19T12:45:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-60.246720000000003,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[21736,"TRANSGRIDV5_20161215152814","2014-11-19T14:40:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-58.30489,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[21740,"TRANSGRIDV5_20161215152814","2014-11-19T13:25:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-57.397559999999999,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[21751,"TRANSGRIDV5_20161215152814","2014-11-19T10:30:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-35.292900000000003,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[21761,"TRANSGRIDV5_20161215152814","2014-11-19T14:30:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-116.85227,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan - Lismore 967 132kV Line","REGULATED","INCLUDED","","PLANNED",1]
[21777,"TRANSGRIDV5_20161215152814","2014-11-19T14:15:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-36.769869999999997,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan - Lismore 967 132kV Line","REGULATED","INCLUDED","","PLANNED",1]
[21788,"TRANSGRIDV5_20161215152814","2014-11-19T09:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-33.555880000000002,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan - Lismore 967 132kV Line","REGULATED","INCLUDED","","PLANNED",1]
[21792,"TRANSGRIDV5_20161215152814","2014-11-19T14:05:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-28.155100000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan - Lismore 967 132kV Line","REGULATED","INCLUDED","","PLANNED",1]
[21805,"TRANSGRIDV5_20161215152814","2014-11-20T06:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.599449999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[21814,"TRANSGRIDV5_20161215152814","2014-11-20T16:35:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-36.944249999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21822,"TRANSGRIDV5_20161215152814","2014-11-20T15:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-20.07647,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21840,"TRANSGRIDV5_20161215152814","2014-11-20T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-22.759060000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21849,"TRANSGRIDV5_20161215152814","2014-11-20T15:40:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-83.927880000000002,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21855,"TRANSGRIDV5_20161215152814","2014-11-20T15:50:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-80.315870000000004,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21870,"TRANSGRIDV5_20161215152814","2014-11-20T15:15:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-41.030059999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21881,"TRANSGRIDV5_20161215152814","2014-11-20T16:50:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-25.25001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21887,"TRANSGRIDV5_20161215152814","2014-11-20T14:00:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-23.50949,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"REGULATED",null,"",null,0]
[21903,"TRANSGRIDV5_20161215152814","2014-11-21T14:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-75.911940000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21913,"TRANSGRIDV5_20161215152814","2014-11-21T16:05:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-73.557959999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21920,"TRANSGRIDV5_20161215152814","2014-11-21T15:15:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-53.84637,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21928,"TRANSGRIDV5_20161215152814","2014-11-21T13:25:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-32.856310000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21947,"TRANSGRIDV5_20161215152814","2014-11-21T13:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-20.53359,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21950,"TRANSGRIDV5_20161215152814","2014-11-21T14:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-20.314609999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21964,"TRANSGRIDV5_20161215152814","2014-11-21T15:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-14.67083,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21976,"TRANSGRIDV5_20161215152814","2014-11-21T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-116.41569,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21985,"TRANSGRIDV5_20161215152814","2014-11-21T14:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-115.23833999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[21991,"TRANSGRIDV5_20161215152814","2014-11-21T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-110.30526,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22002,"TRANSGRIDV5_20161215152814","2014-11-21T11:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-49.097299999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22017,"TRANSGRIDV5_20161215152814","2014-11-21T13:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-43.302590000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22029,"TRANSGRIDV5_20161215152814","2014-11-21T17:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-39.710340000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22039,"TRANSGRIDV5_20161215152814","2014-11-21T12:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-39.099519999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22046,"TRANSGRIDV5_20161215152814","2014-11-21T17:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.84037,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22054,"TRANSGRIDV5_20161215152814","2014-11-21T16:30:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-187.71558999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22073,"TRANSGRIDV5_20161215152814","2014-11-21T15:25:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-185.10299000000001,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22080,"TRANSGRIDV5_20161215152814","2014-11-21T14:50:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-112.16182999999999,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22086,"TRANSGRIDV5_20161215152814","2014-11-21T12:00:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-79.241389999999996,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22096,"TRANSGRIDV5_20161215152814","2014-11-21T11:45:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-78.761430000000004,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22112,"TRANSGRIDV5_20161215152814","2014-11-21T14:20:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-78.400800000000004,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22117,"TRANSGRIDV5_20161215152814","2014-11-21T13:50:00","V>>V_NIL_5","V-NIL","2013-12-03",1,-78.138980000000004,"Out = Nil, avoid O/L either Dederang to Mount Beauty 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22127,"TRANSGRIDV5_20161215152814","2014-11-22T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-85.346069999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22144,"TRANSGRIDV5_20161215152814","2014-11-22T16:30:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2014-08-29",1,-193.93510000000001,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22153,"TRANSGRIDV5_20161215152814","2014-11-22T17:15:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2014-08-29",1,-19.048179999999999,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22161,"TRANSGRIDV5_20161215152814","2014-11-22T15:45:00","N>Q_LSLS_9U8","N-LSLS_9U8","2013-08-21",1,-13.48821,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd, Swamp out when all 3 directlink cable O/S.","OUTAGE","OTHER","Lismore330 - Lismore132 9U9 132kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Essential Energy's outage"]
[22175,"TRANSGRIDV5_20161215152814","2014-11-23T16:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.710570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22188,"TRANSGRIDV5_20161215152814","2014-11-24T16:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-21.523289999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22190,"TRANSGRIDV5_20161215152814","2014-11-24T16:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-21.15457,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22209,"TRANSGRIDV5_20161215152814","2014-11-24T17:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.92248,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22216,"TRANSGRIDV5_20161215152814","2014-11-24T14:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.48143,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22226,"TRANSGRIDV5_20161215152814","2014-11-24T16:00:00","V>>V_NIL_2B_R","V-NIL_R_3-4_HW3-BUS2","2013-12-03",1,-18.149229999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22242,"TRANSGRIDV5_20161215152814","2014-11-24T17:10:00","V>>V_NIL_2B_R","V-NIL_R_3-4_HW3-BUS2","2013-12-03",1,-10.88214,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22243,"TRANSGRIDV5_20161215152814","2014-11-24T12:35:00","V>>V_NIL_2B_R","V-NIL_R_3-4_HW3-BUS2","2013-12-03",1,-10.318350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22253,"TRANSGRIDV5_20161215152814","2014-11-27T16:30:00","N>Q_LSLS_9U8","N-LSLS_9U8","2013-08-21",1,-82.579840000000004,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd, Swamp out when all 3 directlink cable O/S.","OUTAGE","OTHER","Lismore330 - Lismore132 9U9 132kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Essential Energy's outage"]
[22274,"TRANSGRIDV5_20161215152814","2014-11-29T15:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.36389,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22276,"TRANSGRIDV5_20161215152814","2014-11-29T14:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.20665,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22289,"TRANSGRIDV5_20161215152814","2014-11-29T12:15:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-15.975720000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22303,"TRANSGRIDV5_20161215152814","2014-11-29T12:20:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-12.263680000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22311,"TRANSGRIDV5_20161215152814","2014-11-29T11:55:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-10.81442,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22320,"TRANSGRIDV5_20161215152814","2014-11-29T13:50:00","V>SMLBAHO1","V-BEKG","2013-08-21",1,-16.69708,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","OUTAGE","OTHER","Bendigo - Kerang 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[22337,"TRANSGRIDV5_20161215152814","2014-11-29T12:00:00","V>SMLBAHO1","V-BEKG","2013-08-21",1,-10.003170000000001,"Out = Ballarat to Horsham, or Bendigo to Kerang line, avoid O/L or voltage collapse on Buronga to Balranald to Darlington Point (X5) line for trip of Bendigo to Kerang or Ballarat to Horsham line","OUTAGE","OTHER","Bendigo - Kerang 220kV Line","REGULATED",99,"Non Inclusion",null,0]
[22341,"TRANSGRIDV5_20161215152814","2014-11-30T17:40:00","N^^V_NIL_1","V-NIL","2014-09-24",1,-16.152460000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22352,"TRANSGRIDV5_20161215152814","2014-11-30T16:35:00","N^^V_NIL_1","V-NIL","2014-09-24",1,-12.157400000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22368,"TRANSGRIDV5_20161215152814","2014-11-30T19:30:00","N^^V_NIL_1","V-NIL","2014-09-24",1,-11.230029999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22378,"TRANSGRIDV5_20161215152814","2014-11-30T16:40:00","N^^V_NIL_1","V-NIL","2014-09-24",1,-10.302020000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22385,"TRANSGRIDV5_20161215152814","2014-11-30T12:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.226089999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22400,"TRANSGRIDV5_20161215152814","2014-11-30T13:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-16.2666,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22402,"TRANSGRIDV5_20161215152814","2014-11-30T14:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.69403,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22415,"TRANSGRIDV5_20161215152814","2014-11-30T10:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.732860000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22429,"TRANSGRIDV5_20161215152814","2014-11-30T10:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.20654,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22441,"TRANSGRIDV5_20161215152814","2014-11-30T12:25:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-19.775179999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22450,"TRANSGRIDV5_20161215152814","2014-11-30T05:30:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-17.547460000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22456,"TRANSGRIDV5_20161215152814","2014-11-30T05:55:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-17.541029999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22473,"TRANSGRIDV5_20161215152814","2014-11-30T10:00:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-14.545640000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22483,"TRANSGRIDV5_20161215152814","2014-11-30T00:10:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-14.20862,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22488,"TRANSGRIDV5_20161215152814","2014-11-30T10:30:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-12.68763,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22500,"TRANSGRIDV5_20161215152814","2014-11-30T09:10:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-11.176769999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22514,"TRANSGRIDV5_20161215152814","2014-12-01T05:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.69403,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22517,"TRANSGRIDV5_20161215152814","2014-12-01T05:40:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-19.66741,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22536,"TRANSGRIDV5_20161215152814","2014-12-04T02:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.93065,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[22544,"TRANSGRIDV5_20161215152814","2014-12-04T02:45:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-14.45355,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22551,"TRANSGRIDV5_20161215152814","2014-12-04T03:40:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-12.555619999999999,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22565,"TRANSGRIDV5_20161215152814","2014-12-04T02:55:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-10.30916,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","UNPLANNED",1]
[22577,"TRANSGRIDV5_20161215152814","2014-12-06T14:45:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1031.7348300000001,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","UNPLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[22582,"TRANSGRIDV5_20161215152814","2014-12-06T14:35:00","N_WOODLWN1_ZERO","N-WOODLWN1_ZERO","2013-08-21",1,-1031.14743,"Woodlawn unit upper limit of 0 MW","OUTAGE","OTHER","Capital Windfarm 330kV Bus C","NON-REGULATED",4,"Non Prescribed Transmission Service","UNPLANNED",0,"Capital Windfarm substation is a non-prescribed asset"]
[22592,"TRANSGRIDV5_20161215152814","2014-12-06T08:20:00","V::N_DDSM_V3","V-DDSM","2014-02-21",1,-14.96367,"Out = Dederang to South Morang 330 kV line, prevent transient instability for fault and trip of remaining Dederang to South Morang 330 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 220 kV.","OUTAGE","OTHER","Dederang - South Morang No.1 330kV Line","REGULATED",99,"Non Inclusion",null,0]
[22609,"TRANSGRIDV5_20161215152814","2014-12-06T10:25:00","VN_0700","I-VN_0700","2014-01-08",1,-15.67319,"Discretionary Vic to NSW transfer upper limit of  700 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22614,"TRANSGRIDV5_20161215152814","2014-12-06T11:00:00","VN_0700","I-VN_0700","2014-01-08",1,-14.36214,"Discretionary Vic to NSW transfer upper limit of  700 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22626,"TRANSGRIDV5_20161215152814","2014-12-06T11:40:00","VN_0700","I-VN_0700","2014-01-08",1,-11.02342,"Discretionary Vic to NSW transfer upper limit of  700 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22640,"TRANSGRIDV5_20161215152814","2014-12-08T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-6139.3573900000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22643,"TRANSGRIDV5_20161215152814","2014-12-08T16:30:00","N>Q_LSLS_9U8","N-LSLS_9U8","2013-08-21",1,-4489.6556799999998,"Out= One of Lismore330-Lismore132 (9U8,9U9,9W1), avoid OL the line remaining on loss of the 2nd, Swamp out when all 3 directlink cable O/S.","OUTAGE","OTHER","Lismore330 - Lismore132 9U9 132kV Line","REGULATED",99,"Non Inclusion","PLANNED",0,"Essential Energy's outage"]
[22655,"TRANSGRIDV5_20161215152814","2014-12-09T15:30:00","N>Q-MUTW_2","N-MUTW_88","2014-09-12",1,-22383.05559,"Out= Muswellbrook-Tamworth(88), avoid Liddell->Tamworth(84) OL on trip of QLD largest generation; Fb","OUTAGE","OTHER","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22672,"TRANSGRIDV5_20161215152814","2014-12-09T13:55:00","N>Q-MUTW_2","N-MUTW_88","2014-09-12",1,-102.62309999999999,"Out= Muswellbrook-Tamworth(88), avoid Liddell->Tamworth(84) OL on trip of QLD largest generation; Fb","OUTAGE","OTHER","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22676,"TRANSGRIDV5_20161215152814","2014-12-09T14:30:00","N>Q-MUTW_2","N-MUTW_88","2014-09-12",1,-91.273650000000004,"Out= Muswellbrook-Tamworth(88), avoid Liddell->Tamworth(84) OL on trip of QLD largest generation; Fb","OUTAGE","OTHER","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22687,"TRANSGRIDV5_20161215152814","2014-12-09T14:55:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-1029.28181,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,null,null,0]
[22697,"TRANSGRIDV5_20161215152814","2014-12-09T13:40:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-149.00435999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,null,null,0]
[22713,"TRANSGRIDV5_20161215152814","2014-12-09T15:40:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-25.17108,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,null,null,0]
[22724,"TRANSGRIDV5_20161215152814","2014-12-09T03:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.232950000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22728,"TRANSGRIDV5_20161215152814","2014-12-10T00:30:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,10.071160000000001,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22741,"TRANSGRIDV5_20161215152814","2014-12-10T01:35:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,20.656479999999998,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22750,"TRANSGRIDV5_20161215152814","2014-12-10T02:15:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,13.8787,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22768,"TRANSGRIDV5_20161215152814","2014-12-10T06:20:00","F_Q++MUTW_L60","F-N-MUTW_88","2013-08-21",1,16.91506,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22776,"TRANSGRIDV5_20161215152814","2014-12-10T01:55:00","F_Q++MUTW_L60","F-N-MUTW_88","2013-08-21",1,13.520429999999999,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22785,"TRANSGRIDV5_20161215152814","2014-12-10T02:55:00","F_Q++MUTW_L60","F-N-MUTW_88","2013-08-21",1,10.965,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22791,"TRANSGRIDV5_20161215152814","2014-12-10T14:55:00","N>Q-MUTW_2","N-MUTW_88","2014-09-12",1,-29343.335449999999,"Out= Muswellbrook-Tamworth(88), avoid Liddell->Tamworth(84) OL on trip of QLD largest generation; Fb","OUTAGE","OTHER","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22806,"TRANSGRIDV5_20161215152814","2014-12-10T17:05:00","N>Q-MUTW_2","N-MUTW_88","2014-09-12",1,-152.18047999999999,"Out= Muswellbrook-Tamworth(88), avoid Liddell->Tamworth(84) OL on trip of QLD largest generation; Fb","OUTAGE","OTHER","Muswellbrook - Tamworth330 88 330kV Line","REGULATED","INCLUDED","","UNPLANNED",1]
[22817,"TRANSGRIDV5_20161215152814","2014-12-10T17:00:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-14083.30035,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,null,null,0]
[22823,"TRANSGRIDV5_20161215152814","2014-12-10T16:05:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-176.42920000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,null,null,0]
[22839,"TRANSGRIDV5_20161215152814","2014-12-10T16:30:00","S>>BWPA_BRTW_WTTP","S-BWPA","2014-03-04",1,-69.855339999999998,"Out= Blyth West- Para 275kV line with Bungama CB6539 OPEN, avoid O/L Waterloo-Templers 132kV line on trip of Brinkworth-Templers West 275kV line, Feedback","OUTAGE","OTHER","Blyth West - Para 275kV Line","REGULATED",99,"Non Inclusion",null,0]
[22850,"TRANSGRIDV5_20161215152814","2014-12-10T15:40:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-19.893560000000001,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22854,"TRANSGRIDV5_20161215152814","2014-12-10T15:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.03187,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22864,"TRANSGRIDV5_20161215152814","2014-12-10T15:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.12355,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22883,"TRANSGRIDV5_20161215152814","2014-12-10T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.20294,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22886,"TRANSGRIDV5_20161215152814","2014-12-10T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.324529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22900,"TRANSGRIDV5_20161215152814","2014-12-11T09:20:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-10.48265,"SA to Vic on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22912,"TRANSGRIDV5_20161215152814","2014-12-14T05:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.467320000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22921,"TRANSGRIDV5_20161215152814","2014-12-16T16:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.890890000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22927,"TRANSGRIDV5_20161215152814","2014-12-16T13:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.941689999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22938,"TRANSGRIDV5_20161215152814","2014-12-16T14:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.759600000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22953,"TRANSGRIDV5_20161215152814","2014-12-16T12:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22965,"TRANSGRIDV5_20161215152814","2014-12-16T08:50:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-13.46574,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[22975,"TRANSGRIDV5_20161215152814","2014-12-16T18:20:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-16.241969999999998,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[22982,"TRANSGRIDV5_20161215152814","2014-12-16T16:35:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-13.09125,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[22990,"TRANSGRIDV5_20161215152814","2014-12-17T19:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-57.249389999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23009,"TRANSGRIDV5_20161215152814","2014-12-17T16:45:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2014-08-29",1,-13753.11844,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23016,"TRANSGRIDV5_20161215152814","2014-12-17T17:10:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2014-08-29",1,-13711.0725,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23030,"TRANSGRIDV5_20161215152814","2014-12-17T17:45:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2014-08-29",1,-12.110670000000001,"Out= NIL, avoid O/L Liddell to Muswellbrook (83) on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23042,"TRANSGRIDV5_20161215152814","2014-12-17T16:05:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-462.55275,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23048,"TRANSGRIDV5_20161215152814","2014-12-17T15:55:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-454.17349999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23054,"TRANSGRIDV5_20161215152814","2014-12-17T16:30:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-402.0711,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23055,"TRANSGRIDV5_20161215152814","2014-12-17T15:25:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-395.57556,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23056,"TRANSGRIDV5_20161215152814","2014-12-17T14:30:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-382.30878999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23057,"TRANSGRIDV5_20161215152814","2014-12-17T15:15:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-295.22320999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23058,"TRANSGRIDV5_20161215152814","2014-12-17T14:20:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-275.32123999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23059,"TRANSGRIDV5_20161215152814","2014-12-17T15:20:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-232.89107999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23060,"TRANSGRIDV5_20161215152814","2014-12-17T15:30:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-224.16476,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23061,"TRANSGRIDV5_20161215152814","2014-12-17T14:25:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-219.10368,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23062,"TRANSGRIDV5_20161215152814","2014-12-17T13:50:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-212.32923,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23063,"TRANSGRIDV5_20161215152814","2014-12-17T15:05:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-141.44220000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23064,"TRANSGRIDV5_20161215152814","2014-12-17T14:15:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-133.59444999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23065,"TRANSGRIDV5_20161215152814","2014-12-17T14:05:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-132.37058999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23066,"TRANSGRIDV5_20161215152814","2014-12-17T13:55:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-129.64287999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23067,"TRANSGRIDV5_20161215152814","2014-12-17T15:10:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-111.69843,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23068,"TRANSGRIDV5_20161215152814","2014-12-17T13:45:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-56.030360000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23069,"TRANSGRIDV5_20161215152814","2014-12-17T19:45:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-27.837409999999998,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23070,"TRANSGRIDV5_20161215152814","2014-12-17T19:05:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-17",24,-19.282489999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23071,"TRANSGRIDV5_20161215152814","2014-12-17T22:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-19.059909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23072,"TRANSGRIDV5_20161215152814","2014-12-17T22:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.799860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23073,"TRANSGRIDV5_20161215152814","2014-12-17T22:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.11415,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23074,"TRANSGRIDV5_20161215152814","2014-12-17T22:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.81781,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23075,"TRANSGRIDV5_20161215152814","2014-12-17T22:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.71419,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23076,"TRANSGRIDV5_20161215152814","2014-12-17T22:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.56442,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23077,"TRANSGRIDV5_20161215152814","2014-12-17T21:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.40687,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23078,"TRANSGRIDV5_20161215152814","2014-12-17T22:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.01773,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23079,"TRANSGRIDV5_20161215152814","2014-12-17T22:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.94143,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23080,"TRANSGRIDV5_20161215152814","2014-12-17T22:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.89597,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23081,"TRANSGRIDV5_20161215152814","2014-12-17T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.68679,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23082,"TRANSGRIDV5_20161215152814","2014-12-17T21:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.491490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23083,"TRANSGRIDV5_20161215152814","2014-12-17T22:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.13889,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23084,"TRANSGRIDV5_20161215152814","2014-12-17T10:40:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-19.898070000000001,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23085,"TRANSGRIDV5_20161215152814","2014-12-17T10:35:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-14.6669,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23086,"TRANSGRIDV5_20161215152814","2014-12-17T12:05:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-14.63322,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23087,"TRANSGRIDV5_20161215152814","2014-12-17T19:15:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-13.74705,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23088,"TRANSGRIDV5_20161215152814","2014-12-17T10:45:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-11.69126,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23089,"TRANSGRIDV5_20161215152814","2014-12-17T18:55:00","V>>V_LTMS_1","I-LTMS","2013-08-21",1,-10.80461,"Out= LowerTumut-Murray(66), avoid Dederang to Wodonga (DDWO) O/L on Murray-UpperTumut(65) trip; Feedback","OUTAGE","OTHER","Lower Tumut - Murray 66 330kV Line","REGULATED","INCLUDED","","PLANNED",1]
[23090,"TRANSGRIDV5_20161215152814","2014-12-17T07:05:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-11.360609999999999,"Vic to SA on ML upper transfer limit of 0 MW","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23091,"TRANSGRIDV5_20161215152814","2014-12-18T15:00:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-12781.71825,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[23092,"TRANSGRIDV5_20161215152814","2014-12-18T16:00:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-6292.4641700000002,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[23093,"TRANSGRIDV5_20161215152814","2014-12-18T16:30:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-2007.5501200000001,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[23094,"TRANSGRIDV5_20161215152814","2014-12-18T14:30:00","N^^Q_AR_VC_B1","N-AR_VC1","2013-08-21",1,-108.35169,"Out= Armidale SVC, avoid Voltage Collapse on loss of Kogan Creek","OUTAGE","OTHER","Armidale No.1 SVC 330kV","REGULATED","INCLUDED","","PLANNED",1]
[23095,"TRANSGRIDV5_20161215152814","2014-12-18T15:00:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-18",28,-4330.3688000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23096,"TRANSGRIDV5_20161215152814","2014-12-18T16:00:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-18",28,-1972.2116000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23097,"TRANSGRIDV5_20161215152814","2014-12-18T16:30:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-18",28,-625.46294999999998,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23098,"TRANSGRIDV5_20161215152814","2014-12-18T14:30:00","N>LSDU9U6_LSDU9U7","CA_AUTO","2014-12-18",28,-32.094050000000003,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23099,"TRANSGRIDV5_20161215152814","2014-12-18T16:20:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-22.07422,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23100,"TRANSGRIDV5_20161215152814","2014-12-18T16:15:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-21.956510000000002,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23101,"TRANSGRIDV5_20161215152814","2014-12-18T16:25:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-19.514099999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23102,"TRANSGRIDV5_20161215152814","2014-12-18T16:50:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-17.042290000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23103,"TRANSGRIDV5_20161215152814","2014-12-18T16:40:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-16.843019999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23104,"TRANSGRIDV5_20161215152814","2014-12-18T16:45:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-16.612269999999999,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23105,"TRANSGRIDV5_20161215152814","2014-12-18T16:05:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-16.31673,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23106,"TRANSGRIDV5_20161215152814","2014-12-18T16:55:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-16.27974,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23107,"TRANSGRIDV5_20161215152814","2014-12-18T16:35:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-13.000080000000001,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23108,"TRANSGRIDV5_20161215152814","2014-12-18T16:10:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-12.18937,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,null,null,"",null,0]
[23109,"TRANSGRIDV5_20161215152814","2014-12-18T14:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.77158,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23110,"TRANSGRIDV5_20161215152814","2014-12-18T14:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.112410000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23111,"TRANSGRIDV5_20161215152814","2014-12-18T14:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.65042,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23112,"TRANSGRIDV5_20161215152814","2014-12-18T14:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.94068,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23113,"TRANSGRIDV5_20161215152814","2014-12-18T14:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.916840000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23114,"TRANSGRIDV5_20161215152814","2014-12-18T14:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.785729999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23115,"TRANSGRIDV5_20161215152814","2014-12-18T14:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.76248,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23116,"TRANSGRIDV5_20161215152814","2014-12-18T14:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.71574,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23117,"TRANSGRIDV5_20161215152814","2014-12-18T14:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.260910000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23118,"TRANSGRIDV5_20161215152814","2014-12-18T13:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23119,"TRANSGRIDV5_20161215152814","2014-12-18T13:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23120,"TRANSGRIDV5_20161215152814","2014-12-18T14:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23121,"TRANSGRIDV5_20161215152814","2014-12-18T13:55:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-51.138910000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23122,"TRANSGRIDV5_20161215152814","2014-12-18T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-48.505000000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23123,"TRANSGRIDV5_20161215152814","2014-12-18T14:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-48.505000000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23124,"TRANSGRIDV5_20161215152814","2014-12-18T00:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.75309,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23125,"TRANSGRIDV5_20161215152814","2014-12-18T00:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.30161,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23126,"TRANSGRIDV5_20161215152814","2014-12-18T00:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.23481,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23127,"TRANSGRIDV5_20161215152814","2014-12-18T00:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.90297,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23128,"TRANSGRIDV5_20161215152814","2014-12-18T00:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.819750000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23129,"TRANSGRIDV5_20161215152814","2014-12-18T00:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.51064,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23130,"TRANSGRIDV5_20161215152814","2014-12-18T00:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.25733,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23131,"TRANSGRIDV5_20161215152814","2014-12-18T01:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.13974,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23132,"TRANSGRIDV5_20161215152814","2014-12-18T00:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.085940000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23133,"TRANSGRIDV5_20161215152814","2014-12-18T06:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.945,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23134,"TRANSGRIDV5_20161215152814","2014-12-18T00:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.878869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23135,"TRANSGRIDV5_20161215152814","2014-12-18T22:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.57034,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23136,"TRANSGRIDV5_20161215152814","2014-12-18T00:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.346590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23137,"TRANSGRIDV5_20161215152814","2014-12-18T05:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.068239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23138,"TRANSGRIDV5_20161215152814","2014-12-18T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.901059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23139,"TRANSGRIDV5_20161215152814","2014-12-18T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.295680000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23140,"TRANSGRIDV5_20161215152814","2014-12-18T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.023289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23141,"TRANSGRIDV5_20161215152814","2014-12-18T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.072570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23142,"TRANSGRIDV5_20161215152814","2014-12-18T14:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.946289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23143,"TRANSGRIDV5_20161215152814","2014-12-19T22:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.264900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23144,"TRANSGRIDV5_20161215152814","2014-12-19T22:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.937720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23145,"TRANSGRIDV5_20161215152814","2014-12-19T22:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.69811,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23146,"TRANSGRIDV5_20161215152814","2014-12-19T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.475630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23147,"TRANSGRIDV5_20161215152814","2014-12-19T22:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.37726,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23148,"TRANSGRIDV5_20161215152814","2014-12-19T00:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.91826,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23149,"TRANSGRIDV5_20161215152814","2014-12-19T22:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.559799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23150,"TRANSGRIDV5_20161215152814","2014-12-19T22:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.500769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23151,"TRANSGRIDV5_20161215152814","2014-12-20T00:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.847,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23152,"TRANSGRIDV5_20161215152814","2014-12-20T00:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.547420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23153,"TRANSGRIDV5_20161215152814","2014-12-20T00:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.48617,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23154,"TRANSGRIDV5_20161215152814","2014-12-20T00:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.21888,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23155,"TRANSGRIDV5_20161215152814","2014-12-20T00:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.674300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23156,"TRANSGRIDV5_20161215152814","2014-12-20T00:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.646129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23157,"TRANSGRIDV5_20161215152814","2014-12-20T00:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.56875,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23158,"TRANSGRIDV5_20161215152814","2014-12-21T15:40:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-216.98866000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23159,"TRANSGRIDV5_20161215152814","2014-12-21T15:45:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-180.21472,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23160,"TRANSGRIDV5_20161215152814","2014-12-21T16:05:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-18.243970000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23161,"TRANSGRIDV5_20161215152814","2014-12-21T15:35:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-14.411860000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23162,"TRANSGRIDV5_20161215152814","2014-12-21T15:55:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-10.71903,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23163,"TRANSGRIDV5_20161215152814","2014-12-21T19:10:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-147.68337,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23164,"TRANSGRIDV5_20161215152814","2014-12-21T18:05:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-37.839500000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23165,"TRANSGRIDV5_20161215152814","2014-12-21T19:05:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-30.342929999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23166,"TRANSGRIDV5_20161215152814","2014-12-21T19:15:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-23.918949999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23167,"TRANSGRIDV5_20161215152814","2014-12-21T19:00:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-23.385300000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23168,"TRANSGRIDV5_20161215152814","2014-12-21T18:15:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-22.747979999999998,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23169,"TRANSGRIDV5_20161215152814","2014-12-21T18:50:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-19.341889999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23170,"TRANSGRIDV5_20161215152814","2014-12-21T18:55:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-19.071429999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23171,"TRANSGRIDV5_20161215152814","2014-12-21T18:45:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-17.44538,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23172,"TRANSGRIDV5_20161215152814","2014-12-21T18:20:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-15.10854,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23173,"TRANSGRIDV5_20161215152814","2014-12-21T18:40:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-14.61009,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23174,"TRANSGRIDV5_20161215152814","2014-12-21T18:35:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-14.518269999999999,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23175,"TRANSGRIDV5_20161215152814","2014-12-21T19:20:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-12.23461,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23176,"TRANSGRIDV5_20161215152814","2014-12-21T18:30:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-10.90042,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23177,"TRANSGRIDV5_20161215152814","2014-12-21T19:25:00","V>>SML_NIL_7B","V-NIL","2014-01-31",1,-10.721690000000001,"Out = Nil, avoid O/L Buangor to Arrarat 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23178,"TRANSGRIDV5_20161215152814","2014-12-23T01:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-21.30134,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23179,"TRANSGRIDV5_20161215152814","2014-12-23T00:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-18.998259999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23180,"TRANSGRIDV5_20161215152814","2014-12-23T01:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.36102,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23181,"TRANSGRIDV5_20161215152814","2014-12-23T01:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.33811,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23182,"TRANSGRIDV5_20161215152814","2014-12-23T03:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.86049,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23183,"TRANSGRIDV5_20161215152814","2014-12-23T02:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.42024,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23184,"TRANSGRIDV5_20161215152814","2014-12-23T02:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.906929999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23185,"TRANSGRIDV5_20161215152814","2014-12-23T03:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.782249999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23186,"TRANSGRIDV5_20161215152814","2014-12-23T03:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.782249999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23187,"TRANSGRIDV5_20161215152814","2014-12-23T04:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.782249999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23188,"TRANSGRIDV5_20161215152814","2014-12-23T00:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.832599999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23189,"TRANSGRIDV5_20161215152814","2014-12-23T01:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.652480000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23190,"TRANSGRIDV5_20161215152814","2014-12-23T00:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.068660000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23191,"TRANSGRIDV5_20161215152814","2014-12-23T01:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.23582,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23192,"TRANSGRIDV5_20161215152814","2014-12-23T01:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.209070000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23193,"TRANSGRIDV5_20161215152814","2014-12-23T03:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.723710000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23194,"TRANSGRIDV5_20161215152814","2014-12-23T02:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.101520000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23195,"TRANSGRIDV5_20161215152814","2014-12-23T00:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.27436,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23196,"TRANSGRIDV5_20161215152814","2014-12-23T02:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.98094,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23197,"TRANSGRIDV5_20161215152814","2014-12-23T03:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.50667,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23198,"TRANSGRIDV5_20161215152814","2014-12-23T04:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.505570000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23199,"TRANSGRIDV5_20161215152814","2014-12-23T03:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.493499999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23200,"TRANSGRIDV5_20161215152814","2014-12-23T00:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.18538,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23201,"TRANSGRIDV5_20161215152814","2014-12-23T13:30:00","V::N_BUDPQE_R","N-BUDP","2013-08-21",1,-14.42822,"Out = Buronga to Darlington Point 220kV line, avoid transient instability for fault and trip of a Hazelwood to South Morang 500kV line, Basslink VIC to TAS, QLD accelerates, segment 2","OUTAGE","OTHER","Buronga - Darlington Point X5 Line 220kV","REGULATED","INCLUDED","","PLANNED",1]
[23202,"TRANSGRIDV5_20161215152814","2014-12-24T04:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.839650000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED",99,"Non Inclusion",null,0]
[23203,"TRANSGRIDV5_20161215152814","2014-12-24T04:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.300649999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23204,"TRANSGRIDV5_20161215152814","2014-12-24T05:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.86199,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23205,"TRANSGRIDV5_20161215152814","2014-12-24T04:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.39561,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23206,"TRANSGRIDV5_20161215152814","2014-12-24T04:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.333159999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23207,"TRANSGRIDV5_20161215152814","2014-12-24T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.013920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23208,"TRANSGRIDV5_20161215152814","2014-12-24T22:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.77178,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23209,"TRANSGRIDV5_20161215152814","2014-12-24T22:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.706519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23210,"TRANSGRIDV5_20161215152814","2014-12-24T22:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.78764,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23211,"TRANSGRIDV5_20161215152814","2014-12-24T22:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.0372,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23212,"TRANSGRIDV5_20161215152814","2014-12-24T22:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.83606,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23213,"TRANSGRIDV5_20161215152814","2014-12-24T22:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.81218,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23214,"TRANSGRIDV5_20161215152814","2014-12-24T23:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.768280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23215,"TRANSGRIDV5_20161215152814","2014-12-24T22:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.72213,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23216,"TRANSGRIDV5_20161215152814","2014-12-24T22:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.64325,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23217,"TRANSGRIDV5_20161215152814","2014-12-24T22:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.216340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23218,"TRANSGRIDV5_20161215152814","2014-12-25T14:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.69252,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23219,"TRANSGRIDV5_20161215152814","2014-12-25T05:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.38768,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23220,"TRANSGRIDV5_20161215152814","2014-12-25T13:35:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-31.872450000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23221,"TRANSGRIDV5_20161215152814","2014-12-25T13:05:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-25.84064,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23222,"TRANSGRIDV5_20161215152814","2014-12-25T14:00:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-11.11852,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23223,"TRANSGRIDV5_20161215152814","2014-12-25T14:20:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.960760000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23224,"TRANSGRIDV5_20161215152814","2014-12-25T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.624890000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23225,"TRANSGRIDV5_20161215152814","2014-12-25T00:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.74164,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23226,"TRANSGRIDV5_20161215152814","2014-12-25T00:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.931419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23227,"TRANSGRIDV5_20161215152814","2014-12-25T00:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.79584,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23228,"TRANSGRIDV5_20161215152814","2014-12-25T00:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.744070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23229,"TRANSGRIDV5_20161215152814","2014-12-25T00:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.67853,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23230,"TRANSGRIDV5_20161215152814","2014-12-25T01:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.470129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23231,"TRANSGRIDV5_20161215152814","2014-12-25T13:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-32.038249999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23232,"TRANSGRIDV5_20161215152814","2014-12-25T13:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-26.40231,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23233,"TRANSGRIDV5_20161215152814","2014-12-25T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.10177,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23234,"TRANSGRIDV5_20161215152814","2014-12-25T13:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.701359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23235,"TRANSGRIDV5_20161215152814","2014-12-25T14:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.965999999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23236,"TRANSGRIDV5_20161215152814","2014-12-25T16:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.92295,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23237,"TRANSGRIDV5_20161215152814","2014-12-25T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.346,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23238,"TRANSGRIDV5_20161215152814","2014-12-25T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.279719999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23239,"TRANSGRIDV5_20161215152814","2014-12-25T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.98146,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23240,"TRANSGRIDV5_20161215152814","2014-12-25T13:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.944929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23241,"TRANSGRIDV5_20161215152814","2014-12-25T13:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.86356,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23242,"TRANSGRIDV5_20161215152814","2014-12-25T18:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.512169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23243,"TRANSGRIDV5_20161215152814","2014-12-25T13:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.358700000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23244,"TRANSGRIDV5_20161215152814","2014-12-25T13:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.195080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23245,"TRANSGRIDV5_20161215152814","2014-12-25T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.14667,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23246,"TRANSGRIDV5_20161215152814","2014-12-25T14:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.06123,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23247,"TRANSGRIDV5_20161215152814","2014-12-28T23:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.95083,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23248,"TRANSGRIDV5_20161215152814","2014-12-28T08:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.75192,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23249,"TRANSGRIDV5_20161215152814","2014-12-28T08:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.33971,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23250,"TRANSGRIDV5_20161215152814","2014-12-28T08:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.10557,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23251,"TRANSGRIDV5_20161215152814","2014-12-28T08:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.810359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23252,"TRANSGRIDV5_20161215152814","2014-12-28T09:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.80667,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23253,"TRANSGRIDV5_20161215152814","2014-12-28T23:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.764900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23254,"TRANSGRIDV5_20161215152814","2014-12-28T09:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.405620000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23255,"TRANSGRIDV5_20161215152814","2014-12-28T23:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.295719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23256,"TRANSGRIDV5_20161215152814","2014-12-28T22:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.724259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23257,"TRANSGRIDV5_20161215152814","2014-12-28T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.68938,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23258,"TRANSGRIDV5_20161215152814","2014-12-28T22:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.68868,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23259,"TRANSGRIDV5_20161215152814","2014-12-28T16:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.626200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23260,"TRANSGRIDV5_20161215152814","2014-12-28T08:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.612159999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23261,"TRANSGRIDV5_20161215152814","2014-12-28T16:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.31277,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23262,"TRANSGRIDV5_20161215152814","2014-12-28T08:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.31265,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23263,"TRANSGRIDV5_20161215152814","2014-12-28T16:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.261699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23264,"TRANSGRIDV5_20161215152814","2014-12-28T23:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.1861,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23265,"TRANSGRIDV5_20161215152814","2014-12-28T23:40:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-349.68083999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23266,"TRANSGRIDV5_20161215152814","2014-12-28T23:35:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-10.438000000000001,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23267,"TRANSGRIDV5_20161215152814","2014-12-29T09:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-31.489419999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23268,"TRANSGRIDV5_20161215152814","2014-12-29T10:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-28.774519999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23269,"TRANSGRIDV5_20161215152814","2014-12-29T15:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-22.305099999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23270,"TRANSGRIDV5_20161215152814","2014-12-29T14:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-19.529969999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23271,"TRANSGRIDV5_20161215152814","2014-12-29T15:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.933529999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23272,"TRANSGRIDV5_20161215152814","2014-12-29T15:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.735620000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23273,"TRANSGRIDV5_20161215152814","2014-12-29T15:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.529780000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23274,"TRANSGRIDV5_20161215152814","2014-12-29T14:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.346819999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23275,"TRANSGRIDV5_20161215152814","2014-12-29T13:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.14364,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23276,"TRANSGRIDV5_20161215152814","2014-12-29T15:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-14.02101,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23277,"TRANSGRIDV5_20161215152814","2014-12-29T14:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.96017,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23278,"TRANSGRIDV5_20161215152814","2014-12-29T13:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.93092,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23279,"TRANSGRIDV5_20161215152814","2014-12-29T13:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.79034,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23280,"TRANSGRIDV5_20161215152814","2014-12-29T14:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.72381,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23281,"TRANSGRIDV5_20161215152814","2014-12-29T15:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.7082,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23282,"TRANSGRIDV5_20161215152814","2014-12-29T13:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.583349999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23283,"TRANSGRIDV5_20161215152814","2014-12-29T13:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.408939999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23284,"TRANSGRIDV5_20161215152814","2014-12-29T14:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.363049999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23285,"TRANSGRIDV5_20161215152814","2014-12-29T12:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.354189999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23286,"TRANSGRIDV5_20161215152814","2014-12-29T14:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.16944,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23287,"TRANSGRIDV5_20161215152814","2014-12-29T11:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.120990000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23288,"TRANSGRIDV5_20161215152814","2014-12-29T14:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.069699999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23289,"TRANSGRIDV5_20161215152814","2014-12-29T14:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.052289999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23290,"TRANSGRIDV5_20161215152814","2014-12-29T14:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-13.003579999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23291,"TRANSGRIDV5_20161215152814","2014-12-29T12:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.848129999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23292,"TRANSGRIDV5_20161215152814","2014-12-29T13:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.82273,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23293,"TRANSGRIDV5_20161215152814","2014-12-29T12:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.77206,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23294,"TRANSGRIDV5_20161215152814","2014-12-29T13:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.76271,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23295,"TRANSGRIDV5_20161215152814","2014-12-29T11:30:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.718489999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23296,"TRANSGRIDV5_20161215152814","2014-12-29T12:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.69007,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23297,"TRANSGRIDV5_20161215152814","2014-12-29T13:05:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.63106,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23298,"TRANSGRIDV5_20161215152814","2014-12-29T14:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.62365,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23299,"TRANSGRIDV5_20161215152814","2014-12-29T12:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.614089999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23300,"TRANSGRIDV5_20161215152814","2014-12-29T13:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.594480000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23301,"TRANSGRIDV5_20161215152814","2014-12-29T14:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.542590000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23302,"TRANSGRIDV5_20161215152814","2014-12-29T09:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.49066,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23303,"TRANSGRIDV5_20161215152814","2014-12-29T14:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.490449999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23304,"TRANSGRIDV5_20161215152814","2014-12-29T11:25:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.41954,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23305,"TRANSGRIDV5_20161215152814","2014-12-29T11:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.407769999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23306,"TRANSGRIDV5_20161215152814","2014-12-29T12:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.256869999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23307,"TRANSGRIDV5_20161215152814","2014-12-29T12:15:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.214560000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23308,"TRANSGRIDV5_20161215152814","2014-12-29T11:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.108650000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23309,"TRANSGRIDV5_20161215152814","2014-12-29T11:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.083170000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23310,"TRANSGRIDV5_20161215152814","2014-12-29T07:20:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.05775,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23311,"TRANSGRIDV5_20161215152814","2014-12-29T13:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-12.00827,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23312,"TRANSGRIDV5_20161215152814","2014-12-29T08:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.985440000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23313,"TRANSGRIDV5_20161215152814","2014-12-29T13:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.83268,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23314,"TRANSGRIDV5_20161215152814","2014-12-29T08:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.766299999999999,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23315,"TRANSGRIDV5_20161215152814","2014-12-29T13:45:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.745520000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23316,"TRANSGRIDV5_20161215152814","2014-12-29T11:10:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.49311,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23317,"TRANSGRIDV5_20161215152814","2014-12-29T08:50:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.48546,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23318,"TRANSGRIDV5_20161215152814","2014-12-29T11:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.27441,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23319,"TRANSGRIDV5_20161215152814","2014-12-29T11:55:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-11.267530000000001,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23320,"TRANSGRIDV5_20161215152814","2014-12-29T12:00:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.93695,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23321,"TRANSGRIDV5_20161215152814","2014-12-29T15:40:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.90124,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23322,"TRANSGRIDV5_20161215152814","2014-12-29T08:35:00","S>>V_NIL_RBTX_MW4RB","S-NIL","2014-06-11",1,-10.42,"Out= Nil, avoid O/L Morgan Whyalla 4 to Robertstown line on trip of one Robertstown 275/132kV transformer, Feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23323,"TRANSGRIDV5_20161215152814","2014-12-29T06:25:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-58.414160000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23324,"TRANSGRIDV5_20161215152814","2014-12-29T08:35:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-38.956200000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23325,"TRANSGRIDV5_20161215152814","2014-12-29T12:10:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-12.137169999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23326,"TRANSGRIDV5_20161215152814","2014-12-29T05:45:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-11.48382,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23327,"TRANSGRIDV5_20161215152814","2014-12-29T06:30:00","S>V_NIL_NIL_RBNW","S-NIL","2014-06-11",1,-10.142329999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23328,"TRANSGRIDV5_20161215152814","2014-12-29T01:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.171769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23329,"TRANSGRIDV5_20161215152814","2014-12-29T00:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.08971,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23330,"TRANSGRIDV5_20161215152814","2014-12-29T01:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.16926,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23331,"TRANSGRIDV5_20161215152814","2014-12-29T01:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.91789,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23332,"TRANSGRIDV5_20161215152814","2014-12-29T00:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.90076,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23333,"TRANSGRIDV5_20161215152814","2014-12-29T01:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.6875,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23334,"TRANSGRIDV5_20161215152814","2014-12-29T01:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.642060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23335,"TRANSGRIDV5_20161215152814","2014-12-29T00:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.63814,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23336,"TRANSGRIDV5_20161215152814","2014-12-29T01:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.44745,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23337,"TRANSGRIDV5_20161215152814","2014-12-29T00:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.385669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23338,"TRANSGRIDV5_20161215152814","2014-12-29T01:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.126049999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23339,"TRANSGRIDV5_20161215152814","2014-12-29T00:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.906330000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23340,"TRANSGRIDV5_20161215152814","2014-12-29T00:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.87655,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23341,"TRANSGRIDV5_20161215152814","2014-12-29T00:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.673819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23342,"TRANSGRIDV5_20161215152814","2014-12-29T00:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.59276,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23343,"TRANSGRIDV5_20161215152814","2014-12-29T01:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.574909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23344,"TRANSGRIDV5_20161215152814","2014-12-29T02:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.539149999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23345,"TRANSGRIDV5_20161215152814","2014-12-29T02:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.50623,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23346,"TRANSGRIDV5_20161215152814","2014-12-29T02:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.49535,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23347,"TRANSGRIDV5_20161215152814","2014-12-29T00:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.366989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23348,"TRANSGRIDV5_20161215152814","2014-12-29T02:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.20139,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23349,"TRANSGRIDV5_20161215152814","2014-12-29T14:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-22.501570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23350,"TRANSGRIDV5_20161215152814","2014-12-29T15:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-22.267019999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23351,"TRANSGRIDV5_20161215152814","2014-12-29T14:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.394929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23352,"TRANSGRIDV5_20161215152814","2014-12-29T05:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.35595,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23353,"TRANSGRIDV5_20161215152814","2014-12-29T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-16.21209,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23354,"TRANSGRIDV5_20161215152814","2014-12-29T14:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.99776,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23355,"TRANSGRIDV5_20161215152814","2014-12-29T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.990500000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23356,"TRANSGRIDV5_20161215152814","2014-12-29T12:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.967409999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23357,"TRANSGRIDV5_20161215152814","2014-12-29T11:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.94678,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23358,"TRANSGRIDV5_20161215152814","2014-12-29T13:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.863110000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23359,"TRANSGRIDV5_20161215152814","2014-12-29T12:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.81898,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23360,"TRANSGRIDV5_20161215152814","2014-12-29T14:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.80912,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23361,"TRANSGRIDV5_20161215152814","2014-12-29T12:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.76064,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23362,"TRANSGRIDV5_20161215152814","2014-12-29T13:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.741709999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23363,"TRANSGRIDV5_20161215152814","2014-12-29T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.62974,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23364,"TRANSGRIDV5_20161215152814","2014-12-29T13:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.61228,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23365,"TRANSGRIDV5_20161215152814","2014-12-29T14:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.586930000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23366,"TRANSGRIDV5_20161215152814","2014-12-29T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.543189999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23367,"TRANSGRIDV5_20161215152814","2014-12-29T11:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.537419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23368,"TRANSGRIDV5_20161215152814","2014-12-29T13:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.49959,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23369,"TRANSGRIDV5_20161215152814","2014-12-29T13:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.48367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23370,"TRANSGRIDV5_20161215152814","2014-12-29T13:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.47626,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23371,"TRANSGRIDV5_20161215152814","2014-12-29T13:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.46476,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23372,"TRANSGRIDV5_20161215152814","2014-12-29T12:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.461,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23373,"TRANSGRIDV5_20161215152814","2014-12-29T12:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.4267,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23374,"TRANSGRIDV5_20161215152814","2014-12-29T12:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.42257,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23375,"TRANSGRIDV5_20161215152814","2014-12-29T13:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.404059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23376,"TRANSGRIDV5_20161215152814","2014-12-29T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.37158,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23377,"TRANSGRIDV5_20161215152814","2014-12-29T13:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.363390000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23378,"TRANSGRIDV5_20161215152814","2014-12-29T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.262829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23379,"TRANSGRIDV5_20161215152814","2014-12-29T09:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.21367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23380,"TRANSGRIDV5_20161215152814","2014-12-29T11:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.12538,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23381,"TRANSGRIDV5_20161215152814","2014-12-29T11:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.110379999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23382,"TRANSGRIDV5_20161215152814","2014-12-29T11:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-15.000540000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23383,"TRANSGRIDV5_20161215152814","2014-12-29T11:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.98413,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23384,"TRANSGRIDV5_20161215152814","2014-12-29T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.94875,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23385,"TRANSGRIDV5_20161215152814","2014-12-29T14:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.91202,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23386,"TRANSGRIDV5_20161215152814","2014-12-29T14:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.845599999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23387,"TRANSGRIDV5_20161215152814","2014-12-29T12:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.842750000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23388,"TRANSGRIDV5_20161215152814","2014-12-29T13:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.7531,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23389,"TRANSGRIDV5_20161215152814","2014-12-29T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.57136,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23390,"TRANSGRIDV5_20161215152814","2014-12-29T13:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.089700000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23391,"TRANSGRIDV5_20161215152814","2014-12-29T11:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.924200000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23392,"TRANSGRIDV5_20161215152814","2014-12-29T11:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.779260000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23393,"TRANSGRIDV5_20161215152814","2014-12-29T13:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.59137,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23394,"TRANSGRIDV5_20161215152814","2014-12-29T11:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.44828,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23395,"TRANSGRIDV5_20161215152814","2014-12-29T12:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.30979,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23396,"TRANSGRIDV5_20161215152814","2014-12-29T08:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.19746,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23397,"TRANSGRIDV5_20161215152814","2014-12-29T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.983000000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23398,"TRANSGRIDV5_20161215152814","2014-12-29T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.17498,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23399,"TRANSGRIDV5_20161215152814","2014-12-29T10:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.72418,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23400,"TRANSGRIDV5_20161215152814","2014-12-29T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.720219999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23401,"TRANSGRIDV5_20161215152814","2014-12-29T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.657959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23402,"TRANSGRIDV5_20161215152814","2014-12-29T15:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.608090000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23403,"TRANSGRIDV5_20161215152814","2014-12-29T15:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.580209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23404,"TRANSGRIDV5_20161215152814","2014-12-29T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.40381,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23405,"TRANSGRIDV5_20161215152814","2014-12-29T12:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.500360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23406,"TRANSGRIDV5_20161215152814","2014-12-29T17:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.350149999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23407,"TRANSGRIDV5_20161215152814","2014-12-29T12:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.33013,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23408,"TRANSGRIDV5_20161215152814","2014-12-29T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.25367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23409,"TRANSGRIDV5_20161215152814","2014-12-29T17:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.24239,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23410,"TRANSGRIDV5_20161215152814","2014-12-29T17:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.20926,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23411,"TRANSGRIDV5_20161215152814","2014-12-29T06:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.165760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23412,"TRANSGRIDV5_20161215152814","2014-12-29T08:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.125999999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23413,"TRANSGRIDV5_20161215152814","2014-12-29T17:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.10726,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23414,"TRANSGRIDV5_20161215152814","2014-12-29T17:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.083170000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23415,"TRANSGRIDV5_20161215152814","2014-12-29T10:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.036759999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23416,"TRANSGRIDV5_20161215152814","2014-12-30T19:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-26.545200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23417,"TRANSGRIDV5_20161215152814","2014-12-30T19:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-25.509699999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23418,"TRANSGRIDV5_20161215152814","2014-12-30T20:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-24.069500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23419,"TRANSGRIDV5_20161215152814","2014-12-30T20:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-23.678049999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23420,"TRANSGRIDV5_20161215152814","2014-12-30T20:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-20.388549999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23421,"TRANSGRIDV5_20161215152814","2014-12-30T23:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-18.850989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23422,"TRANSGRIDV5_20161215152814","2014-12-30T20:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.67803,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23423,"TRANSGRIDV5_20161215152814","2014-12-30T21:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.578279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23424,"TRANSGRIDV5_20161215152814","2014-12-30T21:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.545110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23425,"TRANSGRIDV5_20161215152814","2014-12-30T20:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.418970000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23426,"TRANSGRIDV5_20161215152814","2014-12-30T20:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.261520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23427,"TRANSGRIDV5_20161215152814","2014-12-30T19:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.25393,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23428,"TRANSGRIDV5_20161215152814","2014-12-30T21:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.252310000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23429,"TRANSGRIDV5_20161215152814","2014-12-30T21:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.208690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23430,"TRANSGRIDV5_20161215152814","2014-12-30T21:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.200880000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23431,"TRANSGRIDV5_20161215152814","2014-12-30T22:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.068349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23432,"TRANSGRIDV5_20161215152814","2014-12-30T22:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-16.015989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23433,"TRANSGRIDV5_20161215152814","2014-12-30T19:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.98466,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23434,"TRANSGRIDV5_20161215152814","2014-12-30T19:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.934010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23435,"TRANSGRIDV5_20161215152814","2014-12-30T19:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.92266,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23436,"TRANSGRIDV5_20161215152814","2014-12-30T19:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.91954,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23437,"TRANSGRIDV5_20161215152814","2014-12-30T19:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.915380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23438,"TRANSGRIDV5_20161215152814","2014-12-30T19:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.82527,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23439,"TRANSGRIDV5_20161215152814","2014-12-30T18:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.71874,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23440,"TRANSGRIDV5_20161215152814","2014-12-30T19:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.642440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23441,"TRANSGRIDV5_20161215152814","2014-12-30T16:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.57366,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23442,"TRANSGRIDV5_20161215152814","2014-12-30T16:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.55349,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23443,"TRANSGRIDV5_20161215152814","2014-12-30T19:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.48218,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23444,"TRANSGRIDV5_20161215152814","2014-12-30T20:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.37299,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23445,"TRANSGRIDV5_20161215152814","2014-12-30T18:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.146509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23446,"TRANSGRIDV5_20161215152814","2014-12-30T18:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.039910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23447,"TRANSGRIDV5_20161215152814","2014-12-30T18:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.80602,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23448,"TRANSGRIDV5_20161215152814","2014-12-30T22:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.47692,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23449,"TRANSGRIDV5_20161215152814","2014-12-30T21:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.095610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23450,"TRANSGRIDV5_20161215152814","2014-12-30T20:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.991350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23451,"TRANSGRIDV5_20161215152814","2014-12-30T21:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.991350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23452,"TRANSGRIDV5_20161215152814","2014-12-30T20:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.73432,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23453,"TRANSGRIDV5_20161215152814","2014-12-30T18:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.62271,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23454,"TRANSGRIDV5_20161215152814","2014-12-30T23:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.61215,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23455,"TRANSGRIDV5_20161215152814","2014-12-30T18:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.996510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23456,"TRANSGRIDV5_20161215152814","2014-12-30T23:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.94558,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23457,"TRANSGRIDV5_20161215152814","2014-12-30T18:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.776999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23458,"TRANSGRIDV5_20161215152814","2014-12-30T20:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.52474,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23459,"TRANSGRIDV5_20161215152814","2014-12-30T19:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.438650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23460,"TRANSGRIDV5_20161215152814","2014-12-30T18:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.423249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23461,"TRANSGRIDV5_20161215152814","2014-12-30T20:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.36411,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23462,"TRANSGRIDV5_20161215152814","2014-12-30T21:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.98258,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23463,"TRANSGRIDV5_20161215152814","2014-12-30T23:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.66357,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23464,"TRANSGRIDV5_20161215152814","2014-12-30T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.38353,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23465,"TRANSGRIDV5_20161215152814","2014-12-30T21:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.21608,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23466,"TRANSGRIDV5_20161215152814","2014-12-30T22:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.125629999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23467,"TRANSGRIDV5_20161215152814","2014-12-30T20:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.11988,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23468,"TRANSGRIDV5_20161215152814","2014-12-30T23:35:00","V>>SML_NIL_7A","V-NIL","2014-01-31",1,-292.32204999999999,"Out = Nil, avoid O/L Ballarat North to Buangor 66kV line for loss of the Ballarat to Waubra to Horsham 220kV line","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23469,"TRANSGRIDV5_20161215152814","2014-12-30T14:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-14.04372,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23470,"TRANSGRIDV5_20161215152814","2014-12-30T13:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.49208,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23471,"TRANSGRIDV5_20161215152814","2014-12-30T13:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-13.47941,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23472,"TRANSGRIDV5_20161215152814","2014-12-30T12:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.93024,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23473,"TRANSGRIDV5_20161215152814","2014-12-30T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-12.801970000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23474,"TRANSGRIDV5_20161215152814","2014-12-30T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-10.897550000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23475,"TRANSGRIDV5_20161215152814","2014-12-31T23:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-29.699919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23476,"TRANSGRIDV5_20161215152814","2014-12-31T23:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-28.586040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23477,"TRANSGRIDV5_20161215152814","2014-12-31T23:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-27.409770000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23478,"TRANSGRIDV5_20161215152814","2014-12-31T23:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-26.027329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23479,"TRANSGRIDV5_20161215152814","2014-12-31T23:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-25.363140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23480,"TRANSGRIDV5_20161215152814","2014-12-31T23:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-25.264880000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23481,"TRANSGRIDV5_20161215152814","2014-12-31T23:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-25.204249999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23482,"TRANSGRIDV5_20161215152814","2014-12-31T23:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-20.549939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23483,"TRANSGRIDV5_20161215152814","2014-12-31T23:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-20.257010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23484,"TRANSGRIDV5_20161215152814","2014-12-31T23:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-18.916060000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23485,"TRANSGRIDV5_20161215152814","2014-12-31T00:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-17.721959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23486,"TRANSGRIDV5_20161215152814","2014-12-31T23:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-17.66329,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23487,"TRANSGRIDV5_20161215152814","2014-12-31T22:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-17.3718,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23488,"TRANSGRIDV5_20161215152814","2014-12-31T22:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-17.04795,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23489,"TRANSGRIDV5_20161215152814","2014-12-31T22:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-17.044129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23490,"TRANSGRIDV5_20161215152814","2014-12-31T22:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.93341,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23491,"TRANSGRIDV5_20161215152814","2014-12-31T00:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.3841,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23492,"TRANSGRIDV5_20161215152814","2014-12-31T22:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-15.331440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23493,"TRANSGRIDV5_20161215152814","2014-12-31T18:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-14.399229999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23494,"TRANSGRIDV5_20161215152814","2014-12-31T09:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-13.074870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23495,"TRANSGRIDV5_20161215152814","2014-12-31T08:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.974909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23496,"TRANSGRIDV5_20161215152814","2014-12-31T00:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.740080000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23497,"TRANSGRIDV5_20161215152814","2014-12-31T22:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.66137,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23498,"TRANSGRIDV5_20161215152814","2014-12-31T19:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.348879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23499,"TRANSGRIDV5_20161215152814","2014-12-31T09:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-12.11124,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23500,"TRANSGRIDV5_20161215152814","2014-12-31T08:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.96706,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23501,"TRANSGRIDV5_20161215152814","2014-12-31T07:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.914820000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23502,"TRANSGRIDV5_20161215152814","2014-12-31T08:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.86281,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23503,"TRANSGRIDV5_20161215152814","2014-12-31T07:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.810930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23504,"TRANSGRIDV5_20161215152814","2014-12-31T23:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.803789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23505,"TRANSGRIDV5_20161215152814","2014-12-31T19:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.70697,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23506,"TRANSGRIDV5_20161215152814","2014-12-31T08:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.704140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23507,"TRANSGRIDV5_20161215152814","2014-12-31T07:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.4559,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23508,"TRANSGRIDV5_20161215152814","2014-12-31T19:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.4528,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23509,"TRANSGRIDV5_20161215152814","2014-12-31T07:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.44036,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23510,"TRANSGRIDV5_20161215152814","2014-12-31T07:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.3986,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23511,"TRANSGRIDV5_20161215152814","2014-12-31T00:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.36896,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23512,"TRANSGRIDV5_20161215152814","2014-12-31T08:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.277839999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23513,"TRANSGRIDV5_20161215152814","2014-12-31T18:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.212949999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23514,"TRANSGRIDV5_20161215152814","2014-12-31T19:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.171559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23515,"TRANSGRIDV5_20161215152814","2014-12-31T07:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.138529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23516,"TRANSGRIDV5_20161215152814","2014-12-31T01:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.112959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23517,"TRANSGRIDV5_20161215152814","2014-12-31T00:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.11204,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23518,"TRANSGRIDV5_20161215152814","2014-12-31T08:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.10261,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23519,"TRANSGRIDV5_20161215152814","2014-12-31T01:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.093769999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23520,"TRANSGRIDV5_20161215152814","2014-12-31T15:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.063420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23521,"TRANSGRIDV5_20161215152814","2014-12-31T00:45:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.05001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23522,"TRANSGRIDV5_20161215152814","2014-12-31T01:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-11.0282,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23523,"TRANSGRIDV5_20161215152814","2014-12-31T18:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.930199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23524,"TRANSGRIDV5_20161215152814","2014-12-31T07:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.88035,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23525,"TRANSGRIDV5_20161215152814","2014-12-31T18:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.878399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23526,"TRANSGRIDV5_20161215152814","2014-12-31T19:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.852270000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23527,"TRANSGRIDV5_20161215152814","2014-12-31T16:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.841609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23528,"TRANSGRIDV5_20161215152814","2014-12-31T00:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.839869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23529,"TRANSGRIDV5_20161215152814","2014-12-31T01:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.833589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23530,"TRANSGRIDV5_20161215152814","2014-12-31T19:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.75994,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23531,"TRANSGRIDV5_20161215152814","2014-12-31T16:05:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.73761,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23532,"TRANSGRIDV5_20161215152814","2014-12-31T09:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.72228,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23533,"TRANSGRIDV5_20161215152814","2014-12-31T09:10:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.68613,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23534,"TRANSGRIDV5_20161215152814","2014-12-31T19:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.669650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23535,"TRANSGRIDV5_20161215152814","2014-12-31T09:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.651149999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23536,"TRANSGRIDV5_20161215152814","2014-12-31T09:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.646520000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23537,"TRANSGRIDV5_20161215152814","2014-12-31T08:15:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.645619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23538,"TRANSGRIDV5_20161215152814","2014-12-31T08:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.613619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23539,"TRANSGRIDV5_20161215152814","2014-12-31T01:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.560309999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23540,"TRANSGRIDV5_20161215152814","2014-12-31T00:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.5137,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23541,"TRANSGRIDV5_20161215152814","2014-12-31T22:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.472390000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23542,"TRANSGRIDV5_20161215152814","2014-12-31T09:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.40972,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23543,"TRANSGRIDV5_20161215152814","2014-12-31T08:35:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.351380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23544,"TRANSGRIDV5_20161215152814","2014-12-31T08:40:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.273860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23545,"TRANSGRIDV5_20161215152814","2014-12-31T19:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.27224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23546,"TRANSGRIDV5_20161215152814","2014-12-31T07:00:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.179779999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23547,"TRANSGRIDV5_20161215152814","2014-12-31T15:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.131690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23548,"TRANSGRIDV5_20161215152814","2014-12-31T16:20:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.12201,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23549,"TRANSGRIDV5_20161215152814","2014-12-31T16:30:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.11595,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23550,"TRANSGRIDV5_20161215152814","2014-12-31T08:50:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.114599999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23551,"TRANSGRIDV5_20161215152814","2014-12-31T08:55:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.07011,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23552,"TRANSGRIDV5_20161215152814","2014-12-31T09:25:00","V::N_NIL_V4","V-NIL","2014-10-22",1,-10.028980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]
[23553,"TRANSGRIDV5_20161215152814","2014-12-31T13:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2013-12-03",1,-11.79833,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,null,null,"",null,0]