{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Schema","Setup","MIC Template","Data Definitions","Valid Data Matrix","Data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schema","index":0,"n_rows":155,"n_cols":1,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["<xs:schema xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:xdb=\"http://xmlns.oracle.com/xdb\" xdb:storeVarrayAsTable=\"true\">"]
[]
["<!--Define exclusion clause element-->"]
["<xs:simpleType name=\"extype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:pattern value=\"[1-7]?|(3[aA])|(8\\([aA-fF]\\))|9|(10)|(11)|(12)|(99)|(INCLUDED)\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define marginal value element-->"]
["<xs:simpleType name=\"mvtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:fractionDigits value=\"5\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define TNSP element-->"]
["<xs:simpleType name=\"tnsptype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"ELECTRANET\" />"]
["<xs:enumeration value=\"TRANSGRID\" />"]
["<xs:enumeration value=\"TRANSEND\" />"]
["<xs:enumeration value=\"POWERLINK\" />"]
["<xs:enumeration value=\"AUSNET SERVICES\" />"]
["<xs:enumeration value=\"MURRAYLINK\" />"]
["<xs:enumeration value=\"DIRECTLINK\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define network condition classifications-->"]
["<xs:simpleType name=\"constrainttype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"SYSTEM NORMAL\" />"]
["<xs:enumeration value=\"OUTAGE\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define outage type classifications-->"]
["<xs:simpleType name=\"plantype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"PLANNED\" />"]
["<xs:enumeration value=\"UNPLANNED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define sub category type for classification-->"]
["<xs:simpleType name=\"subcattype\">"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"NRM\" />"]
["<xs:enumeration value=\"NSA\" />"]
["<xs:enumeration value=\"RAMP\" />"]
["<xs:enumeration value=\"FCAS\" />"]
["<xs:enumeration value=\"RECLASS\" />"]
["<xs:enumeration value=\"NC\" />"]
["<xs:enumeration value=\"DIRECTION\" />"]
["<xs:enumeration value=\"MII\" />"]
["<xs:enumeration value=\"OTHER\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define asset class type-->"]
["<xs:simpleType name=\"assettype\">"]
["<xs:union>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:enumeration value=\"REGULATED\" />"]
["<xs:enumeration value=\"NON-REGULATED\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
["<xs:simpleType>"]
["<xs:restriction base=\"xs:string\">"]
["<xs:minLength value=\"0\"/>"]
["</xs:restriction>"]
["</xs:simpleType>"]
["</xs:union>"]
["</xs:simpleType>"]
[]
["<!--Define weighting type-->"]
["<xs:simpleType name=\"wgtype\">"]
["<xs:restriction base=\"xs:decimal\">"]
["<xs:enumeration value=\"1\" />"]
["<xs:enumeration value=\"0.5\" />"]
["<xs:enumeration value=\"0.33\" />"]
["<xs:enumeration value=\"0\" />"]
["</xs:restriction>"]
["</xs:simpleType>"]
[]
["<!--Define rawdata type-->"]
["<xs:complexType name=\"rawdatatype\" xdb:SQLType=\"RAWDATA_T\">"]
["<xs:sequence>"]
["<xs:element name=\"outage\" type=\"outagetype\" maxOccurs=\"unbounded\" xdb:SQLName=\"OUTAGE\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<!--Define details type-->"]
["<xs:complexType name=\"detailstype\" xdb:SQLType=\"SUBDETAIL_T\">"]
["<xs:sequence>"]
["<xs:element name=\"stpis_version\" type=\"xs:decimal\" xdb:SQLName=\"STPIS_VERSION\" />"]
["<xs:element name=\"last_validated\" type=\"xs:dateTime\" xdb:SQLName=\"LAST_VALIDATED\" />"]
["<xs:element name=\"tnsp\" type=\"tnsptype\" xdb:SQLName=\"TNSP\" xdb:SQLType=\"VARCHAR2\"/>"]
["<xs:element name=\"performancemeasure_year\" type=\"xs:gYear\" xdb:SQLName=\"PMEASURE_YEAR\"/>"]
["<xs:element name=\"performancemeasure_from\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_FROM\" />"]
["<xs:element name=\"performancemeasure_to\" type=\"xs:dateTime\" xdb:SQLName=\"PMEASURE_TO\" />"]
["<xs:element name=\"performancemeasure_count\" type=\"xs:decimal\" xdb:SQLName=\"PMEASURE_COUNT\"/>"]
["<xs:element name=\"exclusion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"EXCLUSION_COUNT\"/>"]
["<xs:element name=\"congestion_count\" type=\"xs:nonNegativeInteger\" xdb:SQLName=\"CONGESTION_COUNT\"/>"]
["<xs:element name=\"template_version\" type=\"xs:string\" xdb:SQLName=\"TEMPLATE_VERSION\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"SUBMISSION_ID\"/>"]
["</xs:complexType>"]
[]
["<!--Define outage type-->"]
["<xs:complexType name=\"outagetype\" xdb:SQLType=\"OUTAGE_T\">"]
["<xs:sequence>"]
["<xs:element name=\"settlementdate\" type=\"xs:dateTime\" xdb:SQLName=\"SETTLEMENTDATE\" />"]
["<xs:element name=\"constraintid\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINTID\" />"]
["<xs:element name=\"constraintset\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_SET\" />"]
["<xs:element name=\"genconid_effectivedate\" type=\"xs:dateTime\" xdb:SQLName=\"GENCONID_EFFECTIVEDATE\" />"]
["<xs:element name=\"genconid_versionno\" type=\"xs:positiveInteger\" xdb:SQLName=\"GENCONID_VERSIONNO\" />"]
["<xs:element name=\"marginal_value\" type=\"mvtype\" xdb:SQLName=\"MARGINAL_VALUE\" xdb:SQLType=\"NUMBER\" />"]
["<xs:element name=\"description\" type=\"xs:string\" xdb:SQLName=\"CONSTRAINT_DESCRIPTION\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"network_condition\" type=\"constrainttype\" xdb:SQLName=\"NETWORK_CONDITION\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"category\" type=\"subcattype\" xdb:SQLName=\"NETWORK_CATEGORY\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"equipment_name\" type=\"xs:string\" xdb:SQLName=\"EQUIPMENT_NAME\" />"]
["<xs:element name=\"asset_class\" type=\"assettype\" xdb:SQLName=\"ASSET_CLASS\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"code\" type=\"extype\" xdb:SQLName=\"CODE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"exclusion_detail\" type=\"xs:string\" xdb:SQLName=\"EXCLUSION_DETAIL\" xdb:SQLType=\"CLOB\" />"]
["<xs:element name=\"outage_type\" type=\"plantype\" xdb:SQLName=\"OUTAGE_TYPE\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"weighting\" type=\"wgtype\" xdb:SQLName=\"WEIGHTING\" xdb:SQLType=\"VARCHAR2\" />"]
["<xs:element name=\"tnsp_comment\" type=\"xs:string\" xdb:SQLName=\"TNSP_COMMENT\" xdb:SQLType=\"CLOB\" />"]
["</xs:sequence>"]
["<xs:attribute name=\"outage_id\" type=\"xs:integer\" use=\"required\" xdb:SQLName=\"OUTAGE_ID\" />"]
["<xs:attribute name=\"submission_id\" type=\"xs:string\" use=\"required\" xdb:SQLName=\"OUTAGE_SUBMISSION_ID\" />"]
["</xs:complexType>"]
[]
["<!--Define root application element type-->"]
["<xs:complexType name=\"apptype\" xdb:SQLType=\"MICAPP_T\">"]
["<xs:sequence>"]
["<xs:element name=\"details\" type=\"detailstype\" />"]
["<xs:element name=\"outages\" type=\"rawdatatype\" />"]
["</xs:sequence>"]
["</xs:complexType>"]
[]
["<xs:element name=\"application\" type=\"apptype\" xdb:defaultTable=\"MIC_SUBMISSION\" />"]
[]
["</xs:schema>"]

{"sheet":"Setup","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TNSP","SCHEME","ENUMERATORS","CDATA","SUBMISSION_ID","TEMPLATEVER","EXCELVER","OSVER"]
["AUSNET SERVICES",2,"NETWORK CONDITION","CONSTRAINTID",{"$f":"'MIC Template'!N15 & \"V\" & TRUNC(TEXT('MIC Template'!N16,\"#.#\"),1) & \"_\" &TEXT(IF(ISBLANK('MIC Template'!N69),NOW(),'MIC Template'!N69),\"YYYYMMDDHHMMSS\")","v":"TRANSGRIDV5_20180116141850"},"AERMIC_VER7",{"$f":"INFO(\"RELEASE\")","v":"14.0"},{"$f":"INFO(\"OSVERSION\")","v":"Windows (32-bit) NT 6.01"}]
["DIRECTLINK",3,"CATEGORY","CONSTRAINTSET"]
["ELECTRANET",4,"ASSET CLASS","DESCRIPTION"]
["MURRAYLINK",4.0999999999999996,"OUTAGE TYPE","EQUIPMENT_NAME"]
["POWERLINK",5,"CODE","EXCLUSION_DETAIL"]
["TRANSEND",null,null,"TNSP_COMMENT"]
["TRANSGRID"]

{"sheet":"MIC Template","index":2,"n_rows":69,"n_cols":16,"rows_kept":69,"cut":false,"hidden":false,"merged":[[18,14,18,15],[18,10,18,12],[29,11,34,15],[35,10,35,15],[37,10,37,12],[39,10,39,12],[40,10,40,12],[68,10,68,12],[37,13,37,15],[39,13,39,15],[40,13,40,15],[68,13,68,15],[38,13,38,14],[38,10,38,12],[42,10,42,12],[42,13,42,15],[43,10,43,15],[44,10,44,12],[44,13,44,14],[45,10,45,12],[46,10,46,12],[0,5,0,22],[7,5,7,22],[13,13,13,15],[13,10,13,12],[14,10,14,12],[8,10,8,15],[15,10,15,12],[16,10,16,12],[17,10,17,12],[14,13,14,15],[15,13,15,15],[16,13,16,15],[17,14,17,15],[47,10,47,12],[49,10,49,12],[50,10,50,12],[51,10,51,12],[52,10,52,12],[48,10,48,12],[53,10,53,12],[54,10,54,12],[55,10,55,12],[56,10,56,12],[57,10,57,12],[58,10,58,12],[59,10,59,12],[63,10,63,12],[65,10,65,12],[64,10,64,12],[61,10,61,12],[60,10,60,12],[62,10,62,12],[45,13,45,14],[46,13,46,14],[47,13,47,14],[49,13,49,14],[50,13,50,14],[48,13,48,14],[51,13,51,14],[52,13,52,14],[53,13,53,14],[54,13,54,14],[55,13,55,14],[64,13,64,14],[65,13,65,14],[56,13,56,14],[57,13,57,14],[58,13,58,14],[59,13,59,14],[63,13,63,14],[61,13,61,14],[60,13,60,14],[62,13,62,14]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"\"Market Impact Parameter Data Template V\" & RIGHT(Setup!$F$2,LEN(Setup!$F$2)-(FIND(\"VER\",Setup!$F$2)+2))","v":"Market Impact Parameter Data Template V7"}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Steps for filling out this template"]
[null,null,null,null,null,null,null,null,null,1,"Complete  details in Table 1"]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 1",null,null,"INPUT"]
[null,null,null,null,null,null,null,null,null,null,"TNSP",null,null,"TRANSGRID"]
[null,null,null,null,null,null,null,null,null,null,"Scheme Version",null,null,5]
[null,null,null,null,null,null,null,null,null,null,"Performance Year",null,null,2017]
[null,null,null,null,null,null,null,null,null,null,"Performance Period",null,null,"From","2017-01-01"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"To","2017-12-31"]
[]
[null,null,null,null,null,null,null,null,null,2,"Enter data into the \"Data\" worksheet."]
[null,null,null,null,null,null,null,null,null,null,"Refer to the ","data definitions ","for valid data formats"]
[]
[null,null,null,null,null,null,null,null,null,3,"Complete the check list to confirm the following:"]
[null,null,null,null,null,null,null,null,null,null,"Data has been sourced from MCC constraint solution table and is on a 5-minute resolution"]
[null,null,null,null,null,null,null,null,null,null,"Evidence has been collated for all exclusion claims to be attached to the submission"]
[null,null,null,null,null,null,null,null,null,null,"All inclusion counts have a code of \"INCLUDED\" and a positive weighting"]
[]
[null,null,null,null,null,null,null,null,null,4,"Click Validate Data button"]
[null,null,null,null,null,null,null,null,null,null,null,"An error message will appear if data is invalid. The rows that contain invalid data will be highlighted yellow.  Errors will need to be amended in accordance with the data field requirements before validation can be completed. Data validation may take some time to complete. During validation, a progress indicator will appear to show progress of validation. "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Please do not close the spreadsheet during validation. "]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 2",null,null,"OUTPUT"]
[null,null,null,null,null,null,null,null,null,null,"Performance measure",null,null,null,null,{"$f":"SUM(VALUE(INDIRECT(\"Data!$Q2:$Q\" & ROWS(Data!$Q:$Q))))","v":6809.5}]
[null,null,null,null,null,null,null,null,null,null,"Exclusion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-SUMPRODUCT(--(Data!$N:$N=\"INCLUDED\"))-1","v":937}]
[null,null,null,null,null,null,null,null,null,null,"Congestion count",null,null,{"$f":"SUMPRODUCT(--(LEN(TRIM(Data!$N:$N))>0))-SUMPRODUCT(--(Data!$N:$N=\"99\"))-1","v":7929}]
[]
[null,null,null,null,null,null,null,null,null,null,"Table 3",null,null,"TNSP SUBMISSION"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEN($N$17)<4,\"\",\"Year: \" &$N$17) & IF(LEN($N$16)<1,\"\",\" Version: \" &$N$16)","v":"Year: 2017 Version: 5"}]
[null,null,null,null,null,null,null,null,null,null,"Code",null,null,"Count DIs",null,"Sum weight"]
[null,null,null,null,null,null,null,null,null,null,1,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K46)","v":24},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K46)","v":0}]
[null,null,null,null,null,null,null,null,null,null,2,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K47)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K47)","v":0}]
[null,null,null,null,null,null,null,null,null,null,3,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K48)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K48)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"3A",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K49)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K49)","v":0}]
[null,null,null,null,null,null,null,null,null,null,4,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K50)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K50)","v":0}]
[null,null,null,null,null,null,null,null,null,null,5,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K51)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K51)","v":0}]
[null,null,null,null,null,null,null,null,null,null,6,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K52)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K52)","v":0}]
[null,null,null,null,null,null,null,null,null,null,7,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K53)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K53)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(a)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K54))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K54)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(b)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K55))","v":11},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K55)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(c)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K56))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K56)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(d)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K57))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K57)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(e)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K58))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K58)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"8(f)",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,UPPER($K59))","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K59)","v":0}]
[null,null,null,null,null,null,null,null,null,null,9,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K60)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K60)","v":0}]
[null,null,null,null,null,null,null,null,null,null,10,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K61)","v":773},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K61)","v":0}]
[null,null,null,null,null,null,null,null,null,null,11,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K62)","v":129},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K62)","v":0}]
[null,null,null,null,null,null,null,null,null,null,12,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K63)","v":0},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K63)","v":0}]
[null,null,null,null,null,null,null,null,null,null,99,null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K64)","v":38759},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K64)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"INCLUDED",null,null,{"$f":"COUNTIFS(Data!$N$2:$N$1048576,$K65)","v":6992},null,{"$f":"SUMIFS(Data!$Q$2:$Q$1048576,Data!$N$2:$N$1048576,$K65)","v":6809.5}]
[null,null,null,null,null,null,null,null,null,null,"Total",null,null,{"$f":"SUM($N$46:$O$65)","v":46688},null,{"$f":"SUM($P$46:$P$65)","v":6809.5}]
[]
[null,null,null,null,null,null,null,null,null,5,"Submit to AER ONLY if the data was successfully validated"]
[null,null,null,null,null,null,null,null,null,null,"Last validation",null,null,"2018-01-16T14:18:50"]

{"sheet":"Data Definitions","index":3,"n_rows":58,"n_cols":4,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["Template instructions and data definitions"]
["What must be submitted?","- TNSP must provide performance data in this workbook in the 'Data' tab. "]
[null,"- The data submitted must conform to the data field requirements set out below. "]
[null,"- Data must be validated prior to the data being submitted to the AER for assessment. "]
[null,"- If the data does not conform to the field requirements then the data will not be able to be validated. "]
[null,"- Submit ALL binding constraints with a marginal value > $10/MWh used to manage TNSP network."]
[null,"- The data must be submitted in a 5 minute resolution and sourced from AEMO's Market Management System MCC_CONSTRAINTSOLUTION table (MCC table).   "]
[null,"- For network outage conditions, if an exclusion is applicable, TNSPs may enter the exclusion clause number in the 'CODE' field. Otherwise the code INCLUDED must be used. "]
[null,"-  The data submitted must fall within the performance period defined in the MIC Template tab. The first valid date time is 00:05 of the day defined the ‘from’ input period. "]
[null,"The last valid date time is 00:00 of the following day defined in the ‘to’ input period."]
[]
["Calcuation of performance measure:","All dispatch intervals with a marginal value greater than $10/MWh, classified as an OUTAGE and identified as INCLUDED, will be used to calculate the TNSP's performance measure. "]
[]
["Data field requirements:","Field","Description","Accepted values"]
[null,"SETTLEMENT DATE","Settlement date/time of the binding network constraint as detailed in the AEMO Market Management System MCC_CONSTRAINTSOLUTION table (MCC table)","dd/mm/yyyy hh:mm\nFirst accepted time value for the performance period is 00:05\n"]
[null,"CONSTRAINT ID","Constraint identifier from the MCC table","text"]
[null,"CONSTRAINT SET","Constraint set refers to the GENCONSET for a constraint.  These are the constraint set(s) that contain the relevant constraint ID that were invoked at the time of the binding constraint. ","text. Multiple values allowed, delimit with semi-colon e.g. V_SET1;V_SET2"]
[null,"EFFECTIVE DATE","Effective date of the constraint ID for the settlement date/time","dd/mm/yyyy hh:mm"]
[null,"VERSION NUMBER","Version number of the binding network constraint for the settlement date/time","integer"]
[null,"MARGINAL VALUE","Marginal value up to 5 decimal places (to be consistent with the MCC table) of the  binding network constraint for the settlement date/time","decimal to 5 significant figures"]
[null,"CONSTRAINT DESCRIPTION","Description of the constraint ID from the MCC table","text"]
[null,"NETWORK CONDITION","Classification of the network constraint as \"System Normal\" or \"Outage\" ","SYSTEM NORMAL | OUTAGE"]
[null,"CATEGORY","Additional categorisation of the network constraint as one of:","Note: this field cannot be left blank"]
[null,null,"-negative residues management ","NRM"]
[null,null,"-network support agreement","NSA"]
[null,null,"-ramping constraint","RAMP"]
[null,null,"-frequency control constraint","FCAS "]
[null,null,"-reclassification","RECLASS"]
[null,null,"-non-conformance","NC"]
[null,null,"-AEMO direction","DIRECTION"]
[null,null,"-manifestly incorrect input","MII "]
[null,null,"-none of the above","OTHER"]
[null,"OUTAGE EQUIPMENT","The equipment that the constraint is invoked to manage","text"]
[null,"ASSET CLASS","Identify whether the equipment is either a regulated asset or non-regulated asset.  If the equipment is in an adjoining region and the TNSP is uncertain whether the equipment is a regulated asset or non-regulated asset, the TNSP should identify it as a regulated asset. Please also indicate in the comments field that the equipment is in an adjoining region. If the equipment is in the TNSP's region, but is not part of the TNSP's network, identify the asset class as non-regulated and indicate in the comments field the type of equipment it is (i.e. generator) and who the asset owner is. ","REGULATED | NON-REGULATED "]
[null,"CODE","Provide the relevant exclusion code under version 2, 3, 4, 4.1 or 5 of the scheme in the specified format, or identify whether it is a non-inclusion in the scheme or an inclusion in the performance count. ","This field cannot be left blank for outages. It must be left blank for system normal conditions."]
[null,null,"Valid exclusion codes are: "]
[null,null,"1 to 7","1 to 7"]
[null,null,"3A","3A (only valid in version 5)"]
[null,null,"8(a)","8(a)"]
[null,null,"8(b)","8(b)"]
[null,null,"8(c) ","8(c) "]
[null,null,"8(d)","8(d)"]
[null,null,"8(e)","8(e)"]
[null,null,"8(f)","8(f)"]
[null,null,9,"9 (only valid in version 4, 4.1 and 5)"]
[null,null,"10 to 12","10 to 12 (only valid in version 5)"]
[null,null,"Or:"]
[null,null,"Non-inclusion. Non-inclusions are binding constraints with MV >$10MWh that are not part of the scheme or not relevant to the TNSP's performance count. Examples include constraints for: ramping,  non-conformance, AEMO direction and negative residues management.  FCAS constraints may be an inclusion or a non-inclusion, depending on whether it was invoked to manage an outage. See the Valid Data Matrix worksheet for more information on where to use code 99.",99]
[null,null,"Or:"]
[null,null,"Inclusion. All inclusions must be identified as included","INCLUDED"]
[null,"EXCLUSION DETAIL","Free text for TNSP to provide details on the exclusion claim (i.e. reference to supportive evidence or outage details). If there is an exclusion code specified, this field must be filled in.","text"]
[null,"OUTAGE TYPE","Where the network condition is \"OUTAGE\", the outage type must be classified as \"PLANNED\" or \"UNPLANNED\". Unplanned outages are outages taken with less than 24 hours notice to AEMO. ","PLANNED | UNPLANNED"]
[null,"WEIGHTING","The following values are valid for weighting:"]
[null,null,"-the count is wholly attributed to TNSP",1]
[null,null,"-the count is shared with one other TNSP",0.5]
[null,null,"-the count is shared with two other TNSPs",0.33]
[null,null,"-not included in the performance count. It must have a code of: \nexclusion code 1 to 7, 3A, 8(a) to 8(f), 9 to 12; or \nnon-inclusion code of 99.",0]
[null,"TNSP COMMENT","Provide any further information that will assist the AER in its assessment of the TNSP data","text"]

{"sheet":"Valid Data Matrix","index":4,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[[29,0,29,10],[30,0,30,10],[31,0,31,10],[32,0,32,10],[6,0,7,0],[6,1,7,1],[6,2,6,10],[8,0,25,0]]}
["Valid category-code data matrix"]
["This matrix shows the valid entries for a specific category-code combination. For example:"]
["There is no valid entry for category=NRM (network residue management) and code=1 (force-majeure event)"]
["There is a valid combination for category=OTHER and code=1 (force-majeure event) and the weight must be zero. Evidence must be provided."]
["There is a valid combination for category=NRM (network residue management) and code=99 with weight=0"]
[]
["NETWORK CONDITION \n= OUTAGE","FIELD=Code","Field=Category"]
[null,null,"NRM","NSA","RAMP","FCAS","RECLASS","NC","DIRECTION","MII","OTHER","Comments"]
["STPIS exclusion clause",1,null,null,null,null,null,null,null,null,null,"Force majeure event"]
[null,2,null,null,null,null,null,null,null,null,null,"Reclassification must satisfy NER cl 4.2.3A and NER cl 4.2.3B"]
[null,3,null,null,null,null,null,null,null,null,null,"Version 4 and 4.1 allows only CODE=3 with OUTAGE_TYPE=UNPLANNED  \nVersion 2, 3 and 5 allow CODE=3 with both PLANNED or UNPLANNED outages  "]
[null,"3A",null,null,null,null,null,null,null,null,null,"This code is only applicable to version 5. Only allows CODE=3A with OUTAGE_TYPE=PLANNED"]
[null,4,null,null,null,null,null,null,null,null,null,"Outage on NON-REGULATED asset"]
[null,5,null,null,null,null,null,null,null,null,null,"Outage for PERSONAL SAFETY reasons"]
[null,6,null,null,null,null,null,null,null,null,null,"AEMO DIRECTION for operational security reasons"]
[null,7,null,null,null,null,null,null,null,null,null,"Network service agreement"]
[null,"8(a)",null,null,null,null,null,null,null,null,null,"Manifestly incorrect input must satisfy NER cl 3.9.2b"]
[null,"8(b)",null,null,null,null,null,null,null,null,null,"AEMO invoked wrong constraint"]
[null,"8(c)",null,null,null,null,null,null,null,null,null,"AEMO scheduling error"]
[null,"8(d)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.12(a) "]
[null,"8(e)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.3"]
[null,"8(f)",null,null,null,null,null,null,null,null,null,"Must satisfy NER cl 3.14.2"]
[null,9,null,null,null,null,null,null,null,null,null,"Network reconfiguration. This code is not applicable to version 2 and  3 "]
[null,10,null,null,null,null,null,null,null,null,null,"Ramping constraints. Applies to version 5 only."]
[null,11,null,null,null,null,null,null,null,null,null,"Transmission connection agreements. Applies to version 5 only."]
[null,12,null,null,null,null,null,null,null,null,null,"Internetwork power tests for NCIPAP. Applies to version 5 only."]
["Non-inclusion",99,null,null,null,null,null,null,null,null,null,"Field=FCAS or OTHER may be relevant to other TNSPs. '99' for RAMP category only applies to version 4.x and below"]
["Inclusion","INCLUDED",null,null,null,null,null,null,null,null,null,"The sum of the weights is the inclusion count"]
[]
["category-code combination is NOT valid"]
["category-code combination is valid but weight must equal 0."]
["category-code combination is valid but weight must equal 0. Supporting evidence must be provided."]
["category-code combination is valid but weight must equal 0.33 or 0.5 or 1 "]

{"sheet":"Data","index":5,"n_rows":84444,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["OUTAGE ID","SUBMISSION ID","SETTLEMENT DATE","CONSTRAINT ID","CONSTRAINT SET","EFFECTIVE DATE","VERSION NUMBER","MARGINAL VALUE","CONSTRAINT DESCRIPTION","NETWORK CONDITION","CATEGORY","OUTAGE EQUIPMENT","ASSET CLASS","CODE","EXCLUSION DETAIL","OUTAGE TYPE","WEIGHTING","TNSP COMMENT"]
[1,"TRANSGRIDV5_20180116135943","2017-01-01T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1273.5231699999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2,"TRANSGRIDV5_20180116135943","2017-01-01T10:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1270.1991,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3,"TRANSGRIDV5_20180116135943","2017-01-01T12:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1264.0470499999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4,"TRANSGRIDV5_20180116135943","2017-01-01T17:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1254.22102,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5,"TRANSGRIDV5_20180116135943","2017-01-01T11:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-270.65123999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6,"TRANSGRIDV5_20180116135943","2017-01-01T11:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-267.22613999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7,"TRANSGRIDV5_20180116135943","2017-01-01T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-241.83402000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8,"TRANSGRIDV5_20180116135943","2017-01-01T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-212.04954000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9,"TRANSGRIDV5_20180116135943","2017-01-01T18:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-148.71430000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10,"TRANSGRIDV5_20180116135943","2017-01-01T15:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-146.55248,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11,"TRANSGRIDV5_20180116135943","2017-01-01T14:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-136.71767,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12,"TRANSGRIDV5_20180116135943","2017-01-01T17:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-132.56892999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13,"TRANSGRIDV5_20180116135943","2017-01-01T12:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-132.39452,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14,"TRANSGRIDV5_20180116135943","2017-01-01T14:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-70.256460000000004,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15,"TRANSGRIDV5_20180116135943","2017-01-01T14:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-55.324280000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16,"TRANSGRIDV5_20180116135943","2017-01-01T15:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.344380000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17,"TRANSGRIDV5_20180116135943","2017-01-01T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-52.251660000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18,"TRANSGRIDV5_20180116135943","2017-01-01T15:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-49.550179999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19,"TRANSGRIDV5_20180116135943","2017-01-01T16:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-48.292900000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20,"TRANSGRIDV5_20180116135943","2017-01-01T15:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-45.427439999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21,"TRANSGRIDV5_20180116135943","2017-01-01T15:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-44.485300000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22,"TRANSGRIDV5_20180116135943","2017-01-01T15:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-42.052770000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23,"TRANSGRIDV5_20180116135943","2017-01-01T15:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.879219999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24,"TRANSGRIDV5_20180116135943","2017-01-01T15:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.629060000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25,"TRANSGRIDV5_20180116135943","2017-01-01T14:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.271990000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26,"TRANSGRIDV5_20180116135943","2017-01-01T19:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.2044,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27,"TRANSGRIDV5_20180116135943","2017-01-01T21:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.113,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28,"TRANSGRIDV5_20180116135943","2017-01-01T21:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-41.09881,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29,"TRANSGRIDV5_20180116135943","2017-01-01T19:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-40.950220000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30,"TRANSGRIDV5_20180116135943","2017-01-01T20:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-40.878520000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31,"TRANSGRIDV5_20180116135943","2017-01-01T11:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-40.825499999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32,"TRANSGRIDV5_20180116135943","2017-01-01T14:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-40.762610000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33,"TRANSGRIDV5_20180116135943","2017-01-01T16:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-40.54927,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34,"TRANSGRIDV5_20180116135943","2017-01-01T18:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.784399999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35,"TRANSGRIDV5_20180116135943","2017-01-01T16:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.661180000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36,"TRANSGRIDV5_20180116135943","2017-01-01T20:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.658459999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37,"TRANSGRIDV5_20180116135943","2017-01-01T20:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.239600000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38,"TRANSGRIDV5_20180116135943","2017-01-01T19:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.093130000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39,"TRANSGRIDV5_20180116135943","2017-01-01T17:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-39.068269999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40,"TRANSGRIDV5_20180116135943","2017-01-01T20:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.714790000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41,"TRANSGRIDV5_20180116135943","2017-01-01T20:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.686399999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42,"TRANSGRIDV5_20180116135943","2017-01-01T20:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.668849999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43,"TRANSGRIDV5_20180116135943","2017-01-01T19:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.582769999999996,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44,"TRANSGRIDV5_20180116135943","2017-01-01T14:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.17503,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45,"TRANSGRIDV5_20180116135943","2017-01-01T14:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-38.149079999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46,"TRANSGRIDV5_20180116135943","2017-01-01T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.201970000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47,"TRANSGRIDV5_20180116135943","2017-01-01T15:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.108989999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48,"TRANSGRIDV5_20180116135943","2017-01-01T13:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.154119999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49,"TRANSGRIDV5_20180116135943","2017-01-01T13:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.459719999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[50,"TRANSGRIDV5_20180116135943","2017-01-01T13:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.454740000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51,"TRANSGRIDV5_20180116135943","2017-01-01T13:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.431579999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[52,"TRANSGRIDV5_20180116135943","2017-01-01T14:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.333860000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[53,"TRANSGRIDV5_20180116135943","2017-01-01T17:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.860250000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[54,"TRANSGRIDV5_20180116135943","2017-01-01T18:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.391330000000004,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[55,"TRANSGRIDV5_20180116135943","2017-01-01T18:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.287599999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[56,"TRANSGRIDV5_20180116135943","2017-01-01T16:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.819159999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[57,"TRANSGRIDV5_20180116135943","2017-01-01T17:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.785870000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[58,"TRANSGRIDV5_20180116135943","2017-01-01T17:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.774419999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[59,"TRANSGRIDV5_20180116135943","2017-01-01T17:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.758240000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[60,"TRANSGRIDV5_20180116135943","2017-01-01T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.343699999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[61,"TRANSGRIDV5_20180116135943","2017-01-01T14:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-24.700150000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[62,"TRANSGRIDV5_20180116135943","2017-01-01T11:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-24.29543,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[63,"TRANSGRIDV5_20180116135943","2017-01-01T15:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.329190000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64,"TRANSGRIDV5_20180116135943","2017-01-01T13:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.434550000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[65,"TRANSGRIDV5_20180116135943","2017-01-01T11:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.294,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[66,"TRANSGRIDV5_20180116135943","2017-01-01T10:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.53058,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[67,"TRANSGRIDV5_20180116135943","2017-01-01T14:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.354199999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68,"TRANSGRIDV5_20180116135943","2017-01-01T18:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.07752,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69,"TRANSGRIDV5_20180116135943","2017-01-01T18:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.6326,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70,"TRANSGRIDV5_20180116135943","2017-01-01T18:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-20.489439999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71,"TRANSGRIDV5_20180116135943","2017-01-01T16:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.923439999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72,"TRANSGRIDV5_20180116135943","2017-01-01T18:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.623529999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73,"TRANSGRIDV5_20180116135943","2017-01-01T19:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.57602,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[74,"TRANSGRIDV5_20180116135943","2017-01-01T19:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.56512,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[75,"TRANSGRIDV5_20180116135943","2017-01-01T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.561679999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76,"TRANSGRIDV5_20180116135943","2017-01-01T19:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.55931,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77,"TRANSGRIDV5_20180116135943","2017-01-01T19:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.511810000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78,"TRANSGRIDV5_20180116135943","2017-01-01T19:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.501059999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79,"TRANSGRIDV5_20180116135943","2017-01-01T21:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.405360000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80,"TRANSGRIDV5_20180116135943","2017-01-01T22:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.389810000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[81,"TRANSGRIDV5_20180116135943","2017-01-01T22:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.389530000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[82,"TRANSGRIDV5_20180116135943","2017-01-01T22:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.374279999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83,"TRANSGRIDV5_20180116135943","2017-01-01T20:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.188569999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84,"TRANSGRIDV5_20180116135943","2017-01-01T19:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.187750000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[85,"TRANSGRIDV5_20180116135943","2017-01-01T19:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.16827,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[86,"TRANSGRIDV5_20180116135943","2017-01-01T18:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.91187,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[87,"TRANSGRIDV5_20180116135943","2017-01-01T11:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.66339,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[88,"TRANSGRIDV5_20180116135943","2017-01-01T10:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-15.39471,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[89,"TRANSGRIDV5_20180116135943","2017-01-01T13:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-15.12086,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[90,"TRANSGRIDV5_20180116135943","2017-01-01T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-14.78797,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[91,"TRANSGRIDV5_20180116135943","2017-01-01T16:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-14.754390000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[92,"TRANSGRIDV5_20180116135943","2017-01-01T20:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-14.276759999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[93,"TRANSGRIDV5_20180116135943","2017-01-01T13:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-14.172319999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[94,"TRANSGRIDV5_20180116135943","2017-01-01T23:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-13.269119999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[95,"TRANSGRIDV5_20180116135943","2017-01-01T23:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-13.227169999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[96,"TRANSGRIDV5_20180116135943","2017-01-01T22:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-13.084519999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[97,"TRANSGRIDV5_20180116135943","2017-01-01T10:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12.133240000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[98,"TRANSGRIDV5_20180116135943","2017-01-01T16:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11.707129999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[99,"TRANSGRIDV5_20180116135943","2017-01-01T18:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11.69117,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[100,"TRANSGRIDV5_20180116135943","2017-01-01T17:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11.151210000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[101,"TRANSGRIDV5_20180116135943","2017-01-01T17:05:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-134.98528999999999,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[102,"TRANSGRIDV5_20180116135943","2017-01-01T16:55:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-32.833530000000003,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[103,"TRANSGRIDV5_20180116135943","2017-01-01T16:30:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-442.63958000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[104,"TRANSGRIDV5_20180116135943","2017-01-01T17:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-441.50997000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[105,"TRANSGRIDV5_20180116135943","2017-01-01T10:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-395.44749999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[106,"TRANSGRIDV5_20180116135943","2017-01-01T12:10:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-395.34480000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[107,"TRANSGRIDV5_20180116135943","2017-01-01T16:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-82.144949999999994,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[108,"TRANSGRIDV5_20180116135943","2017-01-01T11:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-74.760260000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[109,"TRANSGRIDV5_20180116135943","2017-01-01T15:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-71.768979999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[110,"TRANSGRIDV5_20180116135943","2017-01-01T15:55:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-48.928049999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[111,"TRANSGRIDV5_20180116135943","2017-01-01T18:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-48.21687,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[112,"TRANSGRIDV5_20180116135943","2017-01-01T17:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-42.582299999999996,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[113,"TRANSGRIDV5_20180116135943","2017-01-01T14:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-39.421199999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[114,"TRANSGRIDV5_20180116135943","2017-01-01T14:05:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-16.30031,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[115,"TRANSGRIDV5_20180116135943","2017-01-01T16:05:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-15.79013,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[116,"TRANSGRIDV5_20180116135943","2017-01-01T15:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-15.531409999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[117,"TRANSGRIDV5_20180116135943","2017-01-01T15:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-15.5144,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[118,"TRANSGRIDV5_20180116135943","2017-01-01T15:35:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-13.67286,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[119,"TRANSGRIDV5_20180116135943","2017-01-01T14:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-12.36872,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[120,"TRANSGRIDV5_20180116135943","2017-01-01T15:25:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-12.3405,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[121,"TRANSGRIDV5_20180116135943","2017-01-01T15:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-12.15606,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[122,"TRANSGRIDV5_20180116135943","2017-01-01T15:20:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-11.7956,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[123,"TRANSGRIDV5_20180116135943","2017-01-01T16:35:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-11.78631,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[124,"TRANSGRIDV5_20180116135943","2017-01-01T17:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-11.659890000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[125,"TRANSGRIDV5_20180116135943","2017-01-01T16:25:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-11.38808,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[126,"TRANSGRIDV5_20180116135943","2017-01-01T19:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.754160000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[127,"TRANSGRIDV5_20180116135943","2017-01-01T19:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.546519999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[128,"TRANSGRIDV5_20180116135943","2017-01-01T20:05:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.472099999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[129,"TRANSGRIDV5_20180116135943","2017-01-01T15:30:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.45457,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[130,"TRANSGRIDV5_20180116135943","2017-01-01T15:10:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.40645,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[131,"TRANSGRIDV5_20180116135943","2017-01-01T19:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-01",83,-10.2158,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[132,"TRANSGRIDV5_20180116135943","2017-01-01T11:50:00","N>N-NIL_LSDU","N-NIL","2014-02-13",1,-67.378380000000007,"Out = Nil, avoid overloading Lismore to Dunoon line (9U6 or 9U7) on trip of the other Lismore to Dunoon line (9U7 or 9U6), Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[133,"TRANSGRIDV5_20180116135943","2017-01-01T12:05:00","N>N-NIL_LSDU","N-NIL","2014-02-13",1,-31.899730000000002,"Out = Nil, avoid overloading Lismore to Dunoon line (9U6 or 9U7) on trip of the other Lismore to Dunoon line (9U7 or 9U6), Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[134,"TRANSGRIDV5_20180116135943","2017-01-01T16:15:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-50.988169999999997,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[135,"TRANSGRIDV5_20180116135943","2017-01-01T12:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-25.77835,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[136,"TRANSGRIDV5_20180116135943","2017-01-01T17:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-21.7819,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[137,"TRANSGRIDV5_20180116135943","2017-01-01T15:00:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-20.156960000000002,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[138,"TRANSGRIDV5_20180116135943","2017-01-01T14:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-19.027560000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[139,"TRANSGRIDV5_20180116135943","2017-01-01T16:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-16.64499,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[140,"TRANSGRIDV5_20180116135943","2017-01-01T16:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-16.14705,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[141,"TRANSGRIDV5_20180116135943","2017-01-01T15:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-15.775270000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[142,"TRANSGRIDV5_20180116135943","2017-01-01T12:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-15.50803,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[143,"TRANSGRIDV5_20180116135943","2017-01-01T12:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.78899,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[144,"TRANSGRIDV5_20180116135943","2017-01-01T12:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.787100000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[145,"TRANSGRIDV5_20180116135943","2017-01-01T15:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.29584,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[146,"TRANSGRIDV5_20180116135943","2017-01-01T16:00:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.926550000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[147,"TRANSGRIDV5_20180116135943","2017-01-01T16:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.606310000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[148,"TRANSGRIDV5_20180116135943","2017-01-01T15:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.54542,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[149,"TRANSGRIDV5_20180116135943","2017-01-01T16:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.46274,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[150,"TRANSGRIDV5_20180116135943","2017-01-01T14:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-12.705970000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[151,"TRANSGRIDV5_20180116135943","2017-01-01T13:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.69711,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[152,"TRANSGRIDV5_20180116135943","2017-01-01T14:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.616250000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[153,"TRANSGRIDV5_20180116135943","2017-01-01T13:05:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.21818,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[154,"TRANSGRIDV5_20180116135943","2017-01-01T13:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.094810000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[155,"TRANSGRIDV5_20180116135943","2017-01-01T13:10:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.0398,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[156,"TRANSGRIDV5_20180116135943","2017-01-01T00:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-82.997590000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[157,"TRANSGRIDV5_20180116135943","2017-01-01T18:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-31.647459999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[158,"TRANSGRIDV5_20180116135943","2017-01-01T12:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-29.600149999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[159,"TRANSGRIDV5_20180116135943","2017-01-01T10:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-24.148489999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[160,"TRANSGRIDV5_20180116135943","2017-01-01T18:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-22.730879999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[161,"TRANSGRIDV5_20180116135943","2017-01-01T18:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-22.335460000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[162,"TRANSGRIDV5_20180116135943","2017-01-01T10:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-22.058669999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[163,"TRANSGRIDV5_20180116135943","2017-01-01T18:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-21.331440000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[164,"TRANSGRIDV5_20180116135943","2017-01-01T18:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.407029999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[165,"TRANSGRIDV5_20180116135943","2017-01-01T11:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.179300000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[166,"TRANSGRIDV5_20180116135943","2017-01-01T19:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-18.997779999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[167,"TRANSGRIDV5_20180116135943","2017-01-01T11:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-18.938680000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[168,"TRANSGRIDV5_20180116135943","2017-01-01T12:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.451180000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[169,"TRANSGRIDV5_20180116135943","2017-01-01T18:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.405529999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[170,"TRANSGRIDV5_20180116135943","2017-01-01T10:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.388839999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[171,"TRANSGRIDV5_20180116135943","2017-01-01T11:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.281690000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[172,"TRANSGRIDV5_20180116135943","2017-01-01T19:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.05574,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[173,"TRANSGRIDV5_20180116135943","2017-01-01T16:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-16.655850000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[174,"TRANSGRIDV5_20180116135943","2017-01-01T11:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-16.560929999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[175,"TRANSGRIDV5_20180116135943","2017-01-01T11:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.78734,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[176,"TRANSGRIDV5_20180116135943","2017-01-01T16:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.021929999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[177,"TRANSGRIDV5_20180116135943","2017-01-01T16:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.886990000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[178,"TRANSGRIDV5_20180116135943","2017-01-01T13:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.51831,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[179,"TRANSGRIDV5_20180116135943","2017-01-01T16:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.34834,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[180,"TRANSGRIDV5_20180116135943","2017-01-01T19:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.301780000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[181,"TRANSGRIDV5_20180116135943","2017-01-01T10:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.26136,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[182,"TRANSGRIDV5_20180116135943","2017-01-01T19:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.197559999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[183,"TRANSGRIDV5_20180116135943","2017-01-01T15:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.325189999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[184,"TRANSGRIDV5_20180116135943","2017-01-01T11:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.06277,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[185,"TRANSGRIDV5_20180116135943","2017-01-01T11:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.91362,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[186,"TRANSGRIDV5_20180116135943","2017-01-01T11:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.91466,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[187,"TRANSGRIDV5_20180116135943","2017-01-01T10:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.79349,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[188,"TRANSGRIDV5_20180116135943","2017-01-01T17:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.64115,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[189,"TRANSGRIDV5_20180116135943","2017-01-01T10:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.63208,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[190,"TRANSGRIDV5_20180116135943","2017-01-01T11:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.331060000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[191,"TRANSGRIDV5_20180116135943","2017-01-01T09:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.92231,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[192,"TRANSGRIDV5_20180116135943","2017-01-01T18:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.470090000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[193,"TRANSGRIDV5_20180116135943","2017-01-01T11:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.39588,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[194,"TRANSGRIDV5_20180116135943","2017-01-01T18:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.236319999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[195,"TRANSGRIDV5_20180116135943","2017-01-01T00:05:00","SVML_ROC_80","S-NIL","2016-08-23",1,-125.00615000000001,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[196,"TRANSGRIDV5_20180116135943","2017-01-01T00:05:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-81.210419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[197,"TRANSGRIDV5_20180116135943","2017-01-01T00:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-258.43702999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[198,"TRANSGRIDV5_20180116135943","2017-01-01T00:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-217.41405,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[199,"TRANSGRIDV5_20180116135943","2017-01-01T00:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-172.24171000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[200,"TRANSGRIDV5_20180116135943","2017-01-01T00:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-94.101929999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[201,"TRANSGRIDV5_20180116135943","2017-01-01T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.261139999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[202,"TRANSGRIDV5_20180116135943","2017-01-01T00:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.978560000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[203,"TRANSGRIDV5_20180116135943","2017-01-01T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.307169999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[204,"TRANSGRIDV5_20180116135943","2017-01-01T01:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.689390000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[205,"TRANSGRIDV5_20180116135943","2017-01-01T00:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-61.271189999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[206,"TRANSGRIDV5_20180116135943","2017-01-01T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-60.273350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[207,"TRANSGRIDV5_20180116135943","2017-01-01T10:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-55.049259999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[208,"TRANSGRIDV5_20180116135943","2017-01-01T00:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-53.482999999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[209,"TRANSGRIDV5_20180116135943","2017-01-01T10:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-53.08916,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[210,"TRANSGRIDV5_20180116135943","2017-01-01T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-52.95861,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[211,"TRANSGRIDV5_20180116135943","2017-01-01T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-51.29759,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[212,"TRANSGRIDV5_20180116135943","2017-01-01T10:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-44.565469999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[213,"TRANSGRIDV5_20180116135943","2017-01-01T10:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-42.717919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[214,"TRANSGRIDV5_20180116135943","2017-01-01T02:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-41.315530000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[215,"TRANSGRIDV5_20180116135943","2017-01-01T10:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-40.153489999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[216,"TRANSGRIDV5_20180116135943","2017-01-01T10:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-37.89517,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[217,"TRANSGRIDV5_20180116135943","2017-01-01T11:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-36.761789999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[218,"TRANSGRIDV5_20180116135943","2017-01-01T11:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-36.446129999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[219,"TRANSGRIDV5_20180116135943","2017-01-01T02:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-35.517960000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[220,"TRANSGRIDV5_20180116135943","2017-01-01T09:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.177720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[221,"TRANSGRIDV5_20180116135943","2017-01-01T10:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.272080000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[222,"TRANSGRIDV5_20180116135943","2017-01-01T02:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.087609999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[223,"TRANSGRIDV5_20180116135943","2017-01-01T02:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.048360000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[224,"TRANSGRIDV5_20180116135943","2017-01-01T02:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.69191,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[225,"TRANSGRIDV5_20180116135943","2017-01-01T02:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.629750000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[226,"TRANSGRIDV5_20180116135943","2017-01-01T01:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.380240000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[227,"TRANSGRIDV5_20180116135943","2017-01-01T02:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.270340000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[228,"TRANSGRIDV5_20180116135943","2017-01-01T01:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.268090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[229,"TRANSGRIDV5_20180116135943","2017-01-01T10:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.347339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[230,"TRANSGRIDV5_20180116135943","2017-01-01T03:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.314550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[231,"TRANSGRIDV5_20180116135943","2017-01-01T10:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.750440000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[232,"TRANSGRIDV5_20180116135943","2017-01-01T09:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.707260000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[233,"TRANSGRIDV5_20180116135943","2017-01-01T02:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.04177,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[234,"TRANSGRIDV5_20180116135943","2017-01-01T02:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.030380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[235,"TRANSGRIDV5_20180116135943","2017-01-01T01:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.86299,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[236,"TRANSGRIDV5_20180116135943","2017-01-01T01:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.815190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[237,"TRANSGRIDV5_20180116135943","2017-01-01T04:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.49729,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[238,"TRANSGRIDV5_20180116135943","2017-01-01T04:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.48386,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[239,"TRANSGRIDV5_20180116135943","2017-01-01T04:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.480370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[240,"TRANSGRIDV5_20180116135943","2017-01-01T03:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.283110000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[241,"TRANSGRIDV5_20180116135943","2017-01-01T04:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.171250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[242,"TRANSGRIDV5_20180116135943","2017-01-01T04:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.396139999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[243,"TRANSGRIDV5_20180116135943","2017-01-01T03:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.11186,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[244,"TRANSGRIDV5_20180116135943","2017-01-01T09:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.110399999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[245,"TRANSGRIDV5_20180116135943","2017-01-01T11:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.032060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[246,"TRANSGRIDV5_20180116135943","2017-01-01T04:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.99363,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[247,"TRANSGRIDV5_20180116135943","2017-01-01T02:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.741250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[248,"TRANSGRIDV5_20180116135943","2017-01-01T01:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.71611,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[249,"TRANSGRIDV5_20180116135943","2017-01-01T09:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.714680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[250,"TRANSGRIDV5_20180116135943","2017-01-01T01:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.626650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[251,"TRANSGRIDV5_20180116135943","2017-01-01T03:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.353010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[252,"TRANSGRIDV5_20180116135943","2017-01-01T09:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.320799999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[253,"TRANSGRIDV5_20180116135943","2017-01-01T04:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.238630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[254,"TRANSGRIDV5_20180116135943","2017-01-01T01:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.234660000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[255,"TRANSGRIDV5_20180116135943","2017-01-01T04:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.234480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[256,"TRANSGRIDV5_20180116135943","2017-01-01T04:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.889800000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[257,"TRANSGRIDV5_20180116135943","2017-01-01T04:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.85304,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[258,"TRANSGRIDV5_20180116135943","2017-01-01T04:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.82161,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[259,"TRANSGRIDV5_20180116135943","2017-01-01T01:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.471969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[260,"TRANSGRIDV5_20180116135943","2017-01-01T03:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.361969999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[261,"TRANSGRIDV5_20180116135943","2017-01-01T09:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.232939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[262,"TRANSGRIDV5_20180116135943","2017-01-01T09:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.202559999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[263,"TRANSGRIDV5_20180116135943","2017-01-01T09:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.176369999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[264,"TRANSGRIDV5_20180116135943","2017-01-01T05:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.137090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[265,"TRANSGRIDV5_20180116135943","2017-01-01T05:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.136959999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[266,"TRANSGRIDV5_20180116135943","2017-01-01T01:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.755030000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[267,"TRANSGRIDV5_20180116135943","2017-01-01T05:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.716650000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[268,"TRANSGRIDV5_20180116135943","2017-01-01T02:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.564579999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[269,"TRANSGRIDV5_20180116135943","2017-01-01T09:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.198070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[270,"TRANSGRIDV5_20180116135943","2017-01-01T04:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.130980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[271,"TRANSGRIDV5_20180116135943","2017-01-01T05:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.957660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[272,"TRANSGRIDV5_20180116135943","2017-01-01T01:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.763000000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[273,"TRANSGRIDV5_20180116135943","2017-01-01T09:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.69106,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[274,"TRANSGRIDV5_20180116135943","2017-01-01T09:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.677050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[275,"TRANSGRIDV5_20180116135943","2017-01-01T03:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.596039999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[276,"TRANSGRIDV5_20180116135943","2017-01-01T05:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.233499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[277,"TRANSGRIDV5_20180116135943","2017-01-01T05:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.764209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[278,"TRANSGRIDV5_20180116135943","2017-01-01T03:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.448540000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[279,"TRANSGRIDV5_20180116135943","2017-01-01T06:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.003740000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[280,"TRANSGRIDV5_20180116135943","2017-01-01T09:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.682790000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[281,"TRANSGRIDV5_20180116135943","2017-01-01T06:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.505420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[282,"TRANSGRIDV5_20180116135943","2017-01-01T03:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.5032,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[283,"TRANSGRIDV5_20180116135943","2017-01-01T06:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.402740000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[284,"TRANSGRIDV5_20180116135943","2017-01-01T08:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.36626,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[285,"TRANSGRIDV5_20180116135943","2017-01-01T08:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.332789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[286,"TRANSGRIDV5_20180116135943","2017-01-01T07:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.167870000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[287,"TRANSGRIDV5_20180116135943","2017-01-01T05:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.00048,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[288,"TRANSGRIDV5_20180116135943","2017-01-01T03:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.921379999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[289,"TRANSGRIDV5_20180116135943","2017-01-01T05:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.841010000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[290,"TRANSGRIDV5_20180116135943","2017-01-01T02:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.646450000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[291,"TRANSGRIDV5_20180116135943","2017-01-01T03:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.592420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[292,"TRANSGRIDV5_20180116135943","2017-01-01T03:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.571549999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[293,"TRANSGRIDV5_20180116135943","2017-01-01T07:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.969810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[294,"TRANSGRIDV5_20180116135943","2017-01-01T06:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.965,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[295,"TRANSGRIDV5_20180116135943","2017-01-01T07:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.842140000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[296,"TRANSGRIDV5_20180116135943","2017-01-01T07:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.71224,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[297,"TRANSGRIDV5_20180116135943","2017-01-01T07:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.49858,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[298,"TRANSGRIDV5_20180116135943","2017-01-01T07:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.481529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[299,"TRANSGRIDV5_20180116135943","2017-01-01T06:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.89156,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[300,"TRANSGRIDV5_20180116135943","2017-01-01T07:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.810639999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[301,"TRANSGRIDV5_20180116135943","2017-01-01T07:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.791700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[302,"TRANSGRIDV5_20180116135943","2017-01-01T07:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.79092,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[303,"TRANSGRIDV5_20180116135943","2017-01-01T07:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.774089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[304,"TRANSGRIDV5_20180116135943","2017-01-01T07:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.76004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[305,"TRANSGRIDV5_20180116135943","2017-01-01T07:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.53834,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[306,"TRANSGRIDV5_20180116135943","2017-01-01T05:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.515700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[307,"TRANSGRIDV5_20180116135943","2017-01-01T05:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.19022,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[308,"TRANSGRIDV5_20180116135943","2017-01-01T06:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.450570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[309,"TRANSGRIDV5_20180116135943","2017-01-01T06:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.789350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[310,"TRANSGRIDV5_20180116135943","2017-01-01T12:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-51.637349999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[311,"TRANSGRIDV5_20180116135943","2017-01-01T16:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-50.19164,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[312,"TRANSGRIDV5_20180116135943","2017-01-01T12:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-46.321899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[313,"TRANSGRIDV5_20180116135943","2017-01-01T17:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-45.811889999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[314,"TRANSGRIDV5_20180116135943","2017-01-01T11:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-45.698770000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[315,"TRANSGRIDV5_20180116135943","2017-01-01T11:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-45.698770000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[316,"TRANSGRIDV5_20180116135943","2017-01-01T18:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-41.856459999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[317,"TRANSGRIDV5_20180116135943","2017-01-01T11:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-41.042360000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[318,"TRANSGRIDV5_20180116135943","2017-01-01T11:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.979089999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[319,"TRANSGRIDV5_20180116135943","2017-01-01T11:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.316049999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[320,"TRANSGRIDV5_20180116135943","2017-01-01T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.113790000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[321,"TRANSGRIDV5_20180116135943","2017-01-01T12:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-38.965490000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[322,"TRANSGRIDV5_20180116135943","2017-01-01T11:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-38.813070000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[323,"TRANSGRIDV5_20180116135943","2017-01-01T12:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.768689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[324,"TRANSGRIDV5_20180116135943","2017-01-01T12:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.761209999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[325,"TRANSGRIDV5_20180116135943","2017-01-01T11:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.35812,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[326,"TRANSGRIDV5_20180116135943","2017-01-01T13:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.728110000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[327,"TRANSGRIDV5_20180116135943","2017-01-01T13:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.487749999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[328,"TRANSGRIDV5_20180116135943","2017-01-01T22:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.071739999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[329,"TRANSGRIDV5_20180116135943","2017-01-01T16:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.065939999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[330,"TRANSGRIDV5_20180116135943","2017-01-01T11:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-35.976979999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[331,"TRANSGRIDV5_20180116135943","2017-01-01T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-35.975409999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[332,"TRANSGRIDV5_20180116135943","2017-01-01T18:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.240810000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[333,"TRANSGRIDV5_20180116135943","2017-01-01T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.200650000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[334,"TRANSGRIDV5_20180116135943","2017-01-01T18:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-33.92183,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[335,"TRANSGRIDV5_20180116135943","2017-01-01T18:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-32.109490000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[336,"TRANSGRIDV5_20180116135943","2017-01-01T18:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-31.73038,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[337,"TRANSGRIDV5_20180116135943","2017-01-01T11:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-30.449400000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[338,"TRANSGRIDV5_20180116135943","2017-01-01T13:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-29.614560000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[339,"TRANSGRIDV5_20180116135943","2017-01-01T12:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.956119999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[340,"TRANSGRIDV5_20180116135943","2017-01-01T17:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.849460000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[341,"TRANSGRIDV5_20180116135943","2017-01-01T16:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.417639999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[342,"TRANSGRIDV5_20180116135943","2017-01-01T16:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.408709999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[343,"TRANSGRIDV5_20180116135943","2017-01-01T14:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.24325,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[344,"TRANSGRIDV5_20180116135943","2017-01-01T18:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.023260000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[345,"TRANSGRIDV5_20180116135943","2017-01-01T12:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.794930000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[346,"TRANSGRIDV5_20180116135943","2017-01-01T13:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.72062,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[347,"TRANSGRIDV5_20180116135943","2017-01-01T13:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.479679999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[348,"TRANSGRIDV5_20180116135943","2017-01-01T13:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.46406,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[349,"TRANSGRIDV5_20180116135943","2017-01-01T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.378920000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[350,"TRANSGRIDV5_20180116135943","2017-01-01T13:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.196449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[351,"TRANSGRIDV5_20180116135943","2017-01-01T13:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.194839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[352,"TRANSGRIDV5_20180116135943","2017-01-01T19:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.889900000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[353,"TRANSGRIDV5_20180116135943","2017-01-01T16:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.302869999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[354,"TRANSGRIDV5_20180116135943","2017-01-01T16:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.277950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[355,"TRANSGRIDV5_20180116135943","2017-01-01T14:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.929929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[356,"TRANSGRIDV5_20180116135943","2017-01-01T18:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.596039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[357,"TRANSGRIDV5_20180116135943","2017-01-01T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.485420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[358,"TRANSGRIDV5_20180116135943","2017-01-01T19:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.48517,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[359,"TRANSGRIDV5_20180116135943","2017-01-01T16:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.073740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[360,"TRANSGRIDV5_20180116135943","2017-01-01T16:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.846589999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[361,"TRANSGRIDV5_20180116135943","2017-01-01T16:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.635449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[362,"TRANSGRIDV5_20180116135943","2017-01-01T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.63449,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[363,"TRANSGRIDV5_20180116135943","2017-01-01T19:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.915489999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[364,"TRANSGRIDV5_20180116135943","2017-01-01T15:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.75686,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[365,"TRANSGRIDV5_20180116135943","2017-01-01T19:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.729869999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[366,"TRANSGRIDV5_20180116135943","2017-01-01T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.653670000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[367,"TRANSGRIDV5_20180116135943","2017-01-01T18:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.065729999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[368,"TRANSGRIDV5_20180116135943","2017-01-01T18:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.057559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[369,"TRANSGRIDV5_20180116135943","2017-01-01T17:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.70449,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[370,"TRANSGRIDV5_20180116135943","2017-01-01T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.640160000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[371,"TRANSGRIDV5_20180116135943","2017-01-01T17:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.593769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[372,"TRANSGRIDV5_20180116135943","2017-01-01T17:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.48864,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[373,"TRANSGRIDV5_20180116135943","2017-01-01T17:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.485029999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[374,"TRANSGRIDV5_20180116135943","2017-01-01T17:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.34919,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[375,"TRANSGRIDV5_20180116135943","2017-01-01T17:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.331029999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[376,"TRANSGRIDV5_20180116135943","2017-01-01T15:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.992329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[377,"TRANSGRIDV5_20180116135943","2017-01-01T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.963979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[378,"TRANSGRIDV5_20180116135943","2017-01-01T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.963940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[379,"TRANSGRIDV5_20180116135943","2017-01-01T14:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.707699999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[380,"TRANSGRIDV5_20180116135943","2017-01-01T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.69623,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[381,"TRANSGRIDV5_20180116135943","2017-01-01T13:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.52008,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[382,"TRANSGRIDV5_20180116135943","2017-01-01T14:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.513200000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[383,"TRANSGRIDV5_20180116135943","2017-01-01T13:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.511500000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[384,"TRANSGRIDV5_20180116135943","2017-01-01T13:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.50929,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[385,"TRANSGRIDV5_20180116135943","2017-01-01T14:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.152290000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[386,"TRANSGRIDV5_20180116135943","2017-01-01T10:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.097100000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[387,"TRANSGRIDV5_20180116135943","2017-01-01T21:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.8505,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[388,"TRANSGRIDV5_20180116135943","2017-01-01T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.784929999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[389,"TRANSGRIDV5_20180116135943","2017-01-01T13:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.72794,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[390,"TRANSGRIDV5_20180116135943","2017-01-01T19:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.230340000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[391,"TRANSGRIDV5_20180116135943","2017-01-01T21:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.192460000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[392,"TRANSGRIDV5_20180116135943","2017-01-01T19:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.017849999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[393,"TRANSGRIDV5_20180116135943","2017-01-01T19:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.700780000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[394,"TRANSGRIDV5_20180116135943","2017-01-01T18:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.17267,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[395,"TRANSGRIDV5_20180116135943","2017-01-01T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.981480000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[396,"TRANSGRIDV5_20180116135943","2017-01-01T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.886489999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[397,"TRANSGRIDV5_20180116135943","2017-01-01T20:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.709250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[398,"TRANSGRIDV5_20180116135943","2017-01-01T21:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.677810000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[399,"TRANSGRIDV5_20180116135943","2017-01-01T21:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.652010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[400,"TRANSGRIDV5_20180116135943","2017-01-01T14:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.624320000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[401,"TRANSGRIDV5_20180116135943","2017-01-01T20:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.533989999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[402,"TRANSGRIDV5_20180116135943","2017-01-01T20:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.532360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[403,"TRANSGRIDV5_20180116135943","2017-01-01T20:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.529959999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[404,"TRANSGRIDV5_20180116135943","2017-01-01T18:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.52711,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[405,"TRANSGRIDV5_20180116135943","2017-01-01T20:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.526499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[406,"TRANSGRIDV5_20180116135943","2017-01-01T20:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.524480000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[407,"TRANSGRIDV5_20180116135943","2017-01-01T20:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.511410000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[408,"TRANSGRIDV5_20180116135943","2017-01-01T20:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.507400000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[409,"TRANSGRIDV5_20180116135943","2017-01-01T21:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.503540000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[410,"TRANSGRIDV5_20180116135943","2017-01-01T19:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.503080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[411,"TRANSGRIDV5_20180116135943","2017-01-01T21:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.482690000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[412,"TRANSGRIDV5_20180116135943","2017-01-01T21:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.468160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[413,"TRANSGRIDV5_20180116135943","2017-01-01T21:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.461549999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[414,"TRANSGRIDV5_20180116135943","2017-01-01T20:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.310310000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[415,"TRANSGRIDV5_20180116135943","2017-01-01T14:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.141449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[416,"TRANSGRIDV5_20180116135943","2017-01-01T15:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.121359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[417,"TRANSGRIDV5_20180116135943","2017-01-01T18:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.079640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[418,"TRANSGRIDV5_20180116135943","2017-01-01T21:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.99746,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[419,"TRANSGRIDV5_20180116135943","2017-01-01T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.97664,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[420,"TRANSGRIDV5_20180116135943","2017-01-01T23:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.92239,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[421,"TRANSGRIDV5_20180116135943","2017-01-01T19:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.799689999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[422,"TRANSGRIDV5_20180116135943","2017-01-01T20:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.776820000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[423,"TRANSGRIDV5_20180116135943","2017-01-01T20:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.77355,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[424,"TRANSGRIDV5_20180116135943","2017-01-01T19:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.696750000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[425,"TRANSGRIDV5_20180116135943","2017-01-01T22:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.687950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[426,"TRANSGRIDV5_20180116135943","2017-01-01T10:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.686029999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[427,"TRANSGRIDV5_20180116135943","2017-01-01T10:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.68451,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[428,"TRANSGRIDV5_20180116135943","2017-01-01T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.601680000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[429,"TRANSGRIDV5_20180116135943","2017-01-01T23:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.601310000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[430,"TRANSGRIDV5_20180116135943","2017-01-01T20:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.569579999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[431,"TRANSGRIDV5_20180116135943","2017-01-01T19:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.53079,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[432,"TRANSGRIDV5_20180116135943","2017-01-01T19:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.50367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[433,"TRANSGRIDV5_20180116135943","2017-01-01T23:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.322700000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[434,"TRANSGRIDV5_20180116135943","2017-01-01T23:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.279800000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[435,"TRANSGRIDV5_20180116135943","2017-01-01T23:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.2651,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[436,"TRANSGRIDV5_20180116135943","2017-01-01T15:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.233529999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[437,"TRANSGRIDV5_20180116135943","2017-01-01T08:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.005179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[438,"TRANSGRIDV5_20180116135943","2017-01-01T22:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.731580000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[439,"TRANSGRIDV5_20180116135943","2017-01-01T21:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.725619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[440,"TRANSGRIDV5_20180116135943","2017-01-01T22:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.508600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[441,"TRANSGRIDV5_20180116135943","2017-01-01T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.32086,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[442,"TRANSGRIDV5_20180116135943","2017-01-01T17:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.181170000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[443,"TRANSGRIDV5_20180116135943","2017-01-01T17:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.105640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[444,"TRANSGRIDV5_20180116135943","2017-01-01T12:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.784000000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[445,"TRANSGRIDV5_20180116135943","2017-01-01T08:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.74076,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[446,"TRANSGRIDV5_20180116135943","2017-01-01T16:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.72946,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[447,"TRANSGRIDV5_20180116135943","2017-01-01T12:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.35361,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[448,"TRANSGRIDV5_20180116135943","2017-01-01T22:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.15405,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[449,"TRANSGRIDV5_20180116135943","2017-01-01T22:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.63377,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[450,"TRANSGRIDV5_20180116135943","2017-01-01T12:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.468059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[451,"TRANSGRIDV5_20180116135943","2017-01-01T17:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.99465,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[452,"TRANSGRIDV5_20180116135943","2017-01-01T23:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.600849999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[453,"TRANSGRIDV5_20180116135943","2017-01-01T23:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.596109999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[454,"TRANSGRIDV5_20180116135943","2017-01-01T23:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.54393,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[455,"TRANSGRIDV5_20180116135943","2017-01-01T22:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.293139999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[456,"TRANSGRIDV5_20180116135943","2017-01-01T23:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.244529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[457,"TRANSGRIDV5_20180116135943","2017-01-01T08:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.15038,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[458,"TRANSGRIDV5_20180116135943","2017-01-01T22:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.122769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[459,"TRANSGRIDV5_20180116135943","2017-01-01T22:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.848990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[460,"TRANSGRIDV5_20180116135943","2017-01-01T22:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.813700000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[461,"TRANSGRIDV5_20180116135943","2017-01-01T22:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.799659999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[462,"TRANSGRIDV5_20180116135943","2017-01-01T22:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.65091,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[463,"TRANSGRIDV5_20180116135943","2017-01-01T23:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.212680000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[464,"TRANSGRIDV5_20180116135943","2017-01-01T21:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.083399999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[465,"TRANSGRIDV5_20180116135943","2017-01-01T01:55:00","VSML_220","V-NIL","2012-07-04",1,-14.61378,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[466,"TRANSGRIDV5_20180116135943","2017-01-01T01:00:00","VSML_ROC_80","V-NIL","2016-08-23",1,-16.308199999999999,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[467,"TRANSGRIDV5_20180116135943","2017-01-02T11:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1250.61088,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[468,"TRANSGRIDV5_20180116135943","2017-01-02T09:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-142.31631999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[469,"TRANSGRIDV5_20180116135943","2017-01-02T08:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-136.47463999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[470,"TRANSGRIDV5_20180116135943","2017-01-02T08:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-132.0462,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[471,"TRANSGRIDV5_20180116135943","2017-01-02T09:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-132.00459000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[472,"TRANSGRIDV5_20180116135943","2017-01-02T09:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-129.11174,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[473,"TRANSGRIDV5_20180116135943","2017-01-02T15:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-128.20313999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[474,"TRANSGRIDV5_20180116135943","2017-01-02T15:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-128.1429,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[475,"TRANSGRIDV5_20180116135943","2017-01-02T15:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-116.79862,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[476,"TRANSGRIDV5_20180116135943","2017-01-02T09:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-115.25911000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[477,"TRANSGRIDV5_20180116135943","2017-01-02T14:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-113.94417,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[478,"TRANSGRIDV5_20180116135943","2017-01-02T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-113.52408,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[479,"TRANSGRIDV5_20180116135943","2017-01-02T16:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-113.49518,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[480,"TRANSGRIDV5_20180116135943","2017-01-02T16:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-110.33632,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[481,"TRANSGRIDV5_20180116135943","2017-01-02T14:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-86.699939999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[482,"TRANSGRIDV5_20180116135943","2017-01-02T16:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-86.434849999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[483,"TRANSGRIDV5_20180116135943","2017-01-02T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-84.734440000000006,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[484,"TRANSGRIDV5_20180116135943","2017-01-02T16:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-65.244540000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[485,"TRANSGRIDV5_20180116135943","2017-01-02T16:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-64.578059999999994,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[486,"TRANSGRIDV5_20180116135943","2017-01-02T16:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-64.57732,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[487,"TRANSGRIDV5_20180116135943","2017-01-02T16:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-64.434200000000004,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[488,"TRANSGRIDV5_20180116135943","2017-01-02T15:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-37.719790000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[489,"TRANSGRIDV5_20180116135943","2017-01-02T08:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.913249999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[490,"TRANSGRIDV5_20180116135943","2017-01-02T08:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.753639999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[491,"TRANSGRIDV5_20180116135943","2017-01-02T13:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.362349999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[492,"TRANSGRIDV5_20180116135943","2017-01-02T13:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.328580000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[493,"TRANSGRIDV5_20180116135943","2017-01-02T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.04815,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[494,"TRANSGRIDV5_20180116135943","2017-01-02T08:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.921149999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[495,"TRANSGRIDV5_20180116135943","2017-01-02T08:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.89911,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[496,"TRANSGRIDV5_20180116135943","2017-01-02T08:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.883969999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[497,"TRANSGRIDV5_20180116135943","2017-01-02T08:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.695320000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[498,"TRANSGRIDV5_20180116135943","2017-01-02T08:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-33.659410000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[499,"TRANSGRIDV5_20180116135943","2017-01-02T13:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.22043,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[500,"TRANSGRIDV5_20180116135943","2017-01-02T13:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-31.70194,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[501,"TRANSGRIDV5_20180116135943","2017-01-02T15:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-31.52704,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[502,"TRANSGRIDV5_20180116135943","2017-01-02T18:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-30.43449,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[503,"TRANSGRIDV5_20180116135943","2017-01-02T10:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-29.846139999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[504,"TRANSGRIDV5_20180116135943","2017-01-02T10:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-27.708169999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[505,"TRANSGRIDV5_20180116135943","2017-01-02T10:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-27.688649999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[506,"TRANSGRIDV5_20180116135943","2017-01-02T10:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-27.15605,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[507,"TRANSGRIDV5_20180116135943","2017-01-02T08:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-25.928570000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[508,"TRANSGRIDV5_20180116135943","2017-01-02T19:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-22.360579999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[509,"TRANSGRIDV5_20180116135943","2017-01-02T20:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-21.063639999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[510,"TRANSGRIDV5_20180116135943","2017-01-02T11:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.494070000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[511,"TRANSGRIDV5_20180116135943","2017-01-02T11:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.49174,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[512,"TRANSGRIDV5_20180116135943","2017-01-02T13:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.445070000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[513,"TRANSGRIDV5_20180116135943","2017-01-02T11:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.39019,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[514,"TRANSGRIDV5_20180116135943","2017-01-02T14:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.038979999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[515,"TRANSGRIDV5_20180116135943","2017-01-02T14:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.014479999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[516,"TRANSGRIDV5_20180116135943","2017-01-02T13:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.857690000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[517,"TRANSGRIDV5_20180116135943","2017-01-02T19:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.731929999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[518,"TRANSGRIDV5_20180116135943","2017-01-02T16:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.6997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[519,"TRANSGRIDV5_20180116135943","2017-01-02T10:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.59207,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[520,"TRANSGRIDV5_20180116135943","2017-01-02T10:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.187560000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[521,"TRANSGRIDV5_20180116135943","2017-01-02T10:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.062049999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[522,"TRANSGRIDV5_20180116135943","2017-01-02T10:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.023890000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[523,"TRANSGRIDV5_20180116135943","2017-01-02T19:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.834589999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[524,"TRANSGRIDV5_20180116135943","2017-01-02T19:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.826589999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[525,"TRANSGRIDV5_20180116135943","2017-01-02T19:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.767209999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[526,"TRANSGRIDV5_20180116135943","2017-01-02T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.751729999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[527,"TRANSGRIDV5_20180116135943","2017-01-02T19:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.748899999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[528,"TRANSGRIDV5_20180116135943","2017-01-02T11:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.502009999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[529,"TRANSGRIDV5_20180116135943","2017-01-02T11:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.451149999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[530,"TRANSGRIDV5_20180116135943","2017-01-02T20:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.382809999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[531,"TRANSGRIDV5_20180116135943","2017-01-02T11:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.382180000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[532,"TRANSGRIDV5_20180116135943","2017-01-02T11:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.381869999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[533,"TRANSGRIDV5_20180116135943","2017-01-02T11:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.371670000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[534,"TRANSGRIDV5_20180116135943","2017-01-02T09:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.371210000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[535,"TRANSGRIDV5_20180116135943","2017-01-02T11:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.328890000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[536,"TRANSGRIDV5_20180116135943","2017-01-02T11:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.319030000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[537,"TRANSGRIDV5_20180116135943","2017-01-02T18:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.210809999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[538,"TRANSGRIDV5_20180116135943","2017-01-02T13:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.183689999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[539,"TRANSGRIDV5_20180116135943","2017-01-02T12:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.121220000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[540,"TRANSGRIDV5_20180116135943","2017-01-02T13:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.07817,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[541,"TRANSGRIDV5_20180116135943","2017-01-02T13:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.074770000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[542,"TRANSGRIDV5_20180116135943","2017-01-02T13:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.040120000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[543,"TRANSGRIDV5_20180116135943","2017-01-02T12:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.027270000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[544,"TRANSGRIDV5_20180116135943","2017-01-02T12:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.911860000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[545,"TRANSGRIDV5_20180116135943","2017-01-02T14:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.721170000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[546,"TRANSGRIDV5_20180116135943","2017-01-02T17:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.716709999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[547,"TRANSGRIDV5_20180116135943","2017-01-02T17:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.635100000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[548,"TRANSGRIDV5_20180116135943","2017-01-02T16:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.607099999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[549,"TRANSGRIDV5_20180116135943","2017-01-02T17:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.586590000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[550,"TRANSGRIDV5_20180116135943","2017-01-02T16:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.579090000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[551,"TRANSGRIDV5_20180116135943","2017-01-02T16:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.517330000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[552,"TRANSGRIDV5_20180116135943","2017-01-02T17:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.442620000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[553,"TRANSGRIDV5_20180116135943","2017-01-02T19:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-16.024370000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[554,"TRANSGRIDV5_20180116135943","2017-01-02T09:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-15.145770000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[555,"TRANSGRIDV5_20180116135943","2017-01-02T18:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12.711650000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[556,"TRANSGRIDV5_20180116135943","2017-01-02T10:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12.657539999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[557,"TRANSGRIDV5_20180116135943","2017-01-02T17:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12.16661,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[558,"TRANSGRIDV5_20180116135943","2017-01-02T10:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-12.026109999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[559,"TRANSGRIDV5_20180116135943","2017-01-02T13:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11.36726,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[560,"TRANSGRIDV5_20180116135943","2017-01-02T08:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11.0192,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[561,"TRANSGRIDV5_20180116135943","2017-01-02T19:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10.950609999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[562,"TRANSGRIDV5_20180116135943","2017-01-02T00:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10.38022,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[563,"TRANSGRIDV5_20180116135943","2017-01-02T20:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10.208959999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[564,"TRANSGRIDV5_20180116135943","2017-01-02T18:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10.15053,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[565,"TRANSGRIDV5_20180116135943","2017-01-02T19:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-10.067080000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[566,"TRANSGRIDV5_20180116135943","2017-01-02T11:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-395.81867,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[567,"TRANSGRIDV5_20180116135943","2017-01-02T15:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-41.395150000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[568,"TRANSGRIDV5_20180116135943","2017-01-02T15:20:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-40.78246,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[569,"TRANSGRIDV5_20180116135943","2017-01-02T15:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-40.73359,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[570,"TRANSGRIDV5_20180116135943","2017-01-02T16:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-39.296169999999996,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[571,"TRANSGRIDV5_20180116135943","2017-01-02T09:00:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-37.32208,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[572,"TRANSGRIDV5_20180116135943","2017-01-02T16:30:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-36.920830000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[573,"TRANSGRIDV5_20180116135943","2017-01-02T16:35:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-35.72625,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[574,"TRANSGRIDV5_20180116135943","2017-01-02T08:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-35.476320000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[575,"TRANSGRIDV5_20180116135943","2017-01-02T09:05:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-35.041969999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[576,"TRANSGRIDV5_20180116135943","2017-01-02T09:10:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-34.286369999999998,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[577,"TRANSGRIDV5_20180116135943","2017-01-02T08:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-34.093420000000002,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[578,"TRANSGRIDV5_20180116135943","2017-01-02T14:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-32.33878,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[579,"TRANSGRIDV5_20180116135943","2017-01-02T16:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-28.717199999999998,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[580,"TRANSGRIDV5_20180116135943","2017-01-02T09:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-27.61495,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[581,"TRANSGRIDV5_20180116135943","2017-01-02T15:40:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-25.748249999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[582,"TRANSGRIDV5_20180116135943","2017-01-02T14:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-23.801780000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[583,"TRANSGRIDV5_20180116135943","2017-01-02T16:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-21.43572,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[584,"TRANSGRIDV5_20180116135943","2017-01-02T16:15:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-19.69932,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[585,"TRANSGRIDV5_20180116135943","2017-01-02T16:10:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-19.69896,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[586,"TRANSGRIDV5_20180116135943","2017-01-02T16:25:00","N>LSDU_LSDU","CA_AUTO","2017-01-02",59,-19.116289999999999,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[587,"TRANSGRIDV5_20180116135943","2017-01-02T15:40:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-16.424410000000002,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[588,"TRANSGRIDV5_20180116135943","2017-01-02T16:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-11.935650000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[589,"TRANSGRIDV5_20180116135943","2017-01-02T15:25:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-11.096579999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[590,"TRANSGRIDV5_20180116135943","2017-01-02T23:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-152.81560999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[591,"TRANSGRIDV5_20180116135943","2017-01-02T23:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-27.317620000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[592,"TRANSGRIDV5_20180116135943","2017-01-02T23:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-18.098230000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[593,"TRANSGRIDV5_20180116135943","2017-01-02T23:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.233930000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[594,"TRANSGRIDV5_20180116135943","2017-01-02T22:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.288449999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[595,"TRANSGRIDV5_20180116135943","2017-01-02T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.989129999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[596,"TRANSGRIDV5_20180116135943","2017-01-02T23:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.10379,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[597,"TRANSGRIDV5_20180116135943","2017-01-02T22:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.48278,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[598,"TRANSGRIDV5_20180116135943","2017-01-02T23:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.432919999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[599,"TRANSGRIDV5_20180116135943","2017-01-02T22:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.78434,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[600,"TRANSGRIDV5_20180116135943","2017-01-02T22:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.721959999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[601,"TRANSGRIDV5_20180116135943","2017-01-02T22:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.87748,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[602,"TRANSGRIDV5_20180116135943","2017-01-02T23:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.327909999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[603,"TRANSGRIDV5_20180116135943","2017-01-02T09:15:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-47.556510000000003,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[604,"TRANSGRIDV5_20180116135943","2017-01-02T08:45:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-45.420189999999998,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[605,"TRANSGRIDV5_20180116135943","2017-01-02T08:50:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-43.67774,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[606,"TRANSGRIDV5_20180116135943","2017-01-02T08:40:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-43.287570000000002,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[607,"TRANSGRIDV5_20180116135943","2017-01-02T09:00:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-43.210760000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[608,"TRANSGRIDV5_20180116135943","2017-01-02T08:55:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-42.883850000000002,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[609,"TRANSGRIDV5_20180116135943","2017-01-02T08:35:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-42.737319999999997,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[610,"TRANSGRIDV5_20180116135943","2017-01-02T09:20:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-40.13832,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[611,"TRANSGRIDV5_20180116135943","2017-01-02T09:05:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-38.167900000000003,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[612,"TRANSGRIDV5_20180116135943","2017-01-02T06:30:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-36.803280000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[613,"TRANSGRIDV5_20180116135943","2017-01-02T09:30:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-35.711190000000002,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[614,"TRANSGRIDV5_20180116135943","2017-01-02T09:35:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-35.701090000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[615,"TRANSGRIDV5_20180116135943","2017-01-02T09:40:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-35.472499999999997,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[616,"TRANSGRIDV5_20180116135943","2017-01-02T09:25:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-35.318379999999998,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[617,"TRANSGRIDV5_20180116135943","2017-01-02T09:45:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-35.025799999999997,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[618,"TRANSGRIDV5_20180116135943","2017-01-02T07:05:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-33.598059999999997,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[619,"TRANSGRIDV5_20180116135943","2017-01-02T06:25:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-26.225680000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[620,"TRANSGRIDV5_20180116135943","2017-01-02T07:20:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-26.162050000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[621,"TRANSGRIDV5_20180116135943","2017-01-02T09:10:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-24.324200000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[622,"TRANSGRIDV5_20180116135943","2017-01-02T07:35:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-24.213830000000002,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[623,"TRANSGRIDV5_20180116135943","2017-01-02T07:15:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-24.129549999999998,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[624,"TRANSGRIDV5_20180116135943","2017-01-02T06:55:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-13.92883,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[625,"TRANSGRIDV5_20180116135943","2017-01-02T21:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-42.901580000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[626,"TRANSGRIDV5_20180116135943","2017-01-02T18:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-40.769170000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[627,"TRANSGRIDV5_20180116135943","2017-01-02T06:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.179989999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[628,"TRANSGRIDV5_20180116135943","2017-01-02T21:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.607410000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[629,"TRANSGRIDV5_20180116135943","2017-01-02T17:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.124479999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[630,"TRANSGRIDV5_20180116135943","2017-01-02T20:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.55406,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[631,"TRANSGRIDV5_20180116135943","2017-01-02T20:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.094000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[632,"TRANSGRIDV5_20180116135943","2017-01-02T19:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.50149,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[633,"TRANSGRIDV5_20180116135943","2017-01-02T03:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.492599999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[634,"TRANSGRIDV5_20180116135943","2017-01-02T05:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.768470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[635,"TRANSGRIDV5_20180116135943","2017-01-02T06:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.541429999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[636,"TRANSGRIDV5_20180116135943","2017-01-02T20:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.23601,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[637,"TRANSGRIDV5_20180116135943","2017-01-02T03:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.752020000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[638,"TRANSGRIDV5_20180116135943","2017-01-02T20:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.38655,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[639,"TRANSGRIDV5_20180116135943","2017-01-02T00:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.056480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[640,"TRANSGRIDV5_20180116135943","2017-01-02T06:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.905760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[641,"TRANSGRIDV5_20180116135943","2017-01-02T20:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.04819,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[642,"TRANSGRIDV5_20180116135943","2017-01-02T05:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.35051,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[643,"TRANSGRIDV5_20180116135943","2017-01-02T05:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.34258,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[644,"TRANSGRIDV5_20180116135943","2017-01-02T04:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.32531,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[645,"TRANSGRIDV5_20180116135943","2017-01-02T05:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.320499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[646,"TRANSGRIDV5_20180116135943","2017-01-02T20:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.008760000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[647,"TRANSGRIDV5_20180116135943","2017-01-02T23:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-191.88248999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[648,"TRANSGRIDV5_20180116135943","2017-01-02T18:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-56.812399999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[649,"TRANSGRIDV5_20180116135943","2017-01-02T18:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-55.002299999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[650,"TRANSGRIDV5_20180116135943","2017-01-02T22:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-51.207410000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[651,"TRANSGRIDV5_20180116135943","2017-01-02T23:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-46.713209999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[652,"TRANSGRIDV5_20180116135943","2017-01-02T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-43.896059999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[653,"TRANSGRIDV5_20180116135943","2017-01-02T18:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-40.819800000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[654,"TRANSGRIDV5_20180116135943","2017-01-02T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-40.67906,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[655,"TRANSGRIDV5_20180116135943","2017-01-02T18:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.856560000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[656,"TRANSGRIDV5_20180116135943","2017-01-02T15:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.652209999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[657,"TRANSGRIDV5_20180116135943","2017-01-02T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.562950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[658,"TRANSGRIDV5_20180116135943","2017-01-02T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.394120000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[659,"TRANSGRIDV5_20180116135943","2017-01-02T14:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.147590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[660,"TRANSGRIDV5_20180116135943","2017-01-02T12:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.588509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[661,"TRANSGRIDV5_20180116135943","2017-01-02T17:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.524290000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[662,"TRANSGRIDV5_20180116135943","2017-01-02T17:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.138759999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[663,"TRANSGRIDV5_20180116135943","2017-01-02T18:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.080770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[664,"TRANSGRIDV5_20180116135943","2017-01-02T18:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.82593,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[665,"TRANSGRIDV5_20180116135943","2017-01-02T18:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.811929999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[666,"TRANSGRIDV5_20180116135943","2017-01-02T16:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.777819999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[667,"TRANSGRIDV5_20180116135943","2017-01-02T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.301699999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[668,"TRANSGRIDV5_20180116135943","2017-01-02T23:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.058250000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[669,"TRANSGRIDV5_20180116135943","2017-01-02T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-32.603569999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[670,"TRANSGRIDV5_20180116135943","2017-01-02T23:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-32.415959999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[671,"TRANSGRIDV5_20180116135943","2017-01-02T22:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-31.442900000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[672,"TRANSGRIDV5_20180116135943","2017-01-02T18:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-29.827780000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[673,"TRANSGRIDV5_20180116135943","2017-01-02T15:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-29.315950000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[674,"TRANSGRIDV5_20180116135943","2017-01-02T17:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.6859,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[675,"TRANSGRIDV5_20180116135943","2017-01-02T23:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.652560000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[676,"TRANSGRIDV5_20180116135943","2017-01-02T22:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.325279999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[677,"TRANSGRIDV5_20180116135943","2017-01-02T23:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.0686,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[678,"TRANSGRIDV5_20180116135943","2017-01-02T11:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.837350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[679,"TRANSGRIDV5_20180116135943","2017-01-02T16:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.667269999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[680,"TRANSGRIDV5_20180116135943","2017-01-02T19:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.606549999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[681,"TRANSGRIDV5_20180116135943","2017-01-02T18:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.59741,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[682,"TRANSGRIDV5_20180116135943","2017-01-02T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.45318,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[683,"TRANSGRIDV5_20180116135943","2017-01-02T16:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.36468,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[684,"TRANSGRIDV5_20180116135943","2017-01-02T22:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.30781,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[685,"TRANSGRIDV5_20180116135943","2017-01-02T22:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.305319999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[686,"TRANSGRIDV5_20180116135943","2017-01-02T22:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.301179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[687,"TRANSGRIDV5_20180116135943","2017-01-02T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.294070000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[688,"TRANSGRIDV5_20180116135943","2017-01-02T10:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.273820000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[689,"TRANSGRIDV5_20180116135943","2017-01-02T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.27298,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[690,"TRANSGRIDV5_20180116135943","2017-01-02T22:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.267320000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[691,"TRANSGRIDV5_20180116135943","2017-01-02T19:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.240819999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[692,"TRANSGRIDV5_20180116135943","2017-01-02T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.20412,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[693,"TRANSGRIDV5_20180116135943","2017-01-02T22:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.20102,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[694,"TRANSGRIDV5_20180116135943","2017-01-02T14:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.18168,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[695,"TRANSGRIDV5_20180116135943","2017-01-02T13:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.172540000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[696,"TRANSGRIDV5_20180116135943","2017-01-02T12:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.171620000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[697,"TRANSGRIDV5_20180116135943","2017-01-02T11:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.085180000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[698,"TRANSGRIDV5_20180116135943","2017-01-02T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.059090000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[699,"TRANSGRIDV5_20180116135943","2017-01-02T14:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.005279999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[700,"TRANSGRIDV5_20180116135943","2017-01-02T12:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.969080000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[701,"TRANSGRIDV5_20180116135943","2017-01-02T14:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.92962,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[702,"TRANSGRIDV5_20180116135943","2017-01-02T14:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.914719999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[703,"TRANSGRIDV5_20180116135943","2017-01-02T14:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.654949999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[704,"TRANSGRIDV5_20180116135943","2017-01-02T16:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.572310000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[705,"TRANSGRIDV5_20180116135943","2017-01-02T22:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.472359999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[706,"TRANSGRIDV5_20180116135943","2017-01-02T20:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.45795,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[707,"TRANSGRIDV5_20180116135943","2017-01-02T09:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.222470000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[708,"TRANSGRIDV5_20180116135943","2017-01-02T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.04909,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[709,"TRANSGRIDV5_20180116135943","2017-01-02T16:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.0242,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[710,"TRANSGRIDV5_20180116135943","2017-01-02T10:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.90438,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[711,"TRANSGRIDV5_20180116135943","2017-01-02T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.823879999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[712,"TRANSGRIDV5_20180116135943","2017-01-02T13:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.630420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[713,"TRANSGRIDV5_20180116135943","2017-01-02T10:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.581479999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[714,"TRANSGRIDV5_20180116135943","2017-01-02T12:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.497409999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[715,"TRANSGRIDV5_20180116135943","2017-01-02T19:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.452369999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[716,"TRANSGRIDV5_20180116135943","2017-01-02T12:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.428840000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[717,"TRANSGRIDV5_20180116135943","2017-01-02T22:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.400099999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[718,"TRANSGRIDV5_20180116135943","2017-01-02T10:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.304770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[719,"TRANSGRIDV5_20180116135943","2017-01-02T19:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.647659999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[720,"TRANSGRIDV5_20180116135943","2017-01-02T16:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.424330000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[721,"TRANSGRIDV5_20180116135943","2017-01-02T16:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.394690000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[722,"TRANSGRIDV5_20180116135943","2017-01-02T16:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.39442,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[723,"TRANSGRIDV5_20180116135943","2017-01-02T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.385169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[724,"TRANSGRIDV5_20180116135943","2017-01-02T19:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.368500000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[725,"TRANSGRIDV5_20180116135943","2017-01-02T19:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.362369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[726,"TRANSGRIDV5_20180116135943","2017-01-02T18:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.34911,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[727,"TRANSGRIDV5_20180116135943","2017-01-02T19:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.339359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[728,"TRANSGRIDV5_20180116135943","2017-01-02T19:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.335190000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[729,"TRANSGRIDV5_20180116135943","2017-01-02T16:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.306509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[730,"TRANSGRIDV5_20180116135943","2017-01-02T11:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.21566,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[731,"TRANSGRIDV5_20180116135943","2017-01-02T11:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.165369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[732,"TRANSGRIDV5_20180116135943","2017-01-02T16:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.090389999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[733,"TRANSGRIDV5_20180116135943","2017-01-02T19:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.070160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[734,"TRANSGRIDV5_20180116135943","2017-01-02T21:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.060449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[735,"TRANSGRIDV5_20180116135943","2017-01-02T11:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.959530000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[736,"TRANSGRIDV5_20180116135943","2017-01-02T11:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.953669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[737,"TRANSGRIDV5_20180116135943","2017-01-02T11:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.93197,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[738,"TRANSGRIDV5_20180116135943","2017-01-02T10:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.910789999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[739,"TRANSGRIDV5_20180116135943","2017-01-02T11:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.910340000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[740,"TRANSGRIDV5_20180116135943","2017-01-02T13:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.882239999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[741,"TRANSGRIDV5_20180116135943","2017-01-02T11:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.87602,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[742,"TRANSGRIDV5_20180116135943","2017-01-02T11:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.872720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[743,"TRANSGRIDV5_20180116135943","2017-01-02T10:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.645199999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[744,"TRANSGRIDV5_20180116135943","2017-01-02T10:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.644300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[745,"TRANSGRIDV5_20180116135943","2017-01-02T13:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.63747,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[746,"TRANSGRIDV5_20180116135943","2017-01-02T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.635570000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[747,"TRANSGRIDV5_20180116135943","2017-01-02T12:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.59582,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[748,"TRANSGRIDV5_20180116135943","2017-01-02T12:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.59224,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[749,"TRANSGRIDV5_20180116135943","2017-01-02T10:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.56071,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[750,"TRANSGRIDV5_20180116135943","2017-01-02T13:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.54401,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[751,"TRANSGRIDV5_20180116135943","2017-01-02T12:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.539349999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[752,"TRANSGRIDV5_20180116135943","2017-01-02T19:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.425850000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[753,"TRANSGRIDV5_20180116135943","2017-01-02T12:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.361799999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[754,"TRANSGRIDV5_20180116135943","2017-01-02T13:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.25713,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[755,"TRANSGRIDV5_20180116135943","2017-01-02T02:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.05659,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[756,"TRANSGRIDV5_20180116135943","2017-01-02T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.564579999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[757,"TRANSGRIDV5_20180116135943","2017-01-02T23:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.206939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[758,"TRANSGRIDV5_20180116135943","2017-01-02T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.974350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[759,"TRANSGRIDV5_20180116135943","2017-01-02T17:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.906739999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[760,"TRANSGRIDV5_20180116135943","2017-01-02T23:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.7925,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[761,"TRANSGRIDV5_20180116135943","2017-01-02T17:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.704070000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[762,"TRANSGRIDV5_20180116135943","2017-01-02T22:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.65071,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[763,"TRANSGRIDV5_20180116135943","2017-01-02T08:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.605979999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[764,"TRANSGRIDV5_20180116135943","2017-01-02T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.600719999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[765,"TRANSGRIDV5_20180116135943","2017-01-02T12:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.458960000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[766,"TRANSGRIDV5_20180116135943","2017-01-02T09:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.426269999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[767,"TRANSGRIDV5_20180116135943","2017-01-02T08:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.404689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[768,"TRANSGRIDV5_20180116135943","2017-01-02T02:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.393899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[769,"TRANSGRIDV5_20180116135943","2017-01-02T14:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.39124,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[770,"TRANSGRIDV5_20180116135943","2017-01-02T08:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.339030000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[771,"TRANSGRIDV5_20180116135943","2017-01-02T12:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.338840000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[772,"TRANSGRIDV5_20180116135943","2017-01-02T08:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.33371,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[773,"TRANSGRIDV5_20180116135943","2017-01-02T08:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.33334,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[774,"TRANSGRIDV5_20180116135943","2017-01-02T15:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.323519999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[775,"TRANSGRIDV5_20180116135943","2017-01-02T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.133109999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[776,"TRANSGRIDV5_20180116135943","2017-01-02T02:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.911560000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[777,"TRANSGRIDV5_20180116135943","2017-01-02T23:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.569489999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[778,"TRANSGRIDV5_20180116135943","2017-01-02T10:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.520710000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[779,"TRANSGRIDV5_20180116135943","2017-01-02T10:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.51426,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[780,"TRANSGRIDV5_20180116135943","2017-01-02T23:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.511289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[781,"TRANSGRIDV5_20180116135943","2017-01-02T10:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.489629999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[782,"TRANSGRIDV5_20180116135943","2017-01-02T17:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.434799999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[783,"TRANSGRIDV5_20180116135943","2017-01-02T17:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.428260000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[784,"TRANSGRIDV5_20180116135943","2017-01-02T17:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.34441,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[785,"TRANSGRIDV5_20180116135943","2017-01-02T17:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.338799999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[786,"TRANSGRIDV5_20180116135943","2017-01-02T17:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.32668,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[787,"TRANSGRIDV5_20180116135943","2017-01-02T18:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.204450000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[788,"TRANSGRIDV5_20180116135943","2017-01-02T20:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.066610000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[789,"TRANSGRIDV5_20180116135943","2017-01-02T11:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.627179999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[790,"TRANSGRIDV5_20180116135943","2017-01-02T11:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.603300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[791,"TRANSGRIDV5_20180116135943","2017-01-02T05:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.310420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[792,"TRANSGRIDV5_20180116135943","2017-01-02T20:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.252320000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[793,"TRANSGRIDV5_20180116135943","2017-01-02T13:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.227509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[794,"TRANSGRIDV5_20180116135943","2017-01-02T13:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.195789999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[795,"TRANSGRIDV5_20180116135943","2017-01-02T21:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.12876,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[796,"TRANSGRIDV5_20180116135943","2017-01-02T05:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.070180000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[797,"TRANSGRIDV5_20180116135943","2017-01-02T15:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.542079999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[798,"TRANSGRIDV5_20180116135943","2017-01-02T21:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.361740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[799,"TRANSGRIDV5_20180116135943","2017-01-02T21:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.33447,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[800,"TRANSGRIDV5_20180116135943","2017-01-02T06:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.31155,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[801,"TRANSGRIDV5_20180116135943","2017-01-02T00:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.305070000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[802,"TRANSGRIDV5_20180116135943","2017-01-02T21:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.259720000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[803,"TRANSGRIDV5_20180116135943","2017-01-02T21:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.253640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[804,"TRANSGRIDV5_20180116135943","2017-01-02T21:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.236129999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[805,"TRANSGRIDV5_20180116135943","2017-01-02T13:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.16553,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[806,"TRANSGRIDV5_20180116135943","2017-01-02T07:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.163170000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[807,"TRANSGRIDV5_20180116135943","2017-01-02T02:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.089110000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[808,"TRANSGRIDV5_20180116135943","2017-01-02T07:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.031359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[809,"TRANSGRIDV5_20180116135943","2017-01-02T05:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.96848,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[810,"TRANSGRIDV5_20180116135943","2017-01-02T13:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.95412,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[811,"TRANSGRIDV5_20180116135943","2017-01-02T13:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.944099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[812,"TRANSGRIDV5_20180116135943","2017-01-02T21:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.898689999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[813,"TRANSGRIDV5_20180116135943","2017-01-02T21:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.852969999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[814,"TRANSGRIDV5_20180116135943","2017-01-02T03:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.81305,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[815,"TRANSGRIDV5_20180116135943","2017-01-02T01:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.798249999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[816,"TRANSGRIDV5_20180116135943","2017-01-02T00:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.713069999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[817,"TRANSGRIDV5_20180116135943","2017-01-02T20:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.60585,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[818,"TRANSGRIDV5_20180116135943","2017-01-02T23:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.512879999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[819,"TRANSGRIDV5_20180116135943","2017-01-02T08:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.97833,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[820,"TRANSGRIDV5_20180116135943","2017-01-02T13:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.929040000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[821,"TRANSGRIDV5_20180116135943","2017-01-02T06:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.555289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[822,"TRANSGRIDV5_20180116135943","2017-01-02T02:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.17855,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[823,"TRANSGRIDV5_20180116135943","2017-01-02T00:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.08042,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[824,"TRANSGRIDV5_20180116135943","2017-01-02T22:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.031790000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[825,"TRANSGRIDV5_20180116135943","2017-01-02T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.982150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[826,"TRANSGRIDV5_20180116135943","2017-01-02T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.83553,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[827,"TRANSGRIDV5_20180116135943","2017-01-02T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.66466,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[828,"TRANSGRIDV5_20180116135943","2017-01-02T01:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.443809999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[829,"TRANSGRIDV5_20180116135943","2017-01-02T10:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.189069999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[830,"TRANSGRIDV5_20180116135943","2017-01-02T20:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.039899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[831,"TRANSGRIDV5_20180116135943","2017-01-02T21:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.03955,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[832,"TRANSGRIDV5_20180116135943","2017-01-02T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.94913,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[833,"TRANSGRIDV5_20180116135943","2017-01-02T00:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.87825,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[834,"TRANSGRIDV5_20180116135943","2017-01-02T01:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.759309999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[835,"TRANSGRIDV5_20180116135943","2017-01-02T03:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.560169999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[836,"TRANSGRIDV5_20180116135943","2017-01-02T03:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.40944,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[837,"TRANSGRIDV5_20180116135943","2017-01-02T00:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.38818,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[838,"TRANSGRIDV5_20180116135943","2017-01-02T03:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.38588,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[839,"TRANSGRIDV5_20180116135943","2017-01-02T02:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.18567,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[840,"TRANSGRIDV5_20180116135943","2017-01-02T00:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.966150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[841,"TRANSGRIDV5_20180116135943","2017-01-02T06:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.87311,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[842,"TRANSGRIDV5_20180116135943","2017-01-02T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.83067,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[843,"TRANSGRIDV5_20180116135943","2017-01-02T01:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.67029,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[844,"TRANSGRIDV5_20180116135943","2017-01-02T06:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.41732,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[845,"TRANSGRIDV5_20180116135943","2017-01-02T06:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.3804,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[846,"TRANSGRIDV5_20180116135943","2017-01-02T20:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.346080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[847,"TRANSGRIDV5_20180116135943","2017-01-02T19:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.34281,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[848,"TRANSGRIDV5_20180116135943","2017-01-02","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.32498,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[849,"TRANSGRIDV5_20180116135943","2017-01-02T00:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.294409999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[850,"TRANSGRIDV5_20180116135943","2017-01-02T00:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.976839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[851,"TRANSGRIDV5_20180116135943","2017-01-02T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.96753,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[852,"TRANSGRIDV5_20180116135943","2017-01-02T04:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.96367,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[853,"TRANSGRIDV5_20180116135943","2017-01-02T08:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.90521,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[854,"TRANSGRIDV5_20180116135943","2017-01-02T07:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.88585,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[855,"TRANSGRIDV5_20180116135943","2017-01-02T07:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.8523,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[856,"TRANSGRIDV5_20180116135943","2017-01-02T17:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.82141,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[857,"TRANSGRIDV5_20180116135943","2017-01-02T07:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.698980000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[858,"TRANSGRIDV5_20180116135943","2017-01-02T01:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.65118,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[859,"TRANSGRIDV5_20180116135943","2017-01-02T07:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.616099999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[860,"TRANSGRIDV5_20180116135943","2017-01-02T05:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.559990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[861,"TRANSGRIDV5_20180116135943","2017-01-02T18:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.80222,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[862,"TRANSGRIDV5_20180116135943","2017-01-03T06:15:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-71.328909999999993,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[863,"TRANSGRIDV5_20180116135943","2017-01-03T07:00:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-64.797219999999996,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[864,"TRANSGRIDV5_20180116135943","2017-01-03T06:55:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-64.137069999999994,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[865,"TRANSGRIDV5_20180116135943","2017-01-03T06:50:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-58.655059999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[866,"TRANSGRIDV5_20180116135943","2017-01-03T06:20:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-57.122680000000003,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[867,"TRANSGRIDV5_20180116135943","2017-01-03T06:45:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-55.856879999999997,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[868,"TRANSGRIDV5_20180116135943","2017-01-03T06:25:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-48.05171,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[869,"TRANSGRIDV5_20180116135943","2017-01-03T06:30:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-47.24389,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[870,"TRANSGRIDV5_20180116135943","2017-01-03T06:40:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-45.899970000000003,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[871,"TRANSGRIDV5_20180116135943","2017-01-03T06:05:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-45.747790000000002,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[872,"TRANSGRIDV5_20180116135943","2017-01-03T06:10:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-45.614559999999997,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[873,"TRANSGRIDV5_20180116135943","2017-01-03T06:00:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-45.357089999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[874,"TRANSGRIDV5_20180116135943","2017-01-03T06:35:00","#R015063_012_RAMP_F","#R015063_RAMP","2017-01-02",1,-18.820350000000001,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[875,"TRANSGRIDV5_20180116135943","2017-01-03T22:50:00","NSA_V_BDL01_20","NSA-V_BDL01_20","2013-08-21",1,10.790100000000001,"Bairnsdale Unit 1 >= 20 MW for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[876,"TRANSGRIDV5_20180116135943","2017-01-03T18:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-163.98249000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[877,"TRANSGRIDV5_20180116135943","2017-01-03T18:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-146.09648000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[878,"TRANSGRIDV5_20180116135943","2017-01-03T16:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-26.96367,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[879,"TRANSGRIDV5_20180116135943","2017-01-03T20:10:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-24.504449999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[880,"TRANSGRIDV5_20180116135943","2017-01-03T18:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-21.696259999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[881,"TRANSGRIDV5_20180116135943","2017-01-03T20:00:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-20.047080000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[882,"TRANSGRIDV5_20180116135943","2017-01-03T15:25:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-15.46299,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[883,"TRANSGRIDV5_20180116135943","2017-01-03T13:30:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.924329999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[884,"TRANSGRIDV5_20180116135943","2017-01-03T13:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.631640000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[885,"TRANSGRIDV5_20180116135943","2017-01-03T14:10:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-14.185890000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[886,"TRANSGRIDV5_20180116135943","2017-01-03T13:40:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-13.87421,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[887,"TRANSGRIDV5_20180116135943","2017-01-03T13:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-12.607620000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[888,"TRANSGRIDV5_20180116135943","2017-01-03T13:25:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-12.01267,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[889,"TRANSGRIDV5_20180116135943","2017-01-03T13:15:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-11.338200000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[890,"TRANSGRIDV5_20180116135943","2017-01-03T13:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-11.32999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[891,"TRANSGRIDV5_20180116135943","2017-01-03T13:10:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.526730000000001,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[892,"TRANSGRIDV5_20180116135943","2017-01-03T13:50:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-10.15762,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[893,"TRANSGRIDV5_20180116135943","2017-01-03T19:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-146.81713999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[894,"TRANSGRIDV5_20180116135943","2017-01-03T19:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-146.02028000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[895,"TRANSGRIDV5_20180116135943","2017-01-03T19:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-145.48041000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[896,"TRANSGRIDV5_20180116135943","2017-01-03T19:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-92.723460000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[897,"TRANSGRIDV5_20180116135943","2017-01-03T19:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-87.932000000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[898,"TRANSGRIDV5_20180116135943","2017-01-03T19:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-87.772530000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[899,"TRANSGRIDV5_20180116135943","2017-01-03T22:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-38.372210000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[900,"TRANSGRIDV5_20180116135943","2017-01-03T22:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-35.746299999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[901,"TRANSGRIDV5_20180116135943","2017-01-03T22:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-34.695340000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[902,"TRANSGRIDV5_20180116135943","2017-01-03T19:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-32.237900000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[903,"TRANSGRIDV5_20180116135943","2017-01-03T20:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-30.69267,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[904,"TRANSGRIDV5_20180116135943","2017-01-03T19:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-30.091830000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[905,"TRANSGRIDV5_20180116135943","2017-01-03T19:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-28.595289999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[906,"TRANSGRIDV5_20180116135943","2017-01-03T19:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-26.413180000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[907,"TRANSGRIDV5_20180116135943","2017-01-03T23:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-24.681529999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[908,"TRANSGRIDV5_20180116135943","2017-01-03T19:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-24.167860000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[909,"TRANSGRIDV5_20180116135943","2017-01-03T23:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-23.193829999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[910,"TRANSGRIDV5_20180116135943","2017-01-03T18:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-21.867039999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[911,"TRANSGRIDV5_20180116135943","2017-01-03T18:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-21.635909999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[912,"TRANSGRIDV5_20180116135943","2017-01-03T22:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.819379999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[913,"TRANSGRIDV5_20180116135943","2017-01-03T23:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.8079,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[914,"TRANSGRIDV5_20180116135943","2017-01-03T22:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.39536,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[915,"TRANSGRIDV5_20180116135943","2017-01-03T22:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.352900000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[916,"TRANSGRIDV5_20180116135943","2017-01-03T22:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-19.276599999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[917,"TRANSGRIDV5_20180116135943","2017-01-03T15:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-16.888850000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[918,"TRANSGRIDV5_20180116135943","2017-01-03T17:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.82052,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[919,"TRANSGRIDV5_20180116135943","2017-01-03T00:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.75329,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[920,"TRANSGRIDV5_20180116135943","2017-01-03T23:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.27033,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[921,"TRANSGRIDV5_20180116135943","2017-01-03T23:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.70185,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[922,"TRANSGRIDV5_20180116135943","2017-01-03T01:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.470230000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[923,"TRANSGRIDV5_20180116135943","2017-01-03T20:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.137320000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[924,"TRANSGRIDV5_20180116135943","2017-01-03T00:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.52965,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[925,"TRANSGRIDV5_20180116135943","2017-01-03T00:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.508800000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[926,"TRANSGRIDV5_20180116135943","2017-01-03T23:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.4421,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[927,"TRANSGRIDV5_20180116135943","2017-01-03T23:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.559369999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[928,"TRANSGRIDV5_20180116135943","2017-01-03T23:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.31958,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[929,"TRANSGRIDV5_20180116135943","2017-01-03T23:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.21181,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[930,"TRANSGRIDV5_20180116135943","2017-01-03T21:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.97982,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[931,"TRANSGRIDV5_20180116135943","2017-01-03T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.384589999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[932,"TRANSGRIDV5_20180116135943","2017-01-03T03:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.11463,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[933,"TRANSGRIDV5_20180116135943","2017-01-03T08:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-109.03004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[934,"TRANSGRIDV5_20180116135943","2017-01-03T09:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-69.949879999999993,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[935,"TRANSGRIDV5_20180116135943","2017-01-03T09:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-69.891350000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[936,"TRANSGRIDV5_20180116135943","2017-01-03T09:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-69.21463,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[937,"TRANSGRIDV5_20180116135943","2017-01-03T09:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.695449999999994,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[938,"TRANSGRIDV5_20180116135943","2017-01-03T09:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.547449999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[939,"TRANSGRIDV5_20180116135943","2017-01-03T08:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.132620000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[940,"TRANSGRIDV5_20180116135943","2017-01-03T08:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.038219999999995,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[941,"TRANSGRIDV5_20180116135943","2017-01-03T09:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-67.991730000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[942,"TRANSGRIDV5_20180116135943","2017-01-03T09:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-67.950770000000006,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[943,"TRANSGRIDV5_20180116135943","2017-01-03T08:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-67.643569999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[944,"TRANSGRIDV5_20180116135943","2017-01-03T09:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-67.276009999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[945,"TRANSGRIDV5_20180116135943","2017-01-03T08:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.811980000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[946,"TRANSGRIDV5_20180116135943","2017-01-03T08:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.807109999999994,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[947,"TRANSGRIDV5_20180116135943","2017-01-03T08:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.705550000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[948,"TRANSGRIDV5_20180116135943","2017-01-03T08:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.597710000000006,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[949,"TRANSGRIDV5_20180116135943","2017-01-03T09:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.501980000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[950,"TRANSGRIDV5_20180116135943","2017-01-03T09:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.50188,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[951,"TRANSGRIDV5_20180116135943","2017-01-03T07:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.237099999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[952,"TRANSGRIDV5_20180116135943","2017-01-03T07:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.111549999999994,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[953,"TRANSGRIDV5_20180116135943","2017-01-03T08:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-64.197320000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[954,"TRANSGRIDV5_20180116135943","2017-01-03T08:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-64.159139999999994,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[955,"TRANSGRIDV5_20180116135943","2017-01-03T08:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-62.072560000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[956,"TRANSGRIDV5_20180116135943","2017-01-03T09:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-60.317349999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[957,"TRANSGRIDV5_20180116135943","2017-01-03T07:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-56.546900000000001,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[958,"TRANSGRIDV5_20180116135943","2017-01-03T08:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-56.112180000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[959,"TRANSGRIDV5_20180116135943","2017-01-03T07:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.941740000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[960,"TRANSGRIDV5_20180116135943","2017-01-03T07:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.829189999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[961,"TRANSGRIDV5_20180116135943","2017-01-03T07:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.455649999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[962,"TRANSGRIDV5_20180116135943","2017-01-03T07:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-39.596890000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[963,"TRANSGRIDV5_20180116135943","2017-01-03T07:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-39.50835,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[964,"TRANSGRIDV5_20180116135943","2017-01-03T07:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-31.011800000000001,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[965,"TRANSGRIDV5_20180116135943","2017-01-03T07:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-30.5472,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[966,"TRANSGRIDV5_20180116135943","2017-01-03T07:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-30.48986,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang hwts 1 ln 2 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[967,"TRANSGRIDV5_20180116135943","2017-01-03T18:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-275.83532000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[968,"TRANSGRIDV5_20180116135943","2017-01-03T19:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-259.69774000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[969,"TRANSGRIDV5_20180116135943","2017-01-03T18:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-259.55220000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[970,"TRANSGRIDV5_20180116135943","2017-01-03T19:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-257.85196000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[971,"TRANSGRIDV5_20180116135943","2017-01-03T19:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-255.98865000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[972,"TRANSGRIDV5_20180116135943","2017-01-03T12:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-191.09517,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[973,"TRANSGRIDV5_20180116135943","2017-01-03T19:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-171.62886,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[974,"TRANSGRIDV5_20180116135943","2017-01-03T19:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-166.49321,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[975,"TRANSGRIDV5_20180116135943","2017-01-03T19:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-166.32239000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[976,"TRANSGRIDV5_20180116135943","2017-01-03T16:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-102.14445000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[977,"TRANSGRIDV5_20180116135943","2017-01-03T19:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-88.891319999999993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[978,"TRANSGRIDV5_20180116135943","2017-01-03T17:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-84.78501,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[979,"TRANSGRIDV5_20180116135943","2017-01-03T18:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-84.178060000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[980,"TRANSGRIDV5_20180116135943","2017-01-03T19:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-82.092590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[981,"TRANSGRIDV5_20180116135943","2017-01-03T14:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-78.676580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[982,"TRANSGRIDV5_20180116135943","2017-01-03T12:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-78.477209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[983,"TRANSGRIDV5_20180116135943","2017-01-03T17:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-76.376589999999993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[984,"TRANSGRIDV5_20180116135943","2017-01-03T19:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-75.166650000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[985,"TRANSGRIDV5_20180116135943","2017-01-03T20:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-73.832400000000007,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[986,"TRANSGRIDV5_20180116135943","2017-01-03T18:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-73.831249999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[987,"TRANSGRIDV5_20180116135943","2017-01-03T20:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-73.814239999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[988,"TRANSGRIDV5_20180116135943","2017-01-03T18:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-72.51755,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[989,"TRANSGRIDV5_20180116135943","2017-01-03T18:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-72.452889999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[990,"TRANSGRIDV5_20180116135943","2017-01-03T19:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-72.448980000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[991,"TRANSGRIDV5_20180116135943","2017-01-03T20:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-71.759879999999995,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[992,"TRANSGRIDV5_20180116135943","2017-01-03T17:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-71.330160000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[993,"TRANSGRIDV5_20180116135943","2017-01-03T16:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-71.248900000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[994,"TRANSGRIDV5_20180116135943","2017-01-03T16:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-71.233500000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[995,"TRANSGRIDV5_20180116135943","2017-01-03T17:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-71.155119999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[996,"TRANSGRIDV5_20180116135943","2017-01-03T19:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-70.767160000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[997,"TRANSGRIDV5_20180116135943","2017-01-03T20:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-70.749930000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[998,"TRANSGRIDV5_20180116135943","2017-01-03T17:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-70.418480000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[999,"TRANSGRIDV5_20180116135943","2017-01-03T18:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-70.156329999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1000,"TRANSGRIDV5_20180116135943","2017-01-03T16:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.948830000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1001,"TRANSGRIDV5_20180116135943","2017-01-03T16:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.917190000000005,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1002,"TRANSGRIDV5_20180116135943","2017-01-03T16:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.765090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1003,"TRANSGRIDV5_20180116135943","2017-01-03T22:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.689250000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1004,"TRANSGRIDV5_20180116135943","2017-01-03T13:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.232870000000005,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1005,"TRANSGRIDV5_20180116135943","2017-01-03T16:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.128500000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1006,"TRANSGRIDV5_20180116135943","2017-01-03T17:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.117859999999993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1007,"TRANSGRIDV5_20180116135943","2017-01-03T11:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-68.573970000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1008,"TRANSGRIDV5_20180116135943","2017-01-03T20:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-68.474239999999995,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1009,"TRANSGRIDV5_20180116135943","2017-01-03T15:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-68.248609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1010,"TRANSGRIDV5_20180116135943","2017-01-03T16:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-68.139669999999995,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1011,"TRANSGRIDV5_20180116135943","2017-01-03T11:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.888570000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1012,"TRANSGRIDV5_20180116135943","2017-01-03T11:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.711830000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1013,"TRANSGRIDV5_20180116135943","2017-01-03T15:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.603970000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1014,"TRANSGRIDV5_20180116135943","2017-01-03T17:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.2577,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1015,"TRANSGRIDV5_20180116135943","2017-01-03T17:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.103399999999993,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1016,"TRANSGRIDV5_20180116135943","2017-01-03T12:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.030360000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1017,"TRANSGRIDV5_20180116135943","2017-01-03T11:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-67.015000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1018,"TRANSGRIDV5_20180116135943","2017-01-03T17:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-66.83605,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1019,"TRANSGRIDV5_20180116135943","2017-01-03T12:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-66.719880000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1020,"TRANSGRIDV5_20180116135943","2017-01-03T13:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-66.71293,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1021,"TRANSGRIDV5_20180116135943","2017-01-03T17:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-66.370840000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1022,"TRANSGRIDV5_20180116135943","2017-01-03T11:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-66.152929999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1023,"TRANSGRIDV5_20180116135943","2017-01-03T13:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.901210000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1024,"TRANSGRIDV5_20180116135943","2017-01-03T15:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.60566,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1025,"TRANSGRIDV5_20180116135943","2017-01-03T11:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.269180000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1026,"TRANSGRIDV5_20180116135943","2017-01-03T12:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.240899999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1027,"TRANSGRIDV5_20180116135943","2017-01-03T21:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.181160000000006,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1028,"TRANSGRIDV5_20180116135943","2017-01-03T20:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.119100000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1029,"TRANSGRIDV5_20180116135943","2017-01-03T21:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.0334,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1030,"TRANSGRIDV5_20180116135943","2017-01-03T13:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-64.543559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1031,"TRANSGRIDV5_20180116135943","2017-01-03T14:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-64.494209999999995,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1032,"TRANSGRIDV5_20180116135943","2017-01-03T20:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-64.415800000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1033,"TRANSGRIDV5_20180116135943","2017-01-03T11:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-64.000860000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1034,"TRANSGRIDV5_20180116135943","2017-01-03T13:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.905889999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1035,"TRANSGRIDV5_20180116135943","2017-01-03T12:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.901510000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1036,"TRANSGRIDV5_20180116135943","2017-01-03T11:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.4236,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1037,"TRANSGRIDV5_20180116135943","2017-01-03T12:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.254750000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1038,"TRANSGRIDV5_20180116135943","2017-01-03T13:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.196869999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1039,"TRANSGRIDV5_20180116135943","2017-01-03T13:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.182980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1040,"TRANSGRIDV5_20180116135943","2017-01-03T13:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.174190000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1041,"TRANSGRIDV5_20180116135943","2017-01-03T13:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-61.917630000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1042,"TRANSGRIDV5_20180116135943","2017-01-03T13:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-61.282989999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1043,"TRANSGRIDV5_20180116135943","2017-01-03T20:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-59.720660000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1044,"TRANSGRIDV5_20180116135943","2017-01-03T20:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-58.466360000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1045,"TRANSGRIDV5_20180116135943","2017-01-03T20:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-57.84695,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1046,"TRANSGRIDV5_20180116135943","2017-01-03T18:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-57.530999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1047,"TRANSGRIDV5_20180116135943","2017-01-03T17:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-57.270679999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1048,"TRANSGRIDV5_20180116135943","2017-01-03T17:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-55.50553,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1049,"TRANSGRIDV5_20180116135943","2017-01-03T14:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-55.413069999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1050,"TRANSGRIDV5_20180116135943","2017-01-03T12:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-53.773690000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1051,"TRANSGRIDV5_20180116135943","2017-01-03T12:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-53.279089999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1052,"TRANSGRIDV5_20180116135943","2017-01-03T13:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-52.53633,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1053,"TRANSGRIDV5_20180116135943","2017-01-03T19:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-52.18533,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1054,"TRANSGRIDV5_20180116135943","2017-01-03T12:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-51.030720000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1055,"TRANSGRIDV5_20180116135943","2017-01-03T11:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-49.425330000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1056,"TRANSGRIDV5_20180116135943","2017-01-03T12:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-49.263339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1057,"TRANSGRIDV5_20180116135943","2017-01-03T23:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-46.320349999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1058,"TRANSGRIDV5_20180116135943","2017-01-03T18:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-45.91,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1059,"TRANSGRIDV5_20180116135943","2017-01-03T18:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-45.729219999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1060,"TRANSGRIDV5_20180116135943","2017-01-03T21:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-44.845300000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1061,"TRANSGRIDV5_20180116135943","2017-01-03T18:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-44.155679999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1062,"TRANSGRIDV5_20180116135943","2017-01-03T18:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-41.206919999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1063,"TRANSGRIDV5_20180116135943","2017-01-03T15:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-39.563200000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1064,"TRANSGRIDV5_20180116135943","2017-01-03T13:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-38.023899999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1065,"TRANSGRIDV5_20180116135943","2017-01-03T21:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-37.928469999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1066,"TRANSGRIDV5_20180116135943","2017-01-03T20:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-37.135280000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1067,"TRANSGRIDV5_20180116135943","2017-01-03T21:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.942360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1068,"TRANSGRIDV5_20180116135943","2017-01-03T15:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.264299999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1069,"TRANSGRIDV5_20180116135943","2017-01-03T16:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.128880000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1070,"TRANSGRIDV5_20180116135943","2017-01-03T20:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.82827,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1071,"TRANSGRIDV5_20180116135943","2017-01-03T23:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.79515,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1072,"TRANSGRIDV5_20180116135943","2017-01-03T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.799320000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1073,"TRANSGRIDV5_20180116135943","2017-01-03T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.765029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1074,"TRANSGRIDV5_20180116135943","2017-01-03T21:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.652429999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1075,"TRANSGRIDV5_20180116135943","2017-01-03T21:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.629169999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1076,"TRANSGRIDV5_20180116135943","2017-01-03T21:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.407150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1077,"TRANSGRIDV5_20180116135943","2017-01-03T21:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.23171,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1078,"TRANSGRIDV5_20180116135943","2017-01-03T21:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.020669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1079,"TRANSGRIDV5_20180116135943","2017-01-03T16:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.409400000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1080,"TRANSGRIDV5_20180116135943","2017-01-03T09:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.703659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1081,"TRANSGRIDV5_20180116135943","2017-01-03T21:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.734839999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1082,"TRANSGRIDV5_20180116135943","2017-01-03T22:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.715910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1083,"TRANSGRIDV5_20180116135943","2017-01-03T21:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.30838,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1084,"TRANSGRIDV5_20180116135943","2017-01-03T15:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.355399999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1085,"TRANSGRIDV5_20180116135943","2017-01-03T15:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.33901,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1086,"TRANSGRIDV5_20180116135943","2017-01-03T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-95.856459999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1087,"TRANSGRIDV5_20180116135943","2017-01-03T22:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-69.737520000000004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1088,"TRANSGRIDV5_20180116135943","2017-01-03T16:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-64.289739999999995,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1089,"TRANSGRIDV5_20180116135943","2017-01-03T11:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-55.135860000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1090,"TRANSGRIDV5_20180116135943","2017-01-03T22:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-53.700870000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1091,"TRANSGRIDV5_20180116135943","2017-01-03T15:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-51.760109999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1092,"TRANSGRIDV5_20180116135943","2017-01-03T22:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-42.776000000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1093,"TRANSGRIDV5_20180116135943","2017-01-03T23:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-41.252699999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1094,"TRANSGRIDV5_20180116135943","2017-01-03T22:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-41.059240000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1095,"TRANSGRIDV5_20180116135943","2017-01-03T22:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-40.95196,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1096,"TRANSGRIDV5_20180116135943","2017-01-03T10:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-40.783410000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1097,"TRANSGRIDV5_20180116135943","2017-01-03T22:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-40.233310000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1098,"TRANSGRIDV5_20180116135943","2017-01-03T16:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-38.026220000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1099,"TRANSGRIDV5_20180116135943","2017-01-03T10:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.733600000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1100,"TRANSGRIDV5_20180116135943","2017-01-03T23:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.429209999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1101,"TRANSGRIDV5_20180116135943","2017-01-03T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.693779999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1102,"TRANSGRIDV5_20180116135943","2017-01-03T14:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-36.559480000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1103,"TRANSGRIDV5_20180116135943","2017-01-03T10:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-35.064459999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1104,"TRANSGRIDV5_20180116135943","2017-01-03T10:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-35.055149999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1105,"TRANSGRIDV5_20180116135943","2017-01-03T10:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-35.015169999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1106,"TRANSGRIDV5_20180116135943","2017-01-03T14:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.978540000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1107,"TRANSGRIDV5_20180116135943","2017-01-03T14:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.960070000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1108,"TRANSGRIDV5_20180116135943","2017-01-03T11:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.906170000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1109,"TRANSGRIDV5_20180116135943","2017-01-03T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.738169999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1110,"TRANSGRIDV5_20180116135943","2017-01-03T10:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.657809999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1111,"TRANSGRIDV5_20180116135943","2017-01-03T10:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.64837,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1112,"TRANSGRIDV5_20180116135943","2017-01-03T10:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.607190000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1113,"TRANSGRIDV5_20180116135943","2017-01-03T15:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.405639999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1114,"TRANSGRIDV5_20180116135943","2017-01-03T14:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.312269999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1115,"TRANSGRIDV5_20180116135943","2017-01-03T14:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.299979999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1116,"TRANSGRIDV5_20180116135943","2017-01-03T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.244390000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1117,"TRANSGRIDV5_20180116135943","2017-01-03T10:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-34.00676,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1118,"TRANSGRIDV5_20180116135943","2017-01-03T14:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-33.910490000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1119,"TRANSGRIDV5_20180116135943","2017-01-03T10:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-33.512689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1120,"TRANSGRIDV5_20180116135943","2017-01-03T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-33.309420000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1121,"TRANSGRIDV5_20180116135943","2017-01-03T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-30.82959,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1122,"TRANSGRIDV5_20180116135943","2017-01-03T05:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-30.750430000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1123,"TRANSGRIDV5_20180116135943","2017-01-03T23:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-30.74991,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1124,"TRANSGRIDV5_20180116135943","2017-01-03T23:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-29.085039999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1125,"TRANSGRIDV5_20180116135943","2017-01-03T11:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.84468,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1126,"TRANSGRIDV5_20180116135943","2017-01-03T00:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.252870000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1127,"TRANSGRIDV5_20180116135943","2017-01-03T10:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.960740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1128,"TRANSGRIDV5_20180116135943","2017-01-03T10:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.834669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1129,"TRANSGRIDV5_20180116135943","2017-01-03T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.53595,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1130,"TRANSGRIDV5_20180116135943","2017-01-03T01:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.212579999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1131,"TRANSGRIDV5_20180116135943","2017-01-03T23:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.536079999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1132,"TRANSGRIDV5_20180116135943","2017-01-03T22:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.619199999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1133,"TRANSGRIDV5_20180116135943","2017-01-03T05:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.59975,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1134,"TRANSGRIDV5_20180116135943","2017-01-03T22:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.523299999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1135,"TRANSGRIDV5_20180116135943","2017-01-03T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.437629999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1136,"TRANSGRIDV5_20180116135943","2017-01-03T04:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.388010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1137,"TRANSGRIDV5_20180116135943","2017-01-03T22:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.265689999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1138,"TRANSGRIDV5_20180116135943","2017-01-03T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.18244,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1139,"TRANSGRIDV5_20180116135943","2017-01-03T23:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.12172,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1140,"TRANSGRIDV5_20180116135943","2017-01-03T23:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.07254,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1141,"TRANSGRIDV5_20180116135943","2017-01-03T22:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.900829999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1142,"TRANSGRIDV5_20180116135943","2017-01-03T03:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.816479999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1143,"TRANSGRIDV5_20180116135943","2017-01-03","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.284469999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1144,"TRANSGRIDV5_20180116135943","2017-01-03T23:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.066590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1145,"TRANSGRIDV5_20180116135943","2017-01-03T05:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.52103,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1146,"TRANSGRIDV5_20180116135943","2017-01-03T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.25957,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1147,"TRANSGRIDV5_20180116135943","2017-01-03T05:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.026869999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1148,"TRANSGRIDV5_20180116135943","2017-01-03T02:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.33398,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1149,"TRANSGRIDV5_20180116135943","2017-01-03T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.274080000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1150,"TRANSGRIDV5_20180116135943","2017-01-03T00:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.078420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1151,"TRANSGRIDV5_20180116135943","2017-01-03T00:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.870740000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1152,"TRANSGRIDV5_20180116135943","2017-01-03T23:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.77769,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1153,"TRANSGRIDV5_20180116135943","2017-01-03T23:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.737369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1154,"TRANSGRIDV5_20180116135943","2017-01-03T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.63954,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1155,"TRANSGRIDV5_20180116135943","2017-01-03T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.613299999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1156,"TRANSGRIDV5_20180116135943","2017-01-03T01:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.443919999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1157,"TRANSGRIDV5_20180116135943","2017-01-03T12:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.35886,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1158,"TRANSGRIDV5_20180116135943","2017-01-03T04:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.327970000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1159,"TRANSGRIDV5_20180116135943","2017-01-03T04:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.314779999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1160,"TRANSGRIDV5_20180116135943","2017-01-03T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.289380000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1161,"TRANSGRIDV5_20180116135943","2017-01-03T00:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.0869,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1162,"TRANSGRIDV5_20180116135943","2017-01-03T05:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.05855,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1163,"TRANSGRIDV5_20180116135943","2017-01-03T04:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.79222,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1164,"TRANSGRIDV5_20180116135943","2017-01-03T05:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.65418,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1165,"TRANSGRIDV5_20180116135943","2017-01-03T04:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.606010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1166,"TRANSGRIDV5_20180116135943","2017-01-03T04:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.456230000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1167,"TRANSGRIDV5_20180116135943","2017-01-03T04:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.438600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1168,"TRANSGRIDV5_20180116135943","2017-01-03T00:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.432359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1169,"TRANSGRIDV5_20180116135943","2017-01-03T02:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.43167,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1170,"TRANSGRIDV5_20180116135943","2017-01-03T04:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.134499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1171,"TRANSGRIDV5_20180116135943","2017-01-03T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.796520000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1172,"TRANSGRIDV5_20180116135943","2017-01-03T04:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.747050000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1173,"TRANSGRIDV5_20180116135943","2017-01-03T00:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.30236,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1174,"TRANSGRIDV5_20180116135943","2017-01-03T01:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.295100000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1175,"TRANSGRIDV5_20180116135943","2017-01-03T00:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.239529999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1176,"TRANSGRIDV5_20180116135943","2017-01-03T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.159939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1177,"TRANSGRIDV5_20180116135943","2017-01-03T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.998089999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1178,"TRANSGRIDV5_20180116135943","2017-01-03T03:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.714589999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1179,"TRANSGRIDV5_20180116135943","2017-01-03T03:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.66441,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1180,"TRANSGRIDV5_20180116135943","2017-01-03T05:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.64986,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1181,"TRANSGRIDV5_20180116135943","2017-01-03T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.427770000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1182,"TRANSGRIDV5_20180116135943","2017-01-03T03:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.414350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1183,"TRANSGRIDV5_20180116135943","2017-01-03T01:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.369,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1184,"TRANSGRIDV5_20180116135943","2017-01-03T01:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.363910000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1185,"TRANSGRIDV5_20180116135943","2017-01-03T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.360569999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1186,"TRANSGRIDV5_20180116135943","2017-01-03T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.21571,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1187,"TRANSGRIDV5_20180116135943","2017-01-03T03:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.197559999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1188,"TRANSGRIDV5_20180116135943","2017-01-03T01:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.18709,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1189,"TRANSGRIDV5_20180116135943","2017-01-03T01:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.12701,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1190,"TRANSGRIDV5_20180116135943","2017-01-03T03:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.962160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1191,"TRANSGRIDV5_20180116135943","2017-01-03T02:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.92333,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1192,"TRANSGRIDV5_20180116135943","2017-01-03T01:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.92291,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1193,"TRANSGRIDV5_20180116135943","2017-01-03T01:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.838939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1194,"TRANSGRIDV5_20180116135943","2017-01-03T02:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.83699,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1195,"TRANSGRIDV5_20180116135943","2017-01-03T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.80734,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1196,"TRANSGRIDV5_20180116135943","2017-01-03T02:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.79177,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1197,"TRANSGRIDV5_20180116135943","2017-01-03T05:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.73765,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1198,"TRANSGRIDV5_20180116135943","2017-01-03T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.716699999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1199,"TRANSGRIDV5_20180116135943","2017-01-03T05:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.50545,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1200,"TRANSGRIDV5_20180116135943","2017-01-03T05:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.31676,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1201,"TRANSGRIDV5_20180116135943","2017-01-03T04:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.94678,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1202,"TRANSGRIDV5_20180116135943","2017-01-03T01:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.90152,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1203,"TRANSGRIDV5_20180116135943","2017-01-03T05:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.145289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1204,"TRANSGRIDV5_20180116135943","2017-01-03T05:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.985300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1205,"TRANSGRIDV5_20180116135943","2017-01-03T00:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.58107,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1206,"TRANSGRIDV5_20180116135943","2017-01-03T03:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.224489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1207,"TRANSGRIDV5_20180116135943","2017-01-03T01:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.08738,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1208,"TRANSGRIDV5_20180116135943","2017-01-03T03:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.909129999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1209,"TRANSGRIDV5_20180116135943","2017-01-03T00:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.867419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1210,"TRANSGRIDV5_20180116135943","2017-01-03T02:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.52285,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1211,"TRANSGRIDV5_20180116135943","2017-01-03T02:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.393190000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1212,"TRANSGRIDV5_20180116135943","2017-01-04T06:40:00","#R015066_012_RAMP_F","#R015066_RAMP","2017-01-04",1,-48.902569999999997,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1213,"TRANSGRIDV5_20180116135943","2017-01-04T06:55:00","#R015066_012_RAMP_F","#R015066_RAMP","2017-01-04",1,-45.376220000000004,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1214,"TRANSGRIDV5_20180116135943","2017-01-04T07:10:00","#R015066_012_RAMP_F","#R015066_RAMP","2017-01-04",1,-41.317549999999997,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1215,"TRANSGRIDV5_20180116135943","2017-01-04T07:15:00","#R015066_012_RAMP_F","#R015066_RAMP","2017-01-04",1,-38.088839999999998,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1216,"TRANSGRIDV5_20180116135943","2017-01-04T06:30:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-70.993780000000001,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1217,"TRANSGRIDV5_20180116135943","2017-01-04T07:00:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-54.589930000000003,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1218,"TRANSGRIDV5_20180116135943","2017-01-04T06:45:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-51.94265,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1219,"TRANSGRIDV5_20180116135943","2017-01-04T06:25:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-50.132010000000001,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1220,"TRANSGRIDV5_20180116135943","2017-01-04T06:35:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-49.421039999999998,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1221,"TRANSGRIDV5_20180116135943","2017-01-04T06:50:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-45.153669999999998,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1222,"TRANSGRIDV5_20180116135943","2017-01-04T07:05:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-44.908270000000002,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1223,"TRANSGRIDV5_20180116135943","2017-01-04T06:20:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-43.60154,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1224,"TRANSGRIDV5_20180116135943","2017-01-04T06:15:00","#R015066_012_RAMP_V","#R015066_RAMP","2017-01-04",1,-41.719880000000003,"Soft Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","South Morang hwts 1 ln 2 bus","REGULATED","10","Ramping Constraint","PLANNED",0]
[1225,"TRANSGRIDV5_20180116135943","2017-01-04T23:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-1270.78603,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1226,"TRANSGRIDV5_20180116135943","2017-01-04T23:05:00","N>N-NIL_LSDU","N-NIL","2014-02-13",1,-359.27204999999998,"Out = Nil, avoid overloading Lismore to Dunoon line (9U6 or 9U7) on trip of the other Lismore to Dunoon line (9U7 or 9U6), Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1227,"TRANSGRIDV5_20180116135943","2017-01-04T08:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-12.484999999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1228,"TRANSGRIDV5_20180116135943","2017-01-04T22:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-33.143230000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1229,"TRANSGRIDV5_20180116135943","2017-01-04T22:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-31.16422,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1230,"TRANSGRIDV5_20180116135943","2017-01-04T22:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-30.569299999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1231,"TRANSGRIDV5_20180116135943","2017-01-04T22:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-30.394690000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1232,"TRANSGRIDV5_20180116135943","2017-01-04T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-19.132760000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1233,"TRANSGRIDV5_20180116135943","2017-01-04T05:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.728639999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1234,"TRANSGRIDV5_20180116135943","2017-01-04","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.38871,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1235,"TRANSGRIDV5_20180116135943","2017-01-04T00:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.867369999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1236,"TRANSGRIDV5_20180116135943","2017-01-04T22:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.86716,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1237,"TRANSGRIDV5_20180116135943","2017-01-04T22:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.79894,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1238,"TRANSGRIDV5_20180116135943","2017-01-04T03:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.664199999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1239,"TRANSGRIDV5_20180116135943","2017-01-04T22:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.2102,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1240,"TRANSGRIDV5_20180116135943","2017-01-04T03:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.737819999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1241,"TRANSGRIDV5_20180116135943","2017-01-04T03:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.472659999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1242,"TRANSGRIDV5_20180116135943","2017-01-04T04:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.410629999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1243,"TRANSGRIDV5_20180116135943","2017-01-04T03:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.172459999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1244,"TRANSGRIDV5_20180116135943","2017-01-04T03:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.01389,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1245,"TRANSGRIDV5_20180116135943","2017-01-04T03:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.786160000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1246,"TRANSGRIDV5_20180116135943","2017-01-04T22:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.47133,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1247,"TRANSGRIDV5_20180116135943","2017-01-04T03:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.27975,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1248,"TRANSGRIDV5_20180116135943","2017-01-04T03:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.93507,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1249,"TRANSGRIDV5_20180116135943","2017-01-04T00:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.7148,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1250,"TRANSGRIDV5_20180116135943","2017-01-04T00:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.57907,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1251,"TRANSGRIDV5_20180116135943","2017-01-04T23:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.4024,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1252,"TRANSGRIDV5_20180116135943","2017-01-04T08:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-128.55201,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1253,"TRANSGRIDV5_20180116135943","2017-01-04T08:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-125.73258,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1254,"TRANSGRIDV5_20180116135943","2017-01-04T08:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-120.75592,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1255,"TRANSGRIDV5_20180116135943","2017-01-04T09:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-120.42704999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1256,"TRANSGRIDV5_20180116135943","2017-01-04T08:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-100.76119,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1257,"TRANSGRIDV5_20180116135943","2017-01-04T08:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-100.67201,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1258,"TRANSGRIDV5_20180116135943","2017-01-04T09:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-100.23823,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1259,"TRANSGRIDV5_20180116135943","2017-01-04T09:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-75.670950000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1260,"TRANSGRIDV5_20180116135943","2017-01-04T09:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-75.652299999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1261,"TRANSGRIDV5_20180116135943","2017-01-04T09:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-75.635239999999996,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1262,"TRANSGRIDV5_20180116135943","2017-01-04T09:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-75.591700000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1263,"TRANSGRIDV5_20180116135943","2017-01-04T08:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-75.237160000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1264,"TRANSGRIDV5_20180116135943","2017-01-04T09:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.899100000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1265,"TRANSGRIDV5_20180116135943","2017-01-04T08:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.562820000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1266,"TRANSGRIDV5_20180116135943","2017-01-04T10:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.435749999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1267,"TRANSGRIDV5_20180116135943","2017-01-04T10:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.416730000000001,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1268,"TRANSGRIDV5_20180116135943","2017-01-04T09:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.349850000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1269,"TRANSGRIDV5_20180116135943","2017-01-04T10:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-74.082679999999996,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1270,"TRANSGRIDV5_20180116135943","2017-01-04T07:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.785650000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1271,"TRANSGRIDV5_20180116135943","2017-01-04T09:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.744039999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1272,"TRANSGRIDV5_20180116135943","2017-01-04T09:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.730019999999996,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1273,"TRANSGRIDV5_20180116135943","2017-01-04T08:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.705820000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1274,"TRANSGRIDV5_20180116135943","2017-01-04T08:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.086420000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1275,"TRANSGRIDV5_20180116135943","2017-01-04T10:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.084959999999995,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1276,"TRANSGRIDV5_20180116135943","2017-01-04T10:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.048739999999995,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1277,"TRANSGRIDV5_20180116135943","2017-01-04T08:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.032110000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1278,"TRANSGRIDV5_20180116135943","2017-01-04T07:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-73.011960000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1279,"TRANSGRIDV5_20180116135943","2017-01-04T07:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-72.460459999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1280,"TRANSGRIDV5_20180116135943","2017-01-04T08:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-72.301699999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1281,"TRANSGRIDV5_20180116135943","2017-01-04T08:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-72.299130000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1282,"TRANSGRIDV5_20180116135943","2017-01-04T09:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-70.992270000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1283,"TRANSGRIDV5_20180116135943","2017-01-04T10:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-70.968000000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1284,"TRANSGRIDV5_20180116135943","2017-01-04T10:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-70.377250000000004,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1285,"TRANSGRIDV5_20180116135943","2017-01-04T07:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.671639999999996,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1286,"TRANSGRIDV5_20180116135943","2017-01-04T07:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-68.585840000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1287,"TRANSGRIDV5_20180116135943","2017-01-04T07:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-67.187830000000005,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1288,"TRANSGRIDV5_20180116135943","2017-01-04T07:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.822850000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1289,"TRANSGRIDV5_20180116135943","2017-01-04T09:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-66.582130000000006,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1290,"TRANSGRIDV5_20180116135943","2017-01-04T10:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-65.726089999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1291,"TRANSGRIDV5_20180116135943","2017-01-04T13:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-65.117859999999993,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1292,"TRANSGRIDV5_20180116135943","2017-01-04T13:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.75488,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1293,"TRANSGRIDV5_20180116135943","2017-01-04T13:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.753459999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1294,"TRANSGRIDV5_20180116135943","2017-01-04T10:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-43.543689999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1295,"TRANSGRIDV5_20180116135943","2017-01-04T10:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-43.211060000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1296,"TRANSGRIDV5_20180116135943","2017-01-04T07:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-36.855220000000003,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1297,"TRANSGRIDV5_20180116135943","2017-01-04T13:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-16.86787,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang syts 1 ln 1 bus","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1298,"TRANSGRIDV5_20180116135943","2017-01-04T22:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-68.046559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1299,"TRANSGRIDV5_20180116135943","2017-01-04T22:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.722329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1300,"TRANSGRIDV5_20180116135943","2017-01-04T22:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.686070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1301,"TRANSGRIDV5_20180116135943","2017-01-04T22:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-63.661659999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1302,"TRANSGRIDV5_20180116135943","2017-01-04T22:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-45.199750000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1303,"TRANSGRIDV5_20180116135943","2017-01-04T22:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-44.972999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1304,"TRANSGRIDV5_20180116135943","2017-01-04T05:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-41.138750000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1305,"TRANSGRIDV5_20180116135943","2017-01-04T22:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.169809999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1306,"TRANSGRIDV5_20180116135943","2017-01-04","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.01735,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1307,"TRANSGRIDV5_20180116135943","2017-01-04T00:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.000920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1308,"TRANSGRIDV5_20180116135943","2017-01-04T22:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.703249999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1309,"TRANSGRIDV5_20180116135943","2017-01-04T22:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.22213,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1310,"TRANSGRIDV5_20180116135943","2017-01-04T21:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-31.329180000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1311,"TRANSGRIDV5_20180116135943","2017-01-04T21:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.102930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1312,"TRANSGRIDV5_20180116135943","2017-01-04T21:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.097370000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1313,"TRANSGRIDV5_20180116135943","2017-01-04T23:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-29.44791,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1314,"TRANSGRIDV5_20180116135943","2017-01-04T22:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.94586,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1315,"TRANSGRIDV5_20180116135943","2017-01-04T23:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.62012,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1316,"TRANSGRIDV5_20180116135943","2017-01-04T21:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.44003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1317,"TRANSGRIDV5_20180116135943","2017-01-04T00:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.809329999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1318,"TRANSGRIDV5_20180116135943","2017-01-04T00:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.573560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1319,"TRANSGRIDV5_20180116135943","2017-01-04T22:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.170079999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1320,"TRANSGRIDV5_20180116135943","2017-01-04T23:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.977630000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1321,"TRANSGRIDV5_20180116135943","2017-01-04T23:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.520569999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1322,"TRANSGRIDV5_20180116135943","2017-01-04T23:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.256350000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1323,"TRANSGRIDV5_20180116135943","2017-01-04T23:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.741009999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1324,"TRANSGRIDV5_20180116135943","2017-01-04T21:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.467510000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1325,"TRANSGRIDV5_20180116135943","2017-01-04T23:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.09844,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1326,"TRANSGRIDV5_20180116135943","2017-01-04T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.621379999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1327,"TRANSGRIDV5_20180116135943","2017-01-04T01:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.215019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1328,"TRANSGRIDV5_20180116135943","2017-01-04T05:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.973559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1329,"TRANSGRIDV5_20180116135943","2017-01-04T05:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.61111,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1330,"TRANSGRIDV5_20180116135943","2017-01-04T05:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.606649999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1331,"TRANSGRIDV5_20180116135943","2017-01-04T05:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.605609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1332,"TRANSGRIDV5_20180116135943","2017-01-04T21:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.383949999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1333,"TRANSGRIDV5_20180116135943","2017-01-04T21:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.197040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1334,"TRANSGRIDV5_20180116135943","2017-01-04T21:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.261060000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1335,"TRANSGRIDV5_20180116135943","2017-01-04T23:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.53406,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1336,"TRANSGRIDV5_20180116135943","2017-01-04T21:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.371099999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1337,"TRANSGRIDV5_20180116135943","2017-01-04T05:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.04616,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1338,"TRANSGRIDV5_20180116135943","2017-01-04T05:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.01736,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1339,"TRANSGRIDV5_20180116135943","2017-01-04T05:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.862490000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1340,"TRANSGRIDV5_20180116135943","2017-01-04T06:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.80979,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1341,"TRANSGRIDV5_20180116135943","2017-01-04T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.33419,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1342,"TRANSGRIDV5_20180116135943","2017-01-04T05:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.57696,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1343,"TRANSGRIDV5_20180116135943","2017-01-04T23:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.295169999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1344,"TRANSGRIDV5_20180116135943","2017-01-04T20:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.226739999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1345,"TRANSGRIDV5_20180116135943","2017-01-04T23:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.071429999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1346,"TRANSGRIDV5_20180116135943","2017-01-04T21:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.940860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1347,"TRANSGRIDV5_20180116135943","2017-01-04T23:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.552910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1348,"TRANSGRIDV5_20180116135943","2017-01-04T21:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.207989999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1349,"TRANSGRIDV5_20180116135943","2017-01-04T22:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.170120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1350,"TRANSGRIDV5_20180116135943","2017-01-04T01:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.12144,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1351,"TRANSGRIDV5_20180116135943","2017-01-04T21:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.440300000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1352,"TRANSGRIDV5_20180116135943","2017-01-04T05:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.93929,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1353,"TRANSGRIDV5_20180116135943","2017-01-04T06:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.702349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1354,"TRANSGRIDV5_20180116135943","2017-01-04T01:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.61472,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1355,"TRANSGRIDV5_20180116135943","2017-01-04T20:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.42253,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1356,"TRANSGRIDV5_20180116135943","2017-01-04T06:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.485799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1357,"TRANSGRIDV5_20180116135943","2017-01-04T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.522349999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1358,"TRANSGRIDV5_20180116135943","2017-01-04T01:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.72913,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1359,"TRANSGRIDV5_20180116135943","2017-01-04T03:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.752420000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1360,"TRANSGRIDV5_20180116135943","2017-01-04T03:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.353760000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1361,"TRANSGRIDV5_20180116135943","2017-01-04T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.166370000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1362,"TRANSGRIDV5_20180116135943","2017-01-04T03:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.121690000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1363,"TRANSGRIDV5_20180116135943","2017-01-04T04:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.110379999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1364,"TRANSGRIDV5_20180116135943","2017-01-04T03:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.685690000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1365,"TRANSGRIDV5_20180116135943","2017-01-04T03:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.457360000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1366,"TRANSGRIDV5_20180116135943","2017-01-04T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.989100000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1367,"TRANSGRIDV5_20180116135943","2017-01-04T03:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.107600000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1368,"TRANSGRIDV5_20180116135943","2017-01-04T03:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.748419999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1369,"TRANSGRIDV5_20180116135943","2017-01-04T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.54533,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1370,"TRANSGRIDV5_20180116135943","2017-01-04T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.12425,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1371,"TRANSGRIDV5_20180116135943","2017-01-04T23:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.690480000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1372,"TRANSGRIDV5_20180116135943","2017-01-04T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.61279,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1373,"TRANSGRIDV5_20180116135943","2017-01-04T02:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.600339999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1374,"TRANSGRIDV5_20180116135943","2017-01-04T00:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.721589999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1375,"TRANSGRIDV5_20180116135943","2017-01-04T03:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.493030000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1376,"TRANSGRIDV5_20180116135943","2017-01-04T03:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.239319999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1377,"TRANSGRIDV5_20180116135943","2017-01-04T04:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.008279999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1378,"TRANSGRIDV5_20180116135943","2017-01-04T00:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.33652,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1379,"TRANSGRIDV5_20180116135943","2017-01-04T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.204930000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1380,"TRANSGRIDV5_20180116135943","2017-01-04T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.00761,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1381,"TRANSGRIDV5_20180116135943","2017-01-04T02:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.00685,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1382,"TRANSGRIDV5_20180116135943","2017-01-04T04:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.362839999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1383,"TRANSGRIDV5_20180116135943","2017-01-04T04:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.31861,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1384,"TRANSGRIDV5_20180116135943","2017-01-04T05:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.834300000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1385,"TRANSGRIDV5_20180116135943","2017-01-04T04:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.770619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1386,"TRANSGRIDV5_20180116135943","2017-01-04T04:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.576180000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1387,"TRANSGRIDV5_20180116135943","2017-01-04T02:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.39259,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1388,"TRANSGRIDV5_20180116135943","2017-01-04T00:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.44051,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1389,"TRANSGRIDV5_20180116135943","2017-01-04T00:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.37153,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1390,"TRANSGRIDV5_20180116135943","2017-01-04T04:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.145820000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1391,"TRANSGRIDV5_20180116135943","2017-01-04T04:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.22748,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1392,"TRANSGRIDV5_20180116135943","2017-01-04T19:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.81934,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1393,"TRANSGRIDV5_20180116135943","2017-01-04T04:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.44772,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1394,"TRANSGRIDV5_20180116135943","2017-01-04T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.32667,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1395,"TRANSGRIDV5_20180116135943","2017-01-04T01:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.21673,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1396,"TRANSGRIDV5_20180116135943","2017-01-04T04:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.19082,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1397,"TRANSGRIDV5_20180116135943","2017-01-04T01:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.03801,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1398,"TRANSGRIDV5_20180116135943","2017-01-04T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.02722,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1399,"TRANSGRIDV5_20180116135943","2017-01-04T01:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.023020000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1400,"TRANSGRIDV5_20180116135943","2017-01-04T01:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.022270000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1401,"TRANSGRIDV5_20180116135943","2017-01-04T02:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.86253,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1402,"TRANSGRIDV5_20180116135943","2017-01-04T02:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.83841,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1403,"TRANSGRIDV5_20180116135943","2017-01-04T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.837350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1404,"TRANSGRIDV5_20180116135943","2017-01-04T02:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.83432,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1405,"TRANSGRIDV5_20180116135943","2017-01-04T19:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.539529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1406,"TRANSGRIDV5_20180116135943","2017-01-04T05:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.439859999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1407,"TRANSGRIDV5_20180116135943","2017-01-04T01:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.86337,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1408,"TRANSGRIDV5_20180116135943","2017-01-04T00:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.26886,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1409,"TRANSGRIDV5_20180116135943","2017-01-05T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-13.39692,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1410,"TRANSGRIDV5_20180116135943","2017-01-05T04:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.456670000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1411,"TRANSGRIDV5_20180116135943","2017-01-05T02:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.09656,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1412,"TRANSGRIDV5_20180116135943","2017-01-05T00:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.899419999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1413,"TRANSGRIDV5_20180116135943","2017-01-05T00:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.679860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1414,"TRANSGRIDV5_20180116135943","2017-01-05T00:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.007739999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1415,"TRANSGRIDV5_20180116135943","2017-01-05T00:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.869450000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1416,"TRANSGRIDV5_20180116135943","2017-01-05T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.002279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1417,"TRANSGRIDV5_20180116135943","2017-01-05T00:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.925560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1418,"TRANSGRIDV5_20180116135943","2017-01-05","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.08445,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1419,"TRANSGRIDV5_20180116135943","2017-01-05T00:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.37013,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1420,"TRANSGRIDV5_20180116135943","2017-01-05T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.235580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1421,"TRANSGRIDV5_20180116135943","2017-01-05T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.115959999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1422,"TRANSGRIDV5_20180116135943","2017-01-05T00:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.08348,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1423,"TRANSGRIDV5_20180116135943","2017-01-05T06:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.86961,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1424,"TRANSGRIDV5_20180116135943","2017-01-05T05:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.45026,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1425,"TRANSGRIDV5_20180116135943","2017-01-05T05:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.449260000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1426,"TRANSGRIDV5_20180116135943","2017-01-05T05:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.412839999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1427,"TRANSGRIDV5_20180116135943","2017-01-05T05:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.40443,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1428,"TRANSGRIDV5_20180116135943","2017-01-05T06:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.335369999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1429,"TRANSGRIDV5_20180116135943","2017-01-05T05:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.310919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1430,"TRANSGRIDV5_20180116135943","2017-01-05T02:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.079000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1431,"TRANSGRIDV5_20180116135943","2017-01-05T04:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.03725,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1432,"TRANSGRIDV5_20180116135943","2017-01-05T01:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.13791,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1433,"TRANSGRIDV5_20180116135943","2017-01-05T06:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.13171,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1434,"TRANSGRIDV5_20180116135943","2017-01-05T01:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.933619999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1435,"TRANSGRIDV5_20180116135943","2017-01-05T05:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.877879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1436,"TRANSGRIDV5_20180116135943","2017-01-05T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.51857,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1437,"TRANSGRIDV5_20180116135943","2017-01-05T05:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.502560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1438,"TRANSGRIDV5_20180116135943","2017-01-05T04:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.62701,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1439,"TRANSGRIDV5_20180116135943","2017-01-05T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.156359999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1440,"TRANSGRIDV5_20180116135943","2017-01-05T02:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.0656,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1441,"TRANSGRIDV5_20180116135943","2017-01-05T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.52223,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1442,"TRANSGRIDV5_20180116135943","2017-01-05T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.91798,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1443,"TRANSGRIDV5_20180116135943","2017-01-05T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.223669999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1444,"TRANSGRIDV5_20180116135943","2017-01-05T03:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.539429999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1445,"TRANSGRIDV5_20180116135943","2017-01-05T04:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.52896,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1446,"TRANSGRIDV5_20180116135943","2017-01-05T03:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.466710000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1447,"TRANSGRIDV5_20180116135943","2017-01-05T02:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.46668,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1448,"TRANSGRIDV5_20180116135943","2017-01-05T03:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.45725,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1449,"TRANSGRIDV5_20180116135943","2017-01-05T01:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.66682,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1450,"TRANSGRIDV5_20180116135943","2017-01-05T04:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.661429999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1451,"TRANSGRIDV5_20180116135943","2017-01-05T02:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.658899999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1452,"TRANSGRIDV5_20180116135943","2017-01-05T04:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.652329999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1453,"TRANSGRIDV5_20180116135943","2017-01-05T04:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.407769999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1454,"TRANSGRIDV5_20180116135943","2017-01-05T04:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.40686,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1455,"TRANSGRIDV5_20180116135943","2017-01-05T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.36261,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1456,"TRANSGRIDV5_20180116135943","2017-01-05T04:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.11806,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1457,"TRANSGRIDV5_20180116135943","2017-01-05T03:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.00596,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1458,"TRANSGRIDV5_20180116135943","2017-01-05T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.004619999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1459,"TRANSGRIDV5_20180116135943","2017-01-05T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.003450000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1460,"TRANSGRIDV5_20180116135943","2017-01-06T18:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-142.43933999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1461,"TRANSGRIDV5_20180116135943","2017-01-06T16:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-121.74812,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1462,"TRANSGRIDV5_20180116135943","2017-01-06T17:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-106.34959000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1463,"TRANSGRIDV5_20180116135943","2017-01-06T16:25:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-102.80312000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1464,"TRANSGRIDV5_20180116135943","2017-01-06T16:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-102.18565,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1465,"TRANSGRIDV5_20180116135943","2017-01-06T15:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-51.334150000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1466,"TRANSGRIDV5_20180116135943","2017-01-06T15:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-39.931829999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1467,"TRANSGRIDV5_20180116135943","2017-01-06T17:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-37.879440000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1468,"TRANSGRIDV5_20180116135943","2017-01-06T18:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-37.398609999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1469,"TRANSGRIDV5_20180116135943","2017-01-06T17:55:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-30.120640000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1470,"TRANSGRIDV5_20180116135943","2017-01-06T17:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-29.793140000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1471,"TRANSGRIDV5_20180116135943","2017-01-06T18:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-27.977399999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1472,"TRANSGRIDV5_20180116135943","2017-01-06T18:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-27.241070000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1473,"TRANSGRIDV5_20180116135943","2017-01-06T18:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-27.198180000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1474,"TRANSGRIDV5_20180116135943","2017-01-06T17:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-27.103059999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1475,"TRANSGRIDV5_20180116135943","2017-01-06T17:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-25.34047,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1476,"TRANSGRIDV5_20180116135943","2017-01-06T18:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-18.712489999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1477,"TRANSGRIDV5_20180116135943","2017-01-06T18:25:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-18.536740000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1478,"TRANSGRIDV5_20180116135943","2017-01-06T14:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-18.441849999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1479,"TRANSGRIDV5_20180116135943","2017-01-06T18:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-16.69558,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1480,"TRANSGRIDV5_20180116135943","2017-01-06T15:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-12.459070000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1481,"TRANSGRIDV5_20180116135943","2017-01-06T03:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-41.528370000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1482,"TRANSGRIDV5_20180116135943","2017-01-06T01:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.95452,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1483,"TRANSGRIDV5_20180116135943","2017-01-06T03:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.099270000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1484,"TRANSGRIDV5_20180116135943","2017-01-06T01:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.404920000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1485,"TRANSGRIDV5_20180116135943","2017-01-06T00:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.461169999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1486,"TRANSGRIDV5_20180116135943","2017-01-06T15:10:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-181.25622000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1487,"TRANSGRIDV5_20180116135943","2017-01-06T15:15:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-180.92223999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1488,"TRANSGRIDV5_20180116135943","2017-01-06T17:20:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-166.84438,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1489,"TRANSGRIDV5_20180116135943","2017-01-06T14:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-157.42198999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1490,"TRANSGRIDV5_20180116135943","2017-01-06T14:25:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-152.68800999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1491,"TRANSGRIDV5_20180116135943","2017-01-06T14:20:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-151.24563000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1492,"TRANSGRIDV5_20180116135943","2017-01-06T14:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-151.24283,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1493,"TRANSGRIDV5_20180116135943","2017-01-06T17:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-148.35711000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1494,"TRANSGRIDV5_20180116135943","2017-01-06T18:15:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-145.17341999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1495,"TRANSGRIDV5_20180116135943","2017-01-06T13:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-145.08081999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1496,"TRANSGRIDV5_20180116135943","2017-01-06T14:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-142.25533999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1497,"TRANSGRIDV5_20180116135943","2017-01-06T18:25:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-139.57363000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1498,"TRANSGRIDV5_20180116135943","2017-01-06T17:35:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-133.24928,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1499,"TRANSGRIDV5_20180116135943","2017-01-06T14:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-132.99064000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1500,"TRANSGRIDV5_20180116135943","2017-01-06T14:50:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-132.54991000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1501,"TRANSGRIDV5_20180116135943","2017-01-06T17:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-131.88140000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1502,"TRANSGRIDV5_20180116135943","2017-01-06T14:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-131.04494,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1503,"TRANSGRIDV5_20180116135943","2017-01-06T17:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-126.81063,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1504,"TRANSGRIDV5_20180116135943","2017-01-06T18:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-125.72342999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1505,"TRANSGRIDV5_20180116135943","2017-01-06T15:35:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-123.15877,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1506,"TRANSGRIDV5_20180116135943","2017-01-06T18:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-117.7336,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1507,"TRANSGRIDV5_20180116135943","2017-01-06T17:50:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-116.94002,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1508,"TRANSGRIDV5_20180116135943","2017-01-06T18:00:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-113.34117999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1509,"TRANSGRIDV5_20180116135943","2017-01-06T15:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-105.72015,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1510,"TRANSGRIDV5_20180116135943","2017-01-06T15:25:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-49.169919999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1511,"TRANSGRIDV5_20180116135943","2017-01-06T15:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-39.449330000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1512,"TRANSGRIDV5_20180116135943","2017-01-06T03:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-43.70881,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1513,"TRANSGRIDV5_20180116135943","2017-01-06T03:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.666,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1514,"TRANSGRIDV5_20180116135943","2017-01-06T01:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.257190000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1515,"TRANSGRIDV5_20180116135943","2017-01-06T00:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-19.070160000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1516,"TRANSGRIDV5_20180116135943","2017-01-06T01:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.433879999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1517,"TRANSGRIDV5_20180116135943","2017-01-06T02:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.18112,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1518,"TRANSGRIDV5_20180116135943","2017-01-06T03:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.57424,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1519,"TRANSGRIDV5_20180116135943","2017-01-06T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.535499999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1520,"TRANSGRIDV5_20180116135943","2017-01-06T02:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.602519999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1521,"TRANSGRIDV5_20180116135943","2017-01-06T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.562010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1522,"TRANSGRIDV5_20180116135943","2017-01-06T01:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.177060000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1523,"TRANSGRIDV5_20180116135943","2017-01-06T02:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.013819999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1524,"TRANSGRIDV5_20180116135943","2017-01-06T02:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.011939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1525,"TRANSGRIDV5_20180116135943","2017-01-06T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.005759999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1526,"TRANSGRIDV5_20180116135943","2017-01-06T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.004239999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1527,"TRANSGRIDV5_20180116135943","2017-01-06T01:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.97824,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1528,"TRANSGRIDV5_20180116135943","2017-01-06T03:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.973940000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1529,"TRANSGRIDV5_20180116135943","2017-01-06T01:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.97053,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1530,"TRANSGRIDV5_20180116135943","2017-01-06T01:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.970370000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1531,"TRANSGRIDV5_20180116135943","2017-01-06T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.894489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1532,"TRANSGRIDV5_20180116135943","2017-01-06T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.81541,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1533,"TRANSGRIDV5_20180116135943","2017-01-06T00:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.87086,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1534,"TRANSGRIDV5_20180116135943","2017-01-06T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.562469999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1535,"TRANSGRIDV5_20180116135943","2017-01-06T00:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.817349999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1536,"TRANSGRIDV5_20180116135943","2017-01-06T01:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.676640000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1537,"TRANSGRIDV5_20180116135943","2017-01-06T00:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.11736,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1538,"TRANSGRIDV5_20180116135943","2017-01-06T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.711209999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1539,"TRANSGRIDV5_20180116135943","2017-01-06T02:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.70157,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1540,"TRANSGRIDV5_20180116135943","2017-01-06T03:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.654590000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1541,"TRANSGRIDV5_20180116135943","2017-01-06T03:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.62612,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1542,"TRANSGRIDV5_20180116135943","2017-01-06T02:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.456720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1543,"TRANSGRIDV5_20180116135943","2017-01-06T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.45321,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1544,"TRANSGRIDV5_20180116135943","2017-01-06T03:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.452489999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1545,"TRANSGRIDV5_20180116135943","2017-01-06T03:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.137370000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1546,"TRANSGRIDV5_20180116135943","2017-01-06T00:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.922129999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1547,"TRANSGRIDV5_20180116135943","2017-01-06T01:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.344939999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1548,"TRANSGRIDV5_20180116135943","2017-01-07T11:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-75.463539999999995,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1549,"TRANSGRIDV5_20180116135943","2017-01-07T15:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-40.556220000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1550,"TRANSGRIDV5_20180116135943","2017-01-07T16:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-35.023769999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1551,"TRANSGRIDV5_20180116135943","2017-01-07T14:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-29.639980000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1552,"TRANSGRIDV5_20180116135943","2017-01-07T14:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-28.330089999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1553,"TRANSGRIDV5_20180116135943","2017-01-07T14:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-25.105360000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1554,"TRANSGRIDV5_20180116135943","2017-01-07T16:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-25.00778,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1555,"TRANSGRIDV5_20180116135943","2017-01-07T13:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-23.745570000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1556,"TRANSGRIDV5_20180116135943","2017-01-07T15:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-23.69725,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1557,"TRANSGRIDV5_20180116135943","2017-01-07T13:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-23.310860000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1558,"TRANSGRIDV5_20180116135943","2017-01-07T13:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-23.305,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1559,"TRANSGRIDV5_20180116135943","2017-01-07T14:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-22.93524,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1560,"TRANSGRIDV5_20180116135943","2017-01-07T13:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-22.61337,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1561,"TRANSGRIDV5_20180116135943","2017-01-07T13:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-22.47814,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1562,"TRANSGRIDV5_20180116135943","2017-01-07T15:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-20.774149999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1563,"TRANSGRIDV5_20180116135943","2017-01-07T13:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-19.08278,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1564,"TRANSGRIDV5_20180116135943","2017-01-07T15:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-17.144179999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1565,"TRANSGRIDV5_20180116135943","2017-01-07T15:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-15.86773,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1566,"TRANSGRIDV5_20180116135943","2017-01-07T15:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-15.433199999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1567,"TRANSGRIDV5_20180116135943","2017-01-07T16:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-13.46996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1568,"TRANSGRIDV5_20180116135943","2017-01-07T14:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-10.77467,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1569,"TRANSGRIDV5_20180116135943","2017-01-07T14:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-10.44852,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1570,"TRANSGRIDV5_20180116135943","2017-01-07T14:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-10.28702,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1571,"TRANSGRIDV5_20180116135943","2017-01-07T02:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.887360000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1572,"TRANSGRIDV5_20180116135943","2017-01-07T02:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-19.003630000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1573,"TRANSGRIDV5_20180116135943","2017-01-07T03:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.845549999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1574,"TRANSGRIDV5_20180116135943","2017-01-07T02:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.952769999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1575,"TRANSGRIDV5_20180116135943","2017-01-07T02:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.107699999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1576,"TRANSGRIDV5_20180116135943","2017-01-07T03:35:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-14.00643,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1577,"TRANSGRIDV5_20180116135943","2017-01-07T03:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.87763,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1578,"TRANSGRIDV5_20180116135943","2017-01-07T05:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-11.497299999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1579,"TRANSGRIDV5_20180116135943","2017-01-07T02:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.646100000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1580,"TRANSGRIDV5_20180116135943","2017-01-07T04:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.389469999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1581,"TRANSGRIDV5_20180116135943","2017-01-07T01:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.26285,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1582,"TRANSGRIDV5_20180116135943","2017-01-07T03:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.21002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1583,"TRANSGRIDV5_20180116135943","2017-01-07T16:10:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-12011.39,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1584,"TRANSGRIDV5_20180116135943","2017-01-07T17:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-1459.6,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1585,"TRANSGRIDV5_20180116135943","2017-01-07T15:50:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-317.76242999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1586,"TRANSGRIDV5_20180116135943","2017-01-07T16:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-292.7482,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1587,"TRANSGRIDV5_20180116135943","2017-01-07T15:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-282.28546999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1588,"TRANSGRIDV5_20180116135943","2017-01-07T16:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-235.53433000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1589,"TRANSGRIDV5_20180116135943","2017-01-07T13:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-158.44103999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1590,"TRANSGRIDV5_20180116135943","2017-01-07T16:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-138.48961,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1591,"TRANSGRIDV5_20180116135943","2017-01-07T16:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-136.0727,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1592,"TRANSGRIDV5_20180116135943","2017-01-07T15:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-135.88455999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1593,"TRANSGRIDV5_20180116135943","2017-01-07T14:10:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-134.77269000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1594,"TRANSGRIDV5_20180116135943","2017-01-07T13:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-131.65595999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1595,"TRANSGRIDV5_20180116135943","2017-01-07T17:25:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-128.57714999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1596,"TRANSGRIDV5_20180116135943","2017-01-07T13:50:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-127.04812,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1597,"TRANSGRIDV5_20180116135943","2017-01-07T14:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-125.23726000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1598,"TRANSGRIDV5_20180116135943","2017-01-07T13:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-125.15911,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1599,"TRANSGRIDV5_20180116135943","2017-01-07T17:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-124.82989000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1600,"TRANSGRIDV5_20180116135943","2017-01-07T16:00:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-124.47631,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1601,"TRANSGRIDV5_20180116135943","2017-01-07T14:00:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-121.99306,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1602,"TRANSGRIDV5_20180116135943","2017-01-07T17:00:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-121.15212,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1603,"TRANSGRIDV5_20180116135943","2017-01-07T17:15:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-120.84751,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1604,"TRANSGRIDV5_20180116135943","2017-01-07T10:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-117.16901,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1605,"TRANSGRIDV5_20180116135943","2017-01-07T15:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-116.63235,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1606,"TRANSGRIDV5_20180116135943","2017-01-07T15:35:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-108.08526000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1607,"TRANSGRIDV5_20180116135943","2017-01-07T17:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-106.78238,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1608,"TRANSGRIDV5_20180116135943","2017-01-07T17:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-106.62324,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1609,"TRANSGRIDV5_20180116135943","2017-01-07T17:35:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-105.59128,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1610,"TRANSGRIDV5_20180116135943","2017-01-07T17:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-105.07144,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1611,"TRANSGRIDV5_20180116135943","2017-01-07T10:45:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-103.43537999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1612,"TRANSGRIDV5_20180116135943","2017-01-07T17:20:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-101.05419999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1613,"TRANSGRIDV5_20180116135943","2017-01-07T17:10:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-20.675940000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1614,"TRANSGRIDV5_20180116135943","2017-01-07T02:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-30.12866,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1615,"TRANSGRIDV5_20180116135943","2017-01-07T02:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-28.722809999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1616,"TRANSGRIDV5_20180116135943","2017-01-07T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.809609999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1617,"TRANSGRIDV5_20180116135943","2017-01-07T02:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.683990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1618,"TRANSGRIDV5_20180116135943","2017-01-07T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.731639999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1619,"TRANSGRIDV5_20180116135943","2017-01-07T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-24.024830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1620,"TRANSGRIDV5_20180116135943","2017-01-07T03:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.98657,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1621,"TRANSGRIDV5_20180116135943","2017-01-07T02:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.55414,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1622,"TRANSGRIDV5_20180116135943","2017-01-07T05:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.74503,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1623,"TRANSGRIDV5_20180116135943","2017-01-07T02:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.091010000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1624,"TRANSGRIDV5_20180116135943","2017-01-07T04:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.969470000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1625,"TRANSGRIDV5_20180116135943","2017-01-07T03:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.480509999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1626,"TRANSGRIDV5_20180116135943","2017-01-07T01:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.368760000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1627,"TRANSGRIDV5_20180116135943","2017-01-07T01:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.532630000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1628,"TRANSGRIDV5_20180116135943","2017-01-07T01:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.505289999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1629,"TRANSGRIDV5_20180116135943","2017-01-07T02:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.043890000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1630,"TRANSGRIDV5_20180116135943","2017-01-07T01:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.500240000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1631,"TRANSGRIDV5_20180116135943","2017-01-07T04:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.386520000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1632,"TRANSGRIDV5_20180116135943","2017-01-07T01:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.302669999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1633,"TRANSGRIDV5_20180116135943","2017-01-07T03:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.284990000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1634,"TRANSGRIDV5_20180116135943","2017-01-07T03:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.265699999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1635,"TRANSGRIDV5_20180116135943","2017-01-07T03:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.262250000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1636,"TRANSGRIDV5_20180116135943","2017-01-07T03:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.2563,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1637,"TRANSGRIDV5_20180116135943","2017-01-07T03:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.253799999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1638,"TRANSGRIDV5_20180116135943","2017-01-07T03:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.251090000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1639,"TRANSGRIDV5_20180116135943","2017-01-07T02:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.09666,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1640,"TRANSGRIDV5_20180116135943","2017-01-07T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.093219999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1641,"TRANSGRIDV5_20180116135943","2017-01-07T03:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.08278,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1642,"TRANSGRIDV5_20180116135943","2017-01-07T04:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.403460000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1643,"TRANSGRIDV5_20180116135943","2017-01-07T01:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.38528,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1644,"TRANSGRIDV5_20180116135943","2017-01-07T02:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.21984,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1645,"TRANSGRIDV5_20180116135943","2017-01-07T04:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.19741,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1646,"TRANSGRIDV5_20180116135943","2017-01-07T04:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.19661,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1647,"TRANSGRIDV5_20180116135943","2017-01-07T04:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.165089999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1648,"TRANSGRIDV5_20180116135943","2017-01-07T04:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.13147,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1649,"TRANSGRIDV5_20180116135943","2017-01-07T04:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-12.93038,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1650,"TRANSGRIDV5_20180116135943","2017-01-07T02:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.867319999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1651,"TRANSGRIDV5_20180116135943","2017-01-07T01:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.64242,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1652,"TRANSGRIDV5_20180116135943","2017-01-07T12:30:00","VSML_ROC_80","V-NIL","2016-08-23",1,-202.73829000000001,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1653,"TRANSGRIDV5_20180116135943","2017-01-07T13:00:00","VSML_ROC_80","V-NIL","2016-08-23",1,-157.38471999999999,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1654,"TRANSGRIDV5_20180116135943","2017-01-08T09:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-23.345420000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1655,"TRANSGRIDV5_20180116135943","2017-01-08T09:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-22.548449999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1656,"TRANSGRIDV5_20180116135943","2017-01-08T08:55:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-22.133199999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1657,"TRANSGRIDV5_20180116135943","2017-01-08T09:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-21.893540000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1658,"TRANSGRIDV5_20180116135943","2017-01-08T09:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-21.58032,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1659,"TRANSGRIDV5_20180116135943","2017-01-08T09:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-19.246259999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1660,"TRANSGRIDV5_20180116135943","2017-01-08T09:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-15.75137,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1661,"TRANSGRIDV5_20180116135943","2017-01-08T09:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-14.955719999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1662,"TRANSGRIDV5_20180116135943","2017-01-08T09:25:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-13.91272,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1663,"TRANSGRIDV5_20180116135943","2017-01-08T10:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-13.14326,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1664,"TRANSGRIDV5_20180116135943","2017-01-08T11:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-12.86645,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1665,"TRANSGRIDV5_20180116135943","2017-01-08T11:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-12.46471,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1666,"TRANSGRIDV5_20180116135943","2017-01-08T08:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-12.293570000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1667,"TRANSGRIDV5_20180116135943","2017-01-08T08:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-10.80757,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1668,"TRANSGRIDV5_20180116135943","2017-01-08T23:05:00","SVML_ROC_80","S-NIL","2016-08-23",1,-15.14448,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1669,"TRANSGRIDV5_20180116135943","2017-01-08T23:40:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-16.151050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1670,"TRANSGRIDV5_20180116135943","2017-01-08T21:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.803469999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1671,"TRANSGRIDV5_20180116135943","2017-01-08T21:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-43.249380000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1672,"TRANSGRIDV5_20180116135943","2017-01-08T21:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-33.046550000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1673,"TRANSGRIDV5_20180116135943","2017-01-08T22:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-32.389690000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1674,"TRANSGRIDV5_20180116135943","2017-01-08T02:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-30.914169999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1675,"TRANSGRIDV5_20180116135943","2017-01-08T07:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-30.173269999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1676,"TRANSGRIDV5_20180116135943","2017-01-08T07:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.94876,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1677,"TRANSGRIDV5_20180116135943","2017-01-08T03:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-27.702850000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1678,"TRANSGRIDV5_20180116135943","2017-01-08T01:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.567499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1679,"TRANSGRIDV5_20180116135943","2017-01-08T22:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.313410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1680,"TRANSGRIDV5_20180116135943","2017-01-08T06:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.667310000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1681,"TRANSGRIDV5_20180116135943","2017-01-08T04:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.18422,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1682,"TRANSGRIDV5_20180116135943","2017-01-08T04:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.142309999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1683,"TRANSGRIDV5_20180116135943","2017-01-08T04:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.133780000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1684,"TRANSGRIDV5_20180116135943","2017-01-08T06:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-21.318519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1685,"TRANSGRIDV5_20180116135943","2017-01-08T04:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.156089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1686,"TRANSGRIDV5_20180116135943","2017-01-08T06:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.85361,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1687,"TRANSGRIDV5_20180116135943","2017-01-08T01:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.733129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1688,"TRANSGRIDV5_20180116135943","2017-01-08T02:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.701280000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1689,"TRANSGRIDV5_20180116135943","2017-01-08T03:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.48302,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1690,"TRANSGRIDV5_20180116135943","2017-01-08T06:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.3123,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1691,"TRANSGRIDV5_20180116135943","2017-01-08T03:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.283149999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1692,"TRANSGRIDV5_20180116135943","2017-01-08T03:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.244140000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1693,"TRANSGRIDV5_20180116135943","2017-01-08T06:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-17.45448,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1694,"TRANSGRIDV5_20180116135943","2017-01-08T04:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-17.383430000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1695,"TRANSGRIDV5_20180116135943","2017-01-08T01:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-16.775220000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1696,"TRANSGRIDV5_20180116135943","2017-01-08T03:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-16.308700000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1697,"TRANSGRIDV5_20180116135943","2017-01-08T07:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-15.947509999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1698,"TRANSGRIDV5_20180116135943","2017-01-08T06:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-15.327529999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1699,"TRANSGRIDV5_20180116135943","2017-01-08T01:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-15.294499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1700,"TRANSGRIDV5_20180116135943","2017-01-08T06:55:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-14.2654,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1701,"TRANSGRIDV5_20180116135943","2017-01-08T01:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-13.28387,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1702,"TRANSGRIDV5_20180116135943","2017-01-08T02:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-13.18093,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1703,"TRANSGRIDV5_20180116135943","2017-01-08T02:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.59779,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1704,"TRANSGRIDV5_20180116135943","2017-01-08T01:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.362500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1705,"TRANSGRIDV5_20180116135943","2017-01-08T02:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.355420000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1706,"TRANSGRIDV5_20180116135943","2017-01-08T02:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.04848,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1707,"TRANSGRIDV5_20180116135943","2017-01-08T00:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-11.317920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1708,"TRANSGRIDV5_20180116135943","2017-01-08T22:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-48.984279999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1709,"TRANSGRIDV5_20180116135943","2017-01-08T22:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-48.964689999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1710,"TRANSGRIDV5_20180116135943","2017-01-08T22:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-40.775309999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1711,"TRANSGRIDV5_20180116135943","2017-01-08T21:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-38.717460000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1712,"TRANSGRIDV5_20180116135943","2017-01-08T21:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-36.616790000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1713,"TRANSGRIDV5_20180116135943","2017-01-08T22:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-36.169849999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1714,"TRANSGRIDV5_20180116135943","2017-01-08T22:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-35.327210000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1715,"TRANSGRIDV5_20180116135943","2017-01-08T02:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.714919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1716,"TRANSGRIDV5_20180116135943","2017-01-08T22:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.185650000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1717,"TRANSGRIDV5_20180116135943","2017-01-08T01:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.219819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1718,"TRANSGRIDV5_20180116135943","2017-01-08T02:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.16911,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1719,"TRANSGRIDV5_20180116135943","2017-01-08T00:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.315899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1720,"TRANSGRIDV5_20180116135943","2017-01-08T22:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.84365,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1721,"TRANSGRIDV5_20180116135943","2017-01-08T22:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.089700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1722,"TRANSGRIDV5_20180116135943","2017-01-08T23:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.921489999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1723,"TRANSGRIDV5_20180116135943","2017-01-08T21:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.15953,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1724,"TRANSGRIDV5_20180116135943","2017-01-08T23:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.063890000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1725,"TRANSGRIDV5_20180116135943","2017-01-08T22:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.968900000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1726,"TRANSGRIDV5_20180116135943","2017-01-08T04:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.173249999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1727,"TRANSGRIDV5_20180116135943","2017-01-08T23:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.482869999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1728,"TRANSGRIDV5_20180116135943","2017-01-08T23:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.346150000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1729,"TRANSGRIDV5_20180116135943","2017-01-08T03:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.792059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1730,"TRANSGRIDV5_20180116135943","2017-01-08T07:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.46088,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1731,"TRANSGRIDV5_20180116135943","2017-01-08T23:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.94309,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1732,"TRANSGRIDV5_20180116135943","2017-01-08T23:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.839370000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1733,"TRANSGRIDV5_20180116135943","2017-01-08T23:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.32122,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1734,"TRANSGRIDV5_20180116135943","2017-01-08T23:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.226789999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1735,"TRANSGRIDV5_20180116135943","2017-01-08T04:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.95219,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1736,"TRANSGRIDV5_20180116135943","2017-01-08T23:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.46405,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1737,"TRANSGRIDV5_20180116135943","2017-01-08T04:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.323219999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1738,"TRANSGRIDV5_20180116135943","2017-01-08T19:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.948729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1739,"TRANSGRIDV5_20180116135943","2017-01-08T03:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.556279999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1740,"TRANSGRIDV5_20180116135943","2017-01-08T19:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.25662,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1741,"TRANSGRIDV5_20180116135943","2017-01-08T03:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.08714,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1742,"TRANSGRIDV5_20180116135943","2017-01-08T02:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.983359999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1743,"TRANSGRIDV5_20180116135943","2017-01-08T03:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.904439999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1744,"TRANSGRIDV5_20180116135943","2017-01-08T00:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.861219999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1745,"TRANSGRIDV5_20180116135943","2017-01-08T00:50:00","VSML_ROC_80","V-NIL","2016-08-23",1,-20.876799999999999,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1746,"TRANSGRIDV5_20180116135943","2017-01-09T22:35:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-31.035609999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1747,"TRANSGRIDV5_20180116135943","2017-01-09T22:40:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-22.030059999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1748,"TRANSGRIDV5_20180116135943","2017-01-09T21:40:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-18.059229999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1749,"TRANSGRIDV5_20180116135943","2017-01-09T22:05:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-16.891380000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1750,"TRANSGRIDV5_20180116135943","2017-01-09T22:45:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-16.768899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1751,"TRANSGRIDV5_20180116135943","2017-01-09T22:50:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-11.57564,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1752,"TRANSGRIDV5_20180116135943","2017-01-09T00:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.652709999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1753,"TRANSGRIDV5_20180116135943","2017-01-09T01:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-31.825040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1754,"TRANSGRIDV5_20180116135943","2017-01-09T22:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-30.227250000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1755,"TRANSGRIDV5_20180116135943","2017-01-09T22:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-30.202480000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1756,"TRANSGRIDV5_20180116135943","2017-01-09T03:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.936199999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1757,"TRANSGRIDV5_20180116135943","2017-01-09T22:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.900410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1758,"TRANSGRIDV5_20180116135943","2017-01-09T22:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-26.619509999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1759,"TRANSGRIDV5_20180116135943","2017-01-09T22:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-25.62115,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1760,"TRANSGRIDV5_20180116135943","2017-01-09T05:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-25.426680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1761,"TRANSGRIDV5_20180116135943","2017-01-09T21:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-24.86204,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1762,"TRANSGRIDV5_20180116135943","2017-01-09T05:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-23.85012,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1763,"TRANSGRIDV5_20180116135943","2017-01-09T00:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-23.685919999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1764,"TRANSGRIDV5_20180116135943","2017-01-09T01:25:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.453209999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1765,"TRANSGRIDV5_20180116135943","2017-01-09T01:15:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-22.452809999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1766,"TRANSGRIDV5_20180116135943","2017-01-09T01:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-21.868259999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1767,"TRANSGRIDV5_20180116135943","2017-01-09T01:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.908000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1768,"TRANSGRIDV5_20180116135943","2017-01-09T01:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.238150000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1769,"TRANSGRIDV5_20180116135943","2017-01-09T04:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-20.018809999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1770,"TRANSGRIDV5_20180116135943","2017-01-09T05:20:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.965789999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1771,"TRANSGRIDV5_20180116135943","2017-01-09T02:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.679829999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1772,"TRANSGRIDV5_20180116135943","2017-01-09T22:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.678149999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1773,"TRANSGRIDV5_20180116135943","2017-01-09T03:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-19.667999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1774,"TRANSGRIDV5_20180116135943","2017-01-09T05:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.93131,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1775,"TRANSGRIDV5_20180116135943","2017-01-09T22:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-18.470469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1776,"TRANSGRIDV5_20180116135943","2017-01-09T05:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-16.944089999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1777,"TRANSGRIDV5_20180116135943","2017-01-09T00:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-35.758589999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1778,"TRANSGRIDV5_20180116135943","2017-01-09T03:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.88401,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1779,"TRANSGRIDV5_20180116135943","2017-01-09T03:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.838380000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1780,"TRANSGRIDV5_20180116135943","2017-01-09T00:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.392749999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1781,"TRANSGRIDV5_20180116135943","2017-01-09T00:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.324960000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1782,"TRANSGRIDV5_20180116135943","2017-01-09T01:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.20607,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1783,"TRANSGRIDV5_20180116135943","2017-01-09T00:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.0669,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1784,"TRANSGRIDV5_20180116135943","2017-01-09T02:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.349979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1785,"TRANSGRIDV5_20180116135943","2017-01-09","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.254860000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1786,"TRANSGRIDV5_20180116135943","2017-01-09T04:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.048069999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1787,"TRANSGRIDV5_20180116135943","2017-01-09T03:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.039200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1788,"TRANSGRIDV5_20180116135943","2017-01-09T02:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.032139999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1789,"TRANSGRIDV5_20180116135943","2017-01-09T04:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.02384,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1790,"TRANSGRIDV5_20180116135943","2017-01-09T03:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.021540000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1791,"TRANSGRIDV5_20180116135943","2017-01-09T03:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.01322,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1792,"TRANSGRIDV5_20180116135943","2017-01-09T03:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.006060000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1793,"TRANSGRIDV5_20180116135943","2017-01-09T03:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.994050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1794,"TRANSGRIDV5_20180116135943","2017-01-09T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.219000000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1795,"TRANSGRIDV5_20180116135943","2017-01-09T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.553610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1796,"TRANSGRIDV5_20180116135943","2017-01-09T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.24258,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1797,"TRANSGRIDV5_20180116135943","2017-01-09T05:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.91835,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1798,"TRANSGRIDV5_20180116135943","2017-01-09T00:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.89127,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1799,"TRANSGRIDV5_20180116135943","2017-01-09T01:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.48105,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1800,"TRANSGRIDV5_20180116135943","2017-01-09T01:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.46194,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1801,"TRANSGRIDV5_20180116135943","2017-01-09T01:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.13396,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1802,"TRANSGRIDV5_20180116135943","2017-01-09T05:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.047470000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1803,"TRANSGRIDV5_20180116135943","2017-01-09T04:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.02896,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1804,"TRANSGRIDV5_20180116135943","2017-01-09T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.930070000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1805,"TRANSGRIDV5_20180116135943","2017-01-09T02:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.814590000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1806,"TRANSGRIDV5_20180116135943","2017-01-09T02:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.79721,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1807,"TRANSGRIDV5_20180116135943","2017-01-09T02:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.7958,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1808,"TRANSGRIDV5_20180116135943","2017-01-09T04:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.5364,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1809,"TRANSGRIDV5_20180116135943","2017-01-09T04:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.527939999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1810,"TRANSGRIDV5_20180116135943","2017-01-09T04:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.50802,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1811,"TRANSGRIDV5_20180116135943","2017-01-09T05:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.36275,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1812,"TRANSGRIDV5_20180116135943","2017-01-09T01:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.183859999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1813,"TRANSGRIDV5_20180116135943","2017-01-09T04:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.963559999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1814,"TRANSGRIDV5_20180116135943","2017-01-09T03:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.841659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1815,"TRANSGRIDV5_20180116135943","2017-01-09T02:35:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-30.168839999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1816,"TRANSGRIDV5_20180116135943","2017-01-09T01:30:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-17.59102,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1817,"TRANSGRIDV5_20180116135943","2017-01-09T04:35:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-14.85446,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1818,"TRANSGRIDV5_20180116135943","2017-01-09T01:15:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-14.05448,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1819,"TRANSGRIDV5_20180116135943","2017-01-09T02:10:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-13.048310000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1820,"TRANSGRIDV5_20180116135943","2017-01-09T03:20:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-10.79438,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1821,"TRANSGRIDV5_20180116135943","2017-01-09T04:00:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-10.766629999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1822,"TRANSGRIDV5_20180116135943","2017-01-09T02:30:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-49.7211,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1823,"TRANSGRIDV5_20180116135943","2017-01-09T02:05:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-30.446149999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1824,"TRANSGRIDV5_20180116135943","2017-01-09T02:55:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-27.706320000000002,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1825,"TRANSGRIDV5_20180116135943","2017-01-09T02:45:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-24.76877,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1826,"TRANSGRIDV5_20180116135943","2017-01-09T03:40:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-19.120480000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1827,"TRANSGRIDV5_20180116135943","2017-01-09T00:55:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-19.036049999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1828,"TRANSGRIDV5_20180116135943","2017-01-09T01:55:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.845790000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1829,"TRANSGRIDV5_20180116135943","2017-01-09T01:45:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.802050000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1830,"TRANSGRIDV5_20180116135943","2017-01-09T00:45:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.473420000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1831,"TRANSGRIDV5_20180116135943","2017-01-09T02:20:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.230360000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1832,"TRANSGRIDV5_20180116135943","2017-01-09T02:25:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.229040000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1833,"TRANSGRIDV5_20180116135943","2017-01-09T02:00:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-18.212820000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1834,"TRANSGRIDV5_20180116135943","2017-01-09T01:35:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-17.6096,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1835,"TRANSGRIDV5_20180116135943","2017-01-09T00:25:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-16.880289999999999,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1836,"TRANSGRIDV5_20180116135943","2017-01-09T00:30:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-16.590810000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1837,"TRANSGRIDV5_20180116135943","2017-01-09T01:40:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-14.473990000000001,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1838,"TRANSGRIDV5_20180116135943","2017-01-09T01:25:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-14.0542,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1839,"TRANSGRIDV5_20180116135943","2017-01-09T00:35:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-13.16926,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1840,"TRANSGRIDV5_20180116135943","2017-01-09T01:05:00","V:SS_820_HY_TEST_DYN","I-VSS_820_TEST","2016-11-21",1,-12.24939,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1841,"TRANSGRIDV5_20180116135943","2017-01-09T14:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-53.709200000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1842,"TRANSGRIDV5_20180116135943","2017-01-09T14:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-37.679470000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1843,"TRANSGRIDV5_20180116135943","2017-01-09T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-33.103529999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1844,"TRANSGRIDV5_20180116135943","2017-01-09T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-31.975480000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1845,"TRANSGRIDV5_20180116135943","2017-01-09T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.543679999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1846,"TRANSGRIDV5_20180116135943","2017-01-09T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.45748,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1847,"TRANSGRIDV5_20180116135943","2017-01-09T00:20:00","VSML_220","V-NIL","2012-07-04",1,-208.30628999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1848,"TRANSGRIDV5_20180116135943","2017-01-09T01:00:00","VSML_220","V-NIL","2012-07-04",1,-30.168859999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1849,"TRANSGRIDV5_20180116135943","2017-01-09T02:40:00","VSML_220","V-NIL","2012-07-04",1,-30.168839999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1850,"TRANSGRIDV5_20180116135943","2017-01-09T03:00:00","VSML_220","V-NIL","2012-07-04",1,-23.787469999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1851,"TRANSGRIDV5_20180116135943","2017-01-09T00:50:00","VSML_220","V-NIL","2012-07-04",1,-17.208100000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1852,"TRANSGRIDV5_20180116135943","2017-01-09T02:50:00","VSML_220","V-NIL","2012-07-04",1,-16.044070000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1853,"TRANSGRIDV5_20180116135943","2017-01-09T01:50:00","VSML_220","V-NIL","2012-07-04",1,-15.64392,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1854,"TRANSGRIDV5_20180116135943","2017-01-09T01:20:00","VSML_220","V-NIL","2012-07-04",1,-15.162979999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1855,"TRANSGRIDV5_20180116135943","2017-01-09T03:15:00","VSML_220","V-NIL","2012-07-04",1,-13.36918,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1856,"TRANSGRIDV5_20180116135943","2017-01-09T03:10:00","VSML_220","V-NIL","2012-07-04",1,-13.362500000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1857,"TRANSGRIDV5_20180116135943","2017-01-09T02:15:00","VSML_220","V-NIL","2012-07-04",1,-13.344849999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1858,"TRANSGRIDV5_20180116135943","2017-01-09T00:40:00","VSML_220","V-NIL","2012-07-04",1,-12.07521,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1859,"TRANSGRIDV5_20180116135943","2017-01-09T00:05:00","VSML_ROC_80","V-NIL","2016-08-23",1,-241.34036,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1860,"TRANSGRIDV5_20180116135943","2017-01-09T00:10:00","VSML_ROC_80","V-NIL","2016-08-23",1,-23.309609999999999,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1861,"TRANSGRIDV5_20180116135943","2017-01-10T05:10:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-39.713819999999998,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1862,"TRANSGRIDV5_20180116135943","2017-01-10T05:05:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-38.903379999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1863,"TRANSGRIDV5_20180116135943","2017-01-10T05:15:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-35.737009999999998,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1864,"TRANSGRIDV5_20180116135943","2017-01-10T05:25:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-31.671939999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1865,"TRANSGRIDV5_20180116135943","2017-01-10T05:30:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-30.733339999999998,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1866,"TRANSGRIDV5_20180116135943","2017-01-10T05:20:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-21.654199999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1867,"TRANSGRIDV5_20180116135943","2017-01-10T05:45:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-14.523580000000001,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1868,"TRANSGRIDV5_20180116135943","2017-01-10T05:50:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-14.511799999999999,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1869,"TRANSGRIDV5_20180116135943","2017-01-10T05:35:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-14.411060000000001,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1870,"TRANSGRIDV5_20180116135943","2017-01-10T05:00:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-11.50939,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1871,"TRANSGRIDV5_20180116135943","2017-01-10T05:40:00","#R015072_012_RAMP_F","#R015072_RAMP","2017-01-09",1,-10.77732,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1872,"TRANSGRIDV5_20180116135943","2017-01-10T22:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-65.817610000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1873,"TRANSGRIDV5_20180116135943","2017-01-10T22:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.71998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1874,"TRANSGRIDV5_20180116135943","2017-01-10T22:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-10",57,-13.3194,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1875,"TRANSGRIDV5_20180116135943","2017-01-10T22:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-32.946289999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1876,"TRANSGRIDV5_20180116135943","2017-01-10T22:05:00","SVML_ROC_80","S-NIL","2016-08-23",1,-72.785690000000002,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1877,"TRANSGRIDV5_20180116135943","2017-01-10T16:25:00","SVML_ROC_80","S-NIL","2016-08-23",1,-56.4801,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1878,"TRANSGRIDV5_20180116135943","2017-01-10T22:10:00","SVML_ROC_80","S-NIL","2016-08-23",1,-55.76267,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1879,"TRANSGRIDV5_20180116135943","2017-01-10T15:30:00","SVML_ROC_80","S-NIL","2016-08-23",1,-11.668659999999999,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1880,"TRANSGRIDV5_20180116135943","2017-01-10T06:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-71.441569999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1881,"TRANSGRIDV5_20180116135943","2017-01-10T06:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-62.625549999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1882,"TRANSGRIDV5_20180116135943","2017-01-10T06:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-62.170439999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1883,"TRANSGRIDV5_20180116135943","2017-01-10T06:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-61.943759999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1884,"TRANSGRIDV5_20180116135943","2017-01-10T06:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-61.817349999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1885,"TRANSGRIDV5_20180116135943","2017-01-10T06:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-61.543469999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1886,"TRANSGRIDV5_20180116135943","2017-01-10T06:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-61.202080000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1887,"TRANSGRIDV5_20180116135943","2017-01-10T08:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-59.183219999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1888,"TRANSGRIDV5_20180116135943","2017-01-10T08:50:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-58.728000000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1889,"TRANSGRIDV5_20180116135943","2017-01-10T08:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-58.671529999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1890,"TRANSGRIDV5_20180116135943","2017-01-10T08:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-58.180819999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1891,"TRANSGRIDV5_20180116135943","2017-01-10T08:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-57.929729999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1892,"TRANSGRIDV5_20180116135943","2017-01-10T08:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-57.568649999999998,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1893,"TRANSGRIDV5_20180116135943","2017-01-10T06:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-56.03013,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1894,"TRANSGRIDV5_20180116135943","2017-01-10T07:40:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-55.543390000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1895,"TRANSGRIDV5_20180116135943","2017-01-10T08:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-43.757840000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1896,"TRANSGRIDV5_20180116135943","2017-01-10T07:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-41.075220000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1897,"TRANSGRIDV5_20180116135943","2017-01-10T06:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-40.328189999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1898,"TRANSGRIDV5_20180116135943","2017-01-10T06:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-37.51193,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1899,"TRANSGRIDV5_20180116135943","2017-01-10T07:45:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-36.817729999999997,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1900,"TRANSGRIDV5_20180116135943","2017-01-10T07:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-35.090800000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1901,"TRANSGRIDV5_20180116135943","2017-01-10T06:00:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-34.260840000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1902,"TRANSGRIDV5_20180116135943","2017-01-10T06:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-31.106570000000001,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1903,"TRANSGRIDV5_20180116135943","2017-01-10T07:25:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-30.12979,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1904,"TRANSGRIDV5_20180116135943","2017-01-10T07:30:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-29.328289999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1905,"TRANSGRIDV5_20180116135943","2017-01-10T05:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-28.793379999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1906,"TRANSGRIDV5_20180116135943","2017-01-10T07:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-27.6008,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1907,"TRANSGRIDV5_20180116135943","2017-01-10T08:35:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-27.535209999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1908,"TRANSGRIDV5_20180116135943","2017-01-10T08:05:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-27.044029999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1909,"TRANSGRIDV5_20180116135943","2017-01-10T07:15:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-26.889410000000002,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1910,"TRANSGRIDV5_20180116135943","2017-01-10T07:20:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-26.29147,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1911,"TRANSGRIDV5_20180116135943","2017-01-10T07:10:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-15.420489999999999,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1912,"TRANSGRIDV5_20180116135943","2017-01-10T07:55:00","V::N_BYPASS_HW_SY_V4","V-SMTS_BYPASS_HW_SY","2016-11-24",1,-12.81889,"Out=Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line, avoid trans. instability for fault and trip of a HWTS-SYTS or HWTS-SMTS 500kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","S Morang 2 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[1913,"TRANSGRIDV5_20180116135943","2017-01-10T21:35:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-12.94801,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1914,"TRANSGRIDV5_20180116135943","2017-01-10T00:15:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-12.581379999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1915,"TRANSGRIDV5_20180116135943","2017-01-10T21:45:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-12.37337,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1916,"TRANSGRIDV5_20180116135943","2017-01-10T22:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-134.87934999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1917,"TRANSGRIDV5_20180116135943","2017-01-10T22:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-120.56009,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1918,"TRANSGRIDV5_20180116135943","2017-01-10T22:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-98.530600000000007,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1919,"TRANSGRIDV5_20180116135943","2017-01-10T22:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-54.534770000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1920,"TRANSGRIDV5_20180116135943","2017-01-10T22:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-54.398020000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1921,"TRANSGRIDV5_20180116135943","2017-01-10T22:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-53.597430000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1922,"TRANSGRIDV5_20180116135943","2017-01-10T03:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.561140000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1923,"TRANSGRIDV5_20180116135943","2017-01-10T01:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-34.123730000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1924,"TRANSGRIDV5_20180116135943","2017-01-10T22:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.98657,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1925,"TRANSGRIDV5_20180116135943","2017-01-10T22:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.597519999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1926,"TRANSGRIDV5_20180116135943","2017-01-10T22:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.795200000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1927,"TRANSGRIDV5_20180116135943","2017-01-10T22:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.020810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1928,"TRANSGRIDV5_20180116135943","2017-01-10T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.467980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1929,"TRANSGRIDV5_20180116135943","2017-01-10T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-22.521550000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1930,"TRANSGRIDV5_20180116135943","2017-01-10T21:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-21.422499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1931,"TRANSGRIDV5_20180116135943","2017-01-10T21:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.153459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1932,"TRANSGRIDV5_20180116135943","2017-01-10T01:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.666979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1933,"TRANSGRIDV5_20180116135943","2017-01-10T03:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.123270000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1934,"TRANSGRIDV5_20180116135943","2017-01-10T02:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.232320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1935,"TRANSGRIDV5_20180116135943","2017-01-10T02:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.19941,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1936,"TRANSGRIDV5_20180116135943","2017-01-10T03:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.187999999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1937,"TRANSGRIDV5_20180116135943","2017-01-10T22:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.042539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1938,"TRANSGRIDV5_20180116135943","2017-01-10T21:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.909120000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1939,"TRANSGRIDV5_20180116135943","2017-01-10T02:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.81794,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1940,"TRANSGRIDV5_20180116135943","2017-01-10T23:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.007840000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1941,"TRANSGRIDV5_20180116135943","2017-01-10T23:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.65024,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1942,"TRANSGRIDV5_20180116135943","2017-01-10T00:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.109909999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1943,"TRANSGRIDV5_20180116135943","2017-01-10T03:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.884589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1944,"TRANSGRIDV5_20180116135943","2017-01-10T00:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.79095,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1945,"TRANSGRIDV5_20180116135943","2017-01-10T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.163410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1946,"TRANSGRIDV5_20180116135943","2017-01-10T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.12412,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1947,"TRANSGRIDV5_20180116135943","2017-01-10T04:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.688980000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1948,"TRANSGRIDV5_20180116135943","2017-01-10T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.659459999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1949,"TRANSGRIDV5_20180116135943","2017-01-10T03:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.428129999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1950,"TRANSGRIDV5_20180116135943","2017-01-10T03:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.402469999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1951,"TRANSGRIDV5_20180116135943","2017-01-10T03:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.39673,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1952,"TRANSGRIDV5_20180116135943","2017-01-10T04:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.39202,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1953,"TRANSGRIDV5_20180116135943","2017-01-10T01:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.36595,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1954,"TRANSGRIDV5_20180116135943","2017-01-10T03:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.36534,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1955,"TRANSGRIDV5_20180116135943","2017-01-10T02:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.3543,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1956,"TRANSGRIDV5_20180116135943","2017-01-10T04:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.3001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1957,"TRANSGRIDV5_20180116135943","2017-01-10T04:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.22025,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1958,"TRANSGRIDV5_20180116135943","2017-01-10T04:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.176780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1959,"TRANSGRIDV5_20180116135943","2017-01-10T02:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.99188,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1960,"TRANSGRIDV5_20180116135943","2017-01-10T02:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.97418,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1961,"TRANSGRIDV5_20180116135943","2017-01-10T02:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.96543,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1962,"TRANSGRIDV5_20180116135943","2017-01-10T02:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.956899999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1963,"TRANSGRIDV5_20180116135943","2017-01-10T03:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.94497,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1964,"TRANSGRIDV5_20180116135943","2017-01-10T03:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.89786,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1965,"TRANSGRIDV5_20180116135943","2017-01-10T04:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.84854,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1966,"TRANSGRIDV5_20180116135943","2017-01-10T01:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.801920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1967,"TRANSGRIDV5_20180116135943","2017-01-10T02:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.55495,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1968,"TRANSGRIDV5_20180116135943","2017-01-10T02:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.531090000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1969,"TRANSGRIDV5_20180116135943","2017-01-10T01:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.51473,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1970,"TRANSGRIDV5_20180116135943","2017-01-10T04:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.38374,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1971,"TRANSGRIDV5_20180116135943","2017-01-10T04:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.3772,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1972,"TRANSGRIDV5_20180116135943","2017-01-10T04:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.368819999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1973,"TRANSGRIDV5_20180116135943","2017-01-10T01:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.01648,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1974,"TRANSGRIDV5_20180116135943","2017-01-10T23:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.01605,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1975,"TRANSGRIDV5_20180116135943","2017-01-10T14:00:00","V>>N-NIL_HA","N-NIL","2016-07-01",1,-135.29971,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1976,"TRANSGRIDV5_20180116135943","2017-01-10T14:05:00","V>>N-NIL_HA","N-NIL","2016-07-01",1,-133.79414,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1977,"TRANSGRIDV5_20180116135943","2017-01-10T13:55:00","V>>N-NIL_HA","N-NIL","2016-07-01",1,-36.851660000000003,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1978,"TRANSGRIDV5_20180116135943","2017-01-10T13:50:00","V>>N-NIL_HA","N-NIL","2016-07-01",1,-31.771850000000001,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1979,"TRANSGRIDV5_20180116135943","2017-01-10T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-108.6767,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1980,"TRANSGRIDV5_20180116135943","2017-01-10T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-102.58311,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1981,"TRANSGRIDV5_20180116135943","2017-01-10T15:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-101.99928,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1982,"TRANSGRIDV5_20180116135943","2017-01-10T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-99.379149999999996,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1983,"TRANSGRIDV5_20180116135943","2017-01-10T15:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-98.215350000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1984,"TRANSGRIDV5_20180116135943","2017-01-10T15:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-47.750830000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1985,"TRANSGRIDV5_20180116135943","2017-01-10T16:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-44.255369999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1986,"TRANSGRIDV5_20180116135943","2017-01-10T16:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-41.261200000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1987,"TRANSGRIDV5_20180116135943","2017-01-10T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-29.319980000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1988,"TRANSGRIDV5_20180116135943","2017-01-10T16:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.15174,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1989,"TRANSGRIDV5_20180116135943","2017-01-10T15:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.896889999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1990,"TRANSGRIDV5_20180116135943","2017-01-10T15:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.561579999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1991,"TRANSGRIDV5_20180116135943","2017-01-10T15:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-20.24192,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1992,"TRANSGRIDV5_20180116135943","2017-01-10T16:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.09905,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1993,"TRANSGRIDV5_20180116135943","2017-01-10T16:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.886200000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1994,"TRANSGRIDV5_20180116135943","2017-01-10T16:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.847810000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1995,"TRANSGRIDV5_20180116135943","2017-01-10T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.92244,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1996,"TRANSGRIDV5_20180116135943","2017-01-10T16:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.84329,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1997,"TRANSGRIDV5_20180116135943","2017-01-10T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-10.23875,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[1998,"TRANSGRIDV5_20180116135943","2017-01-11T05:05:00","#R015074_012_RAMP_F","#R015074_RAMP","2017-01-10",1,-59.307479999999998,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[1999,"TRANSGRIDV5_20180116135943","2017-01-11T05:15:00","#R015074_012_RAMP_F","#R015074_RAMP","2017-01-10",1,-54.352269999999997,"Hard Ramping constraint for constraint V::N_BYPASS_HW_SY_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Three SMTS 500kV CBs for HWTS & SYTS line (#1 or #2), temporary bypass for HWTS to SYTS direct line","REGULATED","10","Ramping Constraint","PLANNED",0]
[2025,"TRANSGRIDV5_20180116135943","2017-01-11T15:50:00","N>N-X_96H+9W2_1","N-X_96H_9W2","2016-12-07",1,-37.635280000000002,"Out= Coffs Harbour to Koolkhan (96H) and Kempsey-Raleigh (9W2) and 132kV line, avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD","OUTAGE","OTHER","Coffs Harbour to Koolkhan (96H) and Kempsey-Raleigh (9W2) and 132kV lines","REGULATED","INCLUDED","","UNPLANNED",1]
[2070,"TRANSGRIDV5_20180116135943","2017-01-11T17:20:00","NRM_VIC1_SA1","NRM_NIL_ALL","2012-06-12",1,-71.349279999999993,"Negative Residue Management constraint for VIC to SA flow","SYSTEM NORMAL","NRM",null,"","","",null,0]
[2100,"TRANSGRIDV5_20180116135943","2017-01-11T19:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-86.927869999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2126,"TRANSGRIDV5_20180116135943","2017-01-11T18:40:00","SVML_ROC_80","S-NIL","2016-08-23",1,-109.85715999999999,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2197,"TRANSGRIDV5_20180116135943","2017-01-11T21:20:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-24.983360000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2227,"TRANSGRIDV5_20180116135943","2017-01-11T01:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.466670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2253,"TRANSGRIDV5_20180116135943","2017-01-11T00:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.831700000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2324,"TRANSGRIDV5_20180116135943","2017-01-11T17:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.709180000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2350,"TRANSGRIDV5_20180116135943","2017-01-12T05:55:00","#R015078_025_RAMP_F","#R015078_RAMP","2017-01-12",1,-13.102349999999999,"Hard Ramping constraint for constraint V::N_LTWG_V4, Effective Date: 24/11/2016, Version: 1","OUTAGE","RAMP","Lower Tumut to Wagga 330kV line O51","REGULATED","10","Ramping Constraint","PLANNED",0]
[2380,"TRANSGRIDV5_20180116135943","2017-01-12T11:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-35.851039999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2410,"TRANSGRIDV5_20180116135943","2017-01-12T16:20:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-23.981459999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[2477,"TRANSGRIDV5_20180116135943","2017-01-12T01:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.488799999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2507,"TRANSGRIDV5_20180116135943","2017-01-13T18:05:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-13",3,40.226039999999998,"N-Q-MNSP1.ENERGY * -1 >= 95 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2537,"TRANSGRIDV5_20180116135943","2017-01-13T21:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-13",3,16.69605,"N-Q-MNSP1.ENERGY * -1 >= 95 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2604,"TRANSGRIDV5_20180116135943","2017-01-13T13:10:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-158.66387,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2634,"TRANSGRIDV5_20180116135943","2017-01-13T10:45:00","N>N-NIL_LSDU","N-NIL","2014-02-13",1,-29.60521,"Out = Nil, avoid overloading Lismore to Dunoon line (9U6 or 9U7) on trip of the other Lismore to Dunoon line (9U7 or 9U6), Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2660,"TRANSGRIDV5_20180116135943","2017-01-13T20:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-44.383719999999997,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2731,"TRANSGRIDV5_20180116135943","2017-01-13T14:35:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2016-06-21",1,-93.847710000000006,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2761,"TRANSGRIDV5_20180116135943","2017-01-14T20:10:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-14",5,953.02908000000002,"N-Q-MNSP1.ENERGY * -1 >= 90 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2787,"TRANSGRIDV5_20180116135943","2017-01-14T18:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-14",5,13.294560000000001,"N-Q-MNSP1.ENERGY * -1 >= 90 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2858,"TRANSGRIDV5_20180116135943","2017-01-14T18:45:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-11585.86889,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2884,"TRANSGRIDV5_20180116135943","2017-01-14T16:50:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-11595.64106,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[2914,"TRANSGRIDV5_20180116135943","2017-01-14T16:50:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-1982.57113,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[2944,"TRANSGRIDV5_20180116135943","2017-01-14T13:40:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-46.065170000000002,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[3011,"TRANSGRIDV5_20180116135943","2017-01-14T01:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-10.02788,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3041,"TRANSGRIDV5_20180116135943","2017-01-14T16:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-185.62441000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3071,"TRANSGRIDV5_20180116135943","2017-01-14T22:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.036269999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3138,"TRANSGRIDV5_20180116135943","2017-01-14T14:20:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.844909999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3168,"TRANSGRIDV5_20180116135943","2017-01-14T03:10:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.2225,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3194,"TRANSGRIDV5_20180116135943","2017-01-14T11:05:00","V>>V_NIL_2B_R","V-NIL_RADIAL_3-4","2016-06-21",1,-13.13862,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3265,"TRANSGRIDV5_20180116135943","2017-01-15T13:30:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-19.951789999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3295,"TRANSGRIDV5_20180116135943","2017-01-15T18:25:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-42.39143,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3321,"TRANSGRIDV5_20180116135943","2017-01-15T19:20:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-18.859110000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3392,"TRANSGRIDV5_20180116135943","2017-01-15T02:50:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-27.636839999999999,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[3422,"TRANSGRIDV5_20180116135943","2017-01-15T00:55:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-20.61514,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[3438,"TRANSGRIDV5_20180116135943","2017-01-15T05:35:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-18.402280000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[3477,"TRANSGRIDV5_20180116135943","2017-01-16T21:55:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-37.271169999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3544,"TRANSGRIDV5_20180116135943","2017-01-17T05:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-31.68948,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3574,"TRANSGRIDV5_20180116135943","2017-01-17T17:20:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-25.856110000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[3604,"TRANSGRIDV5_20180116135943","2017-01-17T03:45:00","NSA_Q_BARCALDN","NSA-Q_BARCALDN","2015-05-06",1,-1077.1858199999999,"Network Support Agreement for Barcaldine GT to meet local islanded demand for the planned outage of 7153 T71 Clermont to H15 Lilyvale or 7154 T72 Barcaldine to T71 Clermont 132kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3671,"TRANSGRIDV5_20180116135943","2017-01-17T18:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-86.180779999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3701,"TRANSGRIDV5_20180116135943","2017-01-17T17:45:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-890.50287000000003,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3727,"TRANSGRIDV5_20180116135943","2017-01-17T17:10:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-554.19311000000005,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3798,"TRANSGRIDV5_20180116135943","2017-01-18T19:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-186.27799999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3828,"TRANSGRIDV5_20180116135943","2017-01-18T16:00:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-189.21313000000001,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3854,"TRANSGRIDV5_20180116135943","2017-01-18T19:20:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-110.38836000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[3884,"TRANSGRIDV5_20180116135943","2017-01-18T13:20:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-33.61994,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[3955,"TRANSGRIDV5_20180116135943","2017-01-18T02:05:00","V::N_NIL_V1","V-NIL","2016-11-24",1,-56.432899999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[3981,"TRANSGRIDV5_20180116135943","2017-01-18T14:55:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-130.88605000000001,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor 2 220kV BUS; Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[4011,"TRANSGRIDV5_20180116135943","2017-01-18T12:15:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-21.349119999999999,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor 2 220kV BUS; Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[4078,"TRANSGRIDV5_20180116135943","2017-01-19T17:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-80.658450000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4108,"TRANSGRIDV5_20180116135943","2017-01-19T15:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-32.390180000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4138,"TRANSGRIDV5_20180116135943","2017-01-19T14:25:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-18.460450000000002,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4205,"TRANSGRIDV5_20180116135943","2017-01-19T10:50:00","N>LSDU_LSDU","CA_AUTO","2017-01-19",69,-54.936360000000001,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4235,"TRANSGRIDV5_20180116135943","2017-01-19T22:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-50.517910000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4261,"TRANSGRIDV5_20180116135943","2017-01-19T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-15.502050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4332,"TRANSGRIDV5_20180116135943","2017-01-20T22:20:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-20",3,12.948,"N-Q-MNSP1.ENERGY * -1 >= 76 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4362,"TRANSGRIDV5_20180116135943","2017-01-20T14:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-48.405389999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4388,"TRANSGRIDV5_20180116135943","2017-01-20T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-42.585639999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4418,"TRANSGRIDV5_20180116135943","2017-01-20T10:35:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-34.447740000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4489,"TRANSGRIDV5_20180116135943","2017-01-20T15:50:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-43.057110000000002,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[4515,"TRANSGRIDV5_20180116135943","2017-01-20T15:05:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-21.878540000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[4545,"TRANSGRIDV5_20180116135943","2017-01-20T02:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-13.54307,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4612,"TRANSGRIDV5_20180116135943","2017-01-21T10:45:00","N>LSDU_LSDU","CA_AUTO","2017-01-21",91,-68.323999999999998,"Constraint Automation, O/L 9U7/L         @LISM132 for CTG LN9X on trip of LISM132-DUNOON 9U6/L 132KV LINE.  Generated by RTCA[EMS]","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4642,"TRANSGRIDV5_20180116135943","2017-01-21T14:30:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-30.916879999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4672,"TRANSGRIDV5_20180116135943","2017-01-22T03:45:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-11.908770000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[4739,"TRANSGRIDV5_20180116135943","2017-01-22T23:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-111.85396,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4769,"TRANSGRIDV5_20180116135943","2017-01-23T00:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-44.341819999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4799,"TRANSGRIDV5_20180116135943","2017-01-23T01:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-26.652670000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4866,"TRANSGRIDV5_20180116135943","2017-01-23T23:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.470510000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[4896,"TRANSGRIDV5_20180116135943","2017-01-24T15:10:00","#TORRB1_E","#TORRB1_E","2017-01-24",1,-1064.9830199999999,"STSB1.ENERGY * 1 <= 60 (Wt = 360)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[4917,"TRANSGRIDV5_20180116135943","2017-01-24T20:20:00","#TORRB1_E","#TORRB1_E","2017-01-24",1,-74.630790000000005,"STSB1.ENERGY * 1 <= 60 (Wt = 360)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[4951,"TRANSGRIDV5_20180116135943","2017-01-24T19:25:00","#TORRB1_E","#TORRB1_E","2017-01-24",1,-14.380610000000001,"STSB1.ENERGY * 1 <= 60 (Wt = 360)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[5022,"TRANSGRIDV5_20180116135943","2017-01-24T18:50:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-18.830500000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[5048,"TRANSGRIDV5_20180116135943","2017-01-24T01:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-48.696350000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5078,"TRANSGRIDV5_20180116135943","2017-01-24T13:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-92.924379999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5145,"TRANSGRIDV5_20180116135943","2017-01-24T04:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.158720000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5175,"TRANSGRIDV5_20180116135943","2017-01-25T17:40:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-01-25",1,21.923909999999999,"N-Q-MNSP1.ENERGY * -1 >= 71 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5205,"TRANSGRIDV5_20180116135943","2017-01-25T18:35:00","#TORRB1_E","#TORRB1_E","2017-01-25",2,-1079.98937,"STSB1.ENERGY * 1 <= 200 (Wt = 360)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[5272,"TRANSGRIDV5_20180116135943","2017-01-25T16:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.327869999999997,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5302,"TRANSGRIDV5_20180116135943","2017-01-25T18:00:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-17.472470000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5332,"TRANSGRIDV5_20180116135943","2017-01-25T20:25:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-13.221,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[5399,"TRANSGRIDV5_20180116135943","2017-01-26T19:20:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-93.272440000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5429,"TRANSGRIDV5_20180116135943","2017-01-26T12:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-43.194070000000004,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5455,"TRANSGRIDV5_20180116135943","2017-01-26T22:05:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-682.47248000000002,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[5485,"TRANSGRIDV5_20180116135943","2017-01-26T21:10:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-31.967359999999999,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[5556,"TRANSGRIDV5_20180116135943","2017-01-27T08:55:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-51.667290000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5582,"TRANSGRIDV5_20180116135943","2017-01-27T10:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-30.78791,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5612,"TRANSGRIDV5_20180116135943","2017-01-28T18:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-104.73237,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5683,"TRANSGRIDV5_20180116135943","2017-01-28T17:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-76.106110000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5709,"TRANSGRIDV5_20180116135943","2017-01-29T20:05:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-259.19371999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5739,"TRANSGRIDV5_20180116135943","2017-01-29T20:15:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-102.92928999999999,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[5806,"TRANSGRIDV5_20180116135943","2017-01-29T12:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-208.94452000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5836,"TRANSGRIDV5_20180116135943","2017-01-29T00:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-44.570709999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5866,"TRANSGRIDV5_20180116135943","2017-01-29T13:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.865780000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5892,"TRANSGRIDV5_20180116135943","2017-01-29T08:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.151810000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5963,"TRANSGRIDV5_20180116135943","2017-01-29T19:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.245150000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[5989,"TRANSGRIDV5_20180116135943","2017-01-30T17:35:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-41.441879999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[6019,"TRANSGRIDV5_20180116135943","2017-01-30T18:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-40.379750000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6090,"TRANSGRIDV5_20180116135943","2017-01-30T21:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.143859999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6116,"TRANSGRIDV5_20180116135943","2017-01-30T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.987960000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6146,"TRANSGRIDV5_20180116135943","2017-01-30T11:15:00","V>>N-NIL_HA","N-NIL","2016-07-01",1,-84.805080000000004,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6217,"TRANSGRIDV5_20180116135943","2017-01-30T11:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-52.147779999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6243,"TRANSGRIDV5_20180116135943","2017-01-30T13:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-23.971050000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6273,"TRANSGRIDV5_20180116135943","2017-01-31T07:35:00","#R015123_001_RAMP_F","#R015123_RAMP","2017-01-30",1,-18.383859999999999,"Hard Ramping constraint for constraint V>>V_ROTS_TX_2A_R, Effective Date: 22/08/2016, Version: 1","OUTAGE","RAMP","Rowville A1 or A2 500/220 kV txfmr","REGULATED","10","Ramping Constraint","PLANNED",0]
[6340,"TRANSGRIDV5_20180116135943","2017-01-31T15:30:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-87.690070000000006,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6370,"TRANSGRIDV5_20180116135943","2017-01-31T14:30:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-35.648339999999997,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[6420,"TRANSGRIDV5_20180116135943","2017-01-31T06:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-40.092579999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6425,"TRANSGRIDV5_20180116135943","2017-01-31T04:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-21.346029999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6496,"TRANSGRIDV5_20180116135943","2017-01-31T16:45:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-10.59684,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6522,"TRANSGRIDV5_20180116135943","2017-01-31T14:05:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-10.114710000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6552,"TRANSGRIDV5_20180116135943","2017-01-31T02:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-41.150379999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6623,"TRANSGRIDV5_20180116135943","2017-01-31T13:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-27.707249999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6649,"TRANSGRIDV5_20180116135943","2017-01-31T08:40:00","V>>V_ROTS_TX_2A_R","V-ROTX_R","2016-08-22",1,-34.786810000000003,"Out = Rowville A1 or A2 500/220 kV txfmr, avoid pre-contingent overload of the South Morang F2 500/330 kV txfmr, radial mode, YWG1 on 500 kV, feedback","OUTAGE","OTHER","Rowvill500 A2 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[6679,"TRANSGRIDV5_20180116135943","2017-02-01T10:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-50.729579999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6750,"TRANSGRIDV5_20180116135943","2017-02-01T15:40:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-27.976780000000002,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[6776,"TRANSGRIDV5_20180116135943","2017-02-01T17:10:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-15.07137,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[6806,"TRANSGRIDV5_20180116135943","2017-02-01T19:30:00","NQTE_ROC","N-NIL","2010-11-08",2,-14.4381,"Out=Nil, Rate of Change (NSW to Qld) constraint (80 MW / 5 Min) for Terranora Interconnector","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6873,"TRANSGRIDV5_20180116135943","2017-02-02T13:50:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-02-02",2,21.931190000000001,"N-Q-MNSP1.ENERGY * -1 >= 90 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6903,"TRANSGRIDV5_20180116135943","2017-02-02T18:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-11600.963540000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[6933,"TRANSGRIDV5_20180116135943","2017-02-02T08:50:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-28.6416,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[6959,"TRANSGRIDV5_20180116135943","2017-02-02T17:50:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-43.718499999999999,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7030,"TRANSGRIDV5_20180116135943","2017-02-02T19:25:00","NRM_QLD1_NSW1","NRM_NIL_ALL","2012-06-12",1,-1047.37852,"Negative Residue Management constraint for QLD to NSW flow","SYSTEM NORMAL","NRM",null,"","","",null,0]
[7060,"TRANSGRIDV5_20180116135943","2017-02-03T15:10:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-47.499389999999998,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7086,"TRANSGRIDV5_20180116135943","2017-02-03T15:05:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-57.445929999999997,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[7157,"TRANSGRIDV5_20180116135943","2017-02-04T17:05:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-19.987469999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[7183,"TRANSGRIDV5_20180116135943","2017-02-04T22:20:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-13.32996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7213,"TRANSGRIDV5_20180116135943","2017-02-04T06:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-28.492730000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7284,"TRANSGRIDV5_20180116135943","2017-02-04T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.77881,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7310,"TRANSGRIDV5_20180116135943","2017-02-04T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-93.409989999999993,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7340,"TRANSGRIDV5_20180116135943","2017-02-05T16:00:00","N_X_MBTE2_A","N-X_MBTE_2","2013-11-25",1,-302.96926999999999,"Out= two Directlink cables, NSW to Qld limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[7407,"TRANSGRIDV5_20180116135943","2017-02-05T06:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-28.985779999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7437,"TRANSGRIDV5_20180116135943","2017-02-05T05:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.746400000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7467,"TRANSGRIDV5_20180116135943","2017-02-05T14:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-90.624700000000004,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7493,"TRANSGRIDV5_20180116135943","2017-02-05T20:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-86.274349999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7564,"TRANSGRIDV5_20180116135943","2017-02-06T22:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-28.676639999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7594,"TRANSGRIDV5_20180116135943","2017-02-06T12:50:00","N>>N-NIL__B_15M","N-NIL","2016-07-01",1,-132.71349000000001,"Out= Nil, avoid O/L Upper Tumut to Canberra (01) using 15 mins rating on trip of Lower Tumut to Canberra (07) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7620,"TRANSGRIDV5_20180116135943","2017-02-06T17:50:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-62.135939999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[7691,"TRANSGRIDV5_20180116135943","2017-02-06T23:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-21.566199999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7717,"TRANSGRIDV5_20180116135943","2017-02-06T20:25:00","V::N_NIL_S2","V-NIL","2016-11-24",1,-89.667410000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7747,"TRANSGRIDV5_20180116135943","2017-02-06T04:40:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-28.892969999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7777,"TRANSGRIDV5_20180116135943","2017-02-06T22:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-103.81766,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7833,"TRANSGRIDV5_20180116135943","2017-02-06T00:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-33.06597,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7873,"TRANSGRIDV5_20180116135943","2017-02-06T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-135.26554999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7899,"TRANSGRIDV5_20180116135943","2017-02-06T12:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-102.05184,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[7970,"TRANSGRIDV5_20180116135943","2017-02-07T19:25:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-02-07",3,59.192950000000003,"N-Q-MNSP1.ENERGY * -1 >= 75 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8000,"TRANSGRIDV5_20180116135943","2017-02-07T18:45:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-154.95375000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8026,"TRANSGRIDV5_20180116135943","2017-02-07T13:50:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-36.194180000000003,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8097,"TRANSGRIDV5_20180116135943","2017-02-07T16:30:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-34.724049999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[8127,"TRANSGRIDV5_20180116135943","2017-02-07T15:10:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-24.71754,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[8153,"TRANSGRIDV5_20180116135943","2017-02-07T07:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-98.214209999999994,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8224,"TRANSGRIDV5_20180116135943","2017-02-07T10:00:00","V::N_DDSM_V2","V-DDSM","2016-12-16",1,-40.607689999999998,"Out = Dederang to South Morang 330kV line, prevent transient instability for fault and trip of the parallel Dederang to South Morang 330kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Dederang S Morang 1 330kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[8250,"TRANSGRIDV5_20180116135943","2017-02-07T00:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-60.022660000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8280,"TRANSGRIDV5_20180116135943","2017-02-07T23:00:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.244599999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8310,"TRANSGRIDV5_20180116135943","2017-02-07T03:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-22.227989999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8377,"TRANSGRIDV5_20180116135943","2017-02-08T12:55:00","N_NYNGANSF_010","N-NYNGANSF_010","2016-09-06",1,-1131.9335699999999,"Nyngan Solar Farm upper limit of 10 MW","OUTAGE","OTHER","Nyngan132 SVC Unit 66kV SVC","REGULATED","99","Non Inclusion",null,0,"Essential Energy outage"]
[8407,"TRANSGRIDV5_20180116135943","2017-02-08T03:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-35.796259999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8437,"TRANSGRIDV5_20180116135943","2017-02-08T01:10:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.224689999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8504,"TRANSGRIDV5_20180116135943","2017-02-08T22:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-23.36223,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8534,"TRANSGRIDV5_20180116135943","2017-02-08T12:25:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-10.72566,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8560,"TRANSGRIDV5_20180116135943","2017-02-09T18:50:00","#PPCCGT_E","#PPCCGT_E","2017-02-09",1,-1369.02007,"SPPT.ENERGY * 1 <= 214 (Wt = 50)","OUTAGE","OTHER","Pelican Point CCGT","REGULATED","99","Non Inclusion",null,0]
[8631,"TRANSGRIDV5_20180116135943","2017-02-09T03:35:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-34.185580000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8661,"TRANSGRIDV5_20180116135943","2017-02-09T18:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-179.02721,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8687,"TRANSGRIDV5_20180116135943","2017-02-09T15:40:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-18.725539999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8758,"TRANSGRIDV5_20180116135943","2017-02-09T19:15:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-72.378339999999994,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8784,"TRANSGRIDV5_20180116135943","2017-02-09T14:30:00","V>SML_NSWRB_10","V-NIL","2016-06-21",1,-127.26096,"Out = NSW Murraylink runback scheme, avoid O/L of Kerang to Wemen 220 kV line section for loss of Balranald to Darlington Point (X5/1) 220 kV line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8814,"TRANSGRIDV5_20180116135943","2017-02-10T21:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-60.950029999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[8844,"TRANSGRIDV5_20180116135943","2017-02-10T21:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-69.439149999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8911,"TRANSGRIDV5_20180116135943","2017-02-10T15:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-279.69792999999999,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8941,"TRANSGRIDV5_20180116135943","2017-02-10T20:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-87.651449999999997,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[8971,"TRANSGRIDV5_20180116135943","2017-02-10T11:55:00","V>>SML_NIL_1","V-NIL_BATS_MLTS1_15M","2016-06-21",1,-1071.1380999999999,"Out = Nil, avoid O/L Moorabool to Ballarat No.1 220 kV line for loss of Moorabool to Elaine to Ballarat 220 kV line and Mt Mercer Wind Farm, 15 minute line ratings, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9038,"TRANSGRIDV5_20180116135943","2017-02-10T12:10:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-220.24021999999999,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9068,"TRANSGRIDV5_20180116135943","2017-02-10T19:45:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-109.68968,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9094,"TRANSGRIDV5_20180116135943","2017-02-10T19:25:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-18.95,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9165,"TRANSGRIDV5_20180116135943","2017-02-11T15:10:00","N>>Q_LDMU_B","N-LDMU_83","2016-02-09",1,-304.66327999999999,"Out= Liddell-Muswellbrook(83), avoid Liddell->Tamworth(84) OL on largest QLD generator trip ; FBk","OUTAGE","OTHER","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[9195,"TRANSGRIDV5_20180116135943","2017-02-11T18:05:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-23.423960000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[9221,"TRANSGRIDV5_20180116135943","2017-02-11T14:05:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-10.20994,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[9292,"TRANSGRIDV5_20180116135943","2017-02-11T15:45:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-73.025469999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9296,"TRANSGRIDV5_20180116135943","2017-02-11T19:40:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-72.274119999999996,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9347,"TRANSGRIDV5_20180116135943","2017-02-11T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-39.024760000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9377,"TRANSGRIDV5_20180116135943","2017-02-11T23:35:00","V::N_LTWG_V4","N-LTWG_RADIAL","2016-11-24",1,-238.13704999999999,"Out = Lower Tumut to Wagga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Lwr Tumut Wagga 051 330kV LINE; Wagga A 330kV BUS","REGULATED","INCLUDED","","UNPLANNED",1]
[9444,"TRANSGRIDV5_20180116135943","2017-02-11T09:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-105.94828,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9474,"TRANSGRIDV5_20180116135943","2017-02-11T01:55:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-18.322140000000001,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9504,"TRANSGRIDV5_20180116135943","2017-02-11T17:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-137.35809,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9571,"TRANSGRIDV5_20180116135943","2017-02-11T12:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-84.393900000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9601,"TRANSGRIDV5_20180116135943","2017-02-11T15:30:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-295.29056000000003,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9627,"TRANSGRIDV5_20180116135943","2017-02-11T17:55:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-204.40627000000001,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9698,"TRANSGRIDV5_20180116135943","2017-02-11T20:20:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-72.563670000000002,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9728,"TRANSGRIDV5_20180116135943","2017-02-12T20:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-81.135639999999995,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9754,"TRANSGRIDV5_20180116135943","2017-02-12T18:50:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-13068.443960000001,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9784,"TRANSGRIDV5_20180116135943","2017-02-12T14:35:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2016-02-09",1,-209.51627999999999,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[9855,"TRANSGRIDV5_20180116135943","2017-02-12T15:50:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-53.060220000000001,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[9881,"TRANSGRIDV5_20180116135943","2017-02-12T14:35:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-42.893059999999998,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[9911,"TRANSGRIDV5_20180116135943","2017-02-12T18:55:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-19.58811,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[9978,"TRANSGRIDV5_20180116135943","2017-02-12T11:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-28.770879999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10008,"TRANSGRIDV5_20180116135943","2017-02-12T16:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.7424,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10038,"TRANSGRIDV5_20180116135943","2017-02-12T03:25:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-50.183430000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[10105,"TRANSGRIDV5_20180116135943","2017-02-12T01:20:00","V::N_LTWG_V4","N-LTWG_RADIAL","2016-11-24",1,-28.142040000000001,"Out = Lower Tumut to Wagga 330kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Basslink VIC to TAS, Yallourn W Unit 1 on 500 kV.","OUTAGE","OTHER","Lwr Tumut Wagga 051 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[10135,"TRANSGRIDV5_20180116135943","2017-02-12T22:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-32.801729999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10161,"TRANSGRIDV5_20180116135943","2017-02-12T01:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.458320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10232,"TRANSGRIDV5_20180116135943","2017-02-12T10:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-50.65925,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10262,"TRANSGRIDV5_20180116135943","2017-02-12T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-26.214269999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10288,"TRANSGRIDV5_20180116135943","2017-02-12T15:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-21.519449999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10318,"TRANSGRIDV5_20180116135943","2017-02-13T13:15:00","#N-Q-MNSP1_I_E","#N-Q-MNSP1_E","2017-02-13",3,174.52690999999999,"N-Q-MNSP1.ENERGY * -1 >= 80 (Wt = 20)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10389,"TRANSGRIDV5_20180116135943","2017-02-13T08:50:00","N>>Q_LDMU_B","N-LDMU_83","2016-02-09",1,-215.37279000000001,"Out= Liddell-Muswellbrook(83), avoid Liddell->Tamworth(84) OL on largest QLD generator trip ; FBk","OUTAGE","OTHER","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[10415,"TRANSGRIDV5_20180116135943","2017-02-13T07:45:00","N>>Q_LDMU_B","N-LDMU_83","2016-02-09",1,-177.79043999999999,"Out= Liddell-Muswellbrook(83), avoid Liddell->Tamworth(84) OL on largest QLD generator trip ; FBk","OUTAGE","OTHER","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[10445,"TRANSGRIDV5_20180116135943","2017-02-13T13:10:00","N>>Q_LDMU_B","N-LDMU_83","2016-02-09",1,-41.794750000000001,"Out= Liddell-Muswellbrook(83), avoid Liddell->Tamworth(84) OL on largest QLD generator trip ; FBk","OUTAGE","OTHER","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[10512,"TRANSGRIDV5_20180116135943","2017-02-13T02:25:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-47.331969999999998,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood to South Morang 500kV line","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[10542,"TRANSGRIDV5_20180116135943","2017-02-13T05:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-69.043440000000004,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10572,"TRANSGRIDV5_20180116135943","2017-02-13T11:35:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-10-11",1,-114.24909,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A4 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[10639,"TRANSGRIDV5_20180116135943","2017-02-13T12:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-81.307149999999993,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10669,"TRANSGRIDV5_20180116135943","2017-02-13T15:45:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-48.15849,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10699,"TRANSGRIDV5_20180116135943","2017-02-13T16:35:00","V>>V_NIL_5","V-NIL","2016-06-21",1,-41.55471,"Out = Nil, avoid O/L either Mount Beauty to Dederang 220 kV line (flow to North) for trip of the parallel line, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10766,"TRANSGRIDV5_20180116135943","2017-02-14T00:55:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-65.620329999999996,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10775,"TRANSGRIDV5_20180116135943","2017-02-14T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-54.547609999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10821,"TRANSGRIDV5_20180116135943","2017-02-14T09:00:00","V>>V_KTS_TX_A2_2A_R","V-KTTX_A2_OR_A4_R","2016-10-11",1,-17.61683,"Out = Keilor A2 or A4 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A4 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[10851,"TRANSGRIDV5_20180116135943","2017-02-15T02:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-19.146170000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10922,"TRANSGRIDV5_20180116135943","2017-02-15T22:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-25.964970000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10948,"TRANSGRIDV5_20180116135943","2017-02-15T15:50:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-17.48854,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[10978,"TRANSGRIDV5_20180116135943","2017-02-16T00:50:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-54.104370000000003,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11045,"TRANSGRIDV5_20180116135943","2017-02-16T01:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-13.80639,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11075,"TRANSGRIDV5_20180116135943","2017-02-16T15:45:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.089919999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11105,"TRANSGRIDV5_20180116135943","2017-02-17T00:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.28519,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11172,"TRANSGRIDV5_20180116135943","2017-02-18T22:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-34.856960000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11202,"TRANSGRIDV5_20180116135943","2017-02-18T16:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-27.714729999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11232,"TRANSGRIDV5_20180116135943","2017-02-18T16:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-13.82592,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11299,"TRANSGRIDV5_20180116135943","2017-02-18T21:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.38045,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11329,"TRANSGRIDV5_20180116135943","2017-02-18T19:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.314589999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11355,"TRANSGRIDV5_20180116135943","2017-02-18T13:30:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-68.220089999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11385,"TRANSGRIDV5_20180116135943","2017-02-18T15:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-47.351909999999997,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11456,"TRANSGRIDV5_20180116135943","2017-02-19T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-29.207889999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11482,"TRANSGRIDV5_20180116135943","2017-02-19T22:05:00","SVML_ROC_80","S-NIL","2016-08-23",1,-19.233750000000001,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11512,"TRANSGRIDV5_20180116135943","2017-02-19T00:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-42.06962,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11583,"TRANSGRIDV5_20180116135943","2017-02-19T06:20:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-18.67192,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11609,"TRANSGRIDV5_20180116135943","2017-02-19T07:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-11.84525,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11639,"TRANSGRIDV5_20180116135943","2017-02-19T16:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-39.050350000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[11706,"TRANSGRIDV5_20180116135943","2017-02-20T02:10:00","V::N_HWSM_S1","V-HWSM","2016-11-28",1,-23.787710000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[11736,"TRANSGRIDV5_20180116135943","2017-02-20T02:55:00","V::N_HWSM_SD","V-HWSM","2016-11-28",1,-24.399149999999999,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[11766,"TRANSGRIDV5_20180116135943","2017-02-22T19:20:00","#OAKLAND1_E","#OAKLAND1_E","2017-02-22",3,-1110.9712199999999,"VTGT3A.ENERGY * 1 <= 36 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[11792,"TRANSGRIDV5_20180116135943","2017-02-22T12:30:00","#OAKLAND1_E","#OAKLAND1_E","2017-02-22",3,-1089.9147399999999,"VTGT3A.ENERGY * 1 <= 36 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[11863,"TRANSGRIDV5_20180116135943","2017-02-22T15:55:00","#WATERLWF_E","#WATERLWF_E","2017-02-22",1,-183.76580000000001,"SWLE.ENERGY * 1 <= 99 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[11889,"TRANSGRIDV5_20180116135943","2017-02-22T17:10:00","#WATERLWF_E","#WATERLWF_E","2017-02-22",1,-134.19307000000001,"SWLE.ENERGY * 1 <= 99 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[11919,"TRANSGRIDV5_20180116135943","2017-02-22T22:55:00","#WATERLWF_E","#WATERLWF_E","2017-02-22",1,-127.70807000000001,"SWLE.ENERGY * 1 <= 99 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[11990,"TRANSGRIDV5_20180116135943","2017-02-22T02:15:00","V::N_NIL_V1","V-NIL","2016-11-24",1,-36.015630000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12016,"TRANSGRIDV5_20180116135943","2017-02-22T00:55:00","V::N_NIL_V1","V-NIL","2016-11-24",1,-20.703669999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12046,"TRANSGRIDV5_20180116135943","2017-02-23T05:15:00","#R015174_006_RAMP_F","#R015174_RAMP","2017-02-23",1,-63.010829999999999,"Hard Ramping constraint for constraint V::N_SMF2_S1, Effective Date: 10/02/2017, Version: 1","OUTAGE","RAMP","South Morang F2 500/330kV txfmr","REGULATED","10","Ramping Constraint","PLANNED",0]
[12117,"TRANSGRIDV5_20180116135943","2017-02-24T04:00:00","V::N_SMF2_S1","V-SMTXF2_P","2017-02-10",1,-14.25193,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[12143,"TRANSGRIDV5_20180116135943","2017-02-25T03:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-12.8528,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12173,"TRANSGRIDV5_20180116135943","2017-02-25T13:00:00","V::N_NIL_V1","V-NIL","2016-11-24",1,-14.28257,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12240,"TRANSGRIDV5_20180116135943","2017-02-25T11:50:00","V>>V_SMTXF2_6","V-SMTXF2_P","2016-09-19",1,-26.63006,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[12254,"TRANSGRIDV5_20180116135943","2017-02-25T10:55:00","V>>V_SMTXF2_6","V-SMTXF2_P","2016-09-19",1,-21.97738,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[12299,"TRANSGRIDV5_20180116135943","2017-02-26T17:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-30.567209999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12325,"TRANSGRIDV5_20180116135943","2017-02-26T23:00:00","V::N_SMF2_S1","V-SMTXF2_R","2017-02-10",1,-25.301780000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[12396,"TRANSGRIDV5_20180116135943","2017-02-26T04:20:00","V::N_X_HWSM_SMF2_S1","V-X_HWSM_SMF2_STAB","2017-02-22",1,-12.26656,"Out= Hazelwood-South Morang 500kV line & South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[12422,"TRANSGRIDV5_20180116135943","2017-02-27T12:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-60.282699999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12452,"TRANSGRIDV5_20180116135943","2017-02-27T16:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-31.007860000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12523,"TRANSGRIDV5_20180116135943","2017-02-28T14:25:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-110.43651,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12549,"TRANSGRIDV5_20180116135943","2017-02-28T11:50:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-25.98366,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12579,"TRANSGRIDV5_20180116135943","2017-02-28T18:05:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-17.919170000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12650,"TRANSGRIDV5_20180116135943","2017-02-28T21:25:00","VSML_220","V-NIL","2012-07-04",1,-18.660789999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12676,"TRANSGRIDV5_20180116135943","2017-03-01T08:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-40.871589999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12706,"TRANSGRIDV5_20180116135943","2017-03-01T01:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-50.673690000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12773,"TRANSGRIDV5_20180116135943","2017-03-01T03:45:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-12.07527,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12803,"TRANSGRIDV5_20180116135943","2017-03-01T17:00:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-166.0805,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12833,"TRANSGRIDV5_20180116135943","2017-03-01T12:15:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-96.441509999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12859,"TRANSGRIDV5_20180116135943","2017-03-01T03:40:00","VSML_220","V-NIL","2012-07-04",1,-11.3786,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12930,"TRANSGRIDV5_20180116135943","2017-03-02T05:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.245629999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12960,"TRANSGRIDV5_20180116135943","2017-03-02T04:50:00","V:SS_820_HY_TEST","I-VSS_820_TEST","2016-07-28",1,-15.66602,"VIC to SA on Heywood and Murraylink combined upper transfer limit of 820 MW, limit for testing of Heywood interconnection upgrade.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[12986,"TRANSGRIDV5_20180116135943","2017-03-02T13:10:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-76.293049999999994,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13057,"TRANSGRIDV5_20180116135943","2017-03-03T23:40:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1052.28,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13083,"TRANSGRIDV5_20180116135943","2017-03-03T17:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-111.68913999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13113,"TRANSGRIDV5_20180116135943","2017-03-03T04:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-10.66567,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13184,"TRANSGRIDV5_20180116135943","2017-03-04T20:20:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1087.3599999999999,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13210,"TRANSGRIDV5_20180116135943","2017-03-04T22:20:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1063.98,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13240,"TRANSGRIDV5_20180116135943","2017-03-04T05:10:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1047.53,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13307,"TRANSGRIDV5_20180116135943","2017-03-04T02:00:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1019.68,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13337,"TRANSGRIDV5_20180116135943","2017-03-05T18:00:00","#NBHWF1_E","#NBHWF1_E","2017-03-03",2,-1072.75,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13367,"TRANSGRIDV5_20180116135943","2017-03-05T17:40:00","#NYNGAN1_E","#NYNGAN1_E","2017-03-05",1,-1087.73,"NWL82N.ENERGY * 1 <= 20 (Wt = 360)","OUTAGE","OTHER","Nyngan Solar Farm","REGULATED","99","Non Inclusion",null,0]
[13393,"TRANSGRIDV5_20180116135943","2017-03-05T15:40:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-23.173030000000001,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13464,"TRANSGRIDV5_20180116135943","2017-03-05T08:25:00","VSML_220","V-NIL","2012-07-04",1,-52.407690000000002,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13494,"TRANSGRIDV5_20180116135943","2017-03-06T07:30:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1100.42,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13520,"TRANSGRIDV5_20180116135943","2017-03-06T08:25:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1072.3499999999999,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13591,"TRANSGRIDV5_20180116135943","2017-03-06T22:35:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1024.97,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13617,"TRANSGRIDV5_20180116135943","2017-03-06T07:45:00","#NYNGAN1_E","#NYNGAN1_E","2017-03-05",1,-1082.0899999999999,"NWL82N.ENERGY * 1 <= 20 (Wt = 360)","OUTAGE","OTHER","Nyngan Solar Farm","REGULATED","99","Non Inclusion",null,0]
[13647,"TRANSGRIDV5_20180116135943","2017-03-06T05:10:00","#R015217_005_RAMP_F","#R015217_RAMP","2017-03-05",1,-81.863140000000001,"Hard Ramping constraint for constraint V::N_X_MLSM_EMTT_V2, Effective Date: 10/01/2017, Version: 1","OUTAGE","RAMP","one Moorabool to Sydenham to South Morang 500kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[13691,"TRANSGRIDV5_20180116135943","2017-03-06T06:00:00","V::N_X_MLSM_EMTT_V2","V-X_MLSM_EMTT_KTS_R","2017-01-10",1,-36.077779999999997,"Out = one Moorabool to Sydenham to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Moorabool Sydenham 2 500kV LINE; S Morang Sydenham 2 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[13743,"TRANSGRIDV5_20180116135943","2017-03-07T20:35:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1067.8800000000001,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13773,"TRANSGRIDV5_20180116135943","2017-03-07T21:20:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1044.3699999999999,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13799,"TRANSGRIDV5_20180116135943","2017-03-07T21:55:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1033.48,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[13870,"TRANSGRIDV5_20180116135943","2017-03-07T10:20:00","#PPCCGT_E","#PPCCGT_E","2017-03-07",1,-1125.04,"SPPT.ENERGY * 1 <= 170 (Wt = 35)","OUTAGE","OTHER","Pelican Point CCGT","REGULATED","99","Non Inclusion",null,0]
[13900,"TRANSGRIDV5_20180116135943","2017-03-07T04:10:00","#R015223_001_RAMP_V","#R015223_RAMP","2017-03-06",1,-104.99797,"Soft Ramping constraint for constraint V_MACARTHUR_ZERO, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Macarthur Wind Farm","REGULATED","10","Ramping Constraint","PLANNED",0]
[13926,"TRANSGRIDV5_20180116135943","2017-03-07T19:15:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.206720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[13997,"TRANSGRIDV5_20180116135943","2017-03-07T17:30:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-20.625139999999998,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14027,"TRANSGRIDV5_20180116135943","2017-03-07T04:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.911390000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14053,"TRANSGRIDV5_20180116135943","2017-03-08T05:10:00","#NBHWF1_E","#NBHWF1_E","2017-03-06",1,-1059.99,"SBEL1A.ENERGY * 1 <= 34 (Wt = 360)","OUTAGE","OTHER","North Brown Hill Windfarm","REGULATED","99","Non Inclusion",null,0]
[14124,"TRANSGRIDV5_20180116135943","2017-03-08T15:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-52.246000000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14150,"TRANSGRIDV5_20180116135943","2017-03-08T14:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-33.584470000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14180,"TRANSGRIDV5_20180116135943","2017-03-08T16:15:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-11.33881,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14210,"TRANSGRIDV5_20180116135943","2017-03-08T21:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-25.3169,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14277,"TRANSGRIDV5_20180116135943","2017-03-09T06:10:00","#R015241_001_RAMP_V","#R015241_RAMP","2017-03-08",1,-1065.96,"Soft Ramping constraint for constraint N_MOREESF1_ZERO, Effective Date: 18/12/2015, Version: 1","OUTAGE","RAMP","Armidale 5 330kV BUS","REGULATED","10","Ramping Constraint","PLANNED",0]
[14307,"TRANSGRIDV5_20180116135943","2017-03-09T08:25:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,17.66,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale 5 330kV BUS","REGULATED","INCLUDED","","PLANNED",1]
[14337,"TRANSGRIDV5_20180116135943","2017-03-09T14:25:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,11.67947,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale 5 330kV BUS","REGULATED","INCLUDED","","PLANNED",1]
[14404,"TRANSGRIDV5_20180116135943","2017-03-09T17:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-33.73442,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14434,"TRANSGRIDV5_20180116135943","2017-03-09T06:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-24.45045,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[14460,"TRANSGRIDV5_20180116135943","2017-03-09T07:00:00","N_MOREESF1_ZERO","N-MOREESF1_ZERO","2015-12-18",1,-1105.96,"Moree Solar Farm upper limit of 0 MW","OUTAGE","OTHER","Armidale 5 330kV BUS","REGULATED","11","Transmission connection agreements where a lower service standard has been negotiated giving the TNSP the right to disrupt service under certain network conditions where the constraint only affects the parties subject to the agreement.","PLANNED",0,"Refer to attached explanatory note in evidence files."]
[14531,"TRANSGRIDV5_20180116135943","2017-03-10T11:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-39.161279999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14561,"TRANSGRIDV5_20180116135943","2017-03-10T11:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-29.840599999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14587,"TRANSGRIDV5_20180116135943","2017-03-10T11:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-27.53932,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14658,"TRANSGRIDV5_20180116135943","2017-03-11T17:40:00","#HDWF2_E","#HDWF2_E","2017-02-21",1,-222.93768,"SHDW2H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm 2","REGULATED","99","Non Inclusion",null,0]
[14684,"TRANSGRIDV5_20180116135943","2017-03-11T07:15:00","V::N_HWCB_S2","V-HWCB4","2016-12-20",1,-16.052859999999999,"Out = Hazelwood to Cranbourne No.4 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Cranbourne Hazelwood 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[14714,"TRANSGRIDV5_20180116135943","2017-03-11T00:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.695499999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14744,"TRANSGRIDV5_20180116135943","2017-03-12T17:15:00","#HDWF2_E","#HDWF2_E","2017-02-21",1,-234.21136999999999,"SHDW2H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm 2","REGULATED","99","Non Inclusion",null,0]
[14811,"TRANSGRIDV5_20180116135943","2017-03-12T01:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-24.381979999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14841,"TRANSGRIDV5_20180116135943","2017-03-12T03:50:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-14.09986,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14871,"TRANSGRIDV5_20180116135943","2017-03-12T21:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.29515,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14938,"TRANSGRIDV5_20180116135943","2017-03-13T08:45:00","V::N_KTSY_V2","V-KTSY_R","2016-11-08",1,-36.793950000000002,"Out = Keilor to Sydenham 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Keilor Sydenham 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[14968,"TRANSGRIDV5_20180116135943","2017-03-13T23:00:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-29.506810000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[14994,"TRANSGRIDV5_20180116135943","2017-03-13T02:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-16.152190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15065,"TRANSGRIDV5_20180116135943","2017-03-14T01:10:00","V::N_NIL_SD","V-NIL","2016-07-25",1,-49.812930000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15095,"TRANSGRIDV5_20180116135943","2017-03-14T01:30:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-27.385459999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15121,"TRANSGRIDV5_20180116135943","2017-03-15T09:25:00","#R015281_003_RAMP_V","#R015281_RAMP","2017-03-15",1,-23.494450000000001,"Soft Ramping constraint for constraint S>LFTI_PPPW_LFTX5, Effective Date: 04/04/2016, Version: 1","OUTAGE","RAMP","Torrens Island-Lefevre 275kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[15170,"TRANSGRIDV5_20180116135943","2017-03-15T21:00:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-29.540600000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15221,"TRANSGRIDV5_20180116135943","2017-03-15T04:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-55.482469999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15247,"TRANSGRIDV5_20180116135943","2017-03-15T06:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.38538,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15277,"TRANSGRIDV5_20180116135943","2017-03-16T17:10:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-11.21519,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[15344,"TRANSGRIDV5_20180116135943","2017-03-16T17:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-135.52334999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15374,"TRANSGRIDV5_20180116135943","2017-03-16T16:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-46.000100000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15404,"TRANSGRIDV5_20180116135943","2017-03-16T14:00:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-18.065429999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15471,"TRANSGRIDV5_20180116135943","2017-03-17T21:35:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-17.51651,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15501,"TRANSGRIDV5_20180116135943","2017-03-17T01:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-14.08644,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15527,"TRANSGRIDV5_20180116135943","2017-03-17T03:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-11.253539999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15598,"TRANSGRIDV5_20180116135943","2017-03-18T16:05:00","V^SML_NSWRB_2","V-NIL","2016-07-07",1,-98.539990000000003,"Out = NSW Murraylink runback scheme, avoid voltage collapse for loss of Darlington Pt to Buronga (X5) 220kV line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15628,"TRANSGRIDV5_20180116135943","2017-03-18T08:10:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-43.948500000000003,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[15654,"TRANSGRIDV5_20180116135943","2017-03-18T07:30:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-32.077750000000002,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[15684,"TRANSGRIDV5_20180116135943","2017-03-18T06:10:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-25.593489999999999,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[15755,"TRANSGRIDV5_20180116135943","2017-03-18T14:40:00","VSML_220","V-NIL","2012-07-04",1,-107.60951,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15781,"TRANSGRIDV5_20180116135943","2017-03-18T11:55:00","VSML_220","V-NIL","2012-07-04",1,-30.714400000000001,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15811,"TRANSGRIDV5_20180116135943","2017-03-19T05:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-65.916020000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[15878,"TRANSGRIDV5_20180116135943","2017-03-19T08:15:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-32.297750000000001,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[15908,"TRANSGRIDV5_20180116135943","2017-03-19T10:45:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2016-12-07",1,-14.27055,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[15938,"TRANSGRIDV5_20180116135943","2017-03-19T02:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-16.53444,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16005,"TRANSGRIDV5_20180116135943","2017-03-20T10:05:00","#VIC1_E_20170319","#VIC1_E_20170319","2017-03-20",3,-214.96,"Multiple VIC1 LHS <= 210 (Wt = 35)","OUTAGE","OTHER","Mortlake GT","REGULATED","99","Non Inclusion",null,0]
[16035,"TRANSGRIDV5_20180116135943","2017-03-20T12:35:00","#VIC1_E_20170319","#VIC1_E_20170319","2017-03-20",3,-214.96,"Multiple VIC1 LHS <= 210 (Wt = 35)","OUTAGE","OTHER","Mortlake GT","REGULATED","99","Non Inclusion",null,0]
[16061,"TRANSGRIDV5_20180116135943","2017-03-20T13:30:00","SVML_ROC_80","S-NIL","2016-08-23",1,-245.17053000000001,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16132,"TRANSGRIDV5_20180116135943","2017-03-21T10:45:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,83.498000000000005,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16162,"TRANSGRIDV5_20180116135943","2017-03-21T13:35:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,61.403390000000002,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16188,"TRANSGRIDV5_20180116135943","2017-03-21T08:30:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,28.8,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16218,"TRANSGRIDV5_20180116135943","2017-03-21T05:35:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,17.97,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16289,"TRANSGRIDV5_20180116135943","2017-03-21T22:40:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-20.281659999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16315,"TRANSGRIDV5_20180116135943","2017-03-22T04:50:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2017-03-22",1,86.034580000000005,"NSW1-QLD1 >= MIN(-460, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16345,"TRANSGRIDV5_20180116135943","2017-03-22T14:40:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,58.76735,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16412,"TRANSGRIDV5_20180116135943","2017-03-22T13:10:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,17.989999999999998,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16442,"TRANSGRIDV5_20180116135943","2017-03-22T05:55:00","F_Q++MUTW_L60","F-N-MUTW_88","2013-08-21",1,17.97,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16472,"TRANSGRIDV5_20180116135943","2017-03-22T12:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-92.720879999999994,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE; N_W_B 6023 132kV CB","REGULATED","99","Non Inclusion",null,0]
[16539,"TRANSGRIDV5_20180116135943","2017-03-22T01:05:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-30.397500000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16569,"TRANSGRIDV5_20180116135943","2017-03-22T03:25:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-23.055510000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16599,"TRANSGRIDV5_20180116135943","2017-03-22T12:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-122.64919,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16649,"TRANSGRIDV5_20180116135943","2017-03-22T10:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL_3-4","2016-06-21",1,-15.93998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16695,"TRANSGRIDV5_20180116135943","2017-03-22T08:25:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-14.09817,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE; N_W_B 6023 132kV CB","REGULATED","99","Non Inclusion",null,0]
[16721,"TRANSGRIDV5_20180116135943","2017-03-23T10:55:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,37.153219999999997,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16751,"TRANSGRIDV5_20180116135943","2017-03-23T06:05:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,43.30491,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16822,"TRANSGRIDV5_20180116135943","2017-03-24T04:50:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2017-03-24",3,120.35187999999999,"NSW1-QLD1 >= MIN(-507, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[16848,"TRANSGRIDV5_20180116135943","2017-03-24T08:35:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,50.452179999999998,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16878,"TRANSGRIDV5_20180116135943","2017-03-24T07:35:00","F_Q++MUTW_L5","F-N-MUTW_88","2013-08-21",1,33.79448,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16945,"TRANSGRIDV5_20180116135943","2017-03-24T10:20:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,38.567659999999997,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[16975,"TRANSGRIDV5_20180116135943","2017-03-24T08:00:00","F_Q++MUTW_L6","F-N-MUTW_88","2013-08-21",1,17.989999999999998,"Out = Muswellbrook to Tamworth (88) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Muswlbk330 Tamworth 88 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[17005,"TRANSGRIDV5_20180116135943","2017-03-24T20:40:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-47.775669999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17072,"TRANSGRIDV5_20180116135943","2017-03-24T11:30:00","VSML_220","V-NIL","2012-07-04",1,-30.396239999999999,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17102,"TRANSGRIDV5_20180116135943","2017-03-25T11:55:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-130.60837000000001,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 1 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 67 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[17132,"TRANSGRIDV5_20180116135943","2017-03-25T11:25:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-66.235560000000007,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 1 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 67 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[17199,"TRANSGRIDV5_20180116135943","2017-03-25T23:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-64.6023,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17229,"TRANSGRIDV5_20180116135943","2017-03-25T08:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-41.99783,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17255,"TRANSGRIDV5_20180116135943","2017-03-25T02:20:00","V::N_HWSM_SD","V-HWSM","2016-11-28",1,-21.627890000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[17285,"TRANSGRIDV5_20180116135943","2017-03-26T23:25:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-161.44755000000001,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17356,"TRANSGRIDV5_20180116135943","2017-03-26T10:15:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-52.058689999999999,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 1 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 67 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[17382,"TRANSGRIDV5_20180116135943","2017-03-26T02:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-46.337949999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17412,"TRANSGRIDV5_20180116135943","2017-03-26T04:55:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-13.353020000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17479,"TRANSGRIDV5_20180116135943","2017-03-27T07:20:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-230.99,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17509,"TRANSGRIDV5_20180116135943","2017-03-27T17:10:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-214.91301000000001,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17539,"TRANSGRIDV5_20180116135943","2017-03-27T14:25:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-201.49411000000001,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17606,"TRANSGRIDV5_20180116135943","2017-03-27T00:25:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-140.00496999999999,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17636,"TRANSGRIDV5_20180116135943","2017-03-27T03:40:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-133.41995,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[17666,"TRANSGRIDV5_20180116135943","2017-03-27T10:25:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-63.714550000000003,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 1 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 67 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[17692,"TRANSGRIDV5_20180116135943","2017-03-27T12:55:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-10.936360000000001,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 1 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 67 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[17763,"TRANSGRIDV5_20180116135943","2017-03-27T02:45:00","V::N_NIL_V2","V-NIL","2016-11-24",1,-12.355079999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[17789,"TRANSGRIDV5_20180116135943","2017-03-28T21:35:00","#MSTUART2_D_E","#MSTUART2_DE","2017-03-28",13,13930.06342,"QMSP2.ENERGY * 1 = 50 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[17819,"TRANSGRIDV5_20180116135943","2017-03-28T16:15:00","#MSTUART2_D_E","#MSTUART2_DE","2017-03-28",13,13900.20932,"QMSP2.ENERGY * 1 = 50 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[17890,"TRANSGRIDV5_20180116135943","2017-03-28T17:20:00","#MSTUART3_D_E","#MSTUART3_DE","2017-03-28",10,13901.06329,"QMSP3M.ENERGY * 1 = 50 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[17916,"TRANSGRIDV5_20180116135943","2017-03-28T17:05:00","#MSTUART3_D_E","#MSTUART3_DE","2017-03-28",10,13898.082619999999,"QMSP3M.ENERGY * 1 = 50 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[17946,"TRANSGRIDV5_20180116135943","2017-03-28T21:25:00","#MSTUART3_D_E","#MSTUART3_DE","2017-03-28",10,13701.00316,"QMSP3M.ENERGY * 1 = 50 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[18017,"TRANSGRIDV5_20180116135943","2017-03-28T21:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-16.803249999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18043,"TRANSGRIDV5_20180116135943","2017-03-28T17:10:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-11.758620000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18086,"TRANSGRIDV5_20180116135943","2017-03-29T14:15:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-241.1703,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[18139,"TRANSGRIDV5_20180116135943","2017-03-29T12:10:00","#MACARTH1_E","#MACARTH1_E","2017-03-26",1,-195.38003,"VTRT1M.ENERGY * 1 <= 210 (Wt = 360)","OUTAGE","OTHER","Macarthur WF","REGULATED","99","Non Inclusion",null,0]
[18169,"TRANSGRIDV5_20180116135943","2017-03-29T01:40:00","#MSTUART2_D_E","#MSTUART2_DE","2017-03-29",2,13936.21866,"QMSP2.ENERGY * 1 = 30 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[18199,"TRANSGRIDV5_20180116135943","2017-03-29T00:15:00","#MSTUART3_D_E","#MSTUART3_DE","2017-03-29",1,13934.013720000001,"QMSP3M.ENERGY * 1 = 45 (Wt = 755)","OUTAGE","OTHER","Mt Stuart GT ","REGULATED","99","Non Inclusion",null,0]
[18225,"TRANSGRIDV5_20180116135943","2017-03-29T06:00:00","#R015374_001_RAMP_F","#R015374_RAMP","2017-03-28",1,-78.786379999999994,"Hard Ramping constraint for constraint VS_050, Effective Date: 08/01/2014, Version: 1","OUTAGE","RAMP","Heywood 2 500kV BUS","REGULATED","10","Ramping Constraint","PLANNED",0]
[18296,"TRANSGRIDV5_20180116135943","2017-03-29T21:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-181.72074000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18322,"TRANSGRIDV5_20180116135943","2017-03-29T15:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-150.44779,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18352,"TRANSGRIDV5_20180116135943","2017-03-29T11:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-116.56524,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18423,"TRANSGRIDV5_20180116135943","2017-03-30T18:40:00","N^N-X_96H_LS_SVC","N-X_96H_LS_SVC","2016-09-28",1,-31.962,"Out= Coffs Harbour to Koolkhan (96H) 132kV line and Lismore SVC O/S or in reactive power control mode, avoid Voltage collapse on Koolkhan to Lismore (967) trip; TG formulation only","OUTAGE","OTHER","Lismore 1 132kV SVC","REGULATED","1","Force Majeure","UNPLANNED",0,"Short notice outage of Lismore SVC necesitated by flooding in the area, resulting from Cyclone Debbie.  Refer to evidence for information supporting a force majeure exclusion."]
[18449,"TRANSGRIDV5_20180116135943","2017-03-30T09:20:00","N>N-CHKK_TE_1","N-CHKK_96H","2013-08-21",1,-10.95459,"Out= Coffs Harbour to Koolkhan (96H), avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","CoffsH132 Koolkhan 96H 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[18479,"TRANSGRIDV5_20180116135943","2017-03-30T04:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-118.48793999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18550,"TRANSGRIDV5_20180116135943","2017-03-31T11:05:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-88.369489999999999,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 2 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 68 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[18576,"TRANSGRIDV5_20180116135943","2017-03-31T10:30:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-54.464979999999997,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 2 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 68 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[18606,"TRANSGRIDV5_20180116135943","2017-03-31T13:20:00","N^^V_DDMSX5_1","I-X_DDMSX5","2017-01-13",1,-13.69084,"Out = Dederang - Murray (67 or 68) and Darlington Pt - Buronga (X5) lines, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Murray 2 330kV LINE; Drlngtn Pt Balranald X5/1 220kV LINE","REGULATED","INCLUDED","","PLANNED",0.5,"Line 68 outage belongs to Ausnet, refer to evidence.  Line X5 outage is TransGrid's.  Penalties apportioned 50/50 between TransGrid and Ausnet."]
[18673,"TRANSGRIDV5_20180116135943","2017-03-31T06:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.322290000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[18703,"TRANSGRIDV5_20180116135943","2017-03-31T06:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.753769999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[18733,"TRANSGRIDV5_20180116135943","2017-04-01T08:30:00","F_Q++LDTW_L6","F-N-LDTW_84","2013-08-21",1,32.221600000000002,"Out = Liddell to Tamworth (84) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[18759,"TRANSGRIDV5_20180116135943","2017-04-01T08:05:00","F_Q++LDTW_L60","F-N-LDTW_84","2013-08-21",1,48.62,"Out = Liddell to Tamworth (84) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[18830,"TRANSGRIDV5_20180116135943","2017-04-02T00:35:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-39.461289999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[18860,"TRANSGRIDV5_20180116135943","2017-04-02T08:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.050649999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[18886,"TRANSGRIDV5_20180116135943","2017-04-02T03:20:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.72589,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[18957,"TRANSGRIDV5_20180116135943","2017-04-03T12:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-13.99666,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[18983,"TRANSGRIDV5_20180116135943","2017-04-03T10:35:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.583320000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19013,"TRANSGRIDV5_20180116135943","2017-04-03T02:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.206670000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19084,"TRANSGRIDV5_20180116135943","2017-04-04T08:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-26.235759999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19110,"TRANSGRIDV5_20180116135943","2017-04-04T06:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.00263,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19140,"TRANSGRIDV5_20180116135943","2017-04-04T10:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.08061,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19207,"TRANSGRIDV5_20180116135943","2017-04-04T03:55:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-20.539629999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19237,"TRANSGRIDV5_20180116135943","2017-04-05T08:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-29.3095,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19267,"TRANSGRIDV5_20180116135943","2017-04-05T23:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-46.241759999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19293,"TRANSGRIDV5_20180116135943","2017-04-06T01:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-74.732110000000006,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19364,"TRANSGRIDV5_20180116135943","2017-04-06T22:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-24.72146,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19394,"TRANSGRIDV5_20180116135943","2017-04-06T01:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-66.957830000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19420,"TRANSGRIDV5_20180116135943","2017-04-06T03:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-42.33623,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19491,"TRANSGRIDV5_20180116135943","2017-04-07T00:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-50.133249999999997,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19517,"TRANSGRIDV5_20180116135943","2017-04-07T01:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.54462,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19565,"TRANSGRIDV5_20180116135943","2017-04-07T09:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.982659999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19576,"TRANSGRIDV5_20180116135943","2017-04-08T11:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.440550000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19643,"TRANSGRIDV5_20180116135943","2017-04-08T03:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.21373,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19673,"TRANSGRIDV5_20180116135943","2017-04-09T13:35:00","S>NWCB6024+25_TX3","S-NWBCB6024+6025","2015-07-27",1,-186.61846,"Out= North West Bed 132kV CBs 6024 and 6025(this offloads NWB TX2), avoid O/L North West Bend #3 132/66kV TX on trip of North West Bend- Monash #1 132kV line (this splits NWB 132kV bus), Feedback","OUTAGE","OTHER","N_W_B 6024 132kV CB; N_W_B 6025 132kV CB; N_W_Bend 2 132/66/11kV XFMR","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[19699,"TRANSGRIDV5_20180116135943","2017-04-09T12:05:00","S>NWCB6024+25_TX3","S-NWBCB6024+6025","2015-07-27",1,-99.442449999999994,"Out= North West Bed 132kV CBs 6024 and 6025(this offloads NWB TX2), avoid O/L North West Bend #3 132/66kV TX on trip of North West Bend- Monash #1 132kV line (this splits NWB 132kV bus), Feedback","OUTAGE","OTHER","N_W_B 6024 132kV CB; N_W_B 6025 132kV CB; N_W_Bend 2 132/66/11kV XFMR","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[19770,"TRANSGRIDV5_20180116135943","2017-04-09T16:25:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2016-06-21",1,-44.064570000000003,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19800,"TRANSGRIDV5_20180116135943","2017-04-09T22:40:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2016-06-21",1,-24.71292,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[19826,"TRANSGRIDV5_20180116135943","2017-04-10T09:05:00","#R015456_003_RAMP_F","#R015456_RAMP","2017-04-09",1,-143.92232000000001,"Hard Ramping constraint for constraint T>T_BWLF_110_4, Effective Date: 16/06/2016, Version: 1","OUTAGE","RAMP","Bridgewater to Lindisfarne or Bridgewater to Waddamana 110 kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[19897,"TRANSGRIDV5_20180116135943","2017-04-11T05:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-47.526299999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19927,"TRANSGRIDV5_20180116135943","2017-04-11T02:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.938409999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[19953,"TRANSGRIDV5_20180116135943","2017-04-11T08:40:00","Q:N_TW330_CB5102_OSC","N-TW_330_CB5102","2013-08-21",1,-86.05068,"Out= Tamworth 330kV CB 5102, Qld to NSW Oscillatory stability limit","OUTAGE","OTHER","Tamworth 5102 330kV CB","REGULATED","INCLUDED","","PLANNED",1]
[20024,"TRANSGRIDV5_20180116135943","2017-04-12T10:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.60948,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[20050,"TRANSGRIDV5_20180116135943","2017-04-12T08:05:00","Q:N_TW330_CB5102_OSC","N-TW_330_CB5102","2013-08-21",1,-11.69411,"Out= Tamworth 330kV CB 5102, Qld to NSW Oscillatory stability limit","OUTAGE","OTHER","Tamworth 5102 330kV CB","REGULATED","INCLUDED","","PLANNED",1]
[20080,"TRANSGRIDV5_20180116135943","2017-04-14T23:30:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-68.313779999999994,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20110,"TRANSGRIDV5_20180116135943","2017-04-15T00:45:00","N^^V_NIL_1","V-NIL","2016-11-24",1,-18.7241,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20177,"TRANSGRIDV5_20180116135943","2017-04-19T20:10:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-19",1,-1095.00299,"VTGT3A.ENERGY * 1 <= 23 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20207,"TRANSGRIDV5_20180116135943","2017-04-20T13:50:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-20",1,-1141.65301,"VTGT3A.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20237,"TRANSGRIDV5_20180116135943","2017-04-20T13:35:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-20",1,-1116.1022399999999,"VTGT3A.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20304,"TRANSGRIDV5_20180116135943","2017-04-20T08:05:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-20",1,-1108.8235099999999,"VTGT3A.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20334,"TRANSGRIDV5_20180116135943","2017-04-20T06:55:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-20",1,-1103.8108299999999,"VTGT3A.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20360,"TRANSGRIDV5_20180116135943","2017-04-20T01:30:00","#OAKLAND1_E","#OAKLAND1_E","2017-04-20",1,-1083.2043699999999,"VTGT3A.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Oaklands Hill WF","REGULATED","99","Non Inclusion",null,0]
[20431,"TRANSGRIDV5_20180116135943","2017-04-20T20:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-10.457700000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20461,"TRANSGRIDV5_20180116135943","2017-04-21T08:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-60.782989999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20487,"TRANSGRIDV5_20180116135943","2017-04-21T16:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-45.408909999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20558,"TRANSGRIDV5_20180116135943","2017-04-21T01:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.014569999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20584,"TRANSGRIDV5_20180116135943","2017-04-21T09:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.542210000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20614,"TRANSGRIDV5_20180116135943","2017-04-21T03:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-26.959129999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[20644,"TRANSGRIDV5_20180116135943","2017-04-22T13:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-61.848849999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20711,"TRANSGRIDV5_20180116135943","2017-04-22T09:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.439769999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20741,"TRANSGRIDV5_20180116135943","2017-04-23T18:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.30965,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20771,"TRANSGRIDV5_20180116135943","2017-04-24T08:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.953510000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20838,"TRANSGRIDV5_20180116135943","2017-04-24T03:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-75.616780000000006,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20868,"TRANSGRIDV5_20180116135943","2017-04-24T03:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.15465,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[20894,"TRANSGRIDV5_20180116135943","2017-04-25T03:55:00","#AGLHAL_P_E","#AGLHAL_PE","2017-04-25",3,-77.817130000000006,"SHPS1.ENERGY * 1 <= 205 (Wt = 50)","OUTAGE","OTHER","Hallet GT","REGULATED","99","Non Inclusion",null,0]
[20965,"TRANSGRIDV5_20180116135943","2017-04-25T18:55:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1116.8683000000001,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[20995,"TRANSGRIDV5_20180116135943","2017-04-25T21:10:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1087.5719999999999,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[21044,"TRANSGRIDV5_20180116135943","2017-04-25T23:40:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1060.0011199999999,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[21091,"TRANSGRIDV5_20180116135943","2017-04-26T09:25:00","#OSB-AG_C_E","#OSB-AG_C","2017-04-26",1,-1102.04828,"SNBN1.ENERGY * 1 <= 139 (Wt = 48)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[21121,"TRANSGRIDV5_20180116135943","2017-04-26T12:00:00","#OSB-AG_C_E","#OSB-AG_C","2017-04-26",1,-32.80256,"SNBN1.ENERGY * 1 <= 139 (Wt = 48)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[21147,"TRANSGRIDV5_20180116135943","2017-04-26T07:55:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1117.16211,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[21177,"TRANSGRIDV5_20180116135943","2017-04-26T11:30:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1094.9905200000001,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[21244,"TRANSGRIDV5_20180116135943","2017-04-26T04:45:00","#TORRB3_P_E","#TORRB3_PE","2017-04-25",1,-1030.8056899999999,"STSB3.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 3","REGULATED","99","Non Inclusion",null,0]
[21274,"TRANSGRIDV5_20180116135943","2017-04-26T19:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-60.507860000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21304,"TRANSGRIDV5_20180116135943","2017-04-26T04:55:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2017-04-10",1,-17.690919999999998,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21371,"TRANSGRIDV5_20180116135943","2017-04-27T16:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.610399999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21401,"TRANSGRIDV5_20180116135943","2017-04-27T12:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-35.76088,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21427,"TRANSGRIDV5_20180116135943","2017-04-27T16:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.264959999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21498,"TRANSGRIDV5_20180116135943","2017-04-28T08:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-41.419930000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21528,"TRANSGRIDV5_20180116135943","2017-04-28T11:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.9846,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21554,"TRANSGRIDV5_20180116135943","2017-04-28T13:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-23.075859999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21584,"TRANSGRIDV5_20180116135943","2017-04-28T03:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-77.952920000000006,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[21655,"TRANSGRIDV5_20180116135943","2017-05-02T20:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.845239999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21681,"TRANSGRIDV5_20180116135943","2017-05-03T08:10:00","F_Q++ARTW_L5","F-N-ARTW_85","2013-08-21",1,29.651769999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Armidale 85 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[21711,"TRANSGRIDV5_20180116135943","2017-05-03T14:45:00","F_Q++ARTW_L60","F-N-ARTW_85","2013-08-21",1,19.028479999999998,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 85 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[21778,"TRANSGRIDV5_20180116135943","2017-05-04T07:55:00","F_Q++ARTW_L5","F-N-ARTW_85","2013-08-21",1,10.416969999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Armidale 85 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[21808,"TRANSGRIDV5_20180116135943","2017-05-04T08:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.480719999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21838,"TRANSGRIDV5_20180116135943","2017-05-05T07:35:00","F_Q++ARTW_L5","F-N-ARTW_85","2013-08-21",1,17.84,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Armidale 85 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[21905,"TRANSGRIDV5_20180116135943","2017-05-05T18:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.988049999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[21935,"TRANSGRIDV5_20180116135943","2017-05-06T20:45:00","N^^V_MSUT_1","I-MSUT","2015-08-07",1,-22.802389999999999,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Murray Upr Tumut 65 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[21961,"TRANSGRIDV5_20180116135943","2017-05-06T04:35:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-22.14912,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22032,"TRANSGRIDV5_20180116135943","2017-05-07T00:50:00","N^^V_MSUT_1","I-MSUT","2015-08-07",1,-10.06246,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Murray Upr Tumut 65 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[22062,"TRANSGRIDV5_20180116135943","2017-05-08T21:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-45.310540000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22088,"TRANSGRIDV5_20180116135943","2017-05-08T17:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.318010000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22118,"TRANSGRIDV5_20180116135943","2017-05-08T12:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.339040000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22189,"TRANSGRIDV5_20180116135943","2017-05-09T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-52.7,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22215,"TRANSGRIDV5_20180116135943","2017-05-09T23:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.843389999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22245,"TRANSGRIDV5_20180116135943","2017-05-09T19:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-38.360930000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22312,"TRANSGRIDV5_20180116135943","2017-05-09T09:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-13.08109,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22342,"TRANSGRIDV5_20180116135943","2017-05-10T18:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-125.56622,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22372,"TRANSGRIDV5_20180116135943","2017-05-10T09:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-63.656230000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22439,"TRANSGRIDV5_20180116135943","2017-05-10T09:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-34.196260000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22469,"TRANSGRIDV5_20180116135943","2017-05-10T23:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-24.388380000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22507,"TRANSGRIDV5_20180116135943","2017-05-10T10:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.631030000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22565,"TRANSGRIDV5_20180116135943","2017-05-11T12:25:00","N^^V_DDWG","N-JNWG_RADIAL","2015-08-07",1,-125.45634,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Wagga Jinderra 62 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[22595,"TRANSGRIDV5_20180116135943","2017-05-11T15:15:00","N^^V_DDWG","N-JNWG_RADIAL","2015-08-07",1,-51.873710000000003,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Wagga Jinderra 62 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[22621,"TRANSGRIDV5_20180116135943","2017-05-11T14:05:00","N^^V_DDWG","N-JNWG_RADIAL","2015-08-07",1,-19.908770000000001,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Wagga Jinderra 62 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[22651,"TRANSGRIDV5_20180116135943","2017-05-11T22:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-50.630479999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22722,"TRANSGRIDV5_20180116135943","2017-05-11T21:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.945049999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22748,"TRANSGRIDV5_20180116135943","2017-05-11T10:10:00","V>>V-JNWG_RADIAL_1A","N-JNWG_RADIAL","2017-05-11",1,-242.02844999999999,"Outage = Jindera to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload one Murray to Dederang 330kV line for loss of the parallel 330kV line, 15 min line ratings; Feedback","OUTAGE","OTHER","Wagga Jinderra 62 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[22778,"TRANSGRIDV5_20180116135943","2017-05-11T09:50:00","V>>V-JNWG_RADIAL_1A","N-JNWG_RADIAL","2017-05-11",1,-84.650869999999998,"Outage = Jindera to Wagga 330kV line, limit Snowy to Vic interconnector to avoid overload one Murray to Dederang 330kV line for loss of the parallel 330kV line, 15 min line ratings; Feedback","OUTAGE","OTHER","Wagga Jinderra 62 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[22845,"TRANSGRIDV5_20180116135943","2017-05-12T05:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-52.68374,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22875,"TRANSGRIDV5_20180116135943","2017-05-12T04:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.923020000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22905,"TRANSGRIDV5_20180116135943","2017-05-12T21:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.810679999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[22972,"TRANSGRIDV5_20180116135943","2017-05-12T00:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.105530000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23002,"TRANSGRIDV5_20180116135943","2017-05-12T11:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.467370000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23032,"TRANSGRIDV5_20180116135943","2017-05-13T08:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-80.742840000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23099,"TRANSGRIDV5_20180116135943","2017-05-13T04:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.150910000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23129,"TRANSGRIDV5_20180116135943","2017-05-13T01:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.387459999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23155,"TRANSGRIDV5_20180116135943","2017-05-13T08:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.445639999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23185,"TRANSGRIDV5_20180116135943","2017-05-13T13:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.84301,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23256,"TRANSGRIDV5_20180116135943","2017-05-13T09:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.839659999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23282,"TRANSGRIDV5_20180116135943","2017-05-13T09:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.632389999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23312,"TRANSGRIDV5_20180116135943","2017-05-14T09:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-69.579909999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23379,"TRANSGRIDV5_20180116135943","2017-05-14T14:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-41.530239999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23409,"TRANSGRIDV5_20180116135943","2017-05-14T20:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.571820000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23439,"TRANSGRIDV5_20180116135943","2017-05-14T03:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.568060000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23506,"TRANSGRIDV5_20180116135943","2017-05-14T10:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.365659999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23536,"TRANSGRIDV5_20180116135943","2017-05-14T13:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-23.99165,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23566,"TRANSGRIDV5_20180116135943","2017-05-14T11:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-17.501339999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23592,"TRANSGRIDV5_20180116135943","2017-05-15T08:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-105.1694,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23663,"TRANSGRIDV5_20180116135943","2017-05-15T02:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.404020000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23689,"TRANSGRIDV5_20180116135943","2017-05-15T00:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.381929999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23719,"TRANSGRIDV5_20180116135943","2017-05-15T05:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-34.698799999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23790,"TRANSGRIDV5_20180116135943","2017-05-15T15:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.455390000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23816,"TRANSGRIDV5_20180116135943","2017-05-15T14:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.0411,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23846,"TRANSGRIDV5_20180116135943","2017-05-16T09:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-91.173249999999996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23917,"TRANSGRIDV5_20180116135943","2017-05-16T16:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.124770000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23920,"TRANSGRIDV5_20180116135943","2017-05-16T01:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.557670000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[23972,"TRANSGRIDV5_20180116135943","2017-05-16T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.167010000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24039,"TRANSGRIDV5_20180116135943","2017-05-17T13:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-73.594920000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24069,"TRANSGRIDV5_20180116135943","2017-05-17T09:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-48.742640000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24099,"TRANSGRIDV5_20180116135943","2017-05-17T23:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-36.43468,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24125,"TRANSGRIDV5_20180116135943","2017-05-17T19:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-31.301259999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24196,"TRANSGRIDV5_20180116135943","2017-05-18T00:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.861190000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24222,"TRANSGRIDV5_20180116135943","2017-05-18T00:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.85624,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24252,"TRANSGRIDV5_20180116135943","2017-05-18T21:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-19.779350000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24323,"TRANSGRIDV5_20180116135943","2017-05-19T17:00:00","#JLA02_E","#JLA02_E","2017-05-19",1,-107.52697999999999,"VJLGA2.ENERGY * 1 <= 20 (Wt = 360)","OUTAGE","OTHER","Jeeralang GT Unit 2","REGULATED","99","Non Inclusion",null,0]
[24349,"TRANSGRIDV5_20180116135943","2017-05-19T16:20:00","N>N-96H+96R_TE_1","N-X_96H_96R","2013-08-21",1,-10.12899,"Out= Coffs Harbour to Koolkhan (96H) and Glen Innes to Tenterfield (96R) 132kV line, avoid O/L Armidale to Koolkhan (966) on trip of Coffs Harbour to Lismore (89), Swamp out when all 3 directlink cable O/S,TG formulation for PD/ST","OUTAGE","OTHER","Coffs Harbour to Koolkhan (96H) and Lismore to Tenterfield (96L) 132kV line","REGULATED","INCLUDED","","PLANNED",1]
[24379,"TRANSGRIDV5_20180116135943","2017-05-21T03:35:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-29.751239999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24450,"TRANSGRIDV5_20180116135943","2017-05-22T04:45:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-17.733560000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24476,"TRANSGRIDV5_20180116135943","2017-05-23T09:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-77.233189999999993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24506,"TRANSGRIDV5_20180116135943","2017-05-23T20:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.07133,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24573,"TRANSGRIDV5_20180116135943","2017-05-24T19:55:00","#TORRB2_E","#TORRB2_E","2017-05-23",1,-168.43394000000001,"STSB2.ENERGY * 1 <= 60 (Wt = 35)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[24603,"TRANSGRIDV5_20180116135943","2017-05-24T21:45:00","#TORRB2_E","#TORRB2_E","2017-05-23",1,-37.0105,"STSB2.ENERGY * 1 <= 60 (Wt = 35)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[24633,"TRANSGRIDV5_20180116135943","2017-05-24T18:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-89.313090000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24659,"TRANSGRIDV5_20180116135943","2017-05-24T20:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-72.561080000000004,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24730,"TRANSGRIDV5_20180116135943","2017-05-24T09:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.31944,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[24760,"TRANSGRIDV5_20180116135943","2017-05-24T09:55:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-87.427549999999997,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[24786,"TRANSGRIDV5_20180116135943","2017-05-24T09:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.7881,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[24857,"TRANSGRIDV5_20180116135943","2017-05-25T00:10:00","#TORRB2_E","#TORRB2_E","2017-05-25",1,-159.13807,"STSB2.ENERGY * 1 <= 120 (Wt = 35)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[24883,"TRANSGRIDV5_20180116135943","2017-05-25T02:25:00","#TORRB2_E","#TORRB2_E","2017-05-25",1,-103.13976,"STSB2.ENERGY * 1 <= 120 (Wt = 35)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[24913,"TRANSGRIDV5_20180116135943","2017-05-25T11:40:00","#TORRB2_E","#TORRB2_E","2017-05-25",1,-83.562939999999998,"STSB2.ENERGY * 1 <= 120 (Wt = 35)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[24984,"TRANSGRIDV5_20180116135943","2017-05-25T00:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-75.382170000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25010,"TRANSGRIDV5_20180116135943","2017-05-25T09:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.961129999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25040,"TRANSGRIDV5_20180116135943","2017-05-25T21:25:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-24.740379999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25107,"TRANSGRIDV5_20180116135943","2017-05-26T00:35:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-29.8398,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25137,"TRANSGRIDV5_20180116135943","2017-05-26T19:55:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-18.149049999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25167,"TRANSGRIDV5_20180116135943","2017-05-26T06:15:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-12.78833,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25193,"TRANSGRIDV5_20180116135943","2017-05-26T13:50:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-10.180440000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25264,"TRANSGRIDV5_20180116135943","2017-05-28T17:55:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-16.364329999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25294,"TRANSGRIDV5_20180116135943","2017-05-29T08:05:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-42.527659999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25320,"TRANSGRIDV5_20180116135943","2017-05-29T09:50:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-19.94293,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25391,"TRANSGRIDV5_20180116135943","2017-05-31T07:45:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-107.70232,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25399,"TRANSGRIDV5_20180116135943","2017-05-31T07:55:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-97.957610000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25446,"TRANSGRIDV5_20180116135943","2017-05-31T15:15:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-43.399529999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25476,"TRANSGRIDV5_20180116135943","2017-05-31T00:45:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-29.700050000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25543,"TRANSGRIDV5_20180116135943","2017-06-01T09:20:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-26.040099999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25573,"TRANSGRIDV5_20180116135943","2017-06-01T14:10:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-14.043839999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25599,"TRANSGRIDV5_20180116135943","2017-06-02T07:15:00","#MPP_1_E","#MPP_1_E","2017-06-02",1,-1103.7341899999999,"QBCK1.ENERGY * 1 <= 220 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25670,"TRANSGRIDV5_20180116135943","2017-06-02T11:50:00","#MPP_1_E","#MPP_1_E","2017-06-02",1,-1075.36654,"QBCK1.ENERGY * 1 <= 220 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25700,"TRANSGRIDV5_20180116135943","2017-06-02T10:25:00","#MPP_1_E","#MPP_1_E","2017-06-02",1,-1073.0933299999999,"QBCK1.ENERGY * 1 <= 220 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25726,"TRANSGRIDV5_20180116135943","2017-06-02T03:55:00","#MPP_1_E","#MPP_1_E","2017-06-02",1,-1066.8842999999999,"QBCK1.ENERGY * 1 <= 220 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25797,"TRANSGRIDV5_20180116135943","2017-06-03T20:30:00","#MPP_1_E","#MPP_1_E","2017-06-03",1,-1084.04474,"QBCK1.ENERGY * 1 <= 320 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25827,"TRANSGRIDV5_20180116135943","2017-06-03T02:15:00","#MPP_1_E","#MPP_1_E","2017-06-03",1,-1082.5382,"QBCK1.ENERGY * 1 <= 320 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25853,"TRANSGRIDV5_20180116135943","2017-06-03T10:10:00","#MPP_1_E","#MPP_1_E","2017-06-03",1,-1066.94424,"QBCK1.ENERGY * 1 <= 320 (Wt = 360)","OUTAGE","OTHER","Millmerran Power Station","REGULATED","99","Non Inclusion",null,0]
[25924,"TRANSGRIDV5_20180116135943","2017-06-03T20:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-15.12669,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[25950,"TRANSGRIDV5_20180116135943","2017-06-03T12:25:00","Q:N_NIL_OSC","Q-NIL","2013-07-25",1,-43.395049999999998,"Out= Nil, QNI oscillatory stability limit of 1200 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[25980,"TRANSGRIDV5_20180116135943","2017-06-03T05:10:00","Q:N_NIL_OSC","Q-NIL","2013-07-25",1,-23.392690000000002,"Out= Nil, QNI oscillatory stability limit of 1200 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26010,"TRANSGRIDV5_20180116135943","2017-06-03T20:45:00","Q:N_NIL_OSC","Q-NIL","2013-07-25",1,-13.32785,"Out= Nil, QNI oscillatory stability limit of 1200 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26077,"TRANSGRIDV5_20180116135943","2017-06-04T02:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-38.06062,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[26107,"TRANSGRIDV5_20180116135943","2017-06-04T03:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.349970000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[26137,"TRANSGRIDV5_20180116135943","2017-06-04T05:30:00","Q:N_NIL_OSC","Q-NIL","2013-07-25",1,-24.202780000000001,"Out= Nil, QNI oscillatory stability limit of 1200 MW, limit reduced to 950 MW when any one SEQ SVC POD is out, limit is reduced to 853 MW when all three SEQ SVCs or PODs out.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26204,"TRANSGRIDV5_20180116135943","2017-06-05T01:05:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-22.66836,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26234,"TRANSGRIDV5_20180116135943","2017-06-05T03:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-58.185020000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26260,"TRANSGRIDV5_20180116135943","2017-06-06T10:30:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-17.90849,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26331,"TRANSGRIDV5_20180116135943","2017-06-07T12:00:00","Q>N-MUTE_758","I-MUTE_758","2017-04-05",1,-12.23926,"Out= 758 T174 Terranora to H4 Mudgeeraba 110kV line, avoid O/L on remaining Terranora to Mudgeeraba line on trip of Condong generator.","OUTAGE","OTHER","Mudgeeraba Terranora 758 110kV LINE","REGULATED","99","Non Inclusion",null,0,"Essential Energy outage"]
[26361,"TRANSGRIDV5_20180116135943","2017-06-08T09:55:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-15.663819999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26387,"TRANSGRIDV5_20180116135943","2017-06-09T07:55:00","#R015742_003_RAMP_V","#R015742_RAMP","2017-06-09",1,-81.934089999999998,"Soft Ramping constraint for constraint Q>>BCCP_CLWU_LCCP_2, Effective Date: 11/05/2017, Version: 1","OUTAGE","RAMP","Bouldercombe to Calliope River (812) with 7104 and/or 7105 (Callide A to Gladstone South) 132 kV lines closed","REGULATED","10","Ramping Constraint","PLANNED",0]
[26458,"TRANSGRIDV5_20180116135943","2017-06-09T14:45:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-33.438290000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26484,"TRANSGRIDV5_20180116135943","2017-06-09T12:35:00","N^^V_NIL_1","V-NIL;V-NIL_1","2017-04-20",1,-19.37444,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26514,"TRANSGRIDV5_20180116135943","2017-06-09T20:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.151719999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26544,"TRANSGRIDV5_20180116135943","2017-06-10T00:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-72.794640000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26611,"TRANSGRIDV5_20180116135943","2017-06-10T09:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.930199999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26641,"TRANSGRIDV5_20180116135943","2017-06-11T21:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.62011,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26671,"TRANSGRIDV5_20180116135943","2017-06-12T00:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-93.681110000000004,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26738,"TRANSGRIDV5_20180116135943","2017-06-12T23:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.686810000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26768,"TRANSGRIDV5_20180116135943","2017-06-12T03:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-10.93258,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26794,"TRANSGRIDV5_20180116135943","2017-06-12T08:10:00","NSA_Q_GSTONE34_150","NSA-Q_GSTONE34_150","2015-10-07",1,25.39836,"Gladstone 3+4 >= 150 for Network Support Agreement","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26865,"TRANSGRIDV5_20180116135943","2017-06-13T19:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.27993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26902,"TRANSGRIDV5_20180116135943","2017-06-13T15:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-19.103079999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26920,"TRANSGRIDV5_20180116135943","2017-06-13T03:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.900449999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[26991,"TRANSGRIDV5_20180116135943","2017-06-14T01:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-24.375720000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27021,"TRANSGRIDV5_20180116135943","2017-06-14T23:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-10.537050000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27047,"TRANSGRIDV5_20180116135943","2017-06-14T04:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-25.7959,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27077,"TRANSGRIDV5_20180116135943","2017-06-15T16:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.535769999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27144,"TRANSGRIDV5_20180116135943","2017-06-16T20:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.417259999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27174,"TRANSGRIDV5_20180116135943","2017-06-16T05:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.189069999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27204,"TRANSGRIDV5_20180116135943","2017-06-17T09:05:00","N^^V_MSUT_1","I-MSUT","2015-08-07",1,-104.91924,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Murray Upr Tumut 65 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[27271,"TRANSGRIDV5_20180116135943","2017-06-17T19:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-23.918030000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27301,"TRANSGRIDV5_20180116135943","2017-06-17T20:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.120509999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27327,"TRANSGRIDV5_20180116135943","2017-06-17T21:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.12257,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27398,"TRANSGRIDV5_20180116135943","2017-06-18T08:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.96264,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27428,"TRANSGRIDV5_20180116135943","2017-06-18T16:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.532340000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27454,"TRANSGRIDV5_20180116135943","2017-06-18T10:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.899809999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27484,"TRANSGRIDV5_20180116135943","2017-06-18T12:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.92525,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27555,"TRANSGRIDV5_20180116135943","2017-06-19T07:25:00","#R015782_012_RAMP_F","#R015782_RAMP","2017-06-18",1,-15.448650000000001,"Hard Ramping constraint for constraint N^^V_DDSM2, Effective Date: 07/08/2015, Version: 1","OUTAGE","RAMP","Dederang to South Morang 330 kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[27581,"TRANSGRIDV5_20180116135943","2017-06-19T10:10:00","N^^V_DDSM1","V-DDSM","2015-08-07",1,-27.69847,"Out = Dederang to South Morang 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Keilor Thomastown 1 220kV LINE; Dederang S Morang 2 330kV LINE; Keilor A2 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[27611,"TRANSGRIDV5_20180116135943","2017-06-19T08:10:00","N^^V_DDSM1","V-DDSM","2015-08-07",1,-16.793959999999998,"Out = Dederang to South Morang 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Keilor Thomastown 1 220kV LINE; Dederang S Morang 2 330kV LINE; Keilor A2 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[27678,"TRANSGRIDV5_20180116135943","2017-06-19T23:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.213460000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27708,"TRANSGRIDV5_20180116135943","2017-06-19T14:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.74667,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27738,"TRANSGRIDV5_20180116135943","2017-06-19T04:55:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-26.00103,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[27805,"TRANSGRIDV5_20180116135943","2017-06-20T21:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.582270000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27835,"TRANSGRIDV5_20180116135943","2017-06-20T00:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.704809999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27861,"TRANSGRIDV5_20180116135943","2017-06-20T10:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.039709999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27932,"TRANSGRIDV5_20180116135943","2017-06-21T13:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.144820000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27962,"TRANSGRIDV5_20180116135943","2017-06-21T22:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-31.34076,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[27988,"TRANSGRIDV5_20180116135943","2017-06-21T13:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.529450000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28018,"TRANSGRIDV5_20180116135943","2017-06-21T09:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-24.531040000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28089,"TRANSGRIDV5_20180116135943","2017-06-21T02:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.12961,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28115,"TRANSGRIDV5_20180116135943","2017-06-21T04:30:00","Q:N_AR_CP2_AR_2L-G","N-AR_CP2","2014-01-08",1,-28.49625,"Out = Armidale capacitor bank (120MVAr), limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale 6 330/138kV XFMR","REGULATED","INCLUDED","","PLANNED",1]
[28145,"TRANSGRIDV5_20180116135943","2017-06-21T08:10:00","V>>V_NIL_8","V-NIL","2016-06-21",1,-33.619149999999998,"Out = Nil, avoid O/L DDTS to WOTS 330kV line for trip of LowerTumut-Wagga (051) + (991,990,99P) or (990,99M,970) ex_Yass lines - status switched ; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28212,"TRANSGRIDV5_20180116135943","2017-06-22T02:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-27.022259999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28242,"TRANSGRIDV5_20180116135943","2017-06-22T03:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.2791,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28272,"TRANSGRIDV5_20180116135943","2017-06-22T11:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.413820000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28315,"TRANSGRIDV5_20180116135943","2017-06-22T08:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.74972,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28368,"TRANSGRIDV5_20180116135943","2017-06-22T02:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-30.498059999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[28398,"TRANSGRIDV5_20180116135943","2017-06-22T02:10:00","Q:N_AR_CP2_AR_2L-G","N-AR_CP2","2014-01-08",1,-34.52129,"Out = Armidale capacitor bank (120MVAr), limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale 6 330/138kV XFMR","REGULATED","INCLUDED","","PLANNED",1]
[28465,"TRANSGRIDV5_20180116135943","2017-06-23T20:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.94031,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28495,"TRANSGRIDV5_20180116135943","2017-06-23T18:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.407489999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28521,"TRANSGRIDV5_20180116135943","2017-06-24","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.255030000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28551,"TRANSGRIDV5_20180116135943","2017-06-24T01:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-13.51985,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28622,"TRANSGRIDV5_20180116135943","2017-06-26T23:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-91.656390000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28648,"TRANSGRIDV5_20180116135943","2017-06-26T13:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-50.345469999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28678,"TRANSGRIDV5_20180116135943","2017-06-26T14:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.432699999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28745,"TRANSGRIDV5_20180116135943","2017-06-26T20:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.769559999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28775,"TRANSGRIDV5_20180116135943","2017-06-27T23:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-96.383510000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28805,"TRANSGRIDV5_20180116135943","2017-06-27T00:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.349219999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28872,"TRANSGRIDV5_20180116135943","2017-06-27T02:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.52689,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28902,"TRANSGRIDV5_20180116135943","2017-06-27T09:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-10.72822,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlink","REGULATED","99","Non Inclusion",null,0]
[28932,"TRANSGRIDV5_20180116135943","2017-06-28T23:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.603580000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[28999,"TRANSGRIDV5_20180116135943","2017-06-29T08:20:00","#R015844_001_RAMP_V","#R015844_RAMP","2017-06-29",1,-1114.13473,"Soft Ramping constraint for constraint S_NBH_0, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP"," Belalie E 275kV BUS ","REGULATED","10","Ramping Constraint","PLANNED",0]
[29029,"TRANSGRIDV5_20180116135943","2017-06-29T00:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-35.119450000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29055,"TRANSGRIDV5_20180116135943","2017-06-29T06:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.933319999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29085,"TRANSGRIDV5_20180116135943","2017-06-29T04:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-14.76953,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29156,"TRANSGRIDV5_20180116135943","2017-06-30T05:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-47.689540000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29182,"TRANSGRIDV5_20180116135943","2017-06-30T15:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.894829999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29212,"TRANSGRIDV5_20180116135943","2017-06-30T11:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-36.180549999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29279,"TRANSGRIDV5_20180116135943","2017-06-30T01:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.103539999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29309,"TRANSGRIDV5_20180116135943","2017-06-30T03:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.662559999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29339,"TRANSGRIDV5_20180116135943","2017-07-01T15:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-82.555130000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29406,"TRANSGRIDV5_20180116135943","2017-07-01T14:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.247520000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29436,"TRANSGRIDV5_20180116135943","2017-07-01T00:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-34.881639999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29466,"TRANSGRIDV5_20180116135943","2017-07-01T00:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.173290000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29492,"TRANSGRIDV5_20180116135943","2017-07-01T13:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-23.284479999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29563,"TRANSGRIDV5_20180116135943","2017-07-02T14:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-48.255890000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29589,"TRANSGRIDV5_20180116135943","2017-07-02T09:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-36.766869999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29619,"TRANSGRIDV5_20180116135943","2017-07-02T23:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.498830000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29690,"TRANSGRIDV5_20180116135943","2017-07-03T13:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-156.21785,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29716,"TRANSGRIDV5_20180116135943","2017-07-03T05:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-57.610930000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29746,"TRANSGRIDV5_20180116135943","2017-07-03T13:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-34.743969999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29818,"TRANSGRIDV5_20180116135943","2017-07-03T04:40:00","N_NIL_TE_B","N-NIL","2012-07-04",1,-13.12485,"Out=Nil, Terranora Interconnector Qld to NSW flow overall limits","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29842,"TRANSGRIDV5_20180116135943","2017-07-03T09:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-167.48944,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29872,"TRANSGRIDV5_20180116135943","2017-07-03T13:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-35.62791,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29939,"TRANSGRIDV5_20180116135943","2017-07-03T03:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.862,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[29969,"TRANSGRIDV5_20180116135943","2017-07-03T14:00:00","S>>X_MKRB+6573+74_1","S-X_MKRB+6573+74","2017-05-31",1,-19.613399999999999,"Out= Mokota-Robertstown 275kV line AND Robertstown CB6573 and CB6574, avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Canowi-Robertstown 275kV line(this offloads Robt 275/132kV TX1, and Dav-Can 275kV line and trips Hallet GT & WF), Feedback","OUTAGE","OTHER","R_TOWN 6573 275kV CB; R_TOWN 6574 275kV CB; Heywood 1 500kV BUS","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[29999,"TRANSGRIDV5_20180116135943","2017-07-04T15:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-131.26140000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30025,"TRANSGRIDV5_20180116135943","2017-07-04T11:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-89.422499999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30096,"TRANSGRIDV5_20180116135943","2017-07-04T13:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-50.629719999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30122,"TRANSGRIDV5_20180116135943","2017-07-04T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-47.637410000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30152,"TRANSGRIDV5_20180116135943","2017-07-04T12:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.405850000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30223,"TRANSGRIDV5_20180116135943","2017-07-05T08:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-198.16652999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30249,"TRANSGRIDV5_20180116135943","2017-07-05T05:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-93.843549999999993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30279,"TRANSGRIDV5_20180116135943","2017-07-05T22:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-84.827349999999996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30350,"TRANSGRIDV5_20180116135943","2017-07-05T21:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-61.431789999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30376,"TRANSGRIDV5_20180116135943","2017-07-05T15:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-54.696930000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30406,"TRANSGRIDV5_20180116135943","2017-07-05T19:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-50.76643,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30473,"TRANSGRIDV5_20180116135943","2017-07-05T01:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.946370000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30503,"TRANSGRIDV5_20180116135943","2017-07-05T08:25:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-29.54026,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[30533,"TRANSGRIDV5_20180116135943","2017-07-05T05:15:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-15.63517,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[30559,"TRANSGRIDV5_20180116135943","2017-07-05T04:35:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-11.281840000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[30630,"TRANSGRIDV5_20180116135943","2017-07-06T06:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-91.053870000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30660,"TRANSGRIDV5_20180116135943","2017-07-06T09:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-75.06944,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30686,"TRANSGRIDV5_20180116135943","2017-07-06T17:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-61.947380000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30757,"TRANSGRIDV5_20180116135943","2017-07-06T13:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-45.325479999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30783,"TRANSGRIDV5_20180116135943","2017-07-06T15:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.776470000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30813,"TRANSGRIDV5_20180116135943","2017-07-06T02:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.09543,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30884,"TRANSGRIDV5_20180116135943","2017-07-06T03:20:00","N_NIL_TE_B","N-NIL","2012-07-04",1,-28.44314,"Out=Nil, Terranora Interconnector Qld to NSW flow overall limits","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30910,"TRANSGRIDV5_20180116135943","2017-07-06T03:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-31.619350000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[30940,"TRANSGRIDV5_20180116135943","2017-07-07T16:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-62.650060000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31007,"TRANSGRIDV5_20180116135943","2017-07-07T15:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-41.301479999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31037,"TRANSGRIDV5_20180116135943","2017-07-07T03:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.540500000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31067,"TRANSGRIDV5_20180116135943","2017-07-07T14:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.678100000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31093,"TRANSGRIDV5_20180116135943","2017-07-07T05:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.906230000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31164,"TRANSGRIDV5_20180116135943","2017-07-08T10:40:00","N^^V_DDWG","V-DDWO_RADIAL","2015-08-07",1,-110.08224,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Wodonga 330kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[31194,"TRANSGRIDV5_20180116135943","2017-07-08T13:30:00","N^^V_DDWG","V-DDWO_RADIAL","2015-08-07",1,-40.526040000000002,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Wodonga 330kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[31220,"TRANSGRIDV5_20180116135943","2017-07-08T07:50:00","N^^V_DDWG","V-DDWO_RADIAL","2015-08-07",1,-16.939160000000001,"Out = 330 kV line between Dederang to Wodonga to Jindera to Wagga, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang Wodonga 330kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[31257,"TRANSGRIDV5_20180116135943","2017-07-08T03:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-48.803249999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31316,"TRANSGRIDV5_20180116135943","2017-07-08T18:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.660809999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31346,"TRANSGRIDV5_20180116135943","2017-07-08T03:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.862459999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31376,"TRANSGRIDV5_20180116135943","2017-07-08T19:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-10.25052,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31443,"TRANSGRIDV5_20180116135943","2017-07-09T08:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.975909999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31473,"TRANSGRIDV5_20180116135943","2017-07-09T15:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.04739,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31499,"TRANSGRIDV5_20180116135943","2017-07-09T01:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.539259999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31570,"TRANSGRIDV5_20180116135943","2017-07-09T23:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.360379999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31600,"TRANSGRIDV5_20180116135943","2017-07-10T23:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-55.628459999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31626,"TRANSGRIDV5_20180116135943","2017-07-10T14:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-47.619520000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31697,"TRANSGRIDV5_20180116135943","2017-07-10T03:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-31.9541,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31727,"TRANSGRIDV5_20180116135943","2017-07-10T06:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.48235,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31753,"TRANSGRIDV5_20180116135943","2017-07-10T13:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.38475,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31824,"TRANSGRIDV5_20180116135943","2017-07-11T23:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-81.561340000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31850,"TRANSGRIDV5_20180116135943","2017-07-11T05:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-66.205309999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31880,"TRANSGRIDV5_20180116135943","2017-07-11T18:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-57.185519999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31910,"TRANSGRIDV5_20180116135943","2017-07-11T10:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-48.327039999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[31977,"TRANSGRIDV5_20180116135943","2017-07-11T22:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.13109,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32007,"TRANSGRIDV5_20180116135943","2017-07-11T04:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.5305,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32037,"TRANSGRIDV5_20180116135943","2017-07-11T22:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-19.090540000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32104,"TRANSGRIDV5_20180116135943","2017-07-11T02:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-33.898699999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32134,"TRANSGRIDV5_20180116135943","2017-07-11T00:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.822649999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32160,"TRANSGRIDV5_20180116135943","2017-07-11T13:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.53215,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32231,"TRANSGRIDV5_20180116135943","2017-07-12T03:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-31.946179999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32261,"TRANSGRIDV5_20180116135943","2017-07-12T06:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.13664,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32287,"TRANSGRIDV5_20180116135943","2017-07-12T03:15:00","N_NIL_TE_B","N-NIL","2012-07-04",1,-50.568570000000001,"Out=Nil, Terranora Interconnector Qld to NSW flow overall limits","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32358,"TRANSGRIDV5_20180116135943","2017-07-12T15:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-20.986920000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32384,"TRANSGRIDV5_20180116135943","2017-07-12T12:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.926629999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32414,"TRANSGRIDV5_20180116135943","2017-07-12T01:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.162240000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32444,"TRANSGRIDV5_20180116135943","2017-07-12T03:15:00","S>RB_275KV_N_BUS_1","S-RB_275KV_N_BUS","2017-04-27",1,-79.203209999999999,"Out =Robertstown 275kV North Bus(i.e. RB 275/132kV TX1, RB 275kV CBs 6616 and 6573, and RB 132kV CBs 6005 and 6188 O/S), avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Robertstown 275/132kV TX2 (this offloads NWB-RB #1 132kV line).","OUTAGE","OTHER","Robertstwn N 275kV BUS; R_TOWN 6005 132kV CB; R_TOWN 6188 132kV CB; R_TOWN 6573 275kV CB; R_TOWN 6616 275kV CB; Robertstwn 1 275/132kV XFMR","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[32511,"TRANSGRIDV5_20180116135943","2017-07-13T22:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.24736,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32541,"TRANSGRIDV5_20180116135943","2017-07-13T01:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.598510000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32571,"TRANSGRIDV5_20180116135943","2017-07-13T14:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.973859999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32638,"TRANSGRIDV5_20180116135943","2017-07-13T10:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.38,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32668,"TRANSGRIDV5_20180116135943","2017-07-13T12:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.67937,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32694,"TRANSGRIDV5_20180116135943","2017-07-13T02:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.20673,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32736,"TRANSGRIDV5_20180116135943","2017-07-13T09:25:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-15.12604,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32794,"TRANSGRIDV5_20180116135943","2017-07-14T22:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.392029999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32820,"TRANSGRIDV5_20180116135943","2017-07-14T21:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-19.552109999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32891,"TRANSGRIDV5_20180116135943","2017-07-15T18:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-99.628230000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32917,"TRANSGRIDV5_20180116135943","2017-07-15T23:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-77.799109999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32947,"TRANSGRIDV5_20180116135943","2017-07-15T03:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-64.466859999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[32977,"TRANSGRIDV5_20180116135943","2017-07-15T06:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-54.923099999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33044,"TRANSGRIDV5_20180116135943","2017-07-15T21:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.22419,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33074,"TRANSGRIDV5_20180116135943","2017-07-15T01:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.660919999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33104,"TRANSGRIDV5_20180116135943","2017-07-15T16:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-34.582790000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33171,"TRANSGRIDV5_20180116135943","2017-07-16T11:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-52.517740000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33201,"TRANSGRIDV5_20180116135943","2017-07-16T02:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-43.913519999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33227,"TRANSGRIDV5_20180116135943","2017-07-16T12:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-40.406529999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33298,"TRANSGRIDV5_20180116135943","2017-07-16T11:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.047940000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33328,"TRANSGRIDV5_20180116135943","2017-07-16T22:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.89119,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33354,"TRANSGRIDV5_20180116135943","2017-07-17T20:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.060839999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33384,"TRANSGRIDV5_20180116135943","2017-07-17T13:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.417090000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33455,"TRANSGRIDV5_20180116135943","2017-07-17T04:15:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-25.683710000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33481,"TRANSGRIDV5_20180116135943","2017-07-18T21:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-68.555179999999993,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33511,"TRANSGRIDV5_20180116135943","2017-07-18T13:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-48.182510000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33578,"TRANSGRIDV5_20180116135943","2017-07-18T14:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.056149999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33608,"TRANSGRIDV5_20180116135943","2017-07-18T21:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.48489,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33638,"TRANSGRIDV5_20180116135943","2017-07-18T02:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.082929999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33705,"TRANSGRIDV5_20180116135943","2017-07-19T23:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-19.722909999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33735,"TRANSGRIDV5_20180116135943","2017-07-19T23:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.95538,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33761,"TRANSGRIDV5_20180116135943","2017-07-19T04:35:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-33.711370000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33832,"TRANSGRIDV5_20180116135943","2017-07-20T14:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-53.956440000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33862,"TRANSGRIDV5_20180116135943","2017-07-20T14:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-38.483780000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33888,"TRANSGRIDV5_20180116135943","2017-07-20T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-26.20966,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33918,"TRANSGRIDV5_20180116135943","2017-07-20T02:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.794919999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[33989,"TRANSGRIDV5_20180116135943","2017-07-21T10:55:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1121.00308,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34015,"TRANSGRIDV5_20180116135943","2017-07-21T22:30:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1107.8783800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34045,"TRANSGRIDV5_20180116135943","2017-07-21T23:50:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1100.89732,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34112,"TRANSGRIDV5_20180116135943","2017-07-21T01:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-71.871960000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34142,"TRANSGRIDV5_20180116135943","2017-07-21T10:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-41.832270000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34173,"TRANSGRIDV5_20180116135943","2017-07-21T10:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-29.90016,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34238,"TRANSGRIDV5_20180116135943","2017-07-22T23:35:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1138.4119499999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34268,"TRANSGRIDV5_20180116135943","2017-07-22T16:55:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1106.77036,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34298,"TRANSGRIDV5_20180116135943","2017-07-22T17:20:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1104.94254,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34365,"TRANSGRIDV5_20180116135943","2017-07-22T21:15:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1090.85265,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34395,"TRANSGRIDV5_20180116135943","2017-07-22T21:40:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1087.8431800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34421,"TRANSGRIDV5_20180116135943","2017-07-22T13:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1086.8214499999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34451,"TRANSGRIDV5_20180116135943","2017-07-22T05:50:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1080.45895,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34522,"TRANSGRIDV5_20180116135943","2017-07-22T12:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.53778,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[34548,"TRANSGRIDV5_20180116135943","2017-07-22T11:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.777150000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34578,"TRANSGRIDV5_20180116135943","2017-07-22T14:50:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-127.81220999999999,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34645,"TRANSGRIDV5_20180116135943","2017-07-22T04:50:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-25.80087,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34675,"TRANSGRIDV5_20180116135943","2017-07-23T19:40:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1162.2446500000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34705,"TRANSGRIDV5_20180116135943","2017-07-23T00:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1137.64337,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34772,"TRANSGRIDV5_20180116135943","2017-07-23T10:00:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1104.0719899999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34802,"TRANSGRIDV5_20180116135943","2017-07-23T08:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1098.2940000000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34832,"TRANSGRIDV5_20180116135943","2017-07-23T11:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1089.3977600000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34899,"TRANSGRIDV5_20180116135943","2017-07-23T07:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1066.5647300000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[34929,"TRANSGRIDV5_20180116135943","2017-07-23T23:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-78.033789999999996,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34955,"TRANSGRIDV5_20180116135943","2017-07-23T14:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-57.232019999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[34985,"TRANSGRIDV5_20180116135943","2017-07-23T21:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.677770000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35056,"TRANSGRIDV5_20180116135943","2017-07-23T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-10.91236,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35082,"TRANSGRIDV5_20180116135943","2017-07-23T12:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.37116,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35112,"TRANSGRIDV5_20180116135943","2017-07-24T18:00:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1294.65093,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35179,"TRANSGRIDV5_20180116135943","2017-07-24T05:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1129.75674,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35209,"TRANSGRIDV5_20180116135943","2017-07-24T03:50:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1118.0169000000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35239,"TRANSGRIDV5_20180116135943","2017-07-24T19:40:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1106.03565,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35306,"TRANSGRIDV5_20180116135943","2017-07-24T21:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1098.90256,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35336,"TRANSGRIDV5_20180116135943","2017-07-24T21:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1093.9333099999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35366,"TRANSGRIDV5_20180116135943","2017-07-24T13:35:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1087.9066800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35392,"TRANSGRIDV5_20180116135943","2017-07-24T07:15:00","N^^Q_NIL_B1","N-NIL","2013-08-21",1,-26.370429999999999,"Out= Nil, avoid Voltage Collapse on loss of Kogan Creek","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35463,"TRANSGRIDV5_20180116135943","2017-07-24T00:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.49803,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35489,"TRANSGRIDV5_20180116135943","2017-07-24T02:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-17.499970000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[35519,"TRANSGRIDV5_20180116135943","2017-07-25T17:45:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1290.0028,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35590,"TRANSGRIDV5_20180116135943","2017-07-25T21:15:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1111.5444,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35616,"TRANSGRIDV5_20180116135943","2017-07-25T19:35:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1105.9026799999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35652,"TRANSGRIDV5_20180116135943","2017-07-25T08:35:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1101.11979,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35716,"TRANSGRIDV5_20180116135943","2017-07-25T01:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1085.79927,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35742,"TRANSGRIDV5_20180116135943","2017-07-25T01:25:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1068.52925,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35772,"TRANSGRIDV5_20180116135943","2017-07-25T05:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1055.22407,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35839,"TRANSGRIDV5_20180116135943","2017-07-26T19:35:00","#DARTM1_E","#DARTM1_E","2017-07-19",1,-133.07499000000001,"VDPS.ENERGY * 1 <= 150 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[35869,"TRANSGRIDV5_20180116135943","2017-07-26T18:00:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1160.6129800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35899,"TRANSGRIDV5_20180116135943","2017-07-26T23:45:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1149.8531599999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35925,"TRANSGRIDV5_20180116135943","2017-07-26T23:20:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1135.4540400000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[35996,"TRANSGRIDV5_20180116135943","2017-07-26T13:45:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1109.15282,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36022,"TRANSGRIDV5_20180116135943","2017-07-26T17:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1107.31042,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36052,"TRANSGRIDV5_20180116135943","2017-07-26T00:15:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1091.5123799999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36123,"TRANSGRIDV5_20180116135943","2017-07-26T03:55:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1047.12291,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36149,"TRANSGRIDV5_20180116135943","2017-07-26T15:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-38.557830000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36179,"TRANSGRIDV5_20180116135943","2017-07-26T12:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.850969999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36250,"TRANSGRIDV5_20180116135943","2017-07-26T20:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-35.941130000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36276,"TRANSGRIDV5_20180116135943","2017-07-27T07:35:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1192.2212999999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36306,"TRANSGRIDV5_20180116135943","2017-07-27T10:10:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1148.0024800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36373,"TRANSGRIDV5_20180116135943","2017-07-27T13:15:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1109.4279899999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36403,"TRANSGRIDV5_20180116135943","2017-07-27T17:15:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1105.9027799999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36433,"TRANSGRIDV5_20180116135943","2017-07-27T14:45:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1104.9427800000001,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36459,"TRANSGRIDV5_20180116135943","2017-07-27T08:30:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1103.7735499999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36530,"TRANSGRIDV5_20180116135943","2017-07-27T04:05:00","#YWPS2_E","#YWPS2_E","2017-07-21",1,-1079.7530099999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36560,"TRANSGRIDV5_20180116135943","2017-07-27T01:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.973320000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36586,"TRANSGRIDV5_20180116135943","2017-07-27T02:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-78.299869999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[36657,"TRANSGRIDV5_20180116135943","2017-07-27T14:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-34.709220000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[36683,"TRANSGRIDV5_20180116135943","2017-07-27T14:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-27.587710000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[36713,"TRANSGRIDV5_20180116135943","2017-07-27","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.46715,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[36784,"TRANSGRIDV5_20180116135943","2017-07-27T05:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-34.273290000000003,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36810,"TRANSGRIDV5_20180116135943","2017-07-27T01:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-26.04636,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36840,"TRANSGRIDV5_20180116135943","2017-07-27T03:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.150230000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[36907,"TRANSGRIDV5_20180116135943","2017-07-28T09:00:00","#YWPS2_E","#YWPS2_E","2017-07-28",1,-1108.1497999999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36937,"TRANSGRIDV5_20180116135943","2017-07-28T05:10:00","#YWPS2_E","#YWPS2_E","2017-07-28",1,-1080.5237099999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36967,"TRANSGRIDV5_20180116135943","2017-07-28T02:05:00","#YWPS2_E","#YWPS2_E","2017-07-28",1,-1069.2188699999999,"VYP22.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[36993,"TRANSGRIDV5_20180116135943","2017-07-28T13:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-25.66057,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37064,"TRANSGRIDV5_20180116135943","2017-07-28T13:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-13.81742,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[37094,"TRANSGRIDV5_20180116135943","2017-07-29T07:25:00","#R015943_008_RAMP_F","#R015943_RAMP","2017-07-29",1,-12.183920000000001,"Hard Ramping constraint for constraint V::N_HWCB_V2, Effective Date: 07/04/2017, Version: 1","OUTAGE","RAMP","Hazelwood to Cranbourne No.4 500kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[37131,"TRANSGRIDV5_20180116135943","2017-07-29T14:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.081849999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[37190,"TRANSGRIDV5_20180116135943","2017-07-29T15:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.603529999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37216,"TRANSGRIDV5_20180116135943","2017-07-30T20:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-47.592419999999997,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37246,"TRANSGRIDV5_20180116135943","2017-07-30T16:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.525289999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37276,"TRANSGRIDV5_20180116135943","2017-07-30T10:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-19.473120000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[37343,"TRANSGRIDV5_20180116135943","2017-07-30T10:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.531090000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37373,"TRANSGRIDV5_20180116135943","2017-07-31T19:00:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1281.98352,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37399,"TRANSGRIDV5_20180116135943","2017-07-31T17:40:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1149.8626300000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37470,"TRANSGRIDV5_20180116135943","2017-07-31T21:30:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1104.87211,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37500,"TRANSGRIDV5_20180116135943","2017-07-31T06:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-76.538920000000005,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37526,"TRANSGRIDV5_20180116135943","2017-07-31T00:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-39.129840000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37597,"TRANSGRIDV5_20180116135943","2017-07-31T13:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-25.259519999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[37627,"TRANSGRIDV5_20180116135943","2017-07-31T14:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-36.227040000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[37653,"TRANSGRIDV5_20180116135943","2017-08-01T18:05:00","#DARTM1_E","#DARTM1_E","2017-07-19",1,-93.170069999999996,"VDPS.ENERGY * 1 <= 150 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[37724,"TRANSGRIDV5_20180116135943","2017-08-01T05:50:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1148.37309,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37750,"TRANSGRIDV5_20180116135943","2017-08-01T19:40:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1136.80879,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37780,"TRANSGRIDV5_20180116135943","2017-08-01T02:15:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1120.44271,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37810,"TRANSGRIDV5_20180116135943","2017-08-01T04:55:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1113.51865,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37877,"TRANSGRIDV5_20180116135943","2017-08-01T11:25:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1105.1823899999999,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37907,"TRANSGRIDV5_20180116135943","2017-08-01T13:25:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1102.6704400000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[37937,"TRANSGRIDV5_20180116135943","2017-08-01T15:35:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1098.90263,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38004,"TRANSGRIDV5_20180116135943","2017-08-01T04:55:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.86983,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38034,"TRANSGRIDV5_20180116135943","2017-08-01T19:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-43.166249999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38060,"TRANSGRIDV5_20180116135943","2017-08-01T12:10:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-36.08511,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38131,"TRANSGRIDV5_20180116135943","2017-08-01T10:15:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-18.30932,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38161,"TRANSGRIDV5_20180116135943","2017-08-01T19:00:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.298410000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38187,"TRANSGRIDV5_20180116135943","2017-08-01T15:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-15.002219999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38258,"TRANSGRIDV5_20180116135943","2017-08-01T02:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.2247,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38284,"TRANSGRIDV5_20180116135943","2017-08-01T13:30:00","Q:N_BI_POT_WIV_N-2","Q-WIV_N-2","2017-05-16",1,-18.492519999999999,"Out= Nil, limit Qld to NSW on QNI to avoid transient instability on trip of both Wivenhoe pumps","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38314,"TRANSGRIDV5_20180116135943","2017-08-01T12:30:00","Q:N_BI_POT_WIV_N-2","Q-WIV_N-2","2017-05-16",1,-11.02338,"Out= Nil, limit Qld to NSW on QNI to avoid transient instability on trip of both Wivenhoe pumps","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38344,"TRANSGRIDV5_20180116135943","2017-08-01T01:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.609590000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38411,"TRANSGRIDV5_20180116135943","2017-08-02T08:15:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1120.44307,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38441,"TRANSGRIDV5_20180116135943","2017-08-02T22:20:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1113.9558999999999,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38471,"TRANSGRIDV5_20180116135943","2017-08-02T02:20:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1108.0115900000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38538,"TRANSGRIDV5_20180116135943","2017-08-02T23:30:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1101.2494999999999,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38568,"TRANSGRIDV5_20180116135943","2017-08-02T13:50:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1096.1757600000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38593,"TRANSGRIDV5_20180116135943","2017-08-02T15:25:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1093.52944,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[38664,"TRANSGRIDV5_20180116135943","2017-08-02T16:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-30.632670000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38694,"TRANSGRIDV5_20180116135943","2017-08-02T15:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.477260000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38720,"TRANSGRIDV5_20180116135943","2017-08-02T14:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.65057,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38791,"TRANSGRIDV5_20180116135943","2017-08-02T00:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-20.13869,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38817,"TRANSGRIDV5_20180116135943","2017-08-02T11:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-17.518809999999998,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38847,"TRANSGRIDV5_20180116135943","2017-08-02T12:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.72845,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38877,"TRANSGRIDV5_20180116135943","2017-08-02T08:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.14418,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[38944,"TRANSGRIDV5_20180116135943","2017-08-02T03:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.246230000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[38974,"TRANSGRIDV5_20180116135943","2017-08-03T12:30:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1309.7005200000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39004,"TRANSGRIDV5_20180116135943","2017-08-03T07:00:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1241.2082399999999,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39071,"TRANSGRIDV5_20180116135943","2017-08-03T19:00:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1148.81357,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39101,"TRANSGRIDV5_20180116135943","2017-08-03T21:10:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1140.3968600000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39127,"TRANSGRIDV5_20180116135943","2017-08-03T22:05:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1120.4434200000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39198,"TRANSGRIDV5_20180116135943","2017-08-03T03:15:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1094.36393,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39228,"TRANSGRIDV5_20180116135943","2017-08-03T02:40:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1087.63302,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39254,"TRANSGRIDV5_20180116135943","2017-08-03T11:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-189.86032,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39284,"TRANSGRIDV5_20180116135943","2017-08-03T14:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-92.991789999999995,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39355,"TRANSGRIDV5_20180116135943","2017-08-03T15:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-16.993839999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39381,"TRANSGRIDV5_20180116135943","2017-08-03T10:45:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-48.364710000000002,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39411,"TRANSGRIDV5_20180116135943","2017-08-03T03:05:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-36.134369999999997,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39478,"TRANSGRIDV5_20180116135943","2017-08-03T16:55:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-21.32743,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39508,"TRANSGRIDV5_20180116135943","2017-08-03T05:30:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-16.476430000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39538,"TRANSGRIDV5_20180116135943","2017-08-03T05:50:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-12.65588,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39605,"TRANSGRIDV5_20180116135943","2017-08-03T11:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.349730000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39635,"TRANSGRIDV5_20180116135943","2017-08-03T01:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.919230000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39661,"TRANSGRIDV5_20180116135943","2017-08-04T09:30:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1132.8737699999999,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39732,"TRANSGRIDV5_20180116135943","2017-08-04T14:30:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1104.9434200000001,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39762,"TRANSGRIDV5_20180116135943","2017-08-04T03:25:00","#YWPS2_E","#YWPS2_E","2017-07-31",1,-1072.02828,"VYP22.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","Yallourn WF Unit 2","REGULATED","99","Non Inclusion",null,0]
[39788,"TRANSGRIDV5_20180116135943","2017-08-04T09:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-17.974340000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[39818,"TRANSGRIDV5_20180116135943","2017-08-04T12:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-84.089830000000006,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39889,"TRANSGRIDV5_20180116135943","2017-08-04T13:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-37.007570000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39915,"TRANSGRIDV5_20180116135943","2017-08-04T08:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-26.487770000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[39945,"TRANSGRIDV5_20180116135943","2017-08-04T02:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.860990000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE; Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40012,"TRANSGRIDV5_20180116135943","2017-08-04T03:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-40.445500000000003,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40047,"TRANSGRIDV5_20180116135943","2017-08-04T13:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.033180000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40071,"TRANSGRIDV5_20180116135943","2017-08-04T21:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-21.798739999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40138,"TRANSGRIDV5_20180116135943","2017-08-05T16:50:00","F_Q++LDTW_L5","F-N-LDTW_84","2013-08-21",1,19.989999999999998,"Out = Liddell to Tamworth (84) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40168,"TRANSGRIDV5_20180116135943","2017-08-05T15:15:00","F_Q++LDTW_L6","F-N-LDTW_84","2013-08-21",1,19.83764,"Out = Liddell to Tamworth (84) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40198,"TRANSGRIDV5_20180116135943","2017-08-05T15:10:00","F_Q++LDTW_L60","F-N-LDTW_84","2013-08-21",1,18.38852,"Out = Liddell to Tamworth (84) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40265,"TRANSGRIDV5_20180116135943","2017-08-05T01:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-12.91028,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40295,"TRANSGRIDV5_20180116135943","2017-08-05T09:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.22677,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40321,"TRANSGRIDV5_20180116135943","2017-08-06T10:20:00","F_Q++LDTW_L5","F-N-LDTW_84","2013-08-21",1,24.26078,"Out = Liddell to Tamworth (84) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40351,"TRANSGRIDV5_20180116135943","2017-08-06T05:55:00","F_Q++LDTW_L5","F-N-LDTW_84","2013-08-21",1,14.430680000000001,"Out = Liddell to Tamworth (84) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40422,"TRANSGRIDV5_20180116135943","2017-08-06T12:30:00","F_Q++LDTW_L6","F-N-LDTW_84","2013-08-21",1,14.77374,"Out = Liddell to Tamworth (84) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40448,"TRANSGRIDV5_20180116135943","2017-08-06T10:30:00","F_Q++LDTW_L60","F-N-LDTW_84","2013-08-21",1,28.97,"Out = Liddell to Tamworth (84) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40478,"TRANSGRIDV5_20180116135943","2017-08-06T12:30:00","F_Q++LDTW_L60","F-N-LDTW_84","2013-08-21",1,20.960100000000001,"Out = Liddell to Tamworth (84) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Liddell PS 84 330kV LINE","REGULATED","INCLUDED","","UNPLANNED",1]
[40545,"TRANSGRIDV5_20180116135943","2017-08-07T08:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-32.709240000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40575,"TRANSGRIDV5_20180116135943","2017-08-07T10:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-17.318300000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40605,"TRANSGRIDV5_20180116135943","2017-08-07T14:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.227309999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40672,"TRANSGRIDV5_20180116135943","2017-08-07T11:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.350899999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40702,"TRANSGRIDV5_20180116135943","2017-08-08T16:05:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-18.531610000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40732,"TRANSGRIDV5_20180116135943","2017-08-08T10:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-42.671019999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40799,"TRANSGRIDV5_20180116135943","2017-08-08T01:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-19.80847,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40829,"TRANSGRIDV5_20180116135943","2017-08-08T12:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-11.90152,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40855,"TRANSGRIDV5_20180116135943","2017-08-08T04:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.14115,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40885,"TRANSGRIDV5_20180116135943","2017-08-08T11:50:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-18.517330000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[40956,"TRANSGRIDV5_20180116135943","2017-08-09T13:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.94717,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[40982,"TRANSGRIDV5_20180116135943","2017-08-09T12:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.44201,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41012,"TRANSGRIDV5_20180116135943","2017-08-09T13:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.557090000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41079,"TRANSGRIDV5_20180116135943","2017-08-11T08:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.1282,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41109,"TRANSGRIDV5_20180116135943","2017-08-11T08:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-11.43491,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41139,"TRANSGRIDV5_20180116135943","2017-08-11T11:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-15.166270000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41206,"TRANSGRIDV5_20180116135943","2017-08-12T08:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.37444,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41236,"TRANSGRIDV5_20180116135943","2017-08-12T03:10:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-15.769539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41266,"TRANSGRIDV5_20180116135943","2017-08-13T11:05:00","F_Q++LDMU_L5","F-N-LDMU_83","2013-08-21",1,47.48997,"Out = Liddell to Muswellbrook (83) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[41292,"TRANSGRIDV5_20180116135943","2017-08-13T09:20:00","F_Q++LDMU_L6","F-N-LDMU_83","2013-08-21",1,29.46,"Out = Liddell to Muswellbrook (83) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[41363,"TRANSGRIDV5_20180116135943","2017-08-13T09:20:00","F_Q++LDMU_L60","F-N-LDMU_83","2013-08-21",1,12.788,"Out = Liddell to Muswellbrook (83) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Liddell PS Muswlbk330 83 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[41389,"TRANSGRIDV5_20180116135943","2017-08-13T01:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.528030000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41419,"TRANSGRIDV5_20180116135943","2017-08-13T01:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-15.33076,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41490,"TRANSGRIDV5_20180116135943","2017-08-13T03:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.117190000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41526,"TRANSGRIDV5_20180116135943","2017-08-13T12:45:00","S>V_NWRB_RBMWP3","S-NWRB","2015-03-23",1,-1141.6650199999999,"Out=NWB - Robertstown 132kV #1 line, Limit Murraylink SA to Vic flow to avoid OL Robertstown-MWP3 132kV line.","OUTAGE","OTHER","N_W_B 6025 132kV CB; N_W_B 6033 132kV CB; N_W_Bend Robertstwn 1 132kV LINE; R_TOWN 6005 132kV CB; R_TOWN 6148 132kV CB; N_W_B 5171 66kV CB; N_W_Bend 2 132/66/11kV XFMR","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[41545,"TRANSGRIDV5_20180116135943","2017-08-13T05:55:00","S>V_NWRB_RBMWP3","S-NWRB","2015-03-23",1,-33.157989999999998,"Out=NWB - Robertstown 132kV #1 line, Limit Murraylink SA to Vic flow to avoid OL Robertstown-MWP3 132kV line.","OUTAGE","OTHER","N_W_B 6025 132kV CB; N_W_B 6033 132kV CB; N_W_Bend Robertstwn 1 132kV LINE; R_TOWN 6005 132kV CB; R_TOWN 6148 132kV CB; N_W_B 5171 66kV CB; N_W_Bend 2 132/66/11kV XFMR","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[41616,"TRANSGRIDV5_20180116135943","2017-08-13T06:30:00","V::N_HWSM_V2","V-HWSM","2017-04-07",1,-52.820900000000002,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[41642,"TRANSGRIDV5_20180116135943","2017-08-13T03:50:00","V::N_HWSM_V2","V-HWSM","2017-04-07",1,-36.067360000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[41672,"TRANSGRIDV5_20180116135943","2017-08-13T10:45:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-16.917680000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41739,"TRANSGRIDV5_20180116135943","2017-08-14T10:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-53.822899999999997,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41769,"TRANSGRIDV5_20180116135943","2017-08-14T12:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-32.322589999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41799,"TRANSGRIDV5_20180116135943","2017-08-14T05:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.330120000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41825,"TRANSGRIDV5_20180116135943","2017-08-14T00:15:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.02196,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[41896,"TRANSGRIDV5_20180116135943","2017-08-14T12:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.075900000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41922,"TRANSGRIDV5_20180116135943","2017-08-14T05:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.771929999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[41952,"TRANSGRIDV5_20180116135943","2017-08-14T04:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.46706,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42023,"TRANSGRIDV5_20180116135943","2017-08-14T05:05:00","V::N_HWSM_S1","V-HWSM","2017-04-07",1,-43.55639,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates","OUTAGE","OTHER","Hazelwood S Morang 1 500kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[42049,"TRANSGRIDV5_20180116135943","2017-08-14T01:35:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-39.675559999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42079,"TRANSGRIDV5_20180116135943","2017-08-15T09:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-94.695800000000006,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42150,"TRANSGRIDV5_20180116135943","2017-08-15T10:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-39.975189999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42176,"TRANSGRIDV5_20180116135943","2017-08-15T04:05:00","SVML_ROC_80","S-NIL","2016-08-23",1,-12.25691,"Out=Nil, Rate of Change (SA to VIC) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42206,"TRANSGRIDV5_20180116135943","2017-08-15T04:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-16.121839999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42273,"TRANSGRIDV5_20180116135943","2017-08-16T11:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-112.12219,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[42303,"TRANSGRIDV5_20180116135943","2017-08-16T04:50:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-24.74935,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[42333,"TRANSGRIDV5_20180116135943","2017-08-16T10:10:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-13.79425,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[42359,"TRANSGRIDV5_20180116135943","2017-08-16T07:00:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-12.33142,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[42430,"TRANSGRIDV5_20180116135943","2017-08-16T05:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-25.392240000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42456,"TRANSGRIDV5_20180116135943","2017-08-16T02:05:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-16.200510000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42486,"TRANSGRIDV5_20180116135943","2017-08-17T01:25:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-19.734539999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42557,"TRANSGRIDV5_20180116135943","2017-08-18T07:10:00","#WRWF1_E","#WRWF1_E","2017-07-06",2,-85.829759999999993,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[42583,"TRANSGRIDV5_20180116135943","2017-08-18T21:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-29.159749999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42613,"TRANSGRIDV5_20180116135943","2017-08-18T09:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.945229999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42684,"TRANSGRIDV5_20180116135943","2017-08-18T23:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.500689999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42710,"TRANSGRIDV5_20180116135943","2017-08-18T08:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.96372,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42740,"TRANSGRIDV5_20180116135943","2017-08-18T12:40:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-237.85150999999999,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[42807,"TRANSGRIDV5_20180116135943","2017-08-19T10:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-69.756290000000007,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42837,"TRANSGRIDV5_20180116135943","2017-08-19T21:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-53.30274,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42867,"TRANSGRIDV5_20180116135943","2017-08-19T10:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-42.285769999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42893,"TRANSGRIDV5_20180116135943","2017-08-19T20:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-35.682850000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42964,"TRANSGRIDV5_20180116135943","2017-08-19T00:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-19.480329999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[42989,"TRANSGRIDV5_20180116135943","2017-08-19T16:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-14.74338,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43019,"TRANSGRIDV5_20180116135943","2017-08-19T11:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-73.373350000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43090,"TRANSGRIDV5_20180116135943","2017-08-19T14:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-33.836379999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43116,"TRANSGRIDV5_20180116135943","2017-08-19T08:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.07583,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43146,"TRANSGRIDV5_20180116135943","2017-08-19T16:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.47307,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43176,"TRANSGRIDV5_20180116135943","2017-08-19T05:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-15.37355,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43243,"TRANSGRIDV5_20180116135943","2017-08-20T13:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-76.827179999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43273,"TRANSGRIDV5_20180116135943","2017-08-20T15:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-69.703770000000006,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43299,"TRANSGRIDV5_20180116135943","2017-08-20T07:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-61.460070000000002,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43370,"TRANSGRIDV5_20180116135943","2017-08-20T04:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-27.46951,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43400,"TRANSGRIDV5_20180116135943","2017-08-20T06:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-20.499919999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43426,"TRANSGRIDV5_20180116135943","2017-08-20T10:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-83.126310000000004,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43497,"TRANSGRIDV5_20180116135943","2017-08-20T10:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-58.968499999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43527,"TRANSGRIDV5_20180116135943","2017-08-20T01:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-43.072369999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43553,"TRANSGRIDV5_20180116135943","2017-08-20T07:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.095320000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43624,"TRANSGRIDV5_20180116135943","2017-08-20T05:05:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-20.311019999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43650,"TRANSGRIDV5_20180116135943","2017-08-21T12:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-58.996749999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43680,"TRANSGRIDV5_20180116135943","2017-08-21T11:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-39.867519999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43710,"TRANSGRIDV5_20180116135943","2017-08-21T13:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-10.143509999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43777,"TRANSGRIDV5_20180116135943","2017-08-21T11:40:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-35.710830000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43807,"TRANSGRIDV5_20180116135943","2017-08-21T03:45:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-20.224869999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43837,"TRANSGRIDV5_20180116135943","2017-08-22T11:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-36.915230000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[43904,"TRANSGRIDV5_20180116135943","2017-08-22T12:30:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-20.024480000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[43934,"TRANSGRIDV5_20180116135943","2017-08-22T15:30:00","V>>V_KTS_TX_A3_2A_R","V-KTTX_A3_R","2017-04-10",1,-10.61206,"Out = Keilor A3 500/220 kV txfmr, avoid pre-contingent O/L of South Morang F2 500/330 kV txfmr, radial mode, Yallourn W Unit 1 on 500 kV network, feedback","OUTAGE","OTHER","Keilor A3 500/220kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[43960,"TRANSGRIDV5_20180116135943","2017-08-23T07:15:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-172.05985000000001,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44031,"TRANSGRIDV5_20180116135943","2017-08-23T21:35:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-139.13797,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44061,"TRANSGRIDV5_20180116135943","2017-08-23T15:35:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-135.43755999999999,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44087,"TRANSGRIDV5_20180116135943","2017-08-23T08:50:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-133.29,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44158,"TRANSGRIDV5_20180116135943","2017-08-23T11:20:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-125.36006999999999,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44184,"TRANSGRIDV5_20180116135943","2017-08-23T03:10:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-122.83412,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44214,"TRANSGRIDV5_20180116135943","2017-08-23T09:10:00","#R016063_001_RAMP_F","#R016063_RAMP","2017-08-23",1,-1117.04,"Hard Ramping constraint for constraint S-STTX_SNWF, Effective Date: 16/01/2015, Version: 1","OUTAGE","RAMP","Snowtown 132/33kV TX or Snowtown CB4593 or Snowtown CB6265","REGULATED","10","Ramping Constraint","PLANNED",0]
[44244,"TRANSGRIDV5_20180116135943","2017-08-23T11:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-21.908840000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[44311,"TRANSGRIDV5_20180116135943","2017-08-24T09:10:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-199.62388000000001,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44341,"TRANSGRIDV5_20180116135943","2017-08-24T09:00:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-152.25317000000001,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44371,"TRANSGRIDV5_20180116135943","2017-08-24T11:05:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-136.99315000000001,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44442,"TRANSGRIDV5_20180116135943","2017-08-24T03:45:00","#BALDHWF1_E","#BALDHWF1_E","2017-08-23",2,-112.83787,"VMWT9B.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","BALD HILLS WIND FARM","REGULATED","99","Non Inclusion",null,0]
[44467,"TRANSGRIDV5_20180116135943","2017-08-24T01:45:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-19.240100000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44493,"TRANSGRIDV5_20180116135943","2017-08-25T09:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.325959999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[44564,"TRANSGRIDV5_20180116135943","2017-08-26T04:35:00","#WRWF1_E","#WRWF1_E","2017-07-06",2,-105.97992000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[44594,"TRANSGRIDV5_20180116135943","2017-08-26T13:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-34.164299999999997,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[44620,"TRANSGRIDV5_20180116135943","2017-08-26T14:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-29.04261,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[44691,"TRANSGRIDV5_20180116135943","2017-08-26T14:15:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-20.77252,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44717,"TRANSGRIDV5_20180116135943","2017-08-26T22:20:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-16.177720000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44747,"TRANSGRIDV5_20180116135943","2017-08-27T13:45:00","#WRWF1_E","#WRWF1_E","2017-07-06",2,-86.980509999999995,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[44777,"TRANSGRIDV5_20180116135943","2017-08-27T14:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-18.148710000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[44844,"TRANSGRIDV5_20180116135943","2017-08-27T14:55:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-13.65014,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44874,"TRANSGRIDV5_20180116135943","2017-08-27T06:40:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-24.633610000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44904,"TRANSGRIDV5_20180116135943","2017-08-27T02:55:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-25.670719999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[44971,"TRANSGRIDV5_20180116135943","2017-08-28T10:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-112.78573,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45001,"TRANSGRIDV5_20180116135943","2017-08-28T15:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-43.376710000000003,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45027,"TRANSGRIDV5_20180116135943","2017-08-28T12:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-25.69313,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45098,"TRANSGRIDV5_20180116135943","2017-08-28T09:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-23.49419,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45128,"TRANSGRIDV5_20180116135943","2017-08-28T11:00:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-49.485529999999997,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45154,"TRANSGRIDV5_20180116135943","2017-08-28T14:00:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-10.44589,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45184,"TRANSGRIDV5_20180116135943","2017-08-28T12:50:00","VSML_220","V-NIL","2012-07-04",1,-119.93532,"Vic to SA on ML upper transfer limit of 220 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45255,"TRANSGRIDV5_20180116135943","2017-08-29T04:25:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-30.486080000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45281,"TRANSGRIDV5_20180116135943","2017-08-29T08:40:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-25.14808,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45311,"TRANSGRIDV5_20180116135943","2017-08-29T10:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.07666,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[45378,"TRANSGRIDV5_20180116135943","2017-08-29T08:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.666029999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45408,"TRANSGRIDV5_20180116135943","2017-08-29T09:25:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-18.481190000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45438,"TRANSGRIDV5_20180116135943","2017-08-29T10:00:00","VSML_ZERO","I-ML_ZERO","2013-08-21",1,-12.110150000000001,"Vic to SA on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[45505,"TRANSGRIDV5_20180116135943","2017-08-30T21:00:00","#YABULU_E","#YABULU_E","2017-08-28",1,-88.030670000000001,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45535,"TRANSGRIDV5_20180116135943","2017-08-30T10:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-47.310569999999998,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45561,"TRANSGRIDV5_20180116135943","2017-08-30T12:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-23.57517,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45632,"TRANSGRIDV5_20180116135943","2017-08-30T11:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.39964,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45662,"TRANSGRIDV5_20180116135943","2017-08-30T02:45:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-27.038830000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45688,"TRANSGRIDV5_20180116135943","2017-08-31T15:40:00","#YABULU_E","#YABULU_E","2017-08-28",1,-1087.01713,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45718,"TRANSGRIDV5_20180116135943","2017-08-31T13:00:00","#YABULU_E","#YABULU_E","2017-08-28",1,-1083.73395,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45789,"TRANSGRIDV5_20180116135943","2017-08-31T07:05:00","#YABULU_E","#YABULU_E","2017-08-28",1,-90.917640000000006,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45815,"TRANSGRIDV5_20180116135943","2017-08-31T02:00:00","#YABULU_E","#YABULU_E","2017-08-28",1,-86.656639999999996,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45845,"TRANSGRIDV5_20180116135943","2017-08-31T03:55:00","#YABULU_E","#YABULU_E","2017-08-28",1,-83.730029999999999,"QTYP.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[45881,"TRANSGRIDV5_20180116135943","2017-08-31T11:40:00","F_Q++ARTW_L5","F-N-ARTW_85","2013-08-21",1,13.99,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Armidale 85 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[45941,"TRANSGRIDV5_20180116135943","2017-08-31T02:45:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-11.69279,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[45971,"TRANSGRIDV5_20180116135943","2017-09-01T21:20:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1092.1257900000001,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[46038,"TRANSGRIDV5_20180116135943","2017-09-01T14:30:00","#YABULU_E","#YABULU_E","2017-09-01",1,-1064.8839499999999,"QTYP.ENERGY * 1 <= 100 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[46068,"TRANSGRIDV5_20180116135943","2017-09-01T14:40:00","Q:N_NIL_BI_POT","Q-NIL","2014-01-08",1,-15.742660000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability on trip of a Boyne Island potline (400 + j189 MVA)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46098,"TRANSGRIDV5_20180116135943","2017-09-01T05:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-55.744390000000003,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[46165,"TRANSGRIDV5_20180116135943","2017-09-01T02:20:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-12.8314,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46195,"TRANSGRIDV5_20180116135943","2017-09-02T19:05:00","#PPCCGT_P_E","#PPCCGT_PE","2017-09-02",1,-1089.98975,"SPPT.ENERGY * 1 <= 235 (Wt = 50)","OUTAGE","OTHER","Pelican Point Power Station","REGULATED","99","Non Inclusion",null,0]
[46221,"TRANSGRIDV5_20180116135943","2017-09-02T09:45:00","#PPCCGT_P_E","#PPCCGT_PE","2017-09-02",1,-1087.97669,"SPPT.ENERGY * 1 <= 235 (Wt = 50)","OUTAGE","OTHER","Pelican Point Power Station","REGULATED","99","Non Inclusion",null,0]
[46251,"TRANSGRIDV5_20180116135943","2017-09-02T22:30:00","#PPCCGT_P_E","#PPCCGT_PE","2017-09-02",1,-1084.26899,"SPPT.ENERGY * 1 <= 235 (Wt = 50)","OUTAGE","OTHER","Pelican Point Power Station","REGULATED","99","Non Inclusion",null,0]
[46322,"TRANSGRIDV5_20180116135943","2017-09-02T15:45:00","#PPCCGT_P_E","#PPCCGT_PE","2017-09-02",1,-1063.5801200000001,"SPPT.ENERGY * 1 <= 235 (Wt = 50)","OUTAGE","OTHER","Pelican Point Power Station","REGULATED","99","Non Inclusion",null,0]
[46348,"TRANSGRIDV5_20180116135943","2017-09-02T18:15:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1125.02775,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[46378,"TRANSGRIDV5_20180116135943","2017-09-02T10:25:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1089.99,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[46445,"TRANSGRIDV5_20180116135943","2017-09-02T12:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-34.164569999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[46475,"TRANSGRIDV5_20180116135943","2017-09-02T13:20:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.734760000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[46505,"TRANSGRIDV5_20180116135943","2017-09-02T11:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-24.421279999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46572,"TRANSGRIDV5_20180116135943","2017-09-02T19:55:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-38.056989999999999,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46602,"TRANSGRIDV5_20180116135943","2017-09-03T01:20:00","#PPCCGT_P_E","#PPCCGT_PE","2017-09-02",1,-1059.48433,"SPPT.ENERGY * 1 <= 235 (Wt = 50)","OUTAGE","OTHER","Pelican Point Power Station","REGULATED","99","Non Inclusion",null,0]
[46632,"TRANSGRIDV5_20180116135943","2017-09-03T02:25:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1046.7200800000001,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[46699,"TRANSGRIDV5_20180116135943","2017-09-03T06:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-23.454350000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46729,"TRANSGRIDV5_20180116135943","2017-09-03T13:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-16.505310000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46755,"TRANSGRIDV5_20180116135943","2017-09-03T01:00:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-50.775239999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46785,"TRANSGRIDV5_20180116135943","2017-09-03T08:05:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-47.361449999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46856,"TRANSGRIDV5_20180116135943","2017-09-03T11:10:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-30.819790000000001,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46882,"TRANSGRIDV5_20180116135943","2017-09-03T16:15:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-15.77084,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[46912,"TRANSGRIDV5_20180116135943","2017-09-04T10:35:00","#WRWF1_E","#WRWF1_E","2017-07-06",2,-95.990369999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[46979,"TRANSGRIDV5_20180116135943","2017-09-04T14:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-12.75442,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47009,"TRANSGRIDV5_20180116135943","2017-09-05T21:00:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1094.7543599999999,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47039,"TRANSGRIDV5_20180116135943","2017-09-05T23:55:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1075.2746,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47106,"TRANSGRIDV5_20180116135943","2017-09-05T10:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.300269999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47136,"TRANSGRIDV5_20180116135943","2017-09-05T02:45:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-15.518050000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47166,"TRANSGRIDV5_20180116135943","2017-09-06T18:25:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1161.4341400000001,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47192,"TRANSGRIDV5_20180116135943","2017-09-06T08:50:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1109.74578,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47263,"TRANSGRIDV5_20180116135943","2017-09-06T12:20:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1084.6710800000001,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47289,"TRANSGRIDV5_20180116135943","2017-09-06T13:45:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1080.8999100000001,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47319,"TRANSGRIDV5_20180116135943","2017-09-06T13:15:00","#WATERLWF_E","#WATERLWF_E","2017-09-01",1,-1078.69031,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47384,"TRANSGRIDV5_20180116135943","2017-09-06T05:05:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-27.35181,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[47415,"TRANSGRIDV5_20180116135943","2017-09-06T07:45:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-17.68441,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[47445,"TRANSGRIDV5_20180116135943","2017-09-06T16:30:00","SVML_ZERO","I-ML_ZERO","2013-08-21",1,-14.346780000000001,"SA to Vic on ML upper transfer limit of 0 MW","OUTAGE","OTHER","Murrylnk-V Murrylnk-S 165kV LINE","REGULATED","99","Non Inclusion",null,0]
[47516,"TRANSGRIDV5_20180116135943","2017-09-06T03:25:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-18.966339999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47542,"TRANSGRIDV5_20180116135943","2017-09-06T05:35:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-24.204630000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47572,"TRANSGRIDV5_20180116135943","2017-09-07T10:55:00","#WATERLWF_E","#WATERLWF_E","2017-09-07",1,-1085.6287199999999,"SWLE.ENERGY * 1 <= 80 (Wt = 360)","OUTAGE","OTHER","Waterloo Wind Farm","REGULATED","99","Non Inclusion",null,0]
[47639,"TRANSGRIDV5_20180116135943","2017-09-07T10:35:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-27.930810000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[47669,"TRANSGRIDV5_20180116135943","2017-09-07T11:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.58419,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[47699,"TRANSGRIDV5_20180116135943","2017-09-07T10:55:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-18.064319999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47725,"TRANSGRIDV5_20180116135943","2017-09-07T11:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.87083,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47796,"TRANSGRIDV5_20180116135943","2017-09-08T21:10:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.680720000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47822,"TRANSGRIDV5_20180116135943","2017-09-08T06:20:00","N_TARALGAWF_ZERO","N-TARALGAWF_ZERO","2014-12-10",1,-1093.7904100000001,"Taralga WF upper limit of 0 MW","OUTAGE","OTHER","TARALGA WIND FARM","REGULATED","99","Non Inclusion",null,0]
[47852,"TRANSGRIDV5_20180116135943","2017-09-08T10:05:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.58419,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[47923,"TRANSGRIDV5_20180116135943","2017-09-08T10:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-14.004960000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[47949,"TRANSGRIDV5_20180116135943","2017-09-09T06:20:00","#R016125_013_RAMP_F","#R016125_RAMP","2017-09-08",1,-13.84407,"Hard Ramping constraint for constraint V^SML_BAWB_3, Effective Date: 20/07/2017, Version: 1","OUTAGE","RAMP","Ballart220-Waubra 220kV LINE","REGULATED","10","Ramping Constraint","PLANNED",0]
[47979,"TRANSGRIDV5_20180116135943","2017-09-09T12:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-38.993099999999998,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48050,"TRANSGRIDV5_20180116135943","2017-09-09T14:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.629760000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48076,"TRANSGRIDV5_20180116135943","2017-09-09T12:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-29.456440000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48106,"TRANSGRIDV5_20180116135943","2017-09-09T09:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-19.874659999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48173,"TRANSGRIDV5_20180116135943","2017-09-10T10:35:00","N^^V_LTWG","N-LTWG_RADIAL","2015-08-07",1,-20.12285,"Out = Lower Tumut to Wagga 330 kV line, avoid voltage collapse in Southern NSW for either loss of the largest VIC generating unit or Basslink, or loss of a Murray to Dederang 330 kV line","OUTAGE","OTHER","Lwr Tumut Wagga 051 330kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[48203,"TRANSGRIDV5_20180116135943","2017-09-10T12:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.841470000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48233,"TRANSGRIDV5_20180116135943","2017-09-10T14:50:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-21.66572,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48259,"TRANSGRIDV5_20180116135943","2017-09-10T15:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-16.33389,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48330,"TRANSGRIDV5_20180116135943","2017-09-10T11:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.81462,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48356,"TRANSGRIDV5_20180116135943","2017-09-11T09:10:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-1074.57745,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm 3","REGULATED","99","Non Inclusion",null,0]
[48386,"TRANSGRIDV5_20180116135943","2017-09-11T11:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-17.557089999999999,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48457,"TRANSGRIDV5_20180116135943","2017-09-11T02:05:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-21.026700000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48483,"TRANSGRIDV5_20180116135943","2017-09-11T01:10:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-14.67693,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[48513,"TRANSGRIDV5_20180116135943","2017-09-12T10:00:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-22.512820000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE; Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[48584,"TRANSGRIDV5_20180116135943","2017-09-13T05:35:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-88.597899999999996,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48610,"TRANSGRIDV5_20180116135943","2017-09-13T02:05:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-74.970349999999996,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48640,"TRANSGRIDV5_20180116135943","2017-09-13T15:15:00","V::N_KGRC_V2","V-KGRC","2017-04-07",1,-12.7027,"Out = Kerang to Red Cliffs 220kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Kerang-Wemen 220kV LINE","REGULATED","99","Non Inclusion",null,0,"Ausnet"]
[48707,"TRANSGRIDV5_20180116135943","2017-09-14T19:05:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-146.99761000000001,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48737,"TRANSGRIDV5_20180116135943","2017-09-14T07:00:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-101.70774,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48767,"TRANSGRIDV5_20180116135943","2017-09-14T08:15:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-90.429540000000003,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48797,"TRANSGRIDV5_20180116135943","2017-09-14T11:55:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-87.960499999999996,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48863,"TRANSGRIDV5_20180116135943","2017-09-14T11:25:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-87.000479999999996,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48893,"TRANSGRIDV5_20180116135943","2017-09-14T16:35:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-80.150580000000005,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48919,"TRANSGRIDV5_20180116135943","2017-09-14T03:50:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-66.064070000000001,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[48990,"TRANSGRIDV5_20180116135943","2017-09-14T03:20:00","V>>V_NIL_2A_R","V-NIL_RADIAL","2017-04-10",1,-11.93929,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 500kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49016,"TRANSGRIDV5_20180116135943","2017-09-15T05:30:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-89.45729,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[49046,"TRANSGRIDV5_20180116135943","2017-09-15T01:45:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-85.453339999999997,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[49076,"TRANSGRIDV5_20180116135943","2017-09-15T04:25:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-69.950220000000002,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[49143,"TRANSGRIDV5_20180116135943","2017-09-16T12:35:00","#WRWF1_E","#WRWF1_E","2017-09-12",1,-86.455340000000007,"NWRK1W.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[49173,"TRANSGRIDV5_20180116135943","2017-09-16T10:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.56218,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[49199,"TRANSGRIDV5_20180116135943","2017-09-16T10:10:00","Q:N_AR_CP2_AR_2L-G","N-AR_CP2","2014-01-08",1,-14.880839999999999,"Out = Armidale capacitor bank (120MVAr), limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale 3 330/138kV XFMR","REGULATED","INCLUDED","","PLANNED",1]
[49270,"TRANSGRIDV5_20180116135943","2017-09-17T08:40:00","#QPS5_P_E","#QPS5_PE","2017-09-17",1,-1070.80675,"SQPS5Q.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Quarantine GT","REGULATED","99","Non Inclusion",null,0]
[49300,"TRANSGRIDV5_20180116135943","2017-09-17T05:20:00","S>>X_CNRB+CB_02","S-X_CNRB+CB","2017-07-04",1,-129.04936000000001,"Out= Canowie-Robertstown 275kV line + Associated line CBs 6616 & 6571  at Robertstown O/S), avoid O/L Waterloo East-MWP4-Robertstown 132kV line on trip of Mokota-Robertstown 275kV line(this offloads Robertstown #1 275/132kV TX and Trips Hallet Hill WF)","OUTAGE","OTHER","Canowie Robertstwn 275kV LINE","REGULATED","99","Non Inclusion",null,0,"Electranet outage"]
[49326,"TRANSGRIDV5_20180116135943","2017-09-17T22:45:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-21.840920000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49397,"TRANSGRIDV5_20180116135943","2017-09-18T14:00:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-55.121679999999998,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49427,"TRANSGRIDV5_20180116135943","2017-09-19T23:40:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-13.63537,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49453,"TRANSGRIDV5_20180116135943","2017-09-21T04:20:00","V::N_NIL_V1","V-NIL","2017-04-07",1,-27.593419999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[49524,"TRANSGRIDV5_20180116135943","2017-09-22T22:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-84.268249999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[49550,"TRANSGRIDV5_20180116135943","2017-09-22T15:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.327950000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[49580,"TRANSGRIDV5_20180116135943","2017-09-22T15:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.869029999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[49610,"TRANSGRIDV5_20180116135943","2017-09-22T13:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-72.874459999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[49677,"TRANSGRIDV5_20180116135943","2017-09-23T17:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1070.9149,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[49707,"TRANSGRIDV5_20180116135943","2017-09-23T21:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1063.99109,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[49737,"TRANSGRIDV5_20180116135943","2017-09-23T19:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1060.4216899999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[49804,"TRANSGRIDV5_20180116135943","2017-09-23T15:25:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1006.50012,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[49834,"TRANSGRIDV5_20180116135943","2017-09-23T18:35:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1075.24046,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[49860,"TRANSGRIDV5_20180116135943","2017-09-23T14:50:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1068.52541,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[49931,"TRANSGRIDV5_20180116135943","2017-09-23T16:00:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1061.8026199999999,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[49961,"TRANSGRIDV5_20180116135943","2017-09-23T12:25:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1059.05828,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[49987,"TRANSGRIDV5_20180116135943","2017-09-23T21:10:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1055.3835799999999,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50058,"TRANSGRIDV5_20180116135943","2017-09-23T05:25:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1028.2911899999999,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50084,"TRANSGRIDV5_20180116135943","2017-09-23T16:25:00","#TORRB4_P_E","#TORRB4_PE","2017-09-23",3,-1066.74811,"STSB4.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50114,"TRANSGRIDV5_20180116135943","2017-09-23T18:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.73021,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50144,"TRANSGRIDV5_20180116135943","2017-09-23T22:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.2,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50211,"TRANSGRIDV5_20180116135943","2017-09-23T00:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.49615,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50241,"TRANSGRIDV5_20180116135943","2017-09-23T19:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.77,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50300,"TRANSGRIDV5_20180116135943","2017-09-23T04:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.78,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50337,"TRANSGRIDV5_20180116135943","2017-09-23T06:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.730040000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50367,"TRANSGRIDV5_20180116135943","2017-09-23T02:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.730020000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[50393,"TRANSGRIDV5_20180116135943","2017-09-23T06:10:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-37.091670000000001,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[50464,"TRANSGRIDV5_20180116135943","2017-09-23T09:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-21.264779999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[50494,"TRANSGRIDV5_20180116135943","2017-09-23T04:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-31.588539999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[50520,"TRANSGRIDV5_20180116135943","2017-09-23T03:40:00","V::N_NIL_V1","V-NIL","2017-04-07",1,-56.852379999999997,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[50591,"TRANSGRIDV5_20180116135943","2017-09-24","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1065.1935699999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50617,"TRANSGRIDV5_20180116135943","2017-09-24T17:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1059.19191,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50647,"TRANSGRIDV5_20180116135943","2017-09-24T07:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1044.9060999999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50677,"TRANSGRIDV5_20180116135943","2017-09-24T10:45:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1042.0100399999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50744,"TRANSGRIDV5_20180116135943","2017-09-24T06:00:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1008.5348300000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50774,"TRANSGRIDV5_20180116135943","2017-09-24T09:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-1007.33513,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50804,"TRANSGRIDV5_20180116135943","2017-09-24T11:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-09-23",1,-997.15491999999995,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[50871,"TRANSGRIDV5_20180116135943","2017-09-24T16:30:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1042.6067,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50901,"TRANSGRIDV5_20180116135943","2017-09-24T11:00:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1040.8779300000001,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50927,"TRANSGRIDV5_20180116135943","2017-09-24T04:40:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-1020.56004,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[50998,"TRANSGRIDV5_20180116135943","2017-09-24T14:15:00","#TORRB2_P_E","#TORRB2_PE","2017-09-23",1,-997.45441000000005,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[51028,"TRANSGRIDV5_20180116135943","2017-09-24T18:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.730199999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51054,"TRANSGRIDV5_20180116135943","2017-09-24T21:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.868830000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51084,"TRANSGRIDV5_20180116135943","2017-09-24T22:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-75.192620000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51155,"TRANSGRIDV5_20180116135943","2017-09-24T12:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-65.00412,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51181,"TRANSGRIDV5_20180116135943","2017-09-24T06:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.78,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51211,"TRANSGRIDV5_20180116135943","2017-09-24T10:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-62.697920000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51278,"TRANSGRIDV5_20180116135943","2017-09-24T05:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.729950000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51308,"TRANSGRIDV5_20180116135943","2017-09-24T12:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-32.224980000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51338,"TRANSGRIDV5_20180116135943","2017-09-24T04:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-25.873719999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51405,"TRANSGRIDV5_20180116135943","2017-09-24T11:05:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.571760000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51435,"TRANSGRIDV5_20180116135943","2017-09-24T04:20:00","V::N_NIL_V1","V-NIL","2017-04-07",1,-39.67577,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51461,"TRANSGRIDV5_20180116135943","2017-09-24T07:45:00","V::N_NIL_V1","V-NIL","2017-04-07",1,-10.50614,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51532,"TRANSGRIDV5_20180116135943","2017-09-24T06:00:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-25.712,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51562,"TRANSGRIDV5_20180116135943","2017-09-24T20:10:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-11.74381,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51588,"TRANSGRIDV5_20180116135943","2017-09-24T00:30:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-11.03586,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[51618,"TRANSGRIDV5_20180116135943","2017-09-25T16:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-100.29013,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51689,"TRANSGRIDV5_20180116135943","2017-09-25T09:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-84.223529999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51715,"TRANSGRIDV5_20180116135943","2017-09-25T16:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.545259999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51779,"TRANSGRIDV5_20180116135943","2017-09-25T05:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-76.704350000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51811,"TRANSGRIDV5_20180116135943","2017-09-25T12:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-74.273079999999993,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51841,"TRANSGRIDV5_20180116135943","2017-09-25T00:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-67.350579999999994,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51871,"TRANSGRIDV5_20180116135943","2017-09-25T01:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.730130000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51938,"TRANSGRIDV5_20180116135943","2017-09-26T15:50:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-146.21,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[51968,"TRANSGRIDV5_20180116135943","2017-09-26T17:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-119.99,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[51998,"TRANSGRIDV5_20180116135943","2017-09-26T20:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-109.3785,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52065,"TRANSGRIDV5_20180116135943","2017-09-26T23:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-94.233999999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52095,"TRANSGRIDV5_20180116135943","2017-09-26T07:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-89.453460000000007,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52121,"TRANSGRIDV5_20180116135943","2017-09-26T20:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-86.667199999999994,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52151,"TRANSGRIDV5_20180116135943","2017-09-26T21:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.914360000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52222,"TRANSGRIDV5_20180116135943","2017-09-26T01:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-69.186909999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52248,"TRANSGRIDV5_20180116135943","2017-09-26T15:15:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-13.8009,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[52278,"TRANSGRIDV5_20180116135943","2017-09-27T07:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-249,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52345,"TRANSGRIDV5_20180116135943","2017-09-27T15:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-98.449129999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52375,"TRANSGRIDV5_20180116135943","2017-09-27T12:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-94.626450000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52405,"TRANSGRIDV5_20180116135943","2017-09-27T17:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-91.244349999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52472,"TRANSGRIDV5_20180116135943","2017-09-27T16:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-80.266779999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52502,"TRANSGRIDV5_20180116135943","2017-09-27T02:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.98921,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52532,"TRANSGRIDV5_20180116135943","2017-09-27T19:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.926640000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52599,"TRANSGRIDV5_20180116135943","2017-09-27T14:20:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-11.745979999999999,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[52629,"TRANSGRIDV5_20180116135943","2017-09-27T04:40:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-19.004799999999999,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[52655,"TRANSGRIDV5_20180116135943","2017-09-27T04:00:00","V>>V_NIL_2_TIE","V-NIL_HW_TIE","2017-08-15",1,-16.186630000000001,"Out = Nil, avoid pre-contingent O/L of the South Morang F2 500/330 kV transformer, Yallourn unit 1 in 220kV mode, all 220kV buses tied at Hazelwood, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[52685,"TRANSGRIDV5_20180116135943","2017-09-28T06:25:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-135.52287000000001,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[52756,"TRANSGRIDV5_20180116135943","2017-09-28T23:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-104.35039999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52782,"TRANSGRIDV5_20180116135943","2017-09-28T13:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.730140000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52812,"TRANSGRIDV5_20180116135943","2017-09-28T08:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.910499999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52879,"TRANSGRIDV5_20180116135943","2017-09-28T10:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.673730000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52909,"TRANSGRIDV5_20180116135943","2017-09-28T00:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-74.224950000000007,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[52939,"TRANSGRIDV5_20180116135943","2017-09-28T00:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.989999999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53006,"TRANSGRIDV5_20180116135943","2017-09-28T18:25:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-154.36131,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[53036,"TRANSGRIDV5_20180116135943","2017-09-28T17:15:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2017-08-11",1,-154.65447,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[53066,"TRANSGRIDV5_20180116135943","2017-09-28T00:40:00","V::N_NIL_S1","V-NIL","2017-04-07",1,-29.402660000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[53092,"TRANSGRIDV5_20180116135943","2017-09-28T03:25:00","V>>V_NIL_2B_R","V-NIL_RADIAL","2017-04-10",1,-24.872420000000002,"Out = Nil, avoid pre-contingent O/L of South Morang F2 500/330kV transformer, radial mode, YWPS unit 1 on 220kV,  feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[53163,"TRANSGRIDV5_20180116135943","2017-09-29T18:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-85.504829999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53189,"TRANSGRIDV5_20180116135943","2017-09-29T22:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.950090000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53218,"TRANSGRIDV5_20180116135943","2017-09-29T14:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.885339999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53289,"TRANSGRIDV5_20180116135943","2017-09-29T20:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.347480000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53315,"TRANSGRIDV5_20180116135943","2017-09-29T08:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.919139999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53345,"TRANSGRIDV5_20180116135943","2017-09-29T23:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-75.366140000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53416,"TRANSGRIDV5_20180116135943","2017-09-29T02:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.78,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53442,"TRANSGRIDV5_20180116135943","2017-09-29T11:55:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-56.253779999999999,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[53472,"TRANSGRIDV5_20180116135943","2017-09-29T14:45:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-55.223300000000002,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[53539,"TRANSGRIDV5_20180116135943","2017-09-29T18:00:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-28.223610000000001,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[53569,"TRANSGRIDV5_20180116135943","2017-09-29T21:00:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-21.26632,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[53599,"TRANSGRIDV5_20180116135943","2017-09-29T02:30:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-13.1347,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[53625,"TRANSGRIDV5_20180116135943","2017-09-29T07:55:00","V::N_SMF2_SD2","V-SMTXF2_R","2017-04-07",1,-77.838399999999993,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates, YPS G1 on 500kV. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[53696,"TRANSGRIDV5_20180116135943","2017-09-29T14:55:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-61.798340000000003,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[53722,"TRANSGRIDV5_20180116135943","2017-09-29T13:20:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-48.27055,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[53752,"TRANSGRIDV5_20180116135943","2017-09-29T18:10:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-28.197839999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[53823,"TRANSGRIDV5_20180116135943","2017-09-30T11:40:00","#R016228_001_RAMP_V","#R016228_RAMP","2017-09-30",1,-19.543279999999999,"Soft Ramping constraint for constraint S>V_CB6033+6225_TX2, Effective Date: 21/07/2015, Version: 1","OUTAGE","RAMP","N_W_Bend 6225 132kV CB ;N_W_B 6033 132kV CB","REGULATED","10","Ramping Constraint","PLANNED",0]
[53849,"TRANSGRIDV5_20180116135943","2017-09-30T18:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-148.82218,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53879,"TRANSGRIDV5_20180116135943","2017-09-30T17:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.414969999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53950,"TRANSGRIDV5_20180116135943","2017-09-30T23:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-76.349310000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[53976,"TRANSGRIDV5_20180116135943","2017-09-30T14:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-72.856160000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54006,"TRANSGRIDV5_20180116135943","2017-09-30T09:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-71.336749999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54073,"TRANSGRIDV5_20180116135943","2017-09-30T02:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54103,"TRANSGRIDV5_20180116135943","2017-09-30T10:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.78,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54133,"TRANSGRIDV5_20180116135943","2017-09-30T01:15:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-54.274929999999998,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54159,"TRANSGRIDV5_20180116135943","2017-09-30T03:20:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-43.852069999999998,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54230,"TRANSGRIDV5_20180116135943","2017-09-30T06:30:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-11.52167,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54256,"TRANSGRIDV5_20180116135943","2017-09-30T17:50:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-24.665230000000001,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","OUTAGE","OTHER","N_W_B 6033 132kV CB; N_W_Bend 6225 132kV CB; N_W_Bend 3 132/66kV XFMR","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54286,"TRANSGRIDV5_20180116135943","2017-09-30T13:40:00","S>V_CB6033+6225_TX2","S-NWCB6033+6225","2015-07-21",1,-16.1021,"Out= North West Bend_CB6033 and CB6225;  avoid O/L of North West Bend transformer 132/66kV #2 on trip of either Robertstown-NWB #2 132kV line or NWB-Monash #2 132kV line .","OUTAGE","OTHER","N_W_B 6033 132kV CB; N_W_Bend 6225 132kV CB; N_W_Bend 3 132/66kV XFMR","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54357,"TRANSGRIDV5_20180116135943","2017-09-30T00:40:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-35.797719999999998,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54383,"TRANSGRIDV5_20180116135943","2017-09-30T22:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-25.288820000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54413,"TRANSGRIDV5_20180116135943","2017-09-30T15:20:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-23.115860000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54484,"TRANSGRIDV5_20180116135943","2017-09-30T07:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-14.79034,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54510,"TRANSGRIDV5_20180116135943","2017-10-01T18:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.710130000000007,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54540,"TRANSGRIDV5_20180116135943","2017-10-01T23:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-73.720100000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54607,"TRANSGRIDV5_20180116135943","2017-10-01T21:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.048349999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54637,"TRANSGRIDV5_20180116135943","2017-10-01T10:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-69.366770000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54655,"TRANSGRIDV5_20180116135943","2017-10-01T10:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-68.861620000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54692,"TRANSGRIDV5_20180116135943","2017-10-01T14:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-66.023560000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54763,"TRANSGRIDV5_20180116135943","2017-10-01T05:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-63.187779999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[54793,"TRANSGRIDV5_20180116135943","2017-10-01T00:55:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-18.106829999999999,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54819,"TRANSGRIDV5_20180116135943","2017-10-01T06:15:00","S>NWBCB6225_TX1","S-NWB_CB6225","2017-08-02",1,-14.061389999999999,"Out= North West Bend 132kV CB6225, avoid O/L of North West Bend 66/132kV TX1  on trip of North West Bend-Monash #2 132kV line, Feedback","OUTAGE","OTHER","N_W_Bend 6225 132kV CB","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[54890,"TRANSGRIDV5_20180116135943","2017-10-01T00:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-25.477360000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR;","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54916,"TRANSGRIDV5_20180116135943","2017-10-01T06:05:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-19.570460000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR;","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54946,"TRANSGRIDV5_20180116135943","2017-10-01T03:55:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-14.63781,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR;","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[54976,"TRANSGRIDV5_20180116135943","2017-10-02T18:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-249,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55043,"TRANSGRIDV5_20180116135943","2017-10-02T20:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.760710000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55073,"TRANSGRIDV5_20180116135943","2017-10-02T21:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.23724,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55099,"TRANSGRIDV5_20180116135943","2017-10-02T15:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.730869999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55170,"TRANSGRIDV5_20180116135943","2017-10-02T07:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-69.755250000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55200,"TRANSGRIDV5_20180116135943","2017-10-02T06:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55226,"TRANSGRIDV5_20180116135943","2017-10-02T02:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-61.491010000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55297,"TRANSGRIDV5_20180116135943","2017-10-02T00:15:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-11.050929999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[55327,"TRANSGRIDV5_20180116135943","2017-10-03T23:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-106.79,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55353,"TRANSGRIDV5_20180116135943","2017-10-03T14:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-96.346739999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55424,"TRANSGRIDV5_20180116135943","2017-10-03T17:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-91.899850000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55450,"TRANSGRIDV5_20180116135943","2017-10-03T19:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-87.666049999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55480,"TRANSGRIDV5_20180116135943","2017-10-03T20:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-85.308239999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55510,"TRANSGRIDV5_20180116135943","2017-10-03T11:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.703720000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55577,"TRANSGRIDV5_20180116135943","2017-10-03T03:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-72.899060000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55607,"TRANSGRIDV5_20180116135943","2017-10-03T20:10:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-17.33464,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[55637,"TRANSGRIDV5_20180116135943","2017-10-04T14:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-249,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55704,"TRANSGRIDV5_20180116135943","2017-10-04T18:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-97.934560000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55734,"TRANSGRIDV5_20180116135943","2017-10-04T06:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-95.729920000000007,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55760,"TRANSGRIDV5_20180116135943","2017-10-04T22:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-94.224509999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55831,"TRANSGRIDV5_20180116135943","2017-10-04T14:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.99,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55861,"TRANSGRIDV5_20180116135943","2017-10-04T02:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.664689999999993,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55887,"TRANSGRIDV5_20180116135943","2017-10-04T04:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-77.138490000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[55958,"TRANSGRIDV5_20180116135943","2017-10-04T11:10:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-36.011400000000002,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[55984,"TRANSGRIDV5_20180116135943","2017-10-04T04:05:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-35.287419999999997,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[56014,"TRANSGRIDV5_20180116135943","2017-10-04T02:40:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-25.107250000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[56044,"TRANSGRIDV5_20180116135943","2017-10-04T20:45:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-16.94773,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[56111,"TRANSGRIDV5_20180116135943","2017-10-05T15:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-105.03588000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56134,"TRANSGRIDV5_20180116135943","2017-10-05T14:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-94.983710000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56170,"TRANSGRIDV5_20180116135943","2017-10-05T09:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-90.747960000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56237,"TRANSGRIDV5_20180116135943","2017-10-05T13:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.720249999999993,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56267,"TRANSGRIDV5_20180116135943","2017-10-05T11:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-79.256079999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56293,"TRANSGRIDV5_20180116135943","2017-10-05T21:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.21763,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56364,"TRANSGRIDV5_20180116135943","2017-10-05T01:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.675730000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56394,"TRANSGRIDV5_20180116135943","2017-10-05T07:45:00","N_BOCORWF1_ZERO","N-BOCORWF1_ZERO","2014-08-27",1,-1057.8412699999999,"Boco Rock WF upper limit of 0 MW","OUTAGE","OTHER","CoomaNew-BegaTG-StepleFlat 97R 132kV LINE","REGULATED","11","Transmission connection agreements where a lower service standard has been negotiated giving the TNSP the right to disrupt service under certain network conditions where the constraint only affects the parties subject to the agreement.","PLANNED",0,"Please refer to explanatory statement in attachments"]
[56420,"TRANSGRIDV5_20180116135943","2017-10-05T20:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-30.843879999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[56491,"TRANSGRIDV5_20180116135943","2017-10-05T15:30:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-34.362110000000001,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet"]
[56517,"TRANSGRIDV5_20180116135943","2017-10-06T06:15:00","#R016252_049_RAMP_F","#R016252_RAMP","2017-10-06",1,-111.29,"Hard Ramping constraint for constraint T>T_GTSH_IMP_4K, Effective Date: 21/08/2013, Version: 1","OUTAGE","RAMP","Sheffield to Georgetown 220 kV line","REGULATED","10","Ramping Constraint","PLANNED",0]
[56547,"TRANSGRIDV5_20180116135943","2017-10-06T16:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-249,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56577,"TRANSGRIDV5_20180116135943","2017-10-06T22:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-131.27164999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56644,"TRANSGRIDV5_20180116135943","2017-10-06T11:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.224540000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56674,"TRANSGRIDV5_20180116135943","2017-10-06T13:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.30856,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56704,"TRANSGRIDV5_20180116135943","2017-10-06T13:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.430149999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56771,"TRANSGRIDV5_20180116135943","2017-10-06T05:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-68.486159999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56801,"TRANSGRIDV5_20180116135943","2017-10-06T02:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.989999999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[56827,"TRANSGRIDV5_20180116135943","2017-10-06T16:55:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-157.90869000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[56898,"TRANSGRIDV5_20180116135943","2017-10-06T22:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-36.535600000000002,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[56928,"TRANSGRIDV5_20180116135943","2017-10-06T11:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.400399999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[56954,"TRANSGRIDV5_20180116135943","2017-10-06T15:10:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-57.681370000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[56984,"TRANSGRIDV5_20180116135943","2017-10-06T03:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-45.740519999999997,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57055,"TRANSGRIDV5_20180116135943","2017-10-06T12:45:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-16.396889999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57081,"TRANSGRIDV5_20180116135943","2017-10-06T00:55:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-12.97113,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57111,"TRANSGRIDV5_20180116135943","2017-10-07T05:00:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-117.58838,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[57178,"TRANSGRIDV5_20180116135943","2017-10-07T16:20:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-1039.3335099999999,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[57208,"TRANSGRIDV5_20180116135943","2017-10-07T21:45:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-50.69,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[57238,"TRANSGRIDV5_20180116135943","2017-10-07T08:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-209.3895,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57305,"TRANSGRIDV5_20180116135943","2017-10-07T14:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-82.938000000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57335,"TRANSGRIDV5_20180116135943","2017-10-07T17:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.609440000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57361,"TRANSGRIDV5_20180116135943","2017-10-07T20:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-80.502989999999997,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57432,"TRANSGRIDV5_20180116135943","2017-10-07T01:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-73.720029999999994,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57462,"TRANSGRIDV5_20180116135943","2017-10-07T02:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-71.114750000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57488,"TRANSGRIDV5_20180116135943","2017-10-07T05:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-68.868290000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[57518,"TRANSGRIDV5_20180116135943","2017-10-07T15:45:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-153.64116999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[57589,"TRANSGRIDV5_20180116135943","2017-10-07T00:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-26.672499999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[57613,"TRANSGRIDV5_20180116135943","2017-10-07T09:10:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-23.180959999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[57644,"TRANSGRIDV5_20180116135943","2017-10-07T09:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-17.73001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[57711,"TRANSGRIDV5_20180116135943","2017-10-07T15:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-68.269779999999997,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57741,"TRANSGRIDV5_20180116135943","2017-10-07T09:00:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-53.632069999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57771,"TRANSGRIDV5_20180116135943","2017-10-07T09:10:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-43.272359999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57838,"TRANSGRIDV5_20180116135943","2017-10-07T04:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-28.72362,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57868,"TRANSGRIDV5_20180116135943","2017-10-07T07:00:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-22.704270000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57894,"TRANSGRIDV5_20180116135943","2017-10-07T08:55:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-15.214079999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[57965,"TRANSGRIDV5_20180116135943","2017-10-08T08:25:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-72.059709999999995,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[57995,"TRANSGRIDV5_20180116135943","2017-10-08T16:20:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-67.86421,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[58021,"TRANSGRIDV5_20180116135943","2017-10-08T10:40:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-60.693600000000004,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[58051,"TRANSGRIDV5_20180116135943","2017-10-08T02:15:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-52.521540000000002,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[58122,"TRANSGRIDV5_20180116135943","2017-10-08T11:30:00","#TORRB2_P_E","#TORRB2_PE","2017-10-07",1,-28.829440000000002,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[58148,"TRANSGRIDV5_20180116135943","2017-10-08T22:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-113.02495,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58178,"TRANSGRIDV5_20180116135943","2017-10-08T18:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-84.815939999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58245,"TRANSGRIDV5_20180116135943","2017-10-08T12:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-76.270709999999994,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58275,"TRANSGRIDV5_20180116135943","2017-10-08T15:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-74.167810000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58305,"TRANSGRIDV5_20180116135943","2017-10-08T23:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-71.7684,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58372,"TRANSGRIDV5_20180116135943","2017-10-08T08:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.990030000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58402,"TRANSGRIDV5_20180116135943","2017-10-08T03:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58432,"TRANSGRIDV5_20180116135943","2017-10-08T00:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-20.94876,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[58499,"TRANSGRIDV5_20180116135943","2017-10-08T03:45:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-13.6534,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[58529,"TRANSGRIDV5_20180116135943","2017-10-08T11:25:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-55.740299999999998,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[58555,"TRANSGRIDV5_20180116135943","2017-10-08T14:30:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-28.837599999999998,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[58585,"TRANSGRIDV5_20180116135943","2017-10-09T02:15:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-126.19823,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[58656,"TRANSGRIDV5_20180116135943","2017-10-09T14:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-104.73157999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58682,"TRANSGRIDV5_20180116135943","2017-10-09T07:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-99.554919999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58712,"TRANSGRIDV5_20180116135943","2017-10-09T06:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-95.78501,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58779,"TRANSGRIDV5_20180116135943","2017-10-09T20:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.9358,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58809,"TRANSGRIDV5_20180116135943","2017-10-09T11:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.999750000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58839,"TRANSGRIDV5_20180116135943","2017-10-09T11:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-73.720410000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[58906,"TRANSGRIDV5_20180116135943","2017-10-09T18:35:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-29.652429999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[58936,"TRANSGRIDV5_20180116135943","2017-10-09T18:00:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-16.053750000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[58966,"TRANSGRIDV5_20180116135943","2017-10-09T07:20:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-12.79646,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[58992,"TRANSGRIDV5_20180116135943","2017-10-09T17:25:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.569660000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[59050,"TRANSGRIDV5_20180116135943","2017-10-09T02:00:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-10.653930000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[59088,"TRANSGRIDV5_20180116135943","2017-10-09T04:15:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-13.612740000000001,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[59118,"TRANSGRIDV5_20180116135943","2017-10-10T21:50:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-118.79185,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[59189,"TRANSGRIDV5_20180116135943","2017-10-10T17:35:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-101.48166000000001,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59215,"TRANSGRIDV5_20180116135943","2017-10-10T05:55:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-92.700370000000007,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59245,"TRANSGRIDV5_20180116135943","2017-10-10T10:45:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-85.529970000000006,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59316,"TRANSGRIDV5_20180116135943","2017-10-10T11:45:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-74.759469999999993,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59342,"TRANSGRIDV5_20180116135943","2017-10-10T19:10:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-69.433449999999993,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59372,"TRANSGRIDV5_20180116135943","2017-10-10T19:45:00","#TORRB2_P_E","#TORRB2_PE","2017-10-09",3,-66,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[59439,"TRANSGRIDV5_20180116135943","2017-10-10T23:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-91.183400000000006,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[59469,"TRANSGRIDV5_20180116135943","2017-10-10T18:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-197.77,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59499,"TRANSGRIDV5_20180116135943","2017-10-10T16:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-125.32375,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59525,"TRANSGRIDV5_20180116135943","2017-10-10T06:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-106.55222000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59596,"TRANSGRIDV5_20180116135943","2017-10-10T13:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-95.131619999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59622,"TRANSGRIDV5_20180116135943","2017-10-10T08:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-91.414150000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59652,"TRANSGRIDV5_20180116135943","2017-10-10T19:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-84.521050000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59723,"TRANSGRIDV5_20180116135943","2017-10-10T02:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.127020000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[59749,"TRANSGRIDV5_20180116135943","2017-10-10T12:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-33.94164,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[59779,"TRANSGRIDV5_20180116135943","2017-10-10T15:45:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-20.473179999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[59850,"TRANSGRIDV5_20180116135943","2017-10-10T13:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.29884,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[59876,"TRANSGRIDV5_20180116135943","2017-10-10T18:20:00","N>>N-NIL__3_OPENED","N-NIL_RBKU_OPENED","2017-08-11",1,-29.213429999999999,"Out= Nil, avoid O/L Liddell to Muswellbrook (83) using 15 mins rating on trip of Liddell to Tamworth (84) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[59906,"TRANSGRIDV5_20180116135943","2017-10-10T22:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-133.46614,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[59973,"TRANSGRIDV5_20180116135943","2017-10-11T06:25:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-1024.43237,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[60003,"TRANSGRIDV5_20180116135943","2017-10-11T05:00:00","#TORRA1_P_E","#TORRA1_PE","2017-10-11",1,-65.496319999999997,"STSA1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60033,"TRANSGRIDV5_20180116135943","2017-10-11T04:40:00","#TORRA1_P_E","#TORRA1_PE","2017-10-11",1,-30.853580000000001,"STSA1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60059,"TRANSGRIDV5_20180116135943","2017-10-11T03:15:00","#TORRA1_P_E","#TORRA1_PE","2017-10-11",1,-15.81836,"STSA1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60130,"TRANSGRIDV5_20180116135943","2017-10-11T04:25:00","#TORRA2_P_E","#TORRA2_PE","2017-10-11",1,-18.025970000000001,"STSA2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60156,"TRANSGRIDV5_20180116135943","2017-10-11T06:55:00","#TORRA4_P_E","#TORRA4_PE","2017-10-11",1,-1065.12176,"STSA4.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60186,"TRANSGRIDV5_20180116135943","2017-10-11T00:50:00","#TORRA4_P_E","#TORRA4_PE","2017-10-11",1,-41.835590000000003,"STSA4.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60257,"TRANSGRIDV5_20180116135943","2017-10-11T01:05:00","#TORRB2_P_E","#TORRB2_PE","2017-10-11",1,-48.809600000000003,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60283,"TRANSGRIDV5_20180116135943","2017-10-11T04:35:00","#TORRB2_P_E","#TORRB2_PE","2017-10-11",1,-30.31269,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60313,"TRANSGRIDV5_20180116135943","2017-10-11T02:40:00","#TORRB2_P_E","#TORRB2_PE","2017-10-11",1,-10.27971,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island A","REGULATED","99","Non Inclusion",null,0]
[60384,"TRANSGRIDV5_20180116135943","2017-10-11T08:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-115.58311,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60410,"TRANSGRIDV5_20180116135943","2017-10-11T05:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-102.68461000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60440,"TRANSGRIDV5_20180116135943","2017-10-11T12:00:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-98.5,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60507,"TRANSGRIDV5_20180116135943","2017-10-11T20:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-89.007149999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60529,"TRANSGRIDV5_20180116135943","2017-10-11T04:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-81.096109999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60566,"TRANSGRIDV5_20180116135943","2017-10-11T01:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-75.032409999999999,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60592,"TRANSGRIDV5_20180116135943","2017-10-11T02:40:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.730200000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[60663,"TRANSGRIDV5_20180116135943","2017-10-11T19:35:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-17.772410000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[60693,"TRANSGRIDV5_20180116135943","2017-10-11T17:30:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-15.57719,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[60719,"TRANSGRIDV5_20180116135943","2017-10-11T23:20:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-14.854570000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[60790,"TRANSGRIDV5_20180116135943","2017-10-11T23:40:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.86309,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[60816,"TRANSGRIDV5_20180116135943","2017-10-11T06:45:00","N>N-KKLS_TE_2","N-KKLS_967","2013-08-21",1,-47.09534,"Out= Koolkhan to Lismore (967), avoid O/L Glen Innes to Tenterfield (96R) on trip of Coffs Harbour to Lismore (89), swamp out when all 3 directlink O/S, Feedback, TG formulation on PD & ST","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[60846,"TRANSGRIDV5_20180116135943","2017-10-11T07:20:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-128.93163999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[60876,"TRANSGRIDV5_20180116135943","2017-10-11T03:50:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-31.786429999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[60943,"TRANSGRIDV5_20180116135943","2017-10-11T06:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-282.21350000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[60973,"TRANSGRIDV5_20180116135943","2017-10-11T04:15:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-55.316330000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[60999,"TRANSGRIDV5_20180116135943","2017-10-11T02:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-39.773829999999997,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[61070,"TRANSGRIDV5_20180116135943","2017-10-11T18:45:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-25.586200000000002,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[61100,"TRANSGRIDV5_20180116135943","2017-10-11T10:35:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-22.854700000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[61126,"TRANSGRIDV5_20180116135943","2017-10-11T15:25:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-20.88392,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[61197,"TRANSGRIDV5_20180116135943","2017-10-11T10:15:00","VSML_ROC_80","V-NIL","2016-08-23",1,-11.34116,"Out=Nil, Rate of Change (VIC to SA) constraint (80 MW / 5 Min) for Murraylink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[61227,"TRANSGRIDV5_20180116135943","2017-10-12T07:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-318.14999999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61253,"TRANSGRIDV5_20180116135943","2017-10-12T17:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-249.9,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61324,"TRANSGRIDV5_20180116135943","2017-10-12T12:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-145.68,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61350,"TRANSGRIDV5_20180116135943","2017-10-12T19:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-100.05722,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61380,"TRANSGRIDV5_20180116135943","2017-10-12T19:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-95.182580000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61410,"TRANSGRIDV5_20180116135943","2017-10-12T04:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-86.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61477,"TRANSGRIDV5_20180116135943","2017-10-12T03:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-78.002179999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[61507,"TRANSGRIDV5_20180116135943","2017-10-12T16:15:00","F_Q++ARDM_R6","F-N-ARDM_ONE","2013-08-21",1,132,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[61537,"TRANSGRIDV5_20180116135943","2017-10-12T08:30:00","F_Q++ARDM_R6","F-N-ARDM_ONE","2013-08-21",1,55,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[61604,"TRANSGRIDV5_20180116135943","2017-10-12T16:15:00","F_Q++ARDM_R60","F-N-ARDM_ONE","2013-08-21",1,222.47847999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[61634,"TRANSGRIDV5_20180116135943","2017-10-12T15:40:00","F_Q++ARDM_R60","F-N-ARDM_ONE","2013-08-21",1,69.989999999999995,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[61660,"TRANSGRIDV5_20180116135943","2017-10-12T11:25:00","F_Q++ARDM_R60","F-N-ARDM_ONE","2013-08-21",1,60.209290000000003,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[61731,"TRANSGRIDV5_20180116135943","2017-10-12T13:15:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-178.64467999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[61761,"TRANSGRIDV5_20180116135943","2017-10-12T09:25:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-126.71680000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[61787,"TRANSGRIDV5_20180116135943","2017-10-12T11:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-76.470339999999993,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[61858,"TRANSGRIDV5_20180116135943","2017-10-12T23:00:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-13.175000000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[61884,"TRANSGRIDV5_20180116135943","2017-10-12T21:40:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-11.319559999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[61914,"TRANSGRIDV5_20180116135943","2017-10-12T18:20:00","N^Q_NIL_A","N-NIL","2013-08-21",1,-95.241489999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[61944,"TRANSGRIDV5_20180116135943","2017-10-12T00:45:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-15.034840000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[62008,"TRANSGRIDV5_20180116135943","2017-10-12T02:30:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-69.830449999999999,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[62040,"TRANSGRIDV5_20180116135943","2017-10-12T00:20:00","V>>V_SMTXF2_6","V-SMTXF2_R","2017-10-05",1,-31.127269999999999,"Out = South Morang F2 500/220 kV txfmr, avoid O/L of a Thomastown to South Morang 220 kV line for trip of the parallel Thomastown to South Morang 220 kV line, feedback","OUTAGE","OTHER","South Morang F2 500/330kV txfmr","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[62070,"TRANSGRIDV5_20180116135943","2017-10-12T12:40:00","VN_0850","I-VN_0850","2014-01-08",1,-31.178699999999999,"Discretionary Vic to NSW transfer upper limit of  850 MW","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[62137,"TRANSGRIDV5_20180116135943","2017-10-13T18:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-197.77,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62167,"TRANSGRIDV5_20180116135943","2017-10-13T07:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-104.10603,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62193,"TRANSGRIDV5_20180116135943","2017-10-13T05:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-100.18706,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62264,"TRANSGRIDV5_20180116135943","2017-10-13T11:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-91.516819999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62294,"TRANSGRIDV5_20180116135943","2017-10-13T10:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-89.925820000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62320,"TRANSGRIDV5_20180116135943","2017-10-13T08:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-87.939589999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62391,"TRANSGRIDV5_20180116135943","2017-10-13T01:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.989999999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62417,"TRANSGRIDV5_20180116135943","2017-10-13T18:25:00","F_Q++ARDM_R6","F-N-ARDM_ONE","2013-08-21",1,25.447089999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[62447,"TRANSGRIDV5_20180116135943","2017-10-13T16:35:00","F_Q++ARDM_R60","F-N-ARDM_ONE","2013-08-21",1,50,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Raise 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[62477,"TRANSGRIDV5_20180116135943","2017-10-13T15:35:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-122.06456,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore - Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[62544,"TRANSGRIDV5_20180116135943","2017-10-13T15:05:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-14.85984,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore - Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[62574,"TRANSGRIDV5_20180116135943","2017-10-13T00:10:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-12.72444,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore - Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[62604,"TRANSGRIDV5_20180116135943","2017-10-13T21:30:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-11.14343,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore - Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[62671,"TRANSGRIDV5_20180116135943","2017-10-13T03:00:00","V::N_SMF2_SD2","V-SMTXF2_R","2017-04-07",1,-22.188870000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA decelerates, YPS G1 on 500kV. Constraint active for SA flows above 500 MW VIC to SA only, swamped otherwise.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"AusNet"]
[62701,"TRANSGRIDV5_20180116135943","2017-10-14T17:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-250.9,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62727,"TRANSGRIDV5_20180116135943","2017-10-14T18:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-92.382450000000006,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62798,"TRANSGRIDV5_20180116135943","2017-10-14T01:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-87.392669999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62828,"TRANSGRIDV5_20180116135943","2017-10-14T13:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-85.445930000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62854,"TRANSGRIDV5_20180116135943","2017-10-14T04:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.679860000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62884,"TRANSGRIDV5_20180116135943","2017-10-14T12:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-80.343260000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62955,"TRANSGRIDV5_20180116135943","2017-10-14T15:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.668679999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[62981,"TRANSGRIDV5_20180116135943","2017-10-14T17:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.284829999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore Koolkhan 967 132kV LINE","REGULATED","INCLUDED","","PLANNED",1]
[63011,"TRANSGRIDV5_20180116135943","2017-10-15T16:45:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-80.817750000000004,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63078,"TRANSGRIDV5_20180116135943","2017-10-15T12:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-70.075090000000003,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63108,"TRANSGRIDV5_20180116135943","2017-10-15T12:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-69.246020000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63138,"TRANSGRIDV5_20180116135943","2017-10-15T07:30:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-67.790729999999996,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63205,"TRANSGRIDV5_20180116135943","2017-10-15T14:15:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63235,"TRANSGRIDV5_20180116135943","2017-10-15T05:35:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.534400000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63261,"TRANSGRIDV5_20180116135943","2017-10-15T05:50:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.730040000000002,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63332,"TRANSGRIDV5_20180116135943","2017-10-16T11:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-88.188770000000005,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63362,"TRANSGRIDV5_20180116135943","2017-10-16T13:25:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-83.20917,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63388,"TRANSGRIDV5_20180116135943","2017-10-16T09:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-68.990759999999995,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63418,"TRANSGRIDV5_20180116135943","2017-10-16T10:10:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-64.88,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63471,"TRANSGRIDV5_20180116135943","2017-10-16T00:05:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-59.78,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63514,"TRANSGRIDV5_20180116135943","2017-10-16T03:55:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-55.199759999999998,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63544,"TRANSGRIDV5_20180116135943","2017-10-16T06:20:00","#YABULU2_E","#YABULU2_E","2017-09-22",1,-40.360050000000001,"QGAR1.ENERGY * 1 = 0 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63611,"TRANSGRIDV5_20180116135943","2017-10-17T21:05:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-160.00004000000001,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[63641,"TRANSGRIDV5_20180116135943","2017-10-17T15:50:00","#YABULU2_E","#YABULU2_E","2017-10-17",1,-92.333839999999995,"QGAR1.ENERGY * 1 <= 30 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63671,"TRANSGRIDV5_20180116135943","2017-10-17T14:35:00","#YABULU2_E","#YABULU2_E","2017-10-17",1,-77.721159999999998,"QGAR1.ENERGY * 1 <= 30 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63738,"TRANSGRIDV5_20180116135943","2017-10-17T04:05:00","#YABULU2_E","#YABULU2_E","2017-10-17",1,-60.244230000000002,"QGAR1.ENERGY * 1 <= 30 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63768,"TRANSGRIDV5_20180116135943","2017-10-17T01:20:00","#YABULU2_E","#YABULU2_E","2017-10-17",1,-58.916110000000003,"QGAR1.ENERGY * 1 <= 30 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[63794,"TRANSGRIDV5_20180116135943","2017-10-17T16:10:00","Q>>BCRG_CLWU_BCCP","Q-BCRG_811","2017-05-29",1,-23.959810000000001,"Out= Bouldercombe to Raglan (811), avoid O/L Bouldercombe to Calliope River (812) on trip of Calvale to Wurdong (871) line, Feedback","OUTAGE","OTHER","Raglan-Boulderbmb 275kV LINE 811","REGULATED","99","Non Inclusion",null,0,"Powerlink outage"]
[63865,"TRANSGRIDV5_20180116135943","2017-10-17T04:30:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-25.439540000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[63895,"TRANSGRIDV5_20180116135943","2017-10-17T01:55:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-14.148720000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[63921,"TRANSGRIDV5_20180116135943","2017-10-18T06:20:00","#HDWF3_E","#HDWF3_E","2017-08-15",1,-126.18025,"SHDW3H.ENERGY * 1 <= 50 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[63951,"TRANSGRIDV5_20180116135943","2017-10-18T17:10:00","#YABULU2_E","#YABULU2_E","2017-10-18",1,-96.857479999999995,"QGAR1.ENERGY * 1 <= 55 (Wt = 360)","OUTAGE","OTHER","Townsville GT","REGULATED","99","Non Inclusion",null,0]
[64022,"TRANSGRIDV5_20180116135943","2017-10-18T05:10:00","S>>BLMK_CNRB_WEMWP4","S-BLMK","2017-05-31",1,-71.673289999999994,"Out= Belalie-Mokota 275kV line, avoid O/L Waterloo East-Morgan Whyalla 4 132kV on trip of Canowi-Robertstown 275kV line(this trips Hallet wind farm and Hallet GT, and offloads Davenport-Canowie 275kV line), Feedback","OUTAGE","OTHER","Belalie-Mokota 275kV LINE","REGULATED","99","Non Inclusion",null,0,"ElectraNet outage"]
[64048,"TRANSGRIDV5_20180116135943","2017-10-18T04:10:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-29.871259999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[64078,"TRANSGRIDV5_20180116135943","2017-10-18T02:00:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-15.052160000000001,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[64145,"TRANSGRIDV5_20180116135943","2017-10-19T08:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.12397,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64175,"TRANSGRIDV5_20180116135943","2017-10-19T22:40:00","V::N_SMF2_V2","V-SMTXF2_R","2017-04-07",1,-14.885429999999999,"Out = South Morang F2 500/330kV txfmr, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","S Morang F2 500/330kV XFMR","REGULATED","99","Non Inclusion",null,0,"Ausnet outage"]
[64205,"TRANSGRIDV5_20180116135943","2017-10-20T15:25:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,15.39349,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64272,"TRANSGRIDV5_20180116135943","2017-10-20T15:25:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,17.97,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64302,"TRANSGRIDV5_20180116135943","2017-10-20T10:45:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,28.98,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64332,"TRANSGRIDV5_20180116135943","2017-10-20T13:35:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,21.120439999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64399,"TRANSGRIDV5_20180116135943","2017-10-20T15:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-55.340260000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64429,"TRANSGRIDV5_20180116135943","2017-10-20T09:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-38.459719999999997,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64455,"TRANSGRIDV5_20180116135943","2017-10-20T14:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-27.994630000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64485,"TRANSGRIDV5_20180116135943","2017-10-20T15:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.193239999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64556,"TRANSGRIDV5_20180116135943","2017-10-21T09:00:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-45.141530000000003,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64582,"TRANSGRIDV5_20180116135943","2017-10-21T01:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-26.117529999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64612,"TRANSGRIDV5_20180116135943","2017-10-22T11:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-37.803370000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64679,"TRANSGRIDV5_20180116135943","2017-10-22T07:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-26.11871,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[64709,"TRANSGRIDV5_20180116135943","2017-10-22T01:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-43.047879999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64739,"TRANSGRIDV5_20180116135943","2017-10-22T05:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-26.360869999999998,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[64806,"TRANSGRIDV5_20180116135943","2017-10-23T10:05:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,26.16685,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64836,"TRANSGRIDV5_20180116135943","2017-10-23T16:45:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,18.809999999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64866,"TRANSGRIDV5_20180116135943","2017-10-23T10:55:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,13.48,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64924,"TRANSGRIDV5_20180116135943","2017-10-23T16:40:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,19.827860000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64962,"TRANSGRIDV5_20180116135943","2017-10-23T06:15:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,15.89,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[64988,"TRANSGRIDV5_20180116135943","2017-10-23T06:55:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,28.98,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65018,"TRANSGRIDV5_20180116135943","2017-10-23T11:40:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,21.479949999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65089,"TRANSGRIDV5_20180116135943","2017-10-23T05:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-96.447689999999994,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65115,"TRANSGRIDV5_20180116135943","2017-10-23T09:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-59.069870000000002,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65145,"TRANSGRIDV5_20180116135943","2017-10-23T16:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-49.073270000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65216,"TRANSGRIDV5_20180116135943","2017-10-23T16:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-26.066310000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65242,"TRANSGRIDV5_20180116135943","2017-10-23T05:10:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.78026,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65272,"TRANSGRIDV5_20180116135943","2017-10-23T01:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-30.761140000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[65339,"TRANSGRIDV5_20180116135943","2017-10-24T15:25:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,50.806350000000002,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65369,"TRANSGRIDV5_20180116135943","2017-10-24T10:20:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,38.54036,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65399,"TRANSGRIDV5_20180116135943","2017-10-24T10:25:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,33.040080000000003,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65425,"TRANSGRIDV5_20180116135943","2017-10-24T10:55:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,24.14706,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65496,"TRANSGRIDV5_20180116135943","2017-10-24T08:05:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,28.98,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65522,"TRANSGRIDV5_20180116135943","2017-10-24T14:35:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,25.986450000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65552,"TRANSGRIDV5_20180116135943","2017-10-24T14:20:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,14.4,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65623,"TRANSGRIDV5_20180116135943","2017-10-24T05:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-81.010670000000005,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65649,"TRANSGRIDV5_20180116135943","2017-10-24T18:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-61.948,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65679,"TRANSGRIDV5_20180116135943","2017-10-24T08:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-53.741900000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65750,"TRANSGRIDV5_20180116135943","2017-10-24T03:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-31.061229999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65776,"TRANSGRIDV5_20180116135943","2017-10-24T02:35:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.404159999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[65806,"TRANSGRIDV5_20180116135943","2017-10-24T03:45:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-30.608219999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[65873,"TRANSGRIDV5_20180116135943","2017-10-24T19:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-43.305329999999998,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[65903,"TRANSGRIDV5_20180116135943","2017-10-25T16:05:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,64.53,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65933,"TRANSGRIDV5_20180116135943","2017-10-25T11:10:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,49.339300000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[65959,"TRANSGRIDV5_20180116135943","2017-10-25T09:05:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,44.294980000000002,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66030,"TRANSGRIDV5_20180116135943","2017-10-25T18:35:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,20,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66056,"TRANSGRIDV5_20180116135943","2017-10-25T17:35:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,143.79571000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66086,"TRANSGRIDV5_20180116135943","2017-10-25T14:40:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,43.241059999999997,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66157,"TRANSGRIDV5_20180116135943","2017-10-25T18:35:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,17.989999999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66183,"TRANSGRIDV5_20180116135943","2017-10-25T15:15:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,13.205830000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66213,"TRANSGRIDV5_20180116135943","2017-10-25T15:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-228.59331,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66284,"TRANSGRIDV5_20180116135943","2017-10-25T09:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-72.316419999999994,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66310,"TRANSGRIDV5_20180116135943","2017-10-25T12:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-61.253920000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66340,"TRANSGRIDV5_20180116135943","2017-10-25T13:05:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-33.269579999999998,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66403,"TRANSGRIDV5_20180116135943","2017-10-25T17:35:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-20.50478,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[66436,"TRANSGRIDV5_20180116135943","2017-10-25T17:10:00","V>>N-NIL_HA","N-NIL","2017-08-11",1,-23.522279999999999,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[66466,"TRANSGRIDV5_20180116135943","2017-10-26T06:30:00","#R016386_013_RAMP_F","#R016386_RAMP","2017-10-25",1,-34.002400000000002,"Hard Ramping constraint for constraint Q:N_ARSVC_AR_2L-G, Effective Date: 08/01/2014, Version: 1","OUTAGE","RAMP","Armidale SVC ","REGULATED","10","Ramping Constraint","PLANNED",0]
[66492,"TRANSGRIDV5_20180116135943","2017-10-26T16:40:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-101.88479,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[66563,"TRANSGRIDV5_20180116135943","2017-10-26T06:30:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-39.837380000000003,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66593,"TRANSGRIDV5_20180116135943","2017-10-26T07:55:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-19.29917,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC2 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[66619,"TRANSGRIDV5_20180116135943","2017-10-26T07:30:00","Q:N_ARSVC_AR_2L-G","N-AR_VC1","2014-01-08",1,-34.986660000000001,"Outage= Armidale SVC, limit Qld to NSW on QNI to avoid transient instability on 2L-G fault at Armidale","OUTAGE","OTHER","Armidale 1 330kV SVC","REGULATED","INCLUDED","","PLANNED",1]
[66690,"TRANSGRIDV5_20180116135943","2017-10-26T05:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-17.873889999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[66716,"TRANSGRIDV5_20180116135943","2017-10-26T11:35:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-16.963909999999998,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[66746,"TRANSGRIDV5_20180116135943","2017-10-27T06:20:00","#HDWF3_E","#HDWF3_E","2017-10-27",1,-135.00003000000001,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[66776,"TRANSGRIDV5_20180116135943","2017-10-27T11:20:00","#SNOWTWN1_E","#SNOWTWN1_E","2017-10-27",1,-920.00085999999999,"SNWF1T.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","Snowtown Wind Farm","REGULATED","99","Non Inclusion",null,0]
[66843,"TRANSGRIDV5_20180116135943","2017-10-27T15:10:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,12.204459999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66873,"TRANSGRIDV5_20180116135943","2017-10-27T09:55:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,25.493549999999999,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66899,"TRANSGRIDV5_20180116135943","2017-10-27T10:45:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,18.965979999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[66970,"TRANSGRIDV5_20180116135943","2017-10-27T10:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-33.941180000000003,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[67000,"TRANSGRIDV5_20180116135943","2017-10-27T07:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-12.074960000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC3 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[67026,"TRANSGRIDV5_20180116135943","2017-10-27T17:10:00","S>>BLMK_BWPA_BRTW","S-BLMK","2017-10-23",1,-75.563789999999997,"Out= Belalie-Mokota 275kV line, avoid O/L Brinkworth-Templers West 275kV line on trip of Blyth West-Munno Para 275kV line, Feedback","OUTAGE","OTHER","Belalie - Mokota 275kV LINE","REGULATED","99","Non Inclusion",null,0,"ElectraNet outage"]
[67097,"TRANSGRIDV5_20180116135943","2017-10-28T18:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1116.31,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67127,"TRANSGRIDV5_20180116135943","2017-10-28T23:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1093.75,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67153,"TRANSGRIDV5_20180116135943","2017-10-28T05:45:00","#T-V-MNSP1_RAMP_E_F","#T-V-MNSP1_RAMP_E","2017-10-28",1,102.74,"T-V-MNSP1 >= MIN(0, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[67224,"TRANSGRIDV5_20180116135943","2017-10-28T11:40:00","F_Q++ARTW_L60","F-N-ARTW_86","2013-08-21",1,17.96,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 86","REGULATED","INCLUDED","","PLANNED",1]
[67250,"TRANSGRIDV5_20180116135943","2017-10-28T13:55:00","F_Q++ARTW_L60","F-N-ARTW_86","2013-08-21",1,17.696470000000001,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 86","REGULATED","INCLUDED","","PLANNED",1]
[67280,"TRANSGRIDV5_20180116135943","2017-10-29T12:55:00","#HDWF3_E","#HDWF3_E","2017-10-27",1,-199.02,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[67310,"TRANSGRIDV5_20180116135943","2017-10-29T00:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1085.07,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67377,"TRANSGRIDV5_20180116135943","2017-10-29T19:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1062.03,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67407,"TRANSGRIDV5_20180116135943","2017-10-29T02:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1057.43,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67437,"TRANSGRIDV5_20180116135943","2017-10-29T03:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1053.33,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67504,"TRANSGRIDV5_20180116135943","2017-10-29T09:05:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1047.94,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67534,"TRANSGRIDV5_20180116135943","2017-10-29T08:45:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1045.45,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67560,"TRANSGRIDV5_20180116135943","2017-10-29T11:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1037.17,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[67631,"TRANSGRIDV5_20180116135943","2017-10-29T06:50:00","#TORRB2_P_E","#TORRB2_PE","2017-10-28",1,-50.729810000000001,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[67661,"TRANSGRIDV5_20180116135943","2017-10-29T04:30:00","#TORRB2_P_E","#TORRB2_PE","2017-10-28",1,-48.641730000000003,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[67687,"TRANSGRIDV5_20180116135943","2017-10-29T08:10:00","#TORRB2_P_E","#TORRB2_PE","2017-10-28",1,-46.515709999999999,"STSB2.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Torrens Island B unit 2","REGULATED","99","Non Inclusion",null,0]
[67758,"TRANSGRIDV5_20180116135943","2017-10-29T08:40:00","F_Q++ARTW_L6","F-N-ARTW_86","2013-08-21",1,12.36135,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 86","REGULATED","INCLUDED","","PLANNED",1]
[67784,"TRANSGRIDV5_20180116135943","2017-10-29T08:40:00","F_Q++ARTW_L60","F-N-ARTW_86","2013-08-21",1,17.93,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 86","REGULATED","INCLUDED","","PLANNED",1]
[67814,"TRANSGRIDV5_20180116135943","2017-10-29T18:05:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-11.168670000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[67866,"TRANSGRIDV5_20180116135943","2017-10-29T06:10:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-10-15",1,-49.720109999999998,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[67910,"TRANSGRIDV5_20180116135943","2017-10-29T04:40:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-10-15",1,-44.727370000000001,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[67940,"TRANSGRIDV5_20180116135943","2017-10-29T02:05:00","NSA_S_POR03_ISLD","NSA-S_POR03_ISLD","2014-10-15",1,-75.508750000000006,"Network Support Agreement for Port Lincoln Unit 3 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[67970,"TRANSGRIDV5_20180116135943","2017-10-29T03:50:00","NSA_S_POR03_ISLD","NSA-S_POR03_ISLD","2014-10-15",1,-50.69,"Network Support Agreement for Port Lincoln Unit 3 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68037,"TRANSGRIDV5_20180116135943","2017-10-29T11:45:00","NSA_S_POR03_ISLD","NSA-S_POR03_ISLD","2014-10-15",1,-37.501910000000002,"Network Support Agreement for Port Lincoln Unit 3 to meet local islanded demand for the planned outage.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68067,"TRANSGRIDV5_20180116135943","2017-10-29T10:55:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-52.831200000000003,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68093,"TRANSGRIDV5_20180116135943","2017-10-29T11:15:00","V::N_NIL_V1","V-NIL","2017-04-07",1,-23.23554,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 220 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68164,"TRANSGRIDV5_20180116135943","2017-10-30T05:50:00","#NSW1-QLD1_RAMP_I_F","#NSW1-QLD1_RAMP_I","2017-10-30",1,26.525960000000001,"NSW1-QLD1 >= MIN(-402, InitialFlow + 200) (Wt=35)","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68194,"TRANSGRIDV5_20180116135943","2017-10-30T08:00:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1080,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68220,"TRANSGRIDV5_20180116135943","2017-10-30T09:15:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1075.6500000000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68291,"TRANSGRIDV5_20180116135943","2017-10-30T00:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1056.02,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68317,"TRANSGRIDV5_20180116135943","2017-10-30T02:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-10-28",1,-1050.69,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68347,"TRANSGRIDV5_20180116135943","2017-10-30T10:40:00","F_Q++ARTW_L5","F-N-ARTW_86","2013-08-21",1,14.051909999999999,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 86","REGULATED","INCLUDED","","PLANNED",1]
[68377,"TRANSGRIDV5_20180116135943","2017-10-30T16:35:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.48202,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[68444,"TRANSGRIDV5_20180116135943","2017-10-31T23:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.933309999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68474,"TRANSGRIDV5_20180116135943","2017-10-31T07:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-13.20209,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68504,"TRANSGRIDV5_20180116135943","2017-11-01T10:40:00","#BOCORWF1_E","#BOCORWF1_E","2017-11-01",2,-1053.78,"NCMA3B.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","BOCO Rock Wind farm","REGULATED","99","Non Inclusion",null,0]
[68571,"TRANSGRIDV5_20180116135943","2017-11-02T05:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-22.555980000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68601,"TRANSGRIDV5_20180116135943","2017-11-02T09:20:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-15.53558,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68627,"TRANSGRIDV5_20180116135943","2017-11-02T12:50:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-12.98465,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68698,"TRANSGRIDV5_20180116135943","2017-11-03T05:35:00","F_Q++ARTW_L6","F-N-ARTW_85","2013-08-21",1,18.5,"Out = Armidale to Tamworth (85 or 86) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Tamworth Armidale 330kV LINE 85","REGULATED","INCLUDED","","PLANNED",1]
[68728,"TRANSGRIDV5_20180116135943","2017-11-03T19:35:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-27.037009999999999,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68754,"TRANSGRIDV5_20180116135943","2017-11-04T09:30:00","#HDWF3_E","#HDWF3_E","2017-10-27",1,-130.69,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[68784,"TRANSGRIDV5_20180116135943","2017-11-04T19:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-04",1,-1079.9995799999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68855,"TRANSGRIDV5_20180116135943","2017-11-04T09:40:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-1152.0058200000001,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68881,"TRANSGRIDV5_20180116135943","2017-11-04T13:25:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-138.84754000000001,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[68911,"TRANSGRIDV5_20180116135943","2017-11-05T17:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1099.9149600000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[68978,"TRANSGRIDV5_20180116135943","2017-11-05T15:05:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1080.2828,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69008,"TRANSGRIDV5_20180116135943","2017-11-05T14:45:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1077.8537799999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69038,"TRANSGRIDV5_20180116135943","2017-11-05T12:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1069.2437299999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69105,"TRANSGRIDV5_20180116135943","2017-11-05T00:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1061.5310300000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69135,"TRANSGRIDV5_20180116135943","2017-11-05T05:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1058.8691899999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69161,"TRANSGRIDV5_20180116135943","2017-11-05T23:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1055.00162,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69232,"TRANSGRIDV5_20180116135943","2017-11-05T09:15:00","S:VS_650_HY_TEST_DYN","I-SVS_650_TEST","2015-11-25",1,-61.022019999999998,"SA to VIC on Heywood and Murraylink combined upper transfer limit of 650 MW, limit for testing of Heywood interconnection upgrade, dynamic headroom, DS formulation only.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69262,"TRANSGRIDV5_20180116135943","2017-11-06T04:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1066.22532,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69279,"TRANSGRIDV5_20180116135943","2017-11-06T04:25:00","#OSB-AG_P_E","#OSB-AG_PE","2017-11-05",1,-1064.2448099999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 50)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[69317,"TRANSGRIDV5_20180116135943","2017-11-06T12:10:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-74.970860000000002,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[69388,"TRANSGRIDV5_20180116135943","2017-11-07T15:30:00","#SNOWTWN1_E","#SNOWTWN1_E","2017-11-07",1,-1068.7038299999999,"SNWF1T.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","Snowtown Wind Farm","REGULATED","99","Non Inclusion",null,0]
[69414,"TRANSGRIDV5_20180116135943","2017-11-07T14:45:00","#SNOWTWN1_E","#SNOWTWN1_E","2017-11-07",1,-1065.37672,"SNWF1T.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","Snowtown Wind Farm","REGULATED","99","Non Inclusion",null,0]
[69444,"TRANSGRIDV5_20180116135943","2017-11-07T19:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-20.73696,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69511,"TRANSGRIDV5_20180116135943","2017-11-08T17:45:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-33.952370000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69541,"TRANSGRIDV5_20180116135943","2017-11-08T17:15:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-28.595020000000002,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69571,"TRANSGRIDV5_20180116135943","2017-11-08T05:30:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-21.34854,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69638,"TRANSGRIDV5_20180116135943","2017-11-08T18:25:00","N^^V_NIL_1","V-NIL","2017-04-20",1,-11.56635,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69668,"TRANSGRIDV5_20180116135943","2017-11-09T21:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.663200000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69694,"TRANSGRIDV5_20180116135943","2017-11-09T11:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-20.316050000000001,"Out = Nil, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69765,"TRANSGRIDV5_20180116135943","2017-11-10T19:30:00","#MP2_E","#MP2_E","2017-11-10",3,-70.436719999999994,"NMTP2.ENERGY * 1 <= 450 (Wt = 360)","OUTAGE","OTHER","Mt Piper Generator","REGULATED","99","Non Inclusion",null,0]
[69795,"TRANSGRIDV5_20180116135943","2017-11-10T22:50:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-69.613849999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[69821,"TRANSGRIDV5_20180116135943","2017-11-10T23:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-62.438339999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69851,"TRANSGRIDV5_20180116135943","2017-11-10T14:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-47.386969999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69922,"TRANSGRIDV5_20180116135943","2017-11-10T07:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-18.51352,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69948,"TRANSGRIDV5_20180116135943","2017-11-10T06:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-11.931699999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[69978,"TRANSGRIDV5_20180116135943","2017-11-11T09:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-58.114240000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70045,"TRANSGRIDV5_20180116135943","2017-11-11T09:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-29.30611,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70075,"TRANSGRIDV5_20180116135943","2017-11-11T10:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.014060000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70105,"TRANSGRIDV5_20180116135943","2017-11-12T16:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-104.88267,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70172,"TRANSGRIDV5_20180116135943","2017-11-12T12:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.221720000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70202,"TRANSGRIDV5_20180116135943","2017-11-12T04:15:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-34.594650000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70232,"TRANSGRIDV5_20180116135943","2017-11-12T08:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-12.966799999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70299,"TRANSGRIDV5_20180116135943","2017-11-13T08:35:00","N^^V_EPMB_1","V-EPMB","2015-08-07",1,-39.721780000000003,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Eildon PS Mt Beauty 220kV LINE","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[70329,"TRANSGRIDV5_20180116135943","2017-11-13T07:40:00","N^^V_EPMB_1","V-EPMB","2015-08-07",1,-21.45233,"Out = Eildon to Mount Beauty 220 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Eildon PS Mt Beauty 220kV LINE","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[70355,"TRANSGRIDV5_20180116135943","2017-11-13T23:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-61.047759999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70385,"TRANSGRIDV5_20180116135943","2017-11-13T22:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-38.266710000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70456,"TRANSGRIDV5_20180116135943","2017-11-13T00:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-12.534230000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70482,"TRANSGRIDV5_20180116135943","2017-11-13T15:15:00","QNTE_150","I-QNTE_150","2014-01-08",1,-17.609739999999999,"Qld to NSW on Terranora Interconnector upper transfer limit of 150 MW","OUTAGE","OTHER","Koolkhan - Lismore 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[70512,"TRANSGRIDV5_20180116135943","2017-11-14T11:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-67.584639999999993,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70579,"TRANSGRIDV5_20180116135943","2017-11-14T12:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-14.86741,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70609,"TRANSGRIDV5_20180116135943","2017-11-14T12:10:00","N_BROKENH1_ZERO","N-BROKENH1_ZERO","2015-08-13",1,-1096.49216,"Broken Hill Solar Farm upper limit of 0 MW","OUTAGE","OTHER","Buronga - Broken Hill 220kV Line X2","REGULATED","11","Transmission connection agreements where a lower service standard has been negotiated giving the TNSP the right to disrupt service under certain network conditions where the constraint only affects the parties subject to the agreement.","PLANNED",0,"Please refer to explanatory statement in attachments"]
[70639,"TRANSGRIDV5_20180116135943","2017-11-14T10:05:00","N_BROKENH1_ZERO","N-BROKENH1_ZERO","2015-08-13",1,-1074.9526900000001,"Broken Hill Solar Farm upper limit of 0 MW","OUTAGE","OTHER","Buronga - Broken Hill 220kV Line X2","REGULATED","11","Transmission connection agreements where a lower service standard has been negotiated giving the TNSP the right to disrupt service under certain network conditions where the constraint only affects the parties subject to the agreement.","PLANNED",0,"Please refer to explanatory statement in attachments"]
[70706,"TRANSGRIDV5_20180116135943","2017-11-15T14:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-43.445010000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70736,"TRANSGRIDV5_20180116135943","2017-11-15T09:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-26.837,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70782,"TRANSGRIDV5_20180116135943","2017-11-16T23:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-155.56041999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70791,"TRANSGRIDV5_20180116135943","2017-11-16T08:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-102.23143,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70862,"TRANSGRIDV5_20180116135943","2017-11-16T09:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-24.824670000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70888,"TRANSGRIDV5_20180116135943","2017-11-17T10:45:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-10",1,-93.290260000000004,"VHOG1K.ENERGY * 1 <= 5 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[70918,"TRANSGRIDV5_20180116135943","2017-11-17T05:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-74.726730000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[70989,"TRANSGRIDV5_20180116135943","2017-11-17T17:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-44.729950000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71015,"TRANSGRIDV5_20180116135943","2017-11-17T09:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-37.167949999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71045,"TRANSGRIDV5_20180116135943","2017-11-17T20:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.887419999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71116,"TRANSGRIDV5_20180116135943","2017-11-18T01:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-114.85662000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71142,"TRANSGRIDV5_20180116135943","2017-11-18T09:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-50.53593,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71172,"TRANSGRIDV5_20180116135943","2017-11-18T20:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-36.359760000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71239,"TRANSGRIDV5_20180116135943","2017-11-18T02:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-14.79862,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71269,"TRANSGRIDV5_20180116135943","2017-11-19T17:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-112.52211,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71299,"TRANSGRIDV5_20180116135943","2017-11-19T16:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.180590000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71325,"TRANSGRIDV5_20180116135943","2017-11-19T06:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.32996,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71396,"TRANSGRIDV5_20180116135943","2017-11-19T08:00:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-30.66385,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[71422,"TRANSGRIDV5_20180116135943","2017-11-19T07:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-27.537960000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71452,"TRANSGRIDV5_20180116135943","2017-11-20T23:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.328330000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71523,"TRANSGRIDV5_20180116135943","2017-11-20T15:05:00","N^^V_SMTXH1_1","V-SMTS_HTX_R","2015-08-07",1,-56.658659999999998,"Out = South Morang H1 or H2 500/330 kV txfmr, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Sth Morang H1 or H2 500kV txfmr","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[71549,"TRANSGRIDV5_20180116135943","2017-11-20T08:30:00","N^^V_SMTXH1_1","V-SMTS_HTX_R","2015-08-07",1,-39.681100000000001,"Out = South Morang H1 or H2 500/330 kV txfmr, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Sth Morang H1 or H2 500kV txfmr","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[71579,"TRANSGRIDV5_20180116135943","2017-11-20T11:50:00","N^^V_SMTXH1_1","V-SMTS_HTX_R","2015-08-07",1,-34.561010000000003,"Out = South Morang H1 or H2 500/330 kV txfmr, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Sth Morang H1 or H2 500kV txfmr","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[71650,"TRANSGRIDV5_20180116135943","2017-11-21T13:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-158.75809000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71676,"TRANSGRIDV5_20180116135943","2017-11-21T09:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-73.244500000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71706,"TRANSGRIDV5_20180116135943","2017-11-21T21:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-43.979399999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71773,"TRANSGRIDV5_20180116135943","2017-11-21T14:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-137.40545,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71803,"TRANSGRIDV5_20180116135943","2017-11-21T17:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-117.33947999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71833,"TRANSGRIDV5_20180116135943","2017-11-21T19:40:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-21.31963,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71859,"TRANSGRIDV5_20180116135943","2017-11-21T14:10:00","Q>NIL_MUTE_758","Q-NIL","2014-09-02",1,-144.82317,"Out= Nil, ECS for managing 758 H4 Mudgeeraba to T174 Terranora 110kV line, Summer and Winter ECS ratings selected by SCADA status.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[71930,"TRANSGRIDV5_20180116135943","2017-11-22T08:05:00","#HDWF3_E","#HDWF3_E","2017-11-13",1,-1090.0001999999999,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[71956,"TRANSGRIDV5_20180116135943","2017-11-22T10:50:00","#SATGN1_E","#SATGN1_E","2017-11-22",1,-92.075980000000001,"SPAG1E.ENERGY * 1 = 15 (Wt = 30)","OUTAGE","OTHER","Temporary Generation North (TGN) Edinburgh","REGULATED","99","Non Inclusion",null,0]
[71986,"TRANSGRIDV5_20180116135943","2017-11-22T07:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.44182,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72057,"TRANSGRIDV5_20180116135943","2017-11-22T11:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-14.78825,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[72083,"TRANSGRIDV5_20180116135943","2017-11-22T00:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-37.258240000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72113,"TRANSGRIDV5_20180116135943","2017-11-22T04:00:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-143.33940000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72184,"TRANSGRIDV5_20180116135943","2017-11-23T06:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-51.499499999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72210,"TRANSGRIDV5_20180116135943","2017-11-23T08:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-39.083460000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72261,"TRANSGRIDV5_20180116135943","2017-11-23T04:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.048570000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72306,"TRANSGRIDV5_20180116135943","2017-11-23T03:05:00","NSA_S_POR01_ISLD","NSA-S_POR01_ISLD","2014-10-15",1,14125.156349999999,"Network Support Agreement for Port Lincoln Units 1 and 2 to meet local islanded demand for the planned outage.","OUTAGE","OTHER","NSA for Port Lincoln","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[72336,"TRANSGRIDV5_20180116135943","2017-11-23T03:15:00","NSA_S_POR03_ISLD","NSA-S_POR03_ISLD","2014-10-15",1,14120.00387,"Network Support Agreement for Port Lincoln Unit 3 to meet local islanded demand for the planned outage.","OUTAGE","OTHER","NSA for Port Lincoln","REGULATED","99","Non Inclusion",null,0,"ElectraNet"]
[72366,"TRANSGRIDV5_20180116135943","2017-11-24T15:40:00","#MP2_E","#MP2_E","2017-11-24",2,-1073.8499200000001,"NMTP2.ENERGY * 1 <= 660 (Wt = 360)","OUTAGE","OTHER","Mt Piper Generator","REGULATED","99","Non Inclusion",null,0]
[72392,"TRANSGRIDV5_20180116135943","2017-11-24T15:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-88.204499999999996,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72463,"TRANSGRIDV5_20180116135943","2017-11-24T10:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-40.467919999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72493,"TRANSGRIDV5_20180116135943","2017-11-24T10:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-32.190159999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72519,"TRANSGRIDV5_20180116135943","2017-11-24T05:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-23.219390000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72590,"TRANSGRIDV5_20180116135943","2017-11-24T23:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-13.386139999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72616,"TRANSGRIDV5_20180116135943","2017-11-25T06:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-52.384360000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72646,"TRANSGRIDV5_20180116135943","2017-11-25T01:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-27.241029999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72676,"TRANSGRIDV5_20180116135943","2017-11-25T00:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.36411,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72743,"TRANSGRIDV5_20180116135943","2017-11-25T09:20:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-13.40653,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[72773,"TRANSGRIDV5_20180116135943","2017-11-25T00:05:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-42.742280000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72799,"TRANSGRIDV5_20180116135943","2017-11-25T09:20:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.086259999999999,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72870,"TRANSGRIDV5_20180116135943","2017-11-26T06:25:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-17.065149999999999,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[72900,"TRANSGRIDV5_20180116135943","2017-11-26T12:40:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-11.2134,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[72926,"TRANSGRIDV5_20180116135943","2017-11-26T11:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-25.43779,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[72997,"TRANSGRIDV5_20180116135943","2017-11-26T08:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-10.294370000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73027,"TRANSGRIDV5_20180116135943","2017-11-27T13:55:00","#MP2_E","#MP2_E","2017-11-24",2,-14.19196,"NMTP2.ENERGY * 1 <= 660 (Wt = 360)","OUTAGE","OTHER","Mt Piper Generator","REGULATED","99","Non Inclusion",null,0]
[73053,"TRANSGRIDV5_20180116135943","2017-11-27T23:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-100.55216,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73124,"TRANSGRIDV5_20180116135943","2017-11-28T22:25:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-82.214449999999999,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[73150,"TRANSGRIDV5_20180116135943","2017-11-28T15:55:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,37.549970000000002,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73180,"TRANSGRIDV5_20180116135943","2017-11-28T15:05:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,20.62,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73210,"TRANSGRIDV5_20180116135943","2017-11-28T05:55:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,45.984870000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73277,"TRANSGRIDV5_20180116135943","2017-11-28T13:20:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,138.46816000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73307,"TRANSGRIDV5_20180116135943","2017-11-28T17:35:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,44.533169999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73333,"TRANSGRIDV5_20180116135943","2017-11-28T16:50:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,28.99,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73404,"TRANSGRIDV5_20180116135943","2017-11-28T06:50:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,17.98,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8E","REGULATED","INCLUDED","","PLANNED",1]
[73434,"TRANSGRIDV5_20180116135943","2017-11-28T21:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-36.833759999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73460,"TRANSGRIDV5_20180116135943","2017-11-28T15:05:00","N^^V_SMTXH1_1","V-SMTS_HTX_R","2015-08-07",1,-125.54003,"Out = South Morang H1 or H2 500/330 kV txfmr, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","South Morang 500/330 kV txfmr","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[73531,"TRANSGRIDV5_20180116135943","2017-11-28T09:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-28.55189,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[73561,"TRANSGRIDV5_20180116135943","2017-11-28T11:50:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-20.956900000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[73587,"TRANSGRIDV5_20180116135943","2017-11-28T07:45:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-10.73455,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[73658,"TRANSGRIDV5_20180116135943","2017-11-29T21:05:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-173.69,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[73684,"TRANSGRIDV5_20180116135943","2017-11-29T00:25:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-75.580150000000003,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[73740,"TRANSGRIDV5_20180116135943","2017-11-29T18:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-303.73779999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73743,"TRANSGRIDV5_20180116135943","2017-11-29T18:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-263.34965999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73810,"TRANSGRIDV5_20180116135943","2017-11-29T16:55:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-625.14205000000004,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[73840,"TRANSGRIDV5_20180116135943","2017-11-30T11:20:00","#BOCORWF1_E","#BOCORWF1_E","2017-11-30",1,-1224.42903,"NCMA3B.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","BOCO Rock Wind farm","REGULATED","99","Non Inclusion",null,0]
[73870,"TRANSGRIDV5_20180116135943","2017-11-30T16:00:00","#BOCORWF1_E","#BOCORWF1_E","2017-11-30",1,-1108.26053,"NCMA3B.ENERGY * 1 <= 0 (Wt = 360)","OUTAGE","OTHER","BOCO Rock Wind farm","REGULATED","99","Non Inclusion",null,0]
[73937,"TRANSGRIDV5_20180116135943","2017-11-30T06:55:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-362.88,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[73967,"TRANSGRIDV5_20180116135943","2017-11-30T07:40:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-245.77,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[73993,"TRANSGRIDV5_20180116135943","2017-11-30T07:30:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-206.32668000000001,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[74064,"TRANSGRIDV5_20180116135943","2017-11-30T15:45:00","#RT_VIC1_P_E","#RT_VIC1_PE","2017-11-30",1,5255130.52477,"VRT1.ENERGY * 1 = 15 (Wt = 1140)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[74094,"TRANSGRIDV5_20180116135943","2017-11-30T20:20:00","#RT_VIC1_P_E","#RT_VIC1_PE","2017-11-30",1,5255095.0329999998,"VRT1.ENERGY * 1 = 15 (Wt = 1140)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[74120,"TRANSGRIDV5_20180116135943","2017-11-30T18:25:00","#RT_VIC1_P_E","#RT_VIC1_PE","2017-11-30",1,5255085.0329999998,"VRT1.ENERGY * 1 = 15 (Wt = 1140)","SYSTEM NORMAL","OTHER",null,"","",null,null,0]
[74191,"TRANSGRIDV5_20180116135943","2017-11-30T08:30:00","F_Q++ARDM_L5","F-N-ARDM_ONE","2013-08-21",1,16.140080000000001,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 5 min Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8C","REGULATED","INCLUDED","","PLANNED",1]
[74217,"TRANSGRIDV5_20180116135943","2017-11-30T11:20:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,28.99,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8C","REGULATED","INCLUDED","","PLANNED",1]
[74247,"TRANSGRIDV5_20180116135943","2017-11-30T10:15:00","F_Q++ARDM_L6","F-N-ARDM_ONE","2013-08-21",1,17.989999999999998,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 6 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8C","REGULATED","INCLUDED","","PLANNED",1]
[74277,"TRANSGRIDV5_20180116135943","2017-11-30T07:00:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,144.99,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8C","REGULATED","INCLUDED","","PLANNED",1]
[74344,"TRANSGRIDV5_20180116135943","2017-11-30T07:55:00","F_Q++ARDM_L60","F-N-ARDM_ONE","2013-08-21",1,17.97,"Out = one Armidale to Bulli Creek (8C, 8E, 8L or 8M) line, Qld Lower 60 sec Requirement","OUTAGE","FCAS","Armidale - Dumeresq 330kV LINE 8C","REGULATED","INCLUDED","","PLANNED",1]
[74374,"TRANSGRIDV5_20180116135943","2017-11-30T11:15:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-151.68618000000001,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[74404,"TRANSGRIDV5_20180116135943","2017-11-30T04:30:00","N_MBTE1_B","N-MBTE_1","2013-11-25",1,-37.314839999999997,"Out= one Directlink cable, Qld to NSW limit","OUTAGE","OTHER","Directlk-N Directlk-Q DC1 80kV LINE","REGULATED","99","Non Inclusion",null,0]
[74471,"TRANSGRIDV5_20180116135943","2017-11-30T10:05:00","QNTE_150","I-QNTE_150","2014-01-08",1,-53.393500000000003,"Qld to NSW on Terranora Interconnector upper transfer limit of 150 MW","OUTAGE","OTHER","Lismore Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[74501,"TRANSGRIDV5_20180116135943","2017-12-01T20:20:00","#HDWF3_E","#HDWF3_E","2017-11-13",1,-136.41835,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[74527,"TRANSGRIDV5_20180116135943","2017-12-01T23:15:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-140.71816000000001,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[74598,"TRANSGRIDV5_20180116135943","2017-12-01T15:55:00","V>>N-NIL_HA","N-NIL","2017-08-11",1,-19.81887,"Out = Nil, avoid Murray to Upper Tumut(65) O/L on Murray to Lower Tumut(66) trip; Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[74628,"TRANSGRIDV5_20180116135943","2017-12-02T08:00:00","#HDWF3_E","#HDWF3_E","2017-11-13",1,-1067.26,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[74654,"TRANSGRIDV5_20180116135943","2017-12-02T08:05:00","#HPRG1_R5","#HPRG1_F","2017-12-02",1,-23.161110000000001,"(SMTL1H.RAISE5MIN + SMTL1H.RAISEREG) * 1 <= 0 (Wt = 4)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[74684,"TRANSGRIDV5_20180116135943","2017-12-02T08:55:00","#HPRL1_L5","#HPRL1_F","2017-12-02",1,-20.8,"(SMTL2H.LOWER5MIN + SMTL2H.LOWERREG) * 1 <= 0 (Wt = 4)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[74755,"TRANSGRIDV5_20180116135943","2017-12-02T01:50:00","#KIATAWF1_E","#KIATAWF1_E","2017-11-20",1,-133.79442,"VHOG1K.ENERGY * 1 <= 17 (Wt = 360)","OUTAGE","OTHER","Kiata Wind farm","REGULATED","99","Non Inclusion",null,0]
[74781,"TRANSGRIDV5_20180116135943","2017-12-02T23:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1078.4100000000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[74811,"TRANSGRIDV5_20180116135943","2017-12-02T08:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1069.49,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[74878,"TRANSGRIDV5_20180116135943","2017-12-02T18:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1064.94,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[74908,"TRANSGRIDV5_20180116135943","2017-12-02T16:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1063.69,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[74938,"TRANSGRIDV5_20180116135943","2017-12-02T16:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1063.29,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75005,"TRANSGRIDV5_20180116135943","2017-12-02T11:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1059.53,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75035,"TRANSGRIDV5_20180116135943","2017-12-02T04:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1056.58,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75061,"TRANSGRIDV5_20180116135943","2017-12-02T05:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1050.69,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75132,"TRANSGRIDV5_20180116135943","2017-12-02T08:30:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1066.78,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75137,"TRANSGRIDV5_20180116135943","2017-12-02T20:35:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1066.25,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75187,"TRANSGRIDV5_20180116135943","2017-12-02T16:15:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1063.69,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75217,"TRANSGRIDV5_20180116135943","2017-12-02T09:40:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1063.25,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75288,"TRANSGRIDV5_20180116135943","2017-12-02T15:10:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1058.96,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75314,"TRANSGRIDV5_20180116135943","2017-12-02T03:35:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1055.46,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75344,"TRANSGRIDV5_20180116135943","2017-12-03T17:35:00","#HDWF3_E","#HDWF3_E","2017-11-13",1,-1064.52,"SHDW3H.ENERGY * 1 <= 98 (Wt = 360)","OUTAGE","OTHER","Hornsdale Wind Farm","REGULATED","99","Non Inclusion",null,0]
[75411,"TRANSGRIDV5_20180116135943","2017-12-03T10:00:00","#HPRG1_R6","#HPRG1_F","2017-12-03",1,-20.49,"SMTL1H.RAISE6SEC * 1 <= 0 (Wt = 8)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[75441,"TRANSGRIDV5_20180116135943","2017-12-03T08:50:00","#HPRL1_L5","#HPRL1_F","2017-12-03",1,-23.22653,"(SMTL2H.LOWER5MIN + SMTL2H.LOWERREG) * 1 <= 0 (Wt = 4)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[75471,"TRANSGRIDV5_20180116135943","2017-12-03T09:35:00","#HPRL1_RR","#HPRL1_F","2017-12-03",1,-24.99,"SMTL2H.RAISEREG * 1 <= 0 (Wt = 10)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[75538,"TRANSGRIDV5_20180116135943","2017-12-03T05:00:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1069.18,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75568,"TRANSGRIDV5_20180116135943","2017-12-03T17:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1064.26,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75594,"TRANSGRIDV5_20180116135943","2017-12-03T07:40:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1063.69,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75665,"TRANSGRIDV5_20180116135943","2017-12-03T11:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1056.06,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75695,"TRANSGRIDV5_20180116135943","2017-12-03T13:30:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-01",1,-1049.6400000000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[75721,"TRANSGRIDV5_20180116135943","2017-12-03T07:30:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1075.22,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75751,"TRANSGRIDV5_20180116135943","2017-12-03T06:25:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1069.7,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75822,"TRANSGRIDV5_20180116135943","2017-12-03T08:55:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1061.4100000000001,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75848,"TRANSGRIDV5_20180116135943","2017-12-03T14:00:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1056.78,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75878,"TRANSGRIDV5_20180116135943","2017-12-03T13:20:00","#TORRB4_P_E","#TORRB4_PE","2017-12-02",3,-1048.77,"STSB4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island B","REGULATED","99","Non Inclusion",null,0]
[75945,"TRANSGRIDV5_20180116135943","2017-12-04T05:45:00","#R016579_013_RAMP_F","#R016579_RAMP","2017-12-03",1,-12.78828,"Hard Ramping constraint for constraint N^^V_DDWG, Effective Date: 07/08/2015, Version: 1","OUTAGE","RAMP","Wagga - Jindera 330kV LINE 62","REGULATED","10","Ramping Constraint","PLANNED",0]
[75975,"TRANSGRIDV5_20180116135943","2017-12-04T04:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.551589999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76005,"TRANSGRIDV5_20180116135943","2017-12-04T18:55:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-12.57938,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Lismore Koolkhan 132kV LINE 967","REGULATED","INCLUDED","","PLANNED",1]
[76072,"TRANSGRIDV5_20180116135943","2017-12-05T14:10:00","#KSP1_E","#KSP1_E","2017-12-04",1,-161.6,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[76102,"TRANSGRIDV5_20180116135943","2017-12-05T20:20:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-87.000699999999995,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[76132,"TRANSGRIDV5_20180116135943","2017-12-05T05:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-20.428750000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76199,"TRANSGRIDV5_20180116135943","2017-12-06T06:45:00","#HPRG1_R5","#HPRG1_F","2017-12-06",2,-26.666889999999999,"(SMTL1H.RAISE5MIN + SMTL1H.RAISEREG) * 1 <= 0 (Wt = 4)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[76229,"TRANSGRIDV5_20180116135943","2017-12-06T07:50:00","#HPRG1_R6","#HPRG1_F","2017-12-06",2,-20.5,"SMTL1H.RAISE6SEC * 1 <= 0 (Wt = 8)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[76255,"TRANSGRIDV5_20180116135943","2017-12-06T08:05:00","#HPRG1_R60","#HPRG1_F","2017-12-06",2,-14,"SMTL1H.RAISE60SEC * 1 <= 0 (Wt = 6)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[76285,"TRANSGRIDV5_20180116135943","2017-12-06T08:30:00","#HPRL1_L5","#HPRL1_F","2017-12-06",1,-20.8,"(SMTL2H.LOWER5MIN + SMTL2H.LOWERREG) * 1 <= 0 (Wt = 4)","OUTAGE","OTHER","Hornsdale Battery Power Reserve","REGULATED","99","Non Inclusion",null,0]
[76356,"TRANSGRIDV5_20180116135943","2017-12-06T14:35:00","#KSP1_E","#KSP1_E","2017-12-04",1,-161.33706000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[76382,"TRANSGRIDV5_20180116135943","2017-12-06T12:55:00","#KSP1_E","#KSP1_E","2017-12-04",1,-152.87001000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[76412,"TRANSGRIDV5_20180116135943","2017-12-06T16:45:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-89.723050000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[76479,"TRANSGRIDV5_20180116135943","2017-12-06T10:35:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-74.950620000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[76509,"TRANSGRIDV5_20180116135943","2017-12-06T13:55:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-71.598990000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[76539,"TRANSGRIDV5_20180116135943","2017-12-06T21:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-55.557980000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76606,"TRANSGRIDV5_20180116135943","2017-12-06T03:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-11.9139,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76616,"TRANSGRIDV5_20180116135943","2017-12-06T06:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-10.807180000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76665,"TRANSGRIDV5_20180116135943","2017-12-07T14:00:00","#KSP1_E","#KSP1_E","2017-12-04",1,-166.11116999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[76691,"TRANSGRIDV5_20180116135943","2017-12-07T12:10:00","#KSP1_E","#KSP1_E","2017-12-04",1,-152.86999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[76762,"TRANSGRIDV5_20180116135943","2017-12-07T18:30:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-13.82563,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[76788,"TRANSGRIDV5_20180116135943","2017-12-07T21:20:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-10.507860000000001,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[76818,"TRANSGRIDV5_20180116135943","2017-12-07T10:45:00","N^^V_DDSM1","V-DDSM","2015-08-07",1,-28.361460000000001,"Out = Dederang to South Morang 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Dederang - South Morang 330 kV line","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[76889,"TRANSGRIDV5_20180116135943","2017-12-07T02:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-42.999119999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76915,"TRANSGRIDV5_20180116135943","2017-12-07T01:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.843380000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[76945,"TRANSGRIDV5_20180116135943","2017-12-07T09:35:00","NSA_Q_GSTONE34_200","NSA-Q_GSTONE34_200","2015-10-07",1,12.73005,"Gladstone 3+4 >= 200 for Network Support Agreement","OUTAGE","OTHER","Gladstone 3+4 >= 200 for Network Support Agreement","REGULATED","99","Non Inclusion",null,0,"PowerLink outage"]
[77016,"TRANSGRIDV5_20180116135943","2017-12-08T09:05:00","#MP2_E","#MP2_E","2017-11-24",2,-95.41386,"NMTP2.ENERGY * 1 <= 660 (Wt = 360)","OUTAGE","OTHER","Mt Piper Generator","REGULATED","99","Non Inclusion",null,0]
[77042,"TRANSGRIDV5_20180116135943","2017-12-08T08:00:00","#MP2_E","#MP2_E","2017-11-24",2,-73.946100000000001,"NMTP2.ENERGY * 1 <= 660 (Wt = 360)","OUTAGE","OTHER","Mt Piper Generator","REGULATED","99","Non Inclusion",null,0]
[77072,"TRANSGRIDV5_20180116135943","2017-12-08T11:40:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-16.513439999999999,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[77139,"TRANSGRIDV5_20180116135943","2017-12-08T23:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-46.293640000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77169,"TRANSGRIDV5_20180116135943","2017-12-08T04:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-23.259979999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77199,"TRANSGRIDV5_20180116135943","2017-12-08T02:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-11.456849999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77225,"TRANSGRIDV5_20180116135943","2017-12-09T21:35:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-69.529120000000006,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77296,"TRANSGRIDV5_20180116135943","2017-12-09T13:00:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-60.000140000000002,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77322,"TRANSGRIDV5_20180116135943","2017-12-09T17:30:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-14.522629999999999,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[77352,"TRANSGRIDV5_20180116135943","2017-12-09T14:40:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-11.61106,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[77423,"TRANSGRIDV5_20180116135943","2017-12-09T22:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-43.839440000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77449,"TRANSGRIDV5_20180116135943","2017-12-09T06:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-31.871870000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77479,"TRANSGRIDV5_20180116135943","2017-12-09T05:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-25.846409999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77550,"TRANSGRIDV5_20180116135943","2017-12-10T12:25:00","#KSP1_E","#KSP1_E","2017-12-04",1,-147.68039999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[77576,"TRANSGRIDV5_20180116135943","2017-12-10T12:00:00","#KSP1_E","#KSP1_E","2017-12-04",1,-146.37837999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[77606,"TRANSGRIDV5_20180116135943","2017-12-10T06:55:00","#KSP1_E","#KSP1_E","2017-12-04",1,-142.9555,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[77673,"TRANSGRIDV5_20180116135943","2017-12-10T06:45:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-66.010130000000004,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77703,"TRANSGRIDV5_20180116135943","2017-12-10T04:20:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-61.738370000000003,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77733,"TRANSGRIDV5_20180116135943","2017-12-10T01:30:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-60.000109999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77759,"TRANSGRIDV5_20180116135943","2017-12-10T05:50:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-60.000109999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[77830,"TRANSGRIDV5_20180116135943","2017-12-10T21:05:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-10.45303,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[77856,"TRANSGRIDV5_20180116135943","2017-12-10T20:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-58.874049999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77886,"TRANSGRIDV5_20180116135943","2017-12-10T20:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-36.87659,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77957,"TRANSGRIDV5_20180116135943","2017-12-10T11:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-21.996099999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[77983,"TRANSGRIDV5_20180116135943","2017-12-10T15:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-13.62907,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78013,"TRANSGRIDV5_20180116135943","2017-12-11T10:05:00","#KSP1_E","#KSP1_E","2017-12-04",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[78084,"TRANSGRIDV5_20180116135943","2017-12-11T23:35:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-68.810569999999998,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78095,"TRANSGRIDV5_20180116135943","2017-12-11T02:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-66.010109999999997,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78139,"TRANSGRIDV5_20180116135943","2017-12-11T03:30:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-60.000109999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78206,"TRANSGRIDV5_20180116135943","2017-12-11T16:30:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-10.152799999999999,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[78236,"TRANSGRIDV5_20180116135943","2017-12-11T20:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-56.899569999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78266,"TRANSGRIDV5_20180116135943","2017-12-11T10:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-49.251519999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78292,"TRANSGRIDV5_20180116135943","2017-12-11T21:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-42.064680000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78363,"TRANSGRIDV5_20180116135943","2017-12-11T17:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.591170000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78393,"TRANSGRIDV5_20180116135943","2017-12-12T11:45:00","#KSP1_E","#KSP1_E","2017-12-04",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[78419,"TRANSGRIDV5_20180116135943","2017-12-12T18:40:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-105.05285000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78490,"TRANSGRIDV5_20180116135943","2017-12-12T02:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-68.810149999999993,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78516,"TRANSGRIDV5_20180116135943","2017-12-12T05:15:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-66.010670000000005,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78546,"TRANSGRIDV5_20180116135943","2017-12-12T02:15:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-60.000149999999998,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78576,"TRANSGRIDV5_20180116135943","2017-12-12T03:30:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,35.504489999999997,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[78643,"TRANSGRIDV5_20180116135943","2017-12-12T15:55:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,15.10338,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[78673,"TRANSGRIDV5_20180116135943","2017-12-12T23:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-85.814679999999996,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78699,"TRANSGRIDV5_20180116135943","2017-12-12T08:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-47.149259999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78770,"TRANSGRIDV5_20180116135943","2017-12-12T13:50:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-33.016930000000002,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78800,"TRANSGRIDV5_20180116135943","2017-12-12T11:10:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-20.56062,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78826,"TRANSGRIDV5_20180116135943","2017-12-12T12:35:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-16.324390000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[78897,"TRANSGRIDV5_20180116135943","2017-12-13T20:35:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-99.766949999999994,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78927,"TRANSGRIDV5_20180116135943","2017-12-13T01:45:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-59.589970000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[78953,"TRANSGRIDV5_20180116135943","2017-12-13T17:10:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-12.464650000000001,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[79024,"TRANSGRIDV5_20180116135943","2017-12-13T00:30:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-36.225499999999997,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79050,"TRANSGRIDV5_20180116135943","2017-12-14T16:50:00","#KSP1_E","#KSP1_E","2017-12-04",1,-189.53282999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79080,"TRANSGRIDV5_20180116135943","2017-12-14T13:20:00","#KSP1_E","#KSP1_E","2017-12-04",1,-176.51310000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79110,"TRANSGRIDV5_20180116135943","2017-12-14T11:25:00","#KSP1_E","#KSP1_E","2017-12-04",1,-171.04141000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79177,"TRANSGRIDV5_20180116135943","2017-12-14T16:40:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-12.78299,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[79207,"TRANSGRIDV5_20180116135943","2017-12-14T20:35:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-11.208780000000001,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[79233,"TRANSGRIDV5_20180116135943","2017-12-14T00:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-103.26721000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79304,"TRANSGRIDV5_20180116135943","2017-12-14","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.092700000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79334,"TRANSGRIDV5_20180116135943","2017-12-14T02:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-11.978070000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79360,"TRANSGRIDV5_20180116135943","2017-12-15T11:40:00","#KSP1_E","#KSP1_E","2017-12-04",1,-161.91515999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79431,"TRANSGRIDV5_20180116135943","2017-12-15T12:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-63.931139999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79461,"TRANSGRIDV5_20180116135943","2017-12-15T00:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-52.755229999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79487,"TRANSGRIDV5_20180116135943","2017-12-15T21:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-48.102049999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79532,"TRANSGRIDV5_20180116135943","2017-12-15T07:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-38.604349999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79583,"TRANSGRIDV5_20180116135943","2017-12-15T08:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-25.806920000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79613,"TRANSGRIDV5_20180116135943","2017-12-15T08:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.986740000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79643,"TRANSGRIDV5_20180116135943","2017-12-16T10:30:00","#KSP1_E","#KSP1_E","2017-12-04",1,-161.6,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79710,"TRANSGRIDV5_20180116135943","2017-12-16T21:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-78.628020000000006,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[79740,"TRANSGRIDV5_20180116135943","2017-12-16T05:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-109.73278000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79770,"TRANSGRIDV5_20180116135943","2017-12-16T05:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-60.339680000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79837,"TRANSGRIDV5_20180116135943","2017-12-16T03:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-12.80161,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[79867,"TRANSGRIDV5_20180116135943","2017-12-17T14:00:00","#KSP1_E","#KSP1_E","2017-12-04",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79893,"TRANSGRIDV5_20180116135943","2017-12-17T13:00:00","#KSP1_E","#KSP1_E","2017-12-04",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[79964,"TRANSGRIDV5_20180116135943","2017-12-17T13:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-69.890640000000005,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[79994,"TRANSGRIDV5_20180116135943","2017-12-17T13:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-42.86645,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80020,"TRANSGRIDV5_20180116135943","2017-12-17T21:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-18.325890000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80091,"TRANSGRIDV5_20180116135943","2017-12-18T11:25:00","#KSP1_E","#KSP1_E","2017-12-04",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80117,"TRANSGRIDV5_20180116135943","2017-12-18T11:10:00","#KSP1_E","#KSP1_E","2017-12-04",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80147,"TRANSGRIDV5_20180116135943","2017-12-18T16:55:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-138.86179999999999,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[80177,"TRANSGRIDV5_20180116135943","2017-12-18T05:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-29.64395,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80244,"TRANSGRIDV5_20180116135943","2017-12-18T10:40:00","N_X_MBTE_3B","N-X_MBTE_3","2013-11-25",1,-14.619680000000001,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[80274,"TRANSGRIDV5_20180116135943","2017-12-18T14:00:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-97.688820000000007,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80304,"TRANSGRIDV5_20180116135943","2017-12-18T17:00:00","S>NIL_NIL_NWMH2","S-NIL","2016-09-13",1,-44.833579999999998,"Out= Nil, avoid O/L North West Bend-Monash #2 132kV on Nil trip, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80371,"TRANSGRIDV5_20180116135943","2017-12-19T08:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.349980000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80401,"TRANSGRIDV5_20180116135943","2017-12-19T08:45:00","N_X_MBTE2_B","N-X_MBTE_2","2013-11-25",1,-15.38547,"Out= two Directlink cables, Qld to NSW limit","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[80427,"TRANSGRIDV5_20180116135943","2017-12-19T08:25:00","Q:N_NIL_AR_2L-G","Q-NIL","2014-01-08",1,-31.712620000000001,"Out=Nil, limit Qld to NSW on QNI to avoid transient instability for a 2L-G fault at Armidale","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80498,"TRANSGRIDV5_20180116135943","2017-12-19T14:40:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-23.830539999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80528,"TRANSGRIDV5_20180116135943","2017-12-20T23:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-66.121459999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80554,"TRANSGRIDV5_20180116135943","2017-12-21T19:05:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-99.600110000000001,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[80584,"TRANSGRIDV5_20180116135943","2017-12-21T22:10:00","#WRWF1_E","#WRWF1_E","2017-09-24",1,-73.511430000000004,"NWRK1W.ENERGY * 1 <= 53 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[80655,"TRANSGRIDV5_20180116135943","2017-12-21T06:50:00","N^^V_MSUT_1","I-MSUT","2015-08-07",1,-23.216909999999999,"Out = Murray to Upper Tumut 330 kV line, avoid voltage collapse in Southern NSW for loss of the largest VIC generating unit or Basslink","OUTAGE","OTHER","Murray - Upr Tumut 330kV LINE 65","REGULATED","INCLUDED","","PLANNED",1]
[80681,"TRANSGRIDV5_20180116135943","2017-12-21T23:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-85.767330000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80711,"TRANSGRIDV5_20180116135943","2017-12-21T14:50:00","N_X_MBTE_3A","N-X_MBTE_3","2013-11-25",1,-21.606359999999999,"Out= all three Directlink cables, Terranora_I/C_import <= Terranora_Load","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[80778,"TRANSGRIDV5_20180116135943","2017-12-22T14:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-157.63874000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80808,"TRANSGRIDV5_20180116135943","2017-12-22T12:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80838,"TRANSGRIDV5_20180116135943","2017-12-22T23:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-41.107880000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[80905,"TRANSGRIDV5_20180116135943","2017-12-23T17:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-195.87009,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80935,"TRANSGRIDV5_20180116135943","2017-12-23T14:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[80961,"TRANSGRIDV5_20180116135943","2017-12-23T12:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-164.41130999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[81011,"TRANSGRIDV5_20180116135943","2017-12-23T07:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.67612,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[81061,"TRANSGRIDV5_20180116135943","2017-12-23T23:40:00","#TORRA1_P_E","#TORRA1_PE","2017-12-23",1,-1076.2841000000001,"STSA1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81087,"TRANSGRIDV5_20180116135943","2017-12-23T20:40:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-1102.7086999999999,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81117,"TRANSGRIDV5_20180116135943","2017-12-23T22:40:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-1072.9303500000001,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81188,"TRANSGRIDV5_20180116135943","2017-12-24T12:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1076.51404,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[81214,"TRANSGRIDV5_20180116135943","2017-12-24T20:00:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1066.6890699999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[81244,"TRANSGRIDV5_20180116135943","2017-12-24T15:00:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1064.1091699999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[81311,"TRANSGRIDV5_20180116135943","2017-12-24T15:15:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1057.6667199999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[81341,"TRANSGRIDV5_20180116135943","2017-12-24T16:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1050.1089300000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[81371,"TRANSGRIDV5_20180116135943","2017-12-24T00:20:00","#TORRA1_P_E","#TORRA1_PE","2017-12-23",1,-1059.0200600000001,"STSA1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81438,"TRANSGRIDV5_20180116135943","2017-12-24T09:15:00","#TORRA1_P_E","#TORRA1_PE","2017-12-23",1,-65.385599999999997,"STSA1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81468,"TRANSGRIDV5_20180116135943","2017-12-24T06:35:00","#TORRA1_P_E","#TORRA1_PE","2017-12-23",1,-59.654739999999997,"STSA1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81494,"TRANSGRIDV5_20180116135943","2017-12-24T03:55:00","#TORRA1_P_E","#TORRA1_PE","2017-12-23",1,-54.394599999999997,"STSA1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81565,"TRANSGRIDV5_20180116135943","2017-12-24T11:50:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-81.864900000000006,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81595,"TRANSGRIDV5_20180116135943","2017-12-24T09:15:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-65.385599999999997,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81621,"TRANSGRIDV5_20180116135943","2017-12-24T07:25:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-60.081769999999999,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81651,"TRANSGRIDV5_20180116135943","2017-12-24T04:00:00","#TORRA2_P_E","#TORRA2_PE","2017-12-23",1,-53.705190000000002,"STSA2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81722,"TRANSGRIDV5_20180116135943","2017-12-24T11:00:00","#TORRA4_P_E","#TORRA4_PE","2017-12-23",1,-81.78004,"STSA4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81748,"TRANSGRIDV5_20180116135943","2017-12-24T09:40:00","#TORRA4_P_E","#TORRA4_PE","2017-12-23",1,-65.661010000000005,"STSA4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81778,"TRANSGRIDV5_20180116135943","2017-12-24T06:55:00","#TORRA4_P_E","#TORRA4_PE","2017-12-23",1,-59.794989999999999,"STSA4.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81845,"TRANSGRIDV5_20180116135943","2017-12-24T12:20:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-79.457819999999998,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81875,"TRANSGRIDV5_20180116135943","2017-12-24T21:05:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-67.259119999999996,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81905,"TRANSGRIDV5_20180116135943","2017-12-24T20:40:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-64.382800000000003,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[81972,"TRANSGRIDV5_20180116135943","2017-12-24T18:45:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-59.677799999999998,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82002,"TRANSGRIDV5_20180116135943","2017-12-24T07:35:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-57.813519999999997,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82032,"TRANSGRIDV5_20180116135943","2017-12-24T04:00:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-53.705190000000002,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82099,"TRANSGRIDV5_20180116135943","2017-12-24T05:05:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,10.1729,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[82129,"TRANSGRIDV5_20180116135943","2017-12-24T18:35:00","N>>N-NIL__2_OPENED","N-NIL_RBKU_OPENED","2017-11-23",1,-11.075620000000001,"Out= Nil, avoid O/L Liddell to Tamworth (84) using 15 mins rating on trip of Liddell to Muswellbrook (83) line, Feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[82155,"TRANSGRIDV5_20180116135943","2017-12-24T14:15:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-25.16883,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[82185,"TRANSGRIDV5_20180116135943","2017-12-25T18:15:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1073.3442399999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82256,"TRANSGRIDV5_20180116135943","2017-12-25","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1062.2866100000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82282,"TRANSGRIDV5_20180116135943","2017-12-25T20:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1059.4525900000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82312,"TRANSGRIDV5_20180116135943","2017-12-25T06:50:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1051.18525,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82379,"TRANSGRIDV5_20180116135943","2017-12-25T06:35:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1039.66677,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82409,"TRANSGRIDV5_20180116135943","2017-12-25T01:45:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1036.39049,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82439,"TRANSGRIDV5_20180116135943","2017-12-25T07:55:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1026.63348,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[82490,"TRANSGRIDV5_20180116135943","2017-12-25T18:05:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-65.737189999999998,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82535,"TRANSGRIDV5_20180116135943","2017-12-25T21:40:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-62.7776,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82565,"TRANSGRIDV5_20180116135943","2017-12-25T15:50:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-60.047620000000002,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82591,"TRANSGRIDV5_20180116135943","2017-12-25T15:05:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-52.874789999999997,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82662,"TRANSGRIDV5_20180116135943","2017-12-25T05:45:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-39.863399999999999,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82688,"TRANSGRIDV5_20180116135943","2017-12-25T13:30:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-36.541049999999998,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82718,"TRANSGRIDV5_20180116135943","2017-12-25T04:00:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-27.316559999999999,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[82789,"TRANSGRIDV5_20180116135943","2017-12-25T05:30:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-59.899819999999998,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[82815,"TRANSGRIDV5_20180116135943","2017-12-25T16:50:00","I_CTRL_ISSUE_TE","I-CTRL_ISSUE_TE","2012-12-21",1,-12.38808,"DC Link Control Issue Constraint for Terranora","OUTAGE","OTHER","Terranora Interconnector","REGULATED","99","Non Inclusion",null,0]
[82845,"TRANSGRIDV5_20180116135943","2017-12-25T05:25:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-30.831939999999999,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[82912,"TRANSGRIDV5_20180116135943","2017-12-25T04:20:00","V::N_HWSM_V2","V-HWSM","2017-04-07",1,-47.279170000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Hazelwood - S Morang 500kV LINE 1","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[82942,"TRANSGRIDV5_20180116135943","2017-12-25T09:00:00","V::N_HWSM_V2","V-HWSM","2017-04-07",1,-22.147220000000001,"Out = Hazelwood to South Morang 500kV line, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Hazelwood - S Morang 500kV LINE 1","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[82972,"TRANSGRIDV5_20180116135943","2017-12-26T11:10:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1079.7657999999999,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[83039,"TRANSGRIDV5_20180116135943","2017-12-26T00:20:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1047.4878100000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[83069,"TRANSGRIDV5_20180116135943","2017-12-26T06:05:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1043.5651600000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[83099,"TRANSGRIDV5_20180116135943","2017-12-26T04:15:00","#OSB-AG_P_E","#OSB-AG_PE","2017-12-23",1,-1027.1719900000001,"SNBN1.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Osborne GT","REGULATED","99","Non Inclusion",null,0]
[83125,"TRANSGRIDV5_20180116135943","2017-12-26T11:30:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-73.737750000000005,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[83196,"TRANSGRIDV5_20180116135943","2017-12-26T02:05:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-55.018099999999997,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[83222,"TRANSGRIDV5_20180116135943","2017-12-26T02:15:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-44.524540000000002,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[83252,"TRANSGRIDV5_20180116135943","2017-12-26T05:35:00","#TORRB2_P_E","#TORRB2_PE","2017-12-24",2,-28.844449999999998,"STSB2.ENERGY * 1 <= 0 (Wt = 29)","OUTAGE","OTHER","Torrens Island GT","REGULATED","99","Non Inclusion",null,0]
[83323,"TRANSGRIDV5_20180116135943","2017-12-26T20:40:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-60.000160000000001,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83349,"TRANSGRIDV5_20180116135943","2017-12-26T22:00:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-59.900910000000003,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83379,"TRANSGRIDV5_20180116135943","2017-12-26T23:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-96.496350000000007,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83450,"TRANSGRIDV5_20180116135943","2017-12-26T19:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-12.033289999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83476,"TRANSGRIDV5_20180116135943","2017-12-26T03:30:00","S>V_NIL_NIL_RBNW","S-NIL","2016-09-13",1,-19.799430000000001,"Out = Nil, avoid overloading Robertstown-North West Bend #1 or #2 132kV lines for no contingencies, feedback","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83506,"TRANSGRIDV5_20180116135943","2017-12-26T04:05:00","V::N_X_HWSM_HWRO_V2","V-X_HWSM_HWRO3","2017-04-20",1,-33.545569999999998,"Out=Hazelwood-South Morang & Hazelwood-Rowville 500kV lines, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","OUTAGE","OTHER","Hazelwood - S Morang 500kV LINE","REGULATED","99","Non Inclusion",null,0,"AusNet outage"]
[83573,"TRANSGRIDV5_20180116135943","2017-12-27T00:05:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-60.637360000000001,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83603,"TRANSGRIDV5_20180116135943","2017-12-27T01:05:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-59.999679999999998,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83633,"TRANSGRIDV5_20180116135943","2017-12-27T01:45:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-47.00996,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83659,"TRANSGRIDV5_20180116135943","2017-12-27T15:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-322.17061999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83730,"TRANSGRIDV5_20180116135943","2017-12-27T08:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-36.532829999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83756,"TRANSGRIDV5_20180116135943","2017-12-27T09:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.767579999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83786,"TRANSGRIDV5_20180116135943","2017-12-27T18:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-14.97049,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83857,"TRANSGRIDV5_20180116135943","2017-12-28T05:55:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-60.838990000000003,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83883,"TRANSGRIDV5_20180116135943","2017-12-28T02:45:00","#WRWF1_E","#WRWF1_E","2017-12-22",1,-59.89996,"NWRK1W.ENERGY * 1 <= 130 (Wt = 360)","OUTAGE","OTHER","White Rock Wind Farm","REGULATED","99","Non Inclusion",null,0]
[83913,"TRANSGRIDV5_20180116135943","2017-12-28T09:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-83.822119999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83944,"TRANSGRIDV5_20180116135943","2017-12-28T10:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-67.075770000000006,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83945,"TRANSGRIDV5_20180116135943","2017-12-28T10:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-66.985669999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83946,"TRANSGRIDV5_20180116135943","2017-12-28T08:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-66.331320000000005,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83947,"TRANSGRIDV5_20180116135943","2017-12-28T11:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.88758,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83948,"TRANSGRIDV5_20180116135943","2017-12-28T10:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.855869999999996,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83949,"TRANSGRIDV5_20180116135943","2017-12-28T10:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.787319999999994,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83950,"TRANSGRIDV5_20180116135943","2017-12-28T10:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.490350000000007,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83951,"TRANSGRIDV5_20180116135943","2017-12-28T00:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.454710000000006,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83952,"TRANSGRIDV5_20180116135943","2017-12-28T10:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-65.316149999999993,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83953,"TRANSGRIDV5_20180116135943","2017-12-28T08:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-64.757069999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83954,"TRANSGRIDV5_20180116135943","2017-12-28T00:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-64.030609999999996,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83955,"TRANSGRIDV5_20180116135943","2017-12-28T11:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-63.71069,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83956,"TRANSGRIDV5_20180116135943","2017-12-28T11:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-61.802759999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83957,"TRANSGRIDV5_20180116135943","2017-12-28T06:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-60.345500000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83958,"TRANSGRIDV5_20180116135943","2017-12-28T10:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-60.038379999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83959,"TRANSGRIDV5_20180116135943","2017-12-28T11:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-57.053629999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83960,"TRANSGRIDV5_20180116135943","2017-12-28T11:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-56.572400000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83961,"TRANSGRIDV5_20180116135943","2017-12-28T10:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-55.734079999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83962,"TRANSGRIDV5_20180116135943","2017-12-28T06:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-52.778649999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83963,"TRANSGRIDV5_20180116135943","2017-12-28T07:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-51.193570000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83964,"TRANSGRIDV5_20180116135943","2017-12-28T02:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-51.075530000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83965,"TRANSGRIDV5_20180116135943","2017-12-28T07:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-50.055790000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83966,"TRANSGRIDV5_20180116135943","2017-12-28T06:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-49.97757,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83967,"TRANSGRIDV5_20180116135943","2017-12-28T06:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-47.769469999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83968,"TRANSGRIDV5_20180116135943","2017-12-28T12:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-47.446800000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83969,"TRANSGRIDV5_20180116135943","2017-12-28T06:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-46.320819999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83970,"TRANSGRIDV5_20180116135943","2017-12-28T08:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.820520000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83971,"TRANSGRIDV5_20180116135943","2017-12-28T06:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-45.52505,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83972,"TRANSGRIDV5_20180116135943","2017-12-28T05:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-44.42774,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83973,"TRANSGRIDV5_20180116135943","2017-12-28T05:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-44.311570000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83974,"TRANSGRIDV5_20180116135943","2017-12-28T06:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-42.770679999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83975,"TRANSGRIDV5_20180116135943","2017-12-28T01:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-41.237200000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83976,"TRANSGRIDV5_20180116135943","2017-12-28T01:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-40.751130000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83977,"TRANSGRIDV5_20180116135943","2017-12-28T06:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-39.382370000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83978,"TRANSGRIDV5_20180116135943","2017-12-28T00:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-38.087490000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83979,"TRANSGRIDV5_20180116135943","2017-12-28T06:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-37.915900000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83980,"TRANSGRIDV5_20180116135943","2017-12-28T01:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-37.622909999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83981,"TRANSGRIDV5_20180116135943","2017-12-28T11:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-37.102919999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83982,"TRANSGRIDV5_20180116135943","2017-12-28T10:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-35.670389999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83983,"TRANSGRIDV5_20180116135943","2017-12-28T01:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-35.414119999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83984,"TRANSGRIDV5_20180116135943","2017-12-28T11:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-35.307459999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83985,"TRANSGRIDV5_20180116135943","2017-12-28T01:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-35.259779999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83986,"TRANSGRIDV5_20180116135943","2017-12-28T00:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.991889999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83987,"TRANSGRIDV5_20180116135943","2017-12-28T01:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.469239999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83988,"TRANSGRIDV5_20180116135943","2017-12-28T01:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.311250000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83989,"TRANSGRIDV5_20180116135943","2017-12-28T11:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.908630000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83990,"TRANSGRIDV5_20180116135943","2017-12-28T07:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.422739999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83991,"TRANSGRIDV5_20180116135943","2017-12-28T00:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.402889999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83992,"TRANSGRIDV5_20180116135943","2017-12-28T02:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.36401,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83993,"TRANSGRIDV5_20180116135943","2017-12-28T02:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.117669999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83994,"TRANSGRIDV5_20180116135943","2017-12-28T04:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.013919999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83995,"TRANSGRIDV5_20180116135943","2017-12-28T06:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-32.890210000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83996,"TRANSGRIDV5_20180116135943","2017-12-28T01:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-31.709879999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83997,"TRANSGRIDV5_20180116135943","2017-12-28T23:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-31.253170000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83998,"TRANSGRIDV5_20180116135943","2017-12-28T06:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.478840000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[83999,"TRANSGRIDV5_20180116135943","2017-12-28T06:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-27.98958,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84000,"TRANSGRIDV5_20180116135943","2017-12-28T23:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-27.246839999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84001,"TRANSGRIDV5_20180116135943","2017-12-28T04:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-26.607679999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84002,"TRANSGRIDV5_20180116135943","2017-12-28T12:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-26.58445,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84003,"TRANSGRIDV5_20180116135943","2017-12-28T03:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-26.188210000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84004,"TRANSGRIDV5_20180116135943","2017-12-28T03:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-25.812550000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84005,"TRANSGRIDV5_20180116135943","2017-12-28T04:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-25.694109999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84006,"TRANSGRIDV5_20180116135943","2017-12-28T04:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-23.483080000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84007,"TRANSGRIDV5_20180116135943","2017-12-28T23:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-23.001850000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84008,"TRANSGRIDV5_20180116135943","2017-12-28T04:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-21.721620000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84009,"TRANSGRIDV5_20180116135943","2017-12-28T04:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-21.079879999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84010,"TRANSGRIDV5_20180116135943","2017-12-28T05:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-19.710170000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84011,"TRANSGRIDV5_20180116135943","2017-12-28T04:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-18.16676,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84012,"TRANSGRIDV5_20180116135943","2017-12-28T03:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-17.537500000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84013,"TRANSGRIDV5_20180116135943","2017-12-28T01:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.594429999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84014,"TRANSGRIDV5_20180116135943","2017-12-28T01:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-16.533539999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84015,"TRANSGRIDV5_20180116135943","2017-12-28T02:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-15.54163,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84016,"TRANSGRIDV5_20180116135943","2017-12-28T04:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-15.535349999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84017,"TRANSGRIDV5_20180116135943","2017-12-28T04:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-15.37618,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84018,"TRANSGRIDV5_20180116135943","2017-12-28T02:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-12.305009999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84019,"TRANSGRIDV5_20180116135943","2017-12-28T03:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-11.86469,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84020,"TRANSGRIDV5_20180116135943","2017-12-28T05:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-10.30254,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84021,"TRANSGRIDV5_20180116135943","2017-12-29T10:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-357.00205999999997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84022,"TRANSGRIDV5_20180116135943","2017-12-29T10:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-253.88988000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84023,"TRANSGRIDV5_20180116135943","2017-12-29T10:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-243.62834000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84024,"TRANSGRIDV5_20180116135943","2017-12-29T10:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-208.83851999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84025,"TRANSGRIDV5_20180116135943","2017-12-29T10:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-207.61378999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84026,"TRANSGRIDV5_20180116135943","2017-12-29T10:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-199.70062999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84027,"TRANSGRIDV5_20180116135943","2017-12-29T13:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-199.50405000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84028,"TRANSGRIDV5_20180116135943","2017-12-29T13:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-198.46253999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84029,"TRANSGRIDV5_20180116135943","2017-12-29T12:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-196.27466000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84030,"TRANSGRIDV5_20180116135943","2017-12-29T13:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-195.42009999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84031,"TRANSGRIDV5_20180116135943","2017-12-29T09:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-195.26795999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84032,"TRANSGRIDV5_20180116135943","2017-12-29T09:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84033,"TRANSGRIDV5_20180116135943","2017-12-29T09:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84034,"TRANSGRIDV5_20180116135943","2017-12-29T09:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84035,"TRANSGRIDV5_20180116135943","2017-12-29T09:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84036,"TRANSGRIDV5_20180116135943","2017-12-29T10:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84037,"TRANSGRIDV5_20180116135943","2017-12-29T10:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84038,"TRANSGRIDV5_20180116135943","2017-12-29T11:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84039,"TRANSGRIDV5_20180116135943","2017-12-29T11:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84040,"TRANSGRIDV5_20180116135943","2017-12-29T12:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-193.90625,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84041,"TRANSGRIDV5_20180116135943","2017-12-29T12:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-190.07012,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84042,"TRANSGRIDV5_20180116135943","2017-12-29T13:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-189.96308999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84043,"TRANSGRIDV5_20180116135943","2017-12-29T17:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-187.31782000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84044,"TRANSGRIDV5_20180116135943","2017-12-29T11:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-187.0651,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84045,"TRANSGRIDV5_20180116135943","2017-12-29T16:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-187.01573999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84046,"TRANSGRIDV5_20180116135943","2017-12-29T09:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-186.32424,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84047,"TRANSGRIDV5_20180116135943","2017-12-29T15:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-185.91466,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84048,"TRANSGRIDV5_20180116135943","2017-12-29T16:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-185.47803999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84049,"TRANSGRIDV5_20180116135943","2017-12-29T10:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-185.42537999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84050,"TRANSGRIDV5_20180116135943","2017-12-29T10:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-185.35203999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84051,"TRANSGRIDV5_20180116135943","2017-12-29T15:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-185.17840000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84052,"TRANSGRIDV5_20180116135943","2017-12-29T11:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-184.22995,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84053,"TRANSGRIDV5_20180116135943","2017-12-29T10:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-184.15603999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84054,"TRANSGRIDV5_20180116135943","2017-12-29T08:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-184.00541000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84055,"TRANSGRIDV5_20180116135943","2017-12-29T09:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-183.93769,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84056,"TRANSGRIDV5_20180116135943","2017-12-29T10:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-183.93177,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84057,"TRANSGRIDV5_20180116135943","2017-12-29T16:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-183.88284999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84058,"TRANSGRIDV5_20180116135943","2017-12-29T09:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-183.55070000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84059,"TRANSGRIDV5_20180116135943","2017-12-29T15:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-183.44156000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84060,"TRANSGRIDV5_20180116135943","2017-12-29T13:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-182.83859000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84061,"TRANSGRIDV5_20180116135943","2017-12-29T11:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-182.10890000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84062,"TRANSGRIDV5_20180116135943","2017-12-29T15:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-181.96222,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84063,"TRANSGRIDV5_20180116135943","2017-12-29T08:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-181.73944,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84064,"TRANSGRIDV5_20180116135943","2017-12-29T11:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-181.03351000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84065,"TRANSGRIDV5_20180116135943","2017-12-29T15:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.87418,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84066,"TRANSGRIDV5_20180116135943","2017-12-29T15:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.7089,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84067,"TRANSGRIDV5_20180116135943","2017-12-29T15:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.57829000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84068,"TRANSGRIDV5_20180116135943","2017-12-29T11:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.44085000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84069,"TRANSGRIDV5_20180116135943","2017-12-29T15:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.21996999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84070,"TRANSGRIDV5_20180116135943","2017-12-29T13:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.18339,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84071,"TRANSGRIDV5_20180116135943","2017-12-29T11:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.03513000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84072,"TRANSGRIDV5_20180116135943","2017-12-29T15:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-180.00753,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84073,"TRANSGRIDV5_20180116135943","2017-12-29T15:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-179.80909,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84074,"TRANSGRIDV5_20180116135943","2017-12-29T09:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-179.72909999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84075,"TRANSGRIDV5_20180116135943","2017-12-29T15:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-179.71225999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84076,"TRANSGRIDV5_20180116135943","2017-12-29T08:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-179.46866,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84077,"TRANSGRIDV5_20180116135943","2017-12-29T09:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.90513000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84078,"TRANSGRIDV5_20180116135943","2017-12-29T12:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.65899999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84079,"TRANSGRIDV5_20180116135943","2017-12-29T11:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.64904999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84080,"TRANSGRIDV5_20180116135943","2017-12-29T14:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.6309,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84081,"TRANSGRIDV5_20180116135943","2017-12-29T12:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.57065,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84082,"TRANSGRIDV5_20180116135943","2017-12-29T12:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.53639000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84083,"TRANSGRIDV5_20180116135943","2017-12-29T13:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.43016,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84084,"TRANSGRIDV5_20180116135943","2017-12-29T11:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-178.06147000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84085,"TRANSGRIDV5_20180116135943","2017-12-29T08:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84086,"TRANSGRIDV5_20180116135943","2017-12-29T13:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.89944,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84087,"TRANSGRIDV5_20180116135943","2017-12-29T14:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.76128,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84088,"TRANSGRIDV5_20180116135943","2017-12-29T14:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.68520000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84089,"TRANSGRIDV5_20180116135943","2017-12-29T13:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.53740999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84090,"TRANSGRIDV5_20180116135943","2017-12-29T13:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.52725000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84091,"TRANSGRIDV5_20180116135943","2017-12-29T14:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.09720999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84092,"TRANSGRIDV5_20180116135943","2017-12-29T14:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.08999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84093,"TRANSGRIDV5_20180116135943","2017-12-29T14:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.91369,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84094,"TRANSGRIDV5_20180116135943","2017-12-29T13:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.81253000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84095,"TRANSGRIDV5_20180116135943","2017-12-29T12:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.74743000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84096,"TRANSGRIDV5_20180116135943","2017-12-29T11:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.69470999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84097,"TRANSGRIDV5_20180116135943","2017-12-29T12:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.69469000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84098,"TRANSGRIDV5_20180116135943","2017-12-29T14:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.43921,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84099,"TRANSGRIDV5_20180116135943","2017-12-29T15:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.22311999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84100,"TRANSGRIDV5_20180116135943","2017-12-29T13:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-175.70217,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84101,"TRANSGRIDV5_20180116135943","2017-12-29T14:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-175.60616999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84102,"TRANSGRIDV5_20180116135943","2017-12-29T12:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-175.56180000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84103,"TRANSGRIDV5_20180116135943","2017-12-29T09:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-175.21235999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84104,"TRANSGRIDV5_20180116135943","2017-12-29T12:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-175.11288999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84105,"TRANSGRIDV5_20180116135943","2017-12-29T12:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.78,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84106,"TRANSGRIDV5_20180116135943","2017-12-29T09:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.66826,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84107,"TRANSGRIDV5_20180116135943","2017-12-29T08:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.62699000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84108,"TRANSGRIDV5_20180116135943","2017-12-29T14:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.29826,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84109,"TRANSGRIDV5_20180116135943","2017-12-29T12:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.27654999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84110,"TRANSGRIDV5_20180116135943","2017-12-29T08:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.95738,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84111,"TRANSGRIDV5_20180116135943","2017-12-29T11:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.8021,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84112,"TRANSGRIDV5_20180116135943","2017-12-29T14:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.63054,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84113,"TRANSGRIDV5_20180116135943","2017-12-29T14:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.53896,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84114,"TRANSGRIDV5_20180116135943","2017-12-29T14:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.53550999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84115,"TRANSGRIDV5_20180116135943","2017-12-29T08:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.45160999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84116,"TRANSGRIDV5_20180116135943","2017-12-29T08:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84117,"TRANSGRIDV5_20180116135943","2017-12-29T08:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84118,"TRANSGRIDV5_20180116135943","2017-12-29T08:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84119,"TRANSGRIDV5_20180116135943","2017-12-29T08:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84120,"TRANSGRIDV5_20180116135943","2017-12-29T08:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.05020999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84121,"TRANSGRIDV5_20180116135943","2017-12-29T07:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-165.69050999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84122,"TRANSGRIDV5_20180116135943","2017-12-29T07:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-164.86659,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84123,"TRANSGRIDV5_20180116135943","2017-12-29T07:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-164.26586,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84124,"TRANSGRIDV5_20180116135943","2017-12-29T07:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-164.26586,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84125,"TRANSGRIDV5_20180116135943","2017-12-29T07:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-164.13598999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84126,"TRANSGRIDV5_20180116135943","2017-12-29T07:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-159.66677999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84127,"TRANSGRIDV5_20180116135943","2017-12-29T07:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-155.33877000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84128,"TRANSGRIDV5_20180116135943","2017-12-29T07:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-154.04831999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84129,"TRANSGRIDV5_20180116135943","2017-12-29T07:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-153.99678,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84130,"TRANSGRIDV5_20180116135943","2017-12-29T07:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-153.15791999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84131,"TRANSGRIDV5_20180116135943","2017-12-29T07:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-150.93265,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84132,"TRANSGRIDV5_20180116135943","2017-12-29T07:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84133,"TRANSGRIDV5_20180116135943","2017-12-29T22:15:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-11.95349,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84134,"TRANSGRIDV5_20180116135943","2017-12-29T07:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-409.44578999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84135,"TRANSGRIDV5_20180116135943","2017-12-29T06:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-108.50688,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84136,"TRANSGRIDV5_20180116135943","2017-12-29T06:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-107.36966,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84137,"TRANSGRIDV5_20180116135943","2017-12-29T06:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-106.34950000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84138,"TRANSGRIDV5_20180116135943","2017-12-29T07:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-101.59668000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84139,"TRANSGRIDV5_20180116135943","2017-12-29T07:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-97.422719999999998,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84140,"TRANSGRIDV5_20180116135943","2017-12-29T07:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-86.312029999999993,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84141,"TRANSGRIDV5_20180116135943","2017-12-29T06:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-81.668080000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84142,"TRANSGRIDV5_20180116135943","2017-12-29T07:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-71.391580000000005,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84143,"TRANSGRIDV5_20180116135943","2017-12-29T00:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-59.822180000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84144,"TRANSGRIDV5_20180116135943","2017-12-29T06:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-55.810470000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84145,"TRANSGRIDV5_20180116135943","2017-12-29T06:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-55.719009999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84146,"TRANSGRIDV5_20180116135943","2017-12-29T06:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-54.707839999999997,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84147,"TRANSGRIDV5_20180116135943","2017-12-29T06:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-51.597000000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84148,"TRANSGRIDV5_20180116135943","2017-12-29T06:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-47.755450000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84149,"TRANSGRIDV5_20180116135943","2017-12-29T05:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-46.656880000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84150,"TRANSGRIDV5_20180116135943","2017-12-29T07:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-46.417729999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84151,"TRANSGRIDV5_20180116135943","2017-12-29","N^^V_NIL_1","V-NIL","2017-11-09",1,-37.207970000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84152,"TRANSGRIDV5_20180116135943","2017-12-29T05:15:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-34.007440000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84153,"TRANSGRIDV5_20180116135943","2017-12-29T07:35:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-33.932830000000003,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84154,"TRANSGRIDV5_20180116135943","2017-12-29T00:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-29.704350000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84155,"TRANSGRIDV5_20180116135943","2017-12-29T05:55:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-29.296430000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84156,"TRANSGRIDV5_20180116135943","2017-12-29T06:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.94971,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84157,"TRANSGRIDV5_20180116135943","2017-12-29T06:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.84273,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84158,"TRANSGRIDV5_20180116135943","2017-12-29T06:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-28.20992,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84159,"TRANSGRIDV5_20180116135943","2017-12-29T05:50:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-27.95542,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84160,"TRANSGRIDV5_20180116135943","2017-12-29T05:25:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-27.24614,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84161,"TRANSGRIDV5_20180116135943","2017-12-29T05:20:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-26.327400000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84162,"TRANSGRIDV5_20180116135943","2017-12-29T05:45:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-24.81934,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84163,"TRANSGRIDV5_20180116135943","2017-12-29T05:10:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-21.533200000000001,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84164,"TRANSGRIDV5_20180116135943","2017-12-29T05:40:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-19.768540000000002,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84165,"TRANSGRIDV5_20180116135943","2017-12-29T07:30:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-19.47824,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84166,"TRANSGRIDV5_20180116135943","2017-12-29T05:00:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-19.33071,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84167,"TRANSGRIDV5_20180116135943","2017-12-29T05:05:00","N^^V_NIL_1","V-NIL","2017-11-09",1,-18.238099999999999,"Out = Nil, avoid voltage collapse at Darlington Point for loss of the largest Vic generating unit or Basslink","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84168,"TRANSGRIDV5_20180116135943","2017-12-30T16:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84169,"TRANSGRIDV5_20180116135943","2017-12-30T15:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-187.67152999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84170,"TRANSGRIDV5_20180116135943","2017-12-30T16:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-187.01903999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84171,"TRANSGRIDV5_20180116135943","2017-12-30T14:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-177.52511999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84172,"TRANSGRIDV5_20180116135943","2017-12-30T16:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-176.43761000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84173,"TRANSGRIDV5_20180116135943","2017-12-30T16:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-174.31895,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84174,"TRANSGRIDV5_20180116135943","2017-12-30T15:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08006,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84175,"TRANSGRIDV5_20180116135943","2017-12-30T13:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84176,"TRANSGRIDV5_20180116135943","2017-12-30T15:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84177,"TRANSGRIDV5_20180116135943","2017-12-30T15:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84178,"TRANSGRIDV5_20180116135943","2017-12-30T16:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84179,"TRANSGRIDV5_20180116135943","2017-12-30T13:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84180,"TRANSGRIDV5_20180116135943","2017-12-30T13:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84181,"TRANSGRIDV5_20180116135943","2017-12-30T13:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84182,"TRANSGRIDV5_20180116135943","2017-12-30T13:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84183,"TRANSGRIDV5_20180116135943","2017-12-30T14:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84184,"TRANSGRIDV5_20180116135943","2017-12-30T14:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84185,"TRANSGRIDV5_20180116135943","2017-12-30T15:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84186,"TRANSGRIDV5_20180116135943","2017-12-30T15:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.73,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84187,"TRANSGRIDV5_20180116135943","2017-12-30T15:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.73,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84188,"TRANSGRIDV5_20180116135943","2017-12-30T15:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.51391000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84189,"TRANSGRIDV5_20180116135943","2017-12-30T15:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-167.21074999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84190,"TRANSGRIDV5_20180116135943","2017-12-30T14:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-166.82588999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84191,"TRANSGRIDV5_20180116135943","2017-12-30T15:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-165.1199,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84192,"TRANSGRIDV5_20180116135943","2017-12-30T13:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.83552,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84193,"TRANSGRIDV5_20180116135943","2017-12-30T14:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.51624000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84194,"TRANSGRIDV5_20180116135943","2017-12-30T14:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.48933,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84195,"TRANSGRIDV5_20180116135943","2017-12-30T14:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.48642000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84196,"TRANSGRIDV5_20180116135943","2017-12-30T14:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.47345999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84197,"TRANSGRIDV5_20180116135943","2017-12-30T13:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.32523,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84198,"TRANSGRIDV5_20180116135943","2017-12-30T13:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.32070999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84199,"TRANSGRIDV5_20180116135943","2017-12-30T14:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-162.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84200,"TRANSGRIDV5_20180116135943","2017-12-30T14:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-162.38526999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84201,"TRANSGRIDV5_20180116135943","2017-12-30T13:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84202,"TRANSGRIDV5_20180116135943","2017-12-30T13:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84203,"TRANSGRIDV5_20180116135943","2017-12-30T14:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84204,"TRANSGRIDV5_20180116135943","2017-12-30T14:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84205,"TRANSGRIDV5_20180116135943","2017-12-30T12:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.60006000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84206,"TRANSGRIDV5_20180116135943","2017-12-30T13:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.60006000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84207,"TRANSGRIDV5_20180116135943","2017-12-30T12:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.6,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84208,"TRANSGRIDV5_20180116135943","2017-12-30T13:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-158.60990000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84209,"TRANSGRIDV5_20180116135943","2017-12-30T10:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87003000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84210,"TRANSGRIDV5_20180116135943","2017-12-30T12:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84211,"TRANSGRIDV5_20180116135943","2017-12-30T12:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84212,"TRANSGRIDV5_20180116135943","2017-12-30T12:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.66005999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84213,"TRANSGRIDV5_20180116135943","2017-12-30T11:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84214,"TRANSGRIDV5_20180116135943","2017-12-30T11:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84215,"TRANSGRIDV5_20180116135943","2017-12-30T12:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84216,"TRANSGRIDV5_20180116135943","2017-12-30T12:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.66,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84217,"TRANSGRIDV5_20180116135943","2017-12-30T12:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-149.98625000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84218,"TRANSGRIDV5_20180116135943","2017-12-30T11:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-149.76539,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84219,"TRANSGRIDV5_20180116135943","2017-12-30T12:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-149.04335,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84220,"TRANSGRIDV5_20180116135943","2017-12-30T10:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84221,"TRANSGRIDV5_20180116135943","2017-12-30T11:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84222,"TRANSGRIDV5_20180116135943","2017-12-30T11:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84223,"TRANSGRIDV5_20180116135943","2017-12-30T12:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84224,"TRANSGRIDV5_20180116135943","2017-12-30T11:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.61479,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84225,"TRANSGRIDV5_20180116135943","2017-12-30T11:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.58786000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84226,"TRANSGRIDV5_20180116135943","2017-12-30T11:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.44265999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84227,"TRANSGRIDV5_20180116135943","2017-12-30T12:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.3124,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84228,"TRANSGRIDV5_20180116135943","2017-12-30T11:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.28516999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84229,"TRANSGRIDV5_20180116135943","2017-12-30T07:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.12481,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84230,"TRANSGRIDV5_20180116135943","2017-12-30T12:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.88123999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84231,"TRANSGRIDV5_20180116135943","2017-12-30T11:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.86455000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84232,"TRANSGRIDV5_20180116135943","2017-12-30T10:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84233,"TRANSGRIDV5_20180116135943","2017-12-30T10:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84234,"TRANSGRIDV5_20180116135943","2017-12-30T10:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84235,"TRANSGRIDV5_20180116135943","2017-12-30T11:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84236,"TRANSGRIDV5_20180116135943","2017-12-30T11:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84237,"TRANSGRIDV5_20180116135943","2017-12-30T08:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84238,"TRANSGRIDV5_20180116135943","2017-12-30T08:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84239,"TRANSGRIDV5_20180116135943","2017-12-30T09:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84240,"TRANSGRIDV5_20180116135943","2017-12-30T09:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84241,"TRANSGRIDV5_20180116135943","2017-12-30T09:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84242,"TRANSGRIDV5_20180116135943","2017-12-30T10:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84243,"TRANSGRIDV5_20180116135943","2017-12-30T10:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84244,"TRANSGRIDV5_20180116135943","2017-12-30T10:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84245,"TRANSGRIDV5_20180116135943","2017-12-30T10:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84246,"TRANSGRIDV5_20180116135943","2017-12-30T10:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84247,"TRANSGRIDV5_20180116135943","2017-12-30T10:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84248,"TRANSGRIDV5_20180116135943","2017-12-30T10:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84249,"TRANSGRIDV5_20180116135943","2017-12-30T09:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.33734000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84250,"TRANSGRIDV5_20180116135943","2017-12-30T09:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.27985000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84251,"TRANSGRIDV5_20180116135943","2017-12-30T09:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.24915999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84252,"TRANSGRIDV5_20180116135943","2017-12-30T09:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.22353000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84253,"TRANSGRIDV5_20180116135943","2017-12-30T09:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.83527000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84254,"TRANSGRIDV5_20180116135943","2017-12-30T09:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.83527000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84255,"TRANSGRIDV5_20180116135943","2017-12-30T09:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.83527000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84256,"TRANSGRIDV5_20180116135943","2017-12-30T09:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.52122,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84257,"TRANSGRIDV5_20180116135943","2017-12-30T08:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.46943999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84258,"TRANSGRIDV5_20180116135943","2017-12-30T08:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.46078,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84259,"TRANSGRIDV5_20180116135943","2017-12-30T07:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.43916999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84260,"TRANSGRIDV5_20180116135943","2017-12-30T08:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.16757999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84261,"TRANSGRIDV5_20180116135943","2017-12-30T08:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.13815,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84262,"TRANSGRIDV5_20180116135943","2017-12-30T09:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.02898999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84263,"TRANSGRIDV5_20180116135943","2017-12-30T08:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.90893,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84264,"TRANSGRIDV5_20180116135943","2017-12-30T08:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.86622,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84265,"TRANSGRIDV5_20180116135943","2017-12-30T06:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.68797000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84266,"TRANSGRIDV5_20180116135943","2017-12-30T08:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.4546,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84267,"TRANSGRIDV5_20180116135943","2017-12-30T08:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.19367,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84268,"TRANSGRIDV5_20180116135943","2017-12-30T07:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.07772,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84269,"TRANSGRIDV5_20180116135943","2017-12-30T08:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.04024999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84270,"TRANSGRIDV5_20180116135943","2017-12-30T06:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.93101999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84271,"TRANSGRIDV5_20180116135943","2017-12-30T08:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.68031999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84272,"TRANSGRIDV5_20180116135943","2017-12-30T06:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.52997999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84273,"TRANSGRIDV5_20180116135943","2017-12-30T07:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.28917000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84274,"TRANSGRIDV5_20180116135943","2017-12-30T07:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.27992,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84275,"TRANSGRIDV5_20180116135943","2017-12-30T07:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.27653000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84276,"TRANSGRIDV5_20180116135943","2017-12-30T07:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.16561999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84277,"TRANSGRIDV5_20180116135943","2017-12-30T07:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.90049999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84278,"TRANSGRIDV5_20180116135943","2017-12-30T07:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.52449999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84279,"TRANSGRIDV5_20180116135943","2017-12-30T07:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.51224999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84280,"TRANSGRIDV5_20180116135943","2017-12-30T07:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.05936,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84281,"TRANSGRIDV5_20180116135943","2017-12-30T07:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-135.19682,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84282,"TRANSGRIDV5_20180116135943","2017-12-30T13:25:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.734660000000002,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84283,"TRANSGRIDV5_20180116135943","2017-12-30T13:15:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.837520000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84284,"TRANSGRIDV5_20180116135943","2017-12-30T13:10:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.732030000000002,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84285,"TRANSGRIDV5_20180116135943","2017-12-30T13:20:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.321259999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84286,"TRANSGRIDV5_20180116135943","2017-12-30T13:35:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-20.604469999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84287,"TRANSGRIDV5_20180116135943","2017-12-30T13:30:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-12.240790000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84288,"TRANSGRIDV5_20180116135943","2017-12-30T13:05:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-11.797560000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84289,"TRANSGRIDV5_20180116135943","2017-12-30T12:45:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-11.73415,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84290,"TRANSGRIDV5_20180116135943","2017-12-30T19:20:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-10.003360000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84291,"TRANSGRIDV5_20180116135943","2017-12-30T16:40:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-20.100840000000002,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84292,"TRANSGRIDV5_20180116135943","2017-12-30T15:45:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-19.914269999999998,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84293,"TRANSGRIDV5_20180116135943","2017-12-30T16:55:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-19.396190000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84294,"TRANSGRIDV5_20180116135943","2017-12-30T15:55:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-19.040040000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84295,"TRANSGRIDV5_20180116135943","2017-12-30T16:45:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-17.063410000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84296,"TRANSGRIDV5_20180116135943","2017-12-30T15:30:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-16.644580000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84297,"TRANSGRIDV5_20180116135943","2017-12-30T16:00:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-15.11515,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84298,"TRANSGRIDV5_20180116135943","2017-12-30T16:15:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-13.342320000000001,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84299,"TRANSGRIDV5_20180116135943","2017-12-30T15:25:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-12.47386,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84300,"TRANSGRIDV5_20180116135943","2017-12-30T16:20:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-12.28853,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84301,"TRANSGRIDV5_20180116135943","2017-12-30T17:00:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-11.55734,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84302,"TRANSGRIDV5_20180116135943","2017-12-30T16:35:00","V::N_NIL_S2","V-NIL","2017-04-20",1,-10.765029999999999,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, SA accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84303,"TRANSGRIDV5_20180116135943","2017-12-30T02:20:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-14.19697,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84304,"TRANSGRIDV5_20180116135943","2017-12-30T14:30:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-12.87167,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84305,"TRANSGRIDV5_20180116135943","2017-12-30T02:25:00","V::N_NIL_V2","V-NIL","2017-04-20",1,-10.33704,"Out = NIL, prevent transient instability for fault and trip of a HWTS-SMTS 500 kV line, VIC accelerates, Yallourn W G1 on 500 kV.","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84306,"TRANSGRIDV5_20180116135943","2017-12-31T13:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-387.83,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84307,"TRANSGRIDV5_20180116135943","2017-12-31T13:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-194.76,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84308,"TRANSGRIDV5_20180116135943","2017-12-31T13:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08006,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84309,"TRANSGRIDV5_20180116135943","2017-12-31T13:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84310,"TRANSGRIDV5_20180116135943","2017-12-31T13:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84311,"TRANSGRIDV5_20180116135943","2017-12-31T13:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84312,"TRANSGRIDV5_20180116135943","2017-12-31T13:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.08,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84313,"TRANSGRIDV5_20180116135943","2017-12-31T13:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-173.07998000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84314,"TRANSGRIDV5_20180116135943","2017-12-31T11:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98000999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84315,"TRANSGRIDV5_20180116135943","2017-12-31T12:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98000999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84316,"TRANSGRIDV5_20180116135943","2017-12-31T12:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98000999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84317,"TRANSGRIDV5_20180116135943","2017-12-31T13:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98000999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84318,"TRANSGRIDV5_20180116135943","2017-12-31T13:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.98000999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84319,"TRANSGRIDV5_20180116135943","2017-12-31T13:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.61001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84320,"TRANSGRIDV5_20180116135943","2017-12-31T14:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.61001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84321,"TRANSGRIDV5_20180116135943","2017-12-31T14:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.61001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84322,"TRANSGRIDV5_20180116135943","2017-12-31T14:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.61001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84323,"TRANSGRIDV5_20180116135943","2017-12-31T14:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.61001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84324,"TRANSGRIDV5_20180116135943","2017-12-31T13:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.60004000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84325,"TRANSGRIDV5_20180116135943","2017-12-31T14:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-172.60004000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84326,"TRANSGRIDV5_20180116135943","2017-12-31T14:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-163.67998,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84327,"TRANSGRIDV5_20180116135943","2017-12-31T17:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-162.37003000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84328,"TRANSGRIDV5_20180116135943","2017-12-31T12:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61002999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84329,"TRANSGRIDV5_20180116135943","2017-12-31T18:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61002999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84330,"TRANSGRIDV5_20180116135943","2017-12-31T18:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84331,"TRANSGRIDV5_20180116135943","2017-12-31T12:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.60006000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84332,"TRANSGRIDV5_20180116135943","2017-12-31T16:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.60006000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84333,"TRANSGRIDV5_20180116135943","2017-12-31T11:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.6,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84334,"TRANSGRIDV5_20180116135943","2017-12-31T16:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.58000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84335,"TRANSGRIDV5_20180116135943","2017-12-31T17:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.46043,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84336,"TRANSGRIDV5_20180116135943","2017-12-31T18:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.38732999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84337,"TRANSGRIDV5_20180116135943","2017-12-31T16:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.07695000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84338,"TRANSGRIDV5_20180116135943","2017-12-31T17:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.06388999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84339,"TRANSGRIDV5_20180116135943","2017-12-31T17:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.04911000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84340,"TRANSGRIDV5_20180116135943","2017-12-31T17:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-161.04480000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84341,"TRANSGRIDV5_20180116135943","2017-12-31T16:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-160.57831999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84342,"TRANSGRIDV5_20180116135943","2017-12-31T17:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-160.55965,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84343,"TRANSGRIDV5_20180116135943","2017-12-31T17:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-160.55058,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84344,"TRANSGRIDV5_20180116135943","2017-12-31T16:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-160.53720000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84345,"TRANSGRIDV5_20180116135943","2017-12-31T17:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-159.36395999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84346,"TRANSGRIDV5_20180116135943","2017-12-31T17:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-155.92004,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84347,"TRANSGRIDV5_20180116135943","2017-12-31T12:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-153.20735999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84348,"TRANSGRIDV5_20180116135943","2017-12-31T11:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87009,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84349,"TRANSGRIDV5_20180116135943","2017-12-31T12:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87009,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84350,"TRANSGRIDV5_20180116135943","2017-12-31T11:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87003000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84351,"TRANSGRIDV5_20180116135943","2017-12-31T11:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87003000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84352,"TRANSGRIDV5_20180116135943","2017-12-31T11:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84353,"TRANSGRIDV5_20180116135943","2017-12-31T11:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84354,"TRANSGRIDV5_20180116135943","2017-12-31T12:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84355,"TRANSGRIDV5_20180116135943","2017-12-31T12:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84356,"TRANSGRIDV5_20180116135943","2017-12-31T12:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84357,"TRANSGRIDV5_20180116135943","2017-12-31T12:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84358,"TRANSGRIDV5_20180116135943","2017-12-31T12:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84359,"TRANSGRIDV5_20180116135943","2017-12-31T12:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84360,"TRANSGRIDV5_20180116135943","2017-12-31T17:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84361,"TRANSGRIDV5_20180116135943","2017-12-31T17:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-152.87,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84362,"TRANSGRIDV5_20180116135943","2017-12-31T11:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-149.35084000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84363,"TRANSGRIDV5_20180116135943","2017-12-31T11:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-148.88,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84364,"TRANSGRIDV5_20180116135943","2017-12-31T10:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.84,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84365,"TRANSGRIDV5_20180116135943","2017-12-31T11:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.84,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84366,"TRANSGRIDV5_20180116135943","2017-12-31T10:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84367,"TRANSGRIDV5_20180116135943","2017-12-31T11:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84368,"TRANSGRIDV5_20180116135943","2017-12-31T11:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.83001999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84369,"TRANSGRIDV5_20180116135943","2017-12-31T10:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61653999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84370,"TRANSGRIDV5_20180116135943","2017-12-31T07:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61002999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84371,"TRANSGRIDV5_20180116135943","2017-12-31T07:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84372,"TRANSGRIDV5_20180116135943","2017-12-31T08:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84373,"TRANSGRIDV5_20180116135943","2017-12-31T10:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.61000000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84374,"TRANSGRIDV5_20180116135943","2017-12-31T08:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84375,"TRANSGRIDV5_20180116135943","2017-12-31T08:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84376,"TRANSGRIDV5_20180116135943","2017-12-31T09:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84377,"TRANSGRIDV5_20180116135943","2017-12-31T09:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84378,"TRANSGRIDV5_20180116135943","2017-12-31T09:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84379,"TRANSGRIDV5_20180116135943","2017-12-31T10:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84380,"TRANSGRIDV5_20180116135943","2017-12-31T10:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84381,"TRANSGRIDV5_20180116135943","2017-12-31T10:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.60997,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84382,"TRANSGRIDV5_20180116135943","2017-12-31T08:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-147.02096,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84383,"TRANSGRIDV5_20180116135943","2017-12-31T08:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.85906,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84384,"TRANSGRIDV5_20180116135943","2017-12-31T10:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.83527000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84385,"TRANSGRIDV5_20180116135943","2017-12-31T08:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.05037999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84386,"TRANSGRIDV5_20180116135943","2017-12-31T08:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-146.01855,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84387,"TRANSGRIDV5_20180116135943","2017-12-31T10:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.98792,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84388,"TRANSGRIDV5_20180116135943","2017-12-31T10:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.95060000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84389,"TRANSGRIDV5_20180116135943","2017-12-31T10:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.83655999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84390,"TRANSGRIDV5_20180116135943","2017-12-31T08:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.63128,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84391,"TRANSGRIDV5_20180116135943","2017-12-31T08:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.60980000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84392,"TRANSGRIDV5_20180116135943","2017-12-31T08:05:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.20157,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84393,"TRANSGRIDV5_20180116135943","2017-12-31T09:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.19408999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84394,"TRANSGRIDV5_20180116135943","2017-12-31T07:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.19237000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84395,"TRANSGRIDV5_20180116135943","2017-12-31T09:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.15928,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84396,"TRANSGRIDV5_20180116135943","2017-12-31T07:55:00","#KSP1_E","#KSP1_E","2017-12-22",1,-145.11426,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84397,"TRANSGRIDV5_20180116135943","2017-12-31T10:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.77126000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84398,"TRANSGRIDV5_20180116135943","2017-12-31T07:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.40407999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84399,"TRANSGRIDV5_20180116135943","2017-12-31T07:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.39833999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84400,"TRANSGRIDV5_20180116135943","2017-12-31T09:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.3963,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84401,"TRANSGRIDV5_20180116135943","2017-12-31T09:45:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.37522000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84402,"TRANSGRIDV5_20180116135943","2017-12-31T07:40:00","#KSP1_E","#KSP1_E","2017-12-22",1,-144.23409000000001,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84403,"TRANSGRIDV5_20180116135943","2017-12-31T07:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.98658,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84404,"TRANSGRIDV5_20180116135943","2017-12-31T09:35:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.62894,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84405,"TRANSGRIDV5_20180116135943","2017-12-31T09:30:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.62563,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84406,"TRANSGRIDV5_20180116135943","2017-12-31T09:15:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.6131,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84407,"TRANSGRIDV5_20180116135943","2017-12-31T09:10:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.18577999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84408,"TRANSGRIDV5_20180116135943","2017-12-31T08:50:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.13283999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84409,"TRANSGRIDV5_20180116135943","2017-12-31T07:25:00","#KSP1_E","#KSP1_E","2017-12-22",1,-143.10382999999999,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84410,"TRANSGRIDV5_20180116135943","2017-12-31T09:20:00","#KSP1_E","#KSP1_E","2017-12-22",1,-142.84402,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84411,"TRANSGRIDV5_20180116135943","2017-12-31T08:00:00","#KSP1_E","#KSP1_E","2017-12-22",1,-140.81707,"QROG1K.ENERGY * 1 <= 10 (Wt = 360)","OUTAGE","OTHER","Kidston Solar Farm","REGULATED","99","Non Inclusion",null,0]
[84412,"TRANSGRIDV5_20180116135943","2017-12-31T13:35:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-227.08384000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84413,"TRANSGRIDV5_20180116135943","2017-12-31T13:30:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-42.897669999999998,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84414,"TRANSGRIDV5_20180116135943","2017-12-31T11:50:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.523540000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84415,"TRANSGRIDV5_20180116135943","2017-12-31T14:50:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.409479999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84416,"TRANSGRIDV5_20180116135943","2017-12-31T12:30:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.40559,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84417,"TRANSGRIDV5_20180116135943","2017-12-31T13:20:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.29609,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84418,"TRANSGRIDV5_20180116135943","2017-12-31T13:15:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.28256,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84419,"TRANSGRIDV5_20180116135943","2017-12-31T12:55:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.275590000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84420,"TRANSGRIDV5_20180116135943","2017-12-31T13:25:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.194489999999998,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84421,"TRANSGRIDV5_20180116135943","2017-12-31T13:50:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.137370000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84422,"TRANSGRIDV5_20180116135943","2017-12-31T14:40:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.123760000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84423,"TRANSGRIDV5_20180116135943","2017-12-31T14:10:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.11205,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84424,"TRANSGRIDV5_20180116135943","2017-12-31T13:40:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-22.060500000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84425,"TRANSGRIDV5_20180116135943","2017-12-31T13:55:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.986059999999998,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84426,"TRANSGRIDV5_20180116135943","2017-12-31T14:35:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.946459999999998,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84427,"TRANSGRIDV5_20180116135943","2017-12-31T14:20:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.934560000000001,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84428,"TRANSGRIDV5_20180116135943","2017-12-31T13:10:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.67661,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84429,"TRANSGRIDV5_20180116135943","2017-12-31T13:45:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-21.65897,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84430,"TRANSGRIDV5_20180116135943","2017-12-31T14:15:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-19.07461,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84431,"TRANSGRIDV5_20180116135943","2017-12-31T14:30:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-18.518350000000002,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84432,"TRANSGRIDV5_20180116135943","2017-12-31T14:00:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-17.97025,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84433,"TRANSGRIDV5_20180116135943","2017-12-31T13:00:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-16.568069999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84434,"TRANSGRIDV5_20180116135943","2017-12-31T14:55:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-16.322559999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84435,"TRANSGRIDV5_20180116135943","2017-12-31T14:25:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-15.847799999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84436,"TRANSGRIDV5_20180116135943","2017-12-31T14:45:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-15.79097,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84437,"TRANSGRIDV5_20180116135943","2017-12-31T14:05:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-13.602959999999999,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84438,"TRANSGRIDV5_20180116135943","2017-12-31T12:40:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-11.4633,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84439,"TRANSGRIDV5_20180116135943","2017-12-31T12:50:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-11.42127,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84440,"TRANSGRIDV5_20180116135943","2017-12-31T13:05:00","N^^Q_NIL_A","N-NIL","2017-12-06",1,-10.39794,"Out= Nil, avoid Voltage Collapse on loss of Liddell to Muswellbrook (83) line","SYSTEM NORMAL","OTHER",null,"","","",null,0]
[84441,"TRANSGRIDV5_20180116135943","2017-10-09T18:50:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-32.318420000000003,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[84442,"TRANSGRIDV5_20180116135943","2017-10-12T02:10:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-10.959540000000001,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]
[84443,"TRANSGRIDV5_20180116135943","2017-10-12T16:40:00","N^N_KKLS_1","N-KKLS_967","2013-08-21",1,-11.326269999999999,"Out= Koolkhan to Lismore (967), avoid voltage collapse on trip of Coffs Harbour to Lismore (89), swamp out when all 3 Directlink O/S","OUTAGE","OTHER","Koolkhan to Lismore 132kV Line 967","REGULATED","INCLUDED","","PLANNED",1]